| AI Engine Intrinsics User Guide (AIE) v2025.2

Loading...
Searching...
No Matches
Functions
Dynamic Z buffer conjugation
Intrinsics » Vector Operations » MAC intrinsics » Multiplication » Advanced » Integer » Vector MAC combined with vector comparisons » 32 bit x 32 bit » 32 bit Real x 32 bit Complex

## Overview

32 bit real by 32 bit complex using Dynamic Z buffer conjugation

## Functions
v2cacc80 | lmac2_abs (v2cacc80 acc, v16int32 xbuff, int xstart, unsigned int xoffsets, int xstep, v4cint32 zbuff, int zstart, unsigned int zoffsets, int zstep, bool zconj)
| Complex multiply-accumulate intrinsic function with dynamic z buffer conjugation after computing the absolute value in the selected lanes from the input buffer using small X input buffer.
v2cacc80 | lmac2_abs (v2cacc80 acc, v32int32 xbuff, int xstart, unsigned int xoffsets, int xstep, v4cint32 zbuff, int zstart, unsigned int zoffsets, int zstep, bool zconj)
| Complex multiply-accumulate intrinsic function with dynamic z buffer conjugation after computing the absolute value in the selected lanes from the input buffer .
v2cacc80 | lmac2_max (v2cacc80 acc, v16int32 xbuff, int xstart, unsigned int xoffsets, int xstep, int ystart, v4cint32 zbuff, int zstart, unsigned int zoffsets, int zstep, bool zconj)
| Complex multiply-accumulate intrinsic function with dynamic z buffer conjugation after computing the maximum between the selected lanes from the input buffer using small X input buffer.
v2cacc80 | lmac2_max (v2cacc80 acc, v16int32 xbuff, int xstart, unsigned int xoffsets, int xstep, v16int32 ybuff, int ystart, v4cint32 zbuff, int zstart, unsigned int zoffsets, int zstep, bool zconj)
| Complex multiply-accumulate intrinsic function with dynamic z buffer conjugation after computing the maximum between the selected lanes from the input buffer using small X input buffer.
v2cacc80 | lmac2_max (v2cacc80 acc, v32int32 xbuff, int xstart, unsigned int xoffsets, int xstep, int ystart, v4cint32 zbuff, int zstart, unsigned int zoffsets, int zstep, bool zconj)
| Complex multiply-accumulate intrinsic function with dynamic z buffer conjugation after computing the maximum between the selected lanes from the input buffer .
v2cacc80 | lmac2_maxdiff (v2cacc80 acc, v16int32 xbuff, int xstart, unsigned int xoffsets, int xstep, int ystart, v4cint32 zbuff, int zstart, unsigned int zoffsets, int zstep, bool zconj)
| Complex multiply-accumulate intrinsic function with dynamic z buffer conjugation after computing the maximum difference between the selected lanes from the input buffer using small X input buffer.
v2cacc80 | lmac2_maxdiff (v2cacc80 acc, v16int32 xbuff, int xstart, unsigned int xoffsets, int xstep, v16int32 ybuff, int ystart, v4cint32 zbuff, int zstart, unsigned int zoffsets, int zstep, bool zconj)
| Complex multiply-accumulate intrinsic function with dynamic z buffer conjugation after computing the maximum difference between the selected lanes from the input buffer using small X input buffer.
v2cacc80 | lmac2_maxdiff (v2cacc80 acc, v32int32 xbuff, int xstart, unsigned int xoffsets, int xstep, int ystart, v4cint32 zbuff, int zstart, unsigned int zoffsets, int zstep, bool zconj)
| Complex multiply-accumulate intrinsic function with dynamic z buffer conjugation after computing the maximum difference between the selected lanes from the input buffer .
v2cacc80 | lmac2_min (v2cacc80 acc, v16int32 xbuff, int xstart, unsigned int xoffsets, int xstep, int ystart, v4cint32 zbuff, int zstart, unsigned int zoffsets, int zstep, bool zconj)
| Complex multiply-accumulate intrinsic function with dynamic z buffer conjugation after computing the minimum between the selected lanes from the input buffer using small X input buffer.
v2cacc80 | lmac2_min (v2cacc80 acc, v16int32 xbuff, int xstart, unsigned int xoffsets, int xstep, v16int32 ybuff, int ystart, v4cint32 zbuff, int zstart, unsigned int zoffsets, int zstep, bool zconj)
| Complex multiply-accumulate intrinsic function with dynamic z buffer conjugation after computing the minimum between the selected lanes from the input buffer using small X input buffer.
v2cacc80 | lmac2_min (v2cacc80 acc, v32int32 xbuff, int xstart, unsigned int xoffsets, int xstep, int ystart, v4cint32 zbuff, int zstart, unsigned int zoffsets, int zstep, bool zconj)
| Complex multiply-accumulate intrinsic function with dynamic z buffer conjugation after computing the minimum between the selected lanes from the input buffer .
v4cacc80 | lmac4_abs (v4cacc80 acc, v16int32 xbuff, int xstart, unsigned int xoffsets, v4cint32 zbuff, int zstart, unsigned int zoffsets, bool zconj)
| Complex multiply-accumulate intrinsic function with dynamic z buffer conjugation after computing the absolute value in the selected lanes from the input buffer using small X input buffer.
v4cacc80 | lmac4_abs (v4cacc80 acc, v32int32 xbuff, int xstart, unsigned int xoffsets, v4cint32 zbuff, int zstart, unsigned int zoffsets, bool zconj)
| Complex multiply-accumulate intrinsic function with dynamic z buffer conjugation after computing the absolute value in the selected lanes from the input buffer .
v4cacc80 | lmac4_max (v4cacc80 acc, v16int32 xbuff, int xstart, unsigned int xoffsets, int ystart, v4cint32 zbuff, int zstart, unsigned int zoffsets, bool zconj)
| Complex multiply-accumulate intrinsic function with dynamic z buffer conjugation after computing the maximum between the selected lanes from the input buffer using small X input buffer.
v4cacc80 | lmac4_max (v4cacc80 acc, v16int32 xbuff, int xstart, unsigned int xoffsets, v16int32 ybuff, int ystart, v4cint32 zbuff, int zstart, unsigned int zoffsets, bool zconj)
| Complex multiply-accumulate intrinsic function with dynamic z buffer conjugation after computing the maximum between the selected lanes from the input buffer using small X input buffer.
v4cacc80 | lmac4_max (v4cacc80 acc, v32int32 xbuff, int xstart, unsigned int xoffsets, int ystart, v4cint32 zbuff, int zstart, unsigned int zoffsets, bool zconj)
| Complex multiply-accumulate intrinsic function with dynamic z buffer conjugation after computing the maximum between the selected lanes from the input buffer .
v4cacc80 | lmac4_maxdiff (v4cacc80 acc, v16int32 xbuff, int xstart, unsigned int xoffsets, int ystart, v4cint32 zbuff, int zstart, unsigned int zoffsets, bool zconj)
| Complex multiply-accumulate intrinsic function with dynamic z buffer conjugation after computing the maximum difference between the selected lanes from the input buffer using small X input buffer.
v4cacc80 | lmac4_maxdiff (v4cacc80 acc, v16int32 xbuff, int xstart, unsigned int xoffsets, v16int32 ybuff, int ystart, v4cint32 zbuff, int zstart, unsigned int zoffsets, bool zconj)
| Complex multiply-accumulate intrinsic function with dynamic z buffer conjugation after computing the maximum difference between the selected lanes from the input buffer using small X input buffer.
v4cacc80 | lmac4_maxdiff (v4cacc80 acc, v32int32 xbuff, int xstart, unsigned int xoffsets, int ystart, v4cint32 zbuff, int zstart, unsigned int zoffsets, bool zconj)
| Complex multiply-accumulate intrinsic function with dynamic z buffer conjugation after computing the maximum difference between the selected lanes from the input buffer .
v4cacc80 | lmac4_min (v4cacc80 acc, v16int32 xbuff, int xstart, unsigned int xoffsets, int ystart, v4cint32 zbuff, int zstart, unsigned int zoffsets, bool zconj)
| Complex multiply-accumulate intrinsic function with dynamic z buffer conjugation after computing the minimum between the selected lanes from the input buffer using small X input buffer.
v4cacc80 | lmac4_min (v4cacc80 acc, v16int32 xbuff, int xstart, unsigned int xoffsets, v16int32 ybuff, int ystart, v4cint32 zbuff, int zstart, unsigned int zoffsets, bool zconj)
| Complex multiply-accumulate intrinsic function with dynamic z buffer conjugation after computing the minimum between the selected lanes from the input buffer using small X input buffer.
v4cacc80 | lmac4_min (v4cacc80 acc, v32int32 xbuff, int xstart, unsigned int xoffsets, int ystart, v4cint32 zbuff, int zstart, unsigned int zoffsets, bool zconj)
| Complex multiply-accumulate intrinsic function with dynamic z buffer conjugation after computing the minimum between the selected lanes from the input buffer .
v2cacc80 | lmsc2_abs (v2cacc80 acc, v16int32 xbuff, int xstart, unsigned int xoffsets, int xstep, v4cint32 zbuff, int zstart, unsigned int zoffsets, int zstep, bool zconj)
| Complex multiply-subtract intrinsic function with dynamic z buffer conjugation after computing the absolute value in the selected lanes from the input buffer using small X input buffer.
v2cacc80 | lmsc2_abs (v2cacc80 acc, v32int32 xbuff, int xstart, unsigned int xoffsets, int xstep, v4cint32 zbuff, int zstart, unsigned int zoffsets, int zstep, bool zconj)
| Complex multiply-subtract intrinsic function with dynamic z buffer conjugation after computing the absolute value in the selected lanes from the input buffer .
v2cacc80 | lmsc2_max (v2cacc80 acc, v16int32 xbuff, int xstart, unsigned int xoffsets, int xstep, int ystart, v4cint32 zbuff, int zstart, unsigned int zoffsets, int zstep, bool zconj)
| Complex multiply-subtract intrinsic function with dynamic z buffer conjugation after computing the maximum between the selected lanes from the input buffer using small X input buffer.
v2cacc80 | lmsc2_max (v2cacc80 acc, v16int32 xbuff, int xstart, unsigned int xoffsets, int xstep, v16int32 ybuff, int ystart, v4cint32 zbuff, int zstart, unsigned int zoffsets, int zstep, bool zconj)
| Complex multiply-subtract intrinsic function with dynamic z buffer conjugation after computing the maximum between the selected lanes from the input buffer using small X input buffer.
v2cacc80 | lmsc2_max (v2cacc80 acc, v32int32 xbuff, int xstart, unsigned int xoffsets, int xstep, int ystart, v4cint32 zbuff, int zstart, unsigned int zoffsets, int zstep, bool zconj)
| Complex multiply-subtract intrinsic function with dynamic z buffer conjugation after computing the maximum between the selected lanes from the input buffer .
v2cacc80 | lmsc2_maxdiff (v2cacc80 acc, v16int32 xbuff, int xstart, unsigned int xoffsets, int xstep, int ystart, v4cint32 zbuff, int zstart, unsigned int zoffsets, int zstep, bool zconj)
| Complex multiply-subtract intrinsic function with dynamic z buffer conjugation after computing the maximum difference between the selected lanes from the input buffer using small X input buffer.
v2cacc80 | lmsc2_maxdiff (v2cacc80 acc, v16int32 xbuff, int xstart, unsigned int xoffsets, int xstep, v16int32 ybuff, int ystart, v4cint32 zbuff, int zstart, unsigned int zoffsets, int zstep, bool zconj)
| Complex multiply-subtract intrinsic function with dynamic z buffer conjugation after computing the maximum difference between the selected lanes from the input buffer using small X input buffer.
v2cacc80 | lmsc2_maxdiff (v2cacc80 acc, v32int32 xbuff, int xstart, unsigned int xoffsets, int xstep, int ystart, v4cint32 zbuff, int zstart, unsigned int zoffsets, int zstep, bool zconj)
| Complex multiply-subtract intrinsic function with dynamic z buffer conjugation after computing the maximum difference between the selected lanes from the input buffer .
v2cacc80 | lmsc2_min (v2cacc80 acc, v16int32 xbuff, int xstart, unsigned int xoffsets, int xstep, int ystart, v4cint32 zbuff, int zstart, unsigned int zoffsets, int zstep, bool zconj)
| Complex multiply-subtract intrinsic function with dynamic z buffer conjugation after computing the minimum between the selected lanes from the input buffer using small X input buffer.
v2cacc80 | lmsc2_min (v2cacc80 acc, v16int32 xbuff, int xstart, unsigned int xoffsets, int xstep, v16int32 ybuff, int ystart, v4cint32 zbuff, int zstart, unsigned int zoffsets, int zstep, bool zconj)
| Complex multiply-subtract intrinsic function with dynamic z buffer conjugation after computing the minimum between the selected lanes from the input buffer using small X input buffer.
v2cacc80 | lmsc2_min (v2cacc80 acc, v32int32 xbuff, int xstart, unsigned int xoffsets, int xstep, int ystart, v4cint32 zbuff, int zstart, unsigned int zoffsets, int zstep, bool zconj)
| Complex multiply-subtract intrinsic function with dynamic z buffer conjugation after computing the minimum between the selected lanes from the input buffer .
v4cacc80 | lmsc4_abs (v4cacc80 acc, v16int32 xbuff, int xstart, unsigned int xoffsets, v4cint32 zbuff, int zstart, unsigned int zoffsets, bool zconj)
| Complex multiply-subtract intrinsic function with dynamic z buffer conjugation after computing the absolute value in the selected lanes from the input buffer using small X input buffer.
v4cacc80 | lmsc4_abs (v4cacc80 acc, v32int32 xbuff, int xstart, unsigned int xoffsets, v4cint32 zbuff, int zstart, unsigned int zoffsets, bool zconj)
| Complex multiply-subtract intrinsic function with dynamic z buffer conjugation after computing the absolute value in the selected lanes from the input buffer .
v4cacc80 | lmsc4_max (v4cacc80 acc, v16int32 xbuff, int xstart, unsigned int xoffsets, int ystart, v4cint32 zbuff, int zstart, unsigned int zoffsets, bool zconj)
| Complex multiply-subtract intrinsic function with dynamic z buffer conjugation after computing the maximum between the selected lanes from the input buffer using small X input buffer.
v4cacc80 | lmsc4_max (v4cacc80 acc, v16int32 xbuff, int xstart, unsigned int xoffsets, v16int32 ybuff, int ystart, v4cint32 zbuff, int zstart, unsigned int zoffsets, bool zconj)
| Complex multiply-subtract intrinsic function with dynamic z buffer conjugation after computing the maximum between the selected lanes from the input buffer using small X input buffer.
v4cacc80 | lmsc4_max (v4cacc80 acc, v32int32 xbuff, int xstart, unsigned int xoffsets, int ystart, v4cint32 zbuff, int zstart, unsigned int zoffsets, bool zconj)
| Complex multiply-subtract intrinsic function with dynamic z buffer conjugation after computing the maximum between the selected lanes from the input buffer .
v4cacc80 | lmsc4_maxdiff (v4cacc80 acc, v16int32 xbuff, int xstart, unsigned int xoffsets, int ystart, v4cint32 zbuff, int zstart, unsigned int zoffsets, bool zconj)
| Complex multiply-subtract intrinsic function with dynamic z buffer conjugation after computing the maximum difference between the selected lanes from the input buffer using small X input buffer.
v4cacc80 | lmsc4_maxdiff (v4cacc80 acc, v16int32 xbuff, int xstart, unsigned int xoffsets, v16int32 ybuff, int ystart, v4cint32 zbuff, int zstart, unsigned int zoffsets, bool zconj)
| Complex multiply-subtract intrinsic function with dynamic z buffer conjugation after computing the maximum difference between the selected lanes from the input buffer using small X input buffer.
v4cacc80 | lmsc4_maxdiff (v4cacc80 acc, v32int32 xbuff, int xstart, unsigned int xoffsets, int ystart, v4cint32 zbuff, int zstart, unsigned int zoffsets, bool zconj)
| Complex multiply-subtract intrinsic function with dynamic z buffer conjugation after computing the maximum difference between the selected lanes from the input buffer .
v4cacc80 | lmsc4_min (v4cacc80 acc, v16int32 xbuff, int xstart, unsigned int xoffsets, int ystart, v4cint32 zbuff, int zstart, unsigned int zoffsets, bool zconj)
| Complex multiply-subtract intrinsic function with dynamic z buffer conjugation after computing the minimum between the selected lanes from the input buffer using small X input buffer.
v4cacc80 | lmsc4_min (v4cacc80 acc, v16int32 xbuff, int xstart, unsigned int xoffsets, v16int32 ybuff, int ystart, v4cint32 zbuff, int zstart, unsigned int zoffsets, bool zconj)
| Complex multiply-subtract intrinsic function with dynamic z buffer conjugation after computing the minimum between the selected lanes from the input buffer using small X input buffer.
v4cacc80 | lmsc4_min (v4cacc80 acc, v32int32 xbuff, int xstart, unsigned int xoffsets, int ystart, v4cint32 zbuff, int zstart, unsigned int zoffsets, bool zconj)
| Complex multiply-subtract intrinsic function with dynamic z buffer conjugation after computing the minimum between the selected lanes from the input buffer .
v2cacc80 | lmul2_abs (v16int32 xbuff, int xstart, unsigned int xoffsets, int xstep, v4cint32 zbuff, int zstart, unsigned int zoffsets, int zstep, bool zconj)
| Complex multiply intrinsic function with dynamic z buffer conjugation after computing the absolute value in the selected lanes from the input buffer using small X input buffer.
v2cacc80 | lmul2_abs (v32int32 xbuff, int xstart, unsigned int xoffsets, int xstep, v4cint32 zbuff, int zstart, unsigned int zoffsets, int zstep, bool zconj)
| Complex multiply intrinsic function with dynamic z buffer conjugation after computing the absolute value in the selected lanes from the input buffer .
v2cacc80 | lmul2_max (v16int32 xbuff, int xstart, unsigned int xoffsets, int xstep, int ystart, v4cint32 zbuff, int zstart, unsigned int zoffsets, int zstep, bool zconj)
| Complex multiply intrinsic function with dynamic z buffer conjugation after computing the maximum between the selected lanes from the input buffer using small X input buffer.
v2cacc80 | lmul2_max (v16int32 xbuff, int xstart, unsigned int xoffsets, int xstep, v16int32 ybuff, int ystart, v4cint32 zbuff, int zstart, unsigned int zoffsets, int zstep, bool zconj)
| Complex multiply intrinsic function with dynamic z buffer conjugation after computing the maximum between the selected lanes from the input buffer using small X input buffer.
v2cacc80 | lmul2_max (v32int32 xbuff, int xstart, unsigned int xoffsets, int xstep, int ystart, v4cint32 zbuff, int zstart, unsigned int zoffsets, int zstep, bool zconj)
| Complex multiply intrinsic function with dynamic z buffer conjugation after computing the maximum between the selected lanes from the input buffer .
v2cacc80 | lmul2_maxdiff (v16int32 xbuff, int xstart, unsigned int xoffsets, int xstep, int ystart, v4cint32 zbuff, int zstart, unsigned int zoffsets, int zstep, bool zconj)
| Complex multiply intrinsic function with dynamic z buffer conjugation after computing the maximum difference between the selected lanes from the input buffer using small X input buffer.
v2cacc80 | lmul2_maxdiff (v16int32 xbuff, int xstart, unsigned int xoffsets, int xstep, v16int32 ybuff, int ystart, v4cint32 zbuff, int zstart, unsigned int zoffsets, int zstep, bool zconj)
| Complex multiply intrinsic function with dynamic z buffer conjugation after computing the maximum difference between the selected lanes from the input buffer using small X input buffer.
v2cacc80 | lmul2_maxdiff (v32int32 xbuff, int xstart, unsigned int xoffsets, int xstep, int ystart, v4cint32 zbuff, int zstart, unsigned int zoffsets, int zstep, bool zconj)
| Complex multiply intrinsic function with dynamic z buffer conjugation after computing the maximum difference between the selected lanes from the input buffer .
v2cacc80 | lmul2_min (v16int32 xbuff, int xstart, unsigned int xoffsets, int xstep, int ystart, v4cint32 zbuff, int zstart, unsigned int zoffsets, int zstep, bool zconj)
| Complex multiply intrinsic function with dynamic z buffer conjugation after computing the minimum between the selected lanes from the input buffer using small X input buffer.
v2cacc80 | lmul2_min (v16int32 xbuff, int xstart, unsigned int xoffsets, int xstep, v16int32 ybuff, int ystart, v4cint32 zbuff, int zstart, unsigned int zoffsets, int zstep, bool zconj)
| Complex multiply intrinsic function with dynamic z buffer conjugation after computing the minimum between the selected lanes from the input buffer using small X input buffer.
v2cacc80 | lmul2_min (v32int32 xbuff, int xstart, unsigned int xoffsets, int xstep, int ystart, v4cint32 zbuff, int zstart, unsigned int zoffsets, int zstep, bool zconj)
| Complex multiply intrinsic function with dynamic z buffer conjugation after computing the minimum between the selected lanes from the input buffer .
v4cacc80 | lmul4_abs (v16int32 xbuff, int xstart, unsigned int xoffsets, v4cint32 zbuff, int zstart, unsigned int zoffsets, bool zconj)
| Complex multiply intrinsic function with dynamic z buffer conjugation after computing the absolute value in the selected lanes from the input buffer using small X input buffer.
v4cacc80 | lmul4_abs (v32int32 xbuff, int xstart, unsigned int xoffsets, v4cint32 zbuff, int zstart, unsigned int zoffsets, bool zconj)
| Complex multiply intrinsic function with dynamic z buffer conjugation after computing the absolute value in the selected lanes from the input buffer .
v4cacc80 | lmul4_max (v16int32 xbuff, int xstart, unsigned int xoffsets, int ystart, v4cint32 zbuff, int zstart, unsigned int zoffsets, bool zconj)
| Complex multiply intrinsic function with dynamic z buffer conjugation after computing the maximum between the selected lanes from the input buffer using small X input buffer.
v4cacc80 | lmul4_max (v16int32 xbuff, int xstart, unsigned int xoffsets, v16int32 ybuff, int ystart, v4cint32 zbuff, int zstart, unsigned int zoffsets, bool zconj)
| Complex multiply intrinsic function with dynamic z buffer conjugation after computing the maximum between the selected lanes from the input buffer using small X input buffer.
v4cacc80 | lmul4_max (v32int32 xbuff, int xstart, unsigned int xoffsets, int ystart, v4cint32 zbuff, int zstart, unsigned int zoffsets, bool zconj)
| Complex multiply intrinsic function with dynamic z buffer conjugation after computing the maximum between the selected lanes from the input buffer .
v4cacc80 | lmul4_maxdiff (v16int32 xbuff, int xstart, unsigned int xoffsets, int ystart, v4cint32 zbuff, int zstart, unsigned int zoffsets, bool zconj)
| Complex multiply intrinsic function with dynamic z buffer conjugation after computing the maximum difference between the selected lanes from the input buffer using small X input buffer.
v4cacc80 | lmul4_maxdiff (v16int32 xbuff, int xstart, unsigned int xoffsets, v16int32 ybuff, int ystart, v4cint32 zbuff, int zstart, unsigned int zoffsets, bool zconj)
| Complex multiply intrinsic function with dynamic z buffer conjugation after computing the maximum difference between the selected lanes from the input buffer using small X input buffer.
v4cacc80 | lmul4_maxdiff (v32int32 xbuff, int xstart, unsigned int xoffsets, int ystart, v4cint32 zbuff, int zstart, unsigned int zoffsets, bool zconj)
| Complex multiply intrinsic function with dynamic z buffer conjugation after computing the maximum difference between the selected lanes from the input buffer .
v4cacc80 | lmul4_min (v16int32 xbuff, int xstart, unsigned int xoffsets, int ystart, v4cint32 zbuff, int zstart, unsigned int zoffsets, bool zconj)
| Complex multiply intrinsic function with dynamic z buffer conjugation after computing the minimum between the selected lanes from the input buffer using small X input buffer.
v4cacc80 | lmul4_min (v16int32 xbuff, int xstart, unsigned int xoffsets, v16int32 ybuff, int ystart, v4cint32 zbuff, int zstart, unsigned int zoffsets, bool zconj)
| Complex multiply intrinsic function with dynamic z buffer conjugation after computing the minimum between the selected lanes from the input buffer using small X input buffer.
v4cacc80 | lmul4_min (v32int32 xbuff, int xstart, unsigned int xoffsets, int ystart, v4cint32 zbuff, int zstart, unsigned int zoffsets, bool zconj)
| Complex multiply intrinsic function with dynamic z buffer conjugation after computing the minimum between the selected lanes from the input buffer .
v2cacc80 | lnegmul2_abs (v16int32 xbuff, int xstart, unsigned int xoffsets, int xstep, v4cint32 zbuff, int zstart, unsigned int zoffsets, int zstep, bool zconj)
| Complex multiply-negate intrinsic function with dynamic z buffer conjugation after computing the absolute value in the selected lanes from the input buffer using small X input buffer.
v2cacc80 | lnegmul2_abs (v32int32 xbuff, int xstart, unsigned int xoffsets, int xstep, v4cint32 zbuff, int zstart, unsigned int zoffsets, int zstep, bool zconj)
| Complex multiply-negate intrinsic function with dynamic z buffer conjugation after computing the absolute value in the selected lanes from the input buffer .
v2cacc80 | lnegmul2_max (v16int32 xbuff, int xstart, unsigned int xoffsets, int xstep, int ystart, v4cint32 zbuff, int zstart, unsigned int zoffsets, int zstep, bool zconj)
| Complex multiply-negate intrinsic function with dynamic z buffer conjugation after computing the maximum between the selected lanes from the input buffer using small X input buffer.
v2cacc80 | lnegmul2_max (v16int32 xbuff, int xstart, unsigned int xoffsets, int xstep, v16int32 ybuff, int ystart, v4cint32 zbuff, int zstart, unsigned int zoffsets, int zstep, bool zconj)
| Complex multiply-negate intrinsic function with dynamic z buffer conjugation after computing the maximum between the selected lanes from the input buffer using small X input buffer.
v2cacc80 | lnegmul2_max (v32int32 xbuff, int xstart, unsigned int xoffsets, int xstep, int ystart, v4cint32 zbuff, int zstart, unsigned int zoffsets, int zstep, bool zconj)
| Complex multiply-negate intrinsic function with dynamic z buffer conjugation after computing the maximum between the selected lanes from the input buffer .
v2cacc80 | lnegmul2_maxdiff (v16int32 xbuff, int xstart, unsigned int xoffsets, int xstep, int ystart, v4cint32 zbuff, int zstart, unsigned int zoffsets, int zstep, bool zconj)
| Complex multiply-negate intrinsic function with dynamic z buffer conjugation after computing the maximum difference between the selected lanes from the input buffer using small X input buffer.
v2cacc80 | lnegmul2_maxdiff (v16int32 xbuff, int xstart, unsigned int xoffsets, int xstep, v16int32 ybuff, int ystart, v4cint32 zbuff, int zstart, unsigned int zoffsets, int zstep, bool zconj)
| Complex multiply-negate intrinsic function with dynamic z buffer conjugation after computing the maximum difference between the selected lanes from the input buffer using small X input buffer.
v2cacc80 | lnegmul2_maxdiff (v32int32 xbuff, int xstart, unsigned int xoffsets, int xstep, int ystart, v4cint32 zbuff, int zstart, unsigned int zoffsets, int zstep, bool zconj)
| Complex multiply-negate intrinsic function with dynamic z buffer conjugation after computing the maximum difference between the selected lanes from the input buffer .
v2cacc80 | lnegmul2_min (v16int32 xbuff, int xstart, unsigned int xoffsets, int xstep, int ystart, v4cint32 zbuff, int zstart, unsigned int zoffsets, int zstep, bool zconj)
| Complex multiply-negate intrinsic function with dynamic z buffer conjugation after computing the minimum between the selected lanes from the input buffer using small X input buffer.
v2cacc80 | lnegmul2_min (v16int32 xbuff, int xstart, unsigned int xoffsets, int xstep, v16int32 ybuff, int ystart, v4cint32 zbuff, int zstart, unsigned int zoffsets, int zstep, bool zconj)
| Complex multiply-negate intrinsic function with dynamic z buffer conjugation after computing the minimum between the selected lanes from the input buffer using small X input buffer.
v2cacc80 | lnegmul2_min (v32int32 xbuff, int xstart, unsigned int xoffsets, int xstep, int ystart, v4cint32 zbuff, int zstart, unsigned int zoffsets, int zstep, bool zconj)
| Complex multiply-negate intrinsic function with dynamic z buffer conjugation after computing the minimum between the selected lanes from the input buffer .
v4cacc80 | lnegmul4_abs (v16int32 xbuff, int xstart, unsigned int xoffsets, v4cint32 zbuff, int zstart, unsigned int zoffsets, bool zconj)
| Complex multiply-negate intrinsic function with dynamic z buffer conjugation after computing the absolute value in the selected lanes from the input buffer using small X input buffer.
v4cacc80 | lnegmul4_abs (v32int32 xbuff, int xstart, unsigned int xoffsets, v4cint32 zbuff, int zstart, unsigned int zoffsets, bool zconj)
| Complex multiply-negate intrinsic function with dynamic z buffer conjugation after computing the absolute value in the selected lanes from the input buffer .
v4cacc80 | lnegmul4_max (v16int32 xbuff, int xstart, unsigned int xoffsets, int ystart, v4cint32 zbuff, int zstart, unsigned int zoffsets, bool zconj)
| Complex multiply-negate intrinsic function with dynamic z buffer conjugation after computing the maximum between the selected lanes from the input buffer using small X input buffer.
v4cacc80 | lnegmul4_max (v16int32 xbuff, int xstart, unsigned int xoffsets, v16int32 ybuff, int ystart, v4cint32 zbuff, int zstart, unsigned int zoffsets, bool zconj)
| Complex multiply-negate intrinsic function with dynamic z buffer conjugation after computing the maximum between the selected lanes from the input buffer using small X input buffer.
v4cacc80 | lnegmul4_max (v32int32 xbuff, int xstart, unsigned int xoffsets, int ystart, v4cint32 zbuff, int zstart, unsigned int zoffsets, bool zconj)
| Complex multiply-negate intrinsic function with dynamic z buffer conjugation after computing the maximum between the selected lanes from the input buffer .
v4cacc80 | lnegmul4_maxdiff (v16int32 xbuff, int xstart, unsigned int xoffsets, int ystart, v4cint32 zbuff, int zstart, unsigned int zoffsets, bool zconj)
| Complex multiply-negate intrinsic function with dynamic z buffer conjugation after computing the maximum difference between the selected lanes from the input buffer using small X input buffer.
v4cacc80 | lnegmul4_maxdiff (v16int32 xbuff, int xstart, unsigned int xoffsets, v16int32 ybuff, int ystart, v4cint32 zbuff, int zstart, unsigned int zoffsets, bool zconj)
| Complex multiply-negate intrinsic function with dynamic z buffer conjugation after computing the maximum difference between the selected lanes from the input buffer using small X input buffer.
v4cacc80 | lnegmul4_maxdiff (v32int32 xbuff, int xstart, unsigned int xoffsets, int ystart, v4cint32 zbuff, int zstart, unsigned int zoffsets, bool zconj)
| Complex multiply-negate intrinsic function with dynamic z buffer conjugation after computing the maximum difference between the selected lanes from the input buffer .
v4cacc80 | lnegmul4_min (v16int32 xbuff, int xstart, unsigned int xoffsets, int ystart, v4cint32 zbuff, int zstart, unsigned int zoffsets, bool zconj)
| Complex multiply-negate intrinsic function with dynamic z buffer conjugation after computing the minimum between the selected lanes from the input buffer using small X input buffer.
v4cacc80 | lnegmul4_min (v16int32 xbuff, int xstart, unsigned int xoffsets, v16int32 ybuff, int ystart, v4cint32 zbuff, int zstart, unsigned int zoffsets, bool zconj)
| Complex multiply-negate intrinsic function with dynamic z buffer conjugation after computing the minimum between the selected lanes from the input buffer using small X input buffer.
v4cacc80 | lnegmul4_min (v32int32 xbuff, int xstart, unsigned int xoffsets, int ystart, v4cint32 zbuff, int zstart, unsigned int zoffsets, bool zconj)
| Complex multiply-negate intrinsic function with dynamic z buffer conjugation after computing the minimum between the selected lanes from the input buffer .

## Function Documentation

## ◆ lmac2_abs() [1/2]

v2cacc80 lmac2_abs | ( | v2cacc80 | acc,
|  | v16int32 | xbuff,
|  | int | xstart,
|  | unsigned int | xoffsets,
|  | int | xstep,
|  | v4cint32 | zbuff,
|  | int | zstart,
|  | unsigned int | zoffsets,
|  | int | zstep,
|  | bool | zconj
| ) |  |

Complex multiply-accumulate intrinsic function with dynamic z buffer conjugation after computing the absolute value in the selected lanes from the input buffer using small X input buffer.

acc0 += z00*abs(x00) + z01*abs(x01)
acc1 += z10*abs(x10) + z11*abs(x11)

Returns
  Returned accumulation vector (2 x cint80 lanes)

Parameters

  acc | Incoming accumulation vector (2 x cint80 lanes)
  xbuff | Input buffer of 16 elements of type int32
  xstart | Starting position offset applied to all lanes of input from X buffer.
  xoffsets | 4b offset for each lane, applied to the x buffer. LSB apply to first lane
  xstep | Step between each column for selection in the xbuffer.
  zbuff | Input buffer of 4 elements of type cint32
  zstart | Starting position offset applied to all lanes for input from Z buffer. This must be a compile time constant. Only the 4 LSB of the argument are used.
  zoffsets | 4b offset for each lane, applied to input from Z buffer. LSB apply to first lane
  zstep | Step between each column for selection in the zbuffer.
  zconj | Selector for conjugation in Z buffer

Note
  - For more information on how data selection works from the buffers go here. The data buffer and coefficient buffer in this intrinsic use the general scheme.
  - Parameter 'zstart' must be a compile time constant.

## ◆ lmac2_abs() [2/2]

v2cacc80 lmac2_abs | ( | v2cacc80 | acc,
|  | v32int32 | xbuff,
|  | int | xstart,
|  | unsigned int | xoffsets,
|  | int | xstep,
|  | v4cint32 | zbuff,
|  | int | zstart,
|  | unsigned int | zoffsets,
|  | int | zstep,
|  | bool | zconj
| ) |  |

Complex multiply-accumulate intrinsic function with dynamic z buffer conjugation after computing the absolute value in the selected lanes from the input buffer .

acc0 += z00*abs(x00) + z01*abs(x01)
acc1 += z10*abs(x10) + z11*abs(x11)

Returns
  Returned accumulation vector (2 x cint80 lanes)

Parameters

  acc | Incoming accumulation vector (2 x cint80 lanes)
  xbuff | Input buffer of 32 elements of type int32
  xstart | Starting position offset applied to all lanes of input from X buffer.
  xoffsets | 4b offset for each lane, applied to the x buffer. LSB apply to first lane
  xstep | Step between each column for selection in the xbuffer.
  zbuff | Input buffer of 4 elements of type cint32
  zstart | Starting position offset applied to all lanes for input from Z buffer. This must be a compile time constant. Only the 4 LSB of the argument are used.
  zoffsets | 4b offset for each lane, applied to input from Z buffer. LSB apply to first lane
  zstep | Step between each column for selection in the zbuffer.
  zconj | Selector for conjugation in Z buffer

Note
  - For more information on how data selection works from the buffers go here. The data buffer and coefficient buffer in this intrinsic use the general scheme.
  - Parameter 'zstart' must be a compile time constant.

## ◆ lmac2_max() [1/3]

v2cacc80 lmac2_max | ( | v2cacc80 | acc,
|  | v16int32 | xbuff,
|  | int | xstart,
|  | unsigned int | xoffsets,
|  | int | xstep,
|  | int | ystart,
|  | v4cint32 | zbuff,
|  | int | zstart,
|  | unsigned int | zoffsets,
|  | int | zstep,
|  | bool | zconj
| ) |  |

Complex multiply-accumulate intrinsic function with dynamic z buffer conjugation after computing the maximum between the selected lanes from the input buffer using small X input buffer.

acc0 += z00*(max(x00 , y00)) + z01*(max(x01 , y01))
acc1 += z10*(max(x10 , y10)) + z11*(max(x11 , y11))

Returns
  Returned accumulation vector (2 x cint80 lanes)

Parameters

  acc | Incoming accumulation vector (2 x cint80 lanes)
  xbuff | Input buffer of 16 elements of type int32
  xstart | Starting position offset applied to all lanes of input from X buffer.
  xoffsets | 4b offset for each lane, applied to both x and y buffers. LSB apply to first lane
  xstep | Step between each column for selection in the x and y buffers. Ystep is symmetric to xstep (ystep advances by -xstep).
  ystart | Starting position offset applied to all lanes for input from Y buffer.
  zbuff | Input buffer of 4 elements of type cint32
  zstart | Starting position offset applied to all lanes for input from Z buffer. This must be a compile time constant. Only the 4 LSB of the argument are used.
  zoffsets | 4b offset for each lane, applied to input from Z buffer. LSB apply to first lane
  zstep | Step between each column for selection in the zbuffer.
  zconj | Selector for conjugation in Z buffer

Note
  - For more information on how data selection works from the buffers go here. The data buffer and coefficient buffer in this intrinsic use the general scheme.
  - Parameter 'zstart' must be a compile time constant.

## ◆ lmac2_max() [2/3]

v2cacc80 lmac2_max | ( | v2cacc80 | acc,
|  | v16int32 | xbuff,
|  | int | xstart,
|  | unsigned int | xoffsets,
|  | int | xstep,
|  | v16int32 | ybuff,
|  | int | ystart,
|  | v4cint32 | zbuff,
|  | int | zstart,
|  | unsigned int | zoffsets,
|  | int | zstep,
|  | bool | zconj
| ) |  |

Complex multiply-accumulate intrinsic function with dynamic z buffer conjugation after computing the maximum between the selected lanes from the input buffer using small X input buffer.

acc0 += z00*(max(x00 , y00)) + z01*(max(x01 , y01))
acc1 += z10*(max(x10 , y10)) + z11*(max(x11 , y11))

Returns
  Returned accumulation vector (2 x cint80 lanes)

Parameters

  acc | Incoming accumulation vector (2 x cint80 lanes)
  xbuff | Input buffer of 16 elements of type int32
  xstart | Starting position offset applied to all lanes of input from X buffer.
  xoffsets | 4b offset for each lane, applied to both x and y buffers. LSB apply to first lane
  xstep | Step between each column for selection in the x and y buffers. Ystep is symmetric to xstep (ystep advances by -xstep).
  ybuff | Right input buffer of 16 elements of type int32
  ystart | Starting position offset applied to all lanes for input from Y buffer.
  zbuff | Input buffer of 4 elements of type cint32
  zstart | Starting position offset applied to all lanes for input from Z buffer. This must be a compile time constant. Only the 4 LSB of the argument are used.
  zoffsets | 4b offset for each lane, applied to input from Z buffer. LSB apply to first lane
  zstep | Step between each column for selection in the zbuffer.
  zconj | Selector for conjugation in Z buffer

Note
  - For more information on how data selection works from the buffers go here. The data buffer and coefficient buffer in this intrinsic use the general scheme.
  - Parameter 'zstart' must be a compile time constant.

## ◆ lmac2_max() [3/3]

v2cacc80 lmac2_max | ( | v2cacc80 | acc,
|  | v32int32 | xbuff,
|  | int | xstart,
|  | unsigned int | xoffsets,
|  | int | xstep,
|  | int | ystart,
|  | v4cint32 | zbuff,
|  | int | zstart,
|  | unsigned int | zoffsets,
|  | int | zstep,
|  | bool | zconj
| ) |  |

Complex multiply-accumulate intrinsic function with dynamic z buffer conjugation after computing the maximum between the selected lanes from the input buffer .

acc0 += z00*(max(x00 , y00)) + z01*(max(x01 , y01))
acc1 += z10*(max(x10 , y10)) + z11*(max(x11 , y11))

Returns
  Returned accumulation vector (2 x cint80 lanes)

Parameters

  acc | Incoming accumulation vector (2 x cint80 lanes)
  xbuff | Input buffer of 32 elements of type int32
  xstart | Starting position offset applied to all lanes of input from X buffer.
  xoffsets | 4b offset for each lane, applied to both x and y buffers. LSB apply to first lane
  xstep | Step between each column for selection in the x and y buffers. Ystep is symmetric to xstep (ystep advances by -xstep).
  ystart | Starting position offset applied to all lanes for input from Y buffer.
  zbuff | Input buffer of 4 elements of type cint32
  zstart | Starting position offset applied to all lanes for input from Z buffer. This must be a compile time constant. Only the 4 LSB of the argument are used.
  zoffsets | 4b offset for each lane, applied to input from Z buffer. LSB apply to first lane
  zstep | Step between each column for selection in the zbuffer.
  zconj | Selector for conjugation in Z buffer

Note
  - For more information on how data selection works from the buffers go here. The data buffer and coefficient buffer in this intrinsic use the general scheme.
  - Parameter 'zstart' must be a compile time constant.

## ◆ lmac2_maxdiff() [1/3]

v2cacc80 lmac2_maxdiff | ( | v2cacc80 | acc,
|  | v16int32 | xbuff,
|  | int | xstart,
|  | unsigned int | xoffsets,
|  | int | xstep,
|  | int | ystart,
|  | v4cint32 | zbuff,
|  | int | zstart,
|  | unsigned int | zoffsets,
|  | int | zstep,
|  | bool | zconj
| ) |  |

Complex multiply-accumulate intrinsic function with dynamic z buffer conjugation after computing the maximum difference between the selected lanes from the input buffer using small X input buffer.

acc0 += z00*((x00 - y00 > 0) ? (x00 - y00):0) + z01*((x01 - y01 > 0) ? (x01 - y01):0)
acc1 += z10*((x10 - y10 > 0) ? (x10 - y10):0) + z11*((x11 - y11 > 0) ? (x11 - y11):0)

Returns
  Returned accumulation vector (2 x cint80 lanes)

Parameters

  acc | Incoming accumulation vector (2 x cint80 lanes)
  xbuff | Input buffer of 16 elements of type int32
  xstart | Starting position offset applied to all lanes of input from X buffer.
  xoffsets | 4b offset for each lane, applied to both x and y buffers. LSB apply to first lane
  xstep | Step between each column for selection in the x and y buffers. Ystep is symmetric to xstep (ystep advances by -xstep).
  ystart | Starting position offset applied to all lanes for input from Y buffer.
  zbuff | Input buffer of 4 elements of type cint32
  zstart | Starting position offset applied to all lanes for input from Z buffer. This must be a compile time constant. Only the 4 LSB of the argument are used.
  zoffsets | 4b offset for each lane, applied to input from Z buffer. LSB apply to first lane
  zstep | Step between each column for selection in the zbuffer.
  zconj | Selector for conjugation in Z buffer

Note
  - For more information on how data selection works from the buffers go here. The data buffer and coefficient buffer in this intrinsic use the general scheme.
  - Parameter 'zstart' must be a compile time constant.

## ◆ lmac2_maxdiff() [2/3]

v2cacc80 lmac2_maxdiff | ( | v2cacc80 | acc,
|  | v16int32 | xbuff,
|  | int | xstart,
|  | unsigned int | xoffsets,
|  | int | xstep,
|  | v16int32 | ybuff,
|  | int | ystart,
|  | v4cint32 | zbuff,
|  | int | zstart,
|  | unsigned int | zoffsets,
|  | int | zstep,
|  | bool | zconj
| ) |  |

Complex multiply-accumulate intrinsic function with dynamic z buffer conjugation after computing the maximum difference between the selected lanes from the input buffer using small X input buffer.

acc0 += z00*((x00 - y00 > 0) ? (x00 - y00):0) + z01*((x01 - y01 > 0) ? (x01 - y01):0)
acc1 += z10*((x10 - y10 > 0) ? (x10 - y10):0) + z11*((x11 - y11 > 0) ? (x11 - y11):0)

Returns
  Returned accumulation vector (2 x cint80 lanes)

Parameters

  acc | Incoming accumulation vector (2 x cint80 lanes)
  xbuff | Input buffer of 16 elements of type int32
  xstart | Starting position offset applied to all lanes of input from X buffer.
  xoffsets | 4b offset for each lane, applied to both x and y buffers. LSB apply to first lane
  xstep | Step between each column for selection in the x and y buffers. Ystep is symmetric to xstep (ystep advances by -xstep).
  ybuff | Right input buffer of 16 elements of type int32
  ystart | Starting position offset applied to all lanes for input from Y buffer.
  zbuff | Input buffer of 4 elements of type cint32
  zstart | Starting position offset applied to all lanes for input from Z buffer. This must be a compile time constant. Only the 4 LSB of the argument are used.
  zoffsets | 4b offset for each lane, applied to input from Z buffer. LSB apply to first lane
  zstep | Step between each column for selection in the zbuffer.
  zconj | Selector for conjugation in Z buffer

Note
  - For more information on how data selection works from the buffers go here. The data buffer and coefficient buffer in this intrinsic use the general scheme.
  - Parameter 'zstart' must be a compile time constant.

## ◆ lmac2_maxdiff() [3/3]

v2cacc80 lmac2_maxdiff | ( | v2cacc80 | acc,
|  | v32int32 | xbuff,
|  | int | xstart,
|  | unsigned int | xoffsets,
|  | int | xstep,
|  | int | ystart,
|  | v4cint32 | zbuff,
|  | int | zstart,
|  | unsigned int | zoffsets,
|  | int | zstep,
|  | bool | zconj
| ) |  |

Complex multiply-accumulate intrinsic function with dynamic z buffer conjugation after computing the maximum difference between the selected lanes from the input buffer .

acc0 += z00*((x00 - y00 > 0) ? (x00 - y00):0) + z01*((x01 - y01 > 0) ? (x01 - y01):0)
acc1 += z10*((x10 - y10 > 0) ? (x10 - y10):0) + z11*((x11 - y11 > 0) ? (x11 - y11):0)

Returns
  Returned accumulation vector (2 x cint80 lanes)

Parameters

  acc | Incoming accumulation vector (2 x cint80 lanes)
  xbuff | Input buffer of 32 elements of type int32
  xstart | Starting position offset applied to all lanes of input from X buffer.
  xoffsets | 4b offset for each lane, applied to both x and y buffers. LSB apply to first lane
  xstep | Step between each column for selection in the x and y buffers. Ystep is symmetric to xstep (ystep advances by -xstep).
  ystart | Starting position offset applied to all lanes for input from Y buffer.
  zbuff | Input buffer of 4 elements of type cint32
  zstart | Starting position offset applied to all lanes for input from Z buffer. This must be a compile time constant. Only the 4 LSB of the argument are used.
  zoffsets | 4b offset for each lane, applied to input from Z buffer. LSB apply to first lane
  zstep | Step between each column for selection in the zbuffer.
  zconj | Selector for conjugation in Z buffer

Note
  - For more information on how data selection works from the buffers go here. The data buffer and coefficient buffer in this intrinsic use the general scheme.
  - Parameter 'zstart' must be a compile time constant.

## ◆ lmac2_min() [1/3]

v2cacc80 lmac2_min | ( | v2cacc80 | acc,
|  | v16int32 | xbuff,
|  | int | xstart,
|  | unsigned int | xoffsets,
|  | int | xstep,
|  | int | ystart,
|  | v4cint32 | zbuff,
|  | int | zstart,
|  | unsigned int | zoffsets,
|  | int | zstep,
|  | bool | zconj
| ) |  |

Complex multiply-accumulate intrinsic function with dynamic z buffer conjugation after computing the minimum between the selected lanes from the input buffer using small X input buffer.

acc0 += z00*(min(x00 , y00)) + z01*(min(x01 , y01))
acc1 += z10*(min(x10 , y10)) + z11*(min(x11 , y11))

Returns
  Returned accumulation vector (2 x cint80 lanes)

Parameters

  acc | Incoming accumulation vector (2 x cint80 lanes)
  xbuff | Input buffer of 16 elements of type int32
  xstart | Starting position offset applied to all lanes of input from X buffer.
  xoffsets | 4b offset for each lane, applied to both x and y buffers. LSB apply to first lane
  xstep | Step between each column for selection in the x and y buffers. Ystep is symmetric to xstep (ystep advances by -xstep).
  ystart | Starting position offset applied to all lanes for input from Y buffer.
  zbuff | Input buffer of 4 elements of type cint32
  zstart | Starting position offset applied to all lanes for input from Z buffer. This must be a compile time constant. Only the 4 LSB of the argument are used.
  zoffsets | 4b offset for each lane, applied to input from Z buffer. LSB apply to first lane
  zstep | Step between each column for selection in the zbuffer.
  zconj | Selector for conjugation in Z buffer

Note
  - For more information on how data selection works from the buffers go here. The data buffer and coefficient buffer in this intrinsic use the general scheme.
  - Parameter 'zstart' must be a compile time constant.

## ◆ lmac2_min() [2/3]

v2cacc80 lmac2_min | ( | v2cacc80 | acc,
|  | v16int32 | xbuff,
|  | int | xstart,
|  | unsigned int | xoffsets,
|  | int | xstep,
|  | v16int32 | ybuff,
|  | int | ystart,
|  | v4cint32 | zbuff,
|  | int | zstart,
|  | unsigned int | zoffsets,
|  | int | zstep,
|  | bool | zconj
| ) |  |

Complex multiply-accumulate intrinsic function with dynamic z buffer conjugation after computing the minimum between the selected lanes from the input buffer using small X input buffer.

acc0 += z00*(min(x00 , y00)) + z01*(min(x01 , y01))
acc1 += z10*(min(x10 , y10)) + z11*(min(x11 , y11))

Returns
  Returned accumulation vector (2 x cint80 lanes)

Parameters

  acc | Incoming accumulation vector (2 x cint80 lanes)
  xbuff | Input buffer of 16 elements of type int32
  xstart | Starting position offset applied to all lanes of input from X buffer.
  xoffsets | 4b offset for each lane, applied to both x and y buffers. LSB apply to first lane
  xstep | Step between each column for selection in the x and y buffers. Ystep is symmetric to xstep (ystep advances by -xstep).
  ybuff | Right input buffer of 16 elements of type int32
  ystart | Starting position offset applied to all lanes for input from Y buffer.
  zbuff | Input buffer of 4 elements of type cint32
  zstart | Starting position offset applied to all lanes for input from Z buffer. This must be a compile time constant. Only the 4 LSB of the argument are used.
  zoffsets | 4b offset for each lane, applied to input from Z buffer. LSB apply to first lane
  zstep | Step between each column for selection in the zbuffer.
  zconj | Selector for conjugation in Z buffer

Note
  - For more information on how data selection works from the buffers go here. The data buffer and coefficient buffer in this intrinsic use the general scheme.
  - Parameter 'zstart' must be a compile time constant.

## ◆ lmac2_min() [3/3]

v2cacc80 lmac2_min | ( | v2cacc80 | acc,
|  | v32int32 | xbuff,
|  | int | xstart,
|  | unsigned int | xoffsets,
|  | int | xstep,
|  | int | ystart,
|  | v4cint32 | zbuff,
|  | int | zstart,
|  | unsigned int | zoffsets,
|  | int | zstep,
|  | bool | zconj
| ) |  |

Complex multiply-accumulate intrinsic function with dynamic z buffer conjugation after computing the minimum between the selected lanes from the input buffer .

acc0 += z00*(min(x00 , y00)) + z01*(min(x01 , y01))
acc1 += z10*(min(x10 , y10)) + z11*(min(x11 , y11))

Returns
  Returned accumulation vector (2 x cint80 lanes)

Parameters

  acc | Incoming accumulation vector (2 x cint80 lanes)
  xbuff | Input buffer of 32 elements of type int32
  xstart | Starting position offset applied to all lanes of input from X buffer.
  xoffsets | 4b offset for each lane, applied to both x and y buffers. LSB apply to first lane
  xstep | Step between each column for selection in the x and y buffers. Ystep is symmetric to xstep (ystep advances by -xstep).
  ystart | Starting position offset applied to all lanes for input from Y buffer.
  zbuff | Input buffer of 4 elements of type cint32
  zstart | Starting position offset applied to all lanes for input from Z buffer. This must be a compile time constant. Only the 4 LSB of the argument are used.
  zoffsets | 4b offset for each lane, applied to input from Z buffer. LSB apply to first lane
  zstep | Step between each column for selection in the zbuffer.
  zconj | Selector for conjugation in Z buffer

Note
  - For more information on how data selection works from the buffers go here. The data buffer and coefficient buffer in this intrinsic use the general scheme.
  - Parameter 'zstart' must be a compile time constant.

## ◆ lmac4_abs() [1/2]

v4cacc80 lmac4_abs | ( | v4cacc80 | acc,
|  | v16int32 | xbuff,
|  | int | xstart,
|  | unsigned int | xoffsets,
|  | v4cint32 | zbuff,
|  | int | zstart,
|  | unsigned int | zoffsets,
|  | bool | zconj
| ) |  |

Complex multiply-accumulate intrinsic function with dynamic z buffer conjugation after computing the absolute value in the selected lanes from the input buffer using small X input buffer.

acc0 += z00*abs(x00)
acc1 += z10*abs(x10)
acc2 += z20*abs(x20)
acc3 += z30*abs(x30)

Returns
  Returned accumulation vector (4 x cint80 lanes)

Parameters

  acc | Incoming accumulation vector (4 x cint80 lanes)
  xbuff | Input buffer of 16 elements of type int32
  xstart | Starting position offset applied to all lanes of input from X buffer.
  xoffsets | 4b offset for each lane, applied to the x buffer. LSB apply to first lane
  zbuff | Input buffer of 4 elements of type cint32
  zstart | Starting position offset applied to all lanes for input from Z buffer. This must be a compile time constant. Only the 4 LSB of the argument are used.
  zoffsets | 4b offset for each lane, applied to input from Z buffer. LSB apply to first lane
  zconj | Selector for conjugation in Z buffer

Note
  - For more information on how data selection works from the buffers go here. The data buffer and coefficient buffer in this intrinsic use the general scheme.
  - Parameter 'zstart' must be a compile time constant.

## ◆ lmac4_abs() [2/2]

v4cacc80 lmac4_abs | ( | v4cacc80 | acc,
|  | v32int32 | xbuff,
|  | int | xstart,
|  | unsigned int | xoffsets,
|  | v4cint32 | zbuff,
|  | int | zstart,
|  | unsigned int | zoffsets,
|  | bool | zconj
| ) |  |

Complex multiply-accumulate intrinsic function with dynamic z buffer conjugation after computing the absolute value in the selected lanes from the input buffer .

acc0 += z00*abs(x00)
acc1 += z10*abs(x10)
acc2 += z20*abs(x20)
acc3 += z30*abs(x30)

Returns
  Returned accumulation vector (4 x cint80 lanes)

Parameters

  acc | Incoming accumulation vector (4 x cint80 lanes)
  xbuff | Input buffer of 32 elements of type int32
  xstart | Starting position offset applied to all lanes of input from X buffer.
  xoffsets | 4b offset for each lane, applied to the x buffer. LSB apply to first lane
  zbuff | Input buffer of 4 elements of type cint32
  zstart | Starting position offset applied to all lanes for input from Z buffer. This must be a compile time constant. Only the 4 LSB of the argument are used.
  zoffsets | 4b offset for each lane, applied to input from Z buffer. LSB apply to first lane
  zconj | Selector for conjugation in Z buffer

Note
  - For more information on how data selection works from the buffers go here. The data buffer and coefficient buffer in this intrinsic use the general scheme.
  - Parameter 'zstart' must be a compile time constant.

## ◆ lmac4_max() [1/3]

v4cacc80 lmac4_max | ( | v4cacc80 | acc,
|  | v16int32 | xbuff,
|  | int | xstart,
|  | unsigned int | xoffsets,
|  | int | ystart,
|  | v4cint32 | zbuff,
|  | int | zstart,
|  | unsigned int | zoffsets,
|  | bool | zconj
| ) |  |

Complex multiply-accumulate intrinsic function with dynamic z buffer conjugation after computing the maximum between the selected lanes from the input buffer using small X input buffer.

acc0 += z00*(max(x00 , y00))
acc1 += z10*(max(x10 , y10))
acc2 += z20*(max(x20 , y20))
acc3 += z30*(max(x30 , y30))

Returns
  Returned accumulation vector (4 x cint80 lanes)

Parameters

  acc | Incoming accumulation vector (4 x cint80 lanes)
  xbuff | Input buffer of 16 elements of type int32
  xstart | Starting position offset applied to all lanes of input from X buffer.
  xoffsets | 4b offset for each lane, applied to both x and y buffers. LSB apply to first lane
  ystart | Starting position offset applied to all lanes for input from Y buffer.
  zbuff | Input buffer of 4 elements of type cint32
  zstart | Starting position offset applied to all lanes for input from Z buffer. This must be a compile time constant. Only the 4 LSB of the argument are used.
  zoffsets | 4b offset for each lane, applied to input from Z buffer. LSB apply to first lane
  zconj | Selector for conjugation in Z buffer

Note
  - For more information on how data selection works from the buffers go here. The data buffer and coefficient buffer in this intrinsic use the general scheme.
  - Parameter 'zstart' must be a compile time constant.

## ◆ lmac4_max() [2/3]

v4cacc80 lmac4_max | ( | v4cacc80 | acc,
|  | v16int32 | xbuff,
|  | int | xstart,
|  | unsigned int | xoffsets,
|  | v16int32 | ybuff,
|  | int | ystart,
|  | v4cint32 | zbuff,
|  | int | zstart,
|  | unsigned int | zoffsets,
|  | bool | zconj
| ) |  |

Complex multiply-accumulate intrinsic function with dynamic z buffer conjugation after computing the maximum between the selected lanes from the input buffer using small X input buffer.

acc0 += z00*(max(x00 , y00))
acc1 += z10*(max(x10 , y10))
acc2 += z20*(max(x20 , y20))
acc3 += z30*(max(x30 , y30))

Returns
  Returned accumulation vector (4 x cint80 lanes)

Parameters

  acc | Incoming accumulation vector (4 x cint80 lanes)
  xbuff | Input buffer of 16 elements of type int32
  xstart | Starting position offset applied to all lanes of input from X buffer.
  xoffsets | 4b offset for each lane, applied to both x and y buffers. LSB apply to first lane
  ybuff | Right input buffer of 16 elements of type int32
  ystart | Starting position offset applied to all lanes for input from Y buffer.
  zbuff | Input buffer of 4 elements of type cint32
  zstart | Starting position offset applied to all lanes for input from Z buffer. This must be a compile time constant. Only the 4 LSB of the argument are used.
  zoffsets | 4b offset for each lane, applied to input from Z buffer. LSB apply to first lane
  zconj | Selector for conjugation in Z buffer

Note
  - For more information on how data selection works from the buffers go here. The data buffer and coefficient buffer in this intrinsic use the general scheme.
  - Parameter 'zstart' must be a compile time constant.

## ◆ lmac4_max() [3/3]

v4cacc80 lmac4_max | ( | v4cacc80 | acc,
|  | v32int32 | xbuff,
|  | int | xstart,
|  | unsigned int | xoffsets,
|  | int | ystart,
|  | v4cint32 | zbuff,
|  | int | zstart,
|  | unsigned int | zoffsets,
|  | bool | zconj
| ) |  |

Complex multiply-accumulate intrinsic function with dynamic z buffer conjugation after computing the maximum between the selected lanes from the input buffer .

acc0 += z00*(max(x00 , y00))
acc1 += z10*(max(x10 , y10))
acc2 += z20*(max(x20 , y20))
acc3 += z30*(max(x30 , y30))

Returns
  Returned accumulation vector (4 x cint80 lanes)

Parameters

  acc | Incoming accumulation vector (4 x cint80 lanes)
  xbuff | Input buffer of 32 elements of type int32
  xstart | Starting position offset applied to all lanes of input from X buffer.
  xoffsets | 4b offset for each lane, applied to both x and y buffers. LSB apply to first lane
  ystart | Starting position offset applied to all lanes for input from Y buffer.
  zbuff | Input buffer of 4 elements of type cint32
  zstart | Starting position offset applied to all lanes for input from Z buffer. This must be a compile time constant. Only the 4 LSB of the argument are used.
  zoffsets | 4b offset for each lane, applied to input from Z buffer. LSB apply to first lane
  zconj | Selector for conjugation in Z buffer

Note
  - For more information on how data selection works from the buffers go here. The data buffer and coefficient buffer in this intrinsic use the general scheme.
  - Parameter 'zstart' must be a compile time constant.

## ◆ lmac4_maxdiff() [1/3]

v4cacc80 lmac4_maxdiff | ( | v4cacc80 | acc,
|  | v16int32 | xbuff,
|  | int | xstart,
|  | unsigned int | xoffsets,
|  | int | ystart,
|  | v4cint32 | zbuff,
|  | int | zstart,
|  | unsigned int | zoffsets,
|  | bool | zconj
| ) |  |

Complex multiply-accumulate intrinsic function with dynamic z buffer conjugation after computing the maximum difference between the selected lanes from the input buffer using small X input buffer.

acc0 += z00*((x00 - y00 > 0) ? (x00 - y00):0)
acc1 += z10*((x10 - y10 > 0) ? (x10 - y10):0)
acc2 += z20*((x20 - y20 > 0) ? (x20 - y20):0)
acc3 += z30*((x30 - y30 > 0) ? (x30 - y30):0)

Returns
  Returned accumulation vector (4 x cint80 lanes)

Parameters

  acc | Incoming accumulation vector (4 x cint80 lanes)
  xbuff | Input buffer of 16 elements of type int32
  xstart | Starting position offset applied to all lanes of input from X buffer.
  xoffsets | 4b offset for each lane, applied to both x and y buffers. LSB apply to first lane
  ystart | Starting position offset applied to all lanes for input from Y buffer.
  zbuff | Input buffer of 4 elements of type cint32
  zstart | Starting position offset applied to all lanes for input from Z buffer. This must be a compile time constant. Only the 4 LSB of the argument are used.
  zoffsets | 4b offset for each lane, applied to input from Z buffer. LSB apply to first lane
  zconj | Selector for conjugation in Z buffer

Note
  - For more information on how data selection works from the buffers go here. The data buffer and coefficient buffer in this intrinsic use the general scheme.
  - Parameter 'zstart' must be a compile time constant.

## ◆ lmac4_maxdiff() [2/3]

v4cacc80 lmac4_maxdiff | ( | v4cacc80 | acc,
|  | v16int32 | xbuff,
|  | int | xstart,
|  | unsigned int | xoffsets,
|  | v16int32 | ybuff,
|  | int | ystart,
|  | v4cint32 | zbuff,
|  | int | zstart,
|  | unsigned int | zoffsets,
|  | bool | zconj
| ) |  |

Complex multiply-accumulate intrinsic function with dynamic z buffer conjugation after computing the maximum difference between the selected lanes from the input buffer using small X input buffer.

acc0 += z00*((x00 - y00 > 0) ? (x00 - y00):0)
acc1 += z10*((x10 - y10 > 0) ? (x10 - y10):0)
acc2 += z20*((x20 - y20 > 0) ? (x20 - y20):0)
acc3 += z30*((x30 - y30 > 0) ? (x30 - y30):0)

Returns
  Returned accumulation vector (4 x cint80 lanes)

Parameters

  acc | Incoming accumulation vector (4 x cint80 lanes)
  xbuff | Input buffer of 16 elements of type int32
  xstart | Starting position offset applied to all lanes of input from X buffer.
  xoffsets | 4b offset for each lane, applied to both x and y buffers. LSB apply to first lane
  ybuff | Right input buffer of 16 elements of type int32
  ystart | Starting position offset applied to all lanes for input from Y buffer.
  zbuff | Input buffer of 4 elements of type cint32
  zstart | Starting position offset applied to all lanes for input from Z buffer. This must be a compile time constant. Only the 4 LSB of the argument are used.
  zoffsets | 4b offset for each lane, applied to input from Z buffer. LSB apply to first lane
  zconj | Selector for conjugation in Z buffer

Note
  - For more information on how data selection works from the buffers go here. The data buffer and coefficient buffer in this intrinsic use the general scheme.
  - Parameter 'zstart' must be a compile time constant.

## ◆ lmac4_maxdiff() [3/3]

v4cacc80 lmac4_maxdiff | ( | v4cacc80 | acc,
|  | v32int32 | xbuff,
|  | int | xstart,
|  | unsigned int | xoffsets,
|  | int | ystart,
|  | v4cint32 | zbuff,
|  | int | zstart,
|  | unsigned int | zoffsets,
|  | bool | zconj
| ) |  |

Complex multiply-accumulate intrinsic function with dynamic z buffer conjugation after computing the maximum difference between the selected lanes from the input buffer .

acc0 += z00*((x00 - y00 > 0) ? (x00 - y00):0)
acc1 += z10*((x10 - y10 > 0) ? (x10 - y10):0)
acc2 += z20*((x20 - y20 > 0) ? (x20 - y20):0)
acc3 += z30*((x30 - y30 > 0) ? (x30 - y30):0)

Returns
  Returned accumulation vector (4 x cint80 lanes)

Parameters

  acc | Incoming accumulation vector (4 x cint80 lanes)
  xbuff | Input buffer of 32 elements of type int32
  xstart | Starting position offset applied to all lanes of input from X buffer.
  xoffsets | 4b offset for each lane, applied to both x and y buffers. LSB apply to first lane
  ystart | Starting position offset applied to all lanes for input from Y buffer.
  zbuff | Input buffer of 4 elements of type cint32
  zstart | Starting position offset applied to all lanes for input from Z buffer. This must be a compile time constant. Only the 4 LSB of the argument are used.
  zoffsets | 4b offset for each lane, applied to input from Z buffer. LSB apply to first lane
  zconj | Selector for conjugation in Z buffer

Note
  - For more information on how data selection works from the buffers go here. The data buffer and coefficient buffer in this intrinsic use the general scheme.
  - Parameter 'zstart' must be a compile time constant.

## ◆ lmac4_min() [1/3]

v4cacc80 lmac4_min | ( | v4cacc80 | acc,
|  | v16int32 | xbuff,
|  | int | xstart,
|  | unsigned int | xoffsets,
|  | int | ystart,
|  | v4cint32 | zbuff,
|  | int | zstart,
|  | unsigned int | zoffsets,
|  | bool | zconj
| ) |  |

Complex multiply-accumulate intrinsic function with dynamic z buffer conjugation after computing the minimum between the selected lanes from the input buffer using small X input buffer.

acc0 += z00*(min(x00 , y00))
acc1 += z10*(min(x10 , y10))
acc2 += z20*(min(x20 , y20))
acc3 += z30*(min(x30 , y30))

Returns
  Returned accumulation vector (4 x cint80 lanes)

Parameters

  acc | Incoming accumulation vector (4 x cint80 lanes)
  xbuff | Input buffer of 16 elements of type int32
  xstart | Starting position offset applied to all lanes of input from X buffer.
  xoffsets | 4b offset for each lane, applied to both x and y buffers. LSB apply to first lane
  ystart | Starting position offset applied to all lanes for input from Y buffer.
  zbuff | Input buffer of 4 elements of type cint32
  zstart | Starting position offset applied to all lanes for input from Z buffer. This must be a compile time constant. Only the 4 LSB of the argument are used.
  zoffsets | 4b offset for each lane, applied to input from Z buffer. LSB apply to first lane
  zconj | Selector for conjugation in Z buffer

Note
  - For more information on how data selection works from the buffers go here. The data buffer and coefficient buffer in this intrinsic use the general scheme.
  - Parameter 'zstart' must be a compile time constant.

## ◆ lmac4_min() [2/3]

v4cacc80 lmac4_min | ( | v4cacc80 | acc,
|  | v16int32 | xbuff,
|  | int | xstart,
|  | unsigned int | xoffsets,
|  | v16int32 | ybuff,
|  | int | ystart,
|  | v4cint32 | zbuff,
|  | int | zstart,
|  | unsigned int | zoffsets,
|  | bool | zconj
| ) |  |

Complex multiply-accumulate intrinsic function with dynamic z buffer conjugation after computing the minimum between the selected lanes from the input buffer using small X input buffer.

acc0 += z00*(min(x00 , y00))
acc1 += z10*(min(x10 , y10))
acc2 += z20*(min(x20 , y20))
acc3 += z30*(min(x30 , y30))

Returns
  Returned accumulation vector (4 x cint80 lanes)

Parameters

  acc | Incoming accumulation vector (4 x cint80 lanes)
  xbuff | Input buffer of 16 elements of type int32
  xstart | Starting position offset applied to all lanes of input from X buffer.
  xoffsets | 4b offset for each lane, applied to both x and y buffers. LSB apply to first lane
  ybuff | Right input buffer of 16 elements of type int32
  ystart | Starting position offset applied to all lanes for input from Y buffer.
  zbuff | Input buffer of 4 elements of type cint32
  zstart | Starting position offset applied to all lanes for input from Z buffer. This must be a compile time constant. Only the 4 LSB of the argument are used.
  zoffsets | 4b offset for each lane, applied to input from Z buffer. LSB apply to first lane
  zconj | Selector for conjugation in Z buffer

Note
  - For more information on how data selection works from the buffers go here. The data buffer and coefficient buffer in this intrinsic use the general scheme.
  - Parameter 'zstart' must be a compile time constant.

## ◆ lmac4_min() [3/3]

v4cacc80 lmac4_min | ( | v4cacc80 | acc,
|  | v32int32 | xbuff,
|  | int | xstart,
|  | unsigned int | xoffsets,
|  | int | ystart,
|  | v4cint32 | zbuff,
|  | int | zstart,
|  | unsigned int | zoffsets,
|  | bool | zconj
| ) |  |

Complex multiply-accumulate intrinsic function with dynamic z buffer conjugation after computing the minimum between the selected lanes from the input buffer .

acc0 += z00*(min(x00 , y00))
acc1 += z10*(min(x10 , y10))
acc2 += z20*(min(x20 , y20))
acc3 += z30*(min(x30 , y30))

Returns
  Returned accumulation vector (4 x cint80 lanes)

Parameters

  acc | Incoming accumulation vector (4 x cint80 lanes)
  xbuff | Input buffer of 32 elements of type int32
  xstart | Starting position offset applied to all lanes of input from X buffer.
  xoffsets | 4b offset for each lane, applied to both x and y buffers. LSB apply to first lane
  ystart | Starting position offset applied to all lanes for input from Y buffer.
  zbuff | Input buffer of 4 elements of type cint32
  zstart | Starting position offset applied to all lanes for input from Z buffer. This must be a compile time constant. Only the 4 LSB of the argument are used.
  zoffsets | 4b offset for each lane, applied to input from Z buffer. LSB apply to first lane
  zconj | Selector for conjugation in Z buffer

Note
  - For more information on how data selection works from the buffers go here. The data buffer and coefficient buffer in this intrinsic use the general scheme.
  - Parameter 'zstart' must be a compile time constant.

## ◆ lmsc2_abs() [1/2]

v2cacc80 lmsc2_abs | ( | v2cacc80 | acc,
|  | v16int32 | xbuff,
|  | int | xstart,
|  | unsigned int | xoffsets,
|  | int | xstep,
|  | v4cint32 | zbuff,
|  | int | zstart,
|  | unsigned int | zoffsets,
|  | int | zstep,
|  | bool | zconj
| ) |  |

Complex multiply-subtract intrinsic function with dynamic z buffer conjugation after computing the absolute value in the selected lanes from the input buffer using small X input buffer.

acc0 -= z00*abs(x00) + z01*abs(x01)
acc1 -= z10*abs(x10) + z11*abs(x11)

Returns
  Returned accumulation vector (2 x cint80 lanes)

Parameters

  acc | Incoming accumulation vector (2 x cint80 lanes)
  xbuff | Input buffer of 16 elements of type int32
  xstart | Starting position offset applied to all lanes of input from X buffer.
  xoffsets | 4b offset for each lane, applied to the x buffer. LSB apply to first lane
  xstep | Step between each column for selection in the xbuffer.
  zbuff | Input buffer of 4 elements of type cint32
  zstart | Starting position offset applied to all lanes for input from Z buffer. This must be a compile time constant. Only the 4 LSB of the argument are used.
  zoffsets | 4b offset for each lane, applied to input from Z buffer. LSB apply to first lane
  zstep | Step between each column for selection in the zbuffer.
  zconj | Selector for conjugation in Z buffer

Note
  - For more information on how data selection works from the buffers go here. The data buffer and coefficient buffer in this intrinsic use the general scheme.
  - Parameter 'zstart' must be a compile time constant.

## ◆ lmsc2_abs() [2/2]

v2cacc80 lmsc2_abs | ( | v2cacc80 | acc,
|  | v32int32 | xbuff,
|  | int | xstart,
|  | unsigned int | xoffsets,
|  | int | xstep,
|  | v4cint32 | zbuff,
|  | int | zstart,
|  | unsigned int | zoffsets,
|  | int | zstep,
|  | bool | zconj
| ) |  |

Complex multiply-subtract intrinsic function with dynamic z buffer conjugation after computing the absolute value in the selected lanes from the input buffer .

acc0 -= z00*abs(x00) + z01*abs(x01)
acc1 -= z10*abs(x10) + z11*abs(x11)

Returns
  Returned accumulation vector (2 x cint80 lanes)

Parameters

  acc | Incoming accumulation vector (2 x cint80 lanes)
  xbuff | Input buffer of 32 elements of type int32
  xstart | Starting position offset applied to all lanes of input from X buffer.
  xoffsets | 4b offset for each lane, applied to the x buffer. LSB apply to first lane
  xstep | Step between each column for selection in the xbuffer.
  zbuff | Input buffer of 4 elements of type cint32
  zstart | Starting position offset applied to all lanes for input from Z buffer. This must be a compile time constant. Only the 4 LSB of the argument are used.
  zoffsets | 4b offset for each lane, applied to input from Z buffer. LSB apply to first lane
  zstep | Step between each column for selection in the zbuffer.
  zconj | Selector for conjugation in Z buffer

Note
  - For more information on how data selection works from the buffers go here. The data buffer and coefficient buffer in this intrinsic use the general scheme.
  - Parameter 'zstart' must be a compile time constant.

## ◆ lmsc2_max() [1/3]

v2cacc80 lmsc2_max | ( | v2cacc80 | acc,
|  | v16int32 | xbuff,
|  | int | xstart,
|  | unsigned int | xoffsets,
|  | int | xstep,
|  | int | ystart,
|  | v4cint32 | zbuff,
|  | int | zstart,
|  | unsigned int | zoffsets,
|  | int | zstep,
|  | bool | zconj
| ) |  |

Complex multiply-subtract intrinsic function with dynamic z buffer conjugation after computing the maximum between the selected lanes from the input buffer using small X input buffer.

acc0 -= z00*(max(x00 , y00)) + z01*(max(x01 , y01))
acc1 -= z10*(max(x10 , y10)) + z11*(max(x11 , y11))

Returns
  Returned accumulation vector (2 x cint80 lanes)

Parameters

  acc | Incoming accumulation vector (2 x cint80 lanes)
  xbuff | Input buffer of 16 elements of type int32
  xstart | Starting position offset applied to all lanes of input from X buffer.
  xoffsets | 4b offset for each lane, applied to both x and y buffers. LSB apply to first lane
  xstep | Step between each column for selection in the x and y buffers. Ystep is symmetric to xstep (ystep advances by -xstep).
  ystart | Starting position offset applied to all lanes for input from Y buffer.
  zbuff | Input buffer of 4 elements of type cint32
  zstart | Starting position offset applied to all lanes for input from Z buffer. This must be a compile time constant. Only the 4 LSB of the argument are used.
  zoffsets | 4b offset for each lane, applied to input from Z buffer. LSB apply to first lane
  zstep | Step between each column for selection in the zbuffer.
  zconj | Selector for conjugation in Z buffer

Note
  - For more information on how data selection works from the buffers go here. The data buffer and coefficient buffer in this intrinsic use the general scheme.
  - Parameter 'zstart' must be a compile time constant.

## ◆ lmsc2_max() [2/3]

v2cacc80 lmsc2_max | ( | v2cacc80 | acc,
|  | v16int32 | xbuff,
|  | int | xstart,
|  | unsigned int | xoffsets,
|  | int | xstep,
|  | v16int32 | ybuff,
|  | int | ystart,
|  | v4cint32 | zbuff,
|  | int | zstart,
|  | unsigned int | zoffsets,
|  | int | zstep,
|  | bool | zconj
| ) |  |

Complex multiply-subtract intrinsic function with dynamic z buffer conjugation after computing the maximum between the selected lanes from the input buffer using small X input buffer.

acc0 -= z00*(max(x00 , y00)) + z01*(max(x01 , y01))
acc1 -= z10*(max(x10 , y10)) + z11*(max(x11 , y11))

Returns
  Returned accumulation vector (2 x cint80 lanes)

Parameters

  acc | Incoming accumulation vector (2 x cint80 lanes)
  xbuff | Input buffer of 16 elements of type int32
  xstart | Starting position offset applied to all lanes of input from X buffer.
  xoffsets | 4b offset for each lane, applied to both x and y buffers. LSB apply to first lane
  xstep | Step between each column for selection in the x and y buffers. Ystep is symmetric to xstep (ystep advances by -xstep).
  ybuff | Right input buffer of 16 elements of type int32
  ystart | Starting position offset applied to all lanes for input from Y buffer.
  zbuff | Input buffer of 4 elements of type cint32
  zstart | Starting position offset applied to all lanes for input from Z buffer. This must be a compile time constant. Only the 4 LSB of the argument are used.
  zoffsets | 4b offset for each lane, applied to input from Z buffer. LSB apply to first lane
  zstep | Step between each column for selection in the zbuffer.
  zconj | Selector for conjugation in Z buffer

Note
  - For more information on how data selection works from the buffers go here. The data buffer and coefficient buffer in this intrinsic use the general scheme.
  - Parameter 'zstart' must be a compile time constant.

## ◆ lmsc2_max() [3/3]

v2cacc80 lmsc2_max | ( | v2cacc80 | acc,
|  | v32int32 | xbuff,
|  | int | xstart,
|  | unsigned int | xoffsets,
|  | int | xstep,
|  | int | ystart,
|  | v4cint32 | zbuff,
|  | int | zstart,
|  | unsigned int | zoffsets,
|  | int | zstep,
|  | bool | zconj
| ) |  |

Complex multiply-subtract intrinsic function with dynamic z buffer conjugation after computing the maximum between the selected lanes from the input buffer .

acc0 -= z00*(max(x00 , y00)) + z01*(max(x01 , y01))
acc1 -= z10*(max(x10 , y10)) + z11*(max(x11 , y11))

Returns
  Returned accumulation vector (2 x cint80 lanes)

Parameters

  acc | Incoming accumulation vector (2 x cint80 lanes)
  xbuff | Input buffer of 32 elements of type int32
  xstart | Starting position offset applied to all lanes of input from X buffer.
  xoffsets | 4b offset for each lane, applied to both x and y buffers. LSB apply to first lane
  xstep | Step between each column for selection in the x and y buffers. Ystep is symmetric to xstep (ystep advances by -xstep).
  ystart | Starting position offset applied to all lanes for input from Y buffer.
  zbuff | Input buffer of 4 elements of type cint32
  zstart | Starting position offset applied to all lanes for input from Z buffer. This must be a compile time constant. Only the 4 LSB of the argument are used.
  zoffsets | 4b offset for each lane, applied to input from Z buffer. LSB apply to first lane
  zstep | Step between each column for selection in the zbuffer.
  zconj | Selector for conjugation in Z buffer

Note
  - For more information on how data selection works from the buffers go here. The data buffer and coefficient buffer in this intrinsic use the general scheme.
  - Parameter 'zstart' must be a compile time constant.

## ◆ lmsc2_maxdiff() [1/3]

v2cacc80 lmsc2_maxdiff | ( | v2cacc80 | acc,
|  | v16int32 | xbuff,
|  | int | xstart,
|  | unsigned int | xoffsets,
|  | int | xstep,
|  | int | ystart,
|  | v4cint32 | zbuff,
|  | int | zstart,
|  | unsigned int | zoffsets,
|  | int | zstep,
|  | bool | zconj
| ) |  |

Complex multiply-subtract intrinsic function with dynamic z buffer conjugation after computing the maximum difference between the selected lanes from the input buffer using small X input buffer.

acc0 -= z00*((x00 - y00 > 0) ? (x00 - y00):0) + z01*((x01 - y01 > 0) ? (x01 - y01):0)
acc1 -= z10*((x10 - y10 > 0) ? (x10 - y10):0) + z11*((x11 - y11 > 0) ? (x11 - y11):0)

Returns
  Returned accumulation vector (2 x cint80 lanes)

Parameters

  acc | Incoming accumulation vector (2 x cint80 lanes)
  xbuff | Input buffer of 16 elements of type int32
  xstart | Starting position offset applied to all lanes of input from X buffer.
  xoffsets | 4b offset for each lane, applied to both x and y buffers. LSB apply to first lane
  xstep | Step between each column for selection in the x and y buffers. Ystep is symmetric to xstep (ystep advances by -xstep).
  ystart | Starting position offset applied to all lanes for input from Y buffer.
  zbuff | Input buffer of 4 elements of type cint32
  zstart | Starting position offset applied to all lanes for input from Z buffer. This must be a compile time constant. Only the 4 LSB of the argument are used.
  zoffsets | 4b offset for each lane, applied to input from Z buffer. LSB apply to first lane
  zstep | Step between each column for selection in the zbuffer.
  zconj | Selector for conjugation in Z buffer

Note
  - For more information on how data selection works from the buffers go here. The data buffer and coefficient buffer in this intrinsic use the general scheme.
  - Parameter 'zstart' must be a compile time constant.

## ◆ lmsc2_maxdiff() [2/3]

v2cacc80 lmsc2_maxdiff | ( | v2cacc80 | acc,
|  | v16int32 | xbuff,
|  | int | xstart,
|  | unsigned int | xoffsets,
|  | int | xstep,
|  | v16int32 | ybuff,
|  | int | ystart,
|  | v4cint32 | zbuff,
|  | int | zstart,
|  | unsigned int | zoffsets,
|  | int | zstep,
|  | bool | zconj
| ) |  |

Complex multiply-subtract intrinsic function with dynamic z buffer conjugation after computing the maximum difference between the selected lanes from the input buffer using small X input buffer.

acc0 -= z00*((x00 - y00 > 0) ? (x00 - y00):0) + z01*((x01 - y01 > 0) ? (x01 - y01):0)
acc1 -= z10*((x10 - y10 > 0) ? (x10 - y10):0) + z11*((x11 - y11 > 0) ? (x11 - y11):0)

Returns
  Returned accumulation vector (2 x cint80 lanes)

Parameters

  acc | Incoming accumulation vector (2 x cint80 lanes)
  xbuff | Input buffer of 16 elements of type int32
  xstart | Starting position offset applied to all lanes of input from X buffer.
  xoffsets | 4b offset for each lane, applied to both x and y buffers. LSB apply to first lane
  xstep | Step between each column for selection in the x and y buffers. Ystep is symmetric to xstep (ystep advances by -xstep).
  ybuff | Right input buffer of 16 elements of type int32
  ystart | Starting position offset applied to all lanes for input from Y buffer.
  zbuff | Input buffer of 4 elements of type cint32
  zstart | Starting position offset applied to all lanes for input from Z buffer. This must be a compile time constant. Only the 4 LSB of the argument are used.
  zoffsets | 4b offset for each lane, applied to input from Z buffer. LSB apply to first lane
  zstep | Step between each column for selection in the zbuffer.
  zconj | Selector for conjugation in Z buffer

Note
  - For more information on how data selection works from the buffers go here. The data buffer and coefficient buffer in this intrinsic use the general scheme.
  - Parameter 'zstart' must be a compile time constant.

## ◆ lmsc2_maxdiff() [3/3]

v2cacc80 lmsc2_maxdiff | ( | v2cacc80 | acc,
|  | v32int32 | xbuff,
|  | int | xstart,
|  | unsigned int | xoffsets,
|  | int | xstep,
|  | int | ystart,
|  | v4cint32 | zbuff,
|  | int | zstart,
|  | unsigned int | zoffsets,
|  | int | zstep,
|  | bool | zconj
| ) |  |

Complex multiply-subtract intrinsic function with dynamic z buffer conjugation after computing the maximum difference between the selected lanes from the input buffer .

acc0 -= z00*((x00 - y00 > 0) ? (x00 - y00):0) + z01*((x01 - y01 > 0) ? (x01 - y01):0)
acc1 -= z10*((x10 - y10 > 0) ? (x10 - y10):0) + z11*((x11 - y11 > 0) ? (x11 - y11):0)

Returns
  Returned accumulation vector (2 x cint80 lanes)

Parameters

  acc | Incoming accumulation vector (2 x cint80 lanes)
  xbuff | Input buffer of 32 elements of type int32
  xstart | Starting position offset applied to all lanes of input from X buffer.
  xoffsets | 4b offset for each lane, applied to both x and y buffers. LSB apply to first lane
  xstep | Step between each column for selection in the x and y buffers. Ystep is symmetric to xstep (ystep advances by -xstep).
  ystart | Starting position offset applied to all lanes for input from Y buffer.
  zbuff | Input buffer of 4 elements of type cint32
  zstart | Starting position offset applied to all lanes for input from Z buffer. This must be a compile time constant. Only the 4 LSB of the argument are used.
  zoffsets | 4b offset for each lane, applied to input from Z buffer. LSB apply to first lane
  zstep | Step between each column for selection in the zbuffer.
  zconj | Selector for conjugation in Z buffer

Note
  - For more information on how data selection works from the buffers go here. The data buffer and coefficient buffer in this intrinsic use the general scheme.
  - Parameter 'zstart' must be a compile time constant.

## ◆ lmsc2_min() [1/3]

v2cacc80 lmsc2_min | ( | v2cacc80 | acc,
|  | v16int32 | xbuff,
|  | int | xstart,
|  | unsigned int | xoffsets,
|  | int | xstep,
|  | int | ystart,
|  | v4cint32 | zbuff,
|  | int | zstart,
|  | unsigned int | zoffsets,
|  | int | zstep,
|  | bool | zconj
| ) |  |

Complex multiply-subtract intrinsic function with dynamic z buffer conjugation after computing the minimum between the selected lanes from the input buffer using small X input buffer.

acc0 -= z00*(min(x00 , y00)) + z01*(min(x01 , y01))
acc1 -= z10*(min(x10 , y10)) + z11*(min(x11 , y11))

Returns
  Returned accumulation vector (2 x cint80 lanes)

Parameters

  acc | Incoming accumulation vector (2 x cint80 lanes)
  xbuff | Input buffer of 16 elements of type int32
  xstart | Starting position offset applied to all lanes of input from X buffer.
  xoffsets | 4b offset for each lane, applied to both x and y buffers. LSB apply to first lane
  xstep | Step between each column for selection in the x and y buffers. Ystep is symmetric to xstep (ystep advances by -xstep).
  ystart | Starting position offset applied to all lanes for input from Y buffer.
  zbuff | Input buffer of 4 elements of type cint32
  zstart | Starting position offset applied to all lanes for input from Z buffer. This must be a compile time constant. Only the 4 LSB of the argument are used.
  zoffsets | 4b offset for each lane, applied to input from Z buffer. LSB apply to first lane
  zstep | Step between each column for selection in the zbuffer.
  zconj | Selector for conjugation in Z buffer

Note
  - For more information on how data selection works from the buffers go here. The data buffer and coefficient buffer in this intrinsic use the general scheme.
  - Parameter 'zstart' must be a compile time constant.

## ◆ lmsc2_min() [2/3]

v2cacc80 lmsc2_min | ( | v2cacc80 | acc,
|  | v16int32 | xbuff,
|  | int | xstart,
|  | unsigned int | xoffsets,
|  | int | xstep,
|  | v16int32 | ybuff,
|  | int | ystart,
|  | v4cint32 | zbuff,
|  | int | zstart,
|  | unsigned int | zoffsets,
|  | int | zstep,
|  | bool | zconj
| ) |  |

Complex multiply-subtract intrinsic function with dynamic z buffer conjugation after computing the minimum between the selected lanes from the input buffer using small X input buffer.

acc0 -= z00*(min(x00 , y00)) + z01*(min(x01 , y01))
acc1 -= z10*(min(x10 , y10)) + z11*(min(x11 , y11))

Returns
  Returned accumulation vector (2 x cint80 lanes)

Parameters

  acc | Incoming accumulation vector (2 x cint80 lanes)
  xbuff | Input buffer of 16 elements of type int32
  xstart | Starting position offset applied to all lanes of input from X buffer.
  xoffsets | 4b offset for each lane, applied to both x and y buffers. LSB apply to first lane
  xstep | Step between each column for selection in the x and y buffers. Ystep is symmetric to xstep (ystep advances by -xstep).
  ybuff | Right input buffer of 16 elements of type int32
  ystart | Starting position offset applied to all lanes for input from Y buffer.
  zbuff | Input buffer of 4 elements of type cint32
  zstart | Starting position offset applied to all lanes for input from Z buffer. This must be a compile time constant. Only the 4 LSB of the argument are used.
  zoffsets | 4b offset for each lane, applied to input from Z buffer. LSB apply to first lane
  zstep | Step between each column for selection in the zbuffer.
  zconj | Selector for conjugation in Z buffer

Note
  - For more information on how data selection works from the buffers go here. The data buffer and coefficient buffer in this intrinsic use the general scheme.
  - Parameter 'zstart' must be a compile time constant.

## ◆ lmsc2_min() [3/3]

v2cacc80 lmsc2_min | ( | v2cacc80 | acc,
|  | v32int32 | xbuff,
|  | int | xstart,
|  | unsigned int | xoffsets,
|  | int | xstep,
|  | int | ystart,
|  | v4cint32 | zbuff,
|  | int | zstart,
|  | unsigned int | zoffsets,
|  | int | zstep,
|  | bool | zconj
| ) |  |

Complex multiply-subtract intrinsic function with dynamic z buffer conjugation after computing the minimum between the selected lanes from the input buffer .

acc0 -= z00*(min(x00 , y00)) + z01*(min(x01 , y01))
acc1 -= z10*(min(x10 , y10)) + z11*(min(x11 , y11))

Returns
  Returned accumulation vector (2 x cint80 lanes)

Parameters

  acc | Incoming accumulation vector (2 x cint80 lanes)
  xbuff | Input buffer of 32 elements of type int32
  xstart | Starting position offset applied to all lanes of input from X buffer.
  xoffsets | 4b offset for each lane, applied to both x and y buffers. LSB apply to first lane
  xstep | Step between each column for selection in the x and y buffers. Ystep is symmetric to xstep (ystep advances by -xstep).
  ystart | Starting position offset applied to all lanes for input from Y buffer.
  zbuff | Input buffer of 4 elements of type cint32
  zstart | Starting position offset applied to all lanes for input from Z buffer. This must be a compile time constant. Only the 4 LSB of the argument are used.
  zoffsets | 4b offset for each lane, applied to input from Z buffer. LSB apply to first lane
  zstep | Step between each column for selection in the zbuffer.
  zconj | Selector for conjugation in Z buffer

Note
  - For more information on how data selection works from the buffers go here. The data buffer and coefficient buffer in this intrinsic use the general scheme.
  - Parameter 'zstart' must be a compile time constant.

## ◆ lmsc4_abs() [1/2]

v4cacc80 lmsc4_abs | ( | v4cacc80 | acc,
|  | v16int32 | xbuff,
|  | int | xstart,
|  | unsigned int | xoffsets,
|  | v4cint32 | zbuff,
|  | int | zstart,
|  | unsigned int | zoffsets,
|  | bool | zconj
| ) |  |

Complex multiply-subtract intrinsic function with dynamic z buffer conjugation after computing the absolute value in the selected lanes from the input buffer using small X input buffer.

acc0 -= z00*abs(x00)
acc1 -= z10*abs(x10)
acc2 -= z20*abs(x20)
acc3 -= z30*abs(x30)

Returns
  Returned accumulation vector (4 x cint80 lanes)

Parameters

  acc | Incoming accumulation vector (4 x cint80 lanes)
  xbuff | Input buffer of 16 elements of type int32
  xstart | Starting position offset applied to all lanes of input from X buffer.
  xoffsets | 4b offset for each lane, applied to the x buffer. LSB apply to first lane
  zbuff | Input buffer of 4 elements of type cint32
  zstart | Starting position offset applied to all lanes for input from Z buffer. This must be a compile time constant. Only the 4 LSB of the argument are used.
  zoffsets | 4b offset for each lane, applied to input from Z buffer. LSB apply to first lane
  zconj | Selector for conjugation in Z buffer

Note
  - For more information on how data selection works from the buffers go here. The data buffer and coefficient buffer in this intrinsic use the general scheme.
  - Parameter 'zstart' must be a compile time constant.

## ◆ lmsc4_abs() [2/2]

v4cacc80 lmsc4_abs | ( | v4cacc80 | acc,
|  | v32int32 | xbuff,
|  | int | xstart,
|  | unsigned int | xoffsets,
|  | v4cint32 | zbuff,
|  | int | zstart,
|  | unsigned int | zoffsets,
|  | bool | zconj
| ) |  |

Complex multiply-subtract intrinsic function with dynamic z buffer conjugation after computing the absolute value in the selected lanes from the input buffer .

acc0 -= z00*abs(x00)
acc1 -= z10*abs(x10)
acc2 -= z20*abs(x20)
acc3 -= z30*abs(x30)

Returns
  Returned accumulation vector (4 x cint80 lanes)

Parameters

  acc | Incoming accumulation vector (4 x cint80 lanes)
  xbuff | Input buffer of 32 elements of type int32
  xstart | Starting position offset applied to all lanes of input from X buffer.
  xoffsets | 4b offset for each lane, applied to the x buffer. LSB apply to first lane
  zbuff | Input buffer of 4 elements of type cint32
  zstart | Starting position offset applied to all lanes for input from Z buffer. This must be a compile time constant. Only the 4 LSB of the argument are used.
  zoffsets | 4b offset for each lane, applied to input from Z buffer. LSB apply to first lane
  zconj | Selector for conjugation in Z buffer

Note
  - For more information on how data selection works from the buffers go here. The data buffer and coefficient buffer in this intrinsic use the general scheme.
  - Parameter 'zstart' must be a compile time constant.

## ◆ lmsc4_max() [1/3]

v4cacc80 lmsc4_max | ( | v4cacc80 | acc,
|  | v16int32 | xbuff,
|  | int | xstart,
|  | unsigned int | xoffsets,
|  | int | ystart,
|  | v4cint32 | zbuff,
|  | int | zstart,
|  | unsigned int | zoffsets,
|  | bool | zconj
| ) |  |

Complex multiply-subtract intrinsic function with dynamic z buffer conjugation after computing the maximum between the selected lanes from the input buffer using small X input buffer.

acc0 -= z00*(max(x00 , y00))
acc1 -= z10*(max(x10 , y10))
acc2 -= z20*(max(x20 , y20))
acc3 -= z30*(max(x30 , y30))

Returns
  Returned accumulation vector (4 x cint80 lanes)

Parameters

  acc | Incoming accumulation vector (4 x cint80 lanes)
  xbuff | Input buffer of 16 elements of type int32
  xstart | Starting position offset applied to all lanes of input from X buffer.
  xoffsets | 4b offset for each lane, applied to both x and y buffers. LSB apply to first lane
  ystart | Starting position offset applied to all lanes for input from Y buffer.
  zbuff | Input buffer of 4 elements of type cint32
  zstart | Starting position offset applied to all lanes for input from Z buffer. This must be a compile time constant. Only the 4 LSB of the argument are used.
  zoffsets | 4b offset for each lane, applied to input from Z buffer. LSB apply to first lane
  zconj | Selector for conjugation in Z buffer

Note
  - For more information on how data selection works from the buffers go here. The data buffer and coefficient buffer in this intrinsic use the general scheme.
  - Parameter 'zstart' must be a compile time constant.

## ◆ lmsc4_max() [2/3]

v4cacc80 lmsc4_max | ( | v4cacc80 | acc,
|  | v16int32 | xbuff,
|  | int | xstart,
|  | unsigned int | xoffsets,
|  | v16int32 | ybuff,
|  | int | ystart,
|  | v4cint32 | zbuff,
|  | int | zstart,
|  | unsigned int | zoffsets,
|  | bool | zconj
| ) |  |

Complex multiply-subtract intrinsic function with dynamic z buffer conjugation after computing the maximum between the selected lanes from the input buffer using small X input buffer.

acc0 -= z00*(max(x00 , y00))
acc1 -= z10*(max(x10 , y10))
acc2 -= z20*(max(x20 , y20))
acc3 -= z30*(max(x30 , y30))

Returns
  Returned accumulation vector (4 x cint80 lanes)

Parameters

  acc | Incoming accumulation vector (4 x cint80 lanes)
  xbuff | Input buffer of 16 elements of type int32
  xstart | Starting position offset applied to all lanes of input from X buffer.
  xoffsets | 4b offset for each lane, applied to both x and y buffers. LSB apply to first lane
  ybuff | Right input buffer of 16 elements of type int32
  ystart | Starting position offset applied to all lanes for input from Y buffer.
  zbuff | Input buffer of 4 elements of type cint32
  zstart | Starting position offset applied to all lanes for input from Z buffer. This must be a compile time constant. Only the 4 LSB of the argument are used.
  zoffsets | 4b offset for each lane, applied to input from Z buffer. LSB apply to first lane
  zconj | Selector for conjugation in Z buffer

Note
  - For more information on how data selection works from the buffers go here. The data buffer and coefficient buffer in this intrinsic use the general scheme.
  - Parameter 'zstart' must be a compile time constant.

## ◆ lmsc4_max() [3/3]

v4cacc80 lmsc4_max | ( | v4cacc80 | acc,
|  | v32int32 | xbuff,
|  | int | xstart,
|  | unsigned int | xoffsets,
|  | int | ystart,
|  | v4cint32 | zbuff,
|  | int | zstart,
|  | unsigned int | zoffsets,
|  | bool | zconj
| ) |  |

Complex multiply-subtract intrinsic function with dynamic z buffer conjugation after computing the maximum between the selected lanes from the input buffer .

acc0 -= z00*(max(x00 , y00))
acc1 -= z10*(max(x10 , y10))
acc2 -= z20*(max(x20 , y20))
acc3 -= z30*(max(x30 , y30))

Returns
  Returned accumulation vector (4 x cint80 lanes)

Parameters

  acc | Incoming accumulation vector (4 x cint80 lanes)
  xbuff | Input buffer of 32 elements of type int32
  xstart | Starting position offset applied to all lanes of input from X buffer.
  xoffsets | 4b offset for each lane, applied to both x and y buffers. LSB apply to first lane
  ystart | Starting position offset applied to all lanes for input from Y buffer.
  zbuff | Input buffer of 4 elements of type cint32
  zstart | Starting position offset applied to all lanes for input from Z buffer. This must be a compile time constant. Only the 4 LSB of the argument are used.
  zoffsets | 4b offset for each lane, applied to input from Z buffer. LSB apply to first lane
  zconj | Selector for conjugation in Z buffer

Note
  - For more information on how data selection works from the buffers go here. The data buffer and coefficient buffer in this intrinsic use the general scheme.
  - Parameter 'zstart' must be a compile time constant.

## ◆ lmsc4_maxdiff() [1/3]

v4cacc80 lmsc4_maxdiff | ( | v4cacc80 | acc,
|  | v16int32 | xbuff,
|  | int | xstart,
|  | unsigned int | xoffsets,
|  | int | ystart,
|  | v4cint32 | zbuff,
|  | int | zstart,
|  | unsigned int | zoffsets,
|  | bool | zconj
| ) |  |

Complex multiply-subtract intrinsic function with dynamic z buffer conjugation after computing the maximum difference between the selected lanes from the input buffer using small X input buffer.

acc0 -= z00*((x00 - y00 > 0) ? (x00 - y00):0)
acc1 -= z10*((x10 - y10 > 0) ? (x10 - y10):0)
acc2 -= z20*((x20 - y20 > 0) ? (x20 - y20):0)
acc3 -= z30*((x30 - y30 > 0) ? (x30 - y30):0)

Returns
  Returned accumulation vector (4 x cint80 lanes)

Parameters

  acc | Incoming accumulation vector (4 x cint80 lanes)
  xbuff | Input buffer of 16 elements of type int32
  xstart | Starting position offset applied to all lanes of input from X buffer.
  xoffsets | 4b offset for each lane, applied to both x and y buffers. LSB apply to first lane
  ystart | Starting position offset applied to all lanes for input from Y buffer.
  zbuff | Input buffer of 4 elements of type cint32
  zstart | Starting position offset applied to all lanes for input from Z buffer. This must be a compile time constant. Only the 4 LSB of the argument are used.
  zoffsets | 4b offset for each lane, applied to input from Z buffer. LSB apply to first lane
  zconj | Selector for conjugation in Z buffer

Note
  - For more information on how data selection works from the buffers go here. The data buffer and coefficient buffer in this intrinsic use the general scheme.
  - Parameter 'zstart' must be a compile time constant.

## ◆ lmsc4_maxdiff() [2/3]

v4cacc80 lmsc4_maxdiff | ( | v4cacc80 | acc,
|  | v16int32 | xbuff,
|  | int | xstart,
|  | unsigned int | xoffsets,
|  | v16int32 | ybuff,
|  | int | ystart,
|  | v4cint32 | zbuff,
|  | int | zstart,
|  | unsigned int | zoffsets,
|  | bool | zconj
| ) |  |

Complex multiply-subtract intrinsic function with dynamic z buffer conjugation after computing the maximum difference between the selected lanes from the input buffer using small X input buffer.

acc0 -= z00*((x00 - y00 > 0) ? (x00 - y00):0)
acc1 -= z10*((x10 - y10 > 0) ? (x10 - y10):0)
acc2 -= z20*((x20 - y20 > 0) ? (x20 - y20):0)
acc3 -= z30*((x30 - y30 > 0) ? (x30 - y30):0)

Returns
  Returned accumulation vector (4 x cint80 lanes)

Parameters

  acc | Incoming accumulation vector (4 x cint80 lanes)
  xbuff | Input buffer of 16 elements of type int32
  xstart | Starting position offset applied to all lanes of input from X buffer.
  xoffsets | 4b offset for each lane, applied to both x and y buffers. LSB apply to first lane
  ybuff | Right input buffer of 16 elements of type int32
  ystart | Starting position offset applied to all lanes for input from Y buffer.
  zbuff | Input buffer of 4 elements of type cint32
  zstart | Starting position offset applied to all lanes for input from Z buffer. This must be a compile time constant. Only the 4 LSB of the argument are used.
  zoffsets | 4b offset for each lane, applied to input from Z buffer. LSB apply to first lane
  zconj | Selector for conjugation in Z buffer

Note
  - For more information on how data selection works from the buffers go here. The data buffer and coefficient buffer in this intrinsic use the general scheme.
  - Parameter 'zstart' must be a compile time constant.

## ◆ lmsc4_maxdiff() [3/3]

v4cacc80 lmsc4_maxdiff | ( | v4cacc80 | acc,
|  | v32int32 | xbuff,
|  | int | xstart,
|  | unsigned int | xoffsets,
|  | int | ystart,
|  | v4cint32 | zbuff,
|  | int | zstart,
|  | unsigned int | zoffsets,
|  | bool | zconj
| ) |  |

Complex multiply-subtract intrinsic function with dynamic z buffer conjugation after computing the maximum difference between the selected lanes from the input buffer .

acc0 -= z00*((x00 - y00 > 0) ? (x00 - y00):0)
acc1 -= z10*((x10 - y10 > 0) ? (x10 - y10):0)
acc2 -= z20*((x20 - y20 > 0) ? (x20 - y20):0)
acc3 -= z30*((x30 - y30 > 0) ? (x30 - y30):0)

Returns
  Returned accumulation vector (4 x cint80 lanes)

Parameters

  acc | Incoming accumulation vector (4 x cint80 lanes)
  xbuff | Input buffer of 32 elements of type int32
  xstart | Starting position offset applied to all lanes of input from X buffer.
  xoffsets | 4b offset for each lane, applied to both x and y buffers. LSB apply to first lane
  ystart | Starting position offset applied to all lanes for input from Y buffer.
  zbuff | Input buffer of 4 elements of type cint32
  zstart | Starting position offset applied to all lanes for input from Z buffer. This must be a compile time constant. Only the 4 LSB of the argument are used.
  zoffsets | 4b offset for each lane, applied to input from Z buffer. LSB apply to first lane
  zconj | Selector for conjugation in Z buffer

Note
  - For more information on how data selection works from the buffers go here. The data buffer and coefficient buffer in this intrinsic use the general scheme.
  - Parameter 'zstart' must be a compile time constant.

## ◆ lmsc4_min() [1/3]

v4cacc80 lmsc4_min | ( | v4cacc80 | acc,
|  | v16int32 | xbuff,
|  | int | xstart,
|  | unsigned int | xoffsets,
|  | int | ystart,
|  | v4cint32 | zbuff,
|  | int | zstart,
|  | unsigned int | zoffsets,
|  | bool | zconj
| ) |  |

Complex multiply-subtract intrinsic function with dynamic z buffer conjugation after computing the minimum between the selected lanes from the input buffer using small X input buffer.

acc0 -= z00*(min(x00 , y00))
acc1 -= z10*(min(x10 , y10))
acc2 -= z20*(min(x20 , y20))
acc3 -= z30*(min(x30 , y30))

Returns
  Returned accumulation vector (4 x cint80 lanes)

Parameters

  acc | Incoming accumulation vector (4 x cint80 lanes)
  xbuff | Input buffer of 16 elements of type int32
  xstart | Starting position offset applied to all lanes of input from X buffer.
  xoffsets | 4b offset for each lane, applied to both x and y buffers. LSB apply to first lane
  ystart | Starting position offset applied to all lanes for input from Y buffer.
  zbuff | Input buffer of 4 elements of type cint32
  zstart | Starting position offset applied to all lanes for input from Z buffer. This must be a compile time constant. Only the 4 LSB of the argument are used.
  zoffsets | 4b offset for each lane, applied to input from Z buffer. LSB apply to first lane
  zconj | Selector for conjugation in Z buffer

Note
  - For more information on how data selection works from the buffers go here. The data buffer and coefficient buffer in this intrinsic use the general scheme.
  - Parameter 'zstart' must be a compile time constant.

## ◆ lmsc4_min() [2/3]

v4cacc80 lmsc4_min | ( | v4cacc80 | acc,
|  | v16int32 | xbuff,
|  | int | xstart,
|  | unsigned int | xoffsets,
|  | v16int32 | ybuff,
|  | int | ystart,
|  | v4cint32 | zbuff,
|  | int | zstart,
|  | unsigned int | zoffsets,
|  | bool | zconj
| ) |  |

Complex multiply-subtract intrinsic function with dynamic z buffer conjugation after computing the minimum between the selected lanes from the input buffer using small X input buffer.

acc0 -= z00*(min(x00 , y00))
acc1 -= z10*(min(x10 , y10))
acc2 -= z20*(min(x20 , y20))
acc3 -= z30*(min(x30 , y30))

Returns
  Returned accumulation vector (4 x cint80 lanes)

Parameters

  acc | Incoming accumulation vector (4 x cint80 lanes)
  xbuff | Input buffer of 16 elements of type int32
  xstart | Starting position offset applied to all lanes of input from X buffer.
  xoffsets | 4b offset for each lane, applied to both x and y buffers. LSB apply to first lane
  ybuff | Right input buffer of 16 elements of type int32
  ystart | Starting position offset applied to all lanes for input from Y buffer.
  zbuff | Input buffer of 4 elements of type cint32
  zstart | Starting position offset applied to all lanes for input from Z buffer. This must be a compile time constant. Only the 4 LSB of the argument are used.
  zoffsets | 4b offset for each lane, applied to input from Z buffer. LSB apply to first lane
  zconj | Selector for conjugation in Z buffer

Note
  - For more information on how data selection works from the buffers go here. The data buffer and coefficient buffer in this intrinsic use the general scheme.
  - Parameter 'zstart' must be a compile time constant.

## ◆ lmsc4_min() [3/3]

v4cacc80 lmsc4_min | ( | v4cacc80 | acc,
|  | v32int32 | xbuff,
|  | int | xstart,
|  | unsigned int | xoffsets,
|  | int | ystart,
|  | v4cint32 | zbuff,
|  | int | zstart,
|  | unsigned int | zoffsets,
|  | bool | zconj
| ) |  |

Complex multiply-subtract intrinsic function with dynamic z buffer conjugation after computing the minimum between the selected lanes from the input buffer .

acc0 -= z00*(min(x00 , y00))
acc1 -= z10*(min(x10 , y10))
acc2 -= z20*(min(x20 , y20))
acc3 -= z30*(min(x30 , y30))

Returns
  Returned accumulation vector (4 x cint80 lanes)

Parameters

  acc | Incoming accumulation vector (4 x cint80 lanes)
  xbuff | Input buffer of 32 elements of type int32
  xstart | Starting position offset applied to all lanes of input from X buffer.
  xoffsets | 4b offset for each lane, applied to both x and y buffers. LSB apply to first lane
  ystart | Starting position offset applied to all lanes for input from Y buffer.
  zbuff | Input buffer of 4 elements of type cint32
  zstart | Starting position offset applied to all lanes for input from Z buffer. This must be a compile time constant. Only the 4 LSB of the argument are used.
  zoffsets | 4b offset for each lane, applied to input from Z buffer. LSB apply to first lane
  zconj | Selector for conjugation in Z buffer

Note
  - For more information on how data selection works from the buffers go here. The data buffer and coefficient buffer in this intrinsic use the general scheme.
  - Parameter 'zstart' must be a compile time constant.

## ◆ lmul2_abs() [1/2]

v2cacc80 lmul2_abs | ( | v16int32 | xbuff,
|  | int | xstart,
|  | unsigned int | xoffsets,
|  | int | xstep,
|  | v4cint32 | zbuff,
|  | int | zstart,
|  | unsigned int | zoffsets,
|  | int | zstep,
|  | bool | zconj
| ) |  |

Complex multiply intrinsic function with dynamic z buffer conjugation after computing the absolute value in the selected lanes from the input buffer using small X input buffer.

acc0 = z00*abs(x00) + z01*abs(x01)
acc1 = z10*abs(x10) + z11*abs(x11)

Returns
  Returned accumulation vector (2 x cint80 lanes)

Parameters

  xbuff | Input buffer of 16 elements of type int32
  xstart | Starting position offset applied to all lanes of input from X buffer.
  xoffsets | 4b offset for each lane, applied to the x buffer. LSB apply to first lane
  xstep | Step between each column for selection in the xbuffer.
  zbuff | Input buffer of 4 elements of type cint32
  zstart | Starting position offset applied to all lanes for input from Z buffer. This must be a compile time constant. Only the 4 LSB of the argument are used.
  zoffsets | 4b offset for each lane, applied to input from Z buffer. LSB apply to first lane
  zstep | Step between each column for selection in the zbuffer.
  zconj | Selector for conjugation in Z buffer

Note
  - For more information on how data selection works from the buffers go here. The data buffer and coefficient buffer in this intrinsic use the general scheme.
  - Parameter 'zstart' must be a compile time constant.

## ◆ lmul2_abs() [2/2]

v2cacc80 lmul2_abs | ( | v32int32 | xbuff,
|  | int | xstart,
|  | unsigned int | xoffsets,
|  | int | xstep,
|  | v4cint32 | zbuff,
|  | int | zstart,
|  | unsigned int | zoffsets,
|  | int | zstep,
|  | bool | zconj
| ) |  |

Complex multiply intrinsic function with dynamic z buffer conjugation after computing the absolute value in the selected lanes from the input buffer .

acc0 = z00*abs(x00) + z01*abs(x01)
acc1 = z10*abs(x10) + z11*abs(x11)

Returns
  Returned accumulation vector (2 x cint80 lanes)

Parameters

  xbuff | Input buffer of 32 elements of type int32
  xstart | Starting position offset applied to all lanes of input from X buffer.
  xoffsets | 4b offset for each lane, applied to the x buffer. LSB apply to first lane
  xstep | Step between each column for selection in the xbuffer.
  zbuff | Input buffer of 4 elements of type cint32
  zstart | Starting position offset applied to all lanes for input from Z buffer. This must be a compile time constant. Only the 4 LSB of the argument are used.
  zoffsets | 4b offset for each lane, applied to input from Z buffer. LSB apply to first lane
  zstep | Step between each column for selection in the zbuffer.
  zconj | Selector for conjugation in Z buffer

Note
  - For more information on how data selection works from the buffers go here. The data buffer and coefficient buffer in this intrinsic use the general scheme.
  - Parameter 'zstart' must be a compile time constant.

## ◆ lmul2_max() [1/3]

v2cacc80 lmul2_max | ( | v16int32 | xbuff,
|  | int | xstart,
|  | unsigned int | xoffsets,
|  | int | xstep,
|  | int | ystart,
|  | v4cint32 | zbuff,
|  | int | zstart,
|  | unsigned int | zoffsets,
|  | int | zstep,
|  | bool | zconj
| ) |  |

Complex multiply intrinsic function with dynamic z buffer conjugation after computing the maximum between the selected lanes from the input buffer using small X input buffer.

acc0 = z00*(max(x00 , y00)) + z01*(max(x01 , y01))
acc1 = z10*(max(x10 , y10)) + z11*(max(x11 , y11))

Returns
  Returned accumulation vector (2 x cint80 lanes)

Parameters

  xbuff | Input buffer of 16 elements of type int32
  xstart | Starting position offset applied to all lanes of input from X buffer.
  xoffsets | 4b offset for each lane, applied to both x and y buffers. LSB apply to first lane
  xstep | Step between each column for selection in the x and y buffers. Ystep is symmetric to xstep (ystep advances by -xstep).
  ystart | Starting position offset applied to all lanes for input from Y buffer.
  zbuff | Input buffer of 4 elements of type cint32
  zstart | Starting position offset applied to all lanes for input from Z buffer. This must be a compile time constant. Only the 4 LSB of the argument are used.
  zoffsets | 4b offset for each lane, applied to input from Z buffer. LSB apply to first lane
  zstep | Step between each column for selection in the zbuffer.
  zconj | Selector for conjugation in Z buffer

Note
  - For more information on how data selection works from the buffers go here. The data buffer and coefficient buffer in this intrinsic use the general scheme.
  - Parameter 'zstart' must be a compile time constant.

## ◆ lmul2_max() [2/3]

v2cacc80 lmul2_max | ( | v16int32 | xbuff,
|  | int | xstart,
|  | unsigned int | xoffsets,
|  | int | xstep,
|  | v16int32 | ybuff,
|  | int | ystart,
|  | v4cint32 | zbuff,
|  | int | zstart,
|  | unsigned int | zoffsets,
|  | int | zstep,
|  | bool | zconj
| ) |  |

Complex multiply intrinsic function with dynamic z buffer conjugation after computing the maximum between the selected lanes from the input buffer using small X input buffer.

acc0 = z00*(max(x00 , y00)) + z01*(max(x01 , y01))
acc1 = z10*(max(x10 , y10)) + z11*(max(x11 , y11))

Returns
  Returned accumulation vector (2 x cint80 lanes)

Parameters

  xbuff | Input buffer of 16 elements of type int32
  xstart | Starting position offset applied to all lanes of input from X buffer.
  xoffsets | 4b offset for each lane, applied to both x and y buffers. LSB apply to first lane
  xstep | Step between each column for selection in the x and y buffers. Ystep is symmetric to xstep (ystep advances by -xstep).
  ybuff | Right input buffer of 16 elements of type int32
  ystart | Starting position offset applied to all lanes for input from Y buffer.
  zbuff | Input buffer of 4 elements of type cint32
  zstart | Starting position offset applied to all lanes for input from Z buffer. This must be a compile time constant. Only the 4 LSB of the argument are used.
  zoffsets | 4b offset for each lane, applied to input from Z buffer. LSB apply to first lane
  zstep | Step between each column for selection in the zbuffer.
  zconj | Selector for conjugation in Z buffer

Note
  - For more information on how data selection works from the buffers go here. The data buffer and coefficient buffer in this intrinsic use the general scheme.
  - Parameter 'zstart' must be a compile time constant.

## ◆ lmul2_max() [3/3]

v2cacc80 lmul2_max | ( | v32int32 | xbuff,
|  | int | xstart,
|  | unsigned int | xoffsets,
|  | int | xstep,
|  | int | ystart,
|  | v4cint32 | zbuff,
|  | int | zstart,
|  | unsigned int | zoffsets,
|  | int | zstep,
|  | bool | zconj
| ) |  |

Complex multiply intrinsic function with dynamic z buffer conjugation after computing the maximum between the selected lanes from the input buffer .

acc0 = z00*(max(x00 , y00)) + z01*(max(x01 , y01))
acc1 = z10*(max(x10 , y10)) + z11*(max(x11 , y11))

Returns
  Returned accumulation vector (2 x cint80 lanes)

Parameters

  xbuff | Input buffer of 32 elements of type int32
  xstart | Starting position offset applied to all lanes of input from X buffer.
  xoffsets | 4b offset for each lane, applied to both x and y buffers. LSB apply to first lane
  xstep | Step between each column for selection in the x and y buffers. Ystep is symmetric to xstep (ystep advances by -xstep).
  ystart | Starting position offset applied to all lanes for input from Y buffer.
  zbuff | Input buffer of 4 elements of type cint32
  zstart | Starting position offset applied to all lanes for input from Z buffer. This must be a compile time constant. Only the 4 LSB of the argument are used.
  zoffsets | 4b offset for each lane, applied to input from Z buffer. LSB apply to first lane
  zstep | Step between each column for selection in the zbuffer.
  zconj | Selector for conjugation in Z buffer

Note
  - For more information on how data selection works from the buffers go here. The data buffer and coefficient buffer in this intrinsic use the general scheme.
  - Parameter 'zstart' must be a compile time constant.

## ◆ lmul2_maxdiff() [1/3]

v2cacc80 lmul2_maxdiff | ( | v16int32 | xbuff,
|  | int | xstart,
|  | unsigned int | xoffsets,
|  | int | xstep,
|  | int | ystart,
|  | v4cint32 | zbuff,
|  | int | zstart,
|  | unsigned int | zoffsets,
|  | int | zstep,
|  | bool | zconj
| ) |  |

Complex multiply intrinsic function with dynamic z buffer conjugation after computing the maximum difference between the selected lanes from the input buffer using small X input buffer.

acc0 = z00*((x00 - y00 > 0) ? (x00 - y00):0) + z01*((x01 - y01 > 0) ? (x01 - y01):0)
acc1 = z10*((x10 - y10 > 0) ? (x10 - y10):0) + z11*((x11 - y11 > 0) ? (x11 - y11):0)

Returns
  Returned accumulation vector (2 x cint80 lanes)

Parameters

  xbuff | Input buffer of 16 elements of type int32
  xstart | Starting position offset applied to all lanes of input from X buffer.
  xoffsets | 4b offset for each lane, applied to both x and y buffers. LSB apply to first lane
  xstep | Step between each column for selection in the x and y buffers. Ystep is symmetric to xstep (ystep advances by -xstep).
  ystart | Starting position offset applied to all lanes for input from Y buffer.
  zbuff | Input buffer of 4 elements of type cint32
  zstart | Starting position offset applied to all lanes for input from Z buffer. This must be a compile time constant. Only the 4 LSB of the argument are used.
  zoffsets | 4b offset for each lane, applied to input from Z buffer. LSB apply to first lane
  zstep | Step between each column for selection in the zbuffer.
  zconj | Selector for conjugation in Z buffer

Note
  - For more information on how data selection works from the buffers go here. The data buffer and coefficient buffer in this intrinsic use the general scheme.
  - Parameter 'zstart' must be a compile time constant.

## ◆ lmul2_maxdiff() [2/3]

v2cacc80 lmul2_maxdiff | ( | v16int32 | xbuff,
|  | int | xstart,
|  | unsigned int | xoffsets,
|  | int | xstep,
|  | v16int32 | ybuff,
|  | int | ystart,
|  | v4cint32 | zbuff,
|  | int | zstart,
|  | unsigned int | zoffsets,
|  | int | zstep,
|  | bool | zconj
| ) |  |

Complex multiply intrinsic function with dynamic z buffer conjugation after computing the maximum difference between the selected lanes from the input buffer using small X input buffer.

acc0 = z00*((x00 - y00 > 0) ? (x00 - y00):0) + z01*((x01 - y01 > 0) ? (x01 - y01):0)
acc1 = z10*((x10 - y10 > 0) ? (x10 - y10):0) + z11*((x11 - y11 > 0) ? (x11 - y11):0)

Returns
  Returned accumulation vector (2 x cint80 lanes)

Parameters

  xbuff | Input buffer of 16 elements of type int32
  xstart | Starting position offset applied to all lanes of input from X buffer.
  xoffsets | 4b offset for each lane, applied to both x and y buffers. LSB apply to first lane
  xstep | Step between each column for selection in the x and y buffers. Ystep is symmetric to xstep (ystep advances by -xstep).
  ybuff | Right input buffer of 16 elements of type int32
  ystart | Starting position offset applied to all lanes for input from Y buffer.
  zbuff | Input buffer of 4 elements of type cint32
  zstart | Starting position offset applied to all lanes for input from Z buffer. This must be a compile time constant. Only the 4 LSB of the argument are used.
  zoffsets | 4b offset for each lane, applied to input from Z buffer. LSB apply to first lane
  zstep | Step between each column for selection in the zbuffer.
  zconj | Selector for conjugation in Z buffer

Note
  - For more information on how data selection works from the buffers go here. The data buffer and coefficient buffer in this intrinsic use the general scheme.
  - Parameter 'zstart' must be a compile time constant.

## ◆ lmul2_maxdiff() [3/3]

v2cacc80 lmul2_maxdiff | ( | v32int32 | xbuff,
|  | int | xstart,
|  | unsigned int | xoffsets,
|  | int | xstep,
|  | int | ystart,
|  | v4cint32 | zbuff,
|  | int | zstart,
|  | unsigned int | zoffsets,
|  | int | zstep,
|  | bool | zconj
| ) |  |

Complex multiply intrinsic function with dynamic z buffer conjugation after computing the maximum difference between the selected lanes from the input buffer .

acc0 = z00*((x00 - y00 > 0) ? (x00 - y00):0) + z01*((x01 - y01 > 0) ? (x01 - y01):0)
acc1 = z10*((x10 - y10 > 0) ? (x10 - y10):0) + z11*((x11 - y11 > 0) ? (x11 - y11):0)

Returns
  Returned accumulation vector (2 x cint80 lanes)

Parameters

  xbuff | Input buffer of 32 elements of type int32
  xstart | Starting position offset applied to all lanes of input from X buffer.
  xoffsets | 4b offset for each lane, applied to both x and y buffers. LSB apply to first lane
  xstep | Step between each column for selection in the x and y buffers. Ystep is symmetric to xstep (ystep advances by -xstep).
  ystart | Starting position offset applied to all lanes for input from Y buffer.
  zbuff | Input buffer of 4 elements of type cint32
  zstart | Starting position offset applied to all lanes for input from Z buffer. This must be a compile time constant. Only the 4 LSB of the argument are used.
  zoffsets | 4b offset for each lane, applied to input from Z buffer. LSB apply to first lane
  zstep | Step between each column for selection in the zbuffer.
  zconj | Selector for conjugation in Z buffer

Note
  - For more information on how data selection works from the buffers go here. The data buffer and coefficient buffer in this intrinsic use the general scheme.
  - Parameter 'zstart' must be a compile time constant.

## ◆ lmul2_min() [1/3]

v2cacc80 lmul2_min | ( | v16int32 | xbuff,
|  | int | xstart,
|  | unsigned int | xoffsets,
|  | int | xstep,
|  | int | ystart,
|  | v4cint32 | zbuff,
|  | int | zstart,
|  | unsigned int | zoffsets,
|  | int | zstep,
|  | bool | zconj
| ) |  |

Complex multiply intrinsic function with dynamic z buffer conjugation after computing the minimum between the selected lanes from the input buffer using small X input buffer.

acc0 = z00*(min(x00 , y00)) + z01*(min(x01 , y01))
acc1 = z10*(min(x10 , y10)) + z11*(min(x11 , y11))

Returns
  Returned accumulation vector (2 x cint80 lanes)

Parameters

  xbuff | Input buffer of 16 elements of type int32
  xstart | Starting position offset applied to all lanes of input from X buffer.
  xoffsets | 4b offset for each lane, applied to both x and y buffers. LSB apply to first lane
  xstep | Step between each column for selection in the x and y buffers. Ystep is symmetric to xstep (ystep advances by -xstep).
  ystart | Starting position offset applied to all lanes for input from Y buffer.
  zbuff | Input buffer of 4 elements of type cint32
  zstart | Starting position offset applied to all lanes for input from Z buffer. This must be a compile time constant. Only the 4 LSB of the argument are used.
  zoffsets | 4b offset for each lane, applied to input from Z buffer. LSB apply to first lane
  zstep | Step between each column for selection in the zbuffer.
  zconj | Selector for conjugation in Z buffer

Note
  - For more information on how data selection works from the buffers go here. The data buffer and coefficient buffer in this intrinsic use the general scheme.
  - Parameter 'zstart' must be a compile time constant.

## ◆ lmul2_min() [2/3]

v2cacc80 lmul2_min | ( | v16int32 | xbuff,
|  | int | xstart,
|  | unsigned int | xoffsets,
|  | int | xstep,
|  | v16int32 | ybuff,
|  | int | ystart,
|  | v4cint32 | zbuff,
|  | int | zstart,
|  | unsigned int | zoffsets,
|  | int | zstep,
|  | bool | zconj
| ) |  |

Complex multiply intrinsic function with dynamic z buffer conjugation after computing the minimum between the selected lanes from the input buffer using small X input buffer.

acc0 = z00*(min(x00 , y00)) + z01*(min(x01 , y01))
acc1 = z10*(min(x10 , y10)) + z11*(min(x11 , y11))

Returns
  Returned accumulation vector (2 x cint80 lanes)

Parameters

  xbuff | Input buffer of 16 elements of type int32
  xstart | Starting position offset applied to all lanes of input from X buffer.
  xoffsets | 4b offset for each lane, applied to both x and y buffers. LSB apply to first lane
  xstep | Step between each column for selection in the x and y buffers. Ystep is symmetric to xstep (ystep advances by -xstep).
  ybuff | Right input buffer of 16 elements of type int32
  ystart | Starting position offset applied to all lanes for input from Y buffer.
  zbuff | Input buffer of 4 elements of type cint32
  zstart | Starting position offset applied to all lanes for input from Z buffer. This must be a compile time constant. Only the 4 LSB of the argument are used.
  zoffsets | 4b offset for each lane, applied to input from Z buffer. LSB apply to first lane
  zstep | Step between each column for selection in the zbuffer.
  zconj | Selector for conjugation in Z buffer

Note
  - For more information on how data selection works from the buffers go here. The data buffer and coefficient buffer in this intrinsic use the general scheme.
  - Parameter 'zstart' must be a compile time constant.

## ◆ lmul2_min() [3/3]

v2cacc80 lmul2_min | ( | v32int32 | xbuff,
|  | int | xstart,
|  | unsigned int | xoffsets,
|  | int | xstep,
|  | int | ystart,
|  | v4cint32 | zbuff,
|  | int | zstart,
|  | unsigned int | zoffsets,
|  | int | zstep,
|  | bool | zconj
| ) |  |

Complex multiply intrinsic function with dynamic z buffer conjugation after computing the minimum between the selected lanes from the input buffer .

acc0 = z00*(min(x00 , y00)) + z01*(min(x01 , y01))
acc1 = z10*(min(x10 , y10)) + z11*(min(x11 , y11))

Returns
  Returned accumulation vector (2 x cint80 lanes)

Parameters

  xbuff | Input buffer of 32 elements of type int32
  xstart | Starting position offset applied to all lanes of input from X buffer.
  xoffsets | 4b offset for each lane, applied to both x and y buffers. LSB apply to first lane
  xstep | Step between each column for selection in the x and y buffers. Ystep is symmetric to xstep (ystep advances by -xstep).
  ystart | Starting position offset applied to all lanes for input from Y buffer.
  zbuff | Input buffer of 4 elements of type cint32
  zstart | Starting position offset applied to all lanes for input from Z buffer. This must be a compile time constant. Only the 4 LSB of the argument are used.
  zoffsets | 4b offset for each lane, applied to input from Z buffer. LSB apply to first lane
  zstep | Step between each column for selection in the zbuffer.
  zconj | Selector for conjugation in Z buffer

Note
  - For more information on how data selection works from the buffers go here. The data buffer and coefficient buffer in this intrinsic use the general scheme.
  - Parameter 'zstart' must be a compile time constant.

## ◆ lmul4_abs() [1/2]

v4cacc80 lmul4_abs | ( | v16int32 | xbuff,
|  | int | xstart,
|  | unsigned int | xoffsets,
|  | v4cint32 | zbuff,
|  | int | zstart,
|  | unsigned int | zoffsets,
|  | bool | zconj
| ) |  |

Complex multiply intrinsic function with dynamic z buffer conjugation after computing the absolute value in the selected lanes from the input buffer using small X input buffer.

acc0 = z00*abs(x00)
acc1 = z10*abs(x10)
acc2 = z20*abs(x20)
acc3 = z30*abs(x30)

Returns
  Returned accumulation vector (4 x cint80 lanes)

Parameters

  xbuff | Input buffer of 16 elements of type int32
  xstart | Starting position offset applied to all lanes of input from X buffer.
  xoffsets | 4b offset for each lane, applied to the x buffer. LSB apply to first lane
  zbuff | Input buffer of 4 elements of type cint32
  zstart | Starting position offset applied to all lanes for input from Z buffer. This must be a compile time constant. Only the 4 LSB of the argument are used.
  zoffsets | 4b offset for each lane, applied to input from Z buffer. LSB apply to first lane
  zconj | Selector for conjugation in Z buffer

Note
  - For more information on how data selection works from the buffers go here. The data buffer and coefficient buffer in this intrinsic use the general scheme.
  - Parameter 'zstart' must be a compile time constant.

## ◆ lmul4_abs() [2/2]

v4cacc80 lmul4_abs | ( | v32int32 | xbuff,
|  | int | xstart,
|  | unsigned int | xoffsets,
|  | v4cint32 | zbuff,
|  | int | zstart,
|  | unsigned int | zoffsets,
|  | bool | zconj
| ) |  |

Complex multiply intrinsic function with dynamic z buffer conjugation after computing the absolute value in the selected lanes from the input buffer .

acc0 = z00*abs(x00)
acc1 = z10*abs(x10)
acc2 = z20*abs(x20)
acc3 = z30*abs(x30)

Returns
  Returned accumulation vector (4 x cint80 lanes)

Parameters

  xbuff | Input buffer of 32 elements of type int32
  xstart | Starting position offset applied to all lanes of input from X buffer.
  xoffsets | 4b offset for each lane, applied to the x buffer. LSB apply to first lane
  zbuff | Input buffer of 4 elements of type cint32
  zstart | Starting position offset applied to all lanes for input from Z buffer. This must be a compile time constant. Only the 4 LSB of the argument are used.
  zoffsets | 4b offset for each lane, applied to input from Z buffer. LSB apply to first lane
  zconj | Selector for conjugation in Z buffer

Note
  - For more information on how data selection works from the buffers go here. The data buffer and coefficient buffer in this intrinsic use the general scheme.
  - Parameter 'zstart' must be a compile time constant.

## ◆ lmul4_max() [1/3]

v4cacc80 lmul4_max | ( | v16int32 | xbuff,
|  | int | xstart,
|  | unsigned int | xoffsets,
|  | int | ystart,
|  | v4cint32 | zbuff,
|  | int | zstart,
|  | unsigned int | zoffsets,
|  | bool | zconj
| ) |  |

Complex multiply intrinsic function with dynamic z buffer conjugation after computing the maximum between the selected lanes from the input buffer using small X input buffer.

acc0 = z00*(max(x00 , y00))
acc1 = z10*(max(x10 , y10))
acc2 = z20*(max(x20 , y20))
acc3 = z30*(max(x30 , y30))

Returns
  Returned accumulation vector (4 x cint80 lanes)

Parameters

  xbuff | Input buffer of 16 elements of type int32
  xstart | Starting position offset applied to all lanes of input from X buffer.
  xoffsets | 4b offset for each lane, applied to both x and y buffers. LSB apply to first lane
  ystart | Starting position offset applied to all lanes for input from Y buffer.
  zbuff | Input buffer of 4 elements of type cint32
  zstart | Starting position offset applied to all lanes for input from Z buffer. This must be a compile time constant. Only the 4 LSB of the argument are used.
  zoffsets | 4b offset for each lane, applied to input from Z buffer. LSB apply to first lane
  zconj | Selector for conjugation in Z buffer

Note
  - For more information on how data selection works from the buffers go here. The data buffer and coefficient buffer in this intrinsic use the general scheme.
  - Parameter 'zstart' must be a compile time constant.

## ◆ lmul4_max() [2/3]

v4cacc80 lmul4_max | ( | v16int32 | xbuff,
|  | int | xstart,
|  | unsigned int | xoffsets,
|  | v16int32 | ybuff,
|  | int | ystart,
|  | v4cint32 | zbuff,
|  | int | zstart,
|  | unsigned int | zoffsets,
|  | bool | zconj
| ) |  |

Complex multiply intrinsic function with dynamic z buffer conjugation after computing the maximum between the selected lanes from the input buffer using small X input buffer.

acc0 = z00*(max(x00 , y00))
acc1 = z10*(max(x10 , y10))
acc2 = z20*(max(x20 , y20))
acc3 = z30*(max(x30 , y30))

Returns
  Returned accumulation vector (4 x cint80 lanes)

Parameters

  xbuff | Input buffer of 16 elements of type int32
  xstart | Starting position offset applied to all lanes of input from X buffer.
  xoffsets | 4b offset for each lane, applied to both x and y buffers. LSB apply to first lane
  ybuff | Right input buffer of 16 elements of type int32
  ystart | Starting position offset applied to all lanes for input from Y buffer.
  zbuff | Input buffer of 4 elements of type cint32
  zstart | Starting position offset applied to all lanes for input from Z buffer. This must be a compile time constant. Only the 4 LSB of the argument are used.
  zoffsets | 4b offset for each lane, applied to input from Z buffer. LSB apply to first lane
  zconj | Selector for conjugation in Z buffer

Note
  - For more information on how data selection works from the buffers go here. The data buffer and coefficient buffer in this intrinsic use the general scheme.
  - Parameter 'zstart' must be a compile time constant.

## ◆ lmul4_max() [3/3]

v4cacc80 lmul4_max | ( | v32int32 | xbuff,
|  | int | xstart,
|  | unsigned int | xoffsets,
|  | int | ystart,
|  | v4cint32 | zbuff,
|  | int | zstart,
|  | unsigned int | zoffsets,
|  | bool | zconj
| ) |  |

Complex multiply intrinsic function with dynamic z buffer conjugation after computing the maximum between the selected lanes from the input buffer .

acc0 = z00*(max(x00 , y00))
acc1 = z10*(max(x10 , y10))
acc2 = z20*(max(x20 , y20))
acc3 = z30*(max(x30 , y30))

Returns
  Returned accumulation vector (4 x cint80 lanes)

Parameters

  xbuff | Input buffer of 32 elements of type int32
  xstart | Starting position offset applied to all lanes of input from X buffer.
  xoffsets | 4b offset for each lane, applied to both x and y buffers. LSB apply to first lane
  ystart | Starting position offset applied to all lanes for input from Y buffer.
  zbuff | Input buffer of 4 elements of type cint32
  zstart | Starting position offset applied to all lanes for input from Z buffer. This must be a compile time constant. Only the 4 LSB of the argument are used.
  zoffsets | 4b offset for each lane, applied to input from Z buffer. LSB apply to first lane
  zconj | Selector for conjugation in Z buffer

Note
  - For more information on how data selection works from the buffers go here. The data buffer and coefficient buffer in this intrinsic use the general scheme.
  - Parameter 'zstart' must be a compile time constant.

## ◆ lmul4_maxdiff() [1/3]

v4cacc80 lmul4_maxdiff | ( | v16int32 | xbuff,
|  | int | xstart,
|  | unsigned int | xoffsets,
|  | int | ystart,
|  | v4cint32 | zbuff,
|  | int | zstart,
|  | unsigned int | zoffsets,
|  | bool | zconj
| ) |  |

Complex multiply intrinsic function with dynamic z buffer conjugation after computing the maximum difference between the selected lanes from the input buffer using small X input buffer.

acc0 = z00*((x00 - y00 > 0) ? (x00 - y00):0)
acc1 = z10*((x10 - y10 > 0) ? (x10 - y10):0)
acc2 = z20*((x20 - y20 > 0) ? (x20 - y20):0)
acc3 = z30*((x30 - y30 > 0) ? (x30 - y30):0)

Returns
  Returned accumulation vector (4 x cint80 lanes)

Parameters

  xbuff | Input buffer of 16 elements of type int32
  xstart | Starting position offset applied to all lanes of input from X buffer.
  xoffsets | 4b offset for each lane, applied to both x and y buffers. LSB apply to first lane
  ystart | Starting position offset applied to all lanes for input from Y buffer.
  zbuff | Input buffer of 4 elements of type cint32
  zstart | Starting position offset applied to all lanes for input from Z buffer. This must be a compile time constant. Only the 4 LSB of the argument are used.
  zoffsets | 4b offset for each lane, applied to input from Z buffer. LSB apply to first lane
  zconj | Selector for conjugation in Z buffer

Note
  - For more information on how data selection works from the buffers go here. The data buffer and coefficient buffer in this intrinsic use the general scheme.
  - Parameter 'zstart' must be a compile time constant.

## ◆ lmul4_maxdiff() [2/3]

v4cacc80 lmul4_maxdiff | ( | v16int32 | xbuff,
|  | int | xstart,
|  | unsigned int | xoffsets,
|  | v16int32 | ybuff,
|  | int | ystart,
|  | v4cint32 | zbuff,
|  | int | zstart,
|  | unsigned int | zoffsets,
|  | bool | zconj
| ) |  |

Complex multiply intrinsic function with dynamic z buffer conjugation after computing the maximum difference between the selected lanes from the input buffer using small X input buffer.

acc0 = z00*((x00 - y00 > 0) ? (x00 - y00):0)
acc1 = z10*((x10 - y10 > 0) ? (x10 - y10):0)
acc2 = z20*((x20 - y20 > 0) ? (x20 - y20):0)
acc3 = z30*((x30 - y30 > 0) ? (x30 - y30):0)

Returns
  Returned accumulation vector (4 x cint80 lanes)

Parameters

  xbuff | Input buffer of 16 elements of type int32
  xstart | Starting position offset applied to all lanes of input from X buffer.
  xoffsets | 4b offset for each lane, applied to both x and y buffers. LSB apply to first lane
  ybuff | Right input buffer of 16 elements of type int32
  ystart | Starting position offset applied to all lanes for input from Y buffer.
  zbuff | Input buffer of 4 elements of type cint32
  zstart | Starting position offset applied to all lanes for input from Z buffer. This must be a compile time constant. Only the 4 LSB of the argument are used.
  zoffsets | 4b offset for each lane, applied to input from Z buffer. LSB apply to first lane
  zconj | Selector for conjugation in Z buffer

Note
  - For more information on how data selection works from the buffers go here. The data buffer and coefficient buffer in this intrinsic use the general scheme.
  - Parameter 'zstart' must be a compile time constant.

## ◆ lmul4_maxdiff() [3/3]

v4cacc80 lmul4_maxdiff | ( | v32int32 | xbuff,
|  | int | xstart,
|  | unsigned int | xoffsets,
|  | int | ystart,
|  | v4cint32 | zbuff,
|  | int | zstart,
|  | unsigned int | zoffsets,
|  | bool | zconj
| ) |  |

Complex multiply intrinsic function with dynamic z buffer conjugation after computing the maximum difference between the selected lanes from the input buffer .

acc0 = z00*((x00 - y00 > 0) ? (x00 - y00):0)
acc1 = z10*((x10 - y10 > 0) ? (x10 - y10):0)
acc2 = z20*((x20 - y20 > 0) ? (x20 - y20):0)
acc3 = z30*((x30 - y30 > 0) ? (x30 - y30):0)

Returns
  Returned accumulation vector (4 x cint80 lanes)

Parameters

  xbuff | Input buffer of 32 elements of type int32
  xstart | Starting position offset applied to all lanes of input from X buffer.
  xoffsets | 4b offset for each lane, applied to both x and y buffers. LSB apply to first lane
  ystart | Starting position offset applied to all lanes for input from Y buffer.
  zbuff | Input buffer of 4 elements of type cint32
  zstart | Starting position offset applied to all lanes for input from Z buffer. This must be a compile time constant. Only the 4 LSB of the argument are used.
  zoffsets | 4b offset for each lane, applied to input from Z buffer. LSB apply to first lane
  zconj | Selector for conjugation in Z buffer

Note
  - For more information on how data selection works from the buffers go here. The data buffer and coefficient buffer in this intrinsic use the general scheme.
  - Parameter 'zstart' must be a compile time constant.

## ◆ lmul4_min() [1/3]

v4cacc80 lmul4_min | ( | v16int32 | xbuff,
|  | int | xstart,
|  | unsigned int | xoffsets,
|  | int | ystart,
|  | v4cint32 | zbuff,
|  | int | zstart,
|  | unsigned int | zoffsets,
|  | bool | zconj
| ) |  |

Complex multiply intrinsic function with dynamic z buffer conjugation after computing the minimum between the selected lanes from the input buffer using small X input buffer.

acc0 = z00*(min(x00 , y00))
acc1 = z10*(min(x10 , y10))
acc2 = z20*(min(x20 , y20))
acc3 = z30*(min(x30 , y30))

Returns
  Returned accumulation vector (4 x cint80 lanes)

Parameters

  xbuff | Input buffer of 16 elements of type int32
  xstart | Starting position offset applied to all lanes of input from X buffer.
  xoffsets | 4b offset for each lane, applied to both x and y buffers. LSB apply to first lane
  ystart | Starting position offset applied to all lanes for input from Y buffer.
  zbuff | Input buffer of 4 elements of type cint32
  zstart | Starting position offset applied to all lanes for input from Z buffer. This must be a compile time constant. Only the 4 LSB of the argument are used.
  zoffsets | 4b offset for each lane, applied to input from Z buffer. LSB apply to first lane
  zconj | Selector for conjugation in Z buffer

Note
  - For more information on how data selection works from the buffers go here. The data buffer and coefficient buffer in this intrinsic use the general scheme.
  - Parameter 'zstart' must be a compile time constant.

## ◆ lmul4_min() [2/3]

v4cacc80 lmul4_min | ( | v16int32 | xbuff,
|  | int | xstart,
|  | unsigned int | xoffsets,
|  | v16int32 | ybuff,
|  | int | ystart,
|  | v4cint32 | zbuff,
|  | int | zstart,
|  | unsigned int | zoffsets,
|  | bool | zconj
| ) |  |

Complex multiply intrinsic function with dynamic z buffer conjugation after computing the minimum between the selected lanes from the input buffer using small X input buffer.

acc0 = z00*(min(x00 , y00))
acc1 = z10*(min(x10 , y10))
acc2 = z20*(min(x20 , y20))
acc3 = z30*(min(x30 , y30))

Returns
  Returned accumulation vector (4 x cint80 lanes)

Parameters

  xbuff | Input buffer of 16 elements of type int32
  xstart | Starting position offset applied to all lanes of input from X buffer.
  xoffsets | 4b offset for each lane, applied to both x and y buffers. LSB apply to first lane
  ybuff | Right input buffer of 16 elements of type int32
  ystart | Starting position offset applied to all lanes for input from Y buffer.
  zbuff | Input buffer of 4 elements of type cint32
  zstart | Starting position offset applied to all lanes for input from Z buffer. This must be a compile time constant. Only the 4 LSB of the argument are used.
  zoffsets | 4b offset for each lane, applied to input from Z buffer. LSB apply to first lane
  zconj | Selector for conjugation in Z buffer

Note
  - For more information on how data selection works from the buffers go here. The data buffer and coefficient buffer in this intrinsic use the general scheme.
  - Parameter 'zstart' must be a compile time constant.

## ◆ lmul4_min() [3/3]

v4cacc80 lmul4_min | ( | v32int32 | xbuff,
|  | int | xstart,
|  | unsigned int | xoffsets,
|  | int | ystart,
|  | v4cint32 | zbuff,
|  | int | zstart,
|  | unsigned int | zoffsets,
|  | bool | zconj
| ) |  |

Complex multiply intrinsic function with dynamic z buffer conjugation after computing the minimum between the selected lanes from the input buffer .

acc0 = z00*(min(x00 , y00))
acc1 = z10*(min(x10 , y10))
acc2 = z20*(min(x20 , y20))
acc3 = z30*(min(x30 , y30))

Returns
  Returned accumulation vector (4 x cint80 lanes)

Parameters

  xbuff | Input buffer of 32 elements of type int32
  xstart | Starting position offset applied to all lanes of input from X buffer.
  xoffsets | 4b offset for each lane, applied to both x and y buffers. LSB apply to first lane
  ystart | Starting position offset applied to all lanes for input from Y buffer.
  zbuff | Input buffer of 4 elements of type cint32
  zstart | Starting position offset applied to all lanes for input from Z buffer. This must be a compile time constant. Only the 4 LSB of the argument are used.
  zoffsets | 4b offset for each lane, applied to input from Z buffer. LSB apply to first lane
  zconj | Selector for conjugation in Z buffer

Note
  - For more information on how data selection works from the buffers go here. The data buffer and coefficient buffer in this intrinsic use the general scheme.
  - Parameter 'zstart' must be a compile time constant.

## ◆ lnegmul2_abs() [1/2]

v2cacc80 lnegmul2_abs | ( | v16int32 | xbuff,
|  | int | xstart,
|  | unsigned int | xoffsets,
|  | int | xstep,
|  | v4cint32 | zbuff,
|  | int | zstart,
|  | unsigned int | zoffsets,
|  | int | zstep,
|  | bool | zconj
| ) |  |

Complex multiply-negate intrinsic function with dynamic z buffer conjugation after computing the absolute value in the selected lanes from the input buffer using small X input buffer.

acc0 = -( z00*abs(x00) + z01*abs(x01) )
acc1 = -( z10*abs(x10) + z11*abs(x11) )

Returns
  Returned accumulation vector (2 x cint80 lanes)

Parameters

  xbuff | Input buffer of 16 elements of type int32
  xstart | Starting position offset applied to all lanes of input from X buffer.
  xoffsets | 4b offset for each lane, applied to the x buffer. LSB apply to first lane
  xstep | Step between each column for selection in the xbuffer.
  zbuff | Input buffer of 4 elements of type cint32
  zstart | Starting position offset applied to all lanes for input from Z buffer. This must be a compile time constant. Only the 4 LSB of the argument are used.
  zoffsets | 4b offset for each lane, applied to input from Z buffer. LSB apply to first lane
  zstep | Step between each column for selection in the zbuffer.
  zconj | Selector for conjugation in Z buffer

Note
  - For more information on how data selection works from the buffers go here. The data buffer and coefficient buffer in this intrinsic use the general scheme.
  - Parameter 'zstart' must be a compile time constant.

## ◆ lnegmul2_abs() [2/2]

v2cacc80 lnegmul2_abs | ( | v32int32 | xbuff,
|  | int | xstart,
|  | unsigned int | xoffsets,
|  | int | xstep,
|  | v4cint32 | zbuff,
|  | int | zstart,
|  | unsigned int | zoffsets,
|  | int | zstep,
|  | bool | zconj
| ) |  |

Complex multiply-negate intrinsic function with dynamic z buffer conjugation after computing the absolute value in the selected lanes from the input buffer .

acc0 = -( z00*abs(x00) + z01*abs(x01) )
acc1 = -( z10*abs(x10) + z11*abs(x11) )

Returns
  Returned accumulation vector (2 x cint80 lanes)

Parameters

  xbuff | Input buffer of 32 elements of type int32
  xstart | Starting position offset applied to all lanes of input from X buffer.
  xoffsets | 4b offset for each lane, applied to the x buffer. LSB apply to first lane
  xstep | Step between each column for selection in the xbuffer.
  zbuff | Input buffer of 4 elements of type cint32
  zstart | Starting position offset applied to all lanes for input from Z buffer. This must be a compile time constant. Only the 4 LSB of the argument are used.
  zoffsets | 4b offset for each lane, applied to input from Z buffer. LSB apply to first lane
  zstep | Step between each column for selection in the zbuffer.
  zconj | Selector for conjugation in Z buffer

Note
  - For more information on how data selection works from the buffers go here. The data buffer and coefficient buffer in this intrinsic use the general scheme.
  - Parameter 'zstart' must be a compile time constant.

## ◆ lnegmul2_max() [1/3]

v2cacc80 lnegmul2_max | ( | v16int32 | xbuff,
|  | int | xstart,
|  | unsigned int | xoffsets,
|  | int | xstep,
|  | int | ystart,
|  | v4cint32 | zbuff,
|  | int | zstart,
|  | unsigned int | zoffsets,
|  | int | zstep,
|  | bool | zconj
| ) |  |

Complex multiply-negate intrinsic function with dynamic z buffer conjugation after computing the maximum between the selected lanes from the input buffer using small X input buffer.

acc0 = -( z00*(max(x00 , y00)) + z01*(max(x01 , y01)) )
acc1 = -( z10*(max(x10 , y10)) + z11*(max(x11 , y11)) )

Returns
  Returned accumulation vector (2 x cint80 lanes)

Parameters

  xbuff | Input buffer of 16 elements of type int32
  xstart | Starting position offset applied to all lanes of input from X buffer.
  xoffsets | 4b offset for each lane, applied to both x and y buffers. LSB apply to first lane
  xstep | Step between each column for selection in the x and y buffers. Ystep is symmetric to xstep (ystep advances by -xstep).
  ystart | Starting position offset applied to all lanes for input from Y buffer.
  zbuff | Input buffer of 4 elements of type cint32
  zstart | Starting position offset applied to all lanes for input from Z buffer. This must be a compile time constant. Only the 4 LSB of the argument are used.
  zoffsets | 4b offset for each lane, applied to input from Z buffer. LSB apply to first lane
  zstep | Step between each column for selection in the zbuffer.
  zconj | Selector for conjugation in Z buffer

Note
  - For more information on how data selection works from the buffers go here. The data buffer and coefficient buffer in this intrinsic use the general scheme.
  - Parameter 'zstart' must be a compile time constant.

## ◆ lnegmul2_max() [2/3]

v2cacc80 lnegmul2_max | ( | v16int32 | xbuff,
|  | int | xstart,
|  | unsigned int | xoffsets,
|  | int | xstep,
|  | v16int32 | ybuff,
|  | int | ystart,
|  | v4cint32 | zbuff,
|  | int | zstart,
|  | unsigned int | zoffsets,
|  | int | zstep,
|  | bool | zconj
| ) |  |

Complex multiply-negate intrinsic function with dynamic z buffer conjugation after computing the maximum between the selected lanes from the input buffer using small X input buffer.

acc0 = -( z00*(max(x00 , y00)) + z01*(max(x01 , y01)) )
acc1 = -( z10*(max(x10 , y10)) + z11*(max(x11 , y11)) )

Returns
  Returned accumulation vector (2 x cint80 lanes)

Parameters

  xbuff | Input buffer of 16 elements of type int32
  xstart | Starting position offset applied to all lanes of input from X buffer.
  xoffsets | 4b offset for each lane, applied to both x and y buffers. LSB apply to first lane
  xstep | Step between each column for selection in the x and y buffers. Ystep is symmetric to xstep (ystep advances by -xstep).
  ybuff | Right input buffer of 16 elements of type int32
  ystart | Starting position offset applied to all lanes for input from Y buffer.
  zbuff | Input buffer of 4 elements of type cint32
  zstart | Starting position offset applied to all lanes for input from Z buffer. This must be a compile time constant. Only the 4 LSB of the argument are used.
  zoffsets | 4b offset for each lane, applied to input from Z buffer. LSB apply to first lane
  zstep | Step between each column for selection in the zbuffer.
  zconj | Selector for conjugation in Z buffer

Note
  - For more information on how data selection works from the buffers go here. The data buffer and coefficient buffer in this intrinsic use the general scheme.
  - Parameter 'zstart' must be a compile time constant.

## ◆ lnegmul2_max() [3/3]

v2cacc80 lnegmul2_max | ( | v32int32 | xbuff,
|  | int | xstart,
|  | unsigned int | xoffsets,
|  | int | xstep,
|  | int | ystart,
|  | v4cint32 | zbuff,
|  | int | zstart,
|  | unsigned int | zoffsets,
|  | int | zstep,
|  | bool | zconj
| ) |  |

Complex multiply-negate intrinsic function with dynamic z buffer conjugation after computing the maximum between the selected lanes from the input buffer .

acc0 = -( z00*(max(x00 , y00)) + z01*(max(x01 , y01)) )
acc1 = -( z10*(max(x10 , y10)) + z11*(max(x11 , y11)) )

Returns
  Returned accumulation vector (2 x cint80 lanes)

Parameters

  xbuff | Input buffer of 32 elements of type int32
  xstart | Starting position offset applied to all lanes of input from X buffer.
  xoffsets | 4b offset for each lane, applied to both x and y buffers. LSB apply to first lane
  xstep | Step between each column for selection in the x and y buffers. Ystep is symmetric to xstep (ystep advances by -xstep).
  ystart | Starting position offset applied to all lanes for input from Y buffer.
  zbuff | Input buffer of 4 elements of type cint32
  zstart | Starting position offset applied to all lanes for input from Z buffer. This must be a compile time constant. Only the 4 LSB of the argument are used.
  zoffsets | 4b offset for each lane, applied to input from Z buffer. LSB apply to first lane
  zstep | Step between each column for selection in the zbuffer.
  zconj | Selector for conjugation in Z buffer

Note
  - For more information on how data selection works from the buffers go here. The data buffer and coefficient buffer in this intrinsic use the general scheme.
  - Parameter 'zstart' must be a compile time constant.

## ◆ lnegmul2_maxdiff() [1/3]

v2cacc80 lnegmul2_maxdiff | ( | v16int32 | xbuff,
|  | int | xstart,
|  | unsigned int | xoffsets,
|  | int | xstep,
|  | int | ystart,
|  | v4cint32 | zbuff,
|  | int | zstart,
|  | unsigned int | zoffsets,
|  | int | zstep,
|  | bool | zconj
| ) |  |

Complex multiply-negate intrinsic function with dynamic z buffer conjugation after computing the maximum difference between the selected lanes from the input buffer using small X input buffer.

acc0 = -( z00*((x00 - y00 > 0) ? (x00 - y00):0) + z01*((x01 - y01 > 0) ? (x01 - y01):0) )
acc1 = -( z10*((x10 - y10 > 0) ? (x10 - y10):0) + z11*((x11 - y11 > 0) ? (x11 - y11):0) )

Returns
  Returned accumulation vector (2 x cint80 lanes)

Parameters

  xbuff | Input buffer of 16 elements of type int32
  xstart | Starting position offset applied to all lanes of input from X buffer.
  xoffsets | 4b offset for each lane, applied to both x and y buffers. LSB apply to first lane
  xstep | Step between each column for selection in the x and y buffers. Ystep is symmetric to xstep (ystep advances by -xstep).
  ystart | Starting position offset applied to all lanes for input from Y buffer.
  zbuff | Input buffer of 4 elements of type cint32
  zstart | Starting position offset applied to all lanes for input from Z buffer. This must be a compile time constant. Only the 4 LSB of the argument are used.
  zoffsets | 4b offset for each lane, applied to input from Z buffer. LSB apply to first lane
  zstep | Step between each column for selection in the zbuffer.
  zconj | Selector for conjugation in Z buffer

Note
  - For more information on how data selection works from the buffers go here. The data buffer and coefficient buffer in this intrinsic use the general scheme.
  - Parameter 'zstart' must be a compile time constant.

## ◆ lnegmul2_maxdiff() [2/3]

v2cacc80 lnegmul2_maxdiff | ( | v16int32 | xbuff,
|  | int | xstart,
|  | unsigned int | xoffsets,
|  | int | xstep,
|  | v16int32 | ybuff,
|  | int | ystart,
|  | v4cint32 | zbuff,
|  | int | zstart,
|  | unsigned int | zoffsets,
|  | int | zstep,
|  | bool | zconj
| ) |  |

Complex multiply-negate intrinsic function with dynamic z buffer conjugation after computing the maximum difference between the selected lanes from the input buffer using small X input buffer.

acc0 = -( z00*((x00 - y00 > 0) ? (x00 - y00):0) + z01*((x01 - y01 > 0) ? (x01 - y01):0) )
acc1 = -( z10*((x10 - y10 > 0) ? (x10 - y10):0) + z11*((x11 - y11 > 0) ? (x11 - y11):0) )

Returns
  Returned accumulation vector (2 x cint80 lanes)

Parameters

  xbuff | Input buffer of 16 elements of type int32
  xstart | Starting position offset applied to all lanes of input from X buffer.
  xoffsets | 4b offset for each lane, applied to both x and y buffers. LSB apply to first lane
  xstep | Step between each column for selection in the x and y buffers. Ystep is symmetric to xstep (ystep advances by -xstep).
  ybuff | Right input buffer of 16 elements of type int32
  ystart | Starting position offset applied to all lanes for input from Y buffer.
  zbuff | Input buffer of 4 elements of type cint32
  zstart | Starting position offset applied to all lanes for input from Z buffer. This must be a compile time constant. Only the 4 LSB of the argument are used.
  zoffsets | 4b offset for each lane, applied to input from Z buffer. LSB apply to first lane
  zstep | Step between each column for selection in the zbuffer.
  zconj | Selector for conjugation in Z buffer

Note
  - For more information on how data selection works from the buffers go here. The data buffer and coefficient buffer in this intrinsic use the general scheme.
  - Parameter 'zstart' must be a compile time constant.

## ◆ lnegmul2_maxdiff() [3/3]

v2cacc80 lnegmul2_maxdiff | ( | v32int32 | xbuff,
|  | int | xstart,
|  | unsigned int | xoffsets,
|  | int | xstep,
|  | int | ystart,
|  | v4cint32 | zbuff,
|  | int | zstart,
|  | unsigned int | zoffsets,
|  | int | zstep,
|  | bool | zconj
| ) |  |

Complex multiply-negate intrinsic function with dynamic z buffer conjugation after computing the maximum difference between the selected lanes from the input buffer .

acc0 = -( z00*((x00 - y00 > 0) ? (x00 - y00):0) + z01*((x01 - y01 > 0) ? (x01 - y01):0) )
acc1 = -( z10*((x10 - y10 > 0) ? (x10 - y10):0) + z11*((x11 - y11 > 0) ? (x11 - y11):0) )

Returns
  Returned accumulation vector (2 x cint80 lanes)

Parameters

  xbuff | Input buffer of 32 elements of type int32
  xstart | Starting position offset applied to all lanes of input from X buffer.
  xoffsets | 4b offset for each lane, applied to both x and y buffers. LSB apply to first lane
  xstep | Step between each column for selection in the x and y buffers. Ystep is symmetric to xstep (ystep advances by -xstep).
  ystart | Starting position offset applied to all lanes for input from Y buffer.
  zbuff | Input buffer of 4 elements of type cint32
  zstart | Starting position offset applied to all lanes for input from Z buffer. This must be a compile time constant. Only the 4 LSB of the argument are used.
  zoffsets | 4b offset for each lane, applied to input from Z buffer. LSB apply to first lane
  zstep | Step between each column for selection in the zbuffer.
  zconj | Selector for conjugation in Z buffer

Note
  - For more information on how data selection works from the buffers go here. The data buffer and coefficient buffer in this intrinsic use the general scheme.
  - Parameter 'zstart' must be a compile time constant.

## ◆ lnegmul2_min() [1/3]

v2cacc80 lnegmul2_min | ( | v16int32 | xbuff,
|  | int | xstart,
|  | unsigned int | xoffsets,
|  | int | xstep,
|  | int | ystart,
|  | v4cint32 | zbuff,
|  | int | zstart,
|  | unsigned int | zoffsets,
|  | int | zstep,
|  | bool | zconj
| ) |  |

Complex multiply-negate intrinsic function with dynamic z buffer conjugation after computing the minimum between the selected lanes from the input buffer using small X input buffer.

acc0 = -( z00*(min(x00 , y00)) + z01*(min(x01 , y01)) )
acc1 = -( z10*(min(x10 , y10)) + z11*(min(x11 , y11)) )

Returns
  Returned accumulation vector (2 x cint80 lanes)

Parameters

  xbuff | Input buffer of 16 elements of type int32
  xstart | Starting position offset applied to all lanes of input from X buffer.
  xoffsets | 4b offset for each lane, applied to both x and y buffers. LSB apply to first lane
  xstep | Step between each column for selection in the x and y buffers. Ystep is symmetric to xstep (ystep advances by -xstep).
  ystart | Starting position offset applied to all lanes for input from Y buffer.
  zbuff | Input buffer of 4 elements of type cint32
  zstart | Starting position offset applied to all lanes for input from Z buffer. This must be a compile time constant. Only the 4 LSB of the argument are used.
  zoffsets | 4b offset for each lane, applied to input from Z buffer. LSB apply to first lane
  zstep | Step between each column for selection in the zbuffer.
  zconj | Selector for conjugation in Z buffer

Note
  - For more information on how data selection works from the buffers go here. The data buffer and coefficient buffer in this intrinsic use the general scheme.
  - Parameter 'zstart' must be a compile time constant.

## ◆ lnegmul2_min() [2/3]

v2cacc80 lnegmul2_min | ( | v16int32 | xbuff,
|  | int | xstart,
|  | unsigned int | xoffsets,
|  | int | xstep,
|  | v16int32 | ybuff,
|  | int | ystart,
|  | v4cint32 | zbuff,
|  | int | zstart,
|  | unsigned int | zoffsets,
|  | int | zstep,
|  | bool | zconj
| ) |  |

Complex multiply-negate intrinsic function with dynamic z buffer conjugation after computing the minimum between the selected lanes from the input buffer using small X input buffer.

acc0 = -( z00*(min(x00 , y00)) + z01*(min(x01 , y01)) )
acc1 = -( z10*(min(x10 , y10)) + z11*(min(x11 , y11)) )

Returns
  Returned accumulation vector (2 x cint80 lanes)

Parameters

  xbuff | Input buffer of 16 elements of type int32
  xstart | Starting position offset applied to all lanes of input from X buffer.
  xoffsets | 4b offset for each lane, applied to both x and y buffers. LSB apply to first lane
  xstep | Step between each column for selection in the x and y buffers. Ystep is symmetric to xstep (ystep advances by -xstep).
  ybuff | Right input buffer of 16 elements of type int32
  ystart | Starting position offset applied to all lanes for input from Y buffer.
  zbuff | Input buffer of 4 elements of type cint32
  zstart | Starting position offset applied to all lanes for input from Z buffer. This must be a compile time constant. Only the 4 LSB of the argument are used.
  zoffsets | 4b offset for each lane, applied to input from Z buffer. LSB apply to first lane
  zstep | Step between each column for selection in the zbuffer.
  zconj | Selector for conjugation in Z buffer

Note
  - For more information on how data selection works from the buffers go here. The data buffer and coefficient buffer in this intrinsic use the general scheme.
  - Parameter 'zstart' must be a compile time constant.

## ◆ lnegmul2_min() [3/3]

v2cacc80 lnegmul2_min | ( | v32int32 | xbuff,
|  | int | xstart,
|  | unsigned int | xoffsets,
|  | int | xstep,
|  | int | ystart,
|  | v4cint32 | zbuff,
|  | int | zstart,
|  | unsigned int | zoffsets,
|  | int | zstep,
|  | bool | zconj
| ) |  |

Complex multiply-negate intrinsic function with dynamic z buffer conjugation after computing the minimum between the selected lanes from the input buffer .

acc0 = -( z00*(min(x00 , y00)) + z01*(min(x01 , y01)) )
acc1 = -( z10*(min(x10 , y10)) + z11*(min(x11 , y11)) )

Returns
  Returned accumulation vector (2 x cint80 lanes)

Parameters

  xbuff | Input buffer of 32 elements of type int32
  xstart | Starting position offset applied to all lanes of input from X buffer.
  xoffsets | 4b offset for each lane, applied to both x and y buffers. LSB apply to first lane
  xstep | Step between each column for selection in the x and y buffers. Ystep is symmetric to xstep (ystep advances by -xstep).
  ystart | Starting position offset applied to all lanes for input from Y buffer.
  zbuff | Input buffer of 4 elements of type cint32
  zstart | Starting position offset applied to all lanes for input from Z buffer. This must be a compile time constant. Only the 4 LSB of the argument are used.
  zoffsets | 4b offset for each lane, applied to input from Z buffer. LSB apply to first lane
  zstep | Step between each column for selection in the zbuffer.
  zconj | Selector for conjugation in Z buffer

Note
  - For more information on how data selection works from the buffers go here. The data buffer and coefficient buffer in this intrinsic use the general scheme.
  - Parameter 'zstart' must be a compile time constant.

## ◆ lnegmul4_abs() [1/2]

v4cacc80 lnegmul4_abs | ( | v16int32 | xbuff,
|  | int | xstart,
|  | unsigned int | xoffsets,
|  | v4cint32 | zbuff,
|  | int | zstart,
|  | unsigned int | zoffsets,
|  | bool | zconj
| ) |  |

Complex multiply-negate intrinsic function with dynamic z buffer conjugation after computing the absolute value in the selected lanes from the input buffer using small X input buffer.

acc0 = -( z00*abs(x00) )
acc1 = -( z10*abs(x10) )
acc2 = -( z20*abs(x20) )
acc3 = -( z30*abs(x30) )

Returns
  Returned accumulation vector (4 x cint80 lanes)

Parameters

  xbuff | Input buffer of 16 elements of type int32
  xstart | Starting position offset applied to all lanes of input from X buffer.
  xoffsets | 4b offset for each lane, applied to the x buffer. LSB apply to first lane
  zbuff | Input buffer of 4 elements of type cint32
  zstart | Starting position offset applied to all lanes for input from Z buffer. This must be a compile time constant. Only the 4 LSB of the argument are used.
  zoffsets | 4b offset for each lane, applied to input from Z buffer. LSB apply to first lane
  zconj | Selector for conjugation in Z buffer

Note
  - For more information on how data selection works from the buffers go here. The data buffer and coefficient buffer in this intrinsic use the general scheme.
  - Parameter 'zstart' must be a compile time constant.

## ◆ lnegmul4_abs() [2/2]

v4cacc80 lnegmul4_abs | ( | v32int32 | xbuff,
|  | int | xstart,
|  | unsigned int | xoffsets,
|  | v4cint32 | zbuff,
|  | int | zstart,
|  | unsigned int | zoffsets,
|  | bool | zconj
| ) |  |

Complex multiply-negate intrinsic function with dynamic z buffer conjugation after computing the absolute value in the selected lanes from the input buffer .

acc0 = -( z00*abs(x00) )
acc1 = -( z10*abs(x10) )
acc2 = -( z20*abs(x20) )
acc3 = -( z30*abs(x30) )

Returns
  Returned accumulation vector (4 x cint80 lanes)

Parameters

  xbuff | Input buffer of 32 elements of type int32
  xstart | Starting position offset applied to all lanes of input from X buffer.
  xoffsets | 4b offset for each lane, applied to the x buffer. LSB apply to first lane
  zbuff | Input buffer of 4 elements of type cint32
  zstart | Starting position offset applied to all lanes for input from Z buffer. This must be a compile time constant. Only the 4 LSB of the argument are used.
  zoffsets | 4b offset for each lane, applied to input from Z buffer. LSB apply to first lane
  zconj | Selector for conjugation in Z buffer

Note
  - For more information on how data selection works from the buffers go here. The data buffer and coefficient buffer in this intrinsic use the general scheme.
  - Parameter 'zstart' must be a compile time constant.

## ◆ lnegmul4_max() [1/3]

v4cacc80 lnegmul4_max | ( | v16int32 | xbuff,
|  | int | xstart,
|  | unsigned int | xoffsets,
|  | int | ystart,
|  | v4cint32 | zbuff,
|  | int | zstart,
|  | unsigned int | zoffsets,
|  | bool | zconj
| ) |  |

Complex multiply-negate intrinsic function with dynamic z buffer conjugation after computing the maximum between the selected lanes from the input buffer using small X input buffer.

acc0 = -( z00*(max(x00 , y00)) )
acc1 = -( z10*(max(x10 , y10)) )
acc2 = -( z20*(max(x20 , y20)) )
acc3 = -( z30*(max(x30 , y30)) )

Returns
  Returned accumulation vector (4 x cint80 lanes)

Parameters

  xbuff | Input buffer of 16 elements of type int32
  xstart | Starting position offset applied to all lanes of input from X buffer.
  xoffsets | 4b offset for each lane, applied to both x and y buffers. LSB apply to first lane
  ystart | Starting position offset applied to all lanes for input from Y buffer.
  zbuff | Input buffer of 4 elements of type cint32
  zstart | Starting position offset applied to all lanes for input from Z buffer. This must be a compile time constant. Only the 4 LSB of the argument are used.
  zoffsets | 4b offset for each lane, applied to input from Z buffer. LSB apply to first lane
  zconj | Selector for conjugation in Z buffer

Note
  - For more information on how data selection works from the buffers go here. The data buffer and coefficient buffer in this intrinsic use the general scheme.
  - Parameter 'zstart' must be a compile time constant.

## ◆ lnegmul4_max() [2/3]

v4cacc80 lnegmul4_max | ( | v16int32 | xbuff,
|  | int | xstart,
|  | unsigned int | xoffsets,
|  | v16int32 | ybuff,
|  | int | ystart,
|  | v4cint32 | zbuff,
|  | int | zstart,
|  | unsigned int | zoffsets,
|  | bool | zconj
| ) |  |

Complex multiply-negate intrinsic function with dynamic z buffer conjugation after computing the maximum between the selected lanes from the input buffer using small X input buffer.

acc0 = -( z00*(max(x00 , y00)) )
acc1 = -( z10*(max(x10 , y10)) )
acc2 = -( z20*(max(x20 , y20)) )
acc3 = -( z30*(max(x30 , y30)) )

Returns
  Returned accumulation vector (4 x cint80 lanes)

Parameters

  xbuff | Input buffer of 16 elements of type int32
  xstart | Starting position offset applied to all lanes of input from X buffer.
  xoffsets | 4b offset for each lane, applied to both x and y buffers. LSB apply to first lane
  ybuff | Right input buffer of 16 elements of type int32
  ystart | Starting position offset applied to all lanes for input from Y buffer.
  zbuff | Input buffer of 4 elements of type cint32
  zstart | Starting position offset applied to all lanes for input from Z buffer. This must be a compile time constant. Only the 4 LSB of the argument are used.
  zoffsets | 4b offset for each lane, applied to input from Z buffer. LSB apply to first lane
  zconj | Selector for conjugation in Z buffer

Note
  - For more information on how data selection works from the buffers go here. The data buffer and coefficient buffer in this intrinsic use the general scheme.
  - Parameter 'zstart' must be a compile time constant.

## ◆ lnegmul4_max() [3/3]

v4cacc80 lnegmul4_max | ( | v32int32 | xbuff,
|  | int | xstart,
|  | unsigned int | xoffsets,
|  | int | ystart,
|  | v4cint32 | zbuff,
|  | int | zstart,
|  | unsigned int | zoffsets,
|  | bool | zconj
| ) |  |

Complex multiply-negate intrinsic function with dynamic z buffer conjugation after computing the maximum between the selected lanes from the input buffer .

acc0 = -( z00*(max(x00 , y00)) )
acc1 = -( z10*(max(x10 , y10)) )
acc2 = -( z20*(max(x20 , y20)) )
acc3 = -( z30*(max(x30 , y30)) )

Returns
  Returned accumulation vector (4 x cint80 lanes)

Parameters

  xbuff | Input buffer of 32 elements of type int32
  xstart | Starting position offset applied to all lanes of input from X buffer.
  xoffsets | 4b offset for each lane, applied to both x and y buffers. LSB apply to first lane
  ystart | Starting position offset applied to all lanes for input from Y buffer.
  zbuff | Input buffer of 4 elements of type cint32
  zstart | Starting position offset applied to all lanes for input from Z buffer. This must be a compile time constant. Only the 4 LSB of the argument are used.
  zoffsets | 4b offset for each lane, applied to input from Z buffer. LSB apply to first lane
  zconj | Selector for conjugation in Z buffer

Note
  - For more information on how data selection works from the buffers go here. The data buffer and coefficient buffer in this intrinsic use the general scheme.
  - Parameter 'zstart' must be a compile time constant.

## ◆ lnegmul4_maxdiff() [1/3]

v4cacc80 lnegmul4_maxdiff | ( | v16int32 | xbuff,
|  | int | xstart,
|  | unsigned int | xoffsets,
|  | int | ystart,
|  | v4cint32 | zbuff,
|  | int | zstart,
|  | unsigned int | zoffsets,
|  | bool | zconj
| ) |  |

Complex multiply-negate intrinsic function with dynamic z buffer conjugation after computing the maximum difference between the selected lanes from the input buffer using small X input buffer.

acc0 = -( z00*((x00 - y00 > 0) ? (x00 - y00):0) )
acc1 = -( z10*((x10 - y10 > 0) ? (x10 - y10):0) )
acc2 = -( z20*((x20 - y20 > 0) ? (x20 - y20):0) )
acc3 = -( z30*((x30 - y30 > 0) ? (x30 - y30):0) )

Returns
  Returned accumulation vector (4 x cint80 lanes)

Parameters

  xbuff | Input buffer of 16 elements of type int32
  xstart | Starting position offset applied to all lanes of input from X buffer.
  xoffsets | 4b offset for each lane, applied to both x and y buffers. LSB apply to first lane
  ystart | Starting position offset applied to all lanes for input from Y buffer.
  zbuff | Input buffer of 4 elements of type cint32
  zstart | Starting position offset applied to all lanes for input from Z buffer. This must be a compile time constant. Only the 4 LSB of the argument are used.
  zoffsets | 4b offset for each lane, applied to input from Z buffer. LSB apply to first lane
  zconj | Selector for conjugation in Z buffer

Note
  - For more information on how data selection works from the buffers go here. The data buffer and coefficient buffer in this intrinsic use the general scheme.
  - Parameter 'zstart' must be a compile time constant.

## ◆ lnegmul4_maxdiff() [2/3]

v4cacc80 lnegmul4_maxdiff | ( | v16int32 | xbuff,
|  | int | xstart,
|  | unsigned int | xoffsets,
|  | v16int32 | ybuff,
|  | int | ystart,
|  | v4cint32 | zbuff,
|  | int | zstart,
|  | unsigned int | zoffsets,
|  | bool | zconj
| ) |  |

Complex multiply-negate intrinsic function with dynamic z buffer conjugation after computing the maximum difference between the selected lanes from the input buffer using small X input buffer.

acc0 = -( z00*((x00 - y00 > 0) ? (x00 - y00):0) )
acc1 = -( z10*((x10 - y10 > 0) ? (x10 - y10):0) )
acc2 = -( z20*((x20 - y20 > 0) ? (x20 - y20):0) )
acc3 = -( z30*((x30 - y30 > 0) ? (x30 - y30):0) )

Returns
  Returned accumulation vector (4 x cint80 lanes)

Parameters

  xbuff | Input buffer of 16 elements of type int32
  xstart | Starting position offset applied to all lanes of input from X buffer.
  xoffsets | 4b offset for each lane, applied to both x and y buffers. LSB apply to first lane
  ybuff | Right input buffer of 16 elements of type int32
  ystart | Starting position offset applied to all lanes for input from Y buffer.
  zbuff | Input buffer of 4 elements of type cint32
  zstart | Starting position offset applied to all lanes for input from Z buffer. This must be a compile time constant. Only the 4 LSB of the argument are used.
  zoffsets | 4b offset for each lane, applied to input from Z buffer. LSB apply to first lane
  zconj | Selector for conjugation in Z buffer

Note
  - For more information on how data selection works from the buffers go here. The data buffer and coefficient buffer in this intrinsic use the general scheme.
  - Parameter 'zstart' must be a compile time constant.

## ◆ lnegmul4_maxdiff() [3/3]

v4cacc80 lnegmul4_maxdiff | ( | v32int32 | xbuff,
|  | int | xstart,
|  | unsigned int | xoffsets,
|  | int | ystart,
|  | v4cint32 | zbuff,
|  | int | zstart,
|  | unsigned int | zoffsets,
|  | bool | zconj
| ) |  |

Complex multiply-negate intrinsic function with dynamic z buffer conjugation after computing the maximum difference between the selected lanes from the input buffer .

acc0 = -( z00*((x00 - y00 > 0) ? (x00 - y00):0) )
acc1 = -( z10*((x10 - y10 > 0) ? (x10 - y10):0) )
acc2 = -( z20*((x20 - y20 > 0) ? (x20 - y20):0) )
acc3 = -( z30*((x30 - y30 > 0) ? (x30 - y30):0) )

Returns
  Returned accumulation vector (4 x cint80 lanes)

Parameters

  xbuff | Input buffer of 32 elements of type int32
  xstart | Starting position offset applied to all lanes of input from X buffer.
  xoffsets | 4b offset for each lane, applied to both x and y buffers. LSB apply to first lane
  ystart | Starting position offset applied to all lanes for input from Y buffer.
  zbuff | Input buffer of 4 elements of type cint32
  zstart | Starting position offset applied to all lanes for input from Z buffer. This must be a compile time constant. Only the 4 LSB of the argument are used.
  zoffsets | 4b offset for each lane, applied to input from Z buffer. LSB apply to first lane
  zconj | Selector for conjugation in Z buffer

Note
  - For more information on how data selection works from the buffers go here. The data buffer and coefficient buffer in this intrinsic use the general scheme.
  - Parameter 'zstart' must be a compile time constant.

## ◆ lnegmul4_min() [1/3]

v4cacc80 lnegmul4_min | ( | v16int32 | xbuff,
|  | int | xstart,
|  | unsigned int | xoffsets,
|  | int | ystart,
|  | v4cint32 | zbuff,
|  | int | zstart,
|  | unsigned int | zoffsets,
|  | bool | zconj
| ) |  |

Complex multiply-negate intrinsic function with dynamic z buffer conjugation after computing the minimum between the selected lanes from the input buffer using small X input buffer.

acc0 = -( z00*(min(x00 , y00)) )
acc1 = -( z10*(min(x10 , y10)) )
acc2 = -( z20*(min(x20 , y20)) )
acc3 = -( z30*(min(x30 , y30)) )

Returns
  Returned accumulation vector (4 x cint80 lanes)

Parameters

  xbuff | Input buffer of 16 elements of type int32
  xstart | Starting position offset applied to all lanes of input from X buffer.
  xoffsets | 4b offset for each lane, applied to both x and y buffers. LSB apply to first lane
  ystart | Starting position offset applied to all lanes for input from Y buffer.
  zbuff | Input buffer of 4 elements of type cint32
  zstart | Starting position offset applied to all lanes for input from Z buffer. This must be a compile time constant. Only the 4 LSB of the argument are used.
  zoffsets | 4b offset for each lane, applied to input from Z buffer. LSB apply to first lane
  zconj | Selector for conjugation in Z buffer

Note
  - For more information on how data selection works from the buffers go here. The data buffer and coefficient buffer in this intrinsic use the general scheme.
  - Parameter 'zstart' must be a compile time constant.

## ◆ lnegmul4_min() [2/3]

v4cacc80 lnegmul4_min | ( | v16int32 | xbuff,
|  | int | xstart,
|  | unsigned int | xoffsets,
|  | v16int32 | ybuff,
|  | int | ystart,
|  | v4cint32 | zbuff,
|  | int | zstart,
|  | unsigned int | zoffsets,
|  | bool | zconj
| ) |  |

Complex multiply-negate intrinsic function with dynamic z buffer conjugation after computing the minimum between the selected lanes from the input buffer using small X input buffer.

acc0 = -( z00*(min(x00 , y00)) )
acc1 = -( z10*(min(x10 , y10)) )
acc2 = -( z20*(min(x20 , y20)) )
acc3 = -( z30*(min(x30 , y30)) )

Returns
  Returned accumulation vector (4 x cint80 lanes)

Parameters

  xbuff | Input buffer of 16 elements of type int32
  xstart | Starting position offset applied to all lanes of input from X buffer.
  xoffsets | 4b offset for each lane, applied to both x and y buffers. LSB apply to first lane
  ybuff | Right input buffer of 16 elements of type int32
  ystart | Starting position offset applied to all lanes for input from Y buffer.
  zbuff | Input buffer of 4 elements of type cint32
  zstart | Starting position offset applied to all lanes for input from Z buffer. This must be a compile time constant. Only the 4 LSB of the argument are used.
  zoffsets | 4b offset for each lane, applied to input from Z buffer. LSB apply to first lane
  zconj | Selector for conjugation in Z buffer

Note
  - For more information on how data selection works from the buffers go here. The data buffer and coefficient buffer in this intrinsic use the general scheme.
  - Parameter 'zstart' must be a compile time constant.

## ◆ lnegmul4_min() [3/3]

v4cacc80 lnegmul4_min | ( | v32int32 | xbuff,
|  | int | xstart,
|  | unsigned int | xoffsets,
|  | int | ystart,
|  | v4cint32 | zbuff,
|  | int | zstart,
|  | unsigned int | zoffsets,
|  | bool | zconj
| ) |  |

Complex multiply-negate intrinsic function with dynamic z buffer conjugation after computing the minimum between the selected lanes from the input buffer .

acc0 = -( z00*(min(x00 , y00)) )
acc1 = -( z10*(min(x10 , y10)) )
acc2 = -( z20*(min(x20 , y20)) )
acc3 = -( z30*(min(x30 , y30)) )

Returns
  Returned accumulation vector (4 x cint80 lanes)

Parameters

  xbuff | Input buffer of 32 elements of type int32
  xstart | Starting position offset applied to all lanes of input from X buffer.
  xoffsets | 4b offset for each lane, applied to both x and y buffers. LSB apply to first lane
  ystart | Starting position offset applied to all lanes for input from Y buffer.
  zbuff | Input buffer of 4 elements of type cint32
  zstart | Starting position offset applied to all lanes for input from Z buffer. This must be a compile time constant. Only the 4 LSB of the argument are used.
  zoffsets | 4b offset for each lane, applied to input from Z buffer. LSB apply to first lane
  zconj | Selector for conjugation in Z buffer

Note
  - For more information on how data selection works from the buffers go here. The data buffer and coefficient buffer in this intrinsic use the general scheme.
  - Parameter 'zstart' must be a compile time constant.