| AI Engine-ML Intrinsics User Guide (v2025.2)

Loading...
Searching...
No Matches
Multiply-accumulate of 16b x 16b integer datatypes
Vector Operations » Multiply Accumulate

## Overview

Matrix multiplications in which matrix A and matrix B have data elements of 16 bit.

For an explanation how these operations works see Multiply Accumulate.

## Multiplication of (4x2) with (2x8)
v32acc32 | mul_4x2_2x8 (v32uint16 a, v32uint16 b)
v32acc32 | negmul_4x2_2x8 (v32uint16 a, v32uint16 b)
v32acc32 | mac_4x2_2x8 (v32uint16 a, v32uint16 b, v32acc32 acc1)
v32acc32 | msc_4x2_2x8 (v32uint16 a, v32uint16 b, v32acc32 acc1)
v32acc32 | negmac_4x2_2x8 (v32uint16 a, v32uint16 b, v32acc32 acc1)
v32acc32 | negmsc_4x2_2x8 (v32uint16 a, v32uint16 b, v32acc32 acc1)
v32acc32 | addmac_4x2_2x8 (v32uint16 a, v32uint16 b, v32acc32 acc1, v32acc32 acc2)
v32acc32 | addmsc_4x2_2x8 (v32uint16 a, v32uint16 b, v32acc32 acc1, v32acc32 acc2)
v32acc32 | submac_4x2_2x8 (v32uint16 a, v32uint16 b, v32acc32 acc1, v32acc32 acc2)
v32acc32 | submsc_4x2_2x8 (v32uint16 a, v32uint16 b, v32acc32 acc1, v32acc32 acc2)
v32acc32 | mul_4x2_2x8 (v32uint16 a, v32int16 b)
v32acc32 | negmul_4x2_2x8 (v32uint16 a, v32int16 b)
v32acc32 | mac_4x2_2x8 (v32uint16 a, v32int16 b, v32acc32 acc1)
v32acc32 | msc_4x2_2x8 (v32uint16 a, v32int16 b, v32acc32 acc1)
v32acc32 | negmac_4x2_2x8 (v32uint16 a, v32int16 b, v32acc32 acc1)
v32acc32 | negmsc_4x2_2x8 (v32uint16 a, v32int16 b, v32acc32 acc1)
v32acc32 | addmac_4x2_2x8 (v32uint16 a, v32int16 b, v32acc32 acc1, v32acc32 acc2)
v32acc32 | addmsc_4x2_2x8 (v32uint16 a, v32int16 b, v32acc32 acc1, v32acc32 acc2)
v32acc32 | submac_4x2_2x8 (v32uint16 a, v32int16 b, v32acc32 acc1, v32acc32 acc2)
v32acc32 | submsc_4x2_2x8 (v32uint16 a, v32int16 b, v32acc32 acc1, v32acc32 acc2)
v32acc32 | mul_4x2_2x8 (v32int16 a, v32uint16 b)
v32acc32 | negmul_4x2_2x8 (v32int16 a, v32uint16 b)
v32acc32 | mac_4x2_2x8 (v32int16 a, v32uint16 b, v32acc32 acc1)
v32acc32 | msc_4x2_2x8 (v32int16 a, v32uint16 b, v32acc32 acc1)
v32acc32 | negmac_4x2_2x8 (v32int16 a, v32uint16 b, v32acc32 acc1)
v32acc32 | negmsc_4x2_2x8 (v32int16 a, v32uint16 b, v32acc32 acc1)
v32acc32 | addmac_4x2_2x8 (v32int16 a, v32uint16 b, v32acc32 acc1, v32acc32 acc2)
v32acc32 | addmsc_4x2_2x8 (v32int16 a, v32uint16 b, v32acc32 acc1, v32acc32 acc2)
v32acc32 | submac_4x2_2x8 (v32int16 a, v32uint16 b, v32acc32 acc1, v32acc32 acc2)
v32acc32 | submsc_4x2_2x8 (v32int16 a, v32uint16 b, v32acc32 acc1, v32acc32 acc2)
v32acc32 | mul_4x2_2x8 (v32int16 a, v32int16 b)
v32acc32 | negmul_4x2_2x8 (v32int16 a, v32int16 b)
v32acc32 | mac_4x2_2x8 (v32int16 a, v32int16 b, v32acc32 acc1)
v32acc32 | msc_4x2_2x8 (v32int16 a, v32int16 b, v32acc32 acc1)
v32acc32 | negmac_4x2_2x8 (v32int16 a, v32int16 b, v32acc32 acc1)
v32acc32 | negmsc_4x2_2x8 (v32int16 a, v32int16 b, v32acc32 acc1)
v32acc32 | addmac_4x2_2x8 (v32int16 a, v32int16 b, v32acc32 acc1, v32acc32 acc2)
v32acc32 | addmsc_4x2_2x8 (v32int16 a, v32int16 b, v32acc32 acc1, v32acc32 acc2)
v32acc32 | submac_4x2_2x8 (v32int16 a, v32int16 b, v32acc32 acc1, v32acc32 acc2)
v32acc32 | submsc_4x2_2x8 (v32int16 a, v32int16 b, v32acc32 acc1, v32acc32 acc2)

## Multiplication of (4x2) with (2x8) with dynamic sign
v32acc32 | mul_4x2_2x8 (v32uint16 a, int sgn_x, v32uint16 b, int sgn_y)
v32acc32 | negmul_4x2_2x8 (v32uint16 a, int sgn_x, v32uint16 b, int sgn_y)
v32acc32 | mac_4x2_2x8 (v32uint16 a, int sgn_x, v32uint16 b, int sgn_y, v32acc32 acc1)
v32acc32 | msc_4x2_2x8 (v32uint16 a, int sgn_x, v32uint16 b, int sgn_y, v32acc32 acc1)
v32acc32 | negmac_4x2_2x8 (v32uint16 a, int sgn_x, v32uint16 b, int sgn_y, v32acc32 acc1)
v32acc32 | negmsc_4x2_2x8 (v32uint16 a, int sgn_x, v32uint16 b, int sgn_y, v32acc32 acc1)
v32acc32 | addmac_4x2_2x8 (v32uint16 a, int sgn_x, v32uint16 b, int sgn_y, v32acc32 acc1, v32acc32 acc2)
v32acc32 | addmsc_4x2_2x8 (v32uint16 a, int sgn_x, v32uint16 b, int sgn_y, v32acc32 acc1, v32acc32 acc2)
v32acc32 | submac_4x2_2x8 (v32uint16 a, int sgn_x, v32uint16 b, int sgn_y, v32acc32 acc1, v32acc32 acc2)
v32acc32 | submsc_4x2_2x8 (v32uint16 a, int sgn_x, v32uint16 b, int sgn_y, v32acc32 acc1, v32acc32 acc2)
v32acc32 | mul_4x2_2x8 (v32uint16 a, int sgn_x, v32int16 b, int sgn_y)
v32acc32 | negmul_4x2_2x8 (v32uint16 a, int sgn_x, v32int16 b, int sgn_y)
v32acc32 | mac_4x2_2x8 (v32uint16 a, int sgn_x, v32int16 b, int sgn_y, v32acc32 acc1)
v32acc32 | msc_4x2_2x8 (v32uint16 a, int sgn_x, v32int16 b, int sgn_y, v32acc32 acc1)
v32acc32 | negmac_4x2_2x8 (v32uint16 a, int sgn_x, v32int16 b, int sgn_y, v32acc32 acc1)
v32acc32 | negmsc_4x2_2x8 (v32uint16 a, int sgn_x, v32int16 b, int sgn_y, v32acc32 acc1)
v32acc32 | addmac_4x2_2x8 (v32uint16 a, int sgn_x, v32int16 b, int sgn_y, v32acc32 acc1, v32acc32 acc2)
v32acc32 | addmsc_4x2_2x8 (v32uint16 a, int sgn_x, v32int16 b, int sgn_y, v32acc32 acc1, v32acc32 acc2)
v32acc32 | submac_4x2_2x8 (v32uint16 a, int sgn_x, v32int16 b, int sgn_y, v32acc32 acc1, v32acc32 acc2)
v32acc32 | submsc_4x2_2x8 (v32uint16 a, int sgn_x, v32int16 b, int sgn_y, v32acc32 acc1, v32acc32 acc2)
v32acc32 | mul_4x2_2x8 (v32int16 a, int sgn_x, v32uint16 b, int sgn_y)
v32acc32 | negmul_4x2_2x8 (v32int16 a, int sgn_x, v32uint16 b, int sgn_y)
v32acc32 | mac_4x2_2x8 (v32int16 a, int sgn_x, v32uint16 b, int sgn_y, v32acc32 acc1)
v32acc32 | msc_4x2_2x8 (v32int16 a, int sgn_x, v32uint16 b, int sgn_y, v32acc32 acc1)
v32acc32 | negmac_4x2_2x8 (v32int16 a, int sgn_x, v32uint16 b, int sgn_y, v32acc32 acc1)
v32acc32 | negmsc_4x2_2x8 (v32int16 a, int sgn_x, v32uint16 b, int sgn_y, v32acc32 acc1)
v32acc32 | addmac_4x2_2x8 (v32int16 a, int sgn_x, v32uint16 b, int sgn_y, v32acc32 acc1, v32acc32 acc2)
v32acc32 | addmsc_4x2_2x8 (v32int16 a, int sgn_x, v32uint16 b, int sgn_y, v32acc32 acc1, v32acc32 acc2)
v32acc32 | submac_4x2_2x8 (v32int16 a, int sgn_x, v32uint16 b, int sgn_y, v32acc32 acc1, v32acc32 acc2)
v32acc32 | submsc_4x2_2x8 (v32int16 a, int sgn_x, v32uint16 b, int sgn_y, v32acc32 acc1, v32acc32 acc2)
v32acc32 | mul_4x2_2x8 (v32int16 a, int sgn_x, v32int16 b, int sgn_y)
v32acc32 | negmul_4x2_2x8 (v32int16 a, int sgn_x, v32int16 b, int sgn_y)
v32acc32 | mac_4x2_2x8 (v32int16 a, int sgn_x, v32int16 b, int sgn_y, v32acc32 acc1)
v32acc32 | msc_4x2_2x8 (v32int16 a, int sgn_x, v32int16 b, int sgn_y, v32acc32 acc1)
v32acc32 | negmac_4x2_2x8 (v32int16 a, int sgn_x, v32int16 b, int sgn_y, v32acc32 acc1)
v32acc32 | negmsc_4x2_2x8 (v32int16 a, int sgn_x, v32int16 b, int sgn_y, v32acc32 acc1)
v32acc32 | addmac_4x2_2x8 (v32int16 a, int sgn_x, v32int16 b, int sgn_y, v32acc32 acc1, v32acc32 acc2)
v32acc32 | addmsc_4x2_2x8 (v32int16 a, int sgn_x, v32int16 b, int sgn_y, v32acc32 acc1, v32acc32 acc2)
v32acc32 | submac_4x2_2x8 (v32int16 a, int sgn_x, v32int16 b, int sgn_y, v32acc32 acc1, v32acc32 acc2)
v32acc32 | submsc_4x2_2x8 (v32int16 a, int sgn_x, v32int16 b, int sgn_y, v32acc32 acc1, v32acc32 acc2)

## Multiplication of (4x2) with (2x8) with dynamic negation of multiplication result
v32acc32 | mul_4x2_2x8_conf (v32uint16 a, v32uint16 b, int sub_mul)
v32acc32 | negmul_4x2_2x8_conf (v32uint16 a, v32uint16 b, int sub_mul)
v32acc32 | mul_4x2_2x8_conf (v32uint16 a, v32int16 b, int sub_mul)
v32acc32 | negmul_4x2_2x8_conf (v32uint16 a, v32int16 b, int sub_mul)
v32acc32 | mul_4x2_2x8_conf (v32int16 a, v32uint16 b, int sub_mul)
v32acc32 | negmul_4x2_2x8_conf (v32int16 a, v32uint16 b, int sub_mul)
v32acc32 | mul_4x2_2x8_conf (v32int16 a, v32int16 b, int sub_mul)
v32acc32 | negmul_4x2_2x8_conf (v32int16 a, v32int16 b, int sub_mul)

## Multiplication of (4x2) with (2x8) with dynamic negation of multiplication result, zeroing of acc1, and negation of acc1
v32acc32 | mac_4x2_2x8_conf (v32uint16 a, v32uint16 b, v32acc32 acc1, int zero_acc1, int shift16, int sub_mul, int sub_acc1)
v32acc32 | msc_4x2_2x8_conf (v32uint16 a, v32uint16 b, v32acc32 acc1, int zero_acc1, int shift16, int sub_mul, int sub_acc1)
v32acc32 | negmsc_4x2_2x8_conf (v32uint16 a, v32uint16 b, v32acc32 acc1, int zero_acc1, int sub_mul, int sub_acc1)
v32acc32 | negmac_4x2_2x8_conf (v32uint16 a, v32uint16 b, v32acc32 acc1, int zero_acc1, int sub_mul, int sub_acc1)
v32acc32 | addmac_4x2_2x8_conf (v32uint16 a, v32uint16 b, v32acc32 acc1, v32acc32 acc2, int zero_acc1, int shift16, int sub_mul, int sub_acc1, int sub_acc2)
v32acc32 | addmsc_4x2_2x8_conf (v32uint16 a, v32uint16 b, v32acc32 acc1, v32acc32 acc2, int zero_acc1, int shift16, int sub_mul, int sub_acc1, int sub_acc2)
v32acc32 | submac_4x2_2x8_conf (v32uint16 a, v32uint16 b, v32acc32 acc1, v32acc32 acc2, int zero_acc1, int sub_mul, int sub_acc1, int sub_acc2)
v32acc32 | submsc_4x2_2x8_conf (v32uint16 a, v32uint16 b, v32acc32 acc1, v32acc32 acc2, int zero_acc1, int sub_mul, int sub_acc1, int sub_acc2)
v32acc32 | mac_4x2_2x8_conf (v32uint16 a, v32int16 b, v32acc32 acc1, int zero_acc1, int shift16, int sub_mul, int sub_acc1)
v32acc32 | msc_4x2_2x8_conf (v32uint16 a, v32int16 b, v32acc32 acc1, int zero_acc1, int shift16, int sub_mul, int sub_acc1)
v32acc32 | negmsc_4x2_2x8_conf (v32uint16 a, v32int16 b, v32acc32 acc1, int zero_acc1, int sub_mul, int sub_acc1)
v32acc32 | negmac_4x2_2x8_conf (v32uint16 a, v32int16 b, v32acc32 acc1, int zero_acc1, int sub_mul, int sub_acc1)
v32acc32 | addmac_4x2_2x8_conf (v32uint16 a, v32int16 b, v32acc32 acc1, v32acc32 acc2, int zero_acc1, int shift16, int sub_mul, int sub_acc1, int sub_acc2)
v32acc32 | addmsc_4x2_2x8_conf (v32uint16 a, v32int16 b, v32acc32 acc1, v32acc32 acc2, int zero_acc1, int shift16, int sub_mul, int sub_acc1, int sub_acc2)
v32acc32 | submac_4x2_2x8_conf (v32uint16 a, v32int16 b, v32acc32 acc1, v32acc32 acc2, int zero_acc1, int sub_mul, int sub_acc1, int sub_acc2)
v32acc32 | submsc_4x2_2x8_conf (v32uint16 a, v32int16 b, v32acc32 acc1, v32acc32 acc2, int zero_acc1, int sub_mul, int sub_acc1, int sub_acc2)
v32acc32 | mac_4x2_2x8_conf (v32int16 a, v32uint16 b, v32acc32 acc1, int zero_acc1, int shift16, int sub_mul, int sub_acc1)
v32acc32 | msc_4x2_2x8_conf (v32int16 a, v32uint16 b, v32acc32 acc1, int zero_acc1, int shift16, int sub_mul, int sub_acc1)
v32acc32 | negmsc_4x2_2x8_conf (v32int16 a, v32uint16 b, v32acc32 acc1, int zero_acc1, int sub_mul, int sub_acc1)
v32acc32 | negmac_4x2_2x8_conf (v32int16 a, v32uint16 b, v32acc32 acc1, int zero_acc1, int sub_mul, int sub_acc1)
v32acc32 | addmac_4x2_2x8_conf (v32int16 a, v32uint16 b, v32acc32 acc1, v32acc32 acc2, int zero_acc1, int shift16, int sub_mul, int sub_acc1, int sub_acc2)
v32acc32 | addmsc_4x2_2x8_conf (v32int16 a, v32uint16 b, v32acc32 acc1, v32acc32 acc2, int zero_acc1, int shift16, int sub_mul, int sub_acc1, int sub_acc2)
v32acc32 | submac_4x2_2x8_conf (v32int16 a, v32uint16 b, v32acc32 acc1, v32acc32 acc2, int zero_acc1, int sub_mul, int sub_acc1, int sub_acc2)
v32acc32 | submsc_4x2_2x8_conf (v32int16 a, v32uint16 b, v32acc32 acc1, v32acc32 acc2, int zero_acc1, int sub_mul, int sub_acc1, int sub_acc2)
v32acc32 | mac_4x2_2x8_conf (v32int16 a, v32int16 b, v32acc32 acc1, int zero_acc1, int shift16, int sub_mul, int sub_acc1)
v32acc32 | msc_4x2_2x8_conf (v32int16 a, v32int16 b, v32acc32 acc1, int zero_acc1, int shift16, int sub_mul, int sub_acc1)
v32acc32 | negmsc_4x2_2x8_conf (v32int16 a, v32int16 b, v32acc32 acc1, int zero_acc1, int sub_mul, int sub_acc1)
v32acc32 | negmac_4x2_2x8_conf (v32int16 a, v32int16 b, v32acc32 acc1, int zero_acc1, int sub_mul, int sub_acc1)
v32acc32 | addmac_4x2_2x8_conf (v32int16 a, v32int16 b, v32acc32 acc1, v32acc32 acc2, int zero_acc1, int shift16, int sub_mul, int sub_acc1, int sub_acc2)
v32acc32 | addmsc_4x2_2x8_conf (v32int16 a, v32int16 b, v32acc32 acc1, v32acc32 acc2, int zero_acc1, int shift16, int sub_mul, int sub_acc1, int sub_acc2)
v32acc32 | submac_4x2_2x8_conf (v32int16 a, v32int16 b, v32acc32 acc1, v32acc32 acc2, int zero_acc1, int sub_mul, int sub_acc1, int sub_acc2)
v32acc32 | submsc_4x2_2x8_conf (v32int16 a, v32int16 b, v32acc32 acc1, v32acc32 acc2, int zero_acc1, int sub_mul, int sub_acc1, int sub_acc2)

## Multiplication of (4x2) with (2x8) with dynamic sign and dynamic negation of multiplication result
v32acc32 | mul_4x2_2x8_conf (v32uint16 a, int sgn_x, v32uint16 b, int sgn_y, int sub_mul)
v32acc32 | negmul_4x2_2x8_conf (v32uint16 a, int sgn_x, v32uint16 b, int sgn_y, int sub_mul)
v32acc32 | mac_4x2_2x8_conf (v32uint16 a, int sgn_x, v32uint16 b, int sgn_y, v32acc32 acc1, int zero_acc1, int shift16, int sub_mul, int sub_acc1)
v32acc32 | msc_4x2_2x8_conf (v32uint16 a, int sgn_x, v32uint16 b, int sgn_y, v32acc32 acc1, int zero_acc1, int shift16, int sub_mul, int sub_acc1)
v32acc32 | negmsc_4x2_2x8_conf (v32uint16 a, int sgn_x, v32uint16 b, int sgn_y, v32acc32 acc1, int zero_acc1, int sub_mul, int sub_acc1)
v32acc32 | negmac_4x2_2x8_conf (v32uint16 a, int sgn_x, v32uint16 b, int sgn_y, v32acc32 acc1, int zero_acc1, int sub_mul, int sub_acc1)
v32acc32 | addmac_4x2_2x8_conf (v32uint16 a, int sgn_x, v32uint16 b, int sgn_y, v32acc32 acc1, v32acc32 acc2, int zero_acc1, int shift16, int sub_mul, int sub_acc1, int sub_acc2)
v32acc32 | addmsc_4x2_2x8_conf (v32uint16 a, int sgn_x, v32uint16 b, int sgn_y, v32acc32 acc1, v32acc32 acc2, int zero_acc1, int shift16, int sub_mul, int sub_acc1, int sub_acc2)
v32acc32 | submac_4x2_2x8_conf (v32uint16 a, int sgn_x, v32uint16 b, int sgn_y, v32acc32 acc1, v32acc32 acc2, int zero_acc1, int sub_mul, int sub_acc1, int sub_acc2)
v32acc32 | submsc_4x2_2x8_conf (v32uint16 a, int sgn_x, v32uint16 b, int sgn_y, v32acc32 acc1, v32acc32 acc2, int zero_acc1, int sub_mul, int sub_acc1, int sub_acc2)
v32acc32 | mul_4x2_2x8_conf (v32uint16 a, int sgn_x, v32int16 b, int sgn_y, int sub_mul)
v32acc32 | negmul_4x2_2x8_conf (v32uint16 a, int sgn_x, v32int16 b, int sgn_y, int sub_mul)
v32acc32 | mac_4x2_2x8_conf (v32uint16 a, int sgn_x, v32int16 b, int sgn_y, v32acc32 acc1, int zero_acc1, int shift16, int sub_mul, int sub_acc1)
v32acc32 | msc_4x2_2x8_conf (v32uint16 a, int sgn_x, v32int16 b, int sgn_y, v32acc32 acc1, int zero_acc1, int shift16, int sub_mul, int sub_acc1)
v32acc32 | negmsc_4x2_2x8_conf (v32uint16 a, int sgn_x, v32int16 b, int sgn_y, v32acc32 acc1, int zero_acc1, int sub_mul, int sub_acc1)
v32acc32 | negmac_4x2_2x8_conf (v32uint16 a, int sgn_x, v32int16 b, int sgn_y, v32acc32 acc1, int zero_acc1, int sub_mul, int sub_acc1)
v32acc32 | addmac_4x2_2x8_conf (v32uint16 a, int sgn_x, v32int16 b, int sgn_y, v32acc32 acc1, v32acc32 acc2, int zero_acc1, int shift16, int sub_mul, int sub_acc1, int sub_acc2)
v32acc32 | addmsc_4x2_2x8_conf (v32uint16 a, int sgn_x, v32int16 b, int sgn_y, v32acc32 acc1, v32acc32 acc2, int zero_acc1, int shift16, int sub_mul, int sub_acc1, int sub_acc2)
v32acc32 | submac_4x2_2x8_conf (v32uint16 a, int sgn_x, v32int16 b, int sgn_y, v32acc32 acc1, v32acc32 acc2, int zero_acc1, int sub_mul, int sub_acc1, int sub_acc2)
v32acc32 | submsc_4x2_2x8_conf (v32uint16 a, int sgn_x, v32int16 b, int sgn_y, v32acc32 acc1, v32acc32 acc2, int zero_acc1, int sub_mul, int sub_acc1, int sub_acc2)
v32acc32 | mul_4x2_2x8_conf (v32int16 a, int sgn_x, v32uint16 b, int sgn_y, int sub_mul)
v32acc32 | negmul_4x2_2x8_conf (v32int16 a, int sgn_x, v32uint16 b, int sgn_y, int sub_mul)
v32acc32 | mac_4x2_2x8_conf (v32int16 a, int sgn_x, v32uint16 b, int sgn_y, v32acc32 acc1, int zero_acc1, int shift16, int sub_mul, int sub_acc1)
v32acc32 | msc_4x2_2x8_conf (v32int16 a, int sgn_x, v32uint16 b, int sgn_y, v32acc32 acc1, int zero_acc1, int shift16, int sub_mul, int sub_acc1)
v32acc32 | negmsc_4x2_2x8_conf (v32int16 a, int sgn_x, v32uint16 b, int sgn_y, v32acc32 acc1, int zero_acc1, int sub_mul, int sub_acc1)
v32acc32 | negmac_4x2_2x8_conf (v32int16 a, int sgn_x, v32uint16 b, int sgn_y, v32acc32 acc1, int zero_acc1, int sub_mul, int sub_acc1)
v32acc32 | addmac_4x2_2x8_conf (v32int16 a, int sgn_x, v32uint16 b, int sgn_y, v32acc32 acc1, v32acc32 acc2, int zero_acc1, int shift16, int sub_mul, int sub_acc1, int sub_acc2)
v32acc32 | addmsc_4x2_2x8_conf (v32int16 a, int sgn_x, v32uint16 b, int sgn_y, v32acc32 acc1, v32acc32 acc2, int zero_acc1, int shift16, int sub_mul, int sub_acc1, int sub_acc2)
v32acc32 | submac_4x2_2x8_conf (v32int16 a, int sgn_x, v32uint16 b, int sgn_y, v32acc32 acc1, v32acc32 acc2, int zero_acc1, int sub_mul, int sub_acc1, int sub_acc2)
v32acc32 | submsc_4x2_2x8_conf (v32int16 a, int sgn_x, v32uint16 b, int sgn_y, v32acc32 acc1, v32acc32 acc2, int zero_acc1, int sub_mul, int sub_acc1, int sub_acc2)
v32acc32 | mul_4x2_2x8_conf (v32int16 a, int sgn_x, v32int16 b, int sgn_y, int sub_mul)
v32acc32 | negmul_4x2_2x8_conf (v32int16 a, int sgn_x, v32int16 b, int sgn_y, int sub_mul)
v32acc32 | mac_4x2_2x8_conf (v32int16 a, int sgn_x, v32int16 b, int sgn_y, v32acc32 acc1, int zero_acc1, int shift16, int sub_mul, int sub_acc1)
v32acc32 | msc_4x2_2x8_conf (v32int16 a, int sgn_x, v32int16 b, int sgn_y, v32acc32 acc1, int zero_acc1, int shift16, int sub_mul, int sub_acc1)
v32acc32 | negmsc_4x2_2x8_conf (v32int16 a, int sgn_x, v32int16 b, int sgn_y, v32acc32 acc1, int zero_acc1, int sub_mul, int sub_acc1)
v32acc32 | negmac_4x2_2x8_conf (v32int16 a, int sgn_x, v32int16 b, int sgn_y, v32acc32 acc1, int zero_acc1, int sub_mul, int sub_acc1)
v32acc32 | addmac_4x2_2x8_conf (v32int16 a, int sgn_x, v32int16 b, int sgn_y, v32acc32 acc1, v32acc32 acc2, int zero_acc1, int shift16, int sub_mul, int sub_acc1, int sub_acc2)
v32acc32 | addmsc_4x2_2x8_conf (v32int16 a, int sgn_x, v32int16 b, int sgn_y, v32acc32 acc1, v32acc32 acc2, int zero_acc1, int shift16, int sub_mul, int sub_acc1, int sub_acc2)
v32acc32 | submac_4x2_2x8_conf (v32int16 a, int sgn_x, v32int16 b, int sgn_y, v32acc32 acc1, v32acc32 acc2, int zero_acc1, int sub_mul, int sub_acc1, int sub_acc2)
v32acc32 | submsc_4x2_2x8_conf (v32int16 a, int sgn_x, v32int16 b, int sgn_y, v32acc32 acc1, v32acc32 acc2, int zero_acc1, int sub_mul, int sub_acc1, int sub_acc2)

## Channel by channel multiplication of (1x1) with (1x1)
v32acc32 | mul_elem_32 (v32uint16 a, v32uint16 b)
v32acc32 | negmul_elem_32 (v32uint16 a, v32uint16 b)
v32acc32 | mac_elem_32 (v32uint16 a, v32uint16 b, v32acc32 acc1)
v32acc32 | msc_elem_32 (v32uint16 a, v32uint16 b, v32acc32 acc1)
v32acc32 | negmac_elem_32 (v32uint16 a, v32uint16 b, v32acc32 acc1)
v32acc32 | negmsc_elem_32 (v32uint16 a, v32uint16 b, v32acc32 acc1)
v32acc32 | addmac_elem_32 (v32uint16 a, v32uint16 b, v32acc32 acc1, v32acc32 acc2)
v32acc32 | addmsc_elem_32 (v32uint16 a, v32uint16 b, v32acc32 acc1, v32acc32 acc2)
v32acc32 | submac_elem_32 (v32uint16 a, v32uint16 b, v32acc32 acc1, v32acc32 acc2)
v32acc32 | submsc_elem_32 (v32uint16 a, v32uint16 b, v32acc32 acc1, v32acc32 acc2)
v32acc32 | mul_elem_32 (v32uint16 a, v32int16 b)
v32acc32 | negmul_elem_32 (v32uint16 a, v32int16 b)
v32acc32 | mac_elem_32 (v32uint16 a, v32int16 b, v32acc32 acc1)
v32acc32 | msc_elem_32 (v32uint16 a, v32int16 b, v32acc32 acc1)
v32acc32 | negmac_elem_32 (v32uint16 a, v32int16 b, v32acc32 acc1)
v32acc32 | negmsc_elem_32 (v32uint16 a, v32int16 b, v32acc32 acc1)
v32acc32 | addmac_elem_32 (v32uint16 a, v32int16 b, v32acc32 acc1, v32acc32 acc2)
v32acc32 | addmsc_elem_32 (v32uint16 a, v32int16 b, v32acc32 acc1, v32acc32 acc2)
v32acc32 | submac_elem_32 (v32uint16 a, v32int16 b, v32acc32 acc1, v32acc32 acc2)
v32acc32 | submsc_elem_32 (v32uint16 a, v32int16 b, v32acc32 acc1, v32acc32 acc2)
v32acc32 | mul_elem_32 (v32int16 a, v32uint16 b)
v32acc32 | negmul_elem_32 (v32int16 a, v32uint16 b)
v32acc32 | mac_elem_32 (v32int16 a, v32uint16 b, v32acc32 acc1)
v32acc32 | msc_elem_32 (v32int16 a, v32uint16 b, v32acc32 acc1)
v32acc32 | negmac_elem_32 (v32int16 a, v32uint16 b, v32acc32 acc1)
v32acc32 | negmsc_elem_32 (v32int16 a, v32uint16 b, v32acc32 acc1)
v32acc32 | addmac_elem_32 (v32int16 a, v32uint16 b, v32acc32 acc1, v32acc32 acc2)
v32acc32 | addmsc_elem_32 (v32int16 a, v32uint16 b, v32acc32 acc1, v32acc32 acc2)
v32acc32 | submac_elem_32 (v32int16 a, v32uint16 b, v32acc32 acc1, v32acc32 acc2)
v32acc32 | submsc_elem_32 (v32int16 a, v32uint16 b, v32acc32 acc1, v32acc32 acc2)
v32acc32 | mul_elem_32 (v32int16 a, v32int16 b)
v32acc32 | negmul_elem_32 (v32int16 a, v32int16 b)
v32acc32 | mac_elem_32 (v32int16 a, v32int16 b, v32acc32 acc1)
v32acc32 | msc_elem_32 (v32int16 a, v32int16 b, v32acc32 acc1)
v32acc32 | negmac_elem_32 (v32int16 a, v32int16 b, v32acc32 acc1)
v32acc32 | negmsc_elem_32 (v32int16 a, v32int16 b, v32acc32 acc1)
v32acc32 | addmac_elem_32 (v32int16 a, v32int16 b, v32acc32 acc1, v32acc32 acc2)
v32acc32 | addmsc_elem_32 (v32int16 a, v32int16 b, v32acc32 acc1, v32acc32 acc2)
v32acc32 | submac_elem_32 (v32int16 a, v32int16 b, v32acc32 acc1, v32acc32 acc2)
v32acc32 | submsc_elem_32 (v32int16 a, v32int16 b, v32acc32 acc1, v32acc32 acc2)

## Channel by channel multiplication of (1x1) with (1x1) with dynamic sign
v32acc32 | mul_elem_32 (v32uint16 a, int sgn_x, v32uint16 b, int sgn_y)
v32acc32 | negmul_elem_32 (v32uint16 a, int sgn_x, v32uint16 b, int sgn_y)
v32acc32 | mac_elem_32 (v32uint16 a, int sgn_x, v32uint16 b, int sgn_y, v32acc32 acc1)
v32acc32 | msc_elem_32 (v32uint16 a, int sgn_x, v32uint16 b, int sgn_y, v32acc32 acc1)
v32acc32 | negmac_elem_32 (v32uint16 a, int sgn_x, v32uint16 b, int sgn_y, v32acc32 acc1)
v32acc32 | negmsc_elem_32 (v32uint16 a, int sgn_x, v32uint16 b, int sgn_y, v32acc32 acc1)
v32acc32 | addmac_elem_32 (v32uint16 a, int sgn_x, v32uint16 b, int sgn_y, v32acc32 acc1, v32acc32 acc2)
v32acc32 | addmsc_elem_32 (v32uint16 a, int sgn_x, v32uint16 b, int sgn_y, v32acc32 acc1, v32acc32 acc2)
v32acc32 | submac_elem_32 (v32uint16 a, int sgn_x, v32uint16 b, int sgn_y, v32acc32 acc1, v32acc32 acc2)
v32acc32 | submsc_elem_32 (v32uint16 a, int sgn_x, v32uint16 b, int sgn_y, v32acc32 acc1, v32acc32 acc2)
v32acc32 | mul_elem_32 (v32uint16 a, int sgn_x, v32int16 b, int sgn_y)
v32acc32 | negmul_elem_32 (v32uint16 a, int sgn_x, v32int16 b, int sgn_y)
v32acc32 | mac_elem_32 (v32uint16 a, int sgn_x, v32int16 b, int sgn_y, v32acc32 acc1)
v32acc32 | msc_elem_32 (v32uint16 a, int sgn_x, v32int16 b, int sgn_y, v32acc32 acc1)
v32acc32 | negmac_elem_32 (v32uint16 a, int sgn_x, v32int16 b, int sgn_y, v32acc32 acc1)
v32acc32 | negmsc_elem_32 (v32uint16 a, int sgn_x, v32int16 b, int sgn_y, v32acc32 acc1)
v32acc32 | addmac_elem_32 (v32uint16 a, int sgn_x, v32int16 b, int sgn_y, v32acc32 acc1, v32acc32 acc2)
v32acc32 | addmsc_elem_32 (v32uint16 a, int sgn_x, v32int16 b, int sgn_y, v32acc32 acc1, v32acc32 acc2)
v32acc32 | submac_elem_32 (v32uint16 a, int sgn_x, v32int16 b, int sgn_y, v32acc32 acc1, v32acc32 acc2)
v32acc32 | submsc_elem_32 (v32uint16 a, int sgn_x, v32int16 b, int sgn_y, v32acc32 acc1, v32acc32 acc2)
v32acc32 | mul_elem_32 (v32int16 a, int sgn_x, v32uint16 b, int sgn_y)
v32acc32 | negmul_elem_32 (v32int16 a, int sgn_x, v32uint16 b, int sgn_y)
v32acc32 | mac_elem_32 (v32int16 a, int sgn_x, v32uint16 b, int sgn_y, v32acc32 acc1)
v32acc32 | msc_elem_32 (v32int16 a, int sgn_x, v32uint16 b, int sgn_y, v32acc32 acc1)
v32acc32 | negmac_elem_32 (v32int16 a, int sgn_x, v32uint16 b, int sgn_y, v32acc32 acc1)
v32acc32 | negmsc_elem_32 (v32int16 a, int sgn_x, v32uint16 b, int sgn_y, v32acc32 acc1)
v32acc32 | addmac_elem_32 (v32int16 a, int sgn_x, v32uint16 b, int sgn_y, v32acc32 acc1, v32acc32 acc2)
v32acc32 | addmsc_elem_32 (v32int16 a, int sgn_x, v32uint16 b, int sgn_y, v32acc32 acc1, v32acc32 acc2)
v32acc32 | submac_elem_32 (v32int16 a, int sgn_x, v32uint16 b, int sgn_y, v32acc32 acc1, v32acc32 acc2)
v32acc32 | submsc_elem_32 (v32int16 a, int sgn_x, v32uint16 b, int sgn_y, v32acc32 acc1, v32acc32 acc2)
v32acc32 | mul_elem_32 (v32int16 a, int sgn_x, v32int16 b, int sgn_y)
v32acc32 | negmul_elem_32 (v32int16 a, int sgn_x, v32int16 b, int sgn_y)
v32acc32 | mac_elem_32 (v32int16 a, int sgn_x, v32int16 b, int sgn_y, v32acc32 acc1)
v32acc32 | msc_elem_32 (v32int16 a, int sgn_x, v32int16 b, int sgn_y, v32acc32 acc1)
v32acc32 | negmac_elem_32 (v32int16 a, int sgn_x, v32int16 b, int sgn_y, v32acc32 acc1)
v32acc32 | negmsc_elem_32 (v32int16 a, int sgn_x, v32int16 b, int sgn_y, v32acc32 acc1)
v32acc32 | addmac_elem_32 (v32int16 a, int sgn_x, v32int16 b, int sgn_y, v32acc32 acc1, v32acc32 acc2)
v32acc32 | addmsc_elem_32 (v32int16 a, int sgn_x, v32int16 b, int sgn_y, v32acc32 acc1, v32acc32 acc2)
v32acc32 | submac_elem_32 (v32int16 a, int sgn_x, v32int16 b, int sgn_y, v32acc32 acc1, v32acc32 acc2)
v32acc32 | submsc_elem_32 (v32int16 a, int sgn_x, v32int16 b, int sgn_y, v32acc32 acc1, v32acc32 acc2)

## Channel by channel multiplication of (1x1) with (1x1) with dynamic negation of multiplication result
v32acc32 | mul_elem_32_conf (v32uint16 a, v32uint16 b, int sub_mul)
v32acc32 | negmul_elem_32_conf (v32uint16 a, v32uint16 b, int sub_mul)
v32acc32 | mul_elem_32_conf (v32uint16 a, v32int16 b, int sub_mul)
v32acc32 | negmul_elem_32_conf (v32uint16 a, v32int16 b, int sub_mul)
v32acc32 | mul_elem_32_conf (v32int16 a, v32uint16 b, int sub_mul)
v32acc32 | negmul_elem_32_conf (v32int16 a, v32uint16 b, int sub_mul)
v32acc32 | mul_elem_32_conf (v32int16 a, v32int16 b, int sub_mul)
v32acc32 | negmul_elem_32_conf (v32int16 a, v32int16 b, int sub_mul)

## Channel by channel multiplication of (1x1) with (1x1) with dynamic negation of multiplication result, zeroing of acc1, and negation of acc1
v32acc32 | mac_elem_32_conf (v32uint16 a, v32uint16 b, v32acc32 acc1, int zero_acc1, int shift16, int sub_mul, int sub_acc1)
v32acc32 | msc_elem_32_conf (v32uint16 a, v32uint16 b, v32acc32 acc1, int zero_acc1, int shift16, int sub_mul, int sub_acc1)
v32acc32 | negmsc_elem_32_conf (v32uint16 a, v32uint16 b, v32acc32 acc1, int zero_acc1, int sub_mul, int sub_acc1)
v32acc32 | negmac_elem_32_conf (v32uint16 a, v32uint16 b, v32acc32 acc1, int zero_acc1, int sub_mul, int sub_acc1)
v32acc32 | addmac_elem_32_conf (v32uint16 a, v32uint16 b, v32acc32 acc1, v32acc32 acc2, int zero_acc1, int shift16, int sub_mul, int sub_acc1, int sub_acc2)
v32acc32 | addmsc_elem_32_conf (v32uint16 a, v32uint16 b, v32acc32 acc1, v32acc32 acc2, int zero_acc1, int shift16, int sub_mul, int sub_acc1, int sub_acc2)
v32acc32 | submac_elem_32_conf (v32uint16 a, v32uint16 b, v32acc32 acc1, v32acc32 acc2, int zero_acc1, int sub_mul, int sub_acc1, int sub_acc2)
v32acc32 | submsc_elem_32_conf (v32uint16 a, v32uint16 b, v32acc32 acc1, v32acc32 acc2, int zero_acc1, int sub_mul, int sub_acc1, int sub_acc2)
v32acc32 | mac_elem_32_conf (v32uint16 a, v32int16 b, v32acc32 acc1, int zero_acc1, int shift16, int sub_mul, int sub_acc1)
v32acc32 | msc_elem_32_conf (v32uint16 a, v32int16 b, v32acc32 acc1, int zero_acc1, int shift16, int sub_mul, int sub_acc1)
v32acc32 | negmsc_elem_32_conf (v32uint16 a, v32int16 b, v32acc32 acc1, int zero_acc1, int sub_mul, int sub_acc1)
v32acc32 | negmac_elem_32_conf (v32uint16 a, v32int16 b, v32acc32 acc1, int zero_acc1, int sub_mul, int sub_acc1)
v32acc32 | addmac_elem_32_conf (v32uint16 a, v32int16 b, v32acc32 acc1, v32acc32 acc2, int zero_acc1, int shift16, int sub_mul, int sub_acc1, int sub_acc2)
v32acc32 | addmsc_elem_32_conf (v32uint16 a, v32int16 b, v32acc32 acc1, v32acc32 acc2, int zero_acc1, int shift16, int sub_mul, int sub_acc1, int sub_acc2)
v32acc32 | submac_elem_32_conf (v32uint16 a, v32int16 b, v32acc32 acc1, v32acc32 acc2, int zero_acc1, int sub_mul, int sub_acc1, int sub_acc2)
v32acc32 | submsc_elem_32_conf (v32uint16 a, v32int16 b, v32acc32 acc1, v32acc32 acc2, int zero_acc1, int sub_mul, int sub_acc1, int sub_acc2)
v32acc32 | mac_elem_32_conf (v32int16 a, v32uint16 b, v32acc32 acc1, int zero_acc1, int shift16, int sub_mul, int sub_acc1)
v32acc32 | msc_elem_32_conf (v32int16 a, v32uint16 b, v32acc32 acc1, int zero_acc1, int shift16, int sub_mul, int sub_acc1)
v32acc32 | negmsc_elem_32_conf (v32int16 a, v32uint16 b, v32acc32 acc1, int zero_acc1, int sub_mul, int sub_acc1)
v32acc32 | negmac_elem_32_conf (v32int16 a, v32uint16 b, v32acc32 acc1, int zero_acc1, int sub_mul, int sub_acc1)
v32acc32 | addmac_elem_32_conf (v32int16 a, v32uint16 b, v32acc32 acc1, v32acc32 acc2, int zero_acc1, int shift16, int sub_mul, int sub_acc1, int sub_acc2)
v32acc32 | addmsc_elem_32_conf (v32int16 a, v32uint16 b, v32acc32 acc1, v32acc32 acc2, int zero_acc1, int shift16, int sub_mul, int sub_acc1, int sub_acc2)
v32acc32 | submac_elem_32_conf (v32int16 a, v32uint16 b, v32acc32 acc1, v32acc32 acc2, int zero_acc1, int sub_mul, int sub_acc1, int sub_acc2)
v32acc32 | submsc_elem_32_conf (v32int16 a, v32uint16 b, v32acc32 acc1, v32acc32 acc2, int zero_acc1, int sub_mul, int sub_acc1, int sub_acc2)
v32acc32 | mac_elem_32_conf (v32int16 a, v32int16 b, v32acc32 acc1, int zero_acc1, int shift16, int sub_mul, int sub_acc1)
v32acc32 | msc_elem_32_conf (v32int16 a, v32int16 b, v32acc32 acc1, int zero_acc1, int shift16, int sub_mul, int sub_acc1)
v32acc32 | negmsc_elem_32_conf (v32int16 a, v32int16 b, v32acc32 acc1, int zero_acc1, int sub_mul, int sub_acc1)
v32acc32 | negmac_elem_32_conf (v32int16 a, v32int16 b, v32acc32 acc1, int zero_acc1, int sub_mul, int sub_acc1)
v32acc32 | addmac_elem_32_conf (v32int16 a, v32int16 b, v32acc32 acc1, v32acc32 acc2, int zero_acc1, int shift16, int sub_mul, int sub_acc1, int sub_acc2)
v32acc32 | addmsc_elem_32_conf (v32int16 a, v32int16 b, v32acc32 acc1, v32acc32 acc2, int zero_acc1, int shift16, int sub_mul, int sub_acc1, int sub_acc2)
v32acc32 | submac_elem_32_conf (v32int16 a, v32int16 b, v32acc32 acc1, v32acc32 acc2, int zero_acc1, int sub_mul, int sub_acc1, int sub_acc2)
v32acc32 | submsc_elem_32_conf (v32int16 a, v32int16 b, v32acc32 acc1, v32acc32 acc2, int zero_acc1, int sub_mul, int sub_acc1, int sub_acc2)

## Channel by channel multiplication of (1x1) with (1x1) with dynamic sign and dynamic negation of multiplication result
v32acc32 | mul_elem_32_conf (v32uint16 a, int sgn_x, v32uint16 b, int sgn_y, int sub_mul)
v32acc32 | negmul_elem_32_conf (v32uint16 a, int sgn_x, v32uint16 b, int sgn_y, int sub_mul)
v32acc32 | mac_elem_32_conf (v32uint16 a, int sgn_x, v32uint16 b, int sgn_y, v32acc32 acc1, int zero_acc1, int shift16, int sub_mul, int sub_acc1)
v32acc32 | msc_elem_32_conf (v32uint16 a, int sgn_x, v32uint16 b, int sgn_y, v32acc32 acc1, int zero_acc1, int shift16, int sub_mul, int sub_acc1)
v32acc32 | negmsc_elem_32_conf (v32uint16 a, int sgn_x, v32uint16 b, int sgn_y, v32acc32 acc1, int zero_acc1, int sub_mul, int sub_acc1)
v32acc32 | negmac_elem_32_conf (v32uint16 a, int sgn_x, v32uint16 b, int sgn_y, v32acc32 acc1, int zero_acc1, int sub_mul, int sub_acc1)
v32acc32 | addmac_elem_32_conf (v32uint16 a, int sgn_x, v32uint16 b, int sgn_y, v32acc32 acc1, v32acc32 acc2, int zero_acc1, int shift16, int sub_mul, int sub_acc1, int sub_acc2)
v32acc32 | addmsc_elem_32_conf (v32uint16 a, int sgn_x, v32uint16 b, int sgn_y, v32acc32 acc1, v32acc32 acc2, int zero_acc1, int shift16, int sub_mul, int sub_acc1, int sub_acc2)
v32acc32 | submac_elem_32_conf (v32uint16 a, int sgn_x, v32uint16 b, int sgn_y, v32acc32 acc1, v32acc32 acc2, int zero_acc1, int sub_mul, int sub_acc1, int sub_acc2)
v32acc32 | submsc_elem_32_conf (v32uint16 a, int sgn_x, v32uint16 b, int sgn_y, v32acc32 acc1, v32acc32 acc2, int zero_acc1, int sub_mul, int sub_acc1, int sub_acc2)
v32acc32 | mul_elem_32_conf (v32uint16 a, int sgn_x, v32int16 b, int sgn_y, int sub_mul)
v32acc32 | negmul_elem_32_conf (v32uint16 a, int sgn_x, v32int16 b, int sgn_y, int sub_mul)
v32acc32 | mac_elem_32_conf (v32uint16 a, int sgn_x, v32int16 b, int sgn_y, v32acc32 acc1, int zero_acc1, int shift16, int sub_mul, int sub_acc1)
v32acc32 | msc_elem_32_conf (v32uint16 a, int sgn_x, v32int16 b, int sgn_y, v32acc32 acc1, int zero_acc1, int shift16, int sub_mul, int sub_acc1)
v32acc32 | negmsc_elem_32_conf (v32uint16 a, int sgn_x, v32int16 b, int sgn_y, v32acc32 acc1, int zero_acc1, int sub_mul, int sub_acc1)
v32acc32 | negmac_elem_32_conf (v32uint16 a, int sgn_x, v32int16 b, int sgn_y, v32acc32 acc1, int zero_acc1, int sub_mul, int sub_acc1)
v32acc32 | addmac_elem_32_conf (v32uint16 a, int sgn_x, v32int16 b, int sgn_y, v32acc32 acc1, v32acc32 acc2, int zero_acc1, int shift16, int sub_mul, int sub_acc1, int sub_acc2)
v32acc32 | addmsc_elem_32_conf (v32uint16 a, int sgn_x, v32int16 b, int sgn_y, v32acc32 acc1, v32acc32 acc2, int zero_acc1, int shift16, int sub_mul, int sub_acc1, int sub_acc2)
v32acc32 | submac_elem_32_conf (v32uint16 a, int sgn_x, v32int16 b, int sgn_y, v32acc32 acc1, v32acc32 acc2, int zero_acc1, int sub_mul, int sub_acc1, int sub_acc2)
v32acc32 | submsc_elem_32_conf (v32uint16 a, int sgn_x, v32int16 b, int sgn_y, v32acc32 acc1, v32acc32 acc2, int zero_acc1, int sub_mul, int sub_acc1, int sub_acc2)
v32acc32 | mul_elem_32_conf (v32int16 a, int sgn_x, v32uint16 b, int sgn_y, int sub_mul)
v32acc32 | negmul_elem_32_conf (v32int16 a, int sgn_x, v32uint16 b, int sgn_y, int sub_mul)
v32acc32 | mac_elem_32_conf (v32int16 a, int sgn_x, v32uint16 b, int sgn_y, v32acc32 acc1, int zero_acc1, int shift16, int sub_mul, int sub_acc1)
v32acc32 | msc_elem_32_conf (v32int16 a, int sgn_x, v32uint16 b, int sgn_y, v32acc32 acc1, int zero_acc1, int shift16, int sub_mul, int sub_acc1)
v32acc32 | negmsc_elem_32_conf (v32int16 a, int sgn_x, v32uint16 b, int sgn_y, v32acc32 acc1, int zero_acc1, int sub_mul, int sub_acc1)
v32acc32 | negmac_elem_32_conf (v32int16 a, int sgn_x, v32uint16 b, int sgn_y, v32acc32 acc1, int zero_acc1, int sub_mul, int sub_acc1)
v32acc32 | addmac_elem_32_conf (v32int16 a, int sgn_x, v32uint16 b, int sgn_y, v32acc32 acc1, v32acc32 acc2, int zero_acc1, int shift16, int sub_mul, int sub_acc1, int sub_acc2)
v32acc32 | addmsc_elem_32_conf (v32int16 a, int sgn_x, v32uint16 b, int sgn_y, v32acc32 acc1, v32acc32 acc2, int zero_acc1, int shift16, int sub_mul, int sub_acc1, int sub_acc2)
v32acc32 | submac_elem_32_conf (v32int16 a, int sgn_x, v32uint16 b, int sgn_y, v32acc32 acc1, v32acc32 acc2, int zero_acc1, int sub_mul, int sub_acc1, int sub_acc2)
v32acc32 | submsc_elem_32_conf (v32int16 a, int sgn_x, v32uint16 b, int sgn_y, v32acc32 acc1, v32acc32 acc2, int zero_acc1, int sub_mul, int sub_acc1, int sub_acc2)
v32acc32 | mul_elem_32_conf (v32int16 a, int sgn_x, v32int16 b, int sgn_y, int sub_mul)
v32acc32 | negmul_elem_32_conf (v32int16 a, int sgn_x, v32int16 b, int sgn_y, int sub_mul)
v32acc32 | mac_elem_32_conf (v32int16 a, int sgn_x, v32int16 b, int sgn_y, v32acc32 acc1, int zero_acc1, int shift16, int sub_mul, int sub_acc1)
v32acc32 | msc_elem_32_conf (v32int16 a, int sgn_x, v32int16 b, int sgn_y, v32acc32 acc1, int zero_acc1, int shift16, int sub_mul, int sub_acc1)
v32acc32 | negmsc_elem_32_conf (v32int16 a, int sgn_x, v32int16 b, int sgn_y, v32acc32 acc1, int zero_acc1, int sub_mul, int sub_acc1)
v32acc32 | negmac_elem_32_conf (v32int16 a, int sgn_x, v32int16 b, int sgn_y, v32acc32 acc1, int zero_acc1, int sub_mul, int sub_acc1)
v32acc32 | addmac_elem_32_conf (v32int16 a, int sgn_x, v32int16 b, int sgn_y, v32acc32 acc1, v32acc32 acc2, int zero_acc1, int shift16, int sub_mul, int sub_acc1, int sub_acc2)
v32acc32 | addmsc_elem_32_conf (v32int16 a, int sgn_x, v32int16 b, int sgn_y, v32acc32 acc1, v32acc32 acc2, int zero_acc1, int shift16, int sub_mul, int sub_acc1, int sub_acc2)
v32acc32 | submac_elem_32_conf (v32int16 a, int sgn_x, v32int16 b, int sgn_y, v32acc32 acc1, v32acc32 acc2, int zero_acc1, int sub_mul, int sub_acc1, int sub_acc2)
v32acc32 | submsc_elem_32_conf (v32int16 a, int sgn_x, v32int16 b, int sgn_y, v32acc32 acc1, v32acc32 acc2, int zero_acc1, int sub_mul, int sub_acc1, int sub_acc2)

## Multiplication of (2x4) with (4x8)
v16acc64 | mul_2x4_4x8 (v32uint16 a, v32uint16 b)
v16acc64 | negmul_2x4_4x8 (v32uint16 a, v32uint16 b)
v16acc64 | mac_2x4_4x8 (v32uint16 a, v32uint16 b, v16acc64 acc1)
v16acc64 | msc_2x4_4x8 (v32uint16 a, v32uint16 b, v16acc64 acc1)
v16acc64 | negmac_2x4_4x8 (v32uint16 a, v32uint16 b, v16acc64 acc1)
v16acc64 | negmsc_2x4_4x8 (v32uint16 a, v32uint16 b, v16acc64 acc1)
v16acc64 | addmac_2x4_4x8 (v32uint16 a, v32uint16 b, v16acc64 acc1, v16acc64 acc2)
v16acc64 | addmsc_2x4_4x8 (v32uint16 a, v32uint16 b, v16acc64 acc1, v16acc64 acc2)
v16acc64 | submac_2x4_4x8 (v32uint16 a, v32uint16 b, v16acc64 acc1, v16acc64 acc2)
v16acc64 | submsc_2x4_4x8 (v32uint16 a, v32uint16 b, v16acc64 acc1, v16acc64 acc2)
v16acc64 | mul_2x4_4x8 (v32uint16 a, v32int16 b)
v16acc64 | negmul_2x4_4x8 (v32uint16 a, v32int16 b)
v16acc64 | mac_2x4_4x8 (v32uint16 a, v32int16 b, v16acc64 acc1)
v16acc64 | msc_2x4_4x8 (v32uint16 a, v32int16 b, v16acc64 acc1)
v16acc64 | negmac_2x4_4x8 (v32uint16 a, v32int16 b, v16acc64 acc1)
v16acc64 | negmsc_2x4_4x8 (v32uint16 a, v32int16 b, v16acc64 acc1)
v16acc64 | addmac_2x4_4x8 (v32uint16 a, v32int16 b, v16acc64 acc1, v16acc64 acc2)
v16acc64 | addmsc_2x4_4x8 (v32uint16 a, v32int16 b, v16acc64 acc1, v16acc64 acc2)
v16acc64 | submac_2x4_4x8 (v32uint16 a, v32int16 b, v16acc64 acc1, v16acc64 acc2)
v16acc64 | submsc_2x4_4x8 (v32uint16 a, v32int16 b, v16acc64 acc1, v16acc64 acc2)
v16acc64 | mul_2x4_4x8 (v32int16 a, v32uint16 b)
v16acc64 | negmul_2x4_4x8 (v32int16 a, v32uint16 b)
v16acc64 | mac_2x4_4x8 (v32int16 a, v32uint16 b, v16acc64 acc1)
v16acc64 | msc_2x4_4x8 (v32int16 a, v32uint16 b, v16acc64 acc1)
v16acc64 | negmac_2x4_4x8 (v32int16 a, v32uint16 b, v16acc64 acc1)
v16acc64 | negmsc_2x4_4x8 (v32int16 a, v32uint16 b, v16acc64 acc1)
v16acc64 | addmac_2x4_4x8 (v32int16 a, v32uint16 b, v16acc64 acc1, v16acc64 acc2)
v16acc64 | addmsc_2x4_4x8 (v32int16 a, v32uint16 b, v16acc64 acc1, v16acc64 acc2)
v16acc64 | submac_2x4_4x8 (v32int16 a, v32uint16 b, v16acc64 acc1, v16acc64 acc2)
v16acc64 | submsc_2x4_4x8 (v32int16 a, v32uint16 b, v16acc64 acc1, v16acc64 acc2)
v16acc64 | mul_2x4_4x8 (v32int16 a, v32int16 b)
v16acc64 | negmul_2x4_4x8 (v32int16 a, v32int16 b)
v16acc64 | mac_2x4_4x8 (v32int16 a, v32int16 b, v16acc64 acc1)
v16acc64 | msc_2x4_4x8 (v32int16 a, v32int16 b, v16acc64 acc1)
v16acc64 | negmac_2x4_4x8 (v32int16 a, v32int16 b, v16acc64 acc1)
v16acc64 | negmsc_2x4_4x8 (v32int16 a, v32int16 b, v16acc64 acc1)
v16acc64 | addmac_2x4_4x8 (v32int16 a, v32int16 b, v16acc64 acc1, v16acc64 acc2)
v16acc64 | addmsc_2x4_4x8 (v32int16 a, v32int16 b, v16acc64 acc1, v16acc64 acc2)
v16acc64 | submac_2x4_4x8 (v32int16 a, v32int16 b, v16acc64 acc1, v16acc64 acc2)
v16acc64 | submsc_2x4_4x8 (v32int16 a, v32int16 b, v16acc64 acc1, v16acc64 acc2)

## Multiplication of (2x4) with (4x8) with dynamic sign
v16acc64 | mul_2x4_4x8 (v32uint16 a, int sgn_x, v32uint16 b, int sgn_y)
v16acc64 | negmul_2x4_4x8 (v32uint16 a, int sgn_x, v32uint16 b, int sgn_y)
v16acc64 | mac_2x4_4x8 (v32uint16 a, int sgn_x, v32uint16 b, int sgn_y, v16acc64 acc1)
v16acc64 | msc_2x4_4x8 (v32uint16 a, int sgn_x, v32uint16 b, int sgn_y, v16acc64 acc1)
v16acc64 | negmac_2x4_4x8 (v32uint16 a, int sgn_x, v32uint16 b, int sgn_y, v16acc64 acc1)
v16acc64 | negmsc_2x4_4x8 (v32uint16 a, int sgn_x, v32uint16 b, int sgn_y, v16acc64 acc1)
v16acc64 | addmac_2x4_4x8 (v32uint16 a, int sgn_x, v32uint16 b, int sgn_y, v16acc64 acc1, v16acc64 acc2)
v16acc64 | addmsc_2x4_4x8 (v32uint16 a, int sgn_x, v32uint16 b, int sgn_y, v16acc64 acc1, v16acc64 acc2)
v16acc64 | submac_2x4_4x8 (v32uint16 a, int sgn_x, v32uint16 b, int sgn_y, v16acc64 acc1, v16acc64 acc2)
v16acc64 | submsc_2x4_4x8 (v32uint16 a, int sgn_x, v32uint16 b, int sgn_y, v16acc64 acc1, v16acc64 acc2)
v16acc64 | mul_2x4_4x8 (v32uint16 a, int sgn_x, v32int16 b, int sgn_y)
v16acc64 | negmul_2x4_4x8 (v32uint16 a, int sgn_x, v32int16 b, int sgn_y)
v16acc64 | mac_2x4_4x8 (v32uint16 a, int sgn_x, v32int16 b, int sgn_y, v16acc64 acc1)
v16acc64 | msc_2x4_4x8 (v32uint16 a, int sgn_x, v32int16 b, int sgn_y, v16acc64 acc1)
v16acc64 | negmac_2x4_4x8 (v32uint16 a, int sgn_x, v32int16 b, int sgn_y, v16acc64 acc1)
v16acc64 | negmsc_2x4_4x8 (v32uint16 a, int sgn_x, v32int16 b, int sgn_y, v16acc64 acc1)
v16acc64 | addmac_2x4_4x8 (v32uint16 a, int sgn_x, v32int16 b, int sgn_y, v16acc64 acc1, v16acc64 acc2)
v16acc64 | addmsc_2x4_4x8 (v32uint16 a, int sgn_x, v32int16 b, int sgn_y, v16acc64 acc1, v16acc64 acc2)
v16acc64 | submac_2x4_4x8 (v32uint16 a, int sgn_x, v32int16 b, int sgn_y, v16acc64 acc1, v16acc64 acc2)
v16acc64 | submsc_2x4_4x8 (v32uint16 a, int sgn_x, v32int16 b, int sgn_y, v16acc64 acc1, v16acc64 acc2)
v16acc64 | mul_2x4_4x8 (v32int16 a, int sgn_x, v32uint16 b, int sgn_y)
v16acc64 | negmul_2x4_4x8 (v32int16 a, int sgn_x, v32uint16 b, int sgn_y)
v16acc64 | mac_2x4_4x8 (v32int16 a, int sgn_x, v32uint16 b, int sgn_y, v16acc64 acc1)
v16acc64 | msc_2x4_4x8 (v32int16 a, int sgn_x, v32uint16 b, int sgn_y, v16acc64 acc1)
v16acc64 | negmac_2x4_4x8 (v32int16 a, int sgn_x, v32uint16 b, int sgn_y, v16acc64 acc1)
v16acc64 | negmsc_2x4_4x8 (v32int16 a, int sgn_x, v32uint16 b, int sgn_y, v16acc64 acc1)
v16acc64 | addmac_2x4_4x8 (v32int16 a, int sgn_x, v32uint16 b, int sgn_y, v16acc64 acc1, v16acc64 acc2)
v16acc64 | addmsc_2x4_4x8 (v32int16 a, int sgn_x, v32uint16 b, int sgn_y, v16acc64 acc1, v16acc64 acc2)
v16acc64 | submac_2x4_4x8 (v32int16 a, int sgn_x, v32uint16 b, int sgn_y, v16acc64 acc1, v16acc64 acc2)
v16acc64 | submsc_2x4_4x8 (v32int16 a, int sgn_x, v32uint16 b, int sgn_y, v16acc64 acc1, v16acc64 acc2)
v16acc64 | mul_2x4_4x8 (v32int16 a, int sgn_x, v32int16 b, int sgn_y)
v16acc64 | negmul_2x4_4x8 (v32int16 a, int sgn_x, v32int16 b, int sgn_y)
v16acc64 | mac_2x4_4x8 (v32int16 a, int sgn_x, v32int16 b, int sgn_y, v16acc64 acc1)
v16acc64 | msc_2x4_4x8 (v32int16 a, int sgn_x, v32int16 b, int sgn_y, v16acc64 acc1)
v16acc64 | negmac_2x4_4x8 (v32int16 a, int sgn_x, v32int16 b, int sgn_y, v16acc64 acc1)
v16acc64 | negmsc_2x4_4x8 (v32int16 a, int sgn_x, v32int16 b, int sgn_y, v16acc64 acc1)
v16acc64 | addmac_2x4_4x8 (v32int16 a, int sgn_x, v32int16 b, int sgn_y, v16acc64 acc1, v16acc64 acc2)
v16acc64 | addmsc_2x4_4x8 (v32int16 a, int sgn_x, v32int16 b, int sgn_y, v16acc64 acc1, v16acc64 acc2)
v16acc64 | submac_2x4_4x8 (v32int16 a, int sgn_x, v32int16 b, int sgn_y, v16acc64 acc1, v16acc64 acc2)
v16acc64 | submsc_2x4_4x8 (v32int16 a, int sgn_x, v32int16 b, int sgn_y, v16acc64 acc1, v16acc64 acc2)

## Multiplication of (2x4) with (4x8) with dynamic negation of multiplication result
v16acc64 | mul_2x4_4x8_conf (v32uint16 a, v32uint16 b, int sub_mul)
v16acc64 | negmul_2x4_4x8_conf (v32uint16 a, v32uint16 b, int sub_mul)
v16acc64 | mul_2x4_4x8_conf (v32uint16 a, v32int16 b, int sub_mul)
v16acc64 | negmul_2x4_4x8_conf (v32uint16 a, v32int16 b, int sub_mul)
v16acc64 | mul_2x4_4x8_conf (v32int16 a, v32uint16 b, int sub_mul)
v16acc64 | negmul_2x4_4x8_conf (v32int16 a, v32uint16 b, int sub_mul)
v16acc64 | mul_2x4_4x8_conf (v32int16 a, v32int16 b, int sub_mul)
v16acc64 | negmul_2x4_4x8_conf (v32int16 a, v32int16 b, int sub_mul)

## Multiplication of (2x4) with (4x8) with dynamic negation of multiplication result, zeroing of acc1, and negation of acc1
v16acc64 | mac_2x4_4x8_conf (v32uint16 a, v32uint16 b, v16acc64 acc1, int zero_acc1, int shift16, int sub_mul, int sub_acc1)
v16acc64 | msc_2x4_4x8_conf (v32uint16 a, v32uint16 b, v16acc64 acc1, int zero_acc1, int shift16, int sub_mul, int sub_acc1)
v16acc64 | negmsc_2x4_4x8_conf (v32uint16 a, v32uint16 b, v16acc64 acc1, int zero_acc1, int sub_mul, int sub_acc1)
v16acc64 | negmac_2x4_4x8_conf (v32uint16 a, v32uint16 b, v16acc64 acc1, int zero_acc1, int sub_mul, int sub_acc1)
v16acc64 | addmac_2x4_4x8_conf (v32uint16 a, v32uint16 b, v16acc64 acc1, v16acc64 acc2, int zero_acc1, int shift16, int sub_mul, int sub_acc1, int sub_acc2)
v16acc64 | addmsc_2x4_4x8_conf (v32uint16 a, v32uint16 b, v16acc64 acc1, v16acc64 acc2, int zero_acc1, int shift16, int sub_mul, int sub_acc1, int sub_acc2)
v16acc64 | submac_2x4_4x8_conf (v32uint16 a, v32uint16 b, v16acc64 acc1, v16acc64 acc2, int zero_acc1, int sub_mul, int sub_acc1, int sub_acc2)
v16acc64 | submsc_2x4_4x8_conf (v32uint16 a, v32uint16 b, v16acc64 acc1, v16acc64 acc2, int zero_acc1, int sub_mul, int sub_acc1, int sub_acc2)
v16acc64 | mac_2x4_4x8_conf (v32uint16 a, v32int16 b, v16acc64 acc1, int zero_acc1, int shift16, int sub_mul, int sub_acc1)
v16acc64 | msc_2x4_4x8_conf (v32uint16 a, v32int16 b, v16acc64 acc1, int zero_acc1, int shift16, int sub_mul, int sub_acc1)
v16acc64 | negmsc_2x4_4x8_conf (v32uint16 a, v32int16 b, v16acc64 acc1, int zero_acc1, int sub_mul, int sub_acc1)
v16acc64 | negmac_2x4_4x8_conf (v32uint16 a, v32int16 b, v16acc64 acc1, int zero_acc1, int sub_mul, int sub_acc1)
v16acc64 | addmac_2x4_4x8_conf (v32uint16 a, v32int16 b, v16acc64 acc1, v16acc64 acc2, int zero_acc1, int shift16, int sub_mul, int sub_acc1, int sub_acc2)
v16acc64 | addmsc_2x4_4x8_conf (v32uint16 a, v32int16 b, v16acc64 acc1, v16acc64 acc2, int zero_acc1, int shift16, int sub_mul, int sub_acc1, int sub_acc2)
v16acc64 | submac_2x4_4x8_conf (v32uint16 a, v32int16 b, v16acc64 acc1, v16acc64 acc2, int zero_acc1, int sub_mul, int sub_acc1, int sub_acc2)
v16acc64 | submsc_2x4_4x8_conf (v32uint16 a, v32int16 b, v16acc64 acc1, v16acc64 acc2, int zero_acc1, int sub_mul, int sub_acc1, int sub_acc2)
v16acc64 | mac_2x4_4x8_conf (v32int16 a, v32uint16 b, v16acc64 acc1, int zero_acc1, int shift16, int sub_mul, int sub_acc1)
v16acc64 | msc_2x4_4x8_conf (v32int16 a, v32uint16 b, v16acc64 acc1, int zero_acc1, int shift16, int sub_mul, int sub_acc1)
v16acc64 | negmsc_2x4_4x8_conf (v32int16 a, v32uint16 b, v16acc64 acc1, int zero_acc1, int sub_mul, int sub_acc1)
v16acc64 | negmac_2x4_4x8_conf (v32int16 a, v32uint16 b, v16acc64 acc1, int zero_acc1, int sub_mul, int sub_acc1)
v16acc64 | addmac_2x4_4x8_conf (v32int16 a, v32uint16 b, v16acc64 acc1, v16acc64 acc2, int zero_acc1, int shift16, int sub_mul, int sub_acc1, int sub_acc2)
v16acc64 | addmsc_2x4_4x8_conf (v32int16 a, v32uint16 b, v16acc64 acc1, v16acc64 acc2, int zero_acc1, int shift16, int sub_mul, int sub_acc1, int sub_acc2)
v16acc64 | submac_2x4_4x8_conf (v32int16 a, v32uint16 b, v16acc64 acc1, v16acc64 acc2, int zero_acc1, int sub_mul, int sub_acc1, int sub_acc2)
v16acc64 | submsc_2x4_4x8_conf (v32int16 a, v32uint16 b, v16acc64 acc1, v16acc64 acc2, int zero_acc1, int sub_mul, int sub_acc1, int sub_acc2)
v16acc64 | mac_2x4_4x8_conf (v32int16 a, v32int16 b, v16acc64 acc1, int zero_acc1, int shift16, int sub_mul, int sub_acc1)
v16acc64 | msc_2x4_4x8_conf (v32int16 a, v32int16 b, v16acc64 acc1, int zero_acc1, int shift16, int sub_mul, int sub_acc1)
v16acc64 | negmsc_2x4_4x8_conf (v32int16 a, v32int16 b, v16acc64 acc1, int zero_acc1, int sub_mul, int sub_acc1)
v16acc64 | negmac_2x4_4x8_conf (v32int16 a, v32int16 b, v16acc64 acc1, int zero_acc1, int sub_mul, int sub_acc1)
v16acc64 | addmac_2x4_4x8_conf (v32int16 a, v32int16 b, v16acc64 acc1, v16acc64 acc2, int zero_acc1, int shift16, int sub_mul, int sub_acc1, int sub_acc2)
v16acc64 | addmsc_2x4_4x8_conf (v32int16 a, v32int16 b, v16acc64 acc1, v16acc64 acc2, int zero_acc1, int shift16, int sub_mul, int sub_acc1, int sub_acc2)
v16acc64 | submac_2x4_4x8_conf (v32int16 a, v32int16 b, v16acc64 acc1, v16acc64 acc2, int zero_acc1, int sub_mul, int sub_acc1, int sub_acc2)
v16acc64 | submsc_2x4_4x8_conf (v32int16 a, v32int16 b, v16acc64 acc1, v16acc64 acc2, int zero_acc1, int sub_mul, int sub_acc1, int sub_acc2)

## Multiplication of (2x4) with (4x8) with dynamic sign and dynamic negation of multiplication result
v16acc64 | mul_2x4_4x8_conf (v32uint16 a, int sgn_x, v32uint16 b, int sgn_y, int sub_mul)
v16acc64 | negmul_2x4_4x8_conf (v32uint16 a, int sgn_x, v32uint16 b, int sgn_y, int sub_mul)
v16acc64 | mac_2x4_4x8_conf (v32uint16 a, int sgn_x, v32uint16 b, int sgn_y, v16acc64 acc1, int zero_acc1, int shift16, int sub_mul, int sub_acc1)
v16acc64 | msc_2x4_4x8_conf (v32uint16 a, int sgn_x, v32uint16 b, int sgn_y, v16acc64 acc1, int zero_acc1, int shift16, int sub_mul, int sub_acc1)
v16acc64 | negmsc_2x4_4x8_conf (v32uint16 a, int sgn_x, v32uint16 b, int sgn_y, v16acc64 acc1, int zero_acc1, int sub_mul, int sub_acc1)
v16acc64 | negmac_2x4_4x8_conf (v32uint16 a, int sgn_x, v32uint16 b, int sgn_y, v16acc64 acc1, int zero_acc1, int sub_mul, int sub_acc1)
v16acc64 | addmac_2x4_4x8_conf (v32uint16 a, int sgn_x, v32uint16 b, int sgn_y, v16acc64 acc1, v16acc64 acc2, int zero_acc1, int shift16, int sub_mul, int sub_acc1, int sub_acc2)
v16acc64 | addmsc_2x4_4x8_conf (v32uint16 a, int sgn_x, v32uint16 b, int sgn_y, v16acc64 acc1, v16acc64 acc2, int zero_acc1, int shift16, int sub_mul, int sub_acc1, int sub_acc2)
v16acc64 | submac_2x4_4x8_conf (v32uint16 a, int sgn_x, v32uint16 b, int sgn_y, v16acc64 acc1, v16acc64 acc2, int zero_acc1, int sub_mul, int sub_acc1, int sub_acc2)
v16acc64 | submsc_2x4_4x8_conf (v32uint16 a, int sgn_x, v32uint16 b, int sgn_y, v16acc64 acc1, v16acc64 acc2, int zero_acc1, int sub_mul, int sub_acc1, int sub_acc2)
v16acc64 | mul_2x4_4x8_conf (v32uint16 a, int sgn_x, v32int16 b, int sgn_y, int sub_mul)
v16acc64 | negmul_2x4_4x8_conf (v32uint16 a, int sgn_x, v32int16 b, int sgn_y, int sub_mul)
v16acc64 | mac_2x4_4x8_conf (v32uint16 a, int sgn_x, v32int16 b, int sgn_y, v16acc64 acc1, int zero_acc1, int shift16, int sub_mul, int sub_acc1)
v16acc64 | msc_2x4_4x8_conf (v32uint16 a, int sgn_x, v32int16 b, int sgn_y, v16acc64 acc1, int zero_acc1, int shift16, int sub_mul, int sub_acc1)
v16acc64 | negmsc_2x4_4x8_conf (v32uint16 a, int sgn_x, v32int16 b, int sgn_y, v16acc64 acc1, int zero_acc1, int sub_mul, int sub_acc1)
v16acc64 | negmac_2x4_4x8_conf (v32uint16 a, int sgn_x, v32int16 b, int sgn_y, v16acc64 acc1, int zero_acc1, int sub_mul, int sub_acc1)
v16acc64 | addmac_2x4_4x8_conf (v32uint16 a, int sgn_x, v32int16 b, int sgn_y, v16acc64 acc1, v16acc64 acc2, int zero_acc1, int shift16, int sub_mul, int sub_acc1, int sub_acc2)
v16acc64 | addmsc_2x4_4x8_conf (v32uint16 a, int sgn_x, v32int16 b, int sgn_y, v16acc64 acc1, v16acc64 acc2, int zero_acc1, int shift16, int sub_mul, int sub_acc1, int sub_acc2)
v16acc64 | submac_2x4_4x8_conf (v32uint16 a, int sgn_x, v32int16 b, int sgn_y, v16acc64 acc1, v16acc64 acc2, int zero_acc1, int sub_mul, int sub_acc1, int sub_acc2)
v16acc64 | submsc_2x4_4x8_conf (v32uint16 a, int sgn_x, v32int16 b, int sgn_y, v16acc64 acc1, v16acc64 acc2, int zero_acc1, int sub_mul, int sub_acc1, int sub_acc2)
v16acc64 | mul_2x4_4x8_conf (v32int16 a, int sgn_x, v32uint16 b, int sgn_y, int sub_mul)
v16acc64 | negmul_2x4_4x8_conf (v32int16 a, int sgn_x, v32uint16 b, int sgn_y, int sub_mul)
v16acc64 | mac_2x4_4x8_conf (v32int16 a, int sgn_x, v32uint16 b, int sgn_y, v16acc64 acc1, int zero_acc1, int shift16, int sub_mul, int sub_acc1)
v16acc64 | msc_2x4_4x8_conf (v32int16 a, int sgn_x, v32uint16 b, int sgn_y, v16acc64 acc1, int zero_acc1, int shift16, int sub_mul, int sub_acc1)
v16acc64 | negmsc_2x4_4x8_conf (v32int16 a, int sgn_x, v32uint16 b, int sgn_y, v16acc64 acc1, int zero_acc1, int sub_mul, int sub_acc1)
v16acc64 | negmac_2x4_4x8_conf (v32int16 a, int sgn_x, v32uint16 b, int sgn_y, v16acc64 acc1, int zero_acc1, int sub_mul, int sub_acc1)
v16acc64 | addmac_2x4_4x8_conf (v32int16 a, int sgn_x, v32uint16 b, int sgn_y, v16acc64 acc1, v16acc64 acc2, int zero_acc1, int shift16, int sub_mul, int sub_acc1, int sub_acc2)
v16acc64 | addmsc_2x4_4x8_conf (v32int16 a, int sgn_x, v32uint16 b, int sgn_y, v16acc64 acc1, v16acc64 acc2, int zero_acc1, int shift16, int sub_mul, int sub_acc1, int sub_acc2)
v16acc64 | submac_2x4_4x8_conf (v32int16 a, int sgn_x, v32uint16 b, int sgn_y, v16acc64 acc1, v16acc64 acc2, int zero_acc1, int sub_mul, int sub_acc1, int sub_acc2)
v16acc64 | submsc_2x4_4x8_conf (v32int16 a, int sgn_x, v32uint16 b, int sgn_y, v16acc64 acc1, v16acc64 acc2, int zero_acc1, int sub_mul, int sub_acc1, int sub_acc2)
v16acc64 | mul_2x4_4x8_conf (v32int16 a, int sgn_x, v32int16 b, int sgn_y, int sub_mul)
v16acc64 | negmul_2x4_4x8_conf (v32int16 a, int sgn_x, v32int16 b, int sgn_y, int sub_mul)
v16acc64 | mac_2x4_4x8_conf (v32int16 a, int sgn_x, v32int16 b, int sgn_y, v16acc64 acc1, int zero_acc1, int shift16, int sub_mul, int sub_acc1)
v16acc64 | msc_2x4_4x8_conf (v32int16 a, int sgn_x, v32int16 b, int sgn_y, v16acc64 acc1, int zero_acc1, int shift16, int sub_mul, int sub_acc1)
v16acc64 | negmsc_2x4_4x8_conf (v32int16 a, int sgn_x, v32int16 b, int sgn_y, v16acc64 acc1, int zero_acc1, int sub_mul, int sub_acc1)
v16acc64 | negmac_2x4_4x8_conf (v32int16 a, int sgn_x, v32int16 b, int sgn_y, v16acc64 acc1, int zero_acc1, int sub_mul, int sub_acc1)
v16acc64 | addmac_2x4_4x8_conf (v32int16 a, int sgn_x, v32int16 b, int sgn_y, v16acc64 acc1, v16acc64 acc2, int zero_acc1, int shift16, int sub_mul, int sub_acc1, int sub_acc2)
v16acc64 | addmsc_2x4_4x8_conf (v32int16 a, int sgn_x, v32int16 b, int sgn_y, v16acc64 acc1, v16acc64 acc2, int zero_acc1, int shift16, int sub_mul, int sub_acc1, int sub_acc2)
v16acc64 | submac_2x4_4x8_conf (v32int16 a, int sgn_x, v32int16 b, int sgn_y, v16acc64 acc1, v16acc64 acc2, int zero_acc1, int sub_mul, int sub_acc1, int sub_acc2)
v16acc64 | submsc_2x4_4x8_conf (v32int16 a, int sgn_x, v32int16 b, int sgn_y, v16acc64 acc1, v16acc64 acc2, int zero_acc1, int sub_mul, int sub_acc1, int sub_acc2)

## Multiplication of (4x4) with (4x4)
v16acc64 | mul_4x4_4x4 (v32uint16 a, v32uint16 b)
v16acc64 | negmul_4x4_4x4 (v32uint16 a, v32uint16 b)
v16acc64 | mac_4x4_4x4 (v32uint16 a, v32uint16 b, v16acc64 acc1)
v16acc64 | msc_4x4_4x4 (v32uint16 a, v32uint16 b, v16acc64 acc1)
v16acc64 | negmac_4x4_4x4 (v32uint16 a, v32uint16 b, v16acc64 acc1)
v16acc64 | negmsc_4x4_4x4 (v32uint16 a, v32uint16 b, v16acc64 acc1)
v16acc64 | addmac_4x4_4x4 (v32uint16 a, v32uint16 b, v16acc64 acc1, v16acc64 acc2)
v16acc64 | addmsc_4x4_4x4 (v32uint16 a, v32uint16 b, v16acc64 acc1, v16acc64 acc2)
v16acc64 | submac_4x4_4x4 (v32uint16 a, v32uint16 b, v16acc64 acc1, v16acc64 acc2)
v16acc64 | submsc_4x4_4x4 (v32uint16 a, v32uint16 b, v16acc64 acc1, v16acc64 acc2)
v16acc64 | mul_4x4_4x4 (v32uint16 a, v32int16 b)
v16acc64 | negmul_4x4_4x4 (v32uint16 a, v32int16 b)
v16acc64 | mac_4x4_4x4 (v32uint16 a, v32int16 b, v16acc64 acc1)
v16acc64 | msc_4x4_4x4 (v32uint16 a, v32int16 b, v16acc64 acc1)
v16acc64 | negmac_4x4_4x4 (v32uint16 a, v32int16 b, v16acc64 acc1)
v16acc64 | negmsc_4x4_4x4 (v32uint16 a, v32int16 b, v16acc64 acc1)
v16acc64 | addmac_4x4_4x4 (v32uint16 a, v32int16 b, v16acc64 acc1, v16acc64 acc2)
v16acc64 | addmsc_4x4_4x4 (v32uint16 a, v32int16 b, v16acc64 acc1, v16acc64 acc2)
v16acc64 | submac_4x4_4x4 (v32uint16 a, v32int16 b, v16acc64 acc1, v16acc64 acc2)
v16acc64 | submsc_4x4_4x4 (v32uint16 a, v32int16 b, v16acc64 acc1, v16acc64 acc2)
v16acc64 | mul_4x4_4x4 (v32int16 a, v32uint16 b)
v16acc64 | negmul_4x4_4x4 (v32int16 a, v32uint16 b)
v16acc64 | mac_4x4_4x4 (v32int16 a, v32uint16 b, v16acc64 acc1)
v16acc64 | msc_4x4_4x4 (v32int16 a, v32uint16 b, v16acc64 acc1)
v16acc64 | negmac_4x4_4x4 (v32int16 a, v32uint16 b, v16acc64 acc1)
v16acc64 | negmsc_4x4_4x4 (v32int16 a, v32uint16 b, v16acc64 acc1)
v16acc64 | addmac_4x4_4x4 (v32int16 a, v32uint16 b, v16acc64 acc1, v16acc64 acc2)
v16acc64 | addmsc_4x4_4x4 (v32int16 a, v32uint16 b, v16acc64 acc1, v16acc64 acc2)
v16acc64 | submac_4x4_4x4 (v32int16 a, v32uint16 b, v16acc64 acc1, v16acc64 acc2)
v16acc64 | submsc_4x4_4x4 (v32int16 a, v32uint16 b, v16acc64 acc1, v16acc64 acc2)
v16acc64 | mul_4x4_4x4 (v32int16 a, v32int16 b)
v16acc64 | negmul_4x4_4x4 (v32int16 a, v32int16 b)
v16acc64 | mac_4x4_4x4 (v32int16 a, v32int16 b, v16acc64 acc1)
v16acc64 | msc_4x4_4x4 (v32int16 a, v32int16 b, v16acc64 acc1)
v16acc64 | negmac_4x4_4x4 (v32int16 a, v32int16 b, v16acc64 acc1)
v16acc64 | negmsc_4x4_4x4 (v32int16 a, v32int16 b, v16acc64 acc1)
v16acc64 | addmac_4x4_4x4 (v32int16 a, v32int16 b, v16acc64 acc1, v16acc64 acc2)
v16acc64 | addmsc_4x4_4x4 (v32int16 a, v32int16 b, v16acc64 acc1, v16acc64 acc2)
v16acc64 | submac_4x4_4x4 (v32int16 a, v32int16 b, v16acc64 acc1, v16acc64 acc2)
v16acc64 | submsc_4x4_4x4 (v32int16 a, v32int16 b, v16acc64 acc1, v16acc64 acc2)

## Multiplication of (4x4) with (4x4) with dynamic sign
v16acc64 | mul_4x4_4x4 (v32uint16 a, int sgn_x, v32uint16 b, int sgn_y)
v16acc64 | negmul_4x4_4x4 (v32uint16 a, int sgn_x, v32uint16 b, int sgn_y)
v16acc64 | mac_4x4_4x4 (v32uint16 a, int sgn_x, v32uint16 b, int sgn_y, v16acc64 acc1)
v16acc64 | msc_4x4_4x4 (v32uint16 a, int sgn_x, v32uint16 b, int sgn_y, v16acc64 acc1)
v16acc64 | negmac_4x4_4x4 (v32uint16 a, int sgn_x, v32uint16 b, int sgn_y, v16acc64 acc1)
v16acc64 | negmsc_4x4_4x4 (v32uint16 a, int sgn_x, v32uint16 b, int sgn_y, v16acc64 acc1)
v16acc64 | addmac_4x4_4x4 (v32uint16 a, int sgn_x, v32uint16 b, int sgn_y, v16acc64 acc1, v16acc64 acc2)
v16acc64 | addmsc_4x4_4x4 (v32uint16 a, int sgn_x, v32uint16 b, int sgn_y, v16acc64 acc1, v16acc64 acc2)
v16acc64 | submac_4x4_4x4 (v32uint16 a, int sgn_x, v32uint16 b, int sgn_y, v16acc64 acc1, v16acc64 acc2)
v16acc64 | submsc_4x4_4x4 (v32uint16 a, int sgn_x, v32uint16 b, int sgn_y, v16acc64 acc1, v16acc64 acc2)
v16acc64 | mul_4x4_4x4 (v32uint16 a, int sgn_x, v32int16 b, int sgn_y)
v16acc64 | negmul_4x4_4x4 (v32uint16 a, int sgn_x, v32int16 b, int sgn_y)
v16acc64 | mac_4x4_4x4 (v32uint16 a, int sgn_x, v32int16 b, int sgn_y, v16acc64 acc1)
v16acc64 | msc_4x4_4x4 (v32uint16 a, int sgn_x, v32int16 b, int sgn_y, v16acc64 acc1)
v16acc64 | negmac_4x4_4x4 (v32uint16 a, int sgn_x, v32int16 b, int sgn_y, v16acc64 acc1)
v16acc64 | negmsc_4x4_4x4 (v32uint16 a, int sgn_x, v32int16 b, int sgn_y, v16acc64 acc1)
v16acc64 | addmac_4x4_4x4 (v32uint16 a, int sgn_x, v32int16 b, int sgn_y, v16acc64 acc1, v16acc64 acc2)
v16acc64 | addmsc_4x4_4x4 (v32uint16 a, int sgn_x, v32int16 b, int sgn_y, v16acc64 acc1, v16acc64 acc2)
v16acc64 | submac_4x4_4x4 (v32uint16 a, int sgn_x, v32int16 b, int sgn_y, v16acc64 acc1, v16acc64 acc2)
v16acc64 | submsc_4x4_4x4 (v32uint16 a, int sgn_x, v32int16 b, int sgn_y, v16acc64 acc1, v16acc64 acc2)
v16acc64 | mul_4x4_4x4 (v32int16 a, int sgn_x, v32uint16 b, int sgn_y)
v16acc64 | negmul_4x4_4x4 (v32int16 a, int sgn_x, v32uint16 b, int sgn_y)
v16acc64 | mac_4x4_4x4 (v32int16 a, int sgn_x, v32uint16 b, int sgn_y, v16acc64 acc1)
v16acc64 | msc_4x4_4x4 (v32int16 a, int sgn_x, v32uint16 b, int sgn_y, v16acc64 acc1)
v16acc64 | negmac_4x4_4x4 (v32int16 a, int sgn_x, v32uint16 b, int sgn_y, v16acc64 acc1)
v16acc64 | negmsc_4x4_4x4 (v32int16 a, int sgn_x, v32uint16 b, int sgn_y, v16acc64 acc1)
v16acc64 | addmac_4x4_4x4 (v32int16 a, int sgn_x, v32uint16 b, int sgn_y, v16acc64 acc1, v16acc64 acc2)
v16acc64 | addmsc_4x4_4x4 (v32int16 a, int sgn_x, v32uint16 b, int sgn_y, v16acc64 acc1, v16acc64 acc2)
v16acc64 | submac_4x4_4x4 (v32int16 a, int sgn_x, v32uint16 b, int sgn_y, v16acc64 acc1, v16acc64 acc2)
v16acc64 | submsc_4x4_4x4 (v32int16 a, int sgn_x, v32uint16 b, int sgn_y, v16acc64 acc1, v16acc64 acc2)
v16acc64 | mul_4x4_4x4 (v32int16 a, int sgn_x, v32int16 b, int sgn_y)
v16acc64 | negmul_4x4_4x4 (v32int16 a, int sgn_x, v32int16 b, int sgn_y)
v16acc64 | mac_4x4_4x4 (v32int16 a, int sgn_x, v32int16 b, int sgn_y, v16acc64 acc1)
v16acc64 | msc_4x4_4x4 (v32int16 a, int sgn_x, v32int16 b, int sgn_y, v16acc64 acc1)
v16acc64 | negmac_4x4_4x4 (v32int16 a, int sgn_x, v32int16 b, int sgn_y, v16acc64 acc1)
v16acc64 | negmsc_4x4_4x4 (v32int16 a, int sgn_x, v32int16 b, int sgn_y, v16acc64 acc1)
v16acc64 | addmac_4x4_4x4 (v32int16 a, int sgn_x, v32int16 b, int sgn_y, v16acc64 acc1, v16acc64 acc2)
v16acc64 | addmsc_4x4_4x4 (v32int16 a, int sgn_x, v32int16 b, int sgn_y, v16acc64 acc1, v16acc64 acc2)
v16acc64 | submac_4x4_4x4 (v32int16 a, int sgn_x, v32int16 b, int sgn_y, v16acc64 acc1, v16acc64 acc2)
v16acc64 | submsc_4x4_4x4 (v32int16 a, int sgn_x, v32int16 b, int sgn_y, v16acc64 acc1, v16acc64 acc2)

## Multiplication of (4x4) with (4x4) with dynamic negation of multiplication result
v16acc64 | mul_4x4_4x4_conf (v32uint16 a, v32uint16 b, int sub_mul)
v16acc64 | negmul_4x4_4x4_conf (v32uint16 a, v32uint16 b, int sub_mul)
v16acc64 | mul_4x4_4x4_conf (v32uint16 a, v32int16 b, int sub_mul)
v16acc64 | negmul_4x4_4x4_conf (v32uint16 a, v32int16 b, int sub_mul)
v16acc64 | mul_4x4_4x4_conf (v32int16 a, v32uint16 b, int sub_mul)
v16acc64 | negmul_4x4_4x4_conf (v32int16 a, v32uint16 b, int sub_mul)
v16acc64 | mul_4x4_4x4_conf (v32int16 a, v32int16 b, int sub_mul)
v16acc64 | negmul_4x4_4x4_conf (v32int16 a, v32int16 b, int sub_mul)

## Multiplication of (4x4) with (4x4) with dynamic negation of multiplication result, zeroing of acc1, and negation of acc1
v16acc64 | mac_4x4_4x4_conf (v32uint16 a, v32uint16 b, v16acc64 acc1, int zero_acc1, int shift16, int sub_mul, int sub_acc1)
v16acc64 | msc_4x4_4x4_conf (v32uint16 a, v32uint16 b, v16acc64 acc1, int zero_acc1, int shift16, int sub_mul, int sub_acc1)
v16acc64 | negmsc_4x4_4x4_conf (v32uint16 a, v32uint16 b, v16acc64 acc1, int zero_acc1, int sub_mul, int sub_acc1)
v16acc64 | negmac_4x4_4x4_conf (v32uint16 a, v32uint16 b, v16acc64 acc1, int zero_acc1, int sub_mul, int sub_acc1)
v16acc64 | addmac_4x4_4x4_conf (v32uint16 a, v32uint16 b, v16acc64 acc1, v16acc64 acc2, int zero_acc1, int shift16, int sub_mul, int sub_acc1, int sub_acc2)
v16acc64 | addmsc_4x4_4x4_conf (v32uint16 a, v32uint16 b, v16acc64 acc1, v16acc64 acc2, int zero_acc1, int shift16, int sub_mul, int sub_acc1, int sub_acc2)
v16acc64 | submac_4x4_4x4_conf (v32uint16 a, v32uint16 b, v16acc64 acc1, v16acc64 acc2, int zero_acc1, int sub_mul, int sub_acc1, int sub_acc2)
v16acc64 | submsc_4x4_4x4_conf (v32uint16 a, v32uint16 b, v16acc64 acc1, v16acc64 acc2, int zero_acc1, int sub_mul, int sub_acc1, int sub_acc2)
v16acc64 | mac_4x4_4x4_conf (v32uint16 a, v32int16 b, v16acc64 acc1, int zero_acc1, int shift16, int sub_mul, int sub_acc1)
v16acc64 | msc_4x4_4x4_conf (v32uint16 a, v32int16 b, v16acc64 acc1, int zero_acc1, int shift16, int sub_mul, int sub_acc1)
v16acc64 | negmsc_4x4_4x4_conf (v32uint16 a, v32int16 b, v16acc64 acc1, int zero_acc1, int sub_mul, int sub_acc1)
v16acc64 | negmac_4x4_4x4_conf (v32uint16 a, v32int16 b, v16acc64 acc1, int zero_acc1, int sub_mul, int sub_acc1)
v16acc64 | addmac_4x4_4x4_conf (v32uint16 a, v32int16 b, v16acc64 acc1, v16acc64 acc2, int zero_acc1, int shift16, int sub_mul, int sub_acc1, int sub_acc2)
v16acc64 | addmsc_4x4_4x4_conf (v32uint16 a, v32int16 b, v16acc64 acc1, v16acc64 acc2, int zero_acc1, int shift16, int sub_mul, int sub_acc1, int sub_acc2)
v16acc64 | submac_4x4_4x4_conf (v32uint16 a, v32int16 b, v16acc64 acc1, v16acc64 acc2, int zero_acc1, int sub_mul, int sub_acc1, int sub_acc2)
v16acc64 | submsc_4x4_4x4_conf (v32uint16 a, v32int16 b, v16acc64 acc1, v16acc64 acc2, int zero_acc1, int sub_mul, int sub_acc1, int sub_acc2)
v16acc64 | mac_4x4_4x4_conf (v32int16 a, v32uint16 b, v16acc64 acc1, int zero_acc1, int shift16, int sub_mul, int sub_acc1)
v16acc64 | msc_4x4_4x4_conf (v32int16 a, v32uint16 b, v16acc64 acc1, int zero_acc1, int shift16, int sub_mul, int sub_acc1)
v16acc64 | negmsc_4x4_4x4_conf (v32int16 a, v32uint16 b, v16acc64 acc1, int zero_acc1, int sub_mul, int sub_acc1)
v16acc64 | negmac_4x4_4x4_conf (v32int16 a, v32uint16 b, v16acc64 acc1, int zero_acc1, int sub_mul, int sub_acc1)
v16acc64 | addmac_4x4_4x4_conf (v32int16 a, v32uint16 b, v16acc64 acc1, v16acc64 acc2, int zero_acc1, int shift16, int sub_mul, int sub_acc1, int sub_acc2)
v16acc64 | addmsc_4x4_4x4_conf (v32int16 a, v32uint16 b, v16acc64 acc1, v16acc64 acc2, int zero_acc1, int shift16, int sub_mul, int sub_acc1, int sub_acc2)
v16acc64 | submac_4x4_4x4_conf (v32int16 a, v32uint16 b, v16acc64 acc1, v16acc64 acc2, int zero_acc1, int sub_mul, int sub_acc1, int sub_acc2)
v16acc64 | submsc_4x4_4x4_conf (v32int16 a, v32uint16 b, v16acc64 acc1, v16acc64 acc2, int zero_acc1, int sub_mul, int sub_acc1, int sub_acc2)
v16acc64 | mac_4x4_4x4_conf (v32int16 a, v32int16 b, v16acc64 acc1, int zero_acc1, int shift16, int sub_mul, int sub_acc1)
v16acc64 | msc_4x4_4x4_conf (v32int16 a, v32int16 b, v16acc64 acc1, int zero_acc1, int shift16, int sub_mul, int sub_acc1)
v16acc64 | negmsc_4x4_4x4_conf (v32int16 a, v32int16 b, v16acc64 acc1, int zero_acc1, int sub_mul, int sub_acc1)
v16acc64 | negmac_4x4_4x4_conf (v32int16 a, v32int16 b, v16acc64 acc1, int zero_acc1, int sub_mul, int sub_acc1)
v16acc64 | addmac_4x4_4x4_conf (v32int16 a, v32int16 b, v16acc64 acc1, v16acc64 acc2, int zero_acc1, int shift16, int sub_mul, int sub_acc1, int sub_acc2)
v16acc64 | addmsc_4x4_4x4_conf (v32int16 a, v32int16 b, v16acc64 acc1, v16acc64 acc2, int zero_acc1, int shift16, int sub_mul, int sub_acc1, int sub_acc2)
v16acc64 | submac_4x4_4x4_conf (v32int16 a, v32int16 b, v16acc64 acc1, v16acc64 acc2, int zero_acc1, int sub_mul, int sub_acc1, int sub_acc2)
v16acc64 | submsc_4x4_4x4_conf (v32int16 a, v32int16 b, v16acc64 acc1, v16acc64 acc2, int zero_acc1, int sub_mul, int sub_acc1, int sub_acc2)

## Multiplication of (4x4) with (4x4) with dynamic sign and dynamic negation of multiplication result
v16acc64 | mul_4x4_4x4_conf (v32uint16 a, int sgn_x, v32uint16 b, int sgn_y, int sub_mul)
v16acc64 | negmul_4x4_4x4_conf (v32uint16 a, int sgn_x, v32uint16 b, int sgn_y, int sub_mul)
v16acc64 | mac_4x4_4x4_conf (v32uint16 a, int sgn_x, v32uint16 b, int sgn_y, v16acc64 acc1, int zero_acc1, int shift16, int sub_mul, int sub_acc1)
v16acc64 | msc_4x4_4x4_conf (v32uint16 a, int sgn_x, v32uint16 b, int sgn_y, v16acc64 acc1, int zero_acc1, int shift16, int sub_mul, int sub_acc1)
v16acc64 | negmsc_4x4_4x4_conf (v32uint16 a, int sgn_x, v32uint16 b, int sgn_y, v16acc64 acc1, int zero_acc1, int sub_mul, int sub_acc1)
v16acc64 | negmac_4x4_4x4_conf (v32uint16 a, int sgn_x, v32uint16 b, int sgn_y, v16acc64 acc1, int zero_acc1, int sub_mul, int sub_acc1)
v16acc64 | addmac_4x4_4x4_conf (v32uint16 a, int sgn_x, v32uint16 b, int sgn_y, v16acc64 acc1, v16acc64 acc2, int zero_acc1, int shift16, int sub_mul, int sub_acc1, int sub_acc2)
v16acc64 | addmsc_4x4_4x4_conf (v32uint16 a, int sgn_x, v32uint16 b, int sgn_y, v16acc64 acc1, v16acc64 acc2, int zero_acc1, int shift16, int sub_mul, int sub_acc1, int sub_acc2)
v16acc64 | submac_4x4_4x4_conf (v32uint16 a, int sgn_x, v32uint16 b, int sgn_y, v16acc64 acc1, v16acc64 acc2, int zero_acc1, int sub_mul, int sub_acc1, int sub_acc2)
v16acc64 | submsc_4x4_4x4_conf (v32uint16 a, int sgn_x, v32uint16 b, int sgn_y, v16acc64 acc1, v16acc64 acc2, int zero_acc1, int sub_mul, int sub_acc1, int sub_acc2)
v16acc64 | mul_4x4_4x4_conf (v32uint16 a, int sgn_x, v32int16 b, int sgn_y, int sub_mul)
v16acc64 | negmul_4x4_4x4_conf (v32uint16 a, int sgn_x, v32int16 b, int sgn_y, int sub_mul)
v16acc64 | mac_4x4_4x4_conf (v32uint16 a, int sgn_x, v32int16 b, int sgn_y, v16acc64 acc1, int zero_acc1, int shift16, int sub_mul, int sub_acc1)
v16acc64 | msc_4x4_4x4_conf (v32uint16 a, int sgn_x, v32int16 b, int sgn_y, v16acc64 acc1, int zero_acc1, int shift16, int sub_mul, int sub_acc1)
v16acc64 | negmsc_4x4_4x4_conf (v32uint16 a, int sgn_x, v32int16 b, int sgn_y, v16acc64 acc1, int zero_acc1, int sub_mul, int sub_acc1)
v16acc64 | negmac_4x4_4x4_conf (v32uint16 a, int sgn_x, v32int16 b, int sgn_y, v16acc64 acc1, int zero_acc1, int sub_mul, int sub_acc1)
v16acc64 | addmac_4x4_4x4_conf (v32uint16 a, int sgn_x, v32int16 b, int sgn_y, v16acc64 acc1, v16acc64 acc2, int zero_acc1, int shift16, int sub_mul, int sub_acc1, int sub_acc2)
v16acc64 | addmsc_4x4_4x4_conf (v32uint16 a, int sgn_x, v32int16 b, int sgn_y, v16acc64 acc1, v16acc64 acc2, int zero_acc1, int shift16, int sub_mul, int sub_acc1, int sub_acc2)
v16acc64 | submac_4x4_4x4_conf (v32uint16 a, int sgn_x, v32int16 b, int sgn_y, v16acc64 acc1, v16acc64 acc2, int zero_acc1, int sub_mul, int sub_acc1, int sub_acc2)
v16acc64 | submsc_4x4_4x4_conf (v32uint16 a, int sgn_x, v32int16 b, int sgn_y, v16acc64 acc1, v16acc64 acc2, int zero_acc1, int sub_mul, int sub_acc1, int sub_acc2)
v16acc64 | mul_4x4_4x4_conf (v32int16 a, int sgn_x, v32uint16 b, int sgn_y, int sub_mul)
v16acc64 | negmul_4x4_4x4_conf (v32int16 a, int sgn_x, v32uint16 b, int sgn_y, int sub_mul)
v16acc64 | mac_4x4_4x4_conf (v32int16 a, int sgn_x, v32uint16 b, int sgn_y, v16acc64 acc1, int zero_acc1, int shift16, int sub_mul, int sub_acc1)
v16acc64 | msc_4x4_4x4_conf (v32int16 a, int sgn_x, v32uint16 b, int sgn_y, v16acc64 acc1, int zero_acc1, int shift16, int sub_mul, int sub_acc1)
v16acc64 | negmsc_4x4_4x4_conf (v32int16 a, int sgn_x, v32uint16 b, int sgn_y, v16acc64 acc1, int zero_acc1, int sub_mul, int sub_acc1)
v16acc64 | negmac_4x4_4x4_conf (v32int16 a, int sgn_x, v32uint16 b, int sgn_y, v16acc64 acc1, int zero_acc1, int sub_mul, int sub_acc1)
v16acc64 | addmac_4x4_4x4_conf (v32int16 a, int sgn_x, v32uint16 b, int sgn_y, v16acc64 acc1, v16acc64 acc2, int zero_acc1, int shift16, int sub_mul, int sub_acc1, int sub_acc2)
v16acc64 | addmsc_4x4_4x4_conf (v32int16 a, int sgn_x, v32uint16 b, int sgn_y, v16acc64 acc1, v16acc64 acc2, int zero_acc1, int shift16, int sub_mul, int sub_acc1, int sub_acc2)
v16acc64 | submac_4x4_4x4_conf (v32int16 a, int sgn_x, v32uint16 b, int sgn_y, v16acc64 acc1, v16acc64 acc2, int zero_acc1, int sub_mul, int sub_acc1, int sub_acc2)
v16acc64 | submsc_4x4_4x4_conf (v32int16 a, int sgn_x, v32uint16 b, int sgn_y, v16acc64 acc1, v16acc64 acc2, int zero_acc1, int sub_mul, int sub_acc1, int sub_acc2)
v16acc64 | mul_4x4_4x4_conf (v32int16 a, int sgn_x, v32int16 b, int sgn_y, int sub_mul)
v16acc64 | negmul_4x4_4x4_conf (v32int16 a, int sgn_x, v32int16 b, int sgn_y, int sub_mul)
v16acc64 | mac_4x4_4x4_conf (v32int16 a, int sgn_x, v32int16 b, int sgn_y, v16acc64 acc1, int zero_acc1, int shift16, int sub_mul, int sub_acc1)
v16acc64 | msc_4x4_4x4_conf (v32int16 a, int sgn_x, v32int16 b, int sgn_y, v16acc64 acc1, int zero_acc1, int shift16, int sub_mul, int sub_acc1)
v16acc64 | negmsc_4x4_4x4_conf (v32int16 a, int sgn_x, v32int16 b, int sgn_y, v16acc64 acc1, int zero_acc1, int sub_mul, int sub_acc1)
v16acc64 | negmac_4x4_4x4_conf (v32int16 a, int sgn_x, v32int16 b, int sgn_y, v16acc64 acc1, int zero_acc1, int sub_mul, int sub_acc1)
v16acc64 | addmac_4x4_4x4_conf (v32int16 a, int sgn_x, v32int16 b, int sgn_y, v16acc64 acc1, v16acc64 acc2, int zero_acc1, int shift16, int sub_mul, int sub_acc1, int sub_acc2)
v16acc64 | addmsc_4x4_4x4_conf (v32int16 a, int sgn_x, v32int16 b, int sgn_y, v16acc64 acc1, v16acc64 acc2, int zero_acc1, int shift16, int sub_mul, int sub_acc1, int sub_acc2)
v16acc64 | submac_4x4_4x4_conf (v32int16 a, int sgn_x, v32int16 b, int sgn_y, v16acc64 acc1, v16acc64 acc2, int zero_acc1, int sub_mul, int sub_acc1, int sub_acc2)
v16acc64 | submsc_4x4_4x4_conf (v32int16 a, int sgn_x, v32int16 b, int sgn_y, v16acc64 acc1, v16acc64 acc2, int zero_acc1, int sub_mul, int sub_acc1, int sub_acc2)

## Channel by channel multiplication of (1x2) with (2x1)
v16acc64 | mul_elem_16_2 (v32uint16 a, v32uint16 b)
v16acc64 | negmul_elem_16_2 (v32uint16 a, v32uint16 b)
v16acc64 | mac_elem_16_2 (v32uint16 a, v32uint16 b, v16acc64 acc1)
v16acc64 | msc_elem_16_2 (v32uint16 a, v32uint16 b, v16acc64 acc1)
v16acc64 | negmac_elem_16_2 (v32uint16 a, v32uint16 b, v16acc64 acc1)
v16acc64 | negmsc_elem_16_2 (v32uint16 a, v32uint16 b, v16acc64 acc1)
v16acc64 | addmac_elem_16_2 (v32uint16 a, v32uint16 b, v16acc64 acc1, v16acc64 acc2)
v16acc64 | addmsc_elem_16_2 (v32uint16 a, v32uint16 b, v16acc64 acc1, v16acc64 acc2)
v16acc64 | submac_elem_16_2 (v32uint16 a, v32uint16 b, v16acc64 acc1, v16acc64 acc2)
v16acc64 | submsc_elem_16_2 (v32uint16 a, v32uint16 b, v16acc64 acc1, v16acc64 acc2)
v16acc64 | mul_elem_16_2 (v32uint16 a, v32int16 b)
v16acc64 | negmul_elem_16_2 (v32uint16 a, v32int16 b)
v16acc64 | mac_elem_16_2 (v32uint16 a, v32int16 b, v16acc64 acc1)
v16acc64 | msc_elem_16_2 (v32uint16 a, v32int16 b, v16acc64 acc1)
v16acc64 | negmac_elem_16_2 (v32uint16 a, v32int16 b, v16acc64 acc1)
v16acc64 | negmsc_elem_16_2 (v32uint16 a, v32int16 b, v16acc64 acc1)
v16acc64 | addmac_elem_16_2 (v32uint16 a, v32int16 b, v16acc64 acc1, v16acc64 acc2)
v16acc64 | addmsc_elem_16_2 (v32uint16 a, v32int16 b, v16acc64 acc1, v16acc64 acc2)
v16acc64 | submac_elem_16_2 (v32uint16 a, v32int16 b, v16acc64 acc1, v16acc64 acc2)
v16acc64 | submsc_elem_16_2 (v32uint16 a, v32int16 b, v16acc64 acc1, v16acc64 acc2)
v16acc64 | mul_elem_16_2 (v32int16 a, v32uint16 b)
v16acc64 | negmul_elem_16_2 (v32int16 a, v32uint16 b)
v16acc64 | mac_elem_16_2 (v32int16 a, v32uint16 b, v16acc64 acc1)
v16acc64 | msc_elem_16_2 (v32int16 a, v32uint16 b, v16acc64 acc1)
v16acc64 | negmac_elem_16_2 (v32int16 a, v32uint16 b, v16acc64 acc1)
v16acc64 | negmsc_elem_16_2 (v32int16 a, v32uint16 b, v16acc64 acc1)
v16acc64 | addmac_elem_16_2 (v32int16 a, v32uint16 b, v16acc64 acc1, v16acc64 acc2)
v16acc64 | addmsc_elem_16_2 (v32int16 a, v32uint16 b, v16acc64 acc1, v16acc64 acc2)
v16acc64 | submac_elem_16_2 (v32int16 a, v32uint16 b, v16acc64 acc1, v16acc64 acc2)
v16acc64 | submsc_elem_16_2 (v32int16 a, v32uint16 b, v16acc64 acc1, v16acc64 acc2)
v16acc64 | mul_elem_16_2 (v32int16 a, v32int16 b)
v16acc64 | negmul_elem_16_2 (v32int16 a, v32int16 b)
v16acc64 | mac_elem_16_2 (v32int16 a, v32int16 b, v16acc64 acc1)
v16acc64 | msc_elem_16_2 (v32int16 a, v32int16 b, v16acc64 acc1)
v16acc64 | negmac_elem_16_2 (v32int16 a, v32int16 b, v16acc64 acc1)
v16acc64 | negmsc_elem_16_2 (v32int16 a, v32int16 b, v16acc64 acc1)
v16acc64 | addmac_elem_16_2 (v32int16 a, v32int16 b, v16acc64 acc1, v16acc64 acc2)
v16acc64 | addmsc_elem_16_2 (v32int16 a, v32int16 b, v16acc64 acc1, v16acc64 acc2)
v16acc64 | submac_elem_16_2 (v32int16 a, v32int16 b, v16acc64 acc1, v16acc64 acc2)
v16acc64 | submsc_elem_16_2 (v32int16 a, v32int16 b, v16acc64 acc1, v16acc64 acc2)
v16accfloat | mul_elem_16_2 (v32bfloat16 a, v32bfloat16 b)
v16accfloat | negmul_elem_16_2 (v32bfloat16 a, v32bfloat16 b)
v16accfloat | mac_elem_16_2 (v32bfloat16 a, v32bfloat16 b, v16accfloat acc1)
v16accfloat | msc_elem_16_2 (v32bfloat16 a, v32bfloat16 b, v16accfloat acc1)
v16accfloat | addmac_elem_16_2 (v32bfloat16 a, v32bfloat16 b, v16accfloat acc1, v16accfloat acc2)
v16accfloat | addmsc_elem_16_2 (v32bfloat16 a, v32bfloat16 b, v16accfloat acc1, v16accfloat acc2)

## Channel by channel multiplication of (1x2) with (2x1) with dynamic sign
v16acc64 | mul_elem_16_2 (v32uint16 a, int sgn_x, v32uint16 b, int sgn_y)
v16acc64 | negmul_elem_16_2 (v32uint16 a, int sgn_x, v32uint16 b, int sgn_y)
v16acc64 | mac_elem_16_2 (v32uint16 a, int sgn_x, v32uint16 b, int sgn_y, v16acc64 acc1)
v16acc64 | msc_elem_16_2 (v32uint16 a, int sgn_x, v32uint16 b, int sgn_y, v16acc64 acc1)
v16acc64 | negmac_elem_16_2 (v32uint16 a, int sgn_x, v32uint16 b, int sgn_y, v16acc64 acc1)
v16acc64 | negmsc_elem_16_2 (v32uint16 a, int sgn_x, v32uint16 b, int sgn_y, v16acc64 acc1)
v16acc64 | addmac_elem_16_2 (v32uint16 a, int sgn_x, v32uint16 b, int sgn_y, v16acc64 acc1, v16acc64 acc2)
v16acc64 | addmsc_elem_16_2 (v32uint16 a, int sgn_x, v32uint16 b, int sgn_y, v16acc64 acc1, v16acc64 acc2)
v16acc64 | submac_elem_16_2 (v32uint16 a, int sgn_x, v32uint16 b, int sgn_y, v16acc64 acc1, v16acc64 acc2)
v16acc64 | submsc_elem_16_2 (v32uint16 a, int sgn_x, v32uint16 b, int sgn_y, v16acc64 acc1, v16acc64 acc2)
v16acc64 | mul_elem_16_2 (v32uint16 a, int sgn_x, v32int16 b, int sgn_y)
v16acc64 | negmul_elem_16_2 (v32uint16 a, int sgn_x, v32int16 b, int sgn_y)
v16acc64 | mac_elem_16_2 (v32uint16 a, int sgn_x, v32int16 b, int sgn_y, v16acc64 acc1)
v16acc64 | msc_elem_16_2 (v32uint16 a, int sgn_x, v32int16 b, int sgn_y, v16acc64 acc1)
v16acc64 | negmac_elem_16_2 (v32uint16 a, int sgn_x, v32int16 b, int sgn_y, v16acc64 acc1)
v16acc64 | negmsc_elem_16_2 (v32uint16 a, int sgn_x, v32int16 b, int sgn_y, v16acc64 acc1)
v16acc64 | addmac_elem_16_2 (v32uint16 a, int sgn_x, v32int16 b, int sgn_y, v16acc64 acc1, v16acc64 acc2)
v16acc64 | addmsc_elem_16_2 (v32uint16 a, int sgn_x, v32int16 b, int sgn_y, v16acc64 acc1, v16acc64 acc2)
v16acc64 | submac_elem_16_2 (v32uint16 a, int sgn_x, v32int16 b, int sgn_y, v16acc64 acc1, v16acc64 acc2)
v16acc64 | submsc_elem_16_2 (v32uint16 a, int sgn_x, v32int16 b, int sgn_y, v16acc64 acc1, v16acc64 acc2)
v16acc64 | mul_elem_16_2 (v32int16 a, int sgn_x, v32uint16 b, int sgn_y)
v16acc64 | negmul_elem_16_2 (v32int16 a, int sgn_x, v32uint16 b, int sgn_y)
v16acc64 | mac_elem_16_2 (v32int16 a, int sgn_x, v32uint16 b, int sgn_y, v16acc64 acc1)
v16acc64 | msc_elem_16_2 (v32int16 a, int sgn_x, v32uint16 b, int sgn_y, v16acc64 acc1)
v16acc64 | negmac_elem_16_2 (v32int16 a, int sgn_x, v32uint16 b, int sgn_y, v16acc64 acc1)
v16acc64 | negmsc_elem_16_2 (v32int16 a, int sgn_x, v32uint16 b, int sgn_y, v16acc64 acc1)
v16acc64 | addmac_elem_16_2 (v32int16 a, int sgn_x, v32uint16 b, int sgn_y, v16acc64 acc1, v16acc64 acc2)
v16acc64 | addmsc_elem_16_2 (v32int16 a, int sgn_x, v32uint16 b, int sgn_y, v16acc64 acc1, v16acc64 acc2)
v16acc64 | submac_elem_16_2 (v32int16 a, int sgn_x, v32uint16 b, int sgn_y, v16acc64 acc1, v16acc64 acc2)
v16acc64 | submsc_elem_16_2 (v32int16 a, int sgn_x, v32uint16 b, int sgn_y, v16acc64 acc1, v16acc64 acc2)
v16acc64 | mul_elem_16_2 (v32int16 a, int sgn_x, v32int16 b, int sgn_y)
v16acc64 | negmul_elem_16_2 (v32int16 a, int sgn_x, v32int16 b, int sgn_y)
v16acc64 | mac_elem_16_2 (v32int16 a, int sgn_x, v32int16 b, int sgn_y, v16acc64 acc1)
v16acc64 | msc_elem_16_2 (v32int16 a, int sgn_x, v32int16 b, int sgn_y, v16acc64 acc1)
v16acc64 | negmac_elem_16_2 (v32int16 a, int sgn_x, v32int16 b, int sgn_y, v16acc64 acc1)
v16acc64 | negmsc_elem_16_2 (v32int16 a, int sgn_x, v32int16 b, int sgn_y, v16acc64 acc1)
v16acc64 | addmac_elem_16_2 (v32int16 a, int sgn_x, v32int16 b, int sgn_y, v16acc64 acc1, v16acc64 acc2)
v16acc64 | addmsc_elem_16_2 (v32int16 a, int sgn_x, v32int16 b, int sgn_y, v16acc64 acc1, v16acc64 acc2)
v16acc64 | submac_elem_16_2 (v32int16 a, int sgn_x, v32int16 b, int sgn_y, v16acc64 acc1, v16acc64 acc2)
v16acc64 | submsc_elem_16_2 (v32int16 a, int sgn_x, v32int16 b, int sgn_y, v16acc64 acc1, v16acc64 acc2)

## Channel by channel multiplication of (1x2) with (2x1) with dynamic negation of multiplication result
v16acc64 | mul_elem_16_2_conf (v32uint16 a, v32uint16 b, int sub_mul)
v16acc64 | negmul_elem_16_2_conf (v32uint16 a, v32uint16 b, int sub_mul)
v16acc64 | mul_elem_16_2_conf (v32uint16 a, v32int16 b, int sub_mul)
v16acc64 | negmul_elem_16_2_conf (v32uint16 a, v32int16 b, int sub_mul)
v16acc64 | mul_elem_16_2_conf (v32int16 a, v32uint16 b, int sub_mul)
v16acc64 | negmul_elem_16_2_conf (v32int16 a, v32uint16 b, int sub_mul)
v16acc64 | mul_elem_16_2_conf (v32int16 a, v32int16 b, int sub_mul)
v16acc64 | negmul_elem_16_2_conf (v32int16 a, v32int16 b, int sub_mul)
v16accfloat | mul_elem_16_2_conf (v32bfloat16 a, v32bfloat16 b, int sub_mul)
v16accfloat | negmul_elem_16_2_conf (v32bfloat16 a, v32bfloat16 b, int sub_mul)

## Channel by channel multiplication of (1x2) with (2x1) with dynamic negation of multiplication result, zeroing of acc1, and negation of acc1
v16acc64 | mac_elem_16_2_conf (v32uint16 a, v32uint16 b, v16acc64 acc1, int zero_acc1, int shift16, int sub_mul, int sub_acc1)
v16acc64 | msc_elem_16_2_conf (v32uint16 a, v32uint16 b, v16acc64 acc1, int zero_acc1, int shift16, int sub_mul, int sub_acc1)
v16acc64 | negmsc_elem_16_2_conf (v32uint16 a, v32uint16 b, v16acc64 acc1, int zero_acc1, int sub_mul, int sub_acc1)
v16acc64 | negmac_elem_16_2_conf (v32uint16 a, v32uint16 b, v16acc64 acc1, int zero_acc1, int sub_mul, int sub_acc1)
v16acc64 | addmac_elem_16_2_conf (v32uint16 a, v32uint16 b, v16acc64 acc1, v16acc64 acc2, int zero_acc1, int shift16, int sub_mul, int sub_acc1, int sub_acc2)
v16acc64 | addmsc_elem_16_2_conf (v32uint16 a, v32uint16 b, v16acc64 acc1, v16acc64 acc2, int zero_acc1, int shift16, int sub_mul, int sub_acc1, int sub_acc2)
v16acc64 | submac_elem_16_2_conf (v32uint16 a, v32uint16 b, v16acc64 acc1, v16acc64 acc2, int zero_acc1, int sub_mul, int sub_acc1, int sub_acc2)
v16acc64 | submsc_elem_16_2_conf (v32uint16 a, v32uint16 b, v16acc64 acc1, v16acc64 acc2, int zero_acc1, int sub_mul, int sub_acc1, int sub_acc2)
v16acc64 | mac_elem_16_2_conf (v32uint16 a, v32int16 b, v16acc64 acc1, int zero_acc1, int shift16, int sub_mul, int sub_acc1)
v16acc64 | msc_elem_16_2_conf (v32uint16 a, v32int16 b, v16acc64 acc1, int zero_acc1, int shift16, int sub_mul, int sub_acc1)
v16acc64 | negmsc_elem_16_2_conf (v32uint16 a, v32int16 b, v16acc64 acc1, int zero_acc1, int sub_mul, int sub_acc1)
v16acc64 | negmac_elem_16_2_conf (v32uint16 a, v32int16 b, v16acc64 acc1, int zero_acc1, int sub_mul, int sub_acc1)
v16acc64 | addmac_elem_16_2_conf (v32uint16 a, v32int16 b, v16acc64 acc1, v16acc64 acc2, int zero_acc1, int shift16, int sub_mul, int sub_acc1, int sub_acc2)
v16acc64 | addmsc_elem_16_2_conf (v32uint16 a, v32int16 b, v16acc64 acc1, v16acc64 acc2, int zero_acc1, int shift16, int sub_mul, int sub_acc1, int sub_acc2)
v16acc64 | submac_elem_16_2_conf (v32uint16 a, v32int16 b, v16acc64 acc1, v16acc64 acc2, int zero_acc1, int sub_mul, int sub_acc1, int sub_acc2)
v16acc64 | submsc_elem_16_2_conf (v32uint16 a, v32int16 b, v16acc64 acc1, v16acc64 acc2, int zero_acc1, int sub_mul, int sub_acc1, int sub_acc2)
v16acc64 | mac_elem_16_2_conf (v32int16 a, v32uint16 b, v16acc64 acc1, int zero_acc1, int shift16, int sub_mul, int sub_acc1)
v16acc64 | msc_elem_16_2_conf (v32int16 a, v32uint16 b, v16acc64 acc1, int zero_acc1, int shift16, int sub_mul, int sub_acc1)
v16acc64 | negmsc_elem_16_2_conf (v32int16 a, v32uint16 b, v16acc64 acc1, int zero_acc1, int sub_mul, int sub_acc1)
v16acc64 | negmac_elem_16_2_conf (v32int16 a, v32uint16 b, v16acc64 acc1, int zero_acc1, int sub_mul, int sub_acc1)
v16acc64 | addmac_elem_16_2_conf (v32int16 a, v32uint16 b, v16acc64 acc1, v16acc64 acc2, int zero_acc1, int shift16, int sub_mul, int sub_acc1, int sub_acc2)
v16acc64 | addmsc_elem_16_2_conf (v32int16 a, v32uint16 b, v16acc64 acc1, v16acc64 acc2, int zero_acc1, int shift16, int sub_mul, int sub_acc1, int sub_acc2)
v16acc64 | submac_elem_16_2_conf (v32int16 a, v32uint16 b, v16acc64 acc1, v16acc64 acc2, int zero_acc1, int sub_mul, int sub_acc1, int sub_acc2)
v16acc64 | submsc_elem_16_2_conf (v32int16 a, v32uint16 b, v16acc64 acc1, v16acc64 acc2, int zero_acc1, int sub_mul, int sub_acc1, int sub_acc2)
v16acc64 | mac_elem_16_2_conf (v32int16 a, v32int16 b, v16acc64 acc1, int zero_acc1, int shift16, int sub_mul, int sub_acc1)
v16acc64 | msc_elem_16_2_conf (v32int16 a, v32int16 b, v16acc64 acc1, int zero_acc1, int shift16, int sub_mul, int sub_acc1)
v16acc64 | negmsc_elem_16_2_conf (v32int16 a, v32int16 b, v16acc64 acc1, int zero_acc1, int sub_mul, int sub_acc1)
v16acc64 | negmac_elem_16_2_conf (v32int16 a, v32int16 b, v16acc64 acc1, int zero_acc1, int sub_mul, int sub_acc1)
v16acc64 | addmac_elem_16_2_conf (v32int16 a, v32int16 b, v16acc64 acc1, v16acc64 acc2, int zero_acc1, int shift16, int sub_mul, int sub_acc1, int sub_acc2)
v16acc64 | addmsc_elem_16_2_conf (v32int16 a, v32int16 b, v16acc64 acc1, v16acc64 acc2, int zero_acc1, int shift16, int sub_mul, int sub_acc1, int sub_acc2)
v16acc64 | submac_elem_16_2_conf (v32int16 a, v32int16 b, v16acc64 acc1, v16acc64 acc2, int zero_acc1, int sub_mul, int sub_acc1, int sub_acc2)
v16acc64 | submsc_elem_16_2_conf (v32int16 a, v32int16 b, v16acc64 acc1, v16acc64 acc2, int zero_acc1, int sub_mul, int sub_acc1, int sub_acc2)
v16accfloat | mac_elem_16_2_conf (v32bfloat16 a, v32bfloat16 b, v16accfloat acc1, int zero_acc1, int sub_mul, int sub_acc1)
v16accfloat | msc_elem_16_2_conf (v32bfloat16 a, v32bfloat16 b, v16accfloat acc1, int zero_acc1, int sub_mul, int sub_acc1)
v16accfloat | addmac_elem_16_2_conf (v32bfloat16 a, v32bfloat16 b, v16accfloat acc1, v16accfloat acc2, int zero_acc1, int sub_mul, int sub_acc1, int sub_acc2)
v16accfloat | addmsc_elem_16_2_conf (v32bfloat16 a, v32bfloat16 b, v16accfloat acc1, v16accfloat acc2, int zero_acc1, int sub_mul, int sub_acc1, int sub_acc2)

## Channel by channel multiplication of (1x2) with (2x1) with dynamic sign and dynamic negation of multiplication result
v16acc64 | mul_elem_16_2_conf (v32uint16 a, int sgn_x, v32uint16 b, int sgn_y, int sub_mul)
v16acc64 | negmul_elem_16_2_conf (v32uint16 a, int sgn_x, v32uint16 b, int sgn_y, int sub_mul)
v16acc64 | mac_elem_16_2_conf (v32uint16 a, int sgn_x, v32uint16 b, int sgn_y, v16acc64 acc1, int zero_acc1, int shift16, int sub_mul, int sub_acc1)
v16acc64 | msc_elem_16_2_conf (v32uint16 a, int sgn_x, v32uint16 b, int sgn_y, v16acc64 acc1, int zero_acc1, int shift16, int sub_mul, int sub_acc1)
v16acc64 | negmsc_elem_16_2_conf (v32uint16 a, int sgn_x, v32uint16 b, int sgn_y, v16acc64 acc1, int zero_acc1, int sub_mul, int sub_acc1)
v16acc64 | negmac_elem_16_2_conf (v32uint16 a, int sgn_x, v32uint16 b, int sgn_y, v16acc64 acc1, int zero_acc1, int sub_mul, int sub_acc1)
v16acc64 | addmac_elem_16_2_conf (v32uint16 a, int sgn_x, v32uint16 b, int sgn_y, v16acc64 acc1, v16acc64 acc2, int zero_acc1, int shift16, int sub_mul, int sub_acc1, int sub_acc2)
v16acc64 | addmsc_elem_16_2_conf (v32uint16 a, int sgn_x, v32uint16 b, int sgn_y, v16acc64 acc1, v16acc64 acc2, int zero_acc1, int shift16, int sub_mul, int sub_acc1, int sub_acc2)
v16acc64 | submac_elem_16_2_conf (v32uint16 a, int sgn_x, v32uint16 b, int sgn_y, v16acc64 acc1, v16acc64 acc2, int zero_acc1, int sub_mul, int sub_acc1, int sub_acc2)
v16acc64 | submsc_elem_16_2_conf (v32uint16 a, int sgn_x, v32uint16 b, int sgn_y, v16acc64 acc1, v16acc64 acc2, int zero_acc1, int sub_mul, int sub_acc1, int sub_acc2)
v16acc64 | mul_elem_16_2_conf (v32uint16 a, int sgn_x, v32int16 b, int sgn_y, int sub_mul)
v16acc64 | negmul_elem_16_2_conf (v32uint16 a, int sgn_x, v32int16 b, int sgn_y, int sub_mul)
v16acc64 | mac_elem_16_2_conf (v32uint16 a, int sgn_x, v32int16 b, int sgn_y, v16acc64 acc1, int zero_acc1, int shift16, int sub_mul, int sub_acc1)
v16acc64 | msc_elem_16_2_conf (v32uint16 a, int sgn_x, v32int16 b, int sgn_y, v16acc64 acc1, int zero_acc1, int shift16, int sub_mul, int sub_acc1)
v16acc64 | negmsc_elem_16_2_conf (v32uint16 a, int sgn_x, v32int16 b, int sgn_y, v16acc64 acc1, int zero_acc1, int sub_mul, int sub_acc1)
v16acc64 | negmac_elem_16_2_conf (v32uint16 a, int sgn_x, v32int16 b, int sgn_y, v16acc64 acc1, int zero_acc1, int sub_mul, int sub_acc1)
v16acc64 | addmac_elem_16_2_conf (v32uint16 a, int sgn_x, v32int16 b, int sgn_y, v16acc64 acc1, v16acc64 acc2, int zero_acc1, int shift16, int sub_mul, int sub_acc1, int sub_acc2)
v16acc64 | addmsc_elem_16_2_conf (v32uint16 a, int sgn_x, v32int16 b, int sgn_y, v16acc64 acc1, v16acc64 acc2, int zero_acc1, int shift16, int sub_mul, int sub_acc1, int sub_acc2)
v16acc64 | submac_elem_16_2_conf (v32uint16 a, int sgn_x, v32int16 b, int sgn_y, v16acc64 acc1, v16acc64 acc2, int zero_acc1, int sub_mul, int sub_acc1, int sub_acc2)
v16acc64 | submsc_elem_16_2_conf (v32uint16 a, int sgn_x, v32int16 b, int sgn_y, v16acc64 acc1, v16acc64 acc2, int zero_acc1, int sub_mul, int sub_acc1, int sub_acc2)
v16acc64 | mul_elem_16_2_conf (v32int16 a, int sgn_x, v32uint16 b, int sgn_y, int sub_mul)
v16acc64 | negmul_elem_16_2_conf (v32int16 a, int sgn_x, v32uint16 b, int sgn_y, int sub_mul)
v16acc64 | mac_elem_16_2_conf (v32int16 a, int sgn_x, v32uint16 b, int sgn_y, v16acc64 acc1, int zero_acc1, int shift16, int sub_mul, int sub_acc1)
v16acc64 | msc_elem_16_2_conf (v32int16 a, int sgn_x, v32uint16 b, int sgn_y, v16acc64 acc1, int zero_acc1, int shift16, int sub_mul, int sub_acc1)
v16acc64 | negmsc_elem_16_2_conf (v32int16 a, int sgn_x, v32uint16 b, int sgn_y, v16acc64 acc1, int zero_acc1, int sub_mul, int sub_acc1)
v16acc64 | negmac_elem_16_2_conf (v32int16 a, int sgn_x, v32uint16 b, int sgn_y, v16acc64 acc1, int zero_acc1, int sub_mul, int sub_acc1)
v16acc64 | addmac_elem_16_2_conf (v32int16 a, int sgn_x, v32uint16 b, int sgn_y, v16acc64 acc1, v16acc64 acc2, int zero_acc1, int shift16, int sub_mul, int sub_acc1, int sub_acc2)
v16acc64 | addmsc_elem_16_2_conf (v32int16 a, int sgn_x, v32uint16 b, int sgn_y, v16acc64 acc1, v16acc64 acc2, int zero_acc1, int shift16, int sub_mul, int sub_acc1, int sub_acc2)
v16acc64 | submac_elem_16_2_conf (v32int16 a, int sgn_x, v32uint16 b, int sgn_y, v16acc64 acc1, v16acc64 acc2, int zero_acc1, int sub_mul, int sub_acc1, int sub_acc2)
v16acc64 | submsc_elem_16_2_conf (v32int16 a, int sgn_x, v32uint16 b, int sgn_y, v16acc64 acc1, v16acc64 acc2, int zero_acc1, int sub_mul, int sub_acc1, int sub_acc2)
v16acc64 | mul_elem_16_2_conf (v32int16 a, int sgn_x, v32int16 b, int sgn_y, int sub_mul)
v16acc64 | negmul_elem_16_2_conf (v32int16 a, int sgn_x, v32int16 b, int sgn_y, int sub_mul)
v16acc64 | mac_elem_16_2_conf (v32int16 a, int sgn_x, v32int16 b, int sgn_y, v16acc64 acc1, int zero_acc1, int shift16, int sub_mul, int sub_acc1)
v16acc64 | msc_elem_16_2_conf (v32int16 a, int sgn_x, v32int16 b, int sgn_y, v16acc64 acc1, int zero_acc1, int shift16, int sub_mul, int sub_acc1)
v16acc64 | negmsc_elem_16_2_conf (v32int16 a, int sgn_x, v32int16 b, int sgn_y, v16acc64 acc1, int zero_acc1, int sub_mul, int sub_acc1)
v16acc64 | negmac_elem_16_2_conf (v32int16 a, int sgn_x, v32int16 b, int sgn_y, v16acc64 acc1, int zero_acc1, int sub_mul, int sub_acc1)
v16acc64 | addmac_elem_16_2_conf (v32int16 a, int sgn_x, v32int16 b, int sgn_y, v16acc64 acc1, v16acc64 acc2, int zero_acc1, int shift16, int sub_mul, int sub_acc1, int sub_acc2)
v16acc64 | addmsc_elem_16_2_conf (v32int16 a, int sgn_x, v32int16 b, int sgn_y, v16acc64 acc1, v16acc64 acc2, int zero_acc1, int shift16, int sub_mul, int sub_acc1, int sub_acc2)
v16acc64 | submac_elem_16_2_conf (v32int16 a, int sgn_x, v32int16 b, int sgn_y, v16acc64 acc1, v16acc64 acc2, int zero_acc1, int sub_mul, int sub_acc1, int sub_acc2)
v16acc64 | submsc_elem_16_2_conf (v32int16 a, int sgn_x, v32int16 b, int sgn_y, v16acc64 acc1, v16acc64 acc2, int zero_acc1, int sub_mul, int sub_acc1, int sub_acc2)

## Convolution of (16x4) matrix with (4x1) kernel
v16acc64 | mul_conv_16x4 (v32uint16 a, v32uint16 b)
v16acc64 | negmul_conv_16x4 (v32uint16 a, v32uint16 b)
v16acc64 | mac_conv_16x4 (v32uint16 a, v32uint16 b, v16acc64 acc1)
v16acc64 | msc_conv_16x4 (v32uint16 a, v32uint16 b, v16acc64 acc1)
v16acc64 | negmac_conv_16x4 (v32uint16 a, v32uint16 b, v16acc64 acc1)
v16acc64 | negmsc_conv_16x4 (v32uint16 a, v32uint16 b, v16acc64 acc1)
v16acc64 | addmac_conv_16x4 (v32uint16 a, v32uint16 b, v16acc64 acc1, v16acc64 acc2)
v16acc64 | addmsc_conv_16x4 (v32uint16 a, v32uint16 b, v16acc64 acc1, v16acc64 acc2)
v16acc64 | submac_conv_16x4 (v32uint16 a, v32uint16 b, v16acc64 acc1, v16acc64 acc2)
v16acc64 | submsc_conv_16x4 (v32uint16 a, v32uint16 b, v16acc64 acc1, v16acc64 acc2)
v16acc64 | mul_conv_16x4 (v32uint16 a, v32int16 b)
v16acc64 | negmul_conv_16x4 (v32uint16 a, v32int16 b)
v16acc64 | mac_conv_16x4 (v32uint16 a, v32int16 b, v16acc64 acc1)
v16acc64 | msc_conv_16x4 (v32uint16 a, v32int16 b, v16acc64 acc1)
v16acc64 | negmac_conv_16x4 (v32uint16 a, v32int16 b, v16acc64 acc1)
v16acc64 | negmsc_conv_16x4 (v32uint16 a, v32int16 b, v16acc64 acc1)
v16acc64 | addmac_conv_16x4 (v32uint16 a, v32int16 b, v16acc64 acc1, v16acc64 acc2)
v16acc64 | addmsc_conv_16x4 (v32uint16 a, v32int16 b, v16acc64 acc1, v16acc64 acc2)
v16acc64 | submac_conv_16x4 (v32uint16 a, v32int16 b, v16acc64 acc1, v16acc64 acc2)
v16acc64 | submsc_conv_16x4 (v32uint16 a, v32int16 b, v16acc64 acc1, v16acc64 acc2)
v16acc64 | mul_conv_16x4 (v32int16 a, v32uint16 b)
v16acc64 | negmul_conv_16x4 (v32int16 a, v32uint16 b)
v16acc64 | mac_conv_16x4 (v32int16 a, v32uint16 b, v16acc64 acc1)
v16acc64 | msc_conv_16x4 (v32int16 a, v32uint16 b, v16acc64 acc1)
v16acc64 | negmac_conv_16x4 (v32int16 a, v32uint16 b, v16acc64 acc1)
v16acc64 | negmsc_conv_16x4 (v32int16 a, v32uint16 b, v16acc64 acc1)
v16acc64 | addmac_conv_16x4 (v32int16 a, v32uint16 b, v16acc64 acc1, v16acc64 acc2)
v16acc64 | addmsc_conv_16x4 (v32int16 a, v32uint16 b, v16acc64 acc1, v16acc64 acc2)
v16acc64 | submac_conv_16x4 (v32int16 a, v32uint16 b, v16acc64 acc1, v16acc64 acc2)
v16acc64 | submsc_conv_16x4 (v32int16 a, v32uint16 b, v16acc64 acc1, v16acc64 acc2)
v16acc64 | mul_conv_16x4 (v32int16 a, v32int16 b)
v16acc64 | negmul_conv_16x4 (v32int16 a, v32int16 b)
v16acc64 | mac_conv_16x4 (v32int16 a, v32int16 b, v16acc64 acc1)
v16acc64 | msc_conv_16x4 (v32int16 a, v32int16 b, v16acc64 acc1)
v16acc64 | negmac_conv_16x4 (v32int16 a, v32int16 b, v16acc64 acc1)
v16acc64 | negmsc_conv_16x4 (v32int16 a, v32int16 b, v16acc64 acc1)
v16acc64 | addmac_conv_16x4 (v32int16 a, v32int16 b, v16acc64 acc1, v16acc64 acc2)
v16acc64 | addmsc_conv_16x4 (v32int16 a, v32int16 b, v16acc64 acc1, v16acc64 acc2)
v16acc64 | submac_conv_16x4 (v32int16 a, v32int16 b, v16acc64 acc1, v16acc64 acc2)
v16acc64 | submsc_conv_16x4 (v32int16 a, v32int16 b, v16acc64 acc1, v16acc64 acc2)

## Convolution of (16x4) matrix with (4x1) kernel with dynamic sign
v16acc64 | mul_conv_16x4 (v32uint16 a, int sgn_x, v32uint16 b, int sgn_y)
v16acc64 | negmul_conv_16x4 (v32uint16 a, int sgn_x, v32uint16 b, int sgn_y)
v16acc64 | mac_conv_16x4 (v32uint16 a, int sgn_x, v32uint16 b, int sgn_y, v16acc64 acc1)
v16acc64 | msc_conv_16x4 (v32uint16 a, int sgn_x, v32uint16 b, int sgn_y, v16acc64 acc1)
v16acc64 | negmac_conv_16x4 (v32uint16 a, int sgn_x, v32uint16 b, int sgn_y, v16acc64 acc1)
v16acc64 | negmsc_conv_16x4 (v32uint16 a, int sgn_x, v32uint16 b, int sgn_y, v16acc64 acc1)
v16acc64 | addmac_conv_16x4 (v32uint16 a, int sgn_x, v32uint16 b, int sgn_y, v16acc64 acc1, v16acc64 acc2)
v16acc64 | addmsc_conv_16x4 (v32uint16 a, int sgn_x, v32uint16 b, int sgn_y, v16acc64 acc1, v16acc64 acc2)
v16acc64 | submac_conv_16x4 (v32uint16 a, int sgn_x, v32uint16 b, int sgn_y, v16acc64 acc1, v16acc64 acc2)
v16acc64 | submsc_conv_16x4 (v32uint16 a, int sgn_x, v32uint16 b, int sgn_y, v16acc64 acc1, v16acc64 acc2)
v16acc64 | mul_conv_16x4 (v32uint16 a, int sgn_x, v32int16 b, int sgn_y)
v16acc64 | negmul_conv_16x4 (v32uint16 a, int sgn_x, v32int16 b, int sgn_y)
v16acc64 | mac_conv_16x4 (v32uint16 a, int sgn_x, v32int16 b, int sgn_y, v16acc64 acc1)
v16acc64 | msc_conv_16x4 (v32uint16 a, int sgn_x, v32int16 b, int sgn_y, v16acc64 acc1)
v16acc64 | negmac_conv_16x4 (v32uint16 a, int sgn_x, v32int16 b, int sgn_y, v16acc64 acc1)
v16acc64 | negmsc_conv_16x4 (v32uint16 a, int sgn_x, v32int16 b, int sgn_y, v16acc64 acc1)
v16acc64 | addmac_conv_16x4 (v32uint16 a, int sgn_x, v32int16 b, int sgn_y, v16acc64 acc1, v16acc64 acc2)
v16acc64 | addmsc_conv_16x4 (v32uint16 a, int sgn_x, v32int16 b, int sgn_y, v16acc64 acc1, v16acc64 acc2)
v16acc64 | submac_conv_16x4 (v32uint16 a, int sgn_x, v32int16 b, int sgn_y, v16acc64 acc1, v16acc64 acc2)
v16acc64 | submsc_conv_16x4 (v32uint16 a, int sgn_x, v32int16 b, int sgn_y, v16acc64 acc1, v16acc64 acc2)
v16acc64 | mul_conv_16x4 (v32int16 a, int sgn_x, v32uint16 b, int sgn_y)
v16acc64 | negmul_conv_16x4 (v32int16 a, int sgn_x, v32uint16 b, int sgn_y)
v16acc64 | mac_conv_16x4 (v32int16 a, int sgn_x, v32uint16 b, int sgn_y, v16acc64 acc1)
v16acc64 | msc_conv_16x4 (v32int16 a, int sgn_x, v32uint16 b, int sgn_y, v16acc64 acc1)
v16acc64 | negmac_conv_16x4 (v32int16 a, int sgn_x, v32uint16 b, int sgn_y, v16acc64 acc1)
v16acc64 | negmsc_conv_16x4 (v32int16 a, int sgn_x, v32uint16 b, int sgn_y, v16acc64 acc1)
v16acc64 | addmac_conv_16x4 (v32int16 a, int sgn_x, v32uint16 b, int sgn_y, v16acc64 acc1, v16acc64 acc2)
v16acc64 | addmsc_conv_16x4 (v32int16 a, int sgn_x, v32uint16 b, int sgn_y, v16acc64 acc1, v16acc64 acc2)
v16acc64 | submac_conv_16x4 (v32int16 a, int sgn_x, v32uint16 b, int sgn_y, v16acc64 acc1, v16acc64 acc2)
v16acc64 | submsc_conv_16x4 (v32int16 a, int sgn_x, v32uint16 b, int sgn_y, v16acc64 acc1, v16acc64 acc2)
v16acc64 | mul_conv_16x4 (v32int16 a, int sgn_x, v32int16 b, int sgn_y)
v16acc64 | negmul_conv_16x4 (v32int16 a, int sgn_x, v32int16 b, int sgn_y)
v16acc64 | mac_conv_16x4 (v32int16 a, int sgn_x, v32int16 b, int sgn_y, v16acc64 acc1)
v16acc64 | msc_conv_16x4 (v32int16 a, int sgn_x, v32int16 b, int sgn_y, v16acc64 acc1)
v16acc64 | negmac_conv_16x4 (v32int16 a, int sgn_x, v32int16 b, int sgn_y, v16acc64 acc1)
v16acc64 | negmsc_conv_16x4 (v32int16 a, int sgn_x, v32int16 b, int sgn_y, v16acc64 acc1)
v16acc64 | addmac_conv_16x4 (v32int16 a, int sgn_x, v32int16 b, int sgn_y, v16acc64 acc1, v16acc64 acc2)
v16acc64 | addmsc_conv_16x4 (v32int16 a, int sgn_x, v32int16 b, int sgn_y, v16acc64 acc1, v16acc64 acc2)
v16acc64 | submac_conv_16x4 (v32int16 a, int sgn_x, v32int16 b, int sgn_y, v16acc64 acc1, v16acc64 acc2)
v16acc64 | submsc_conv_16x4 (v32int16 a, int sgn_x, v32int16 b, int sgn_y, v16acc64 acc1, v16acc64 acc2)

## Convolution of (16x4) matrix with (4x1) kernel with dynamic negation of multiplication result
v16acc64 | mul_conv_16x4_conf (v32uint16 a, v32uint16 b, int sub_mul)
v16acc64 | negmul_conv_16x4_conf (v32uint16 a, v32uint16 b, int sub_mul)
v16acc64 | mul_conv_16x4_conf (v32uint16 a, v32int16 b, int sub_mul)
v16acc64 | negmul_conv_16x4_conf (v32uint16 a, v32int16 b, int sub_mul)
v16acc64 | mul_conv_16x4_conf (v32int16 a, v32uint16 b, int sub_mul)
v16acc64 | negmul_conv_16x4_conf (v32int16 a, v32uint16 b, int sub_mul)
v16acc64 | mul_conv_16x4_conf (v32int16 a, v32int16 b, int sub_mul)
v16acc64 | negmul_conv_16x4_conf (v32int16 a, v32int16 b, int sub_mul)

## Convolution of (16x4) matrix with (4x1) kernel with dynamic negation of multiplication result, zeroing of acc1, and negation of acc1
v16acc64 | mac_conv_16x4_conf (v32uint16 a, v32uint16 b, v16acc64 acc1, int zero_acc1, int shift16, int sub_mul, int sub_acc1)
v16acc64 | msc_conv_16x4_conf (v32uint16 a, v32uint16 b, v16acc64 acc1, int zero_acc1, int shift16, int sub_mul, int sub_acc1)
v16acc64 | negmsc_conv_16x4_conf (v32uint16 a, v32uint16 b, v16acc64 acc1, int zero_acc1, int sub_mul, int sub_acc1)
v16acc64 | negmac_conv_16x4_conf (v32uint16 a, v32uint16 b, v16acc64 acc1, int zero_acc1, int sub_mul, int sub_acc1)
v16acc64 | addmac_conv_16x4_conf (v32uint16 a, v32uint16 b, v16acc64 acc1, v16acc64 acc2, int zero_acc1, int shift16, int sub_mul, int sub_acc1, int sub_acc2)
v16acc64 | addmsc_conv_16x4_conf (v32uint16 a, v32uint16 b, v16acc64 acc1, v16acc64 acc2, int zero_acc1, int shift16, int sub_mul, int sub_acc1, int sub_acc2)
v16acc64 | submac_conv_16x4_conf (v32uint16 a, v32uint16 b, v16acc64 acc1, v16acc64 acc2, int zero_acc1, int sub_mul, int sub_acc1, int sub_acc2)
v16acc64 | submsc_conv_16x4_conf (v32uint16 a, v32uint16 b, v16acc64 acc1, v16acc64 acc2, int zero_acc1, int sub_mul, int sub_acc1, int sub_acc2)
v16acc64 | mac_conv_16x4_conf (v32uint16 a, v32int16 b, v16acc64 acc1, int zero_acc1, int shift16, int sub_mul, int sub_acc1)
v16acc64 | msc_conv_16x4_conf (v32uint16 a, v32int16 b, v16acc64 acc1, int zero_acc1, int shift16, int sub_mul, int sub_acc1)
v16acc64 | negmsc_conv_16x4_conf (v32uint16 a, v32int16 b, v16acc64 acc1, int zero_acc1, int sub_mul, int sub_acc1)
v16acc64 | negmac_conv_16x4_conf (v32uint16 a, v32int16 b, v16acc64 acc1, int zero_acc1, int sub_mul, int sub_acc1)
v16acc64 | addmac_conv_16x4_conf (v32uint16 a, v32int16 b, v16acc64 acc1, v16acc64 acc2, int zero_acc1, int shift16, int sub_mul, int sub_acc1, int sub_acc2)
v16acc64 | addmsc_conv_16x4_conf (v32uint16 a, v32int16 b, v16acc64 acc1, v16acc64 acc2, int zero_acc1, int shift16, int sub_mul, int sub_acc1, int sub_acc2)
v16acc64 | submac_conv_16x4_conf (v32uint16 a, v32int16 b, v16acc64 acc1, v16acc64 acc2, int zero_acc1, int sub_mul, int sub_acc1, int sub_acc2)
v16acc64 | submsc_conv_16x4_conf (v32uint16 a, v32int16 b, v16acc64 acc1, v16acc64 acc2, int zero_acc1, int sub_mul, int sub_acc1, int sub_acc2)
v16acc64 | mac_conv_16x4_conf (v32int16 a, v32uint16 b, v16acc64 acc1, int zero_acc1, int shift16, int sub_mul, int sub_acc1)
v16acc64 | msc_conv_16x4_conf (v32int16 a, v32uint16 b, v16acc64 acc1, int zero_acc1, int shift16, int sub_mul, int sub_acc1)
v16acc64 | negmsc_conv_16x4_conf (v32int16 a, v32uint16 b, v16acc64 acc1, int zero_acc1, int sub_mul, int sub_acc1)
v16acc64 | negmac_conv_16x4_conf (v32int16 a, v32uint16 b, v16acc64 acc1, int zero_acc1, int sub_mul, int sub_acc1)
v16acc64 | addmac_conv_16x4_conf (v32int16 a, v32uint16 b, v16acc64 acc1, v16acc64 acc2, int zero_acc1, int shift16, int sub_mul, int sub_acc1, int sub_acc2)
v16acc64 | addmsc_conv_16x4_conf (v32int16 a, v32uint16 b, v16acc64 acc1, v16acc64 acc2, int zero_acc1, int shift16, int sub_mul, int sub_acc1, int sub_acc2)
v16acc64 | submac_conv_16x4_conf (v32int16 a, v32uint16 b, v16acc64 acc1, v16acc64 acc2, int zero_acc1, int sub_mul, int sub_acc1, int sub_acc2)
v16acc64 | submsc_conv_16x4_conf (v32int16 a, v32uint16 b, v16acc64 acc1, v16acc64 acc2, int zero_acc1, int sub_mul, int sub_acc1, int sub_acc2)
v16acc64 | mac_conv_16x4_conf (v32int16 a, v32int16 b, v16acc64 acc1, int zero_acc1, int shift16, int sub_mul, int sub_acc1)
v16acc64 | msc_conv_16x4_conf (v32int16 a, v32int16 b, v16acc64 acc1, int zero_acc1, int shift16, int sub_mul, int sub_acc1)
v16acc64 | negmsc_conv_16x4_conf (v32int16 a, v32int16 b, v16acc64 acc1, int zero_acc1, int sub_mul, int sub_acc1)
v16acc64 | negmac_conv_16x4_conf (v32int16 a, v32int16 b, v16acc64 acc1, int zero_acc1, int sub_mul, int sub_acc1)
v16acc64 | addmac_conv_16x4_conf (v32int16 a, v32int16 b, v16acc64 acc1, v16acc64 acc2, int zero_acc1, int shift16, int sub_mul, int sub_acc1, int sub_acc2)
v16acc64 | addmsc_conv_16x4_conf (v32int16 a, v32int16 b, v16acc64 acc1, v16acc64 acc2, int zero_acc1, int shift16, int sub_mul, int sub_acc1, int sub_acc2)
v16acc64 | submac_conv_16x4_conf (v32int16 a, v32int16 b, v16acc64 acc1, v16acc64 acc2, int zero_acc1, int sub_mul, int sub_acc1, int sub_acc2)
v16acc64 | submsc_conv_16x4_conf (v32int16 a, v32int16 b, v16acc64 acc1, v16acc64 acc2, int zero_acc1, int sub_mul, int sub_acc1, int sub_acc2)

## Convolution of (16x4) matrix with (4x1) kernel with dynamic sign and dynamic negation of multiplication result
v16acc64 | mul_conv_16x4_conf (v32uint16 a, int sgn_x, v32uint16 b, int sgn_y, int sub_mul)
v16acc64 | negmul_conv_16x4_conf (v32uint16 a, int sgn_x, v32uint16 b, int sgn_y, int sub_mul)
v16acc64 | mac_conv_16x4_conf (v32uint16 a, int sgn_x, v32uint16 b, int sgn_y, v16acc64 acc1, int zero_acc1, int shift16, int sub_mul, int sub_acc1)
v16acc64 | msc_conv_16x4_conf (v32uint16 a, int sgn_x, v32uint16 b, int sgn_y, v16acc64 acc1, int zero_acc1, int shift16, int sub_mul, int sub_acc1)
v16acc64 | negmsc_conv_16x4_conf (v32uint16 a, int sgn_x, v32uint16 b, int sgn_y, v16acc64 acc1, int zero_acc1, int sub_mul, int sub_acc1)
v16acc64 | negmac_conv_16x4_conf (v32uint16 a, int sgn_x, v32uint16 b, int sgn_y, v16acc64 acc1, int zero_acc1, int sub_mul, int sub_acc1)
v16acc64 | addmac_conv_16x4_conf (v32uint16 a, int sgn_x, v32uint16 b, int sgn_y, v16acc64 acc1, v16acc64 acc2, int zero_acc1, int shift16, int sub_mul, int sub_acc1, int sub_acc2)
v16acc64 | addmsc_conv_16x4_conf (v32uint16 a, int sgn_x, v32uint16 b, int sgn_y, v16acc64 acc1, v16acc64 acc2, int zero_acc1, int shift16, int sub_mul, int sub_acc1, int sub_acc2)
v16acc64 | submac_conv_16x4_conf (v32uint16 a, int sgn_x, v32uint16 b, int sgn_y, v16acc64 acc1, v16acc64 acc2, int zero_acc1, int sub_mul, int sub_acc1, int sub_acc2)
v16acc64 | submsc_conv_16x4_conf (v32uint16 a, int sgn_x, v32uint16 b, int sgn_y, v16acc64 acc1, v16acc64 acc2, int zero_acc1, int sub_mul, int sub_acc1, int sub_acc2)
v16acc64 | mul_conv_16x4_conf (v32uint16 a, int sgn_x, v32int16 b, int sgn_y, int sub_mul)
v16acc64 | negmul_conv_16x4_conf (v32uint16 a, int sgn_x, v32int16 b, int sgn_y, int sub_mul)
v16acc64 | mac_conv_16x4_conf (v32uint16 a, int sgn_x, v32int16 b, int sgn_y, v16acc64 acc1, int zero_acc1, int shift16, int sub_mul, int sub_acc1)
v16acc64 | msc_conv_16x4_conf (v32uint16 a, int sgn_x, v32int16 b, int sgn_y, v16acc64 acc1, int zero_acc1, int shift16, int sub_mul, int sub_acc1)
v16acc64 | negmsc_conv_16x4_conf (v32uint16 a, int sgn_x, v32int16 b, int sgn_y, v16acc64 acc1, int zero_acc1, int sub_mul, int sub_acc1)
v16acc64 | negmac_conv_16x4_conf (v32uint16 a, int sgn_x, v32int16 b, int sgn_y, v16acc64 acc1, int zero_acc1, int sub_mul, int sub_acc1)
v16acc64 | addmac_conv_16x4_conf (v32uint16 a, int sgn_x, v32int16 b, int sgn_y, v16acc64 acc1, v16acc64 acc2, int zero_acc1, int shift16, int sub_mul, int sub_acc1, int sub_acc2)
v16acc64 | addmsc_conv_16x4_conf (v32uint16 a, int sgn_x, v32int16 b, int sgn_y, v16acc64 acc1, v16acc64 acc2, int zero_acc1, int shift16, int sub_mul, int sub_acc1, int sub_acc2)
v16acc64 | submac_conv_16x4_conf (v32uint16 a, int sgn_x, v32int16 b, int sgn_y, v16acc64 acc1, v16acc64 acc2, int zero_acc1, int sub_mul, int sub_acc1, int sub_acc2)
v16acc64 | submsc_conv_16x4_conf (v32uint16 a, int sgn_x, v32int16 b, int sgn_y, v16acc64 acc1, v16acc64 acc2, int zero_acc1, int sub_mul, int sub_acc1, int sub_acc2)
v16acc64 | mul_conv_16x4_conf (v32int16 a, int sgn_x, v32uint16 b, int sgn_y, int sub_mul)
v16acc64 | negmul_conv_16x4_conf (v32int16 a, int sgn_x, v32uint16 b, int sgn_y, int sub_mul)
v16acc64 | mac_conv_16x4_conf (v32int16 a, int sgn_x, v32uint16 b, int sgn_y, v16acc64 acc1, int zero_acc1, int shift16, int sub_mul, int sub_acc1)
v16acc64 | msc_conv_16x4_conf (v32int16 a, int sgn_x, v32uint16 b, int sgn_y, v16acc64 acc1, int zero_acc1, int shift16, int sub_mul, int sub_acc1)
v16acc64 | negmsc_conv_16x4_conf (v32int16 a, int sgn_x, v32uint16 b, int sgn_y, v16acc64 acc1, int zero_acc1, int sub_mul, int sub_acc1)
v16acc64 | negmac_conv_16x4_conf (v32int16 a, int sgn_x, v32uint16 b, int sgn_y, v16acc64 acc1, int zero_acc1, int sub_mul, int sub_acc1)
v16acc64 | addmac_conv_16x4_conf (v32int16 a, int sgn_x, v32uint16 b, int sgn_y, v16acc64 acc1, v16acc64 acc2, int zero_acc1, int shift16, int sub_mul, int sub_acc1, int sub_acc2)
v16acc64 | addmsc_conv_16x4_conf (v32int16 a, int sgn_x, v32uint16 b, int sgn_y, v16acc64 acc1, v16acc64 acc2, int zero_acc1, int shift16, int sub_mul, int sub_acc1, int sub_acc2)
v16acc64 | submac_conv_16x4_conf (v32int16 a, int sgn_x, v32uint16 b, int sgn_y, v16acc64 acc1, v16acc64 acc2, int zero_acc1, int sub_mul, int sub_acc1, int sub_acc2)
v16acc64 | submsc_conv_16x4_conf (v32int16 a, int sgn_x, v32uint16 b, int sgn_y, v16acc64 acc1, v16acc64 acc2, int zero_acc1, int sub_mul, int sub_acc1, int sub_acc2)
v16acc64 | mul_conv_16x4_conf (v32int16 a, int sgn_x, v32int16 b, int sgn_y, int sub_mul)
v16acc64 | negmul_conv_16x4_conf (v32int16 a, int sgn_x, v32int16 b, int sgn_y, int sub_mul)
v16acc64 | mac_conv_16x4_conf (v32int16 a, int sgn_x, v32int16 b, int sgn_y, v16acc64 acc1, int zero_acc1, int shift16, int sub_mul, int sub_acc1)
v16acc64 | msc_conv_16x4_conf (v32int16 a, int sgn_x, v32int16 b, int sgn_y, v16acc64 acc1, int zero_acc1, int shift16, int sub_mul, int sub_acc1)
v16acc64 | negmsc_conv_16x4_conf (v32int16 a, int sgn_x, v32int16 b, int sgn_y, v16acc64 acc1, int zero_acc1, int sub_mul, int sub_acc1)
v16acc64 | negmac_conv_16x4_conf (v32int16 a, int sgn_x, v32int16 b, int sgn_y, v16acc64 acc1, int zero_acc1, int sub_mul, int sub_acc1)
v16acc64 | addmac_conv_16x4_conf (v32int16 a, int sgn_x, v32int16 b, int sgn_y, v16acc64 acc1, v16acc64 acc2, int zero_acc1, int shift16, int sub_mul, int sub_acc1, int sub_acc2)
v16acc64 | addmsc_conv_16x4_conf (v32int16 a, int sgn_x, v32int16 b, int sgn_y, v16acc64 acc1, v16acc64 acc2, int zero_acc1, int shift16, int sub_mul, int sub_acc1, int sub_acc2)
v16acc64 | submac_conv_16x4_conf (v32int16 a, int sgn_x, v32int16 b, int sgn_y, v16acc64 acc1, v16acc64 acc2, int zero_acc1, int sub_mul, int sub_acc1, int sub_acc2)
v16acc64 | submsc_conv_16x4_conf (v32int16 a, int sgn_x, v32int16 b, int sgn_y, v16acc64 acc1, v16acc64 acc2, int zero_acc1, int sub_mul, int sub_acc1, int sub_acc2)

## Function Documentation

## ◆ addmac_2x4_4x8() [1/8]

v16acc64 addmac_2x4_4x8 | ( | v32int16 | a,
|  | int | sgn_x,
|  | v32int16 | b,
|  | int | sgn_y,
|  | v16acc64 | acc1,
|  | v16acc64 | acc2 )

Parameters

  a | Matrix A
  sgn_x | Sign mask for matrix A
  b | Matrix B
  sgn_y | Sign mask for matrix B
  acc1 | Accumulator 1 input
  acc2 | Accumulator 2 input

Returns
  Result of operation

## ◆ addmac_2x4_4x8() [2/8]

v16acc64 addmac_2x4_4x8 | ( | v32int16 | a,
|  | int | sgn_x,
|  | v32uint16 | b,
|  | int | sgn_y,
|  | v16acc64 | acc1,
|  | v16acc64 | acc2 )

Parameters

  a | Matrix A
  sgn_x | Sign mask for matrix A
  b | Matrix B
  sgn_y | Sign mask for matrix B
  acc1 | Accumulator 1 input
  acc2 | Accumulator 2 input

Returns
  Result of operation

## ◆ addmac_2x4_4x8() [3/8]

v16acc64 addmac_2x4_4x8 | ( | v32int16 | a,
|  | v32int16 | b,
|  | v16acc64 | acc1,
|  | v16acc64 | acc2 )

Parameters

  a | Matrix A
  b | Matrix B
  acc1 | Accumulator 1 input
  acc2 | Accumulator 2 input

Returns
  Result of operation

## ◆ addmac_2x4_4x8() [4/8]

v16acc64 addmac_2x4_4x8 | ( | v32int16 | a,
|  | v32uint16 | b,
|  | v16acc64 | acc1,
|  | v16acc64 | acc2 )

Parameters

  a | Matrix A
  b | Matrix B
  acc1 | Accumulator 1 input
  acc2 | Accumulator 2 input

Returns
  Result of operation

## ◆ addmac_2x4_4x8() [5/8]

v16acc64 addmac_2x4_4x8 | ( | v32uint16 | a,
|  | int | sgn_x,
|  | v32int16 | b,
|  | int | sgn_y,
|  | v16acc64 | acc1,
|  | v16acc64 | acc2 )

Parameters

  a | Matrix A
  sgn_x | Sign mask for matrix A
  b | Matrix B
  sgn_y | Sign mask for matrix B
  acc1 | Accumulator 1 input
  acc2 | Accumulator 2 input

Returns
  Result of operation

## ◆ addmac_2x4_4x8() [6/8]

v16acc64 addmac_2x4_4x8 | ( | v32uint16 | a,
|  | int | sgn_x,
|  | v32uint16 | b,
|  | int | sgn_y,
|  | v16acc64 | acc1,
|  | v16acc64 | acc2 )

Parameters

  a | Matrix A
  sgn_x | Sign mask for matrix A
  b | Matrix B
  sgn_y | Sign mask for matrix B
  acc1 | Accumulator 1 input
  acc2 | Accumulator 2 input

Returns
  Result of operation

## ◆ addmac_2x4_4x8() [7/8]

v16acc64 addmac_2x4_4x8 | ( | v32uint16 | a,
|  | v32int16 | b,
|  | v16acc64 | acc1,
|  | v16acc64 | acc2 )

Parameters

  a | Matrix A
  b | Matrix B
  acc1 | Accumulator 1 input
  acc2 | Accumulator 2 input

Returns
  Result of operation

## ◆ addmac_2x4_4x8() [8/8]

v16acc64 addmac_2x4_4x8 | ( | v32uint16 | a,
|  | v32uint16 | b,
|  | v16acc64 | acc1,
|  | v16acc64 | acc2 )

Parameters

  a | Matrix A
  b | Matrix B
  acc1 | Accumulator 1 input
  acc2 | Accumulator 2 input

Returns
  Result of operation

## ◆ addmac_2x4_4x8_conf() [1/8]

v16acc64 addmac_2x4_4x8_conf | ( | v32int16 | a,
|  | int | sgn_x,
|  | v32int16 | b,
|  | int | sgn_y,
|  | v16acc64 | acc1,
|  | v16acc64 | acc2,
|  | int | zero_acc1,
|  | int | shift16,
|  | int | sub_mul,
|  | int | sub_acc1,
|  | int | sub_acc2 )

Parameters

  a | Matrix A
  sgn_x | Sign mask for matrix A
  b | Matrix B
  sgn_y | Sign mask for matrix B
  acc1 | Accumulator 1 input
  acc2 | Accumulator 2 input
  zero_acc1 | Zeroing mask for acc1
  shift16 | Shift mask of input accumulator acc1
  sub_mul | Negation mask of multiplication result
  sub_acc1 | Negation mask of acc1
  sub_acc2 | Negation mask of acc2

Returns
  Result of operation

## ◆ addmac_2x4_4x8_conf() [2/8]

v16acc64 addmac_2x4_4x8_conf | ( | v32int16 | a,
|  | int | sgn_x,
|  | v32uint16 | b,
|  | int | sgn_y,
|  | v16acc64 | acc1,
|  | v16acc64 | acc2,
|  | int | zero_acc1,
|  | int | shift16,
|  | int | sub_mul,
|  | int | sub_acc1,
|  | int | sub_acc2 )

Parameters

  a | Matrix A
  sgn_x | Sign mask for matrix A
  b | Matrix B
  sgn_y | Sign mask for matrix B
  acc1 | Accumulator 1 input
  acc2 | Accumulator 2 input
  zero_acc1 | Zeroing mask for acc1
  shift16 | Shift mask of input accumulator acc1
  sub_mul | Negation mask of multiplication result
  sub_acc1 | Negation mask of acc1
  sub_acc2 | Negation mask of acc2

Returns
  Result of operation

## ◆ addmac_2x4_4x8_conf() [3/8]

v16acc64 addmac_2x4_4x8_conf | ( | v32int16 | a,
|  | v32int16 | b,
|  | v16acc64 | acc1,
|  | v16acc64 | acc2,
|  | int | zero_acc1,
|  | int | shift16,
|  | int | sub_mul,
|  | int | sub_acc1,
|  | int | sub_acc2 )

Parameters

  a | Matrix A
  b | Matrix B
  acc1 | Accumulator 1 input
  acc2 | Accumulator 2 input
  zero_acc1 | Zeroing mask for acc1
  shift16 | Shift mask of input accumulator acc1
  sub_mul | Negation mask of multiplication result
  sub_acc1 | Negation mask of acc1
  sub_acc2 | Negation mask of acc2

Returns
  Result of operation

## ◆ addmac_2x4_4x8_conf() [4/8]

v16acc64 addmac_2x4_4x8_conf | ( | v32int16 | a,
|  | v32uint16 | b,
|  | v16acc64 | acc1,
|  | v16acc64 | acc2,
|  | int | zero_acc1,
|  | int | shift16,
|  | int | sub_mul,
|  | int | sub_acc1,
|  | int | sub_acc2 )

Parameters

  a | Matrix A
  b | Matrix B
  acc1 | Accumulator 1 input
  acc2 | Accumulator 2 input
  zero_acc1 | Zeroing mask for acc1
  shift16 | Shift mask of input accumulator acc1
  sub_mul | Negation mask of multiplication result
  sub_acc1 | Negation mask of acc1
  sub_acc2 | Negation mask of acc2

Returns
  Result of operation

## ◆ addmac_2x4_4x8_conf() [5/8]

v16acc64 addmac_2x4_4x8_conf | ( | v32uint16 | a,
|  | int | sgn_x,
|  | v32int16 | b,
|  | int | sgn_y,
|  | v16acc64 | acc1,
|  | v16acc64 | acc2,
|  | int | zero_acc1,
|  | int | shift16,
|  | int | sub_mul,
|  | int | sub_acc1,
|  | int | sub_acc2 )

Parameters

  a | Matrix A
  sgn_x | Sign mask for matrix A
  b | Matrix B
  sgn_y | Sign mask for matrix B
  acc1 | Accumulator 1 input
  acc2 | Accumulator 2 input
  zero_acc1 | Zeroing mask for acc1
  shift16 | Shift mask of input accumulator acc1
  sub_mul | Negation mask of multiplication result
  sub_acc1 | Negation mask of acc1
  sub_acc2 | Negation mask of acc2

Returns
  Result of operation

## ◆ addmac_2x4_4x8_conf() [6/8]

v16acc64 addmac_2x4_4x8_conf | ( | v32uint16 | a,
|  | int | sgn_x,
|  | v32uint16 | b,
|  | int | sgn_y,
|  | v16acc64 | acc1,
|  | v16acc64 | acc2,
|  | int | zero_acc1,
|  | int | shift16,
|  | int | sub_mul,
|  | int | sub_acc1,
|  | int | sub_acc2 )

Parameters

  a | Matrix A
  sgn_x | Sign mask for matrix A
  b | Matrix B
  sgn_y | Sign mask for matrix B
  acc1 | Accumulator 1 input
  acc2 | Accumulator 2 input
  zero_acc1 | Zeroing mask for acc1
  shift16 | Shift mask of input accumulator acc1
  sub_mul | Negation mask of multiplication result
  sub_acc1 | Negation mask of acc1
  sub_acc2 | Negation mask of acc2

Returns
  Result of operation

## ◆ addmac_2x4_4x8_conf() [7/8]

v16acc64 addmac_2x4_4x8_conf | ( | v32uint16 | a,
|  | v32int16 | b,
|  | v16acc64 | acc1,
|  | v16acc64 | acc2,
|  | int | zero_acc1,
|  | int | shift16,
|  | int | sub_mul,
|  | int | sub_acc1,
|  | int | sub_acc2 )

Parameters

  a | Matrix A
  b | Matrix B
  acc1 | Accumulator 1 input
  acc2 | Accumulator 2 input
  zero_acc1 | Zeroing mask for acc1
  shift16 | Shift mask of input accumulator acc1
  sub_mul | Negation mask of multiplication result
  sub_acc1 | Negation mask of acc1
  sub_acc2 | Negation mask of acc2

Returns
  Result of operation

## ◆ addmac_2x4_4x8_conf() [8/8]

v16acc64 addmac_2x4_4x8_conf | ( | v32uint16 | a,
|  | v32uint16 | b,
|  | v16acc64 | acc1,
|  | v16acc64 | acc2,
|  | int | zero_acc1,
|  | int | shift16,
|  | int | sub_mul,
|  | int | sub_acc1,
|  | int | sub_acc2 )

Parameters

  a | Matrix A
  b | Matrix B
  acc1 | Accumulator 1 input
  acc2 | Accumulator 2 input
  zero_acc1 | Zeroing mask for acc1
  shift16 | Shift mask of input accumulator acc1
  sub_mul | Negation mask of multiplication result
  sub_acc1 | Negation mask of acc1
  sub_acc2 | Negation mask of acc2

Returns
  Result of operation

## ◆ addmac_4x2_2x8() [1/8]

v32acc32 addmac_4x2_2x8 | ( | v32int16 | a,
|  | int | sgn_x,
|  | v32int16 | b,
|  | int | sgn_y,
|  | v32acc32 | acc1,
|  | v32acc32 | acc2 )

Parameters

  a | Matrix A
  sgn_x | Sign mask for matrix A
  b | Matrix B
  sgn_y | Sign mask for matrix B
  acc1 | Accumulator 1 input
  acc2 | Accumulator 2 input

Returns
  Result of operation

## ◆ addmac_4x2_2x8() [2/8]

v32acc32 addmac_4x2_2x8 | ( | v32int16 | a,
|  | int | sgn_x,
|  | v32uint16 | b,
|  | int | sgn_y,
|  | v32acc32 | acc1,
|  | v32acc32 | acc2 )

Parameters

  a | Matrix A
  sgn_x | Sign mask for matrix A
  b | Matrix B
  sgn_y | Sign mask for matrix B
  acc1 | Accumulator 1 input
  acc2 | Accumulator 2 input

Returns
  Result of operation

## ◆ addmac_4x2_2x8() [3/8]

v32acc32 addmac_4x2_2x8 | ( | v32int16 | a,
|  | v32int16 | b,
|  | v32acc32 | acc1,
|  | v32acc32 | acc2 )

Parameters

  a | Matrix A
  b | Matrix B
  acc1 | Accumulator 1 input
  acc2 | Accumulator 2 input

Returns
  Result of operation

## ◆ addmac_4x2_2x8() [4/8]

v32acc32 addmac_4x2_2x8 | ( | v32int16 | a,
|  | v32uint16 | b,
|  | v32acc32 | acc1,
|  | v32acc32 | acc2 )

Parameters

  a | Matrix A
  b | Matrix B
  acc1 | Accumulator 1 input
  acc2 | Accumulator 2 input

Returns
  Result of operation

## ◆ addmac_4x2_2x8() [5/8]

v32acc32 addmac_4x2_2x8 | ( | v32uint16 | a,
|  | int | sgn_x,
|  | v32int16 | b,
|  | int | sgn_y,
|  | v32acc32 | acc1,
|  | v32acc32 | acc2 )

Parameters

  a | Matrix A
  sgn_x | Sign mask for matrix A
  b | Matrix B
  sgn_y | Sign mask for matrix B
  acc1 | Accumulator 1 input
  acc2 | Accumulator 2 input

Returns
  Result of operation

## ◆ addmac_4x2_2x8() [6/8]

v32acc32 addmac_4x2_2x8 | ( | v32uint16 | a,
|  | int | sgn_x,
|  | v32uint16 | b,
|  | int | sgn_y,
|  | v32acc32 | acc1,
|  | v32acc32 | acc2 )

Parameters

  a | Matrix A
  sgn_x | Sign mask for matrix A
  b | Matrix B
  sgn_y | Sign mask for matrix B
  acc1 | Accumulator 1 input
  acc2 | Accumulator 2 input

Returns
  Result of operation

## ◆ addmac_4x2_2x8() [7/8]

v32acc32 addmac_4x2_2x8 | ( | v32uint16 | a,
|  | v32int16 | b,
|  | v32acc32 | acc1,
|  | v32acc32 | acc2 )

Parameters

  a | Matrix A
  b | Matrix B
  acc1 | Accumulator 1 input
  acc2 | Accumulator 2 input

Returns
  Result of operation

## ◆ addmac_4x2_2x8() [8/8]

v32acc32 addmac_4x2_2x8 | ( | v32uint16 | a,
|  | v32uint16 | b,
|  | v32acc32 | acc1,
|  | v32acc32 | acc2 )

Parameters

  a | Matrix A
  b | Matrix B
  acc1 | Accumulator 1 input
  acc2 | Accumulator 2 input

Returns
  Result of operation

## ◆ addmac_4x2_2x8_conf() [1/8]

v32acc32 addmac_4x2_2x8_conf | ( | v32int16 | a,
|  | int | sgn_x,
|  | v32int16 | b,
|  | int | sgn_y,
|  | v32acc32 | acc1,
|  | v32acc32 | acc2,
|  | int | zero_acc1,
|  | int | shift16,
|  | int | sub_mul,
|  | int | sub_acc1,
|  | int | sub_acc2 )

Parameters

  a | Matrix A
  sgn_x | Sign mask for matrix A
  b | Matrix B
  sgn_y | Sign mask for matrix B
  acc1 | Accumulator 1 input
  acc2 | Accumulator 2 input
  zero_acc1 | Zeroing mask for acc1
  shift16 | Shift mask of input accumulator acc1
  sub_mul | Negation mask of multiplication result
  sub_acc1 | Negation mask of acc1
  sub_acc2 | Negation mask of acc2

Returns
  Result of operation

## ◆ addmac_4x2_2x8_conf() [2/8]

v32acc32 addmac_4x2_2x8_conf | ( | v32int16 | a,
|  | int | sgn_x,
|  | v32uint16 | b,
|  | int | sgn_y,
|  | v32acc32 | acc1,
|  | v32acc32 | acc2,
|  | int | zero_acc1,
|  | int | shift16,
|  | int | sub_mul,
|  | int | sub_acc1,
|  | int | sub_acc2 )

Parameters

  a | Matrix A
  sgn_x | Sign mask for matrix A
  b | Matrix B
  sgn_y | Sign mask for matrix B
  acc1 | Accumulator 1 input
  acc2 | Accumulator 2 input
  zero_acc1 | Zeroing mask for acc1
  shift16 | Shift mask of input accumulator acc1
  sub_mul | Negation mask of multiplication result
  sub_acc1 | Negation mask of acc1
  sub_acc2 | Negation mask of acc2

Returns
  Result of operation

## ◆ addmac_4x2_2x8_conf() [3/8]

v32acc32 addmac_4x2_2x8_conf | ( | v32int16 | a,
|  | v32int16 | b,
|  | v32acc32 | acc1,
|  | v32acc32 | acc2,
|  | int | zero_acc1,
|  | int | shift16,
|  | int | sub_mul,
|  | int | sub_acc1,
|  | int | sub_acc2 )

Parameters

  a | Matrix A
  b | Matrix B
  acc1 | Accumulator 1 input
  acc2 | Accumulator 2 input
  zero_acc1 | Zeroing mask for acc1
  shift16 | Shift mask of input accumulator acc1
  sub_mul | Negation mask of multiplication result
  sub_acc1 | Negation mask of acc1
  sub_acc2 | Negation mask of acc2

Returns
  Result of operation

## ◆ addmac_4x2_2x8_conf() [4/8]

v32acc32 addmac_4x2_2x8_conf | ( | v32int16 | a,
|  | v32uint16 | b,
|  | v32acc32 | acc1,
|  | v32acc32 | acc2,
|  | int | zero_acc1,
|  | int | shift16,
|  | int | sub_mul,
|  | int | sub_acc1,
|  | int | sub_acc2 )

Parameters

  a | Matrix A
  b | Matrix B
  acc1 | Accumulator 1 input
  acc2 | Accumulator 2 input
  zero_acc1 | Zeroing mask for acc1
  shift16 | Shift mask of input accumulator acc1
  sub_mul | Negation mask of multiplication result
  sub_acc1 | Negation mask of acc1
  sub_acc2 | Negation mask of acc2

Returns
  Result of operation

## ◆ addmac_4x2_2x8_conf() [5/8]

v32acc32 addmac_4x2_2x8_conf | ( | v32uint16 | a,
|  | int | sgn_x,
|  | v32int16 | b,
|  | int | sgn_y,
|  | v32acc32 | acc1,
|  | v32acc32 | acc2,
|  | int | zero_acc1,
|  | int | shift16,
|  | int | sub_mul,
|  | int | sub_acc1,
|  | int | sub_acc2 )

Parameters

  a | Matrix A
  sgn_x | Sign mask for matrix A
  b | Matrix B
  sgn_y | Sign mask for matrix B
  acc1 | Accumulator 1 input
  acc2 | Accumulator 2 input
  zero_acc1 | Zeroing mask for acc1
  shift16 | Shift mask of input accumulator acc1
  sub_mul | Negation mask of multiplication result
  sub_acc1 | Negation mask of acc1
  sub_acc2 | Negation mask of acc2

Returns
  Result of operation

## ◆ addmac_4x2_2x8_conf() [6/8]

v32acc32 addmac_4x2_2x8_conf | ( | v32uint16 | a,
|  | int | sgn_x,
|  | v32uint16 | b,
|  | int | sgn_y,
|  | v32acc32 | acc1,
|  | v32acc32 | acc2,
|  | int | zero_acc1,
|  | int | shift16,
|  | int | sub_mul,
|  | int | sub_acc1,
|  | int | sub_acc2 )

Parameters

  a | Matrix A
  sgn_x | Sign mask for matrix A
  b | Matrix B
  sgn_y | Sign mask for matrix B
  acc1 | Accumulator 1 input
  acc2 | Accumulator 2 input
  zero_acc1 | Zeroing mask for acc1
  shift16 | Shift mask of input accumulator acc1
  sub_mul | Negation mask of multiplication result
  sub_acc1 | Negation mask of acc1
  sub_acc2 | Negation mask of acc2

Returns
  Result of operation

## ◆ addmac_4x2_2x8_conf() [7/8]

v32acc32 addmac_4x2_2x8_conf | ( | v32uint16 | a,
|  | v32int16 | b,
|  | v32acc32 | acc1,
|  | v32acc32 | acc2,
|  | int | zero_acc1,
|  | int | shift16,
|  | int | sub_mul,
|  | int | sub_acc1,
|  | int | sub_acc2 )

Parameters

  a | Matrix A
  b | Matrix B
  acc1 | Accumulator 1 input
  acc2 | Accumulator 2 input
  zero_acc1 | Zeroing mask for acc1
  shift16 | Shift mask of input accumulator acc1
  sub_mul | Negation mask of multiplication result
  sub_acc1 | Negation mask of acc1
  sub_acc2 | Negation mask of acc2

Returns
  Result of operation

## ◆ addmac_4x2_2x8_conf() [8/8]

v32acc32 addmac_4x2_2x8_conf | ( | v32uint16 | a,
|  | v32uint16 | b,
|  | v32acc32 | acc1,
|  | v32acc32 | acc2,
|  | int | zero_acc1,
|  | int | shift16,
|  | int | sub_mul,
|  | int | sub_acc1,
|  | int | sub_acc2 )

Parameters

  a | Matrix A
  b | Matrix B
  acc1 | Accumulator 1 input
  acc2 | Accumulator 2 input
  zero_acc1 | Zeroing mask for acc1
  shift16 | Shift mask of input accumulator acc1
  sub_mul | Negation mask of multiplication result
  sub_acc1 | Negation mask of acc1
  sub_acc2 | Negation mask of acc2

Returns
  Result of operation

## ◆ addmac_4x4_4x4() [1/8]

v16acc64 addmac_4x4_4x4 | ( | v32int16 | a,
|  | int | sgn_x,
|  | v32int16 | b,
|  | int | sgn_y,
|  | v16acc64 | acc1,
|  | v16acc64 | acc2 )

Parameters

  a | Matrix A
  sgn_x | Sign mask for matrix A
  b | Matrix B
  sgn_y | Sign mask for matrix B
  acc1 | Accumulator 1 input
  acc2 | Accumulator 2 input

Returns
  Result of operation

## ◆ addmac_4x4_4x4() [2/8]

v16acc64 addmac_4x4_4x4 | ( | v32int16 | a,
|  | int | sgn_x,
|  | v32uint16 | b,
|  | int | sgn_y,
|  | v16acc64 | acc1,
|  | v16acc64 | acc2 )

Parameters

  a | Matrix A
  sgn_x | Sign mask for matrix A
  b | Matrix B
  sgn_y | Sign mask for matrix B
  acc1 | Accumulator 1 input
  acc2 | Accumulator 2 input

Returns
  Result of operation

## ◆ addmac_4x4_4x4() [3/8]

v16acc64 addmac_4x4_4x4 | ( | v32int16 | a,
|  | v32int16 | b,
|  | v16acc64 | acc1,
|  | v16acc64 | acc2 )

Parameters

  a | Matrix A
  b | Matrix B
  acc1 | Accumulator 1 input
  acc2 | Accumulator 2 input

Returns
  Result of operation

## ◆ addmac_4x4_4x4() [4/8]

v16acc64 addmac_4x4_4x4 | ( | v32int16 | a,
|  | v32uint16 | b,
|  | v16acc64 | acc1,
|  | v16acc64 | acc2 )

Parameters

  a | Matrix A
  b | Matrix B
  acc1 | Accumulator 1 input
  acc2 | Accumulator 2 input

Returns
  Result of operation

## ◆ addmac_4x4_4x4() [5/8]

v16acc64 addmac_4x4_4x4 | ( | v32uint16 | a,
|  | int | sgn_x,
|  | v32int16 | b,
|  | int | sgn_y,
|  | v16acc64 | acc1,
|  | v16acc64 | acc2 )

Parameters

  a | Matrix A
  sgn_x | Sign mask for matrix A
  b | Matrix B
  sgn_y | Sign mask for matrix B
  acc1 | Accumulator 1 input
  acc2 | Accumulator 2 input

Returns
  Result of operation

## ◆ addmac_4x4_4x4() [6/8]

v16acc64 addmac_4x4_4x4 | ( | v32uint16 | a,
|  | int | sgn_x,
|  | v32uint16 | b,
|  | int | sgn_y,
|  | v16acc64 | acc1,
|  | v16acc64 | acc2 )

Parameters

  a | Matrix A
  sgn_x | Sign mask for matrix A
  b | Matrix B
  sgn_y | Sign mask for matrix B
  acc1 | Accumulator 1 input
  acc2 | Accumulator 2 input

Returns
  Result of operation

## ◆ addmac_4x4_4x4() [7/8]

v16acc64 addmac_4x4_4x4 | ( | v32uint16 | a,
|  | v32int16 | b,
|  | v16acc64 | acc1,
|  | v16acc64 | acc2 )

Parameters

  a | Matrix A
  b | Matrix B
  acc1 | Accumulator 1 input
  acc2 | Accumulator 2 input

Returns
  Result of operation

## ◆ addmac_4x4_4x4() [8/8]

v16acc64 addmac_4x4_4x4 | ( | v32uint16 | a,
|  | v32uint16 | b,
|  | v16acc64 | acc1,
|  | v16acc64 | acc2 )

Parameters

  a | Matrix A
  b | Matrix B
  acc1 | Accumulator 1 input
  acc2 | Accumulator 2 input

Returns
  Result of operation

## ◆ addmac_4x4_4x4_conf() [1/8]

v16acc64 addmac_4x4_4x4_conf | ( | v32int16 | a,
|  | int | sgn_x,
|  | v32int16 | b,
|  | int | sgn_y,
|  | v16acc64 | acc1,
|  | v16acc64 | acc2,
|  | int | zero_acc1,
|  | int | shift16,
|  | int | sub_mul,
|  | int | sub_acc1,
|  | int | sub_acc2 )

Parameters

  a | Matrix A
  sgn_x | Sign mask for matrix A
  b | Matrix B
  sgn_y | Sign mask for matrix B
  acc1 | Accumulator 1 input
  acc2 | Accumulator 2 input
  zero_acc1 | Zeroing mask for acc1
  shift16 | Shift mask of input accumulator acc1
  sub_mul | Negation mask of multiplication result
  sub_acc1 | Negation mask of acc1
  sub_acc2 | Negation mask of acc2

Returns
  Result of operation

## ◆ addmac_4x4_4x4_conf() [2/8]

v16acc64 addmac_4x4_4x4_conf | ( | v32int16 | a,
|  | int | sgn_x,
|  | v32uint16 | b,
|  | int | sgn_y,
|  | v16acc64 | acc1,
|  | v16acc64 | acc2,
|  | int | zero_acc1,
|  | int | shift16,
|  | int | sub_mul,
|  | int | sub_acc1,
|  | int | sub_acc2 )

Parameters

  a | Matrix A
  sgn_x | Sign mask for matrix A
  b | Matrix B
  sgn_y | Sign mask for matrix B
  acc1 | Accumulator 1 input
  acc2 | Accumulator 2 input
  zero_acc1 | Zeroing mask for acc1
  shift16 | Shift mask of input accumulator acc1
  sub_mul | Negation mask of multiplication result
  sub_acc1 | Negation mask of acc1
  sub_acc2 | Negation mask of acc2

Returns
  Result of operation

## ◆ addmac_4x4_4x4_conf() [3/8]

v16acc64 addmac_4x4_4x4_conf | ( | v32int16 | a,
|  | v32int16 | b,
|  | v16acc64 | acc1,
|  | v16acc64 | acc2,
|  | int | zero_acc1,
|  | int | shift16,
|  | int | sub_mul,
|  | int | sub_acc1,
|  | int | sub_acc2 )

Parameters

  a | Matrix A
  b | Matrix B
  acc1 | Accumulator 1 input
  acc2 | Accumulator 2 input
  zero_acc1 | Zeroing mask for acc1
  shift16 | Shift mask of input accumulator acc1
  sub_mul | Negation mask of multiplication result
  sub_acc1 | Negation mask of acc1
  sub_acc2 | Negation mask of acc2

Returns
  Result of operation

## ◆ addmac_4x4_4x4_conf() [4/8]

v16acc64 addmac_4x4_4x4_conf | ( | v32int16 | a,
|  | v32uint16 | b,
|  | v16acc64 | acc1,
|  | v16acc64 | acc2,
|  | int | zero_acc1,
|  | int | shift16,
|  | int | sub_mul,
|  | int | sub_acc1,
|  | int | sub_acc2 )

Parameters

  a | Matrix A
  b | Matrix B
  acc1 | Accumulator 1 input
  acc2 | Accumulator 2 input
  zero_acc1 | Zeroing mask for acc1
  shift16 | Shift mask of input accumulator acc1
  sub_mul | Negation mask of multiplication result
  sub_acc1 | Negation mask of acc1
  sub_acc2 | Negation mask of acc2

Returns
  Result of operation

## ◆ addmac_4x4_4x4_conf() [5/8]

v16acc64 addmac_4x4_4x4_conf | ( | v32uint16 | a,
|  | int | sgn_x,
|  | v32int16 | b,
|  | int | sgn_y,
|  | v16acc64 | acc1,
|  | v16acc64 | acc2,
|  | int | zero_acc1,
|  | int | shift16,
|  | int | sub_mul,
|  | int | sub_acc1,
|  | int | sub_acc2 )

Parameters

  a | Matrix A
  sgn_x | Sign mask for matrix A
  b | Matrix B
  sgn_y | Sign mask for matrix B
  acc1 | Accumulator 1 input
  acc2 | Accumulator 2 input
  zero_acc1 | Zeroing mask for acc1
  shift16 | Shift mask of input accumulator acc1
  sub_mul | Negation mask of multiplication result
  sub_acc1 | Negation mask of acc1
  sub_acc2 | Negation mask of acc2

Returns
  Result of operation

## ◆ addmac_4x4_4x4_conf() [6/8]

v16acc64 addmac_4x4_4x4_conf | ( | v32uint16 | a,
|  | int | sgn_x,
|  | v32uint16 | b,
|  | int | sgn_y,
|  | v16acc64 | acc1,
|  | v16acc64 | acc2,
|  | int | zero_acc1,
|  | int | shift16,
|  | int | sub_mul,
|  | int | sub_acc1,
|  | int | sub_acc2 )

Parameters

  a | Matrix A
  sgn_x | Sign mask for matrix A
  b | Matrix B
  sgn_y | Sign mask for matrix B
  acc1 | Accumulator 1 input
  acc2 | Accumulator 2 input
  zero_acc1 | Zeroing mask for acc1
  shift16 | Shift mask of input accumulator acc1
  sub_mul | Negation mask of multiplication result
  sub_acc1 | Negation mask of acc1
  sub_acc2 | Negation mask of acc2

Returns
  Result of operation

## ◆ addmac_4x4_4x4_conf() [7/8]

v16acc64 addmac_4x4_4x4_conf | ( | v32uint16 | a,
|  | v32int16 | b,
|  | v16acc64 | acc1,
|  | v16acc64 | acc2,
|  | int | zero_acc1,
|  | int | shift16,
|  | int | sub_mul,
|  | int | sub_acc1,
|  | int | sub_acc2 )

Parameters

  a | Matrix A
  b | Matrix B
  acc1 | Accumulator 1 input
  acc2 | Accumulator 2 input
  zero_acc1 | Zeroing mask for acc1
  shift16 | Shift mask of input accumulator acc1
  sub_mul | Negation mask of multiplication result
  sub_acc1 | Negation mask of acc1
  sub_acc2 | Negation mask of acc2

Returns
  Result of operation

## ◆ addmac_4x4_4x4_conf() [8/8]

v16acc64 addmac_4x4_4x4_conf | ( | v32uint16 | a,
|  | v32uint16 | b,
|  | v16acc64 | acc1,
|  | v16acc64 | acc2,
|  | int | zero_acc1,
|  | int | shift16,
|  | int | sub_mul,
|  | int | sub_acc1,
|  | int | sub_acc2 )

Parameters

  a | Matrix A
  b | Matrix B
  acc1 | Accumulator 1 input
  acc2 | Accumulator 2 input
  zero_acc1 | Zeroing mask for acc1
  shift16 | Shift mask of input accumulator acc1
  sub_mul | Negation mask of multiplication result
  sub_acc1 | Negation mask of acc1
  sub_acc2 | Negation mask of acc2

Returns
  Result of operation

## ◆ addmac_conv_16x4() [1/8]

v16acc64 addmac_conv_16x4 | ( | v32int16 | a,
|  | int | sgn_x,
|  | v32int16 | b,
|  | int | sgn_y,
|  | v16acc64 | acc1,
|  | v16acc64 | acc2 )

Parameters

  a | Matrix A
  sgn_x | Sign mask for matrix A
  b | Matrix B
  sgn_y | Sign mask for matrix B
  acc1 | Accumulator 1 input
  acc2 | Accumulator 2 input

Returns
  Result of operation

## ◆ addmac_conv_16x4() [2/8]

v16acc64 addmac_conv_16x4 | ( | v32int16 | a,
|  | int | sgn_x,
|  | v32uint16 | b,
|  | int | sgn_y,
|  | v16acc64 | acc1,
|  | v16acc64 | acc2 )

Parameters

  a | Matrix A
  sgn_x | Sign mask for matrix A
  b | Matrix B
  sgn_y | Sign mask for matrix B
  acc1 | Accumulator 1 input
  acc2 | Accumulator 2 input

Returns
  Result of operation

## ◆ addmac_conv_16x4() [3/8]

v16acc64 addmac_conv_16x4 | ( | v32int16 | a,
|  | v32int16 | b,
|  | v16acc64 | acc1,
|  | v16acc64 | acc2 )

Parameters

  a | Matrix A
  b | Matrix B
  acc1 | Accumulator 1 input
  acc2 | Accumulator 2 input

Returns
  Result of operation

## ◆ addmac_conv_16x4() [4/8]

v16acc64 addmac_conv_16x4 | ( | v32int16 | a,
|  | v32uint16 | b,
|  | v16acc64 | acc1,
|  | v16acc64 | acc2 )

Parameters

  a | Matrix A
  b | Matrix B
  acc1 | Accumulator 1 input
  acc2 | Accumulator 2 input

Returns
  Result of operation

## ◆ addmac_conv_16x4() [5/8]

v16acc64 addmac_conv_16x4 | ( | v32uint16 | a,
|  | int | sgn_x,
|  | v32int16 | b,
|  | int | sgn_y,
|  | v16acc64 | acc1,
|  | v16acc64 | acc2 )

Parameters

  a | Matrix A
  sgn_x | Sign mask for matrix A
  b | Matrix B
  sgn_y | Sign mask for matrix B
  acc1 | Accumulator 1 input
  acc2 | Accumulator 2 input

Returns
  Result of operation

## ◆ addmac_conv_16x4() [6/8]

v16acc64 addmac_conv_16x4 | ( | v32uint16 | a,
|  | int | sgn_x,
|  | v32uint16 | b,
|  | int | sgn_y,
|  | v16acc64 | acc1,
|  | v16acc64 | acc2 )

Parameters

  a | Matrix A
  sgn_x | Sign mask for matrix A
  b | Matrix B
  sgn_y | Sign mask for matrix B
  acc1 | Accumulator 1 input
  acc2 | Accumulator 2 input

Returns
  Result of operation

## ◆ addmac_conv_16x4() [7/8]

v16acc64 addmac_conv_16x4 | ( | v32uint16 | a,
|  | v32int16 | b,
|  | v16acc64 | acc1,
|  | v16acc64 | acc2 )

Parameters

  a | Matrix A
  b | Matrix B
  acc1 | Accumulator 1 input
  acc2 | Accumulator 2 input

Returns
  Result of operation

## ◆ addmac_conv_16x4() [8/8]

v16acc64 addmac_conv_16x4 | ( | v32uint16 | a,
|  | v32uint16 | b,
|  | v16acc64 | acc1,
|  | v16acc64 | acc2 )

Parameters

  a | Matrix A
  b | Matrix B
  acc1 | Accumulator 1 input
  acc2 | Accumulator 2 input

Returns
  Result of operation

## ◆ addmac_conv_16x4_conf() [1/8]

v16acc64 addmac_conv_16x4_conf | ( | v32int16 | a,
|  | int | sgn_x,
|  | v32int16 | b,
|  | int | sgn_y,
|  | v16acc64 | acc1,
|  | v16acc64 | acc2,
|  | int | zero_acc1,
|  | int | shift16,
|  | int | sub_mul,
|  | int | sub_acc1,
|  | int | sub_acc2 )

Parameters

  a | Matrix A
  sgn_x | Sign mask for matrix A
  b | Matrix B
  sgn_y | Sign mask for matrix B
  acc1 | Accumulator 1 input
  acc2 | Accumulator 2 input
  zero_acc1 | Zeroing mask for acc1
  shift16 | Shift mask of input accumulator acc1
  sub_mul | Negation mask of multiplication result
  sub_acc1 | Negation mask of acc1
  sub_acc2 | Negation mask of acc2

Returns
  Result of operation

## ◆ addmac_conv_16x4_conf() [2/8]

v16acc64 addmac_conv_16x4_conf | ( | v32int16 | a,
|  | int | sgn_x,
|  | v32uint16 | b,
|  | int | sgn_y,
|  | v16acc64 | acc1,
|  | v16acc64 | acc2,
|  | int | zero_acc1,
|  | int | shift16,
|  | int | sub_mul,
|  | int | sub_acc1,
|  | int | sub_acc2 )

Parameters

  a | Matrix A
  sgn_x | Sign mask for matrix A
  b | Matrix B
  sgn_y | Sign mask for matrix B
  acc1 | Accumulator 1 input
  acc2 | Accumulator 2 input
  zero_acc1 | Zeroing mask for acc1
  shift16 | Shift mask of input accumulator acc1
  sub_mul | Negation mask of multiplication result
  sub_acc1 | Negation mask of acc1
  sub_acc2 | Negation mask of acc2

Returns
  Result of operation

## ◆ addmac_conv_16x4_conf() [3/8]

v16acc64 addmac_conv_16x4_conf | ( | v32int16 | a,
|  | v32int16 | b,
|  | v16acc64 | acc1,
|  | v16acc64 | acc2,
|  | int | zero_acc1,
|  | int | shift16,
|  | int | sub_mul,
|  | int | sub_acc1,
|  | int | sub_acc2 )

Parameters

  a | Matrix A
  b | Matrix B
  acc1 | Accumulator 1 input
  acc2 | Accumulator 2 input
  zero_acc1 | Zeroing mask for acc1
  shift16 | Shift mask of input accumulator acc1
  sub_mul | Negation mask of multiplication result
  sub_acc1 | Negation mask of acc1
  sub_acc2 | Negation mask of acc2

Returns
  Result of operation

## ◆ addmac_conv_16x4_conf() [4/8]

v16acc64 addmac_conv_16x4_conf | ( | v32int16 | a,
|  | v32uint16 | b,
|  | v16acc64 | acc1,
|  | v16acc64 | acc2,
|  | int | zero_acc1,
|  | int | shift16,
|  | int | sub_mul,
|  | int | sub_acc1,
|  | int | sub_acc2 )

Parameters

  a | Matrix A
  b | Matrix B
  acc1 | Accumulator 1 input
  acc2 | Accumulator 2 input
  zero_acc1 | Zeroing mask for acc1
  shift16 | Shift mask of input accumulator acc1
  sub_mul | Negation mask of multiplication result
  sub_acc1 | Negation mask of acc1
  sub_acc2 | Negation mask of acc2

Returns
  Result of operation

## ◆ addmac_conv_16x4_conf() [5/8]

v16acc64 addmac_conv_16x4_conf | ( | v32uint16 | a,
|  | int | sgn_x,
|  | v32int16 | b,
|  | int | sgn_y,
|  | v16acc64 | acc1,
|  | v16acc64 | acc2,
|  | int | zero_acc1,
|  | int | shift16,
|  | int | sub_mul,
|  | int | sub_acc1,
|  | int | sub_acc2 )

Parameters

  a | Matrix A
  sgn_x | Sign mask for matrix A
  b | Matrix B
  sgn_y | Sign mask for matrix B
  acc1 | Accumulator 1 input
  acc2 | Accumulator 2 input
  zero_acc1 | Zeroing mask for acc1
  shift16 | Shift mask of input accumulator acc1
  sub_mul | Negation mask of multiplication result
  sub_acc1 | Negation mask of acc1
  sub_acc2 | Negation mask of acc2

Returns
  Result of operation

## ◆ addmac_conv_16x4_conf() [6/8]

v16acc64 addmac_conv_16x4_conf | ( | v32uint16 | a,
|  | int | sgn_x,
|  | v32uint16 | b,
|  | int | sgn_y,
|  | v16acc64 | acc1,
|  | v16acc64 | acc2,
|  | int | zero_acc1,
|  | int | shift16,
|  | int | sub_mul,
|  | int | sub_acc1,
|  | int | sub_acc2 )

Parameters

  a | Matrix A
  sgn_x | Sign mask for matrix A
  b | Matrix B
  sgn_y | Sign mask for matrix B
  acc1 | Accumulator 1 input
  acc2 | Accumulator 2 input
  zero_acc1 | Zeroing mask for acc1
  shift16 | Shift mask of input accumulator acc1
  sub_mul | Negation mask of multiplication result
  sub_acc1 | Negation mask of acc1
  sub_acc2 | Negation mask of acc2

Returns
  Result of operation

## ◆ addmac_conv_16x4_conf() [7/8]

v16acc64 addmac_conv_16x4_conf | ( | v32uint16 | a,
|  | v32int16 | b,
|  | v16acc64 | acc1,
|  | v16acc64 | acc2,
|  | int | zero_acc1,
|  | int | shift16,
|  | int | sub_mul,
|  | int | sub_acc1,
|  | int | sub_acc2 )

Parameters

  a | Matrix A
  b | Matrix B
  acc1 | Accumulator 1 input
  acc2 | Accumulator 2 input
  zero_acc1 | Zeroing mask for acc1
  shift16 | Shift mask of input accumulator acc1
  sub_mul | Negation mask of multiplication result
  sub_acc1 | Negation mask of acc1
  sub_acc2 | Negation mask of acc2

Returns
  Result of operation

## ◆ addmac_conv_16x4_conf() [8/8]

v16acc64 addmac_conv_16x4_conf | ( | v32uint16 | a,
|  | v32uint16 | b,
|  | v16acc64 | acc1,
|  | v16acc64 | acc2,
|  | int | zero_acc1,
|  | int | shift16,
|  | int | sub_mul,
|  | int | sub_acc1,
|  | int | sub_acc2 )

Parameters

  a | Matrix A
  b | Matrix B
  acc1 | Accumulator 1 input
  acc2 | Accumulator 2 input
  zero_acc1 | Zeroing mask for acc1
  shift16 | Shift mask of input accumulator acc1
  sub_mul | Negation mask of multiplication result
  sub_acc1 | Negation mask of acc1
  sub_acc2 | Negation mask of acc2

Returns
  Result of operation

## ◆ addmac_elem_16_2() [1/9]

v16accfloat addmac_elem_16_2 | ( | v32bfloat16 | a,
|  | v32bfloat16 | b,
|  | v16accfloat | acc1,
|  | v16accfloat | acc2 )

Parameters

  a | Matrix A
  b | Matrix B
  acc1 | Accumulator 1 input
  acc2 | Accumulator 2 input

Returns
  Result of operation

## ◆ addmac_elem_16_2() [2/9]

v16acc64 addmac_elem_16_2 | ( | v32int16 | a,
|  | int | sgn_x,
|  | v32int16 | b,
|  | int | sgn_y,
|  | v16acc64 | acc1,
|  | v16acc64 | acc2 )

Parameters

  a | Matrix A
  sgn_x | Sign mask for matrix A
  b | Matrix B
  sgn_y | Sign mask for matrix B
  acc1 | Accumulator 1 input
  acc2 | Accumulator 2 input

Returns
  Result of operation

## ◆ addmac_elem_16_2() [3/9]

v16acc64 addmac_elem_16_2 | ( | v32int16 | a,
|  | int | sgn_x,
|  | v32uint16 | b,
|  | int | sgn_y,
|  | v16acc64 | acc1,
|  | v16acc64 | acc2 )

Parameters

  a | Matrix A
  sgn_x | Sign mask for matrix A
  b | Matrix B
  sgn_y | Sign mask for matrix B
  acc1 | Accumulator 1 input
  acc2 | Accumulator 2 input

Returns
  Result of operation

## ◆ addmac_elem_16_2() [4/9]

v16acc64 addmac_elem_16_2 | ( | v32int16 | a,
|  | v32int16 | b,
|  | v16acc64 | acc1,
|  | v16acc64 | acc2 )

Parameters

  a | Matrix A
  b | Matrix B
  acc1 | Accumulator 1 input
  acc2 | Accumulator 2 input

Returns
  Result of operation

## ◆ addmac_elem_16_2() [5/9]

v16acc64 addmac_elem_16_2 | ( | v32int16 | a,
|  | v32uint16 | b,
|  | v16acc64 | acc1,
|  | v16acc64 | acc2 )

Parameters

  a | Matrix A
  b | Matrix B
  acc1 | Accumulator 1 input
  acc2 | Accumulator 2 input

Returns
  Result of operation

## ◆ addmac_elem_16_2() [6/9]

v16acc64 addmac_elem_16_2 | ( | v32uint16 | a,
|  | int | sgn_x,
|  | v32int16 | b,
|  | int | sgn_y,
|  | v16acc64 | acc1,
|  | v16acc64 | acc2 )

Parameters

  a | Matrix A
  sgn_x | Sign mask for matrix A
  b | Matrix B
  sgn_y | Sign mask for matrix B
  acc1 | Accumulator 1 input
  acc2 | Accumulator 2 input

Returns
  Result of operation

## ◆ addmac_elem_16_2() [7/9]

v16acc64 addmac_elem_16_2 | ( | v32uint16 | a,
|  | int | sgn_x,
|  | v32uint16 | b,
|  | int | sgn_y,
|  | v16acc64 | acc1,
|  | v16acc64 | acc2 )

Parameters

  a | Matrix A
  sgn_x | Sign mask for matrix A
  b | Matrix B
  sgn_y | Sign mask for matrix B
  acc1 | Accumulator 1 input
  acc2 | Accumulator 2 input

Returns
  Result of operation

## ◆ addmac_elem_16_2() [8/9]

v16acc64 addmac_elem_16_2 | ( | v32uint16 | a,
|  | v32int16 | b,
|  | v16acc64 | acc1,
|  | v16acc64 | acc2 )

Parameters

  a | Matrix A
  b | Matrix B
  acc1 | Accumulator 1 input
  acc2 | Accumulator 2 input

Returns
  Result of operation

## ◆ addmac_elem_16_2() [9/9]

v16acc64 addmac_elem_16_2 | ( | v32uint16 | a,
|  | v32uint16 | b,
|  | v16acc64 | acc1,
|  | v16acc64 | acc2 )

Parameters

  a | Matrix A
  b | Matrix B
  acc1 | Accumulator 1 input
  acc2 | Accumulator 2 input

Returns
  Result of operation

## ◆ addmac_elem_16_2_conf() [1/9]

v16accfloat addmac_elem_16_2_conf | ( | v32bfloat16 | a,
|  | v32bfloat16 | b,
|  | v16accfloat | acc1,
|  | v16accfloat | acc2,
|  | int | zero_acc1,
|  | int | sub_mul,
|  | int | sub_acc1,
|  | int | sub_acc2 )

Parameters

  a | Matrix A
  b | Matrix B
  acc1 | Accumulator 1 input
  acc2 | Accumulator 2 input
  zero_acc1 | Zeroing mask for acc1
  sub_mul | Negation mask of multiplication result
  sub_acc1 | Negation mask of acc1
  sub_acc2 | Negation mask of acc2

Returns
  Result of operation

## ◆ addmac_elem_16_2_conf() [2/9]

v16acc64 addmac_elem_16_2_conf | ( | v32int16 | a,
|  | int | sgn_x,
|  | v32int16 | b,
|  | int | sgn_y,
|  | v16acc64 | acc1,
|  | v16acc64 | acc2,
|  | int | zero_acc1,
|  | int | shift16,
|  | int | sub_mul,
|  | int | sub_acc1,
|  | int | sub_acc2 )

Parameters

  a | Matrix A
  sgn_x | Sign mask for matrix A
  b | Matrix B
  sgn_y | Sign mask for matrix B
  acc1 | Accumulator 1 input
  acc2 | Accumulator 2 input
  zero_acc1 | Zeroing mask for acc1
  shift16 | Shift mask of input accumulator acc1
  sub_mul | Negation mask of multiplication result
  sub_acc1 | Negation mask of acc1
  sub_acc2 | Negation mask of acc2

Returns
  Result of operation

## ◆ addmac_elem_16_2_conf() [3/9]

v16acc64 addmac_elem_16_2_conf | ( | v32int16 | a,
|  | int | sgn_x,
|  | v32uint16 | b,
|  | int | sgn_y,
|  | v16acc64 | acc1,
|  | v16acc64 | acc2,
|  | int | zero_acc1,
|  | int | shift16,
|  | int | sub_mul,
|  | int | sub_acc1,
|  | int | sub_acc2 )

Parameters

  a | Matrix A
  sgn_x | Sign mask for matrix A
  b | Matrix B
  sgn_y | Sign mask for matrix B
  acc1 | Accumulator 1 input
  acc2 | Accumulator 2 input
  zero_acc1 | Zeroing mask for acc1
  shift16 | Shift mask of input accumulator acc1
  sub_mul | Negation mask of multiplication result
  sub_acc1 | Negation mask of acc1
  sub_acc2 | Negation mask of acc2

Returns
  Result of operation

## ◆ addmac_elem_16_2_conf() [4/9]

v16acc64 addmac_elem_16_2_conf | ( | v32int16 | a,
|  | v32int16 | b,
|  | v16acc64 | acc1,
|  | v16acc64 | acc2,
|  | int | zero_acc1,
|  | int | shift16,
|  | int | sub_mul,
|  | int | sub_acc1,
|  | int | sub_acc2 )

Parameters

  a | Matrix A
  b | Matrix B
  acc1 | Accumulator 1 input
  acc2 | Accumulator 2 input
  zero_acc1 | Zeroing mask for acc1
  shift16 | Shift mask of input accumulator acc1
  sub_mul | Negation mask of multiplication result
  sub_acc1 | Negation mask of acc1
  sub_acc2 | Negation mask of acc2

Returns
  Result of operation

## ◆ addmac_elem_16_2_conf() [5/9]

v16acc64 addmac_elem_16_2_conf | ( | v32int16 | a,
|  | v32uint16 | b,
|  | v16acc64 | acc1,
|  | v16acc64 | acc2,
|  | int | zero_acc1,
|  | int | shift16,
|  | int | sub_mul,
|  | int | sub_acc1,
|  | int | sub_acc2 )

Parameters

  a | Matrix A
  b | Matrix B
  acc1 | Accumulator 1 input
  acc2 | Accumulator 2 input
  zero_acc1 | Zeroing mask for acc1
  shift16 | Shift mask of input accumulator acc1
  sub_mul | Negation mask of multiplication result
  sub_acc1 | Negation mask of acc1
  sub_acc2 | Negation mask of acc2

Returns
  Result of operation

## ◆ addmac_elem_16_2_conf() [6/9]

v16acc64 addmac_elem_16_2_conf | ( | v32uint16 | a,
|  | int | sgn_x,
|  | v32int16 | b,
|  | int | sgn_y,
|  | v16acc64 | acc1,
|  | v16acc64 | acc2,
|  | int | zero_acc1,
|  | int | shift16,
|  | int | sub_mul,
|  | int | sub_acc1,
|  | int | sub_acc2 )

Parameters

  a | Matrix A
  sgn_x | Sign mask for matrix A
  b | Matrix B
  sgn_y | Sign mask for matrix B
  acc1 | Accumulator 1 input
  acc2 | Accumulator 2 input
  zero_acc1 | Zeroing mask for acc1
  shift16 | Shift mask of input accumulator acc1
  sub_mul | Negation mask of multiplication result
  sub_acc1 | Negation mask of acc1
  sub_acc2 | Negation mask of acc2

Returns
  Result of operation

## ◆ addmac_elem_16_2_conf() [7/9]

v16acc64 addmac_elem_16_2_conf | ( | v32uint16 | a,
|  | int | sgn_x,
|  | v32uint16 | b,
|  | int | sgn_y,
|  | v16acc64 | acc1,
|  | v16acc64 | acc2,
|  | int | zero_acc1,
|  | int | shift16,
|  | int | sub_mul,
|  | int | sub_acc1,
|  | int | sub_acc2 )

Parameters

  a | Matrix A
  sgn_x | Sign mask for matrix A
  b | Matrix B
  sgn_y | Sign mask for matrix B
  acc1 | Accumulator 1 input
  acc2 | Accumulator 2 input
  zero_acc1 | Zeroing mask for acc1
  shift16 | Shift mask of input accumulator acc1
  sub_mul | Negation mask of multiplication result
  sub_acc1 | Negation mask of acc1
  sub_acc2 | Negation mask of acc2

Returns
  Result of operation

## ◆ addmac_elem_16_2_conf() [8/9]

v16acc64 addmac_elem_16_2_conf | ( | v32uint16 | a,
|  | v32int16 | b,
|  | v16acc64 | acc1,
|  | v16acc64 | acc2,
|  | int | zero_acc1,
|  | int | shift16,
|  | int | sub_mul,
|  | int | sub_acc1,
|  | int | sub_acc2 )

Parameters

  a | Matrix A
  b | Matrix B
  acc1 | Accumulator 1 input
  acc2 | Accumulator 2 input
  zero_acc1 | Zeroing mask for acc1
  shift16 | Shift mask of input accumulator acc1
  sub_mul | Negation mask of multiplication result
  sub_acc1 | Negation mask of acc1
  sub_acc2 | Negation mask of acc2

Returns
  Result of operation

## ◆ addmac_elem_16_2_conf() [9/9]

v16acc64 addmac_elem_16_2_conf | ( | v32uint16 | a,
|  | v32uint16 | b,
|  | v16acc64 | acc1,
|  | v16acc64 | acc2,
|  | int | zero_acc1,
|  | int | shift16,
|  | int | sub_mul,
|  | int | sub_acc1,
|  | int | sub_acc2 )

Parameters

  a | Matrix A
  b | Matrix B
  acc1 | Accumulator 1 input
  acc2 | Accumulator 2 input
  zero_acc1 | Zeroing mask for acc1
  shift16 | Shift mask of input accumulator acc1
  sub_mul | Negation mask of multiplication result
  sub_acc1 | Negation mask of acc1
  sub_acc2 | Negation mask of acc2

Returns
  Result of operation

## ◆ addmac_elem_32() [1/8]

v32acc32 addmac_elem_32 | ( | v32int16 | a,
|  | int | sgn_x,
|  | v32int16 | b,
|  | int | sgn_y,
|  | v32acc32 | acc1,
|  | v32acc32 | acc2 )

Parameters

  a | Matrix A
  sgn_x | Sign mask for matrix A
  b | Matrix B
  sgn_y | Sign mask for matrix B
  acc1 | Accumulator 1 input
  acc2 | Accumulator 2 input

Returns
  Result of operation

## ◆ addmac_elem_32() [2/8]

v32acc32 addmac_elem_32 | ( | v32int16 | a,
|  | int | sgn_x,
|  | v32uint16 | b,
|  | int | sgn_y,
|  | v32acc32 | acc1,
|  | v32acc32 | acc2 )

Parameters

  a | Matrix A
  sgn_x | Sign mask for matrix A
  b | Matrix B
  sgn_y | Sign mask for matrix B
  acc1 | Accumulator 1 input
  acc2 | Accumulator 2 input

Returns
  Result of operation

## ◆ addmac_elem_32() [3/8]

v32acc32 addmac_elem_32 | ( | v32int16 | a,
|  | v32int16 | b,
|  | v32acc32 | acc1,
|  | v32acc32 | acc2 )

Parameters

  a | Matrix A
  b | Matrix B
  acc1 | Accumulator 1 input
  acc2 | Accumulator 2 input

Returns
  Result of operation

## ◆ addmac_elem_32() [4/8]

v32acc32 addmac_elem_32 | ( | v32int16 | a,
|  | v32uint16 | b,
|  | v32acc32 | acc1,
|  | v32acc32 | acc2 )

Parameters

  a | Matrix A
  b | Matrix B
  acc1 | Accumulator 1 input
  acc2 | Accumulator 2 input

Returns
  Result of operation

## ◆ addmac_elem_32() [5/8]

v32acc32 addmac_elem_32 | ( | v32uint16 | a,
|  | int | sgn_x,
|  | v32int16 | b,
|  | int | sgn_y,
|  | v32acc32 | acc1,
|  | v32acc32 | acc2 )

Parameters

  a | Matrix A
  sgn_x | Sign mask for matrix A
  b | Matrix B
  sgn_y | Sign mask for matrix B
  acc1 | Accumulator 1 input
  acc2 | Accumulator 2 input

Returns
  Result of operation

## ◆ addmac_elem_32() [6/8]

v32acc32 addmac_elem_32 | ( | v32uint16 | a,
|  | int | sgn_x,
|  | v32uint16 | b,
|  | int | sgn_y,
|  | v32acc32 | acc1,
|  | v32acc32 | acc2 )

Parameters

  a | Matrix A
  sgn_x | Sign mask for matrix A
  b | Matrix B
  sgn_y | Sign mask for matrix B
  acc1 | Accumulator 1 input
  acc2 | Accumulator 2 input

Returns
  Result of operation

## ◆ addmac_elem_32() [7/8]

v32acc32 addmac_elem_32 | ( | v32uint16 | a,
|  | v32int16 | b,
|  | v32acc32 | acc1,
|  | v32acc32 | acc2 )

Parameters

  a | Matrix A
  b | Matrix B
  acc1 | Accumulator 1 input
  acc2 | Accumulator 2 input

Returns
  Result of operation

## ◆ addmac_elem_32() [8/8]

v32acc32 addmac_elem_32 | ( | v32uint16 | a,
|  | v32uint16 | b,
|  | v32acc32 | acc1,
|  | v32acc32 | acc2 )

Parameters

  a | Matrix A
  b | Matrix B
  acc1 | Accumulator 1 input
  acc2 | Accumulator 2 input

Returns
  Result of operation

## ◆ addmac_elem_32_conf() [1/8]

v32acc32 addmac_elem_32_conf | ( | v32int16 | a,
|  | int | sgn_x,
|  | v32int16 | b,
|  | int | sgn_y,
|  | v32acc32 | acc1,
|  | v32acc32 | acc2,
|  | int | zero_acc1,
|  | int | shift16,
|  | int | sub_mul,
|  | int | sub_acc1,
|  | int | sub_acc2 )

Parameters

  a | Matrix A
  sgn_x | Sign mask for matrix A
  b | Matrix B
  sgn_y | Sign mask for matrix B
  acc1 | Accumulator 1 input
  acc2 | Accumulator 2 input
  zero_acc1 | Zeroing mask for acc1
  shift16 | Shift mask of input accumulator acc1
  sub_mul | Negation mask of multiplication result
  sub_acc1 | Negation mask of acc1
  sub_acc2 | Negation mask of acc2

Returns
  Result of operation

## ◆ addmac_elem_32_conf() [2/8]

v32acc32 addmac_elem_32_conf | ( | v32int16 | a,
|  | int | sgn_x,
|  | v32uint16 | b,
|  | int | sgn_y,
|  | v32acc32 | acc1,
|  | v32acc32 | acc2,
|  | int | zero_acc1,
|  | int | shift16,
|  | int | sub_mul,
|  | int | sub_acc1,
|  | int | sub_acc2 )

Parameters

  a | Matrix A
  sgn_x | Sign mask for matrix A
  b | Matrix B
  sgn_y | Sign mask for matrix B
  acc1 | Accumulator 1 input
  acc2 | Accumulator 2 input
  zero_acc1 | Zeroing mask for acc1
  shift16 | Shift mask of input accumulator acc1
  sub_mul | Negation mask of multiplication result
  sub_acc1 | Negation mask of acc1
  sub_acc2 | Negation mask of acc2

Returns
  Result of operation

## ◆ addmac_elem_32_conf() [3/8]

v32acc32 addmac_elem_32_conf | ( | v32int16 | a,
|  | v32int16 | b,
|  | v32acc32 | acc1,
|  | v32acc32 | acc2,
|  | int | zero_acc1,
|  | int | shift16,
|  | int | sub_mul,
|  | int | sub_acc1,
|  | int | sub_acc2 )

Parameters

  a | Matrix A
  b | Matrix B
  acc1 | Accumulator 1 input
  acc2 | Accumulator 2 input
  zero_acc1 | Zeroing mask for acc1
  shift16 | Shift mask of input accumulator acc1
  sub_mul | Negation mask of multiplication result
  sub_acc1 | Negation mask of acc1
  sub_acc2 | Negation mask of acc2

Returns
  Result of operation

## ◆ addmac_elem_32_conf() [4/8]

v32acc32 addmac_elem_32_conf | ( | v32int16 | a,
|  | v32uint16 | b,
|  | v32acc32 | acc1,
|  | v32acc32 | acc2,
|  | int | zero_acc1,
|  | int | shift16,
|  | int | sub_mul,
|  | int | sub_acc1,
|  | int | sub_acc2 )

Parameters

  a | Matrix A
  b | Matrix B
  acc1 | Accumulator 1 input
  acc2 | Accumulator 2 input
  zero_acc1 | Zeroing mask for acc1
  shift16 | Shift mask of input accumulator acc1
  sub_mul | Negation mask of multiplication result
  sub_acc1 | Negation mask of acc1
  sub_acc2 | Negation mask of acc2

Returns
  Result of operation

## ◆ addmac_elem_32_conf() [5/8]

v32acc32 addmac_elem_32_conf | ( | v32uint16 | a,
|  | int | sgn_x,
|  | v32int16 | b,
|  | int | sgn_y,
|  | v32acc32 | acc1,
|  | v32acc32 | acc2,
|  | int | zero_acc1,
|  | int | shift16,
|  | int | sub_mul,
|  | int | sub_acc1,
|  | int | sub_acc2 )

Parameters

  a | Matrix A
  sgn_x | Sign mask for matrix A
  b | Matrix B
  sgn_y | Sign mask for matrix B
  acc1 | Accumulator 1 input
  acc2 | Accumulator 2 input
  zero_acc1 | Zeroing mask for acc1
  shift16 | Shift mask of input accumulator acc1
  sub_mul | Negation mask of multiplication result
  sub_acc1 | Negation mask of acc1
  sub_acc2 | Negation mask of acc2

Returns
  Result of operation

## ◆ addmac_elem_32_conf() [6/8]

v32acc32 addmac_elem_32_conf | ( | v32uint16 | a,
|  | int | sgn_x,
|  | v32uint16 | b,
|  | int | sgn_y,
|  | v32acc32 | acc1,
|  | v32acc32 | acc2,
|  | int | zero_acc1,
|  | int | shift16,
|  | int | sub_mul,
|  | int | sub_acc1,
|  | int | sub_acc2 )

Parameters

  a | Matrix A
  sgn_x | Sign mask for matrix A
  b | Matrix B
  sgn_y | Sign mask for matrix B
  acc1 | Accumulator 1 input
  acc2 | Accumulator 2 input
  zero_acc1 | Zeroing mask for acc1
  shift16 | Shift mask of input accumulator acc1
  sub_mul | Negation mask of multiplication result
  sub_acc1 | Negation mask of acc1
  sub_acc2 | Negation mask of acc2

Returns
  Result of operation

## ◆ addmac_elem_32_conf() [7/8]

v32acc32 addmac_elem_32_conf | ( | v32uint16 | a,
|  | v32int16 | b,
|  | v32acc32 | acc1,
|  | v32acc32 | acc2,
|  | int | zero_acc1,
|  | int | shift16,
|  | int | sub_mul,
|  | int | sub_acc1,
|  | int | sub_acc2 )

Parameters

  a | Matrix A
  b | Matrix B
  acc1 | Accumulator 1 input
  acc2 | Accumulator 2 input
  zero_acc1 | Zeroing mask for acc1
  shift16 | Shift mask of input accumulator acc1
  sub_mul | Negation mask of multiplication result
  sub_acc1 | Negation mask of acc1
  sub_acc2 | Negation mask of acc2

Returns
  Result of operation

## ◆ addmac_elem_32_conf() [8/8]

v32acc32 addmac_elem_32_conf | ( | v32uint16 | a,
|  | v32uint16 | b,
|  | v32acc32 | acc1,
|  | v32acc32 | acc2,
|  | int | zero_acc1,
|  | int | shift16,
|  | int | sub_mul,
|  | int | sub_acc1,
|  | int | sub_acc2 )

Parameters

  a | Matrix A
  b | Matrix B
  acc1 | Accumulator 1 input
  acc2 | Accumulator 2 input
  zero_acc1 | Zeroing mask for acc1
  shift16 | Shift mask of input accumulator acc1
  sub_mul | Negation mask of multiplication result
  sub_acc1 | Negation mask of acc1
  sub_acc2 | Negation mask of acc2

Returns
  Result of operation

## ◆ addmsc_2x4_4x8() [1/8]

v16acc64 addmsc_2x4_4x8 | ( | v32int16 | a,
|  | int | sgn_x,
|  | v32int16 | b,
|  | int | sgn_y,
|  | v16acc64 | acc1,
|  | v16acc64 | acc2 )

Parameters

  a | Matrix A
  sgn_x | Sign mask for matrix A
  b | Matrix B
  sgn_y | Sign mask for matrix B
  acc1 | Accumulator 1 input
  acc2 | Accumulator 2 input

Returns
  Result of operation

## ◆ addmsc_2x4_4x8() [2/8]

v16acc64 addmsc_2x4_4x8 | ( | v32int16 | a,
|  | int | sgn_x,
|  | v32uint16 | b,
|  | int | sgn_y,
|  | v16acc64 | acc1,
|  | v16acc64 | acc2 )

Parameters

  a | Matrix A
  sgn_x | Sign mask for matrix A
  b | Matrix B
  sgn_y | Sign mask for matrix B
  acc1 | Accumulator 1 input
  acc2 | Accumulator 2 input

Returns
  Result of operation

## ◆ addmsc_2x4_4x8() [3/8]

v16acc64 addmsc_2x4_4x8 | ( | v32int16 | a,
|  | v32int16 | b,
|  | v16acc64 | acc1,
|  | v16acc64 | acc2 )

Parameters

  a | Matrix A
  b | Matrix B
  acc1 | Accumulator 1 input
  acc2 | Accumulator 2 input

Returns
  Result of operation

## ◆ addmsc_2x4_4x8() [4/8]

v16acc64 addmsc_2x4_4x8 | ( | v32int16 | a,
|  | v32uint16 | b,
|  | v16acc64 | acc1,
|  | v16acc64 | acc2 )

Parameters

  a | Matrix A
  b | Matrix B
  acc1 | Accumulator 1 input
  acc2 | Accumulator 2 input

Returns
  Result of operation

## ◆ addmsc_2x4_4x8() [5/8]

v16acc64 addmsc_2x4_4x8 | ( | v32uint16 | a,
|  | int | sgn_x,
|  | v32int16 | b,
|  | int | sgn_y,
|  | v16acc64 | acc1,
|  | v16acc64 | acc2 )

Parameters

  a | Matrix A
  sgn_x | Sign mask for matrix A
  b | Matrix B
  sgn_y | Sign mask for matrix B
  acc1 | Accumulator 1 input
  acc2 | Accumulator 2 input

Returns
  Result of operation

## ◆ addmsc_2x4_4x8() [6/8]

v16acc64 addmsc_2x4_4x8 | ( | v32uint16 | a,
|  | int | sgn_x,
|  | v32uint16 | b,
|  | int | sgn_y,
|  | v16acc64 | acc1,
|  | v16acc64 | acc2 )

Parameters

  a | Matrix A
  sgn_x | Sign mask for matrix A
  b | Matrix B
  sgn_y | Sign mask for matrix B
  acc1 | Accumulator 1 input
  acc2 | Accumulator 2 input

Returns
  Result of operation

## ◆ addmsc_2x4_4x8() [7/8]

v16acc64 addmsc_2x4_4x8 | ( | v32uint16 | a,
|  | v32int16 | b,
|  | v16acc64 | acc1,
|  | v16acc64 | acc2 )

Parameters

  a | Matrix A
  b | Matrix B
  acc1 | Accumulator 1 input
  acc2 | Accumulator 2 input

Returns
  Result of operation

## ◆ addmsc_2x4_4x8() [8/8]

v16acc64 addmsc_2x4_4x8 | ( | v32uint16 | a,
|  | v32uint16 | b,
|  | v16acc64 | acc1,
|  | v16acc64 | acc2 )

Parameters

  a | Matrix A
  b | Matrix B
  acc1 | Accumulator 1 input
  acc2 | Accumulator 2 input

Returns
  Result of operation

## ◆ addmsc_2x4_4x8_conf() [1/8]

v16acc64 addmsc_2x4_4x8_conf | ( | v32int16 | a,
|  | int | sgn_x,
|  | v32int16 | b,
|  | int | sgn_y,
|  | v16acc64 | acc1,
|  | v16acc64 | acc2,
|  | int | zero_acc1,
|  | int | shift16,
|  | int | sub_mul,
|  | int | sub_acc1,
|  | int | sub_acc2 )

Parameters

  a | Matrix A
  sgn_x | Sign mask for matrix A
  b | Matrix B
  sgn_y | Sign mask for matrix B
  acc1 | Accumulator 1 input
  acc2 | Accumulator 2 input
  zero_acc1 | Zeroing mask for acc1
  shift16 | Shift mask of input accumulator acc1
  sub_mul | Negation mask of multiplication result.
  sub_acc1 | Negation mask of acc1
  sub_acc2 | Negation mask of acc2

Returns
  Result of operation

## ◆ addmsc_2x4_4x8_conf() [2/8]

v16acc64 addmsc_2x4_4x8_conf | ( | v32int16 | a,
|  | int | sgn_x,
|  | v32uint16 | b,
|  | int | sgn_y,
|  | v16acc64 | acc1,
|  | v16acc64 | acc2,
|  | int | zero_acc1,
|  | int | shift16,
|  | int | sub_mul,
|  | int | sub_acc1,
|  | int | sub_acc2 )

Parameters

  a | Matrix A
  sgn_x | Sign mask for matrix A
  b | Matrix B
  sgn_y | Sign mask for matrix B
  acc1 | Accumulator 1 input
  acc2 | Accumulator 2 input
  zero_acc1 | Zeroing mask for acc1
  shift16 | Shift mask of input accumulator acc1
  sub_mul | Negation mask of multiplication result.
  sub_acc1 | Negation mask of acc1
  sub_acc2 | Negation mask of acc2

Returns
  Result of operation

## ◆ addmsc_2x4_4x8_conf() [3/8]

v16acc64 addmsc_2x4_4x8_conf | ( | v32int16 | a,
|  | v32int16 | b,
|  | v16acc64 | acc1,
|  | v16acc64 | acc2,
|  | int | zero_acc1,
|  | int | shift16,
|  | int | sub_mul,
|  | int | sub_acc1,
|  | int | sub_acc2 )

Parameters

  a | Matrix A
  b | Matrix B
  acc1 | Accumulator 1 input
  acc2 | Accumulator 2 input
  zero_acc1 | Zeroing mask for acc1
  shift16 | Shift mask of input accumulator acc1
  sub_mul | Negation mask of multiplication result
  sub_acc1 | Negation mask of acc1
  sub_acc2 | Negation mask of acc2

Returns
  Result of operation

## ◆ addmsc_2x4_4x8_conf() [4/8]

v16acc64 addmsc_2x4_4x8_conf | ( | v32int16 | a,
|  | v32uint16 | b,
|  | v16acc64 | acc1,
|  | v16acc64 | acc2,
|  | int | zero_acc1,
|  | int | shift16,
|  | int | sub_mul,
|  | int | sub_acc1,
|  | int | sub_acc2 )

Parameters

  a | Matrix A
  b | Matrix B
  acc1 | Accumulator 1 input
  acc2 | Accumulator 2 input
  zero_acc1 | Zeroing mask for acc1
  shift16 | Shift mask of input accumulator acc1
  sub_mul | Negation mask of multiplication result
  sub_acc1 | Negation mask of acc1
  sub_acc2 | Negation mask of acc2

Returns
  Result of operation

## ◆ addmsc_2x4_4x8_conf() [5/8]

v16acc64 addmsc_2x4_4x8_conf | ( | v32uint16 | a,
|  | int | sgn_x,
|  | v32int16 | b,
|  | int | sgn_y,
|  | v16acc64 | acc1,
|  | v16acc64 | acc2,
|  | int | zero_acc1,
|  | int | shift16,
|  | int | sub_mul,
|  | int | sub_acc1,
|  | int | sub_acc2 )

Parameters

  a | Matrix A
  sgn_x | Sign mask for matrix A
  b | Matrix B
  sgn_y | Sign mask for matrix B
  acc1 | Accumulator 1 input
  acc2 | Accumulator 2 input
  zero_acc1 | Zeroing mask for acc1
  shift16 | Shift mask of input accumulator acc1
  sub_mul | Negation mask of multiplication result.
  sub_acc1 | Negation mask of acc1
  sub_acc2 | Negation mask of acc2

Returns
  Result of operation

## ◆ addmsc_2x4_4x8_conf() [6/8]

v16acc64 addmsc_2x4_4x8_conf | ( | v32uint16 | a,
|  | int | sgn_x,
|  | v32uint16 | b,
|  | int | sgn_y,
|  | v16acc64 | acc1,
|  | v16acc64 | acc2,
|  | int | zero_acc1,
|  | int | shift16,
|  | int | sub_mul,
|  | int | sub_acc1,
|  | int | sub_acc2 )

Parameters

  a | Matrix A
  sgn_x | Sign mask for matrix A
  b | Matrix B
  sgn_y | Sign mask for matrix B
  acc1 | Accumulator 1 input
  acc2 | Accumulator 2 input
  zero_acc1 | Zeroing mask for acc1
  shift16 | Shift mask of input accumulator acc1
  sub_mul | Negation mask of multiplication result.
  sub_acc1 | Negation mask of acc1
  sub_acc2 | Negation mask of acc2

Returns
  Result of operation

## ◆ addmsc_2x4_4x8_conf() [7/8]

v16acc64 addmsc_2x4_4x8_conf | ( | v32uint16 | a,
|  | v32int16 | b,
|  | v16acc64 | acc1,
|  | v16acc64 | acc2,
|  | int | zero_acc1,
|  | int | shift16,
|  | int | sub_mul,
|  | int | sub_acc1,
|  | int | sub_acc2 )

Parameters

  a | Matrix A
  b | Matrix B
  acc1 | Accumulator 1 input
  acc2 | Accumulator 2 input
  zero_acc1 | Zeroing mask for acc1
  shift16 | Shift mask of input accumulator acc1
  sub_mul | Negation mask of multiplication result
  sub_acc1 | Negation mask of acc1
  sub_acc2 | Negation mask of acc2

Returns
  Result of operation

## ◆ addmsc_2x4_4x8_conf() [8/8]

v16acc64 addmsc_2x4_4x8_conf | ( | v32uint16 | a,
|  | v32uint16 | b,
|  | v16acc64 | acc1,
|  | v16acc64 | acc2,
|  | int | zero_acc1,
|  | int | shift16,
|  | int | sub_mul,
|  | int | sub_acc1,
|  | int | sub_acc2 )

Parameters

  a | Matrix A
  b | Matrix B
  acc1 | Accumulator 1 input
  acc2 | Accumulator 2 input
  zero_acc1 | Zeroing mask for acc1
  shift16 | Shift mask of input accumulator acc1
  sub_mul | Negation mask of multiplication result
  sub_acc1 | Negation mask of acc1
  sub_acc2 | Negation mask of acc2

Returns
  Result of operation

## ◆ addmsc_4x2_2x8() [1/8]

v32acc32 addmsc_4x2_2x8 | ( | v32int16 | a,
|  | int | sgn_x,
|  | v32int16 | b,
|  | int | sgn_y,
|  | v32acc32 | acc1,
|  | v32acc32 | acc2 )

Parameters

  a | Matrix A
  sgn_x | Sign mask for matrix A
  b | Matrix B
  sgn_y | Sign mask for matrix B
  acc1 | Accumulator 1 input
  acc2 | Accumulator 2 input

Returns
  Result of operation

## ◆ addmsc_4x2_2x8() [2/8]

v32acc32 addmsc_4x2_2x8 | ( | v32int16 | a,
|  | int | sgn_x,
|  | v32uint16 | b,
|  | int | sgn_y,
|  | v32acc32 | acc1,
|  | v32acc32 | acc2 )

Parameters

  a | Matrix A
  sgn_x | Sign mask for matrix A
  b | Matrix B
  sgn_y | Sign mask for matrix B
  acc1 | Accumulator 1 input
  acc2 | Accumulator 2 input

Returns
  Result of operation

## ◆ addmsc_4x2_2x8() [3/8]

v32acc32 addmsc_4x2_2x8 | ( | v32int16 | a,
|  | v32int16 | b,
|  | v32acc32 | acc1,
|  | v32acc32 | acc2 )

Parameters

  a | Matrix A
  b | Matrix B
  acc1 | Accumulator 1 input
  acc2 | Accumulator 2 input

Returns
  Result of operation

## ◆ addmsc_4x2_2x8() [4/8]

v32acc32 addmsc_4x2_2x8 | ( | v32int16 | a,
|  | v32uint16 | b,
|  | v32acc32 | acc1,
|  | v32acc32 | acc2 )

Parameters

  a | Matrix A
  b | Matrix B
  acc1 | Accumulator 1 input
  acc2 | Accumulator 2 input

Returns
  Result of operation

## ◆ addmsc_4x2_2x8() [5/8]

v32acc32 addmsc_4x2_2x8 | ( | v32uint16 | a,
|  | int | sgn_x,
|  | v32int16 | b,
|  | int | sgn_y,
|  | v32acc32 | acc1,
|  | v32acc32 | acc2 )

Parameters

  a | Matrix A
  sgn_x | Sign mask for matrix A
  b | Matrix B
  sgn_y | Sign mask for matrix B
  acc1 | Accumulator 1 input
  acc2 | Accumulator 2 input

Returns
  Result of operation

## ◆ addmsc_4x2_2x8() [6/8]

v32acc32 addmsc_4x2_2x8 | ( | v32uint16 | a,
|  | int | sgn_x,
|  | v32uint16 | b,
|  | int | sgn_y,
|  | v32acc32 | acc1,
|  | v32acc32 | acc2 )

Parameters

  a | Matrix A
  sgn_x | Sign mask for matrix A
  b | Matrix B
  sgn_y | Sign mask for matrix B
  acc1 | Accumulator 1 input
  acc2 | Accumulator 2 input

Returns
  Result of operation

## ◆ addmsc_4x2_2x8() [7/8]

v32acc32 addmsc_4x2_2x8 | ( | v32uint16 | a,
|  | v32int16 | b,
|  | v32acc32 | acc1,
|  | v32acc32 | acc2 )

Parameters

  a | Matrix A
  b | Matrix B
  acc1 | Accumulator 1 input
  acc2 | Accumulator 2 input

Returns
  Result of operation

## ◆ addmsc_4x2_2x8() [8/8]

v32acc32 addmsc_4x2_2x8 | ( | v32uint16 | a,
|  | v32uint16 | b,
|  | v32acc32 | acc1,
|  | v32acc32 | acc2 )

Parameters

  a | Matrix A
  b | Matrix B
  acc1 | Accumulator 1 input
  acc2 | Accumulator 2 input

Returns
  Result of operation

## ◆ addmsc_4x2_2x8_conf() [1/8]

v32acc32 addmsc_4x2_2x8_conf | ( | v32int16 | a,
|  | int | sgn_x,
|  | v32int16 | b,
|  | int | sgn_y,
|  | v32acc32 | acc1,
|  | v32acc32 | acc2,
|  | int | zero_acc1,
|  | int | shift16,
|  | int | sub_mul,
|  | int | sub_acc1,
|  | int | sub_acc2 )

Parameters

  a | Matrix A
  sgn_x | Sign mask for matrix A
  b | Matrix B
  sgn_y | Sign mask for matrix B
  acc1 | Accumulator 1 input
  acc2 | Accumulator 2 input
  zero_acc1 | Zeroing mask for acc1
  shift16 | Shift mask of input accumulator acc1
  sub_mul | Negation mask of multiplication result.
  sub_acc1 | Negation mask of acc1
  sub_acc2 | Negation mask of acc2

Returns
  Result of operation

## ◆ addmsc_4x2_2x8_conf() [2/8]

v32acc32 addmsc_4x2_2x8_conf | ( | v32int16 | a,
|  | int | sgn_x,
|  | v32uint16 | b,
|  | int | sgn_y,
|  | v32acc32 | acc1,
|  | v32acc32 | acc2,
|  | int | zero_acc1,
|  | int | shift16,
|  | int | sub_mul,
|  | int | sub_acc1,
|  | int | sub_acc2 )

Parameters

  a | Matrix A
  sgn_x | Sign mask for matrix A
  b | Matrix B
  sgn_y | Sign mask for matrix B
  acc1 | Accumulator 1 input
  acc2 | Accumulator 2 input
  zero_acc1 | Zeroing mask for acc1
  shift16 | Shift mask of input accumulator acc1
  sub_mul | Negation mask of multiplication result.
  sub_acc1 | Negation mask of acc1
  sub_acc2 | Negation mask of acc2

Returns
  Result of operation

## ◆ addmsc_4x2_2x8_conf() [3/8]

v32acc32 addmsc_4x2_2x8_conf | ( | v32int16 | a,
|  | v32int16 | b,
|  | v32acc32 | acc1,
|  | v32acc32 | acc2,
|  | int | zero_acc1,
|  | int | shift16,
|  | int | sub_mul,
|  | int | sub_acc1,
|  | int | sub_acc2 )

Parameters

  a | Matrix A
  b | Matrix B
  acc1 | Accumulator 1 input
  acc2 | Accumulator 2 input
  zero_acc1 | Zeroing mask for acc1
  shift16 | Shift mask of input accumulator acc1
  sub_mul | Negation mask of multiplication result
  sub_acc1 | Negation mask of acc1
  sub_acc2 | Negation mask of acc2

Returns
  Result of operation

## ◆ addmsc_4x2_2x8_conf() [4/8]

v32acc32 addmsc_4x2_2x8_conf | ( | v32int16 | a,
|  | v32uint16 | b,
|  | v32acc32 | acc1,
|  | v32acc32 | acc2,
|  | int | zero_acc1,
|  | int | shift16,
|  | int | sub_mul,
|  | int | sub_acc1,
|  | int | sub_acc2 )

Parameters

  a | Matrix A
  b | Matrix B
  acc1 | Accumulator 1 input
  acc2 | Accumulator 2 input
  zero_acc1 | Zeroing mask for acc1
  shift16 | Shift mask of input accumulator acc1
  sub_mul | Negation mask of multiplication result
  sub_acc1 | Negation mask of acc1
  sub_acc2 | Negation mask of acc2

Returns
  Result of operation

## ◆ addmsc_4x2_2x8_conf() [5/8]

v32acc32 addmsc_4x2_2x8_conf | ( | v32uint16 | a,
|  | int | sgn_x,
|  | v32int16 | b,
|  | int | sgn_y,
|  | v32acc32 | acc1,
|  | v32acc32 | acc2,
|  | int | zero_acc1,
|  | int | shift16,
|  | int | sub_mul,
|  | int | sub_acc1,
|  | int | sub_acc2 )

Parameters

  a | Matrix A
  sgn_x | Sign mask for matrix A
  b | Matrix B
  sgn_y | Sign mask for matrix B
  acc1 | Accumulator 1 input
  acc2 | Accumulator 2 input
  zero_acc1 | Zeroing mask for acc1
  shift16 | Shift mask of input accumulator acc1
  sub_mul | Negation mask of multiplication result.
  sub_acc1 | Negation mask of acc1
  sub_acc2 | Negation mask of acc2

Returns
  Result of operation

## ◆ addmsc_4x2_2x8_conf() [6/8]

v32acc32 addmsc_4x2_2x8_conf | ( | v32uint16 | a,
|  | int | sgn_x,
|  | v32uint16 | b,
|  | int | sgn_y,
|  | v32acc32 | acc1,
|  | v32acc32 | acc2,
|  | int | zero_acc1,
|  | int | shift16,
|  | int | sub_mul,
|  | int | sub_acc1,
|  | int | sub_acc2 )

Parameters

  a | Matrix A
  sgn_x | Sign mask for matrix A
  b | Matrix B
  sgn_y | Sign mask for matrix B
  acc1 | Accumulator 1 input
  acc2 | Accumulator 2 input
  zero_acc1 | Zeroing mask for acc1
  shift16 | Shift mask of input accumulator acc1
  sub_mul | Negation mask of multiplication result.
  sub_acc1 | Negation mask of acc1
  sub_acc2 | Negation mask of acc2

Returns
  Result of operation

## ◆ addmsc_4x2_2x8_conf() [7/8]

v32acc32 addmsc_4x2_2x8_conf | ( | v32uint16 | a,
|  | v32int16 | b,
|  | v32acc32 | acc1,
|  | v32acc32 | acc2,
|  | int | zero_acc1,
|  | int | shift16,
|  | int | sub_mul,
|  | int | sub_acc1,
|  | int | sub_acc2 )

Parameters

  a | Matrix A
  b | Matrix B
  acc1 | Accumulator 1 input
  acc2 | Accumulator 2 input
  zero_acc1 | Zeroing mask for acc1
  shift16 | Shift mask of input accumulator acc1
  sub_mul | Negation mask of multiplication result
  sub_acc1 | Negation mask of acc1
  sub_acc2 | Negation mask of acc2

Returns
  Result of operation

## ◆ addmsc_4x2_2x8_conf() [8/8]

v32acc32 addmsc_4x2_2x8_conf | ( | v32uint16 | a,
|  | v32uint16 | b,
|  | v32acc32 | acc1,
|  | v32acc32 | acc2,
|  | int | zero_acc1,
|  | int | shift16,
|  | int | sub_mul,
|  | int | sub_acc1,
|  | int | sub_acc2 )

Parameters

  a | Matrix A
  b | Matrix B
  acc1 | Accumulator 1 input
  acc2 | Accumulator 2 input
  zero_acc1 | Zeroing mask for acc1
  shift16 | Shift mask of input accumulator acc1
  sub_mul | Negation mask of multiplication result
  sub_acc1 | Negation mask of acc1
  sub_acc2 | Negation mask of acc2

Returns
  Result of operation

## ◆ addmsc_4x4_4x4() [1/8]

v16acc64 addmsc_4x4_4x4 | ( | v32int16 | a,
|  | int | sgn_x,
|  | v32int16 | b,
|  | int | sgn_y,
|  | v16acc64 | acc1,
|  | v16acc64 | acc2 )

Parameters

  a | Matrix A
  sgn_x | Sign mask for matrix A
  b | Matrix B
  sgn_y | Sign mask for matrix B
  acc1 | Accumulator 1 input
  acc2 | Accumulator 2 input

Returns
  Result of operation

## ◆ addmsc_4x4_4x4() [2/8]

v16acc64 addmsc_4x4_4x4 | ( | v32int16 | a,
|  | int | sgn_x,
|  | v32uint16 | b,
|  | int | sgn_y,
|  | v16acc64 | acc1,
|  | v16acc64 | acc2 )

Parameters

  a | Matrix A
  sgn_x | Sign mask for matrix A
  b | Matrix B
  sgn_y | Sign mask for matrix B
  acc1 | Accumulator 1 input
  acc2 | Accumulator 2 input

Returns
  Result of operation

## ◆ addmsc_4x4_4x4() [3/8]

v16acc64 addmsc_4x4_4x4 | ( | v32int16 | a,
|  | v32int16 | b,
|  | v16acc64 | acc1,
|  | v16acc64 | acc2 )

Parameters

  a | Matrix A
  b | Matrix B
  acc1 | Accumulator 1 input
  acc2 | Accumulator 2 input

Returns
  Result of operation

## ◆ addmsc_4x4_4x4() [4/8]

v16acc64 addmsc_4x4_4x4 | ( | v32int16 | a,
|  | v32uint16 | b,
|  | v16acc64 | acc1,
|  | v16acc64 | acc2 )

Parameters

  a | Matrix A
  b | Matrix B
  acc1 | Accumulator 1 input
  acc2 | Accumulator 2 input

Returns
  Result of operation

## ◆ addmsc_4x4_4x4() [5/8]

v16acc64 addmsc_4x4_4x4 | ( | v32uint16 | a,
|  | int | sgn_x,
|  | v32int16 | b,
|  | int | sgn_y,
|  | v16acc64 | acc1,
|  | v16acc64 | acc2 )

Parameters

  a | Matrix A
  sgn_x | Sign mask for matrix A
  b | Matrix B
  sgn_y | Sign mask for matrix B
  acc1 | Accumulator 1 input
  acc2 | Accumulator 2 input

Returns
  Result of operation

## ◆ addmsc_4x4_4x4() [6/8]

v16acc64 addmsc_4x4_4x4 | ( | v32uint16 | a,
|  | int | sgn_x,
|  | v32uint16 | b,
|  | int | sgn_y,
|  | v16acc64 | acc1,
|  | v16acc64 | acc2 )

Parameters

  a | Matrix A
  sgn_x | Sign mask for matrix A
  b | Matrix B
  sgn_y | Sign mask for matrix B
  acc1 | Accumulator 1 input
  acc2 | Accumulator 2 input

Returns
  Result of operation

## ◆ addmsc_4x4_4x4() [7/8]

v16acc64 addmsc_4x4_4x4 | ( | v32uint16 | a,
|  | v32int16 | b,
|  | v16acc64 | acc1,
|  | v16acc64 | acc2 )

Parameters

  a | Matrix A
  b | Matrix B
  acc1 | Accumulator 1 input
  acc2 | Accumulator 2 input

Returns
  Result of operation

## ◆ addmsc_4x4_4x4() [8/8]

v16acc64 addmsc_4x4_4x4 | ( | v32uint16 | a,
|  | v32uint16 | b,
|  | v16acc64 | acc1,
|  | v16acc64 | acc2 )

Parameters

  a | Matrix A
  b | Matrix B
  acc1 | Accumulator 1 input
  acc2 | Accumulator 2 input

Returns
  Result of operation

## ◆ addmsc_4x4_4x4_conf() [1/8]

v16acc64 addmsc_4x4_4x4_conf | ( | v32int16 | a,
|  | int | sgn_x,
|  | v32int16 | b,
|  | int | sgn_y,
|  | v16acc64 | acc1,
|  | v16acc64 | acc2,
|  | int | zero_acc1,
|  | int | shift16,
|  | int | sub_mul,
|  | int | sub_acc1,
|  | int | sub_acc2 )

Parameters

  a | Matrix A
  sgn_x | Sign mask for matrix A
  b | Matrix B
  sgn_y | Sign mask for matrix B
  acc1 | Accumulator 1 input
  acc2 | Accumulator 2 input
  zero_acc1 | Zeroing mask for acc1
  shift16 | Shift mask of input accumulator acc1
  sub_mul | Negation mask of multiplication result.
  sub_acc1 | Negation mask of acc1
  sub_acc2 | Negation mask of acc2

Returns
  Result of operation

## ◆ addmsc_4x4_4x4_conf() [2/8]

v16acc64 addmsc_4x4_4x4_conf | ( | v32int16 | a,
|  | int | sgn_x,
|  | v32uint16 | b,
|  | int | sgn_y,
|  | v16acc64 | acc1,
|  | v16acc64 | acc2,
|  | int | zero_acc1,
|  | int | shift16,
|  | int | sub_mul,
|  | int | sub_acc1,
|  | int | sub_acc2 )

Parameters

  a | Matrix A
  sgn_x | Sign mask for matrix A
  b | Matrix B
  sgn_y | Sign mask for matrix B
  acc1 | Accumulator 1 input
  acc2 | Accumulator 2 input
  zero_acc1 | Zeroing mask for acc1
  shift16 | Shift mask of input accumulator acc1
  sub_mul | Negation mask of multiplication result.
  sub_acc1 | Negation mask of acc1
  sub_acc2 | Negation mask of acc2

Returns
  Result of operation

## ◆ addmsc_4x4_4x4_conf() [3/8]

v16acc64 addmsc_4x4_4x4_conf | ( | v32int16 | a,
|  | v32int16 | b,
|  | v16acc64 | acc1,
|  | v16acc64 | acc2,
|  | int | zero_acc1,
|  | int | shift16,
|  | int | sub_mul,
|  | int | sub_acc1,
|  | int | sub_acc2 )

Parameters

  a | Matrix A
  b | Matrix B
  acc1 | Accumulator 1 input
  acc2 | Accumulator 2 input
  zero_acc1 | Zeroing mask for acc1
  shift16 | Shift mask of input accumulator acc1
  sub_mul | Negation mask of multiplication result
  sub_acc1 | Negation mask of acc1
  sub_acc2 | Negation mask of acc2

Returns
  Result of operation

## ◆ addmsc_4x4_4x4_conf() [4/8]

v16acc64 addmsc_4x4_4x4_conf | ( | v32int16 | a,
|  | v32uint16 | b,
|  | v16acc64 | acc1,
|  | v16acc64 | acc2,
|  | int | zero_acc1,
|  | int | shift16,
|  | int | sub_mul,
|  | int | sub_acc1,
|  | int | sub_acc2 )

Parameters

  a | Matrix A
  b | Matrix B
  acc1 | Accumulator 1 input
  acc2 | Accumulator 2 input
  zero_acc1 | Zeroing mask for acc1
  shift16 | Shift mask of input accumulator acc1
  sub_mul | Negation mask of multiplication result
  sub_acc1 | Negation mask of acc1
  sub_acc2 | Negation mask of acc2

Returns
  Result of operation

## ◆ addmsc_4x4_4x4_conf() [5/8]

v16acc64 addmsc_4x4_4x4_conf | ( | v32uint16 | a,
|  | int | sgn_x,
|  | v32int16 | b,
|  | int | sgn_y,
|  | v16acc64 | acc1,
|  | v16acc64 | acc2,
|  | int | zero_acc1,
|  | int | shift16,
|  | int | sub_mul,
|  | int | sub_acc1,
|  | int | sub_acc2 )

Parameters

  a | Matrix A
  sgn_x | Sign mask for matrix A
  b | Matrix B
  sgn_y | Sign mask for matrix B
  acc1 | Accumulator 1 input
  acc2 | Accumulator 2 input
  zero_acc1 | Zeroing mask for acc1
  shift16 | Shift mask of input accumulator acc1
  sub_mul | Negation mask of multiplication result.
  sub_acc1 | Negation mask of acc1
  sub_acc2 | Negation mask of acc2

Returns
  Result of operation

## ◆ addmsc_4x4_4x4_conf() [6/8]

v16acc64 addmsc_4x4_4x4_conf | ( | v32uint16 | a,
|  | int | sgn_x,
|  | v32uint16 | b,
|  | int | sgn_y,
|  | v16acc64 | acc1,
|  | v16acc64 | acc2,
|  | int | zero_acc1,
|  | int | shift16,
|  | int | sub_mul,
|  | int | sub_acc1,
|  | int | sub_acc2 )

Parameters

  a | Matrix A
  sgn_x | Sign mask for matrix A
  b | Matrix B
  sgn_y | Sign mask for matrix B
  acc1 | Accumulator 1 input
  acc2 | Accumulator 2 input
  zero_acc1 | Zeroing mask for acc1
  shift16 | Shift mask of input accumulator acc1
  sub_mul | Negation mask of multiplication result.
  sub_acc1 | Negation mask of acc1
  sub_acc2 | Negation mask of acc2

Returns
  Result of operation

## ◆ addmsc_4x4_4x4_conf() [7/8]

v16acc64 addmsc_4x4_4x4_conf | ( | v32uint16 | a,
|  | v32int16 | b,
|  | v16acc64 | acc1,
|  | v16acc64 | acc2,
|  | int | zero_acc1,
|  | int | shift16,
|  | int | sub_mul,
|  | int | sub_acc1,
|  | int | sub_acc2 )

Parameters

  a | Matrix A
  b | Matrix B
  acc1 | Accumulator 1 input
  acc2 | Accumulator 2 input
  zero_acc1 | Zeroing mask for acc1
  shift16 | Shift mask of input accumulator acc1
  sub_mul | Negation mask of multiplication result
  sub_acc1 | Negation mask of acc1
  sub_acc2 | Negation mask of acc2

Returns
  Result of operation

## ◆ addmsc_4x4_4x4_conf() [8/8]

v16acc64 addmsc_4x4_4x4_conf | ( | v32uint16 | a,
|  | v32uint16 | b,
|  | v16acc64 | acc1,
|  | v16acc64 | acc2,
|  | int | zero_acc1,
|  | int | shift16,
|  | int | sub_mul,
|  | int | sub_acc1,
|  | int | sub_acc2 )

Parameters

  a | Matrix A
  b | Matrix B
  acc1 | Accumulator 1 input
  acc2 | Accumulator 2 input
  zero_acc1 | Zeroing mask for acc1
  shift16 | Shift mask of input accumulator acc1
  sub_mul | Negation mask of multiplication result
  sub_acc1 | Negation mask of acc1
  sub_acc2 | Negation mask of acc2

Returns
  Result of operation

## ◆ addmsc_conv_16x4() [1/8]

v16acc64 addmsc_conv_16x4 | ( | v32int16 | a,
|  | int | sgn_x,
|  | v32int16 | b,
|  | int | sgn_y,
|  | v16acc64 | acc1,
|  | v16acc64 | acc2 )

Parameters

  a | Matrix A
  sgn_x | Sign mask for matrix A
  b | Matrix B
  sgn_y | Sign mask for matrix B
  acc1 | Accumulator 1 input
  acc2 | Accumulator 2 input

Returns
  Result of operation

## ◆ addmsc_conv_16x4() [2/8]

v16acc64 addmsc_conv_16x4 | ( | v32int16 | a,
|  | int | sgn_x,
|  | v32uint16 | b,
|  | int | sgn_y,
|  | v16acc64 | acc1,
|  | v16acc64 | acc2 )

Parameters

  a | Matrix A
  sgn_x | Sign mask for matrix A
  b | Matrix B
  sgn_y | Sign mask for matrix B
  acc1 | Accumulator 1 input
  acc2 | Accumulator 2 input

Returns
  Result of operation

## ◆ addmsc_conv_16x4() [3/8]

v16acc64 addmsc_conv_16x4 | ( | v32int16 | a,
|  | v32int16 | b,
|  | v16acc64 | acc1,
|  | v16acc64 | acc2 )

Parameters

  a | Matrix A
  b | Matrix B
  acc1 | Accumulator 1 input
  acc2 | Accumulator 2 input

Returns
  Result of operation

## ◆ addmsc_conv_16x4() [4/8]

v16acc64 addmsc_conv_16x4 | ( | v32int16 | a,
|  | v32uint16 | b,
|  | v16acc64 | acc1,
|  | v16acc64 | acc2 )

Parameters

  a | Matrix A
  b | Matrix B
  acc1 | Accumulator 1 input
  acc2 | Accumulator 2 input

Returns
  Result of operation

## ◆ addmsc_conv_16x4() [5/8]

v16acc64 addmsc_conv_16x4 | ( | v32uint16 | a,
|  | int | sgn_x,
|  | v32int16 | b,
|  | int | sgn_y,
|  | v16acc64 | acc1,
|  | v16acc64 | acc2 )

Parameters

  a | Matrix A
  sgn_x | Sign mask for matrix A
  b | Matrix B
  sgn_y | Sign mask for matrix B
  acc1 | Accumulator 1 input
  acc2 | Accumulator 2 input

Returns
  Result of operation

## ◆ addmsc_conv_16x4() [6/8]

v16acc64 addmsc_conv_16x4 | ( | v32uint16 | a,
|  | int | sgn_x,
|  | v32uint16 | b,
|  | int | sgn_y,
|  | v16acc64 | acc1,
|  | v16acc64 | acc2 )

Parameters

  a | Matrix A
  sgn_x | Sign mask for matrix A
  b | Matrix B
  sgn_y | Sign mask for matrix B
  acc1 | Accumulator 1 input
  acc2 | Accumulator 2 input

Returns
  Result of operation

## ◆ addmsc_conv_16x4() [7/8]

v16acc64 addmsc_conv_16x4 | ( | v32uint16 | a,
|  | v32int16 | b,
|  | v16acc64 | acc1,
|  | v16acc64 | acc2 )

Parameters

  a | Matrix A
  b | Matrix B
  acc1 | Accumulator 1 input
  acc2 | Accumulator 2 input

Returns
  Result of operation

## ◆ addmsc_conv_16x4() [8/8]

v16acc64 addmsc_conv_16x4 | ( | v32uint16 | a,
|  | v32uint16 | b,
|  | v16acc64 | acc1,
|  | v16acc64 | acc2 )

Parameters

  a | Matrix A
  b | Matrix B
  acc1 | Accumulator 1 input
  acc2 | Accumulator 2 input

Returns
  Result of operation

## ◆ addmsc_conv_16x4_conf() [1/8]

v16acc64 addmsc_conv_16x4_conf | ( | v32int16 | a,
|  | int | sgn_x,
|  | v32int16 | b,
|  | int | sgn_y,
|  | v16acc64 | acc1,
|  | v16acc64 | acc2,
|  | int | zero_acc1,
|  | int | shift16,
|  | int | sub_mul,
|  | int | sub_acc1,
|  | int | sub_acc2 )

Parameters

  a | Matrix A
  sgn_x | Sign mask for matrix A
  b | Matrix B
  sgn_y | Sign mask for matrix B
  acc1 | Accumulator 1 input
  acc2 | Accumulator 2 input
  zero_acc1 | Zeroing mask for acc1
  shift16 | Shift mask of input accumulator acc1
  sub_mul | Negation mask of multiplication result.
  sub_acc1 | Negation mask of acc1
  sub_acc2 | Negation mask of acc2

Returns
  Result of operation

## ◆ addmsc_conv_16x4_conf() [2/8]

v16acc64 addmsc_conv_16x4_conf | ( | v32int16 | a,
|  | int | sgn_x,
|  | v32uint16 | b,
|  | int | sgn_y,
|  | v16acc64 | acc1,
|  | v16acc64 | acc2,
|  | int | zero_acc1,
|  | int | shift16,
|  | int | sub_mul,
|  | int | sub_acc1,
|  | int | sub_acc2 )

Parameters

  a | Matrix A
  sgn_x | Sign mask for matrix A
  b | Matrix B
  sgn_y | Sign mask for matrix B
  acc1 | Accumulator 1 input
  acc2 | Accumulator 2 input
  zero_acc1 | Zeroing mask for acc1
  shift16 | Shift mask of input accumulator acc1
  sub_mul | Negation mask of multiplication result.
  sub_acc1 | Negation mask of acc1
  sub_acc2 | Negation mask of acc2

Returns
  Result of operation

## ◆ addmsc_conv_16x4_conf() [3/8]

v16acc64 addmsc_conv_16x4_conf | ( | v32int16 | a,
|  | v32int16 | b,
|  | v16acc64 | acc1,
|  | v16acc64 | acc2,
|  | int | zero_acc1,
|  | int | shift16,
|  | int | sub_mul,
|  | int | sub_acc1,
|  | int | sub_acc2 )

Parameters

  a | Matrix A
  b | Matrix B
  acc1 | Accumulator 1 input
  acc2 | Accumulator 2 input
  zero_acc1 | Zeroing mask for acc1
  shift16 | Shift mask of input accumulator acc1
  sub_mul | Negation mask of multiplication result
  sub_acc1 | Negation mask of acc1
  sub_acc2 | Negation mask of acc2

Returns
  Result of operation

## ◆ addmsc_conv_16x4_conf() [4/8]

v16acc64 addmsc_conv_16x4_conf | ( | v32int16 | a,
|  | v32uint16 | b,
|  | v16acc64 | acc1,
|  | v16acc64 | acc2,
|  | int | zero_acc1,
|  | int | shift16,
|  | int | sub_mul,
|  | int | sub_acc1,
|  | int | sub_acc2 )

Parameters

  a | Matrix A
  b | Matrix B
  acc1 | Accumulator 1 input
  acc2 | Accumulator 2 input
  zero_acc1 | Zeroing mask for acc1
  shift16 | Shift mask of input accumulator acc1
  sub_mul | Negation mask of multiplication result
  sub_acc1 | Negation mask of acc1
  sub_acc2 | Negation mask of acc2

Returns
  Result of operation

## ◆ addmsc_conv_16x4_conf() [5/8]

v16acc64 addmsc_conv_16x4_conf | ( | v32uint16 | a,
|  | int | sgn_x,
|  | v32int16 | b,
|  | int | sgn_y,
|  | v16acc64 | acc1,
|  | v16acc64 | acc2,
|  | int | zero_acc1,
|  | int | shift16,
|  | int | sub_mul,
|  | int | sub_acc1,
|  | int | sub_acc2 )

Parameters

  a | Matrix A
  sgn_x | Sign mask for matrix A
  b | Matrix B
  sgn_y | Sign mask for matrix B
  acc1 | Accumulator 1 input
  acc2 | Accumulator 2 input
  zero_acc1 | Zeroing mask for acc1
  shift16 | Shift mask of input accumulator acc1
  sub_mul | Negation mask of multiplication result.
  sub_acc1 | Negation mask of acc1
  sub_acc2 | Negation mask of acc2

Returns
  Result of operation

## ◆ addmsc_conv_16x4_conf() [6/8]

v16acc64 addmsc_conv_16x4_conf | ( | v32uint16 | a,
|  | int | sgn_x,
|  | v32uint16 | b,
|  | int | sgn_y,
|  | v16acc64 | acc1,
|  | v16acc64 | acc2,
|  | int | zero_acc1,
|  | int | shift16,
|  | int | sub_mul,
|  | int | sub_acc1,
|  | int | sub_acc2 )

Parameters

  a | Matrix A
  sgn_x | Sign mask for matrix A
  b | Matrix B
  sgn_y | Sign mask for matrix B
  acc1 | Accumulator 1 input
  acc2 | Accumulator 2 input
  zero_acc1 | Zeroing mask for acc1
  shift16 | Shift mask of input accumulator acc1
  sub_mul | Negation mask of multiplication result.
  sub_acc1 | Negation mask of acc1
  sub_acc2 | Negation mask of acc2

Returns
  Result of operation

## ◆ addmsc_conv_16x4_conf() [7/8]

v16acc64 addmsc_conv_16x4_conf | ( | v32uint16 | a,
|  | v32int16 | b,
|  | v16acc64 | acc1,
|  | v16acc64 | acc2,
|  | int | zero_acc1,
|  | int | shift16,
|  | int | sub_mul,
|  | int | sub_acc1,
|  | int | sub_acc2 )

Parameters

  a | Matrix A
  b | Matrix B
  acc1 | Accumulator 1 input
  acc2 | Accumulator 2 input
  zero_acc1 | Zeroing mask for acc1
  shift16 | Shift mask of input accumulator acc1
  sub_mul | Negation mask of multiplication result
  sub_acc1 | Negation mask of acc1
  sub_acc2 | Negation mask of acc2

Returns
  Result of operation

## ◆ addmsc_conv_16x4_conf() [8/8]

v16acc64 addmsc_conv_16x4_conf | ( | v32uint16 | a,
|  | v32uint16 | b,
|  | v16acc64 | acc1,
|  | v16acc64 | acc2,
|  | int | zero_acc1,
|  | int | shift16,
|  | int | sub_mul,
|  | int | sub_acc1,
|  | int | sub_acc2 )

Parameters

  a | Matrix A
  b | Matrix B
  acc1 | Accumulator 1 input
  acc2 | Accumulator 2 input
  zero_acc1 | Zeroing mask for acc1
  shift16 | Shift mask of input accumulator acc1
  sub_mul | Negation mask of multiplication result
  sub_acc1 | Negation mask of acc1
  sub_acc2 | Negation mask of acc2

Returns
  Result of operation

## ◆ addmsc_elem_16_2() [1/9]

v16accfloat addmsc_elem_16_2 | ( | v32bfloat16 | a,
|  | v32bfloat16 | b,
|  | v16accfloat | acc1,
|  | v16accfloat | acc2 )

Parameters

  a | Matrix A
  b | Matrix B
  acc1 | Accumulator 1 input
  acc2 | Accumulator 2 input

Returns
  Result of operation

## ◆ addmsc_elem_16_2() [2/9]

v16acc64 addmsc_elem_16_2 | ( | v32int16 | a,
|  | int | sgn_x,
|  | v32int16 | b,
|  | int | sgn_y,
|  | v16acc64 | acc1,
|  | v16acc64 | acc2 )

Parameters

  a | Matrix A
  sgn_x | Sign mask for matrix A
  b | Matrix B
  sgn_y | Sign mask for matrix B
  acc1 | Accumulator 1 input
  acc2 | Accumulator 2 input

Returns
  Result of operation

## ◆ addmsc_elem_16_2() [3/9]

v16acc64 addmsc_elem_16_2 | ( | v32int16 | a,
|  | int | sgn_x,
|  | v32uint16 | b,
|  | int | sgn_y,
|  | v16acc64 | acc1,
|  | v16acc64 | acc2 )

Parameters

  a | Matrix A
  sgn_x | Sign mask for matrix A
  b | Matrix B
  sgn_y | Sign mask for matrix B
  acc1 | Accumulator 1 input
  acc2 | Accumulator 2 input

Returns
  Result of operation

## ◆ addmsc_elem_16_2() [4/9]

v16acc64 addmsc_elem_16_2 | ( | v32int16 | a,
|  | v32int16 | b,
|  | v16acc64 | acc1,
|  | v16acc64 | acc2 )

Parameters

  a | Matrix A
  b | Matrix B
  acc1 | Accumulator 1 input
  acc2 | Accumulator 2 input

Returns
  Result of operation

## ◆ addmsc_elem_16_2() [5/9]

v16acc64 addmsc_elem_16_2 | ( | v32int16 | a,
|  | v32uint16 | b,
|  | v16acc64 | acc1,
|  | v16acc64 | acc2 )

Parameters

  a | Matrix A
  b | Matrix B
  acc1 | Accumulator 1 input
  acc2 | Accumulator 2 input

Returns
  Result of operation

## ◆ addmsc_elem_16_2() [6/9]

v16acc64 addmsc_elem_16_2 | ( | v32uint16 | a,
|  | int | sgn_x,
|  | v32int16 | b,
|  | int | sgn_y,
|  | v16acc64 | acc1,
|  | v16acc64 | acc2 )

Parameters

  a | Matrix A
  sgn_x | Sign mask for matrix A
  b | Matrix B
  sgn_y | Sign mask for matrix B
  acc1 | Accumulator 1 input
  acc2 | Accumulator 2 input

Returns
  Result of operation

## ◆ addmsc_elem_16_2() [7/9]

v16acc64 addmsc_elem_16_2 | ( | v32uint16 | a,
|  | int | sgn_x,
|  | v32uint16 | b,
|  | int | sgn_y,
|  | v16acc64 | acc1,
|  | v16acc64 | acc2 )

Parameters

  a | Matrix A
  sgn_x | Sign mask for matrix A
  b | Matrix B
  sgn_y | Sign mask for matrix B
  acc1 | Accumulator 1 input
  acc2 | Accumulator 2 input

Returns
  Result of operation

## ◆ addmsc_elem_16_2() [8/9]

v16acc64 addmsc_elem_16_2 | ( | v32uint16 | a,
|  | v32int16 | b,
|  | v16acc64 | acc1,
|  | v16acc64 | acc2 )

Parameters

  a | Matrix A
  b | Matrix B
  acc1 | Accumulator 1 input
  acc2 | Accumulator 2 input

Returns
  Result of operation

## ◆ addmsc_elem_16_2() [9/9]

v16acc64 addmsc_elem_16_2 | ( | v32uint16 | a,
|  | v32uint16 | b,
|  | v16acc64 | acc1,
|  | v16acc64 | acc2 )

Parameters

  a | Matrix A
  b | Matrix B
  acc1 | Accumulator 1 input
  acc2 | Accumulator 2 input

Returns
  Result of operation

## ◆ addmsc_elem_16_2_conf() [1/9]

v16accfloat addmsc_elem_16_2_conf | ( | v32bfloat16 | a,
|  | v32bfloat16 | b,
|  | v16accfloat | acc1,
|  | v16accfloat | acc2,
|  | int | zero_acc1,
|  | int | sub_mul,
|  | int | sub_acc1,
|  | int | sub_acc2 )

Parameters

  a | Matrix A
  b | Matrix B
  acc1 | Accumulator 1 input
  acc2 | Accumulator 2 input
  zero_acc1 | Zeroing mask for acc1
  sub_mul | Negation mask of multiplication result
  sub_acc1 | Negation mask of acc1
  sub_acc2 | Negation mask of acc2

Returns
  Result of operation

## ◆ addmsc_elem_16_2_conf() [2/9]

v16acc64 addmsc_elem_16_2_conf | ( | v32int16 | a,
|  | int | sgn_x,
|  | v32int16 | b,
|  | int | sgn_y,
|  | v16acc64 | acc1,
|  | v16acc64 | acc2,
|  | int | zero_acc1,
|  | int | shift16,
|  | int | sub_mul,
|  | int | sub_acc1,
|  | int | sub_acc2 )

Parameters

  a | Matrix A
  sgn_x | Sign mask for matrix A
  b | Matrix B
  sgn_y | Sign mask for matrix B
  acc1 | Accumulator 1 input
  acc2 | Accumulator 2 input
  zero_acc1 | Zeroing mask for acc1
  shift16 | Shift mask of input accumulator acc1
  sub_mul | Negation mask of multiplication result.
  sub_acc1 | Negation mask of acc1
  sub_acc2 | Negation mask of acc2

Returns
  Result of operation

## ◆ addmsc_elem_16_2_conf() [3/9]

v16acc64 addmsc_elem_16_2_conf | ( | v32int16 | a,
|  | int | sgn_x,
|  | v32uint16 | b,
|  | int | sgn_y,
|  | v16acc64 | acc1,
|  | v16acc64 | acc2,
|  | int | zero_acc1,
|  | int | shift16,
|  | int | sub_mul,
|  | int | sub_acc1,
|  | int | sub_acc2 )

Parameters

  a | Matrix A
  sgn_x | Sign mask for matrix A
  b | Matrix B
  sgn_y | Sign mask for matrix B
  acc1 | Accumulator 1 input
  acc2 | Accumulator 2 input
  zero_acc1 | Zeroing mask for acc1
  shift16 | Shift mask of input accumulator acc1
  sub_mul | Negation mask of multiplication result.
  sub_acc1 | Negation mask of acc1
  sub_acc2 | Negation mask of acc2

Returns
  Result of operation

## ◆ addmsc_elem_16_2_conf() [4/9]

v16acc64 addmsc_elem_16_2_conf | ( | v32int16 | a,
|  | v32int16 | b,
|  | v16acc64 | acc1,
|  | v16acc64 | acc2,
|  | int | zero_acc1,
|  | int | shift16,
|  | int | sub_mul,
|  | int | sub_acc1,
|  | int | sub_acc2 )

Parameters

  a | Matrix A
  b | Matrix B
  acc1 | Accumulator 1 input
  acc2 | Accumulator 2 input
  zero_acc1 | Zeroing mask for acc1
  shift16 | Shift mask of input accumulator acc1
  sub_mul | Negation mask of multiplication result
  sub_acc1 | Negation mask of acc1
  sub_acc2 | Negation mask of acc2

Returns
  Result of operation

## ◆ addmsc_elem_16_2_conf() [5/9]

v16acc64 addmsc_elem_16_2_conf | ( | v32int16 | a,
|  | v32uint16 | b,
|  | v16acc64 | acc1,
|  | v16acc64 | acc2,
|  | int | zero_acc1,
|  | int | shift16,
|  | int | sub_mul,
|  | int | sub_acc1,
|  | int | sub_acc2 )

Parameters

  a | Matrix A
  b | Matrix B
  acc1 | Accumulator 1 input
  acc2 | Accumulator 2 input
  zero_acc1 | Zeroing mask for acc1
  shift16 | Shift mask of input accumulator acc1
  sub_mul | Negation mask of multiplication result
  sub_acc1 | Negation mask of acc1
  sub_acc2 | Negation mask of acc2

Returns
  Result of operation

## ◆ addmsc_elem_16_2_conf() [6/9]

v16acc64 addmsc_elem_16_2_conf | ( | v32uint16 | a,
|  | int | sgn_x,
|  | v32int16 | b,
|  | int | sgn_y,
|  | v16acc64 | acc1,
|  | v16acc64 | acc2,
|  | int | zero_acc1,
|  | int | shift16,
|  | int | sub_mul,
|  | int | sub_acc1,
|  | int | sub_acc2 )

Parameters

  a | Matrix A
  sgn_x | Sign mask for matrix A
  b | Matrix B
  sgn_y | Sign mask for matrix B
  acc1 | Accumulator 1 input
  acc2 | Accumulator 2 input
  zero_acc1 | Zeroing mask for acc1
  shift16 | Shift mask of input accumulator acc1
  sub_mul | Negation mask of multiplication result.
  sub_acc1 | Negation mask of acc1
  sub_acc2 | Negation mask of acc2

Returns
  Result of operation

## ◆ addmsc_elem_16_2_conf() [7/9]

v16acc64 addmsc_elem_16_2_conf | ( | v32uint16 | a,
|  | int | sgn_x,
|  | v32uint16 | b,
|  | int | sgn_y,
|  | v16acc64 | acc1,
|  | v16acc64 | acc2,
|  | int | zero_acc1,
|  | int | shift16,
|  | int | sub_mul,
|  | int | sub_acc1,
|  | int | sub_acc2 )

Parameters

  a | Matrix A
  sgn_x | Sign mask for matrix A
  b | Matrix B
  sgn_y | Sign mask for matrix B
  acc1 | Accumulator 1 input
  acc2 | Accumulator 2 input
  zero_acc1 | Zeroing mask for acc1
  shift16 | Shift mask of input accumulator acc1
  sub_mul | Negation mask of multiplication result.
  sub_acc1 | Negation mask of acc1
  sub_acc2 | Negation mask of acc2

Returns
  Result of operation

## ◆ addmsc_elem_16_2_conf() [8/9]

v16acc64 addmsc_elem_16_2_conf | ( | v32uint16 | a,
|  | v32int16 | b,
|  | v16acc64 | acc1,
|  | v16acc64 | acc2,
|  | int | zero_acc1,
|  | int | shift16,
|  | int | sub_mul,
|  | int | sub_acc1,
|  | int | sub_acc2 )

Parameters

  a | Matrix A
  b | Matrix B
  acc1 | Accumulator 1 input
  acc2 | Accumulator 2 input
  zero_acc1 | Zeroing mask for acc1
  shift16 | Shift mask of input accumulator acc1
  sub_mul | Negation mask of multiplication result
  sub_acc1 | Negation mask of acc1
  sub_acc2 | Negation mask of acc2

Returns
  Result of operation

## ◆ addmsc_elem_16_2_conf() [9/9]

v16acc64 addmsc_elem_16_2_conf | ( | v32uint16 | a,
|  | v32uint16 | b,
|  | v16acc64 | acc1,
|  | v16acc64 | acc2,
|  | int | zero_acc1,
|  | int | shift16,
|  | int | sub_mul,
|  | int | sub_acc1,
|  | int | sub_acc2 )

Parameters

  a | Matrix A
  b | Matrix B
  acc1 | Accumulator 1 input
  acc2 | Accumulator 2 input
  zero_acc1 | Zeroing mask for acc1
  shift16 | Shift mask of input accumulator acc1
  sub_mul | Negation mask of multiplication result
  sub_acc1 | Negation mask of acc1
  sub_acc2 | Negation mask of acc2

Returns
  Result of operation

## ◆ addmsc_elem_32() [1/8]

v32acc32 addmsc_elem_32 | ( | v32int16 | a,
|  | int | sgn_x,
|  | v32int16 | b,
|  | int | sgn_y,
|  | v32acc32 | acc1,
|  | v32acc32 | acc2 )

Parameters

  a | Matrix A
  sgn_x | Sign mask for matrix A
  b | Matrix B
  sgn_y | Sign mask for matrix B
  acc1 | Accumulator 1 input
  acc2 | Accumulator 2 input

Returns
  Result of operation

## ◆ addmsc_elem_32() [2/8]

v32acc32 addmsc_elem_32 | ( | v32int16 | a,
|  | int | sgn_x,
|  | v32uint16 | b,
|  | int | sgn_y,
|  | v32acc32 | acc1,
|  | v32acc32 | acc2 )

Parameters

  a | Matrix A
  sgn_x | Sign mask for matrix A
  b | Matrix B
  sgn_y | Sign mask for matrix B
  acc1 | Accumulator 1 input
  acc2 | Accumulator 2 input

Returns
  Result of operation

## ◆ addmsc_elem_32() [3/8]

v32acc32 addmsc_elem_32 | ( | v32int16 | a,
|  | v32int16 | b,
|  | v32acc32 | acc1,
|  | v32acc32 | acc2 )

Parameters

  a | Matrix A
  b | Matrix B
  acc1 | Accumulator 1 input
  acc2 | Accumulator 2 input

Returns
  Result of operation

## ◆ addmsc_elem_32() [4/8]

v32acc32 addmsc_elem_32 | ( | v32int16 | a,
|  | v32uint16 | b,
|  | v32acc32 | acc1,
|  | v32acc32 | acc2 )

Parameters

  a | Matrix A
  b | Matrix B
  acc1 | Accumulator 1 input
  acc2 | Accumulator 2 input

Returns
  Result of operation

## ◆ addmsc_elem_32() [5/8]

v32acc32 addmsc_elem_32 | ( | v32uint16 | a,
|  | int | sgn_x,
|  | v32int16 | b,
|  | int | sgn_y,
|  | v32acc32 | acc1,
|  | v32acc32 | acc2 )

Parameters

  a | Matrix A
  sgn_x | Sign mask for matrix A
  b | Matrix B
  sgn_y | Sign mask for matrix B
  acc1 | Accumulator 1 input
  acc2 | Accumulator 2 input

Returns
  Result of operation

## ◆ addmsc_elem_32() [6/8]

v32acc32 addmsc_elem_32 | ( | v32uint16 | a,
|  | int | sgn_x,
|  | v32uint16 | b,
|  | int | sgn_y,
|  | v32acc32 | acc1,
|  | v32acc32 | acc2 )

Parameters

  a | Matrix A
  sgn_x | Sign mask for matrix A
  b | Matrix B
  sgn_y | Sign mask for matrix B
  acc1 | Accumulator 1 input
  acc2 | Accumulator 2 input

Returns
  Result of operation

## ◆ addmsc_elem_32() [7/8]

v32acc32 addmsc_elem_32 | ( | v32uint16 | a,
|  | v32int16 | b,
|  | v32acc32 | acc1,
|  | v32acc32 | acc2 )

Parameters

  a | Matrix A
  b | Matrix B
  acc1 | Accumulator 1 input
  acc2 | Accumulator 2 input

Returns
  Result of operation

## ◆ addmsc_elem_32() [8/8]

v32acc32 addmsc_elem_32 | ( | v32uint16 | a,
|  | v32uint16 | b,
|  | v32acc32 | acc1,
|  | v32acc32 | acc2 )

Parameters

  a | Matrix A
  b | Matrix B
  acc1 | Accumulator 1 input
  acc2 | Accumulator 2 input

Returns
  Result of operation

## ◆ addmsc_elem_32_conf() [1/8]

v32acc32 addmsc_elem_32_conf | ( | v32int16 | a,
|  | int | sgn_x,
|  | v32int16 | b,
|  | int | sgn_y,
|  | v32acc32 | acc1,
|  | v32acc32 | acc2,
|  | int | zero_acc1,
|  | int | shift16,
|  | int | sub_mul,
|  | int | sub_acc1,
|  | int | sub_acc2 )

Parameters

  a | Matrix A
  sgn_x | Sign mask for matrix A
  b | Matrix B
  sgn_y | Sign mask for matrix B
  acc1 | Accumulator 1 input
  acc2 | Accumulator 2 input
  zero_acc1 | Zeroing mask for acc1
  shift16 | Shift mask of input accumulator acc1
  sub_mul | Negation mask of multiplication result.
  sub_acc1 | Negation mask of acc1
  sub_acc2 | Negation mask of acc2

Returns
  Result of operation

## ◆ addmsc_elem_32_conf() [2/8]

v32acc32 addmsc_elem_32_conf | ( | v32int16 | a,
|  | int | sgn_x,
|  | v32uint16 | b,
|  | int | sgn_y,
|  | v32acc32 | acc1,
|  | v32acc32 | acc2,
|  | int | zero_acc1,
|  | int | shift16,
|  | int | sub_mul,
|  | int | sub_acc1,
|  | int | sub_acc2 )

Parameters

  a | Matrix A
  sgn_x | Sign mask for matrix A
  b | Matrix B
  sgn_y | Sign mask for matrix B
  acc1 | Accumulator 1 input
  acc2 | Accumulator 2 input
  zero_acc1 | Zeroing mask for acc1
  shift16 | Shift mask of input accumulator acc1
  sub_mul | Negation mask of multiplication result.
  sub_acc1 | Negation mask of acc1
  sub_acc2 | Negation mask of acc2

Returns
  Result of operation

## ◆ addmsc_elem_32_conf() [3/8]

v32acc32 addmsc_elem_32_conf | ( | v32int16 | a,
|  | v32int16 | b,
|  | v32acc32 | acc1,
|  | v32acc32 | acc2,
|  | int | zero_acc1,
|  | int | shift16,
|  | int | sub_mul,
|  | int | sub_acc1,
|  | int | sub_acc2 )

Parameters

  a | Matrix A
  b | Matrix B
  acc1 | Accumulator 1 input
  acc2 | Accumulator 2 input
  zero_acc1 | Zeroing mask for acc1
  shift16 | Shift mask of input accumulator acc1
  sub_mul | Negation mask of multiplication result
  sub_acc1 | Negation mask of acc1
  sub_acc2 | Negation mask of acc2

Returns
  Result of operation

## ◆ addmsc_elem_32_conf() [4/8]

v32acc32 addmsc_elem_32_conf | ( | v32int16 | a,
|  | v32uint16 | b,
|  | v32acc32 | acc1,
|  | v32acc32 | acc2,
|  | int | zero_acc1,
|  | int | shift16,
|  | int | sub_mul,
|  | int | sub_acc1,
|  | int | sub_acc2 )

Parameters

  a | Matrix A
  b | Matrix B
  acc1 | Accumulator 1 input
  acc2 | Accumulator 2 input
  zero_acc1 | Zeroing mask for acc1
  shift16 | Shift mask of input accumulator acc1
  sub_mul | Negation mask of multiplication result
  sub_acc1 | Negation mask of acc1
  sub_acc2 | Negation mask of acc2

Returns
  Result of operation

## ◆ addmsc_elem_32_conf() [5/8]

v32acc32 addmsc_elem_32_conf | ( | v32uint16 | a,
|  | int | sgn_x,
|  | v32int16 | b,
|  | int | sgn_y,
|  | v32acc32 | acc1,
|  | v32acc32 | acc2,
|  | int | zero_acc1,
|  | int | shift16,
|  | int | sub_mul,
|  | int | sub_acc1,
|  | int | sub_acc2 )

Parameters

  a | Matrix A
  sgn_x | Sign mask for matrix A
  b | Matrix B
  sgn_y | Sign mask for matrix B
  acc1 | Accumulator 1 input
  acc2 | Accumulator 2 input
  zero_acc1 | Zeroing mask for acc1
  shift16 | Shift mask of input accumulator acc1
  sub_mul | Negation mask of multiplication result.
  sub_acc1 | Negation mask of acc1
  sub_acc2 | Negation mask of acc2

Returns
  Result of operation

## ◆ addmsc_elem_32_conf() [6/8]

v32acc32 addmsc_elem_32_conf | ( | v32uint16 | a,
|  | int | sgn_x,
|  | v32uint16 | b,
|  | int | sgn_y,
|  | v32acc32 | acc1,
|  | v32acc32 | acc2,
|  | int | zero_acc1,
|  | int | shift16,
|  | int | sub_mul,
|  | int | sub_acc1,
|  | int | sub_acc2 )

Parameters

  a | Matrix A
  sgn_x | Sign mask for matrix A
  b | Matrix B
  sgn_y | Sign mask for matrix B
  acc1 | Accumulator 1 input
  acc2 | Accumulator 2 input
  zero_acc1 | Zeroing mask for acc1
  shift16 | Shift mask of input accumulator acc1
  sub_mul | Negation mask of multiplication result.
  sub_acc1 | Negation mask of acc1
  sub_acc2 | Negation mask of acc2

Returns
  Result of operation

## ◆ addmsc_elem_32_conf() [7/8]

v32acc32 addmsc_elem_32_conf | ( | v32uint16 | a,
|  | v32int16 | b,
|  | v32acc32 | acc1,
|  | v32acc32 | acc2,
|  | int | zero_acc1,
|  | int | shift16,
|  | int | sub_mul,
|  | int | sub_acc1,
|  | int | sub_acc2 )

Parameters

  a | Matrix A
  b | Matrix B
  acc1 | Accumulator 1 input
  acc2 | Accumulator 2 input
  zero_acc1 | Zeroing mask for acc1
  shift16 | Shift mask of input accumulator acc1
  sub_mul | Negation mask of multiplication result
  sub_acc1 | Negation mask of acc1
  sub_acc2 | Negation mask of acc2

Returns
  Result of operation

## ◆ addmsc_elem_32_conf() [8/8]

v32acc32 addmsc_elem_32_conf | ( | v32uint16 | a,
|  | v32uint16 | b,
|  | v32acc32 | acc1,
|  | v32acc32 | acc2,
|  | int | zero_acc1,
|  | int | shift16,
|  | int | sub_mul,
|  | int | sub_acc1,
|  | int | sub_acc2 )

Parameters

  a | Matrix A
  b | Matrix B
  acc1 | Accumulator 1 input
  acc2 | Accumulator 2 input
  zero_acc1 | Zeroing mask for acc1
  shift16 | Shift mask of input accumulator acc1
  sub_mul | Negation mask of multiplication result
  sub_acc1 | Negation mask of acc1
  sub_acc2 | Negation mask of acc2

Returns
  Result of operation

## ◆ mac_2x4_4x8() [1/8]

v16acc64 mac_2x4_4x8 | ( | v32int16 | a,
|  | int | sgn_x,
|  | v32int16 | b,
|  | int | sgn_y,
|  | v16acc64 | acc1 )

Parameters

  a | Matrix A
  sgn_x | Sign mask for matrix A
  b | Matrix B
  sgn_y | Sign mask for matrix B
  acc1 | Accumulator 1 input

Returns
  Result of operation

## ◆ mac_2x4_4x8() [2/8]

v16acc64 mac_2x4_4x8 | ( | v32int16 | a,
|  | int | sgn_x,
|  | v32uint16 | b,
|  | int | sgn_y,
|  | v16acc64 | acc1 )

Parameters

  a | Matrix A
  sgn_x | Sign mask for matrix A
  b | Matrix B
  sgn_y | Sign mask for matrix B
  acc1 | Accumulator 1 input

Returns
  Result of operation

## ◆ mac_2x4_4x8() [3/8]

v16acc64 mac_2x4_4x8 | ( | v32int16 | a,
|  | v32int16 | b,
|  | v16acc64 | acc1 )

Parameters

  a | Matrix A
  b | Matrix B
  acc1 | Accumulator 1 input

Returns
  Result of operation

## ◆ mac_2x4_4x8() [4/8]

v16acc64 mac_2x4_4x8 | ( | v32int16 | a,
|  | v32uint16 | b,
|  | v16acc64 | acc1 )

Parameters

  a | Matrix A
  b | Matrix B
  acc1 | Accumulator 1 input

Returns
  Result of operation

## ◆ mac_2x4_4x8() [5/8]

v16acc64 mac_2x4_4x8 | ( | v32uint16 | a,
|  | int | sgn_x,
|  | v32int16 | b,
|  | int | sgn_y,
|  | v16acc64 | acc1 )

Parameters

  a | Matrix A
  sgn_x | Sign mask for matrix A
  b | Matrix B
  sgn_y | Sign mask for matrix B
  acc1 | Accumulator 1 input

Returns
  Result of operation

## ◆ mac_2x4_4x8() [6/8]

v16acc64 mac_2x4_4x8 | ( | v32uint16 | a,
|  | int | sgn_x,
|  | v32uint16 | b,
|  | int | sgn_y,
|  | v16acc64 | acc1 )

Parameters

  a | Matrix A
  sgn_x | Sign mask for matrix A
  b | Matrix B
  sgn_y | Sign mask for matrix B
  acc1 | Accumulator 1 input

Returns
  Result of operation

## ◆ mac_2x4_4x8() [7/8]

v16acc64 mac_2x4_4x8 | ( | v32uint16 | a,
|  | v32int16 | b,
|  | v16acc64 | acc1 )

Parameters

  a | Matrix A
  b | Matrix B
  acc1 | Accumulator 1 input

Returns
  Result of operation

## ◆ mac_2x4_4x8() [8/8]

v16acc64 mac_2x4_4x8 | ( | v32uint16 | a,
|  | v32uint16 | b,
|  | v16acc64 | acc1 )

Parameters

  a | Matrix A
  b | Matrix B
  acc1 | Accumulator 1 input

Returns
  Result of operation

## ◆ mac_2x4_4x8_conf() [1/8]

v16acc64 mac_2x4_4x8_conf | ( | v32int16 | a,
|  | int | sgn_x,
|  | v32int16 | b,
|  | int | sgn_y,
|  | v16acc64 | acc1,
|  | int | zero_acc1,
|  | int | shift16,
|  | int | sub_mul,
|  | int | sub_acc1 )

Parameters

  a | Matrix A
  sgn_x | Sign mask for matrix A
  b | Matrix B
  sgn_y | Sign mask for matrix B
  acc1 | Accumulator 1 input
  zero_acc1 | Zeroing mask for acc1
  shift16 | Shift mask of input accumulator acc1
  sub_mul | Negation mask of multiplication result
  sub_acc1 | Negation mask of acc1

Returns
  Result of operation

## ◆ mac_2x4_4x8_conf() [2/8]

v16acc64 mac_2x4_4x8_conf | ( | v32int16 | a,
|  | int | sgn_x,
|  | v32uint16 | b,
|  | int | sgn_y,
|  | v16acc64 | acc1,
|  | int | zero_acc1,
|  | int | shift16,
|  | int | sub_mul,
|  | int | sub_acc1 )

Parameters

  a | Matrix A
  sgn_x | Sign mask for matrix A
  b | Matrix B
  sgn_y | Sign mask for matrix B
  acc1 | Accumulator 1 input
  zero_acc1 | Zeroing mask for acc1
  shift16 | Shift mask of input accumulator acc1
  sub_mul | Negation mask of multiplication result
  sub_acc1 | Negation mask of acc1

Returns
  Result of operation

## ◆ mac_2x4_4x8_conf() [3/8]

v16acc64 mac_2x4_4x8_conf | ( | v32int16 | a,
|  | v32int16 | b,
|  | v16acc64 | acc1,
|  | int | zero_acc1,
|  | int | shift16,
|  | int | sub_mul,
|  | int | sub_acc1 )

Parameters

  a | Matrix A
  b | Matrix B
  acc1 | Accumulator 1 input
  zero_acc1 | Zeroing mask for acc1
  shift16 | Shift mask of input accumulator acc1
  sub_mul | Negation mask of multiplication result
  sub_acc1 | Negation mask of acc1

Returns
  Result of operation

## ◆ mac_2x4_4x8_conf() [4/8]

v16acc64 mac_2x4_4x8_conf | ( | v32int16 | a,
|  | v32uint16 | b,
|  | v16acc64 | acc1,
|  | int | zero_acc1,
|  | int | shift16,
|  | int | sub_mul,
|  | int | sub_acc1 )

Parameters

  a | Matrix A
  b | Matrix B
  acc1 | Accumulator 1 input
  zero_acc1 | Zeroing mask for acc1
  shift16 | Shift mask of input accumulator acc1
  sub_mul | Negation mask of multiplication result
  sub_acc1 | Negation mask of acc1

Returns
  Result of operation

## ◆ mac_2x4_4x8_conf() [5/8]

v16acc64 mac_2x4_4x8_conf | ( | v32uint16 | a,
|  | int | sgn_x,
|  | v32int16 | b,
|  | int | sgn_y,
|  | v16acc64 | acc1,
|  | int | zero_acc1,
|  | int | shift16,
|  | int | sub_mul,
|  | int | sub_acc1 )

Parameters

  a | Matrix A
  sgn_x | Sign mask for matrix A
  b | Matrix B
  sgn_y | Sign mask for matrix B
  acc1 | Accumulator 1 input
  zero_acc1 | Zeroing mask for acc1
  shift16 | Shift mask of input accumulator acc1
  sub_mul | Negation mask of multiplication result
  sub_acc1 | Negation mask of acc1

Returns
  Result of operation

## ◆ mac_2x4_4x8_conf() [6/8]

v16acc64 mac_2x4_4x8_conf | ( | v32uint16 | a,
|  | int | sgn_x,
|  | v32uint16 | b,
|  | int | sgn_y,
|  | v16acc64 | acc1,
|  | int | zero_acc1,
|  | int | shift16,
|  | int | sub_mul,
|  | int | sub_acc1 )

Parameters

  a | Matrix A
  sgn_x | Sign mask for matrix A
  b | Matrix B
  sgn_y | Sign mask for matrix B
  acc1 | Accumulator 1 input
  zero_acc1 | Zeroing mask for acc1
  shift16 | Shift mask of input accumulator acc1
  sub_mul | Negation mask of multiplication result
  sub_acc1 | Negation mask of acc1

Returns
  Result of operation

## ◆ mac_2x4_4x8_conf() [7/8]

v16acc64 mac_2x4_4x8_conf | ( | v32uint16 | a,
|  | v32int16 | b,
|  | v16acc64 | acc1,
|  | int | zero_acc1,
|  | int | shift16,
|  | int | sub_mul,
|  | int | sub_acc1 )

Parameters

  a | Matrix A
  b | Matrix B
  acc1 | Accumulator 1 input
  zero_acc1 | Zeroing mask for acc1
  shift16 | Shift mask of input accumulator acc1
  sub_mul | Negation mask of multiplication result
  sub_acc1 | Negation mask of acc1

Returns
  Result of operation

## ◆ mac_2x4_4x8_conf() [8/8]

v16acc64 mac_2x4_4x8_conf | ( | v32uint16 | a,
|  | v32uint16 | b,
|  | v16acc64 | acc1,
|  | int | zero_acc1,
|  | int | shift16,
|  | int | sub_mul,
|  | int | sub_acc1 )

Parameters

  a | Matrix A
  b | Matrix B
  acc1 | Accumulator 1 input
  zero_acc1 | Zeroing mask for acc1
  shift16 | Shift mask of input accumulator acc1
  sub_mul | Negation mask of multiplication result
  sub_acc1 | Negation mask of acc1

Returns
  Result of operation

## ◆ mac_4x2_2x8() [1/8]

v32acc32 mac_4x2_2x8 | ( | v32int16 | a,
|  | int | sgn_x,
|  | v32int16 | b,
|  | int | sgn_y,
|  | v32acc32 | acc1 )

Parameters

  a | Matrix A
  sgn_x | Sign mask for matrix A
  b | Matrix B
  sgn_y | Sign mask for matrix B
  acc1 | Accumulator 1 input

Returns
  Result of operation

## ◆ mac_4x2_2x8() [2/8]

v32acc32 mac_4x2_2x8 | ( | v32int16 | a,
|  | int | sgn_x,
|  | v32uint16 | b,
|  | int | sgn_y,
|  | v32acc32 | acc1 )

Parameters

  a | Matrix A
  sgn_x | Sign mask for matrix A
  b | Matrix B
  sgn_y | Sign mask for matrix B
  acc1 | Accumulator 1 input

Returns
  Result of operation

## ◆ mac_4x2_2x8() [3/8]

v32acc32 mac_4x2_2x8 | ( | v32int16 | a,
|  | v32int16 | b,
|  | v32acc32 | acc1 )

Parameters

  a | Matrix A
  b | Matrix B
  acc1 | Accumulator 1 input

Returns
  Result of operation

## ◆ mac_4x2_2x8() [4/8]

v32acc32 mac_4x2_2x8 | ( | v32int16 | a,
|  | v32uint16 | b,
|  | v32acc32 | acc1 )

Parameters

  a | Matrix A
  b | Matrix B
  acc1 | Accumulator 1 input

Returns
  Result of operation

## ◆ mac_4x2_2x8() [5/8]

v32acc32 mac_4x2_2x8 | ( | v32uint16 | a,
|  | int | sgn_x,
|  | v32int16 | b,
|  | int | sgn_y,
|  | v32acc32 | acc1 )

Parameters

  a | Matrix A
  sgn_x | Sign mask for matrix A
  b | Matrix B
  sgn_y | Sign mask for matrix B
  acc1 | Accumulator 1 input

Returns
  Result of operation

## ◆ mac_4x2_2x8() [6/8]

v32acc32 mac_4x2_2x8 | ( | v32uint16 | a,
|  | int | sgn_x,
|  | v32uint16 | b,
|  | int | sgn_y,
|  | v32acc32 | acc1 )

Parameters

  a | Matrix A
  sgn_x | Sign mask for matrix A
  b | Matrix B
  sgn_y | Sign mask for matrix B
  acc1 | Accumulator 1 input

Returns
  Result of operation

## ◆ mac_4x2_2x8() [7/8]

v32acc32 mac_4x2_2x8 | ( | v32uint16 | a,
|  | v32int16 | b,
|  | v32acc32 | acc1 )

Parameters

  a | Matrix A
  b | Matrix B
  acc1 | Accumulator 1 input

Returns
  Result of operation

## ◆ mac_4x2_2x8() [8/8]

v32acc32 mac_4x2_2x8 | ( | v32uint16 | a,
|  | v32uint16 | b,
|  | v32acc32 | acc1 )

Parameters

  a | Matrix A
  b | Matrix B
  acc1 | Accumulator 1 input

Returns
  Result of operation

## ◆ mac_4x2_2x8_conf() [1/8]

v32acc32 mac_4x2_2x8_conf | ( | v32int16 | a,
|  | int | sgn_x,
|  | v32int16 | b,
|  | int | sgn_y,
|  | v32acc32 | acc1,
|  | int | zero_acc1,
|  | int | shift16,
|  | int | sub_mul,
|  | int | sub_acc1 )

Parameters

  a | Matrix A
  sgn_x | Sign mask for matrix A
  b | Matrix B
  sgn_y | Sign mask for matrix B
  acc1 | Accumulator 1 input
  zero_acc1 | Zeroing mask for acc1
  shift16 | Shift mask of input accumulator acc1
  sub_mul | Negation mask of multiplication result
  sub_acc1 | Negation mask of acc1

Returns
  Result of operation

## ◆ mac_4x2_2x8_conf() [2/8]

v32acc32 mac_4x2_2x8_conf | ( | v32int16 | a,
|  | int | sgn_x,
|  | v32uint16 | b,
|  | int | sgn_y,
|  | v32acc32 | acc1,
|  | int | zero_acc1,
|  | int | shift16,
|  | int | sub_mul,
|  | int | sub_acc1 )

Parameters

  a | Matrix A
  sgn_x | Sign mask for matrix A
  b | Matrix B
  sgn_y | Sign mask for matrix B
  acc1 | Accumulator 1 input
  zero_acc1 | Zeroing mask for acc1
  shift16 | Shift mask of input accumulator acc1
  sub_mul | Negation mask of multiplication result
  sub_acc1 | Negation mask of acc1

Returns
  Result of operation

## ◆ mac_4x2_2x8_conf() [3/8]

v32acc32 mac_4x2_2x8_conf | ( | v32int16 | a,
|  | v32int16 | b,
|  | v32acc32 | acc1,
|  | int | zero_acc1,
|  | int | shift16,
|  | int | sub_mul,
|  | int | sub_acc1 )

Parameters

  a | Matrix A
  b | Matrix B
  acc1 | Accumulator 1 input
  zero_acc1 | Zeroing mask for acc1
  shift16 | Shift mask of input accumulator acc1
  sub_mul | Negation mask of multiplication result
  sub_acc1 | Negation mask of acc1

Returns
  Result of operation

## ◆ mac_4x2_2x8_conf() [4/8]

v32acc32 mac_4x2_2x8_conf | ( | v32int16 | a,
|  | v32uint16 | b,
|  | v32acc32 | acc1,
|  | int | zero_acc1,
|  | int | shift16,
|  | int | sub_mul,
|  | int | sub_acc1 )

Parameters

  a | Matrix A
  b | Matrix B
  acc1 | Accumulator 1 input
  zero_acc1 | Zeroing mask for acc1
  shift16 | Shift mask of input accumulator acc1
  sub_mul | Negation mask of multiplication result
  sub_acc1 | Negation mask of acc1

Returns
  Result of operation

## ◆ mac_4x2_2x8_conf() [5/8]

v32acc32 mac_4x2_2x8_conf | ( | v32uint16 | a,
|  | int | sgn_x,
|  | v32int16 | b,
|  | int | sgn_y,
|  | v32acc32 | acc1,
|  | int | zero_acc1,
|  | int | shift16,
|  | int | sub_mul,
|  | int | sub_acc1 )

Parameters

  a | Matrix A
  sgn_x | Sign mask for matrix A
  b | Matrix B
  sgn_y | Sign mask for matrix B
  acc1 | Accumulator 1 input
  zero_acc1 | Zeroing mask for acc1
  shift16 | Shift mask of input accumulator acc1
  sub_mul | Negation mask of multiplication result
  sub_acc1 | Negation mask of acc1

Returns
  Result of operation

## ◆ mac_4x2_2x8_conf() [6/8]

v32acc32 mac_4x2_2x8_conf | ( | v32uint16 | a,
|  | int | sgn_x,
|  | v32uint16 | b,
|  | int | sgn_y,
|  | v32acc32 | acc1,
|  | int | zero_acc1,
|  | int | shift16,
|  | int | sub_mul,
|  | int | sub_acc1 )

Parameters

  a | Matrix A
  sgn_x | Sign mask for matrix A
  b | Matrix B
  sgn_y | Sign mask for matrix B
  acc1 | Accumulator 1 input
  zero_acc1 | Zeroing mask for acc1
  shift16 | Shift mask of input accumulator acc1
  sub_mul | Negation mask of multiplication result
  sub_acc1 | Negation mask of acc1

Returns
  Result of operation

## ◆ mac_4x2_2x8_conf() [7/8]

v32acc32 mac_4x2_2x8_conf | ( | v32uint16 | a,
|  | v32int16 | b,
|  | v32acc32 | acc1,
|  | int | zero_acc1,
|  | int | shift16,
|  | int | sub_mul,
|  | int | sub_acc1 )

Parameters

  a | Matrix A
  b | Matrix B
  acc1 | Accumulator 1 input
  zero_acc1 | Zeroing mask for acc1
  shift16 | Shift mask of input accumulator acc1
  sub_mul | Negation mask of multiplication result
  sub_acc1 | Negation mask of acc1

Returns
  Result of operation

## ◆ mac_4x2_2x8_conf() [8/8]

v32acc32 mac_4x2_2x8_conf | ( | v32uint16 | a,
|  | v32uint16 | b,
|  | v32acc32 | acc1,
|  | int | zero_acc1,
|  | int | shift16,
|  | int | sub_mul,
|  | int | sub_acc1 )

Parameters

  a | Matrix A
  b | Matrix B
  acc1 | Accumulator 1 input
  zero_acc1 | Zeroing mask for acc1
  shift16 | Shift mask of input accumulator acc1
  sub_mul | Negation mask of multiplication result
  sub_acc1 | Negation mask of acc1

Returns
  Result of operation

## ◆ mac_4x4_4x4() [1/8]

v16acc64 mac_4x4_4x4 | ( | v32int16 | a,
|  | int | sgn_x,
|  | v32int16 | b,
|  | int | sgn_y,
|  | v16acc64 | acc1 )

Parameters

  a | Matrix A
  sgn_x | Sign mask for matrix A
  b | Matrix B
  sgn_y | Sign mask for matrix B
  acc1 | Accumulator 1 input

Returns
  Result of operation

## ◆ mac_4x4_4x4() [2/8]

v16acc64 mac_4x4_4x4 | ( | v32int16 | a,
|  | int | sgn_x,
|  | v32uint16 | b,
|  | int | sgn_y,
|  | v16acc64 | acc1 )

Parameters

  a | Matrix A
  sgn_x | Sign mask for matrix A
  b | Matrix B
  sgn_y | Sign mask for matrix B
  acc1 | Accumulator 1 input

Returns
  Result of operation

## ◆ mac_4x4_4x4() [3/8]

v16acc64 mac_4x4_4x4 | ( | v32int16 | a,
|  | v32int16 | b,
|  | v16acc64 | acc1 )

Parameters

  a | Matrix A
  b | Matrix B
  acc1 | Accumulator 1 input

Returns
  Result of operation

## ◆ mac_4x4_4x4() [4/8]

v16acc64 mac_4x4_4x4 | ( | v32int16 | a,
|  | v32uint16 | b,
|  | v16acc64 | acc1 )

Parameters

  a | Matrix A
  b | Matrix B
  acc1 | Accumulator 1 input

Returns
  Result of operation

## ◆ mac_4x4_4x4() [5/8]

v16acc64 mac_4x4_4x4 | ( | v32uint16 | a,
|  | int | sgn_x,
|  | v32int16 | b,
|  | int | sgn_y,
|  | v16acc64 | acc1 )

Parameters

  a | Matrix A
  sgn_x | Sign mask for matrix A
  b | Matrix B
  sgn_y | Sign mask for matrix B
  acc1 | Accumulator 1 input

Returns
  Result of operation

## ◆ mac_4x4_4x4() [6/8]

v16acc64 mac_4x4_4x4 | ( | v32uint16 | a,
|  | int | sgn_x,
|  | v32uint16 | b,
|  | int | sgn_y,
|  | v16acc64 | acc1 )

Parameters

  a | Matrix A
  sgn_x | Sign mask for matrix A
  b | Matrix B
  sgn_y | Sign mask for matrix B
  acc1 | Accumulator 1 input

Returns
  Result of operation

## ◆ mac_4x4_4x4() [7/8]

v16acc64 mac_4x4_4x4 | ( | v32uint16 | a,
|  | v32int16 | b,
|  | v16acc64 | acc1 )

Parameters

  a | Matrix A
  b | Matrix B
  acc1 | Accumulator 1 input

Returns
  Result of operation

## ◆ mac_4x4_4x4() [8/8]

v16acc64 mac_4x4_4x4 | ( | v32uint16 | a,
|  | v32uint16 | b,
|  | v16acc64 | acc1 )

Parameters

  a | Matrix A
  b | Matrix B
  acc1 | Accumulator 1 input

Returns
  Result of operation

## ◆ mac_4x4_4x4_conf() [1/8]

v16acc64 mac_4x4_4x4_conf | ( | v32int16 | a,
|  | int | sgn_x,
|  | v32int16 | b,
|  | int | sgn_y,
|  | v16acc64 | acc1,
|  | int | zero_acc1,
|  | int | shift16,
|  | int | sub_mul,
|  | int | sub_acc1 )

Parameters

  a | Matrix A
  sgn_x | Sign mask for matrix A
  b | Matrix B
  sgn_y | Sign mask for matrix B
  acc1 | Accumulator 1 input
  zero_acc1 | Zeroing mask for acc1
  shift16 | Shift mask of input accumulator acc1
  sub_mul | Negation mask of multiplication result
  sub_acc1 | Negation mask of acc1

Returns
  Result of operation

## ◆ mac_4x4_4x4_conf() [2/8]

v16acc64 mac_4x4_4x4_conf | ( | v32int16 | a,
|  | int | sgn_x,
|  | v32uint16 | b,
|  | int | sgn_y,
|  | v16acc64 | acc1,
|  | int | zero_acc1,
|  | int | shift16,
|  | int | sub_mul,
|  | int | sub_acc1 )

Parameters

  a | Matrix A
  sgn_x | Sign mask for matrix A
  b | Matrix B
  sgn_y | Sign mask for matrix B
  acc1 | Accumulator 1 input
  zero_acc1 | Zeroing mask for acc1
  shift16 | Shift mask of input accumulator acc1
  sub_mul | Negation mask of multiplication result
  sub_acc1 | Negation mask of acc1

Returns
  Result of operation

## ◆ mac_4x4_4x4_conf() [3/8]

v16acc64 mac_4x4_4x4_conf | ( | v32int16 | a,
|  | v32int16 | b,
|  | v16acc64 | acc1,
|  | int | zero_acc1,
|  | int | shift16,
|  | int | sub_mul,
|  | int | sub_acc1 )

Parameters

  a | Matrix A
  b | Matrix B
  acc1 | Accumulator 1 input
  zero_acc1 | Zeroing mask for acc1
  shift16 | Shift mask of input accumulator acc1
  sub_mul | Negation mask of multiplication result
  sub_acc1 | Negation mask of acc1

Returns
  Result of operation

## ◆ mac_4x4_4x4_conf() [4/8]

v16acc64 mac_4x4_4x4_conf | ( | v32int16 | a,
|  | v32uint16 | b,
|  | v16acc64 | acc1,
|  | int | zero_acc1,
|  | int | shift16,
|  | int | sub_mul,
|  | int | sub_acc1 )

Parameters

  a | Matrix A
  b | Matrix B
  acc1 | Accumulator 1 input
  zero_acc1 | Zeroing mask for acc1
  shift16 | Shift mask of input accumulator acc1
  sub_mul | Negation mask of multiplication result
  sub_acc1 | Negation mask of acc1

Returns
  Result of operation

## ◆ mac_4x4_4x4_conf() [5/8]

v16acc64 mac_4x4_4x4_conf | ( | v32uint16 | a,
|  | int | sgn_x,
|  | v32int16 | b,
|  | int | sgn_y,
|  | v16acc64 | acc1,
|  | int | zero_acc1,
|  | int | shift16,
|  | int | sub_mul,
|  | int | sub_acc1 )

Parameters

  a | Matrix A
  sgn_x | Sign mask for matrix A
  b | Matrix B
  sgn_y | Sign mask for matrix B
  acc1 | Accumulator 1 input
  zero_acc1 | Zeroing mask for acc1
  shift16 | Shift mask of input accumulator acc1
  sub_mul | Negation mask of multiplication result
  sub_acc1 | Negation mask of acc1

Returns
  Result of operation

## ◆ mac_4x4_4x4_conf() [6/8]

v16acc64 mac_4x4_4x4_conf | ( | v32uint16 | a,
|  | int | sgn_x,
|  | v32uint16 | b,
|  | int | sgn_y,
|  | v16acc64 | acc1,
|  | int | zero_acc1,
|  | int | shift16,
|  | int | sub_mul,
|  | int | sub_acc1 )

Parameters

  a | Matrix A
  sgn_x | Sign mask for matrix A
  b | Matrix B
  sgn_y | Sign mask for matrix B
  acc1 | Accumulator 1 input
  zero_acc1 | Zeroing mask for acc1
  shift16 | Shift mask of input accumulator acc1
  sub_mul | Negation mask of multiplication result
  sub_acc1 | Negation mask of acc1

Returns
  Result of operation

## ◆ mac_4x4_4x4_conf() [7/8]

v16acc64 mac_4x4_4x4_conf | ( | v32uint16 | a,
|  | v32int16 | b,
|  | v16acc64 | acc1,
|  | int | zero_acc1,
|  | int | shift16,
|  | int | sub_mul,
|  | int | sub_acc1 )

Parameters

  a | Matrix A
  b | Matrix B
  acc1 | Accumulator 1 input
  zero_acc1 | Zeroing mask for acc1
  shift16 | Shift mask of input accumulator acc1
  sub_mul | Negation mask of multiplication result
  sub_acc1 | Negation mask of acc1

Returns
  Result of operation

## ◆ mac_4x4_4x4_conf() [8/8]

v16acc64 mac_4x4_4x4_conf | ( | v32uint16 | a,
|  | v32uint16 | b,
|  | v16acc64 | acc1,
|  | int | zero_acc1,
|  | int | shift16,
|  | int | sub_mul,
|  | int | sub_acc1 )

Parameters

  a | Matrix A
  b | Matrix B
  acc1 | Accumulator 1 input
  zero_acc1 | Zeroing mask for acc1
  shift16 | Shift mask of input accumulator acc1
  sub_mul | Negation mask of multiplication result
  sub_acc1 | Negation mask of acc1

Returns
  Result of operation

## ◆ mac_conv_16x4() [1/8]

v16acc64 mac_conv_16x4 | ( | v32int16 | a,
|  | int | sgn_x,
|  | v32int16 | b,
|  | int | sgn_y,
|  | v16acc64 | acc1 )

Parameters

  a | Matrix A
  sgn_x | Sign mask for matrix A
  b | Matrix B
  sgn_y | Sign mask for matrix B
  acc1 | Accumulator 1 input

Returns
  Result of operation

## ◆ mac_conv_16x4() [2/8]

v16acc64 mac_conv_16x4 | ( | v32int16 | a,
|  | int | sgn_x,
|  | v32uint16 | b,
|  | int | sgn_y,
|  | v16acc64 | acc1 )

Parameters

  a | Matrix A
  sgn_x | Sign mask for matrix A
  b | Matrix B
  sgn_y | Sign mask for matrix B
  acc1 | Accumulator 1 input

Returns
  Result of operation

## ◆ mac_conv_16x4() [3/8]

v16acc64 mac_conv_16x4 | ( | v32int16 | a,
|  | v32int16 | b,
|  | v16acc64 | acc1 )

Parameters

  a | Matrix A
  b | Matrix B
  acc1 | Accumulator 1 input

Returns
  Result of operation

## ◆ mac_conv_16x4() [4/8]

v16acc64 mac_conv_16x4 | ( | v32int16 | a,
|  | v32uint16 | b,
|  | v16acc64 | acc1 )

Parameters

  a | Matrix A
  b | Matrix B
  acc1 | Accumulator 1 input

Returns
  Result of operation

## ◆ mac_conv_16x4() [5/8]

v16acc64 mac_conv_16x4 | ( | v32uint16 | a,
|  | int | sgn_x,
|  | v32int16 | b,
|  | int | sgn_y,
|  | v16acc64 | acc1 )

Parameters

  a | Matrix A
  sgn_x | Sign mask for matrix A
  b | Matrix B
  sgn_y | Sign mask for matrix B
  acc1 | Accumulator 1 input

Returns
  Result of operation

## ◆ mac_conv_16x4() [6/8]

v16acc64 mac_conv_16x4 | ( | v32uint16 | a,
|  | int | sgn_x,
|  | v32uint16 | b,
|  | int | sgn_y,
|  | v16acc64 | acc1 )

Parameters

  a | Matrix A
  sgn_x | Sign mask for matrix A
  b | Matrix B
  sgn_y | Sign mask for matrix B
  acc1 | Accumulator 1 input

Returns
  Result of operation

## ◆ mac_conv_16x4() [7/8]

v16acc64 mac_conv_16x4 | ( | v32uint16 | a,
|  | v32int16 | b,
|  | v16acc64 | acc1 )

Parameters

  a | Matrix A
  b | Matrix B
  acc1 | Accumulator 1 input

Returns
  Result of operation

## ◆ mac_conv_16x4() [8/8]

v16acc64 mac_conv_16x4 | ( | v32uint16 | a,
|  | v32uint16 | b,
|  | v16acc64 | acc1 )

Parameters

  a | Matrix A
  b | Matrix B
  acc1 | Accumulator 1 input

Returns
  Result of operation

## ◆ mac_conv_16x4_conf() [1/8]

v16acc64 mac_conv_16x4_conf | ( | v32int16 | a,
|  | int | sgn_x,
|  | v32int16 | b,
|  | int | sgn_y,
|  | v16acc64 | acc1,
|  | int | zero_acc1,
|  | int | shift16,
|  | int | sub_mul,
|  | int | sub_acc1 )

Parameters

  a | Matrix A
  sgn_x | Sign mask for matrix A
  b | Matrix B
  sgn_y | Sign mask for matrix B
  acc1 | Accumulator 1 input
  zero_acc1 | Zeroing mask for acc1
  shift16 | Shift mask of input accumulator acc1
  sub_mul | Negation mask of multiplication result
  sub_acc1 | Negation mask of acc1

Returns
  Result of operation

## ◆ mac_conv_16x4_conf() [2/8]

v16acc64 mac_conv_16x4_conf | ( | v32int16 | a,
|  | int | sgn_x,
|  | v32uint16 | b,
|  | int | sgn_y,
|  | v16acc64 | acc1,
|  | int | zero_acc1,
|  | int | shift16,
|  | int | sub_mul,
|  | int | sub_acc1 )

Parameters

  a | Matrix A
  sgn_x | Sign mask for matrix A
  b | Matrix B
  sgn_y | Sign mask for matrix B
  acc1 | Accumulator 1 input
  zero_acc1 | Zeroing mask for acc1
  shift16 | Shift mask of input accumulator acc1
  sub_mul | Negation mask of multiplication result
  sub_acc1 | Negation mask of acc1

Returns
  Result of operation

## ◆ mac_conv_16x4_conf() [3/8]

v16acc64 mac_conv_16x4_conf | ( | v32int16 | a,
|  | v32int16 | b,
|  | v16acc64 | acc1,
|  | int | zero_acc1,
|  | int | shift16,
|  | int | sub_mul,
|  | int | sub_acc1 )

Parameters

  a | Matrix A
  b | Matrix B
  acc1 | Accumulator 1 input
  zero_acc1 | Zeroing mask for acc1
  shift16 | Shift mask of input accumulator acc1
  sub_mul | Negation mask of multiplication result
  sub_acc1 | Negation mask of acc1

Returns
  Result of operation

## ◆ mac_conv_16x4_conf() [4/8]

v16acc64 mac_conv_16x4_conf | ( | v32int16 | a,
|  | v32uint16 | b,
|  | v16acc64 | acc1,
|  | int | zero_acc1,
|  | int | shift16,
|  | int | sub_mul,
|  | int | sub_acc1 )

Parameters

  a | Matrix A
  b | Matrix B
  acc1 | Accumulator 1 input
  zero_acc1 | Zeroing mask for acc1
  shift16 | Shift mask of input accumulator acc1
  sub_mul | Negation mask of multiplication result
  sub_acc1 | Negation mask of acc1

Returns
  Result of operation

## ◆ mac_conv_16x4_conf() [5/8]

v16acc64 mac_conv_16x4_conf | ( | v32uint16 | a,
|  | int | sgn_x,
|  | v32int16 | b,
|  | int | sgn_y,
|  | v16acc64 | acc1,
|  | int | zero_acc1,
|  | int | shift16,
|  | int | sub_mul,
|  | int | sub_acc1 )

Parameters

  a | Matrix A
  sgn_x | Sign mask for matrix A
  b | Matrix B
  sgn_y | Sign mask for matrix B
  acc1 | Accumulator 1 input
  zero_acc1 | Zeroing mask for acc1
  shift16 | Shift mask of input accumulator acc1
  sub_mul | Negation mask of multiplication result
  sub_acc1 | Negation mask of acc1

Returns
  Result of operation

## ◆ mac_conv_16x4_conf() [6/8]

v16acc64 mac_conv_16x4_conf | ( | v32uint16 | a,
|  | int | sgn_x,
|  | v32uint16 | b,
|  | int | sgn_y,
|  | v16acc64 | acc1,
|  | int | zero_acc1,
|  | int | shift16,
|  | int | sub_mul,
|  | int | sub_acc1 )

Parameters

  a | Matrix A
  sgn_x | Sign mask for matrix A
  b | Matrix B
  sgn_y | Sign mask for matrix B
  acc1 | Accumulator 1 input
  zero_acc1 | Zeroing mask for acc1
  shift16 | Shift mask of input accumulator acc1
  sub_mul | Negation mask of multiplication result
  sub_acc1 | Negation mask of acc1

Returns
  Result of operation

## ◆ mac_conv_16x4_conf() [7/8]

v16acc64 mac_conv_16x4_conf | ( | v32uint16 | a,
|  | v32int16 | b,
|  | v16acc64 | acc1,
|  | int | zero_acc1,
|  | int | shift16,
|  | int | sub_mul,
|  | int | sub_acc1 )

Parameters

  a | Matrix A
  b | Matrix B
  acc1 | Accumulator 1 input
  zero_acc1 | Zeroing mask for acc1
  shift16 | Shift mask of input accumulator acc1
  sub_mul | Negation mask of multiplication result
  sub_acc1 | Negation mask of acc1

Returns
  Result of operation

## ◆ mac_conv_16x4_conf() [8/8]

v16acc64 mac_conv_16x4_conf | ( | v32uint16 | a,
|  | v32uint16 | b,
|  | v16acc64 | acc1,
|  | int | zero_acc1,
|  | int | shift16,
|  | int | sub_mul,
|  | int | sub_acc1 )

Parameters

  a | Matrix A
  b | Matrix B
  acc1 | Accumulator 1 input
  zero_acc1 | Zeroing mask for acc1
  shift16 | Shift mask of input accumulator acc1
  sub_mul | Negation mask of multiplication result
  sub_acc1 | Negation mask of acc1

Returns
  Result of operation

## ◆ mac_elem_16_2() [1/9]

v16accfloat mac_elem_16_2 | ( | v32bfloat16 | a,
|  | v32bfloat16 | b,
|  | v16accfloat | acc1 )

Parameters

  a | Matrix A
  b | Matrix B
  acc1 | Accumulator 1 input

Returns
  Result of operation

## ◆ mac_elem_16_2() [2/9]

v16acc64 mac_elem_16_2 | ( | v32int16 | a,
|  | int | sgn_x,
|  | v32int16 | b,
|  | int | sgn_y,
|  | v16acc64 | acc1 )

Parameters

  a | Matrix A
  sgn_x | Sign mask for matrix A
  b | Matrix B
  sgn_y | Sign mask for matrix B
  acc1 | Accumulator 1 input

Returns
  Result of operation

## ◆ mac_elem_16_2() [3/9]

v16acc64 mac_elem_16_2 | ( | v32int16 | a,
|  | int | sgn_x,
|  | v32uint16 | b,
|  | int | sgn_y,
|  | v16acc64 | acc1 )

Parameters

  a | Matrix A
  sgn_x | Sign mask for matrix A
  b | Matrix B
  sgn_y | Sign mask for matrix B
  acc1 | Accumulator 1 input

Returns
  Result of operation

## ◆ mac_elem_16_2() [4/9]

v16acc64 mac_elem_16_2 | ( | v32int16 | a,
|  | v32int16 | b,
|  | v16acc64 | acc1 )

Parameters

  a | Matrix A
  b | Matrix B
  acc1 | Accumulator 1 input

Returns
  Result of operation

## ◆ mac_elem_16_2() [5/9]

v16acc64 mac_elem_16_2 | ( | v32int16 | a,
|  | v32uint16 | b,
|  | v16acc64 | acc1 )

Parameters

  a | Matrix A
  b | Matrix B
  acc1 | Accumulator 1 input

Returns
  Result of operation

## ◆ mac_elem_16_2() [6/9]

v16acc64 mac_elem_16_2 | ( | v32uint16 | a,
|  | int | sgn_x,
|  | v32int16 | b,
|  | int | sgn_y,
|  | v16acc64 | acc1 )

Parameters

  a | Matrix A
  sgn_x | Sign mask for matrix A
  b | Matrix B
  sgn_y | Sign mask for matrix B
  acc1 | Accumulator 1 input

Returns
  Result of operation

## ◆ mac_elem_16_2() [7/9]

v16acc64 mac_elem_16_2 | ( | v32uint16 | a,
|  | int | sgn_x,
|  | v32uint16 | b,
|  | int | sgn_y,
|  | v16acc64 | acc1 )

Parameters

  a | Matrix A
  sgn_x | Sign mask for matrix A
  b | Matrix B
  sgn_y | Sign mask for matrix B
  acc1 | Accumulator 1 input

Returns
  Result of operation

## ◆ mac_elem_16_2() [8/9]

v16acc64 mac_elem_16_2 | ( | v32uint16 | a,
|  | v32int16 | b,
|  | v16acc64 | acc1 )

Parameters

  a | Matrix A
  b | Matrix B
  acc1 | Accumulator 1 input

Returns
  Result of operation

## ◆ mac_elem_16_2() [9/9]

v16acc64 mac_elem_16_2 | ( | v32uint16 | a,
|  | v32uint16 | b,
|  | v16acc64 | acc1 )

Parameters

  a | Matrix A
  b | Matrix B
  acc1 | Accumulator 1 input

Returns
  Result of operation

## ◆ mac_elem_16_2_conf() [1/9]

v16accfloat mac_elem_16_2_conf | ( | v32bfloat16 | a,
|  | v32bfloat16 | b,
|  | v16accfloat | acc1,
|  | int | zero_acc1,
|  | int | sub_mul,
|  | int | sub_acc1 )

Parameters

  a | Matrix A
  b | Matrix B
  acc1 | Accumulator 1 input
  zero_acc1 | Zeroing mask for acc1
  sub_mul | Negation mask of multiplication result
  sub_acc1 | Negation mask of acc1

Returns
  Result of operation

## ◆ mac_elem_16_2_conf() [2/9]

v16acc64 mac_elem_16_2_conf | ( | v32int16 | a,
|  | int | sgn_x,
|  | v32int16 | b,
|  | int | sgn_y,
|  | v16acc64 | acc1,
|  | int | zero_acc1,
|  | int | shift16,
|  | int | sub_mul,
|  | int | sub_acc1 )

Parameters

  a | Matrix A
  sgn_x | Sign mask for matrix A
  b | Matrix B
  sgn_y | Sign mask for matrix B
  acc1 | Accumulator 1 input
  zero_acc1 | Zeroing mask for acc1
  shift16 | Shift mask of input accumulator acc1
  sub_mul | Negation mask of multiplication result
  sub_acc1 | Negation mask of acc1

Returns
  Result of operation

## ◆ mac_elem_16_2_conf() [3/9]

v16acc64 mac_elem_16_2_conf | ( | v32int16 | a,
|  | int | sgn_x,
|  | v32uint16 | b,
|  | int | sgn_y,
|  | v16acc64 | acc1,
|  | int | zero_acc1,
|  | int | shift16,
|  | int | sub_mul,
|  | int | sub_acc1 )

Parameters

  a | Matrix A
  sgn_x | Sign mask for matrix A
  b | Matrix B
  sgn_y | Sign mask for matrix B
  acc1 | Accumulator 1 input
  zero_acc1 | Zeroing mask for acc1
  shift16 | Shift mask of input accumulator acc1
  sub_mul | Negation mask of multiplication result
  sub_acc1 | Negation mask of acc1

Returns
  Result of operation

## ◆ mac_elem_16_2_conf() [4/9]

v16acc64 mac_elem_16_2_conf | ( | v32int16 | a,
|  | v32int16 | b,
|  | v16acc64 | acc1,
|  | int | zero_acc1,
|  | int | shift16,
|  | int | sub_mul,
|  | int | sub_acc1 )

Parameters

  a | Matrix A
  b | Matrix B
  acc1 | Accumulator 1 input
  zero_acc1 | Zeroing mask for acc1
  shift16 | Shift mask of input accumulator acc1
  sub_mul | Negation mask of multiplication result
  sub_acc1 | Negation mask of acc1

Returns
  Result of operation

## ◆ mac_elem_16_2_conf() [5/9]

v16acc64 mac_elem_16_2_conf | ( | v32int16 | a,
|  | v32uint16 | b,
|  | v16acc64 | acc1,
|  | int | zero_acc1,
|  | int | shift16,
|  | int | sub_mul,
|  | int | sub_acc1 )

Parameters

  a | Matrix A
  b | Matrix B
  acc1 | Accumulator 1 input
  zero_acc1 | Zeroing mask for acc1
  shift16 | Shift mask of input accumulator acc1
  sub_mul | Negation mask of multiplication result
  sub_acc1 | Negation mask of acc1

Returns
  Result of operation

## ◆ mac_elem_16_2_conf() [6/9]

v16acc64 mac_elem_16_2_conf | ( | v32uint16 | a,
|  | int | sgn_x,
|  | v32int16 | b,
|  | int | sgn_y,
|  | v16acc64 | acc1,
|  | int | zero_acc1,
|  | int | shift16,
|  | int | sub_mul,
|  | int | sub_acc1 )

Parameters

  a | Matrix A
  sgn_x | Sign mask for matrix A
  b | Matrix B
  sgn_y | Sign mask for matrix B
  acc1 | Accumulator 1 input
  zero_acc1 | Zeroing mask for acc1
  shift16 | Shift mask of input accumulator acc1
  sub_mul | Negation mask of multiplication result
  sub_acc1 | Negation mask of acc1

Returns
  Result of operation

## ◆ mac_elem_16_2_conf() [7/9]

v16acc64 mac_elem_16_2_conf | ( | v32uint16 | a,
|  | int | sgn_x,
|  | v32uint16 | b,
|  | int | sgn_y,
|  | v16acc64 | acc1,
|  | int | zero_acc1,
|  | int | shift16,
|  | int | sub_mul,
|  | int | sub_acc1 )

Parameters

  a | Matrix A
  sgn_x | Sign mask for matrix A
  b | Matrix B
  sgn_y | Sign mask for matrix B
  acc1 | Accumulator 1 input
  zero_acc1 | Zeroing mask for acc1
  shift16 | Shift mask of input accumulator acc1
  sub_mul | Negation mask of multiplication result
  sub_acc1 | Negation mask of acc1

Returns
  Result of operation

## ◆ mac_elem_16_2_conf() [8/9]

v16acc64 mac_elem_16_2_conf | ( | v32uint16 | a,
|  | v32int16 | b,
|  | v16acc64 | acc1,
|  | int | zero_acc1,
|  | int | shift16,
|  | int | sub_mul,
|  | int | sub_acc1 )

Parameters

  a | Matrix A
  b | Matrix B
  acc1 | Accumulator 1 input
  zero_acc1 | Zeroing mask for acc1
  shift16 | Shift mask of input accumulator acc1
  sub_mul | Negation mask of multiplication result
  sub_acc1 | Negation mask of acc1

Returns
  Result of operation

## ◆ mac_elem_16_2_conf() [9/9]

v16acc64 mac_elem_16_2_conf | ( | v32uint16 | a,
|  | v32uint16 | b,
|  | v16acc64 | acc1,
|  | int | zero_acc1,
|  | int | shift16,
|  | int | sub_mul,
|  | int | sub_acc1 )

Parameters

  a | Matrix A
  b | Matrix B
  acc1 | Accumulator 1 input
  zero_acc1 | Zeroing mask for acc1
  shift16 | Shift mask of input accumulator acc1
  sub_mul | Negation mask of multiplication result
  sub_acc1 | Negation mask of acc1

Returns
  Result of operation

## ◆ mac_elem_32() [1/8]

v32acc32 mac_elem_32 | ( | v32int16 | a,
|  | int | sgn_x,
|  | v32int16 | b,
|  | int | sgn_y,
|  | v32acc32 | acc1 )

Parameters

  a | Matrix A
  sgn_x | Sign mask for matrix A
  b | Matrix B
  sgn_y | Sign mask for matrix B
  acc1 | Accumulator 1 input

Returns
  Result of operation

## ◆ mac_elem_32() [2/8]

v32acc32 mac_elem_32 | ( | v32int16 | a,
|  | int | sgn_x,
|  | v32uint16 | b,
|  | int | sgn_y,
|  | v32acc32 | acc1 )

Parameters

  a | Matrix A
  sgn_x | Sign mask for matrix A
  b | Matrix B
  sgn_y | Sign mask for matrix B
  acc1 | Accumulator 1 input

Returns
  Result of operation

## ◆ mac_elem_32() [3/8]

v32acc32 mac_elem_32 | ( | v32int16 | a,
|  | v32int16 | b,
|  | v32acc32 | acc1 )

Parameters

  a | Matrix A
  b | Matrix B
  acc1 | Accumulator 1 input

Returns
  Result of operation

## ◆ mac_elem_32() [4/8]

v32acc32 mac_elem_32 | ( | v32int16 | a,
|  | v32uint16 | b,
|  | v32acc32 | acc1 )

Parameters

  a | Matrix A
  b | Matrix B
  acc1 | Accumulator 1 input

Returns
  Result of operation

## ◆ mac_elem_32() [5/8]

v32acc32 mac_elem_32 | ( | v32uint16 | a,
|  | int | sgn_x,
|  | v32int16 | b,
|  | int | sgn_y,
|  | v32acc32 | acc1 )

Parameters

  a | Matrix A
  sgn_x | Sign mask for matrix A
  b | Matrix B
  sgn_y | Sign mask for matrix B
  acc1 | Accumulator 1 input

Returns
  Result of operation

## ◆ mac_elem_32() [6/8]

v32acc32 mac_elem_32 | ( | v32uint16 | a,
|  | int | sgn_x,
|  | v32uint16 | b,
|  | int | sgn_y,
|  | v32acc32 | acc1 )

Parameters

  a | Matrix A
  sgn_x | Sign mask for matrix A
  b | Matrix B
  sgn_y | Sign mask for matrix B
  acc1 | Accumulator 1 input

Returns
  Result of operation

## ◆ mac_elem_32() [7/8]

v32acc32 mac_elem_32 | ( | v32uint16 | a,
|  | v32int16 | b,
|  | v32acc32 | acc1 )

Parameters

  a | Matrix A
  b | Matrix B
  acc1 | Accumulator 1 input

Returns
  Result of operation

## ◆ mac_elem_32() [8/8]

v32acc32 mac_elem_32 | ( | v32uint16 | a,
|  | v32uint16 | b,
|  | v32acc32 | acc1 )

Parameters

  a | Matrix A
  b | Matrix B
  acc1 | Accumulator 1 input

Returns
  Result of operation

## ◆ mac_elem_32_conf() [1/8]

v32acc32 mac_elem_32_conf | ( | v32int16 | a,
|  | int | sgn_x,
|  | v32int16 | b,
|  | int | sgn_y,
|  | v32acc32 | acc1,
|  | int | zero_acc1,
|  | int | shift16,
|  | int | sub_mul,
|  | int | sub_acc1 )

Parameters

  a | Matrix A
  sgn_x | Sign mask for matrix A
  b | Matrix B
  sgn_y | Sign mask for matrix B
  acc1 | Accumulator 1 input
  zero_acc1 | Zeroing mask for acc1
  shift16 | Shift mask of input accumulator acc1
  sub_mul | Negation mask of multiplication result
  sub_acc1 | Negation mask of acc1

Returns
  Result of operation

## ◆ mac_elem_32_conf() [2/8]

v32acc32 mac_elem_32_conf | ( | v32int16 | a,
|  | int | sgn_x,
|  | v32uint16 | b,
|  | int | sgn_y,
|  | v32acc32 | acc1,
|  | int | zero_acc1,
|  | int | shift16,
|  | int | sub_mul,
|  | int | sub_acc1 )

Parameters

  a | Matrix A
  sgn_x | Sign mask for matrix A
  b | Matrix B
  sgn_y | Sign mask for matrix B
  acc1 | Accumulator 1 input
  zero_acc1 | Zeroing mask for acc1
  shift16 | Shift mask of input accumulator acc1
  sub_mul | Negation mask of multiplication result
  sub_acc1 | Negation mask of acc1

Returns
  Result of operation

## ◆ mac_elem_32_conf() [3/8]

v32acc32 mac_elem_32_conf | ( | v32int16 | a,
|  | v32int16 | b,
|  | v32acc32 | acc1,
|  | int | zero_acc1,
|  | int | shift16,
|  | int | sub_mul,
|  | int | sub_acc1 )

Parameters

  a | Matrix A
  b | Matrix B
  acc1 | Accumulator 1 input
  zero_acc1 | Zeroing mask for acc1
  shift16 | Shift mask of input accumulator acc1
  sub_mul | Negation mask of multiplication result
  sub_acc1 | Negation mask of acc1

Returns
  Result of operation

## ◆ mac_elem_32_conf() [4/8]

v32acc32 mac_elem_32_conf | ( | v32int16 | a,
|  | v32uint16 | b,
|  | v32acc32 | acc1,
|  | int | zero_acc1,
|  | int | shift16,
|  | int | sub_mul,
|  | int | sub_acc1 )

Parameters

  a | Matrix A
  b | Matrix B
  acc1 | Accumulator 1 input
  zero_acc1 | Zeroing mask for acc1
  shift16 | Shift mask of input accumulator acc1
  sub_mul | Negation mask of multiplication result
  sub_acc1 | Negation mask of acc1

Returns
  Result of operation

## ◆ mac_elem_32_conf() [5/8]

v32acc32 mac_elem_32_conf | ( | v32uint16 | a,
|  | int | sgn_x,
|  | v32int16 | b,
|  | int | sgn_y,
|  | v32acc32 | acc1,
|  | int | zero_acc1,
|  | int | shift16,
|  | int | sub_mul,
|  | int | sub_acc1 )

Parameters

  a | Matrix A
  sgn_x | Sign mask for matrix A
  b | Matrix B
  sgn_y | Sign mask for matrix B
  acc1 | Accumulator 1 input
  zero_acc1 | Zeroing mask for acc1
  shift16 | Shift mask of input accumulator acc1
  sub_mul | Negation mask of multiplication result
  sub_acc1 | Negation mask of acc1

Returns
  Result of operation

## ◆ mac_elem_32_conf() [6/8]

v32acc32 mac_elem_32_conf | ( | v32uint16 | a,
|  | int | sgn_x,
|  | v32uint16 | b,
|  | int | sgn_y,
|  | v32acc32 | acc1,
|  | int | zero_acc1,
|  | int | shift16,
|  | int | sub_mul,
|  | int | sub_acc1 )

Parameters

  a | Matrix A
  sgn_x | Sign mask for matrix A
  b | Matrix B
  sgn_y | Sign mask for matrix B
  acc1 | Accumulator 1 input
  zero_acc1 | Zeroing mask for acc1
  shift16 | Shift mask of input accumulator acc1
  sub_mul | Negation mask of multiplication result
  sub_acc1 | Negation mask of acc1

Returns
  Result of operation

## ◆ mac_elem_32_conf() [7/8]

v32acc32 mac_elem_32_conf | ( | v32uint16 | a,
|  | v32int16 | b,
|  | v32acc32 | acc1,
|  | int | zero_acc1,
|  | int | shift16,
|  | int | sub_mul,
|  | int | sub_acc1 )

Parameters

  a | Matrix A
  b | Matrix B
  acc1 | Accumulator 1 input
  zero_acc1 | Zeroing mask for acc1
  shift16 | Shift mask of input accumulator acc1
  sub_mul | Negation mask of multiplication result
  sub_acc1 | Negation mask of acc1

Returns
  Result of operation

## ◆ mac_elem_32_conf() [8/8]

v32acc32 mac_elem_32_conf | ( | v32uint16 | a,
|  | v32uint16 | b,
|  | v32acc32 | acc1,
|  | int | zero_acc1,
|  | int | shift16,
|  | int | sub_mul,
|  | int | sub_acc1 )

Parameters

  a | Matrix A
  b | Matrix B
  acc1 | Accumulator 1 input
  zero_acc1 | Zeroing mask for acc1
  shift16 | Shift mask of input accumulator acc1
  sub_mul | Negation mask of multiplication result
  sub_acc1 | Negation mask of acc1

Returns
  Result of operation

## ◆ msc_2x4_4x8() [1/8]

v16acc64 msc_2x4_4x8 | ( | v32int16 | a,
|  | int | sgn_x,
|  | v32int16 | b,
|  | int | sgn_y,
|  | v16acc64 | acc1 )

Parameters

  a | Matrix A
  sgn_x | Sign mask for matrix A
  b | Matrix B
  sgn_y | Sign mask for matrix B
  acc1 | Accumulator 1 input

Returns
  Result of operation

## ◆ msc_2x4_4x8() [2/8]

v16acc64 msc_2x4_4x8 | ( | v32int16 | a,
|  | int | sgn_x,
|  | v32uint16 | b,
|  | int | sgn_y,
|  | v16acc64 | acc1 )

Parameters

  a | Matrix A
  sgn_x | Sign mask for matrix A
  b | Matrix B
  sgn_y | Sign mask for matrix B
  acc1 | Accumulator 1 input

Returns
  Result of operation

## ◆ msc_2x4_4x8() [3/8]

v16acc64 msc_2x4_4x8 | ( | v32int16 | a,
|  | v32int16 | b,
|  | v16acc64 | acc1 )

Parameters

  a | Matrix A
  b | Matrix B
  acc1 | Accumulator 1 input

Returns
  Result of operation

## ◆ msc_2x4_4x8() [4/8]

v16acc64 msc_2x4_4x8 | ( | v32int16 | a,
|  | v32uint16 | b,
|  | v16acc64 | acc1 )

Parameters

  a | Matrix A
  b | Matrix B
  acc1 | Accumulator 1 input

Returns
  Result of operation

## ◆ msc_2x4_4x8() [5/8]

v16acc64 msc_2x4_4x8 | ( | v32uint16 | a,
|  | int | sgn_x,
|  | v32int16 | b,
|  | int | sgn_y,
|  | v16acc64 | acc1 )

Parameters

  a | Matrix A
  sgn_x | Sign mask for matrix A
  b | Matrix B
  sgn_y | Sign mask for matrix B
  acc1 | Accumulator 1 input

Returns
  Result of operation

## ◆ msc_2x4_4x8() [6/8]

v16acc64 msc_2x4_4x8 | ( | v32uint16 | a,
|  | int | sgn_x,
|  | v32uint16 | b,
|  | int | sgn_y,
|  | v16acc64 | acc1 )

Parameters

  a | Matrix A
  sgn_x | Sign mask for matrix A
  b | Matrix B
  sgn_y | Sign mask for matrix B
  acc1 | Accumulator 1 input

Returns
  Result of operation

## ◆ msc_2x4_4x8() [7/8]

v16acc64 msc_2x4_4x8 | ( | v32uint16 | a,
|  | v32int16 | b,
|  | v16acc64 | acc1 )

Parameters

  a | Matrix A
  b | Matrix B
  acc1 | Accumulator 1 input

Returns
  Result of operation

## ◆ msc_2x4_4x8() [8/8]

v16acc64 msc_2x4_4x8 | ( | v32uint16 | a,
|  | v32uint16 | b,
|  | v16acc64 | acc1 )

Parameters

  a | Matrix A
  b | Matrix B
  acc1 | Accumulator 1 input

Returns
  Result of operation

## ◆ msc_2x4_4x8_conf() [1/8]

v16acc64 msc_2x4_4x8_conf | ( | v32int16 | a,
|  | int | sgn_x,
|  | v32int16 | b,
|  | int | sgn_y,
|  | v16acc64 | acc1,
|  | int | zero_acc1,
|  | int | shift16,
|  | int | sub_mul,
|  | int | sub_acc1 )

Parameters

  a | Matrix A
  sgn_x | Sign mask for matrix A
  b | Matrix B
  sgn_y | Sign mask for matrix B
  acc1 | Accumulator 1 input
  zero_acc1 | Zeroing mask for acc1
  shift16 | Shift mask of input accumulator acc1
  sub_mul | Negation mask of multiplication result. If a bit is set the corresponding output accumulator lane is negated.
  sub_acc1 | Negation mask of acc1. If a bit is set the corresponding accumulator lane of acc1 is negated.

Returns
  Result of operation

## ◆ msc_2x4_4x8_conf() [2/8]

v16acc64 msc_2x4_4x8_conf | ( | v32int16 | a,
|  | int | sgn_x,
|  | v32uint16 | b,
|  | int | sgn_y,
|  | v16acc64 | acc1,
|  | int | zero_acc1,
|  | int | shift16,
|  | int | sub_mul,
|  | int | sub_acc1 )

Parameters

  a | Matrix A
  sgn_x | Sign mask for matrix A
  b | Matrix B
  sgn_y | Sign mask for matrix B
  acc1 | Accumulator 1 input
  zero_acc1 | Zeroing mask for acc1
  shift16 | Shift mask of input accumulator acc1
  sub_mul | Negation mask of multiplication result. If a bit is set the corresponding output accumulator lane is negated.
  sub_acc1 | Negation mask of acc1. If a bit is set the corresponding accumulator lane of acc1 is negated.

Returns
  Result of operation

## ◆ msc_2x4_4x8_conf() [3/8]

v16acc64 msc_2x4_4x8_conf | ( | v32int16 | a,
|  | v32int16 | b,
|  | v16acc64 | acc1,
|  | int | zero_acc1,
|  | int | shift16,
|  | int | sub_mul,
|  | int | sub_acc1 )

Parameters

  a | Matrix A
  b | Matrix B
  acc1 | Accumulator 1 input
  zero_acc1 | Zeroing mask for acc1
  shift16 | Shift mask of input accumulator acc1
  sub_mul | Negation mask of multiplication result
  sub_acc1 | Negation mask of acc1

Returns
  Result of operation

## ◆ msc_2x4_4x8_conf() [4/8]

v16acc64 msc_2x4_4x8_conf | ( | v32int16 | a,
|  | v32uint16 | b,
|  | v16acc64 | acc1,
|  | int | zero_acc1,
|  | int | shift16,
|  | int | sub_mul,
|  | int | sub_acc1 )

Parameters

  a | Matrix A
  b | Matrix B
  acc1 | Accumulator 1 input
  zero_acc1 | Zeroing mask for acc1
  shift16 | Shift mask of input accumulator acc1
  sub_mul | Negation mask of multiplication result
  sub_acc1 | Negation mask of acc1

Returns
  Result of operation

## ◆ msc_2x4_4x8_conf() [5/8]

v16acc64 msc_2x4_4x8_conf | ( | v32uint16 | a,
|  | int | sgn_x,
|  | v32int16 | b,
|  | int | sgn_y,
|  | v16acc64 | acc1,
|  | int | zero_acc1,
|  | int | shift16,
|  | int | sub_mul,
|  | int | sub_acc1 )

Parameters

  a | Matrix A
  sgn_x | Sign mask for matrix A
  b | Matrix B
  sgn_y | Sign mask for matrix B
  acc1 | Accumulator 1 input
  zero_acc1 | Zeroing mask for acc1
  shift16 | Shift mask of input accumulator acc1
  sub_mul | Negation mask of multiplication result. If a bit is set the corresponding output accumulator lane is negated.
  sub_acc1 | Negation mask of acc1. If a bit is set the corresponding accumulator lane of acc1 is negated.

Returns
  Result of operation

## ◆ msc_2x4_4x8_conf() [6/8]

v16acc64 msc_2x4_4x8_conf | ( | v32uint16 | a,
|  | int | sgn_x,
|  | v32uint16 | b,
|  | int | sgn_y,
|  | v16acc64 | acc1,
|  | int | zero_acc1,
|  | int | shift16,
|  | int | sub_mul,
|  | int | sub_acc1 )

Parameters

  a | Matrix A
  sgn_x | Sign mask for matrix A
  b | Matrix B
  sgn_y | Sign mask for matrix B
  acc1 | Accumulator 1 input
  zero_acc1 | Zeroing mask for acc1
  shift16 | Shift mask of input accumulator acc1
  sub_mul | Negation mask of multiplication result. If a bit is set the corresponding output accumulator lane is negated.
  sub_acc1 | Negation mask of acc1. If a bit is set the corresponding accumulator lane of acc1 is negated.

Returns
  Result of operation

## ◆ msc_2x4_4x8_conf() [7/8]

v16acc64 msc_2x4_4x8_conf | ( | v32uint16 | a,
|  | v32int16 | b,
|  | v16acc64 | acc1,
|  | int | zero_acc1,
|  | int | shift16,
|  | int | sub_mul,
|  | int | sub_acc1 )

Parameters

  a | Matrix A
  b | Matrix B
  acc1 | Accumulator 1 input
  zero_acc1 | Zeroing mask for acc1
  shift16 | Shift mask of input accumulator acc1
  sub_mul | Negation mask of multiplication result
  sub_acc1 | Negation mask of acc1

Returns
  Result of operation

## ◆ msc_2x4_4x8_conf() [8/8]

v16acc64 msc_2x4_4x8_conf | ( | v32uint16 | a,
|  | v32uint16 | b,
|  | v16acc64 | acc1,
|  | int | zero_acc1,
|  | int | shift16,
|  | int | sub_mul,
|  | int | sub_acc1 )

Parameters

  a | Matrix A
  b | Matrix B
  acc1 | Accumulator 1 input
  zero_acc1 | Zeroing mask for acc1
  shift16 | Shift mask of input accumulator acc1
  sub_mul | Negation mask of multiplication result
  sub_acc1 | Negation mask of acc1

Returns
  Result of operation

## ◆ msc_4x2_2x8() [1/8]

v32acc32 msc_4x2_2x8 | ( | v32int16 | a,
|  | int | sgn_x,
|  | v32int16 | b,
|  | int | sgn_y,
|  | v32acc32 | acc1 )

Parameters

  a | Matrix A
  sgn_x | Sign mask for matrix A
  b | Matrix B
  sgn_y | Sign mask for matrix B
  acc1 | Accumulator 1 input

Returns
  Result of operation

## ◆ msc_4x2_2x8() [2/8]

v32acc32 msc_4x2_2x8 | ( | v32int16 | a,
|  | int | sgn_x,
|  | v32uint16 | b,
|  | int | sgn_y,
|  | v32acc32 | acc1 )

Parameters

  a | Matrix A
  sgn_x | Sign mask for matrix A
  b | Matrix B
  sgn_y | Sign mask for matrix B
  acc1 | Accumulator 1 input

Returns
  Result of operation

## ◆ msc_4x2_2x8() [3/8]

v32acc32 msc_4x2_2x8 | ( | v32int16 | a,
|  | v32int16 | b,
|  | v32acc32 | acc1 )

Parameters

  a | Matrix A
  b | Matrix B
  acc1 | Accumulator 1 input

Returns
  Result of operation

## ◆ msc_4x2_2x8() [4/8]

v32acc32 msc_4x2_2x8 | ( | v32int16 | a,
|  | v32uint16 | b,
|  | v32acc32 | acc1 )

Parameters

  a | Matrix A
  b | Matrix B
  acc1 | Accumulator 1 input

Returns
  Result of operation

## ◆ msc_4x2_2x8() [5/8]

v32acc32 msc_4x2_2x8 | ( | v32uint16 | a,
|  | int | sgn_x,
|  | v32int16 | b,
|  | int | sgn_y,
|  | v32acc32 | acc1 )

Parameters

  a | Matrix A
  sgn_x | Sign mask for matrix A
  b | Matrix B
  sgn_y | Sign mask for matrix B
  acc1 | Accumulator 1 input

Returns
  Result of operation

## ◆ msc_4x2_2x8() [6/8]

v32acc32 msc_4x2_2x8 | ( | v32uint16 | a,
|  | int | sgn_x,
|  | v32uint16 | b,
|  | int | sgn_y,
|  | v32acc32 | acc1 )

Parameters

  a | Matrix A
  sgn_x | Sign mask for matrix A
  b | Matrix B
  sgn_y | Sign mask for matrix B
  acc1 | Accumulator 1 input

Returns
  Result of operation

## ◆ msc_4x2_2x8() [7/8]

v32acc32 msc_4x2_2x8 | ( | v32uint16 | a,
|  | v32int16 | b,
|  | v32acc32 | acc1 )

Parameters

  a | Matrix A
  b | Matrix B
  acc1 | Accumulator 1 input

Returns
  Result of operation

## ◆ msc_4x2_2x8() [8/8]

v32acc32 msc_4x2_2x8 | ( | v32uint16 | a,
|  | v32uint16 | b,
|  | v32acc32 | acc1 )

Parameters

  a | Matrix A
  b | Matrix B
  acc1 | Accumulator 1 input

Returns
  Result of operation

## ◆ msc_4x2_2x8_conf() [1/8]

v32acc32 msc_4x2_2x8_conf | ( | v32int16 | a,
|  | int | sgn_x,
|  | v32int16 | b,
|  | int | sgn_y,
|  | v32acc32 | acc1,
|  | int | zero_acc1,
|  | int | shift16,
|  | int | sub_mul,
|  | int | sub_acc1 )

Parameters

  a | Matrix A
  sgn_x | Sign mask for matrix A
  b | Matrix B
  sgn_y | Sign mask for matrix B
  acc1 | Accumulator 1 input
  zero_acc1 | Zeroing mask for acc1
  shift16 | Shift mask of input accumulator acc1
  sub_mul | Negation mask of multiplication result. If a bit is set the corresponding output accumulator lane is negated.
  sub_acc1 | Negation mask of acc1. If a bit is set the corresponding accumulator lane of acc1 is negated.

Returns
  Result of operation

## ◆ msc_4x2_2x8_conf() [2/8]

v32acc32 msc_4x2_2x8_conf | ( | v32int16 | a,
|  | int | sgn_x,
|  | v32uint16 | b,
|  | int | sgn_y,
|  | v32acc32 | acc1,
|  | int | zero_acc1,
|  | int | shift16,
|  | int | sub_mul,
|  | int | sub_acc1 )

Parameters

  a | Matrix A
  sgn_x | Sign mask for matrix A
  b | Matrix B
  sgn_y | Sign mask for matrix B
  acc1 | Accumulator 1 input
  zero_acc1 | Zeroing mask for acc1
  shift16 | Shift mask of input accumulator acc1
  sub_mul | Negation mask of multiplication result. If a bit is set the corresponding output accumulator lane is negated.
  sub_acc1 | Negation mask of acc1. If a bit is set the corresponding accumulator lane of acc1 is negated.

Returns
  Result of operation

## ◆ msc_4x2_2x8_conf() [3/8]

v32acc32 msc_4x2_2x8_conf | ( | v32int16 | a,
|  | v32int16 | b,
|  | v32acc32 | acc1,
|  | int | zero_acc1,
|  | int | shift16,
|  | int | sub_mul,
|  | int | sub_acc1 )

Parameters

  a | Matrix A
  b | Matrix B
  acc1 | Accumulator 1 input
  zero_acc1 | Zeroing mask for acc1
  shift16 | Shift mask of input accumulator acc1
  sub_mul | Negation mask of multiplication result
  sub_acc1 | Negation mask of acc1

Returns
  Result of operation

## ◆ msc_4x2_2x8_conf() [4/8]

v32acc32 msc_4x2_2x8_conf | ( | v32int16 | a,
|  | v32uint16 | b,
|  | v32acc32 | acc1,
|  | int | zero_acc1,
|  | int | shift16,
|  | int | sub_mul,
|  | int | sub_acc1 )

Parameters

  a | Matrix A
  b | Matrix B
  acc1 | Accumulator 1 input
  zero_acc1 | Zeroing mask for acc1
  shift16 | Shift mask of input accumulator acc1
  sub_mul | Negation mask of multiplication result
  sub_acc1 | Negation mask of acc1

Returns
  Result of operation

## ◆ msc_4x2_2x8_conf() [5/8]

v32acc32 msc_4x2_2x8_conf | ( | v32uint16 | a,
|  | int | sgn_x,
|  | v32int16 | b,
|  | int | sgn_y,
|  | v32acc32 | acc1,
|  | int | zero_acc1,
|  | int | shift16,
|  | int | sub_mul,
|  | int | sub_acc1 )

Parameters

  a | Matrix A
  sgn_x | Sign mask for matrix A
  b | Matrix B
  sgn_y | Sign mask for matrix B
  acc1 | Accumulator 1 input
  zero_acc1 | Zeroing mask for acc1
  shift16 | Shift mask of input accumulator acc1
  sub_mul | Negation mask of multiplication result. If a bit is set the corresponding output accumulator lane is negated.
  sub_acc1 | Negation mask of acc1. If a bit is set the corresponding accumulator lane of acc1 is negated.

Returns
  Result of operation

## ◆ msc_4x2_2x8_conf() [6/8]

v32acc32 msc_4x2_2x8_conf | ( | v32uint16 | a,
|  | int | sgn_x,
|  | v32uint16 | b,
|  | int | sgn_y,
|  | v32acc32 | acc1,
|  | int | zero_acc1,
|  | int | shift16,
|  | int | sub_mul,
|  | int | sub_acc1 )

Parameters

  a | Matrix A
  sgn_x | Sign mask for matrix A
  b | Matrix B
  sgn_y | Sign mask for matrix B
  acc1 | Accumulator 1 input
  zero_acc1 | Zeroing mask for acc1
  shift16 | Shift mask of input accumulator acc1
  sub_mul | Negation mask of multiplication result. If a bit is set the corresponding output accumulator lane is negated.
  sub_acc1 | Negation mask of acc1. If a bit is set the corresponding accumulator lane of acc1 is negated.

Returns
  Result of operation

## ◆ msc_4x2_2x8_conf() [7/8]

v32acc32 msc_4x2_2x8_conf | ( | v32uint16 | a,
|  | v32int16 | b,
|  | v32acc32 | acc1,
|  | int | zero_acc1,
|  | int | shift16,
|  | int | sub_mul,
|  | int | sub_acc1 )

Parameters

  a | Matrix A
  b | Matrix B
  acc1 | Accumulator 1 input
  zero_acc1 | Zeroing mask for acc1
  shift16 | Shift mask of input accumulator acc1
  sub_mul | Negation mask of multiplication result
  sub_acc1 | Negation mask of acc1

Returns
  Result of operation

## ◆ msc_4x2_2x8_conf() [8/8]

v32acc32 msc_4x2_2x8_conf | ( | v32uint16 | a,
|  | v32uint16 | b,
|  | v32acc32 | acc1,
|  | int | zero_acc1,
|  | int | shift16,
|  | int | sub_mul,
|  | int | sub_acc1 )

Parameters

  a | Matrix A
  b | Matrix B
  acc1 | Accumulator 1 input
  zero_acc1 | Zeroing mask for acc1
  shift16 | Shift mask of input accumulator acc1
  sub_mul | Negation mask of multiplication result
  sub_acc1 | Negation mask of acc1

Returns
  Result of operation

## ◆ msc_4x4_4x4() [1/8]

v16acc64 msc_4x4_4x4 | ( | v32int16 | a,
|  | int | sgn_x,
|  | v32int16 | b,
|  | int | sgn_y,
|  | v16acc64 | acc1 )

Parameters

  a | Matrix A
  sgn_x | Sign mask for matrix A
  b | Matrix B
  sgn_y | Sign mask for matrix B
  acc1 | Accumulator 1 input

Returns
  Result of operation

## ◆ msc_4x4_4x4() [2/8]

v16acc64 msc_4x4_4x4 | ( | v32int16 | a,
|  | int | sgn_x,
|  | v32uint16 | b,
|  | int | sgn_y,
|  | v16acc64 | acc1 )

Parameters

  a | Matrix A
  sgn_x | Sign mask for matrix A
  b | Matrix B
  sgn_y | Sign mask for matrix B
  acc1 | Accumulator 1 input

Returns
  Result of operation

## ◆ msc_4x4_4x4() [3/8]

v16acc64 msc_4x4_4x4 | ( | v32int16 | a,
|  | v32int16 | b,
|  | v16acc64 | acc1 )

Parameters

  a | Matrix A
  b | Matrix B
  acc1 | Accumulator 1 input

Returns
  Result of operation

## ◆ msc_4x4_4x4() [4/8]

v16acc64 msc_4x4_4x4 | ( | v32int16 | a,
|  | v32uint16 | b,
|  | v16acc64 | acc1 )

Parameters

  a | Matrix A
  b | Matrix B
  acc1 | Accumulator 1 input

Returns
  Result of operation

## ◆ msc_4x4_4x4() [5/8]

v16acc64 msc_4x4_4x4 | ( | v32uint16 | a,
|  | int | sgn_x,
|  | v32int16 | b,
|  | int | sgn_y,
|  | v16acc64 | acc1 )

Parameters

  a | Matrix A
  sgn_x | Sign mask for matrix A
  b | Matrix B
  sgn_y | Sign mask for matrix B
  acc1 | Accumulator 1 input

Returns
  Result of operation

## ◆ msc_4x4_4x4() [6/8]

v16acc64 msc_4x4_4x4 | ( | v32uint16 | a,
|  | int | sgn_x,
|  | v32uint16 | b,
|  | int | sgn_y,
|  | v16acc64 | acc1 )

Parameters

  a | Matrix A
  sgn_x | Sign mask for matrix A
  b | Matrix B
  sgn_y | Sign mask for matrix B
  acc1 | Accumulator 1 input

Returns
  Result of operation

## ◆ msc_4x4_4x4() [7/8]

v16acc64 msc_4x4_4x4 | ( | v32uint16 | a,
|  | v32int16 | b,
|  | v16acc64 | acc1 )

Parameters

  a | Matrix A
  b | Matrix B
  acc1 | Accumulator 1 input

Returns
  Result of operation

## ◆ msc_4x4_4x4() [8/8]

v16acc64 msc_4x4_4x4 | ( | v32uint16 | a,
|  | v32uint16 | b,
|  | v16acc64 | acc1 )

Parameters

  a | Matrix A
  b | Matrix B
  acc1 | Accumulator 1 input

Returns
  Result of operation

## ◆ msc_4x4_4x4_conf() [1/8]

v16acc64 msc_4x4_4x4_conf | ( | v32int16 | a,
|  | int | sgn_x,
|  | v32int16 | b,
|  | int | sgn_y,
|  | v16acc64 | acc1,
|  | int | zero_acc1,
|  | int | shift16,
|  | int | sub_mul,
|  | int | sub_acc1 )

Parameters

  a | Matrix A
  sgn_x | Sign mask for matrix A
  b | Matrix B
  sgn_y | Sign mask for matrix B
  acc1 | Accumulator 1 input
  zero_acc1 | Zeroing mask for acc1
  shift16 | Shift mask of input accumulator acc1
  sub_mul | Negation mask of multiplication result. If a bit is set the corresponding output accumulator lane is negated.
  sub_acc1 | Negation mask of acc1. If a bit is set the corresponding accumulator lane of acc1 is negated.

Returns
  Result of operation

## ◆ msc_4x4_4x4_conf() [2/8]

v16acc64 msc_4x4_4x4_conf | ( | v32int16 | a,
|  | int | sgn_x,
|  | v32uint16 | b,
|  | int | sgn_y,
|  | v16acc64 | acc1,
|  | int | zero_acc1,
|  | int | shift16,
|  | int | sub_mul,
|  | int | sub_acc1 )

Parameters

  a | Matrix A
  sgn_x | Sign mask for matrix A
  b | Matrix B
  sgn_y | Sign mask for matrix B
  acc1 | Accumulator 1 input
  zero_acc1 | Zeroing mask for acc1
  shift16 | Shift mask of input accumulator acc1
  sub_mul | Negation mask of multiplication result. If a bit is set the corresponding output accumulator lane is negated.
  sub_acc1 | Negation mask of acc1. If a bit is set the corresponding accumulator lane of acc1 is negated.

Returns
  Result of operation

## ◆ msc_4x4_4x4_conf() [3/8]

v16acc64 msc_4x4_4x4_conf | ( | v32int16 | a,
|  | v32int16 | b,
|  | v16acc64 | acc1,
|  | int | zero_acc1,
|  | int | shift16,
|  | int | sub_mul,
|  | int | sub_acc1 )

Parameters

  a | Matrix A
  b | Matrix B
  acc1 | Accumulator 1 input
  zero_acc1 | Zeroing mask for acc1
  shift16 | Shift mask of input accumulator acc1
  sub_mul | Negation mask of multiplication result
  sub_acc1 | Negation mask of acc1

Returns
  Result of operation

## ◆ msc_4x4_4x4_conf() [4/8]

v16acc64 msc_4x4_4x4_conf | ( | v32int16 | a,
|  | v32uint16 | b,
|  | v16acc64 | acc1,
|  | int | zero_acc1,
|  | int | shift16,
|  | int | sub_mul,
|  | int | sub_acc1 )

Parameters

  a | Matrix A
  b | Matrix B
  acc1 | Accumulator 1 input
  zero_acc1 | Zeroing mask for acc1
  shift16 | Shift mask of input accumulator acc1
  sub_mul | Negation mask of multiplication result
  sub_acc1 | Negation mask of acc1

Returns
  Result of operation

## ◆ msc_4x4_4x4_conf() [5/8]

v16acc64 msc_4x4_4x4_conf | ( | v32uint16 | a,
|  | int | sgn_x,
|  | v32int16 | b,
|  | int | sgn_y,
|  | v16acc64 | acc1,
|  | int | zero_acc1,
|  | int | shift16,
|  | int | sub_mul,
|  | int | sub_acc1 )

Parameters

  a | Matrix A
  sgn_x | Sign mask for matrix A
  b | Matrix B
  sgn_y | Sign mask for matrix B
  acc1 | Accumulator 1 input
  zero_acc1 | Zeroing mask for acc1
  shift16 | Shift mask of input accumulator acc1
  sub_mul | Negation mask of multiplication result. If a bit is set the corresponding output accumulator lane is negated.
  sub_acc1 | Negation mask of acc1. If a bit is set the corresponding accumulator lane of acc1 is negated.

Returns
  Result of operation

## ◆ msc_4x4_4x4_conf() [6/8]

v16acc64 msc_4x4_4x4_conf | ( | v32uint16 | a,
|  | int | sgn_x,
|  | v32uint16 | b,
|  | int | sgn_y,
|  | v16acc64 | acc1,
|  | int | zero_acc1,
|  | int | shift16,
|  | int | sub_mul,
|  | int | sub_acc1 )

Parameters

  a | Matrix A
  sgn_x | Sign mask for matrix A
  b | Matrix B
  sgn_y | Sign mask for matrix B
  acc1 | Accumulator 1 input
  zero_acc1 | Zeroing mask for acc1
  shift16 | Shift mask of input accumulator acc1
  sub_mul | Negation mask of multiplication result. If a bit is set the corresponding output accumulator lane is negated.
  sub_acc1 | Negation mask of acc1. If a bit is set the corresponding accumulator lane of acc1 is negated.

Returns
  Result of operation

## ◆ msc_4x4_4x4_conf() [7/8]

v16acc64 msc_4x4_4x4_conf | ( | v32uint16 | a,
|  | v32int16 | b,
|  | v16acc64 | acc1,
|  | int | zero_acc1,
|  | int | shift16,
|  | int | sub_mul,
|  | int | sub_acc1 )

Parameters

  a | Matrix A
  b | Matrix B
  acc1 | Accumulator 1 input
  zero_acc1 | Zeroing mask for acc1
  shift16 | Shift mask of input accumulator acc1
  sub_mul | Negation mask of multiplication result
  sub_acc1 | Negation mask of acc1

Returns
  Result of operation

## ◆ msc_4x4_4x4_conf() [8/8]

v16acc64 msc_4x4_4x4_conf | ( | v32uint16 | a,
|  | v32uint16 | b,
|  | v16acc64 | acc1,
|  | int | zero_acc1,
|  | int | shift16,
|  | int | sub_mul,
|  | int | sub_acc1 )

Parameters

  a | Matrix A
  b | Matrix B
  acc1 | Accumulator 1 input
  zero_acc1 | Zeroing mask for acc1
  shift16 | Shift mask of input accumulator acc1
  sub_mul | Negation mask of multiplication result
  sub_acc1 | Negation mask of acc1

Returns
  Result of operation

## ◆ msc_conv_16x4() [1/8]

v16acc64 msc_conv_16x4 | ( | v32int16 | a,
|  | int | sgn_x,
|  | v32int16 | b,
|  | int | sgn_y,
|  | v16acc64 | acc1 )

Parameters

  a | Matrix A
  sgn_x | Sign mask for matrix A
  b | Matrix B
  sgn_y | Sign mask for matrix B
  acc1 | Accumulator 1 input

Returns
  Result of operation

## ◆ msc_conv_16x4() [2/8]

v16acc64 msc_conv_16x4 | ( | v32int16 | a,
|  | int | sgn_x,
|  | v32uint16 | b,
|  | int | sgn_y,
|  | v16acc64 | acc1 )

Parameters

  a | Matrix A
  sgn_x | Sign mask for matrix A
  b | Matrix B
  sgn_y | Sign mask for matrix B
  acc1 | Accumulator 1 input

Returns
  Result of operation

## ◆ msc_conv_16x4() [3/8]

v16acc64 msc_conv_16x4 | ( | v32int16 | a,
|  | v32int16 | b,
|  | v16acc64 | acc1 )

Parameters

  a | Matrix A
  b | Matrix B
  acc1 | Accumulator 1 input

Returns
  Result of operation

## ◆ msc_conv_16x4() [4/8]

v16acc64 msc_conv_16x4 | ( | v32int16 | a,
|  | v32uint16 | b,
|  | v16acc64 | acc1 )

Parameters

  a | Matrix A
  b | Matrix B
  acc1 | Accumulator 1 input

Returns
  Result of operation

## ◆ msc_conv_16x4() [5/8]

v16acc64 msc_conv_16x4 | ( | v32uint16 | a,
|  | int | sgn_x,
|  | v32int16 | b,
|  | int | sgn_y,
|  | v16acc64 | acc1 )

Parameters

  a | Matrix A
  sgn_x | Sign mask for matrix A
  b | Matrix B
  sgn_y | Sign mask for matrix B
  acc1 | Accumulator 1 input

Returns
  Result of operation

## ◆ msc_conv_16x4() [6/8]

v16acc64 msc_conv_16x4 | ( | v32uint16 | a,
|  | int | sgn_x,
|  | v32uint16 | b,
|  | int | sgn_y,
|  | v16acc64 | acc1 )

Parameters

  a | Matrix A
  sgn_x | Sign mask for matrix A
  b | Matrix B
  sgn_y | Sign mask for matrix B
  acc1 | Accumulator 1 input

Returns
  Result of operation

## ◆ msc_conv_16x4() [7/8]

v16acc64 msc_conv_16x4 | ( | v32uint16 | a,
|  | v32int16 | b,
|  | v16acc64 | acc1 )

Parameters

  a | Matrix A
  b | Matrix B
  acc1 | Accumulator 1 input

Returns
  Result of operation

## ◆ msc_conv_16x4() [8/8]

v16acc64 msc_conv_16x4 | ( | v32uint16 | a,
|  | v32uint16 | b,
|  | v16acc64 | acc1 )

Parameters

  a | Matrix A
  b | Matrix B
  acc1 | Accumulator 1 input

Returns
  Result of operation

## ◆ msc_conv_16x4_conf() [1/8]

v16acc64 msc_conv_16x4_conf | ( | v32int16 | a,
|  | int | sgn_x,
|  | v32int16 | b,
|  | int | sgn_y,
|  | v16acc64 | acc1,
|  | int | zero_acc1,
|  | int | shift16,
|  | int | sub_mul,
|  | int | sub_acc1 )

Parameters

  a | Matrix A
  sgn_x | Sign mask for matrix A
  b | Matrix B
  sgn_y | Sign mask for matrix B
  acc1 | Accumulator 1 input
  zero_acc1 | Zeroing mask for acc1
  shift16 | Shift mask of input accumulator acc1
  sub_mul | Negation mask of multiplication result. If a bit is set the corresponding output accumulator lane is negated.
  sub_acc1 | Negation mask of acc1. If a bit is set the corresponding accumulator lane of acc1 is negated.

Returns
  Result of operation

## ◆ msc_conv_16x4_conf() [2/8]

v16acc64 msc_conv_16x4_conf | ( | v32int16 | a,
|  | int | sgn_x,
|  | v32uint16 | b,
|  | int | sgn_y,
|  | v16acc64 | acc1,
|  | int | zero_acc1,
|  | int | shift16,
|  | int | sub_mul,
|  | int | sub_acc1 )

Parameters

  a | Matrix A
  sgn_x | Sign mask for matrix A
  b | Matrix B
  sgn_y | Sign mask for matrix B
  acc1 | Accumulator 1 input
  zero_acc1 | Zeroing mask for acc1
  shift16 | Shift mask of input accumulator acc1
  sub_mul | Negation mask of multiplication result. If a bit is set the corresponding output accumulator lane is negated.
  sub_acc1 | Negation mask of acc1. If a bit is set the corresponding accumulator lane of acc1 is negated.

Returns
  Result of operation

## ◆ msc_conv_16x4_conf() [3/8]

v16acc64 msc_conv_16x4_conf | ( | v32int16 | a,
|  | v32int16 | b,
|  | v16acc64 | acc1,
|  | int | zero_acc1,
|  | int | shift16,
|  | int | sub_mul,
|  | int | sub_acc1 )

Parameters

  a | Matrix A
  b | Matrix B
  acc1 | Accumulator 1 input
  zero_acc1 | Zeroing mask for acc1
  shift16 | Shift mask of input accumulator acc1
  sub_mul | Negation mask of multiplication result
  sub_acc1 | Negation mask of acc1

Returns
  Result of operation

## ◆ msc_conv_16x4_conf() [4/8]

v16acc64 msc_conv_16x4_conf | ( | v32int16 | a,
|  | v32uint16 | b,
|  | v16acc64 | acc1,
|  | int | zero_acc1,
|  | int | shift16,
|  | int | sub_mul,
|  | int | sub_acc1 )

Parameters

  a | Matrix A
  b | Matrix B
  acc1 | Accumulator 1 input
  zero_acc1 | Zeroing mask for acc1
  shift16 | Shift mask of input accumulator acc1
  sub_mul | Negation mask of multiplication result
  sub_acc1 | Negation mask of acc1

Returns
  Result of operation

## ◆ msc_conv_16x4_conf() [5/8]

v16acc64 msc_conv_16x4_conf | ( | v32uint16 | a,
|  | int | sgn_x,
|  | v32int16 | b,
|  | int | sgn_y,
|  | v16acc64 | acc1,
|  | int | zero_acc1,
|  | int | shift16,
|  | int | sub_mul,
|  | int | sub_acc1 )

Parameters

  a | Matrix A
  sgn_x | Sign mask for matrix A
  b | Matrix B
  sgn_y | Sign mask for matrix B
  acc1 | Accumulator 1 input
  zero_acc1 | Zeroing mask for acc1
  shift16 | Shift mask of input accumulator acc1
  sub_mul | Negation mask of multiplication result. If a bit is set the corresponding output accumulator lane is negated.
  sub_acc1 | Negation mask of acc1. If a bit is set the corresponding accumulator lane of acc1 is negated.

Returns
  Result of operation

## ◆ msc_conv_16x4_conf() [6/8]

v16acc64 msc_conv_16x4_conf | ( | v32uint16 | a,
|  | int | sgn_x,
|  | v32uint16 | b,
|  | int | sgn_y,
|  | v16acc64 | acc1,
|  | int | zero_acc1,
|  | int | shift16,
|  | int | sub_mul,
|  | int | sub_acc1 )

Parameters

  a | Matrix A
  sgn_x | Sign mask for matrix A
  b | Matrix B
  sgn_y | Sign mask for matrix B
  acc1 | Accumulator 1 input
  zero_acc1 | Zeroing mask for acc1
  shift16 | Shift mask of input accumulator acc1
  sub_mul | Negation mask of multiplication result. If a bit is set the corresponding output accumulator lane is negated.
  sub_acc1 | Negation mask of acc1. If a bit is set the corresponding accumulator lane of acc1 is negated.

Returns
  Result of operation

## ◆ msc_conv_16x4_conf() [7/8]

v16acc64 msc_conv_16x4_conf | ( | v32uint16 | a,
|  | v32int16 | b,
|  | v16acc64 | acc1,
|  | int | zero_acc1,
|  | int | shift16,
|  | int | sub_mul,
|  | int | sub_acc1 )

Parameters

  a | Matrix A
  b | Matrix B
  acc1 | Accumulator 1 input
  zero_acc1 | Zeroing mask for acc1
  shift16 | Shift mask of input accumulator acc1
  sub_mul | Negation mask of multiplication result
  sub_acc1 | Negation mask of acc1

Returns
  Result of operation

## ◆ msc_conv_16x4_conf() [8/8]

v16acc64 msc_conv_16x4_conf | ( | v32uint16 | a,
|  | v32uint16 | b,
|  | v16acc64 | acc1,
|  | int | zero_acc1,
|  | int | shift16,
|  | int | sub_mul,
|  | int | sub_acc1 )

Parameters

  a | Matrix A
  b | Matrix B
  acc1 | Accumulator 1 input
  zero_acc1 | Zeroing mask for acc1
  shift16 | Shift mask of input accumulator acc1
  sub_mul | Negation mask of multiplication result
  sub_acc1 | Negation mask of acc1

Returns
  Result of operation

## ◆ msc_elem_16_2() [1/9]

v16accfloat msc_elem_16_2 | ( | v32bfloat16 | a,
|  | v32bfloat16 | b,
|  | v16accfloat | acc1 )

Parameters

  a | Matrix A
  b | Matrix B
  acc1 | Accumulator 1 input

Returns
  Result of operation

## ◆ msc_elem_16_2() [2/9]

v16acc64 msc_elem_16_2 | ( | v32int16 | a,
|  | int | sgn_x,
|  | v32int16 | b,
|  | int | sgn_y,
|  | v16acc64 | acc1 )

Parameters

  a | Matrix A
  sgn_x | Sign mask for matrix A
  b | Matrix B
  sgn_y | Sign mask for matrix B
  acc1 | Accumulator 1 input

Returns
  Result of operation

## ◆ msc_elem_16_2() [3/9]

v16acc64 msc_elem_16_2 | ( | v32int16 | a,
|  | int | sgn_x,
|  | v32uint16 | b,
|  | int | sgn_y,
|  | v16acc64 | acc1 )

Parameters

  a | Matrix A
  sgn_x | Sign mask for matrix A
  b | Matrix B
  sgn_y | Sign mask for matrix B
  acc1 | Accumulator 1 input

Returns
  Result of operation

## ◆ msc_elem_16_2() [4/9]

v16acc64 msc_elem_16_2 | ( | v32int16 | a,
|  | v32int16 | b,
|  | v16acc64 | acc1 )

Parameters

  a | Matrix A
  b | Matrix B
  acc1 | Accumulator 1 input

Returns
  Result of operation

## ◆ msc_elem_16_2() [5/9]

v16acc64 msc_elem_16_2 | ( | v32int16 | a,
|  | v32uint16 | b,
|  | v16acc64 | acc1 )

Parameters

  a | Matrix A
  b | Matrix B
  acc1 | Accumulator 1 input

Returns
  Result of operation

## ◆ msc_elem_16_2() [6/9]

v16acc64 msc_elem_16_2 | ( | v32uint16 | a,
|  | int | sgn_x,
|  | v32int16 | b,
|  | int | sgn_y,
|  | v16acc64 | acc1 )

Parameters

  a | Matrix A
  sgn_x | Sign mask for matrix A
  b | Matrix B
  sgn_y | Sign mask for matrix B
  acc1 | Accumulator 1 input

Returns
  Result of operation

## ◆ msc_elem_16_2() [7/9]

v16acc64 msc_elem_16_2 | ( | v32uint16 | a,
|  | int | sgn_x,
|  | v32uint16 | b,
|  | int | sgn_y,
|  | v16acc64 | acc1 )

Parameters

  a | Matrix A
  sgn_x | Sign mask for matrix A
  b | Matrix B
  sgn_y | Sign mask for matrix B
  acc1 | Accumulator 1 input

Returns
  Result of operation

## ◆ msc_elem_16_2() [8/9]

v16acc64 msc_elem_16_2 | ( | v32uint16 | a,
|  | v32int16 | b,
|  | v16acc64 | acc1 )

Parameters

  a | Matrix A
  b | Matrix B
  acc1 | Accumulator 1 input

Returns
  Result of operation

## ◆ msc_elem_16_2() [9/9]

v16acc64 msc_elem_16_2 | ( | v32uint16 | a,
|  | v32uint16 | b,
|  | v16acc64 | acc1 )

Parameters

  a | Matrix A
  b | Matrix B
  acc1 | Accumulator 1 input

Returns
  Result of operation

## ◆ msc_elem_16_2_conf() [1/9]

v16accfloat msc_elem_16_2_conf | ( | v32bfloat16 | a,
|  | v32bfloat16 | b,
|  | v16accfloat | acc1,
|  | int | zero_acc1,
|  | int | sub_mul,
|  | int | sub_acc1 )

Parameters

  a | Matrix A
  b | Matrix B
  acc1 | Accumulator 1 input
  zero_acc1 | Zeroing mask for acc1
  sub_mul | Negation mask of multiplication result
  sub_acc1 | Negation mask of acc1

Returns
  Result of operation

## ◆ msc_elem_16_2_conf() [2/9]

v16acc64 msc_elem_16_2_conf | ( | v32int16 | a,
|  | int | sgn_x,
|  | v32int16 | b,
|  | int | sgn_y,
|  | v16acc64 | acc1,
|  | int | zero_acc1,
|  | int | shift16,
|  | int | sub_mul,
|  | int | sub_acc1 )

Parameters

  a | Matrix A
  sgn_x | Sign mask for matrix A
  b | Matrix B
  sgn_y | Sign mask for matrix B
  acc1 | Accumulator 1 input
  zero_acc1 | Zeroing mask for acc1
  shift16 | Shift mask of input accumulator acc1
  sub_mul | Negation mask of multiplication result. If a bit is set the corresponding output accumulator lane is negated.
  sub_acc1 | Negation mask of acc1. If a bit is set the corresponding accumulator lane of acc1 is negated.

Returns
  Result of operation

## ◆ msc_elem_16_2_conf() [3/9]

v16acc64 msc_elem_16_2_conf | ( | v32int16 | a,
|  | int | sgn_x,
|  | v32uint16 | b,
|  | int | sgn_y,
|  | v16acc64 | acc1,
|  | int | zero_acc1,
|  | int | shift16,
|  | int | sub_mul,
|  | int | sub_acc1 )

Parameters

  a | Matrix A
  sgn_x | Sign mask for matrix A
  b | Matrix B
  sgn_y | Sign mask for matrix B
  acc1 | Accumulator 1 input
  zero_acc1 | Zeroing mask for acc1
  shift16 | Shift mask of input accumulator acc1
  sub_mul | Negation mask of multiplication result. If a bit is set the corresponding output accumulator lane is negated.
  sub_acc1 | Negation mask of acc1. If a bit is set the corresponding accumulator lane of acc1 is negated.

Returns
  Result of operation

## ◆ msc_elem_16_2_conf() [4/9]

v16acc64 msc_elem_16_2_conf | ( | v32int16 | a,
|  | v32int16 | b,
|  | v16acc64 | acc1,
|  | int | zero_acc1,
|  | int | shift16,
|  | int | sub_mul,
|  | int | sub_acc1 )

Parameters

  a | Matrix A
  b | Matrix B
  acc1 | Accumulator 1 input
  zero_acc1 | Zeroing mask for acc1
  shift16 | Shift mask of input accumulator acc1
  sub_mul | Negation mask of multiplication result
  sub_acc1 | Negation mask of acc1

Returns
  Result of operation

## ◆ msc_elem_16_2_conf() [5/9]

v16acc64 msc_elem_16_2_conf | ( | v32int16 | a,
|  | v32uint16 | b,
|  | v16acc64 | acc1,
|  | int | zero_acc1,
|  | int | shift16,
|  | int | sub_mul,
|  | int | sub_acc1 )

Parameters

  a | Matrix A
  b | Matrix B
  acc1 | Accumulator 1 input
  zero_acc1 | Zeroing mask for acc1
  shift16 | Shift mask of input accumulator acc1
  sub_mul | Negation mask of multiplication result
  sub_acc1 | Negation mask of acc1

Returns
  Result of operation

## ◆ msc_elem_16_2_conf() [6/9]

v16acc64 msc_elem_16_2_conf | ( | v32uint16 | a,
|  | int | sgn_x,
|  | v32int16 | b,
|  | int | sgn_y,
|  | v16acc64 | acc1,
|  | int | zero_acc1,
|  | int | shift16,
|  | int | sub_mul,
|  | int | sub_acc1 )

Parameters

  a | Matrix A
  sgn_x | Sign mask for matrix A
  b | Matrix B
  sgn_y | Sign mask for matrix B
  acc1 | Accumulator 1 input
  zero_acc1 | Zeroing mask for acc1
  shift16 | Shift mask of input accumulator acc1
  sub_mul | Negation mask of multiplication result. If a bit is set the corresponding output accumulator lane is negated.
  sub_acc1 | Negation mask of acc1. If a bit is set the corresponding accumulator lane of acc1 is negated.

Returns
  Result of operation

## ◆ msc_elem_16_2_conf() [7/9]

v16acc64 msc_elem_16_2_conf | ( | v32uint16 | a,
|  | int | sgn_x,
|  | v32uint16 | b,
|  | int | sgn_y,
|  | v16acc64 | acc1,
|  | int | zero_acc1,
|  | int | shift16,
|  | int | sub_mul,
|  | int | sub_acc1 )

Parameters

  a | Matrix A
  sgn_x | Sign mask for matrix A
  b | Matrix B
  sgn_y | Sign mask for matrix B
  acc1 | Accumulator 1 input
  zero_acc1 | Zeroing mask for acc1
  shift16 | Shift mask of input accumulator acc1
  sub_mul | Negation mask of multiplication result. If a bit is set the corresponding output accumulator lane is negated.
  sub_acc1 | Negation mask of acc1. If a bit is set the corresponding accumulator lane of acc1 is negated.

Returns
  Result of operation

## ◆ msc_elem_16_2_conf() [8/9]

v16acc64 msc_elem_16_2_conf | ( | v32uint16 | a,
|  | v32int16 | b,
|  | v16acc64 | acc1,
|  | int | zero_acc1,
|  | int | shift16,
|  | int | sub_mul,
|  | int | sub_acc1 )

Parameters

  a | Matrix A
  b | Matrix B
  acc1 | Accumulator 1 input
  zero_acc1 | Zeroing mask for acc1
  shift16 | Shift mask of input accumulator acc1
  sub_mul | Negation mask of multiplication result
  sub_acc1 | Negation mask of acc1

Returns
  Result of operation

## ◆ msc_elem_16_2_conf() [9/9]

v16acc64 msc_elem_16_2_conf | ( | v32uint16 | a,
|  | v32uint16 | b,
|  | v16acc64 | acc1,
|  | int | zero_acc1,
|  | int | shift16,
|  | int | sub_mul,
|  | int | sub_acc1 )

Parameters

  a | Matrix A
  b | Matrix B
  acc1 | Accumulator 1 input
  zero_acc1 | Zeroing mask for acc1
  shift16 | Shift mask of input accumulator acc1
  sub_mul | Negation mask of multiplication result
  sub_acc1 | Negation mask of acc1

Returns
  Result of operation

## ◆ msc_elem_32() [1/8]

v32acc32 msc_elem_32 | ( | v32int16 | a,
|  | int | sgn_x,
|  | v32int16 | b,
|  | int | sgn_y,
|  | v32acc32 | acc1 )

Parameters

  a | Matrix A
  sgn_x | Sign mask for matrix A
  b | Matrix B
  sgn_y | Sign mask for matrix B
  acc1 | Accumulator 1 input

Returns
  Result of operation

## ◆ msc_elem_32() [2/8]

v32acc32 msc_elem_32 | ( | v32int16 | a,
|  | int | sgn_x,
|  | v32uint16 | b,
|  | int | sgn_y,
|  | v32acc32 | acc1 )

Parameters

  a | Matrix A
  sgn_x | Sign mask for matrix A
  b | Matrix B
  sgn_y | Sign mask for matrix B
  acc1 | Accumulator 1 input

Returns
  Result of operation

## ◆ msc_elem_32() [3/8]

v32acc32 msc_elem_32 | ( | v32int16 | a,
|  | v32int16 | b,
|  | v32acc32 | acc1 )

Parameters

  a | Matrix A
  b | Matrix B
  acc1 | Accumulator 1 input

Returns
  Result of operation

## ◆ msc_elem_32() [4/8]

v32acc32 msc_elem_32 | ( | v32int16 | a,
|  | v32uint16 | b,
|  | v32acc32 | acc1 )

Parameters

  a | Matrix A
  b | Matrix B
  acc1 | Accumulator 1 input

Returns
  Result of operation

## ◆ msc_elem_32() [5/8]

v32acc32 msc_elem_32 | ( | v32uint16 | a,
|  | int | sgn_x,
|  | v32int16 | b,
|  | int | sgn_y,
|  | v32acc32 | acc1 )

Parameters

  a | Matrix A
  sgn_x | Sign mask for matrix A
  b | Matrix B
  sgn_y | Sign mask for matrix B
  acc1 | Accumulator 1 input

Returns
  Result of operation

## ◆ msc_elem_32() [6/8]

v32acc32 msc_elem_32 | ( | v32uint16 | a,
|  | int | sgn_x,
|  | v32uint16 | b,
|  | int | sgn_y,
|  | v32acc32 | acc1 )

Parameters

  a | Matrix A
  sgn_x | Sign mask for matrix A
  b | Matrix B
  sgn_y | Sign mask for matrix B
  acc1 | Accumulator 1 input

Returns
  Result of operation

## ◆ msc_elem_32() [7/8]

v32acc32 msc_elem_32 | ( | v32uint16 | a,
|  | v32int16 | b,
|  | v32acc32 | acc1 )

Parameters

  a | Matrix A
  b | Matrix B
  acc1 | Accumulator 1 input

Returns
  Result of operation

## ◆ msc_elem_32() [8/8]

v32acc32 msc_elem_32 | ( | v32uint16 | a,
|  | v32uint16 | b,
|  | v32acc32 | acc1 )

Parameters

  a | Matrix A
  b | Matrix B
  acc1 | Accumulator 1 input

Returns
  Result of operation

## ◆ msc_elem_32_conf() [1/8]

v32acc32 msc_elem_32_conf | ( | v32int16 | a,
|  | int | sgn_x,
|  | v32int16 | b,
|  | int | sgn_y,
|  | v32acc32 | acc1,
|  | int | zero_acc1,
|  | int | shift16,
|  | int | sub_mul,
|  | int | sub_acc1 )

Parameters

  a | Matrix A
  sgn_x | Sign mask for matrix A
  b | Matrix B
  sgn_y | Sign mask for matrix B
  acc1 | Accumulator 1 input
  zero_acc1 | Zeroing mask for acc1
  shift16 | Shift mask of input accumulator acc1
  sub_mul | Negation mask of multiplication result. If a bit is set the corresponding output accumulator lane is negated.
  sub_acc1 | Negation mask of acc1. If a bit is set the corresponding accumulator lane of acc1 is negated.

Returns
  Result of operation

## ◆ msc_elem_32_conf() [2/8]

v32acc32 msc_elem_32_conf | ( | v32int16 | a,
|  | int | sgn_x,
|  | v32uint16 | b,
|  | int | sgn_y,
|  | v32acc32 | acc1,
|  | int | zero_acc1,
|  | int | shift16,
|  | int | sub_mul,
|  | int | sub_acc1 )

Parameters

  a | Matrix A
  sgn_x | Sign mask for matrix A
  b | Matrix B
  sgn_y | Sign mask for matrix B
  acc1 | Accumulator 1 input
  zero_acc1 | Zeroing mask for acc1
  shift16 | Shift mask of input accumulator acc1
  sub_mul | Negation mask of multiplication result. If a bit is set the corresponding output accumulator lane is negated.
  sub_acc1 | Negation mask of acc1. If a bit is set the corresponding accumulator lane of acc1 is negated.

Returns
  Result of operation

## ◆ msc_elem_32_conf() [3/8]

v32acc32 msc_elem_32_conf | ( | v32int16 | a,
|  | v32int16 | b,
|  | v32acc32 | acc1,
|  | int | zero_acc1,
|  | int | shift16,
|  | int | sub_mul,
|  | int | sub_acc1 )

Parameters

  a | Matrix A
  b | Matrix B
  acc1 | Accumulator 1 input
  zero_acc1 | Zeroing mask for acc1
  shift16 | Shift mask of input accumulator acc1
  sub_mul | Negation mask of multiplication result
  sub_acc1 | Negation mask of acc1

Returns
  Result of operation

## ◆ msc_elem_32_conf() [4/8]

v32acc32 msc_elem_32_conf | ( | v32int16 | a,
|  | v32uint16 | b,
|  | v32acc32 | acc1,
|  | int | zero_acc1,
|  | int | shift16,
|  | int | sub_mul,
|  | int | sub_acc1 )

Parameters

  a | Matrix A
  b | Matrix B
  acc1 | Accumulator 1 input
  zero_acc1 | Zeroing mask for acc1
  shift16 | Shift mask of input accumulator acc1
  sub_mul | Negation mask of multiplication result
  sub_acc1 | Negation mask of acc1

Returns
  Result of operation

## ◆ msc_elem_32_conf() [5/8]

v32acc32 msc_elem_32_conf | ( | v32uint16 | a,
|  | int | sgn_x,
|  | v32int16 | b,
|  | int | sgn_y,
|  | v32acc32 | acc1,
|  | int | zero_acc1,
|  | int | shift16,
|  | int | sub_mul,
|  | int | sub_acc1 )

Parameters

  a | Matrix A
  sgn_x | Sign mask for matrix A
  b | Matrix B
  sgn_y | Sign mask for matrix B
  acc1 | Accumulator 1 input
  zero_acc1 | Zeroing mask for acc1
  shift16 | Shift mask of input accumulator acc1
  sub_mul | Negation mask of multiplication result. If a bit is set the corresponding output accumulator lane is negated.
  sub_acc1 | Negation mask of acc1. If a bit is set the corresponding accumulator lane of acc1 is negated.

Returns
  Result of operation

## ◆ msc_elem_32_conf() [6/8]

v32acc32 msc_elem_32_conf | ( | v32uint16 | a,
|  | int | sgn_x,
|  | v32uint16 | b,
|  | int | sgn_y,
|  | v32acc32 | acc1,
|  | int | zero_acc1,
|  | int | shift16,
|  | int | sub_mul,
|  | int | sub_acc1 )

Parameters

  a | Matrix A
  sgn_x | Sign mask for matrix A
  b | Matrix B
  sgn_y | Sign mask for matrix B
  acc1 | Accumulator 1 input
  zero_acc1 | Zeroing mask for acc1
  shift16 | Shift mask of input accumulator acc1
  sub_mul | Negation mask of multiplication result. If a bit is set the corresponding output accumulator lane is negated.
  sub_acc1 | Negation mask of acc1. If a bit is set the corresponding accumulator lane of acc1 is negated.

Returns
  Result of operation

## ◆ msc_elem_32_conf() [7/8]

v32acc32 msc_elem_32_conf | ( | v32uint16 | a,
|  | v32int16 | b,
|  | v32acc32 | acc1,
|  | int | zero_acc1,
|  | int | shift16,
|  | int | sub_mul,
|  | int | sub_acc1 )

Parameters

  a | Matrix A
  b | Matrix B
  acc1 | Accumulator 1 input
  zero_acc1 | Zeroing mask for acc1
  shift16 | Shift mask of input accumulator acc1
  sub_mul | Negation mask of multiplication result
  sub_acc1 | Negation mask of acc1

Returns
  Result of operation

## ◆ msc_elem_32_conf() [8/8]

v32acc32 msc_elem_32_conf | ( | v32uint16 | a,
|  | v32uint16 | b,
|  | v32acc32 | acc1,
|  | int | zero_acc1,
|  | int | shift16,
|  | int | sub_mul,
|  | int | sub_acc1 )

Parameters

  a | Matrix A
  b | Matrix B
  acc1 | Accumulator 1 input
  zero_acc1 | Zeroing mask for acc1
  shift16 | Shift mask of input accumulator acc1
  sub_mul | Negation mask of multiplication result
  sub_acc1 | Negation mask of acc1

Returns
  Result of operation

## ◆ mul_2x4_4x8() [1/8]

v16acc64 mul_2x4_4x8 | ( | v32int16 | a,
|  | int | sgn_x,
|  | v32int16 | b,
|  | int | sgn_y )

Parameters

  a | Matrix A
  sgn_x | Sign mask for matrix A
  b | Matrix B
  sgn_y | Sign mask for matrix B

Returns
  Result of operation

## ◆ mul_2x4_4x8() [2/8]

v16acc64 mul_2x4_4x8 | ( | v32int16 | a,
|  | int | sgn_x,
|  | v32uint16 | b,
|  | int | sgn_y )

Parameters

  a | Matrix A
  sgn_x | Sign mask for matrix A
  b | Matrix B
  sgn_y | Sign mask for matrix B

Returns
  Result of operation

## ◆ mul_2x4_4x8() [3/8]

v16acc64 mul_2x4_4x8 | ( | v32int16 | a,
|  | v32int16 | b )

Parameters

  a | Matrix A
  b | Matrix B

Returns
  Result of operation

## ◆ mul_2x4_4x8() [4/8]

v16acc64 mul_2x4_4x8 | ( | v32int16 | a,
|  | v32uint16 | b )

Parameters

  a | Matrix A
  b | Matrix B

Returns
  Result of operation

## ◆ mul_2x4_4x8() [5/8]

v16acc64 mul_2x4_4x8 | ( | v32uint16 | a,
|  | int | sgn_x,
|  | v32int16 | b,
|  | int | sgn_y )

Parameters

  a | Matrix A
  sgn_x | Sign mask for matrix A
  b | Matrix B
  sgn_y | Sign mask for matrix B

Returns
  Result of operation

## ◆ mul_2x4_4x8() [6/8]

v16acc64 mul_2x4_4x8 | ( | v32uint16 | a,
|  | int | sgn_x,
|  | v32uint16 | b,
|  | int | sgn_y )

Parameters

  a | Matrix A
  sgn_x | Sign mask for matrix A
  b | Matrix B
  sgn_y | Sign mask for matrix B

Returns
  Result of operation

## ◆ mul_2x4_4x8() [7/8]

v16acc64 mul_2x4_4x8 | ( | v32uint16 | a,
|  | v32int16 | b )

Parameters

  a | Matrix A
  b | Matrix B

Returns
  Result of operation

## ◆ mul_2x4_4x8() [8/8]

v16acc64 mul_2x4_4x8 | ( | v32uint16 | a,
|  | v32uint16 | b )

Parameters

  a | Matrix A
  b | Matrix B

Returns
  Result of operation

## ◆ mul_2x4_4x8_conf() [1/8]

v16acc64 mul_2x4_4x8_conf | ( | v32int16 | a,
|  | int | sgn_x,
|  | v32int16 | b,
|  | int | sgn_y,
|  | int | sub_mul )

Parameters

  a | Matrix A
  sgn_x | Sign mask for matrix A
  b | Matrix B
  sgn_y | Sign mask for matrix B
  sub_mul | Negation mask of multiplication result. If a bit is set the corresponding output accumulator lane is negated.

Returns
  Result of operation

## ◆ mul_2x4_4x8_conf() [2/8]

v16acc64 mul_2x4_4x8_conf | ( | v32int16 | a,
|  | int | sgn_x,
|  | v32uint16 | b,
|  | int | sgn_y,
|  | int | sub_mul )

Parameters

  a | Matrix A
  sgn_x | Sign mask for matrix A
  b | Matrix B
  sgn_y | Sign mask for matrix B
  sub_mul | Negation mask of multiplication result. If a bit is set the corresponding output accumulator lane is negated.

Returns
  Result of operation

## ◆ mul_2x4_4x8_conf() [3/8]

v16acc64 mul_2x4_4x8_conf | ( | v32int16 | a,
|  | v32int16 | b,
|  | int | sub_mul )

Parameters

  a | Matrix A
  b | Matrix B
  sub_mul | Negation mask for multiplication result

Returns
  Result of operation

## ◆ mul_2x4_4x8_conf() [4/8]

v16acc64 mul_2x4_4x8_conf | ( | v32int16 | a,
|  | v32uint16 | b,
|  | int | sub_mul )

Parameters

  a | Matrix A
  b | Matrix B
  sub_mul | Negation mask for multiplication result

Returns
  Result of operation

## ◆ mul_2x4_4x8_conf() [5/8]

v16acc64 mul_2x4_4x8_conf | ( | v32uint16 | a,
|  | int | sgn_x,
|  | v32int16 | b,
|  | int | sgn_y,
|  | int | sub_mul )

Parameters

  a | Matrix A
  sgn_x | Sign mask for matrix A
  b | Matrix B
  sgn_y | Sign mask for matrix B
  sub_mul | Negation mask of multiplication result. If a bit is set the corresponding output accumulator lane is negated.

Returns
  Result of operation

## ◆ mul_2x4_4x8_conf() [6/8]

v16acc64 mul_2x4_4x8_conf | ( | v32uint16 | a,
|  | int | sgn_x,
|  | v32uint16 | b,
|  | int | sgn_y,
|  | int | sub_mul )

Parameters

  a | Matrix A
  sgn_x | Sign mask for matrix A
  b | Matrix B
  sgn_y | Sign mask for matrix B
  sub_mul | Negation mask of multiplication result. If a bit is set the corresponding output accumulator lane is negated.

Returns
  Result of operation

## ◆ mul_2x4_4x8_conf() [7/8]

v16acc64 mul_2x4_4x8_conf | ( | v32uint16 | a,
|  | v32int16 | b,
|  | int | sub_mul )

Parameters

  a | Matrix A
  b | Matrix B
  sub_mul | Negation mask for multiplication result

Returns
  Result of operation

## ◆ mul_2x4_4x8_conf() [8/8]

v16acc64 mul_2x4_4x8_conf | ( | v32uint16 | a,
|  | v32uint16 | b,
|  | int | sub_mul )

Parameters

  a | Matrix A
  b | Matrix B
  sub_mul | Negation mask for multiplication result

Returns
  Result of operation

## ◆ mul_4x2_2x8() [1/8]

v32acc32 mul_4x2_2x8 | ( | v32int16 | a,
|  | int | sgn_x,
|  | v32int16 | b,
|  | int | sgn_y )

Parameters

  a | Matrix A
  sgn_x | Sign mask for matrix A
  b | Matrix B
  sgn_y | Sign mask for matrix B

Returns
  Result of operation

## ◆ mul_4x2_2x8() [2/8]

v32acc32 mul_4x2_2x8 | ( | v32int16 | a,
|  | int | sgn_x,
|  | v32uint16 | b,
|  | int | sgn_y )

Parameters

  a | Matrix A
  sgn_x | Sign mask for matrix A
  b | Matrix B
  sgn_y | Sign mask for matrix B

Returns
  Result of operation

## ◆ mul_4x2_2x8() [3/8]

v32acc32 mul_4x2_2x8 | ( | v32int16 | a,
|  | v32int16 | b )

Parameters

  a | Matrix A
  b | Matrix B

Returns
  Result of operation

## ◆ mul_4x2_2x8() [4/8]

v32acc32 mul_4x2_2x8 | ( | v32int16 | a,
|  | v32uint16 | b )

Parameters

  a | Matrix A
  b | Matrix B

Returns
  Result of operation

## ◆ mul_4x2_2x8() [5/8]

v32acc32 mul_4x2_2x8 | ( | v32uint16 | a,
|  | int | sgn_x,
|  | v32int16 | b,
|  | int | sgn_y )

Parameters

  a | Matrix A
  sgn_x | Sign mask for matrix A
  b | Matrix B
  sgn_y | Sign mask for matrix B

Returns
  Result of operation

## ◆ mul_4x2_2x8() [6/8]

v32acc32 mul_4x2_2x8 | ( | v32uint16 | a,
|  | int | sgn_x,
|  | v32uint16 | b,
|  | int | sgn_y )

Parameters

  a | Matrix A
  sgn_x | Sign mask for matrix A
  b | Matrix B
  sgn_y | Sign mask for matrix B

Returns
  Result of operation

## ◆ mul_4x2_2x8() [7/8]

v32acc32 mul_4x2_2x8 | ( | v32uint16 | a,
|  | v32int16 | b )

Parameters

  a | Matrix A
  b | Matrix B

Returns
  Result of operation

## ◆ mul_4x2_2x8() [8/8]

v32acc32 mul_4x2_2x8 | ( | v32uint16 | a,
|  | v32uint16 | b )

Parameters

  a | Matrix A
  b | Matrix B

Returns
  Result of operation

## ◆ mul_4x2_2x8_conf() [1/8]

v32acc32 mul_4x2_2x8_conf | ( | v32int16 | a,
|  | int | sgn_x,
|  | v32int16 | b,
|  | int | sgn_y,
|  | int | sub_mul )

Parameters

  a | Matrix A
  sgn_x | Sign mask for matrix A
  b | Matrix B
  sgn_y | Sign mask for matrix B
  sub_mul | Negation mask of multiplication result. If a bit is set the corresponding output accumulator lane is negated.

Returns
  Result of operation

## ◆ mul_4x2_2x8_conf() [2/8]

v32acc32 mul_4x2_2x8_conf | ( | v32int16 | a,
|  | int | sgn_x,
|  | v32uint16 | b,
|  | int | sgn_y,
|  | int | sub_mul )

Parameters

  a | Matrix A
  sgn_x | Sign mask for matrix A
  b | Matrix B
  sgn_y | Sign mask for matrix B
  sub_mul | Negation mask of multiplication result. If a bit is set the corresponding output accumulator lane is negated.

Returns
  Result of operation

## ◆ mul_4x2_2x8_conf() [3/8]

v32acc32 mul_4x2_2x8_conf | ( | v32int16 | a,
|  | v32int16 | b,
|  | int | sub_mul )

Parameters

  a | Matrix A
  b | Matrix B
  sub_mul | Negation mask for multiplication result

Returns
  Result of operation

## ◆ mul_4x2_2x8_conf() [4/8]

v32acc32 mul_4x2_2x8_conf | ( | v32int16 | a,
|  | v32uint16 | b,
|  | int | sub_mul )

Parameters

  a | Matrix A
  b | Matrix B
  sub_mul | Negation mask for multiplication result

Returns
  Result of operation

## ◆ mul_4x2_2x8_conf() [5/8]

v32acc32 mul_4x2_2x8_conf | ( | v32uint16 | a,
|  | int | sgn_x,
|  | v32int16 | b,
|  | int | sgn_y,
|  | int | sub_mul )

Parameters

  a | Matrix A
  sgn_x | Sign mask for matrix A
  b | Matrix B
  sgn_y | Sign mask for matrix B
  sub_mul | Negation mask of multiplication result. If a bit is set the corresponding output accumulator lane is negated.

Returns
  Result of operation

## ◆ mul_4x2_2x8_conf() [6/8]

v32acc32 mul_4x2_2x8_conf | ( | v32uint16 | a,
|  | int | sgn_x,
|  | v32uint16 | b,
|  | int | sgn_y,
|  | int | sub_mul )

Parameters

  a | Matrix A
  sgn_x | Sign mask for matrix A
  b | Matrix B
  sgn_y | Sign mask for matrix B
  sub_mul | Negation mask of multiplication result. If a bit is set the corresponding output accumulator lane is negated.

Returns
  Result of operation

## ◆ mul_4x2_2x8_conf() [7/8]

v32acc32 mul_4x2_2x8_conf | ( | v32uint16 | a,
|  | v32int16 | b,
|  | int | sub_mul )

Parameters

  a | Matrix A
  b | Matrix B
  sub_mul | Negation mask for multiplication result

Returns
  Result of operation

## ◆ mul_4x2_2x8_conf() [8/8]

v32acc32 mul_4x2_2x8_conf | ( | v32uint16 | a,
|  | v32uint16 | b,
|  | int | sub_mul )

Parameters

  a | Matrix A
  b | Matrix B
  sub_mul | Negation mask for multiplication result

Returns
  Result of operation

## ◆ mul_4x4_4x4() [1/8]

v16acc64 mul_4x4_4x4 | ( | v32int16 | a,
|  | int | sgn_x,
|  | v32int16 | b,
|  | int | sgn_y )

Parameters

  a | Matrix A
  sgn_x | Sign mask for matrix A
  b | Matrix B
  sgn_y | Sign mask for matrix B

Returns
  Result of operation

## ◆ mul_4x4_4x4() [2/8]

v16acc64 mul_4x4_4x4 | ( | v32int16 | a,
|  | int | sgn_x,
|  | v32uint16 | b,
|  | int | sgn_y )

Parameters

  a | Matrix A
  sgn_x | Sign mask for matrix A
  b | Matrix B
  sgn_y | Sign mask for matrix B

Returns
  Result of operation

## ◆ mul_4x4_4x4() [3/8]

v16acc64 mul_4x4_4x4 | ( | v32int16 | a,
|  | v32int16 | b )

Parameters

  a | Matrix A
  b | Matrix B

Returns
  Result of operation

## ◆ mul_4x4_4x4() [4/8]

v16acc64 mul_4x4_4x4 | ( | v32int16 | a,
|  | v32uint16 | b )

Parameters

  a | Matrix A
  b | Matrix B

Returns
  Result of operation

## ◆ mul_4x4_4x4() [5/8]

v16acc64 mul_4x4_4x4 | ( | v32uint16 | a,
|  | int | sgn_x,
|  | v32int16 | b,
|  | int | sgn_y )

Parameters

  a | Matrix A
  sgn_x | Sign mask for matrix A
  b | Matrix B
  sgn_y | Sign mask for matrix B

Returns
  Result of operation

## ◆ mul_4x4_4x4() [6/8]

v16acc64 mul_4x4_4x4 | ( | v32uint16 | a,
|  | int | sgn_x,
|  | v32uint16 | b,
|  | int | sgn_y )

Parameters

  a | Matrix A
  sgn_x | Sign mask for matrix A
  b | Matrix B
  sgn_y | Sign mask for matrix B

Returns
  Result of operation

## ◆ mul_4x4_4x4() [7/8]

v16acc64 mul_4x4_4x4 | ( | v32uint16 | a,
|  | v32int16 | b )

Parameters

  a | Matrix A
  b | Matrix B

Returns
  Result of operation

## ◆ mul_4x4_4x4() [8/8]

v16acc64 mul_4x4_4x4 | ( | v32uint16 | a,
|  | v32uint16 | b )

Parameters

  a | Matrix A
  b | Matrix B

Returns
  Result of operation

## ◆ mul_4x4_4x4_conf() [1/8]

v16acc64 mul_4x4_4x4_conf | ( | v32int16 | a,
|  | int | sgn_x,
|  | v32int16 | b,
|  | int | sgn_y,
|  | int | sub_mul )

Parameters

  a | Matrix A
  sgn_x | Sign mask for matrix A
  b | Matrix B
  sgn_y | Sign mask for matrix B
  sub_mul | Negation mask of multiplication result. If a bit is set the corresponding output accumulator lane is negated.

Returns
  Result of operation

## ◆ mul_4x4_4x4_conf() [2/8]

v16acc64 mul_4x4_4x4_conf | ( | v32int16 | a,
|  | int | sgn_x,
|  | v32uint16 | b,
|  | int | sgn_y,
|  | int | sub_mul )

Parameters

  a | Matrix A
  sgn_x | Sign mask for matrix A
  b | Matrix B
  sgn_y | Sign mask for matrix B
  sub_mul | Negation mask of multiplication result. If a bit is set the corresponding output accumulator lane is negated.

Returns
  Result of operation

## ◆ mul_4x4_4x4_conf() [3/8]

v16acc64 mul_4x4_4x4_conf | ( | v32int16 | a,
|  | v32int16 | b,
|  | int | sub_mul )

Parameters

  a | Matrix A
  b | Matrix B
  sub_mul | Negation mask for multiplication result

Returns
  Result of operation

## ◆ mul_4x4_4x4_conf() [4/8]

v16acc64 mul_4x4_4x4_conf | ( | v32int16 | a,
|  | v32uint16 | b,
|  | int | sub_mul )

Parameters

  a | Matrix A
  b | Matrix B
  sub_mul | Negation mask for multiplication result

Returns
  Result of operation

## ◆ mul_4x4_4x4_conf() [5/8]

v16acc64 mul_4x4_4x4_conf | ( | v32uint16 | a,
|  | int | sgn_x,
|  | v32int16 | b,
|  | int | sgn_y,
|  | int | sub_mul )

Parameters

  a | Matrix A
  sgn_x | Sign mask for matrix A
  b | Matrix B
  sgn_y | Sign mask for matrix B
  sub_mul | Negation mask of multiplication result. If a bit is set the corresponding output accumulator lane is negated.

Returns
  Result of operation

## ◆ mul_4x4_4x4_conf() [6/8]

v16acc64 mul_4x4_4x4_conf | ( | v32uint16 | a,
|  | int | sgn_x,
|  | v32uint16 | b,
|  | int | sgn_y,
|  | int | sub_mul )

Parameters

  a | Matrix A
  sgn_x | Sign mask for matrix A
  b | Matrix B
  sgn_y | Sign mask for matrix B
  sub_mul | Negation mask of multiplication result. If a bit is set the corresponding output accumulator lane is negated.

Returns
  Result of operation

## ◆ mul_4x4_4x4_conf() [7/8]

v16acc64 mul_4x4_4x4_conf | ( | v32uint16 | a,
|  | v32int16 | b,
|  | int | sub_mul )

Parameters

  a | Matrix A
  b | Matrix B
  sub_mul | Negation mask for multiplication result

Returns
  Result of operation

## ◆ mul_4x4_4x4_conf() [8/8]

v16acc64 mul_4x4_4x4_conf | ( | v32uint16 | a,
|  | v32uint16 | b,
|  | int | sub_mul )

Parameters

  a | Matrix A
  b | Matrix B
  sub_mul | Negation mask for multiplication result

Returns
  Result of operation

## ◆ mul_conv_16x4() [1/8]

v16acc64 mul_conv_16x4 | ( | v32int16 | a,
|  | int | sgn_x,
|  | v32int16 | b,
|  | int | sgn_y )

Parameters

  a | Matrix A
  sgn_x | Sign mask for matrix A
  b | Matrix B
  sgn_y | Sign mask for matrix B

Returns
  Result of operation

## ◆ mul_conv_16x4() [2/8]

v16acc64 mul_conv_16x4 | ( | v32int16 | a,
|  | int | sgn_x,
|  | v32uint16 | b,
|  | int | sgn_y )

Parameters

  a | Matrix A
  sgn_x | Sign mask for matrix A
  b | Matrix B
  sgn_y | Sign mask for matrix B

Returns
  Result of operation

## ◆ mul_conv_16x4() [3/8]

v16acc64 mul_conv_16x4 | ( | v32int16 | a,
|  | v32int16 | b )

Parameters

  a | Matrix A
  b | Matrix B

Returns
  Result of operation

## ◆ mul_conv_16x4() [4/8]

v16acc64 mul_conv_16x4 | ( | v32int16 | a,
|  | v32uint16 | b )

Parameters

  a | Matrix A
  b | Matrix B

Returns
  Result of operation

## ◆ mul_conv_16x4() [5/8]

v16acc64 mul_conv_16x4 | ( | v32uint16 | a,
|  | int | sgn_x,
|  | v32int16 | b,
|  | int | sgn_y )

Parameters

  a | Matrix A
  sgn_x | Sign mask for matrix A
  b | Matrix B
  sgn_y | Sign mask for matrix B

Returns
  Result of operation

## ◆ mul_conv_16x4() [6/8]

v16acc64 mul_conv_16x4 | ( | v32uint16 | a,
|  | int | sgn_x,
|  | v32uint16 | b,
|  | int | sgn_y )

Parameters

  a | Matrix A
  sgn_x | Sign mask for matrix A
  b | Matrix B
  sgn_y | Sign mask for matrix B

Returns
  Result of operation

## ◆ mul_conv_16x4() [7/8]

v16acc64 mul_conv_16x4 | ( | v32uint16 | a,
|  | v32int16 | b )

Parameters

  a | Matrix A
  b | Matrix B

Returns
  Result of operation

## ◆ mul_conv_16x4() [8/8]

v16acc64 mul_conv_16x4 | ( | v32uint16 | a,
|  | v32uint16 | b )

Parameters

  a | Matrix A
  b | Matrix B

Returns
  Result of operation

## ◆ mul_conv_16x4_conf() [1/8]

v16acc64 mul_conv_16x4_conf | ( | v32int16 | a,
|  | int | sgn_x,
|  | v32int16 | b,
|  | int | sgn_y,
|  | int | sub_mul )

Parameters

  a | Matrix A
  sgn_x | Sign mask for matrix A
  b | Matrix B
  sgn_y | Sign mask for matrix B
  sub_mul | Negation mask of multiplication result. If a bit is set the corresponding output accumulator lane is negated.

Returns
  Result of operation

## ◆ mul_conv_16x4_conf() [2/8]

v16acc64 mul_conv_16x4_conf | ( | v32int16 | a,
|  | int | sgn_x,
|  | v32uint16 | b,
|  | int | sgn_y,
|  | int | sub_mul )

Parameters

  a | Matrix A
  sgn_x | Sign mask for matrix A
  b | Matrix B
  sgn_y | Sign mask for matrix B
  sub_mul | Negation mask of multiplication result. If a bit is set the corresponding output accumulator lane is negated.

Returns
  Result of operation

## ◆ mul_conv_16x4_conf() [3/8]

v16acc64 mul_conv_16x4_conf | ( | v32int16 | a,
|  | v32int16 | b,
|  | int | sub_mul )

Parameters

  a | Matrix A
  b | Matrix B
  sub_mul | Negation mask for multiplication result

Returns
  Result of operation

## ◆ mul_conv_16x4_conf() [4/8]

v16acc64 mul_conv_16x4_conf | ( | v32int16 | a,
|  | v32uint16 | b,
|  | int | sub_mul )

Parameters

  a | Matrix A
  b | Matrix B
  sub_mul | Negation mask for multiplication result

Returns
  Result of operation

## ◆ mul_conv_16x4_conf() [5/8]

v16acc64 mul_conv_16x4_conf | ( | v32uint16 | a,
|  | int | sgn_x,
|  | v32int16 | b,
|  | int | sgn_y,
|  | int | sub_mul )

Parameters

  a | Matrix A
  sgn_x | Sign mask for matrix A
  b | Matrix B
  sgn_y | Sign mask for matrix B
  sub_mul | Negation mask of multiplication result. If a bit is set the corresponding output accumulator lane is negated.

Returns
  Result of operation

## ◆ mul_conv_16x4_conf() [6/8]

v16acc64 mul_conv_16x4_conf | ( | v32uint16 | a,
|  | int | sgn_x,
|  | v32uint16 | b,
|  | int | sgn_y,
|  | int | sub_mul )

Parameters

  a | Matrix A
  sgn_x | Sign mask for matrix A
  b | Matrix B
  sgn_y | Sign mask for matrix B
  sub_mul | Negation mask of multiplication result. If a bit is set the corresponding output accumulator lane is negated.

Returns
  Result of operation

## ◆ mul_conv_16x4_conf() [7/8]

v16acc64 mul_conv_16x4_conf | ( | v32uint16 | a,
|  | v32int16 | b,
|  | int | sub_mul )

Parameters

  a | Matrix A
  b | Matrix B
  sub_mul | Negation mask for multiplication result

Returns
  Result of operation

## ◆ mul_conv_16x4_conf() [8/8]

v16acc64 mul_conv_16x4_conf | ( | v32uint16 | a,
|  | v32uint16 | b,
|  | int | sub_mul )

Parameters

  a | Matrix A
  b | Matrix B
  sub_mul | Negation mask for multiplication result

Returns
  Result of operation

## ◆ mul_elem_16_2() [1/9]

v16accfloat mul_elem_16_2 | ( | v32bfloat16 | a,
|  | v32bfloat16 | b )

Parameters

  a | Matrix A
  b | Matrix B

Returns
  Result of operation

## ◆ mul_elem_16_2() [2/9]

v16acc64 mul_elem_16_2 | ( | v32int16 | a,
|  | int | sgn_x,
|  | v32int16 | b,
|  | int | sgn_y )

Parameters

  a | Matrix A
  sgn_x | Sign mask for matrix A
  b | Matrix B
  sgn_y | Sign mask for matrix B

Returns
  Result of operation

## ◆ mul_elem_16_2() [3/9]

v16acc64 mul_elem_16_2 | ( | v32int16 | a,
|  | int | sgn_x,
|  | v32uint16 | b,
|  | int | sgn_y )

Parameters

  a | Matrix A
  sgn_x | Sign mask for matrix A
  b | Matrix B
  sgn_y | Sign mask for matrix B

Returns
  Result of operation

## ◆ mul_elem_16_2() [4/9]

v16acc64 mul_elem_16_2 | ( | v32int16 | a,
|  | v32int16 | b )

Parameters

  a | Matrix A
  b | Matrix B

Returns
  Result of operation

## ◆ mul_elem_16_2() [5/9]

v16acc64 mul_elem_16_2 | ( | v32int16 | a,
|  | v32uint16 | b )

Parameters

  a | Matrix A
  b | Matrix B

Returns
  Result of operation

## ◆ mul_elem_16_2() [6/9]

v16acc64 mul_elem_16_2 | ( | v32uint16 | a,
|  | int | sgn_x,
|  | v32int16 | b,
|  | int | sgn_y )

Parameters

  a | Matrix A
  sgn_x | Sign mask for matrix A
  b | Matrix B
  sgn_y | Sign mask for matrix B

Returns
  Result of operation

## ◆ mul_elem_16_2() [7/9]

v16acc64 mul_elem_16_2 | ( | v32uint16 | a,
|  | int | sgn_x,
|  | v32uint16 | b,
|  | int | sgn_y )

Parameters

  a | Matrix A
  sgn_x | Sign mask for matrix A
  b | Matrix B
  sgn_y | Sign mask for matrix B

Returns
  Result of operation

## ◆ mul_elem_16_2() [8/9]

v16acc64 mul_elem_16_2 | ( | v32uint16 | a,
|  | v32int16 | b )

Parameters

  a | Matrix A
  b | Matrix B

Returns
  Result of operation

## ◆ mul_elem_16_2() [9/9]

v16acc64 mul_elem_16_2 | ( | v32uint16 | a,
|  | v32uint16 | b )

Parameters

  a | Matrix A
  b | Matrix B

Returns
  Result of operation

## ◆ mul_elem_16_2_conf() [1/9]

v16accfloat mul_elem_16_2_conf | ( | v32bfloat16 | a,
|  | v32bfloat16 | b,
|  | int | sub_mul )

Parameters

  a | Matrix A
  b | Matrix B
  sub_mul | Negation mask for multiplication result

Returns
  Result of operation

## ◆ mul_elem_16_2_conf() [2/9]

v16acc64 mul_elem_16_2_conf | ( | v32int16 | a,
|  | int | sgn_x,
|  | v32int16 | b,
|  | int | sgn_y,
|  | int | sub_mul )

Parameters

  a | Matrix A
  sgn_x | Sign mask for matrix A
  b | Matrix B
  sgn_y | Sign mask for matrix B
  sub_mul | Negation mask of multiplication result. If a bit is set the corresponding output accumulator lane is negated.

Returns
  Result of operation

## ◆ mul_elem_16_2_conf() [3/9]

v16acc64 mul_elem_16_2_conf | ( | v32int16 | a,
|  | int | sgn_x,
|  | v32uint16 | b,
|  | int | sgn_y,
|  | int | sub_mul )

Parameters

  a | Matrix A
  sgn_x | Sign mask for matrix A
  b | Matrix B
  sgn_y | Sign mask for matrix B
  sub_mul | Negation mask of multiplication result. If a bit is set the corresponding output accumulator lane is negated.

Returns
  Result of operation

## ◆ mul_elem_16_2_conf() [4/9]

v16acc64 mul_elem_16_2_conf | ( | v32int16 | a,
|  | v32int16 | b,
|  | int | sub_mul )

Parameters

  a | Matrix A
  b | Matrix B
  sub_mul | Negation mask for multiplication result

Returns
  Result of operation

## ◆ mul_elem_16_2_conf() [5/9]

v16acc64 mul_elem_16_2_conf | ( | v32int16 | a,
|  | v32uint16 | b,
|  | int | sub_mul )

Parameters

  a | Matrix A
  b | Matrix B
  sub_mul | Negation mask for multiplication result

Returns
  Result of operation

## ◆ mul_elem_16_2_conf() [6/9]

v16acc64 mul_elem_16_2_conf | ( | v32uint16 | a,
|  | int | sgn_x,
|  | v32int16 | b,
|  | int | sgn_y,
|  | int | sub_mul )

Parameters

  a | Matrix A
  sgn_x | Sign mask for matrix A
  b | Matrix B
  sgn_y | Sign mask for matrix B
  sub_mul | Negation mask of multiplication result. If a bit is set the corresponding output accumulator lane is negated.

Returns
  Result of operation

## ◆ mul_elem_16_2_conf() [7/9]

v16acc64 mul_elem_16_2_conf | ( | v32uint16 | a,
|  | int | sgn_x,
|  | v32uint16 | b,
|  | int | sgn_y,
|  | int | sub_mul )

Parameters

  a | Matrix A
  sgn_x | Sign mask for matrix A
  b | Matrix B
  sgn_y | Sign mask for matrix B
  sub_mul | Negation mask of multiplication result. If a bit is set the corresponding output accumulator lane is negated.

Returns
  Result of operation

## ◆ mul_elem_16_2_conf() [8/9]

v16acc64 mul_elem_16_2_conf | ( | v32uint16 | a,
|  | v32int16 | b,
|  | int | sub_mul )

Parameters

  a | Matrix A
  b | Matrix B
  sub_mul | Negation mask for multiplication result

Returns
  Result of operation

## ◆ mul_elem_16_2_conf() [9/9]

v16acc64 mul_elem_16_2_conf | ( | v32uint16 | a,
|  | v32uint16 | b,
|  | int | sub_mul )

Parameters

  a | Matrix A
  b | Matrix B
  sub_mul | Negation mask for multiplication result

Returns
  Result of operation

## ◆ mul_elem_32() [1/8]

v32acc32 mul_elem_32 | ( | v32int16 | a,
|  | int | sgn_x,
|  | v32int16 | b,
|  | int | sgn_y )

Parameters

  a | Matrix A
  sgn_x | Sign mask for matrix A
  b | Matrix B
  sgn_y | Sign mask for matrix B

Returns
  Result of operation

## ◆ mul_elem_32() [2/8]

v32acc32 mul_elem_32 | ( | v32int16 | a,
|  | int | sgn_x,
|  | v32uint16 | b,
|  | int | sgn_y )

Parameters

  a | Matrix A
  sgn_x | Sign mask for matrix A
  b | Matrix B
  sgn_y | Sign mask for matrix B

Returns
  Result of operation

## ◆ mul_elem_32() [3/8]

v32acc32 mul_elem_32 | ( | v32int16 | a,
|  | v32int16 | b )

Parameters

  a | Matrix A
  b | Matrix B

Returns
  Result of operation

## ◆ mul_elem_32() [4/8]

v32acc32 mul_elem_32 | ( | v32int16 | a,
|  | v32uint16 | b )

Parameters

  a | Matrix A
  b | Matrix B

Returns
  Result of operation

## ◆ mul_elem_32() [5/8]

v32acc32 mul_elem_32 | ( | v32uint16 | a,
|  | int | sgn_x,
|  | v32int16 | b,
|  | int | sgn_y )

Parameters

  a | Matrix A
  sgn_x | Sign mask for matrix A
  b | Matrix B
  sgn_y | Sign mask for matrix B

Returns
  Result of operation

## ◆ mul_elem_32() [6/8]

v32acc32 mul_elem_32 | ( | v32uint16 | a,
|  | int | sgn_x,
|  | v32uint16 | b,
|  | int | sgn_y )

Parameters

  a | Matrix A
  sgn_x | Sign mask for matrix A
  b | Matrix B
  sgn_y | Sign mask for matrix B

Returns
  Result of operation

## ◆ mul_elem_32() [7/8]

v32acc32 mul_elem_32 | ( | v32uint16 | a,
|  | v32int16 | b )

Parameters

  a | Matrix A
  b | Matrix B

Returns
  Result of operation

## ◆ mul_elem_32() [8/8]

v32acc32 mul_elem_32 | ( | v32uint16 | a,
|  | v32uint16 | b )

Parameters

  a | Matrix A
  b | Matrix B

Returns
  Result of operation

## ◆ mul_elem_32_conf() [1/8]

v32acc32 mul_elem_32_conf | ( | v32int16 | a,
|  | int | sgn_x,
|  | v32int16 | b,
|  | int | sgn_y,
|  | int | sub_mul )

Parameters

  a | Matrix A
  sgn_x | Sign mask for matrix A
  b | Matrix B
  sgn_y | Sign mask for matrix B
  sub_mul | Negation mask of multiplication result. If a bit is set the corresponding output accumulator lane is negated.

Returns
  Result of operation

## ◆ mul_elem_32_conf() [2/8]

v32acc32 mul_elem_32_conf | ( | v32int16 | a,
|  | int | sgn_x,
|  | v32uint16 | b,
|  | int | sgn_y,
|  | int | sub_mul )

Parameters

  a | Matrix A
  sgn_x | Sign mask for matrix A
  b | Matrix B
  sgn_y | Sign mask for matrix B
  sub_mul | Negation mask of multiplication result. If a bit is set the corresponding output accumulator lane is negated.

Returns
  Result of operation

## ◆ mul_elem_32_conf() [3/8]

v32acc32 mul_elem_32_conf | ( | v32int16 | a,
|  | v32int16 | b,
|  | int | sub_mul )

Parameters

  a | Matrix A
  b | Matrix B
  sub_mul | Negation mask for multiplication result

Returns
  Result of operation

## ◆ mul_elem_32_conf() [4/8]

v32acc32 mul_elem_32_conf | ( | v32int16 | a,
|  | v32uint16 | b,
|  | int | sub_mul )

Parameters

  a | Matrix A
  b | Matrix B
  sub_mul | Negation mask for multiplication result

Returns
  Result of operation

## ◆ mul_elem_32_conf() [5/8]

v32acc32 mul_elem_32_conf | ( | v32uint16 | a,
|  | int | sgn_x,
|  | v32int16 | b,
|  | int | sgn_y,
|  | int | sub_mul )

Parameters

  a | Matrix A
  sgn_x | Sign mask for matrix A
  b | Matrix B
  sgn_y | Sign mask for matrix B
  sub_mul | Negation mask of multiplication result. If a bit is set the corresponding output accumulator lane is negated.

Returns
  Result of operation

## ◆ mul_elem_32_conf() [6/8]

v32acc32 mul_elem_32_conf | ( | v32uint16 | a,
|  | int | sgn_x,
|  | v32uint16 | b,
|  | int | sgn_y,
|  | int | sub_mul )

Parameters

  a | Matrix A
  sgn_x | Sign mask for matrix A
  b | Matrix B
  sgn_y | Sign mask for matrix B
  sub_mul | Negation mask of multiplication result. If a bit is set the corresponding output accumulator lane is negated.

Returns
  Result of operation

## ◆ mul_elem_32_conf() [7/8]

v32acc32 mul_elem_32_conf | ( | v32uint16 | a,
|  | v32int16 | b,
|  | int | sub_mul )

Parameters

  a | Matrix A
  b | Matrix B
  sub_mul | Negation mask for multiplication result

Returns
  Result of operation

## ◆ mul_elem_32_conf() [8/8]

v32acc32 mul_elem_32_conf | ( | v32uint16 | a,
|  | v32uint16 | b,
|  | int | sub_mul )

Parameters

  a | Matrix A
  b | Matrix B
  sub_mul | Negation mask for multiplication result

Returns
  Result of operation

## ◆ negmac_2x4_4x8() [1/8]

v16acc64 negmac_2x4_4x8 | ( | v32int16 | a,
|  | int | sgn_x,
|  | v32int16 | b,
|  | int | sgn_y,
|  | v16acc64 | acc1 )

Parameters

  a | Matrix A
  sgn_x | Sign mask for matrix A
  b | Matrix B
  sgn_y | Sign mask for matrix B
  acc1 | Accumulator 1 input

Returns
  Result of operation

## ◆ negmac_2x4_4x8() [2/8]

v16acc64 negmac_2x4_4x8 | ( | v32int16 | a,
|  | int | sgn_x,
|  | v32uint16 | b,
|  | int | sgn_y,
|  | v16acc64 | acc1 )

Parameters

  a | Matrix A
  sgn_x | Sign mask for matrix A
  b | Matrix B
  sgn_y | Sign mask for matrix B
  acc1 | Accumulator 1 input

Returns
  Result of operation

## ◆ negmac_2x4_4x8() [3/8]

v16acc64 negmac_2x4_4x8 | ( | v32int16 | a,
|  | v32int16 | b,
|  | v16acc64 | acc1 )

Parameters

  a | Matrix A
  b | Matrix B
  acc1 | Accumulator 1 input

Returns
  Result of MAC operation

## ◆ negmac_2x4_4x8() [4/8]

v16acc64 negmac_2x4_4x8 | ( | v32int16 | a,
|  | v32uint16 | b,
|  | v16acc64 | acc1 )

Parameters

  a | Matrix A
  b | Matrix B
  acc1 | Accumulator 1 input

Returns
  Result of MAC operation

## ◆ negmac_2x4_4x8() [5/8]

v16acc64 negmac_2x4_4x8 | ( | v32uint16 | a,
|  | int | sgn_x,
|  | v32int16 | b,
|  | int | sgn_y,
|  | v16acc64 | acc1 )

Parameters

  a | Matrix A
  sgn_x | Sign mask for matrix A
  b | Matrix B
  sgn_y | Sign mask for matrix B
  acc1 | Accumulator 1 input

Returns
  Result of operation

## ◆ negmac_2x4_4x8() [6/8]

v16acc64 negmac_2x4_4x8 | ( | v32uint16 | a,
|  | int | sgn_x,
|  | v32uint16 | b,
|  | int | sgn_y,
|  | v16acc64 | acc1 )

Parameters

  a | Matrix A
  sgn_x | Sign mask for matrix A
  b | Matrix B
  sgn_y | Sign mask for matrix B
  acc1 | Accumulator 1 input

Returns
  Result of operation

## ◆ negmac_2x4_4x8() [7/8]

v16acc64 negmac_2x4_4x8 | ( | v32uint16 | a,
|  | v32int16 | b,
|  | v16acc64 | acc1 )

Parameters

  a | Matrix A
  b | Matrix B
  acc1 | Accumulator 1 input

Returns
  Result of MAC operation

## ◆ negmac_2x4_4x8() [8/8]

v16acc64 negmac_2x4_4x8 | ( | v32uint16 | a,
|  | v32uint16 | b,
|  | v16acc64 | acc1 )

Parameters

  a | Matrix A
  b | Matrix B
  acc1 | Accumulator 1 input

Returns
  Result of MAC operation

## ◆ negmac_2x4_4x8_conf() [1/8]

v16acc64 negmac_2x4_4x8_conf | ( | v32int16 | a,
|  | int | sgn_x,
|  | v32int16 | b,
|  | int | sgn_y,
|  | v16acc64 | acc1,
|  | int | zero_acc1,
|  | int | sub_mul,
|  | int | sub_acc1 )

Parameters

  a | Matrix A
  sgn_x | Sign mask for matrix A
  b | Matrix B
  sgn_y | Sign mask for matrix B
  acc1 | Accumulator 1 input
  zero_acc1 | Zeroing mask for acc1
  sub_mul | Negation mask of multiplication result
  sub_acc1 | Negation mask of acc1

Returns
  Result of operation

## ◆ negmac_2x4_4x8_conf() [2/8]

v16acc64 negmac_2x4_4x8_conf | ( | v32int16 | a,
|  | int | sgn_x,
|  | v32uint16 | b,
|  | int | sgn_y,
|  | v16acc64 | acc1,
|  | int | zero_acc1,
|  | int | sub_mul,
|  | int | sub_acc1 )

Parameters

  a | Matrix A
  sgn_x | Sign mask for matrix A
  b | Matrix B
  sgn_y | Sign mask for matrix B
  acc1 | Accumulator 1 input
  zero_acc1 | Zeroing mask for acc1
  sub_mul | Negation mask of multiplication result
  sub_acc1 | Negation mask of acc1

Returns
  Result of operation

## ◆ negmac_2x4_4x8_conf() [3/8]

v16acc64 negmac_2x4_4x8_conf | ( | v32int16 | a,
|  | v32int16 | b,
|  | v16acc64 | acc1,
|  | int | zero_acc1,
|  | int | sub_mul,
|  | int | sub_acc1 )

Parameters

  a | Matrix A
  b | Matrix B
  acc1 | Accumulator 1 input
  zero_acc1 | Zeroing mask for acc1
  sub_mul | Negation mask of multiplication result
  sub_acc1 | Negation mask of acc1

Returns
  Result of operation

## ◆ negmac_2x4_4x8_conf() [4/8]

v16acc64 negmac_2x4_4x8_conf | ( | v32int16 | a,
|  | v32uint16 | b,
|  | v16acc64 | acc1,
|  | int | zero_acc1,
|  | int | sub_mul,
|  | int | sub_acc1 )

Parameters

  a | Matrix A
  b | Matrix B
  acc1 | Accumulator 1 input
  zero_acc1 | Zeroing mask for acc1
  sub_mul | Negation mask of multiplication result
  sub_acc1 | Negation mask of acc1

Returns
  Result of operation

## ◆ negmac_2x4_4x8_conf() [5/8]

v16acc64 negmac_2x4_4x8_conf | ( | v32uint16 | a,
|  | int | sgn_x,
|  | v32int16 | b,
|  | int | sgn_y,
|  | v16acc64 | acc1,
|  | int | zero_acc1,
|  | int | sub_mul,
|  | int | sub_acc1 )

Parameters

  a | Matrix A
  sgn_x | Sign mask for matrix A
  b | Matrix B
  sgn_y | Sign mask for matrix B
  acc1 | Accumulator 1 input
  zero_acc1 | Zeroing mask for acc1
  sub_mul | Negation mask of multiplication result
  sub_acc1 | Negation mask of acc1

Returns
  Result of operation

## ◆ negmac_2x4_4x8_conf() [6/8]

v16acc64 negmac_2x4_4x8_conf | ( | v32uint16 | a,
|  | int | sgn_x,
|  | v32uint16 | b,
|  | int | sgn_y,
|  | v16acc64 | acc1,
|  | int | zero_acc1,
|  | int | sub_mul,
|  | int | sub_acc1 )

Parameters

  a | Matrix A
  sgn_x | Sign mask for matrix A
  b | Matrix B
  sgn_y | Sign mask for matrix B
  acc1 | Accumulator 1 input
  zero_acc1 | Zeroing mask for acc1
  sub_mul | Negation mask of multiplication result
  sub_acc1 | Negation mask of acc1

Returns
  Result of operation

## ◆ negmac_2x4_4x8_conf() [7/8]

v16acc64 negmac_2x4_4x8_conf | ( | v32uint16 | a,
|  | v32int16 | b,
|  | v16acc64 | acc1,
|  | int | zero_acc1,
|  | int | sub_mul,
|  | int | sub_acc1 )

Parameters

  a | Matrix A
  b | Matrix B
  acc1 | Accumulator 1 input
  zero_acc1 | Zeroing mask for acc1
  sub_mul | Negation mask of multiplication result
  sub_acc1 | Negation mask of acc1

Returns
  Result of operation

## ◆ negmac_2x4_4x8_conf() [8/8]

v16acc64 negmac_2x4_4x8_conf | ( | v32uint16 | a,
|  | v32uint16 | b,
|  | v16acc64 | acc1,
|  | int | zero_acc1,
|  | int | sub_mul,
|  | int | sub_acc1 )

Parameters

  a | Matrix A
  b | Matrix B
  acc1 | Accumulator 1 input
  zero_acc1 | Zeroing mask for acc1
  sub_mul | Negation mask of multiplication result
  sub_acc1 | Negation mask of acc1

Returns
  Result of operation

## ◆ negmac_4x2_2x8() [1/8]

v32acc32 negmac_4x2_2x8 | ( | v32int16 | a,
|  | int | sgn_x,
|  | v32int16 | b,
|  | int | sgn_y,
|  | v32acc32 | acc1 )

Parameters

  a | Matrix A
  sgn_x | Sign mask for matrix A
  b | Matrix B
  sgn_y | Sign mask for matrix B
  acc1 | Accumulator 1 input

Returns
  Result of operation

## ◆ negmac_4x2_2x8() [2/8]

v32acc32 negmac_4x2_2x8 | ( | v32int16 | a,
|  | int | sgn_x,
|  | v32uint16 | b,
|  | int | sgn_y,
|  | v32acc32 | acc1 )

Parameters

  a | Matrix A
  sgn_x | Sign mask for matrix A
  b | Matrix B
  sgn_y | Sign mask for matrix B
  acc1 | Accumulator 1 input

Returns
  Result of operation

## ◆ negmac_4x2_2x8() [3/8]

v32acc32 negmac_4x2_2x8 | ( | v32int16 | a,
|  | v32int16 | b,
|  | v32acc32 | acc1 )

Parameters

  a | Matrix A
  b | Matrix B
  acc1 | Accumulator 1 input

Returns
  Result of MAC operation

## ◆ negmac_4x2_2x8() [4/8]

v32acc32 negmac_4x2_2x8 | ( | v32int16 | a,
|  | v32uint16 | b,
|  | v32acc32 | acc1 )

Parameters

  a | Matrix A
  b | Matrix B
  acc1 | Accumulator 1 input

Returns
  Result of MAC operation

## ◆ negmac_4x2_2x8() [5/8]

v32acc32 negmac_4x2_2x8 | ( | v32uint16 | a,
|  | int | sgn_x,
|  | v32int16 | b,
|  | int | sgn_y,
|  | v32acc32 | acc1 )

Parameters

  a | Matrix A
  sgn_x | Sign mask for matrix A
  b | Matrix B
  sgn_y | Sign mask for matrix B
  acc1 | Accumulator 1 input

Returns
  Result of operation

## ◆ negmac_4x2_2x8() [6/8]

v32acc32 negmac_4x2_2x8 | ( | v32uint16 | a,
|  | int | sgn_x,
|  | v32uint16 | b,
|  | int | sgn_y,
|  | v32acc32 | acc1 )

Parameters

  a | Matrix A
  sgn_x | Sign mask for matrix A
  b | Matrix B
  sgn_y | Sign mask for matrix B
  acc1 | Accumulator 1 input

Returns
  Result of operation

## ◆ negmac_4x2_2x8() [7/8]

v32acc32 negmac_4x2_2x8 | ( | v32uint16 | a,
|  | v32int16 | b,
|  | v32acc32 | acc1 )

Parameters

  a | Matrix A
  b | Matrix B
  acc1 | Accumulator 1 input

Returns
  Result of MAC operation

## ◆ negmac_4x2_2x8() [8/8]

v32acc32 negmac_4x2_2x8 | ( | v32uint16 | a,
|  | v32uint16 | b,
|  | v32acc32 | acc1 )

Parameters

  a | Matrix A
  b | Matrix B
  acc1 | Accumulator 1 input

Returns
  Result of MAC operation

## ◆ negmac_4x2_2x8_conf() [1/8]

v32acc32 negmac_4x2_2x8_conf | ( | v32int16 | a,
|  | int | sgn_x,
|  | v32int16 | b,
|  | int | sgn_y,
|  | v32acc32 | acc1,
|  | int | zero_acc1,
|  | int | sub_mul,
|  | int | sub_acc1 )

Parameters

  a | Matrix A
  sgn_x | Sign mask for matrix A
  b | Matrix B
  sgn_y | Sign mask for matrix B
  acc1 | Accumulator 1 input
  zero_acc1 | Zeroing mask for acc1
  sub_mul | Negation mask of multiplication result
  sub_acc1 | Negation mask of acc1

Returns
  Result of operation

## ◆ negmac_4x2_2x8_conf() [2/8]

v32acc32 negmac_4x2_2x8_conf | ( | v32int16 | a,
|  | int | sgn_x,
|  | v32uint16 | b,
|  | int | sgn_y,
|  | v32acc32 | acc1,
|  | int | zero_acc1,
|  | int | sub_mul,
|  | int | sub_acc1 )

Parameters

  a | Matrix A
  sgn_x | Sign mask for matrix A
  b | Matrix B
  sgn_y | Sign mask for matrix B
  acc1 | Accumulator 1 input
  zero_acc1 | Zeroing mask for acc1
  sub_mul | Negation mask of multiplication result
  sub_acc1 | Negation mask of acc1

Returns
  Result of operation

## ◆ negmac_4x2_2x8_conf() [3/8]

v32acc32 negmac_4x2_2x8_conf | ( | v32int16 | a,
|  | v32int16 | b,
|  | v32acc32 | acc1,
|  | int | zero_acc1,
|  | int | sub_mul,
|  | int | sub_acc1 )

Parameters

  a | Matrix A
  b | Matrix B
  acc1 | Accumulator 1 input
  zero_acc1 | Zeroing mask for acc1
  sub_mul | Negation mask of multiplication result
  sub_acc1 | Negation mask of acc1

Returns
  Result of operation

## ◆ negmac_4x2_2x8_conf() [4/8]

v32acc32 negmac_4x2_2x8_conf | ( | v32int16 | a,
|  | v32uint16 | b,
|  | v32acc32 | acc1,
|  | int | zero_acc1,
|  | int | sub_mul,
|  | int | sub_acc1 )

Parameters

  a | Matrix A
  b | Matrix B
  acc1 | Accumulator 1 input
  zero_acc1 | Zeroing mask for acc1
  sub_mul | Negation mask of multiplication result
  sub_acc1 | Negation mask of acc1

Returns
  Result of operation

## ◆ negmac_4x2_2x8_conf() [5/8]

v32acc32 negmac_4x2_2x8_conf | ( | v32uint16 | a,
|  | int | sgn_x,
|  | v32int16 | b,
|  | int | sgn_y,
|  | v32acc32 | acc1,
|  | int | zero_acc1,
|  | int | sub_mul,
|  | int | sub_acc1 )

Parameters

  a | Matrix A
  sgn_x | Sign mask for matrix A
  b | Matrix B
  sgn_y | Sign mask for matrix B
  acc1 | Accumulator 1 input
  zero_acc1 | Zeroing mask for acc1
  sub_mul | Negation mask of multiplication result
  sub_acc1 | Negation mask of acc1

Returns
  Result of operation

## ◆ negmac_4x2_2x8_conf() [6/8]

v32acc32 negmac_4x2_2x8_conf | ( | v32uint16 | a,
|  | int | sgn_x,
|  | v32uint16 | b,
|  | int | sgn_y,
|  | v32acc32 | acc1,
|  | int | zero_acc1,
|  | int | sub_mul,
|  | int | sub_acc1 )

Parameters

  a | Matrix A
  sgn_x | Sign mask for matrix A
  b | Matrix B
  sgn_y | Sign mask for matrix B
  acc1 | Accumulator 1 input
  zero_acc1 | Zeroing mask for acc1
  sub_mul | Negation mask of multiplication result
  sub_acc1 | Negation mask of acc1

Returns
  Result of operation

## ◆ negmac_4x2_2x8_conf() [7/8]

v32acc32 negmac_4x2_2x8_conf | ( | v32uint16 | a,
|  | v32int16 | b,
|  | v32acc32 | acc1,
|  | int | zero_acc1,
|  | int | sub_mul,
|  | int | sub_acc1 )

Parameters

  a | Matrix A
  b | Matrix B
  acc1 | Accumulator 1 input
  zero_acc1 | Zeroing mask for acc1
  sub_mul | Negation mask of multiplication result
  sub_acc1 | Negation mask of acc1

Returns
  Result of operation

## ◆ negmac_4x2_2x8_conf() [8/8]

v32acc32 negmac_4x2_2x8_conf | ( | v32uint16 | a,
|  | v32uint16 | b,
|  | v32acc32 | acc1,
|  | int | zero_acc1,
|  | int | sub_mul,
|  | int | sub_acc1 )

Parameters

  a | Matrix A
  b | Matrix B
  acc1 | Accumulator 1 input
  zero_acc1 | Zeroing mask for acc1
  sub_mul | Negation mask of multiplication result
  sub_acc1 | Negation mask of acc1

Returns
  Result of operation

## ◆ negmac_4x4_4x4() [1/8]

v16acc64 negmac_4x4_4x4 | ( | v32int16 | a,
|  | int | sgn_x,
|  | v32int16 | b,
|  | int | sgn_y,
|  | v16acc64 | acc1 )

Parameters

  a | Matrix A
  sgn_x | Sign mask for matrix A
  b | Matrix B
  sgn_y | Sign mask for matrix B
  acc1 | Accumulator 1 input

Returns
  Result of operation

## ◆ negmac_4x4_4x4() [2/8]

v16acc64 negmac_4x4_4x4 | ( | v32int16 | a,
|  | int | sgn_x,
|  | v32uint16 | b,
|  | int | sgn_y,
|  | v16acc64 | acc1 )

Parameters

  a | Matrix A
  sgn_x | Sign mask for matrix A
  b | Matrix B
  sgn_y | Sign mask for matrix B
  acc1 | Accumulator 1 input

Returns
  Result of operation

## ◆ negmac_4x4_4x4() [3/8]

v16acc64 negmac_4x4_4x4 | ( | v32int16 | a,
|  | v32int16 | b,
|  | v16acc64 | acc1 )

Parameters

  a | Matrix A
  b | Matrix B
  acc1 | Accumulator 1 input

Returns
  Result of MAC operation

## ◆ negmac_4x4_4x4() [4/8]

v16acc64 negmac_4x4_4x4 | ( | v32int16 | a,
|  | v32uint16 | b,
|  | v16acc64 | acc1 )

Parameters

  a | Matrix A
  b | Matrix B
  acc1 | Accumulator 1 input

Returns
  Result of MAC operation

## ◆ negmac_4x4_4x4() [5/8]

v16acc64 negmac_4x4_4x4 | ( | v32uint16 | a,
|  | int | sgn_x,
|  | v32int16 | b,
|  | int | sgn_y,
|  | v16acc64 | acc1 )

Parameters

  a | Matrix A
  sgn_x | Sign mask for matrix A
  b | Matrix B
  sgn_y | Sign mask for matrix B
  acc1 | Accumulator 1 input

Returns
  Result of operation

## ◆ negmac_4x4_4x4() [6/8]

v16acc64 negmac_4x4_4x4 | ( | v32uint16 | a,
|  | int | sgn_x,
|  | v32uint16 | b,
|  | int | sgn_y,
|  | v16acc64 | acc1 )

Parameters

  a | Matrix A
  sgn_x | Sign mask for matrix A
  b | Matrix B
  sgn_y | Sign mask for matrix B
  acc1 | Accumulator 1 input

Returns
  Result of operation

## ◆ negmac_4x4_4x4() [7/8]

v16acc64 negmac_4x4_4x4 | ( | v32uint16 | a,
|  | v32int16 | b,
|  | v16acc64 | acc1 )

Parameters

  a | Matrix A
  b | Matrix B
  acc1 | Accumulator 1 input

Returns
  Result of MAC operation

## ◆ negmac_4x4_4x4() [8/8]

v16acc64 negmac_4x4_4x4 | ( | v32uint16 | a,
|  | v32uint16 | b,
|  | v16acc64 | acc1 )

Parameters

  a | Matrix A
  b | Matrix B
  acc1 | Accumulator 1 input

Returns
  Result of MAC operation

## ◆ negmac_4x4_4x4_conf() [1/8]

v16acc64 negmac_4x4_4x4_conf | ( | v32int16 | a,
|  | int | sgn_x,
|  | v32int16 | b,
|  | int | sgn_y,
|  | v16acc64 | acc1,
|  | int | zero_acc1,
|  | int | sub_mul,
|  | int | sub_acc1 )

Parameters

  a | Matrix A
  sgn_x | Sign mask for matrix A
  b | Matrix B
  sgn_y | Sign mask for matrix B
  acc1 | Accumulator 1 input
  zero_acc1 | Zeroing mask for acc1
  sub_mul | Negation mask of multiplication result
  sub_acc1 | Negation mask of acc1

Returns
  Result of operation

## ◆ negmac_4x4_4x4_conf() [2/8]

v16acc64 negmac_4x4_4x4_conf | ( | v32int16 | a,
|  | int | sgn_x,
|  | v32uint16 | b,
|  | int | sgn_y,
|  | v16acc64 | acc1,
|  | int | zero_acc1,
|  | int | sub_mul,
|  | int | sub_acc1 )

Parameters

  a | Matrix A
  sgn_x | Sign mask for matrix A
  b | Matrix B
  sgn_y | Sign mask for matrix B
  acc1 | Accumulator 1 input
  zero_acc1 | Zeroing mask for acc1
  sub_mul | Negation mask of multiplication result
  sub_acc1 | Negation mask of acc1

Returns
  Result of operation

## ◆ negmac_4x4_4x4_conf() [3/8]

v16acc64 negmac_4x4_4x4_conf | ( | v32int16 | a,
|  | v32int16 | b,
|  | v16acc64 | acc1,
|  | int | zero_acc1,
|  | int | sub_mul,
|  | int | sub_acc1 )

Parameters

  a | Matrix A
  b | Matrix B
  acc1 | Accumulator 1 input
  zero_acc1 | Zeroing mask for acc1
  sub_mul | Negation mask of multiplication result
  sub_acc1 | Negation mask of acc1

Returns
  Result of operation

## ◆ negmac_4x4_4x4_conf() [4/8]

v16acc64 negmac_4x4_4x4_conf | ( | v32int16 | a,
|  | v32uint16 | b,
|  | v16acc64 | acc1,
|  | int | zero_acc1,
|  | int | sub_mul,
|  | int | sub_acc1 )

Parameters

  a | Matrix A
  b | Matrix B
  acc1 | Accumulator 1 input
  zero_acc1 | Zeroing mask for acc1
  sub_mul | Negation mask of multiplication result
  sub_acc1 | Negation mask of acc1

Returns
  Result of operation

## ◆ negmac_4x4_4x4_conf() [5/8]

v16acc64 negmac_4x4_4x4_conf | ( | v32uint16 | a,
|  | int | sgn_x,
|  | v32int16 | b,
|  | int | sgn_y,
|  | v16acc64 | acc1,
|  | int | zero_acc1,
|  | int | sub_mul,
|  | int | sub_acc1 )

Parameters

  a | Matrix A
  sgn_x | Sign mask for matrix A
  b | Matrix B
  sgn_y | Sign mask for matrix B
  acc1 | Accumulator 1 input
  zero_acc1 | Zeroing mask for acc1
  sub_mul | Negation mask of multiplication result
  sub_acc1 | Negation mask of acc1

Returns
  Result of operation

## ◆ negmac_4x4_4x4_conf() [6/8]

v16acc64 negmac_4x4_4x4_conf | ( | v32uint16 | a,
|  | int | sgn_x,
|  | v32uint16 | b,
|  | int | sgn_y,
|  | v16acc64 | acc1,
|  | int | zero_acc1,
|  | int | sub_mul,
|  | int | sub_acc1 )

Parameters

  a | Matrix A
  sgn_x | Sign mask for matrix A
  b | Matrix B
  sgn_y | Sign mask for matrix B
  acc1 | Accumulator 1 input
  zero_acc1 | Zeroing mask for acc1
  sub_mul | Negation mask of multiplication result
  sub_acc1 | Negation mask of acc1

Returns
  Result of operation

## ◆ negmac_4x4_4x4_conf() [7/8]

v16acc64 negmac_4x4_4x4_conf | ( | v32uint16 | a,
|  | v32int16 | b,
|  | v16acc64 | acc1,
|  | int | zero_acc1,
|  | int | sub_mul,
|  | int | sub_acc1 )

Parameters

  a | Matrix A
  b | Matrix B
  acc1 | Accumulator 1 input
  zero_acc1 | Zeroing mask for acc1
  sub_mul | Negation mask of multiplication result
  sub_acc1 | Negation mask of acc1

Returns
  Result of operation

## ◆ negmac_4x4_4x4_conf() [8/8]

v16acc64 negmac_4x4_4x4_conf | ( | v32uint16 | a,
|  | v32uint16 | b,
|  | v16acc64 | acc1,
|  | int | zero_acc1,
|  | int | sub_mul,
|  | int | sub_acc1 )

Parameters

  a | Matrix A
  b | Matrix B
  acc1 | Accumulator 1 input
  zero_acc1 | Zeroing mask for acc1
  sub_mul | Negation mask of multiplication result
  sub_acc1 | Negation mask of acc1

Returns
  Result of operation

## ◆ negmac_conv_16x4() [1/8]

v16acc64 negmac_conv_16x4 | ( | v32int16 | a,
|  | int | sgn_x,
|  | v32int16 | b,
|  | int | sgn_y,
|  | v16acc64 | acc1 )

Parameters

  a | Matrix A
  sgn_x | Sign mask for matrix A
  b | Matrix B
  sgn_y | Sign mask for matrix B
  acc1 | Accumulator 1 input

Returns
  Result of operation

## ◆ negmac_conv_16x4() [2/8]

v16acc64 negmac_conv_16x4 | ( | v32int16 | a,
|  | int | sgn_x,
|  | v32uint16 | b,
|  | int | sgn_y,
|  | v16acc64 | acc1 )

Parameters

  a | Matrix A
  sgn_x | Sign mask for matrix A
  b | Matrix B
  sgn_y | Sign mask for matrix B
  acc1 | Accumulator 1 input

Returns
  Result of operation

## ◆ negmac_conv_16x4() [3/8]

v16acc64 negmac_conv_16x4 | ( | v32int16 | a,
|  | v32int16 | b,
|  | v16acc64 | acc1 )

Parameters

  a | Matrix A
  b | Matrix B
  acc1 | Accumulator 1 input

Returns
  Result of MAC operation

## ◆ negmac_conv_16x4() [4/8]

v16acc64 negmac_conv_16x4 | ( | v32int16 | a,
|  | v32uint16 | b,
|  | v16acc64 | acc1 )

Parameters

  a | Matrix A
  b | Matrix B
  acc1 | Accumulator 1 input

Returns
  Result of MAC operation

## ◆ negmac_conv_16x4() [5/8]

v16acc64 negmac_conv_16x4 | ( | v32uint16 | a,
|  | int | sgn_x,
|  | v32int16 | b,
|  | int | sgn_y,
|  | v16acc64 | acc1 )

Parameters

  a | Matrix A
  sgn_x | Sign mask for matrix A
  b | Matrix B
  sgn_y | Sign mask for matrix B
  acc1 | Accumulator 1 input

Returns
  Result of operation

## ◆ negmac_conv_16x4() [6/8]

v16acc64 negmac_conv_16x4 | ( | v32uint16 | a,
|  | int | sgn_x,
|  | v32uint16 | b,
|  | int | sgn_y,
|  | v16acc64 | acc1 )

Parameters

  a | Matrix A
  sgn_x | Sign mask for matrix A
  b | Matrix B
  sgn_y | Sign mask for matrix B
  acc1 | Accumulator 1 input

Returns
  Result of operation

## ◆ negmac_conv_16x4() [7/8]

v16acc64 negmac_conv_16x4 | ( | v32uint16 | a,
|  | v32int16 | b,
|  | v16acc64 | acc1 )

Parameters

  a | Matrix A
  b | Matrix B
  acc1 | Accumulator 1 input

Returns
  Result of MAC operation

## ◆ negmac_conv_16x4() [8/8]

v16acc64 negmac_conv_16x4 | ( | v32uint16 | a,
|  | v32uint16 | b,
|  | v16acc64 | acc1 )

Parameters

  a | Matrix A
  b | Matrix B
  acc1 | Accumulator 1 input

Returns
  Result of MAC operation

## ◆ negmac_conv_16x4_conf() [1/8]

v16acc64 negmac_conv_16x4_conf | ( | v32int16 | a,
|  | int | sgn_x,
|  | v32int16 | b,
|  | int | sgn_y,
|  | v16acc64 | acc1,
|  | int | zero_acc1,
|  | int | sub_mul,
|  | int | sub_acc1 )

Parameters

  a | Matrix A
  sgn_x | Sign mask for matrix A
  b | Matrix B
  sgn_y | Sign mask for matrix B
  acc1 | Accumulator 1 input
  zero_acc1 | Zeroing mask for acc1
  sub_mul | Negation mask of multiplication result
  sub_acc1 | Negation mask of acc1

Returns
  Result of operation

## ◆ negmac_conv_16x4_conf() [2/8]

v16acc64 negmac_conv_16x4_conf | ( | v32int16 | a,
|  | int | sgn_x,
|  | v32uint16 | b,
|  | int | sgn_y,
|  | v16acc64 | acc1,
|  | int | zero_acc1,
|  | int | sub_mul,
|  | int | sub_acc1 )

Parameters

  a | Matrix A
  sgn_x | Sign mask for matrix A
  b | Matrix B
  sgn_y | Sign mask for matrix B
  acc1 | Accumulator 1 input
  zero_acc1 | Zeroing mask for acc1
  sub_mul | Negation mask of multiplication result
  sub_acc1 | Negation mask of acc1

Returns
  Result of operation

## ◆ negmac_conv_16x4_conf() [3/8]

v16acc64 negmac_conv_16x4_conf | ( | v32int16 | a,
|  | v32int16 | b,
|  | v16acc64 | acc1,
|  | int | zero_acc1,
|  | int | sub_mul,
|  | int | sub_acc1 )

Parameters

  a | Matrix A
  b | Matrix B
  acc1 | Accumulator 1 input
  zero_acc1 | Zeroing mask for acc1
  sub_mul | Negation mask of multiplication result
  sub_acc1 | Negation mask of acc1

Returns
  Result of operation

## ◆ negmac_conv_16x4_conf() [4/8]

v16acc64 negmac_conv_16x4_conf | ( | v32int16 | a,
|  | v32uint16 | b,
|  | v16acc64 | acc1,
|  | int | zero_acc1,
|  | int | sub_mul,
|  | int | sub_acc1 )

Parameters

  a | Matrix A
  b | Matrix B
  acc1 | Accumulator 1 input
  zero_acc1 | Zeroing mask for acc1
  sub_mul | Negation mask of multiplication result
  sub_acc1 | Negation mask of acc1

Returns
  Result of operation

## ◆ negmac_conv_16x4_conf() [5/8]

v16acc64 negmac_conv_16x4_conf | ( | v32uint16 | a,
|  | int | sgn_x,
|  | v32int16 | b,
|  | int | sgn_y,
|  | v16acc64 | acc1,
|  | int | zero_acc1,
|  | int | sub_mul,
|  | int | sub_acc1 )

Parameters

  a | Matrix A
  sgn_x | Sign mask for matrix A
  b | Matrix B
  sgn_y | Sign mask for matrix B
  acc1 | Accumulator 1 input
  zero_acc1 | Zeroing mask for acc1
  sub_mul | Negation mask of multiplication result
  sub_acc1 | Negation mask of acc1

Returns
  Result of operation

## ◆ negmac_conv_16x4_conf() [6/8]

v16acc64 negmac_conv_16x4_conf | ( | v32uint16 | a,
|  | int | sgn_x,
|  | v32uint16 | b,
|  | int | sgn_y,
|  | v16acc64 | acc1,
|  | int | zero_acc1,
|  | int | sub_mul,
|  | int | sub_acc1 )

Parameters

  a | Matrix A
  sgn_x | Sign mask for matrix A
  b | Matrix B
  sgn_y | Sign mask for matrix B
  acc1 | Accumulator 1 input
  zero_acc1 | Zeroing mask for acc1
  sub_mul | Negation mask of multiplication result
  sub_acc1 | Negation mask of acc1

Returns
  Result of operation

## ◆ negmac_conv_16x4_conf() [7/8]

v16acc64 negmac_conv_16x4_conf | ( | v32uint16 | a,
|  | v32int16 | b,
|  | v16acc64 | acc1,
|  | int | zero_acc1,
|  | int | sub_mul,
|  | int | sub_acc1 )

Parameters

  a | Matrix A
  b | Matrix B
  acc1 | Accumulator 1 input
  zero_acc1 | Zeroing mask for acc1
  sub_mul | Negation mask of multiplication result
  sub_acc1 | Negation mask of acc1

Returns
  Result of operation

## ◆ negmac_conv_16x4_conf() [8/8]

v16acc64 negmac_conv_16x4_conf | ( | v32uint16 | a,
|  | v32uint16 | b,
|  | v16acc64 | acc1,
|  | int | zero_acc1,
|  | int | sub_mul,
|  | int | sub_acc1 )

Parameters

  a | Matrix A
  b | Matrix B
  acc1 | Accumulator 1 input
  zero_acc1 | Zeroing mask for acc1
  sub_mul | Negation mask of multiplication result
  sub_acc1 | Negation mask of acc1

Returns
  Result of operation

## ◆ negmac_elem_16_2() [1/8]

v16acc64 negmac_elem_16_2 | ( | v32int16 | a,
|  | int | sgn_x,
|  | v32int16 | b,
|  | int | sgn_y,
|  | v16acc64 | acc1 )

Parameters

  a | Matrix A
  sgn_x | Sign mask for matrix A
  b | Matrix B
  sgn_y | Sign mask for matrix B
  acc1 | Accumulator 1 input

Returns
  Result of operation

## ◆ negmac_elem_16_2() [2/8]

v16acc64 negmac_elem_16_2 | ( | v32int16 | a,
|  | int | sgn_x,
|  | v32uint16 | b,
|  | int | sgn_y,
|  | v16acc64 | acc1 )

Parameters

  a | Matrix A
  sgn_x | Sign mask for matrix A
  b | Matrix B
  sgn_y | Sign mask for matrix B
  acc1 | Accumulator 1 input

Returns
  Result of operation

## ◆ negmac_elem_16_2() [3/8]

v16acc64 negmac_elem_16_2 | ( | v32int16 | a,
|  | v32int16 | b,
|  | v16acc64 | acc1 )

Parameters

  a | Matrix A
  b | Matrix B
  acc1 | Accumulator 1 input

Returns
  Result of MAC operation

## ◆ negmac_elem_16_2() [4/8]

v16acc64 negmac_elem_16_2 | ( | v32int16 | a,
|  | v32uint16 | b,
|  | v16acc64 | acc1 )

Parameters

  a | Matrix A
  b | Matrix B
  acc1 | Accumulator 1 input

Returns
  Result of MAC operation

## ◆ negmac_elem_16_2() [5/8]

v16acc64 negmac_elem_16_2 | ( | v32uint16 | a,
|  | int | sgn_x,
|  | v32int16 | b,
|  | int | sgn_y,
|  | v16acc64 | acc1 )

Parameters

  a | Matrix A
  sgn_x | Sign mask for matrix A
  b | Matrix B
  sgn_y | Sign mask for matrix B
  acc1 | Accumulator 1 input

Returns
  Result of operation

## ◆ negmac_elem_16_2() [6/8]

v16acc64 negmac_elem_16_2 | ( | v32uint16 | a,
|  | int | sgn_x,
|  | v32uint16 | b,
|  | int | sgn_y,
|  | v16acc64 | acc1 )

Parameters

  a | Matrix A
  sgn_x | Sign mask for matrix A
  b | Matrix B
  sgn_y | Sign mask for matrix B
  acc1 | Accumulator 1 input

Returns
  Result of operation

## ◆ negmac_elem_16_2() [7/8]

v16acc64 negmac_elem_16_2 | ( | v32uint16 | a,
|  | v32int16 | b,
|  | v16acc64 | acc1 )

Parameters

  a | Matrix A
  b | Matrix B
  acc1 | Accumulator 1 input

Returns
  Result of MAC operation

## ◆ negmac_elem_16_2() [8/8]

v16acc64 negmac_elem_16_2 | ( | v32uint16 | a,
|  | v32uint16 | b,
|  | v16acc64 | acc1 )

Parameters

  a | Matrix A
  b | Matrix B
  acc1 | Accumulator 1 input

Returns
  Result of MAC operation

## ◆ negmac_elem_16_2_conf() [1/8]

v16acc64 negmac_elem_16_2_conf | ( | v32int16 | a,
|  | int | sgn_x,
|  | v32int16 | b,
|  | int | sgn_y,
|  | v16acc64 | acc1,
|  | int | zero_acc1,
|  | int | sub_mul,
|  | int | sub_acc1 )

Parameters

  a | Matrix A
  sgn_x | Sign mask for matrix A
  b | Matrix B
  sgn_y | Sign mask for matrix B
  acc1 | Accumulator 1 input
  zero_acc1 | Zeroing mask for acc1
  sub_mul | Negation mask of multiplication result
  sub_acc1 | Negation mask of acc1

Returns
  Result of operation

## ◆ negmac_elem_16_2_conf() [2/8]

v16acc64 negmac_elem_16_2_conf | ( | v32int16 | a,
|  | int | sgn_x,
|  | v32uint16 | b,
|  | int | sgn_y,
|  | v16acc64 | acc1,
|  | int | zero_acc1,
|  | int | sub_mul,
|  | int | sub_acc1 )

Parameters

  a | Matrix A
  sgn_x | Sign mask for matrix A
  b | Matrix B
  sgn_y | Sign mask for matrix B
  acc1 | Accumulator 1 input
  zero_acc1 | Zeroing mask for acc1
  sub_mul | Negation mask of multiplication result
  sub_acc1 | Negation mask of acc1

Returns
  Result of operation

## ◆ negmac_elem_16_2_conf() [3/8]

v16acc64 negmac_elem_16_2_conf | ( | v32int16 | a,
|  | v32int16 | b,
|  | v16acc64 | acc1,
|  | int | zero_acc1,
|  | int | sub_mul,
|  | int | sub_acc1 )

Parameters

  a | Matrix A
  b | Matrix B
  acc1 | Accumulator 1 input
  zero_acc1 | Zeroing mask for acc1
  sub_mul | Negation mask of multiplication result
  sub_acc1 | Negation mask of acc1

Returns
  Result of operation

## ◆ negmac_elem_16_2_conf() [4/8]

v16acc64 negmac_elem_16_2_conf | ( | v32int16 | a,
|  | v32uint16 | b,
|  | v16acc64 | acc1,
|  | int | zero_acc1,
|  | int | sub_mul,
|  | int | sub_acc1 )

Parameters

  a | Matrix A
  b | Matrix B
  acc1 | Accumulator 1 input
  zero_acc1 | Zeroing mask for acc1
  sub_mul | Negation mask of multiplication result
  sub_acc1 | Negation mask of acc1

Returns
  Result of operation

## ◆ negmac_elem_16_2_conf() [5/8]

v16acc64 negmac_elem_16_2_conf | ( | v32uint16 | a,
|  | int | sgn_x,
|  | v32int16 | b,
|  | int | sgn_y,
|  | v16acc64 | acc1,
|  | int | zero_acc1,
|  | int | sub_mul,
|  | int | sub_acc1 )

Parameters

  a | Matrix A
  sgn_x | Sign mask for matrix A
  b | Matrix B
  sgn_y | Sign mask for matrix B
  acc1 | Accumulator 1 input
  zero_acc1 | Zeroing mask for acc1
  sub_mul | Negation mask of multiplication result
  sub_acc1 | Negation mask of acc1

Returns
  Result of operation

## ◆ negmac_elem_16_2_conf() [6/8]

v16acc64 negmac_elem_16_2_conf | ( | v32uint16 | a,
|  | int | sgn_x,
|  | v32uint16 | b,
|  | int | sgn_y,
|  | v16acc64 | acc1,
|  | int | zero_acc1,
|  | int | sub_mul,
|  | int | sub_acc1 )

Parameters

  a | Matrix A
  sgn_x | Sign mask for matrix A
  b | Matrix B
  sgn_y | Sign mask for matrix B
  acc1 | Accumulator 1 input
  zero_acc1 | Zeroing mask for acc1
  sub_mul | Negation mask of multiplication result
  sub_acc1 | Negation mask of acc1

Returns
  Result of operation

## ◆ negmac_elem_16_2_conf() [7/8]

v16acc64 negmac_elem_16_2_conf | ( | v32uint16 | a,
|  | v32int16 | b,
|  | v16acc64 | acc1,
|  | int | zero_acc1,
|  | int | sub_mul,
|  | int | sub_acc1 )

Parameters

  a | Matrix A
  b | Matrix B
  acc1 | Accumulator 1 input
  zero_acc1 | Zeroing mask for acc1
  sub_mul | Negation mask of multiplication result
  sub_acc1 | Negation mask of acc1

Returns
  Result of operation

## ◆ negmac_elem_16_2_conf() [8/8]

v16acc64 negmac_elem_16_2_conf | ( | v32uint16 | a,
|  | v32uint16 | b,
|  | v16acc64 | acc1,
|  | int | zero_acc1,
|  | int | sub_mul,
|  | int | sub_acc1 )

Parameters

  a | Matrix A
  b | Matrix B
  acc1 | Accumulator 1 input
  zero_acc1 | Zeroing mask for acc1
  sub_mul | Negation mask of multiplication result
  sub_acc1 | Negation mask of acc1

Returns
  Result of operation

## ◆ negmac_elem_32() [1/8]

v32acc32 negmac_elem_32 | ( | v32int16 | a,
|  | int | sgn_x,
|  | v32int16 | b,
|  | int | sgn_y,
|  | v32acc32 | acc1 )

Parameters

  a | Matrix A
  sgn_x | Sign mask for matrix A
  b | Matrix B
  sgn_y | Sign mask for matrix B
  acc1 | Accumulator 1 input

Returns
  Result of operation

## ◆ negmac_elem_32() [2/8]

v32acc32 negmac_elem_32 | ( | v32int16 | a,
|  | int | sgn_x,
|  | v32uint16 | b,
|  | int | sgn_y,
|  | v32acc32 | acc1 )

Parameters

  a | Matrix A
  sgn_x | Sign mask for matrix A
  b | Matrix B
  sgn_y | Sign mask for matrix B
  acc1 | Accumulator 1 input

Returns
  Result of operation

## ◆ negmac_elem_32() [3/8]

v32acc32 negmac_elem_32 | ( | v32int16 | a,
|  | v32int16 | b,
|  | v32acc32 | acc1 )

Parameters

  a | Matrix A
  b | Matrix B
  acc1 | Accumulator 1 input

Returns
  Result of MAC operation

## ◆ negmac_elem_32() [4/8]

v32acc32 negmac_elem_32 | ( | v32int16 | a,
|  | v32uint16 | b,
|  | v32acc32 | acc1 )

Parameters

  a | Matrix A
  b | Matrix B
  acc1 | Accumulator 1 input

Returns
  Result of MAC operation

## ◆ negmac_elem_32() [5/8]

v32acc32 negmac_elem_32 | ( | v32uint16 | a,
|  | int | sgn_x,
|  | v32int16 | b,
|  | int | sgn_y,
|  | v32acc32 | acc1 )

Parameters

  a | Matrix A
  sgn_x | Sign mask for matrix A
  b | Matrix B
  sgn_y | Sign mask for matrix B
  acc1 | Accumulator 1 input

Returns
  Result of operation

## ◆ negmac_elem_32() [6/8]

v32acc32 negmac_elem_32 | ( | v32uint16 | a,
|  | int | sgn_x,
|  | v32uint16 | b,
|  | int | sgn_y,
|  | v32acc32 | acc1 )

Parameters

  a | Matrix A
  sgn_x | Sign mask for matrix A
  b | Matrix B
  sgn_y | Sign mask for matrix B
  acc1 | Accumulator 1 input

Returns
  Result of operation

## ◆ negmac_elem_32() [7/8]

v32acc32 negmac_elem_32 | ( | v32uint16 | a,
|  | v32int16 | b,
|  | v32acc32 | acc1 )

Parameters

  a | Matrix A
  b | Matrix B
  acc1 | Accumulator 1 input

Returns
  Result of MAC operation

## ◆ negmac_elem_32() [8/8]

v32acc32 negmac_elem_32 | ( | v32uint16 | a,
|  | v32uint16 | b,
|  | v32acc32 | acc1 )

Parameters

  a | Matrix A
  b | Matrix B
  acc1 | Accumulator 1 input

Returns
  Result of MAC operation

## ◆ negmac_elem_32_conf() [1/8]

v32acc32 negmac_elem_32_conf | ( | v32int16 | a,
|  | int | sgn_x,
|  | v32int16 | b,
|  | int | sgn_y,
|  | v32acc32 | acc1,
|  | int | zero_acc1,
|  | int | sub_mul,
|  | int | sub_acc1 )

Parameters

  a | Matrix A
  sgn_x | Sign mask for matrix A
  b | Matrix B
  sgn_y | Sign mask for matrix B
  acc1 | Accumulator 1 input
  zero_acc1 | Zeroing mask for acc1
  sub_mul | Negation mask of multiplication result
  sub_acc1 | Negation mask of acc1

Returns
  Result of operation

## ◆ negmac_elem_32_conf() [2/8]

v32acc32 negmac_elem_32_conf | ( | v32int16 | a,
|  | int | sgn_x,
|  | v32uint16 | b,
|  | int | sgn_y,
|  | v32acc32 | acc1,
|  | int | zero_acc1,
|  | int | sub_mul,
|  | int | sub_acc1 )

Parameters

  a | Matrix A
  sgn_x | Sign mask for matrix A
  b | Matrix B
  sgn_y | Sign mask for matrix B
  acc1 | Accumulator 1 input
  zero_acc1 | Zeroing mask for acc1
  sub_mul | Negation mask of multiplication result
  sub_acc1 | Negation mask of acc1

Returns
  Result of operation

## ◆ negmac_elem_32_conf() [3/8]

v32acc32 negmac_elem_32_conf | ( | v32int16 | a,
|  | v32int16 | b,
|  | v32acc32 | acc1,
|  | int | zero_acc1,
|  | int | sub_mul,
|  | int | sub_acc1 )

Parameters

  a | Matrix A
  b | Matrix B
  acc1 | Accumulator 1 input
  zero_acc1 | Zeroing mask for acc1
  sub_mul | Negation mask of multiplication result
  sub_acc1 | Negation mask of acc1

Returns
  Result of operation

## ◆ negmac_elem_32_conf() [4/8]

v32acc32 negmac_elem_32_conf | ( | v32int16 | a,
|  | v32uint16 | b,
|  | v32acc32 | acc1,
|  | int | zero_acc1,
|  | int | sub_mul,
|  | int | sub_acc1 )

Parameters

  a | Matrix A
  b | Matrix B
  acc1 | Accumulator 1 input
  zero_acc1 | Zeroing mask for acc1
  sub_mul | Negation mask of multiplication result
  sub_acc1 | Negation mask of acc1

Returns
  Result of operation

## ◆ negmac_elem_32_conf() [5/8]

v32acc32 negmac_elem_32_conf | ( | v32uint16 | a,
|  | int | sgn_x,
|  | v32int16 | b,
|  | int | sgn_y,
|  | v32acc32 | acc1,
|  | int | zero_acc1,
|  | int | sub_mul,
|  | int | sub_acc1 )

Parameters

  a | Matrix A
  sgn_x | Sign mask for matrix A
  b | Matrix B
  sgn_y | Sign mask for matrix B
  acc1 | Accumulator 1 input
  zero_acc1 | Zeroing mask for acc1
  sub_mul | Negation mask of multiplication result
  sub_acc1 | Negation mask of acc1

Returns
  Result of operation

## ◆ negmac_elem_32_conf() [6/8]

v32acc32 negmac_elem_32_conf | ( | v32uint16 | a,
|  | int | sgn_x,
|  | v32uint16 | b,
|  | int | sgn_y,
|  | v32acc32 | acc1,
|  | int | zero_acc1,
|  | int | sub_mul,
|  | int | sub_acc1 )

Parameters

  a | Matrix A
  sgn_x | Sign mask for matrix A
  b | Matrix B
  sgn_y | Sign mask for matrix B
  acc1 | Accumulator 1 input
  zero_acc1 | Zeroing mask for acc1
  sub_mul | Negation mask of multiplication result
  sub_acc1 | Negation mask of acc1

Returns
  Result of operation

## ◆ negmac_elem_32_conf() [7/8]

v32acc32 negmac_elem_32_conf | ( | v32uint16 | a,
|  | v32int16 | b,
|  | v32acc32 | acc1,
|  | int | zero_acc1,
|  | int | sub_mul,
|  | int | sub_acc1 )

Parameters

  a | Matrix A
  b | Matrix B
  acc1 | Accumulator 1 input
  zero_acc1 | Zeroing mask for acc1
  sub_mul | Negation mask of multiplication result
  sub_acc1 | Negation mask of acc1

Returns
  Result of operation

## ◆ negmac_elem_32_conf() [8/8]

v32acc32 negmac_elem_32_conf | ( | v32uint16 | a,
|  | v32uint16 | b,
|  | v32acc32 | acc1,
|  | int | zero_acc1,
|  | int | sub_mul,
|  | int | sub_acc1 )

Parameters

  a | Matrix A
  b | Matrix B
  acc1 | Accumulator 1 input
  zero_acc1 | Zeroing mask for acc1
  sub_mul | Negation mask of multiplication result
  sub_acc1 | Negation mask of acc1

Returns
  Result of operation

## ◆ negmsc_2x4_4x8() [1/8]

v16acc64 negmsc_2x4_4x8 | ( | v32int16 | a,
|  | int | sgn_x,
|  | v32int16 | b,
|  | int | sgn_y,
|  | v16acc64 | acc1 )

Parameters

  a | Matrix A
  sgn_x | Sign mask for matrix A
  b | Matrix B
  sgn_y | Sign mask for matrix B
  acc1 | Accumulator 1 input

Returns
  Result of operation

## ◆ negmsc_2x4_4x8() [2/8]

v16acc64 negmsc_2x4_4x8 | ( | v32int16 | a,
|  | int | sgn_x,
|  | v32uint16 | b,
|  | int | sgn_y,
|  | v16acc64 | acc1 )

Parameters

  a | Matrix A
  sgn_x | Sign mask for matrix A
  b | Matrix B
  sgn_y | Sign mask for matrix B
  acc1 | Accumulator 1 input

Returns
  Result of operation

## ◆ negmsc_2x4_4x8() [3/8]

v16acc64 negmsc_2x4_4x8 | ( | v32int16 | a,
|  | v32int16 | b,
|  | v16acc64 | acc1 )

Parameters

  a | Matrix A
  b | Matrix B
  acc1 | Accumulator 1 input

Returns
  Result of operation

## ◆ negmsc_2x4_4x8() [4/8]

v16acc64 negmsc_2x4_4x8 | ( | v32int16 | a,
|  | v32uint16 | b,
|  | v16acc64 | acc1 )

Parameters

  a | Matrix A
  b | Matrix B
  acc1 | Accumulator 1 input

Returns
  Result of operation

## ◆ negmsc_2x4_4x8() [5/8]

v16acc64 negmsc_2x4_4x8 | ( | v32uint16 | a,
|  | int | sgn_x,
|  | v32int16 | b,
|  | int | sgn_y,
|  | v16acc64 | acc1 )

Parameters

  a | Matrix A
  sgn_x | Sign mask for matrix A
  b | Matrix B
  sgn_y | Sign mask for matrix B
  acc1 | Accumulator 1 input

Returns
  Result of operation

## ◆ negmsc_2x4_4x8() [6/8]

v16acc64 negmsc_2x4_4x8 | ( | v32uint16 | a,
|  | int | sgn_x,
|  | v32uint16 | b,
|  | int | sgn_y,
|  | v16acc64 | acc1 )

Parameters

  a | Matrix A
  sgn_x | Sign mask for matrix A
  b | Matrix B
  sgn_y | Sign mask for matrix B
  acc1 | Accumulator 1 input

Returns
  Result of operation

## ◆ negmsc_2x4_4x8() [7/8]

v16acc64 negmsc_2x4_4x8 | ( | v32uint16 | a,
|  | v32int16 | b,
|  | v16acc64 | acc1 )

Parameters

  a | Matrix A
  b | Matrix B
  acc1 | Accumulator 1 input

Returns
  Result of operation

## ◆ negmsc_2x4_4x8() [8/8]

v16acc64 negmsc_2x4_4x8 | ( | v32uint16 | a,
|  | v32uint16 | b,
|  | v16acc64 | acc1 )

Parameters

  a | Matrix A
  b | Matrix B
  acc1 | Accumulator 1 input

Returns
  Result of operation

## ◆ negmsc_2x4_4x8_conf() [1/8]

v16acc64 negmsc_2x4_4x8_conf | ( | v32int16 | a,
|  | int | sgn_x,
|  | v32int16 | b,
|  | int | sgn_y,
|  | v16acc64 | acc1,
|  | int | zero_acc1,
|  | int | sub_mul,
|  | int | sub_acc1 )

Parameters

  a | Matrix A
  sgn_x | Sign mask for matrix A
  b | Matrix B
  sgn_y | Sign mask for matrix B
  acc1 | Accumulator 1 input
  zero_acc1 | Zeroing mask for acc1
  sub_mul | Negation mask of multiplication result
  sub_acc1 | Negation mask of acc1

Returns
  Result of operation

## ◆ negmsc_2x4_4x8_conf() [2/8]

v16acc64 negmsc_2x4_4x8_conf | ( | v32int16 | a,
|  | int | sgn_x,
|  | v32uint16 | b,
|  | int | sgn_y,
|  | v16acc64 | acc1,
|  | int | zero_acc1,
|  | int | sub_mul,
|  | int | sub_acc1 )

Parameters

  a | Matrix A
  sgn_x | Sign mask for matrix A
  b | Matrix B
  sgn_y | Sign mask for matrix B
  acc1 | Accumulator 1 input
  zero_acc1 | Zeroing mask for acc1
  sub_mul | Negation mask of multiplication result
  sub_acc1 | Negation mask of acc1

Returns
  Result of operation

## ◆ negmsc_2x4_4x8_conf() [3/8]

v16acc64 negmsc_2x4_4x8_conf | ( | v32int16 | a,
|  | v32int16 | b,
|  | v16acc64 | acc1,
|  | int | zero_acc1,
|  | int | sub_mul,
|  | int | sub_acc1 )

Parameters

  a | Matrix A
  b | Matrix B
  acc1 | Accumulator 1 input
  zero_acc1 | Zeroing mask for acc1
  sub_mul | Negation mask of multiplication result
  sub_acc1 | Negation mask of acc1. If a bit is set the corresponding accumulator lane of acc1 is negated.

Returns
  Result of operation

## ◆ negmsc_2x4_4x8_conf() [4/8]

v16acc64 negmsc_2x4_4x8_conf | ( | v32int16 | a,
|  | v32uint16 | b,
|  | v16acc64 | acc1,
|  | int | zero_acc1,
|  | int | sub_mul,
|  | int | sub_acc1 )

Parameters

  a | Matrix A
  b | Matrix B
  acc1 | Accumulator 1 input
  zero_acc1 | Zeroing mask for acc1
  sub_mul | Negation mask of multiplication result
  sub_acc1 | Negation mask of acc1. If a bit is set the corresponding accumulator lane of acc1 is negated.

Returns
  Result of operation

## ◆ negmsc_2x4_4x8_conf() [5/8]

v16acc64 negmsc_2x4_4x8_conf | ( | v32uint16 | a,
|  | int | sgn_x,
|  | v32int16 | b,
|  | int | sgn_y,
|  | v16acc64 | acc1,
|  | int | zero_acc1,
|  | int | sub_mul,
|  | int | sub_acc1 )

Parameters

  a | Matrix A
  sgn_x | Sign mask for matrix A
  b | Matrix B
  sgn_y | Sign mask for matrix B
  acc1 | Accumulator 1 input
  zero_acc1 | Zeroing mask for acc1
  sub_mul | Negation mask of multiplication result
  sub_acc1 | Negation mask of acc1

Returns
  Result of operation

## ◆ negmsc_2x4_4x8_conf() [6/8]

v16acc64 negmsc_2x4_4x8_conf | ( | v32uint16 | a,
|  | int | sgn_x,
|  | v32uint16 | b,
|  | int | sgn_y,
|  | v16acc64 | acc1,
|  | int | zero_acc1,
|  | int | sub_mul,
|  | int | sub_acc1 )

Parameters

  a | Matrix A
  sgn_x | Sign mask for matrix A
  b | Matrix B
  sgn_y | Sign mask for matrix B
  acc1 | Accumulator 1 input
  zero_acc1 | Zeroing mask for acc1
  sub_mul | Negation mask of multiplication result
  sub_acc1 | Negation mask of acc1

Returns
  Result of operation

## ◆ negmsc_2x4_4x8_conf() [7/8]

v16acc64 negmsc_2x4_4x8_conf | ( | v32uint16 | a,
|  | v32int16 | b,
|  | v16acc64 | acc1,
|  | int | zero_acc1,
|  | int | sub_mul,
|  | int | sub_acc1 )

Parameters

  a | Matrix A
  b | Matrix B
  acc1 | Accumulator 1 input
  zero_acc1 | Zeroing mask for acc1
  sub_mul | Negation mask of multiplication result
  sub_acc1 | Negation mask of acc1. If a bit is set the corresponding accumulator lane of acc1 is negated.

Returns
  Result of operation

## ◆ negmsc_2x4_4x8_conf() [8/8]

v16acc64 negmsc_2x4_4x8_conf | ( | v32uint16 | a,
|  | v32uint16 | b,
|  | v16acc64 | acc1,
|  | int | zero_acc1,
|  | int | sub_mul,
|  | int | sub_acc1 )

Parameters

  a | Matrix A
  b | Matrix B
  acc1 | Accumulator 1 input
  zero_acc1 | Zeroing mask for acc1
  sub_mul | Negation mask of multiplication result
  sub_acc1 | Negation mask of acc1. If a bit is set the corresponding accumulator lane of acc1 is negated.

Returns
  Result of operation

## ◆ negmsc_4x2_2x8() [1/8]

v32acc32 negmsc_4x2_2x8 | ( | v32int16 | a,
|  | int | sgn_x,
|  | v32int16 | b,
|  | int | sgn_y,
|  | v32acc32 | acc1 )

Parameters

  a | Matrix A
  sgn_x | Sign mask for matrix A
  b | Matrix B
  sgn_y | Sign mask for matrix B
  acc1 | Accumulator 1 input

Returns
  Result of operation

## ◆ negmsc_4x2_2x8() [2/8]

v32acc32 negmsc_4x2_2x8 | ( | v32int16 | a,
|  | int | sgn_x,
|  | v32uint16 | b,
|  | int | sgn_y,
|  | v32acc32 | acc1 )

Parameters

  a | Matrix A
  sgn_x | Sign mask for matrix A
  b | Matrix B
  sgn_y | Sign mask for matrix B
  acc1 | Accumulator 1 input

Returns
  Result of operation

## ◆ negmsc_4x2_2x8() [3/8]

v32acc32 negmsc_4x2_2x8 | ( | v32int16 | a,
|  | v32int16 | b,
|  | v32acc32 | acc1 )

Parameters

  a | Matrix A
  b | Matrix B
  acc1 | Accumulator 1 input

Returns
  Result of operation

## ◆ negmsc_4x2_2x8() [4/8]

v32acc32 negmsc_4x2_2x8 | ( | v32int16 | a,
|  | v32uint16 | b,
|  | v32acc32 | acc1 )

Parameters

  a | Matrix A
  b | Matrix B
  acc1 | Accumulator 1 input

Returns
  Result of operation

## ◆ negmsc_4x2_2x8() [5/8]

v32acc32 negmsc_4x2_2x8 | ( | v32uint16 | a,
|  | int | sgn_x,
|  | v32int16 | b,
|  | int | sgn_y,
|  | v32acc32 | acc1 )

Parameters

  a | Matrix A
  sgn_x | Sign mask for matrix A
  b | Matrix B
  sgn_y | Sign mask for matrix B
  acc1 | Accumulator 1 input

Returns
  Result of operation

## ◆ negmsc_4x2_2x8() [6/8]

v32acc32 negmsc_4x2_2x8 | ( | v32uint16 | a,
|  | int | sgn_x,
|  | v32uint16 | b,
|  | int | sgn_y,
|  | v32acc32 | acc1 )

Parameters

  a | Matrix A
  sgn_x | Sign mask for matrix A
  b | Matrix B
  sgn_y | Sign mask for matrix B
  acc1 | Accumulator 1 input

Returns
  Result of operation

## ◆ negmsc_4x2_2x8() [7/8]

v32acc32 negmsc_4x2_2x8 | ( | v32uint16 | a,
|  | v32int16 | b,
|  | v32acc32 | acc1 )

Parameters

  a | Matrix A
  b | Matrix B
  acc1 | Accumulator 1 input

Returns
  Result of operation

## ◆ negmsc_4x2_2x8() [8/8]

v32acc32 negmsc_4x2_2x8 | ( | v32uint16 | a,
|  | v32uint16 | b,
|  | v32acc32 | acc1 )

Parameters

  a | Matrix A
  b | Matrix B
  acc1 | Accumulator 1 input

Returns
  Result of operation

## ◆ negmsc_4x2_2x8_conf() [1/8]

v32acc32 negmsc_4x2_2x8_conf | ( | v32int16 | a,
|  | int | sgn_x,
|  | v32int16 | b,
|  | int | sgn_y,
|  | v32acc32 | acc1,
|  | int | zero_acc1,
|  | int | sub_mul,
|  | int | sub_acc1 )

Parameters

  a | Matrix A
  sgn_x | Sign mask for matrix A
  b | Matrix B
  sgn_y | Sign mask for matrix B
  acc1 | Accumulator 1 input
  zero_acc1 | Zeroing mask for acc1
  sub_mul | Negation mask of multiplication result
  sub_acc1 | Negation mask of acc1

Returns
  Result of operation

## ◆ negmsc_4x2_2x8_conf() [2/8]

v32acc32 negmsc_4x2_2x8_conf | ( | v32int16 | a,
|  | int | sgn_x,
|  | v32uint16 | b,
|  | int | sgn_y,
|  | v32acc32 | acc1,
|  | int | zero_acc1,
|  | int | sub_mul,
|  | int | sub_acc1 )

Parameters

  a | Matrix A
  sgn_x | Sign mask for matrix A
  b | Matrix B
  sgn_y | Sign mask for matrix B
  acc1 | Accumulator 1 input
  zero_acc1 | Zeroing mask for acc1
  sub_mul | Negation mask of multiplication result
  sub_acc1 | Negation mask of acc1

Returns
  Result of operation

## ◆ negmsc_4x2_2x8_conf() [3/8]

v32acc32 negmsc_4x2_2x8_conf | ( | v32int16 | a,
|  | v32int16 | b,
|  | v32acc32 | acc1,
|  | int | zero_acc1,
|  | int | sub_mul,
|  | int | sub_acc1 )

Parameters

  a | Matrix A
  b | Matrix B
  acc1 | Accumulator 1 input
  zero_acc1 | Zeroing mask for acc1
  sub_mul | Negation mask of multiplication result
  sub_acc1 | Negation mask of acc1. If a bit is set the corresponding accumulator lane of acc1 is negated.

Returns
  Result of operation

## ◆ negmsc_4x2_2x8_conf() [4/8]

v32acc32 negmsc_4x2_2x8_conf | ( | v32int16 | a,
|  | v32uint16 | b,
|  | v32acc32 | acc1,
|  | int | zero_acc1,
|  | int | sub_mul,
|  | int | sub_acc1 )

Parameters

  a | Matrix A
  b | Matrix B
  acc1 | Accumulator 1 input
  zero_acc1 | Zeroing mask for acc1
  sub_mul | Negation mask of multiplication result
  sub_acc1 | Negation mask of acc1. If a bit is set the corresponding accumulator lane of acc1 is negated.

Returns
  Result of operation

## ◆ negmsc_4x2_2x8_conf() [5/8]

v32acc32 negmsc_4x2_2x8_conf | ( | v32uint16 | a,
|  | int | sgn_x,
|  | v32int16 | b,
|  | int | sgn_y,
|  | v32acc32 | acc1,
|  | int | zero_acc1,
|  | int | sub_mul,
|  | int | sub_acc1 )

Parameters

  a | Matrix A
  sgn_x | Sign mask for matrix A
  b | Matrix B
  sgn_y | Sign mask for matrix B
  acc1 | Accumulator 1 input
  zero_acc1 | Zeroing mask for acc1
  sub_mul | Negation mask of multiplication result
  sub_acc1 | Negation mask of acc1

Returns
  Result of operation

## ◆ negmsc_4x2_2x8_conf() [6/8]

v32acc32 negmsc_4x2_2x8_conf | ( | v32uint16 | a,
|  | int | sgn_x,
|  | v32uint16 | b,
|  | int | sgn_y,
|  | v32acc32 | acc1,
|  | int | zero_acc1,
|  | int | sub_mul,
|  | int | sub_acc1 )

Parameters

  a | Matrix A
  sgn_x | Sign mask for matrix A
  b | Matrix B
  sgn_y | Sign mask for matrix B
  acc1 | Accumulator 1 input
  zero_acc1 | Zeroing mask for acc1
  sub_mul | Negation mask of multiplication result
  sub_acc1 | Negation mask of acc1

Returns
  Result of operation

## ◆ negmsc_4x2_2x8_conf() [7/8]

v32acc32 negmsc_4x2_2x8_conf | ( | v32uint16 | a,
|  | v32int16 | b,
|  | v32acc32 | acc1,
|  | int | zero_acc1,
|  | int | sub_mul,
|  | int | sub_acc1 )

Parameters

  a | Matrix A
  b | Matrix B
  acc1 | Accumulator 1 input
  zero_acc1 | Zeroing mask for acc1
  sub_mul | Negation mask of multiplication result
  sub_acc1 | Negation mask of acc1. If a bit is set the corresponding accumulator lane of acc1 is negated.

Returns
  Result of operation

## ◆ negmsc_4x2_2x8_conf() [8/8]

v32acc32 negmsc_4x2_2x8_conf | ( | v32uint16 | a,
|  | v32uint16 | b,
|  | v32acc32 | acc1,
|  | int | zero_acc1,
|  | int | sub_mul,
|  | int | sub_acc1 )

Parameters

  a | Matrix A
  b | Matrix B
  acc1 | Accumulator 1 input
  zero_acc1 | Zeroing mask for acc1
  sub_mul | Negation mask of multiplication result
  sub_acc1 | Negation mask of acc1. If a bit is set the corresponding accumulator lane of acc1 is negated.

Returns
  Result of operation

## ◆ negmsc_4x4_4x4() [1/8]

v16acc64 negmsc_4x4_4x4 | ( | v32int16 | a,
|  | int | sgn_x,
|  | v32int16 | b,
|  | int | sgn_y,
|  | v16acc64 | acc1 )

Parameters

  a | Matrix A
  sgn_x | Sign mask for matrix A
  b | Matrix B
  sgn_y | Sign mask for matrix B
  acc1 | Accumulator 1 input

Returns
  Result of operation

## ◆ negmsc_4x4_4x4() [2/8]

v16acc64 negmsc_4x4_4x4 | ( | v32int16 | a,
|  | int | sgn_x,
|  | v32uint16 | b,
|  | int | sgn_y,
|  | v16acc64 | acc1 )

Parameters

  a | Matrix A
  sgn_x | Sign mask for matrix A
  b | Matrix B
  sgn_y | Sign mask for matrix B
  acc1 | Accumulator 1 input

Returns
  Result of operation

## ◆ negmsc_4x4_4x4() [3/8]

v16acc64 negmsc_4x4_4x4 | ( | v32int16 | a,
|  | v32int16 | b,
|  | v16acc64 | acc1 )

Parameters

  a | Matrix A
  b | Matrix B
  acc1 | Accumulator 1 input

Returns
  Result of operation

## ◆ negmsc_4x4_4x4() [4/8]

v16acc64 negmsc_4x4_4x4 | ( | v32int16 | a,
|  | v32uint16 | b,
|  | v16acc64 | acc1 )

Parameters

  a | Matrix A
  b | Matrix B
  acc1 | Accumulator 1 input

Returns
  Result of operation

## ◆ negmsc_4x4_4x4() [5/8]

v16acc64 negmsc_4x4_4x4 | ( | v32uint16 | a,
|  | int | sgn_x,
|  | v32int16 | b,
|  | int | sgn_y,
|  | v16acc64 | acc1 )

Parameters

  a | Matrix A
  sgn_x | Sign mask for matrix A
  b | Matrix B
  sgn_y | Sign mask for matrix B
  acc1 | Accumulator 1 input

Returns
  Result of operation

## ◆ negmsc_4x4_4x4() [6/8]

v16acc64 negmsc_4x4_4x4 | ( | v32uint16 | a,
|  | int | sgn_x,
|  | v32uint16 | b,
|  | int | sgn_y,
|  | v16acc64 | acc1 )

Parameters

  a | Matrix A
  sgn_x | Sign mask for matrix A
  b | Matrix B
  sgn_y | Sign mask for matrix B
  acc1 | Accumulator 1 input

Returns
  Result of operation

## ◆ negmsc_4x4_4x4() [7/8]

v16acc64 negmsc_4x4_4x4 | ( | v32uint16 | a,
|  | v32int16 | b,
|  | v16acc64 | acc1 )

Parameters

  a | Matrix A
  b | Matrix B
  acc1 | Accumulator 1 input

Returns
  Result of operation

## ◆ negmsc_4x4_4x4() [8/8]

v16acc64 negmsc_4x4_4x4 | ( | v32uint16 | a,
|  | v32uint16 | b,
|  | v16acc64 | acc1 )

Parameters

  a | Matrix A
  b | Matrix B
  acc1 | Accumulator 1 input

Returns
  Result of operation

## ◆ negmsc_4x4_4x4_conf() [1/8]

v16acc64 negmsc_4x4_4x4_conf | ( | v32int16 | a,
|  | int | sgn_x,
|  | v32int16 | b,
|  | int | sgn_y,
|  | v16acc64 | acc1,
|  | int | zero_acc1,
|  | int | sub_mul,
|  | int | sub_acc1 )

Parameters

  a | Matrix A
  sgn_x | Sign mask for matrix A
  b | Matrix B
  sgn_y | Sign mask for matrix B
  acc1 | Accumulator 1 input
  zero_acc1 | Zeroing mask for acc1
  sub_mul | Negation mask of multiplication result
  sub_acc1 | Negation mask of acc1

Returns
  Result of operation

## ◆ negmsc_4x4_4x4_conf() [2/8]

v16acc64 negmsc_4x4_4x4_conf | ( | v32int16 | a,
|  | int | sgn_x,
|  | v32uint16 | b,
|  | int | sgn_y,
|  | v16acc64 | acc1,
|  | int | zero_acc1,
|  | int | sub_mul,
|  | int | sub_acc1 )

Parameters

  a | Matrix A
  sgn_x | Sign mask for matrix A
  b | Matrix B
  sgn_y | Sign mask for matrix B
  acc1 | Accumulator 1 input
  zero_acc1 | Zeroing mask for acc1
  sub_mul | Negation mask of multiplication result
  sub_acc1 | Negation mask of acc1

Returns
  Result of operation

## ◆ negmsc_4x4_4x4_conf() [3/8]

v16acc64 negmsc_4x4_4x4_conf | ( | v32int16 | a,
|  | v32int16 | b,
|  | v16acc64 | acc1,
|  | int | zero_acc1,
|  | int | sub_mul,
|  | int | sub_acc1 )

Parameters

  a | Matrix A
  b | Matrix B
  acc1 | Accumulator 1 input
  zero_acc1 | Zeroing mask for acc1
  sub_mul | Negation mask of multiplication result
  sub_acc1 | Negation mask of acc1. If a bit is set the corresponding accumulator lane of acc1 is negated.

Returns
  Result of operation

## ◆ negmsc_4x4_4x4_conf() [4/8]

v16acc64 negmsc_4x4_4x4_conf | ( | v32int16 | a,
|  | v32uint16 | b,
|  | v16acc64 | acc1,
|  | int | zero_acc1,
|  | int | sub_mul,
|  | int | sub_acc1 )

Parameters

  a | Matrix A
  b | Matrix B
  acc1 | Accumulator 1 input
  zero_acc1 | Zeroing mask for acc1
  sub_mul | Negation mask of multiplication result
  sub_acc1 | Negation mask of acc1. If a bit is set the corresponding accumulator lane of acc1 is negated.

Returns
  Result of operation

## ◆ negmsc_4x4_4x4_conf() [5/8]

v16acc64 negmsc_4x4_4x4_conf | ( | v32uint16 | a,
|  | int | sgn_x,
|  | v32int16 | b,
|  | int | sgn_y,
|  | v16acc64 | acc1,
|  | int | zero_acc1,
|  | int | sub_mul,
|  | int | sub_acc1 )

Parameters

  a | Matrix A
  sgn_x | Sign mask for matrix A
  b | Matrix B
  sgn_y | Sign mask for matrix B
  acc1 | Accumulator 1 input
  zero_acc1 | Zeroing mask for acc1
  sub_mul | Negation mask of multiplication result
  sub_acc1 | Negation mask of acc1

Returns
  Result of operation

## ◆ negmsc_4x4_4x4_conf() [6/8]

v16acc64 negmsc_4x4_4x4_conf | ( | v32uint16 | a,
|  | int | sgn_x,
|  | v32uint16 | b,
|  | int | sgn_y,
|  | v16acc64 | acc1,
|  | int | zero_acc1,
|  | int | sub_mul,
|  | int | sub_acc1 )

Parameters

  a | Matrix A
  sgn_x | Sign mask for matrix A
  b | Matrix B
  sgn_y | Sign mask for matrix B
  acc1 | Accumulator 1 input
  zero_acc1 | Zeroing mask for acc1
  sub_mul | Negation mask of multiplication result
  sub_acc1 | Negation mask of acc1

Returns
  Result of operation

## ◆ negmsc_4x4_4x4_conf() [7/8]

v16acc64 negmsc_4x4_4x4_conf | ( | v32uint16 | a,
|  | v32int16 | b,
|  | v16acc64 | acc1,
|  | int | zero_acc1,
|  | int | sub_mul,
|  | int | sub_acc1 )

Parameters

  a | Matrix A
  b | Matrix B
  acc1 | Accumulator 1 input
  zero_acc1 | Zeroing mask for acc1
  sub_mul | Negation mask of multiplication result
  sub_acc1 | Negation mask of acc1. If a bit is set the corresponding accumulator lane of acc1 is negated.

Returns
  Result of operation

## ◆ negmsc_4x4_4x4_conf() [8/8]

v16acc64 negmsc_4x4_4x4_conf | ( | v32uint16 | a,
|  | v32uint16 | b,
|  | v16acc64 | acc1,
|  | int | zero_acc1,
|  | int | sub_mul,
|  | int | sub_acc1 )

Parameters

  a | Matrix A
  b | Matrix B
  acc1 | Accumulator 1 input
  zero_acc1 | Zeroing mask for acc1
  sub_mul | Negation mask of multiplication result
  sub_acc1 | Negation mask of acc1. If a bit is set the corresponding accumulator lane of acc1 is negated.

Returns
  Result of operation

## ◆ negmsc_conv_16x4() [1/8]

v16acc64 negmsc_conv_16x4 | ( | v32int16 | a,
|  | int | sgn_x,
|  | v32int16 | b,
|  | int | sgn_y,
|  | v16acc64 | acc1 )

Parameters

  a | Matrix A
  sgn_x | Sign mask for matrix A
  b | Matrix B
  sgn_y | Sign mask for matrix B
  acc1 | Accumulator 1 input

Returns
  Result of operation

## ◆ negmsc_conv_16x4() [2/8]

v16acc64 negmsc_conv_16x4 | ( | v32int16 | a,
|  | int | sgn_x,
|  | v32uint16 | b,
|  | int | sgn_y,
|  | v16acc64 | acc1 )

Parameters

  a | Matrix A
  sgn_x | Sign mask for matrix A
  b | Matrix B
  sgn_y | Sign mask for matrix B
  acc1 | Accumulator 1 input

Returns
  Result of operation

## ◆ negmsc_conv_16x4() [3/8]

v16acc64 negmsc_conv_16x4 | ( | v32int16 | a,
|  | v32int16 | b,
|  | v16acc64 | acc1 )

Parameters

  a | Matrix A
  b | Matrix B
  acc1 | Accumulator 1 input

Returns
  Result of operation

## ◆ negmsc_conv_16x4() [4/8]

v16acc64 negmsc_conv_16x4 | ( | v32int16 | a,
|  | v32uint16 | b,
|  | v16acc64 | acc1 )

Parameters

  a | Matrix A
  b | Matrix B
  acc1 | Accumulator 1 input

Returns
  Result of operation

## ◆ negmsc_conv_16x4() [5/8]

v16acc64 negmsc_conv_16x4 | ( | v32uint16 | a,
|  | int | sgn_x,
|  | v32int16 | b,
|  | int | sgn_y,
|  | v16acc64 | acc1 )

Parameters

  a | Matrix A
  sgn_x | Sign mask for matrix A
  b | Matrix B
  sgn_y | Sign mask for matrix B
  acc1 | Accumulator 1 input

Returns
  Result of operation

## ◆ negmsc_conv_16x4() [6/8]

v16acc64 negmsc_conv_16x4 | ( | v32uint16 | a,
|  | int | sgn_x,
|  | v32uint16 | b,
|  | int | sgn_y,
|  | v16acc64 | acc1 )

Parameters

  a | Matrix A
  sgn_x | Sign mask for matrix A
  b | Matrix B
  sgn_y | Sign mask for matrix B
  acc1 | Accumulator 1 input

Returns
  Result of operation

## ◆ negmsc_conv_16x4() [7/8]

v16acc64 negmsc_conv_16x4 | ( | v32uint16 | a,
|  | v32int16 | b,
|  | v16acc64 | acc1 )

Parameters

  a | Matrix A
  b | Matrix B
  acc1 | Accumulator 1 input

Returns
  Result of operation

## ◆ negmsc_conv_16x4() [8/8]

v16acc64 negmsc_conv_16x4 | ( | v32uint16 | a,
|  | v32uint16 | b,
|  | v16acc64 | acc1 )

Parameters

  a | Matrix A
  b | Matrix B
  acc1 | Accumulator 1 input

Returns
  Result of operation

## ◆ negmsc_conv_16x4_conf() [1/8]

v16acc64 negmsc_conv_16x4_conf | ( | v32int16 | a,
|  | int | sgn_x,
|  | v32int16 | b,
|  | int | sgn_y,
|  | v16acc64 | acc1,
|  | int | zero_acc1,
|  | int | sub_mul,
|  | int | sub_acc1 )

Parameters

  a | Matrix A
  sgn_x | Sign mask for matrix A
  b | Matrix B
  sgn_y | Sign mask for matrix B
  acc1 | Accumulator 1 input
  zero_acc1 | Zeroing mask for acc1
  sub_mul | Negation mask of multiplication result
  sub_acc1 | Negation mask of acc1

Returns
  Result of operation

## ◆ negmsc_conv_16x4_conf() [2/8]

v16acc64 negmsc_conv_16x4_conf | ( | v32int16 | a,
|  | int | sgn_x,
|  | v32uint16 | b,
|  | int | sgn_y,
|  | v16acc64 | acc1,
|  | int | zero_acc1,
|  | int | sub_mul,
|  | int | sub_acc1 )

Parameters

  a | Matrix A
  sgn_x | Sign mask for matrix A
  b | Matrix B
  sgn_y | Sign mask for matrix B
  acc1 | Accumulator 1 input
  zero_acc1 | Zeroing mask for acc1
  sub_mul | Negation mask of multiplication result
  sub_acc1 | Negation mask of acc1

Returns
  Result of operation

## ◆ negmsc_conv_16x4_conf() [3/8]

v16acc64 negmsc_conv_16x4_conf | ( | v32int16 | a,
|  | v32int16 | b,
|  | v16acc64 | acc1,
|  | int | zero_acc1,
|  | int | sub_mul,
|  | int | sub_acc1 )

Parameters

  a | Matrix A
  b | Matrix B
  acc1 | Accumulator 1 input
  zero_acc1 | Zeroing mask for acc1
  sub_mul | Negation mask of multiplication result
  sub_acc1 | Negation mask of acc1. If a bit is set the corresponding accumulator lane of acc1 is negated.

Returns
  Result of operation

## ◆ negmsc_conv_16x4_conf() [4/8]

v16acc64 negmsc_conv_16x4_conf | ( | v32int16 | a,
|  | v32uint16 | b,
|  | v16acc64 | acc1,
|  | int | zero_acc1,
|  | int | sub_mul,
|  | int | sub_acc1 )

Parameters

  a | Matrix A
  b | Matrix B
  acc1 | Accumulator 1 input
  zero_acc1 | Zeroing mask for acc1
  sub_mul | Negation mask of multiplication result
  sub_acc1 | Negation mask of acc1. If a bit is set the corresponding accumulator lane of acc1 is negated.

Returns
  Result of operation

## ◆ negmsc_conv_16x4_conf() [5/8]

v16acc64 negmsc_conv_16x4_conf | ( | v32uint16 | a,
|  | int | sgn_x,
|  | v32int16 | b,
|  | int | sgn_y,
|  | v16acc64 | acc1,
|  | int | zero_acc1,
|  | int | sub_mul,
|  | int | sub_acc1 )

Parameters

  a | Matrix A
  sgn_x | Sign mask for matrix A
  b | Matrix B
  sgn_y | Sign mask for matrix B
  acc1 | Accumulator 1 input
  zero_acc1 | Zeroing mask for acc1
  sub_mul | Negation mask of multiplication result
  sub_acc1 | Negation mask of acc1

Returns
  Result of operation

## ◆ negmsc_conv_16x4_conf() [6/8]

v16acc64 negmsc_conv_16x4_conf | ( | v32uint16 | a,
|  | int | sgn_x,
|  | v32uint16 | b,
|  | int | sgn_y,
|  | v16acc64 | acc1,
|  | int | zero_acc1,
|  | int | sub_mul,
|  | int | sub_acc1 )

Parameters

  a | Matrix A
  sgn_x | Sign mask for matrix A
  b | Matrix B
  sgn_y | Sign mask for matrix B
  acc1 | Accumulator 1 input
  zero_acc1 | Zeroing mask for acc1
  sub_mul | Negation mask of multiplication result
  sub_acc1 | Negation mask of acc1

Returns
  Result of operation

## ◆ negmsc_conv_16x4_conf() [7/8]

v16acc64 negmsc_conv_16x4_conf | ( | v32uint16 | a,
|  | v32int16 | b,
|  | v16acc64 | acc1,
|  | int | zero_acc1,
|  | int | sub_mul,
|  | int | sub_acc1 )

Parameters

  a | Matrix A
  b | Matrix B
  acc1 | Accumulator 1 input
  zero_acc1 | Zeroing mask for acc1
  sub_mul | Negation mask of multiplication result
  sub_acc1 | Negation mask of acc1. If a bit is set the corresponding accumulator lane of acc1 is negated.

Returns
  Result of operation

## ◆ negmsc_conv_16x4_conf() [8/8]

v16acc64 negmsc_conv_16x4_conf | ( | v32uint16 | a,
|  | v32uint16 | b,
|  | v16acc64 | acc1,
|  | int | zero_acc1,
|  | int | sub_mul,
|  | int | sub_acc1 )

Parameters

  a | Matrix A
  b | Matrix B
  acc1 | Accumulator 1 input
  zero_acc1 | Zeroing mask for acc1
  sub_mul | Negation mask of multiplication result
  sub_acc1 | Negation mask of acc1. If a bit is set the corresponding accumulator lane of acc1 is negated.

Returns
  Result of operation

## ◆ negmsc_elem_16_2() [1/8]

v16acc64 negmsc_elem_16_2 | ( | v32int16 | a,
|  | int | sgn_x,
|  | v32int16 | b,
|  | int | sgn_y,
|  | v16acc64 | acc1 )

Parameters

  a | Matrix A
  sgn_x | Sign mask for matrix A
  b | Matrix B
  sgn_y | Sign mask for matrix B
  acc1 | Accumulator 1 input

Returns
  Result of operation

## ◆ negmsc_elem_16_2() [2/8]

v16acc64 negmsc_elem_16_2 | ( | v32int16 | a,
|  | int | sgn_x,
|  | v32uint16 | b,
|  | int | sgn_y,
|  | v16acc64 | acc1 )

Parameters

  a | Matrix A
  sgn_x | Sign mask for matrix A
  b | Matrix B
  sgn_y | Sign mask for matrix B
  acc1 | Accumulator 1 input

Returns
  Result of operation

## ◆ negmsc_elem_16_2() [3/8]

v16acc64 negmsc_elem_16_2 | ( | v32int16 | a,
|  | v32int16 | b,
|  | v16acc64 | acc1 )

Parameters

  a | Matrix A
  b | Matrix B
  acc1 | Accumulator 1 input

Returns
  Result of operation

## ◆ negmsc_elem_16_2() [4/8]

v16acc64 negmsc_elem_16_2 | ( | v32int16 | a,
|  | v32uint16 | b,
|  | v16acc64 | acc1 )

Parameters

  a | Matrix A
  b | Matrix B
  acc1 | Accumulator 1 input

Returns
  Result of operation

## ◆ negmsc_elem_16_2() [5/8]

v16acc64 negmsc_elem_16_2 | ( | v32uint16 | a,
|  | int | sgn_x,
|  | v32int16 | b,
|  | int | sgn_y,
|  | v16acc64 | acc1 )

Parameters

  a | Matrix A
  sgn_x | Sign mask for matrix A
  b | Matrix B
  sgn_y | Sign mask for matrix B
  acc1 | Accumulator 1 input

Returns
  Result of operation

## ◆ negmsc_elem_16_2() [6/8]

v16acc64 negmsc_elem_16_2 | ( | v32uint16 | a,
|  | int | sgn_x,
|  | v32uint16 | b,
|  | int | sgn_y,
|  | v16acc64 | acc1 )

Parameters

  a | Matrix A
  sgn_x | Sign mask for matrix A
  b | Matrix B
  sgn_y | Sign mask for matrix B
  acc1 | Accumulator 1 input

Returns
  Result of operation

## ◆ negmsc_elem_16_2() [7/8]

v16acc64 negmsc_elem_16_2 | ( | v32uint16 | a,
|  | v32int16 | b,
|  | v16acc64 | acc1 )

Parameters

  a | Matrix A
  b | Matrix B
  acc1 | Accumulator 1 input

Returns
  Result of operation

## ◆ negmsc_elem_16_2() [8/8]

v16acc64 negmsc_elem_16_2 | ( | v32uint16 | a,
|  | v32uint16 | b,
|  | v16acc64 | acc1 )

Parameters

  a | Matrix A
  b | Matrix B
  acc1 | Accumulator 1 input

Returns
  Result of operation

## ◆ negmsc_elem_16_2_conf() [1/8]

v16acc64 negmsc_elem_16_2_conf | ( | v32int16 | a,
|  | int | sgn_x,
|  | v32int16 | b,
|  | int | sgn_y,
|  | v16acc64 | acc1,
|  | int | zero_acc1,
|  | int | sub_mul,
|  | int | sub_acc1 )

Parameters

  a | Matrix A
  sgn_x | Sign mask for matrix A
  b | Matrix B
  sgn_y | Sign mask for matrix B
  acc1 | Accumulator 1 input
  zero_acc1 | Zeroing mask for acc1
  sub_mul | Negation mask of multiplication result
  sub_acc1 | Negation mask of acc1

Returns
  Result of operation

## ◆ negmsc_elem_16_2_conf() [2/8]

v16acc64 negmsc_elem_16_2_conf | ( | v32int16 | a,
|  | int | sgn_x,
|  | v32uint16 | b,
|  | int | sgn_y,
|  | v16acc64 | acc1,
|  | int | zero_acc1,
|  | int | sub_mul,
|  | int | sub_acc1 )

Parameters

  a | Matrix A
  sgn_x | Sign mask for matrix A
  b | Matrix B
  sgn_y | Sign mask for matrix B
  acc1 | Accumulator 1 input
  zero_acc1 | Zeroing mask for acc1
  sub_mul | Negation mask of multiplication result
  sub_acc1 | Negation mask of acc1

Returns
  Result of operation

## ◆ negmsc_elem_16_2_conf() [3/8]

v16acc64 negmsc_elem_16_2_conf | ( | v32int16 | a,
|  | v32int16 | b,
|  | v16acc64 | acc1,
|  | int | zero_acc1,
|  | int | sub_mul,
|  | int | sub_acc1 )

Parameters

  a | Matrix A
  b | Matrix B
  acc1 | Accumulator 1 input
  zero_acc1 | Zeroing mask for acc1
  sub_mul | Negation mask of multiplication result
  sub_acc1 | Negation mask of acc1. If a bit is set the corresponding accumulator lane of acc1 is negated.

Returns
  Result of operation

## ◆ negmsc_elem_16_2_conf() [4/8]

v16acc64 negmsc_elem_16_2_conf | ( | v32int16 | a,
|  | v32uint16 | b,
|  | v16acc64 | acc1,
|  | int | zero_acc1,
|  | int | sub_mul,
|  | int | sub_acc1 )

Parameters

  a | Matrix A
  b | Matrix B
  acc1 | Accumulator 1 input
  zero_acc1 | Zeroing mask for acc1
  sub_mul | Negation mask of multiplication result
  sub_acc1 | Negation mask of acc1. If a bit is set the corresponding accumulator lane of acc1 is negated.

Returns
  Result of operation

## ◆ negmsc_elem_16_2_conf() [5/8]

v16acc64 negmsc_elem_16_2_conf | ( | v32uint16 | a,
|  | int | sgn_x,
|  | v32int16 | b,
|  | int | sgn_y,
|  | v16acc64 | acc1,
|  | int | zero_acc1,
|  | int | sub_mul,
|  | int | sub_acc1 )

Parameters

  a | Matrix A
  sgn_x | Sign mask for matrix A
  b | Matrix B
  sgn_y | Sign mask for matrix B
  acc1 | Accumulator 1 input
  zero_acc1 | Zeroing mask for acc1
  sub_mul | Negation mask of multiplication result
  sub_acc1 | Negation mask of acc1

Returns
  Result of operation

## ◆ negmsc_elem_16_2_conf() [6/8]

v16acc64 negmsc_elem_16_2_conf | ( | v32uint16 | a,
|  | int | sgn_x,
|  | v32uint16 | b,
|  | int | sgn_y,
|  | v16acc64 | acc1,
|  | int | zero_acc1,
|  | int | sub_mul,
|  | int | sub_acc1 )

Parameters

  a | Matrix A
  sgn_x | Sign mask for matrix A
  b | Matrix B
  sgn_y | Sign mask for matrix B
  acc1 | Accumulator 1 input
  zero_acc1 | Zeroing mask for acc1
  sub_mul | Negation mask of multiplication result
  sub_acc1 | Negation mask of acc1

Returns
  Result of operation

## ◆ negmsc_elem_16_2_conf() [7/8]

v16acc64 negmsc_elem_16_2_conf | ( | v32uint16 | a,
|  | v32int16 | b,
|  | v16acc64 | acc1,
|  | int | zero_acc1,
|  | int | sub_mul,
|  | int | sub_acc1 )

Parameters

  a | Matrix A
  b | Matrix B
  acc1 | Accumulator 1 input
  zero_acc1 | Zeroing mask for acc1
  sub_mul | Negation mask of multiplication result
  sub_acc1 | Negation mask of acc1. If a bit is set the corresponding accumulator lane of acc1 is negated.

Returns
  Result of operation

## ◆ negmsc_elem_16_2_conf() [8/8]

v16acc64 negmsc_elem_16_2_conf | ( | v32uint16 | a,
|  | v32uint16 | b,
|  | v16acc64 | acc1,
|  | int | zero_acc1,
|  | int | sub_mul,
|  | int | sub_acc1 )

Parameters

  a | Matrix A
  b | Matrix B
  acc1 | Accumulator 1 input
  zero_acc1 | Zeroing mask for acc1
  sub_mul | Negation mask of multiplication result
  sub_acc1 | Negation mask of acc1. If a bit is set the corresponding accumulator lane of acc1 is negated.

Returns
  Result of operation

## ◆ negmsc_elem_32() [1/8]

v32acc32 negmsc_elem_32 | ( | v32int16 | a,
|  | int | sgn_x,
|  | v32int16 | b,
|  | int | sgn_y,
|  | v32acc32 | acc1 )

Parameters

  a | Matrix A
  sgn_x | Sign mask for matrix A
  b | Matrix B
  sgn_y | Sign mask for matrix B
  acc1 | Accumulator 1 input

Returns
  Result of operation

## ◆ negmsc_elem_32() [2/8]

v32acc32 negmsc_elem_32 | ( | v32int16 | a,
|  | int | sgn_x,
|  | v32uint16 | b,
|  | int | sgn_y,
|  | v32acc32 | acc1 )

Parameters

  a | Matrix A
  sgn_x | Sign mask for matrix A
  b | Matrix B
  sgn_y | Sign mask for matrix B
  acc1 | Accumulator 1 input

Returns
  Result of operation

## ◆ negmsc_elem_32() [3/8]

v32acc32 negmsc_elem_32 | ( | v32int16 | a,
|  | v32int16 | b,
|  | v32acc32 | acc1 )

Parameters

  a | Matrix A
  b | Matrix B
  acc1 | Accumulator 1 input

Returns
  Result of operation

## ◆ negmsc_elem_32() [4/8]

v32acc32 negmsc_elem_32 | ( | v32int16 | a,
|  | v32uint16 | b,
|  | v32acc32 | acc1 )

Parameters

  a | Matrix A
  b | Matrix B
  acc1 | Accumulator 1 input

Returns
  Result of operation

## ◆ negmsc_elem_32() [5/8]

v32acc32 negmsc_elem_32 | ( | v32uint16 | a,
|  | int | sgn_x,
|  | v32int16 | b,
|  | int | sgn_y,
|  | v32acc32 | acc1 )

Parameters

  a | Matrix A
  sgn_x | Sign mask for matrix A
  b | Matrix B
  sgn_y | Sign mask for matrix B
  acc1 | Accumulator 1 input

Returns
  Result of operation

## ◆ negmsc_elem_32() [6/8]

v32acc32 negmsc_elem_32 | ( | v32uint16 | a,
|  | int | sgn_x,
|  | v32uint16 | b,
|  | int | sgn_y,
|  | v32acc32 | acc1 )

Parameters

  a | Matrix A
  sgn_x | Sign mask for matrix A
  b | Matrix B
  sgn_y | Sign mask for matrix B
  acc1 | Accumulator 1 input

Returns
  Result of operation

## ◆ negmsc_elem_32() [7/8]

v32acc32 negmsc_elem_32 | ( | v32uint16 | a,
|  | v32int16 | b,
|  | v32acc32 | acc1 )

Parameters

  a | Matrix A
  b | Matrix B
  acc1 | Accumulator 1 input

Returns
  Result of operation

## ◆ negmsc_elem_32() [8/8]

v32acc32 negmsc_elem_32 | ( | v32uint16 | a,
|  | v32uint16 | b,
|  | v32acc32 | acc1 )

Parameters

  a | Matrix A
  b | Matrix B
  acc1 | Accumulator 1 input

Returns
  Result of operation

## ◆ negmsc_elem_32_conf() [1/8]

v32acc32 negmsc_elem_32_conf | ( | v32int16 | a,
|  | int | sgn_x,
|  | v32int16 | b,
|  | int | sgn_y,
|  | v32acc32 | acc1,
|  | int | zero_acc1,
|  | int | sub_mul,
|  | int | sub_acc1 )

Parameters

  a | Matrix A
  sgn_x | Sign mask for matrix A
  b | Matrix B
  sgn_y | Sign mask for matrix B
  acc1 | Accumulator 1 input
  zero_acc1 | Zeroing mask for acc1
  sub_mul | Negation mask of multiplication result
  sub_acc1 | Negation mask of acc1

Returns
  Result of operation

## ◆ negmsc_elem_32_conf() [2/8]

v32acc32 negmsc_elem_32_conf | ( | v32int16 | a,
|  | int | sgn_x,
|  | v32uint16 | b,
|  | int | sgn_y,
|  | v32acc32 | acc1,
|  | int | zero_acc1,
|  | int | sub_mul,
|  | int | sub_acc1 )

Parameters

  a | Matrix A
  sgn_x | Sign mask for matrix A
  b | Matrix B
  sgn_y | Sign mask for matrix B
  acc1 | Accumulator 1 input
  zero_acc1 | Zeroing mask for acc1
  sub_mul | Negation mask of multiplication result
  sub_acc1 | Negation mask of acc1

Returns
  Result of operation

## ◆ negmsc_elem_32_conf() [3/8]

v32acc32 negmsc_elem_32_conf | ( | v32int16 | a,
|  | v32int16 | b,
|  | v32acc32 | acc1,
|  | int | zero_acc1,
|  | int | sub_mul,
|  | int | sub_acc1 )

Parameters

  a | Matrix A
  b | Matrix B
  acc1 | Accumulator 1 input
  zero_acc1 | Zeroing mask for acc1
  sub_mul | Negation mask of multiplication result
  sub_acc1 | Negation mask of acc1. If a bit is set the corresponding accumulator lane of acc1 is negated.

Returns
  Result of operation

## ◆ negmsc_elem_32_conf() [4/8]

v32acc32 negmsc_elem_32_conf | ( | v32int16 | a,
|  | v32uint16 | b,
|  | v32acc32 | acc1,
|  | int | zero_acc1,
|  | int | sub_mul,
|  | int | sub_acc1 )

Parameters

  a | Matrix A
  b | Matrix B
  acc1 | Accumulator 1 input
  zero_acc1 | Zeroing mask for acc1
  sub_mul | Negation mask of multiplication result
  sub_acc1 | Negation mask of acc1. If a bit is set the corresponding accumulator lane of acc1 is negated.

Returns
  Result of operation

## ◆ negmsc_elem_32_conf() [5/8]

v32acc32 negmsc_elem_32_conf | ( | v32uint16 | a,
|  | int | sgn_x,
|  | v32int16 | b,
|  | int | sgn_y,
|  | v32acc32 | acc1,
|  | int | zero_acc1,
|  | int | sub_mul,
|  | int | sub_acc1 )

Parameters

  a | Matrix A
  sgn_x | Sign mask for matrix A
  b | Matrix B
  sgn_y | Sign mask for matrix B
  acc1 | Accumulator 1 input
  zero_acc1 | Zeroing mask for acc1
  sub_mul | Negation mask of multiplication result
  sub_acc1 | Negation mask of acc1

Returns
  Result of operation

## ◆ negmsc_elem_32_conf() [6/8]

v32acc32 negmsc_elem_32_conf | ( | v32uint16 | a,
|  | int | sgn_x,
|  | v32uint16 | b,
|  | int | sgn_y,
|  | v32acc32 | acc1,
|  | int | zero_acc1,
|  | int | sub_mul,
|  | int | sub_acc1 )

Parameters

  a | Matrix A
  sgn_x | Sign mask for matrix A
  b | Matrix B
  sgn_y | Sign mask for matrix B
  acc1 | Accumulator 1 input
  zero_acc1 | Zeroing mask for acc1
  sub_mul | Negation mask of multiplication result
  sub_acc1 | Negation mask of acc1

Returns
  Result of operation

## ◆ negmsc_elem_32_conf() [7/8]

v32acc32 negmsc_elem_32_conf | ( | v32uint16 | a,
|  | v32int16 | b,
|  | v32acc32 | acc1,
|  | int | zero_acc1,
|  | int | sub_mul,
|  | int | sub_acc1 )

Parameters

  a | Matrix A
  b | Matrix B
  acc1 | Accumulator 1 input
  zero_acc1 | Zeroing mask for acc1
  sub_mul | Negation mask of multiplication result
  sub_acc1 | Negation mask of acc1. If a bit is set the corresponding accumulator lane of acc1 is negated.

Returns
  Result of operation

## ◆ negmsc_elem_32_conf() [8/8]

v32acc32 negmsc_elem_32_conf | ( | v32uint16 | a,
|  | v32uint16 | b,
|  | v32acc32 | acc1,
|  | int | zero_acc1,
|  | int | sub_mul,
|  | int | sub_acc1 )

Parameters

  a | Matrix A
  b | Matrix B
  acc1 | Accumulator 1 input
  zero_acc1 | Zeroing mask for acc1
  sub_mul | Negation mask of multiplication result
  sub_acc1 | Negation mask of acc1. If a bit is set the corresponding accumulator lane of acc1 is negated.

Returns
  Result of operation

## ◆ negmul_2x4_4x8() [1/8]

v16acc64 negmul_2x4_4x8 | ( | v32int16 | a,
|  | int | sgn_x,
|  | v32int16 | b,
|  | int | sgn_y )

Parameters

  a | Matrix A
  sgn_x | Sign mask for matrix A
  b | Matrix B
  sgn_y | Sign mask for matrix B

Returns
  Result of operation

## ◆ negmul_2x4_4x8() [2/8]

v16acc64 negmul_2x4_4x8 | ( | v32int16 | a,
|  | int | sgn_x,
|  | v32uint16 | b,
|  | int | sgn_y )

Parameters

  a | Matrix A
  sgn_x | Sign mask for matrix A
  b | Matrix B
  sgn_y | Sign mask for matrix B

Returns
  Result of operation

## ◆ negmul_2x4_4x8() [3/8]

v16acc64 negmul_2x4_4x8 | ( | v32int16 | a,
|  | v32int16 | b )

Parameters

  a | Matrix A
  b | Matrix B

Returns
  Result of operation

## ◆ negmul_2x4_4x8() [4/8]

v16acc64 negmul_2x4_4x8 | ( | v32int16 | a,
|  | v32uint16 | b )

Parameters

  a | Matrix A
  b | Matrix B

Returns
  Result of operation

## ◆ negmul_2x4_4x8() [5/8]

v16acc64 negmul_2x4_4x8 | ( | v32uint16 | a,
|  | int | sgn_x,
|  | v32int16 | b,
|  | int | sgn_y )

Parameters

  a | Matrix A
  sgn_x | Sign mask for matrix A
  b | Matrix B
  sgn_y | Sign mask for matrix B

Returns
  Result of operation

## ◆ negmul_2x4_4x8() [6/8]

v16acc64 negmul_2x4_4x8 | ( | v32uint16 | a,
|  | int | sgn_x,
|  | v32uint16 | b,
|  | int | sgn_y )

Parameters

  a | Matrix A
  sgn_x | Sign mask for matrix A
  b | Matrix B
  sgn_y | Sign mask for matrix B

Returns
  Result of operation

## ◆ negmul_2x4_4x8() [7/8]

v16acc64 negmul_2x4_4x8 | ( | v32uint16 | a,
|  | v32int16 | b )

Parameters

  a | Matrix A
  b | Matrix B

Returns
  Result of operation

## ◆ negmul_2x4_4x8() [8/8]

v16acc64 negmul_2x4_4x8 | ( | v32uint16 | a,
|  | v32uint16 | b )

Parameters

  a | Matrix A
  b | Matrix B

Returns
  Result of operation

## ◆ negmul_2x4_4x8_conf() [1/8]

v16acc64 negmul_2x4_4x8_conf | ( | v32int16 | a,
|  | int | sgn_x,
|  | v32int16 | b,
|  | int | sgn_y,
|  | int | sub_mul )

Parameters

  a | Matrix A
  sgn_x | Sign mask for matrix A
  b | Matrix B
  sgn_y | Sign mask for matrix B
  sub_mul | Negation mask of multiplication result

Returns
  Result of operation

## ◆ negmul_2x4_4x8_conf() [2/8]

v16acc64 negmul_2x4_4x8_conf | ( | v32int16 | a,
|  | int | sgn_x,
|  | v32uint16 | b,
|  | int | sgn_y,
|  | int | sub_mul )

Parameters

  a | Matrix A
  sgn_x | Sign mask for matrix A
  b | Matrix B
  sgn_y | Sign mask for matrix B
  sub_mul | Negation mask of multiplication result

Returns
  Result of operation

## ◆ negmul_2x4_4x8_conf() [3/8]

v16acc64 negmul_2x4_4x8_conf | ( | v32int16 | a,
|  | v32int16 | b,
|  | int | sub_mul )

Parameters

  a | Matrix A
  b | Matrix B
  sub_mul | Negation mask for multiplication result. If a bit of sub_mul is set the corresponding vector lane of the output accumulator will be negated.

Returns
  Result of operation

## ◆ negmul_2x4_4x8_conf() [4/8]

v16acc64 negmul_2x4_4x8_conf | ( | v32int16 | a,
|  | v32uint16 | b,
|  | int | sub_mul )

Parameters

  a | Matrix A
  b | Matrix B
  sub_mul | Negation mask for multiplication result. If a bit of sub_mul is set the corresponding vector lane of the output accumulator will be negated.

Returns
  Result of operation

## ◆ negmul_2x4_4x8_conf() [5/8]

v16acc64 negmul_2x4_4x8_conf | ( | v32uint16 | a,
|  | int | sgn_x,
|  | v32int16 | b,
|  | int | sgn_y,
|  | int | sub_mul )

Parameters

  a | Matrix A
  sgn_x | Sign mask for matrix A
  b | Matrix B
  sgn_y | Sign mask for matrix B
  sub_mul | Negation mask of multiplication result

Returns
  Result of operation

## ◆ negmul_2x4_4x8_conf() [6/8]

v16acc64 negmul_2x4_4x8_conf | ( | v32uint16 | a,
|  | int | sgn_x,
|  | v32uint16 | b,
|  | int | sgn_y,
|  | int | sub_mul )

Parameters

  a | Matrix A
  sgn_x | Sign mask for matrix A
  b | Matrix B
  sgn_y | Sign mask for matrix B
  sub_mul | Negation mask of multiplication result

Returns
  Result of operation

## ◆ negmul_2x4_4x8_conf() [7/8]

v16acc64 negmul_2x4_4x8_conf | ( | v32uint16 | a,
|  | v32int16 | b,
|  | int | sub_mul )

Parameters

  a | Matrix A
  b | Matrix B
  sub_mul | Negation mask for multiplication result. If a bit of sub_mul is set the corresponding vector lane of the output accumulator will be negated.

Returns
  Result of operation

## ◆ negmul_2x4_4x8_conf() [8/8]

v16acc64 negmul_2x4_4x8_conf | ( | v32uint16 | a,
|  | v32uint16 | b,
|  | int | sub_mul )

Parameters

  a | Matrix A
  b | Matrix B
  sub_mul | Negation mask for multiplication result. If a bit of sub_mul is set the corresponding vector lane of the output accumulator will be negated.

Returns
  Result of operation

## ◆ negmul_4x2_2x8() [1/8]

v32acc32 negmul_4x2_2x8 | ( | v32int16 | a,
|  | int | sgn_x,
|  | v32int16 | b,
|  | int | sgn_y )

Parameters

  a | Matrix A
  sgn_x | Sign mask for matrix A
  b | Matrix B
  sgn_y | Sign mask for matrix B

Returns
  Result of operation

## ◆ negmul_4x2_2x8() [2/8]

v32acc32 negmul_4x2_2x8 | ( | v32int16 | a,
|  | int | sgn_x,
|  | v32uint16 | b,
|  | int | sgn_y )

Parameters

  a | Matrix A
  sgn_x | Sign mask for matrix A
  b | Matrix B
  sgn_y | Sign mask for matrix B

Returns
  Result of operation

## ◆ negmul_4x2_2x8() [3/8]

v32acc32 negmul_4x2_2x8 | ( | v32int16 | a,
|  | v32int16 | b )

Parameters

  a | Matrix A
  b | Matrix B

Returns
  Result of operation

## ◆ negmul_4x2_2x8() [4/8]

v32acc32 negmul_4x2_2x8 | ( | v32int16 | a,
|  | v32uint16 | b )

Parameters

  a | Matrix A
  b | Matrix B

Returns
  Result of operation

## ◆ negmul_4x2_2x8() [5/8]

v32acc32 negmul_4x2_2x8 | ( | v32uint16 | a,
|  | int | sgn_x,
|  | v32int16 | b,
|  | int | sgn_y )

Parameters

  a | Matrix A
  sgn_x | Sign mask for matrix A
  b | Matrix B
  sgn_y | Sign mask for matrix B

Returns
  Result of operation

## ◆ negmul_4x2_2x8() [6/8]

v32acc32 negmul_4x2_2x8 | ( | v32uint16 | a,
|  | int | sgn_x,
|  | v32uint16 | b,
|  | int | sgn_y )

Parameters

  a | Matrix A
  sgn_x | Sign mask for matrix A
  b | Matrix B
  sgn_y | Sign mask for matrix B

Returns
  Result of operation

## ◆ negmul_4x2_2x8() [7/8]

v32acc32 negmul_4x2_2x8 | ( | v32uint16 | a,
|  | v32int16 | b )

Parameters

  a | Matrix A
  b | Matrix B

Returns
  Result of operation

## ◆ negmul_4x2_2x8() [8/8]

v32acc32 negmul_4x2_2x8 | ( | v32uint16 | a,
|  | v32uint16 | b )

Parameters

  a | Matrix A
  b | Matrix B

Returns
  Result of operation

## ◆ negmul_4x2_2x8_conf() [1/8]

v32acc32 negmul_4x2_2x8_conf | ( | v32int16 | a,
|  | int | sgn_x,
|  | v32int16 | b,
|  | int | sgn_y,
|  | int | sub_mul )

Parameters

  a | Matrix A
  sgn_x | Sign mask for matrix A
  b | Matrix B
  sgn_y | Sign mask for matrix B
  sub_mul | Negation mask of multiplication result

Returns
  Result of operation

## ◆ negmul_4x2_2x8_conf() [2/8]

v32acc32 negmul_4x2_2x8_conf | ( | v32int16 | a,
|  | int | sgn_x,
|  | v32uint16 | b,
|  | int | sgn_y,
|  | int | sub_mul )

Parameters

  a | Matrix A
  sgn_x | Sign mask for matrix A
  b | Matrix B
  sgn_y | Sign mask for matrix B
  sub_mul | Negation mask of multiplication result

Returns
  Result of operation

## ◆ negmul_4x2_2x8_conf() [3/8]

v32acc32 negmul_4x2_2x8_conf | ( | v32int16 | a,
|  | v32int16 | b,
|  | int | sub_mul )

Parameters

  a | Matrix A
  b | Matrix B
  sub_mul | Negation mask for multiplication result. If a bit of sub_mul is set the corresponding vector lane of the output accumulator will be negated.

Returns
  Result of operation

## ◆ negmul_4x2_2x8_conf() [4/8]

v32acc32 negmul_4x2_2x8_conf | ( | v32int16 | a,
|  | v32uint16 | b,
|  | int | sub_mul )

Parameters

  a | Matrix A
  b | Matrix B
  sub_mul | Negation mask for multiplication result. If a bit of sub_mul is set the corresponding vector lane of the output accumulator will be negated.

Returns
  Result of operation

## ◆ negmul_4x2_2x8_conf() [5/8]

v32acc32 negmul_4x2_2x8_conf | ( | v32uint16 | a,
|  | int | sgn_x,
|  | v32int16 | b,
|  | int | sgn_y,
|  | int | sub_mul )

Parameters

  a | Matrix A
  sgn_x | Sign mask for matrix A
  b | Matrix B
  sgn_y | Sign mask for matrix B
  sub_mul | Negation mask of multiplication result

Returns
  Result of operation

## ◆ negmul_4x2_2x8_conf() [6/8]

v32acc32 negmul_4x2_2x8_conf | ( | v32uint16 | a,
|  | int | sgn_x,
|  | v32uint16 | b,
|  | int | sgn_y,
|  | int | sub_mul )

Parameters

  a | Matrix A
  sgn_x | Sign mask for matrix A
  b | Matrix B
  sgn_y | Sign mask for matrix B
  sub_mul | Negation mask of multiplication result

Returns
  Result of operation

## ◆ negmul_4x2_2x8_conf() [7/8]

v32acc32 negmul_4x2_2x8_conf | ( | v32uint16 | a,
|  | v32int16 | b,
|  | int | sub_mul )

Parameters

  a | Matrix A
  b | Matrix B
  sub_mul | Negation mask for multiplication result. If a bit of sub_mul is set the corresponding vector lane of the output accumulator will be negated.

Returns
  Result of operation

## ◆ negmul_4x2_2x8_conf() [8/8]

v32acc32 negmul_4x2_2x8_conf | ( | v32uint16 | a,
|  | v32uint16 | b,
|  | int | sub_mul )

Parameters

  a | Matrix A
  b | Matrix B
  sub_mul | Negation mask for multiplication result. If a bit of sub_mul is set the corresponding vector lane of the output accumulator will be negated.

Returns
  Result of operation

## ◆ negmul_4x4_4x4() [1/8]

v16acc64 negmul_4x4_4x4 | ( | v32int16 | a,
|  | int | sgn_x,
|  | v32int16 | b,
|  | int | sgn_y )

Parameters

  a | Matrix A
  sgn_x | Sign mask for matrix A
  b | Matrix B
  sgn_y | Sign mask for matrix B

Returns
  Result of operation

## ◆ negmul_4x4_4x4() [2/8]

v16acc64 negmul_4x4_4x4 | ( | v32int16 | a,
|  | int | sgn_x,
|  | v32uint16 | b,
|  | int | sgn_y )

Parameters

  a | Matrix A
  sgn_x | Sign mask for matrix A
  b | Matrix B
  sgn_y | Sign mask for matrix B

Returns
  Result of operation

## ◆ negmul_4x4_4x4() [3/8]

v16acc64 negmul_4x4_4x4 | ( | v32int16 | a,
|  | v32int16 | b )

Parameters

  a | Matrix A
  b | Matrix B

Returns
  Result of operation

## ◆ negmul_4x4_4x4() [4/8]

v16acc64 negmul_4x4_4x4 | ( | v32int16 | a,
|  | v32uint16 | b )

Parameters

  a | Matrix A
  b | Matrix B

Returns
  Result of operation

## ◆ negmul_4x4_4x4() [5/8]

v16acc64 negmul_4x4_4x4 | ( | v32uint16 | a,
|  | int | sgn_x,
|  | v32int16 | b,
|  | int | sgn_y )

Parameters

  a | Matrix A
  sgn_x | Sign mask for matrix A
  b | Matrix B
  sgn_y | Sign mask for matrix B

Returns
  Result of operation

## ◆ negmul_4x4_4x4() [6/8]

v16acc64 negmul_4x4_4x4 | ( | v32uint16 | a,
|  | int | sgn_x,
|  | v32uint16 | b,
|  | int | sgn_y )

Parameters

  a | Matrix A
  sgn_x | Sign mask for matrix A
  b | Matrix B
  sgn_y | Sign mask for matrix B

Returns
  Result of operation

## ◆ negmul_4x4_4x4() [7/8]

v16acc64 negmul_4x4_4x4 | ( | v32uint16 | a,
|  | v32int16 | b )

Parameters

  a | Matrix A
  b | Matrix B

Returns
  Result of operation

## ◆ negmul_4x4_4x4() [8/8]

v16acc64 negmul_4x4_4x4 | ( | v32uint16 | a,
|  | v32uint16 | b )

Parameters

  a | Matrix A
  b | Matrix B

Returns
  Result of operation

## ◆ negmul_4x4_4x4_conf() [1/8]

v16acc64 negmul_4x4_4x4_conf | ( | v32int16 | a,
|  | int | sgn_x,
|  | v32int16 | b,
|  | int | sgn_y,
|  | int | sub_mul )

Parameters

  a | Matrix A
  sgn_x | Sign mask for matrix A
  b | Matrix B
  sgn_y | Sign mask for matrix B
  sub_mul | Negation mask of multiplication result

Returns
  Result of operation

## ◆ negmul_4x4_4x4_conf() [2/8]

v16acc64 negmul_4x4_4x4_conf | ( | v32int16 | a,
|  | int | sgn_x,
|  | v32uint16 | b,
|  | int | sgn_y,
|  | int | sub_mul )

Parameters

  a | Matrix A
  sgn_x | Sign mask for matrix A
  b | Matrix B
  sgn_y | Sign mask for matrix B
  sub_mul | Negation mask of multiplication result

Returns
  Result of operation

## ◆ negmul_4x4_4x4_conf() [3/8]

v16acc64 negmul_4x4_4x4_conf | ( | v32int16 | a,
|  | v32int16 | b,
|  | int | sub_mul )

Parameters

  a | Matrix A
  b | Matrix B
  sub_mul | Negation mask for multiplication result. If a bit of sub_mul is set the corresponding vector lane of the output accumulator will be negated.

Returns
  Result of operation

## ◆ negmul_4x4_4x4_conf() [4/8]

v16acc64 negmul_4x4_4x4_conf | ( | v32int16 | a,
|  | v32uint16 | b,
|  | int | sub_mul )

Parameters

  a | Matrix A
  b | Matrix B
  sub_mul | Negation mask for multiplication result. If a bit of sub_mul is set the corresponding vector lane of the output accumulator will be negated.

Returns
  Result of operation

## ◆ negmul_4x4_4x4_conf() [5/8]

v16acc64 negmul_4x4_4x4_conf | ( | v32uint16 | a,
|  | int | sgn_x,
|  | v32int16 | b,
|  | int | sgn_y,
|  | int | sub_mul )

Parameters

  a | Matrix A
  sgn_x | Sign mask for matrix A
  b | Matrix B
  sgn_y | Sign mask for matrix B
  sub_mul | Negation mask of multiplication result

Returns
  Result of operation

## ◆ negmul_4x4_4x4_conf() [6/8]

v16acc64 negmul_4x4_4x4_conf | ( | v32uint16 | a,
|  | int | sgn_x,
|  | v32uint16 | b,
|  | int | sgn_y,
|  | int | sub_mul )

Parameters

  a | Matrix A
  sgn_x | Sign mask for matrix A
  b | Matrix B
  sgn_y | Sign mask for matrix B
  sub_mul | Negation mask of multiplication result

Returns
  Result of operation

## ◆ negmul_4x4_4x4_conf() [7/8]

v16acc64 negmul_4x4_4x4_conf | ( | v32uint16 | a,
|  | v32int16 | b,
|  | int | sub_mul )

Parameters

  a | Matrix A
  b | Matrix B
  sub_mul | Negation mask for multiplication result. If a bit of sub_mul is set the corresponding vector lane of the output accumulator will be negated.

Returns
  Result of operation

## ◆ negmul_4x4_4x4_conf() [8/8]

v16acc64 negmul_4x4_4x4_conf | ( | v32uint16 | a,
|  | v32uint16 | b,
|  | int | sub_mul )

Parameters

  a | Matrix A
  b | Matrix B
  sub_mul | Negation mask for multiplication result. If a bit of sub_mul is set the corresponding vector lane of the output accumulator will be negated.

Returns
  Result of operation

## ◆ negmul_conv_16x4() [1/8]

v16acc64 negmul_conv_16x4 | ( | v32int16 | a,
|  | int | sgn_x,
|  | v32int16 | b,
|  | int | sgn_y )

Parameters

  a | Matrix A
  sgn_x | Sign mask for matrix A
  b | Matrix B
  sgn_y | Sign mask for matrix B

Returns
  Result of operation

## ◆ negmul_conv_16x4() [2/8]

v16acc64 negmul_conv_16x4 | ( | v32int16 | a,
|  | int | sgn_x,
|  | v32uint16 | b,
|  | int | sgn_y )

Parameters

  a | Matrix A
  sgn_x | Sign mask for matrix A
  b | Matrix B
  sgn_y | Sign mask for matrix B

Returns
  Result of operation

## ◆ negmul_conv_16x4() [3/8]

v16acc64 negmul_conv_16x4 | ( | v32int16 | a,
|  | v32int16 | b )

Parameters

  a | Matrix A
  b | Matrix B

Returns
  Result of operation

## ◆ negmul_conv_16x4() [4/8]

v16acc64 negmul_conv_16x4 | ( | v32int16 | a,
|  | v32uint16 | b )

Parameters

  a | Matrix A
  b | Matrix B

Returns
  Result of operation

## ◆ negmul_conv_16x4() [5/8]

v16acc64 negmul_conv_16x4 | ( | v32uint16 | a,
|  | int | sgn_x,
|  | v32int16 | b,
|  | int | sgn_y )

Parameters

  a | Matrix A
  sgn_x | Sign mask for matrix A
  b | Matrix B
  sgn_y | Sign mask for matrix B

Returns
  Result of operation

## ◆ negmul_conv_16x4() [6/8]

v16acc64 negmul_conv_16x4 | ( | v32uint16 | a,
|  | int | sgn_x,
|  | v32uint16 | b,
|  | int | sgn_y )

Parameters

  a | Matrix A
  sgn_x | Sign mask for matrix A
  b | Matrix B
  sgn_y | Sign mask for matrix B

Returns
  Result of operation

## ◆ negmul_conv_16x4() [7/8]

v16acc64 negmul_conv_16x4 | ( | v32uint16 | a,
|  | v32int16 | b )

Parameters

  a | Matrix A
  b | Matrix B

Returns
  Result of operation

## ◆ negmul_conv_16x4() [8/8]

v16acc64 negmul_conv_16x4 | ( | v32uint16 | a,
|  | v32uint16 | b )

Parameters

  a | Matrix A
  b | Matrix B

Returns
  Result of operation

## ◆ negmul_conv_16x4_conf() [1/8]

v16acc64 negmul_conv_16x4_conf | ( | v32int16 | a,
|  | int | sgn_x,
|  | v32int16 | b,
|  | int | sgn_y,
|  | int | sub_mul )

Parameters

  a | Matrix A
  sgn_x | Sign mask for matrix A
  b | Matrix B
  sgn_y | Sign mask for matrix B
  sub_mul | Negation mask of multiplication result

Returns
  Result of operation

## ◆ negmul_conv_16x4_conf() [2/8]

v16acc64 negmul_conv_16x4_conf | ( | v32int16 | a,
|  | int | sgn_x,
|  | v32uint16 | b,
|  | int | sgn_y,
|  | int | sub_mul )

Parameters

  a | Matrix A
  sgn_x | Sign mask for matrix A
  b | Matrix B
  sgn_y | Sign mask for matrix B
  sub_mul | Negation mask of multiplication result

Returns
  Result of operation

## ◆ negmul_conv_16x4_conf() [3/8]

v16acc64 negmul_conv_16x4_conf | ( | v32int16 | a,
|  | v32int16 | b,
|  | int | sub_mul )

Parameters

  a | Matrix A
  b | Matrix B
  sub_mul | Negation mask for multiplication result. If a bit of sub_mul is set the corresponding vector lane of the output accumulator will be negated.

Returns
  Result of operation

## ◆ negmul_conv_16x4_conf() [4/8]

v16acc64 negmul_conv_16x4_conf | ( | v32int16 | a,
|  | v32uint16 | b,
|  | int | sub_mul )

Parameters

  a | Matrix A
  b | Matrix B
  sub_mul | Negation mask for multiplication result. If a bit of sub_mul is set the corresponding vector lane of the output accumulator will be negated.

Returns
  Result of operation

## ◆ negmul_conv_16x4_conf() [5/8]

v16acc64 negmul_conv_16x4_conf | ( | v32uint16 | a,
|  | int | sgn_x,
|  | v32int16 | b,
|  | int | sgn_y,
|  | int | sub_mul )

Parameters

  a | Matrix A
  sgn_x | Sign mask for matrix A
  b | Matrix B
  sgn_y | Sign mask for matrix B
  sub_mul | Negation mask of multiplication result

Returns
  Result of operation

## ◆ negmul_conv_16x4_conf() [6/8]

v16acc64 negmul_conv_16x4_conf | ( | v32uint16 | a,
|  | int | sgn_x,
|  | v32uint16 | b,
|  | int | sgn_y,
|  | int | sub_mul )

Parameters

  a | Matrix A
  sgn_x | Sign mask for matrix A
  b | Matrix B
  sgn_y | Sign mask for matrix B
  sub_mul | Negation mask of multiplication result

Returns
  Result of operation

## ◆ negmul_conv_16x4_conf() [7/8]

v16acc64 negmul_conv_16x4_conf | ( | v32uint16 | a,
|  | v32int16 | b,
|  | int | sub_mul )

Parameters

  a | Matrix A
  b | Matrix B
  sub_mul | Negation mask for multiplication result. If a bit of sub_mul is set the corresponding vector lane of the output accumulator will be negated.

Returns
  Result of operation

## ◆ negmul_conv_16x4_conf() [8/8]

v16acc64 negmul_conv_16x4_conf | ( | v32uint16 | a,
|  | v32uint16 | b,
|  | int | sub_mul )

Parameters

  a | Matrix A
  b | Matrix B
  sub_mul | Negation mask for multiplication result. If a bit of sub_mul is set the corresponding vector lane of the output accumulator will be negated.

Returns
  Result of operation

## ◆ negmul_elem_16_2() [1/9]

v16accfloat negmul_elem_16_2 | ( | v32bfloat16 | a,
|  | v32bfloat16 | b )

Parameters

  a | Matrix A
  b | Matrix B

Returns
  Result of operation

## ◆ negmul_elem_16_2() [2/9]

v16acc64 negmul_elem_16_2 | ( | v32int16 | a,
|  | int | sgn_x,
|  | v32int16 | b,
|  | int | sgn_y )

Parameters

  a | Matrix A
  sgn_x | Sign mask for matrix A
  b | Matrix B
  sgn_y | Sign mask for matrix B

Returns
  Result of operation

## ◆ negmul_elem_16_2() [3/9]

v16acc64 negmul_elem_16_2 | ( | v32int16 | a,
|  | int | sgn_x,
|  | v32uint16 | b,
|  | int | sgn_y )

Parameters

  a | Matrix A
  sgn_x | Sign mask for matrix A
  b | Matrix B
  sgn_y | Sign mask for matrix B

Returns
  Result of operation

## ◆ negmul_elem_16_2() [4/9]

v16acc64 negmul_elem_16_2 | ( | v32int16 | a,
|  | v32int16 | b )

Parameters

  a | Matrix A
  b | Matrix B

Returns
  Result of operation

## ◆ negmul_elem_16_2() [5/9]

v16acc64 negmul_elem_16_2 | ( | v32int16 | a,
|  | v32uint16 | b )

Parameters

  a | Matrix A
  b | Matrix B

Returns
  Result of operation

## ◆ negmul_elem_16_2() [6/9]

v16acc64 negmul_elem_16_2 | ( | v32uint16 | a,
|  | int | sgn_x,
|  | v32int16 | b,
|  | int | sgn_y )

Parameters

  a | Matrix A
  sgn_x | Sign mask for matrix A
  b | Matrix B
  sgn_y | Sign mask for matrix B

Returns
  Result of operation

## ◆ negmul_elem_16_2() [7/9]

v16acc64 negmul_elem_16_2 | ( | v32uint16 | a,
|  | int | sgn_x,
|  | v32uint16 | b,
|  | int | sgn_y )

Parameters

  a | Matrix A
  sgn_x | Sign mask for matrix A
  b | Matrix B
  sgn_y | Sign mask for matrix B

Returns
  Result of operation

## ◆ negmul_elem_16_2() [8/9]

v16acc64 negmul_elem_16_2 | ( | v32uint16 | a,
|  | v32int16 | b )

Parameters

  a | Matrix A
  b | Matrix B

Returns
  Result of operation

## ◆ negmul_elem_16_2() [9/9]

v16acc64 negmul_elem_16_2 | ( | v32uint16 | a,
|  | v32uint16 | b )

Parameters

  a | Matrix A
  b | Matrix B

Returns
  Result of operation

## ◆ negmul_elem_16_2_conf() [1/9]

v16accfloat negmul_elem_16_2_conf | ( | v32bfloat16 | a,
|  | v32bfloat16 | b,
|  | int | sub_mul )

Parameters

  a | Matrix A
  b | Matrix B
  sub_mul | Negation mask for multiplication result. If a bit of sub_mul is set the corresponding vector lane of the output accumulator will be negated.

Returns
  Result of operation

## ◆ negmul_elem_16_2_conf() [2/9]

v16acc64 negmul_elem_16_2_conf | ( | v32int16 | a,
|  | int | sgn_x,
|  | v32int16 | b,
|  | int | sgn_y,
|  | int | sub_mul )

Parameters

  a | Matrix A
  sgn_x | Sign mask for matrix A
  b | Matrix B
  sgn_y | Sign mask for matrix B
  sub_mul | Negation mask of multiplication result

Returns
  Result of operation

## ◆ negmul_elem_16_2_conf() [3/9]

v16acc64 negmul_elem_16_2_conf | ( | v32int16 | a,
|  | int | sgn_x,
|  | v32uint16 | b,
|  | int | sgn_y,
|  | int | sub_mul )

Parameters

  a | Matrix A
  sgn_x | Sign mask for matrix A
  b | Matrix B
  sgn_y | Sign mask for matrix B
  sub_mul | Negation mask of multiplication result

Returns
  Result of operation

## ◆ negmul_elem_16_2_conf() [4/9]

v16acc64 negmul_elem_16_2_conf | ( | v32int16 | a,
|  | v32int16 | b,
|  | int | sub_mul )

Parameters

  a | Matrix A
  b | Matrix B
  sub_mul | Negation mask for multiplication result. If a bit of sub_mul is set the corresponding vector lane of the output accumulator will be negated.

Returns
  Result of operation

## ◆ negmul_elem_16_2_conf() [5/9]

v16acc64 negmul_elem_16_2_conf | ( | v32int16 | a,
|  | v32uint16 | b,
|  | int | sub_mul )

Parameters

  a | Matrix A
  b | Matrix B
  sub_mul | Negation mask for multiplication result. If a bit of sub_mul is set the corresponding vector lane of the output accumulator will be negated.

Returns
  Result of operation

## ◆ negmul_elem_16_2_conf() [6/9]

v16acc64 negmul_elem_16_2_conf | ( | v32uint16 | a,
|  | int | sgn_x,
|  | v32int16 | b,
|  | int | sgn_y,
|  | int | sub_mul )

Parameters

  a | Matrix A
  sgn_x | Sign mask for matrix A
  b | Matrix B
  sgn_y | Sign mask for matrix B
  sub_mul | Negation mask of multiplication result

Returns
  Result of operation

## ◆ negmul_elem_16_2_conf() [7/9]

v16acc64 negmul_elem_16_2_conf | ( | v32uint16 | a,
|  | int | sgn_x,
|  | v32uint16 | b,
|  | int | sgn_y,
|  | int | sub_mul )

Parameters

  a | Matrix A
  sgn_x | Sign mask for matrix A
  b | Matrix B
  sgn_y | Sign mask for matrix B
  sub_mul | Negation mask of multiplication result

Returns
  Result of operation

## ◆ negmul_elem_16_2_conf() [8/9]

v16acc64 negmul_elem_16_2_conf | ( | v32uint16 | a,
|  | v32int16 | b,
|  | int | sub_mul )

Parameters

  a | Matrix A
  b | Matrix B
  sub_mul | Negation mask for multiplication result. If a bit of sub_mul is set the corresponding vector lane of the output accumulator will be negated.

Returns
  Result of operation

## ◆ negmul_elem_16_2_conf() [9/9]

v16acc64 negmul_elem_16_2_conf | ( | v32uint16 | a,
|  | v32uint16 | b,
|  | int | sub_mul )

Parameters

  a | Matrix A
  b | Matrix B
  sub_mul | Negation mask for multiplication result. If a bit of sub_mul is set the corresponding vector lane of the output accumulator will be negated.

Returns
  Result of operation

## ◆ negmul_elem_32() [1/8]

v32acc32 negmul_elem_32 | ( | v32int16 | a,
|  | int | sgn_x,
|  | v32int16 | b,
|  | int | sgn_y )

Parameters

  a | Matrix A
  sgn_x | Sign mask for matrix A
  b | Matrix B
  sgn_y | Sign mask for matrix B

Returns
  Result of operation

## ◆ negmul_elem_32() [2/8]

v32acc32 negmul_elem_32 | ( | v32int16 | a,
|  | int | sgn_x,
|  | v32uint16 | b,
|  | int | sgn_y )

Parameters

  a | Matrix A
  sgn_x | Sign mask for matrix A
  b | Matrix B
  sgn_y | Sign mask for matrix B

Returns
  Result of operation

## ◆ negmul_elem_32() [3/8]

v32acc32 negmul_elem_32 | ( | v32int16 | a,
|  | v32int16 | b )

Parameters

  a | Matrix A
  b | Matrix B

Returns
  Result of operation

## ◆ negmul_elem_32() [4/8]

v32acc32 negmul_elem_32 | ( | v32int16 | a,
|  | v32uint16 | b )

Parameters

  a | Matrix A
  b | Matrix B

Returns
  Result of operation

## ◆ negmul_elem_32() [5/8]

v32acc32 negmul_elem_32 | ( | v32uint16 | a,
|  | int | sgn_x,
|  | v32int16 | b,
|  | int | sgn_y )

Parameters

  a | Matrix A
  sgn_x | Sign mask for matrix A
  b | Matrix B
  sgn_y | Sign mask for matrix B

Returns
  Result of operation

## ◆ negmul_elem_32() [6/8]

v32acc32 negmul_elem_32 | ( | v32uint16 | a,
|  | int | sgn_x,
|  | v32uint16 | b,
|  | int | sgn_y )

Parameters

  a | Matrix A
  sgn_x | Sign mask for matrix A
  b | Matrix B
  sgn_y | Sign mask for matrix B

Returns
  Result of operation

## ◆ negmul_elem_32() [7/8]

v32acc32 negmul_elem_32 | ( | v32uint16 | a,
|  | v32int16 | b )

Parameters

  a | Matrix A
  b | Matrix B

Returns
  Result of operation

## ◆ negmul_elem_32() [8/8]

v32acc32 negmul_elem_32 | ( | v32uint16 | a,
|  | v32uint16 | b )

Parameters

  a | Matrix A
  b | Matrix B

Returns
  Result of operation

## ◆ negmul_elem_32_conf() [1/8]

v32acc32 negmul_elem_32_conf | ( | v32int16 | a,
|  | int | sgn_x,
|  | v32int16 | b,
|  | int | sgn_y,
|  | int | sub_mul )

Parameters

  a | Matrix A
  sgn_x | Sign mask for matrix A
  b | Matrix B
  sgn_y | Sign mask for matrix B
  sub_mul | Negation mask of multiplication result

Returns
  Result of operation

## ◆ negmul_elem_32_conf() [2/8]

v32acc32 negmul_elem_32_conf | ( | v32int16 | a,
|  | int | sgn_x,
|  | v32uint16 | b,
|  | int | sgn_y,
|  | int | sub_mul )

Parameters

  a | Matrix A
  sgn_x | Sign mask for matrix A
  b | Matrix B
  sgn_y | Sign mask for matrix B
  sub_mul | Negation mask of multiplication result

Returns
  Result of operation

## ◆ negmul_elem_32_conf() [3/8]

v32acc32 negmul_elem_32_conf | ( | v32int16 | a,
|  | v32int16 | b,
|  | int | sub_mul )

Parameters

  a | Matrix A
  b | Matrix B
  sub_mul | Negation mask for multiplication result. If a bit of sub_mul is set the corresponding vector lane of the output accumulator will be negated.

Returns
  Result of operation

## ◆ negmul_elem_32_conf() [4/8]

v32acc32 negmul_elem_32_conf | ( | v32int16 | a,
|  | v32uint16 | b,
|  | int | sub_mul )

Parameters

  a | Matrix A
  b | Matrix B
  sub_mul | Negation mask for multiplication result. If a bit of sub_mul is set the corresponding vector lane of the output accumulator will be negated.

Returns
  Result of operation

## ◆ negmul_elem_32_conf() [5/8]

v32acc32 negmul_elem_32_conf | ( | v32uint16 | a,
|  | int | sgn_x,
|  | v32int16 | b,
|  | int | sgn_y,
|  | int | sub_mul )

Parameters

  a | Matrix A
  sgn_x | Sign mask for matrix A
  b | Matrix B
  sgn_y | Sign mask for matrix B
  sub_mul | Negation mask of multiplication result

Returns
  Result of operation

## ◆ negmul_elem_32_conf() [6/8]

v32acc32 negmul_elem_32_conf | ( | v32uint16 | a,
|  | int | sgn_x,
|  | v32uint16 | b,
|  | int | sgn_y,
|  | int | sub_mul )

Parameters

  a | Matrix A
  sgn_x | Sign mask for matrix A
  b | Matrix B
  sgn_y | Sign mask for matrix B
  sub_mul | Negation mask of multiplication result

Returns
  Result of operation

## ◆ negmul_elem_32_conf() [7/8]

v32acc32 negmul_elem_32_conf | ( | v32uint16 | a,
|  | v32int16 | b,
|  | int | sub_mul )

Parameters

  a | Matrix A
  b | Matrix B
  sub_mul | Negation mask for multiplication result. If a bit of sub_mul is set the corresponding vector lane of the output accumulator will be negated.

Returns
  Result of operation

## ◆ negmul_elem_32_conf() [8/8]

v32acc32 negmul_elem_32_conf | ( | v32uint16 | a,
|  | v32uint16 | b,
|  | int | sub_mul )

Parameters

  a | Matrix A
  b | Matrix B
  sub_mul | Negation mask for multiplication result. If a bit of sub_mul is set the corresponding vector lane of the output accumulator will be negated.

Returns
  Result of operation

## ◆ submac_2x4_4x8() [1/8]

v16acc64 submac_2x4_4x8 | ( | v32int16 | a,
|  | int | sgn_x,
|  | v32int16 | b,
|  | int | sgn_y,
|  | v16acc64 | acc1,
|  | v16acc64 | acc2 )

Parameters

  a | Matrix A
  sgn_x | Sign mask for matrix A
  b | Matrix B
  sgn_y | Sign mask for matrix B
  acc1 | Accumulator 1 input
  acc2 | Accumulator 2 input

Returns
  Result of operation

## ◆ submac_2x4_4x8() [2/8]

v16acc64 submac_2x4_4x8 | ( | v32int16 | a,
|  | int | sgn_x,
|  | v32uint16 | b,
|  | int | sgn_y,
|  | v16acc64 | acc1,
|  | v16acc64 | acc2 )

Parameters

  a | Matrix A
  sgn_x | Sign mask for matrix A
  b | Matrix B
  sgn_y | Sign mask for matrix B
  acc1 | Accumulator 1 input
  acc2 | Accumulator 2 input

Returns
  Result of operation

## ◆ submac_2x4_4x8() [3/8]

v16acc64 submac_2x4_4x8 | ( | v32int16 | a,
|  | v32int16 | b,
|  | v16acc64 | acc1,
|  | v16acc64 | acc2 )

Parameters

  a | Matrix A
  b | Matrix B
  acc1 | Accumulator 1 input
  acc2 | Accumulator 2 input

Returns
  Result of operation

## ◆ submac_2x4_4x8() [4/8]

v16acc64 submac_2x4_4x8 | ( | v32int16 | a,
|  | v32uint16 | b,
|  | v16acc64 | acc1,
|  | v16acc64 | acc2 )

Parameters

  a | Matrix A
  b | Matrix B
  acc1 | Accumulator 1 input
  acc2 | Accumulator 2 input

Returns
  Result of operation

## ◆ submac_2x4_4x8() [5/8]

v16acc64 submac_2x4_4x8 | ( | v32uint16 | a,
|  | int | sgn_x,
|  | v32int16 | b,
|  | int | sgn_y,
|  | v16acc64 | acc1,
|  | v16acc64 | acc2 )

Parameters

  a | Matrix A
  sgn_x | Sign mask for matrix A
  b | Matrix B
  sgn_y | Sign mask for matrix B
  acc1 | Accumulator 1 input
  acc2 | Accumulator 2 input

Returns
  Result of operation

## ◆ submac_2x4_4x8() [6/8]

v16acc64 submac_2x4_4x8 | ( | v32uint16 | a,
|  | int | sgn_x,
|  | v32uint16 | b,
|  | int | sgn_y,
|  | v16acc64 | acc1,
|  | v16acc64 | acc2 )

Parameters

  a | Matrix A
  sgn_x | Sign mask for matrix A
  b | Matrix B
  sgn_y | Sign mask for matrix B
  acc1 | Accumulator 1 input
  acc2 | Accumulator 2 input

Returns
  Result of operation

## ◆ submac_2x4_4x8() [7/8]

v16acc64 submac_2x4_4x8 | ( | v32uint16 | a,
|  | v32int16 | b,
|  | v16acc64 | acc1,
|  | v16acc64 | acc2 )

Parameters

  a | Matrix A
  b | Matrix B
  acc1 | Accumulator 1 input
  acc2 | Accumulator 2 input

Returns
  Result of operation

## ◆ submac_2x4_4x8() [8/8]

v16acc64 submac_2x4_4x8 | ( | v32uint16 | a,
|  | v32uint16 | b,
|  | v16acc64 | acc1,
|  | v16acc64 | acc2 )

Parameters

  a | Matrix A
  b | Matrix B
  acc1 | Accumulator 1 input
  acc2 | Accumulator 2 input

Returns
  Result of operation

## ◆ submac_2x4_4x8_conf() [1/8]

v16acc64 submac_2x4_4x8_conf | ( | v32int16 | a,
|  | int | sgn_x,
|  | v32int16 | b,
|  | int | sgn_y,
|  | v16acc64 | acc1,
|  | v16acc64 | acc2,
|  | int | zero_acc1,
|  | int | sub_mul,
|  | int | sub_acc1,
|  | int | sub_acc2 )

Parameters

  a | Matrix A
  sgn_x | Sign mask for matrix A
  b | Matrix B
  sgn_y | Sign mask for matrix B
  acc1 | Accumulator 1 input
  acc2 | Accumulator 2 input
  zero_acc1 | Zeroing mask for acc1
  sub_mul | Negation mask of multiplication result
  sub_acc1 | Negation mask of acc1
  sub_acc2 | Negation mask of acc2

Returns
  Result of operation

## ◆ submac_2x4_4x8_conf() [2/8]

v16acc64 submac_2x4_4x8_conf | ( | v32int16 | a,
|  | int | sgn_x,
|  | v32uint16 | b,
|  | int | sgn_y,
|  | v16acc64 | acc1,
|  | v16acc64 | acc2,
|  | int | zero_acc1,
|  | int | sub_mul,
|  | int | sub_acc1,
|  | int | sub_acc2 )

Parameters

  a | Matrix A
  sgn_x | Sign mask for matrix A
  b | Matrix B
  sgn_y | Sign mask for matrix B
  acc1 | Accumulator 1 input
  acc2 | Accumulator 2 input
  zero_acc1 | Zeroing mask for acc1
  sub_mul | Negation mask of multiplication result
  sub_acc1 | Negation mask of acc1
  sub_acc2 | Negation mask of acc2

Returns
  Result of operation

## ◆ submac_2x4_4x8_conf() [3/8]

v16acc64 submac_2x4_4x8_conf | ( | v32int16 | a,
|  | v32int16 | b,
|  | v16acc64 | acc1,
|  | v16acc64 | acc2,
|  | int | zero_acc1,
|  | int | sub_mul,
|  | int | sub_acc1,
|  | int | sub_acc2 )

Parameters

  a | Matrix A
  b | Matrix B
  acc1 | Accumulator 1 input
  acc2 | Accumulator 2 input
  zero_acc1 | Zeroing mask for acc1
  sub_mul | Negation mask of multiplication result
  sub_acc1 | Negation mask of acc1
  sub_acc2 | Negation mask of acc2

Returns
  Result of operation

## ◆ submac_2x4_4x8_conf() [4/8]

v16acc64 submac_2x4_4x8_conf | ( | v32int16 | a,
|  | v32uint16 | b,
|  | v16acc64 | acc1,
|  | v16acc64 | acc2,
|  | int | zero_acc1,
|  | int | sub_mul,
|  | int | sub_acc1,
|  | int | sub_acc2 )

Parameters

  a | Matrix A
  b | Matrix B
  acc1 | Accumulator 1 input
  acc2 | Accumulator 2 input
  zero_acc1 | Zeroing mask for acc1
  sub_mul | Negation mask of multiplication result
  sub_acc1 | Negation mask of acc1
  sub_acc2 | Negation mask of acc2

Returns
  Result of operation

## ◆ submac_2x4_4x8_conf() [5/8]

v16acc64 submac_2x4_4x8_conf | ( | v32uint16 | a,
|  | int | sgn_x,
|  | v32int16 | b,
|  | int | sgn_y,
|  | v16acc64 | acc1,
|  | v16acc64 | acc2,
|  | int | zero_acc1,
|  | int | sub_mul,
|  | int | sub_acc1,
|  | int | sub_acc2 )

Parameters

  a | Matrix A
  sgn_x | Sign mask for matrix A
  b | Matrix B
  sgn_y | Sign mask for matrix B
  acc1 | Accumulator 1 input
  acc2 | Accumulator 2 input
  zero_acc1 | Zeroing mask for acc1
  sub_mul | Negation mask of multiplication result
  sub_acc1 | Negation mask of acc1
  sub_acc2 | Negation mask of acc2

Returns
  Result of operation

## ◆ submac_2x4_4x8_conf() [6/8]

v16acc64 submac_2x4_4x8_conf | ( | v32uint16 | a,
|  | int | sgn_x,
|  | v32uint16 | b,
|  | int | sgn_y,
|  | v16acc64 | acc1,
|  | v16acc64 | acc2,
|  | int | zero_acc1,
|  | int | sub_mul,
|  | int | sub_acc1,
|  | int | sub_acc2 )

Parameters

  a | Matrix A
  sgn_x | Sign mask for matrix A
  b | Matrix B
  sgn_y | Sign mask for matrix B
  acc1 | Accumulator 1 input
  acc2 | Accumulator 2 input
  zero_acc1 | Zeroing mask for acc1
  sub_mul | Negation mask of multiplication result
  sub_acc1 | Negation mask of acc1
  sub_acc2 | Negation mask of acc2

Returns
  Result of operation

## ◆ submac_2x4_4x8_conf() [7/8]

v16acc64 submac_2x4_4x8_conf | ( | v32uint16 | a,
|  | v32int16 | b,
|  | v16acc64 | acc1,
|  | v16acc64 | acc2,
|  | int | zero_acc1,
|  | int | sub_mul,
|  | int | sub_acc1,
|  | int | sub_acc2 )

Parameters

  a | Matrix A
  b | Matrix B
  acc1 | Accumulator 1 input
  acc2 | Accumulator 2 input
  zero_acc1 | Zeroing mask for acc1
  sub_mul | Negation mask of multiplication result
  sub_acc1 | Negation mask of acc1
  sub_acc2 | Negation mask of acc2

Returns
  Result of operation

## ◆ submac_2x4_4x8_conf() [8/8]

v16acc64 submac_2x4_4x8_conf | ( | v32uint16 | a,
|  | v32uint16 | b,
|  | v16acc64 | acc1,
|  | v16acc64 | acc2,
|  | int | zero_acc1,
|  | int | sub_mul,
|  | int | sub_acc1,
|  | int | sub_acc2 )

Parameters

  a | Matrix A
  b | Matrix B
  acc1 | Accumulator 1 input
  acc2 | Accumulator 2 input
  zero_acc1 | Zeroing mask for acc1
  sub_mul | Negation mask of multiplication result
  sub_acc1 | Negation mask of acc1
  sub_acc2 | Negation mask of acc2

Returns
  Result of operation

## ◆ submac_4x2_2x8() [1/8]

v32acc32 submac_4x2_2x8 | ( | v32int16 | a,
|  | int | sgn_x,
|  | v32int16 | b,
|  | int | sgn_y,
|  | v32acc32 | acc1,
|  | v32acc32 | acc2 )

Parameters

  a | Matrix A
  sgn_x | Sign mask for matrix A
  b | Matrix B
  sgn_y | Sign mask for matrix B
  acc1 | Accumulator 1 input
  acc2 | Accumulator 2 input

Returns
  Result of operation

## ◆ submac_4x2_2x8() [2/8]

v32acc32 submac_4x2_2x8 | ( | v32int16 | a,
|  | int | sgn_x,
|  | v32uint16 | b,
|  | int | sgn_y,
|  | v32acc32 | acc1,
|  | v32acc32 | acc2 )

Parameters

  a | Matrix A
  sgn_x | Sign mask for matrix A
  b | Matrix B
  sgn_y | Sign mask for matrix B
  acc1 | Accumulator 1 input
  acc2 | Accumulator 2 input

Returns
  Result of operation

## ◆ submac_4x2_2x8() [3/8]

v32acc32 submac_4x2_2x8 | ( | v32int16 | a,
|  | v32int16 | b,
|  | v32acc32 | acc1,
|  | v32acc32 | acc2 )

Parameters

  a | Matrix A
  b | Matrix B
  acc1 | Accumulator 1 input
  acc2 | Accumulator 2 input

Returns
  Result of operation

## ◆ submac_4x2_2x8() [4/8]

v32acc32 submac_4x2_2x8 | ( | v32int16 | a,
|  | v32uint16 | b,
|  | v32acc32 | acc1,
|  | v32acc32 | acc2 )

Parameters

  a | Matrix A
  b | Matrix B
  acc1 | Accumulator 1 input
  acc2 | Accumulator 2 input

Returns
  Result of operation

## ◆ submac_4x2_2x8() [5/8]

v32acc32 submac_4x2_2x8 | ( | v32uint16 | a,
|  | int | sgn_x,
|  | v32int16 | b,
|  | int | sgn_y,
|  | v32acc32 | acc1,
|  | v32acc32 | acc2 )

Parameters

  a | Matrix A
  sgn_x | Sign mask for matrix A
  b | Matrix B
  sgn_y | Sign mask for matrix B
  acc1 | Accumulator 1 input
  acc2 | Accumulator 2 input

Returns
  Result of operation

## ◆ submac_4x2_2x8() [6/8]

v32acc32 submac_4x2_2x8 | ( | v32uint16 | a,
|  | int | sgn_x,
|  | v32uint16 | b,
|  | int | sgn_y,
|  | v32acc32 | acc1,
|  | v32acc32 | acc2 )

Parameters

  a | Matrix A
  sgn_x | Sign mask for matrix A
  b | Matrix B
  sgn_y | Sign mask for matrix B
  acc1 | Accumulator 1 input
  acc2 | Accumulator 2 input

Returns
  Result of operation

## ◆ submac_4x2_2x8() [7/8]

v32acc32 submac_4x2_2x8 | ( | v32uint16 | a,
|  | v32int16 | b,
|  | v32acc32 | acc1,
|  | v32acc32 | acc2 )

Parameters

  a | Matrix A
  b | Matrix B
  acc1 | Accumulator 1 input
  acc2 | Accumulator 2 input

Returns
  Result of operation

## ◆ submac_4x2_2x8() [8/8]

v32acc32 submac_4x2_2x8 | ( | v32uint16 | a,
|  | v32uint16 | b,
|  | v32acc32 | acc1,
|  | v32acc32 | acc2 )

Parameters

  a | Matrix A
  b | Matrix B
  acc1 | Accumulator 1 input
  acc2 | Accumulator 2 input

Returns
  Result of operation

## ◆ submac_4x2_2x8_conf() [1/8]

v32acc32 submac_4x2_2x8_conf | ( | v32int16 | a,
|  | int | sgn_x,
|  | v32int16 | b,
|  | int | sgn_y,
|  | v32acc32 | acc1,
|  | v32acc32 | acc2,
|  | int | zero_acc1,
|  | int | sub_mul,
|  | int | sub_acc1,
|  | int | sub_acc2 )

Parameters

  a | Matrix A
  sgn_x | Sign mask for matrix A
  b | Matrix B
  sgn_y | Sign mask for matrix B
  acc1 | Accumulator 1 input
  acc2 | Accumulator 2 input
  zero_acc1 | Zeroing mask for acc1
  sub_mul | Negation mask of multiplication result
  sub_acc1 | Negation mask of acc1
  sub_acc2 | Negation mask of acc2

Returns
  Result of operation

## ◆ submac_4x2_2x8_conf() [2/8]

v32acc32 submac_4x2_2x8_conf | ( | v32int16 | a,
|  | int | sgn_x,
|  | v32uint16 | b,
|  | int | sgn_y,
|  | v32acc32 | acc1,
|  | v32acc32 | acc2,
|  | int | zero_acc1,
|  | int | sub_mul,
|  | int | sub_acc1,
|  | int | sub_acc2 )

Parameters

  a | Matrix A
  sgn_x | Sign mask for matrix A
  b | Matrix B
  sgn_y | Sign mask for matrix B
  acc1 | Accumulator 1 input
  acc2 | Accumulator 2 input
  zero_acc1 | Zeroing mask for acc1
  sub_mul | Negation mask of multiplication result
  sub_acc1 | Negation mask of acc1
  sub_acc2 | Negation mask of acc2

Returns
  Result of operation

## ◆ submac_4x2_2x8_conf() [3/8]

v32acc32 submac_4x2_2x8_conf | ( | v32int16 | a,
|  | v32int16 | b,
|  | v32acc32 | acc1,
|  | v32acc32 | acc2,
|  | int | zero_acc1,
|  | int | sub_mul,
|  | int | sub_acc1,
|  | int | sub_acc2 )

Parameters

  a | Matrix A
  b | Matrix B
  acc1 | Accumulator 1 input
  acc2 | Accumulator 2 input
  zero_acc1 | Zeroing mask for acc1
  sub_mul | Negation mask of multiplication result
  sub_acc1 | Negation mask of acc1
  sub_acc2 | Negation mask of acc2

Returns
  Result of operation

## ◆ submac_4x2_2x8_conf() [4/8]

v32acc32 submac_4x2_2x8_conf | ( | v32int16 | a,
|  | v32uint16 | b,
|  | v32acc32 | acc1,
|  | v32acc32 | acc2,
|  | int | zero_acc1,
|  | int | sub_mul,
|  | int | sub_acc1,
|  | int | sub_acc2 )

Parameters

  a | Matrix A
  b | Matrix B
  acc1 | Accumulator 1 input
  acc2 | Accumulator 2 input
  zero_acc1 | Zeroing mask for acc1
  sub_mul | Negation mask of multiplication result
  sub_acc1 | Negation mask of acc1
  sub_acc2 | Negation mask of acc2

Returns
  Result of operation

## ◆ submac_4x2_2x8_conf() [5/8]

v32acc32 submac_4x2_2x8_conf | ( | v32uint16 | a,
|  | int | sgn_x,
|  | v32int16 | b,
|  | int | sgn_y,
|  | v32acc32 | acc1,
|  | v32acc32 | acc2,
|  | int | zero_acc1,
|  | int | sub_mul,
|  | int | sub_acc1,
|  | int | sub_acc2 )

Parameters

  a | Matrix A
  sgn_x | Sign mask for matrix A
  b | Matrix B
  sgn_y | Sign mask for matrix B
  acc1 | Accumulator 1 input
  acc2 | Accumulator 2 input
  zero_acc1 | Zeroing mask for acc1
  sub_mul | Negation mask of multiplication result
  sub_acc1 | Negation mask of acc1
  sub_acc2 | Negation mask of acc2

Returns
  Result of operation

## ◆ submac_4x2_2x8_conf() [6/8]

v32acc32 submac_4x2_2x8_conf | ( | v32uint16 | a,
|  | int | sgn_x,
|  | v32uint16 | b,
|  | int | sgn_y,
|  | v32acc32 | acc1,
|  | v32acc32 | acc2,
|  | int | zero_acc1,
|  | int | sub_mul,
|  | int | sub_acc1,
|  | int | sub_acc2 )

Parameters

  a | Matrix A
  sgn_x | Sign mask for matrix A
  b | Matrix B
  sgn_y | Sign mask for matrix B
  acc1 | Accumulator 1 input
  acc2 | Accumulator 2 input
  zero_acc1 | Zeroing mask for acc1
  sub_mul | Negation mask of multiplication result
  sub_acc1 | Negation mask of acc1
  sub_acc2 | Negation mask of acc2

Returns
  Result of operation

## ◆ submac_4x2_2x8_conf() [7/8]

v32acc32 submac_4x2_2x8_conf | ( | v32uint16 | a,
|  | v32int16 | b,
|  | v32acc32 | acc1,
|  | v32acc32 | acc2,
|  | int | zero_acc1,
|  | int | sub_mul,
|  | int | sub_acc1,
|  | int | sub_acc2 )

Parameters

  a | Matrix A
  b | Matrix B
  acc1 | Accumulator 1 input
  acc2 | Accumulator 2 input
  zero_acc1 | Zeroing mask for acc1
  sub_mul | Negation mask of multiplication result
  sub_acc1 | Negation mask of acc1
  sub_acc2 | Negation mask of acc2

Returns
  Result of operation

## ◆ submac_4x2_2x8_conf() [8/8]

v32acc32 submac_4x2_2x8_conf | ( | v32uint16 | a,
|  | v32uint16 | b,
|  | v32acc32 | acc1,
|  | v32acc32 | acc2,
|  | int | zero_acc1,
|  | int | sub_mul,
|  | int | sub_acc1,
|  | int | sub_acc2 )

Parameters

  a | Matrix A
  b | Matrix B
  acc1 | Accumulator 1 input
  acc2 | Accumulator 2 input
  zero_acc1 | Zeroing mask for acc1
  sub_mul | Negation mask of multiplication result
  sub_acc1 | Negation mask of acc1
  sub_acc2 | Negation mask of acc2

Returns
  Result of operation

## ◆ submac_4x4_4x4() [1/8]

v16acc64 submac_4x4_4x4 | ( | v32int16 | a,
|  | int | sgn_x,
|  | v32int16 | b,
|  | int | sgn_y,
|  | v16acc64 | acc1,
|  | v16acc64 | acc2 )

Parameters

  a | Matrix A
  sgn_x | Sign mask for matrix A
  b | Matrix B
  sgn_y | Sign mask for matrix B
  acc1 | Accumulator 1 input
  acc2 | Accumulator 2 input

Returns
  Result of operation

## ◆ submac_4x4_4x4() [2/8]

v16acc64 submac_4x4_4x4 | ( | v32int16 | a,
|  | int | sgn_x,
|  | v32uint16 | b,
|  | int | sgn_y,
|  | v16acc64 | acc1,
|  | v16acc64 | acc2 )

Parameters

  a | Matrix A
  sgn_x | Sign mask for matrix A
  b | Matrix B
  sgn_y | Sign mask for matrix B
  acc1 | Accumulator 1 input
  acc2 | Accumulator 2 input

Returns
  Result of operation

## ◆ submac_4x4_4x4() [3/8]

v16acc64 submac_4x4_4x4 | ( | v32int16 | a,
|  | v32int16 | b,
|  | v16acc64 | acc1,
|  | v16acc64 | acc2 )

Parameters

  a | Matrix A
  b | Matrix B
  acc1 | Accumulator 1 input
  acc2 | Accumulator 2 input

Returns
  Result of operation

## ◆ submac_4x4_4x4() [4/8]

v16acc64 submac_4x4_4x4 | ( | v32int16 | a,
|  | v32uint16 | b,
|  | v16acc64 | acc1,
|  | v16acc64 | acc2 )

Parameters

  a | Matrix A
  b | Matrix B
  acc1 | Accumulator 1 input
  acc2 | Accumulator 2 input

Returns
  Result of operation

## ◆ submac_4x4_4x4() [5/8]

v16acc64 submac_4x4_4x4 | ( | v32uint16 | a,
|  | int | sgn_x,
|  | v32int16 | b,
|  | int | sgn_y,
|  | v16acc64 | acc1,
|  | v16acc64 | acc2 )

Parameters

  a | Matrix A
  sgn_x | Sign mask for matrix A
  b | Matrix B
  sgn_y | Sign mask for matrix B
  acc1 | Accumulator 1 input
  acc2 | Accumulator 2 input

Returns
  Result of operation

## ◆ submac_4x4_4x4() [6/8]

v16acc64 submac_4x4_4x4 | ( | v32uint16 | a,
|  | int | sgn_x,
|  | v32uint16 | b,
|  | int | sgn_y,
|  | v16acc64 | acc1,
|  | v16acc64 | acc2 )

Parameters

  a | Matrix A
  sgn_x | Sign mask for matrix A
  b | Matrix B
  sgn_y | Sign mask for matrix B
  acc1 | Accumulator 1 input
  acc2 | Accumulator 2 input

Returns
  Result of operation

## ◆ submac_4x4_4x4() [7/8]

v16acc64 submac_4x4_4x4 | ( | v32uint16 | a,
|  | v32int16 | b,
|  | v16acc64 | acc1,
|  | v16acc64 | acc2 )

Parameters

  a | Matrix A
  b | Matrix B
  acc1 | Accumulator 1 input
  acc2 | Accumulator 2 input

Returns
  Result of operation

## ◆ submac_4x4_4x4() [8/8]

v16acc64 submac_4x4_4x4 | ( | v32uint16 | a,
|  | v32uint16 | b,
|  | v16acc64 | acc1,
|  | v16acc64 | acc2 )

Parameters

  a | Matrix A
  b | Matrix B
  acc1 | Accumulator 1 input
  acc2 | Accumulator 2 input

Returns
  Result of operation

## ◆ submac_4x4_4x4_conf() [1/8]

v16acc64 submac_4x4_4x4_conf | ( | v32int16 | a,
|  | int | sgn_x,
|  | v32int16 | b,
|  | int | sgn_y,
|  | v16acc64 | acc1,
|  | v16acc64 | acc2,
|  | int | zero_acc1,
|  | int | sub_mul,
|  | int | sub_acc1,
|  | int | sub_acc2 )

Parameters

  a | Matrix A
  sgn_x | Sign mask for matrix A
  b | Matrix B
  sgn_y | Sign mask for matrix B
  acc1 | Accumulator 1 input
  acc2 | Accumulator 2 input
  zero_acc1 | Zeroing mask for acc1
  sub_mul | Negation mask of multiplication result
  sub_acc1 | Negation mask of acc1
  sub_acc2 | Negation mask of acc2

Returns
  Result of operation

## ◆ submac_4x4_4x4_conf() [2/8]

v16acc64 submac_4x4_4x4_conf | ( | v32int16 | a,
|  | int | sgn_x,
|  | v32uint16 | b,
|  | int | sgn_y,
|  | v16acc64 | acc1,
|  | v16acc64 | acc2,
|  | int | zero_acc1,
|  | int | sub_mul,
|  | int | sub_acc1,
|  | int | sub_acc2 )

Parameters

  a | Matrix A
  sgn_x | Sign mask for matrix A
  b | Matrix B
  sgn_y | Sign mask for matrix B
  acc1 | Accumulator 1 input
  acc2 | Accumulator 2 input
  zero_acc1 | Zeroing mask for acc1
  sub_mul | Negation mask of multiplication result
  sub_acc1 | Negation mask of acc1
  sub_acc2 | Negation mask of acc2

Returns
  Result of operation

## ◆ submac_4x4_4x4_conf() [3/8]

v16acc64 submac_4x4_4x4_conf | ( | v32int16 | a,
|  | v32int16 | b,
|  | v16acc64 | acc1,
|  | v16acc64 | acc2,
|  | int | zero_acc1,
|  | int | sub_mul,
|  | int | sub_acc1,
|  | int | sub_acc2 )

Parameters

  a | Matrix A
  b | Matrix B
  acc1 | Accumulator 1 input
  acc2 | Accumulator 2 input
  zero_acc1 | Zeroing mask for acc1
  sub_mul | Negation mask of multiplication result
  sub_acc1 | Negation mask of acc1
  sub_acc2 | Negation mask of acc2

Returns
  Result of operation

## ◆ submac_4x4_4x4_conf() [4/8]

v16acc64 submac_4x4_4x4_conf | ( | v32int16 | a,
|  | v32uint16 | b,
|  | v16acc64 | acc1,
|  | v16acc64 | acc2,
|  | int | zero_acc1,
|  | int | sub_mul,
|  | int | sub_acc1,
|  | int | sub_acc2 )

Parameters

  a | Matrix A
  b | Matrix B
  acc1 | Accumulator 1 input
  acc2 | Accumulator 2 input
  zero_acc1 | Zeroing mask for acc1
  sub_mul | Negation mask of multiplication result
  sub_acc1 | Negation mask of acc1
  sub_acc2 | Negation mask of acc2

Returns
  Result of operation

## ◆ submac_4x4_4x4_conf() [5/8]

v16acc64 submac_4x4_4x4_conf | ( | v32uint16 | a,
|  | int | sgn_x,
|  | v32int16 | b,
|  | int | sgn_y,
|  | v16acc64 | acc1,
|  | v16acc64 | acc2,
|  | int | zero_acc1,
|  | int | sub_mul,
|  | int | sub_acc1,
|  | int | sub_acc2 )

Parameters

  a | Matrix A
  sgn_x | Sign mask for matrix A
  b | Matrix B
  sgn_y | Sign mask for matrix B
  acc1 | Accumulator 1 input
  acc2 | Accumulator 2 input
  zero_acc1 | Zeroing mask for acc1
  sub_mul | Negation mask of multiplication result
  sub_acc1 | Negation mask of acc1
  sub_acc2 | Negation mask of acc2

Returns
  Result of operation

## ◆ submac_4x4_4x4_conf() [6/8]

v16acc64 submac_4x4_4x4_conf | ( | v32uint16 | a,
|  | int | sgn_x,
|  | v32uint16 | b,
|  | int | sgn_y,
|  | v16acc64 | acc1,
|  | v16acc64 | acc2,
|  | int | zero_acc1,
|  | int | sub_mul,
|  | int | sub_acc1,
|  | int | sub_acc2 )

Parameters

  a | Matrix A
  sgn_x | Sign mask for matrix A
  b | Matrix B
  sgn_y | Sign mask for matrix B
  acc1 | Accumulator 1 input
  acc2 | Accumulator 2 input
  zero_acc1 | Zeroing mask for acc1
  sub_mul | Negation mask of multiplication result
  sub_acc1 | Negation mask of acc1
  sub_acc2 | Negation mask of acc2

Returns
  Result of operation

## ◆ submac_4x4_4x4_conf() [7/8]

v16acc64 submac_4x4_4x4_conf | ( | v32uint16 | a,
|  | v32int16 | b,
|  | v16acc64 | acc1,
|  | v16acc64 | acc2,
|  | int | zero_acc1,
|  | int | sub_mul,
|  | int | sub_acc1,
|  | int | sub_acc2 )

Parameters

  a | Matrix A
  b | Matrix B
  acc1 | Accumulator 1 input
  acc2 | Accumulator 2 input
  zero_acc1 | Zeroing mask for acc1
  sub_mul | Negation mask of multiplication result
  sub_acc1 | Negation mask of acc1
  sub_acc2 | Negation mask of acc2

Returns
  Result of operation

## ◆ submac_4x4_4x4_conf() [8/8]

v16acc64 submac_4x4_4x4_conf | ( | v32uint16 | a,
|  | v32uint16 | b,
|  | v16acc64 | acc1,
|  | v16acc64 | acc2,
|  | int | zero_acc1,
|  | int | sub_mul,
|  | int | sub_acc1,
|  | int | sub_acc2 )

Parameters

  a | Matrix A
  b | Matrix B
  acc1 | Accumulator 1 input
  acc2 | Accumulator 2 input
  zero_acc1 | Zeroing mask for acc1
  sub_mul | Negation mask of multiplication result
  sub_acc1 | Negation mask of acc1
  sub_acc2 | Negation mask of acc2

Returns
  Result of operation

## ◆ submac_conv_16x4() [1/8]

v16acc64 submac_conv_16x4 | ( | v32int16 | a,
|  | int | sgn_x,
|  | v32int16 | b,
|  | int | sgn_y,
|  | v16acc64 | acc1,
|  | v16acc64 | acc2 )

Parameters

  a | Matrix A
  sgn_x | Sign mask for matrix A
  b | Matrix B
  sgn_y | Sign mask for matrix B
  acc1 | Accumulator 1 input
  acc2 | Accumulator 2 input

Returns
  Result of operation

## ◆ submac_conv_16x4() [2/8]

v16acc64 submac_conv_16x4 | ( | v32int16 | a,
|  | int | sgn_x,
|  | v32uint16 | b,
|  | int | sgn_y,
|  | v16acc64 | acc1,
|  | v16acc64 | acc2 )

Parameters

  a | Matrix A
  sgn_x | Sign mask for matrix A
  b | Matrix B
  sgn_y | Sign mask for matrix B
  acc1 | Accumulator 1 input
  acc2 | Accumulator 2 input

Returns
  Result of operation

## ◆ submac_conv_16x4() [3/8]

v16acc64 submac_conv_16x4 | ( | v32int16 | a,
|  | v32int16 | b,
|  | v16acc64 | acc1,
|  | v16acc64 | acc2 )

Parameters

  a | Matrix A
  b | Matrix B
  acc1 | Accumulator 1 input
  acc2 | Accumulator 2 input

Returns
  Result of operation

## ◆ submac_conv_16x4() [4/8]

v16acc64 submac_conv_16x4 | ( | v32int16 | a,
|  | v32uint16 | b,
|  | v16acc64 | acc1,
|  | v16acc64 | acc2 )

Parameters

  a | Matrix A
  b | Matrix B
  acc1 | Accumulator 1 input
  acc2 | Accumulator 2 input

Returns
  Result of operation

## ◆ submac_conv_16x4() [5/8]

v16acc64 submac_conv_16x4 | ( | v32uint16 | a,
|  | int | sgn_x,
|  | v32int16 | b,
|  | int | sgn_y,
|  | v16acc64 | acc1,
|  | v16acc64 | acc2 )

Parameters

  a | Matrix A
  sgn_x | Sign mask for matrix A
  b | Matrix B
  sgn_y | Sign mask for matrix B
  acc1 | Accumulator 1 input
  acc2 | Accumulator 2 input

Returns
  Result of operation

## ◆ submac_conv_16x4() [6/8]

v16acc64 submac_conv_16x4 | ( | v32uint16 | a,
|  | int | sgn_x,
|  | v32uint16 | b,
|  | int | sgn_y,
|  | v16acc64 | acc1,
|  | v16acc64 | acc2 )

Parameters

  a | Matrix A
  sgn_x | Sign mask for matrix A
  b | Matrix B
  sgn_y | Sign mask for matrix B
  acc1 | Accumulator 1 input
  acc2 | Accumulator 2 input

Returns
  Result of operation

## ◆ submac_conv_16x4() [7/8]

v16acc64 submac_conv_16x4 | ( | v32uint16 | a,
|  | v32int16 | b,
|  | v16acc64 | acc1,
|  | v16acc64 | acc2 )

Parameters

  a | Matrix A
  b | Matrix B
  acc1 | Accumulator 1 input
  acc2 | Accumulator 2 input

Returns
  Result of operation

## ◆ submac_conv_16x4() [8/8]

v16acc64 submac_conv_16x4 | ( | v32uint16 | a,
|  | v32uint16 | b,
|  | v16acc64 | acc1,
|  | v16acc64 | acc2 )

Parameters

  a | Matrix A
  b | Matrix B
  acc1 | Accumulator 1 input
  acc2 | Accumulator 2 input

Returns
  Result of operation

## ◆ submac_conv_16x4_conf() [1/8]

v16acc64 submac_conv_16x4_conf | ( | v32int16 | a,
|  | int | sgn_x,
|  | v32int16 | b,
|  | int | sgn_y,
|  | v16acc64 | acc1,
|  | v16acc64 | acc2,
|  | int | zero_acc1,
|  | int | sub_mul,
|  | int | sub_acc1,
|  | int | sub_acc2 )

Parameters

  a | Matrix A
  sgn_x | Sign mask for matrix A
  b | Matrix B
  sgn_y | Sign mask for matrix B
  acc1 | Accumulator 1 input
  acc2 | Accumulator 2 input
  zero_acc1 | Zeroing mask for acc1
  sub_mul | Negation mask of multiplication result
  sub_acc1 | Negation mask of acc1
  sub_acc2 | Negation mask of acc2

Returns
  Result of operation

## ◆ submac_conv_16x4_conf() [2/8]

v16acc64 submac_conv_16x4_conf | ( | v32int16 | a,
|  | int | sgn_x,
|  | v32uint16 | b,
|  | int | sgn_y,
|  | v16acc64 | acc1,
|  | v16acc64 | acc2,
|  | int | zero_acc1,
|  | int | sub_mul,
|  | int | sub_acc1,
|  | int | sub_acc2 )

Parameters

  a | Matrix A
  sgn_x | Sign mask for matrix A
  b | Matrix B
  sgn_y | Sign mask for matrix B
  acc1 | Accumulator 1 input
  acc2 | Accumulator 2 input
  zero_acc1 | Zeroing mask for acc1
  sub_mul | Negation mask of multiplication result
  sub_acc1 | Negation mask of acc1
  sub_acc2 | Negation mask of acc2

Returns
  Result of operation

## ◆ submac_conv_16x4_conf() [3/8]

v16acc64 submac_conv_16x4_conf | ( | v32int16 | a,
|  | v32int16 | b,
|  | v16acc64 | acc1,
|  | v16acc64 | acc2,
|  | int | zero_acc1,
|  | int | sub_mul,
|  | int | sub_acc1,
|  | int | sub_acc2 )

Parameters

  a | Matrix A
  b | Matrix B
  acc1 | Accumulator 1 input
  acc2 | Accumulator 2 input
  zero_acc1 | Zeroing mask for acc1
  sub_mul | Negation mask of multiplication result
  sub_acc1 | Negation mask of acc1
  sub_acc2 | Negation mask of acc2

Returns
  Result of operation

## ◆ submac_conv_16x4_conf() [4/8]

v16acc64 submac_conv_16x4_conf | ( | v32int16 | a,
|  | v32uint16 | b,
|  | v16acc64 | acc1,
|  | v16acc64 | acc2,
|  | int | zero_acc1,
|  | int | sub_mul,
|  | int | sub_acc1,
|  | int | sub_acc2 )

Parameters

  a | Matrix A
  b | Matrix B
  acc1 | Accumulator 1 input
  acc2 | Accumulator 2 input
  zero_acc1 | Zeroing mask for acc1
  sub_mul | Negation mask of multiplication result
  sub_acc1 | Negation mask of acc1
  sub_acc2 | Negation mask of acc2

Returns
  Result of operation

## ◆ submac_conv_16x4_conf() [5/8]

v16acc64 submac_conv_16x4_conf | ( | v32uint16 | a,
|  | int | sgn_x,
|  | v32int16 | b,
|  | int | sgn_y,
|  | v16acc64 | acc1,
|  | v16acc64 | acc2,
|  | int | zero_acc1,
|  | int | sub_mul,
|  | int | sub_acc1,
|  | int | sub_acc2 )

Parameters

  a | Matrix A
  sgn_x | Sign mask for matrix A
  b | Matrix B
  sgn_y | Sign mask for matrix B
  acc1 | Accumulator 1 input
  acc2 | Accumulator 2 input
  zero_acc1 | Zeroing mask for acc1
  sub_mul | Negation mask of multiplication result
  sub_acc1 | Negation mask of acc1
  sub_acc2 | Negation mask of acc2

Returns
  Result of operation

## ◆ submac_conv_16x4_conf() [6/8]

v16acc64 submac_conv_16x4_conf | ( | v32uint16 | a,
|  | int | sgn_x,
|  | v32uint16 | b,
|  | int | sgn_y,
|  | v16acc64 | acc1,
|  | v16acc64 | acc2,
|  | int | zero_acc1,
|  | int | sub_mul,
|  | int | sub_acc1,
|  | int | sub_acc2 )

Parameters

  a | Matrix A
  sgn_x | Sign mask for matrix A
  b | Matrix B
  sgn_y | Sign mask for matrix B
  acc1 | Accumulator 1 input
  acc2 | Accumulator 2 input
  zero_acc1 | Zeroing mask for acc1
  sub_mul | Negation mask of multiplication result
  sub_acc1 | Negation mask of acc1
  sub_acc2 | Negation mask of acc2

Returns
  Result of operation

## ◆ submac_conv_16x4_conf() [7/8]

v16acc64 submac_conv_16x4_conf | ( | v32uint16 | a,
|  | v32int16 | b,
|  | v16acc64 | acc1,
|  | v16acc64 | acc2,
|  | int | zero_acc1,
|  | int | sub_mul,
|  | int | sub_acc1,
|  | int | sub_acc2 )

Parameters

  a | Matrix A
  b | Matrix B
  acc1 | Accumulator 1 input
  acc2 | Accumulator 2 input
  zero_acc1 | Zeroing mask for acc1
  sub_mul | Negation mask of multiplication result
  sub_acc1 | Negation mask of acc1
  sub_acc2 | Negation mask of acc2

Returns
  Result of operation

## ◆ submac_conv_16x4_conf() [8/8]

v16acc64 submac_conv_16x4_conf | ( | v32uint16 | a,
|  | v32uint16 | b,
|  | v16acc64 | acc1,
|  | v16acc64 | acc2,
|  | int | zero_acc1,
|  | int | sub_mul,
|  | int | sub_acc1,
|  | int | sub_acc2 )

Parameters

  a | Matrix A
  b | Matrix B
  acc1 | Accumulator 1 input
  acc2 | Accumulator 2 input
  zero_acc1 | Zeroing mask for acc1
  sub_mul | Negation mask of multiplication result
  sub_acc1 | Negation mask of acc1
  sub_acc2 | Negation mask of acc2

Returns
  Result of operation

## ◆ submac_elem_16_2() [1/8]

v16acc64 submac_elem_16_2 | ( | v32int16 | a,
|  | int | sgn_x,
|  | v32int16 | b,
|  | int | sgn_y,
|  | v16acc64 | acc1,
|  | v16acc64 | acc2 )

Parameters

  a | Matrix A
  sgn_x | Sign mask for matrix A
  b | Matrix B
  sgn_y | Sign mask for matrix B
  acc1 | Accumulator 1 input
  acc2 | Accumulator 2 input

Returns
  Result of operation

## ◆ submac_elem_16_2() [2/8]

v16acc64 submac_elem_16_2 | ( | v32int16 | a,
|  | int | sgn_x,
|  | v32uint16 | b,
|  | int | sgn_y,
|  | v16acc64 | acc1,
|  | v16acc64 | acc2 )

Parameters

  a | Matrix A
  sgn_x | Sign mask for matrix A
  b | Matrix B
  sgn_y | Sign mask for matrix B
  acc1 | Accumulator 1 input
  acc2 | Accumulator 2 input

Returns
  Result of operation

## ◆ submac_elem_16_2() [3/8]

v16acc64 submac_elem_16_2 | ( | v32int16 | a,
|  | v32int16 | b,
|  | v16acc64 | acc1,
|  | v16acc64 | acc2 )

Parameters

  a | Matrix A
  b | Matrix B
  acc1 | Accumulator 1 input
  acc2 | Accumulator 2 input

Returns
  Result of operation

## ◆ submac_elem_16_2() [4/8]

v16acc64 submac_elem_16_2 | ( | v32int16 | a,
|  | v32uint16 | b,
|  | v16acc64 | acc1,
|  | v16acc64 | acc2 )

Parameters

  a | Matrix A
  b | Matrix B
  acc1 | Accumulator 1 input
  acc2 | Accumulator 2 input

Returns
  Result of operation

## ◆ submac_elem_16_2() [5/8]

v16acc64 submac_elem_16_2 | ( | v32uint16 | a,
|  | int | sgn_x,
|  | v32int16 | b,
|  | int | sgn_y,
|  | v16acc64 | acc1,
|  | v16acc64 | acc2 )

Parameters

  a | Matrix A
  sgn_x | Sign mask for matrix A
  b | Matrix B
  sgn_y | Sign mask for matrix B
  acc1 | Accumulator 1 input
  acc2 | Accumulator 2 input

Returns
  Result of operation

## ◆ submac_elem_16_2() [6/8]

v16acc64 submac_elem_16_2 | ( | v32uint16 | a,
|  | int | sgn_x,
|  | v32uint16 | b,
|  | int | sgn_y,
|  | v16acc64 | acc1,
|  | v16acc64 | acc2 )

Parameters

  a | Matrix A
  sgn_x | Sign mask for matrix A
  b | Matrix B
  sgn_y | Sign mask for matrix B
  acc1 | Accumulator 1 input
  acc2 | Accumulator 2 input

Returns
  Result of operation

## ◆ submac_elem_16_2() [7/8]

v16acc64 submac_elem_16_2 | ( | v32uint16 | a,
|  | v32int16 | b,
|  | v16acc64 | acc1,
|  | v16acc64 | acc2 )

Parameters

  a | Matrix A
  b | Matrix B
  acc1 | Accumulator 1 input
  acc2 | Accumulator 2 input

Returns
  Result of operation

## ◆ submac_elem_16_2() [8/8]

v16acc64 submac_elem_16_2 | ( | v32uint16 | a,
|  | v32uint16 | b,
|  | v16acc64 | acc1,
|  | v16acc64 | acc2 )

Parameters

  a | Matrix A
  b | Matrix B
  acc1 | Accumulator 1 input
  acc2 | Accumulator 2 input

Returns
  Result of operation

## ◆ submac_elem_16_2_conf() [1/8]

v16acc64 submac_elem_16_2_conf | ( | v32int16 | a,
|  | int | sgn_x,
|  | v32int16 | b,
|  | int | sgn_y,
|  | v16acc64 | acc1,
|  | v16acc64 | acc2,
|  | int | zero_acc1,
|  | int | sub_mul,
|  | int | sub_acc1,
|  | int | sub_acc2 )

Parameters

  a | Matrix A
  sgn_x | Sign mask for matrix A
  b | Matrix B
  sgn_y | Sign mask for matrix B
  acc1 | Accumulator 1 input
  acc2 | Accumulator 2 input
  zero_acc1 | Zeroing mask for acc1
  sub_mul | Negation mask of multiplication result
  sub_acc1 | Negation mask of acc1
  sub_acc2 | Negation mask of acc2

Returns
  Result of operation

## ◆ submac_elem_16_2_conf() [2/8]

v16acc64 submac_elem_16_2_conf | ( | v32int16 | a,
|  | int | sgn_x,
|  | v32uint16 | b,
|  | int | sgn_y,
|  | v16acc64 | acc1,
|  | v16acc64 | acc2,
|  | int | zero_acc1,
|  | int | sub_mul,
|  | int | sub_acc1,
|  | int | sub_acc2 )

Parameters

  a | Matrix A
  sgn_x | Sign mask for matrix A
  b | Matrix B
  sgn_y | Sign mask for matrix B
  acc1 | Accumulator 1 input
  acc2 | Accumulator 2 input
  zero_acc1 | Zeroing mask for acc1
  sub_mul | Negation mask of multiplication result
  sub_acc1 | Negation mask of acc1
  sub_acc2 | Negation mask of acc2

Returns
  Result of operation

## ◆ submac_elem_16_2_conf() [3/8]

v16acc64 submac_elem_16_2_conf | ( | v32int16 | a,
|  | v32int16 | b,
|  | v16acc64 | acc1,
|  | v16acc64 | acc2,
|  | int | zero_acc1,
|  | int | sub_mul,
|  | int | sub_acc1,
|  | int | sub_acc2 )

Parameters

  a | Matrix A
  b | Matrix B
  acc1 | Accumulator 1 input
  acc2 | Accumulator 2 input
  zero_acc1 | Zeroing mask for acc1
  sub_mul | Negation mask of multiplication result
  sub_acc1 | Negation mask of acc1
  sub_acc2 | Negation mask of acc2

Returns
  Result of operation

## ◆ submac_elem_16_2_conf() [4/8]

v16acc64 submac_elem_16_2_conf | ( | v32int16 | a,
|  | v32uint16 | b,
|  | v16acc64 | acc1,
|  | v16acc64 | acc2,
|  | int | zero_acc1,
|  | int | sub_mul,
|  | int | sub_acc1,
|  | int | sub_acc2 )

Parameters

  a | Matrix A
  b | Matrix B
  acc1 | Accumulator 1 input
  acc2 | Accumulator 2 input
  zero_acc1 | Zeroing mask for acc1
  sub_mul | Negation mask of multiplication result
  sub_acc1 | Negation mask of acc1
  sub_acc2 | Negation mask of acc2

Returns
  Result of operation

## ◆ submac_elem_16_2_conf() [5/8]

v16acc64 submac_elem_16_2_conf | ( | v32uint16 | a,
|  | int | sgn_x,
|  | v32int16 | b,
|  | int | sgn_y,
|  | v16acc64 | acc1,
|  | v16acc64 | acc2,
|  | int | zero_acc1,
|  | int | sub_mul,
|  | int | sub_acc1,
|  | int | sub_acc2 )

Parameters

  a | Matrix A
  sgn_x | Sign mask for matrix A
  b | Matrix B
  sgn_y | Sign mask for matrix B
  acc1 | Accumulator 1 input
  acc2 | Accumulator 2 input
  zero_acc1 | Zeroing mask for acc1
  sub_mul | Negation mask of multiplication result
  sub_acc1 | Negation mask of acc1
  sub_acc2 | Negation mask of acc2

Returns
  Result of operation

## ◆ submac_elem_16_2_conf() [6/8]

v16acc64 submac_elem_16_2_conf | ( | v32uint16 | a,
|  | int | sgn_x,
|  | v32uint16 | b,
|  | int | sgn_y,
|  | v16acc64 | acc1,
|  | v16acc64 | acc2,
|  | int | zero_acc1,
|  | int | sub_mul,
|  | int | sub_acc1,
|  | int | sub_acc2 )

Parameters

  a | Matrix A
  sgn_x | Sign mask for matrix A
  b | Matrix B
  sgn_y | Sign mask for matrix B
  acc1 | Accumulator 1 input
  acc2 | Accumulator 2 input
  zero_acc1 | Zeroing mask for acc1
  sub_mul | Negation mask of multiplication result
  sub_acc1 | Negation mask of acc1
  sub_acc2 | Negation mask of acc2

Returns
  Result of operation

## ◆ submac_elem_16_2_conf() [7/8]

v16acc64 submac_elem_16_2_conf | ( | v32uint16 | a,
|  | v32int16 | b,
|  | v16acc64 | acc1,
|  | v16acc64 | acc2,
|  | int | zero_acc1,
|  | int | sub_mul,
|  | int | sub_acc1,
|  | int | sub_acc2 )

Parameters

  a | Matrix A
  b | Matrix B
  acc1 | Accumulator 1 input
  acc2 | Accumulator 2 input
  zero_acc1 | Zeroing mask for acc1
  sub_mul | Negation mask of multiplication result
  sub_acc1 | Negation mask of acc1
  sub_acc2 | Negation mask of acc2

Returns
  Result of operation

## ◆ submac_elem_16_2_conf() [8/8]

v16acc64 submac_elem_16_2_conf | ( | v32uint16 | a,
|  | v32uint16 | b,
|  | v16acc64 | acc1,
|  | v16acc64 | acc2,
|  | int | zero_acc1,
|  | int | sub_mul,
|  | int | sub_acc1,
|  | int | sub_acc2 )

Parameters

  a | Matrix A
  b | Matrix B
  acc1 | Accumulator 1 input
  acc2 | Accumulator 2 input
  zero_acc1 | Zeroing mask for acc1
  sub_mul | Negation mask of multiplication result
  sub_acc1 | Negation mask of acc1
  sub_acc2 | Negation mask of acc2

Returns
  Result of operation

## ◆ submac_elem_32() [1/8]

v32acc32 submac_elem_32 | ( | v32int16 | a,
|  | int | sgn_x,
|  | v32int16 | b,
|  | int | sgn_y,
|  | v32acc32 | acc1,
|  | v32acc32 | acc2 )

Parameters

  a | Matrix A
  sgn_x | Sign mask for matrix A
  b | Matrix B
  sgn_y | Sign mask for matrix B
  acc1 | Accumulator 1 input
  acc2 | Accumulator 2 input

Returns
  Result of operation

## ◆ submac_elem_32() [2/8]

v32acc32 submac_elem_32 | ( | v32int16 | a,
|  | int | sgn_x,
|  | v32uint16 | b,
|  | int | sgn_y,
|  | v32acc32 | acc1,
|  | v32acc32 | acc2 )

Parameters

  a | Matrix A
  sgn_x | Sign mask for matrix A
  b | Matrix B
  sgn_y | Sign mask for matrix B
  acc1 | Accumulator 1 input
  acc2 | Accumulator 2 input

Returns
  Result of operation

## ◆ submac_elem_32() [3/8]

v32acc32 submac_elem_32 | ( | v32int16 | a,
|  | v32int16 | b,
|  | v32acc32 | acc1,
|  | v32acc32 | acc2 )

Parameters

  a | Matrix A
  b | Matrix B
  acc1 | Accumulator 1 input
  acc2 | Accumulator 2 input

Returns
  Result of operation

## ◆ submac_elem_32() [4/8]

v32acc32 submac_elem_32 | ( | v32int16 | a,
|  | v32uint16 | b,
|  | v32acc32 | acc1,
|  | v32acc32 | acc2 )

Parameters

  a | Matrix A
  b | Matrix B
  acc1 | Accumulator 1 input
  acc2 | Accumulator 2 input

Returns
  Result of operation

## ◆ submac_elem_32() [5/8]

v32acc32 submac_elem_32 | ( | v32uint16 | a,
|  | int | sgn_x,
|  | v32int16 | b,
|  | int | sgn_y,
|  | v32acc32 | acc1,
|  | v32acc32 | acc2 )

Parameters

  a | Matrix A
  sgn_x | Sign mask for matrix A
  b | Matrix B
  sgn_y | Sign mask for matrix B
  acc1 | Accumulator 1 input
  acc2 | Accumulator 2 input

Returns
  Result of operation

## ◆ submac_elem_32() [6/8]

v32acc32 submac_elem_32 | ( | v32uint16 | a,
|  | int | sgn_x,
|  | v32uint16 | b,
|  | int | sgn_y,
|  | v32acc32 | acc1,
|  | v32acc32 | acc2 )

Parameters

  a | Matrix A
  sgn_x | Sign mask for matrix A
  b | Matrix B
  sgn_y | Sign mask for matrix B
  acc1 | Accumulator 1 input
  acc2 | Accumulator 2 input

Returns
  Result of operation

## ◆ submac_elem_32() [7/8]

v32acc32 submac_elem_32 | ( | v32uint16 | a,
|  | v32int16 | b,
|  | v32acc32 | acc1,
|  | v32acc32 | acc2 )

Parameters

  a | Matrix A
  b | Matrix B
  acc1 | Accumulator 1 input
  acc2 | Accumulator 2 input

Returns
  Result of operation

## ◆ submac_elem_32() [8/8]

v32acc32 submac_elem_32 | ( | v32uint16 | a,
|  | v32uint16 | b,
|  | v32acc32 | acc1,
|  | v32acc32 | acc2 )

Parameters

  a | Matrix A
  b | Matrix B
  acc1 | Accumulator 1 input
  acc2 | Accumulator 2 input

Returns
  Result of operation

## ◆ submac_elem_32_conf() [1/8]

v32acc32 submac_elem_32_conf | ( | v32int16 | a,
|  | int | sgn_x,
|  | v32int16 | b,
|  | int | sgn_y,
|  | v32acc32 | acc1,
|  | v32acc32 | acc2,
|  | int | zero_acc1,
|  | int | sub_mul,
|  | int | sub_acc1,
|  | int | sub_acc2 )

Parameters

  a | Matrix A
  sgn_x | Sign mask for matrix A
  b | Matrix B
  sgn_y | Sign mask for matrix B
  acc1 | Accumulator 1 input
  acc2 | Accumulator 2 input
  zero_acc1 | Zeroing mask for acc1
  sub_mul | Negation mask of multiplication result
  sub_acc1 | Negation mask of acc1
  sub_acc2 | Negation mask of acc2

Returns
  Result of operation

## ◆ submac_elem_32_conf() [2/8]

v32acc32 submac_elem_32_conf | ( | v32int16 | a,
|  | int | sgn_x,
|  | v32uint16 | b,
|  | int | sgn_y,
|  | v32acc32 | acc1,
|  | v32acc32 | acc2,
|  | int | zero_acc1,
|  | int | sub_mul,
|  | int | sub_acc1,
|  | int | sub_acc2 )

Parameters

  a | Matrix A
  sgn_x | Sign mask for matrix A
  b | Matrix B
  sgn_y | Sign mask for matrix B
  acc1 | Accumulator 1 input
  acc2 | Accumulator 2 input
  zero_acc1 | Zeroing mask for acc1
  sub_mul | Negation mask of multiplication result
  sub_acc1 | Negation mask of acc1
  sub_acc2 | Negation mask of acc2

Returns
  Result of operation

## ◆ submac_elem_32_conf() [3/8]

v32acc32 submac_elem_32_conf | ( | v32int16 | a,
|  | v32int16 | b,
|  | v32acc32 | acc1,
|  | v32acc32 | acc2,
|  | int | zero_acc1,
|  | int | sub_mul,
|  | int | sub_acc1,
|  | int | sub_acc2 )

Parameters

  a | Matrix A
  b | Matrix B
  acc1 | Accumulator 1 input
  acc2 | Accumulator 2 input
  zero_acc1 | Zeroing mask for acc1
  sub_mul | Negation mask of multiplication result
  sub_acc1 | Negation mask of acc1
  sub_acc2 | Negation mask of acc2

Returns
  Result of operation

## ◆ submac_elem_32_conf() [4/8]

v32acc32 submac_elem_32_conf | ( | v32int16 | a,
|  | v32uint16 | b,
|  | v32acc32 | acc1,
|  | v32acc32 | acc2,
|  | int | zero_acc1,
|  | int | sub_mul,
|  | int | sub_acc1,
|  | int | sub_acc2 )

Parameters

  a | Matrix A
  b | Matrix B
  acc1 | Accumulator 1 input
  acc2 | Accumulator 2 input
  zero_acc1 | Zeroing mask for acc1
  sub_mul | Negation mask of multiplication result
  sub_acc1 | Negation mask of acc1
  sub_acc2 | Negation mask of acc2

Returns
  Result of operation

## ◆ submac_elem_32_conf() [5/8]

v32acc32 submac_elem_32_conf | ( | v32uint16 | a,
|  | int | sgn_x,
|  | v32int16 | b,
|  | int | sgn_y,
|  | v32acc32 | acc1,
|  | v32acc32 | acc2,
|  | int | zero_acc1,
|  | int | sub_mul,
|  | int | sub_acc1,
|  | int | sub_acc2 )

Parameters

  a | Matrix A
  sgn_x | Sign mask for matrix A
  b | Matrix B
  sgn_y | Sign mask for matrix B
  acc1 | Accumulator 1 input
  acc2 | Accumulator 2 input
  zero_acc1 | Zeroing mask for acc1
  sub_mul | Negation mask of multiplication result
  sub_acc1 | Negation mask of acc1
  sub_acc2 | Negation mask of acc2

Returns
  Result of operation

## ◆ submac_elem_32_conf() [6/8]

v32acc32 submac_elem_32_conf | ( | v32uint16 | a,
|  | int | sgn_x,
|  | v32uint16 | b,
|  | int | sgn_y,
|  | v32acc32 | acc1,
|  | v32acc32 | acc2,
|  | int | zero_acc1,
|  | int | sub_mul,
|  | int | sub_acc1,
|  | int | sub_acc2 )

Parameters

  a | Matrix A
  sgn_x | Sign mask for matrix A
  b | Matrix B
  sgn_y | Sign mask for matrix B
  acc1 | Accumulator 1 input
  acc2 | Accumulator 2 input
  zero_acc1 | Zeroing mask for acc1
  sub_mul | Negation mask of multiplication result
  sub_acc1 | Negation mask of acc1
  sub_acc2 | Negation mask of acc2

Returns
  Result of operation

## ◆ submac_elem_32_conf() [7/8]

v32acc32 submac_elem_32_conf | ( | v32uint16 | a,
|  | v32int16 | b,
|  | v32acc32 | acc1,
|  | v32acc32 | acc2,
|  | int | zero_acc1,
|  | int | sub_mul,
|  | int | sub_acc1,
|  | int | sub_acc2 )

Parameters

  a | Matrix A
  b | Matrix B
  acc1 | Accumulator 1 input
  acc2 | Accumulator 2 input
  zero_acc1 | Zeroing mask for acc1
  sub_mul | Negation mask of multiplication result
  sub_acc1 | Negation mask of acc1
  sub_acc2 | Negation mask of acc2

Returns
  Result of operation

## ◆ submac_elem_32_conf() [8/8]

v32acc32 submac_elem_32_conf | ( | v32uint16 | a,
|  | v32uint16 | b,
|  | v32acc32 | acc1,
|  | v32acc32 | acc2,
|  | int | zero_acc1,
|  | int | sub_mul,
|  | int | sub_acc1,
|  | int | sub_acc2 )

Parameters

  a | Matrix A
  b | Matrix B
  acc1 | Accumulator 1 input
  acc2 | Accumulator 2 input
  zero_acc1 | Zeroing mask for acc1
  sub_mul | Negation mask of multiplication result
  sub_acc1 | Negation mask of acc1
  sub_acc2 | Negation mask of acc2

Returns
  Result of operation

## ◆ submsc_2x4_4x8() [1/8]

v16acc64 submsc_2x4_4x8 | ( | v32int16 | a,
|  | int | sgn_x,
|  | v32int16 | b,
|  | int | sgn_y,
|  | v16acc64 | acc1,
|  | v16acc64 | acc2 )

Parameters

  a | Matrix A
  sgn_x | Sign mask for matrix A
  b | Matrix B
  sgn_y | Sign mask for matrix B
  acc1 | Accumulator 1 input
  acc2 | Accumulator 2 input

Returns
  Result of operation

## ◆ submsc_2x4_4x8() [2/8]

v16acc64 submsc_2x4_4x8 | ( | v32int16 | a,
|  | int | sgn_x,
|  | v32uint16 | b,
|  | int | sgn_y,
|  | v16acc64 | acc1,
|  | v16acc64 | acc2 )

Parameters

  a | Matrix A
  sgn_x | Sign mask for matrix A
  b | Matrix B
  sgn_y | Sign mask for matrix B
  acc1 | Accumulator 1 input
  acc2 | Accumulator 2 input

Returns
  Result of operation

## ◆ submsc_2x4_4x8() [3/8]

v16acc64 submsc_2x4_4x8 | ( | v32int16 | a,
|  | v32int16 | b,
|  | v16acc64 | acc1,
|  | v16acc64 | acc2 )

Parameters

  a | Matrix A
  b | Matrix B
  acc1 | Accumulator 1 input
  acc2 | Accumulator 2 input

Returns
  Result of operation

## ◆ submsc_2x4_4x8() [4/8]

v16acc64 submsc_2x4_4x8 | ( | v32int16 | a,
|  | v32uint16 | b,
|  | v16acc64 | acc1,
|  | v16acc64 | acc2 )

Parameters

  a | Matrix A
  b | Matrix B
  acc1 | Accumulator 1 input
  acc2 | Accumulator 2 input

Returns
  Result of operation

## ◆ submsc_2x4_4x8() [5/8]

v16acc64 submsc_2x4_4x8 | ( | v32uint16 | a,
|  | int | sgn_x,
|  | v32int16 | b,
|  | int | sgn_y,
|  | v16acc64 | acc1,
|  | v16acc64 | acc2 )

Parameters

  a | Matrix A
  sgn_x | Sign mask for matrix A
  b | Matrix B
  sgn_y | Sign mask for matrix B
  acc1 | Accumulator 1 input
  acc2 | Accumulator 2 input

Returns
  Result of operation

## ◆ submsc_2x4_4x8() [6/8]

v16acc64 submsc_2x4_4x8 | ( | v32uint16 | a,
|  | int | sgn_x,
|  | v32uint16 | b,
|  | int | sgn_y,
|  | v16acc64 | acc1,
|  | v16acc64 | acc2 )

Parameters

  a | Matrix A
  sgn_x | Sign mask for matrix A
  b | Matrix B
  sgn_y | Sign mask for matrix B
  acc1 | Accumulator 1 input
  acc2 | Accumulator 2 input

Returns
  Result of operation

## ◆ submsc_2x4_4x8() [7/8]

v16acc64 submsc_2x4_4x8 | ( | v32uint16 | a,
|  | v32int16 | b,
|  | v16acc64 | acc1,
|  | v16acc64 | acc2 )

Parameters

  a | Matrix A
  b | Matrix B
  acc1 | Accumulator 1 input
  acc2 | Accumulator 2 input

Returns
  Result of operation

## ◆ submsc_2x4_4x8() [8/8]

v16acc64 submsc_2x4_4x8 | ( | v32uint16 | a,
|  | v32uint16 | b,
|  | v16acc64 | acc1,
|  | v16acc64 | acc2 )

Parameters

  a | Matrix A
  b | Matrix B
  acc1 | Accumulator 1 input
  acc2 | Accumulator 2 input

Returns
  Result of operation

## ◆ submsc_2x4_4x8_conf() [1/8]

v16acc64 submsc_2x4_4x8_conf | ( | v32int16 | a,
|  | int | sgn_x,
|  | v32int16 | b,
|  | int | sgn_y,
|  | v16acc64 | acc1,
|  | v16acc64 | acc2,
|  | int | zero_acc1,
|  | int | sub_mul,
|  | int | sub_acc1,
|  | int | sub_acc2 )

Parameters

  a | Matrix A
  sgn_x | Sign mask for matrix A
  b | Matrix B
  sgn_y | Sign mask for matrix B
  acc1 | Accumulator 1 input
  acc2 | Accumulator 2 input
  zero_acc1 | Zeroing mask for acc1
  sub_mul | Negation mask of multiplication result.
  sub_acc1 | Negation mask of acc1
  sub_acc2 | Negation mask of acc2

Returns
  Result of operation

## ◆ submsc_2x4_4x8_conf() [2/8]

v16acc64 submsc_2x4_4x8_conf | ( | v32int16 | a,
|  | int | sgn_x,
|  | v32uint16 | b,
|  | int | sgn_y,
|  | v16acc64 | acc1,
|  | v16acc64 | acc2,
|  | int | zero_acc1,
|  | int | sub_mul,
|  | int | sub_acc1,
|  | int | sub_acc2 )

Parameters

  a | Matrix A
  sgn_x | Sign mask for matrix A
  b | Matrix B
  sgn_y | Sign mask for matrix B
  acc1 | Accumulator 1 input
  acc2 | Accumulator 2 input
  zero_acc1 | Zeroing mask for acc1
  sub_mul | Negation mask of multiplication result.
  sub_acc1 | Negation mask of acc1
  sub_acc2 | Negation mask of acc2

Returns
  Result of operation

## ◆ submsc_2x4_4x8_conf() [3/8]

v16acc64 submsc_2x4_4x8_conf | ( | v32int16 | a,
|  | v32int16 | b,
|  | v16acc64 | acc1,
|  | v16acc64 | acc2,
|  | int | zero_acc1,
|  | int | sub_mul,
|  | int | sub_acc1,
|  | int | sub_acc2 )

Parameters

  a | Matrix A
  b | Matrix B
  acc1 | Accumulator 1 input
  acc2 | Accumulator 2 input
  zero_acc1 | Zeroing mask for acc1
  sub_mul | Negation mask of multiplication result
  sub_acc1 | Negation mask of acc1
  sub_acc2 | Negation mask of acc2

Returns
  Result of operation

## ◆ submsc_2x4_4x8_conf() [4/8]

v16acc64 submsc_2x4_4x8_conf | ( | v32int16 | a,
|  | v32uint16 | b,
|  | v16acc64 | acc1,
|  | v16acc64 | acc2,
|  | int | zero_acc1,
|  | int | sub_mul,
|  | int | sub_acc1,
|  | int | sub_acc2 )

Parameters

  a | Matrix A
  b | Matrix B
  acc1 | Accumulator 1 input
  acc2 | Accumulator 2 input
  zero_acc1 | Zeroing mask for acc1
  sub_mul | Negation mask of multiplication result
  sub_acc1 | Negation mask of acc1
  sub_acc2 | Negation mask of acc2

Returns
  Result of operation

## ◆ submsc_2x4_4x8_conf() [5/8]

v16acc64 submsc_2x4_4x8_conf | ( | v32uint16 | a,
|  | int | sgn_x,
|  | v32int16 | b,
|  | int | sgn_y,
|  | v16acc64 | acc1,
|  | v16acc64 | acc2,
|  | int | zero_acc1,
|  | int | sub_mul,
|  | int | sub_acc1,
|  | int | sub_acc2 )

Parameters

  a | Matrix A
  sgn_x | Sign mask for matrix A
  b | Matrix B
  sgn_y | Sign mask for matrix B
  acc1 | Accumulator 1 input
  acc2 | Accumulator 2 input
  zero_acc1 | Zeroing mask for acc1
  sub_mul | Negation mask of multiplication result.
  sub_acc1 | Negation mask of acc1
  sub_acc2 | Negation mask of acc2

Returns
  Result of operation

## ◆ submsc_2x4_4x8_conf() [6/8]

v16acc64 submsc_2x4_4x8_conf | ( | v32uint16 | a,
|  | int | sgn_x,
|  | v32uint16 | b,
|  | int | sgn_y,
|  | v16acc64 | acc1,
|  | v16acc64 | acc2,
|  | int | zero_acc1,
|  | int | sub_mul,
|  | int | sub_acc1,
|  | int | sub_acc2 )

Parameters

  a | Matrix A
  sgn_x | Sign mask for matrix A
  b | Matrix B
  sgn_y | Sign mask for matrix B
  acc1 | Accumulator 1 input
  acc2 | Accumulator 2 input
  zero_acc1 | Zeroing mask for acc1
  sub_mul | Negation mask of multiplication result.
  sub_acc1 | Negation mask of acc1
  sub_acc2 | Negation mask of acc2

Returns
  Result of operation

## ◆ submsc_2x4_4x8_conf() [7/8]

v16acc64 submsc_2x4_4x8_conf | ( | v32uint16 | a,
|  | v32int16 | b,
|  | v16acc64 | acc1,
|  | v16acc64 | acc2,
|  | int | zero_acc1,
|  | int | sub_mul,
|  | int | sub_acc1,
|  | int | sub_acc2 )

Parameters

  a | Matrix A
  b | Matrix B
  acc1 | Accumulator 1 input
  acc2 | Accumulator 2 input
  zero_acc1 | Zeroing mask for acc1
  sub_mul | Negation mask of multiplication result
  sub_acc1 | Negation mask of acc1
  sub_acc2 | Negation mask of acc2

Returns
  Result of operation

## ◆ submsc_2x4_4x8_conf() [8/8]

v16acc64 submsc_2x4_4x8_conf | ( | v32uint16 | a,
|  | v32uint16 | b,
|  | v16acc64 | acc1,
|  | v16acc64 | acc2,
|  | int | zero_acc1,
|  | int | sub_mul,
|  | int | sub_acc1,
|  | int | sub_acc2 )

Parameters

  a | Matrix A
  b | Matrix B
  acc1 | Accumulator 1 input
  acc2 | Accumulator 2 input
  zero_acc1 | Zeroing mask for acc1
  sub_mul | Negation mask of multiplication result
  sub_acc1 | Negation mask of acc1
  sub_acc2 | Negation mask of acc2

Returns
  Result of operation

## ◆ submsc_4x2_2x8() [1/8]

v32acc32 submsc_4x2_2x8 | ( | v32int16 | a,
|  | int | sgn_x,
|  | v32int16 | b,
|  | int | sgn_y,
|  | v32acc32 | acc1,
|  | v32acc32 | acc2 )

Parameters

  a | Matrix A
  sgn_x | Sign mask for matrix A
  b | Matrix B
  sgn_y | Sign mask for matrix B
  acc1 | Accumulator 1 input
  acc2 | Accumulator 2 input

Returns
  Result of operation

## ◆ submsc_4x2_2x8() [2/8]

v32acc32 submsc_4x2_2x8 | ( | v32int16 | a,
|  | int | sgn_x,
|  | v32uint16 | b,
|  | int | sgn_y,
|  | v32acc32 | acc1,
|  | v32acc32 | acc2 )

Parameters

  a | Matrix A
  sgn_x | Sign mask for matrix A
  b | Matrix B
  sgn_y | Sign mask for matrix B
  acc1 | Accumulator 1 input
  acc2 | Accumulator 2 input

Returns
  Result of operation

## ◆ submsc_4x2_2x8() [3/8]

v32acc32 submsc_4x2_2x8 | ( | v32int16 | a,
|  | v32int16 | b,
|  | v32acc32 | acc1,
|  | v32acc32 | acc2 )

Parameters

  a | Matrix A
  b | Matrix B
  acc1 | Accumulator 1 input
  acc2 | Accumulator 2 input

Returns
  Result of operation

## ◆ submsc_4x2_2x8() [4/8]

v32acc32 submsc_4x2_2x8 | ( | v32int16 | a,
|  | v32uint16 | b,
|  | v32acc32 | acc1,
|  | v32acc32 | acc2 )

Parameters

  a | Matrix A
  b | Matrix B
  acc1 | Accumulator 1 input
  acc2 | Accumulator 2 input

Returns
  Result of operation

## ◆ submsc_4x2_2x8() [5/8]

v32acc32 submsc_4x2_2x8 | ( | v32uint16 | a,
|  | int | sgn_x,
|  | v32int16 | b,
|  | int | sgn_y,
|  | v32acc32 | acc1,
|  | v32acc32 | acc2 )

Parameters

  a | Matrix A
  sgn_x | Sign mask for matrix A
  b | Matrix B
  sgn_y | Sign mask for matrix B
  acc1 | Accumulator 1 input
  acc2 | Accumulator 2 input

Returns
  Result of operation

## ◆ submsc_4x2_2x8() [6/8]

v32acc32 submsc_4x2_2x8 | ( | v32uint16 | a,
|  | int | sgn_x,
|  | v32uint16 | b,
|  | int | sgn_y,
|  | v32acc32 | acc1,
|  | v32acc32 | acc2 )

Parameters

  a | Matrix A
  sgn_x | Sign mask for matrix A
  b | Matrix B
  sgn_y | Sign mask for matrix B
  acc1 | Accumulator 1 input
  acc2 | Accumulator 2 input

Returns
  Result of operation

## ◆ submsc_4x2_2x8() [7/8]

v32acc32 submsc_4x2_2x8 | ( | v32uint16 | a,
|  | v32int16 | b,
|  | v32acc32 | acc1,
|  | v32acc32 | acc2 )

Parameters

  a | Matrix A
  b | Matrix B
  acc1 | Accumulator 1 input
  acc2 | Accumulator 2 input

Returns
  Result of operation

## ◆ submsc_4x2_2x8() [8/8]

v32acc32 submsc_4x2_2x8 | ( | v32uint16 | a,
|  | v32uint16 | b,
|  | v32acc32 | acc1,
|  | v32acc32 | acc2 )

Parameters

  a | Matrix A
  b | Matrix B
  acc1 | Accumulator 1 input
  acc2 | Accumulator 2 input

Returns
  Result of operation

## ◆ submsc_4x2_2x8_conf() [1/8]

v32acc32 submsc_4x2_2x8_conf | ( | v32int16 | a,
|  | int | sgn_x,
|  | v32int16 | b,
|  | int | sgn_y,
|  | v32acc32 | acc1,
|  | v32acc32 | acc2,
|  | int | zero_acc1,
|  | int | sub_mul,
|  | int | sub_acc1,
|  | int | sub_acc2 )

Parameters

  a | Matrix A
  sgn_x | Sign mask for matrix A
  b | Matrix B
  sgn_y | Sign mask for matrix B
  acc1 | Accumulator 1 input
  acc2 | Accumulator 2 input
  zero_acc1 | Zeroing mask for acc1
  sub_mul | Negation mask of multiplication result.
  sub_acc1 | Negation mask of acc1
  sub_acc2 | Negation mask of acc2

Returns
  Result of operation

## ◆ submsc_4x2_2x8_conf() [2/8]

v32acc32 submsc_4x2_2x8_conf | ( | v32int16 | a,
|  | int | sgn_x,
|  | v32uint16 | b,
|  | int | sgn_y,
|  | v32acc32 | acc1,
|  | v32acc32 | acc2,
|  | int | zero_acc1,
|  | int | sub_mul,
|  | int | sub_acc1,
|  | int | sub_acc2 )

Parameters

  a | Matrix A
  sgn_x | Sign mask for matrix A
  b | Matrix B
  sgn_y | Sign mask for matrix B
  acc1 | Accumulator 1 input
  acc2 | Accumulator 2 input
  zero_acc1 | Zeroing mask for acc1
  sub_mul | Negation mask of multiplication result.
  sub_acc1 | Negation mask of acc1
  sub_acc2 | Negation mask of acc2

Returns
  Result of operation

## ◆ submsc_4x2_2x8_conf() [3/8]

v32acc32 submsc_4x2_2x8_conf | ( | v32int16 | a,
|  | v32int16 | b,
|  | v32acc32 | acc1,
|  | v32acc32 | acc2,
|  | int | zero_acc1,
|  | int | sub_mul,
|  | int | sub_acc1,
|  | int | sub_acc2 )

Parameters

  a | Matrix A
  b | Matrix B
  acc1 | Accumulator 1 input
  acc2 | Accumulator 2 input
  zero_acc1 | Zeroing mask for acc1
  sub_mul | Negation mask of multiplication result
  sub_acc1 | Negation mask of acc1
  sub_acc2 | Negation mask of acc2

Returns
  Result of operation

## ◆ submsc_4x2_2x8_conf() [4/8]

v32acc32 submsc_4x2_2x8_conf | ( | v32int16 | a,
|  | v32uint16 | b,
|  | v32acc32 | acc1,
|  | v32acc32 | acc2,
|  | int | zero_acc1,
|  | int | sub_mul,
|  | int | sub_acc1,
|  | int | sub_acc2 )

Parameters

  a | Matrix A
  b | Matrix B
  acc1 | Accumulator 1 input
  acc2 | Accumulator 2 input
  zero_acc1 | Zeroing mask for acc1
  sub_mul | Negation mask of multiplication result
  sub_acc1 | Negation mask of acc1
  sub_acc2 | Negation mask of acc2

Returns
  Result of operation

## ◆ submsc_4x2_2x8_conf() [5/8]

v32acc32 submsc_4x2_2x8_conf | ( | v32uint16 | a,
|  | int | sgn_x,
|  | v32int16 | b,
|  | int | sgn_y,
|  | v32acc32 | acc1,
|  | v32acc32 | acc2,
|  | int | zero_acc1,
|  | int | sub_mul,
|  | int | sub_acc1,
|  | int | sub_acc2 )

Parameters

  a | Matrix A
  sgn_x | Sign mask for matrix A
  b | Matrix B
  sgn_y | Sign mask for matrix B
  acc1 | Accumulator 1 input
  acc2 | Accumulator 2 input
  zero_acc1 | Zeroing mask for acc1
  sub_mul | Negation mask of multiplication result.
  sub_acc1 | Negation mask of acc1
  sub_acc2 | Negation mask of acc2

Returns
  Result of operation

## ◆ submsc_4x2_2x8_conf() [6/8]

v32acc32 submsc_4x2_2x8_conf | ( | v32uint16 | a,
|  | int | sgn_x,
|  | v32uint16 | b,
|  | int | sgn_y,
|  | v32acc32 | acc1,
|  | v32acc32 | acc2,
|  | int | zero_acc1,
|  | int | sub_mul,
|  | int | sub_acc1,
|  | int | sub_acc2 )

Parameters

  a | Matrix A
  sgn_x | Sign mask for matrix A
  b | Matrix B
  sgn_y | Sign mask for matrix B
  acc1 | Accumulator 1 input
  acc2 | Accumulator 2 input
  zero_acc1 | Zeroing mask for acc1
  sub_mul | Negation mask of multiplication result.
  sub_acc1 | Negation mask of acc1
  sub_acc2 | Negation mask of acc2

Returns
  Result of operation

## ◆ submsc_4x2_2x8_conf() [7/8]

v32acc32 submsc_4x2_2x8_conf | ( | v32uint16 | a,
|  | v32int16 | b,
|  | v32acc32 | acc1,
|  | v32acc32 | acc2,
|  | int | zero_acc1,
|  | int | sub_mul,
|  | int | sub_acc1,
|  | int | sub_acc2 )

Parameters

  a | Matrix A
  b | Matrix B
  acc1 | Accumulator 1 input
  acc2 | Accumulator 2 input
  zero_acc1 | Zeroing mask for acc1
  sub_mul | Negation mask of multiplication result
  sub_acc1 | Negation mask of acc1
  sub_acc2 | Negation mask of acc2

Returns
  Result of operation

## ◆ submsc_4x2_2x8_conf() [8/8]

v32acc32 submsc_4x2_2x8_conf | ( | v32uint16 | a,
|  | v32uint16 | b,
|  | v32acc32 | acc1,
|  | v32acc32 | acc2,
|  | int | zero_acc1,
|  | int | sub_mul,
|  | int | sub_acc1,
|  | int | sub_acc2 )

Parameters

  a | Matrix A
  b | Matrix B
  acc1 | Accumulator 1 input
  acc2 | Accumulator 2 input
  zero_acc1 | Zeroing mask for acc1
  sub_mul | Negation mask of multiplication result
  sub_acc1 | Negation mask of acc1
  sub_acc2 | Negation mask of acc2

Returns
  Result of operation

## ◆ submsc_4x4_4x4() [1/8]

v16acc64 submsc_4x4_4x4 | ( | v32int16 | a,
|  | int | sgn_x,
|  | v32int16 | b,
|  | int | sgn_y,
|  | v16acc64 | acc1,
|  | v16acc64 | acc2 )

Parameters

  a | Matrix A
  sgn_x | Sign mask for matrix A
  b | Matrix B
  sgn_y | Sign mask for matrix B
  acc1 | Accumulator 1 input
  acc2 | Accumulator 2 input

Returns
  Result of operation

## ◆ submsc_4x4_4x4() [2/8]

v16acc64 submsc_4x4_4x4 | ( | v32int16 | a,
|  | int | sgn_x,
|  | v32uint16 | b,
|  | int | sgn_y,
|  | v16acc64 | acc1,
|  | v16acc64 | acc2 )

Parameters

  a | Matrix A
  sgn_x | Sign mask for matrix A
  b | Matrix B
  sgn_y | Sign mask for matrix B
  acc1 | Accumulator 1 input
  acc2 | Accumulator 2 input

Returns
  Result of operation

## ◆ submsc_4x4_4x4() [3/8]

v16acc64 submsc_4x4_4x4 | ( | v32int16 | a,
|  | v32int16 | b,
|  | v16acc64 | acc1,
|  | v16acc64 | acc2 )

Parameters

  a | Matrix A
  b | Matrix B
  acc1 | Accumulator 1 input
  acc2 | Accumulator 2 input

Returns
  Result of operation

## ◆ submsc_4x4_4x4() [4/8]

v16acc64 submsc_4x4_4x4 | ( | v32int16 | a,
|  | v32uint16 | b,
|  | v16acc64 | acc1,
|  | v16acc64 | acc2 )

Parameters

  a | Matrix A
  b | Matrix B
  acc1 | Accumulator 1 input
  acc2 | Accumulator 2 input

Returns
  Result of operation

## ◆ submsc_4x4_4x4() [5/8]

v16acc64 submsc_4x4_4x4 | ( | v32uint16 | a,
|  | int | sgn_x,
|  | v32int16 | b,
|  | int | sgn_y,
|  | v16acc64 | acc1,
|  | v16acc64 | acc2 )

Parameters

  a | Matrix A
  sgn_x | Sign mask for matrix A
  b | Matrix B
  sgn_y | Sign mask for matrix B
  acc1 | Accumulator 1 input
  acc2 | Accumulator 2 input

Returns
  Result of operation

## ◆ submsc_4x4_4x4() [6/8]

v16acc64 submsc_4x4_4x4 | ( | v32uint16 | a,
|  | int | sgn_x,
|  | v32uint16 | b,
|  | int | sgn_y,
|  | v16acc64 | acc1,
|  | v16acc64 | acc2 )

Parameters

  a | Matrix A
  sgn_x | Sign mask for matrix A
  b | Matrix B
  sgn_y | Sign mask for matrix B
  acc1 | Accumulator 1 input
  acc2 | Accumulator 2 input

Returns
  Result of operation

## ◆ submsc_4x4_4x4() [7/8]

v16acc64 submsc_4x4_4x4 | ( | v32uint16 | a,
|  | v32int16 | b,
|  | v16acc64 | acc1,
|  | v16acc64 | acc2 )

Parameters

  a | Matrix A
  b | Matrix B
  acc1 | Accumulator 1 input
  acc2 | Accumulator 2 input

Returns
  Result of operation

## ◆ submsc_4x4_4x4() [8/8]

v16acc64 submsc_4x4_4x4 | ( | v32uint16 | a,
|  | v32uint16 | b,
|  | v16acc64 | acc1,
|  | v16acc64 | acc2 )

Parameters

  a | Matrix A
  b | Matrix B
  acc1 | Accumulator 1 input
  acc2 | Accumulator 2 input

Returns
  Result of operation

## ◆ submsc_4x4_4x4_conf() [1/8]

v16acc64 submsc_4x4_4x4_conf | ( | v32int16 | a,
|  | int | sgn_x,
|  | v32int16 | b,
|  | int | sgn_y,
|  | v16acc64 | acc1,
|  | v16acc64 | acc2,
|  | int | zero_acc1,
|  | int | sub_mul,
|  | int | sub_acc1,
|  | int | sub_acc2 )

Parameters

  a | Matrix A
  sgn_x | Sign mask for matrix A
  b | Matrix B
  sgn_y | Sign mask for matrix B
  acc1 | Accumulator 1 input
  acc2 | Accumulator 2 input
  zero_acc1 | Zeroing mask for acc1
  sub_mul | Negation mask of multiplication result.
  sub_acc1 | Negation mask of acc1
  sub_acc2 | Negation mask of acc2

Returns
  Result of operation

## ◆ submsc_4x4_4x4_conf() [2/8]

v16acc64 submsc_4x4_4x4_conf | ( | v32int16 | a,
|  | int | sgn_x,
|  | v32uint16 | b,
|  | int | sgn_y,
|  | v16acc64 | acc1,
|  | v16acc64 | acc2,
|  | int | zero_acc1,
|  | int | sub_mul,
|  | int | sub_acc1,
|  | int | sub_acc2 )

Parameters

  a | Matrix A
  sgn_x | Sign mask for matrix A
  b | Matrix B
  sgn_y | Sign mask for matrix B
  acc1 | Accumulator 1 input
  acc2 | Accumulator 2 input
  zero_acc1 | Zeroing mask for acc1
  sub_mul | Negation mask of multiplication result.
  sub_acc1 | Negation mask of acc1
  sub_acc2 | Negation mask of acc2

Returns
  Result of operation

## ◆ submsc_4x4_4x4_conf() [3/8]

v16acc64 submsc_4x4_4x4_conf | ( | v32int16 | a,
|  | v32int16 | b,
|  | v16acc64 | acc1,
|  | v16acc64 | acc2,
|  | int | zero_acc1,
|  | int | sub_mul,
|  | int | sub_acc1,
|  | int | sub_acc2 )

Parameters

  a | Matrix A
  b | Matrix B
  acc1 | Accumulator 1 input
  acc2 | Accumulator 2 input
  zero_acc1 | Zeroing mask for acc1
  sub_mul | Negation mask of multiplication result
  sub_acc1 | Negation mask of acc1
  sub_acc2 | Negation mask of acc2

Returns
  Result of operation

## ◆ submsc_4x4_4x4_conf() [4/8]

v16acc64 submsc_4x4_4x4_conf | ( | v32int16 | a,
|  | v32uint16 | b,
|  | v16acc64 | acc1,
|  | v16acc64 | acc2,
|  | int | zero_acc1,
|  | int | sub_mul,
|  | int | sub_acc1,
|  | int | sub_acc2 )

Parameters

  a | Matrix A
  b | Matrix B
  acc1 | Accumulator 1 input
  acc2 | Accumulator 2 input
  zero_acc1 | Zeroing mask for acc1
  sub_mul | Negation mask of multiplication result
  sub_acc1 | Negation mask of acc1
  sub_acc2 | Negation mask of acc2

Returns
  Result of operation

## ◆ submsc_4x4_4x4_conf() [5/8]

v16acc64 submsc_4x4_4x4_conf | ( | v32uint16 | a,
|  | int | sgn_x,
|  | v32int16 | b,
|  | int | sgn_y,
|  | v16acc64 | acc1,
|  | v16acc64 | acc2,
|  | int | zero_acc1,
|  | int | sub_mul,
|  | int | sub_acc1,
|  | int | sub_acc2 )

Parameters

  a | Matrix A
  sgn_x | Sign mask for matrix A
  b | Matrix B
  sgn_y | Sign mask for matrix B
  acc1 | Accumulator 1 input
  acc2 | Accumulator 2 input
  zero_acc1 | Zeroing mask for acc1
  sub_mul | Negation mask of multiplication result.
  sub_acc1 | Negation mask of acc1
  sub_acc2 | Negation mask of acc2

Returns
  Result of operation

## ◆ submsc_4x4_4x4_conf() [6/8]

v16acc64 submsc_4x4_4x4_conf | ( | v32uint16 | a,
|  | int | sgn_x,
|  | v32uint16 | b,
|  | int | sgn_y,
|  | v16acc64 | acc1,
|  | v16acc64 | acc2,
|  | int | zero_acc1,
|  | int | sub_mul,
|  | int | sub_acc1,
|  | int | sub_acc2 )

Parameters

  a | Matrix A
  sgn_x | Sign mask for matrix A
  b | Matrix B
  sgn_y | Sign mask for matrix B
  acc1 | Accumulator 1 input
  acc2 | Accumulator 2 input
  zero_acc1 | Zeroing mask for acc1
  sub_mul | Negation mask of multiplication result.
  sub_acc1 | Negation mask of acc1
  sub_acc2 | Negation mask of acc2

Returns
  Result of operation

## ◆ submsc_4x4_4x4_conf() [7/8]

v16acc64 submsc_4x4_4x4_conf | ( | v32uint16 | a,
|  | v32int16 | b,
|  | v16acc64 | acc1,
|  | v16acc64 | acc2,
|  | int | zero_acc1,
|  | int | sub_mul,
|  | int | sub_acc1,
|  | int | sub_acc2 )

Parameters

  a | Matrix A
  b | Matrix B
  acc1 | Accumulator 1 input
  acc2 | Accumulator 2 input
  zero_acc1 | Zeroing mask for acc1
  sub_mul | Negation mask of multiplication result
  sub_acc1 | Negation mask of acc1
  sub_acc2 | Negation mask of acc2

Returns
  Result of operation

## ◆ submsc_4x4_4x4_conf() [8/8]

v16acc64 submsc_4x4_4x4_conf | ( | v32uint16 | a,
|  | v32uint16 | b,
|  | v16acc64 | acc1,
|  | v16acc64 | acc2,
|  | int | zero_acc1,
|  | int | sub_mul,
|  | int | sub_acc1,
|  | int | sub_acc2 )

Parameters

  a | Matrix A
  b | Matrix B
  acc1 | Accumulator 1 input
  acc2 | Accumulator 2 input
  zero_acc1 | Zeroing mask for acc1
  sub_mul | Negation mask of multiplication result
  sub_acc1 | Negation mask of acc1
  sub_acc2 | Negation mask of acc2

Returns
  Result of operation

## ◆ submsc_conv_16x4() [1/8]

v16acc64 submsc_conv_16x4 | ( | v32int16 | a,
|  | int | sgn_x,
|  | v32int16 | b,
|  | int | sgn_y,
|  | v16acc64 | acc1,
|  | v16acc64 | acc2 )

Parameters

  a | Matrix A
  sgn_x | Sign mask for matrix A
  b | Matrix B
  sgn_y | Sign mask for matrix B
  acc1 | Accumulator 1 input
  acc2 | Accumulator 2 input

Returns
  Result of operation

## ◆ submsc_conv_16x4() [2/8]

v16acc64 submsc_conv_16x4 | ( | v32int16 | a,
|  | int | sgn_x,
|  | v32uint16 | b,
|  | int | sgn_y,
|  | v16acc64 | acc1,
|  | v16acc64 | acc2 )

Parameters

  a | Matrix A
  sgn_x | Sign mask for matrix A
  b | Matrix B
  sgn_y | Sign mask for matrix B
  acc1 | Accumulator 1 input
  acc2 | Accumulator 2 input

Returns
  Result of operation

## ◆ submsc_conv_16x4() [3/8]

v16acc64 submsc_conv_16x4 | ( | v32int16 | a,
|  | v32int16 | b,
|  | v16acc64 | acc1,
|  | v16acc64 | acc2 )

Parameters

  a | Matrix A
  b | Matrix B
  acc1 | Accumulator 1 input
  acc2 | Accumulator 2 input

Returns
  Result of operation

## ◆ submsc_conv_16x4() [4/8]

v16acc64 submsc_conv_16x4 | ( | v32int16 | a,
|  | v32uint16 | b,
|  | v16acc64 | acc1,
|  | v16acc64 | acc2 )

Parameters

  a | Matrix A
  b | Matrix B
  acc1 | Accumulator 1 input
  acc2 | Accumulator 2 input

Returns
  Result of operation

## ◆ submsc_conv_16x4() [5/8]

v16acc64 submsc_conv_16x4 | ( | v32uint16 | a,
|  | int | sgn_x,
|  | v32int16 | b,
|  | int | sgn_y,
|  | v16acc64 | acc1,
|  | v16acc64 | acc2 )

Parameters

  a | Matrix A
  sgn_x | Sign mask for matrix A
  b | Matrix B
  sgn_y | Sign mask for matrix B
  acc1 | Accumulator 1 input
  acc2 | Accumulator 2 input

Returns
  Result of operation

## ◆ submsc_conv_16x4() [6/8]

v16acc64 submsc_conv_16x4 | ( | v32uint16 | a,
|  | int | sgn_x,
|  | v32uint16 | b,
|  | int | sgn_y,
|  | v16acc64 | acc1,
|  | v16acc64 | acc2 )

Parameters

  a | Matrix A
  sgn_x | Sign mask for matrix A
  b | Matrix B
  sgn_y | Sign mask for matrix B
  acc1 | Accumulator 1 input
  acc2 | Accumulator 2 input

Returns
  Result of operation

## ◆ submsc_conv_16x4() [7/8]

v16acc64 submsc_conv_16x4 | ( | v32uint16 | a,
|  | v32int16 | b,
|  | v16acc64 | acc1,
|  | v16acc64 | acc2 )

Parameters

  a | Matrix A
  b | Matrix B
  acc1 | Accumulator 1 input
  acc2 | Accumulator 2 input

Returns
  Result of operation

## ◆ submsc_conv_16x4() [8/8]

v16acc64 submsc_conv_16x4 | ( | v32uint16 | a,
|  | v32uint16 | b,
|  | v16acc64 | acc1,
|  | v16acc64 | acc2 )

Parameters

  a | Matrix A
  b | Matrix B
  acc1 | Accumulator 1 input
  acc2 | Accumulator 2 input

Returns
  Result of operation

## ◆ submsc_conv_16x4_conf() [1/8]

v16acc64 submsc_conv_16x4_conf | ( | v32int16 | a,
|  | int | sgn_x,
|  | v32int16 | b,
|  | int | sgn_y,
|  | v16acc64 | acc1,
|  | v16acc64 | acc2,
|  | int | zero_acc1,
|  | int | sub_mul,
|  | int | sub_acc1,
|  | int | sub_acc2 )

Parameters

  a | Matrix A
  sgn_x | Sign mask for matrix A
  b | Matrix B
  sgn_y | Sign mask for matrix B
  acc1 | Accumulator 1 input
  acc2 | Accumulator 2 input
  zero_acc1 | Zeroing mask for acc1
  sub_mul | Negation mask of multiplication result.
  sub_acc1 | Negation mask of acc1
  sub_acc2 | Negation mask of acc2

Returns
  Result of operation

## ◆ submsc_conv_16x4_conf() [2/8]

v16acc64 submsc_conv_16x4_conf | ( | v32int16 | a,
|  | int | sgn_x,
|  | v32uint16 | b,
|  | int | sgn_y,
|  | v16acc64 | acc1,
|  | v16acc64 | acc2,
|  | int | zero_acc1,
|  | int | sub_mul,
|  | int | sub_acc1,
|  | int | sub_acc2 )

Parameters

  a | Matrix A
  sgn_x | Sign mask for matrix A
  b | Matrix B
  sgn_y | Sign mask for matrix B
  acc1 | Accumulator 1 input
  acc2 | Accumulator 2 input
  zero_acc1 | Zeroing mask for acc1
  sub_mul | Negation mask of multiplication result.
  sub_acc1 | Negation mask of acc1
  sub_acc2 | Negation mask of acc2

Returns
  Result of operation

## ◆ submsc_conv_16x4_conf() [3/8]

v16acc64 submsc_conv_16x4_conf | ( | v32int16 | a,
|  | v32int16 | b,
|  | v16acc64 | acc1,
|  | v16acc64 | acc2,
|  | int | zero_acc1,
|  | int | sub_mul,
|  | int | sub_acc1,
|  | int | sub_acc2 )

Parameters

  a | Matrix A
  b | Matrix B
  acc1 | Accumulator 1 input
  acc2 | Accumulator 2 input
  zero_acc1 | Zeroing mask for acc1
  sub_mul | Negation mask of multiplication result
  sub_acc1 | Negation mask of acc1
  sub_acc2 | Negation mask of acc2

Returns
  Result of operation

## ◆ submsc_conv_16x4_conf() [4/8]

v16acc64 submsc_conv_16x4_conf | ( | v32int16 | a,
|  | v32uint16 | b,
|  | v16acc64 | acc1,
|  | v16acc64 | acc2,
|  | int | zero_acc1,
|  | int | sub_mul,
|  | int | sub_acc1,
|  | int | sub_acc2 )

Parameters

  a | Matrix A
  b | Matrix B
  acc1 | Accumulator 1 input
  acc2 | Accumulator 2 input
  zero_acc1 | Zeroing mask for acc1
  sub_mul | Negation mask of multiplication result
  sub_acc1 | Negation mask of acc1
  sub_acc2 | Negation mask of acc2

Returns
  Result of operation

## ◆ submsc_conv_16x4_conf() [5/8]

v16acc64 submsc_conv_16x4_conf | ( | v32uint16 | a,
|  | int | sgn_x,
|  | v32int16 | b,
|  | int | sgn_y,
|  | v16acc64 | acc1,
|  | v16acc64 | acc2,
|  | int | zero_acc1,
|  | int | sub_mul,
|  | int | sub_acc1,
|  | int | sub_acc2 )

Parameters

  a | Matrix A
  sgn_x | Sign mask for matrix A
  b | Matrix B
  sgn_y | Sign mask for matrix B
  acc1 | Accumulator 1 input
  acc2 | Accumulator 2 input
  zero_acc1 | Zeroing mask for acc1
  sub_mul | Negation mask of multiplication result.
  sub_acc1 | Negation mask of acc1
  sub_acc2 | Negation mask of acc2

Returns
  Result of operation

## ◆ submsc_conv_16x4_conf() [6/8]

v16acc64 submsc_conv_16x4_conf | ( | v32uint16 | a,
|  | int | sgn_x,
|  | v32uint16 | b,
|  | int | sgn_y,
|  | v16acc64 | acc1,
|  | v16acc64 | acc2,
|  | int | zero_acc1,
|  | int | sub_mul,
|  | int | sub_acc1,
|  | int | sub_acc2 )

Parameters

  a | Matrix A
  sgn_x | Sign mask for matrix A
  b | Matrix B
  sgn_y | Sign mask for matrix B
  acc1 | Accumulator 1 input
  acc2 | Accumulator 2 input
  zero_acc1 | Zeroing mask for acc1
  sub_mul | Negation mask of multiplication result.
  sub_acc1 | Negation mask of acc1
  sub_acc2 | Negation mask of acc2

Returns
  Result of operation

## ◆ submsc_conv_16x4_conf() [7/8]

v16acc64 submsc_conv_16x4_conf | ( | v32uint16 | a,
|  | v32int16 | b,
|  | v16acc64 | acc1,
|  | v16acc64 | acc2,
|  | int | zero_acc1,
|  | int | sub_mul,
|  | int | sub_acc1,
|  | int | sub_acc2 )

Parameters

  a | Matrix A
  b | Matrix B
  acc1 | Accumulator 1 input
  acc2 | Accumulator 2 input
  zero_acc1 | Zeroing mask for acc1
  sub_mul | Negation mask of multiplication result
  sub_acc1 | Negation mask of acc1
  sub_acc2 | Negation mask of acc2

Returns
  Result of operation

## ◆ submsc_conv_16x4_conf() [8/8]

v16acc64 submsc_conv_16x4_conf | ( | v32uint16 | a,
|  | v32uint16 | b,
|  | v16acc64 | acc1,
|  | v16acc64 | acc2,
|  | int | zero_acc1,
|  | int | sub_mul,
|  | int | sub_acc1,
|  | int | sub_acc2 )

Parameters

  a | Matrix A
  b | Matrix B
  acc1 | Accumulator 1 input
  acc2 | Accumulator 2 input
  zero_acc1 | Zeroing mask for acc1
  sub_mul | Negation mask of multiplication result
  sub_acc1 | Negation mask of acc1
  sub_acc2 | Negation mask of acc2

Returns
  Result of operation

## ◆ submsc_elem_16_2() [1/8]

v16acc64 submsc_elem_16_2 | ( | v32int16 | a,
|  | int | sgn_x,
|  | v32int16 | b,
|  | int | sgn_y,
|  | v16acc64 | acc1,
|  | v16acc64 | acc2 )

Parameters

  a | Matrix A
  sgn_x | Sign mask for matrix A
  b | Matrix B
  sgn_y | Sign mask for matrix B
  acc1 | Accumulator 1 input
  acc2 | Accumulator 2 input

Returns
  Result of operation

## ◆ submsc_elem_16_2() [2/8]

v16acc64 submsc_elem_16_2 | ( | v32int16 | a,
|  | int | sgn_x,
|  | v32uint16 | b,
|  | int | sgn_y,
|  | v16acc64 | acc1,
|  | v16acc64 | acc2 )

Parameters

  a | Matrix A
  sgn_x | Sign mask for matrix A
  b | Matrix B
  sgn_y | Sign mask for matrix B
  acc1 | Accumulator 1 input
  acc2 | Accumulator 2 input

Returns
  Result of operation

## ◆ submsc_elem_16_2() [3/8]

v16acc64 submsc_elem_16_2 | ( | v32int16 | a,
|  | v32int16 | b,
|  | v16acc64 | acc1,
|  | v16acc64 | acc2 )

Parameters

  a | Matrix A
  b | Matrix B
  acc1 | Accumulator 1 input
  acc2 | Accumulator 2 input

Returns
  Result of operation

## ◆ submsc_elem_16_2() [4/8]

v16acc64 submsc_elem_16_2 | ( | v32int16 | a,
|  | v32uint16 | b,
|  | v16acc64 | acc1,
|  | v16acc64 | acc2 )

Parameters

  a | Matrix A
  b | Matrix B
  acc1 | Accumulator 1 input
  acc2 | Accumulator 2 input

Returns
  Result of operation

## ◆ submsc_elem_16_2() [5/8]

v16acc64 submsc_elem_16_2 | ( | v32uint16 | a,
|  | int | sgn_x,
|  | v32int16 | b,
|  | int | sgn_y,
|  | v16acc64 | acc1,
|  | v16acc64 | acc2 )

Parameters

  a | Matrix A
  sgn_x | Sign mask for matrix A
  b | Matrix B
  sgn_y | Sign mask for matrix B
  acc1 | Accumulator 1 input
  acc2 | Accumulator 2 input

Returns
  Result of operation

## ◆ submsc_elem_16_2() [6/8]

v16acc64 submsc_elem_16_2 | ( | v32uint16 | a,
|  | int | sgn_x,
|  | v32uint16 | b,
|  | int | sgn_y,
|  | v16acc64 | acc1,
|  | v16acc64 | acc2 )

Parameters

  a | Matrix A
  sgn_x | Sign mask for matrix A
  b | Matrix B
  sgn_y | Sign mask for matrix B
  acc1 | Accumulator 1 input
  acc2 | Accumulator 2 input

Returns
  Result of operation

## ◆ submsc_elem_16_2() [7/8]

v16acc64 submsc_elem_16_2 | ( | v32uint16 | a,
|  | v32int16 | b,
|  | v16acc64 | acc1,
|  | v16acc64 | acc2 )

Parameters

  a | Matrix A
  b | Matrix B
  acc1 | Accumulator 1 input
  acc2 | Accumulator 2 input

Returns
  Result of operation

## ◆ submsc_elem_16_2() [8/8]

v16acc64 submsc_elem_16_2 | ( | v32uint16 | a,
|  | v32uint16 | b,
|  | v16acc64 | acc1,
|  | v16acc64 | acc2 )

Parameters

  a | Matrix A
  b | Matrix B
  acc1 | Accumulator 1 input
  acc2 | Accumulator 2 input

Returns
  Result of operation

## ◆ submsc_elem_16_2_conf() [1/8]

v16acc64 submsc_elem_16_2_conf | ( | v32int16 | a,
|  | int | sgn_x,
|  | v32int16 | b,
|  | int | sgn_y,
|  | v16acc64 | acc1,
|  | v16acc64 | acc2,
|  | int | zero_acc1,
|  | int | sub_mul,
|  | int | sub_acc1,
|  | int | sub_acc2 )

Parameters

  a | Matrix A
  sgn_x | Sign mask for matrix A
  b | Matrix B
  sgn_y | Sign mask for matrix B
  acc1 | Accumulator 1 input
  acc2 | Accumulator 2 input
  zero_acc1 | Zeroing mask for acc1
  sub_mul | Negation mask of multiplication result.
  sub_acc1 | Negation mask of acc1
  sub_acc2 | Negation mask of acc2

Returns
  Result of operation

## ◆ submsc_elem_16_2_conf() [2/8]

v16acc64 submsc_elem_16_2_conf | ( | v32int16 | a,
|  | int | sgn_x,
|  | v32uint16 | b,
|  | int | sgn_y,
|  | v16acc64 | acc1,
|  | v16acc64 | acc2,
|  | int | zero_acc1,
|  | int | sub_mul,
|  | int | sub_acc1,
|  | int | sub_acc2 )

Parameters

  a | Matrix A
  sgn_x | Sign mask for matrix A
  b | Matrix B
  sgn_y | Sign mask for matrix B
  acc1 | Accumulator 1 input
  acc2 | Accumulator 2 input
  zero_acc1 | Zeroing mask for acc1
  sub_mul | Negation mask of multiplication result.
  sub_acc1 | Negation mask of acc1
  sub_acc2 | Negation mask of acc2

Returns
  Result of operation

## ◆ submsc_elem_16_2_conf() [3/8]

v16acc64 submsc_elem_16_2_conf | ( | v32int16 | a,
|  | v32int16 | b,
|  | v16acc64 | acc1,
|  | v16acc64 | acc2,
|  | int | zero_acc1,
|  | int | sub_mul,
|  | int | sub_acc1,
|  | int | sub_acc2 )

Parameters

  a | Matrix A
  b | Matrix B
  acc1 | Accumulator 1 input
  acc2 | Accumulator 2 input
  zero_acc1 | Zeroing mask for acc1
  sub_mul | Negation mask of multiplication result
  sub_acc1 | Negation mask of acc1
  sub_acc2 | Negation mask of acc2

Returns
  Result of operation

## ◆ submsc_elem_16_2_conf() [4/8]

v16acc64 submsc_elem_16_2_conf | ( | v32int16 | a,
|  | v32uint16 | b,
|  | v16acc64 | acc1,
|  | v16acc64 | acc2,
|  | int | zero_acc1,
|  | int | sub_mul,
|  | int | sub_acc1,
|  | int | sub_acc2 )

Parameters

  a | Matrix A
  b | Matrix B
  acc1 | Accumulator 1 input
  acc2 | Accumulator 2 input
  zero_acc1 | Zeroing mask for acc1
  sub_mul | Negation mask of multiplication result
  sub_acc1 | Negation mask of acc1
  sub_acc2 | Negation mask of acc2

Returns
  Result of operation

## ◆ submsc_elem_16_2_conf() [5/8]

v16acc64 submsc_elem_16_2_conf | ( | v32uint16 | a,
|  | int | sgn_x,
|  | v32int16 | b,
|  | int | sgn_y,
|  | v16acc64 | acc1,
|  | v16acc64 | acc2,
|  | int | zero_acc1,
|  | int | sub_mul,
|  | int | sub_acc1,
|  | int | sub_acc2 )

Parameters

  a | Matrix A
  sgn_x | Sign mask for matrix A
  b | Matrix B
  sgn_y | Sign mask for matrix B
  acc1 | Accumulator 1 input
  acc2 | Accumulator 2 input
  zero_acc1 | Zeroing mask for acc1
  sub_mul | Negation mask of multiplication result.
  sub_acc1 | Negation mask of acc1
  sub_acc2 | Negation mask of acc2

Returns
  Result of operation

## ◆ submsc_elem_16_2_conf() [6/8]

v16acc64 submsc_elem_16_2_conf | ( | v32uint16 | a,
|  | int | sgn_x,
|  | v32uint16 | b,
|  | int | sgn_y,
|  | v16acc64 | acc1,
|  | v16acc64 | acc2,
|  | int | zero_acc1,
|  | int | sub_mul,
|  | int | sub_acc1,
|  | int | sub_acc2 )

Parameters

  a | Matrix A
  sgn_x | Sign mask for matrix A
  b | Matrix B
  sgn_y | Sign mask for matrix B
  acc1 | Accumulator 1 input
  acc2 | Accumulator 2 input
  zero_acc1 | Zeroing mask for acc1
  sub_mul | Negation mask of multiplication result.
  sub_acc1 | Negation mask of acc1
  sub_acc2 | Negation mask of acc2

Returns
  Result of operation

## ◆ submsc_elem_16_2_conf() [7/8]

v16acc64 submsc_elem_16_2_conf | ( | v32uint16 | a,
|  | v32int16 | b,
|  | v16acc64 | acc1,
|  | v16acc64 | acc2,
|  | int | zero_acc1,
|  | int | sub_mul,
|  | int | sub_acc1,
|  | int | sub_acc2 )

Parameters

  a | Matrix A
  b | Matrix B
  acc1 | Accumulator 1 input
  acc2 | Accumulator 2 input
  zero_acc1 | Zeroing mask for acc1
  sub_mul | Negation mask of multiplication result
  sub_acc1 | Negation mask of acc1
  sub_acc2 | Negation mask of acc2

Returns
  Result of operation

## ◆ submsc_elem_16_2_conf() [8/8]

v16acc64 submsc_elem_16_2_conf | ( | v32uint16 | a,
|  | v32uint16 | b,
|  | v16acc64 | acc1,
|  | v16acc64 | acc2,
|  | int | zero_acc1,
|  | int | sub_mul,
|  | int | sub_acc1,
|  | int | sub_acc2 )

Parameters

  a | Matrix A
  b | Matrix B
  acc1 | Accumulator 1 input
  acc2 | Accumulator 2 input
  zero_acc1 | Zeroing mask for acc1
  sub_mul | Negation mask of multiplication result
  sub_acc1 | Negation mask of acc1
  sub_acc2 | Negation mask of acc2

Returns
  Result of operation

## ◆ submsc_elem_32() [1/8]

v32acc32 submsc_elem_32 | ( | v32int16 | a,
|  | int | sgn_x,
|  | v32int16 | b,
|  | int | sgn_y,
|  | v32acc32 | acc1,
|  | v32acc32 | acc2 )

Parameters

  a | Matrix A
  sgn_x | Sign mask for matrix A
  b | Matrix B
  sgn_y | Sign mask for matrix B
  acc1 | Accumulator 1 input
  acc2 | Accumulator 2 input

Returns
  Result of operation

## ◆ submsc_elem_32() [2/8]

v32acc32 submsc_elem_32 | ( | v32int16 | a,
|  | int | sgn_x,
|  | v32uint16 | b,
|  | int | sgn_y,
|  | v32acc32 | acc1,
|  | v32acc32 | acc2 )

Parameters

  a | Matrix A
  sgn_x | Sign mask for matrix A
  b | Matrix B
  sgn_y | Sign mask for matrix B
  acc1 | Accumulator 1 input
  acc2 | Accumulator 2 input

Returns
  Result of operation

## ◆ submsc_elem_32() [3/8]

v32acc32 submsc_elem_32 | ( | v32int16 | a,
|  | v32int16 | b,
|  | v32acc32 | acc1,
|  | v32acc32 | acc2 )

Parameters

  a | Matrix A
  b | Matrix B
  acc1 | Accumulator 1 input
  acc2 | Accumulator 2 input

Returns
  Result of operation

## ◆ submsc_elem_32() [4/8]

v32acc32 submsc_elem_32 | ( | v32int16 | a,
|  | v32uint16 | b,
|  | v32acc32 | acc1,
|  | v32acc32 | acc2 )

Parameters

  a | Matrix A
  b | Matrix B
  acc1 | Accumulator 1 input
  acc2 | Accumulator 2 input

Returns
  Result of operation

## ◆ submsc_elem_32() [5/8]

v32acc32 submsc_elem_32 | ( | v32uint16 | a,
|  | int | sgn_x,
|  | v32int16 | b,
|  | int | sgn_y,
|  | v32acc32 | acc1,
|  | v32acc32 | acc2 )

Parameters

  a | Matrix A
  sgn_x | Sign mask for matrix A
  b | Matrix B
  sgn_y | Sign mask for matrix B
  acc1 | Accumulator 1 input
  acc2 | Accumulator 2 input

Returns
  Result of operation

## ◆ submsc_elem_32() [6/8]

v32acc32 submsc_elem_32 | ( | v32uint16 | a,
|  | int | sgn_x,
|  | v32uint16 | b,
|  | int | sgn_y,
|  | v32acc32 | acc1,
|  | v32acc32 | acc2 )

Parameters

  a | Matrix A
  sgn_x | Sign mask for matrix A
  b | Matrix B
  sgn_y | Sign mask for matrix B
  acc1 | Accumulator 1 input
  acc2 | Accumulator 2 input

Returns
  Result of operation

## ◆ submsc_elem_32() [7/8]

v32acc32 submsc_elem_32 | ( | v32uint16 | a,
|  | v32int16 | b,
|  | v32acc32 | acc1,
|  | v32acc32 | acc2 )

Parameters

  a | Matrix A
  b | Matrix B
  acc1 | Accumulator 1 input
  acc2 | Accumulator 2 input

Returns
  Result of operation

## ◆ submsc_elem_32() [8/8]

v32acc32 submsc_elem_32 | ( | v32uint16 | a,
|  | v32uint16 | b,
|  | v32acc32 | acc1,
|  | v32acc32 | acc2 )

Parameters

  a | Matrix A
  b | Matrix B
  acc1 | Accumulator 1 input
  acc2 | Accumulator 2 input

Returns
  Result of operation

## ◆ submsc_elem_32_conf() [1/8]

v32acc32 submsc_elem_32_conf | ( | v32int16 | a,
|  | int | sgn_x,
|  | v32int16 | b,
|  | int | sgn_y,
|  | v32acc32 | acc1,
|  | v32acc32 | acc2,
|  | int | zero_acc1,
|  | int | sub_mul,
|  | int | sub_acc1,
|  | int | sub_acc2 )

Parameters

  a | Matrix A
  sgn_x | Sign mask for matrix A
  b | Matrix B
  sgn_y | Sign mask for matrix B
  acc1 | Accumulator 1 input
  acc2 | Accumulator 2 input
  zero_acc1 | Zeroing mask for acc1
  sub_mul | Negation mask of multiplication result.
  sub_acc1 | Negation mask of acc1
  sub_acc2 | Negation mask of acc2

Returns
  Result of operation

## ◆ submsc_elem_32_conf() [2/8]

v32acc32 submsc_elem_32_conf | ( | v32int16 | a,
|  | int | sgn_x,
|  | v32uint16 | b,
|  | int | sgn_y,
|  | v32acc32 | acc1,
|  | v32acc32 | acc2,
|  | int | zero_acc1,
|  | int | sub_mul,
|  | int | sub_acc1,
|  | int | sub_acc2 )

Parameters

  a | Matrix A
  sgn_x | Sign mask for matrix A
  b | Matrix B
  sgn_y | Sign mask for matrix B
  acc1 | Accumulator 1 input
  acc2 | Accumulator 2 input
  zero_acc1 | Zeroing mask for acc1
  sub_mul | Negation mask of multiplication result.
  sub_acc1 | Negation mask of acc1
  sub_acc2 | Negation mask of acc2

Returns
  Result of operation

## ◆ submsc_elem_32_conf() [3/8]

v32acc32 submsc_elem_32_conf | ( | v32int16 | a,
|  | v32int16 | b,
|  | v32acc32 | acc1,
|  | v32acc32 | acc2,
|  | int | zero_acc1,
|  | int | sub_mul,
|  | int | sub_acc1,
|  | int | sub_acc2 )

Parameters

  a | Matrix A
  b | Matrix B
  acc1 | Accumulator 1 input
  acc2 | Accumulator 2 input
  zero_acc1 | Zeroing mask for acc1
  sub_mul | Negation mask of multiplication result
  sub_acc1 | Negation mask of acc1
  sub_acc2 | Negation mask of acc2

Returns
  Result of operation

## ◆ submsc_elem_32_conf() [4/8]

v32acc32 submsc_elem_32_conf | ( | v32int16 | a,
|  | v32uint16 | b,
|  | v32acc32 | acc1,
|  | v32acc32 | acc2,
|  | int | zero_acc1,
|  | int | sub_mul,
|  | int | sub_acc1,
|  | int | sub_acc2 )

Parameters

  a | Matrix A
  b | Matrix B
  acc1 | Accumulator 1 input
  acc2 | Accumulator 2 input
  zero_acc1 | Zeroing mask for acc1
  sub_mul | Negation mask of multiplication result
  sub_acc1 | Negation mask of acc1
  sub_acc2 | Negation mask of acc2

Returns
  Result of operation

## ◆ submsc_elem_32_conf() [5/8]

v32acc32 submsc_elem_32_conf | ( | v32uint16 | a,
|  | int | sgn_x,
|  | v32int16 | b,
|  | int | sgn_y,
|  | v32acc32 | acc1,
|  | v32acc32 | acc2,
|  | int | zero_acc1,
|  | int | sub_mul,
|  | int | sub_acc1,
|  | int | sub_acc2 )

Parameters

  a | Matrix A
  sgn_x | Sign mask for matrix A
  b | Matrix B
  sgn_y | Sign mask for matrix B
  acc1 | Accumulator 1 input
  acc2 | Accumulator 2 input
  zero_acc1 | Zeroing mask for acc1
  sub_mul | Negation mask of multiplication result.
  sub_acc1 | Negation mask of acc1
  sub_acc2 | Negation mask of acc2

Returns
  Result of operation

## ◆ submsc_elem_32_conf() [6/8]

v32acc32 submsc_elem_32_conf | ( | v32uint16 | a,
|  | int | sgn_x,
|  | v32uint16 | b,
|  | int | sgn_y,
|  | v32acc32 | acc1,
|  | v32acc32 | acc2,
|  | int | zero_acc1,
|  | int | sub_mul,
|  | int | sub_acc1,
|  | int | sub_acc2 )

Parameters

  a | Matrix A
  sgn_x | Sign mask for matrix A
  b | Matrix B
  sgn_y | Sign mask for matrix B
  acc1 | Accumulator 1 input
  acc2 | Accumulator 2 input
  zero_acc1 | Zeroing mask for acc1
  sub_mul | Negation mask of multiplication result.
  sub_acc1 | Negation mask of acc1
  sub_acc2 | Negation mask of acc2

Returns
  Result of operation

## ◆ submsc_elem_32_conf() [7/8]

v32acc32 submsc_elem_32_conf | ( | v32uint16 | a,
|  | v32int16 | b,
|  | v32acc32 | acc1,
|  | v32acc32 | acc2,
|  | int | zero_acc1,
|  | int | sub_mul,
|  | int | sub_acc1,
|  | int | sub_acc2 )

Parameters

  a | Matrix A
  b | Matrix B
  acc1 | Accumulator 1 input
  acc2 | Accumulator 2 input
  zero_acc1 | Zeroing mask for acc1
  sub_mul | Negation mask of multiplication result
  sub_acc1 | Negation mask of acc1
  sub_acc2 | Negation mask of acc2

Returns
  Result of operation

## ◆ submsc_elem_32_conf() [8/8]

v32acc32 submsc_elem_32_conf | ( | v32uint16 | a,
|  | v32uint16 | b,
|  | v32acc32 | acc1,
|  | v32acc32 | acc2,
|  | int | zero_acc1,
|  | int | sub_mul,
|  | int | sub_acc1,
|  | int | sub_acc2 )

Parameters

  a | Matrix A
  b | Matrix B
  acc1 | Accumulator 1 input
  acc2 | Accumulator 2 input
  zero_acc1 | Zeroing mask for acc1
  sub_mul | Negation mask of multiplication result
  sub_acc1 | Negation mask of acc1
  sub_acc2 | Negation mask of acc2

Returns
  Result of operation