| AI Engine-ML Intrinsics User Guide (v2025.2)

Loading...
Searching...
No Matches
Multiply-accumulate of 8b x 8b integer datatypes
Vector Operations » Multiply Accumulate

## Overview

Matrix multiplications in which matrix A and matrix B have data elements of 8 bit.

For an explanation how these operations works see Multiply Accumulate.

## Multiplication of (4x8) with (8x8)
v32acc32 | mul_4x8_8x8 (v64uint8 a, v64uint8 b)
v32acc32 | negmul_4x8_8x8 (v64uint8 a, v64uint8 b)
v32acc32 | mac_4x8_8x8 (v64uint8 a, v64uint8 b, v32acc32 acc1)
v32acc32 | msc_4x8_8x8 (v64uint8 a, v64uint8 b, v32acc32 acc1)
v32acc32 | negmac_4x8_8x8 (v64uint8 a, v64uint8 b, v32acc32 acc1)
v32acc32 | negmsc_4x8_8x8 (v64uint8 a, v64uint8 b, v32acc32 acc1)
v32acc32 | addmac_4x8_8x8 (v64uint8 a, v64uint8 b, v32acc32 acc1, v32acc32 acc2)
v32acc32 | addmsc_4x8_8x8 (v64uint8 a, v64uint8 b, v32acc32 acc1, v32acc32 acc2)
v32acc32 | submac_4x8_8x8 (v64uint8 a, v64uint8 b, v32acc32 acc1, v32acc32 acc2)
v32acc32 | submsc_4x8_8x8 (v64uint8 a, v64uint8 b, v32acc32 acc1, v32acc32 acc2)
v32acc32 | mul_4x8_8x8 (v64uint8 a, v64int8 b)
v32acc32 | negmul_4x8_8x8 (v64uint8 a, v64int8 b)
v32acc32 | mac_4x8_8x8 (v64uint8 a, v64int8 b, v32acc32 acc1)
v32acc32 | msc_4x8_8x8 (v64uint8 a, v64int8 b, v32acc32 acc1)
v32acc32 | negmac_4x8_8x8 (v64uint8 a, v64int8 b, v32acc32 acc1)
v32acc32 | negmsc_4x8_8x8 (v64uint8 a, v64int8 b, v32acc32 acc1)
v32acc32 | addmac_4x8_8x8 (v64uint8 a, v64int8 b, v32acc32 acc1, v32acc32 acc2)
v32acc32 | addmsc_4x8_8x8 (v64uint8 a, v64int8 b, v32acc32 acc1, v32acc32 acc2)
v32acc32 | submac_4x8_8x8 (v64uint8 a, v64int8 b, v32acc32 acc1, v32acc32 acc2)
v32acc32 | submsc_4x8_8x8 (v64uint8 a, v64int8 b, v32acc32 acc1, v32acc32 acc2)
v32acc32 | mul_4x8_8x8 (v64int8 a, v64uint8 b)
v32acc32 | negmul_4x8_8x8 (v64int8 a, v64uint8 b)
v32acc32 | mac_4x8_8x8 (v64int8 a, v64uint8 b, v32acc32 acc1)
v32acc32 | msc_4x8_8x8 (v64int8 a, v64uint8 b, v32acc32 acc1)
v32acc32 | negmac_4x8_8x8 (v64int8 a, v64uint8 b, v32acc32 acc1)
v32acc32 | negmsc_4x8_8x8 (v64int8 a, v64uint8 b, v32acc32 acc1)
v32acc32 | addmac_4x8_8x8 (v64int8 a, v64uint8 b, v32acc32 acc1, v32acc32 acc2)
v32acc32 | addmsc_4x8_8x8 (v64int8 a, v64uint8 b, v32acc32 acc1, v32acc32 acc2)
v32acc32 | submac_4x8_8x8 (v64int8 a, v64uint8 b, v32acc32 acc1, v32acc32 acc2)
v32acc32 | submsc_4x8_8x8 (v64int8 a, v64uint8 b, v32acc32 acc1, v32acc32 acc2)
v32acc32 | mul_4x8_8x8 (v64int8 a, v64int8 b)
v32acc32 | negmul_4x8_8x8 (v64int8 a, v64int8 b)
v32acc32 | mac_4x8_8x8 (v64int8 a, v64int8 b, v32acc32 acc1)
v32acc32 | msc_4x8_8x8 (v64int8 a, v64int8 b, v32acc32 acc1)
v32acc32 | negmac_4x8_8x8 (v64int8 a, v64int8 b, v32acc32 acc1)
v32acc32 | negmsc_4x8_8x8 (v64int8 a, v64int8 b, v32acc32 acc1)
v32acc32 | addmac_4x8_8x8 (v64int8 a, v64int8 b, v32acc32 acc1, v32acc32 acc2)
v32acc32 | addmsc_4x8_8x8 (v64int8 a, v64int8 b, v32acc32 acc1, v32acc32 acc2)
v32acc32 | submac_4x8_8x8 (v64int8 a, v64int8 b, v32acc32 acc1, v32acc32 acc2)
v32acc32 | submsc_4x8_8x8 (v64int8 a, v64int8 b, v32acc32 acc1, v32acc32 acc2)

## Multiplication of (4x8) with (8x8) with dynamic sign
v32acc32 | mul_4x8_8x8 (v64uint8 a, int sgn_x, v64uint8 b, int sgn_y)
v32acc32 | negmul_4x8_8x8 (v64uint8 a, int sgn_x, v64uint8 b, int sgn_y)
v32acc32 | mac_4x8_8x8 (v64uint8 a, int sgn_x, v64uint8 b, int sgn_y, v32acc32 acc1)
v32acc32 | msc_4x8_8x8 (v64uint8 a, int sgn_x, v64uint8 b, int sgn_y, v32acc32 acc1)
v32acc32 | negmac_4x8_8x8 (v64uint8 a, int sgn_x, v64uint8 b, int sgn_y, v32acc32 acc1)
v32acc32 | negmsc_4x8_8x8 (v64uint8 a, int sgn_x, v64uint8 b, int sgn_y, v32acc32 acc1)
v32acc32 | addmac_4x8_8x8 (v64uint8 a, int sgn_x, v64uint8 b, int sgn_y, v32acc32 acc1, v32acc32 acc2)
v32acc32 | addmsc_4x8_8x8 (v64uint8 a, int sgn_x, v64uint8 b, int sgn_y, v32acc32 acc1, v32acc32 acc2)
v32acc32 | submac_4x8_8x8 (v64uint8 a, int sgn_x, v64uint8 b, int sgn_y, v32acc32 acc1, v32acc32 acc2)
v32acc32 | submsc_4x8_8x8 (v64uint8 a, int sgn_x, v64uint8 b, int sgn_y, v32acc32 acc1, v32acc32 acc2)
v32acc32 | mul_4x8_8x8 (v64uint8 a, int sgn_x, v64int8 b, int sgn_y)
v32acc32 | negmul_4x8_8x8 (v64uint8 a, int sgn_x, v64int8 b, int sgn_y)
v32acc32 | mac_4x8_8x8 (v64uint8 a, int sgn_x, v64int8 b, int sgn_y, v32acc32 acc1)
v32acc32 | msc_4x8_8x8 (v64uint8 a, int sgn_x, v64int8 b, int sgn_y, v32acc32 acc1)
v32acc32 | negmac_4x8_8x8 (v64uint8 a, int sgn_x, v64int8 b, int sgn_y, v32acc32 acc1)
v32acc32 | negmsc_4x8_8x8 (v64uint8 a, int sgn_x, v64int8 b, int sgn_y, v32acc32 acc1)
v32acc32 | addmac_4x8_8x8 (v64uint8 a, int sgn_x, v64int8 b, int sgn_y, v32acc32 acc1, v32acc32 acc2)
v32acc32 | addmsc_4x8_8x8 (v64uint8 a, int sgn_x, v64int8 b, int sgn_y, v32acc32 acc1, v32acc32 acc2)
v32acc32 | submac_4x8_8x8 (v64uint8 a, int sgn_x, v64int8 b, int sgn_y, v32acc32 acc1, v32acc32 acc2)
v32acc32 | submsc_4x8_8x8 (v64uint8 a, int sgn_x, v64int8 b, int sgn_y, v32acc32 acc1, v32acc32 acc2)
v32acc32 | mul_4x8_8x8 (v64int8 a, int sgn_x, v64uint8 b, int sgn_y)
v32acc32 | negmul_4x8_8x8 (v64int8 a, int sgn_x, v64uint8 b, int sgn_y)
v32acc32 | mac_4x8_8x8 (v64int8 a, int sgn_x, v64uint8 b, int sgn_y, v32acc32 acc1)
v32acc32 | msc_4x8_8x8 (v64int8 a, int sgn_x, v64uint8 b, int sgn_y, v32acc32 acc1)
v32acc32 | negmac_4x8_8x8 (v64int8 a, int sgn_x, v64uint8 b, int sgn_y, v32acc32 acc1)
v32acc32 | negmsc_4x8_8x8 (v64int8 a, int sgn_x, v64uint8 b, int sgn_y, v32acc32 acc1)
v32acc32 | addmac_4x8_8x8 (v64int8 a, int sgn_x, v64uint8 b, int sgn_y, v32acc32 acc1, v32acc32 acc2)
v32acc32 | addmsc_4x8_8x8 (v64int8 a, int sgn_x, v64uint8 b, int sgn_y, v32acc32 acc1, v32acc32 acc2)
v32acc32 | submac_4x8_8x8 (v64int8 a, int sgn_x, v64uint8 b, int sgn_y, v32acc32 acc1, v32acc32 acc2)
v32acc32 | submsc_4x8_8x8 (v64int8 a, int sgn_x, v64uint8 b, int sgn_y, v32acc32 acc1, v32acc32 acc2)
v32acc32 | mul_4x8_8x8 (v64int8 a, int sgn_x, v64int8 b, int sgn_y)
v32acc32 | negmul_4x8_8x8 (v64int8 a, int sgn_x, v64int8 b, int sgn_y)
v32acc32 | mac_4x8_8x8 (v64int8 a, int sgn_x, v64int8 b, int sgn_y, v32acc32 acc1)
v32acc32 | msc_4x8_8x8 (v64int8 a, int sgn_x, v64int8 b, int sgn_y, v32acc32 acc1)
v32acc32 | negmac_4x8_8x8 (v64int8 a, int sgn_x, v64int8 b, int sgn_y, v32acc32 acc1)
v32acc32 | negmsc_4x8_8x8 (v64int8 a, int sgn_x, v64int8 b, int sgn_y, v32acc32 acc1)
v32acc32 | addmac_4x8_8x8 (v64int8 a, int sgn_x, v64int8 b, int sgn_y, v32acc32 acc1, v32acc32 acc2)
v32acc32 | addmsc_4x8_8x8 (v64int8 a, int sgn_x, v64int8 b, int sgn_y, v32acc32 acc1, v32acc32 acc2)
v32acc32 | submac_4x8_8x8 (v64int8 a, int sgn_x, v64int8 b, int sgn_y, v32acc32 acc1, v32acc32 acc2)
v32acc32 | submsc_4x8_8x8 (v64int8 a, int sgn_x, v64int8 b, int sgn_y, v32acc32 acc1, v32acc32 acc2)

## Multiplication of (4x8) with (8x8) with dynamic negation of multiplication result
v32acc32 | mul_4x8_8x8_conf (v64uint8 a, v64uint8 b, int sub_mul)
v32acc32 | negmul_4x8_8x8_conf (v64uint8 a, v64uint8 b, int sub_mul)
v32acc32 | mul_4x8_8x8_conf (v64uint8 a, v64int8 b, int sub_mul)
v32acc32 | negmul_4x8_8x8_conf (v64uint8 a, v64int8 b, int sub_mul)
v32acc32 | mul_4x8_8x8_conf (v64int8 a, v64uint8 b, int sub_mul)
v32acc32 | negmul_4x8_8x8_conf (v64int8 a, v64uint8 b, int sub_mul)
v32acc32 | mul_4x8_8x8_conf (v64int8 a, v64int8 b, int sub_mul)
v32acc32 | negmul_4x8_8x8_conf (v64int8 a, v64int8 b, int sub_mul)

## Multiplication of (4x8) with (8x8) with dynamic negation of multiplication result, zeroing of acc1, and negation of acc1
v32acc32 | mac_4x8_8x8_conf (v64uint8 a, v64uint8 b, v32acc32 acc1, int zero_acc1, int shift16, int sub_mul, int sub_acc1)
v32acc32 | msc_4x8_8x8_conf (v64uint8 a, v64uint8 b, v32acc32 acc1, int zero_acc1, int shift16, int sub_mul, int sub_acc1)
v32acc32 | negmsc_4x8_8x8_conf (v64uint8 a, v64uint8 b, v32acc32 acc1, int zero_acc1, int sub_mul, int sub_acc1)
v32acc32 | negmac_4x8_8x8_conf (v64uint8 a, v64uint8 b, v32acc32 acc1, int zero_acc1, int sub_mul, int sub_acc1)
v32acc32 | addmac_4x8_8x8_conf (v64uint8 a, v64uint8 b, v32acc32 acc1, v32acc32 acc2, int zero_acc1, int shift16, int sub_mul, int sub_acc1, int sub_acc2)
v32acc32 | addmsc_4x8_8x8_conf (v64uint8 a, v64uint8 b, v32acc32 acc1, v32acc32 acc2, int zero_acc1, int shift16, int sub_mul, int sub_acc1, int sub_acc2)
v32acc32 | submac_4x8_8x8_conf (v64uint8 a, v64uint8 b, v32acc32 acc1, v32acc32 acc2, int zero_acc1, int sub_mul, int sub_acc1, int sub_acc2)
v32acc32 | submsc_4x8_8x8_conf (v64uint8 a, v64uint8 b, v32acc32 acc1, v32acc32 acc2, int zero_acc1, int sub_mul, int sub_acc1, int sub_acc2)
v32acc32 | mac_4x8_8x8_conf (v64uint8 a, v64int8 b, v32acc32 acc1, int zero_acc1, int shift16, int sub_mul, int sub_acc1)
v32acc32 | msc_4x8_8x8_conf (v64uint8 a, v64int8 b, v32acc32 acc1, int zero_acc1, int shift16, int sub_mul, int sub_acc1)
v32acc32 | negmsc_4x8_8x8_conf (v64uint8 a, v64int8 b, v32acc32 acc1, int zero_acc1, int sub_mul, int sub_acc1)
v32acc32 | negmac_4x8_8x8_conf (v64uint8 a, v64int8 b, v32acc32 acc1, int zero_acc1, int sub_mul, int sub_acc1)
v32acc32 | addmac_4x8_8x8_conf (v64uint8 a, v64int8 b, v32acc32 acc1, v32acc32 acc2, int zero_acc1, int shift16, int sub_mul, int sub_acc1, int sub_acc2)
v32acc32 | addmsc_4x8_8x8_conf (v64uint8 a, v64int8 b, v32acc32 acc1, v32acc32 acc2, int zero_acc1, int shift16, int sub_mul, int sub_acc1, int sub_acc2)
v32acc32 | submac_4x8_8x8_conf (v64uint8 a, v64int8 b, v32acc32 acc1, v32acc32 acc2, int zero_acc1, int sub_mul, int sub_acc1, int sub_acc2)
v32acc32 | submsc_4x8_8x8_conf (v64uint8 a, v64int8 b, v32acc32 acc1, v32acc32 acc2, int zero_acc1, int sub_mul, int sub_acc1, int sub_acc2)
v32acc32 | mac_4x8_8x8_conf (v64int8 a, v64uint8 b, v32acc32 acc1, int zero_acc1, int shift16, int sub_mul, int sub_acc1)
v32acc32 | msc_4x8_8x8_conf (v64int8 a, v64uint8 b, v32acc32 acc1, int zero_acc1, int shift16, int sub_mul, int sub_acc1)
v32acc32 | negmsc_4x8_8x8_conf (v64int8 a, v64uint8 b, v32acc32 acc1, int zero_acc1, int sub_mul, int sub_acc1)
v32acc32 | negmac_4x8_8x8_conf (v64int8 a, v64uint8 b, v32acc32 acc1, int zero_acc1, int sub_mul, int sub_acc1)
v32acc32 | addmac_4x8_8x8_conf (v64int8 a, v64uint8 b, v32acc32 acc1, v32acc32 acc2, int zero_acc1, int shift16, int sub_mul, int sub_acc1, int sub_acc2)
v32acc32 | addmsc_4x8_8x8_conf (v64int8 a, v64uint8 b, v32acc32 acc1, v32acc32 acc2, int zero_acc1, int shift16, int sub_mul, int sub_acc1, int sub_acc2)
v32acc32 | submac_4x8_8x8_conf (v64int8 a, v64uint8 b, v32acc32 acc1, v32acc32 acc2, int zero_acc1, int sub_mul, int sub_acc1, int sub_acc2)
v32acc32 | submsc_4x8_8x8_conf (v64int8 a, v64uint8 b, v32acc32 acc1, v32acc32 acc2, int zero_acc1, int sub_mul, int sub_acc1, int sub_acc2)
v32acc32 | mac_4x8_8x8_conf (v64int8 a, v64int8 b, v32acc32 acc1, int zero_acc1, int shift16, int sub_mul, int sub_acc1)
v32acc32 | msc_4x8_8x8_conf (v64int8 a, v64int8 b, v32acc32 acc1, int zero_acc1, int shift16, int sub_mul, int sub_acc1)
v32acc32 | negmsc_4x8_8x8_conf (v64int8 a, v64int8 b, v32acc32 acc1, int zero_acc1, int sub_mul, int sub_acc1)
v32acc32 | negmac_4x8_8x8_conf (v64int8 a, v64int8 b, v32acc32 acc1, int zero_acc1, int sub_mul, int sub_acc1)
v32acc32 | addmac_4x8_8x8_conf (v64int8 a, v64int8 b, v32acc32 acc1, v32acc32 acc2, int zero_acc1, int shift16, int sub_mul, int sub_acc1, int sub_acc2)
v32acc32 | addmsc_4x8_8x8_conf (v64int8 a, v64int8 b, v32acc32 acc1, v32acc32 acc2, int zero_acc1, int shift16, int sub_mul, int sub_acc1, int sub_acc2)
v32acc32 | submac_4x8_8x8_conf (v64int8 a, v64int8 b, v32acc32 acc1, v32acc32 acc2, int zero_acc1, int sub_mul, int sub_acc1, int sub_acc2)
v32acc32 | submsc_4x8_8x8_conf (v64int8 a, v64int8 b, v32acc32 acc1, v32acc32 acc2, int zero_acc1, int sub_mul, int sub_acc1, int sub_acc2)

## Multiplication of (4x8) with (8x8) with dynamic sign and dynamic negation of multiplication result
v32acc32 | mul_4x8_8x8_conf (v64uint8 a, int sgn_x, v64uint8 b, int sgn_y, int sub_mul)
v32acc32 | negmul_4x8_8x8_conf (v64uint8 a, int sgn_x, v64uint8 b, int sgn_y, int sub_mul)
v32acc32 | mac_4x8_8x8_conf (v64uint8 a, int sgn_x, v64uint8 b, int sgn_y, v32acc32 acc1, int zero_acc1, int shift16, int sub_mul, int sub_acc1)
v32acc32 | msc_4x8_8x8_conf (v64uint8 a, int sgn_x, v64uint8 b, int sgn_y, v32acc32 acc1, int zero_acc1, int shift16, int sub_mul, int sub_acc1)
v32acc32 | negmsc_4x8_8x8_conf (v64uint8 a, int sgn_x, v64uint8 b, int sgn_y, v32acc32 acc1, int zero_acc1, int sub_mul, int sub_acc1)
v32acc32 | negmac_4x8_8x8_conf (v64uint8 a, int sgn_x, v64uint8 b, int sgn_y, v32acc32 acc1, int zero_acc1, int sub_mul, int sub_acc1)
v32acc32 | addmac_4x8_8x8_conf (v64uint8 a, int sgn_x, v64uint8 b, int sgn_y, v32acc32 acc1, v32acc32 acc2, int zero_acc1, int shift16, int sub_mul, int sub_acc1, int sub_acc2)
v32acc32 | addmsc_4x8_8x8_conf (v64uint8 a, int sgn_x, v64uint8 b, int sgn_y, v32acc32 acc1, v32acc32 acc2, int zero_acc1, int shift16, int sub_mul, int sub_acc1, int sub_acc2)
v32acc32 | submac_4x8_8x8_conf (v64uint8 a, int sgn_x, v64uint8 b, int sgn_y, v32acc32 acc1, v32acc32 acc2, int zero_acc1, int sub_mul, int sub_acc1, int sub_acc2)
v32acc32 | submsc_4x8_8x8_conf (v64uint8 a, int sgn_x, v64uint8 b, int sgn_y, v32acc32 acc1, v32acc32 acc2, int zero_acc1, int sub_mul, int sub_acc1, int sub_acc2)
v32acc32 | mul_4x8_8x8_conf (v64uint8 a, int sgn_x, v64int8 b, int sgn_y, int sub_mul)
v32acc32 | negmul_4x8_8x8_conf (v64uint8 a, int sgn_x, v64int8 b, int sgn_y, int sub_mul)
v32acc32 | mac_4x8_8x8_conf (v64uint8 a, int sgn_x, v64int8 b, int sgn_y, v32acc32 acc1, int zero_acc1, int shift16, int sub_mul, int sub_acc1)
v32acc32 | msc_4x8_8x8_conf (v64uint8 a, int sgn_x, v64int8 b, int sgn_y, v32acc32 acc1, int zero_acc1, int shift16, int sub_mul, int sub_acc1)
v32acc32 | negmsc_4x8_8x8_conf (v64uint8 a, int sgn_x, v64int8 b, int sgn_y, v32acc32 acc1, int zero_acc1, int sub_mul, int sub_acc1)
v32acc32 | negmac_4x8_8x8_conf (v64uint8 a, int sgn_x, v64int8 b, int sgn_y, v32acc32 acc1, int zero_acc1, int sub_mul, int sub_acc1)
v32acc32 | addmac_4x8_8x8_conf (v64uint8 a, int sgn_x, v64int8 b, int sgn_y, v32acc32 acc1, v32acc32 acc2, int zero_acc1, int shift16, int sub_mul, int sub_acc1, int sub_acc2)
v32acc32 | addmsc_4x8_8x8_conf (v64uint8 a, int sgn_x, v64int8 b, int sgn_y, v32acc32 acc1, v32acc32 acc2, int zero_acc1, int shift16, int sub_mul, int sub_acc1, int sub_acc2)
v32acc32 | submac_4x8_8x8_conf (v64uint8 a, int sgn_x, v64int8 b, int sgn_y, v32acc32 acc1, v32acc32 acc2, int zero_acc1, int sub_mul, int sub_acc1, int sub_acc2)
v32acc32 | submsc_4x8_8x8_conf (v64uint8 a, int sgn_x, v64int8 b, int sgn_y, v32acc32 acc1, v32acc32 acc2, int zero_acc1, int sub_mul, int sub_acc1, int sub_acc2)
v32acc32 | mul_4x8_8x8_conf (v64int8 a, int sgn_x, v64uint8 b, int sgn_y, int sub_mul)
v32acc32 | negmul_4x8_8x8_conf (v64int8 a, int sgn_x, v64uint8 b, int sgn_y, int sub_mul)
v32acc32 | mac_4x8_8x8_conf (v64int8 a, int sgn_x, v64uint8 b, int sgn_y, v32acc32 acc1, int zero_acc1, int shift16, int sub_mul, int sub_acc1)
v32acc32 | msc_4x8_8x8_conf (v64int8 a, int sgn_x, v64uint8 b, int sgn_y, v32acc32 acc1, int zero_acc1, int shift16, int sub_mul, int sub_acc1)
v32acc32 | negmsc_4x8_8x8_conf (v64int8 a, int sgn_x, v64uint8 b, int sgn_y, v32acc32 acc1, int zero_acc1, int sub_mul, int sub_acc1)
v32acc32 | negmac_4x8_8x8_conf (v64int8 a, int sgn_x, v64uint8 b, int sgn_y, v32acc32 acc1, int zero_acc1, int sub_mul, int sub_acc1)
v32acc32 | addmac_4x8_8x8_conf (v64int8 a, int sgn_x, v64uint8 b, int sgn_y, v32acc32 acc1, v32acc32 acc2, int zero_acc1, int shift16, int sub_mul, int sub_acc1, int sub_acc2)
v32acc32 | addmsc_4x8_8x8_conf (v64int8 a, int sgn_x, v64uint8 b, int sgn_y, v32acc32 acc1, v32acc32 acc2, int zero_acc1, int shift16, int sub_mul, int sub_acc1, int sub_acc2)
v32acc32 | submac_4x8_8x8_conf (v64int8 a, int sgn_x, v64uint8 b, int sgn_y, v32acc32 acc1, v32acc32 acc2, int zero_acc1, int sub_mul, int sub_acc1, int sub_acc2)
v32acc32 | submsc_4x8_8x8_conf (v64int8 a, int sgn_x, v64uint8 b, int sgn_y, v32acc32 acc1, v32acc32 acc2, int zero_acc1, int sub_mul, int sub_acc1, int sub_acc2)
v32acc32 | mul_4x8_8x8_conf (v64int8 a, int sgn_x, v64int8 b, int sgn_y, int sub_mul)
v32acc32 | negmul_4x8_8x8_conf (v64int8 a, int sgn_x, v64int8 b, int sgn_y, int sub_mul)
v32acc32 | mac_4x8_8x8_conf (v64int8 a, int sgn_x, v64int8 b, int sgn_y, v32acc32 acc1, int zero_acc1, int shift16, int sub_mul, int sub_acc1)
v32acc32 | msc_4x8_8x8_conf (v64int8 a, int sgn_x, v64int8 b, int sgn_y, v32acc32 acc1, int zero_acc1, int shift16, int sub_mul, int sub_acc1)
v32acc32 | negmsc_4x8_8x8_conf (v64int8 a, int sgn_x, v64int8 b, int sgn_y, v32acc32 acc1, int zero_acc1, int sub_mul, int sub_acc1)
v32acc32 | negmac_4x8_8x8_conf (v64int8 a, int sgn_x, v64int8 b, int sgn_y, v32acc32 acc1, int zero_acc1, int sub_mul, int sub_acc1)
v32acc32 | addmac_4x8_8x8_conf (v64int8 a, int sgn_x, v64int8 b, int sgn_y, v32acc32 acc1, v32acc32 acc2, int zero_acc1, int shift16, int sub_mul, int sub_acc1, int sub_acc2)
v32acc32 | addmsc_4x8_8x8_conf (v64int8 a, int sgn_x, v64int8 b, int sgn_y, v32acc32 acc1, v32acc32 acc2, int zero_acc1, int shift16, int sub_mul, int sub_acc1, int sub_acc2)
v32acc32 | submac_4x8_8x8_conf (v64int8 a, int sgn_x, v64int8 b, int sgn_y, v32acc32 acc1, v32acc32 acc2, int zero_acc1, int sub_mul, int sub_acc1, int sub_acc2)
v32acc32 | submsc_4x8_8x8_conf (v64int8 a, int sgn_x, v64int8 b, int sgn_y, v32acc32 acc1, v32acc32 acc2, int zero_acc1, int sub_mul, int sub_acc1, int sub_acc2)

## Channel by channel mutliplication of (1x2) with (2x1)
v32acc32 | mul_elem_32_2 (v64uint8 a, v64uint8 b)
v32acc32 | negmul_elem_32_2 (v64uint8 a, v64uint8 b)
v32acc32 | mac_elem_32_2 (v64uint8 a, v64uint8 b, v32acc32 acc1)
v32acc32 | msc_elem_32_2 (v64uint8 a, v64uint8 b, v32acc32 acc1)
v32acc32 | negmac_elem_32_2 (v64uint8 a, v64uint8 b, v32acc32 acc1)
v32acc32 | negmsc_elem_32_2 (v64uint8 a, v64uint8 b, v32acc32 acc1)
v32acc32 | addmac_elem_32_2 (v64uint8 a, v64uint8 b, v32acc32 acc1, v32acc32 acc2)
v32acc32 | addmsc_elem_32_2 (v64uint8 a, v64uint8 b, v32acc32 acc1, v32acc32 acc2)
v32acc32 | submac_elem_32_2 (v64uint8 a, v64uint8 b, v32acc32 acc1, v32acc32 acc2)
v32acc32 | submsc_elem_32_2 (v64uint8 a, v64uint8 b, v32acc32 acc1, v32acc32 acc2)
v32acc32 | mul_elem_32_2 (v64uint8 a, v64int8 b)
v32acc32 | negmul_elem_32_2 (v64uint8 a, v64int8 b)
v32acc32 | mac_elem_32_2 (v64uint8 a, v64int8 b, v32acc32 acc1)
v32acc32 | msc_elem_32_2 (v64uint8 a, v64int8 b, v32acc32 acc1)
v32acc32 | negmac_elem_32_2 (v64uint8 a, v64int8 b, v32acc32 acc1)
v32acc32 | negmsc_elem_32_2 (v64uint8 a, v64int8 b, v32acc32 acc1)
v32acc32 | addmac_elem_32_2 (v64uint8 a, v64int8 b, v32acc32 acc1, v32acc32 acc2)
v32acc32 | addmsc_elem_32_2 (v64uint8 a, v64int8 b, v32acc32 acc1, v32acc32 acc2)
v32acc32 | submac_elem_32_2 (v64uint8 a, v64int8 b, v32acc32 acc1, v32acc32 acc2)
v32acc32 | submsc_elem_32_2 (v64uint8 a, v64int8 b, v32acc32 acc1, v32acc32 acc2)
v32acc32 | mul_elem_32_2 (v64int8 a, v64uint8 b)
v32acc32 | negmul_elem_32_2 (v64int8 a, v64uint8 b)
v32acc32 | mac_elem_32_2 (v64int8 a, v64uint8 b, v32acc32 acc1)
v32acc32 | msc_elem_32_2 (v64int8 a, v64uint8 b, v32acc32 acc1)
v32acc32 | negmac_elem_32_2 (v64int8 a, v64uint8 b, v32acc32 acc1)
v32acc32 | negmsc_elem_32_2 (v64int8 a, v64uint8 b, v32acc32 acc1)
v32acc32 | addmac_elem_32_2 (v64int8 a, v64uint8 b, v32acc32 acc1, v32acc32 acc2)
v32acc32 | addmsc_elem_32_2 (v64int8 a, v64uint8 b, v32acc32 acc1, v32acc32 acc2)
v32acc32 | submac_elem_32_2 (v64int8 a, v64uint8 b, v32acc32 acc1, v32acc32 acc2)
v32acc32 | submsc_elem_32_2 (v64int8 a, v64uint8 b, v32acc32 acc1, v32acc32 acc2)
v32acc32 | mul_elem_32_2 (v64int8 a, v64int8 b)
v32acc32 | negmul_elem_32_2 (v64int8 a, v64int8 b)
v32acc32 | mac_elem_32_2 (v64int8 a, v64int8 b, v32acc32 acc1)
v32acc32 | msc_elem_32_2 (v64int8 a, v64int8 b, v32acc32 acc1)
v32acc32 | negmac_elem_32_2 (v64int8 a, v64int8 b, v32acc32 acc1)
v32acc32 | negmsc_elem_32_2 (v64int8 a, v64int8 b, v32acc32 acc1)
v32acc32 | addmac_elem_32_2 (v64int8 a, v64int8 b, v32acc32 acc1, v32acc32 acc2)
v32acc32 | addmsc_elem_32_2 (v64int8 a, v64int8 b, v32acc32 acc1, v32acc32 acc2)
v32acc32 | submac_elem_32_2 (v64int8 a, v64int8 b, v32acc32 acc1, v32acc32 acc2)
v32acc32 | submsc_elem_32_2 (v64int8 a, v64int8 b, v32acc32 acc1, v32acc32 acc2)

## Channel by channel mutliplication of (1x2) with (2x1) with dynamic sign
v32acc32 | mul_elem_32_2 (v64uint8 a, int sgn_x, v64uint8 b, int sgn_y)
v32acc32 | negmul_elem_32_2 (v64uint8 a, int sgn_x, v64uint8 b, int sgn_y)
v32acc32 | mac_elem_32_2 (v64uint8 a, int sgn_x, v64uint8 b, int sgn_y, v32acc32 acc1)
v32acc32 | msc_elem_32_2 (v64uint8 a, int sgn_x, v64uint8 b, int sgn_y, v32acc32 acc1)
v32acc32 | negmac_elem_32_2 (v64uint8 a, int sgn_x, v64uint8 b, int sgn_y, v32acc32 acc1)
v32acc32 | negmsc_elem_32_2 (v64uint8 a, int sgn_x, v64uint8 b, int sgn_y, v32acc32 acc1)
v32acc32 | addmac_elem_32_2 (v64uint8 a, int sgn_x, v64uint8 b, int sgn_y, v32acc32 acc1, v32acc32 acc2)
v32acc32 | addmsc_elem_32_2 (v64uint8 a, int sgn_x, v64uint8 b, int sgn_y, v32acc32 acc1, v32acc32 acc2)
v32acc32 | submac_elem_32_2 (v64uint8 a, int sgn_x, v64uint8 b, int sgn_y, v32acc32 acc1, v32acc32 acc2)
v32acc32 | submsc_elem_32_2 (v64uint8 a, int sgn_x, v64uint8 b, int sgn_y, v32acc32 acc1, v32acc32 acc2)
v32acc32 | mul_elem_32_2 (v64uint8 a, int sgn_x, v64int8 b, int sgn_y)
v32acc32 | negmul_elem_32_2 (v64uint8 a, int sgn_x, v64int8 b, int sgn_y)
v32acc32 | mac_elem_32_2 (v64uint8 a, int sgn_x, v64int8 b, int sgn_y, v32acc32 acc1)
v32acc32 | msc_elem_32_2 (v64uint8 a, int sgn_x, v64int8 b, int sgn_y, v32acc32 acc1)
v32acc32 | negmac_elem_32_2 (v64uint8 a, int sgn_x, v64int8 b, int sgn_y, v32acc32 acc1)
v32acc32 | negmsc_elem_32_2 (v64uint8 a, int sgn_x, v64int8 b, int sgn_y, v32acc32 acc1)
v32acc32 | addmac_elem_32_2 (v64uint8 a, int sgn_x, v64int8 b, int sgn_y, v32acc32 acc1, v32acc32 acc2)
v32acc32 | addmsc_elem_32_2 (v64uint8 a, int sgn_x, v64int8 b, int sgn_y, v32acc32 acc1, v32acc32 acc2)
v32acc32 | submac_elem_32_2 (v64uint8 a, int sgn_x, v64int8 b, int sgn_y, v32acc32 acc1, v32acc32 acc2)
v32acc32 | submsc_elem_32_2 (v64uint8 a, int sgn_x, v64int8 b, int sgn_y, v32acc32 acc1, v32acc32 acc2)
v32acc32 | mul_elem_32_2 (v64int8 a, int sgn_x, v64uint8 b, int sgn_y)
v32acc32 | negmul_elem_32_2 (v64int8 a, int sgn_x, v64uint8 b, int sgn_y)
v32acc32 | mac_elem_32_2 (v64int8 a, int sgn_x, v64uint8 b, int sgn_y, v32acc32 acc1)
v32acc32 | msc_elem_32_2 (v64int8 a, int sgn_x, v64uint8 b, int sgn_y, v32acc32 acc1)
v32acc32 | negmac_elem_32_2 (v64int8 a, int sgn_x, v64uint8 b, int sgn_y, v32acc32 acc1)
v32acc32 | negmsc_elem_32_2 (v64int8 a, int sgn_x, v64uint8 b, int sgn_y, v32acc32 acc1)
v32acc32 | addmac_elem_32_2 (v64int8 a, int sgn_x, v64uint8 b, int sgn_y, v32acc32 acc1, v32acc32 acc2)
v32acc32 | addmsc_elem_32_2 (v64int8 a, int sgn_x, v64uint8 b, int sgn_y, v32acc32 acc1, v32acc32 acc2)
v32acc32 | submac_elem_32_2 (v64int8 a, int sgn_x, v64uint8 b, int sgn_y, v32acc32 acc1, v32acc32 acc2)
v32acc32 | submsc_elem_32_2 (v64int8 a, int sgn_x, v64uint8 b, int sgn_y, v32acc32 acc1, v32acc32 acc2)
v32acc32 | mul_elem_32_2 (v64int8 a, int sgn_x, v64int8 b, int sgn_y)
v32acc32 | negmul_elem_32_2 (v64int8 a, int sgn_x, v64int8 b, int sgn_y)
v32acc32 | mac_elem_32_2 (v64int8 a, int sgn_x, v64int8 b, int sgn_y, v32acc32 acc1)
v32acc32 | msc_elem_32_2 (v64int8 a, int sgn_x, v64int8 b, int sgn_y, v32acc32 acc1)
v32acc32 | negmac_elem_32_2 (v64int8 a, int sgn_x, v64int8 b, int sgn_y, v32acc32 acc1)
v32acc32 | negmsc_elem_32_2 (v64int8 a, int sgn_x, v64int8 b, int sgn_y, v32acc32 acc1)
v32acc32 | addmac_elem_32_2 (v64int8 a, int sgn_x, v64int8 b, int sgn_y, v32acc32 acc1, v32acc32 acc2)
v32acc32 | addmsc_elem_32_2 (v64int8 a, int sgn_x, v64int8 b, int sgn_y, v32acc32 acc1, v32acc32 acc2)
v32acc32 | submac_elem_32_2 (v64int8 a, int sgn_x, v64int8 b, int sgn_y, v32acc32 acc1, v32acc32 acc2)
v32acc32 | submsc_elem_32_2 (v64int8 a, int sgn_x, v64int8 b, int sgn_y, v32acc32 acc1, v32acc32 acc2)

## Channel by channel mutliplication of (1x2) with (2x1) with dynamic negation of multiplication result
v32acc32 | mul_elem_32_2_conf (v64uint8 a, v64uint8 b, int sub_mul)
v32acc32 | negmul_elem_32_2_conf (v64uint8 a, v64uint8 b, int sub_mul)
v32acc32 | mul_elem_32_2_conf (v64uint8 a, v64int8 b, int sub_mul)
v32acc32 | negmul_elem_32_2_conf (v64uint8 a, v64int8 b, int sub_mul)
v32acc32 | mul_elem_32_2_conf (v64int8 a, v64uint8 b, int sub_mul)
v32acc32 | negmul_elem_32_2_conf (v64int8 a, v64uint8 b, int sub_mul)
v32acc32 | mul_elem_32_2_conf (v64int8 a, v64int8 b, int sub_mul)
v32acc32 | negmul_elem_32_2_conf (v64int8 a, v64int8 b, int sub_mul)

## Channel by channel mutliplication of (1x2) with (2x1) with dynamic negation of multiplication result, zeroing of acc1, and negation of acc1
v32acc32 | mac_elem_32_2_conf (v64uint8 a, v64uint8 b, v32acc32 acc1, int zero_acc1, int shift16, int sub_mul, int sub_acc1)
v32acc32 | msc_elem_32_2_conf (v64uint8 a, v64uint8 b, v32acc32 acc1, int zero_acc1, int shift16, int sub_mul, int sub_acc1)
v32acc32 | negmsc_elem_32_2_conf (v64uint8 a, v64uint8 b, v32acc32 acc1, int zero_acc1, int sub_mul, int sub_acc1)
v32acc32 | negmac_elem_32_2_conf (v64uint8 a, v64uint8 b, v32acc32 acc1, int zero_acc1, int sub_mul, int sub_acc1)
v32acc32 | addmac_elem_32_2_conf (v64uint8 a, v64uint8 b, v32acc32 acc1, v32acc32 acc2, int zero_acc1, int shift16, int sub_mul, int sub_acc1, int sub_acc2)
v32acc32 | addmsc_elem_32_2_conf (v64uint8 a, v64uint8 b, v32acc32 acc1, v32acc32 acc2, int zero_acc1, int shift16, int sub_mul, int sub_acc1, int sub_acc2)
v32acc32 | submac_elem_32_2_conf (v64uint8 a, v64uint8 b, v32acc32 acc1, v32acc32 acc2, int zero_acc1, int sub_mul, int sub_acc1, int sub_acc2)
v32acc32 | submsc_elem_32_2_conf (v64uint8 a, v64uint8 b, v32acc32 acc1, v32acc32 acc2, int zero_acc1, int sub_mul, int sub_acc1, int sub_acc2)
v32acc32 | mac_elem_32_2_conf (v64uint8 a, v64int8 b, v32acc32 acc1, int zero_acc1, int shift16, int sub_mul, int sub_acc1)
v32acc32 | msc_elem_32_2_conf (v64uint8 a, v64int8 b, v32acc32 acc1, int zero_acc1, int shift16, int sub_mul, int sub_acc1)
v32acc32 | negmsc_elem_32_2_conf (v64uint8 a, v64int8 b, v32acc32 acc1, int zero_acc1, int sub_mul, int sub_acc1)
v32acc32 | negmac_elem_32_2_conf (v64uint8 a, v64int8 b, v32acc32 acc1, int zero_acc1, int sub_mul, int sub_acc1)
v32acc32 | addmac_elem_32_2_conf (v64uint8 a, v64int8 b, v32acc32 acc1, v32acc32 acc2, int zero_acc1, int shift16, int sub_mul, int sub_acc1, int sub_acc2)
v32acc32 | addmsc_elem_32_2_conf (v64uint8 a, v64int8 b, v32acc32 acc1, v32acc32 acc2, int zero_acc1, int shift16, int sub_mul, int sub_acc1, int sub_acc2)
v32acc32 | submac_elem_32_2_conf (v64uint8 a, v64int8 b, v32acc32 acc1, v32acc32 acc2, int zero_acc1, int sub_mul, int sub_acc1, int sub_acc2)
v32acc32 | submsc_elem_32_2_conf (v64uint8 a, v64int8 b, v32acc32 acc1, v32acc32 acc2, int zero_acc1, int sub_mul, int sub_acc1, int sub_acc2)
v32acc32 | mac_elem_32_2_conf (v64int8 a, v64uint8 b, v32acc32 acc1, int zero_acc1, int shift16, int sub_mul, int sub_acc1)
v32acc32 | msc_elem_32_2_conf (v64int8 a, v64uint8 b, v32acc32 acc1, int zero_acc1, int shift16, int sub_mul, int sub_acc1)
v32acc32 | negmsc_elem_32_2_conf (v64int8 a, v64uint8 b, v32acc32 acc1, int zero_acc1, int sub_mul, int sub_acc1)
v32acc32 | negmac_elem_32_2_conf (v64int8 a, v64uint8 b, v32acc32 acc1, int zero_acc1, int sub_mul, int sub_acc1)
v32acc32 | addmac_elem_32_2_conf (v64int8 a, v64uint8 b, v32acc32 acc1, v32acc32 acc2, int zero_acc1, int shift16, int sub_mul, int sub_acc1, int sub_acc2)
v32acc32 | addmsc_elem_32_2_conf (v64int8 a, v64uint8 b, v32acc32 acc1, v32acc32 acc2, int zero_acc1, int shift16, int sub_mul, int sub_acc1, int sub_acc2)
v32acc32 | submac_elem_32_2_conf (v64int8 a, v64uint8 b, v32acc32 acc1, v32acc32 acc2, int zero_acc1, int sub_mul, int sub_acc1, int sub_acc2)
v32acc32 | submsc_elem_32_2_conf (v64int8 a, v64uint8 b, v32acc32 acc1, v32acc32 acc2, int zero_acc1, int sub_mul, int sub_acc1, int sub_acc2)
v32acc32 | mac_elem_32_2_conf (v64int8 a, v64int8 b, v32acc32 acc1, int zero_acc1, int shift16, int sub_mul, int sub_acc1)
v32acc32 | msc_elem_32_2_conf (v64int8 a, v64int8 b, v32acc32 acc1, int zero_acc1, int shift16, int sub_mul, int sub_acc1)
v32acc32 | negmsc_elem_32_2_conf (v64int8 a, v64int8 b, v32acc32 acc1, int zero_acc1, int sub_mul, int sub_acc1)
v32acc32 | negmac_elem_32_2_conf (v64int8 a, v64int8 b, v32acc32 acc1, int zero_acc1, int sub_mul, int sub_acc1)
v32acc32 | addmac_elem_32_2_conf (v64int8 a, v64int8 b, v32acc32 acc1, v32acc32 acc2, int zero_acc1, int shift16, int sub_mul, int sub_acc1, int sub_acc2)
v32acc32 | addmsc_elem_32_2_conf (v64int8 a, v64int8 b, v32acc32 acc1, v32acc32 acc2, int zero_acc1, int shift16, int sub_mul, int sub_acc1, int sub_acc2)
v32acc32 | submac_elem_32_2_conf (v64int8 a, v64int8 b, v32acc32 acc1, v32acc32 acc2, int zero_acc1, int sub_mul, int sub_acc1, int sub_acc2)
v32acc32 | submsc_elem_32_2_conf (v64int8 a, v64int8 b, v32acc32 acc1, v32acc32 acc2, int zero_acc1, int sub_mul, int sub_acc1, int sub_acc2)

## Channel by channel mutliplication of (1x2) with (2x1) with dynamic sign and dynamic negation of multiplication result
v32acc32 | mul_elem_32_2_conf (v64uint8 a, int sgn_x, v64uint8 b, int sgn_y, int sub_mul)
v32acc32 | negmul_elem_32_2_conf (v64uint8 a, int sgn_x, v64uint8 b, int sgn_y, int sub_mul)
v32acc32 | mac_elem_32_2_conf (v64uint8 a, int sgn_x, v64uint8 b, int sgn_y, v32acc32 acc1, int zero_acc1, int shift16, int sub_mul, int sub_acc1)
v32acc32 | msc_elem_32_2_conf (v64uint8 a, int sgn_x, v64uint8 b, int sgn_y, v32acc32 acc1, int zero_acc1, int shift16, int sub_mul, int sub_acc1)
v32acc32 | negmsc_elem_32_2_conf (v64uint8 a, int sgn_x, v64uint8 b, int sgn_y, v32acc32 acc1, int zero_acc1, int sub_mul, int sub_acc1)
v32acc32 | negmac_elem_32_2_conf (v64uint8 a, int sgn_x, v64uint8 b, int sgn_y, v32acc32 acc1, int zero_acc1, int sub_mul, int sub_acc1)
v32acc32 | addmac_elem_32_2_conf (v64uint8 a, int sgn_x, v64uint8 b, int sgn_y, v32acc32 acc1, v32acc32 acc2, int zero_acc1, int shift16, int sub_mul, int sub_acc1, int sub_acc2)
v32acc32 | addmsc_elem_32_2_conf (v64uint8 a, int sgn_x, v64uint8 b, int sgn_y, v32acc32 acc1, v32acc32 acc2, int zero_acc1, int shift16, int sub_mul, int sub_acc1, int sub_acc2)
v32acc32 | submac_elem_32_2_conf (v64uint8 a, int sgn_x, v64uint8 b, int sgn_y, v32acc32 acc1, v32acc32 acc2, int zero_acc1, int sub_mul, int sub_acc1, int sub_acc2)
v32acc32 | submsc_elem_32_2_conf (v64uint8 a, int sgn_x, v64uint8 b, int sgn_y, v32acc32 acc1, v32acc32 acc2, int zero_acc1, int sub_mul, int sub_acc1, int sub_acc2)
v32acc32 | mul_elem_32_2_conf (v64uint8 a, int sgn_x, v64int8 b, int sgn_y, int sub_mul)
v32acc32 | negmul_elem_32_2_conf (v64uint8 a, int sgn_x, v64int8 b, int sgn_y, int sub_mul)
v32acc32 | mac_elem_32_2_conf (v64uint8 a, int sgn_x, v64int8 b, int sgn_y, v32acc32 acc1, int zero_acc1, int shift16, int sub_mul, int sub_acc1)
v32acc32 | msc_elem_32_2_conf (v64uint8 a, int sgn_x, v64int8 b, int sgn_y, v32acc32 acc1, int zero_acc1, int shift16, int sub_mul, int sub_acc1)
v32acc32 | negmsc_elem_32_2_conf (v64uint8 a, int sgn_x, v64int8 b, int sgn_y, v32acc32 acc1, int zero_acc1, int sub_mul, int sub_acc1)
v32acc32 | negmac_elem_32_2_conf (v64uint8 a, int sgn_x, v64int8 b, int sgn_y, v32acc32 acc1, int zero_acc1, int sub_mul, int sub_acc1)
v32acc32 | addmac_elem_32_2_conf (v64uint8 a, int sgn_x, v64int8 b, int sgn_y, v32acc32 acc1, v32acc32 acc2, int zero_acc1, int shift16, int sub_mul, int sub_acc1, int sub_acc2)
v32acc32 | addmsc_elem_32_2_conf (v64uint8 a, int sgn_x, v64int8 b, int sgn_y, v32acc32 acc1, v32acc32 acc2, int zero_acc1, int shift16, int sub_mul, int sub_acc1, int sub_acc2)
v32acc32 | submac_elem_32_2_conf (v64uint8 a, int sgn_x, v64int8 b, int sgn_y, v32acc32 acc1, v32acc32 acc2, int zero_acc1, int sub_mul, int sub_acc1, int sub_acc2)
v32acc32 | submsc_elem_32_2_conf (v64uint8 a, int sgn_x, v64int8 b, int sgn_y, v32acc32 acc1, v32acc32 acc2, int zero_acc1, int sub_mul, int sub_acc1, int sub_acc2)
v32acc32 | mul_elem_32_2_conf (v64int8 a, int sgn_x, v64uint8 b, int sgn_y, int sub_mul)
v32acc32 | negmul_elem_32_2_conf (v64int8 a, int sgn_x, v64uint8 b, int sgn_y, int sub_mul)
v32acc32 | mac_elem_32_2_conf (v64int8 a, int sgn_x, v64uint8 b, int sgn_y, v32acc32 acc1, int zero_acc1, int shift16, int sub_mul, int sub_acc1)
v32acc32 | msc_elem_32_2_conf (v64int8 a, int sgn_x, v64uint8 b, int sgn_y, v32acc32 acc1, int zero_acc1, int shift16, int sub_mul, int sub_acc1)
v32acc32 | negmsc_elem_32_2_conf (v64int8 a, int sgn_x, v64uint8 b, int sgn_y, v32acc32 acc1, int zero_acc1, int sub_mul, int sub_acc1)
v32acc32 | negmac_elem_32_2_conf (v64int8 a, int sgn_x, v64uint8 b, int sgn_y, v32acc32 acc1, int zero_acc1, int sub_mul, int sub_acc1)
v32acc32 | addmac_elem_32_2_conf (v64int8 a, int sgn_x, v64uint8 b, int sgn_y, v32acc32 acc1, v32acc32 acc2, int zero_acc1, int shift16, int sub_mul, int sub_acc1, int sub_acc2)
v32acc32 | addmsc_elem_32_2_conf (v64int8 a, int sgn_x, v64uint8 b, int sgn_y, v32acc32 acc1, v32acc32 acc2, int zero_acc1, int shift16, int sub_mul, int sub_acc1, int sub_acc2)
v32acc32 | submac_elem_32_2_conf (v64int8 a, int sgn_x, v64uint8 b, int sgn_y, v32acc32 acc1, v32acc32 acc2, int zero_acc1, int sub_mul, int sub_acc1, int sub_acc2)
v32acc32 | submsc_elem_32_2_conf (v64int8 a, int sgn_x, v64uint8 b, int sgn_y, v32acc32 acc1, v32acc32 acc2, int zero_acc1, int sub_mul, int sub_acc1, int sub_acc2)
v32acc32 | mul_elem_32_2_conf (v64int8 a, int sgn_x, v64int8 b, int sgn_y, int sub_mul)
v32acc32 | negmul_elem_32_2_conf (v64int8 a, int sgn_x, v64int8 b, int sgn_y, int sub_mul)
v32acc32 | mac_elem_32_2_conf (v64int8 a, int sgn_x, v64int8 b, int sgn_y, v32acc32 acc1, int zero_acc1, int shift16, int sub_mul, int sub_acc1)
v32acc32 | msc_elem_32_2_conf (v64int8 a, int sgn_x, v64int8 b, int sgn_y, v32acc32 acc1, int zero_acc1, int shift16, int sub_mul, int sub_acc1)
v32acc32 | negmsc_elem_32_2_conf (v64int8 a, int sgn_x, v64int8 b, int sgn_y, v32acc32 acc1, int zero_acc1, int sub_mul, int sub_acc1)
v32acc32 | negmac_elem_32_2_conf (v64int8 a, int sgn_x, v64int8 b, int sgn_y, v32acc32 acc1, int zero_acc1, int sub_mul, int sub_acc1)
v32acc32 | addmac_elem_32_2_conf (v64int8 a, int sgn_x, v64int8 b, int sgn_y, v32acc32 acc1, v32acc32 acc2, int zero_acc1, int shift16, int sub_mul, int sub_acc1, int sub_acc2)
v32acc32 | addmsc_elem_32_2_conf (v64int8 a, int sgn_x, v64int8 b, int sgn_y, v32acc32 acc1, v32acc32 acc2, int zero_acc1, int shift16, int sub_mul, int sub_acc1, int sub_acc2)
v32acc32 | submac_elem_32_2_conf (v64int8 a, int sgn_x, v64int8 b, int sgn_y, v32acc32 acc1, v32acc32 acc2, int zero_acc1, int sub_mul, int sub_acc1, int sub_acc2)
v32acc32 | submsc_elem_32_2_conf (v64int8 a, int sgn_x, v64int8 b, int sgn_y, v32acc32 acc1, v32acc32 acc2, int zero_acc1, int sub_mul, int sub_acc1, int sub_acc2)

## Convolution of (4x4) matrix with (4x1) kernel and 8 channels
v32acc32 | mul_conv_4x4_8ch (v64uint8 a, v64uint8 b)
v32acc32 | negmul_conv_4x4_8ch (v64uint8 a, v64uint8 b)
v32acc32 | mac_conv_4x4_8ch (v64uint8 a, v64uint8 b, v32acc32 acc1)
v32acc32 | msc_conv_4x4_8ch (v64uint8 a, v64uint8 b, v32acc32 acc1)
v32acc32 | negmac_conv_4x4_8ch (v64uint8 a, v64uint8 b, v32acc32 acc1)
v32acc32 | negmsc_conv_4x4_8ch (v64uint8 a, v64uint8 b, v32acc32 acc1)
v32acc32 | addmac_conv_4x4_8ch (v64uint8 a, v64uint8 b, v32acc32 acc1, v32acc32 acc2)
v32acc32 | addmsc_conv_4x4_8ch (v64uint8 a, v64uint8 b, v32acc32 acc1, v32acc32 acc2)
v32acc32 | submac_conv_4x4_8ch (v64uint8 a, v64uint8 b, v32acc32 acc1, v32acc32 acc2)
v32acc32 | submsc_conv_4x4_8ch (v64uint8 a, v64uint8 b, v32acc32 acc1, v32acc32 acc2)
v32acc32 | mul_conv_4x4_8ch (v64uint8 a, v64int8 b)
v32acc32 | negmul_conv_4x4_8ch (v64uint8 a, v64int8 b)
v32acc32 | mac_conv_4x4_8ch (v64uint8 a, v64int8 b, v32acc32 acc1)
v32acc32 | msc_conv_4x4_8ch (v64uint8 a, v64int8 b, v32acc32 acc1)
v32acc32 | negmac_conv_4x4_8ch (v64uint8 a, v64int8 b, v32acc32 acc1)
v32acc32 | negmsc_conv_4x4_8ch (v64uint8 a, v64int8 b, v32acc32 acc1)
v32acc32 | addmac_conv_4x4_8ch (v64uint8 a, v64int8 b, v32acc32 acc1, v32acc32 acc2)
v32acc32 | addmsc_conv_4x4_8ch (v64uint8 a, v64int8 b, v32acc32 acc1, v32acc32 acc2)
v32acc32 | submac_conv_4x4_8ch (v64uint8 a, v64int8 b, v32acc32 acc1, v32acc32 acc2)
v32acc32 | submsc_conv_4x4_8ch (v64uint8 a, v64int8 b, v32acc32 acc1, v32acc32 acc2)
v32acc32 | mul_conv_4x4_8ch (v64int8 a, v64uint8 b)
v32acc32 | negmul_conv_4x4_8ch (v64int8 a, v64uint8 b)
v32acc32 | mac_conv_4x4_8ch (v64int8 a, v64uint8 b, v32acc32 acc1)
v32acc32 | msc_conv_4x4_8ch (v64int8 a, v64uint8 b, v32acc32 acc1)
v32acc32 | negmac_conv_4x4_8ch (v64int8 a, v64uint8 b, v32acc32 acc1)
v32acc32 | negmsc_conv_4x4_8ch (v64int8 a, v64uint8 b, v32acc32 acc1)
v32acc32 | addmac_conv_4x4_8ch (v64int8 a, v64uint8 b, v32acc32 acc1, v32acc32 acc2)
v32acc32 | addmsc_conv_4x4_8ch (v64int8 a, v64uint8 b, v32acc32 acc1, v32acc32 acc2)
v32acc32 | submac_conv_4x4_8ch (v64int8 a, v64uint8 b, v32acc32 acc1, v32acc32 acc2)
v32acc32 | submsc_conv_4x4_8ch (v64int8 a, v64uint8 b, v32acc32 acc1, v32acc32 acc2)
v32acc32 | mul_conv_4x4_8ch (v64int8 a, v64int8 b)
v32acc32 | negmul_conv_4x4_8ch (v64int8 a, v64int8 b)
v32acc32 | mac_conv_4x4_8ch (v64int8 a, v64int8 b, v32acc32 acc1)
v32acc32 | msc_conv_4x4_8ch (v64int8 a, v64int8 b, v32acc32 acc1)
v32acc32 | negmac_conv_4x4_8ch (v64int8 a, v64int8 b, v32acc32 acc1)
v32acc32 | negmsc_conv_4x4_8ch (v64int8 a, v64int8 b, v32acc32 acc1)
v32acc32 | addmac_conv_4x4_8ch (v64int8 a, v64int8 b, v32acc32 acc1, v32acc32 acc2)
v32acc32 | addmsc_conv_4x4_8ch (v64int8 a, v64int8 b, v32acc32 acc1, v32acc32 acc2)
v32acc32 | submac_conv_4x4_8ch (v64int8 a, v64int8 b, v32acc32 acc1, v32acc32 acc2)
v32acc32 | submsc_conv_4x4_8ch (v64int8 a, v64int8 b, v32acc32 acc1, v32acc32 acc2)

## Convolution of (4x4) matrix with (4x1) kernel and 8 channels with dynamic sign
v32acc32 | mul_conv_4x4_8ch (v64uint8 a, int sgn_x, v64uint8 b, int sgn_y)
v32acc32 | negmul_conv_4x4_8ch (v64uint8 a, int sgn_x, v64uint8 b, int sgn_y)
v32acc32 | mac_conv_4x4_8ch (v64uint8 a, int sgn_x, v64uint8 b, int sgn_y, v32acc32 acc1)
v32acc32 | msc_conv_4x4_8ch (v64uint8 a, int sgn_x, v64uint8 b, int sgn_y, v32acc32 acc1)
v32acc32 | negmac_conv_4x4_8ch (v64uint8 a, int sgn_x, v64uint8 b, int sgn_y, v32acc32 acc1)
v32acc32 | negmsc_conv_4x4_8ch (v64uint8 a, int sgn_x, v64uint8 b, int sgn_y, v32acc32 acc1)
v32acc32 | addmac_conv_4x4_8ch (v64uint8 a, int sgn_x, v64uint8 b, int sgn_y, v32acc32 acc1, v32acc32 acc2)
v32acc32 | addmsc_conv_4x4_8ch (v64uint8 a, int sgn_x, v64uint8 b, int sgn_y, v32acc32 acc1, v32acc32 acc2)
v32acc32 | submac_conv_4x4_8ch (v64uint8 a, int sgn_x, v64uint8 b, int sgn_y, v32acc32 acc1, v32acc32 acc2)
v32acc32 | submsc_conv_4x4_8ch (v64uint8 a, int sgn_x, v64uint8 b, int sgn_y, v32acc32 acc1, v32acc32 acc2)
v32acc32 | mul_conv_4x4_8ch (v64uint8 a, int sgn_x, v64int8 b, int sgn_y)
v32acc32 | negmul_conv_4x4_8ch (v64uint8 a, int sgn_x, v64int8 b, int sgn_y)
v32acc32 | mac_conv_4x4_8ch (v64uint8 a, int sgn_x, v64int8 b, int sgn_y, v32acc32 acc1)
v32acc32 | msc_conv_4x4_8ch (v64uint8 a, int sgn_x, v64int8 b, int sgn_y, v32acc32 acc1)
v32acc32 | negmac_conv_4x4_8ch (v64uint8 a, int sgn_x, v64int8 b, int sgn_y, v32acc32 acc1)
v32acc32 | negmsc_conv_4x4_8ch (v64uint8 a, int sgn_x, v64int8 b, int sgn_y, v32acc32 acc1)
v32acc32 | addmac_conv_4x4_8ch (v64uint8 a, int sgn_x, v64int8 b, int sgn_y, v32acc32 acc1, v32acc32 acc2)
v32acc32 | addmsc_conv_4x4_8ch (v64uint8 a, int sgn_x, v64int8 b, int sgn_y, v32acc32 acc1, v32acc32 acc2)
v32acc32 | submac_conv_4x4_8ch (v64uint8 a, int sgn_x, v64int8 b, int sgn_y, v32acc32 acc1, v32acc32 acc2)
v32acc32 | submsc_conv_4x4_8ch (v64uint8 a, int sgn_x, v64int8 b, int sgn_y, v32acc32 acc1, v32acc32 acc2)
v32acc32 | mul_conv_4x4_8ch (v64int8 a, int sgn_x, v64uint8 b, int sgn_y)
v32acc32 | negmul_conv_4x4_8ch (v64int8 a, int sgn_x, v64uint8 b, int sgn_y)
v32acc32 | mac_conv_4x4_8ch (v64int8 a, int sgn_x, v64uint8 b, int sgn_y, v32acc32 acc1)
v32acc32 | msc_conv_4x4_8ch (v64int8 a, int sgn_x, v64uint8 b, int sgn_y, v32acc32 acc1)
v32acc32 | negmac_conv_4x4_8ch (v64int8 a, int sgn_x, v64uint8 b, int sgn_y, v32acc32 acc1)
v32acc32 | negmsc_conv_4x4_8ch (v64int8 a, int sgn_x, v64uint8 b, int sgn_y, v32acc32 acc1)
v32acc32 | addmac_conv_4x4_8ch (v64int8 a, int sgn_x, v64uint8 b, int sgn_y, v32acc32 acc1, v32acc32 acc2)
v32acc32 | addmsc_conv_4x4_8ch (v64int8 a, int sgn_x, v64uint8 b, int sgn_y, v32acc32 acc1, v32acc32 acc2)
v32acc32 | submac_conv_4x4_8ch (v64int8 a, int sgn_x, v64uint8 b, int sgn_y, v32acc32 acc1, v32acc32 acc2)
v32acc32 | submsc_conv_4x4_8ch (v64int8 a, int sgn_x, v64uint8 b, int sgn_y, v32acc32 acc1, v32acc32 acc2)
v32acc32 | mul_conv_4x4_8ch (v64int8 a, int sgn_x, v64int8 b, int sgn_y)
v32acc32 | negmul_conv_4x4_8ch (v64int8 a, int sgn_x, v64int8 b, int sgn_y)
v32acc32 | mac_conv_4x4_8ch (v64int8 a, int sgn_x, v64int8 b, int sgn_y, v32acc32 acc1)
v32acc32 | msc_conv_4x4_8ch (v64int8 a, int sgn_x, v64int8 b, int sgn_y, v32acc32 acc1)
v32acc32 | negmac_conv_4x4_8ch (v64int8 a, int sgn_x, v64int8 b, int sgn_y, v32acc32 acc1)
v32acc32 | negmsc_conv_4x4_8ch (v64int8 a, int sgn_x, v64int8 b, int sgn_y, v32acc32 acc1)
v32acc32 | addmac_conv_4x4_8ch (v64int8 a, int sgn_x, v64int8 b, int sgn_y, v32acc32 acc1, v32acc32 acc2)
v32acc32 | addmsc_conv_4x4_8ch (v64int8 a, int sgn_x, v64int8 b, int sgn_y, v32acc32 acc1, v32acc32 acc2)
v32acc32 | submac_conv_4x4_8ch (v64int8 a, int sgn_x, v64int8 b, int sgn_y, v32acc32 acc1, v32acc32 acc2)
v32acc32 | submsc_conv_4x4_8ch (v64int8 a, int sgn_x, v64int8 b, int sgn_y, v32acc32 acc1, v32acc32 acc2)

## Convolution of (4x4) matrix with (4x1) kernel and 8 channels with dynamic negation of multiplication result
v32acc32 | mul_conv_4x4_8ch_conf (v64uint8 a, v64uint8 b, int sub_mul)
v32acc32 | negmul_conv_4x4_8ch_conf (v64uint8 a, v64uint8 b, int sub_mul)
v32acc32 | mul_conv_4x4_8ch_conf (v64uint8 a, v64int8 b, int sub_mul)
v32acc32 | negmul_conv_4x4_8ch_conf (v64uint8 a, v64int8 b, int sub_mul)
v32acc32 | mul_conv_4x4_8ch_conf (v64int8 a, v64uint8 b, int sub_mul)
v32acc32 | negmul_conv_4x4_8ch_conf (v64int8 a, v64uint8 b, int sub_mul)
v32acc32 | mul_conv_4x4_8ch_conf (v64int8 a, v64int8 b, int sub_mul)
v32acc32 | negmul_conv_4x4_8ch_conf (v64int8 a, v64int8 b, int sub_mul)

## Convolution of (4x4) matrix with (4x1) kernel and 8 channels with dynamic negation of multiplication result, zeroing of acc1, and negation of acc1
v32acc32 | mac_conv_4x4_8ch_conf (v64uint8 a, v64uint8 b, v32acc32 acc1, int zero_acc1, int shift16, int sub_mul, int sub_acc1)
v32acc32 | msc_conv_4x4_8ch_conf (v64uint8 a, v64uint8 b, v32acc32 acc1, int zero_acc1, int shift16, int sub_mul, int sub_acc1)
v32acc32 | negmsc_conv_4x4_8ch_conf (v64uint8 a, v64uint8 b, v32acc32 acc1, int zero_acc1, int sub_mul, int sub_acc1)
v32acc32 | negmac_conv_4x4_8ch_conf (v64uint8 a, v64uint8 b, v32acc32 acc1, int zero_acc1, int sub_mul, int sub_acc1)
v32acc32 | addmac_conv_4x4_8ch_conf (v64uint8 a, v64uint8 b, v32acc32 acc1, v32acc32 acc2, int zero_acc1, int shift16, int sub_mul, int sub_acc1, int sub_acc2)
v32acc32 | addmsc_conv_4x4_8ch_conf (v64uint8 a, v64uint8 b, v32acc32 acc1, v32acc32 acc2, int zero_acc1, int shift16, int sub_mul, int sub_acc1, int sub_acc2)
v32acc32 | submac_conv_4x4_8ch_conf (v64uint8 a, v64uint8 b, v32acc32 acc1, v32acc32 acc2, int zero_acc1, int sub_mul, int sub_acc1, int sub_acc2)
v32acc32 | submsc_conv_4x4_8ch_conf (v64uint8 a, v64uint8 b, v32acc32 acc1, v32acc32 acc2, int zero_acc1, int sub_mul, int sub_acc1, int sub_acc2)
v32acc32 | mac_conv_4x4_8ch_conf (v64uint8 a, v64int8 b, v32acc32 acc1, int zero_acc1, int shift16, int sub_mul, int sub_acc1)
v32acc32 | msc_conv_4x4_8ch_conf (v64uint8 a, v64int8 b, v32acc32 acc1, int zero_acc1, int shift16, int sub_mul, int sub_acc1)
v32acc32 | negmsc_conv_4x4_8ch_conf (v64uint8 a, v64int8 b, v32acc32 acc1, int zero_acc1, int sub_mul, int sub_acc1)
v32acc32 | negmac_conv_4x4_8ch_conf (v64uint8 a, v64int8 b, v32acc32 acc1, int zero_acc1, int sub_mul, int sub_acc1)
v32acc32 | addmac_conv_4x4_8ch_conf (v64uint8 a, v64int8 b, v32acc32 acc1, v32acc32 acc2, int zero_acc1, int shift16, int sub_mul, int sub_acc1, int sub_acc2)
v32acc32 | addmsc_conv_4x4_8ch_conf (v64uint8 a, v64int8 b, v32acc32 acc1, v32acc32 acc2, int zero_acc1, int shift16, int sub_mul, int sub_acc1, int sub_acc2)
v32acc32 | submac_conv_4x4_8ch_conf (v64uint8 a, v64int8 b, v32acc32 acc1, v32acc32 acc2, int zero_acc1, int sub_mul, int sub_acc1, int sub_acc2)
v32acc32 | submsc_conv_4x4_8ch_conf (v64uint8 a, v64int8 b, v32acc32 acc1, v32acc32 acc2, int zero_acc1, int sub_mul, int sub_acc1, int sub_acc2)
v32acc32 | mac_conv_4x4_8ch_conf (v64int8 a, v64uint8 b, v32acc32 acc1, int zero_acc1, int shift16, int sub_mul, int sub_acc1)
v32acc32 | msc_conv_4x4_8ch_conf (v64int8 a, v64uint8 b, v32acc32 acc1, int zero_acc1, int shift16, int sub_mul, int sub_acc1)
v32acc32 | negmsc_conv_4x4_8ch_conf (v64int8 a, v64uint8 b, v32acc32 acc1, int zero_acc1, int sub_mul, int sub_acc1)
v32acc32 | negmac_conv_4x4_8ch_conf (v64int8 a, v64uint8 b, v32acc32 acc1, int zero_acc1, int sub_mul, int sub_acc1)
v32acc32 | addmac_conv_4x4_8ch_conf (v64int8 a, v64uint8 b, v32acc32 acc1, v32acc32 acc2, int zero_acc1, int shift16, int sub_mul, int sub_acc1, int sub_acc2)
v32acc32 | addmsc_conv_4x4_8ch_conf (v64int8 a, v64uint8 b, v32acc32 acc1, v32acc32 acc2, int zero_acc1, int shift16, int sub_mul, int sub_acc1, int sub_acc2)
v32acc32 | submac_conv_4x4_8ch_conf (v64int8 a, v64uint8 b, v32acc32 acc1, v32acc32 acc2, int zero_acc1, int sub_mul, int sub_acc1, int sub_acc2)
v32acc32 | submsc_conv_4x4_8ch_conf (v64int8 a, v64uint8 b, v32acc32 acc1, v32acc32 acc2, int zero_acc1, int sub_mul, int sub_acc1, int sub_acc2)
v32acc32 | mac_conv_4x4_8ch_conf (v64int8 a, v64int8 b, v32acc32 acc1, int zero_acc1, int shift16, int sub_mul, int sub_acc1)
v32acc32 | msc_conv_4x4_8ch_conf (v64int8 a, v64int8 b, v32acc32 acc1, int zero_acc1, int shift16, int sub_mul, int sub_acc1)
v32acc32 | negmsc_conv_4x4_8ch_conf (v64int8 a, v64int8 b, v32acc32 acc1, int zero_acc1, int sub_mul, int sub_acc1)
v32acc32 | negmac_conv_4x4_8ch_conf (v64int8 a, v64int8 b, v32acc32 acc1, int zero_acc1, int sub_mul, int sub_acc1)
v32acc32 | addmac_conv_4x4_8ch_conf (v64int8 a, v64int8 b, v32acc32 acc1, v32acc32 acc2, int zero_acc1, int shift16, int sub_mul, int sub_acc1, int sub_acc2)
v32acc32 | addmsc_conv_4x4_8ch_conf (v64int8 a, v64int8 b, v32acc32 acc1, v32acc32 acc2, int zero_acc1, int shift16, int sub_mul, int sub_acc1, int sub_acc2)
v32acc32 | submac_conv_4x4_8ch_conf (v64int8 a, v64int8 b, v32acc32 acc1, v32acc32 acc2, int zero_acc1, int sub_mul, int sub_acc1, int sub_acc2)
v32acc32 | submsc_conv_4x4_8ch_conf (v64int8 a, v64int8 b, v32acc32 acc1, v32acc32 acc2, int zero_acc1, int sub_mul, int sub_acc1, int sub_acc2)

## Convolution of (4x4) matrix with (4x1) kernel and 8 channels with dynamic sign and dynamic negation of multiplication result
v32acc32 | mul_conv_4x4_8ch_conf (v64uint8 a, int sgn_x, v64uint8 b, int sgn_y, int sub_mul)
v32acc32 | negmul_conv_4x4_8ch_conf (v64uint8 a, int sgn_x, v64uint8 b, int sgn_y, int sub_mul)
v32acc32 | mac_conv_4x4_8ch_conf (v64uint8 a, int sgn_x, v64uint8 b, int sgn_y, v32acc32 acc1, int zero_acc1, int shift16, int sub_mul, int sub_acc1)
v32acc32 | msc_conv_4x4_8ch_conf (v64uint8 a, int sgn_x, v64uint8 b, int sgn_y, v32acc32 acc1, int zero_acc1, int shift16, int sub_mul, int sub_acc1)
v32acc32 | negmsc_conv_4x4_8ch_conf (v64uint8 a, int sgn_x, v64uint8 b, int sgn_y, v32acc32 acc1, int zero_acc1, int sub_mul, int sub_acc1)
v32acc32 | negmac_conv_4x4_8ch_conf (v64uint8 a, int sgn_x, v64uint8 b, int sgn_y, v32acc32 acc1, int zero_acc1, int sub_mul, int sub_acc1)
v32acc32 | addmac_conv_4x4_8ch_conf (v64uint8 a, int sgn_x, v64uint8 b, int sgn_y, v32acc32 acc1, v32acc32 acc2, int zero_acc1, int shift16, int sub_mul, int sub_acc1, int sub_acc2)
v32acc32 | addmsc_conv_4x4_8ch_conf (v64uint8 a, int sgn_x, v64uint8 b, int sgn_y, v32acc32 acc1, v32acc32 acc2, int zero_acc1, int shift16, int sub_mul, int sub_acc1, int sub_acc2)
v32acc32 | submac_conv_4x4_8ch_conf (v64uint8 a, int sgn_x, v64uint8 b, int sgn_y, v32acc32 acc1, v32acc32 acc2, int zero_acc1, int sub_mul, int sub_acc1, int sub_acc2)
v32acc32 | submsc_conv_4x4_8ch_conf (v64uint8 a, int sgn_x, v64uint8 b, int sgn_y, v32acc32 acc1, v32acc32 acc2, int zero_acc1, int sub_mul, int sub_acc1, int sub_acc2)
v32acc32 | mul_conv_4x4_8ch_conf (v64uint8 a, int sgn_x, v64int8 b, int sgn_y, int sub_mul)
v32acc32 | negmul_conv_4x4_8ch_conf (v64uint8 a, int sgn_x, v64int8 b, int sgn_y, int sub_mul)
v32acc32 | mac_conv_4x4_8ch_conf (v64uint8 a, int sgn_x, v64int8 b, int sgn_y, v32acc32 acc1, int zero_acc1, int shift16, int sub_mul, int sub_acc1)
v32acc32 | msc_conv_4x4_8ch_conf (v64uint8 a, int sgn_x, v64int8 b, int sgn_y, v32acc32 acc1, int zero_acc1, int shift16, int sub_mul, int sub_acc1)
v32acc32 | negmsc_conv_4x4_8ch_conf (v64uint8 a, int sgn_x, v64int8 b, int sgn_y, v32acc32 acc1, int zero_acc1, int sub_mul, int sub_acc1)
v32acc32 | negmac_conv_4x4_8ch_conf (v64uint8 a, int sgn_x, v64int8 b, int sgn_y, v32acc32 acc1, int zero_acc1, int sub_mul, int sub_acc1)
v32acc32 | addmac_conv_4x4_8ch_conf (v64uint8 a, int sgn_x, v64int8 b, int sgn_y, v32acc32 acc1, v32acc32 acc2, int zero_acc1, int shift16, int sub_mul, int sub_acc1, int sub_acc2)
v32acc32 | addmsc_conv_4x4_8ch_conf (v64uint8 a, int sgn_x, v64int8 b, int sgn_y, v32acc32 acc1, v32acc32 acc2, int zero_acc1, int shift16, int sub_mul, int sub_acc1, int sub_acc2)
v32acc32 | submac_conv_4x4_8ch_conf (v64uint8 a, int sgn_x, v64int8 b, int sgn_y, v32acc32 acc1, v32acc32 acc2, int zero_acc1, int sub_mul, int sub_acc1, int sub_acc2)
v32acc32 | submsc_conv_4x4_8ch_conf (v64uint8 a, int sgn_x, v64int8 b, int sgn_y, v32acc32 acc1, v32acc32 acc2, int zero_acc1, int sub_mul, int sub_acc1, int sub_acc2)
v32acc32 | mul_conv_4x4_8ch_conf (v64int8 a, int sgn_x, v64uint8 b, int sgn_y, int sub_mul)
v32acc32 | negmul_conv_4x4_8ch_conf (v64int8 a, int sgn_x, v64uint8 b, int sgn_y, int sub_mul)
v32acc32 | mac_conv_4x4_8ch_conf (v64int8 a, int sgn_x, v64uint8 b, int sgn_y, v32acc32 acc1, int zero_acc1, int shift16, int sub_mul, int sub_acc1)
v32acc32 | msc_conv_4x4_8ch_conf (v64int8 a, int sgn_x, v64uint8 b, int sgn_y, v32acc32 acc1, int zero_acc1, int shift16, int sub_mul, int sub_acc1)
v32acc32 | negmsc_conv_4x4_8ch_conf (v64int8 a, int sgn_x, v64uint8 b, int sgn_y, v32acc32 acc1, int zero_acc1, int sub_mul, int sub_acc1)
v32acc32 | negmac_conv_4x4_8ch_conf (v64int8 a, int sgn_x, v64uint8 b, int sgn_y, v32acc32 acc1, int zero_acc1, int sub_mul, int sub_acc1)
v32acc32 | addmac_conv_4x4_8ch_conf (v64int8 a, int sgn_x, v64uint8 b, int sgn_y, v32acc32 acc1, v32acc32 acc2, int zero_acc1, int shift16, int sub_mul, int sub_acc1, int sub_acc2)
v32acc32 | addmsc_conv_4x4_8ch_conf (v64int8 a, int sgn_x, v64uint8 b, int sgn_y, v32acc32 acc1, v32acc32 acc2, int zero_acc1, int shift16, int sub_mul, int sub_acc1, int sub_acc2)
v32acc32 | submac_conv_4x4_8ch_conf (v64int8 a, int sgn_x, v64uint8 b, int sgn_y, v32acc32 acc1, v32acc32 acc2, int zero_acc1, int sub_mul, int sub_acc1, int sub_acc2)
v32acc32 | submsc_conv_4x4_8ch_conf (v64int8 a, int sgn_x, v64uint8 b, int sgn_y, v32acc32 acc1, v32acc32 acc2, int zero_acc1, int sub_mul, int sub_acc1, int sub_acc2)
v32acc32 | mul_conv_4x4_8ch_conf (v64int8 a, int sgn_x, v64int8 b, int sgn_y, int sub_mul)
v32acc32 | negmul_conv_4x4_8ch_conf (v64int8 a, int sgn_x, v64int8 b, int sgn_y, int sub_mul)
v32acc32 | mac_conv_4x4_8ch_conf (v64int8 a, int sgn_x, v64int8 b, int sgn_y, v32acc32 acc1, int zero_acc1, int shift16, int sub_mul, int sub_acc1)
v32acc32 | msc_conv_4x4_8ch_conf (v64int8 a, int sgn_x, v64int8 b, int sgn_y, v32acc32 acc1, int zero_acc1, int shift16, int sub_mul, int sub_acc1)
v32acc32 | negmsc_conv_4x4_8ch_conf (v64int8 a, int sgn_x, v64int8 b, int sgn_y, v32acc32 acc1, int zero_acc1, int sub_mul, int sub_acc1)
v32acc32 | negmac_conv_4x4_8ch_conf (v64int8 a, int sgn_x, v64int8 b, int sgn_y, v32acc32 acc1, int zero_acc1, int sub_mul, int sub_acc1)
v32acc32 | addmac_conv_4x4_8ch_conf (v64int8 a, int sgn_x, v64int8 b, int sgn_y, v32acc32 acc1, v32acc32 acc2, int zero_acc1, int shift16, int sub_mul, int sub_acc1, int sub_acc2)
v32acc32 | addmsc_conv_4x4_8ch_conf (v64int8 a, int sgn_x, v64int8 b, int sgn_y, v32acc32 acc1, v32acc32 acc2, int zero_acc1, int shift16, int sub_mul, int sub_acc1, int sub_acc2)
v32acc32 | submac_conv_4x4_8ch_conf (v64int8 a, int sgn_x, v64int8 b, int sgn_y, v32acc32 acc1, v32acc32 acc2, int zero_acc1, int sub_mul, int sub_acc1, int sub_acc2)
v32acc32 | submsc_conv_4x4_8ch_conf (v64int8 a, int sgn_x, v64int8 b, int sgn_y, v32acc32 acc1, v32acc32 acc2, int zero_acc1, int sub_mul, int sub_acc1, int sub_acc2)

## Convolution of (8x8) matrix with (8x1) kernel and 4 channels
v32acc32 | mul_conv_8x8_4ch (v64uint8 a, v64uint8 b)
v32acc32 | negmul_conv_8x8_4ch (v64uint8 a, v64uint8 b)
v32acc32 | mac_conv_8x8_4ch (v64uint8 a, v64uint8 b, v32acc32 acc1)
v32acc32 | msc_conv_8x8_4ch (v64uint8 a, v64uint8 b, v32acc32 acc1)
v32acc32 | negmac_conv_8x8_4ch (v64uint8 a, v64uint8 b, v32acc32 acc1)
v32acc32 | negmsc_conv_8x8_4ch (v64uint8 a, v64uint8 b, v32acc32 acc1)
v32acc32 | addmac_conv_8x8_4ch (v64uint8 a, v64uint8 b, v32acc32 acc1, v32acc32 acc2)
v32acc32 | addmsc_conv_8x8_4ch (v64uint8 a, v64uint8 b, v32acc32 acc1, v32acc32 acc2)
v32acc32 | submac_conv_8x8_4ch (v64uint8 a, v64uint8 b, v32acc32 acc1, v32acc32 acc2)
v32acc32 | submsc_conv_8x8_4ch (v64uint8 a, v64uint8 b, v32acc32 acc1, v32acc32 acc2)
v32acc32 | mul_conv_8x8_4ch (v64uint8 a, v64int8 b)
v32acc32 | negmul_conv_8x8_4ch (v64uint8 a, v64int8 b)
v32acc32 | mac_conv_8x8_4ch (v64uint8 a, v64int8 b, v32acc32 acc1)
v32acc32 | msc_conv_8x8_4ch (v64uint8 a, v64int8 b, v32acc32 acc1)
v32acc32 | negmac_conv_8x8_4ch (v64uint8 a, v64int8 b, v32acc32 acc1)
v32acc32 | negmsc_conv_8x8_4ch (v64uint8 a, v64int8 b, v32acc32 acc1)
v32acc32 | addmac_conv_8x8_4ch (v64uint8 a, v64int8 b, v32acc32 acc1, v32acc32 acc2)
v32acc32 | addmsc_conv_8x8_4ch (v64uint8 a, v64int8 b, v32acc32 acc1, v32acc32 acc2)
v32acc32 | submac_conv_8x8_4ch (v64uint8 a, v64int8 b, v32acc32 acc1, v32acc32 acc2)
v32acc32 | submsc_conv_8x8_4ch (v64uint8 a, v64int8 b, v32acc32 acc1, v32acc32 acc2)
v32acc32 | mul_conv_8x8_4ch (v64int8 a, v64uint8 b)
v32acc32 | negmul_conv_8x8_4ch (v64int8 a, v64uint8 b)
v32acc32 | mac_conv_8x8_4ch (v64int8 a, v64uint8 b, v32acc32 acc1)
v32acc32 | msc_conv_8x8_4ch (v64int8 a, v64uint8 b, v32acc32 acc1)
v32acc32 | negmac_conv_8x8_4ch (v64int8 a, v64uint8 b, v32acc32 acc1)
v32acc32 | negmsc_conv_8x8_4ch (v64int8 a, v64uint8 b, v32acc32 acc1)
v32acc32 | addmac_conv_8x8_4ch (v64int8 a, v64uint8 b, v32acc32 acc1, v32acc32 acc2)
v32acc32 | addmsc_conv_8x8_4ch (v64int8 a, v64uint8 b, v32acc32 acc1, v32acc32 acc2)
v32acc32 | submac_conv_8x8_4ch (v64int8 a, v64uint8 b, v32acc32 acc1, v32acc32 acc2)
v32acc32 | submsc_conv_8x8_4ch (v64int8 a, v64uint8 b, v32acc32 acc1, v32acc32 acc2)
v32acc32 | mul_conv_8x8_4ch (v64int8 a, v64int8 b)
v32acc32 | negmul_conv_8x8_4ch (v64int8 a, v64int8 b)
v32acc32 | mac_conv_8x8_4ch (v64int8 a, v64int8 b, v32acc32 acc1)
v32acc32 | msc_conv_8x8_4ch (v64int8 a, v64int8 b, v32acc32 acc1)
v32acc32 | negmac_conv_8x8_4ch (v64int8 a, v64int8 b, v32acc32 acc1)
v32acc32 | negmsc_conv_8x8_4ch (v64int8 a, v64int8 b, v32acc32 acc1)
v32acc32 | addmac_conv_8x8_4ch (v64int8 a, v64int8 b, v32acc32 acc1, v32acc32 acc2)
v32acc32 | addmsc_conv_8x8_4ch (v64int8 a, v64int8 b, v32acc32 acc1, v32acc32 acc2)
v32acc32 | submac_conv_8x8_4ch (v64int8 a, v64int8 b, v32acc32 acc1, v32acc32 acc2)
v32acc32 | submsc_conv_8x8_4ch (v64int8 a, v64int8 b, v32acc32 acc1, v32acc32 acc2)

## Convolution of (8x8) matrix with (8x1) kernel and 4 channels with dynamic sign
v32acc32 | mul_conv_8x8_4ch (v64uint8 a, int sgn_x, v64uint8 b, int sgn_y)
v32acc32 | negmul_conv_8x8_4ch (v64uint8 a, int sgn_x, v64uint8 b, int sgn_y)
v32acc32 | mac_conv_8x8_4ch (v64uint8 a, int sgn_x, v64uint8 b, int sgn_y, v32acc32 acc1)
v32acc32 | msc_conv_8x8_4ch (v64uint8 a, int sgn_x, v64uint8 b, int sgn_y, v32acc32 acc1)
v32acc32 | negmac_conv_8x8_4ch (v64uint8 a, int sgn_x, v64uint8 b, int sgn_y, v32acc32 acc1)
v32acc32 | negmsc_conv_8x8_4ch (v64uint8 a, int sgn_x, v64uint8 b, int sgn_y, v32acc32 acc1)
v32acc32 | addmac_conv_8x8_4ch (v64uint8 a, int sgn_x, v64uint8 b, int sgn_y, v32acc32 acc1, v32acc32 acc2)
v32acc32 | addmsc_conv_8x8_4ch (v64uint8 a, int sgn_x, v64uint8 b, int sgn_y, v32acc32 acc1, v32acc32 acc2)
v32acc32 | submac_conv_8x8_4ch (v64uint8 a, int sgn_x, v64uint8 b, int sgn_y, v32acc32 acc1, v32acc32 acc2)
v32acc32 | submsc_conv_8x8_4ch (v64uint8 a, int sgn_x, v64uint8 b, int sgn_y, v32acc32 acc1, v32acc32 acc2)
v32acc32 | mul_conv_8x8_4ch (v64uint8 a, int sgn_x, v64int8 b, int sgn_y)
v32acc32 | negmul_conv_8x8_4ch (v64uint8 a, int sgn_x, v64int8 b, int sgn_y)
v32acc32 | mac_conv_8x8_4ch (v64uint8 a, int sgn_x, v64int8 b, int sgn_y, v32acc32 acc1)
v32acc32 | msc_conv_8x8_4ch (v64uint8 a, int sgn_x, v64int8 b, int sgn_y, v32acc32 acc1)
v32acc32 | negmac_conv_8x8_4ch (v64uint8 a, int sgn_x, v64int8 b, int sgn_y, v32acc32 acc1)
v32acc32 | negmsc_conv_8x8_4ch (v64uint8 a, int sgn_x, v64int8 b, int sgn_y, v32acc32 acc1)
v32acc32 | addmac_conv_8x8_4ch (v64uint8 a, int sgn_x, v64int8 b, int sgn_y, v32acc32 acc1, v32acc32 acc2)
v32acc32 | addmsc_conv_8x8_4ch (v64uint8 a, int sgn_x, v64int8 b, int sgn_y, v32acc32 acc1, v32acc32 acc2)
v32acc32 | submac_conv_8x8_4ch (v64uint8 a, int sgn_x, v64int8 b, int sgn_y, v32acc32 acc1, v32acc32 acc2)
v32acc32 | submsc_conv_8x8_4ch (v64uint8 a, int sgn_x, v64int8 b, int sgn_y, v32acc32 acc1, v32acc32 acc2)
v32acc32 | mul_conv_8x8_4ch (v64int8 a, int sgn_x, v64uint8 b, int sgn_y)
v32acc32 | negmul_conv_8x8_4ch (v64int8 a, int sgn_x, v64uint8 b, int sgn_y)
v32acc32 | mac_conv_8x8_4ch (v64int8 a, int sgn_x, v64uint8 b, int sgn_y, v32acc32 acc1)
v32acc32 | msc_conv_8x8_4ch (v64int8 a, int sgn_x, v64uint8 b, int sgn_y, v32acc32 acc1)
v32acc32 | negmac_conv_8x8_4ch (v64int8 a, int sgn_x, v64uint8 b, int sgn_y, v32acc32 acc1)
v32acc32 | negmsc_conv_8x8_4ch (v64int8 a, int sgn_x, v64uint8 b, int sgn_y, v32acc32 acc1)
v32acc32 | addmac_conv_8x8_4ch (v64int8 a, int sgn_x, v64uint8 b, int sgn_y, v32acc32 acc1, v32acc32 acc2)
v32acc32 | addmsc_conv_8x8_4ch (v64int8 a, int sgn_x, v64uint8 b, int sgn_y, v32acc32 acc1, v32acc32 acc2)
v32acc32 | submac_conv_8x8_4ch (v64int8 a, int sgn_x, v64uint8 b, int sgn_y, v32acc32 acc1, v32acc32 acc2)
v32acc32 | submsc_conv_8x8_4ch (v64int8 a, int sgn_x, v64uint8 b, int sgn_y, v32acc32 acc1, v32acc32 acc2)
v32acc32 | mul_conv_8x8_4ch (v64int8 a, int sgn_x, v64int8 b, int sgn_y)
v32acc32 | negmul_conv_8x8_4ch (v64int8 a, int sgn_x, v64int8 b, int sgn_y)
v32acc32 | mac_conv_8x8_4ch (v64int8 a, int sgn_x, v64int8 b, int sgn_y, v32acc32 acc1)
v32acc32 | msc_conv_8x8_4ch (v64int8 a, int sgn_x, v64int8 b, int sgn_y, v32acc32 acc1)
v32acc32 | negmac_conv_8x8_4ch (v64int8 a, int sgn_x, v64int8 b, int sgn_y, v32acc32 acc1)
v32acc32 | negmsc_conv_8x8_4ch (v64int8 a, int sgn_x, v64int8 b, int sgn_y, v32acc32 acc1)
v32acc32 | addmac_conv_8x8_4ch (v64int8 a, int sgn_x, v64int8 b, int sgn_y, v32acc32 acc1, v32acc32 acc2)
v32acc32 | addmsc_conv_8x8_4ch (v64int8 a, int sgn_x, v64int8 b, int sgn_y, v32acc32 acc1, v32acc32 acc2)
v32acc32 | submac_conv_8x8_4ch (v64int8 a, int sgn_x, v64int8 b, int sgn_y, v32acc32 acc1, v32acc32 acc2)
v32acc32 | submsc_conv_8x8_4ch (v64int8 a, int sgn_x, v64int8 b, int sgn_y, v32acc32 acc1, v32acc32 acc2)

## Convolution of (8x8) matrix with (8x1) kernel and 4 channels with dynamic negation of multiplication result
v32acc32 | mul_conv_8x8_4ch_conf (v64uint8 a, v64uint8 b, int sub_mul)
v32acc32 | negmul_conv_8x8_4ch_conf (v64uint8 a, v64uint8 b, int sub_mul)
v32acc32 | mul_conv_8x8_4ch_conf (v64uint8 a, v64int8 b, int sub_mul)
v32acc32 | negmul_conv_8x8_4ch_conf (v64uint8 a, v64int8 b, int sub_mul)
v32acc32 | mul_conv_8x8_4ch_conf (v64int8 a, v64uint8 b, int sub_mul)
v32acc32 | negmul_conv_8x8_4ch_conf (v64int8 a, v64uint8 b, int sub_mul)
v32acc32 | mul_conv_8x8_4ch_conf (v64int8 a, v64int8 b, int sub_mul)
v32acc32 | negmul_conv_8x8_4ch_conf (v64int8 a, v64int8 b, int sub_mul)

## Convolution of (8x8) matrix with (8x1) kernel and 4 channels with dynamic negation of multiplication result, zeroing of acc1, and negation of acc1
v32acc32 | mac_conv_8x8_4ch_conf (v64uint8 a, v64uint8 b, v32acc32 acc1, int zero_acc1, int shift16, int sub_mul, int sub_acc1)
v32acc32 | msc_conv_8x8_4ch_conf (v64uint8 a, v64uint8 b, v32acc32 acc1, int zero_acc1, int shift16, int sub_mul, int sub_acc1)
v32acc32 | negmsc_conv_8x8_4ch_conf (v64uint8 a, v64uint8 b, v32acc32 acc1, int zero_acc1, int sub_mul, int sub_acc1)
v32acc32 | negmac_conv_8x8_4ch_conf (v64uint8 a, v64uint8 b, v32acc32 acc1, int zero_acc1, int sub_mul, int sub_acc1)
v32acc32 | addmac_conv_8x8_4ch_conf (v64uint8 a, v64uint8 b, v32acc32 acc1, v32acc32 acc2, int zero_acc1, int shift16, int sub_mul, int sub_acc1, int sub_acc2)
v32acc32 | addmsc_conv_8x8_4ch_conf (v64uint8 a, v64uint8 b, v32acc32 acc1, v32acc32 acc2, int zero_acc1, int shift16, int sub_mul, int sub_acc1, int sub_acc2)
v32acc32 | submac_conv_8x8_4ch_conf (v64uint8 a, v64uint8 b, v32acc32 acc1, v32acc32 acc2, int zero_acc1, int sub_mul, int sub_acc1, int sub_acc2)
v32acc32 | submsc_conv_8x8_4ch_conf (v64uint8 a, v64uint8 b, v32acc32 acc1, v32acc32 acc2, int zero_acc1, int sub_mul, int sub_acc1, int sub_acc2)
v32acc32 | mac_conv_8x8_4ch_conf (v64uint8 a, v64int8 b, v32acc32 acc1, int zero_acc1, int shift16, int sub_mul, int sub_acc1)
v32acc32 | msc_conv_8x8_4ch_conf (v64uint8 a, v64int8 b, v32acc32 acc1, int zero_acc1, int shift16, int sub_mul, int sub_acc1)
v32acc32 | negmsc_conv_8x8_4ch_conf (v64uint8 a, v64int8 b, v32acc32 acc1, int zero_acc1, int sub_mul, int sub_acc1)
v32acc32 | negmac_conv_8x8_4ch_conf (v64uint8 a, v64int8 b, v32acc32 acc1, int zero_acc1, int sub_mul, int sub_acc1)
v32acc32 | addmac_conv_8x8_4ch_conf (v64uint8 a, v64int8 b, v32acc32 acc1, v32acc32 acc2, int zero_acc1, int shift16, int sub_mul, int sub_acc1, int sub_acc2)
v32acc32 | addmsc_conv_8x8_4ch_conf (v64uint8 a, v64int8 b, v32acc32 acc1, v32acc32 acc2, int zero_acc1, int shift16, int sub_mul, int sub_acc1, int sub_acc2)
v32acc32 | submac_conv_8x8_4ch_conf (v64uint8 a, v64int8 b, v32acc32 acc1, v32acc32 acc2, int zero_acc1, int sub_mul, int sub_acc1, int sub_acc2)
v32acc32 | submsc_conv_8x8_4ch_conf (v64uint8 a, v64int8 b, v32acc32 acc1, v32acc32 acc2, int zero_acc1, int sub_mul, int sub_acc1, int sub_acc2)
v32acc32 | mac_conv_8x8_4ch_conf (v64int8 a, v64uint8 b, v32acc32 acc1, int zero_acc1, int shift16, int sub_mul, int sub_acc1)
v32acc32 | msc_conv_8x8_4ch_conf (v64int8 a, v64uint8 b, v32acc32 acc1, int zero_acc1, int shift16, int sub_mul, int sub_acc1)
v32acc32 | negmsc_conv_8x8_4ch_conf (v64int8 a, v64uint8 b, v32acc32 acc1, int zero_acc1, int sub_mul, int sub_acc1)
v32acc32 | negmac_conv_8x8_4ch_conf (v64int8 a, v64uint8 b, v32acc32 acc1, int zero_acc1, int sub_mul, int sub_acc1)
v32acc32 | addmac_conv_8x8_4ch_conf (v64int8 a, v64uint8 b, v32acc32 acc1, v32acc32 acc2, int zero_acc1, int shift16, int sub_mul, int sub_acc1, int sub_acc2)
v32acc32 | addmsc_conv_8x8_4ch_conf (v64int8 a, v64uint8 b, v32acc32 acc1, v32acc32 acc2, int zero_acc1, int shift16, int sub_mul, int sub_acc1, int sub_acc2)
v32acc32 | submac_conv_8x8_4ch_conf (v64int8 a, v64uint8 b, v32acc32 acc1, v32acc32 acc2, int zero_acc1, int sub_mul, int sub_acc1, int sub_acc2)
v32acc32 | submsc_conv_8x8_4ch_conf (v64int8 a, v64uint8 b, v32acc32 acc1, v32acc32 acc2, int zero_acc1, int sub_mul, int sub_acc1, int sub_acc2)
v32acc32 | mac_conv_8x8_4ch_conf (v64int8 a, v64int8 b, v32acc32 acc1, int zero_acc1, int shift16, int sub_mul, int sub_acc1)
v32acc32 | msc_conv_8x8_4ch_conf (v64int8 a, v64int8 b, v32acc32 acc1, int zero_acc1, int shift16, int sub_mul, int sub_acc1)
v32acc32 | negmsc_conv_8x8_4ch_conf (v64int8 a, v64int8 b, v32acc32 acc1, int zero_acc1, int sub_mul, int sub_acc1)
v32acc32 | negmac_conv_8x8_4ch_conf (v64int8 a, v64int8 b, v32acc32 acc1, int zero_acc1, int sub_mul, int sub_acc1)
v32acc32 | addmac_conv_8x8_4ch_conf (v64int8 a, v64int8 b, v32acc32 acc1, v32acc32 acc2, int zero_acc1, int shift16, int sub_mul, int sub_acc1, int sub_acc2)
v32acc32 | addmsc_conv_8x8_4ch_conf (v64int8 a, v64int8 b, v32acc32 acc1, v32acc32 acc2, int zero_acc1, int shift16, int sub_mul, int sub_acc1, int sub_acc2)
v32acc32 | submac_conv_8x8_4ch_conf (v64int8 a, v64int8 b, v32acc32 acc1, v32acc32 acc2, int zero_acc1, int sub_mul, int sub_acc1, int sub_acc2)
v32acc32 | submsc_conv_8x8_4ch_conf (v64int8 a, v64int8 b, v32acc32 acc1, v32acc32 acc2, int zero_acc1, int sub_mul, int sub_acc1, int sub_acc2)

## Convolution of (8x8) matrix with (8x1) kernel and 4 channels with dynamic sign and dynamic negation of multiplication result
v32acc32 | mul_conv_8x8_4ch_conf (v64uint8 a, int sgn_x, v64uint8 b, int sgn_y, int sub_mul)
v32acc32 | negmul_conv_8x8_4ch_conf (v64uint8 a, int sgn_x, v64uint8 b, int sgn_y, int sub_mul)
v32acc32 | mac_conv_8x8_4ch_conf (v64uint8 a, int sgn_x, v64uint8 b, int sgn_y, v32acc32 acc1, int zero_acc1, int shift16, int sub_mul, int sub_acc1)
v32acc32 | msc_conv_8x8_4ch_conf (v64uint8 a, int sgn_x, v64uint8 b, int sgn_y, v32acc32 acc1, int zero_acc1, int shift16, int sub_mul, int sub_acc1)
v32acc32 | negmsc_conv_8x8_4ch_conf (v64uint8 a, int sgn_x, v64uint8 b, int sgn_y, v32acc32 acc1, int zero_acc1, int sub_mul, int sub_acc1)
v32acc32 | negmac_conv_8x8_4ch_conf (v64uint8 a, int sgn_x, v64uint8 b, int sgn_y, v32acc32 acc1, int zero_acc1, int sub_mul, int sub_acc1)
v32acc32 | addmac_conv_8x8_4ch_conf (v64uint8 a, int sgn_x, v64uint8 b, int sgn_y, v32acc32 acc1, v32acc32 acc2, int zero_acc1, int shift16, int sub_mul, int sub_acc1, int sub_acc2)
v32acc32 | addmsc_conv_8x8_4ch_conf (v64uint8 a, int sgn_x, v64uint8 b, int sgn_y, v32acc32 acc1, v32acc32 acc2, int zero_acc1, int shift16, int sub_mul, int sub_acc1, int sub_acc2)
v32acc32 | submac_conv_8x8_4ch_conf (v64uint8 a, int sgn_x, v64uint8 b, int sgn_y, v32acc32 acc1, v32acc32 acc2, int zero_acc1, int sub_mul, int sub_acc1, int sub_acc2)
v32acc32 | submsc_conv_8x8_4ch_conf (v64uint8 a, int sgn_x, v64uint8 b, int sgn_y, v32acc32 acc1, v32acc32 acc2, int zero_acc1, int sub_mul, int sub_acc1, int sub_acc2)
v32acc32 | mul_conv_8x8_4ch_conf (v64uint8 a, int sgn_x, v64int8 b, int sgn_y, int sub_mul)
v32acc32 | negmul_conv_8x8_4ch_conf (v64uint8 a, int sgn_x, v64int8 b, int sgn_y, int sub_mul)
v32acc32 | mac_conv_8x8_4ch_conf (v64uint8 a, int sgn_x, v64int8 b, int sgn_y, v32acc32 acc1, int zero_acc1, int shift16, int sub_mul, int sub_acc1)
v32acc32 | msc_conv_8x8_4ch_conf (v64uint8 a, int sgn_x, v64int8 b, int sgn_y, v32acc32 acc1, int zero_acc1, int shift16, int sub_mul, int sub_acc1)
v32acc32 | negmsc_conv_8x8_4ch_conf (v64uint8 a, int sgn_x, v64int8 b, int sgn_y, v32acc32 acc1, int zero_acc1, int sub_mul, int sub_acc1)
v32acc32 | negmac_conv_8x8_4ch_conf (v64uint8 a, int sgn_x, v64int8 b, int sgn_y, v32acc32 acc1, int zero_acc1, int sub_mul, int sub_acc1)
v32acc32 | addmac_conv_8x8_4ch_conf (v64uint8 a, int sgn_x, v64int8 b, int sgn_y, v32acc32 acc1, v32acc32 acc2, int zero_acc1, int shift16, int sub_mul, int sub_acc1, int sub_acc2)
v32acc32 | addmsc_conv_8x8_4ch_conf (v64uint8 a, int sgn_x, v64int8 b, int sgn_y, v32acc32 acc1, v32acc32 acc2, int zero_acc1, int shift16, int sub_mul, int sub_acc1, int sub_acc2)
v32acc32 | submac_conv_8x8_4ch_conf (v64uint8 a, int sgn_x, v64int8 b, int sgn_y, v32acc32 acc1, v32acc32 acc2, int zero_acc1, int sub_mul, int sub_acc1, int sub_acc2)
v32acc32 | submsc_conv_8x8_4ch_conf (v64uint8 a, int sgn_x, v64int8 b, int sgn_y, v32acc32 acc1, v32acc32 acc2, int zero_acc1, int sub_mul, int sub_acc1, int sub_acc2)
v32acc32 | mul_conv_8x8_4ch_conf (v64int8 a, int sgn_x, v64uint8 b, int sgn_y, int sub_mul)
v32acc32 | negmul_conv_8x8_4ch_conf (v64int8 a, int sgn_x, v64uint8 b, int sgn_y, int sub_mul)
v32acc32 | mac_conv_8x8_4ch_conf (v64int8 a, int sgn_x, v64uint8 b, int sgn_y, v32acc32 acc1, int zero_acc1, int shift16, int sub_mul, int sub_acc1)
v32acc32 | msc_conv_8x8_4ch_conf (v64int8 a, int sgn_x, v64uint8 b, int sgn_y, v32acc32 acc1, int zero_acc1, int shift16, int sub_mul, int sub_acc1)
v32acc32 | negmsc_conv_8x8_4ch_conf (v64int8 a, int sgn_x, v64uint8 b, int sgn_y, v32acc32 acc1, int zero_acc1, int sub_mul, int sub_acc1)
v32acc32 | negmac_conv_8x8_4ch_conf (v64int8 a, int sgn_x, v64uint8 b, int sgn_y, v32acc32 acc1, int zero_acc1, int sub_mul, int sub_acc1)
v32acc32 | addmac_conv_8x8_4ch_conf (v64int8 a, int sgn_x, v64uint8 b, int sgn_y, v32acc32 acc1, v32acc32 acc2, int zero_acc1, int shift16, int sub_mul, int sub_acc1, int sub_acc2)
v32acc32 | addmsc_conv_8x8_4ch_conf (v64int8 a, int sgn_x, v64uint8 b, int sgn_y, v32acc32 acc1, v32acc32 acc2, int zero_acc1, int shift16, int sub_mul, int sub_acc1, int sub_acc2)
v32acc32 | submac_conv_8x8_4ch_conf (v64int8 a, int sgn_x, v64uint8 b, int sgn_y, v32acc32 acc1, v32acc32 acc2, int zero_acc1, int sub_mul, int sub_acc1, int sub_acc2)
v32acc32 | submsc_conv_8x8_4ch_conf (v64int8 a, int sgn_x, v64uint8 b, int sgn_y, v32acc32 acc1, v32acc32 acc2, int zero_acc1, int sub_mul, int sub_acc1, int sub_acc2)
v32acc32 | mul_conv_8x8_4ch_conf (v64int8 a, int sgn_x, v64int8 b, int sgn_y, int sub_mul)
v32acc32 | negmul_conv_8x8_4ch_conf (v64int8 a, int sgn_x, v64int8 b, int sgn_y, int sub_mul)
v32acc32 | mac_conv_8x8_4ch_conf (v64int8 a, int sgn_x, v64int8 b, int sgn_y, v32acc32 acc1, int zero_acc1, int shift16, int sub_mul, int sub_acc1)
v32acc32 | msc_conv_8x8_4ch_conf (v64int8 a, int sgn_x, v64int8 b, int sgn_y, v32acc32 acc1, int zero_acc1, int shift16, int sub_mul, int sub_acc1)
v32acc32 | negmsc_conv_8x8_4ch_conf (v64int8 a, int sgn_x, v64int8 b, int sgn_y, v32acc32 acc1, int zero_acc1, int sub_mul, int sub_acc1)
v32acc32 | negmac_conv_8x8_4ch_conf (v64int8 a, int sgn_x, v64int8 b, int sgn_y, v32acc32 acc1, int zero_acc1, int sub_mul, int sub_acc1)
v32acc32 | addmac_conv_8x8_4ch_conf (v64int8 a, int sgn_x, v64int8 b, int sgn_y, v32acc32 acc1, v32acc32 acc2, int zero_acc1, int shift16, int sub_mul, int sub_acc1, int sub_acc2)
v32acc32 | addmsc_conv_8x8_4ch_conf (v64int8 a, int sgn_x, v64int8 b, int sgn_y, v32acc32 acc1, v32acc32 acc2, int zero_acc1, int shift16, int sub_mul, int sub_acc1, int sub_acc2)
v32acc32 | submac_conv_8x8_4ch_conf (v64int8 a, int sgn_x, v64int8 b, int sgn_y, v32acc32 acc1, v32acc32 acc2, int zero_acc1, int sub_mul, int sub_acc1, int sub_acc2)
v32acc32 | submsc_conv_8x8_4ch_conf (v64int8 a, int sgn_x, v64int8 b, int sgn_y, v32acc32 acc1, v32acc32 acc2, int zero_acc1, int sub_mul, int sub_acc1, int sub_acc2)

## Convolution of (32x8) matrix with (8x1) kernel
v32acc32 | mul_conv_32x8 (v64uint8 a, v64uint8 b)
v32acc32 | negmul_conv_32x8 (v64uint8 a, v64uint8 b)
v32acc32 | mac_conv_32x8 (v64uint8 a, v64uint8 b, v32acc32 acc1)
v32acc32 | msc_conv_32x8 (v64uint8 a, v64uint8 b, v32acc32 acc1)
v32acc32 | negmac_conv_32x8 (v64uint8 a, v64uint8 b, v32acc32 acc1)
v32acc32 | negmsc_conv_32x8 (v64uint8 a, v64uint8 b, v32acc32 acc1)
v32acc32 | addmac_conv_32x8 (v64uint8 a, v64uint8 b, v32acc32 acc1, v32acc32 acc2)
v32acc32 | addmsc_conv_32x8 (v64uint8 a, v64uint8 b, v32acc32 acc1, v32acc32 acc2)
v32acc32 | submac_conv_32x8 (v64uint8 a, v64uint8 b, v32acc32 acc1, v32acc32 acc2)
v32acc32 | submsc_conv_32x8 (v64uint8 a, v64uint8 b, v32acc32 acc1, v32acc32 acc2)
v32acc32 | mul_conv_32x8 (v64uint8 a, v64int8 b)
v32acc32 | negmul_conv_32x8 (v64uint8 a, v64int8 b)
v32acc32 | mac_conv_32x8 (v64uint8 a, v64int8 b, v32acc32 acc1)
v32acc32 | msc_conv_32x8 (v64uint8 a, v64int8 b, v32acc32 acc1)
v32acc32 | negmac_conv_32x8 (v64uint8 a, v64int8 b, v32acc32 acc1)
v32acc32 | negmsc_conv_32x8 (v64uint8 a, v64int8 b, v32acc32 acc1)
v32acc32 | addmac_conv_32x8 (v64uint8 a, v64int8 b, v32acc32 acc1, v32acc32 acc2)
v32acc32 | addmsc_conv_32x8 (v64uint8 a, v64int8 b, v32acc32 acc1, v32acc32 acc2)
v32acc32 | submac_conv_32x8 (v64uint8 a, v64int8 b, v32acc32 acc1, v32acc32 acc2)
v32acc32 | submsc_conv_32x8 (v64uint8 a, v64int8 b, v32acc32 acc1, v32acc32 acc2)
v32acc32 | mul_conv_32x8 (v64int8 a, v64uint8 b)
v32acc32 | negmul_conv_32x8 (v64int8 a, v64uint8 b)
v32acc32 | mac_conv_32x8 (v64int8 a, v64uint8 b, v32acc32 acc1)
v32acc32 | msc_conv_32x8 (v64int8 a, v64uint8 b, v32acc32 acc1)
v32acc32 | negmac_conv_32x8 (v64int8 a, v64uint8 b, v32acc32 acc1)
v32acc32 | negmsc_conv_32x8 (v64int8 a, v64uint8 b, v32acc32 acc1)
v32acc32 | addmac_conv_32x8 (v64int8 a, v64uint8 b, v32acc32 acc1, v32acc32 acc2)
v32acc32 | addmsc_conv_32x8 (v64int8 a, v64uint8 b, v32acc32 acc1, v32acc32 acc2)
v32acc32 | submac_conv_32x8 (v64int8 a, v64uint8 b, v32acc32 acc1, v32acc32 acc2)
v32acc32 | submsc_conv_32x8 (v64int8 a, v64uint8 b, v32acc32 acc1, v32acc32 acc2)
v32acc32 | mul_conv_32x8 (v64int8 a, v64int8 b)
v32acc32 | negmul_conv_32x8 (v64int8 a, v64int8 b)
v32acc32 | mac_conv_32x8 (v64int8 a, v64int8 b, v32acc32 acc1)
v32acc32 | msc_conv_32x8 (v64int8 a, v64int8 b, v32acc32 acc1)
v32acc32 | negmac_conv_32x8 (v64int8 a, v64int8 b, v32acc32 acc1)
v32acc32 | negmsc_conv_32x8 (v64int8 a, v64int8 b, v32acc32 acc1)
v32acc32 | addmac_conv_32x8 (v64int8 a, v64int8 b, v32acc32 acc1, v32acc32 acc2)
v32acc32 | addmsc_conv_32x8 (v64int8 a, v64int8 b, v32acc32 acc1, v32acc32 acc2)
v32acc32 | submac_conv_32x8 (v64int8 a, v64int8 b, v32acc32 acc1, v32acc32 acc2)
v32acc32 | submsc_conv_32x8 (v64int8 a, v64int8 b, v32acc32 acc1, v32acc32 acc2)

## Convolution of (32x8) matrix with (8x1) kernel with dynamic sign
v32acc32 | mul_conv_32x8 (v64uint8 a, int sgn_x, v64uint8 b, int sgn_y)
v32acc32 | negmul_conv_32x8 (v64uint8 a, int sgn_x, v64uint8 b, int sgn_y)
v32acc32 | mac_conv_32x8 (v64uint8 a, int sgn_x, v64uint8 b, int sgn_y, v32acc32 acc1)
v32acc32 | msc_conv_32x8 (v64uint8 a, int sgn_x, v64uint8 b, int sgn_y, v32acc32 acc1)
v32acc32 | negmac_conv_32x8 (v64uint8 a, int sgn_x, v64uint8 b, int sgn_y, v32acc32 acc1)
v32acc32 | negmsc_conv_32x8 (v64uint8 a, int sgn_x, v64uint8 b, int sgn_y, v32acc32 acc1)
v32acc32 | addmac_conv_32x8 (v64uint8 a, int sgn_x, v64uint8 b, int sgn_y, v32acc32 acc1, v32acc32 acc2)
v32acc32 | addmsc_conv_32x8 (v64uint8 a, int sgn_x, v64uint8 b, int sgn_y, v32acc32 acc1, v32acc32 acc2)
v32acc32 | submac_conv_32x8 (v64uint8 a, int sgn_x, v64uint8 b, int sgn_y, v32acc32 acc1, v32acc32 acc2)
v32acc32 | submsc_conv_32x8 (v64uint8 a, int sgn_x, v64uint8 b, int sgn_y, v32acc32 acc1, v32acc32 acc2)
v32acc32 | mul_conv_32x8 (v64uint8 a, int sgn_x, v64int8 b, int sgn_y)
v32acc32 | negmul_conv_32x8 (v64uint8 a, int sgn_x, v64int8 b, int sgn_y)
v32acc32 | mac_conv_32x8 (v64uint8 a, int sgn_x, v64int8 b, int sgn_y, v32acc32 acc1)
v32acc32 | msc_conv_32x8 (v64uint8 a, int sgn_x, v64int8 b, int sgn_y, v32acc32 acc1)
v32acc32 | negmac_conv_32x8 (v64uint8 a, int sgn_x, v64int8 b, int sgn_y, v32acc32 acc1)
v32acc32 | negmsc_conv_32x8 (v64uint8 a, int sgn_x, v64int8 b, int sgn_y, v32acc32 acc1)
v32acc32 | addmac_conv_32x8 (v64uint8 a, int sgn_x, v64int8 b, int sgn_y, v32acc32 acc1, v32acc32 acc2)
v32acc32 | addmsc_conv_32x8 (v64uint8 a, int sgn_x, v64int8 b, int sgn_y, v32acc32 acc1, v32acc32 acc2)
v32acc32 | submac_conv_32x8 (v64uint8 a, int sgn_x, v64int8 b, int sgn_y, v32acc32 acc1, v32acc32 acc2)
v32acc32 | submsc_conv_32x8 (v64uint8 a, int sgn_x, v64int8 b, int sgn_y, v32acc32 acc1, v32acc32 acc2)
v32acc32 | mul_conv_32x8 (v64int8 a, int sgn_x, v64uint8 b, int sgn_y)
v32acc32 | negmul_conv_32x8 (v64int8 a, int sgn_x, v64uint8 b, int sgn_y)
v32acc32 | mac_conv_32x8 (v64int8 a, int sgn_x, v64uint8 b, int sgn_y, v32acc32 acc1)
v32acc32 | msc_conv_32x8 (v64int8 a, int sgn_x, v64uint8 b, int sgn_y, v32acc32 acc1)
v32acc32 | negmac_conv_32x8 (v64int8 a, int sgn_x, v64uint8 b, int sgn_y, v32acc32 acc1)
v32acc32 | negmsc_conv_32x8 (v64int8 a, int sgn_x, v64uint8 b, int sgn_y, v32acc32 acc1)
v32acc32 | addmac_conv_32x8 (v64int8 a, int sgn_x, v64uint8 b, int sgn_y, v32acc32 acc1, v32acc32 acc2)
v32acc32 | addmsc_conv_32x8 (v64int8 a, int sgn_x, v64uint8 b, int sgn_y, v32acc32 acc1, v32acc32 acc2)
v32acc32 | submac_conv_32x8 (v64int8 a, int sgn_x, v64uint8 b, int sgn_y, v32acc32 acc1, v32acc32 acc2)
v32acc32 | submsc_conv_32x8 (v64int8 a, int sgn_x, v64uint8 b, int sgn_y, v32acc32 acc1, v32acc32 acc2)
v32acc32 | mul_conv_32x8 (v64int8 a, int sgn_x, v64int8 b, int sgn_y)
v32acc32 | negmul_conv_32x8 (v64int8 a, int sgn_x, v64int8 b, int sgn_y)
v32acc32 | mac_conv_32x8 (v64int8 a, int sgn_x, v64int8 b, int sgn_y, v32acc32 acc1)
v32acc32 | msc_conv_32x8 (v64int8 a, int sgn_x, v64int8 b, int sgn_y, v32acc32 acc1)
v32acc32 | negmac_conv_32x8 (v64int8 a, int sgn_x, v64int8 b, int sgn_y, v32acc32 acc1)
v32acc32 | negmsc_conv_32x8 (v64int8 a, int sgn_x, v64int8 b, int sgn_y, v32acc32 acc1)
v32acc32 | addmac_conv_32x8 (v64int8 a, int sgn_x, v64int8 b, int sgn_y, v32acc32 acc1, v32acc32 acc2)
v32acc32 | addmsc_conv_32x8 (v64int8 a, int sgn_x, v64int8 b, int sgn_y, v32acc32 acc1, v32acc32 acc2)
v32acc32 | submac_conv_32x8 (v64int8 a, int sgn_x, v64int8 b, int sgn_y, v32acc32 acc1, v32acc32 acc2)
v32acc32 | submsc_conv_32x8 (v64int8 a, int sgn_x, v64int8 b, int sgn_y, v32acc32 acc1, v32acc32 acc2)

## Convolution of (32x8) matrix with (8x1) kernel with dynamic negation of multiplication result
v32acc32 | mul_conv_32x8_conf (v64uint8 a, v64uint8 b, int sub_mul)
v32acc32 | negmul_conv_32x8_conf (v64uint8 a, v64uint8 b, int sub_mul)
v32acc32 | mul_conv_32x8_conf (v64uint8 a, v64int8 b, int sub_mul)
v32acc32 | negmul_conv_32x8_conf (v64uint8 a, v64int8 b, int sub_mul)
v32acc32 | mul_conv_32x8_conf (v64int8 a, v64uint8 b, int sub_mul)
v32acc32 | negmul_conv_32x8_conf (v64int8 a, v64uint8 b, int sub_mul)
v32acc32 | mul_conv_32x8_conf (v64int8 a, v64int8 b, int sub_mul)
v32acc32 | negmul_conv_32x8_conf (v64int8 a, v64int8 b, int sub_mul)

## Convolution of (32x8) matrix with (8x1) kernel with dynamic negation of multiplication result, zeroing of acc1, and negation of acc1
v32acc32 | mac_conv_32x8_conf (v64uint8 a, v64uint8 b, v32acc32 acc1, int zero_acc1, int shift16, int sub_mul, int sub_acc1)
v32acc32 | msc_conv_32x8_conf (v64uint8 a, v64uint8 b, v32acc32 acc1, int zero_acc1, int shift16, int sub_mul, int sub_acc1)
v32acc32 | negmsc_conv_32x8_conf (v64uint8 a, v64uint8 b, v32acc32 acc1, int zero_acc1, int sub_mul, int sub_acc1)
v32acc32 | negmac_conv_32x8_conf (v64uint8 a, v64uint8 b, v32acc32 acc1, int zero_acc1, int sub_mul, int sub_acc1)
v32acc32 | addmac_conv_32x8_conf (v64uint8 a, v64uint8 b, v32acc32 acc1, v32acc32 acc2, int zero_acc1, int shift16, int sub_mul, int sub_acc1, int sub_acc2)
v32acc32 | addmsc_conv_32x8_conf (v64uint8 a, v64uint8 b, v32acc32 acc1, v32acc32 acc2, int zero_acc1, int shift16, int sub_mul, int sub_acc1, int sub_acc2)
v32acc32 | submac_conv_32x8_conf (v64uint8 a, v64uint8 b, v32acc32 acc1, v32acc32 acc2, int zero_acc1, int sub_mul, int sub_acc1, int sub_acc2)
v32acc32 | submsc_conv_32x8_conf (v64uint8 a, v64uint8 b, v32acc32 acc1, v32acc32 acc2, int zero_acc1, int sub_mul, int sub_acc1, int sub_acc2)
v32acc32 | mac_conv_32x8_conf (v64uint8 a, v64int8 b, v32acc32 acc1, int zero_acc1, int shift16, int sub_mul, int sub_acc1)
v32acc32 | msc_conv_32x8_conf (v64uint8 a, v64int8 b, v32acc32 acc1, int zero_acc1, int shift16, int sub_mul, int sub_acc1)
v32acc32 | negmsc_conv_32x8_conf (v64uint8 a, v64int8 b, v32acc32 acc1, int zero_acc1, int sub_mul, int sub_acc1)
v32acc32 | negmac_conv_32x8_conf (v64uint8 a, v64int8 b, v32acc32 acc1, int zero_acc1, int sub_mul, int sub_acc1)
v32acc32 | addmac_conv_32x8_conf (v64uint8 a, v64int8 b, v32acc32 acc1, v32acc32 acc2, int zero_acc1, int shift16, int sub_mul, int sub_acc1, int sub_acc2)
v32acc32 | addmsc_conv_32x8_conf (v64uint8 a, v64int8 b, v32acc32 acc1, v32acc32 acc2, int zero_acc1, int shift16, int sub_mul, int sub_acc1, int sub_acc2)
v32acc32 | submac_conv_32x8_conf (v64uint8 a, v64int8 b, v32acc32 acc1, v32acc32 acc2, int zero_acc1, int sub_mul, int sub_acc1, int sub_acc2)
v32acc32 | submsc_conv_32x8_conf (v64uint8 a, v64int8 b, v32acc32 acc1, v32acc32 acc2, int zero_acc1, int sub_mul, int sub_acc1, int sub_acc2)
v32acc32 | mac_conv_32x8_conf (v64int8 a, v64uint8 b, v32acc32 acc1, int zero_acc1, int shift16, int sub_mul, int sub_acc1)
v32acc32 | msc_conv_32x8_conf (v64int8 a, v64uint8 b, v32acc32 acc1, int zero_acc1, int shift16, int sub_mul, int sub_acc1)
v32acc32 | negmsc_conv_32x8_conf (v64int8 a, v64uint8 b, v32acc32 acc1, int zero_acc1, int sub_mul, int sub_acc1)
v32acc32 | negmac_conv_32x8_conf (v64int8 a, v64uint8 b, v32acc32 acc1, int zero_acc1, int sub_mul, int sub_acc1)
v32acc32 | addmac_conv_32x8_conf (v64int8 a, v64uint8 b, v32acc32 acc1, v32acc32 acc2, int zero_acc1, int shift16, int sub_mul, int sub_acc1, int sub_acc2)
v32acc32 | addmsc_conv_32x8_conf (v64int8 a, v64uint8 b, v32acc32 acc1, v32acc32 acc2, int zero_acc1, int shift16, int sub_mul, int sub_acc1, int sub_acc2)
v32acc32 | submac_conv_32x8_conf (v64int8 a, v64uint8 b, v32acc32 acc1, v32acc32 acc2, int zero_acc1, int sub_mul, int sub_acc1, int sub_acc2)
v32acc32 | submsc_conv_32x8_conf (v64int8 a, v64uint8 b, v32acc32 acc1, v32acc32 acc2, int zero_acc1, int sub_mul, int sub_acc1, int sub_acc2)
v32acc32 | mac_conv_32x8_conf (v64int8 a, v64int8 b, v32acc32 acc1, int zero_acc1, int shift16, int sub_mul, int sub_acc1)
v32acc32 | msc_conv_32x8_conf (v64int8 a, v64int8 b, v32acc32 acc1, int zero_acc1, int shift16, int sub_mul, int sub_acc1)
v32acc32 | negmsc_conv_32x8_conf (v64int8 a, v64int8 b, v32acc32 acc1, int zero_acc1, int sub_mul, int sub_acc1)
v32acc32 | negmac_conv_32x8_conf (v64int8 a, v64int8 b, v32acc32 acc1, int zero_acc1, int sub_mul, int sub_acc1)
v32acc32 | addmac_conv_32x8_conf (v64int8 a, v64int8 b, v32acc32 acc1, v32acc32 acc2, int zero_acc1, int shift16, int sub_mul, int sub_acc1, int sub_acc2)
v32acc32 | addmsc_conv_32x8_conf (v64int8 a, v64int8 b, v32acc32 acc1, v32acc32 acc2, int zero_acc1, int shift16, int sub_mul, int sub_acc1, int sub_acc2)
v32acc32 | submac_conv_32x8_conf (v64int8 a, v64int8 b, v32acc32 acc1, v32acc32 acc2, int zero_acc1, int sub_mul, int sub_acc1, int sub_acc2)
v32acc32 | submsc_conv_32x8_conf (v64int8 a, v64int8 b, v32acc32 acc1, v32acc32 acc2, int zero_acc1, int sub_mul, int sub_acc1, int sub_acc2)

## Convolution of (32x8) matrix with (8x1) kernel with dynamic sign and dynamic negation of multiplication result
v32acc32 | mul_conv_32x8_conf (v64uint8 a, int sgn_x, v64uint8 b, int sgn_y, int sub_mul)
v32acc32 | negmul_conv_32x8_conf (v64uint8 a, int sgn_x, v64uint8 b, int sgn_y, int sub_mul)
v32acc32 | mac_conv_32x8_conf (v64uint8 a, int sgn_x, v64uint8 b, int sgn_y, v32acc32 acc1, int zero_acc1, int shift16, int sub_mul, int sub_acc1)
v32acc32 | msc_conv_32x8_conf (v64uint8 a, int sgn_x, v64uint8 b, int sgn_y, v32acc32 acc1, int zero_acc1, int shift16, int sub_mul, int sub_acc1)
v32acc32 | negmsc_conv_32x8_conf (v64uint8 a, int sgn_x, v64uint8 b, int sgn_y, v32acc32 acc1, int zero_acc1, int sub_mul, int sub_acc1)
v32acc32 | negmac_conv_32x8_conf (v64uint8 a, int sgn_x, v64uint8 b, int sgn_y, v32acc32 acc1, int zero_acc1, int sub_mul, int sub_acc1)
v32acc32 | addmac_conv_32x8_conf (v64uint8 a, int sgn_x, v64uint8 b, int sgn_y, v32acc32 acc1, v32acc32 acc2, int zero_acc1, int shift16, int sub_mul, int sub_acc1, int sub_acc2)
v32acc32 | addmsc_conv_32x8_conf (v64uint8 a, int sgn_x, v64uint8 b, int sgn_y, v32acc32 acc1, v32acc32 acc2, int zero_acc1, int shift16, int sub_mul, int sub_acc1, int sub_acc2)
v32acc32 | submac_conv_32x8_conf (v64uint8 a, int sgn_x, v64uint8 b, int sgn_y, v32acc32 acc1, v32acc32 acc2, int zero_acc1, int sub_mul, int sub_acc1, int sub_acc2)
v32acc32 | submsc_conv_32x8_conf (v64uint8 a, int sgn_x, v64uint8 b, int sgn_y, v32acc32 acc1, v32acc32 acc2, int zero_acc1, int sub_mul, int sub_acc1, int sub_acc2)
v32acc32 | mul_conv_32x8_conf (v64uint8 a, int sgn_x, v64int8 b, int sgn_y, int sub_mul)
v32acc32 | negmul_conv_32x8_conf (v64uint8 a, int sgn_x, v64int8 b, int sgn_y, int sub_mul)
v32acc32 | mac_conv_32x8_conf (v64uint8 a, int sgn_x, v64int8 b, int sgn_y, v32acc32 acc1, int zero_acc1, int shift16, int sub_mul, int sub_acc1)
v32acc32 | msc_conv_32x8_conf (v64uint8 a, int sgn_x, v64int8 b, int sgn_y, v32acc32 acc1, int zero_acc1, int shift16, int sub_mul, int sub_acc1)
v32acc32 | negmsc_conv_32x8_conf (v64uint8 a, int sgn_x, v64int8 b, int sgn_y, v32acc32 acc1, int zero_acc1, int sub_mul, int sub_acc1)
v32acc32 | negmac_conv_32x8_conf (v64uint8 a, int sgn_x, v64int8 b, int sgn_y, v32acc32 acc1, int zero_acc1, int sub_mul, int sub_acc1)
v32acc32 | addmac_conv_32x8_conf (v64uint8 a, int sgn_x, v64int8 b, int sgn_y, v32acc32 acc1, v32acc32 acc2, int zero_acc1, int shift16, int sub_mul, int sub_acc1, int sub_acc2)
v32acc32 | addmsc_conv_32x8_conf (v64uint8 a, int sgn_x, v64int8 b, int sgn_y, v32acc32 acc1, v32acc32 acc2, int zero_acc1, int shift16, int sub_mul, int sub_acc1, int sub_acc2)
v32acc32 | submac_conv_32x8_conf (v64uint8 a, int sgn_x, v64int8 b, int sgn_y, v32acc32 acc1, v32acc32 acc2, int zero_acc1, int sub_mul, int sub_acc1, int sub_acc2)
v32acc32 | submsc_conv_32x8_conf (v64uint8 a, int sgn_x, v64int8 b, int sgn_y, v32acc32 acc1, v32acc32 acc2, int zero_acc1, int sub_mul, int sub_acc1, int sub_acc2)
v32acc32 | mul_conv_32x8_conf (v64int8 a, int sgn_x, v64uint8 b, int sgn_y, int sub_mul)
v32acc32 | negmul_conv_32x8_conf (v64int8 a, int sgn_x, v64uint8 b, int sgn_y, int sub_mul)
v32acc32 | mac_conv_32x8_conf (v64int8 a, int sgn_x, v64uint8 b, int sgn_y, v32acc32 acc1, int zero_acc1, int shift16, int sub_mul, int sub_acc1)
v32acc32 | msc_conv_32x8_conf (v64int8 a, int sgn_x, v64uint8 b, int sgn_y, v32acc32 acc1, int zero_acc1, int shift16, int sub_mul, int sub_acc1)
v32acc32 | negmsc_conv_32x8_conf (v64int8 a, int sgn_x, v64uint8 b, int sgn_y, v32acc32 acc1, int zero_acc1, int sub_mul, int sub_acc1)
v32acc32 | negmac_conv_32x8_conf (v64int8 a, int sgn_x, v64uint8 b, int sgn_y, v32acc32 acc1, int zero_acc1, int sub_mul, int sub_acc1)
v32acc32 | addmac_conv_32x8_conf (v64int8 a, int sgn_x, v64uint8 b, int sgn_y, v32acc32 acc1, v32acc32 acc2, int zero_acc1, int shift16, int sub_mul, int sub_acc1, int sub_acc2)
v32acc32 | addmsc_conv_32x8_conf (v64int8 a, int sgn_x, v64uint8 b, int sgn_y, v32acc32 acc1, v32acc32 acc2, int zero_acc1, int shift16, int sub_mul, int sub_acc1, int sub_acc2)
v32acc32 | submac_conv_32x8_conf (v64int8 a, int sgn_x, v64uint8 b, int sgn_y, v32acc32 acc1, v32acc32 acc2, int zero_acc1, int sub_mul, int sub_acc1, int sub_acc2)
v32acc32 | submsc_conv_32x8_conf (v64int8 a, int sgn_x, v64uint8 b, int sgn_y, v32acc32 acc1, v32acc32 acc2, int zero_acc1, int sub_mul, int sub_acc1, int sub_acc2)
v32acc32 | mul_conv_32x8_conf (v64int8 a, int sgn_x, v64int8 b, int sgn_y, int sub_mul)
v32acc32 | negmul_conv_32x8_conf (v64int8 a, int sgn_x, v64int8 b, int sgn_y, int sub_mul)
v32acc32 | mac_conv_32x8_conf (v64int8 a, int sgn_x, v64int8 b, int sgn_y, v32acc32 acc1, int zero_acc1, int shift16, int sub_mul, int sub_acc1)
v32acc32 | msc_conv_32x8_conf (v64int8 a, int sgn_x, v64int8 b, int sgn_y, v32acc32 acc1, int zero_acc1, int shift16, int sub_mul, int sub_acc1)
v32acc32 | negmsc_conv_32x8_conf (v64int8 a, int sgn_x, v64int8 b, int sgn_y, v32acc32 acc1, int zero_acc1, int sub_mul, int sub_acc1)
v32acc32 | negmac_conv_32x8_conf (v64int8 a, int sgn_x, v64int8 b, int sgn_y, v32acc32 acc1, int zero_acc1, int sub_mul, int sub_acc1)
v32acc32 | addmac_conv_32x8_conf (v64int8 a, int sgn_x, v64int8 b, int sgn_y, v32acc32 acc1, v32acc32 acc2, int zero_acc1, int shift16, int sub_mul, int sub_acc1, int sub_acc2)
v32acc32 | addmsc_conv_32x8_conf (v64int8 a, int sgn_x, v64int8 b, int sgn_y, v32acc32 acc1, v32acc32 acc2, int zero_acc1, int shift16, int sub_mul, int sub_acc1, int sub_acc2)
v32acc32 | submac_conv_32x8_conf (v64int8 a, int sgn_x, v64int8 b, int sgn_y, v32acc32 acc1, v32acc32 acc2, int zero_acc1, int sub_mul, int sub_acc1, int sub_acc2)
v32acc32 | submsc_conv_32x8_conf (v64int8 a, int sgn_x, v64int8 b, int sgn_y, v32acc32 acc1, v32acc32 acc2, int zero_acc1, int sub_mul, int sub_acc1, int sub_acc2)

## Function Documentation

## ◆ addmac_4x8_8x8() [1/8]

v32acc32 addmac_4x8_8x8 | ( | v64int8 | a,
|  | int | sgn_x,
|  | v64int8 | b,
|  | int | sgn_y,
|  | v32acc32 | acc1,
|  | v32acc32 | acc2 )

Parameters

  a | Matrix A
  sgn_x | Sign mask for matrix A
  b | Matrix B
  sgn_y | Sign mask for matrix B
  acc1 | Accumulator 1 input
  acc2 | Accumulator 2 input

Returns
  Result of operation

## ◆ addmac_4x8_8x8() [2/8]

v32acc32 addmac_4x8_8x8 | ( | v64int8 | a,
|  | int | sgn_x,
|  | v64uint8 | b,
|  | int | sgn_y,
|  | v32acc32 | acc1,
|  | v32acc32 | acc2 )

Parameters

  a | Matrix A
  sgn_x | Sign mask for matrix A
  b | Matrix B
  sgn_y | Sign mask for matrix B
  acc1 | Accumulator 1 input
  acc2 | Accumulator 2 input

Returns
  Result of operation

## ◆ addmac_4x8_8x8() [3/8]

v32acc32 addmac_4x8_8x8 | ( | v64int8 | a,
|  | v64int8 | b,
|  | v32acc32 | acc1,
|  | v32acc32 | acc2 )

Parameters

  a | Matrix A
  b | Matrix B
  acc1 | Accumulator 1 input
  acc2 | Accumulator 2 input

Returns
  Result of operation

## ◆ addmac_4x8_8x8() [4/8]

v32acc32 addmac_4x8_8x8 | ( | v64int8 | a,
|  | v64uint8 | b,
|  | v32acc32 | acc1,
|  | v32acc32 | acc2 )

Parameters

  a | Matrix A
  b | Matrix B
  acc1 | Accumulator 1 input
  acc2 | Accumulator 2 input

Returns
  Result of operation

## ◆ addmac_4x8_8x8() [5/8]

v32acc32 addmac_4x8_8x8 | ( | v64uint8 | a,
|  | int | sgn_x,
|  | v64int8 | b,
|  | int | sgn_y,
|  | v32acc32 | acc1,
|  | v32acc32 | acc2 )

Parameters

  a | Matrix A
  sgn_x | Sign mask for matrix A
  b | Matrix B
  sgn_y | Sign mask for matrix B
  acc1 | Accumulator 1 input
  acc2 | Accumulator 2 input

Returns
  Result of operation

## ◆ addmac_4x8_8x8() [6/8]

v32acc32 addmac_4x8_8x8 | ( | v64uint8 | a,
|  | int | sgn_x,
|  | v64uint8 | b,
|  | int | sgn_y,
|  | v32acc32 | acc1,
|  | v32acc32 | acc2 )

Parameters

  a | Matrix A
  sgn_x | Sign mask for matrix A
  b | Matrix B
  sgn_y | Sign mask for matrix B
  acc1 | Accumulator 1 input
  acc2 | Accumulator 2 input

Returns
  Result of operation

## ◆ addmac_4x8_8x8() [7/8]

v32acc32 addmac_4x8_8x8 | ( | v64uint8 | a,
|  | v64int8 | b,
|  | v32acc32 | acc1,
|  | v32acc32 | acc2 )

Parameters

  a | Matrix A
  b | Matrix B
  acc1 | Accumulator 1 input
  acc2 | Accumulator 2 input

Returns
  Result of operation

## ◆ addmac_4x8_8x8() [8/8]

v32acc32 addmac_4x8_8x8 | ( | v64uint8 | a,
|  | v64uint8 | b,
|  | v32acc32 | acc1,
|  | v32acc32 | acc2 )

Parameters

  a | Matrix A
  b | Matrix B
  acc1 | Accumulator 1 input
  acc2 | Accumulator 2 input

Returns
  Result of operation

## ◆ addmac_4x8_8x8_conf() [1/8]

v32acc32 addmac_4x8_8x8_conf | ( | v64int8 | a,
|  | int | sgn_x,
|  | v64int8 | b,
|  | int | sgn_y,
|  | v32acc32 | acc1,
|  | v32acc32 | acc2,
|  | int | zero_acc1,
|  | int | shift16,
|  | int | sub_mul,
|  | int | sub_acc1,
|  | int | sub_acc2 )

Parameters

  a | Matrix A
  sgn_x | Sign mask for matrix A
  b | Matrix B
  sgn_y | Sign mask for matrix B
  acc1 | Accumulator 1 input
  acc2 | Accumulator 2 input
  zero_acc1 | Zeroing mask for acc1
  shift16 | Shift mask of input accumulator acc1
  sub_mul | Negation mask of multiplication result
  sub_acc1 | Negation mask of acc1
  sub_acc2 | Negation mask of acc2

Returns
  Result of operation

## ◆ addmac_4x8_8x8_conf() [2/8]

v32acc32 addmac_4x8_8x8_conf | ( | v64int8 | a,
|  | int | sgn_x,
|  | v64uint8 | b,
|  | int | sgn_y,
|  | v32acc32 | acc1,
|  | v32acc32 | acc2,
|  | int | zero_acc1,
|  | int | shift16,
|  | int | sub_mul,
|  | int | sub_acc1,
|  | int | sub_acc2 )

Parameters

  a | Matrix A
  sgn_x | Sign mask for matrix A
  b | Matrix B
  sgn_y | Sign mask for matrix B
  acc1 | Accumulator 1 input
  acc2 | Accumulator 2 input
  zero_acc1 | Zeroing mask for acc1
  shift16 | Shift mask of input accumulator acc1
  sub_mul | Negation mask of multiplication result
  sub_acc1 | Negation mask of acc1
  sub_acc2 | Negation mask of acc2

Returns
  Result of operation

## ◆ addmac_4x8_8x8_conf() [3/8]

v32acc32 addmac_4x8_8x8_conf | ( | v64int8 | a,
|  | v64int8 | b,
|  | v32acc32 | acc1,
|  | v32acc32 | acc2,
|  | int | zero_acc1,
|  | int | shift16,
|  | int | sub_mul,
|  | int | sub_acc1,
|  | int | sub_acc2 )

Parameters

  a | Matrix A
  b | Matrix B
  acc1 | Accumulator 1 input
  acc2 | Accumulator 2 input
  zero_acc1 | Zeroing mask for acc1
  shift16 | Shift mask of input accumulator acc1
  sub_mul | Negation mask of multiplication result
  sub_acc1 | Negation mask of acc1
  sub_acc2 | Negation mask of acc2

Returns
  Result of operation

## ◆ addmac_4x8_8x8_conf() [4/8]

v32acc32 addmac_4x8_8x8_conf | ( | v64int8 | a,
|  | v64uint8 | b,
|  | v32acc32 | acc1,
|  | v32acc32 | acc2,
|  | int | zero_acc1,
|  | int | shift16,
|  | int | sub_mul,
|  | int | sub_acc1,
|  | int | sub_acc2 )

Parameters

  a | Matrix A
  b | Matrix B
  acc1 | Accumulator 1 input
  acc2 | Accumulator 2 input
  zero_acc1 | Zeroing mask for acc1
  shift16 | Shift mask of input accumulator acc1
  sub_mul | Negation mask of multiplication result
  sub_acc1 | Negation mask of acc1
  sub_acc2 | Negation mask of acc2

Returns
  Result of operation

## ◆ addmac_4x8_8x8_conf() [5/8]

v32acc32 addmac_4x8_8x8_conf | ( | v64uint8 | a,
|  | int | sgn_x,
|  | v64int8 | b,
|  | int | sgn_y,
|  | v32acc32 | acc1,
|  | v32acc32 | acc2,
|  | int | zero_acc1,
|  | int | shift16,
|  | int | sub_mul,
|  | int | sub_acc1,
|  | int | sub_acc2 )

Parameters

  a | Matrix A
  sgn_x | Sign mask for matrix A
  b | Matrix B
  sgn_y | Sign mask for matrix B
  acc1 | Accumulator 1 input
  acc2 | Accumulator 2 input
  zero_acc1 | Zeroing mask for acc1
  shift16 | Shift mask of input accumulator acc1
  sub_mul | Negation mask of multiplication result
  sub_acc1 | Negation mask of acc1
  sub_acc2 | Negation mask of acc2

Returns
  Result of operation

## ◆ addmac_4x8_8x8_conf() [6/8]

v32acc32 addmac_4x8_8x8_conf | ( | v64uint8 | a,
|  | int | sgn_x,
|  | v64uint8 | b,
|  | int | sgn_y,
|  | v32acc32 | acc1,
|  | v32acc32 | acc2,
|  | int | zero_acc1,
|  | int | shift16,
|  | int | sub_mul,
|  | int | sub_acc1,
|  | int | sub_acc2 )

Parameters

  a | Matrix A
  sgn_x | Sign mask for matrix A
  b | Matrix B
  sgn_y | Sign mask for matrix B
  acc1 | Accumulator 1 input
  acc2 | Accumulator 2 input
  zero_acc1 | Zeroing mask for acc1
  shift16 | Shift mask of input accumulator acc1
  sub_mul | Negation mask of multiplication result
  sub_acc1 | Negation mask of acc1
  sub_acc2 | Negation mask of acc2

Returns
  Result of operation

## ◆ addmac_4x8_8x8_conf() [7/8]

v32acc32 addmac_4x8_8x8_conf | ( | v64uint8 | a,
|  | v64int8 | b,
|  | v32acc32 | acc1,
|  | v32acc32 | acc2,
|  | int | zero_acc1,
|  | int | shift16,
|  | int | sub_mul,
|  | int | sub_acc1,
|  | int | sub_acc2 )

Parameters

  a | Matrix A
  b | Matrix B
  acc1 | Accumulator 1 input
  acc2 | Accumulator 2 input
  zero_acc1 | Zeroing mask for acc1
  shift16 | Shift mask of input accumulator acc1
  sub_mul | Negation mask of multiplication result
  sub_acc1 | Negation mask of acc1
  sub_acc2 | Negation mask of acc2

Returns
  Result of operation

## ◆ addmac_4x8_8x8_conf() [8/8]

v32acc32 addmac_4x8_8x8_conf | ( | v64uint8 | a,
|  | v64uint8 | b,
|  | v32acc32 | acc1,
|  | v32acc32 | acc2,
|  | int | zero_acc1,
|  | int | shift16,
|  | int | sub_mul,
|  | int | sub_acc1,
|  | int | sub_acc2 )

Parameters

  a | Matrix A
  b | Matrix B
  acc1 | Accumulator 1 input
  acc2 | Accumulator 2 input
  zero_acc1 | Zeroing mask for acc1
  shift16 | Shift mask of input accumulator acc1
  sub_mul | Negation mask of multiplication result
  sub_acc1 | Negation mask of acc1
  sub_acc2 | Negation mask of acc2

Returns
  Result of operation

## ◆ addmac_conv_32x8() [1/8]

v32acc32 addmac_conv_32x8 | ( | v64int8 | a,
|  | int | sgn_x,
|  | v64int8 | b,
|  | int | sgn_y,
|  | v32acc32 | acc1,
|  | v32acc32 | acc2 )

Parameters

  a | Matrix A
  sgn_x | Sign mask for matrix A
  b | Matrix B
  sgn_y | Sign mask for matrix B
  acc1 | Accumulator 1 input
  acc2 | Accumulator 2 input

Returns
  Result of operation

## ◆ addmac_conv_32x8() [2/8]

v32acc32 addmac_conv_32x8 | ( | v64int8 | a,
|  | int | sgn_x,
|  | v64uint8 | b,
|  | int | sgn_y,
|  | v32acc32 | acc1,
|  | v32acc32 | acc2 )

Parameters

  a | Matrix A
  sgn_x | Sign mask for matrix A
  b | Matrix B
  sgn_y | Sign mask for matrix B
  acc1 | Accumulator 1 input
  acc2 | Accumulator 2 input

Returns
  Result of operation

## ◆ addmac_conv_32x8() [3/8]

v32acc32 addmac_conv_32x8 | ( | v64int8 | a,
|  | v64int8 | b,
|  | v32acc32 | acc1,
|  | v32acc32 | acc2 )

Parameters

  a | Matrix A
  b | Matrix B
  acc1 | Accumulator 1 input
  acc2 | Accumulator 2 input

Returns
  Result of operation

## ◆ addmac_conv_32x8() [4/8]

v32acc32 addmac_conv_32x8 | ( | v64int8 | a,
|  | v64uint8 | b,
|  | v32acc32 | acc1,
|  | v32acc32 | acc2 )

Parameters

  a | Matrix A
  b | Matrix B
  acc1 | Accumulator 1 input
  acc2 | Accumulator 2 input

Returns
  Result of operation

## ◆ addmac_conv_32x8() [5/8]

v32acc32 addmac_conv_32x8 | ( | v64uint8 | a,
|  | int | sgn_x,
|  | v64int8 | b,
|  | int | sgn_y,
|  | v32acc32 | acc1,
|  | v32acc32 | acc2 )

Parameters

  a | Matrix A
  sgn_x | Sign mask for matrix A
  b | Matrix B
  sgn_y | Sign mask for matrix B
  acc1 | Accumulator 1 input
  acc2 | Accumulator 2 input

Returns
  Result of operation

## ◆ addmac_conv_32x8() [6/8]

v32acc32 addmac_conv_32x8 | ( | v64uint8 | a,
|  | int | sgn_x,
|  | v64uint8 | b,
|  | int | sgn_y,
|  | v32acc32 | acc1,
|  | v32acc32 | acc2 )

Parameters

  a | Matrix A
  sgn_x | Sign mask for matrix A
  b | Matrix B
  sgn_y | Sign mask for matrix B
  acc1 | Accumulator 1 input
  acc2 | Accumulator 2 input

Returns
  Result of operation

## ◆ addmac_conv_32x8() [7/8]

v32acc32 addmac_conv_32x8 | ( | v64uint8 | a,
|  | v64int8 | b,
|  | v32acc32 | acc1,
|  | v32acc32 | acc2 )

Parameters

  a | Matrix A
  b | Matrix B
  acc1 | Accumulator 1 input
  acc2 | Accumulator 2 input

Returns
  Result of operation

## ◆ addmac_conv_32x8() [8/8]

v32acc32 addmac_conv_32x8 | ( | v64uint8 | a,
|  | v64uint8 | b,
|  | v32acc32 | acc1,
|  | v32acc32 | acc2 )

Parameters

  a | Matrix A
  b | Matrix B
  acc1 | Accumulator 1 input
  acc2 | Accumulator 2 input

Returns
  Result of operation

## ◆ addmac_conv_32x8_conf() [1/8]

v32acc32 addmac_conv_32x8_conf | ( | v64int8 | a,
|  | int | sgn_x,
|  | v64int8 | b,
|  | int | sgn_y,
|  | v32acc32 | acc1,
|  | v32acc32 | acc2,
|  | int | zero_acc1,
|  | int | shift16,
|  | int | sub_mul,
|  | int | sub_acc1,
|  | int | sub_acc2 )

Parameters

  a | Matrix A
  sgn_x | Sign mask for matrix A
  b | Matrix B
  sgn_y | Sign mask for matrix B
  acc1 | Accumulator 1 input
  acc2 | Accumulator 2 input
  zero_acc1 | Zeroing mask for acc1
  shift16 | Shift mask of input accumulator acc1
  sub_mul | Negation mask of multiplication result
  sub_acc1 | Negation mask of acc1
  sub_acc2 | Negation mask of acc2

Returns
  Result of operation

## ◆ addmac_conv_32x8_conf() [2/8]

v32acc32 addmac_conv_32x8_conf | ( | v64int8 | a,
|  | int | sgn_x,
|  | v64uint8 | b,
|  | int | sgn_y,
|  | v32acc32 | acc1,
|  | v32acc32 | acc2,
|  | int | zero_acc1,
|  | int | shift16,
|  | int | sub_mul,
|  | int | sub_acc1,
|  | int | sub_acc2 )

Parameters

  a | Matrix A
  sgn_x | Sign mask for matrix A
  b | Matrix B
  sgn_y | Sign mask for matrix B
  acc1 | Accumulator 1 input
  acc2 | Accumulator 2 input
  zero_acc1 | Zeroing mask for acc1
  shift16 | Shift mask of input accumulator acc1
  sub_mul | Negation mask of multiplication result
  sub_acc1 | Negation mask of acc1
  sub_acc2 | Negation mask of acc2

Returns
  Result of operation

## ◆ addmac_conv_32x8_conf() [3/8]

v32acc32 addmac_conv_32x8_conf | ( | v64int8 | a,
|  | v64int8 | b,
|  | v32acc32 | acc1,
|  | v32acc32 | acc2,
|  | int | zero_acc1,
|  | int | shift16,
|  | int | sub_mul,
|  | int | sub_acc1,
|  | int | sub_acc2 )

Parameters

  a | Matrix A
  b | Matrix B
  acc1 | Accumulator 1 input
  acc2 | Accumulator 2 input
  zero_acc1 | Zeroing mask for acc1
  shift16 | Shift mask of input accumulator acc1
  sub_mul | Negation mask of multiplication result
  sub_acc1 | Negation mask of acc1
  sub_acc2 | Negation mask of acc2

Returns
  Result of operation

## ◆ addmac_conv_32x8_conf() [4/8]

v32acc32 addmac_conv_32x8_conf | ( | v64int8 | a,
|  | v64uint8 | b,
|  | v32acc32 | acc1,
|  | v32acc32 | acc2,
|  | int | zero_acc1,
|  | int | shift16,
|  | int | sub_mul,
|  | int | sub_acc1,
|  | int | sub_acc2 )

Parameters

  a | Matrix A
  b | Matrix B
  acc1 | Accumulator 1 input
  acc2 | Accumulator 2 input
  zero_acc1 | Zeroing mask for acc1
  shift16 | Shift mask of input accumulator acc1
  sub_mul | Negation mask of multiplication result
  sub_acc1 | Negation mask of acc1
  sub_acc2 | Negation mask of acc2

Returns
  Result of operation

## ◆ addmac_conv_32x8_conf() [5/8]

v32acc32 addmac_conv_32x8_conf | ( | v64uint8 | a,
|  | int | sgn_x,
|  | v64int8 | b,
|  | int | sgn_y,
|  | v32acc32 | acc1,
|  | v32acc32 | acc2,
|  | int | zero_acc1,
|  | int | shift16,
|  | int | sub_mul,
|  | int | sub_acc1,
|  | int | sub_acc2 )

Parameters

  a | Matrix A
  sgn_x | Sign mask for matrix A
  b | Matrix B
  sgn_y | Sign mask for matrix B
  acc1 | Accumulator 1 input
  acc2 | Accumulator 2 input
  zero_acc1 | Zeroing mask for acc1
  shift16 | Shift mask of input accumulator acc1
  sub_mul | Negation mask of multiplication result
  sub_acc1 | Negation mask of acc1
  sub_acc2 | Negation mask of acc2

Returns
  Result of operation

## ◆ addmac_conv_32x8_conf() [6/8]

v32acc32 addmac_conv_32x8_conf | ( | v64uint8 | a,
|  | int | sgn_x,
|  | v64uint8 | b,
|  | int | sgn_y,
|  | v32acc32 | acc1,
|  | v32acc32 | acc2,
|  | int | zero_acc1,
|  | int | shift16,
|  | int | sub_mul,
|  | int | sub_acc1,
|  | int | sub_acc2 )

Parameters

  a | Matrix A
  sgn_x | Sign mask for matrix A
  b | Matrix B
  sgn_y | Sign mask for matrix B
  acc1 | Accumulator 1 input
  acc2 | Accumulator 2 input
  zero_acc1 | Zeroing mask for acc1
  shift16 | Shift mask of input accumulator acc1
  sub_mul | Negation mask of multiplication result
  sub_acc1 | Negation mask of acc1
  sub_acc2 | Negation mask of acc2

Returns
  Result of operation

## ◆ addmac_conv_32x8_conf() [7/8]

v32acc32 addmac_conv_32x8_conf | ( | v64uint8 | a,
|  | v64int8 | b,
|  | v32acc32 | acc1,
|  | v32acc32 | acc2,
|  | int | zero_acc1,
|  | int | shift16,
|  | int | sub_mul,
|  | int | sub_acc1,
|  | int | sub_acc2 )

Parameters

  a | Matrix A
  b | Matrix B
  acc1 | Accumulator 1 input
  acc2 | Accumulator 2 input
  zero_acc1 | Zeroing mask for acc1
  shift16 | Shift mask of input accumulator acc1
  sub_mul | Negation mask of multiplication result
  sub_acc1 | Negation mask of acc1
  sub_acc2 | Negation mask of acc2

Returns
  Result of operation

## ◆ addmac_conv_32x8_conf() [8/8]

v32acc32 addmac_conv_32x8_conf | ( | v64uint8 | a,
|  | v64uint8 | b,
|  | v32acc32 | acc1,
|  | v32acc32 | acc2,
|  | int | zero_acc1,
|  | int | shift16,
|  | int | sub_mul,
|  | int | sub_acc1,
|  | int | sub_acc2 )

Parameters

  a | Matrix A
  b | Matrix B
  acc1 | Accumulator 1 input
  acc2 | Accumulator 2 input
  zero_acc1 | Zeroing mask for acc1
  shift16 | Shift mask of input accumulator acc1
  sub_mul | Negation mask of multiplication result
  sub_acc1 | Negation mask of acc1
  sub_acc2 | Negation mask of acc2

Returns
  Result of operation

## ◆ addmac_conv_4x4_8ch() [1/8]

v32acc32 addmac_conv_4x4_8ch | ( | v64int8 | a,
|  | int | sgn_x,
|  | v64int8 | b,
|  | int | sgn_y,
|  | v32acc32 | acc1,
|  | v32acc32 | acc2 )

Parameters

  a | Matrix A
  sgn_x | Sign mask for matrix A
  b | Matrix B
  sgn_y | Sign mask for matrix B
  acc1 | Accumulator 1 input
  acc2 | Accumulator 2 input

Returns
  Result of operation

## ◆ addmac_conv_4x4_8ch() [2/8]

v32acc32 addmac_conv_4x4_8ch | ( | v64int8 | a,
|  | int | sgn_x,
|  | v64uint8 | b,
|  | int | sgn_y,
|  | v32acc32 | acc1,
|  | v32acc32 | acc2 )

Parameters

  a | Matrix A
  sgn_x | Sign mask for matrix A
  b | Matrix B
  sgn_y | Sign mask for matrix B
  acc1 | Accumulator 1 input
  acc2 | Accumulator 2 input

Returns
  Result of operation

## ◆ addmac_conv_4x4_8ch() [3/8]

v32acc32 addmac_conv_4x4_8ch | ( | v64int8 | a,
|  | v64int8 | b,
|  | v32acc32 | acc1,
|  | v32acc32 | acc2 )

Parameters

  a | Matrix A
  b | Matrix B
  acc1 | Accumulator 1 input
  acc2 | Accumulator 2 input

Returns
  Result of operation

## ◆ addmac_conv_4x4_8ch() [4/8]

v32acc32 addmac_conv_4x4_8ch | ( | v64int8 | a,
|  | v64uint8 | b,
|  | v32acc32 | acc1,
|  | v32acc32 | acc2 )

Parameters

  a | Matrix A
  b | Matrix B
  acc1 | Accumulator 1 input
  acc2 | Accumulator 2 input

Returns
  Result of operation

## ◆ addmac_conv_4x4_8ch() [5/8]

v32acc32 addmac_conv_4x4_8ch | ( | v64uint8 | a,
|  | int | sgn_x,
|  | v64int8 | b,
|  | int | sgn_y,
|  | v32acc32 | acc1,
|  | v32acc32 | acc2 )

Parameters

  a | Matrix A
  sgn_x | Sign mask for matrix A
  b | Matrix B
  sgn_y | Sign mask for matrix B
  acc1 | Accumulator 1 input
  acc2 | Accumulator 2 input

Returns
  Result of operation

## ◆ addmac_conv_4x4_8ch() [6/8]

v32acc32 addmac_conv_4x4_8ch | ( | v64uint8 | a,
|  | int | sgn_x,
|  | v64uint8 | b,
|  | int | sgn_y,
|  | v32acc32 | acc1,
|  | v32acc32 | acc2 )

Parameters

  a | Matrix A
  sgn_x | Sign mask for matrix A
  b | Matrix B
  sgn_y | Sign mask for matrix B
  acc1 | Accumulator 1 input
  acc2 | Accumulator 2 input

Returns
  Result of operation

## ◆ addmac_conv_4x4_8ch() [7/8]

v32acc32 addmac_conv_4x4_8ch | ( | v64uint8 | a,
|  | v64int8 | b,
|  | v32acc32 | acc1,
|  | v32acc32 | acc2 )

Parameters

  a | Matrix A
  b | Matrix B
  acc1 | Accumulator 1 input
  acc2 | Accumulator 2 input

Returns
  Result of operation

## ◆ addmac_conv_4x4_8ch() [8/8]

v32acc32 addmac_conv_4x4_8ch | ( | v64uint8 | a,
|  | v64uint8 | b,
|  | v32acc32 | acc1,
|  | v32acc32 | acc2 )

Parameters

  a | Matrix A
  b | Matrix B
  acc1 | Accumulator 1 input
  acc2 | Accumulator 2 input

Returns
  Result of operation

## ◆ addmac_conv_4x4_8ch_conf() [1/8]

v32acc32 addmac_conv_4x4_8ch_conf | ( | v64int8 | a,
|  | int | sgn_x,
|  | v64int8 | b,
|  | int | sgn_y,
|  | v32acc32 | acc1,
|  | v32acc32 | acc2,
|  | int | zero_acc1,
|  | int | shift16,
|  | int | sub_mul,
|  | int | sub_acc1,
|  | int | sub_acc2 )

Parameters

  a | Matrix A
  sgn_x | Sign mask for matrix A
  b | Matrix B
  sgn_y | Sign mask for matrix B
  acc1 | Accumulator 1 input
  acc2 | Accumulator 2 input
  zero_acc1 | Zeroing mask for acc1
  shift16 | Shift mask of input accumulator acc1
  sub_mul | Negation mask of multiplication result
  sub_acc1 | Negation mask of acc1
  sub_acc2 | Negation mask of acc2

Returns
  Result of operation

## ◆ addmac_conv_4x4_8ch_conf() [2/8]

v32acc32 addmac_conv_4x4_8ch_conf | ( | v64int8 | a,
|  | int | sgn_x,
|  | v64uint8 | b,
|  | int | sgn_y,
|  | v32acc32 | acc1,
|  | v32acc32 | acc2,
|  | int | zero_acc1,
|  | int | shift16,
|  | int | sub_mul,
|  | int | sub_acc1,
|  | int | sub_acc2 )

Parameters

  a | Matrix A
  sgn_x | Sign mask for matrix A
  b | Matrix B
  sgn_y | Sign mask for matrix B
  acc1 | Accumulator 1 input
  acc2 | Accumulator 2 input
  zero_acc1 | Zeroing mask for acc1
  shift16 | Shift mask of input accumulator acc1
  sub_mul | Negation mask of multiplication result
  sub_acc1 | Negation mask of acc1
  sub_acc2 | Negation mask of acc2

Returns
  Result of operation

## ◆ addmac_conv_4x4_8ch_conf() [3/8]

v32acc32 addmac_conv_4x4_8ch_conf | ( | v64int8 | a,
|  | v64int8 | b,
|  | v32acc32 | acc1,
|  | v32acc32 | acc2,
|  | int | zero_acc1,
|  | int | shift16,
|  | int | sub_mul,
|  | int | sub_acc1,
|  | int | sub_acc2 )

Parameters

  a | Matrix A
  b | Matrix B
  acc1 | Accumulator 1 input
  acc2 | Accumulator 2 input
  zero_acc1 | Zeroing mask for acc1
  shift16 | Shift mask of input accumulator acc1
  sub_mul | Negation mask of multiplication result
  sub_acc1 | Negation mask of acc1
  sub_acc2 | Negation mask of acc2

Returns
  Result of operation

## ◆ addmac_conv_4x4_8ch_conf() [4/8]

v32acc32 addmac_conv_4x4_8ch_conf | ( | v64int8 | a,
|  | v64uint8 | b,
|  | v32acc32 | acc1,
|  | v32acc32 | acc2,
|  | int | zero_acc1,
|  | int | shift16,
|  | int | sub_mul,
|  | int | sub_acc1,
|  | int | sub_acc2 )

Parameters

  a | Matrix A
  b | Matrix B
  acc1 | Accumulator 1 input
  acc2 | Accumulator 2 input
  zero_acc1 | Zeroing mask for acc1
  shift16 | Shift mask of input accumulator acc1
  sub_mul | Negation mask of multiplication result
  sub_acc1 | Negation mask of acc1
  sub_acc2 | Negation mask of acc2

Returns
  Result of operation

## ◆ addmac_conv_4x4_8ch_conf() [5/8]

v32acc32 addmac_conv_4x4_8ch_conf | ( | v64uint8 | a,
|  | int | sgn_x,
|  | v64int8 | b,
|  | int | sgn_y,
|  | v32acc32 | acc1,
|  | v32acc32 | acc2,
|  | int | zero_acc1,
|  | int | shift16,
|  | int | sub_mul,
|  | int | sub_acc1,
|  | int | sub_acc2 )

Parameters

  a | Matrix A
  sgn_x | Sign mask for matrix A
  b | Matrix B
  sgn_y | Sign mask for matrix B
  acc1 | Accumulator 1 input
  acc2 | Accumulator 2 input
  zero_acc1 | Zeroing mask for acc1
  shift16 | Shift mask of input accumulator acc1
  sub_mul | Negation mask of multiplication result
  sub_acc1 | Negation mask of acc1
  sub_acc2 | Negation mask of acc2

Returns
  Result of operation

## ◆ addmac_conv_4x4_8ch_conf() [6/8]

v32acc32 addmac_conv_4x4_8ch_conf | ( | v64uint8 | a,
|  | int | sgn_x,
|  | v64uint8 | b,
|  | int | sgn_y,
|  | v32acc32 | acc1,
|  | v32acc32 | acc2,
|  | int | zero_acc1,
|  | int | shift16,
|  | int | sub_mul,
|  | int | sub_acc1,
|  | int | sub_acc2 )

Parameters

  a | Matrix A
  sgn_x | Sign mask for matrix A
  b | Matrix B
  sgn_y | Sign mask for matrix B
  acc1 | Accumulator 1 input
  acc2 | Accumulator 2 input
  zero_acc1 | Zeroing mask for acc1
  shift16 | Shift mask of input accumulator acc1
  sub_mul | Negation mask of multiplication result
  sub_acc1 | Negation mask of acc1
  sub_acc2 | Negation mask of acc2

Returns
  Result of operation

## ◆ addmac_conv_4x4_8ch_conf() [7/8]

v32acc32 addmac_conv_4x4_8ch_conf | ( | v64uint8 | a,
|  | v64int8 | b,
|  | v32acc32 | acc1,
|  | v32acc32 | acc2,
|  | int | zero_acc1,
|  | int | shift16,
|  | int | sub_mul,
|  | int | sub_acc1,
|  | int | sub_acc2 )

Parameters

  a | Matrix A
  b | Matrix B
  acc1 | Accumulator 1 input
  acc2 | Accumulator 2 input
  zero_acc1 | Zeroing mask for acc1
  shift16 | Shift mask of input accumulator acc1
  sub_mul | Negation mask of multiplication result
  sub_acc1 | Negation mask of acc1
  sub_acc2 | Negation mask of acc2

Returns
  Result of operation

## ◆ addmac_conv_4x4_8ch_conf() [8/8]

v32acc32 addmac_conv_4x4_8ch_conf | ( | v64uint8 | a,
|  | v64uint8 | b,
|  | v32acc32 | acc1,
|  | v32acc32 | acc2,
|  | int | zero_acc1,
|  | int | shift16,
|  | int | sub_mul,
|  | int | sub_acc1,
|  | int | sub_acc2 )

Parameters

  a | Matrix A
  b | Matrix B
  acc1 | Accumulator 1 input
  acc2 | Accumulator 2 input
  zero_acc1 | Zeroing mask for acc1
  shift16 | Shift mask of input accumulator acc1
  sub_mul | Negation mask of multiplication result
  sub_acc1 | Negation mask of acc1
  sub_acc2 | Negation mask of acc2

Returns
  Result of operation

## ◆ addmac_conv_8x8_4ch() [1/8]

v32acc32 addmac_conv_8x8_4ch | ( | v64int8 | a,
|  | int | sgn_x,
|  | v64int8 | b,
|  | int | sgn_y,
|  | v32acc32 | acc1,
|  | v32acc32 | acc2 )

Parameters

  a | Matrix A
  sgn_x | Sign mask for matrix A
  b | Matrix B
  sgn_y | Sign mask for matrix B
  acc1 | Accumulator 1 input
  acc2 | Accumulator 2 input

Returns
  Result of operation

## ◆ addmac_conv_8x8_4ch() [2/8]

v32acc32 addmac_conv_8x8_4ch | ( | v64int8 | a,
|  | int | sgn_x,
|  | v64uint8 | b,
|  | int | sgn_y,
|  | v32acc32 | acc1,
|  | v32acc32 | acc2 )

Parameters

  a | Matrix A
  sgn_x | Sign mask for matrix A
  b | Matrix B
  sgn_y | Sign mask for matrix B
  acc1 | Accumulator 1 input
  acc2 | Accumulator 2 input

Returns
  Result of operation

## ◆ addmac_conv_8x8_4ch() [3/8]

v32acc32 addmac_conv_8x8_4ch | ( | v64int8 | a,
|  | v64int8 | b,
|  | v32acc32 | acc1,
|  | v32acc32 | acc2 )

Parameters

  a | Matrix A
  b | Matrix B
  acc1 | Accumulator 1 input
  acc2 | Accumulator 2 input

Returns
  Result of operation

## ◆ addmac_conv_8x8_4ch() [4/8]

v32acc32 addmac_conv_8x8_4ch | ( | v64int8 | a,
|  | v64uint8 | b,
|  | v32acc32 | acc1,
|  | v32acc32 | acc2 )

Parameters

  a | Matrix A
  b | Matrix B
  acc1 | Accumulator 1 input
  acc2 | Accumulator 2 input

Returns
  Result of operation

## ◆ addmac_conv_8x8_4ch() [5/8]

v32acc32 addmac_conv_8x8_4ch | ( | v64uint8 | a,
|  | int | sgn_x,
|  | v64int8 | b,
|  | int | sgn_y,
|  | v32acc32 | acc1,
|  | v32acc32 | acc2 )

Parameters

  a | Matrix A
  sgn_x | Sign mask for matrix A
  b | Matrix B
  sgn_y | Sign mask for matrix B
  acc1 | Accumulator 1 input
  acc2 | Accumulator 2 input

Returns
  Result of operation

## ◆ addmac_conv_8x8_4ch() [6/8]

v32acc32 addmac_conv_8x8_4ch | ( | v64uint8 | a,
|  | int | sgn_x,
|  | v64uint8 | b,
|  | int | sgn_y,
|  | v32acc32 | acc1,
|  | v32acc32 | acc2 )

Parameters

  a | Matrix A
  sgn_x | Sign mask for matrix A
  b | Matrix B
  sgn_y | Sign mask for matrix B
  acc1 | Accumulator 1 input
  acc2 | Accumulator 2 input

Returns
  Result of operation

## ◆ addmac_conv_8x8_4ch() [7/8]

v32acc32 addmac_conv_8x8_4ch | ( | v64uint8 | a,
|  | v64int8 | b,
|  | v32acc32 | acc1,
|  | v32acc32 | acc2 )

Parameters

  a | Matrix A
  b | Matrix B
  acc1 | Accumulator 1 input
  acc2 | Accumulator 2 input

Returns
  Result of operation

## ◆ addmac_conv_8x8_4ch() [8/8]

v32acc32 addmac_conv_8x8_4ch | ( | v64uint8 | a,
|  | v64uint8 | b,
|  | v32acc32 | acc1,
|  | v32acc32 | acc2 )

Parameters

  a | Matrix A
  b | Matrix B
  acc1 | Accumulator 1 input
  acc2 | Accumulator 2 input

Returns
  Result of operation

## ◆ addmac_conv_8x8_4ch_conf() [1/8]

v32acc32 addmac_conv_8x8_4ch_conf | ( | v64int8 | a,
|  | int | sgn_x,
|  | v64int8 | b,
|  | int | sgn_y,
|  | v32acc32 | acc1,
|  | v32acc32 | acc2,
|  | int | zero_acc1,
|  | int | shift16,
|  | int | sub_mul,
|  | int | sub_acc1,
|  | int | sub_acc2 )

Parameters

  a | Matrix A
  sgn_x | Sign mask for matrix A
  b | Matrix B
  sgn_y | Sign mask for matrix B
  acc1 | Accumulator 1 input
  acc2 | Accumulator 2 input
  zero_acc1 | Zeroing mask for acc1
  shift16 | Shift mask of input accumulator acc1
  sub_mul | Negation mask of multiplication result
  sub_acc1 | Negation mask of acc1
  sub_acc2 | Negation mask of acc2

Returns
  Result of operation

## ◆ addmac_conv_8x8_4ch_conf() [2/8]

v32acc32 addmac_conv_8x8_4ch_conf | ( | v64int8 | a,
|  | int | sgn_x,
|  | v64uint8 | b,
|  | int | sgn_y,
|  | v32acc32 | acc1,
|  | v32acc32 | acc2,
|  | int | zero_acc1,
|  | int | shift16,
|  | int | sub_mul,
|  | int | sub_acc1,
|  | int | sub_acc2 )

Parameters

  a | Matrix A
  sgn_x | Sign mask for matrix A
  b | Matrix B
  sgn_y | Sign mask for matrix B
  acc1 | Accumulator 1 input
  acc2 | Accumulator 2 input
  zero_acc1 | Zeroing mask for acc1
  shift16 | Shift mask of input accumulator acc1
  sub_mul | Negation mask of multiplication result
  sub_acc1 | Negation mask of acc1
  sub_acc2 | Negation mask of acc2

Returns
  Result of operation

## ◆ addmac_conv_8x8_4ch_conf() [3/8]

v32acc32 addmac_conv_8x8_4ch_conf | ( | v64int8 | a,
|  | v64int8 | b,
|  | v32acc32 | acc1,
|  | v32acc32 | acc2,
|  | int | zero_acc1,
|  | int | shift16,
|  | int | sub_mul,
|  | int | sub_acc1,
|  | int | sub_acc2 )

Parameters

  a | Matrix A
  b | Matrix B
  acc1 | Accumulator 1 input
  acc2 | Accumulator 2 input
  zero_acc1 | Zeroing mask for acc1
  shift16 | Shift mask of input accumulator acc1
  sub_mul | Negation mask of multiplication result
  sub_acc1 | Negation mask of acc1
  sub_acc2 | Negation mask of acc2

Returns
  Result of operation

## ◆ addmac_conv_8x8_4ch_conf() [4/8]

v32acc32 addmac_conv_8x8_4ch_conf | ( | v64int8 | a,
|  | v64uint8 | b,
|  | v32acc32 | acc1,
|  | v32acc32 | acc2,
|  | int | zero_acc1,
|  | int | shift16,
|  | int | sub_mul,
|  | int | sub_acc1,
|  | int | sub_acc2 )

Parameters

  a | Matrix A
  b | Matrix B
  acc1 | Accumulator 1 input
  acc2 | Accumulator 2 input
  zero_acc1 | Zeroing mask for acc1
  shift16 | Shift mask of input accumulator acc1
  sub_mul | Negation mask of multiplication result
  sub_acc1 | Negation mask of acc1
  sub_acc2 | Negation mask of acc2

Returns
  Result of operation

## ◆ addmac_conv_8x8_4ch_conf() [5/8]

v32acc32 addmac_conv_8x8_4ch_conf | ( | v64uint8 | a,
|  | int | sgn_x,
|  | v64int8 | b,
|  | int | sgn_y,
|  | v32acc32 | acc1,
|  | v32acc32 | acc2,
|  | int | zero_acc1,
|  | int | shift16,
|  | int | sub_mul,
|  | int | sub_acc1,
|  | int | sub_acc2 )

Parameters

  a | Matrix A
  sgn_x | Sign mask for matrix A
  b | Matrix B
  sgn_y | Sign mask for matrix B
  acc1 | Accumulator 1 input
  acc2 | Accumulator 2 input
  zero_acc1 | Zeroing mask for acc1
  shift16 | Shift mask of input accumulator acc1
  sub_mul | Negation mask of multiplication result
  sub_acc1 | Negation mask of acc1
  sub_acc2 | Negation mask of acc2

Returns
  Result of operation

## ◆ addmac_conv_8x8_4ch_conf() [6/8]

v32acc32 addmac_conv_8x8_4ch_conf | ( | v64uint8 | a,
|  | int | sgn_x,
|  | v64uint8 | b,
|  | int | sgn_y,
|  | v32acc32 | acc1,
|  | v32acc32 | acc2,
|  | int | zero_acc1,
|  | int | shift16,
|  | int | sub_mul,
|  | int | sub_acc1,
|  | int | sub_acc2 )

Parameters

  a | Matrix A
  sgn_x | Sign mask for matrix A
  b | Matrix B
  sgn_y | Sign mask for matrix B
  acc1 | Accumulator 1 input
  acc2 | Accumulator 2 input
  zero_acc1 | Zeroing mask for acc1
  shift16 | Shift mask of input accumulator acc1
  sub_mul | Negation mask of multiplication result
  sub_acc1 | Negation mask of acc1
  sub_acc2 | Negation mask of acc2

Returns
  Result of operation

## ◆ addmac_conv_8x8_4ch_conf() [7/8]

v32acc32 addmac_conv_8x8_4ch_conf | ( | v64uint8 | a,
|  | v64int8 | b,
|  | v32acc32 | acc1,
|  | v32acc32 | acc2,
|  | int | zero_acc1,
|  | int | shift16,
|  | int | sub_mul,
|  | int | sub_acc1,
|  | int | sub_acc2 )

Parameters

  a | Matrix A
  b | Matrix B
  acc1 | Accumulator 1 input
  acc2 | Accumulator 2 input
  zero_acc1 | Zeroing mask for acc1
  shift16 | Shift mask of input accumulator acc1
  sub_mul | Negation mask of multiplication result
  sub_acc1 | Negation mask of acc1
  sub_acc2 | Negation mask of acc2

Returns
  Result of operation

## ◆ addmac_conv_8x8_4ch_conf() [8/8]

v32acc32 addmac_conv_8x8_4ch_conf | ( | v64uint8 | a,
|  | v64uint8 | b,
|  | v32acc32 | acc1,
|  | v32acc32 | acc2,
|  | int | zero_acc1,
|  | int | shift16,
|  | int | sub_mul,
|  | int | sub_acc1,
|  | int | sub_acc2 )

Parameters

  a | Matrix A
  b | Matrix B
  acc1 | Accumulator 1 input
  acc2 | Accumulator 2 input
  zero_acc1 | Zeroing mask for acc1
  shift16 | Shift mask of input accumulator acc1
  sub_mul | Negation mask of multiplication result
  sub_acc1 | Negation mask of acc1
  sub_acc2 | Negation mask of acc2

Returns
  Result of operation

## ◆ addmac_elem_32_2() [1/8]

v32acc32 addmac_elem_32_2 | ( | v64int8 | a,
|  | int | sgn_x,
|  | v64int8 | b,
|  | int | sgn_y,
|  | v32acc32 | acc1,
|  | v32acc32 | acc2 )

Parameters

  a | Matrix A
  sgn_x | Sign mask for matrix A
  b | Matrix B
  sgn_y | Sign mask for matrix B
  acc1 | Accumulator 1 input
  acc2 | Accumulator 2 input

Returns
  Result of operation

## ◆ addmac_elem_32_2() [2/8]

v32acc32 addmac_elem_32_2 | ( | v64int8 | a,
|  | int | sgn_x,
|  | v64uint8 | b,
|  | int | sgn_y,
|  | v32acc32 | acc1,
|  | v32acc32 | acc2 )

Parameters

  a | Matrix A
  sgn_x | Sign mask for matrix A
  b | Matrix B
  sgn_y | Sign mask for matrix B
  acc1 | Accumulator 1 input
  acc2 | Accumulator 2 input

Returns
  Result of operation

## ◆ addmac_elem_32_2() [3/8]

v32acc32 addmac_elem_32_2 | ( | v64int8 | a,
|  | v64int8 | b,
|  | v32acc32 | acc1,
|  | v32acc32 | acc2 )

Parameters

  a | Matrix A
  b | Matrix B
  acc1 | Accumulator 1 input
  acc2 | Accumulator 2 input

Returns
  Result of operation

## ◆ addmac_elem_32_2() [4/8]

v32acc32 addmac_elem_32_2 | ( | v64int8 | a,
|  | v64uint8 | b,
|  | v32acc32 | acc1,
|  | v32acc32 | acc2 )

Parameters

  a | Matrix A
  b | Matrix B
  acc1 | Accumulator 1 input
  acc2 | Accumulator 2 input

Returns
  Result of operation

## ◆ addmac_elem_32_2() [5/8]

v32acc32 addmac_elem_32_2 | ( | v64uint8 | a,
|  | int | sgn_x,
|  | v64int8 | b,
|  | int | sgn_y,
|  | v32acc32 | acc1,
|  | v32acc32 | acc2 )

Parameters

  a | Matrix A
  sgn_x | Sign mask for matrix A
  b | Matrix B
  sgn_y | Sign mask for matrix B
  acc1 | Accumulator 1 input
  acc2 | Accumulator 2 input

Returns
  Result of operation

## ◆ addmac_elem_32_2() [6/8]

v32acc32 addmac_elem_32_2 | ( | v64uint8 | a,
|  | int | sgn_x,
|  | v64uint8 | b,
|  | int | sgn_y,
|  | v32acc32 | acc1,
|  | v32acc32 | acc2 )

Parameters

  a | Matrix A
  sgn_x | Sign mask for matrix A
  b | Matrix B
  sgn_y | Sign mask for matrix B
  acc1 | Accumulator 1 input
  acc2 | Accumulator 2 input

Returns
  Result of operation

## ◆ addmac_elem_32_2() [7/8]

v32acc32 addmac_elem_32_2 | ( | v64uint8 | a,
|  | v64int8 | b,
|  | v32acc32 | acc1,
|  | v32acc32 | acc2 )

Parameters

  a | Matrix A
  b | Matrix B
  acc1 | Accumulator 1 input
  acc2 | Accumulator 2 input

Returns
  Result of operation

## ◆ addmac_elem_32_2() [8/8]

v32acc32 addmac_elem_32_2 | ( | v64uint8 | a,
|  | v64uint8 | b,
|  | v32acc32 | acc1,
|  | v32acc32 | acc2 )

Parameters

  a | Matrix A
  b | Matrix B
  acc1 | Accumulator 1 input
  acc2 | Accumulator 2 input

Returns
  Result of operation

## ◆ addmac_elem_32_2_conf() [1/8]

v32acc32 addmac_elem_32_2_conf | ( | v64int8 | a,
|  | int | sgn_x,
|  | v64int8 | b,
|  | int | sgn_y,
|  | v32acc32 | acc1,
|  | v32acc32 | acc2,
|  | int | zero_acc1,
|  | int | shift16,
|  | int | sub_mul,
|  | int | sub_acc1,
|  | int | sub_acc2 )

Parameters

  a | Matrix A
  sgn_x | Sign mask for matrix A
  b | Matrix B
  sgn_y | Sign mask for matrix B
  acc1 | Accumulator 1 input
  acc2 | Accumulator 2 input
  zero_acc1 | Zeroing mask for acc1
  shift16 | Shift mask of input accumulator acc1
  sub_mul | Negation mask of multiplication result
  sub_acc1 | Negation mask of acc1
  sub_acc2 | Negation mask of acc2

Returns
  Result of operation

## ◆ addmac_elem_32_2_conf() [2/8]

v32acc32 addmac_elem_32_2_conf | ( | v64int8 | a,
|  | int | sgn_x,
|  | v64uint8 | b,
|  | int | sgn_y,
|  | v32acc32 | acc1,
|  | v32acc32 | acc2,
|  | int | zero_acc1,
|  | int | shift16,
|  | int | sub_mul,
|  | int | sub_acc1,
|  | int | sub_acc2 )

Parameters

  a | Matrix A
  sgn_x | Sign mask for matrix A
  b | Matrix B
  sgn_y | Sign mask for matrix B
  acc1 | Accumulator 1 input
  acc2 | Accumulator 2 input
  zero_acc1 | Zeroing mask for acc1
  shift16 | Shift mask of input accumulator acc1
  sub_mul | Negation mask of multiplication result
  sub_acc1 | Negation mask of acc1
  sub_acc2 | Negation mask of acc2

Returns
  Result of operation

## ◆ addmac_elem_32_2_conf() [3/8]

v32acc32 addmac_elem_32_2_conf | ( | v64int8 | a,
|  | v64int8 | b,
|  | v32acc32 | acc1,
|  | v32acc32 | acc2,
|  | int | zero_acc1,
|  | int | shift16,
|  | int | sub_mul,
|  | int | sub_acc1,
|  | int | sub_acc2 )

Parameters

  a | Matrix A
  b | Matrix B
  acc1 | Accumulator 1 input
  acc2 | Accumulator 2 input
  zero_acc1 | Zeroing mask for acc1
  shift16 | Shift mask of input accumulator acc1
  sub_mul | Negation mask of multiplication result
  sub_acc1 | Negation mask of acc1
  sub_acc2 | Negation mask of acc2

Returns
  Result of operation

## ◆ addmac_elem_32_2_conf() [4/8]

v32acc32 addmac_elem_32_2_conf | ( | v64int8 | a,
|  | v64uint8 | b,
|  | v32acc32 | acc1,
|  | v32acc32 | acc2,
|  | int | zero_acc1,
|  | int | shift16,
|  | int | sub_mul,
|  | int | sub_acc1,
|  | int | sub_acc2 )

Parameters

  a | Matrix A
  b | Matrix B
  acc1 | Accumulator 1 input
  acc2 | Accumulator 2 input
  zero_acc1 | Zeroing mask for acc1
  shift16 | Shift mask of input accumulator acc1
  sub_mul | Negation mask of multiplication result
  sub_acc1 | Negation mask of acc1
  sub_acc2 | Negation mask of acc2

Returns
  Result of operation

## ◆ addmac_elem_32_2_conf() [5/8]

v32acc32 addmac_elem_32_2_conf | ( | v64uint8 | a,
|  | int | sgn_x,
|  | v64int8 | b,
|  | int | sgn_y,
|  | v32acc32 | acc1,
|  | v32acc32 | acc2,
|  | int | zero_acc1,
|  | int | shift16,
|  | int | sub_mul,
|  | int | sub_acc1,
|  | int | sub_acc2 )

Parameters

  a | Matrix A
  sgn_x | Sign mask for matrix A
  b | Matrix B
  sgn_y | Sign mask for matrix B
  acc1 | Accumulator 1 input
  acc2 | Accumulator 2 input
  zero_acc1 | Zeroing mask for acc1
  shift16 | Shift mask of input accumulator acc1
  sub_mul | Negation mask of multiplication result
  sub_acc1 | Negation mask of acc1
  sub_acc2 | Negation mask of acc2

Returns
  Result of operation

## ◆ addmac_elem_32_2_conf() [6/8]

v32acc32 addmac_elem_32_2_conf | ( | v64uint8 | a,
|  | int | sgn_x,
|  | v64uint8 | b,
|  | int | sgn_y,
|  | v32acc32 | acc1,
|  | v32acc32 | acc2,
|  | int | zero_acc1,
|  | int | shift16,
|  | int | sub_mul,
|  | int | sub_acc1,
|  | int | sub_acc2 )

Parameters

  a | Matrix A
  sgn_x | Sign mask for matrix A
  b | Matrix B
  sgn_y | Sign mask for matrix B
  acc1 | Accumulator 1 input
  acc2 | Accumulator 2 input
  zero_acc1 | Zeroing mask for acc1
  shift16 | Shift mask of input accumulator acc1
  sub_mul | Negation mask of multiplication result
  sub_acc1 | Negation mask of acc1
  sub_acc2 | Negation mask of acc2

Returns
  Result of operation

## ◆ addmac_elem_32_2_conf() [7/8]

v32acc32 addmac_elem_32_2_conf | ( | v64uint8 | a,
|  | v64int8 | b,
|  | v32acc32 | acc1,
|  | v32acc32 | acc2,
|  | int | zero_acc1,
|  | int | shift16,
|  | int | sub_mul,
|  | int | sub_acc1,
|  | int | sub_acc2 )

Parameters

  a | Matrix A
  b | Matrix B
  acc1 | Accumulator 1 input
  acc2 | Accumulator 2 input
  zero_acc1 | Zeroing mask for acc1
  shift16 | Shift mask of input accumulator acc1
  sub_mul | Negation mask of multiplication result
  sub_acc1 | Negation mask of acc1
  sub_acc2 | Negation mask of acc2

Returns
  Result of operation

## ◆ addmac_elem_32_2_conf() [8/8]

v32acc32 addmac_elem_32_2_conf | ( | v64uint8 | a,
|  | v64uint8 | b,
|  | v32acc32 | acc1,
|  | v32acc32 | acc2,
|  | int | zero_acc1,
|  | int | shift16,
|  | int | sub_mul,
|  | int | sub_acc1,
|  | int | sub_acc2 )

Parameters

  a | Matrix A
  b | Matrix B
  acc1 | Accumulator 1 input
  acc2 | Accumulator 2 input
  zero_acc1 | Zeroing mask for acc1
  shift16 | Shift mask of input accumulator acc1
  sub_mul | Negation mask of multiplication result
  sub_acc1 | Negation mask of acc1
  sub_acc2 | Negation mask of acc2

Returns
  Result of operation

## ◆ addmsc_4x8_8x8() [1/8]

v32acc32 addmsc_4x8_8x8 | ( | v64int8 | a,
|  | int | sgn_x,
|  | v64int8 | b,
|  | int | sgn_y,
|  | v32acc32 | acc1,
|  | v32acc32 | acc2 )

Parameters

  a | Matrix A
  sgn_x | Sign mask for matrix A
  b | Matrix B
  sgn_y | Sign mask for matrix B
  acc1 | Accumulator 1 input
  acc2 | Accumulator 2 input

Returns
  Result of operation

## ◆ addmsc_4x8_8x8() [2/8]

v32acc32 addmsc_4x8_8x8 | ( | v64int8 | a,
|  | int | sgn_x,
|  | v64uint8 | b,
|  | int | sgn_y,
|  | v32acc32 | acc1,
|  | v32acc32 | acc2 )

Parameters

  a | Matrix A
  sgn_x | Sign mask for matrix A
  b | Matrix B
  sgn_y | Sign mask for matrix B
  acc1 | Accumulator 1 input
  acc2 | Accumulator 2 input

Returns
  Result of operation

## ◆ addmsc_4x8_8x8() [3/8]

v32acc32 addmsc_4x8_8x8 | ( | v64int8 | a,
|  | v64int8 | b,
|  | v32acc32 | acc1,
|  | v32acc32 | acc2 )

Parameters

  a | Matrix A
  b | Matrix B
  acc1 | Accumulator 1 input
  acc2 | Accumulator 2 input

Returns
  Result of operation

## ◆ addmsc_4x8_8x8() [4/8]

v32acc32 addmsc_4x8_8x8 | ( | v64int8 | a,
|  | v64uint8 | b,
|  | v32acc32 | acc1,
|  | v32acc32 | acc2 )

Parameters

  a | Matrix A
  b | Matrix B
  acc1 | Accumulator 1 input
  acc2 | Accumulator 2 input

Returns
  Result of operation

## ◆ addmsc_4x8_8x8() [5/8]

v32acc32 addmsc_4x8_8x8 | ( | v64uint8 | a,
|  | int | sgn_x,
|  | v64int8 | b,
|  | int | sgn_y,
|  | v32acc32 | acc1,
|  | v32acc32 | acc2 )

Parameters

  a | Matrix A
  sgn_x | Sign mask for matrix A
  b | Matrix B
  sgn_y | Sign mask for matrix B
  acc1 | Accumulator 1 input
  acc2 | Accumulator 2 input

Returns
  Result of operation

## ◆ addmsc_4x8_8x8() [6/8]

v32acc32 addmsc_4x8_8x8 | ( | v64uint8 | a,
|  | int | sgn_x,
|  | v64uint8 | b,
|  | int | sgn_y,
|  | v32acc32 | acc1,
|  | v32acc32 | acc2 )

Parameters

  a | Matrix A
  sgn_x | Sign mask for matrix A
  b | Matrix B
  sgn_y | Sign mask for matrix B
  acc1 | Accumulator 1 input
  acc2 | Accumulator 2 input

Returns
  Result of operation

## ◆ addmsc_4x8_8x8() [7/8]

v32acc32 addmsc_4x8_8x8 | ( | v64uint8 | a,
|  | v64int8 | b,
|  | v32acc32 | acc1,
|  | v32acc32 | acc2 )

Parameters

  a | Matrix A
  b | Matrix B
  acc1 | Accumulator 1 input
  acc2 | Accumulator 2 input

Returns
  Result of operation

## ◆ addmsc_4x8_8x8() [8/8]

v32acc32 addmsc_4x8_8x8 | ( | v64uint8 | a,
|  | v64uint8 | b,
|  | v32acc32 | acc1,
|  | v32acc32 | acc2 )

Parameters

  a | Matrix A
  b | Matrix B
  acc1 | Accumulator 1 input
  acc2 | Accumulator 2 input

Returns
  Result of operation

## ◆ addmsc_4x8_8x8_conf() [1/8]

v32acc32 addmsc_4x8_8x8_conf | ( | v64int8 | a,
|  | int | sgn_x,
|  | v64int8 | b,
|  | int | sgn_y,
|  | v32acc32 | acc1,
|  | v32acc32 | acc2,
|  | int | zero_acc1,
|  | int | shift16,
|  | int | sub_mul,
|  | int | sub_acc1,
|  | int | sub_acc2 )

Parameters

  a | Matrix A
  sgn_x | Sign mask for matrix A
  b | Matrix B
  sgn_y | Sign mask for matrix B
  acc1 | Accumulator 1 input
  acc2 | Accumulator 2 input
  zero_acc1 | Zeroing mask for acc1
  shift16 | Shift mask of input accumulator acc1
  sub_mul | Negation mask of multiplication result.
  sub_acc1 | Negation mask of acc1
  sub_acc2 | Negation mask of acc2

Returns
  Result of operation

## ◆ addmsc_4x8_8x8_conf() [2/8]

v32acc32 addmsc_4x8_8x8_conf | ( | v64int8 | a,
|  | int | sgn_x,
|  | v64uint8 | b,
|  | int | sgn_y,
|  | v32acc32 | acc1,
|  | v32acc32 | acc2,
|  | int | zero_acc1,
|  | int | shift16,
|  | int | sub_mul,
|  | int | sub_acc1,
|  | int | sub_acc2 )

Parameters

  a | Matrix A
  sgn_x | Sign mask for matrix A
  b | Matrix B
  sgn_y | Sign mask for matrix B
  acc1 | Accumulator 1 input
  acc2 | Accumulator 2 input
  zero_acc1 | Zeroing mask for acc1
  shift16 | Shift mask of input accumulator acc1
  sub_mul | Negation mask of multiplication result.
  sub_acc1 | Negation mask of acc1
  sub_acc2 | Negation mask of acc2

Returns
  Result of operation

## ◆ addmsc_4x8_8x8_conf() [3/8]

v32acc32 addmsc_4x8_8x8_conf | ( | v64int8 | a,
|  | v64int8 | b,
|  | v32acc32 | acc1,
|  | v32acc32 | acc2,
|  | int | zero_acc1,
|  | int | shift16,
|  | int | sub_mul,
|  | int | sub_acc1,
|  | int | sub_acc2 )

Parameters

  a | Matrix A
  b | Matrix B
  acc1 | Accumulator 1 input
  acc2 | Accumulator 2 input
  zero_acc1 | Zeroing mask for acc1
  shift16 | Shift mask of input accumulator acc1
  sub_mul | Negation mask of multiplication result
  sub_acc1 | Negation mask of acc1
  sub_acc2 | Negation mask of acc2

Returns
  Result of operation

## ◆ addmsc_4x8_8x8_conf() [4/8]

v32acc32 addmsc_4x8_8x8_conf | ( | v64int8 | a,
|  | v64uint8 | b,
|  | v32acc32 | acc1,
|  | v32acc32 | acc2,
|  | int | zero_acc1,
|  | int | shift16,
|  | int | sub_mul,
|  | int | sub_acc1,
|  | int | sub_acc2 )

Parameters

  a | Matrix A
  b | Matrix B
  acc1 | Accumulator 1 input
  acc2 | Accumulator 2 input
  zero_acc1 | Zeroing mask for acc1
  shift16 | Shift mask of input accumulator acc1
  sub_mul | Negation mask of multiplication result
  sub_acc1 | Negation mask of acc1
  sub_acc2 | Negation mask of acc2

Returns
  Result of operation

## ◆ addmsc_4x8_8x8_conf() [5/8]

v32acc32 addmsc_4x8_8x8_conf | ( | v64uint8 | a,
|  | int | sgn_x,
|  | v64int8 | b,
|  | int | sgn_y,
|  | v32acc32 | acc1,
|  | v32acc32 | acc2,
|  | int | zero_acc1,
|  | int | shift16,
|  | int | sub_mul,
|  | int | sub_acc1,
|  | int | sub_acc2 )

Parameters

  a | Matrix A
  sgn_x | Sign mask for matrix A
  b | Matrix B
  sgn_y | Sign mask for matrix B
  acc1 | Accumulator 1 input
  acc2 | Accumulator 2 input
  zero_acc1 | Zeroing mask for acc1
  shift16 | Shift mask of input accumulator acc1
  sub_mul | Negation mask of multiplication result.
  sub_acc1 | Negation mask of acc1
  sub_acc2 | Negation mask of acc2

Returns
  Result of operation

## ◆ addmsc_4x8_8x8_conf() [6/8]

v32acc32 addmsc_4x8_8x8_conf | ( | v64uint8 | a,
|  | int | sgn_x,
|  | v64uint8 | b,
|  | int | sgn_y,
|  | v32acc32 | acc1,
|  | v32acc32 | acc2,
|  | int | zero_acc1,
|  | int | shift16,
|  | int | sub_mul,
|  | int | sub_acc1,
|  | int | sub_acc2 )

Parameters

  a | Matrix A
  sgn_x | Sign mask for matrix A
  b | Matrix B
  sgn_y | Sign mask for matrix B
  acc1 | Accumulator 1 input
  acc2 | Accumulator 2 input
  zero_acc1 | Zeroing mask for acc1
  shift16 | Shift mask of input accumulator acc1
  sub_mul | Negation mask of multiplication result.
  sub_acc1 | Negation mask of acc1
  sub_acc2 | Negation mask of acc2

Returns
  Result of operation

## ◆ addmsc_4x8_8x8_conf() [7/8]

v32acc32 addmsc_4x8_8x8_conf | ( | v64uint8 | a,
|  | v64int8 | b,
|  | v32acc32 | acc1,
|  | v32acc32 | acc2,
|  | int | zero_acc1,
|  | int | shift16,
|  | int | sub_mul,
|  | int | sub_acc1,
|  | int | sub_acc2 )

Parameters

  a | Matrix A
  b | Matrix B
  acc1 | Accumulator 1 input
  acc2 | Accumulator 2 input
  zero_acc1 | Zeroing mask for acc1
  shift16 | Shift mask of input accumulator acc1
  sub_mul | Negation mask of multiplication result
  sub_acc1 | Negation mask of acc1
  sub_acc2 | Negation mask of acc2

Returns
  Result of operation

## ◆ addmsc_4x8_8x8_conf() [8/8]

v32acc32 addmsc_4x8_8x8_conf | ( | v64uint8 | a,
|  | v64uint8 | b,
|  | v32acc32 | acc1,
|  | v32acc32 | acc2,
|  | int | zero_acc1,
|  | int | shift16,
|  | int | sub_mul,
|  | int | sub_acc1,
|  | int | sub_acc2 )

Parameters

  a | Matrix A
  b | Matrix B
  acc1 | Accumulator 1 input
  acc2 | Accumulator 2 input
  zero_acc1 | Zeroing mask for acc1
  shift16 | Shift mask of input accumulator acc1
  sub_mul | Negation mask of multiplication result
  sub_acc1 | Negation mask of acc1
  sub_acc2 | Negation mask of acc2

Returns
  Result of operation

## ◆ addmsc_conv_32x8() [1/8]

v32acc32 addmsc_conv_32x8 | ( | v64int8 | a,
|  | int | sgn_x,
|  | v64int8 | b,
|  | int | sgn_y,
|  | v32acc32 | acc1,
|  | v32acc32 | acc2 )

Parameters

  a | Matrix A
  sgn_x | Sign mask for matrix A
  b | Matrix B
  sgn_y | Sign mask for matrix B
  acc1 | Accumulator 1 input
  acc2 | Accumulator 2 input

Returns
  Result of operation

## ◆ addmsc_conv_32x8() [2/8]

v32acc32 addmsc_conv_32x8 | ( | v64int8 | a,
|  | int | sgn_x,
|  | v64uint8 | b,
|  | int | sgn_y,
|  | v32acc32 | acc1,
|  | v32acc32 | acc2 )

Parameters

  a | Matrix A
  sgn_x | Sign mask for matrix A
  b | Matrix B
  sgn_y | Sign mask for matrix B
  acc1 | Accumulator 1 input
  acc2 | Accumulator 2 input

Returns
  Result of operation

## ◆ addmsc_conv_32x8() [3/8]

v32acc32 addmsc_conv_32x8 | ( | v64int8 | a,
|  | v64int8 | b,
|  | v32acc32 | acc1,
|  | v32acc32 | acc2 )

Parameters

  a | Matrix A
  b | Matrix B
  acc1 | Accumulator 1 input
  acc2 | Accumulator 2 input

Returns
  Result of operation

## ◆ addmsc_conv_32x8() [4/8]

v32acc32 addmsc_conv_32x8 | ( | v64int8 | a,
|  | v64uint8 | b,
|  | v32acc32 | acc1,
|  | v32acc32 | acc2 )

Parameters

  a | Matrix A
  b | Matrix B
  acc1 | Accumulator 1 input
  acc2 | Accumulator 2 input

Returns
  Result of operation

## ◆ addmsc_conv_32x8() [5/8]

v32acc32 addmsc_conv_32x8 | ( | v64uint8 | a,
|  | int | sgn_x,
|  | v64int8 | b,
|  | int | sgn_y,
|  | v32acc32 | acc1,
|  | v32acc32 | acc2 )

Parameters

  a | Matrix A
  sgn_x | Sign mask for matrix A
  b | Matrix B
  sgn_y | Sign mask for matrix B
  acc1 | Accumulator 1 input
  acc2 | Accumulator 2 input

Returns
  Result of operation

## ◆ addmsc_conv_32x8() [6/8]

v32acc32 addmsc_conv_32x8 | ( | v64uint8 | a,
|  | int | sgn_x,
|  | v64uint8 | b,
|  | int | sgn_y,
|  | v32acc32 | acc1,
|  | v32acc32 | acc2 )

Parameters

  a | Matrix A
  sgn_x | Sign mask for matrix A
  b | Matrix B
  sgn_y | Sign mask for matrix B
  acc1 | Accumulator 1 input
  acc2 | Accumulator 2 input

Returns
  Result of operation

## ◆ addmsc_conv_32x8() [7/8]

v32acc32 addmsc_conv_32x8 | ( | v64uint8 | a,
|  | v64int8 | b,
|  | v32acc32 | acc1,
|  | v32acc32 | acc2 )

Parameters

  a | Matrix A
  b | Matrix B
  acc1 | Accumulator 1 input
  acc2 | Accumulator 2 input

Returns
  Result of operation

## ◆ addmsc_conv_32x8() [8/8]

v32acc32 addmsc_conv_32x8 | ( | v64uint8 | a,
|  | v64uint8 | b,
|  | v32acc32 | acc1,
|  | v32acc32 | acc2 )

Parameters

  a | Matrix A
  b | Matrix B
  acc1 | Accumulator 1 input
  acc2 | Accumulator 2 input

Returns
  Result of operation

## ◆ addmsc_conv_32x8_conf() [1/8]

v32acc32 addmsc_conv_32x8_conf | ( | v64int8 | a,
|  | int | sgn_x,
|  | v64int8 | b,
|  | int | sgn_y,
|  | v32acc32 | acc1,
|  | v32acc32 | acc2,
|  | int | zero_acc1,
|  | int | shift16,
|  | int | sub_mul,
|  | int | sub_acc1,
|  | int | sub_acc2 )

Parameters

  a | Matrix A
  sgn_x | Sign mask for matrix A
  b | Matrix B
  sgn_y | Sign mask for matrix B
  acc1 | Accumulator 1 input
  acc2 | Accumulator 2 input
  zero_acc1 | Zeroing mask for acc1
  shift16 | Shift mask of input accumulator acc1
  sub_mul | Negation mask of multiplication result.
  sub_acc1 | Negation mask of acc1
  sub_acc2 | Negation mask of acc2

Returns
  Result of operation

## ◆ addmsc_conv_32x8_conf() [2/8]

v32acc32 addmsc_conv_32x8_conf | ( | v64int8 | a,
|  | int | sgn_x,
|  | v64uint8 | b,
|  | int | sgn_y,
|  | v32acc32 | acc1,
|  | v32acc32 | acc2,
|  | int | zero_acc1,
|  | int | shift16,
|  | int | sub_mul,
|  | int | sub_acc1,
|  | int | sub_acc2 )

Parameters

  a | Matrix A
  sgn_x | Sign mask for matrix A
  b | Matrix B
  sgn_y | Sign mask for matrix B
  acc1 | Accumulator 1 input
  acc2 | Accumulator 2 input
  zero_acc1 | Zeroing mask for acc1
  shift16 | Shift mask of input accumulator acc1
  sub_mul | Negation mask of multiplication result.
  sub_acc1 | Negation mask of acc1
  sub_acc2 | Negation mask of acc2

Returns
  Result of operation

## ◆ addmsc_conv_32x8_conf() [3/8]

v32acc32 addmsc_conv_32x8_conf | ( | v64int8 | a,
|  | v64int8 | b,
|  | v32acc32 | acc1,
|  | v32acc32 | acc2,
|  | int | zero_acc1,
|  | int | shift16,
|  | int | sub_mul,
|  | int | sub_acc1,
|  | int | sub_acc2 )

Parameters

  a | Matrix A
  b | Matrix B
  acc1 | Accumulator 1 input
  acc2 | Accumulator 2 input
  zero_acc1 | Zeroing mask for acc1
  shift16 | Shift mask of input accumulator acc1
  sub_mul | Negation mask of multiplication result
  sub_acc1 | Negation mask of acc1
  sub_acc2 | Negation mask of acc2

Returns
  Result of operation

## ◆ addmsc_conv_32x8_conf() [4/8]

v32acc32 addmsc_conv_32x8_conf | ( | v64int8 | a,
|  | v64uint8 | b,
|  | v32acc32 | acc1,
|  | v32acc32 | acc2,
|  | int | zero_acc1,
|  | int | shift16,
|  | int | sub_mul,
|  | int | sub_acc1,
|  | int | sub_acc2 )

Parameters

  a | Matrix A
  b | Matrix B
  acc1 | Accumulator 1 input
  acc2 | Accumulator 2 input
  zero_acc1 | Zeroing mask for acc1
  shift16 | Shift mask of input accumulator acc1
  sub_mul | Negation mask of multiplication result
  sub_acc1 | Negation mask of acc1
  sub_acc2 | Negation mask of acc2

Returns
  Result of operation

## ◆ addmsc_conv_32x8_conf() [5/8]

v32acc32 addmsc_conv_32x8_conf | ( | v64uint8 | a,
|  | int | sgn_x,
|  | v64int8 | b,
|  | int | sgn_y,
|  | v32acc32 | acc1,
|  | v32acc32 | acc2,
|  | int | zero_acc1,
|  | int | shift16,
|  | int | sub_mul,
|  | int | sub_acc1,
|  | int | sub_acc2 )

Parameters

  a | Matrix A
  sgn_x | Sign mask for matrix A
  b | Matrix B
  sgn_y | Sign mask for matrix B
  acc1 | Accumulator 1 input
  acc2 | Accumulator 2 input
  zero_acc1 | Zeroing mask for acc1
  shift16 | Shift mask of input accumulator acc1
  sub_mul | Negation mask of multiplication result.
  sub_acc1 | Negation mask of acc1
  sub_acc2 | Negation mask of acc2

Returns
  Result of operation

## ◆ addmsc_conv_32x8_conf() [6/8]

v32acc32 addmsc_conv_32x8_conf | ( | v64uint8 | a,
|  | int | sgn_x,
|  | v64uint8 | b,
|  | int | sgn_y,
|  | v32acc32 | acc1,
|  | v32acc32 | acc2,
|  | int | zero_acc1,
|  | int | shift16,
|  | int | sub_mul,
|  | int | sub_acc1,
|  | int | sub_acc2 )

Parameters

  a | Matrix A
  sgn_x | Sign mask for matrix A
  b | Matrix B
  sgn_y | Sign mask for matrix B
  acc1 | Accumulator 1 input
  acc2 | Accumulator 2 input
  zero_acc1 | Zeroing mask for acc1
  shift16 | Shift mask of input accumulator acc1
  sub_mul | Negation mask of multiplication result.
  sub_acc1 | Negation mask of acc1
  sub_acc2 | Negation mask of acc2

Returns
  Result of operation

## ◆ addmsc_conv_32x8_conf() [7/8]

v32acc32 addmsc_conv_32x8_conf | ( | v64uint8 | a,
|  | v64int8 | b,
|  | v32acc32 | acc1,
|  | v32acc32 | acc2,
|  | int | zero_acc1,
|  | int | shift16,
|  | int | sub_mul,
|  | int | sub_acc1,
|  | int | sub_acc2 )

Parameters

  a | Matrix A
  b | Matrix B
  acc1 | Accumulator 1 input
  acc2 | Accumulator 2 input
  zero_acc1 | Zeroing mask for acc1
  shift16 | Shift mask of input accumulator acc1
  sub_mul | Negation mask of multiplication result
  sub_acc1 | Negation mask of acc1
  sub_acc2 | Negation mask of acc2

Returns
  Result of operation

## ◆ addmsc_conv_32x8_conf() [8/8]

v32acc32 addmsc_conv_32x8_conf | ( | v64uint8 | a,
|  | v64uint8 | b,
|  | v32acc32 | acc1,
|  | v32acc32 | acc2,
|  | int | zero_acc1,
|  | int | shift16,
|  | int | sub_mul,
|  | int | sub_acc1,
|  | int | sub_acc2 )

Parameters

  a | Matrix A
  b | Matrix B
  acc1 | Accumulator 1 input
  acc2 | Accumulator 2 input
  zero_acc1 | Zeroing mask for acc1
  shift16 | Shift mask of input accumulator acc1
  sub_mul | Negation mask of multiplication result
  sub_acc1 | Negation mask of acc1
  sub_acc2 | Negation mask of acc2

Returns
  Result of operation

## ◆ addmsc_conv_4x4_8ch() [1/8]

v32acc32 addmsc_conv_4x4_8ch | ( | v64int8 | a,
|  | int | sgn_x,
|  | v64int8 | b,
|  | int | sgn_y,
|  | v32acc32 | acc1,
|  | v32acc32 | acc2 )

Parameters

  a | Matrix A
  sgn_x | Sign mask for matrix A
  b | Matrix B
  sgn_y | Sign mask for matrix B
  acc1 | Accumulator 1 input
  acc2 | Accumulator 2 input

Returns
  Result of operation

## ◆ addmsc_conv_4x4_8ch() [2/8]

v32acc32 addmsc_conv_4x4_8ch | ( | v64int8 | a,
|  | int | sgn_x,
|  | v64uint8 | b,
|  | int | sgn_y,
|  | v32acc32 | acc1,
|  | v32acc32 | acc2 )

Parameters

  a | Matrix A
  sgn_x | Sign mask for matrix A
  b | Matrix B
  sgn_y | Sign mask for matrix B
  acc1 | Accumulator 1 input
  acc2 | Accumulator 2 input

Returns
  Result of operation

## ◆ addmsc_conv_4x4_8ch() [3/8]

v32acc32 addmsc_conv_4x4_8ch | ( | v64int8 | a,
|  | v64int8 | b,
|  | v32acc32 | acc1,
|  | v32acc32 | acc2 )

Parameters

  a | Matrix A
  b | Matrix B
  acc1 | Accumulator 1 input
  acc2 | Accumulator 2 input

Returns
  Result of operation

## ◆ addmsc_conv_4x4_8ch() [4/8]

v32acc32 addmsc_conv_4x4_8ch | ( | v64int8 | a,
|  | v64uint8 | b,
|  | v32acc32 | acc1,
|  | v32acc32 | acc2 )

Parameters

  a | Matrix A
  b | Matrix B
  acc1 | Accumulator 1 input
  acc2 | Accumulator 2 input

Returns
  Result of operation

## ◆ addmsc_conv_4x4_8ch() [5/8]

v32acc32 addmsc_conv_4x4_8ch | ( | v64uint8 | a,
|  | int | sgn_x,
|  | v64int8 | b,
|  | int | sgn_y,
|  | v32acc32 | acc1,
|  | v32acc32 | acc2 )

Parameters

  a | Matrix A
  sgn_x | Sign mask for matrix A
  b | Matrix B
  sgn_y | Sign mask for matrix B
  acc1 | Accumulator 1 input
  acc2 | Accumulator 2 input

Returns
  Result of operation

## ◆ addmsc_conv_4x4_8ch() [6/8]

v32acc32 addmsc_conv_4x4_8ch | ( | v64uint8 | a,
|  | int | sgn_x,
|  | v64uint8 | b,
|  | int | sgn_y,
|  | v32acc32 | acc1,
|  | v32acc32 | acc2 )

Parameters

  a | Matrix A
  sgn_x | Sign mask for matrix A
  b | Matrix B
  sgn_y | Sign mask for matrix B
  acc1 | Accumulator 1 input
  acc2 | Accumulator 2 input

Returns
  Result of operation

## ◆ addmsc_conv_4x4_8ch() [7/8]

v32acc32 addmsc_conv_4x4_8ch | ( | v64uint8 | a,
|  | v64int8 | b,
|  | v32acc32 | acc1,
|  | v32acc32 | acc2 )

Parameters

  a | Matrix A
  b | Matrix B
  acc1 | Accumulator 1 input
  acc2 | Accumulator 2 input

Returns
  Result of operation

## ◆ addmsc_conv_4x4_8ch() [8/8]

v32acc32 addmsc_conv_4x4_8ch | ( | v64uint8 | a,
|  | v64uint8 | b,
|  | v32acc32 | acc1,
|  | v32acc32 | acc2 )

Parameters

  a | Matrix A
  b | Matrix B
  acc1 | Accumulator 1 input
  acc2 | Accumulator 2 input

Returns
  Result of operation

## ◆ addmsc_conv_4x4_8ch_conf() [1/8]

v32acc32 addmsc_conv_4x4_8ch_conf | ( | v64int8 | a,
|  | int | sgn_x,
|  | v64int8 | b,
|  | int | sgn_y,
|  | v32acc32 | acc1,
|  | v32acc32 | acc2,
|  | int | zero_acc1,
|  | int | shift16,
|  | int | sub_mul,
|  | int | sub_acc1,
|  | int | sub_acc2 )

Parameters

  a | Matrix A
  sgn_x | Sign mask for matrix A
  b | Matrix B
  sgn_y | Sign mask for matrix B
  acc1 | Accumulator 1 input
  acc2 | Accumulator 2 input
  zero_acc1 | Zeroing mask for acc1
  shift16 | Shift mask of input accumulator acc1
  sub_mul | Negation mask of multiplication result.
  sub_acc1 | Negation mask of acc1
  sub_acc2 | Negation mask of acc2

Returns
  Result of operation

## ◆ addmsc_conv_4x4_8ch_conf() [2/8]

v32acc32 addmsc_conv_4x4_8ch_conf | ( | v64int8 | a,
|  | int | sgn_x,
|  | v64uint8 | b,
|  | int | sgn_y,
|  | v32acc32 | acc1,
|  | v32acc32 | acc2,
|  | int | zero_acc1,
|  | int | shift16,
|  | int | sub_mul,
|  | int | sub_acc1,
|  | int | sub_acc2 )

Parameters

  a | Matrix A
  sgn_x | Sign mask for matrix A
  b | Matrix B
  sgn_y | Sign mask for matrix B
  acc1 | Accumulator 1 input
  acc2 | Accumulator 2 input
  zero_acc1 | Zeroing mask for acc1
  shift16 | Shift mask of input accumulator acc1
  sub_mul | Negation mask of multiplication result.
  sub_acc1 | Negation mask of acc1
  sub_acc2 | Negation mask of acc2

Returns
  Result of operation

## ◆ addmsc_conv_4x4_8ch_conf() [3/8]

v32acc32 addmsc_conv_4x4_8ch_conf | ( | v64int8 | a,
|  | v64int8 | b,
|  | v32acc32 | acc1,
|  | v32acc32 | acc2,
|  | int | zero_acc1,
|  | int | shift16,
|  | int | sub_mul,
|  | int | sub_acc1,
|  | int | sub_acc2 )

Parameters

  a | Matrix A
  b | Matrix B
  acc1 | Accumulator 1 input
  acc2 | Accumulator 2 input
  zero_acc1 | Zeroing mask for acc1
  shift16 | Shift mask of input accumulator acc1
  sub_mul | Negation mask of multiplication result
  sub_acc1 | Negation mask of acc1
  sub_acc2 | Negation mask of acc2

Returns
  Result of operation

## ◆ addmsc_conv_4x4_8ch_conf() [4/8]

v32acc32 addmsc_conv_4x4_8ch_conf | ( | v64int8 | a,
|  | v64uint8 | b,
|  | v32acc32 | acc1,
|  | v32acc32 | acc2,
|  | int | zero_acc1,
|  | int | shift16,
|  | int | sub_mul,
|  | int | sub_acc1,
|  | int | sub_acc2 )

Parameters

  a | Matrix A
  b | Matrix B
  acc1 | Accumulator 1 input
  acc2 | Accumulator 2 input
  zero_acc1 | Zeroing mask for acc1
  shift16 | Shift mask of input accumulator acc1
  sub_mul | Negation mask of multiplication result
  sub_acc1 | Negation mask of acc1
  sub_acc2 | Negation mask of acc2

Returns
  Result of operation

## ◆ addmsc_conv_4x4_8ch_conf() [5/8]

v32acc32 addmsc_conv_4x4_8ch_conf | ( | v64uint8 | a,
|  | int | sgn_x,
|  | v64int8 | b,
|  | int | sgn_y,
|  | v32acc32 | acc1,
|  | v32acc32 | acc2,
|  | int | zero_acc1,
|  | int | shift16,
|  | int | sub_mul,
|  | int | sub_acc1,
|  | int | sub_acc2 )

Parameters

  a | Matrix A
  sgn_x | Sign mask for matrix A
  b | Matrix B
  sgn_y | Sign mask for matrix B
  acc1 | Accumulator 1 input
  acc2 | Accumulator 2 input
  zero_acc1 | Zeroing mask for acc1
  shift16 | Shift mask of input accumulator acc1
  sub_mul | Negation mask of multiplication result.
  sub_acc1 | Negation mask of acc1
  sub_acc2 | Negation mask of acc2

Returns
  Result of operation

## ◆ addmsc_conv_4x4_8ch_conf() [6/8]

v32acc32 addmsc_conv_4x4_8ch_conf | ( | v64uint8 | a,
|  | int | sgn_x,
|  | v64uint8 | b,
|  | int | sgn_y,
|  | v32acc32 | acc1,
|  | v32acc32 | acc2,
|  | int | zero_acc1,
|  | int | shift16,
|  | int | sub_mul,
|  | int | sub_acc1,
|  | int | sub_acc2 )

Parameters

  a | Matrix A
  sgn_x | Sign mask for matrix A
  b | Matrix B
  sgn_y | Sign mask for matrix B
  acc1 | Accumulator 1 input
  acc2 | Accumulator 2 input
  zero_acc1 | Zeroing mask for acc1
  shift16 | Shift mask of input accumulator acc1
  sub_mul | Negation mask of multiplication result.
  sub_acc1 | Negation mask of acc1
  sub_acc2 | Negation mask of acc2

Returns
  Result of operation

## ◆ addmsc_conv_4x4_8ch_conf() [7/8]

v32acc32 addmsc_conv_4x4_8ch_conf | ( | v64uint8 | a,
|  | v64int8 | b,
|  | v32acc32 | acc1,
|  | v32acc32 | acc2,
|  | int | zero_acc1,
|  | int | shift16,
|  | int | sub_mul,
|  | int | sub_acc1,
|  | int | sub_acc2 )

Parameters

  a | Matrix A
  b | Matrix B
  acc1 | Accumulator 1 input
  acc2 | Accumulator 2 input
  zero_acc1 | Zeroing mask for acc1
  shift16 | Shift mask of input accumulator acc1
  sub_mul | Negation mask of multiplication result
  sub_acc1 | Negation mask of acc1
  sub_acc2 | Negation mask of acc2

Returns
  Result of operation

## ◆ addmsc_conv_4x4_8ch_conf() [8/8]

v32acc32 addmsc_conv_4x4_8ch_conf | ( | v64uint8 | a,
|  | v64uint8 | b,
|  | v32acc32 | acc1,
|  | v32acc32 | acc2,
|  | int | zero_acc1,
|  | int | shift16,
|  | int | sub_mul,
|  | int | sub_acc1,
|  | int | sub_acc2 )

Parameters

  a | Matrix A
  b | Matrix B
  acc1 | Accumulator 1 input
  acc2 | Accumulator 2 input
  zero_acc1 | Zeroing mask for acc1
  shift16 | Shift mask of input accumulator acc1
  sub_mul | Negation mask of multiplication result
  sub_acc1 | Negation mask of acc1
  sub_acc2 | Negation mask of acc2

Returns
  Result of operation

## ◆ addmsc_conv_8x8_4ch() [1/8]

v32acc32 addmsc_conv_8x8_4ch | ( | v64int8 | a,
|  | int | sgn_x,
|  | v64int8 | b,
|  | int | sgn_y,
|  | v32acc32 | acc1,
|  | v32acc32 | acc2 )

Parameters

  a | Matrix A
  sgn_x | Sign mask for matrix A
  b | Matrix B
  sgn_y | Sign mask for matrix B
  acc1 | Accumulator 1 input
  acc2 | Accumulator 2 input

Returns
  Result of operation

## ◆ addmsc_conv_8x8_4ch() [2/8]

v32acc32 addmsc_conv_8x8_4ch | ( | v64int8 | a,
|  | int | sgn_x,
|  | v64uint8 | b,
|  | int | sgn_y,
|  | v32acc32 | acc1,
|  | v32acc32 | acc2 )

Parameters

  a | Matrix A
  sgn_x | Sign mask for matrix A
  b | Matrix B
  sgn_y | Sign mask for matrix B
  acc1 | Accumulator 1 input
  acc2 | Accumulator 2 input

Returns
  Result of operation

## ◆ addmsc_conv_8x8_4ch() [3/8]

v32acc32 addmsc_conv_8x8_4ch | ( | v64int8 | a,
|  | v64int8 | b,
|  | v32acc32 | acc1,
|  | v32acc32 | acc2 )

Parameters

  a | Matrix A
  b | Matrix B
  acc1 | Accumulator 1 input
  acc2 | Accumulator 2 input

Returns
  Result of operation

## ◆ addmsc_conv_8x8_4ch() [4/8]

v32acc32 addmsc_conv_8x8_4ch | ( | v64int8 | a,
|  | v64uint8 | b,
|  | v32acc32 | acc1,
|  | v32acc32 | acc2 )

Parameters

  a | Matrix A
  b | Matrix B
  acc1 | Accumulator 1 input
  acc2 | Accumulator 2 input

Returns
  Result of operation

## ◆ addmsc_conv_8x8_4ch() [5/8]

v32acc32 addmsc_conv_8x8_4ch | ( | v64uint8 | a,
|  | int | sgn_x,
|  | v64int8 | b,
|  | int | sgn_y,
|  | v32acc32 | acc1,
|  | v32acc32 | acc2 )

Parameters

  a | Matrix A
  sgn_x | Sign mask for matrix A
  b | Matrix B
  sgn_y | Sign mask for matrix B
  acc1 | Accumulator 1 input
  acc2 | Accumulator 2 input

Returns
  Result of operation

## ◆ addmsc_conv_8x8_4ch() [6/8]

v32acc32 addmsc_conv_8x8_4ch | ( | v64uint8 | a,
|  | int | sgn_x,
|  | v64uint8 | b,
|  | int | sgn_y,
|  | v32acc32 | acc1,
|  | v32acc32 | acc2 )

Parameters

  a | Matrix A
  sgn_x | Sign mask for matrix A
  b | Matrix B
  sgn_y | Sign mask for matrix B
  acc1 | Accumulator 1 input
  acc2 | Accumulator 2 input

Returns
  Result of operation

## ◆ addmsc_conv_8x8_4ch() [7/8]

v32acc32 addmsc_conv_8x8_4ch | ( | v64uint8 | a,
|  | v64int8 | b,
|  | v32acc32 | acc1,
|  | v32acc32 | acc2 )

Parameters

  a | Matrix A
  b | Matrix B
  acc1 | Accumulator 1 input
  acc2 | Accumulator 2 input

Returns
  Result of operation

## ◆ addmsc_conv_8x8_4ch() [8/8]

v32acc32 addmsc_conv_8x8_4ch | ( | v64uint8 | a,
|  | v64uint8 | b,
|  | v32acc32 | acc1,
|  | v32acc32 | acc2 )

Parameters

  a | Matrix A
  b | Matrix B
  acc1 | Accumulator 1 input
  acc2 | Accumulator 2 input

Returns
  Result of operation

## ◆ addmsc_conv_8x8_4ch_conf() [1/8]

v32acc32 addmsc_conv_8x8_4ch_conf | ( | v64int8 | a,
|  | int | sgn_x,
|  | v64int8 | b,
|  | int | sgn_y,
|  | v32acc32 | acc1,
|  | v32acc32 | acc2,
|  | int | zero_acc1,
|  | int | shift16,
|  | int | sub_mul,
|  | int | sub_acc1,
|  | int | sub_acc2 )

Parameters

  a | Matrix A
  sgn_x | Sign mask for matrix A
  b | Matrix B
  sgn_y | Sign mask for matrix B
  acc1 | Accumulator 1 input
  acc2 | Accumulator 2 input
  zero_acc1 | Zeroing mask for acc1
  shift16 | Shift mask of input accumulator acc1
  sub_mul | Negation mask of multiplication result.
  sub_acc1 | Negation mask of acc1
  sub_acc2 | Negation mask of acc2

Returns
  Result of operation

## ◆ addmsc_conv_8x8_4ch_conf() [2/8]

v32acc32 addmsc_conv_8x8_4ch_conf | ( | v64int8 | a,
|  | int | sgn_x,
|  | v64uint8 | b,
|  | int | sgn_y,
|  | v32acc32 | acc1,
|  | v32acc32 | acc2,
|  | int | zero_acc1,
|  | int | shift16,
|  | int | sub_mul,
|  | int | sub_acc1,
|  | int | sub_acc2 )

Parameters

  a | Matrix A
  sgn_x | Sign mask for matrix A
  b | Matrix B
  sgn_y | Sign mask for matrix B
  acc1 | Accumulator 1 input
  acc2 | Accumulator 2 input
  zero_acc1 | Zeroing mask for acc1
  shift16 | Shift mask of input accumulator acc1
  sub_mul | Negation mask of multiplication result.
  sub_acc1 | Negation mask of acc1
  sub_acc2 | Negation mask of acc2

Returns
  Result of operation

## ◆ addmsc_conv_8x8_4ch_conf() [3/8]

v32acc32 addmsc_conv_8x8_4ch_conf | ( | v64int8 | a,
|  | v64int8 | b,
|  | v32acc32 | acc1,
|  | v32acc32 | acc2,
|  | int | zero_acc1,
|  | int | shift16,
|  | int | sub_mul,
|  | int | sub_acc1,
|  | int | sub_acc2 )

Parameters

  a | Matrix A
  b | Matrix B
  acc1 | Accumulator 1 input
  acc2 | Accumulator 2 input
  zero_acc1 | Zeroing mask for acc1
  shift16 | Shift mask of input accumulator acc1
  sub_mul | Negation mask of multiplication result
  sub_acc1 | Negation mask of acc1
  sub_acc2 | Negation mask of acc2

Returns
  Result of operation

## ◆ addmsc_conv_8x8_4ch_conf() [4/8]

v32acc32 addmsc_conv_8x8_4ch_conf | ( | v64int8 | a,
|  | v64uint8 | b,
|  | v32acc32 | acc1,
|  | v32acc32 | acc2,
|  | int | zero_acc1,
|  | int | shift16,
|  | int | sub_mul,
|  | int | sub_acc1,
|  | int | sub_acc2 )

Parameters

  a | Matrix A
  b | Matrix B
  acc1 | Accumulator 1 input
  acc2 | Accumulator 2 input
  zero_acc1 | Zeroing mask for acc1
  shift16 | Shift mask of input accumulator acc1
  sub_mul | Negation mask of multiplication result
  sub_acc1 | Negation mask of acc1
  sub_acc2 | Negation mask of acc2

Returns
  Result of operation

## ◆ addmsc_conv_8x8_4ch_conf() [5/8]

v32acc32 addmsc_conv_8x8_4ch_conf | ( | v64uint8 | a,
|  | int | sgn_x,
|  | v64int8 | b,
|  | int | sgn_y,
|  | v32acc32 | acc1,
|  | v32acc32 | acc2,
|  | int | zero_acc1,
|  | int | shift16,
|  | int | sub_mul,
|  | int | sub_acc1,
|  | int | sub_acc2 )

Parameters

  a | Matrix A
  sgn_x | Sign mask for matrix A
  b | Matrix B
  sgn_y | Sign mask for matrix B
  acc1 | Accumulator 1 input
  acc2 | Accumulator 2 input
  zero_acc1 | Zeroing mask for acc1
  shift16 | Shift mask of input accumulator acc1
  sub_mul | Negation mask of multiplication result.
  sub_acc1 | Negation mask of acc1
  sub_acc2 | Negation mask of acc2

Returns
  Result of operation

## ◆ addmsc_conv_8x8_4ch_conf() [6/8]

v32acc32 addmsc_conv_8x8_4ch_conf | ( | v64uint8 | a,
|  | int | sgn_x,
|  | v64uint8 | b,
|  | int | sgn_y,
|  | v32acc32 | acc1,
|  | v32acc32 | acc2,
|  | int | zero_acc1,
|  | int | shift16,
|  | int | sub_mul,
|  | int | sub_acc1,
|  | int | sub_acc2 )

Parameters

  a | Matrix A
  sgn_x | Sign mask for matrix A
  b | Matrix B
  sgn_y | Sign mask for matrix B
  acc1 | Accumulator 1 input
  acc2 | Accumulator 2 input
  zero_acc1 | Zeroing mask for acc1
  shift16 | Shift mask of input accumulator acc1
  sub_mul | Negation mask of multiplication result.
  sub_acc1 | Negation mask of acc1
  sub_acc2 | Negation mask of acc2

Returns
  Result of operation

## ◆ addmsc_conv_8x8_4ch_conf() [7/8]

v32acc32 addmsc_conv_8x8_4ch_conf | ( | v64uint8 | a,
|  | v64int8 | b,
|  | v32acc32 | acc1,
|  | v32acc32 | acc2,
|  | int | zero_acc1,
|  | int | shift16,
|  | int | sub_mul,
|  | int | sub_acc1,
|  | int | sub_acc2 )

Parameters

  a | Matrix A
  b | Matrix B
  acc1 | Accumulator 1 input
  acc2 | Accumulator 2 input
  zero_acc1 | Zeroing mask for acc1
  shift16 | Shift mask of input accumulator acc1
  sub_mul | Negation mask of multiplication result
  sub_acc1 | Negation mask of acc1
  sub_acc2 | Negation mask of acc2

Returns
  Result of operation

## ◆ addmsc_conv_8x8_4ch_conf() [8/8]

v32acc32 addmsc_conv_8x8_4ch_conf | ( | v64uint8 | a,
|  | v64uint8 | b,
|  | v32acc32 | acc1,
|  | v32acc32 | acc2,
|  | int | zero_acc1,
|  | int | shift16,
|  | int | sub_mul,
|  | int | sub_acc1,
|  | int | sub_acc2 )

Parameters

  a | Matrix A
  b | Matrix B
  acc1 | Accumulator 1 input
  acc2 | Accumulator 2 input
  zero_acc1 | Zeroing mask for acc1
  shift16 | Shift mask of input accumulator acc1
  sub_mul | Negation mask of multiplication result
  sub_acc1 | Negation mask of acc1
  sub_acc2 | Negation mask of acc2

Returns
  Result of operation

## ◆ addmsc_elem_32_2() [1/8]

v32acc32 addmsc_elem_32_2 | ( | v64int8 | a,
|  | int | sgn_x,
|  | v64int8 | b,
|  | int | sgn_y,
|  | v32acc32 | acc1,
|  | v32acc32 | acc2 )

Parameters

  a | Matrix A
  sgn_x | Sign mask for matrix A
  b | Matrix B
  sgn_y | Sign mask for matrix B
  acc1 | Accumulator 1 input
  acc2 | Accumulator 2 input

Returns
  Result of operation

## ◆ addmsc_elem_32_2() [2/8]

v32acc32 addmsc_elem_32_2 | ( | v64int8 | a,
|  | int | sgn_x,
|  | v64uint8 | b,
|  | int | sgn_y,
|  | v32acc32 | acc1,
|  | v32acc32 | acc2 )

Parameters

  a | Matrix A
  sgn_x | Sign mask for matrix A
  b | Matrix B
  sgn_y | Sign mask for matrix B
  acc1 | Accumulator 1 input
  acc2 | Accumulator 2 input

Returns
  Result of operation

## ◆ addmsc_elem_32_2() [3/8]

v32acc32 addmsc_elem_32_2 | ( | v64int8 | a,
|  | v64int8 | b,
|  | v32acc32 | acc1,
|  | v32acc32 | acc2 )

Parameters

  a | Matrix A
  b | Matrix B
  acc1 | Accumulator 1 input
  acc2 | Accumulator 2 input

Returns
  Result of operation

## ◆ addmsc_elem_32_2() [4/8]

v32acc32 addmsc_elem_32_2 | ( | v64int8 | a,
|  | v64uint8 | b,
|  | v32acc32 | acc1,
|  | v32acc32 | acc2 )

Parameters

  a | Matrix A
  b | Matrix B
  acc1 | Accumulator 1 input
  acc2 | Accumulator 2 input

Returns
  Result of operation

## ◆ addmsc_elem_32_2() [5/8]

v32acc32 addmsc_elem_32_2 | ( | v64uint8 | a,
|  | int | sgn_x,
|  | v64int8 | b,
|  | int | sgn_y,
|  | v32acc32 | acc1,
|  | v32acc32 | acc2 )

Parameters

  a | Matrix A
  sgn_x | Sign mask for matrix A
  b | Matrix B
  sgn_y | Sign mask for matrix B
  acc1 | Accumulator 1 input
  acc2 | Accumulator 2 input

Returns
  Result of operation

## ◆ addmsc_elem_32_2() [6/8]

v32acc32 addmsc_elem_32_2 | ( | v64uint8 | a,
|  | int | sgn_x,
|  | v64uint8 | b,
|  | int | sgn_y,
|  | v32acc32 | acc1,
|  | v32acc32 | acc2 )

Parameters

  a | Matrix A
  sgn_x | Sign mask for matrix A
  b | Matrix B
  sgn_y | Sign mask for matrix B
  acc1 | Accumulator 1 input
  acc2 | Accumulator 2 input

Returns
  Result of operation

## ◆ addmsc_elem_32_2() [7/8]

v32acc32 addmsc_elem_32_2 | ( | v64uint8 | a,
|  | v64int8 | b,
|  | v32acc32 | acc1,
|  | v32acc32 | acc2 )

Parameters

  a | Matrix A
  b | Matrix B
  acc1 | Accumulator 1 input
  acc2 | Accumulator 2 input

Returns
  Result of operation

## ◆ addmsc_elem_32_2() [8/8]

v32acc32 addmsc_elem_32_2 | ( | v64uint8 | a,
|  | v64uint8 | b,
|  | v32acc32 | acc1,
|  | v32acc32 | acc2 )

Parameters

  a | Matrix A
  b | Matrix B
  acc1 | Accumulator 1 input
  acc2 | Accumulator 2 input

Returns
  Result of operation

## ◆ addmsc_elem_32_2_conf() [1/8]

v32acc32 addmsc_elem_32_2_conf | ( | v64int8 | a,
|  | int | sgn_x,
|  | v64int8 | b,
|  | int | sgn_y,
|  | v32acc32 | acc1,
|  | v32acc32 | acc2,
|  | int | zero_acc1,
|  | int | shift16,
|  | int | sub_mul,
|  | int | sub_acc1,
|  | int | sub_acc2 )

Parameters

  a | Matrix A
  sgn_x | Sign mask for matrix A
  b | Matrix B
  sgn_y | Sign mask for matrix B
  acc1 | Accumulator 1 input
  acc2 | Accumulator 2 input
  zero_acc1 | Zeroing mask for acc1
  shift16 | Shift mask of input accumulator acc1
  sub_mul | Negation mask of multiplication result.
  sub_acc1 | Negation mask of acc1
  sub_acc2 | Negation mask of acc2

Returns
  Result of operation

## ◆ addmsc_elem_32_2_conf() [2/8]

v32acc32 addmsc_elem_32_2_conf | ( | v64int8 | a,
|  | int | sgn_x,
|  | v64uint8 | b,
|  | int | sgn_y,
|  | v32acc32 | acc1,
|  | v32acc32 | acc2,
|  | int | zero_acc1,
|  | int | shift16,
|  | int | sub_mul,
|  | int | sub_acc1,
|  | int | sub_acc2 )

Parameters

  a | Matrix A
  sgn_x | Sign mask for matrix A
  b | Matrix B
  sgn_y | Sign mask for matrix B
  acc1 | Accumulator 1 input
  acc2 | Accumulator 2 input
  zero_acc1 | Zeroing mask for acc1
  shift16 | Shift mask of input accumulator acc1
  sub_mul | Negation mask of multiplication result.
  sub_acc1 | Negation mask of acc1
  sub_acc2 | Negation mask of acc2

Returns
  Result of operation

## ◆ addmsc_elem_32_2_conf() [3/8]

v32acc32 addmsc_elem_32_2_conf | ( | v64int8 | a,
|  | v64int8 | b,
|  | v32acc32 | acc1,
|  | v32acc32 | acc2,
|  | int | zero_acc1,
|  | int | shift16,
|  | int | sub_mul,
|  | int | sub_acc1,
|  | int | sub_acc2 )

Parameters

  a | Matrix A
  b | Matrix B
  acc1 | Accumulator 1 input
  acc2 | Accumulator 2 input
  zero_acc1 | Zeroing mask for acc1
  shift16 | Shift mask of input accumulator acc1
  sub_mul | Negation mask of multiplication result
  sub_acc1 | Negation mask of acc1
  sub_acc2 | Negation mask of acc2

Returns
  Result of operation

## ◆ addmsc_elem_32_2_conf() [4/8]

v32acc32 addmsc_elem_32_2_conf | ( | v64int8 | a,
|  | v64uint8 | b,
|  | v32acc32 | acc1,
|  | v32acc32 | acc2,
|  | int | zero_acc1,
|  | int | shift16,
|  | int | sub_mul,
|  | int | sub_acc1,
|  | int | sub_acc2 )

Parameters

  a | Matrix A
  b | Matrix B
  acc1 | Accumulator 1 input
  acc2 | Accumulator 2 input
  zero_acc1 | Zeroing mask for acc1
  shift16 | Shift mask of input accumulator acc1
  sub_mul | Negation mask of multiplication result
  sub_acc1 | Negation mask of acc1
  sub_acc2 | Negation mask of acc2

Returns
  Result of operation

## ◆ addmsc_elem_32_2_conf() [5/8]

v32acc32 addmsc_elem_32_2_conf | ( | v64uint8 | a,
|  | int | sgn_x,
|  | v64int8 | b,
|  | int | sgn_y,
|  | v32acc32 | acc1,
|  | v32acc32 | acc2,
|  | int | zero_acc1,
|  | int | shift16,
|  | int | sub_mul,
|  | int | sub_acc1,
|  | int | sub_acc2 )

Parameters

  a | Matrix A
  sgn_x | Sign mask for matrix A
  b | Matrix B
  sgn_y | Sign mask for matrix B
  acc1 | Accumulator 1 input
  acc2 | Accumulator 2 input
  zero_acc1 | Zeroing mask for acc1
  shift16 | Shift mask of input accumulator acc1
  sub_mul | Negation mask of multiplication result.
  sub_acc1 | Negation mask of acc1
  sub_acc2 | Negation mask of acc2

Returns
  Result of operation

## ◆ addmsc_elem_32_2_conf() [6/8]

v32acc32 addmsc_elem_32_2_conf | ( | v64uint8 | a,
|  | int | sgn_x,
|  | v64uint8 | b,
|  | int | sgn_y,
|  | v32acc32 | acc1,
|  | v32acc32 | acc2,
|  | int | zero_acc1,
|  | int | shift16,
|  | int | sub_mul,
|  | int | sub_acc1,
|  | int | sub_acc2 )

Parameters

  a | Matrix A
  sgn_x | Sign mask for matrix A
  b | Matrix B
  sgn_y | Sign mask for matrix B
  acc1 | Accumulator 1 input
  acc2 | Accumulator 2 input
  zero_acc1 | Zeroing mask for acc1
  shift16 | Shift mask of input accumulator acc1
  sub_mul | Negation mask of multiplication result.
  sub_acc1 | Negation mask of acc1
  sub_acc2 | Negation mask of acc2

Returns
  Result of operation

## ◆ addmsc_elem_32_2_conf() [7/8]

v32acc32 addmsc_elem_32_2_conf | ( | v64uint8 | a,
|  | v64int8 | b,
|  | v32acc32 | acc1,
|  | v32acc32 | acc2,
|  | int | zero_acc1,
|  | int | shift16,
|  | int | sub_mul,
|  | int | sub_acc1,
|  | int | sub_acc2 )

Parameters

  a | Matrix A
  b | Matrix B
  acc1 | Accumulator 1 input
  acc2 | Accumulator 2 input
  zero_acc1 | Zeroing mask for acc1
  shift16 | Shift mask of input accumulator acc1
  sub_mul | Negation mask of multiplication result
  sub_acc1 | Negation mask of acc1
  sub_acc2 | Negation mask of acc2

Returns
  Result of operation

## ◆ addmsc_elem_32_2_conf() [8/8]

v32acc32 addmsc_elem_32_2_conf | ( | v64uint8 | a,
|  | v64uint8 | b,
|  | v32acc32 | acc1,
|  | v32acc32 | acc2,
|  | int | zero_acc1,
|  | int | shift16,
|  | int | sub_mul,
|  | int | sub_acc1,
|  | int | sub_acc2 )

Parameters

  a | Matrix A
  b | Matrix B
  acc1 | Accumulator 1 input
  acc2 | Accumulator 2 input
  zero_acc1 | Zeroing mask for acc1
  shift16 | Shift mask of input accumulator acc1
  sub_mul | Negation mask of multiplication result
  sub_acc1 | Negation mask of acc1
  sub_acc2 | Negation mask of acc2

Returns
  Result of operation

## ◆ mac_4x8_8x8() [1/8]

v32acc32 mac_4x8_8x8 | ( | v64int8 | a,
|  | int | sgn_x,
|  | v64int8 | b,
|  | int | sgn_y,
|  | v32acc32 | acc1 )

Parameters

  a | Matrix A
  sgn_x | Sign mask for matrix A
  b | Matrix B
  sgn_y | Sign mask for matrix B
  acc1 | Accumulator 1 input

Returns
  Result of operation

## ◆ mac_4x8_8x8() [2/8]

v32acc32 mac_4x8_8x8 | ( | v64int8 | a,
|  | int | sgn_x,
|  | v64uint8 | b,
|  | int | sgn_y,
|  | v32acc32 | acc1 )

Parameters

  a | Matrix A
  sgn_x | Sign mask for matrix A
  b | Matrix B
  sgn_y | Sign mask for matrix B
  acc1 | Accumulator 1 input

Returns
  Result of operation

## ◆ mac_4x8_8x8() [3/8]

v32acc32 mac_4x8_8x8 | ( | v64int8 | a,
|  | v64int8 | b,
|  | v32acc32 | acc1 )

Parameters

  a | Matrix A
  b | Matrix B
  acc1 | Accumulator 1 input

Returns
  Result of operation

## ◆ mac_4x8_8x8() [4/8]

v32acc32 mac_4x8_8x8 | ( | v64int8 | a,
|  | v64uint8 | b,
|  | v32acc32 | acc1 )

Parameters

  a | Matrix A
  b | Matrix B
  acc1 | Accumulator 1 input

Returns
  Result of operation

## ◆ mac_4x8_8x8() [5/8]

v32acc32 mac_4x8_8x8 | ( | v64uint8 | a,
|  | int | sgn_x,
|  | v64int8 | b,
|  | int | sgn_y,
|  | v32acc32 | acc1 )

Parameters

  a | Matrix A
  sgn_x | Sign mask for matrix A
  b | Matrix B
  sgn_y | Sign mask for matrix B
  acc1 | Accumulator 1 input

Returns
  Result of operation

## ◆ mac_4x8_8x8() [6/8]

v32acc32 mac_4x8_8x8 | ( | v64uint8 | a,
|  | int | sgn_x,
|  | v64uint8 | b,
|  | int | sgn_y,
|  | v32acc32 | acc1 )

Parameters

  a | Matrix A
  sgn_x | Sign mask for matrix A
  b | Matrix B
  sgn_y | Sign mask for matrix B
  acc1 | Accumulator 1 input

Returns
  Result of operation

## ◆ mac_4x8_8x8() [7/8]

v32acc32 mac_4x8_8x8 | ( | v64uint8 | a,
|  | v64int8 | b,
|  | v32acc32 | acc1 )

Parameters

  a | Matrix A
  b | Matrix B
  acc1 | Accumulator 1 input

Returns
  Result of operation

## ◆ mac_4x8_8x8() [8/8]

v32acc32 mac_4x8_8x8 | ( | v64uint8 | a,
|  | v64uint8 | b,
|  | v32acc32 | acc1 )

Parameters

  a | Matrix A
  b | Matrix B
  acc1 | Accumulator 1 input

Returns
  Result of operation

## ◆ mac_4x8_8x8_conf() [1/8]

v32acc32 mac_4x8_8x8_conf | ( | v64int8 | a,
|  | int | sgn_x,
|  | v64int8 | b,
|  | int | sgn_y,
|  | v32acc32 | acc1,
|  | int | zero_acc1,
|  | int | shift16,
|  | int | sub_mul,
|  | int | sub_acc1 )

Parameters

  a | Matrix A
  sgn_x | Sign mask for matrix A
  b | Matrix B
  sgn_y | Sign mask for matrix B
  acc1 | Accumulator 1 input
  zero_acc1 | Zeroing mask for acc1
  shift16 | Shift mask of input accumulator acc1
  sub_mul | Negation mask of multiplication result
  sub_acc1 | Negation mask of acc1

Returns
  Result of operation

## ◆ mac_4x8_8x8_conf() [2/8]

v32acc32 mac_4x8_8x8_conf | ( | v64int8 | a,
|  | int | sgn_x,
|  | v64uint8 | b,
|  | int | sgn_y,
|  | v32acc32 | acc1,
|  | int | zero_acc1,
|  | int | shift16,
|  | int | sub_mul,
|  | int | sub_acc1 )

Parameters

  a | Matrix A
  sgn_x | Sign mask for matrix A
  b | Matrix B
  sgn_y | Sign mask for matrix B
  acc1 | Accumulator 1 input
  zero_acc1 | Zeroing mask for acc1
  shift16 | Shift mask of input accumulator acc1
  sub_mul | Negation mask of multiplication result
  sub_acc1 | Negation mask of acc1

Returns
  Result of operation

## ◆ mac_4x8_8x8_conf() [3/8]

v32acc32 mac_4x8_8x8_conf | ( | v64int8 | a,
|  | v64int8 | b,
|  | v32acc32 | acc1,
|  | int | zero_acc1,
|  | int | shift16,
|  | int | sub_mul,
|  | int | sub_acc1 )

Parameters

  a | Matrix A
  b | Matrix B
  acc1 | Accumulator 1 input
  zero_acc1 | Zeroing mask for acc1
  shift16 | Shift mask of input accumulator acc1
  sub_mul | Negation mask of multiplication result
  sub_acc1 | Negation mask of acc1

Returns
  Result of operation

## ◆ mac_4x8_8x8_conf() [4/8]

v32acc32 mac_4x8_8x8_conf | ( | v64int8 | a,
|  | v64uint8 | b,
|  | v32acc32 | acc1,
|  | int | zero_acc1,
|  | int | shift16,
|  | int | sub_mul,
|  | int | sub_acc1 )

Parameters

  a | Matrix A
  b | Matrix B
  acc1 | Accumulator 1 input
  zero_acc1 | Zeroing mask for acc1
  shift16 | Shift mask of input accumulator acc1
  sub_mul | Negation mask of multiplication result
  sub_acc1 | Negation mask of acc1

Returns
  Result of operation

## ◆ mac_4x8_8x8_conf() [5/8]

v32acc32 mac_4x8_8x8_conf | ( | v64uint8 | a,
|  | int | sgn_x,
|  | v64int8 | b,
|  | int | sgn_y,
|  | v32acc32 | acc1,
|  | int | zero_acc1,
|  | int | shift16,
|  | int | sub_mul,
|  | int | sub_acc1 )

Parameters

  a | Matrix A
  sgn_x | Sign mask for matrix A
  b | Matrix B
  sgn_y | Sign mask for matrix B
  acc1 | Accumulator 1 input
  zero_acc1 | Zeroing mask for acc1
  shift16 | Shift mask of input accumulator acc1
  sub_mul | Negation mask of multiplication result
  sub_acc1 | Negation mask of acc1

Returns
  Result of operation

## ◆ mac_4x8_8x8_conf() [6/8]

v32acc32 mac_4x8_8x8_conf | ( | v64uint8 | a,
|  | int | sgn_x,
|  | v64uint8 | b,
|  | int | sgn_y,
|  | v32acc32 | acc1,
|  | int | zero_acc1,
|  | int | shift16,
|  | int | sub_mul,
|  | int | sub_acc1 )

Parameters

  a | Matrix A
  sgn_x | Sign mask for matrix A
  b | Matrix B
  sgn_y | Sign mask for matrix B
  acc1 | Accumulator 1 input
  zero_acc1 | Zeroing mask for acc1
  shift16 | Shift mask of input accumulator acc1
  sub_mul | Negation mask of multiplication result
  sub_acc1 | Negation mask of acc1

Returns
  Result of operation

## ◆ mac_4x8_8x8_conf() [7/8]

v32acc32 mac_4x8_8x8_conf | ( | v64uint8 | a,
|  | v64int8 | b,
|  | v32acc32 | acc1,
|  | int | zero_acc1,
|  | int | shift16,
|  | int | sub_mul,
|  | int | sub_acc1 )

Parameters

  a | Matrix A
  b | Matrix B
  acc1 | Accumulator 1 input
  zero_acc1 | Zeroing mask for acc1
  shift16 | Shift mask of input accumulator acc1
  sub_mul | Negation mask of multiplication result
  sub_acc1 | Negation mask of acc1

Returns
  Result of operation

## ◆ mac_4x8_8x8_conf() [8/8]

v32acc32 mac_4x8_8x8_conf | ( | v64uint8 | a,
|  | v64uint8 | b,
|  | v32acc32 | acc1,
|  | int | zero_acc1,
|  | int | shift16,
|  | int | sub_mul,
|  | int | sub_acc1 )

Parameters

  a | Matrix A
  b | Matrix B
  acc1 | Accumulator 1 input
  zero_acc1 | Zeroing mask for acc1
  shift16 | Shift mask of input accumulator acc1
  sub_mul | Negation mask of multiplication result
  sub_acc1 | Negation mask of acc1

Returns
  Result of operation

## ◆ mac_conv_32x8() [1/8]

v32acc32 mac_conv_32x8 | ( | v64int8 | a,
|  | int | sgn_x,
|  | v64int8 | b,
|  | int | sgn_y,
|  | v32acc32 | acc1 )

Parameters

  a | Matrix A
  sgn_x | Sign mask for matrix A
  b | Matrix B
  sgn_y | Sign mask for matrix B
  acc1 | Accumulator 1 input

Returns
  Result of operation

## ◆ mac_conv_32x8() [2/8]

v32acc32 mac_conv_32x8 | ( | v64int8 | a,
|  | int | sgn_x,
|  | v64uint8 | b,
|  | int | sgn_y,
|  | v32acc32 | acc1 )

Parameters

  a | Matrix A
  sgn_x | Sign mask for matrix A
  b | Matrix B
  sgn_y | Sign mask for matrix B
  acc1 | Accumulator 1 input

Returns
  Result of operation

## ◆ mac_conv_32x8() [3/8]

v32acc32 mac_conv_32x8 | ( | v64int8 | a,
|  | v64int8 | b,
|  | v32acc32 | acc1 )

Parameters

  a | Matrix A
  b | Matrix B
  acc1 | Accumulator 1 input

Returns
  Result of operation

## ◆ mac_conv_32x8() [4/8]

v32acc32 mac_conv_32x8 | ( | v64int8 | a,
|  | v64uint8 | b,
|  | v32acc32 | acc1 )

Parameters

  a | Matrix A
  b | Matrix B
  acc1 | Accumulator 1 input

Returns
  Result of operation

## ◆ mac_conv_32x8() [5/8]

v32acc32 mac_conv_32x8 | ( | v64uint8 | a,
|  | int | sgn_x,
|  | v64int8 | b,
|  | int | sgn_y,
|  | v32acc32 | acc1 )

Parameters

  a | Matrix A
  sgn_x | Sign mask for matrix A
  b | Matrix B
  sgn_y | Sign mask for matrix B
  acc1 | Accumulator 1 input

Returns
  Result of operation

## ◆ mac_conv_32x8() [6/8]

v32acc32 mac_conv_32x8 | ( | v64uint8 | a,
|  | int | sgn_x,
|  | v64uint8 | b,
|  | int | sgn_y,
|  | v32acc32 | acc1 )

Parameters

  a | Matrix A
  sgn_x | Sign mask for matrix A
  b | Matrix B
  sgn_y | Sign mask for matrix B
  acc1 | Accumulator 1 input

Returns
  Result of operation

## ◆ mac_conv_32x8() [7/8]

v32acc32 mac_conv_32x8 | ( | v64uint8 | a,
|  | v64int8 | b,
|  | v32acc32 | acc1 )

Parameters

  a | Matrix A
  b | Matrix B
  acc1 | Accumulator 1 input

Returns
  Result of operation

## ◆ mac_conv_32x8() [8/8]

v32acc32 mac_conv_32x8 | ( | v64uint8 | a,
|  | v64uint8 | b,
|  | v32acc32 | acc1 )

Parameters

  a | Matrix A
  b | Matrix B
  acc1 | Accumulator 1 input

Returns
  Result of operation

## ◆ mac_conv_32x8_conf() [1/8]

v32acc32 mac_conv_32x8_conf | ( | v64int8 | a,
|  | int | sgn_x,
|  | v64int8 | b,
|  | int | sgn_y,
|  | v32acc32 | acc1,
|  | int | zero_acc1,
|  | int | shift16,
|  | int | sub_mul,
|  | int | sub_acc1 )

Parameters

  a | Matrix A
  sgn_x | Sign mask for matrix A
  b | Matrix B
  sgn_y | Sign mask for matrix B
  acc1 | Accumulator 1 input
  zero_acc1 | Zeroing mask for acc1
  shift16 | Shift mask of input accumulator acc1
  sub_mul | Negation mask of multiplication result
  sub_acc1 | Negation mask of acc1

Returns
  Result of operation

## ◆ mac_conv_32x8_conf() [2/8]

v32acc32 mac_conv_32x8_conf | ( | v64int8 | a,
|  | int | sgn_x,
|  | v64uint8 | b,
|  | int | sgn_y,
|  | v32acc32 | acc1,
|  | int | zero_acc1,
|  | int | shift16,
|  | int | sub_mul,
|  | int | sub_acc1 )

Parameters

  a | Matrix A
  sgn_x | Sign mask for matrix A
  b | Matrix B
  sgn_y | Sign mask for matrix B
  acc1 | Accumulator 1 input
  zero_acc1 | Zeroing mask for acc1
  shift16 | Shift mask of input accumulator acc1
  sub_mul | Negation mask of multiplication result
  sub_acc1 | Negation mask of acc1

Returns
  Result of operation

## ◆ mac_conv_32x8_conf() [3/8]

v32acc32 mac_conv_32x8_conf | ( | v64int8 | a,
|  | v64int8 | b,
|  | v32acc32 | acc1,
|  | int | zero_acc1,
|  | int | shift16,
|  | int | sub_mul,
|  | int | sub_acc1 )

Parameters

  a | Matrix A
  b | Matrix B
  acc1 | Accumulator 1 input
  zero_acc1 | Zeroing mask for acc1
  shift16 | Shift mask of input accumulator acc1
  sub_mul | Negation mask of multiplication result
  sub_acc1 | Negation mask of acc1

Returns
  Result of operation

## ◆ mac_conv_32x8_conf() [4/8]

v32acc32 mac_conv_32x8_conf | ( | v64int8 | a,
|  | v64uint8 | b,
|  | v32acc32 | acc1,
|  | int | zero_acc1,
|  | int | shift16,
|  | int | sub_mul,
|  | int | sub_acc1 )

Parameters

  a | Matrix A
  b | Matrix B
  acc1 | Accumulator 1 input
  zero_acc1 | Zeroing mask for acc1
  shift16 | Shift mask of input accumulator acc1
  sub_mul | Negation mask of multiplication result
  sub_acc1 | Negation mask of acc1

Returns
  Result of operation

## ◆ mac_conv_32x8_conf() [5/8]

v32acc32 mac_conv_32x8_conf | ( | v64uint8 | a,
|  | int | sgn_x,
|  | v64int8 | b,
|  | int | sgn_y,
|  | v32acc32 | acc1,
|  | int | zero_acc1,
|  | int | shift16,
|  | int | sub_mul,
|  | int | sub_acc1 )

Parameters

  a | Matrix A
  sgn_x | Sign mask for matrix A
  b | Matrix B
  sgn_y | Sign mask for matrix B
  acc1 | Accumulator 1 input
  zero_acc1 | Zeroing mask for acc1
  shift16 | Shift mask of input accumulator acc1
  sub_mul | Negation mask of multiplication result
  sub_acc1 | Negation mask of acc1

Returns
  Result of operation

## ◆ mac_conv_32x8_conf() [6/8]

v32acc32 mac_conv_32x8_conf | ( | v64uint8 | a,
|  | int | sgn_x,
|  | v64uint8 | b,
|  | int | sgn_y,
|  | v32acc32 | acc1,
|  | int | zero_acc1,
|  | int | shift16,
|  | int | sub_mul,
|  | int | sub_acc1 )

Parameters

  a | Matrix A
  sgn_x | Sign mask for matrix A
  b | Matrix B
  sgn_y | Sign mask for matrix B
  acc1 | Accumulator 1 input
  zero_acc1 | Zeroing mask for acc1
  shift16 | Shift mask of input accumulator acc1
  sub_mul | Negation mask of multiplication result
  sub_acc1 | Negation mask of acc1

Returns
  Result of operation

## ◆ mac_conv_32x8_conf() [7/8]

v32acc32 mac_conv_32x8_conf | ( | v64uint8 | a,
|  | v64int8 | b,
|  | v32acc32 | acc1,
|  | int | zero_acc1,
|  | int | shift16,
|  | int | sub_mul,
|  | int | sub_acc1 )

Parameters

  a | Matrix A
  b | Matrix B
  acc1 | Accumulator 1 input
  zero_acc1 | Zeroing mask for acc1
  shift16 | Shift mask of input accumulator acc1
  sub_mul | Negation mask of multiplication result
  sub_acc1 | Negation mask of acc1

Returns
  Result of operation

## ◆ mac_conv_32x8_conf() [8/8]

v32acc32 mac_conv_32x8_conf | ( | v64uint8 | a,
|  | v64uint8 | b,
|  | v32acc32 | acc1,
|  | int | zero_acc1,
|  | int | shift16,
|  | int | sub_mul,
|  | int | sub_acc1 )

Parameters

  a | Matrix A
  b | Matrix B
  acc1 | Accumulator 1 input
  zero_acc1 | Zeroing mask for acc1
  shift16 | Shift mask of input accumulator acc1
  sub_mul | Negation mask of multiplication result
  sub_acc1 | Negation mask of acc1

Returns
  Result of operation

## ◆ mac_conv_4x4_8ch() [1/8]

v32acc32 mac_conv_4x4_8ch | ( | v64int8 | a,
|  | int | sgn_x,
|  | v64int8 | b,
|  | int | sgn_y,
|  | v32acc32 | acc1 )

Parameters

  a | Matrix A
  sgn_x | Sign mask for matrix A
  b | Matrix B
  sgn_y | Sign mask for matrix B
  acc1 | Accumulator 1 input

Returns
  Result of operation

## ◆ mac_conv_4x4_8ch() [2/8]

v32acc32 mac_conv_4x4_8ch | ( | v64int8 | a,
|  | int | sgn_x,
|  | v64uint8 | b,
|  | int | sgn_y,
|  | v32acc32 | acc1 )

Parameters

  a | Matrix A
  sgn_x | Sign mask for matrix A
  b | Matrix B
  sgn_y | Sign mask for matrix B
  acc1 | Accumulator 1 input

Returns
  Result of operation

## ◆ mac_conv_4x4_8ch() [3/8]

v32acc32 mac_conv_4x4_8ch | ( | v64int8 | a,
|  | v64int8 | b,
|  | v32acc32 | acc1 )

Parameters

  a | Matrix A
  b | Matrix B
  acc1 | Accumulator 1 input

Returns
  Result of operation

## ◆ mac_conv_4x4_8ch() [4/8]

v32acc32 mac_conv_4x4_8ch | ( | v64int8 | a,
|  | v64uint8 | b,
|  | v32acc32 | acc1 )

Parameters

  a | Matrix A
  b | Matrix B
  acc1 | Accumulator 1 input

Returns
  Result of operation

## ◆ mac_conv_4x4_8ch() [5/8]

v32acc32 mac_conv_4x4_8ch | ( | v64uint8 | a,
|  | int | sgn_x,
|  | v64int8 | b,
|  | int | sgn_y,
|  | v32acc32 | acc1 )

Parameters

  a | Matrix A
  sgn_x | Sign mask for matrix A
  b | Matrix B
  sgn_y | Sign mask for matrix B
  acc1 | Accumulator 1 input

Returns
  Result of operation

## ◆ mac_conv_4x4_8ch() [6/8]

v32acc32 mac_conv_4x4_8ch | ( | v64uint8 | a,
|  | int | sgn_x,
|  | v64uint8 | b,
|  | int | sgn_y,
|  | v32acc32 | acc1 )

Parameters

  a | Matrix A
  sgn_x | Sign mask for matrix A
  b | Matrix B
  sgn_y | Sign mask for matrix B
  acc1 | Accumulator 1 input

Returns
  Result of operation

## ◆ mac_conv_4x4_8ch() [7/8]

v32acc32 mac_conv_4x4_8ch | ( | v64uint8 | a,
|  | v64int8 | b,
|  | v32acc32 | acc1 )

Parameters

  a | Matrix A
  b | Matrix B
  acc1 | Accumulator 1 input

Returns
  Result of operation

## ◆ mac_conv_4x4_8ch() [8/8]

v32acc32 mac_conv_4x4_8ch | ( | v64uint8 | a,
|  | v64uint8 | b,
|  | v32acc32 | acc1 )

Parameters

  a | Matrix A
  b | Matrix B
  acc1 | Accumulator 1 input

Returns
  Result of operation

## ◆ mac_conv_4x4_8ch_conf() [1/8]

v32acc32 mac_conv_4x4_8ch_conf | ( | v64int8 | a,
|  | int | sgn_x,
|  | v64int8 | b,
|  | int | sgn_y,
|  | v32acc32 | acc1,
|  | int | zero_acc1,
|  | int | shift16,
|  | int | sub_mul,
|  | int | sub_acc1 )

Parameters

  a | Matrix A
  sgn_x | Sign mask for matrix A
  b | Matrix B
  sgn_y | Sign mask for matrix B
  acc1 | Accumulator 1 input
  zero_acc1 | Zeroing mask for acc1
  shift16 | Shift mask of input accumulator acc1
  sub_mul | Negation mask of multiplication result
  sub_acc1 | Negation mask of acc1

Returns
  Result of operation

## ◆ mac_conv_4x4_8ch_conf() [2/8]

v32acc32 mac_conv_4x4_8ch_conf | ( | v64int8 | a,
|  | int | sgn_x,
|  | v64uint8 | b,
|  | int | sgn_y,
|  | v32acc32 | acc1,
|  | int | zero_acc1,
|  | int | shift16,
|  | int | sub_mul,
|  | int | sub_acc1 )

Parameters

  a | Matrix A
  sgn_x | Sign mask for matrix A
  b | Matrix B
  sgn_y | Sign mask for matrix B
  acc1 | Accumulator 1 input
  zero_acc1 | Zeroing mask for acc1
  shift16 | Shift mask of input accumulator acc1
  sub_mul | Negation mask of multiplication result
  sub_acc1 | Negation mask of acc1

Returns
  Result of operation

## ◆ mac_conv_4x4_8ch_conf() [3/8]

v32acc32 mac_conv_4x4_8ch_conf | ( | v64int8 | a,
|  | v64int8 | b,
|  | v32acc32 | acc1,
|  | int | zero_acc1,
|  | int | shift16,
|  | int | sub_mul,
|  | int | sub_acc1 )

Parameters

  a | Matrix A
  b | Matrix B
  acc1 | Accumulator 1 input
  zero_acc1 | Zeroing mask for acc1
  shift16 | Shift mask of input accumulator acc1
  sub_mul | Negation mask of multiplication result
  sub_acc1 | Negation mask of acc1

Returns
  Result of operation

## ◆ mac_conv_4x4_8ch_conf() [4/8]

v32acc32 mac_conv_4x4_8ch_conf | ( | v64int8 | a,
|  | v64uint8 | b,
|  | v32acc32 | acc1,
|  | int | zero_acc1,
|  | int | shift16,
|  | int | sub_mul,
|  | int | sub_acc1 )

Parameters

  a | Matrix A
  b | Matrix B
  acc1 | Accumulator 1 input
  zero_acc1 | Zeroing mask for acc1
  shift16 | Shift mask of input accumulator acc1
  sub_mul | Negation mask of multiplication result
  sub_acc1 | Negation mask of acc1

Returns
  Result of operation

## ◆ mac_conv_4x4_8ch_conf() [5/8]

v32acc32 mac_conv_4x4_8ch_conf | ( | v64uint8 | a,
|  | int | sgn_x,
|  | v64int8 | b,
|  | int | sgn_y,
|  | v32acc32 | acc1,
|  | int | zero_acc1,
|  | int | shift16,
|  | int | sub_mul,
|  | int | sub_acc1 )

Parameters

  a | Matrix A
  sgn_x | Sign mask for matrix A
  b | Matrix B
  sgn_y | Sign mask for matrix B
  acc1 | Accumulator 1 input
  zero_acc1 | Zeroing mask for acc1
  shift16 | Shift mask of input accumulator acc1
  sub_mul | Negation mask of multiplication result
  sub_acc1 | Negation mask of acc1

Returns
  Result of operation

## ◆ mac_conv_4x4_8ch_conf() [6/8]

v32acc32 mac_conv_4x4_8ch_conf | ( | v64uint8 | a,
|  | int | sgn_x,
|  | v64uint8 | b,
|  | int | sgn_y,
|  | v32acc32 | acc1,
|  | int | zero_acc1,
|  | int | shift16,
|  | int | sub_mul,
|  | int | sub_acc1 )

Parameters

  a | Matrix A
  sgn_x | Sign mask for matrix A
  b | Matrix B
  sgn_y | Sign mask for matrix B
  acc1 | Accumulator 1 input
  zero_acc1 | Zeroing mask for acc1
  shift16 | Shift mask of input accumulator acc1
  sub_mul | Negation mask of multiplication result
  sub_acc1 | Negation mask of acc1

Returns
  Result of operation

## ◆ mac_conv_4x4_8ch_conf() [7/8]

v32acc32 mac_conv_4x4_8ch_conf | ( | v64uint8 | a,
|  | v64int8 | b,
|  | v32acc32 | acc1,
|  | int | zero_acc1,
|  | int | shift16,
|  | int | sub_mul,
|  | int | sub_acc1 )

Parameters

  a | Matrix A
  b | Matrix B
  acc1 | Accumulator 1 input
  zero_acc1 | Zeroing mask for acc1
  shift16 | Shift mask of input accumulator acc1
  sub_mul | Negation mask of multiplication result
  sub_acc1 | Negation mask of acc1

Returns
  Result of operation

## ◆ mac_conv_4x4_8ch_conf() [8/8]

v32acc32 mac_conv_4x4_8ch_conf | ( | v64uint8 | a,
|  | v64uint8 | b,
|  | v32acc32 | acc1,
|  | int | zero_acc1,
|  | int | shift16,
|  | int | sub_mul,
|  | int | sub_acc1 )

Parameters

  a | Matrix A
  b | Matrix B
  acc1 | Accumulator 1 input
  zero_acc1 | Zeroing mask for acc1
  shift16 | Shift mask of input accumulator acc1
  sub_mul | Negation mask of multiplication result
  sub_acc1 | Negation mask of acc1

Returns
  Result of operation

## ◆ mac_conv_8x8_4ch() [1/8]

v32acc32 mac_conv_8x8_4ch | ( | v64int8 | a,
|  | int | sgn_x,
|  | v64int8 | b,
|  | int | sgn_y,
|  | v32acc32 | acc1 )

Parameters

  a | Matrix A
  sgn_x | Sign mask for matrix A
  b | Matrix B
  sgn_y | Sign mask for matrix B
  acc1 | Accumulator 1 input

Returns
  Result of operation

## ◆ mac_conv_8x8_4ch() [2/8]

v32acc32 mac_conv_8x8_4ch | ( | v64int8 | a,
|  | int | sgn_x,
|  | v64uint8 | b,
|  | int | sgn_y,
|  | v32acc32 | acc1 )

Parameters

  a | Matrix A
  sgn_x | Sign mask for matrix A
  b | Matrix B
  sgn_y | Sign mask for matrix B
  acc1 | Accumulator 1 input

Returns
  Result of operation

## ◆ mac_conv_8x8_4ch() [3/8]

v32acc32 mac_conv_8x8_4ch | ( | v64int8 | a,
|  | v64int8 | b,
|  | v32acc32 | acc1 )

Parameters

  a | Matrix A
  b | Matrix B
  acc1 | Accumulator 1 input

Returns
  Result of operation

## ◆ mac_conv_8x8_4ch() [4/8]

v32acc32 mac_conv_8x8_4ch | ( | v64int8 | a,
|  | v64uint8 | b,
|  | v32acc32 | acc1 )

Parameters

  a | Matrix A
  b | Matrix B
  acc1 | Accumulator 1 input

Returns
  Result of operation

## ◆ mac_conv_8x8_4ch() [5/8]

v32acc32 mac_conv_8x8_4ch | ( | v64uint8 | a,
|  | int | sgn_x,
|  | v64int8 | b,
|  | int | sgn_y,
|  | v32acc32 | acc1 )

Parameters

  a | Matrix A
  sgn_x | Sign mask for matrix A
  b | Matrix B
  sgn_y | Sign mask for matrix B
  acc1 | Accumulator 1 input

Returns
  Result of operation

## ◆ mac_conv_8x8_4ch() [6/8]

v32acc32 mac_conv_8x8_4ch | ( | v64uint8 | a,
|  | int | sgn_x,
|  | v64uint8 | b,
|  | int | sgn_y,
|  | v32acc32 | acc1 )

Parameters

  a | Matrix A
  sgn_x | Sign mask for matrix A
  b | Matrix B
  sgn_y | Sign mask for matrix B
  acc1 | Accumulator 1 input

Returns
  Result of operation

## ◆ mac_conv_8x8_4ch() [7/8]

v32acc32 mac_conv_8x8_4ch | ( | v64uint8 | a,
|  | v64int8 | b,
|  | v32acc32 | acc1 )

Parameters

  a | Matrix A
  b | Matrix B
  acc1 | Accumulator 1 input

Returns
  Result of operation

## ◆ mac_conv_8x8_4ch() [8/8]

v32acc32 mac_conv_8x8_4ch | ( | v64uint8 | a,
|  | v64uint8 | b,
|  | v32acc32 | acc1 )

Parameters

  a | Matrix A
  b | Matrix B
  acc1 | Accumulator 1 input

Returns
  Result of operation

## ◆ mac_conv_8x8_4ch_conf() [1/8]

v32acc32 mac_conv_8x8_4ch_conf | ( | v64int8 | a,
|  | int | sgn_x,
|  | v64int8 | b,
|  | int | sgn_y,
|  | v32acc32 | acc1,
|  | int | zero_acc1,
|  | int | shift16,
|  | int | sub_mul,
|  | int | sub_acc1 )

Parameters

  a | Matrix A
  sgn_x | Sign mask for matrix A
  b | Matrix B
  sgn_y | Sign mask for matrix B
  acc1 | Accumulator 1 input
  zero_acc1 | Zeroing mask for acc1
  shift16 | Shift mask of input accumulator acc1
  sub_mul | Negation mask of multiplication result
  sub_acc1 | Negation mask of acc1

Returns
  Result of operation

## ◆ mac_conv_8x8_4ch_conf() [2/8]

v32acc32 mac_conv_8x8_4ch_conf | ( | v64int8 | a,
|  | int | sgn_x,
|  | v64uint8 | b,
|  | int | sgn_y,
|  | v32acc32 | acc1,
|  | int | zero_acc1,
|  | int | shift16,
|  | int | sub_mul,
|  | int | sub_acc1 )

Parameters

  a | Matrix A
  sgn_x | Sign mask for matrix A
  b | Matrix B
  sgn_y | Sign mask for matrix B
  acc1 | Accumulator 1 input
  zero_acc1 | Zeroing mask for acc1
  shift16 | Shift mask of input accumulator acc1
  sub_mul | Negation mask of multiplication result
  sub_acc1 | Negation mask of acc1

Returns
  Result of operation

## ◆ mac_conv_8x8_4ch_conf() [3/8]

v32acc32 mac_conv_8x8_4ch_conf | ( | v64int8 | a,
|  | v64int8 | b,
|  | v32acc32 | acc1,
|  | int | zero_acc1,
|  | int | shift16,
|  | int | sub_mul,
|  | int | sub_acc1 )

Parameters

  a | Matrix A
  b | Matrix B
  acc1 | Accumulator 1 input
  zero_acc1 | Zeroing mask for acc1
  shift16 | Shift mask of input accumulator acc1
  sub_mul | Negation mask of multiplication result
  sub_acc1 | Negation mask of acc1

Returns
  Result of operation

## ◆ mac_conv_8x8_4ch_conf() [4/8]

v32acc32 mac_conv_8x8_4ch_conf | ( | v64int8 | a,
|  | v64uint8 | b,
|  | v32acc32 | acc1,
|  | int | zero_acc1,
|  | int | shift16,
|  | int | sub_mul,
|  | int | sub_acc1 )

Parameters

  a | Matrix A
  b | Matrix B
  acc1 | Accumulator 1 input
  zero_acc1 | Zeroing mask for acc1
  shift16 | Shift mask of input accumulator acc1
  sub_mul | Negation mask of multiplication result
  sub_acc1 | Negation mask of acc1

Returns
  Result of operation

## ◆ mac_conv_8x8_4ch_conf() [5/8]

v32acc32 mac_conv_8x8_4ch_conf | ( | v64uint8 | a,
|  | int | sgn_x,
|  | v64int8 | b,
|  | int | sgn_y,
|  | v32acc32 | acc1,
|  | int | zero_acc1,
|  | int | shift16,
|  | int | sub_mul,
|  | int | sub_acc1 )

Parameters

  a | Matrix A
  sgn_x | Sign mask for matrix A
  b | Matrix B
  sgn_y | Sign mask for matrix B
  acc1 | Accumulator 1 input
  zero_acc1 | Zeroing mask for acc1
  shift16 | Shift mask of input accumulator acc1
  sub_mul | Negation mask of multiplication result
  sub_acc1 | Negation mask of acc1

Returns
  Result of operation

## ◆ mac_conv_8x8_4ch_conf() [6/8]

v32acc32 mac_conv_8x8_4ch_conf | ( | v64uint8 | a,
|  | int | sgn_x,
|  | v64uint8 | b,
|  | int | sgn_y,
|  | v32acc32 | acc1,
|  | int | zero_acc1,
|  | int | shift16,
|  | int | sub_mul,
|  | int | sub_acc1 )

Parameters

  a | Matrix A
  sgn_x | Sign mask for matrix A
  b | Matrix B
  sgn_y | Sign mask for matrix B
  acc1 | Accumulator 1 input
  zero_acc1 | Zeroing mask for acc1
  shift16 | Shift mask of input accumulator acc1
  sub_mul | Negation mask of multiplication result
  sub_acc1 | Negation mask of acc1

Returns
  Result of operation

## ◆ mac_conv_8x8_4ch_conf() [7/8]

v32acc32 mac_conv_8x8_4ch_conf | ( | v64uint8 | a,
|  | v64int8 | b,
|  | v32acc32 | acc1,
|  | int | zero_acc1,
|  | int | shift16,
|  | int | sub_mul,
|  | int | sub_acc1 )

Parameters

  a | Matrix A
  b | Matrix B
  acc1 | Accumulator 1 input
  zero_acc1 | Zeroing mask for acc1
  shift16 | Shift mask of input accumulator acc1
  sub_mul | Negation mask of multiplication result
  sub_acc1 | Negation mask of acc1

Returns
  Result of operation

## ◆ mac_conv_8x8_4ch_conf() [8/8]

v32acc32 mac_conv_8x8_4ch_conf | ( | v64uint8 | a,
|  | v64uint8 | b,
|  | v32acc32 | acc1,
|  | int | zero_acc1,
|  | int | shift16,
|  | int | sub_mul,
|  | int | sub_acc1 )

Parameters

  a | Matrix A
  b | Matrix B
  acc1 | Accumulator 1 input
  zero_acc1 | Zeroing mask for acc1
  shift16 | Shift mask of input accumulator acc1
  sub_mul | Negation mask of multiplication result
  sub_acc1 | Negation mask of acc1

Returns
  Result of operation

## ◆ mac_elem_32_2() [1/8]

v32acc32 mac_elem_32_2 | ( | v64int8 | a,
|  | int | sgn_x,
|  | v64int8 | b,
|  | int | sgn_y,
|  | v32acc32 | acc1 )

Parameters

  a | Matrix A
  sgn_x | Sign mask for matrix A
  b | Matrix B
  sgn_y | Sign mask for matrix B
  acc1 | Accumulator 1 input

Returns
  Result of operation

## ◆ mac_elem_32_2() [2/8]

v32acc32 mac_elem_32_2 | ( | v64int8 | a,
|  | int | sgn_x,
|  | v64uint8 | b,
|  | int | sgn_y,
|  | v32acc32 | acc1 )

Parameters

  a | Matrix A
  sgn_x | Sign mask for matrix A
  b | Matrix B
  sgn_y | Sign mask for matrix B
  acc1 | Accumulator 1 input

Returns
  Result of operation

## ◆ mac_elem_32_2() [3/8]

v32acc32 mac_elem_32_2 | ( | v64int8 | a,
|  | v64int8 | b,
|  | v32acc32 | acc1 )

Parameters

  a | Matrix A
  b | Matrix B
  acc1 | Accumulator 1 input

Returns
  Result of operation

## ◆ mac_elem_32_2() [4/8]

v32acc32 mac_elem_32_2 | ( | v64int8 | a,
|  | v64uint8 | b,
|  | v32acc32 | acc1 )

Parameters

  a | Matrix A
  b | Matrix B
  acc1 | Accumulator 1 input

Returns
  Result of operation

## ◆ mac_elem_32_2() [5/8]

v32acc32 mac_elem_32_2 | ( | v64uint8 | a,
|  | int | sgn_x,
|  | v64int8 | b,
|  | int | sgn_y,
|  | v32acc32 | acc1 )

Parameters

  a | Matrix A
  sgn_x | Sign mask for matrix A
  b | Matrix B
  sgn_y | Sign mask for matrix B
  acc1 | Accumulator 1 input

Returns
  Result of operation

## ◆ mac_elem_32_2() [6/8]

v32acc32 mac_elem_32_2 | ( | v64uint8 | a,
|  | int | sgn_x,
|  | v64uint8 | b,
|  | int | sgn_y,
|  | v32acc32 | acc1 )

Parameters

  a | Matrix A
  sgn_x | Sign mask for matrix A
  b | Matrix B
  sgn_y | Sign mask for matrix B
  acc1 | Accumulator 1 input

Returns
  Result of operation

## ◆ mac_elem_32_2() [7/8]

v32acc32 mac_elem_32_2 | ( | v64uint8 | a,
|  | v64int8 | b,
|  | v32acc32 | acc1 )

Parameters

  a | Matrix A
  b | Matrix B
  acc1 | Accumulator 1 input

Returns
  Result of operation

## ◆ mac_elem_32_2() [8/8]

v32acc32 mac_elem_32_2 | ( | v64uint8 | a,
|  | v64uint8 | b,
|  | v32acc32 | acc1 )

Parameters

  a | Matrix A
  b | Matrix B
  acc1 | Accumulator 1 input

Returns
  Result of operation

## ◆ mac_elem_32_2_conf() [1/8]

v32acc32 mac_elem_32_2_conf | ( | v64int8 | a,
|  | int | sgn_x,
|  | v64int8 | b,
|  | int | sgn_y,
|  | v32acc32 | acc1,
|  | int | zero_acc1,
|  | int | shift16,
|  | int | sub_mul,
|  | int | sub_acc1 )

Parameters

  a | Matrix A
  sgn_x | Sign mask for matrix A
  b | Matrix B
  sgn_y | Sign mask for matrix B
  acc1 | Accumulator 1 input
  zero_acc1 | Zeroing mask for acc1
  shift16 | Shift mask of input accumulator acc1
  sub_mul | Negation mask of multiplication result
  sub_acc1 | Negation mask of acc1

Returns
  Result of operation

## ◆ mac_elem_32_2_conf() [2/8]

v32acc32 mac_elem_32_2_conf | ( | v64int8 | a,
|  | int | sgn_x,
|  | v64uint8 | b,
|  | int | sgn_y,
|  | v32acc32 | acc1,
|  | int | zero_acc1,
|  | int | shift16,
|  | int | sub_mul,
|  | int | sub_acc1 )

Parameters

  a | Matrix A
  sgn_x | Sign mask for matrix A
  b | Matrix B
  sgn_y | Sign mask for matrix B
  acc1 | Accumulator 1 input
  zero_acc1 | Zeroing mask for acc1
  shift16 | Shift mask of input accumulator acc1
  sub_mul | Negation mask of multiplication result
  sub_acc1 | Negation mask of acc1

Returns
  Result of operation

## ◆ mac_elem_32_2_conf() [3/8]

v32acc32 mac_elem_32_2_conf | ( | v64int8 | a,
|  | v64int8 | b,
|  | v32acc32 | acc1,
|  | int | zero_acc1,
|  | int | shift16,
|  | int | sub_mul,
|  | int | sub_acc1 )

Parameters

  a | Matrix A
  b | Matrix B
  acc1 | Accumulator 1 input
  zero_acc1 | Zeroing mask for acc1
  shift16 | Shift mask of input accumulator acc1
  sub_mul | Negation mask of multiplication result
  sub_acc1 | Negation mask of acc1

Returns
  Result of operation

## ◆ mac_elem_32_2_conf() [4/8]

v32acc32 mac_elem_32_2_conf | ( | v64int8 | a,
|  | v64uint8 | b,
|  | v32acc32 | acc1,
|  | int | zero_acc1,
|  | int | shift16,
|  | int | sub_mul,
|  | int | sub_acc1 )

Parameters

  a | Matrix A
  b | Matrix B
  acc1 | Accumulator 1 input
  zero_acc1 | Zeroing mask for acc1
  shift16 | Shift mask of input accumulator acc1
  sub_mul | Negation mask of multiplication result
  sub_acc1 | Negation mask of acc1

Returns
  Result of operation

## ◆ mac_elem_32_2_conf() [5/8]

v32acc32 mac_elem_32_2_conf | ( | v64uint8 | a,
|  | int | sgn_x,
|  | v64int8 | b,
|  | int | sgn_y,
|  | v32acc32 | acc1,
|  | int | zero_acc1,
|  | int | shift16,
|  | int | sub_mul,
|  | int | sub_acc1 )

Parameters

  a | Matrix A
  sgn_x | Sign mask for matrix A
  b | Matrix B
  sgn_y | Sign mask for matrix B
  acc1 | Accumulator 1 input
  zero_acc1 | Zeroing mask for acc1
  shift16 | Shift mask of input accumulator acc1
  sub_mul | Negation mask of multiplication result
  sub_acc1 | Negation mask of acc1

Returns
  Result of operation

## ◆ mac_elem_32_2_conf() [6/8]

v32acc32 mac_elem_32_2_conf | ( | v64uint8 | a,
|  | int | sgn_x,
|  | v64uint8 | b,
|  | int | sgn_y,
|  | v32acc32 | acc1,
|  | int | zero_acc1,
|  | int | shift16,
|  | int | sub_mul,
|  | int | sub_acc1 )

Parameters

  a | Matrix A
  sgn_x | Sign mask for matrix A
  b | Matrix B
  sgn_y | Sign mask for matrix B
  acc1 | Accumulator 1 input
  zero_acc1 | Zeroing mask for acc1
  shift16 | Shift mask of input accumulator acc1
  sub_mul | Negation mask of multiplication result
  sub_acc1 | Negation mask of acc1

Returns
  Result of operation

## ◆ mac_elem_32_2_conf() [7/8]

v32acc32 mac_elem_32_2_conf | ( | v64uint8 | a,
|  | v64int8 | b,
|  | v32acc32 | acc1,
|  | int | zero_acc1,
|  | int | shift16,
|  | int | sub_mul,
|  | int | sub_acc1 )

Parameters

  a | Matrix A
  b | Matrix B
  acc1 | Accumulator 1 input
  zero_acc1 | Zeroing mask for acc1
  shift16 | Shift mask of input accumulator acc1
  sub_mul | Negation mask of multiplication result
  sub_acc1 | Negation mask of acc1

Returns
  Result of operation

## ◆ mac_elem_32_2_conf() [8/8]

v32acc32 mac_elem_32_2_conf | ( | v64uint8 | a,
|  | v64uint8 | b,
|  | v32acc32 | acc1,
|  | int | zero_acc1,
|  | int | shift16,
|  | int | sub_mul,
|  | int | sub_acc1 )

Parameters

  a | Matrix A
  b | Matrix B
  acc1 | Accumulator 1 input
  zero_acc1 | Zeroing mask for acc1
  shift16 | Shift mask of input accumulator acc1
  sub_mul | Negation mask of multiplication result
  sub_acc1 | Negation mask of acc1

Returns
  Result of operation

## ◆ msc_4x8_8x8() [1/8]

v32acc32 msc_4x8_8x8 | ( | v64int8 | a,
|  | int | sgn_x,
|  | v64int8 | b,
|  | int | sgn_y,
|  | v32acc32 | acc1 )

Parameters

  a | Matrix A
  sgn_x | Sign mask for matrix A
  b | Matrix B
  sgn_y | Sign mask for matrix B
  acc1 | Accumulator 1 input

Returns
  Result of operation

## ◆ msc_4x8_8x8() [2/8]

v32acc32 msc_4x8_8x8 | ( | v64int8 | a,
|  | int | sgn_x,
|  | v64uint8 | b,
|  | int | sgn_y,
|  | v32acc32 | acc1 )

Parameters

  a | Matrix A
  sgn_x | Sign mask for matrix A
  b | Matrix B
  sgn_y | Sign mask for matrix B
  acc1 | Accumulator 1 input

Returns
  Result of operation

## ◆ msc_4x8_8x8() [3/8]

v32acc32 msc_4x8_8x8 | ( | v64int8 | a,
|  | v64int8 | b,
|  | v32acc32 | acc1 )

Parameters

  a | Matrix A
  b | Matrix B
  acc1 | Accumulator 1 input

Returns
  Result of operation

## ◆ msc_4x8_8x8() [4/8]

v32acc32 msc_4x8_8x8 | ( | v64int8 | a,
|  | v64uint8 | b,
|  | v32acc32 | acc1 )

Parameters

  a | Matrix A
  b | Matrix B
  acc1 | Accumulator 1 input

Returns
  Result of operation

## ◆ msc_4x8_8x8() [5/8]

v32acc32 msc_4x8_8x8 | ( | v64uint8 | a,
|  | int | sgn_x,
|  | v64int8 | b,
|  | int | sgn_y,
|  | v32acc32 | acc1 )

Parameters

  a | Matrix A
  sgn_x | Sign mask for matrix A
  b | Matrix B
  sgn_y | Sign mask for matrix B
  acc1 | Accumulator 1 input

Returns
  Result of operation

## ◆ msc_4x8_8x8() [6/8]

v32acc32 msc_4x8_8x8 | ( | v64uint8 | a,
|  | int | sgn_x,
|  | v64uint8 | b,
|  | int | sgn_y,
|  | v32acc32 | acc1 )

Parameters

  a | Matrix A
  sgn_x | Sign mask for matrix A
  b | Matrix B
  sgn_y | Sign mask for matrix B
  acc1 | Accumulator 1 input

Returns
  Result of operation

## ◆ msc_4x8_8x8() [7/8]

v32acc32 msc_4x8_8x8 | ( | v64uint8 | a,
|  | v64int8 | b,
|  | v32acc32 | acc1 )

Parameters

  a | Matrix A
  b | Matrix B
  acc1 | Accumulator 1 input

Returns
  Result of operation

## ◆ msc_4x8_8x8() [8/8]

v32acc32 msc_4x8_8x8 | ( | v64uint8 | a,
|  | v64uint8 | b,
|  | v32acc32 | acc1 )

Parameters

  a | Matrix A
  b | Matrix B
  acc1 | Accumulator 1 input

Returns
  Result of operation

## ◆ msc_4x8_8x8_conf() [1/8]

v32acc32 msc_4x8_8x8_conf | ( | v64int8 | a,
|  | int | sgn_x,
|  | v64int8 | b,
|  | int | sgn_y,
|  | v32acc32 | acc1,
|  | int | zero_acc1,
|  | int | shift16,
|  | int | sub_mul,
|  | int | sub_acc1 )

Parameters

  a | Matrix A
  sgn_x | Sign mask for matrix A
  b | Matrix B
  sgn_y | Sign mask for matrix B
  acc1 | Accumulator 1 input
  zero_acc1 | Zeroing mask for acc1
  shift16 | Shift mask of input accumulator acc1
  sub_mul | Negation mask of multiplication result. If a bit is set the corresponding output accumulator lane is negated.
  sub_acc1 | Negation mask of acc1. If a bit is set the corresponding accumulator lane of acc1 is negated.

Returns
  Result of operation

## ◆ msc_4x8_8x8_conf() [2/8]

v32acc32 msc_4x8_8x8_conf | ( | v64int8 | a,
|  | int | sgn_x,
|  | v64uint8 | b,
|  | int | sgn_y,
|  | v32acc32 | acc1,
|  | int | zero_acc1,
|  | int | shift16,
|  | int | sub_mul,
|  | int | sub_acc1 )

Parameters

  a | Matrix A
  sgn_x | Sign mask for matrix A
  b | Matrix B
  sgn_y | Sign mask for matrix B
  acc1 | Accumulator 1 input
  zero_acc1 | Zeroing mask for acc1
  shift16 | Shift mask of input accumulator acc1
  sub_mul | Negation mask of multiplication result. If a bit is set the corresponding output accumulator lane is negated.
  sub_acc1 | Negation mask of acc1. If a bit is set the corresponding accumulator lane of acc1 is negated.

Returns
  Result of operation

## ◆ msc_4x8_8x8_conf() [3/8]

v32acc32 msc_4x8_8x8_conf | ( | v64int8 | a,
|  | v64int8 | b,
|  | v32acc32 | acc1,
|  | int | zero_acc1,
|  | int | shift16,
|  | int | sub_mul,
|  | int | sub_acc1 )

Parameters

  a | Matrix A
  b | Matrix B
  acc1 | Accumulator 1 input
  zero_acc1 | Zeroing mask for acc1
  shift16 | Shift mask of input accumulator acc1
  sub_mul | Negation mask of multiplication result
  sub_acc1 | Negation mask of acc1

Returns
  Result of operation

## ◆ msc_4x8_8x8_conf() [4/8]

v32acc32 msc_4x8_8x8_conf | ( | v64int8 | a,
|  | v64uint8 | b,
|  | v32acc32 | acc1,
|  | int | zero_acc1,
|  | int | shift16,
|  | int | sub_mul,
|  | int | sub_acc1 )

Parameters

  a | Matrix A
  b | Matrix B
  acc1 | Accumulator 1 input
  zero_acc1 | Zeroing mask for acc1
  shift16 | Shift mask of input accumulator acc1
  sub_mul | Negation mask of multiplication result
  sub_acc1 | Negation mask of acc1

Returns
  Result of operation

## ◆ msc_4x8_8x8_conf() [5/8]

v32acc32 msc_4x8_8x8_conf | ( | v64uint8 | a,
|  | int | sgn_x,
|  | v64int8 | b,
|  | int | sgn_y,
|  | v32acc32 | acc1,
|  | int | zero_acc1,
|  | int | shift16,
|  | int | sub_mul,
|  | int | sub_acc1 )

Parameters

  a | Matrix A
  sgn_x | Sign mask for matrix A
  b | Matrix B
  sgn_y | Sign mask for matrix B
  acc1 | Accumulator 1 input
  zero_acc1 | Zeroing mask for acc1
  shift16 | Shift mask of input accumulator acc1
  sub_mul | Negation mask of multiplication result. If a bit is set the corresponding output accumulator lane is negated.
  sub_acc1 | Negation mask of acc1. If a bit is set the corresponding accumulator lane of acc1 is negated.

Returns
  Result of operation

## ◆ msc_4x8_8x8_conf() [6/8]

v32acc32 msc_4x8_8x8_conf | ( | v64uint8 | a,
|  | int | sgn_x,
|  | v64uint8 | b,
|  | int | sgn_y,
|  | v32acc32 | acc1,
|  | int | zero_acc1,
|  | int | shift16,
|  | int | sub_mul,
|  | int | sub_acc1 )

Parameters

  a | Matrix A
  sgn_x | Sign mask for matrix A
  b | Matrix B
  sgn_y | Sign mask for matrix B
  acc1 | Accumulator 1 input
  zero_acc1 | Zeroing mask for acc1
  shift16 | Shift mask of input accumulator acc1
  sub_mul | Negation mask of multiplication result. If a bit is set the corresponding output accumulator lane is negated.
  sub_acc1 | Negation mask of acc1. If a bit is set the corresponding accumulator lane of acc1 is negated.

Returns
  Result of operation

## ◆ msc_4x8_8x8_conf() [7/8]

v32acc32 msc_4x8_8x8_conf | ( | v64uint8 | a,
|  | v64int8 | b,
|  | v32acc32 | acc1,
|  | int | zero_acc1,
|  | int | shift16,
|  | int | sub_mul,
|  | int | sub_acc1 )

Parameters

  a | Matrix A
  b | Matrix B
  acc1 | Accumulator 1 input
  zero_acc1 | Zeroing mask for acc1
  shift16 | Shift mask of input accumulator acc1
  sub_mul | Negation mask of multiplication result
  sub_acc1 | Negation mask of acc1

Returns
  Result of operation

## ◆ msc_4x8_8x8_conf() [8/8]

v32acc32 msc_4x8_8x8_conf | ( | v64uint8 | a,
|  | v64uint8 | b,
|  | v32acc32 | acc1,
|  | int | zero_acc1,
|  | int | shift16,
|  | int | sub_mul,
|  | int | sub_acc1 )

Parameters

  a | Matrix A
  b | Matrix B
  acc1 | Accumulator 1 input
  zero_acc1 | Zeroing mask for acc1
  shift16 | Shift mask of input accumulator acc1
  sub_mul | Negation mask of multiplication result
  sub_acc1 | Negation mask of acc1

Returns
  Result of operation

## ◆ msc_conv_32x8() [1/8]

v32acc32 msc_conv_32x8 | ( | v64int8 | a,
|  | int | sgn_x,
|  | v64int8 | b,
|  | int | sgn_y,
|  | v32acc32 | acc1 )

Parameters

  a | Matrix A
  sgn_x | Sign mask for matrix A
  b | Matrix B
  sgn_y | Sign mask for matrix B
  acc1 | Accumulator 1 input

Returns
  Result of operation

## ◆ msc_conv_32x8() [2/8]

v32acc32 msc_conv_32x8 | ( | v64int8 | a,
|  | int | sgn_x,
|  | v64uint8 | b,
|  | int | sgn_y,
|  | v32acc32 | acc1 )

Parameters

  a | Matrix A
  sgn_x | Sign mask for matrix A
  b | Matrix B
  sgn_y | Sign mask for matrix B
  acc1 | Accumulator 1 input

Returns
  Result of operation

## ◆ msc_conv_32x8() [3/8]

v32acc32 msc_conv_32x8 | ( | v64int8 | a,
|  | v64int8 | b,
|  | v32acc32 | acc1 )

Parameters

  a | Matrix A
  b | Matrix B
  acc1 | Accumulator 1 input

Returns
  Result of operation

## ◆ msc_conv_32x8() [4/8]

v32acc32 msc_conv_32x8 | ( | v64int8 | a,
|  | v64uint8 | b,
|  | v32acc32 | acc1 )

Parameters

  a | Matrix A
  b | Matrix B
  acc1 | Accumulator 1 input

Returns
  Result of operation

## ◆ msc_conv_32x8() [5/8]

v32acc32 msc_conv_32x8 | ( | v64uint8 | a,
|  | int | sgn_x,
|  | v64int8 | b,
|  | int | sgn_y,
|  | v32acc32 | acc1 )

Parameters

  a | Matrix A
  sgn_x | Sign mask for matrix A
  b | Matrix B
  sgn_y | Sign mask for matrix B
  acc1 | Accumulator 1 input

Returns
  Result of operation

## ◆ msc_conv_32x8() [6/8]

v32acc32 msc_conv_32x8 | ( | v64uint8 | a,
|  | int | sgn_x,
|  | v64uint8 | b,
|  | int | sgn_y,
|  | v32acc32 | acc1 )

Parameters

  a | Matrix A
  sgn_x | Sign mask for matrix A
  b | Matrix B
  sgn_y | Sign mask for matrix B
  acc1 | Accumulator 1 input

Returns
  Result of operation

## ◆ msc_conv_32x8() [7/8]

v32acc32 msc_conv_32x8 | ( | v64uint8 | a,
|  | v64int8 | b,
|  | v32acc32 | acc1 )

Parameters

  a | Matrix A
  b | Matrix B
  acc1 | Accumulator 1 input

Returns
  Result of operation

## ◆ msc_conv_32x8() [8/8]

v32acc32 msc_conv_32x8 | ( | v64uint8 | a,
|  | v64uint8 | b,
|  | v32acc32 | acc1 )

Parameters

  a | Matrix A
  b | Matrix B
  acc1 | Accumulator 1 input

Returns
  Result of operation

## ◆ msc_conv_32x8_conf() [1/8]

v32acc32 msc_conv_32x8_conf | ( | v64int8 | a,
|  | int | sgn_x,
|  | v64int8 | b,
|  | int | sgn_y,
|  | v32acc32 | acc1,
|  | int | zero_acc1,
|  | int | shift16,
|  | int | sub_mul,
|  | int | sub_acc1 )

Parameters

  a | Matrix A
  sgn_x | Sign mask for matrix A
  b | Matrix B
  sgn_y | Sign mask for matrix B
  acc1 | Accumulator 1 input
  zero_acc1 | Zeroing mask for acc1
  shift16 | Shift mask of input accumulator acc1
  sub_mul | Negation mask of multiplication result. If a bit is set the corresponding output accumulator lane is negated.
  sub_acc1 | Negation mask of acc1. If a bit is set the corresponding accumulator lane of acc1 is negated.

Returns
  Result of operation

## ◆ msc_conv_32x8_conf() [2/8]

v32acc32 msc_conv_32x8_conf | ( | v64int8 | a,
|  | int | sgn_x,
|  | v64uint8 | b,
|  | int | sgn_y,
|  | v32acc32 | acc1,
|  | int | zero_acc1,
|  | int | shift16,
|  | int | sub_mul,
|  | int | sub_acc1 )

Parameters

  a | Matrix A
  sgn_x | Sign mask for matrix A
  b | Matrix B
  sgn_y | Sign mask for matrix B
  acc1 | Accumulator 1 input
  zero_acc1 | Zeroing mask for acc1
  shift16 | Shift mask of input accumulator acc1
  sub_mul | Negation mask of multiplication result. If a bit is set the corresponding output accumulator lane is negated.
  sub_acc1 | Negation mask of acc1. If a bit is set the corresponding accumulator lane of acc1 is negated.

Returns
  Result of operation

## ◆ msc_conv_32x8_conf() [3/8]

v32acc32 msc_conv_32x8_conf | ( | v64int8 | a,
|  | v64int8 | b,
|  | v32acc32 | acc1,
|  | int | zero_acc1,
|  | int | shift16,
|  | int | sub_mul,
|  | int | sub_acc1 )

Parameters

  a | Matrix A
  b | Matrix B
  acc1 | Accumulator 1 input
  zero_acc1 | Zeroing mask for acc1
  shift16 | Shift mask of input accumulator acc1
  sub_mul | Negation mask of multiplication result
  sub_acc1 | Negation mask of acc1

Returns
  Result of operation

## ◆ msc_conv_32x8_conf() [4/8]

v32acc32 msc_conv_32x8_conf | ( | v64int8 | a,
|  | v64uint8 | b,
|  | v32acc32 | acc1,
|  | int | zero_acc1,
|  | int | shift16,
|  | int | sub_mul,
|  | int | sub_acc1 )

Parameters

  a | Matrix A
  b | Matrix B
  acc1 | Accumulator 1 input
  zero_acc1 | Zeroing mask for acc1
  shift16 | Shift mask of input accumulator acc1
  sub_mul | Negation mask of multiplication result
  sub_acc1 | Negation mask of acc1

Returns
  Result of operation

## ◆ msc_conv_32x8_conf() [5/8]

v32acc32 msc_conv_32x8_conf | ( | v64uint8 | a,
|  | int | sgn_x,
|  | v64int8 | b,
|  | int | sgn_y,
|  | v32acc32 | acc1,
|  | int | zero_acc1,
|  | int | shift16,
|  | int | sub_mul,
|  | int | sub_acc1 )

Parameters

  a | Matrix A
  sgn_x | Sign mask for matrix A
  b | Matrix B
  sgn_y | Sign mask for matrix B
  acc1 | Accumulator 1 input
  zero_acc1 | Zeroing mask for acc1
  shift16 | Shift mask of input accumulator acc1
  sub_mul | Negation mask of multiplication result. If a bit is set the corresponding output accumulator lane is negated.
  sub_acc1 | Negation mask of acc1. If a bit is set the corresponding accumulator lane of acc1 is negated.

Returns
  Result of operation

## ◆ msc_conv_32x8_conf() [6/8]

v32acc32 msc_conv_32x8_conf | ( | v64uint8 | a,
|  | int | sgn_x,
|  | v64uint8 | b,
|  | int | sgn_y,
|  | v32acc32 | acc1,
|  | int | zero_acc1,
|  | int | shift16,
|  | int | sub_mul,
|  | int | sub_acc1 )

Parameters

  a | Matrix A
  sgn_x | Sign mask for matrix A
  b | Matrix B
  sgn_y | Sign mask for matrix B
  acc1 | Accumulator 1 input
  zero_acc1 | Zeroing mask for acc1
  shift16 | Shift mask of input accumulator acc1
  sub_mul | Negation mask of multiplication result. If a bit is set the corresponding output accumulator lane is negated.
  sub_acc1 | Negation mask of acc1. If a bit is set the corresponding accumulator lane of acc1 is negated.

Returns
  Result of operation

## ◆ msc_conv_32x8_conf() [7/8]

v32acc32 msc_conv_32x8_conf | ( | v64uint8 | a,
|  | v64int8 | b,
|  | v32acc32 | acc1,
|  | int | zero_acc1,
|  | int | shift16,
|  | int | sub_mul,
|  | int | sub_acc1 )

Parameters

  a | Matrix A
  b | Matrix B
  acc1 | Accumulator 1 input
  zero_acc1 | Zeroing mask for acc1
  shift16 | Shift mask of input accumulator acc1
  sub_mul | Negation mask of multiplication result
  sub_acc1 | Negation mask of acc1

Returns
  Result of operation

## ◆ msc_conv_32x8_conf() [8/8]

v32acc32 msc_conv_32x8_conf | ( | v64uint8 | a,
|  | v64uint8 | b,
|  | v32acc32 | acc1,
|  | int | zero_acc1,
|  | int | shift16,
|  | int | sub_mul,
|  | int | sub_acc1 )

Parameters

  a | Matrix A
  b | Matrix B
  acc1 | Accumulator 1 input
  zero_acc1 | Zeroing mask for acc1
  shift16 | Shift mask of input accumulator acc1
  sub_mul | Negation mask of multiplication result
  sub_acc1 | Negation mask of acc1

Returns
  Result of operation

## ◆ msc_conv_4x4_8ch() [1/8]

v32acc32 msc_conv_4x4_8ch | ( | v64int8 | a,
|  | int | sgn_x,
|  | v64int8 | b,
|  | int | sgn_y,
|  | v32acc32 | acc1 )

Parameters

  a | Matrix A
  sgn_x | Sign mask for matrix A
  b | Matrix B
  sgn_y | Sign mask for matrix B
  acc1 | Accumulator 1 input

Returns
  Result of operation

## ◆ msc_conv_4x4_8ch() [2/8]

v32acc32 msc_conv_4x4_8ch | ( | v64int8 | a,
|  | int | sgn_x,
|  | v64uint8 | b,
|  | int | sgn_y,
|  | v32acc32 | acc1 )

Parameters

  a | Matrix A
  sgn_x | Sign mask for matrix A
  b | Matrix B
  sgn_y | Sign mask for matrix B
  acc1 | Accumulator 1 input

Returns
  Result of operation

## ◆ msc_conv_4x4_8ch() [3/8]

v32acc32 msc_conv_4x4_8ch | ( | v64int8 | a,
|  | v64int8 | b,
|  | v32acc32 | acc1 )

Parameters

  a | Matrix A
  b | Matrix B
  acc1 | Accumulator 1 input

Returns
  Result of operation

## ◆ msc_conv_4x4_8ch() [4/8]

v32acc32 msc_conv_4x4_8ch | ( | v64int8 | a,
|  | v64uint8 | b,
|  | v32acc32 | acc1 )

Parameters

  a | Matrix A
  b | Matrix B
  acc1 | Accumulator 1 input

Returns
  Result of operation

## ◆ msc_conv_4x4_8ch() [5/8]

v32acc32 msc_conv_4x4_8ch | ( | v64uint8 | a,
|  | int | sgn_x,
|  | v64int8 | b,
|  | int | sgn_y,
|  | v32acc32 | acc1 )

Parameters

  a | Matrix A
  sgn_x | Sign mask for matrix A
  b | Matrix B
  sgn_y | Sign mask for matrix B
  acc1 | Accumulator 1 input

Returns
  Result of operation

## ◆ msc_conv_4x4_8ch() [6/8]

v32acc32 msc_conv_4x4_8ch | ( | v64uint8 | a,
|  | int | sgn_x,
|  | v64uint8 | b,
|  | int | sgn_y,
|  | v32acc32 | acc1 )

Parameters

  a | Matrix A
  sgn_x | Sign mask for matrix A
  b | Matrix B
  sgn_y | Sign mask for matrix B
  acc1 | Accumulator 1 input

Returns
  Result of operation

## ◆ msc_conv_4x4_8ch() [7/8]

v32acc32 msc_conv_4x4_8ch | ( | v64uint8 | a,
|  | v64int8 | b,
|  | v32acc32 | acc1 )

Parameters

  a | Matrix A
  b | Matrix B
  acc1 | Accumulator 1 input

Returns
  Result of operation

## ◆ msc_conv_4x4_8ch() [8/8]

v32acc32 msc_conv_4x4_8ch | ( | v64uint8 | a,
|  | v64uint8 | b,
|  | v32acc32 | acc1 )

Parameters

  a | Matrix A
  b | Matrix B
  acc1 | Accumulator 1 input

Returns
  Result of operation

## ◆ msc_conv_4x4_8ch_conf() [1/8]

v32acc32 msc_conv_4x4_8ch_conf | ( | v64int8 | a,
|  | int | sgn_x,
|  | v64int8 | b,
|  | int | sgn_y,
|  | v32acc32 | acc1,
|  | int | zero_acc1,
|  | int | shift16,
|  | int | sub_mul,
|  | int | sub_acc1 )

Parameters

  a | Matrix A
  sgn_x | Sign mask for matrix A
  b | Matrix B
  sgn_y | Sign mask for matrix B
  acc1 | Accumulator 1 input
  zero_acc1 | Zeroing mask for acc1
  shift16 | Shift mask of input accumulator acc1
  sub_mul | Negation mask of multiplication result. If a bit is set the corresponding output accumulator lane is negated.
  sub_acc1 | Negation mask of acc1. If a bit is set the corresponding accumulator lane of acc1 is negated.

Returns
  Result of operation

## ◆ msc_conv_4x4_8ch_conf() [2/8]

v32acc32 msc_conv_4x4_8ch_conf | ( | v64int8 | a,
|  | int | sgn_x,
|  | v64uint8 | b,
|  | int | sgn_y,
|  | v32acc32 | acc1,
|  | int | zero_acc1,
|  | int | shift16,
|  | int | sub_mul,
|  | int | sub_acc1 )

Parameters

  a | Matrix A
  sgn_x | Sign mask for matrix A
  b | Matrix B
  sgn_y | Sign mask for matrix B
  acc1 | Accumulator 1 input
  zero_acc1 | Zeroing mask for acc1
  shift16 | Shift mask of input accumulator acc1
  sub_mul | Negation mask of multiplication result. If a bit is set the corresponding output accumulator lane is negated.
  sub_acc1 | Negation mask of acc1. If a bit is set the corresponding accumulator lane of acc1 is negated.

Returns
  Result of operation

## ◆ msc_conv_4x4_8ch_conf() [3/8]

v32acc32 msc_conv_4x4_8ch_conf | ( | v64int8 | a,
|  | v64int8 | b,
|  | v32acc32 | acc1,
|  | int | zero_acc1,
|  | int | shift16,
|  | int | sub_mul,
|  | int | sub_acc1 )

Parameters

  a | Matrix A
  b | Matrix B
  acc1 | Accumulator 1 input
  zero_acc1 | Zeroing mask for acc1
  shift16 | Shift mask of input accumulator acc1
  sub_mul | Negation mask of multiplication result
  sub_acc1 | Negation mask of acc1

Returns
  Result of operation

## ◆ msc_conv_4x4_8ch_conf() [4/8]

v32acc32 msc_conv_4x4_8ch_conf | ( | v64int8 | a,
|  | v64uint8 | b,
|  | v32acc32 | acc1,
|  | int | zero_acc1,
|  | int | shift16,
|  | int | sub_mul,
|  | int | sub_acc1 )

Parameters

  a | Matrix A
  b | Matrix B
  acc1 | Accumulator 1 input
  zero_acc1 | Zeroing mask for acc1
  shift16 | Shift mask of input accumulator acc1
  sub_mul | Negation mask of multiplication result
  sub_acc1 | Negation mask of acc1

Returns
  Result of operation

## ◆ msc_conv_4x4_8ch_conf() [5/8]

v32acc32 msc_conv_4x4_8ch_conf | ( | v64uint8 | a,
|  | int | sgn_x,
|  | v64int8 | b,
|  | int | sgn_y,
|  | v32acc32 | acc1,
|  | int | zero_acc1,
|  | int | shift16,
|  | int | sub_mul,
|  | int | sub_acc1 )

Parameters

  a | Matrix A
  sgn_x | Sign mask for matrix A
  b | Matrix B
  sgn_y | Sign mask for matrix B
  acc1 | Accumulator 1 input
  zero_acc1 | Zeroing mask for acc1
  shift16 | Shift mask of input accumulator acc1
  sub_mul | Negation mask of multiplication result. If a bit is set the corresponding output accumulator lane is negated.
  sub_acc1 | Negation mask of acc1. If a bit is set the corresponding accumulator lane of acc1 is negated.

Returns
  Result of operation

## ◆ msc_conv_4x4_8ch_conf() [6/8]

v32acc32 msc_conv_4x4_8ch_conf | ( | v64uint8 | a,
|  | int | sgn_x,
|  | v64uint8 | b,
|  | int | sgn_y,
|  | v32acc32 | acc1,
|  | int | zero_acc1,
|  | int | shift16,
|  | int | sub_mul,
|  | int | sub_acc1 )

Parameters

  a | Matrix A
  sgn_x | Sign mask for matrix A
  b | Matrix B
  sgn_y | Sign mask for matrix B
  acc1 | Accumulator 1 input
  zero_acc1 | Zeroing mask for acc1
  shift16 | Shift mask of input accumulator acc1
  sub_mul | Negation mask of multiplication result. If a bit is set the corresponding output accumulator lane is negated.
  sub_acc1 | Negation mask of acc1. If a bit is set the corresponding accumulator lane of acc1 is negated.

Returns
  Result of operation

## ◆ msc_conv_4x4_8ch_conf() [7/8]

v32acc32 msc_conv_4x4_8ch_conf | ( | v64uint8 | a,
|  | v64int8 | b,
|  | v32acc32 | acc1,
|  | int | zero_acc1,
|  | int | shift16,
|  | int | sub_mul,
|  | int | sub_acc1 )

Parameters

  a | Matrix A
  b | Matrix B
  acc1 | Accumulator 1 input
  zero_acc1 | Zeroing mask for acc1
  shift16 | Shift mask of input accumulator acc1
  sub_mul | Negation mask of multiplication result
  sub_acc1 | Negation mask of acc1

Returns
  Result of operation

## ◆ msc_conv_4x4_8ch_conf() [8/8]

v32acc32 msc_conv_4x4_8ch_conf | ( | v64uint8 | a,
|  | v64uint8 | b,
|  | v32acc32 | acc1,
|  | int | zero_acc1,
|  | int | shift16,
|  | int | sub_mul,
|  | int | sub_acc1 )

Parameters

  a | Matrix A
  b | Matrix B
  acc1 | Accumulator 1 input
  zero_acc1 | Zeroing mask for acc1
  shift16 | Shift mask of input accumulator acc1
  sub_mul | Negation mask of multiplication result
  sub_acc1 | Negation mask of acc1

Returns
  Result of operation

## ◆ msc_conv_8x8_4ch() [1/8]

v32acc32 msc_conv_8x8_4ch | ( | v64int8 | a,
|  | int | sgn_x,
|  | v64int8 | b,
|  | int | sgn_y,
|  | v32acc32 | acc1 )

Parameters

  a | Matrix A
  sgn_x | Sign mask for matrix A
  b | Matrix B
  sgn_y | Sign mask for matrix B
  acc1 | Accumulator 1 input

Returns
  Result of operation

## ◆ msc_conv_8x8_4ch() [2/8]

v32acc32 msc_conv_8x8_4ch | ( | v64int8 | a,
|  | int | sgn_x,
|  | v64uint8 | b,
|  | int | sgn_y,
|  | v32acc32 | acc1 )

Parameters

  a | Matrix A
  sgn_x | Sign mask for matrix A
  b | Matrix B
  sgn_y | Sign mask for matrix B
  acc1 | Accumulator 1 input

Returns
  Result of operation

## ◆ msc_conv_8x8_4ch() [3/8]

v32acc32 msc_conv_8x8_4ch | ( | v64int8 | a,
|  | v64int8 | b,
|  | v32acc32 | acc1 )

Parameters

  a | Matrix A
  b | Matrix B
  acc1 | Accumulator 1 input

Returns
  Result of operation

## ◆ msc_conv_8x8_4ch() [4/8]

v32acc32 msc_conv_8x8_4ch | ( | v64int8 | a,
|  | v64uint8 | b,
|  | v32acc32 | acc1 )

Parameters

  a | Matrix A
  b | Matrix B
  acc1 | Accumulator 1 input

Returns
  Result of operation

## ◆ msc_conv_8x8_4ch() [5/8]

v32acc32 msc_conv_8x8_4ch | ( | v64uint8 | a,
|  | int | sgn_x,
|  | v64int8 | b,
|  | int | sgn_y,
|  | v32acc32 | acc1 )

Parameters

  a | Matrix A
  sgn_x | Sign mask for matrix A
  b | Matrix B
  sgn_y | Sign mask for matrix B
  acc1 | Accumulator 1 input

Returns
  Result of operation

## ◆ msc_conv_8x8_4ch() [6/8]

v32acc32 msc_conv_8x8_4ch | ( | v64uint8 | a,
|  | int | sgn_x,
|  | v64uint8 | b,
|  | int | sgn_y,
|  | v32acc32 | acc1 )

Parameters

  a | Matrix A
  sgn_x | Sign mask for matrix A
  b | Matrix B
  sgn_y | Sign mask for matrix B
  acc1 | Accumulator 1 input

Returns
  Result of operation

## ◆ msc_conv_8x8_4ch() [7/8]

v32acc32 msc_conv_8x8_4ch | ( | v64uint8 | a,
|  | v64int8 | b,
|  | v32acc32 | acc1 )

Parameters

  a | Matrix A
  b | Matrix B
  acc1 | Accumulator 1 input

Returns
  Result of operation

## ◆ msc_conv_8x8_4ch() [8/8]

v32acc32 msc_conv_8x8_4ch | ( | v64uint8 | a,
|  | v64uint8 | b,
|  | v32acc32 | acc1 )

Parameters

  a | Matrix A
  b | Matrix B
  acc1 | Accumulator 1 input

Returns
  Result of operation

## ◆ msc_conv_8x8_4ch_conf() [1/8]

v32acc32 msc_conv_8x8_4ch_conf | ( | v64int8 | a,
|  | int | sgn_x,
|  | v64int8 | b,
|  | int | sgn_y,
|  | v32acc32 | acc1,
|  | int | zero_acc1,
|  | int | shift16,
|  | int | sub_mul,
|  | int | sub_acc1 )

Parameters

  a | Matrix A
  sgn_x | Sign mask for matrix A
  b | Matrix B
  sgn_y | Sign mask for matrix B
  acc1 | Accumulator 1 input
  zero_acc1 | Zeroing mask for acc1
  shift16 | Shift mask of input accumulator acc1
  sub_mul | Negation mask of multiplication result. If a bit is set the corresponding output accumulator lane is negated.
  sub_acc1 | Negation mask of acc1. If a bit is set the corresponding accumulator lane of acc1 is negated.

Returns
  Result of operation

## ◆ msc_conv_8x8_4ch_conf() [2/8]

v32acc32 msc_conv_8x8_4ch_conf | ( | v64int8 | a,
|  | int | sgn_x,
|  | v64uint8 | b,
|  | int | sgn_y,
|  | v32acc32 | acc1,
|  | int | zero_acc1,
|  | int | shift16,
|  | int | sub_mul,
|  | int | sub_acc1 )

Parameters

  a | Matrix A
  sgn_x | Sign mask for matrix A
  b | Matrix B
  sgn_y | Sign mask for matrix B
  acc1 | Accumulator 1 input
  zero_acc1 | Zeroing mask for acc1
  shift16 | Shift mask of input accumulator acc1
  sub_mul | Negation mask of multiplication result. If a bit is set the corresponding output accumulator lane is negated.
  sub_acc1 | Negation mask of acc1. If a bit is set the corresponding accumulator lane of acc1 is negated.

Returns
  Result of operation

## ◆ msc_conv_8x8_4ch_conf() [3/8]

v32acc32 msc_conv_8x8_4ch_conf | ( | v64int8 | a,
|  | v64int8 | b,
|  | v32acc32 | acc1,
|  | int | zero_acc1,
|  | int | shift16,
|  | int | sub_mul,
|  | int | sub_acc1 )

Parameters

  a | Matrix A
  b | Matrix B
  acc1 | Accumulator 1 input
  zero_acc1 | Zeroing mask for acc1
  shift16 | Shift mask of input accumulator acc1
  sub_mul | Negation mask of multiplication result
  sub_acc1 | Negation mask of acc1

Returns
  Result of operation

## ◆ msc_conv_8x8_4ch_conf() [4/8]

v32acc32 msc_conv_8x8_4ch_conf | ( | v64int8 | a,
|  | v64uint8 | b,
|  | v32acc32 | acc1,
|  | int | zero_acc1,
|  | int | shift16,
|  | int | sub_mul,
|  | int | sub_acc1 )

Parameters

  a | Matrix A
  b | Matrix B
  acc1 | Accumulator 1 input
  zero_acc1 | Zeroing mask for acc1
  shift16 | Shift mask of input accumulator acc1
  sub_mul | Negation mask of multiplication result
  sub_acc1 | Negation mask of acc1

Returns
  Result of operation

## ◆ msc_conv_8x8_4ch_conf() [5/8]

v32acc32 msc_conv_8x8_4ch_conf | ( | v64uint8 | a,
|  | int | sgn_x,
|  | v64int8 | b,
|  | int | sgn_y,
|  | v32acc32 | acc1,
|  | int | zero_acc1,
|  | int | shift16,
|  | int | sub_mul,
|  | int | sub_acc1 )

Parameters

  a | Matrix A
  sgn_x | Sign mask for matrix A
  b | Matrix B
  sgn_y | Sign mask for matrix B
  acc1 | Accumulator 1 input
  zero_acc1 | Zeroing mask for acc1
  shift16 | Shift mask of input accumulator acc1
  sub_mul | Negation mask of multiplication result. If a bit is set the corresponding output accumulator lane is negated.
  sub_acc1 | Negation mask of acc1. If a bit is set the corresponding accumulator lane of acc1 is negated.

Returns
  Result of operation

## ◆ msc_conv_8x8_4ch_conf() [6/8]

v32acc32 msc_conv_8x8_4ch_conf | ( | v64uint8 | a,
|  | int | sgn_x,
|  | v64uint8 | b,
|  | int | sgn_y,
|  | v32acc32 | acc1,
|  | int | zero_acc1,
|  | int | shift16,
|  | int | sub_mul,
|  | int | sub_acc1 )

Parameters

  a | Matrix A
  sgn_x | Sign mask for matrix A
  b | Matrix B
  sgn_y | Sign mask for matrix B
  acc1 | Accumulator 1 input
  zero_acc1 | Zeroing mask for acc1
  shift16 | Shift mask of input accumulator acc1
  sub_mul | Negation mask of multiplication result. If a bit is set the corresponding output accumulator lane is negated.
  sub_acc1 | Negation mask of acc1. If a bit is set the corresponding accumulator lane of acc1 is negated.

Returns
  Result of operation

## ◆ msc_conv_8x8_4ch_conf() [7/8]

v32acc32 msc_conv_8x8_4ch_conf | ( | v64uint8 | a,
|  | v64int8 | b,
|  | v32acc32 | acc1,
|  | int | zero_acc1,
|  | int | shift16,
|  | int | sub_mul,
|  | int | sub_acc1 )

Parameters

  a | Matrix A
  b | Matrix B
  acc1 | Accumulator 1 input
  zero_acc1 | Zeroing mask for acc1
  shift16 | Shift mask of input accumulator acc1
  sub_mul | Negation mask of multiplication result
  sub_acc1 | Negation mask of acc1

Returns
  Result of operation

## ◆ msc_conv_8x8_4ch_conf() [8/8]

v32acc32 msc_conv_8x8_4ch_conf | ( | v64uint8 | a,
|  | v64uint8 | b,
|  | v32acc32 | acc1,
|  | int | zero_acc1,
|  | int | shift16,
|  | int | sub_mul,
|  | int | sub_acc1 )

Parameters

  a | Matrix A
  b | Matrix B
  acc1 | Accumulator 1 input
  zero_acc1 | Zeroing mask for acc1
  shift16 | Shift mask of input accumulator acc1
  sub_mul | Negation mask of multiplication result
  sub_acc1 | Negation mask of acc1

Returns
  Result of operation

## ◆ msc_elem_32_2() [1/8]

v32acc32 msc_elem_32_2 | ( | v64int8 | a,
|  | int | sgn_x,
|  | v64int8 | b,
|  | int | sgn_y,
|  | v32acc32 | acc1 )

Parameters

  a | Matrix A
  sgn_x | Sign mask for matrix A
  b | Matrix B
  sgn_y | Sign mask for matrix B
  acc1 | Accumulator 1 input

Returns
  Result of operation

## ◆ msc_elem_32_2() [2/8]

v32acc32 msc_elem_32_2 | ( | v64int8 | a,
|  | int | sgn_x,
|  | v64uint8 | b,
|  | int | sgn_y,
|  | v32acc32 | acc1 )

Parameters

  a | Matrix A
  sgn_x | Sign mask for matrix A
  b | Matrix B
  sgn_y | Sign mask for matrix B
  acc1 | Accumulator 1 input

Returns
  Result of operation

## ◆ msc_elem_32_2() [3/8]

v32acc32 msc_elem_32_2 | ( | v64int8 | a,
|  | v64int8 | b,
|  | v32acc32 | acc1 )

Parameters

  a | Matrix A
  b | Matrix B
  acc1 | Accumulator 1 input

Returns
  Result of operation

## ◆ msc_elem_32_2() [4/8]

v32acc32 msc_elem_32_2 | ( | v64int8 | a,
|  | v64uint8 | b,
|  | v32acc32 | acc1 )

Parameters

  a | Matrix A
  b | Matrix B
  acc1 | Accumulator 1 input

Returns
  Result of operation

## ◆ msc_elem_32_2() [5/8]

v32acc32 msc_elem_32_2 | ( | v64uint8 | a,
|  | int | sgn_x,
|  | v64int8 | b,
|  | int | sgn_y,
|  | v32acc32 | acc1 )

Parameters

  a | Matrix A
  sgn_x | Sign mask for matrix A
  b | Matrix B
  sgn_y | Sign mask for matrix B
  acc1 | Accumulator 1 input

Returns
  Result of operation

## ◆ msc_elem_32_2() [6/8]

v32acc32 msc_elem_32_2 | ( | v64uint8 | a,
|  | int | sgn_x,
|  | v64uint8 | b,
|  | int | sgn_y,
|  | v32acc32 | acc1 )

Parameters

  a | Matrix A
  sgn_x | Sign mask for matrix A
  b | Matrix B
  sgn_y | Sign mask for matrix B
  acc1 | Accumulator 1 input

Returns
  Result of operation

## ◆ msc_elem_32_2() [7/8]

v32acc32 msc_elem_32_2 | ( | v64uint8 | a,
|  | v64int8 | b,
|  | v32acc32 | acc1 )

Parameters

  a | Matrix A
  b | Matrix B
  acc1 | Accumulator 1 input

Returns
  Result of operation

## ◆ msc_elem_32_2() [8/8]

v32acc32 msc_elem_32_2 | ( | v64uint8 | a,
|  | v64uint8 | b,
|  | v32acc32 | acc1 )

Parameters

  a | Matrix A
  b | Matrix B
  acc1 | Accumulator 1 input

Returns
  Result of operation

## ◆ msc_elem_32_2_conf() [1/8]

v32acc32 msc_elem_32_2_conf | ( | v64int8 | a,
|  | int | sgn_x,
|  | v64int8 | b,
|  | int | sgn_y,
|  | v32acc32 | acc1,
|  | int | zero_acc1,
|  | int | shift16,
|  | int | sub_mul,
|  | int | sub_acc1 )

Parameters

  a | Matrix A
  sgn_x | Sign mask for matrix A
  b | Matrix B
  sgn_y | Sign mask for matrix B
  acc1 | Accumulator 1 input
  zero_acc1 | Zeroing mask for acc1
  shift16 | Shift mask of input accumulator acc1
  sub_mul | Negation mask of multiplication result. If a bit is set the corresponding output accumulator lane is negated.
  sub_acc1 | Negation mask of acc1. If a bit is set the corresponding accumulator lane of acc1 is negated.

Returns
  Result of operation

## ◆ msc_elem_32_2_conf() [2/8]

v32acc32 msc_elem_32_2_conf | ( | v64int8 | a,
|  | int | sgn_x,
|  | v64uint8 | b,
|  | int | sgn_y,
|  | v32acc32 | acc1,
|  | int | zero_acc1,
|  | int | shift16,
|  | int | sub_mul,
|  | int | sub_acc1 )

Parameters

  a | Matrix A
  sgn_x | Sign mask for matrix A
  b | Matrix B
  sgn_y | Sign mask for matrix B
  acc1 | Accumulator 1 input
  zero_acc1 | Zeroing mask for acc1
  shift16 | Shift mask of input accumulator acc1
  sub_mul | Negation mask of multiplication result. If a bit is set the corresponding output accumulator lane is negated.
  sub_acc1 | Negation mask of acc1. If a bit is set the corresponding accumulator lane of acc1 is negated.

Returns
  Result of operation

## ◆ msc_elem_32_2_conf() [3/8]

v32acc32 msc_elem_32_2_conf | ( | v64int8 | a,
|  | v64int8 | b,
|  | v32acc32 | acc1,
|  | int | zero_acc1,
|  | int | shift16,
|  | int | sub_mul,
|  | int | sub_acc1 )

Parameters

  a | Matrix A
  b | Matrix B
  acc1 | Accumulator 1 input
  zero_acc1 | Zeroing mask for acc1
  shift16 | Shift mask of input accumulator acc1
  sub_mul | Negation mask of multiplication result
  sub_acc1 | Negation mask of acc1

Returns
  Result of operation

## ◆ msc_elem_32_2_conf() [4/8]

v32acc32 msc_elem_32_2_conf | ( | v64int8 | a,
|  | v64uint8 | b,
|  | v32acc32 | acc1,
|  | int | zero_acc1,
|  | int | shift16,
|  | int | sub_mul,
|  | int | sub_acc1 )

Parameters

  a | Matrix A
  b | Matrix B
  acc1 | Accumulator 1 input
  zero_acc1 | Zeroing mask for acc1
  shift16 | Shift mask of input accumulator acc1
  sub_mul | Negation mask of multiplication result
  sub_acc1 | Negation mask of acc1

Returns
  Result of operation

## ◆ msc_elem_32_2_conf() [5/8]

v32acc32 msc_elem_32_2_conf | ( | v64uint8 | a,
|  | int | sgn_x,
|  | v64int8 | b,
|  | int | sgn_y,
|  | v32acc32 | acc1,
|  | int | zero_acc1,
|  | int | shift16,
|  | int | sub_mul,
|  | int | sub_acc1 )

Parameters

  a | Matrix A
  sgn_x | Sign mask for matrix A
  b | Matrix B
  sgn_y | Sign mask for matrix B
  acc1 | Accumulator 1 input
  zero_acc1 | Zeroing mask for acc1
  shift16 | Shift mask of input accumulator acc1
  sub_mul | Negation mask of multiplication result. If a bit is set the corresponding output accumulator lane is negated.
  sub_acc1 | Negation mask of acc1. If a bit is set the corresponding accumulator lane of acc1 is negated.

Returns
  Result of operation

## ◆ msc_elem_32_2_conf() [6/8]

v32acc32 msc_elem_32_2_conf | ( | v64uint8 | a,
|  | int | sgn_x,
|  | v64uint8 | b,
|  | int | sgn_y,
|  | v32acc32 | acc1,
|  | int | zero_acc1,
|  | int | shift16,
|  | int | sub_mul,
|  | int | sub_acc1 )

Parameters

  a | Matrix A
  sgn_x | Sign mask for matrix A
  b | Matrix B
  sgn_y | Sign mask for matrix B
  acc1 | Accumulator 1 input
  zero_acc1 | Zeroing mask for acc1
  shift16 | Shift mask of input accumulator acc1
  sub_mul | Negation mask of multiplication result. If a bit is set the corresponding output accumulator lane is negated.
  sub_acc1 | Negation mask of acc1. If a bit is set the corresponding accumulator lane of acc1 is negated.

Returns
  Result of operation

## ◆ msc_elem_32_2_conf() [7/8]

v32acc32 msc_elem_32_2_conf | ( | v64uint8 | a,
|  | v64int8 | b,
|  | v32acc32 | acc1,
|  | int | zero_acc1,
|  | int | shift16,
|  | int | sub_mul,
|  | int | sub_acc1 )

Parameters

  a | Matrix A
  b | Matrix B
  acc1 | Accumulator 1 input
  zero_acc1 | Zeroing mask for acc1
  shift16 | Shift mask of input accumulator acc1
  sub_mul | Negation mask of multiplication result
  sub_acc1 | Negation mask of acc1

Returns
  Result of operation

## ◆ msc_elem_32_2_conf() [8/8]

v32acc32 msc_elem_32_2_conf | ( | v64uint8 | a,
|  | v64uint8 | b,
|  | v32acc32 | acc1,
|  | int | zero_acc1,
|  | int | shift16,
|  | int | sub_mul,
|  | int | sub_acc1 )

Parameters

  a | Matrix A
  b | Matrix B
  acc1 | Accumulator 1 input
  zero_acc1 | Zeroing mask for acc1
  shift16 | Shift mask of input accumulator acc1
  sub_mul | Negation mask of multiplication result
  sub_acc1 | Negation mask of acc1

Returns
  Result of operation

## ◆ mul_4x8_8x8() [1/8]

v32acc32 mul_4x8_8x8 | ( | v64int8 | a,
|  | int | sgn_x,
|  | v64int8 | b,
|  | int | sgn_y )

Parameters

  a | Matrix A
  sgn_x | Sign mask for matrix A
  b | Matrix B
  sgn_y | Sign mask for matrix B

Returns
  Result of operation

## ◆ mul_4x8_8x8() [2/8]

v32acc32 mul_4x8_8x8 | ( | v64int8 | a,
|  | int | sgn_x,
|  | v64uint8 | b,
|  | int | sgn_y )

Parameters

  a | Matrix A
  sgn_x | Sign mask for matrix A
  b | Matrix B
  sgn_y | Sign mask for matrix B

Returns
  Result of operation

## ◆ mul_4x8_8x8() [3/8]

v32acc32 mul_4x8_8x8 | ( | v64int8 | a,
|  | v64int8 | b )

Parameters

  a | Matrix A
  b | Matrix B

Returns
  Result of operation

## ◆ mul_4x8_8x8() [4/8]

v32acc32 mul_4x8_8x8 | ( | v64int8 | a,
|  | v64uint8 | b )

Parameters

  a | Matrix A
  b | Matrix B

Returns
  Result of operation

## ◆ mul_4x8_8x8() [5/8]

v32acc32 mul_4x8_8x8 | ( | v64uint8 | a,
|  | int | sgn_x,
|  | v64int8 | b,
|  | int | sgn_y )

Parameters

  a | Matrix A
  sgn_x | Sign mask for matrix A
  b | Matrix B
  sgn_y | Sign mask for matrix B

Returns
  Result of operation

## ◆ mul_4x8_8x8() [6/8]

v32acc32 mul_4x8_8x8 | ( | v64uint8 | a,
|  | int | sgn_x,
|  | v64uint8 | b,
|  | int | sgn_y )

Parameters

  a | Matrix A
  sgn_x | Sign mask for matrix A
  b | Matrix B
  sgn_y | Sign mask for matrix B

Returns
  Result of operation

## ◆ mul_4x8_8x8() [7/8]

v32acc32 mul_4x8_8x8 | ( | v64uint8 | a,
|  | v64int8 | b )

Parameters

  a | Matrix A
  b | Matrix B

Returns
  Result of operation

## ◆ mul_4x8_8x8() [8/8]

v32acc32 mul_4x8_8x8 | ( | v64uint8 | a,
|  | v64uint8 | b )

Parameters

  a | Matrix A
  b | Matrix B

Returns
  Result of operation

## ◆ mul_4x8_8x8_conf() [1/8]

v32acc32 mul_4x8_8x8_conf | ( | v64int8 | a,
|  | int | sgn_x,
|  | v64int8 | b,
|  | int | sgn_y,
|  | int | sub_mul )

Parameters

  a | Matrix A
  sgn_x | Sign mask for matrix A
  b | Matrix B
  sgn_y | Sign mask for matrix B
  sub_mul | Negation mask of multiplication result. If a bit is set the corresponding output accumulator lane is negated.

Returns
  Result of operation

## ◆ mul_4x8_8x8_conf() [2/8]

v32acc32 mul_4x8_8x8_conf | ( | v64int8 | a,
|  | int | sgn_x,
|  | v64uint8 | b,
|  | int | sgn_y,
|  | int | sub_mul )

Parameters

  a | Matrix A
  sgn_x | Sign mask for matrix A
  b | Matrix B
  sgn_y | Sign mask for matrix B
  sub_mul | Negation mask of multiplication result. If a bit is set the corresponding output accumulator lane is negated.

Returns
  Result of operation

## ◆ mul_4x8_8x8_conf() [3/8]

v32acc32 mul_4x8_8x8_conf | ( | v64int8 | a,
|  | v64int8 | b,
|  | int | sub_mul )

Parameters

  a | Matrix A
  b | Matrix B
  sub_mul | Negation mask for multiplication result

Returns
  Result of operation

## ◆ mul_4x8_8x8_conf() [4/8]

v32acc32 mul_4x8_8x8_conf | ( | v64int8 | a,
|  | v64uint8 | b,
|  | int | sub_mul )

Parameters

  a | Matrix A
  b | Matrix B
  sub_mul | Negation mask for multiplication result

Returns
  Result of operation

## ◆ mul_4x8_8x8_conf() [5/8]

v32acc32 mul_4x8_8x8_conf | ( | v64uint8 | a,
|  | int | sgn_x,
|  | v64int8 | b,
|  | int | sgn_y,
|  | int | sub_mul )

Parameters

  a | Matrix A
  sgn_x | Sign mask for matrix A
  b | Matrix B
  sgn_y | Sign mask for matrix B
  sub_mul | Negation mask of multiplication result. If a bit is set the corresponding output accumulator lane is negated.

Returns
  Result of operation

## ◆ mul_4x8_8x8_conf() [6/8]

v32acc32 mul_4x8_8x8_conf | ( | v64uint8 | a,
|  | int | sgn_x,
|  | v64uint8 | b,
|  | int | sgn_y,
|  | int | sub_mul )

Parameters

  a | Matrix A
  sgn_x | Sign mask for matrix A
  b | Matrix B
  sgn_y | Sign mask for matrix B
  sub_mul | Negation mask of multiplication result. If a bit is set the corresponding output accumulator lane is negated.

Returns
  Result of operation

## ◆ mul_4x8_8x8_conf() [7/8]

v32acc32 mul_4x8_8x8_conf | ( | v64uint8 | a,
|  | v64int8 | b,
|  | int | sub_mul )

Parameters

  a | Matrix A
  b | Matrix B
  sub_mul | Negation mask for multiplication result

Returns
  Result of operation

## ◆ mul_4x8_8x8_conf() [8/8]

v32acc32 mul_4x8_8x8_conf | ( | v64uint8 | a,
|  | v64uint8 | b,
|  | int | sub_mul )

Parameters

  a | Matrix A
  b | Matrix B
  sub_mul | Negation mask for multiplication result

Returns
  Result of operation

## ◆ mul_conv_32x8() [1/8]

v32acc32 mul_conv_32x8 | ( | v64int8 | a,
|  | int | sgn_x,
|  | v64int8 | b,
|  | int | sgn_y )

Parameters

  a | Matrix A
  sgn_x | Sign mask for matrix A
  b | Matrix B
  sgn_y | Sign mask for matrix B

Returns
  Result of operation

## ◆ mul_conv_32x8() [2/8]

v32acc32 mul_conv_32x8 | ( | v64int8 | a,
|  | int | sgn_x,
|  | v64uint8 | b,
|  | int | sgn_y )

Parameters

  a | Matrix A
  sgn_x | Sign mask for matrix A
  b | Matrix B
  sgn_y | Sign mask for matrix B

Returns
  Result of operation

## ◆ mul_conv_32x8() [3/8]

v32acc32 mul_conv_32x8 | ( | v64int8 | a,
|  | v64int8 | b )

Parameters

  a | Matrix A
  b | Matrix B

Returns
  Result of operation

## ◆ mul_conv_32x8() [4/8]

v32acc32 mul_conv_32x8 | ( | v64int8 | a,
|  | v64uint8 | b )

Parameters

  a | Matrix A
  b | Matrix B

Returns
  Result of operation

## ◆ mul_conv_32x8() [5/8]

v32acc32 mul_conv_32x8 | ( | v64uint8 | a,
|  | int | sgn_x,
|  | v64int8 | b,
|  | int | sgn_y )

Parameters

  a | Matrix A
  sgn_x | Sign mask for matrix A
  b | Matrix B
  sgn_y | Sign mask for matrix B

Returns
  Result of operation

## ◆ mul_conv_32x8() [6/8]

v32acc32 mul_conv_32x8 | ( | v64uint8 | a,
|  | int | sgn_x,
|  | v64uint8 | b,
|  | int | sgn_y )

Parameters

  a | Matrix A
  sgn_x | Sign mask for matrix A
  b | Matrix B
  sgn_y | Sign mask for matrix B

Returns
  Result of operation

## ◆ mul_conv_32x8() [7/8]

v32acc32 mul_conv_32x8 | ( | v64uint8 | a,
|  | v64int8 | b )

Parameters

  a | Matrix A
  b | Matrix B

Returns
  Result of operation

## ◆ mul_conv_32x8() [8/8]

v32acc32 mul_conv_32x8 | ( | v64uint8 | a,
|  | v64uint8 | b )

Parameters

  a | Matrix A
  b | Matrix B

Returns
  Result of operation

## ◆ mul_conv_32x8_conf() [1/8]

v32acc32 mul_conv_32x8_conf | ( | v64int8 | a,
|  | int | sgn_x,
|  | v64int8 | b,
|  | int | sgn_y,
|  | int | sub_mul )

Parameters

  a | Matrix A
  sgn_x | Sign mask for matrix A
  b | Matrix B
  sgn_y | Sign mask for matrix B
  sub_mul | Negation mask of multiplication result. If a bit is set the corresponding output accumulator lane is negated.

Returns
  Result of operation

## ◆ mul_conv_32x8_conf() [2/8]

v32acc32 mul_conv_32x8_conf | ( | v64int8 | a,
|  | int | sgn_x,
|  | v64uint8 | b,
|  | int | sgn_y,
|  | int | sub_mul )

Parameters

  a | Matrix A
  sgn_x | Sign mask for matrix A
  b | Matrix B
  sgn_y | Sign mask for matrix B
  sub_mul | Negation mask of multiplication result. If a bit is set the corresponding output accumulator lane is negated.

Returns
  Result of operation

## ◆ mul_conv_32x8_conf() [3/8]

v32acc32 mul_conv_32x8_conf | ( | v64int8 | a,
|  | v64int8 | b,
|  | int | sub_mul )

Parameters

  a | Matrix A
  b | Matrix B
  sub_mul | Negation mask for multiplication result

Returns
  Result of operation

## ◆ mul_conv_32x8_conf() [4/8]

v32acc32 mul_conv_32x8_conf | ( | v64int8 | a,
|  | v64uint8 | b,
|  | int | sub_mul )

Parameters

  a | Matrix A
  b | Matrix B
  sub_mul | Negation mask for multiplication result

Returns
  Result of operation

## ◆ mul_conv_32x8_conf() [5/8]

v32acc32 mul_conv_32x8_conf | ( | v64uint8 | a,
|  | int | sgn_x,
|  | v64int8 | b,
|  | int | sgn_y,
|  | int | sub_mul )

Parameters

  a | Matrix A
  sgn_x | Sign mask for matrix A
  b | Matrix B
  sgn_y | Sign mask for matrix B
  sub_mul | Negation mask of multiplication result. If a bit is set the corresponding output accumulator lane is negated.

Returns
  Result of operation

## ◆ mul_conv_32x8_conf() [6/8]

v32acc32 mul_conv_32x8_conf | ( | v64uint8 | a,
|  | int | sgn_x,
|  | v64uint8 | b,
|  | int | sgn_y,
|  | int | sub_mul )

Parameters

  a | Matrix A
  sgn_x | Sign mask for matrix A
  b | Matrix B
  sgn_y | Sign mask for matrix B
  sub_mul | Negation mask of multiplication result. If a bit is set the corresponding output accumulator lane is negated.

Returns
  Result of operation

## ◆ mul_conv_32x8_conf() [7/8]

v32acc32 mul_conv_32x8_conf | ( | v64uint8 | a,
|  | v64int8 | b,
|  | int | sub_mul )

Parameters

  a | Matrix A
  b | Matrix B
  sub_mul | Negation mask for multiplication result

Returns
  Result of operation

## ◆ mul_conv_32x8_conf() [8/8]

v32acc32 mul_conv_32x8_conf | ( | v64uint8 | a,
|  | v64uint8 | b,
|  | int | sub_mul )

Parameters

  a | Matrix A
  b | Matrix B
  sub_mul | Negation mask for multiplication result

Returns
  Result of operation

## ◆ mul_conv_4x4_8ch() [1/8]

v32acc32 mul_conv_4x4_8ch | ( | v64int8 | a,
|  | int | sgn_x,
|  | v64int8 | b,
|  | int | sgn_y )

Parameters

  a | Matrix A
  sgn_x | Sign mask for matrix A
  b | Matrix B
  sgn_y | Sign mask for matrix B

Returns
  Result of operation

## ◆ mul_conv_4x4_8ch() [2/8]

v32acc32 mul_conv_4x4_8ch | ( | v64int8 | a,
|  | int | sgn_x,
|  | v64uint8 | b,
|  | int | sgn_y )

Parameters

  a | Matrix A
  sgn_x | Sign mask for matrix A
  b | Matrix B
  sgn_y | Sign mask for matrix B

Returns
  Result of operation

## ◆ mul_conv_4x4_8ch() [3/8]

v32acc32 mul_conv_4x4_8ch | ( | v64int8 | a,
|  | v64int8 | b )

Parameters

  a | Matrix A
  b | Matrix B

Returns
  Result of operation

## ◆ mul_conv_4x4_8ch() [4/8]

v32acc32 mul_conv_4x4_8ch | ( | v64int8 | a,
|  | v64uint8 | b )

Parameters

  a | Matrix A
  b | Matrix B

Returns
  Result of operation

## ◆ mul_conv_4x4_8ch() [5/8]

v32acc32 mul_conv_4x4_8ch | ( | v64uint8 | a,
|  | int | sgn_x,
|  | v64int8 | b,
|  | int | sgn_y )

Parameters

  a | Matrix A
  sgn_x | Sign mask for matrix A
  b | Matrix B
  sgn_y | Sign mask for matrix B

Returns
  Result of operation

## ◆ mul_conv_4x4_8ch() [6/8]

v32acc32 mul_conv_4x4_8ch | ( | v64uint8 | a,
|  | int | sgn_x,
|  | v64uint8 | b,
|  | int | sgn_y )

Parameters

  a | Matrix A
  sgn_x | Sign mask for matrix A
  b | Matrix B
  sgn_y | Sign mask for matrix B

Returns
  Result of operation

## ◆ mul_conv_4x4_8ch() [7/8]

v32acc32 mul_conv_4x4_8ch | ( | v64uint8 | a,
|  | v64int8 | b )

Parameters

  a | Matrix A
  b | Matrix B

Returns
  Result of operation

## ◆ mul_conv_4x4_8ch() [8/8]

v32acc32 mul_conv_4x4_8ch | ( | v64uint8 | a,
|  | v64uint8 | b )

Parameters

  a | Matrix A
  b | Matrix B

Returns
  Result of operation

## ◆ mul_conv_4x4_8ch_conf() [1/8]

v32acc32 mul_conv_4x4_8ch_conf | ( | v64int8 | a,
|  | int | sgn_x,
|  | v64int8 | b,
|  | int | sgn_y,
|  | int | sub_mul )

Parameters

  a | Matrix A
  sgn_x | Sign mask for matrix A
  b | Matrix B
  sgn_y | Sign mask for matrix B
  sub_mul | Negation mask of multiplication result. If a bit is set the corresponding output accumulator lane is negated.

Returns
  Result of operation

## ◆ mul_conv_4x4_8ch_conf() [2/8]

v32acc32 mul_conv_4x4_8ch_conf | ( | v64int8 | a,
|  | int | sgn_x,
|  | v64uint8 | b,
|  | int | sgn_y,
|  | int | sub_mul )

Parameters

  a | Matrix A
  sgn_x | Sign mask for matrix A
  b | Matrix B
  sgn_y | Sign mask for matrix B
  sub_mul | Negation mask of multiplication result. If a bit is set the corresponding output accumulator lane is negated.

Returns
  Result of operation

## ◆ mul_conv_4x4_8ch_conf() [3/8]

v32acc32 mul_conv_4x4_8ch_conf | ( | v64int8 | a,
|  | v64int8 | b,
|  | int | sub_mul )

Parameters

  a | Matrix A
  b | Matrix B
  sub_mul | Negation mask for multiplication result

Returns
  Result of operation

## ◆ mul_conv_4x4_8ch_conf() [4/8]

v32acc32 mul_conv_4x4_8ch_conf | ( | v64int8 | a,
|  | v64uint8 | b,
|  | int | sub_mul )

Parameters

  a | Matrix A
  b | Matrix B
  sub_mul | Negation mask for multiplication result

Returns
  Result of operation

## ◆ mul_conv_4x4_8ch_conf() [5/8]

v32acc32 mul_conv_4x4_8ch_conf | ( | v64uint8 | a,
|  | int | sgn_x,
|  | v64int8 | b,
|  | int | sgn_y,
|  | int | sub_mul )

Parameters

  a | Matrix A
  sgn_x | Sign mask for matrix A
  b | Matrix B
  sgn_y | Sign mask for matrix B
  sub_mul | Negation mask of multiplication result. If a bit is set the corresponding output accumulator lane is negated.

Returns
  Result of operation

## ◆ mul_conv_4x4_8ch_conf() [6/8]

v32acc32 mul_conv_4x4_8ch_conf | ( | v64uint8 | a,
|  | int | sgn_x,
|  | v64uint8 | b,
|  | int | sgn_y,
|  | int | sub_mul )

Parameters

  a | Matrix A
  sgn_x | Sign mask for matrix A
  b | Matrix B
  sgn_y | Sign mask for matrix B
  sub_mul | Negation mask of multiplication result. If a bit is set the corresponding output accumulator lane is negated.

Returns
  Result of operation

## ◆ mul_conv_4x4_8ch_conf() [7/8]

v32acc32 mul_conv_4x4_8ch_conf | ( | v64uint8 | a,
|  | v64int8 | b,
|  | int | sub_mul )

Parameters

  a | Matrix A
  b | Matrix B
  sub_mul | Negation mask for multiplication result

Returns
  Result of operation

## ◆ mul_conv_4x4_8ch_conf() [8/8]

v32acc32 mul_conv_4x4_8ch_conf | ( | v64uint8 | a,
|  | v64uint8 | b,
|  | int | sub_mul )

Parameters

  a | Matrix A
  b | Matrix B
  sub_mul | Negation mask for multiplication result

Returns
  Result of operation

## ◆ mul_conv_8x8_4ch() [1/8]

v32acc32 mul_conv_8x8_4ch | ( | v64int8 | a,
|  | int | sgn_x,
|  | v64int8 | b,
|  | int | sgn_y )

Parameters

  a | Matrix A
  sgn_x | Sign mask for matrix A
  b | Matrix B
  sgn_y | Sign mask for matrix B

Returns
  Result of operation

## ◆ mul_conv_8x8_4ch() [2/8]

v32acc32 mul_conv_8x8_4ch | ( | v64int8 | a,
|  | int | sgn_x,
|  | v64uint8 | b,
|  | int | sgn_y )

Parameters

  a | Matrix A
  sgn_x | Sign mask for matrix A
  b | Matrix B
  sgn_y | Sign mask for matrix B

Returns
  Result of operation

## ◆ mul_conv_8x8_4ch() [3/8]

v32acc32 mul_conv_8x8_4ch | ( | v64int8 | a,
|  | v64int8 | b )

Parameters

  a | Matrix A
  b | Matrix B

Returns
  Result of operation

## ◆ mul_conv_8x8_4ch() [4/8]

v32acc32 mul_conv_8x8_4ch | ( | v64int8 | a,
|  | v64uint8 | b )

Parameters

  a | Matrix A
  b | Matrix B

Returns
  Result of operation

## ◆ mul_conv_8x8_4ch() [5/8]

v32acc32 mul_conv_8x8_4ch | ( | v64uint8 | a,
|  | int | sgn_x,
|  | v64int8 | b,
|  | int | sgn_y )

Parameters

  a | Matrix A
  sgn_x | Sign mask for matrix A
  b | Matrix B
  sgn_y | Sign mask for matrix B

Returns
  Result of operation

## ◆ mul_conv_8x8_4ch() [6/8]

v32acc32 mul_conv_8x8_4ch | ( | v64uint8 | a,
|  | int | sgn_x,
|  | v64uint8 | b,
|  | int | sgn_y )

Parameters

  a | Matrix A
  sgn_x | Sign mask for matrix A
  b | Matrix B
  sgn_y | Sign mask for matrix B

Returns
  Result of operation

## ◆ mul_conv_8x8_4ch() [7/8]

v32acc32 mul_conv_8x8_4ch | ( | v64uint8 | a,
|  | v64int8 | b )

Parameters

  a | Matrix A
  b | Matrix B

Returns
  Result of operation

## ◆ mul_conv_8x8_4ch() [8/8]

v32acc32 mul_conv_8x8_4ch | ( | v64uint8 | a,
|  | v64uint8 | b )

Parameters

  a | Matrix A
  b | Matrix B

Returns
  Result of operation

## ◆ mul_conv_8x8_4ch_conf() [1/8]

v32acc32 mul_conv_8x8_4ch_conf | ( | v64int8 | a,
|  | int | sgn_x,
|  | v64int8 | b,
|  | int | sgn_y,
|  | int | sub_mul )

Parameters

  a | Matrix A
  sgn_x | Sign mask for matrix A
  b | Matrix B
  sgn_y | Sign mask for matrix B
  sub_mul | Negation mask of multiplication result. If a bit is set the corresponding output accumulator lane is negated.

Returns
  Result of operation

## ◆ mul_conv_8x8_4ch_conf() [2/8]

v32acc32 mul_conv_8x8_4ch_conf | ( | v64int8 | a,
|  | int | sgn_x,
|  | v64uint8 | b,
|  | int | sgn_y,
|  | int | sub_mul )

Parameters

  a | Matrix A
  sgn_x | Sign mask for matrix A
  b | Matrix B
  sgn_y | Sign mask for matrix B
  sub_mul | Negation mask of multiplication result. If a bit is set the corresponding output accumulator lane is negated.

Returns
  Result of operation

## ◆ mul_conv_8x8_4ch_conf() [3/8]

v32acc32 mul_conv_8x8_4ch_conf | ( | v64int8 | a,
|  | v64int8 | b,
|  | int | sub_mul )

Parameters

  a | Matrix A
  b | Matrix B
  sub_mul | Negation mask for multiplication result

Returns
  Result of operation

## ◆ mul_conv_8x8_4ch_conf() [4/8]

v32acc32 mul_conv_8x8_4ch_conf | ( | v64int8 | a,
|  | v64uint8 | b,
|  | int | sub_mul )

Parameters

  a | Matrix A
  b | Matrix B
  sub_mul | Negation mask for multiplication result

Returns
  Result of operation

## ◆ mul_conv_8x8_4ch_conf() [5/8]

v32acc32 mul_conv_8x8_4ch_conf | ( | v64uint8 | a,
|  | int | sgn_x,
|  | v64int8 | b,
|  | int | sgn_y,
|  | int | sub_mul )

Parameters

  a | Matrix A
  sgn_x | Sign mask for matrix A
  b | Matrix B
  sgn_y | Sign mask for matrix B
  sub_mul | Negation mask of multiplication result. If a bit is set the corresponding output accumulator lane is negated.

Returns
  Result of operation

## ◆ mul_conv_8x8_4ch_conf() [6/8]

v32acc32 mul_conv_8x8_4ch_conf | ( | v64uint8 | a,
|  | int | sgn_x,
|  | v64uint8 | b,
|  | int | sgn_y,
|  | int | sub_mul )

Parameters

  a | Matrix A
  sgn_x | Sign mask for matrix A
  b | Matrix B
  sgn_y | Sign mask for matrix B
  sub_mul | Negation mask of multiplication result. If a bit is set the corresponding output accumulator lane is negated.

Returns
  Result of operation

## ◆ mul_conv_8x8_4ch_conf() [7/8]

v32acc32 mul_conv_8x8_4ch_conf | ( | v64uint8 | a,
|  | v64int8 | b,
|  | int | sub_mul )

Parameters

  a | Matrix A
  b | Matrix B
  sub_mul | Negation mask for multiplication result

Returns
  Result of operation

## ◆ mul_conv_8x8_4ch_conf() [8/8]

v32acc32 mul_conv_8x8_4ch_conf | ( | v64uint8 | a,
|  | v64uint8 | b,
|  | int | sub_mul )

Parameters

  a | Matrix A
  b | Matrix B
  sub_mul | Negation mask for multiplication result

Returns
  Result of operation

## ◆ mul_elem_32_2() [1/8]

v32acc32 mul_elem_32_2 | ( | v64int8 | a,
|  | int | sgn_x,
|  | v64int8 | b,
|  | int | sgn_y )

Parameters

  a | Matrix A
  sgn_x | Sign mask for matrix A
  b | Matrix B
  sgn_y | Sign mask for matrix B

Returns
  Result of operation

## ◆ mul_elem_32_2() [2/8]

v32acc32 mul_elem_32_2 | ( | v64int8 | a,
|  | int | sgn_x,
|  | v64uint8 | b,
|  | int | sgn_y )

Parameters

  a | Matrix A
  sgn_x | Sign mask for matrix A
  b | Matrix B
  sgn_y | Sign mask for matrix B

Returns
  Result of operation

## ◆ mul_elem_32_2() [3/8]

v32acc32 mul_elem_32_2 | ( | v64int8 | a,
|  | v64int8 | b )

Parameters

  a | Matrix A
  b | Matrix B

Returns
  Result of operation

## ◆ mul_elem_32_2() [4/8]

v32acc32 mul_elem_32_2 | ( | v64int8 | a,
|  | v64uint8 | b )

Parameters

  a | Matrix A
  b | Matrix B

Returns
  Result of operation

## ◆ mul_elem_32_2() [5/8]

v32acc32 mul_elem_32_2 | ( | v64uint8 | a,
|  | int | sgn_x,
|  | v64int8 | b,
|  | int | sgn_y )

Parameters

  a | Matrix A
  sgn_x | Sign mask for matrix A
  b | Matrix B
  sgn_y | Sign mask for matrix B

Returns
  Result of operation

## ◆ mul_elem_32_2() [6/8]

v32acc32 mul_elem_32_2 | ( | v64uint8 | a,
|  | int | sgn_x,
|  | v64uint8 | b,
|  | int | sgn_y )

Parameters

  a | Matrix A
  sgn_x | Sign mask for matrix A
  b | Matrix B
  sgn_y | Sign mask for matrix B

Returns
  Result of operation

## ◆ mul_elem_32_2() [7/8]

v32acc32 mul_elem_32_2 | ( | v64uint8 | a,
|  | v64int8 | b )

Parameters

  a | Matrix A
  b | Matrix B

Returns
  Result of operation

## ◆ mul_elem_32_2() [8/8]

v32acc32 mul_elem_32_2 | ( | v64uint8 | a,
|  | v64uint8 | b )

Parameters

  a | Matrix A
  b | Matrix B

Returns
  Result of operation

## ◆ mul_elem_32_2_conf() [1/8]

v32acc32 mul_elem_32_2_conf | ( | v64int8 | a,
|  | int | sgn_x,
|  | v64int8 | b,
|  | int | sgn_y,
|  | int | sub_mul )

Parameters

  a | Matrix A
  sgn_x | Sign mask for matrix A
  b | Matrix B
  sgn_y | Sign mask for matrix B
  sub_mul | Negation mask of multiplication result. If a bit is set the corresponding output accumulator lane is negated.

Returns
  Result of operation

## ◆ mul_elem_32_2_conf() [2/8]

v32acc32 mul_elem_32_2_conf | ( | v64int8 | a,
|  | int | sgn_x,
|  | v64uint8 | b,
|  | int | sgn_y,
|  | int | sub_mul )

Parameters

  a | Matrix A
  sgn_x | Sign mask for matrix A
  b | Matrix B
  sgn_y | Sign mask for matrix B
  sub_mul | Negation mask of multiplication result. If a bit is set the corresponding output accumulator lane is negated.

Returns
  Result of operation

## ◆ mul_elem_32_2_conf() [3/8]

v32acc32 mul_elem_32_2_conf | ( | v64int8 | a,
|  | v64int8 | b,
|  | int | sub_mul )

Parameters

  a | Matrix A
  b | Matrix B
  sub_mul | Negation mask for multiplication result

Returns
  Result of operation

## ◆ mul_elem_32_2_conf() [4/8]

v32acc32 mul_elem_32_2_conf | ( | v64int8 | a,
|  | v64uint8 | b,
|  | int | sub_mul )

Parameters

  a | Matrix A
  b | Matrix B
  sub_mul | Negation mask for multiplication result

Returns
  Result of operation

## ◆ mul_elem_32_2_conf() [5/8]

v32acc32 mul_elem_32_2_conf | ( | v64uint8 | a,
|  | int | sgn_x,
|  | v64int8 | b,
|  | int | sgn_y,
|  | int | sub_mul )

Parameters

  a | Matrix A
  sgn_x | Sign mask for matrix A
  b | Matrix B
  sgn_y | Sign mask for matrix B
  sub_mul | Negation mask of multiplication result. If a bit is set the corresponding output accumulator lane is negated.

Returns
  Result of operation

## ◆ mul_elem_32_2_conf() [6/8]

v32acc32 mul_elem_32_2_conf | ( | v64uint8 | a,
|  | int | sgn_x,
|  | v64uint8 | b,
|  | int | sgn_y,
|  | int | sub_mul )

Parameters

  a | Matrix A
  sgn_x | Sign mask for matrix A
  b | Matrix B
  sgn_y | Sign mask for matrix B
  sub_mul | Negation mask of multiplication result. If a bit is set the corresponding output accumulator lane is negated.

Returns
  Result of operation

## ◆ mul_elem_32_2_conf() [7/8]

v32acc32 mul_elem_32_2_conf | ( | v64uint8 | a,
|  | v64int8 | b,
|  | int | sub_mul )

Parameters

  a | Matrix A
  b | Matrix B
  sub_mul | Negation mask for multiplication result

Returns
  Result of operation

## ◆ mul_elem_32_2_conf() [8/8]

v32acc32 mul_elem_32_2_conf | ( | v64uint8 | a,
|  | v64uint8 | b,
|  | int | sub_mul )

Parameters

  a | Matrix A
  b | Matrix B
  sub_mul | Negation mask for multiplication result

Returns
  Result of operation

## ◆ negmac_4x8_8x8() [1/8]

v32acc32 negmac_4x8_8x8 | ( | v64int8 | a,
|  | int | sgn_x,
|  | v64int8 | b,
|  | int | sgn_y,
|  | v32acc32 | acc1 )

Parameters

  a | Matrix A
  sgn_x | Sign mask for matrix A
  b | Matrix B
  sgn_y | Sign mask for matrix B
  acc1 | Accumulator 1 input

Returns
  Result of operation

## ◆ negmac_4x8_8x8() [2/8]

v32acc32 negmac_4x8_8x8 | ( | v64int8 | a,
|  | int | sgn_x,
|  | v64uint8 | b,
|  | int | sgn_y,
|  | v32acc32 | acc1 )

Parameters

  a | Matrix A
  sgn_x | Sign mask for matrix A
  b | Matrix B
  sgn_y | Sign mask for matrix B
  acc1 | Accumulator 1 input

Returns
  Result of operation

## ◆ negmac_4x8_8x8() [3/8]

v32acc32 negmac_4x8_8x8 | ( | v64int8 | a,
|  | v64int8 | b,
|  | v32acc32 | acc1 )

Parameters

  a | Matrix A
  b | Matrix B
  acc1 | Accumulator 1 input

Returns
  Result of MAC operation

## ◆ negmac_4x8_8x8() [4/8]

v32acc32 negmac_4x8_8x8 | ( | v64int8 | a,
|  | v64uint8 | b,
|  | v32acc32 | acc1 )

Parameters

  a | Matrix A
  b | Matrix B
  acc1 | Accumulator 1 input

Returns
  Result of MAC operation

## ◆ negmac_4x8_8x8() [5/8]

v32acc32 negmac_4x8_8x8 | ( | v64uint8 | a,
|  | int | sgn_x,
|  | v64int8 | b,
|  | int | sgn_y,
|  | v32acc32 | acc1 )

Parameters

  a | Matrix A
  sgn_x | Sign mask for matrix A
  b | Matrix B
  sgn_y | Sign mask for matrix B
  acc1 | Accumulator 1 input

Returns
  Result of operation

## ◆ negmac_4x8_8x8() [6/8]

v32acc32 negmac_4x8_8x8 | ( | v64uint8 | a,
|  | int | sgn_x,
|  | v64uint8 | b,
|  | int | sgn_y,
|  | v32acc32 | acc1 )

Parameters

  a | Matrix A
  sgn_x | Sign mask for matrix A
  b | Matrix B
  sgn_y | Sign mask for matrix B
  acc1 | Accumulator 1 input

Returns
  Result of operation

## ◆ negmac_4x8_8x8() [7/8]

v32acc32 negmac_4x8_8x8 | ( | v64uint8 | a,
|  | v64int8 | b,
|  | v32acc32 | acc1 )

Parameters

  a | Matrix A
  b | Matrix B
  acc1 | Accumulator 1 input

Returns
  Result of MAC operation

## ◆ negmac_4x8_8x8() [8/8]

v32acc32 negmac_4x8_8x8 | ( | v64uint8 | a,
|  | v64uint8 | b,
|  | v32acc32 | acc1 )

Parameters

  a | Matrix A
  b | Matrix B
  acc1 | Accumulator 1 input

Returns
  Result of MAC operation

## ◆ negmac_4x8_8x8_conf() [1/8]

v32acc32 negmac_4x8_8x8_conf | ( | v64int8 | a,
|  | int | sgn_x,
|  | v64int8 | b,
|  | int | sgn_y,
|  | v32acc32 | acc1,
|  | int | zero_acc1,
|  | int | sub_mul,
|  | int | sub_acc1 )

Parameters

  a | Matrix A
  sgn_x | Sign mask for matrix A
  b | Matrix B
  sgn_y | Sign mask for matrix B
  acc1 | Accumulator 1 input
  zero_acc1 | Zeroing mask for acc1
  sub_mul | Negation mask of multiplication result
  sub_acc1 | Negation mask of acc1

Returns
  Result of operation

## ◆ negmac_4x8_8x8_conf() [2/8]

v32acc32 negmac_4x8_8x8_conf | ( | v64int8 | a,
|  | int | sgn_x,
|  | v64uint8 | b,
|  | int | sgn_y,
|  | v32acc32 | acc1,
|  | int | zero_acc1,
|  | int | sub_mul,
|  | int | sub_acc1 )

Parameters

  a | Matrix A
  sgn_x | Sign mask for matrix A
  b | Matrix B
  sgn_y | Sign mask for matrix B
  acc1 | Accumulator 1 input
  zero_acc1 | Zeroing mask for acc1
  sub_mul | Negation mask of multiplication result
  sub_acc1 | Negation mask of acc1

Returns
  Result of operation

## ◆ negmac_4x8_8x8_conf() [3/8]

v32acc32 negmac_4x8_8x8_conf | ( | v64int8 | a,
|  | v64int8 | b,
|  | v32acc32 | acc1,
|  | int | zero_acc1,
|  | int | sub_mul,
|  | int | sub_acc1 )

Parameters

  a | Matrix A
  b | Matrix B
  acc1 | Accumulator 1 input
  zero_acc1 | Zeroing mask for acc1
  sub_mul | Negation mask of multiplication result
  sub_acc1 | Negation mask of acc1

Returns
  Result of operation

## ◆ negmac_4x8_8x8_conf() [4/8]

v32acc32 negmac_4x8_8x8_conf | ( | v64int8 | a,
|  | v64uint8 | b,
|  | v32acc32 | acc1,
|  | int | zero_acc1,
|  | int | sub_mul,
|  | int | sub_acc1 )

Parameters

  a | Matrix A
  b | Matrix B
  acc1 | Accumulator 1 input
  zero_acc1 | Zeroing mask for acc1
  sub_mul | Negation mask of multiplication result
  sub_acc1 | Negation mask of acc1

Returns
  Result of operation

## ◆ negmac_4x8_8x8_conf() [5/8]

v32acc32 negmac_4x8_8x8_conf | ( | v64uint8 | a,
|  | int | sgn_x,
|  | v64int8 | b,
|  | int | sgn_y,
|  | v32acc32 | acc1,
|  | int | zero_acc1,
|  | int | sub_mul,
|  | int | sub_acc1 )

Parameters

  a | Matrix A
  sgn_x | Sign mask for matrix A
  b | Matrix B
  sgn_y | Sign mask for matrix B
  acc1 | Accumulator 1 input
  zero_acc1 | Zeroing mask for acc1
  sub_mul | Negation mask of multiplication result
  sub_acc1 | Negation mask of acc1

Returns
  Result of operation

## ◆ negmac_4x8_8x8_conf() [6/8]

v32acc32 negmac_4x8_8x8_conf | ( | v64uint8 | a,
|  | int | sgn_x,
|  | v64uint8 | b,
|  | int | sgn_y,
|  | v32acc32 | acc1,
|  | int | zero_acc1,
|  | int | sub_mul,
|  | int | sub_acc1 )

Parameters

  a | Matrix A
  sgn_x | Sign mask for matrix A
  b | Matrix B
  sgn_y | Sign mask for matrix B
  acc1 | Accumulator 1 input
  zero_acc1 | Zeroing mask for acc1
  sub_mul | Negation mask of multiplication result
  sub_acc1 | Negation mask of acc1

Returns
  Result of operation

## ◆ negmac_4x8_8x8_conf() [7/8]

v32acc32 negmac_4x8_8x8_conf | ( | v64uint8 | a,
|  | v64int8 | b,
|  | v32acc32 | acc1,
|  | int | zero_acc1,
|  | int | sub_mul,
|  | int | sub_acc1 )

Parameters

  a | Matrix A
  b | Matrix B
  acc1 | Accumulator 1 input
  zero_acc1 | Zeroing mask for acc1
  sub_mul | Negation mask of multiplication result
  sub_acc1 | Negation mask of acc1

Returns
  Result of operation

## ◆ negmac_4x8_8x8_conf() [8/8]

v32acc32 negmac_4x8_8x8_conf | ( | v64uint8 | a,
|  | v64uint8 | b,
|  | v32acc32 | acc1,
|  | int | zero_acc1,
|  | int | sub_mul,
|  | int | sub_acc1 )

Parameters

  a | Matrix A
  b | Matrix B
  acc1 | Accumulator 1 input
  zero_acc1 | Zeroing mask for acc1
  sub_mul | Negation mask of multiplication result
  sub_acc1 | Negation mask of acc1

Returns
  Result of operation

## ◆ negmac_conv_32x8() [1/8]

v32acc32 negmac_conv_32x8 | ( | v64int8 | a,
|  | int | sgn_x,
|  | v64int8 | b,
|  | int | sgn_y,
|  | v32acc32 | acc1 )

Parameters

  a | Matrix A
  sgn_x | Sign mask for matrix A
  b | Matrix B
  sgn_y | Sign mask for matrix B
  acc1 | Accumulator 1 input

Returns
  Result of operation

## ◆ negmac_conv_32x8() [2/8]

v32acc32 negmac_conv_32x8 | ( | v64int8 | a,
|  | int | sgn_x,
|  | v64uint8 | b,
|  | int | sgn_y,
|  | v32acc32 | acc1 )

Parameters

  a | Matrix A
  sgn_x | Sign mask for matrix A
  b | Matrix B
  sgn_y | Sign mask for matrix B
  acc1 | Accumulator 1 input

Returns
  Result of operation

## ◆ negmac_conv_32x8() [3/8]

v32acc32 negmac_conv_32x8 | ( | v64int8 | a,
|  | v64int8 | b,
|  | v32acc32 | acc1 )

Parameters

  a | Matrix A
  b | Matrix B
  acc1 | Accumulator 1 input

Returns
  Result of MAC operation

## ◆ negmac_conv_32x8() [4/8]

v32acc32 negmac_conv_32x8 | ( | v64int8 | a,
|  | v64uint8 | b,
|  | v32acc32 | acc1 )

Parameters

  a | Matrix A
  b | Matrix B
  acc1 | Accumulator 1 input

Returns
  Result of MAC operation

## ◆ negmac_conv_32x8() [5/8]

v32acc32 negmac_conv_32x8 | ( | v64uint8 | a,
|  | int | sgn_x,
|  | v64int8 | b,
|  | int | sgn_y,
|  | v32acc32 | acc1 )

Parameters

  a | Matrix A
  sgn_x | Sign mask for matrix A
  b | Matrix B
  sgn_y | Sign mask for matrix B
  acc1 | Accumulator 1 input

Returns
  Result of operation

## ◆ negmac_conv_32x8() [6/8]

v32acc32 negmac_conv_32x8 | ( | v64uint8 | a,
|  | int | sgn_x,
|  | v64uint8 | b,
|  | int | sgn_y,
|  | v32acc32 | acc1 )

Parameters

  a | Matrix A
  sgn_x | Sign mask for matrix A
  b | Matrix B
  sgn_y | Sign mask for matrix B
  acc1 | Accumulator 1 input

Returns
  Result of operation

## ◆ negmac_conv_32x8() [7/8]

v32acc32 negmac_conv_32x8 | ( | v64uint8 | a,
|  | v64int8 | b,
|  | v32acc32 | acc1 )

Parameters

  a | Matrix A
  b | Matrix B
  acc1 | Accumulator 1 input

Returns
  Result of MAC operation

## ◆ negmac_conv_32x8() [8/8]

v32acc32 negmac_conv_32x8 | ( | v64uint8 | a,
|  | v64uint8 | b,
|  | v32acc32 | acc1 )

Parameters

  a | Matrix A
  b | Matrix B
  acc1 | Accumulator 1 input

Returns
  Result of MAC operation

## ◆ negmac_conv_32x8_conf() [1/8]

v32acc32 negmac_conv_32x8_conf | ( | v64int8 | a,
|  | int | sgn_x,
|  | v64int8 | b,
|  | int | sgn_y,
|  | v32acc32 | acc1,
|  | int | zero_acc1,
|  | int | sub_mul,
|  | int | sub_acc1 )

Parameters

  a | Matrix A
  sgn_x | Sign mask for matrix A
  b | Matrix B
  sgn_y | Sign mask for matrix B
  acc1 | Accumulator 1 input
  zero_acc1 | Zeroing mask for acc1
  sub_mul | Negation mask of multiplication result
  sub_acc1 | Negation mask of acc1

Returns
  Result of operation

## ◆ negmac_conv_32x8_conf() [2/8]

v32acc32 negmac_conv_32x8_conf | ( | v64int8 | a,
|  | int | sgn_x,
|  | v64uint8 | b,
|  | int | sgn_y,
|  | v32acc32 | acc1,
|  | int | zero_acc1,
|  | int | sub_mul,
|  | int | sub_acc1 )

Parameters

  a | Matrix A
  sgn_x | Sign mask for matrix A
  b | Matrix B
  sgn_y | Sign mask for matrix B
  acc1 | Accumulator 1 input
  zero_acc1 | Zeroing mask for acc1
  sub_mul | Negation mask of multiplication result
  sub_acc1 | Negation mask of acc1

Returns
  Result of operation

## ◆ negmac_conv_32x8_conf() [3/8]

v32acc32 negmac_conv_32x8_conf | ( | v64int8 | a,
|  | v64int8 | b,
|  | v32acc32 | acc1,
|  | int | zero_acc1,
|  | int | sub_mul,
|  | int | sub_acc1 )

Parameters

  a | Matrix A
  b | Matrix B
  acc1 | Accumulator 1 input
  zero_acc1 | Zeroing mask for acc1
  sub_mul | Negation mask of multiplication result
  sub_acc1 | Negation mask of acc1

Returns
  Result of operation

## ◆ negmac_conv_32x8_conf() [4/8]

v32acc32 negmac_conv_32x8_conf | ( | v64int8 | a,
|  | v64uint8 | b,
|  | v32acc32 | acc1,
|  | int | zero_acc1,
|  | int | sub_mul,
|  | int | sub_acc1 )

Parameters

  a | Matrix A
  b | Matrix B
  acc1 | Accumulator 1 input
  zero_acc1 | Zeroing mask for acc1
  sub_mul | Negation mask of multiplication result
  sub_acc1 | Negation mask of acc1

Returns
  Result of operation

## ◆ negmac_conv_32x8_conf() [5/8]

v32acc32 negmac_conv_32x8_conf | ( | v64uint8 | a,
|  | int | sgn_x,
|  | v64int8 | b,
|  | int | sgn_y,
|  | v32acc32 | acc1,
|  | int | zero_acc1,
|  | int | sub_mul,
|  | int | sub_acc1 )

Parameters

  a | Matrix A
  sgn_x | Sign mask for matrix A
  b | Matrix B
  sgn_y | Sign mask for matrix B
  acc1 | Accumulator 1 input
  zero_acc1 | Zeroing mask for acc1
  sub_mul | Negation mask of multiplication result
  sub_acc1 | Negation mask of acc1

Returns
  Result of operation

## ◆ negmac_conv_32x8_conf() [6/8]

v32acc32 negmac_conv_32x8_conf | ( | v64uint8 | a,
|  | int | sgn_x,
|  | v64uint8 | b,
|  | int | sgn_y,
|  | v32acc32 | acc1,
|  | int | zero_acc1,
|  | int | sub_mul,
|  | int | sub_acc1 )

Parameters

  a | Matrix A
  sgn_x | Sign mask for matrix A
  b | Matrix B
  sgn_y | Sign mask for matrix B
  acc1 | Accumulator 1 input
  zero_acc1 | Zeroing mask for acc1
  sub_mul | Negation mask of multiplication result
  sub_acc1 | Negation mask of acc1

Returns
  Result of operation

## ◆ negmac_conv_32x8_conf() [7/8]

v32acc32 negmac_conv_32x8_conf | ( | v64uint8 | a,
|  | v64int8 | b,
|  | v32acc32 | acc1,
|  | int | zero_acc1,
|  | int | sub_mul,
|  | int | sub_acc1 )

Parameters

  a | Matrix A
  b | Matrix B
  acc1 | Accumulator 1 input
  zero_acc1 | Zeroing mask for acc1
  sub_mul | Negation mask of multiplication result
  sub_acc1 | Negation mask of acc1

Returns
  Result of operation

## ◆ negmac_conv_32x8_conf() [8/8]

v32acc32 negmac_conv_32x8_conf | ( | v64uint8 | a,
|  | v64uint8 | b,
|  | v32acc32 | acc1,
|  | int | zero_acc1,
|  | int | sub_mul,
|  | int | sub_acc1 )

Parameters

  a | Matrix A
  b | Matrix B
  acc1 | Accumulator 1 input
  zero_acc1 | Zeroing mask for acc1
  sub_mul | Negation mask of multiplication result
  sub_acc1 | Negation mask of acc1

Returns
  Result of operation

## ◆ negmac_conv_4x4_8ch() [1/8]

v32acc32 negmac_conv_4x4_8ch | ( | v64int8 | a,
|  | int | sgn_x,
|  | v64int8 | b,
|  | int | sgn_y,
|  | v32acc32 | acc1 )

Parameters

  a | Matrix A
  sgn_x | Sign mask for matrix A
  b | Matrix B
  sgn_y | Sign mask for matrix B
  acc1 | Accumulator 1 input

Returns
  Result of operation

## ◆ negmac_conv_4x4_8ch() [2/8]

v32acc32 negmac_conv_4x4_8ch | ( | v64int8 | a,
|  | int | sgn_x,
|  | v64uint8 | b,
|  | int | sgn_y,
|  | v32acc32 | acc1 )

Parameters

  a | Matrix A
  sgn_x | Sign mask for matrix A
  b | Matrix B
  sgn_y | Sign mask for matrix B
  acc1 | Accumulator 1 input

Returns
  Result of operation

## ◆ negmac_conv_4x4_8ch() [3/8]

v32acc32 negmac_conv_4x4_8ch | ( | v64int8 | a,
|  | v64int8 | b,
|  | v32acc32 | acc1 )

Parameters

  a | Matrix A
  b | Matrix B
  acc1 | Accumulator 1 input

Returns
  Result of MAC operation

## ◆ negmac_conv_4x4_8ch() [4/8]

v32acc32 negmac_conv_4x4_8ch | ( | v64int8 | a,
|  | v64uint8 | b,
|  | v32acc32 | acc1 )

Parameters

  a | Matrix A
  b | Matrix B
  acc1 | Accumulator 1 input

Returns
  Result of MAC operation

## ◆ negmac_conv_4x4_8ch() [5/8]

v32acc32 negmac_conv_4x4_8ch | ( | v64uint8 | a,
|  | int | sgn_x,
|  | v64int8 | b,
|  | int | sgn_y,
|  | v32acc32 | acc1 )

Parameters

  a | Matrix A
  sgn_x | Sign mask for matrix A
  b | Matrix B
  sgn_y | Sign mask for matrix B
  acc1 | Accumulator 1 input

Returns
  Result of operation

## ◆ negmac_conv_4x4_8ch() [6/8]

v32acc32 negmac_conv_4x4_8ch | ( | v64uint8 | a,
|  | int | sgn_x,
|  | v64uint8 | b,
|  | int | sgn_y,
|  | v32acc32 | acc1 )

Parameters

  a | Matrix A
  sgn_x | Sign mask for matrix A
  b | Matrix B
  sgn_y | Sign mask for matrix B
  acc1 | Accumulator 1 input

Returns
  Result of operation

## ◆ negmac_conv_4x4_8ch() [7/8]

v32acc32 negmac_conv_4x4_8ch | ( | v64uint8 | a,
|  | v64int8 | b,
|  | v32acc32 | acc1 )

Parameters

  a | Matrix A
  b | Matrix B
  acc1 | Accumulator 1 input

Returns
  Result of MAC operation

## ◆ negmac_conv_4x4_8ch() [8/8]

v32acc32 negmac_conv_4x4_8ch | ( | v64uint8 | a,
|  | v64uint8 | b,
|  | v32acc32 | acc1 )

Parameters

  a | Matrix A
  b | Matrix B
  acc1 | Accumulator 1 input

Returns
  Result of MAC operation

## ◆ negmac_conv_4x4_8ch_conf() [1/8]

v32acc32 negmac_conv_4x4_8ch_conf | ( | v64int8 | a,
|  | int | sgn_x,
|  | v64int8 | b,
|  | int | sgn_y,
|  | v32acc32 | acc1,
|  | int | zero_acc1,
|  | int | sub_mul,
|  | int | sub_acc1 )

Parameters

  a | Matrix A
  sgn_x | Sign mask for matrix A
  b | Matrix B
  sgn_y | Sign mask for matrix B
  acc1 | Accumulator 1 input
  zero_acc1 | Zeroing mask for acc1
  sub_mul | Negation mask of multiplication result
  sub_acc1 | Negation mask of acc1

Returns
  Result of operation

## ◆ negmac_conv_4x4_8ch_conf() [2/8]

v32acc32 negmac_conv_4x4_8ch_conf | ( | v64int8 | a,
|  | int | sgn_x,
|  | v64uint8 | b,
|  | int | sgn_y,
|  | v32acc32 | acc1,
|  | int | zero_acc1,
|  | int | sub_mul,
|  | int | sub_acc1 )

Parameters

  a | Matrix A
  sgn_x | Sign mask for matrix A
  b | Matrix B
  sgn_y | Sign mask for matrix B
  acc1 | Accumulator 1 input
  zero_acc1 | Zeroing mask for acc1
  sub_mul | Negation mask of multiplication result
  sub_acc1 | Negation mask of acc1

Returns
  Result of operation

## ◆ negmac_conv_4x4_8ch_conf() [3/8]

v32acc32 negmac_conv_4x4_8ch_conf | ( | v64int8 | a,
|  | v64int8 | b,
|  | v32acc32 | acc1,
|  | int | zero_acc1,
|  | int | sub_mul,
|  | int | sub_acc1 )

Parameters

  a | Matrix A
  b | Matrix B
  acc1 | Accumulator 1 input
  zero_acc1 | Zeroing mask for acc1
  sub_mul | Negation mask of multiplication result
  sub_acc1 | Negation mask of acc1

Returns
  Result of operation

## ◆ negmac_conv_4x4_8ch_conf() [4/8]

v32acc32 negmac_conv_4x4_8ch_conf | ( | v64int8 | a,
|  | v64uint8 | b,
|  | v32acc32 | acc1,
|  | int | zero_acc1,
|  | int | sub_mul,
|  | int | sub_acc1 )

Parameters

  a | Matrix A
  b | Matrix B
  acc1 | Accumulator 1 input
  zero_acc1 | Zeroing mask for acc1
  sub_mul | Negation mask of multiplication result
  sub_acc1 | Negation mask of acc1

Returns
  Result of operation

## ◆ negmac_conv_4x4_8ch_conf() [5/8]

v32acc32 negmac_conv_4x4_8ch_conf | ( | v64uint8 | a,
|  | int | sgn_x,
|  | v64int8 | b,
|  | int | sgn_y,
|  | v32acc32 | acc1,
|  | int | zero_acc1,
|  | int | sub_mul,
|  | int | sub_acc1 )

Parameters

  a | Matrix A
  sgn_x | Sign mask for matrix A
  b | Matrix B
  sgn_y | Sign mask for matrix B
  acc1 | Accumulator 1 input
  zero_acc1 | Zeroing mask for acc1
  sub_mul | Negation mask of multiplication result
  sub_acc1 | Negation mask of acc1

Returns
  Result of operation

## ◆ negmac_conv_4x4_8ch_conf() [6/8]

v32acc32 negmac_conv_4x4_8ch_conf | ( | v64uint8 | a,
|  | int | sgn_x,
|  | v64uint8 | b,
|  | int | sgn_y,
|  | v32acc32 | acc1,
|  | int | zero_acc1,
|  | int | sub_mul,
|  | int | sub_acc1 )

Parameters

  a | Matrix A
  sgn_x | Sign mask for matrix A
  b | Matrix B
  sgn_y | Sign mask for matrix B
  acc1 | Accumulator 1 input
  zero_acc1 | Zeroing mask for acc1
  sub_mul | Negation mask of multiplication result
  sub_acc1 | Negation mask of acc1

Returns
  Result of operation

## ◆ negmac_conv_4x4_8ch_conf() [7/8]

v32acc32 negmac_conv_4x4_8ch_conf | ( | v64uint8 | a,
|  | v64int8 | b,
|  | v32acc32 | acc1,
|  | int | zero_acc1,
|  | int | sub_mul,
|  | int | sub_acc1 )

Parameters

  a | Matrix A
  b | Matrix B
  acc1 | Accumulator 1 input
  zero_acc1 | Zeroing mask for acc1
  sub_mul | Negation mask of multiplication result
  sub_acc1 | Negation mask of acc1

Returns
  Result of operation

## ◆ negmac_conv_4x4_8ch_conf() [8/8]

v32acc32 negmac_conv_4x4_8ch_conf | ( | v64uint8 | a,
|  | v64uint8 | b,
|  | v32acc32 | acc1,
|  | int | zero_acc1,
|  | int | sub_mul,
|  | int | sub_acc1 )

Parameters

  a | Matrix A
  b | Matrix B
  acc1 | Accumulator 1 input
  zero_acc1 | Zeroing mask for acc1
  sub_mul | Negation mask of multiplication result
  sub_acc1 | Negation mask of acc1

Returns
  Result of operation

## ◆ negmac_conv_8x8_4ch() [1/8]

v32acc32 negmac_conv_8x8_4ch | ( | v64int8 | a,
|  | int | sgn_x,
|  | v64int8 | b,
|  | int | sgn_y,
|  | v32acc32 | acc1 )

Parameters

  a | Matrix A
  sgn_x | Sign mask for matrix A
  b | Matrix B
  sgn_y | Sign mask for matrix B
  acc1 | Accumulator 1 input

Returns
  Result of operation

## ◆ negmac_conv_8x8_4ch() [2/8]

v32acc32 negmac_conv_8x8_4ch | ( | v64int8 | a,
|  | int | sgn_x,
|  | v64uint8 | b,
|  | int | sgn_y,
|  | v32acc32 | acc1 )

Parameters

  a | Matrix A
  sgn_x | Sign mask for matrix A
  b | Matrix B
  sgn_y | Sign mask for matrix B
  acc1 | Accumulator 1 input

Returns
  Result of operation

## ◆ negmac_conv_8x8_4ch() [3/8]

v32acc32 negmac_conv_8x8_4ch | ( | v64int8 | a,
|  | v64int8 | b,
|  | v32acc32 | acc1 )

Parameters

  a | Matrix A
  b | Matrix B
  acc1 | Accumulator 1 input

Returns
  Result of MAC operation

## ◆ negmac_conv_8x8_4ch() [4/8]

v32acc32 negmac_conv_8x8_4ch | ( | v64int8 | a,
|  | v64uint8 | b,
|  | v32acc32 | acc1 )

Parameters

  a | Matrix A
  b | Matrix B
  acc1 | Accumulator 1 input

Returns
  Result of MAC operation

## ◆ negmac_conv_8x8_4ch() [5/8]

v32acc32 negmac_conv_8x8_4ch | ( | v64uint8 | a,
|  | int | sgn_x,
|  | v64int8 | b,
|  | int | sgn_y,
|  | v32acc32 | acc1 )

Parameters

  a | Matrix A
  sgn_x | Sign mask for matrix A
  b | Matrix B
  sgn_y | Sign mask for matrix B
  acc1 | Accumulator 1 input

Returns
  Result of operation

## ◆ negmac_conv_8x8_4ch() [6/8]

v32acc32 negmac_conv_8x8_4ch | ( | v64uint8 | a,
|  | int | sgn_x,
|  | v64uint8 | b,
|  | int | sgn_y,
|  | v32acc32 | acc1 )

Parameters

  a | Matrix A
  sgn_x | Sign mask for matrix A
  b | Matrix B
  sgn_y | Sign mask for matrix B
  acc1 | Accumulator 1 input

Returns
  Result of operation

## ◆ negmac_conv_8x8_4ch() [7/8]

v32acc32 negmac_conv_8x8_4ch | ( | v64uint8 | a,
|  | v64int8 | b,
|  | v32acc32 | acc1 )

Parameters

  a | Matrix A
  b | Matrix B
  acc1 | Accumulator 1 input

Returns
  Result of MAC operation

## ◆ negmac_conv_8x8_4ch() [8/8]

v32acc32 negmac_conv_8x8_4ch | ( | v64uint8 | a,
|  | v64uint8 | b,
|  | v32acc32 | acc1 )

Parameters

  a | Matrix A
  b | Matrix B
  acc1 | Accumulator 1 input

Returns
  Result of MAC operation

## ◆ negmac_conv_8x8_4ch_conf() [1/8]

v32acc32 negmac_conv_8x8_4ch_conf | ( | v64int8 | a,
|  | int | sgn_x,
|  | v64int8 | b,
|  | int | sgn_y,
|  | v32acc32 | acc1,
|  | int | zero_acc1,
|  | int | sub_mul,
|  | int | sub_acc1 )

Parameters

  a | Matrix A
  sgn_x | Sign mask for matrix A
  b | Matrix B
  sgn_y | Sign mask for matrix B
  acc1 | Accumulator 1 input
  zero_acc1 | Zeroing mask for acc1
  sub_mul | Negation mask of multiplication result
  sub_acc1 | Negation mask of acc1

Returns
  Result of operation

## ◆ negmac_conv_8x8_4ch_conf() [2/8]

v32acc32 negmac_conv_8x8_4ch_conf | ( | v64int8 | a,
|  | int | sgn_x,
|  | v64uint8 | b,
|  | int | sgn_y,
|  | v32acc32 | acc1,
|  | int | zero_acc1,
|  | int | sub_mul,
|  | int | sub_acc1 )

Parameters

  a | Matrix A
  sgn_x | Sign mask for matrix A
  b | Matrix B
  sgn_y | Sign mask for matrix B
  acc1 | Accumulator 1 input
  zero_acc1 | Zeroing mask for acc1
  sub_mul | Negation mask of multiplication result
  sub_acc1 | Negation mask of acc1

Returns
  Result of operation

## ◆ negmac_conv_8x8_4ch_conf() [3/8]

v32acc32 negmac_conv_8x8_4ch_conf | ( | v64int8 | a,
|  | v64int8 | b,
|  | v32acc32 | acc1,
|  | int | zero_acc1,
|  | int | sub_mul,
|  | int | sub_acc1 )

Parameters

  a | Matrix A
  b | Matrix B
  acc1 | Accumulator 1 input
  zero_acc1 | Zeroing mask for acc1
  sub_mul | Negation mask of multiplication result
  sub_acc1 | Negation mask of acc1

Returns
  Result of operation

## ◆ negmac_conv_8x8_4ch_conf() [4/8]

v32acc32 negmac_conv_8x8_4ch_conf | ( | v64int8 | a,
|  | v64uint8 | b,
|  | v32acc32 | acc1,
|  | int | zero_acc1,
|  | int | sub_mul,
|  | int | sub_acc1 )

Parameters

  a | Matrix A
  b | Matrix B
  acc1 | Accumulator 1 input
  zero_acc1 | Zeroing mask for acc1
  sub_mul | Negation mask of multiplication result
  sub_acc1 | Negation mask of acc1

Returns
  Result of operation

## ◆ negmac_conv_8x8_4ch_conf() [5/8]

v32acc32 negmac_conv_8x8_4ch_conf | ( | v64uint8 | a,
|  | int | sgn_x,
|  | v64int8 | b,
|  | int | sgn_y,
|  | v32acc32 | acc1,
|  | int | zero_acc1,
|  | int | sub_mul,
|  | int | sub_acc1 )

Parameters

  a | Matrix A
  sgn_x | Sign mask for matrix A
  b | Matrix B
  sgn_y | Sign mask for matrix B
  acc1 | Accumulator 1 input
  zero_acc1 | Zeroing mask for acc1
  sub_mul | Negation mask of multiplication result
  sub_acc1 | Negation mask of acc1

Returns
  Result of operation

## ◆ negmac_conv_8x8_4ch_conf() [6/8]

v32acc32 negmac_conv_8x8_4ch_conf | ( | v64uint8 | a,
|  | int | sgn_x,
|  | v64uint8 | b,
|  | int | sgn_y,
|  | v32acc32 | acc1,
|  | int | zero_acc1,
|  | int | sub_mul,
|  | int | sub_acc1 )

Parameters

  a | Matrix A
  sgn_x | Sign mask for matrix A
  b | Matrix B
  sgn_y | Sign mask for matrix B
  acc1 | Accumulator 1 input
  zero_acc1 | Zeroing mask for acc1
  sub_mul | Negation mask of multiplication result
  sub_acc1 | Negation mask of acc1

Returns
  Result of operation

## ◆ negmac_conv_8x8_4ch_conf() [7/8]

v32acc32 negmac_conv_8x8_4ch_conf | ( | v64uint8 | a,
|  | v64int8 | b,
|  | v32acc32 | acc1,
|  | int | zero_acc1,
|  | int | sub_mul,
|  | int | sub_acc1 )

Parameters

  a | Matrix A
  b | Matrix B
  acc1 | Accumulator 1 input
  zero_acc1 | Zeroing mask for acc1
  sub_mul | Negation mask of multiplication result
  sub_acc1 | Negation mask of acc1

Returns
  Result of operation

## ◆ negmac_conv_8x8_4ch_conf() [8/8]

v32acc32 negmac_conv_8x8_4ch_conf | ( | v64uint8 | a,
|  | v64uint8 | b,
|  | v32acc32 | acc1,
|  | int | zero_acc1,
|  | int | sub_mul,
|  | int | sub_acc1 )

Parameters

  a | Matrix A
  b | Matrix B
  acc1 | Accumulator 1 input
  zero_acc1 | Zeroing mask for acc1
  sub_mul | Negation mask of multiplication result
  sub_acc1 | Negation mask of acc1

Returns
  Result of operation

## ◆ negmac_elem_32_2() [1/8]

v32acc32 negmac_elem_32_2 | ( | v64int8 | a,
|  | int | sgn_x,
|  | v64int8 | b,
|  | int | sgn_y,
|  | v32acc32 | acc1 )

Parameters

  a | Matrix A
  sgn_x | Sign mask for matrix A
  b | Matrix B
  sgn_y | Sign mask for matrix B
  acc1 | Accumulator 1 input

Returns
  Result of operation

## ◆ negmac_elem_32_2() [2/8]

v32acc32 negmac_elem_32_2 | ( | v64int8 | a,
|  | int | sgn_x,
|  | v64uint8 | b,
|  | int | sgn_y,
|  | v32acc32 | acc1 )

Parameters

  a | Matrix A
  sgn_x | Sign mask for matrix A
  b | Matrix B
  sgn_y | Sign mask for matrix B
  acc1 | Accumulator 1 input

Returns
  Result of operation

## ◆ negmac_elem_32_2() [3/8]

v32acc32 negmac_elem_32_2 | ( | v64int8 | a,
|  | v64int8 | b,
|  | v32acc32 | acc1 )

Parameters

  a | Matrix A
  b | Matrix B
  acc1 | Accumulator 1 input

Returns
  Result of MAC operation

## ◆ negmac_elem_32_2() [4/8]

v32acc32 negmac_elem_32_2 | ( | v64int8 | a,
|  | v64uint8 | b,
|  | v32acc32 | acc1 )

Parameters

  a | Matrix A
  b | Matrix B
  acc1 | Accumulator 1 input

Returns
  Result of MAC operation

## ◆ negmac_elem_32_2() [5/8]

v32acc32 negmac_elem_32_2 | ( | v64uint8 | a,
|  | int | sgn_x,
|  | v64int8 | b,
|  | int | sgn_y,
|  | v32acc32 | acc1 )

Parameters

  a | Matrix A
  sgn_x | Sign mask for matrix A
  b | Matrix B
  sgn_y | Sign mask for matrix B
  acc1 | Accumulator 1 input

Returns
  Result of operation

## ◆ negmac_elem_32_2() [6/8]

v32acc32 negmac_elem_32_2 | ( | v64uint8 | a,
|  | int | sgn_x,
|  | v64uint8 | b,
|  | int | sgn_y,
|  | v32acc32 | acc1 )

Parameters

  a | Matrix A
  sgn_x | Sign mask for matrix A
  b | Matrix B
  sgn_y | Sign mask for matrix B
  acc1 | Accumulator 1 input

Returns
  Result of operation

## ◆ negmac_elem_32_2() [7/8]

v32acc32 negmac_elem_32_2 | ( | v64uint8 | a,
|  | v64int8 | b,
|  | v32acc32 | acc1 )

Parameters

  a | Matrix A
  b | Matrix B
  acc1 | Accumulator 1 input

Returns
  Result of MAC operation

## ◆ negmac_elem_32_2() [8/8]

v32acc32 negmac_elem_32_2 | ( | v64uint8 | a,
|  | v64uint8 | b,
|  | v32acc32 | acc1 )

Parameters

  a | Matrix A
  b | Matrix B
  acc1 | Accumulator 1 input

Returns
  Result of MAC operation

## ◆ negmac_elem_32_2_conf() [1/8]

v32acc32 negmac_elem_32_2_conf | ( | v64int8 | a,
|  | int | sgn_x,
|  | v64int8 | b,
|  | int | sgn_y,
|  | v32acc32 | acc1,
|  | int | zero_acc1,
|  | int | sub_mul,
|  | int | sub_acc1 )

Parameters

  a | Matrix A
  sgn_x | Sign mask for matrix A
  b | Matrix B
  sgn_y | Sign mask for matrix B
  acc1 | Accumulator 1 input
  zero_acc1 | Zeroing mask for acc1
  sub_mul | Negation mask of multiplication result
  sub_acc1 | Negation mask of acc1

Returns
  Result of operation

## ◆ negmac_elem_32_2_conf() [2/8]

v32acc32 negmac_elem_32_2_conf | ( | v64int8 | a,
|  | int | sgn_x,
|  | v64uint8 | b,
|  | int | sgn_y,
|  | v32acc32 | acc1,
|  | int | zero_acc1,
|  | int | sub_mul,
|  | int | sub_acc1 )

Parameters

  a | Matrix A
  sgn_x | Sign mask for matrix A
  b | Matrix B
  sgn_y | Sign mask for matrix B
  acc1 | Accumulator 1 input
  zero_acc1 | Zeroing mask for acc1
  sub_mul | Negation mask of multiplication result
  sub_acc1 | Negation mask of acc1

Returns
  Result of operation

## ◆ negmac_elem_32_2_conf() [3/8]

v32acc32 negmac_elem_32_2_conf | ( | v64int8 | a,
|  | v64int8 | b,
|  | v32acc32 | acc1,
|  | int | zero_acc1,
|  | int | sub_mul,
|  | int | sub_acc1 )

Parameters

  a | Matrix A
  b | Matrix B
  acc1 | Accumulator 1 input
  zero_acc1 | Zeroing mask for acc1
  sub_mul | Negation mask of multiplication result
  sub_acc1 | Negation mask of acc1

Returns
  Result of operation

## ◆ negmac_elem_32_2_conf() [4/8]

v32acc32 negmac_elem_32_2_conf | ( | v64int8 | a,
|  | v64uint8 | b,
|  | v32acc32 | acc1,
|  | int | zero_acc1,
|  | int | sub_mul,
|  | int | sub_acc1 )

Parameters

  a | Matrix A
  b | Matrix B
  acc1 | Accumulator 1 input
  zero_acc1 | Zeroing mask for acc1
  sub_mul | Negation mask of multiplication result
  sub_acc1 | Negation mask of acc1

Returns
  Result of operation

## ◆ negmac_elem_32_2_conf() [5/8]

v32acc32 negmac_elem_32_2_conf | ( | v64uint8 | a,
|  | int | sgn_x,
|  | v64int8 | b,
|  | int | sgn_y,
|  | v32acc32 | acc1,
|  | int | zero_acc1,
|  | int | sub_mul,
|  | int | sub_acc1 )

Parameters

  a | Matrix A
  sgn_x | Sign mask for matrix A
  b | Matrix B
  sgn_y | Sign mask for matrix B
  acc1 | Accumulator 1 input
  zero_acc1 | Zeroing mask for acc1
  sub_mul | Negation mask of multiplication result
  sub_acc1 | Negation mask of acc1

Returns
  Result of operation

## ◆ negmac_elem_32_2_conf() [6/8]

v32acc32 negmac_elem_32_2_conf | ( | v64uint8 | a,
|  | int | sgn_x,
|  | v64uint8 | b,
|  | int | sgn_y,
|  | v32acc32 | acc1,
|  | int | zero_acc1,
|  | int | sub_mul,
|  | int | sub_acc1 )

Parameters

  a | Matrix A
  sgn_x | Sign mask for matrix A
  b | Matrix B
  sgn_y | Sign mask for matrix B
  acc1 | Accumulator 1 input
  zero_acc1 | Zeroing mask for acc1
  sub_mul | Negation mask of multiplication result
  sub_acc1 | Negation mask of acc1

Returns
  Result of operation

## ◆ negmac_elem_32_2_conf() [7/8]

v32acc32 negmac_elem_32_2_conf | ( | v64uint8 | a,
|  | v64int8 | b,
|  | v32acc32 | acc1,
|  | int | zero_acc1,
|  | int | sub_mul,
|  | int | sub_acc1 )

Parameters

  a | Matrix A
  b | Matrix B
  acc1 | Accumulator 1 input
  zero_acc1 | Zeroing mask for acc1
  sub_mul | Negation mask of multiplication result
  sub_acc1 | Negation mask of acc1

Returns
  Result of operation

## ◆ negmac_elem_32_2_conf() [8/8]

v32acc32 negmac_elem_32_2_conf | ( | v64uint8 | a,
|  | v64uint8 | b,
|  | v32acc32 | acc1,
|  | int | zero_acc1,
|  | int | sub_mul,
|  | int | sub_acc1 )

Parameters

  a | Matrix A
  b | Matrix B
  acc1 | Accumulator 1 input
  zero_acc1 | Zeroing mask for acc1
  sub_mul | Negation mask of multiplication result
  sub_acc1 | Negation mask of acc1

Returns
  Result of operation

## ◆ negmsc_4x8_8x8() [1/8]

v32acc32 negmsc_4x8_8x8 | ( | v64int8 | a,
|  | int | sgn_x,
|  | v64int8 | b,
|  | int | sgn_y,
|  | v32acc32 | acc1 )

Parameters

  a | Matrix A
  sgn_x | Sign mask for matrix A
  b | Matrix B
  sgn_y | Sign mask for matrix B
  acc1 | Accumulator 1 input

Returns
  Result of operation

## ◆ negmsc_4x8_8x8() [2/8]

v32acc32 negmsc_4x8_8x8 | ( | v64int8 | a,
|  | int | sgn_x,
|  | v64uint8 | b,
|  | int | sgn_y,
|  | v32acc32 | acc1 )

Parameters

  a | Matrix A
  sgn_x | Sign mask for matrix A
  b | Matrix B
  sgn_y | Sign mask for matrix B
  acc1 | Accumulator 1 input

Returns
  Result of operation

## ◆ negmsc_4x8_8x8() [3/8]

v32acc32 negmsc_4x8_8x8 | ( | v64int8 | a,
|  | v64int8 | b,
|  | v32acc32 | acc1 )

Parameters

  a | Matrix A
  b | Matrix B
  acc1 | Accumulator 1 input

Returns
  Result of operation

## ◆ negmsc_4x8_8x8() [4/8]

v32acc32 negmsc_4x8_8x8 | ( | v64int8 | a,
|  | v64uint8 | b,
|  | v32acc32 | acc1 )

Parameters

  a | Matrix A
  b | Matrix B
  acc1 | Accumulator 1 input

Returns
  Result of operation

## ◆ negmsc_4x8_8x8() [5/8]

v32acc32 negmsc_4x8_8x8 | ( | v64uint8 | a,
|  | int | sgn_x,
|  | v64int8 | b,
|  | int | sgn_y,
|  | v32acc32 | acc1 )

Parameters

  a | Matrix A
  sgn_x | Sign mask for matrix A
  b | Matrix B
  sgn_y | Sign mask for matrix B
  acc1 | Accumulator 1 input

Returns
  Result of operation

## ◆ negmsc_4x8_8x8() [6/8]

v32acc32 negmsc_4x8_8x8 | ( | v64uint8 | a,
|  | int | sgn_x,
|  | v64uint8 | b,
|  | int | sgn_y,
|  | v32acc32 | acc1 )

Parameters

  a | Matrix A
  sgn_x | Sign mask for matrix A
  b | Matrix B
  sgn_y | Sign mask for matrix B
  acc1 | Accumulator 1 input

Returns
  Result of operation

## ◆ negmsc_4x8_8x8() [7/8]

v32acc32 negmsc_4x8_8x8 | ( | v64uint8 | a,
|  | v64int8 | b,
|  | v32acc32 | acc1 )

Parameters

  a | Matrix A
  b | Matrix B
  acc1 | Accumulator 1 input

Returns
  Result of operation

## ◆ negmsc_4x8_8x8() [8/8]

v32acc32 negmsc_4x8_8x8 | ( | v64uint8 | a,
|  | v64uint8 | b,
|  | v32acc32 | acc1 )

Parameters

  a | Matrix A
  b | Matrix B
  acc1 | Accumulator 1 input

Returns
  Result of operation

## ◆ negmsc_4x8_8x8_conf() [1/8]

v32acc32 negmsc_4x8_8x8_conf | ( | v64int8 | a,
|  | int | sgn_x,
|  | v64int8 | b,
|  | int | sgn_y,
|  | v32acc32 | acc1,
|  | int | zero_acc1,
|  | int | sub_mul,
|  | int | sub_acc1 )

Parameters

  a | Matrix A
  sgn_x | Sign mask for matrix A
  b | Matrix B
  sgn_y | Sign mask for matrix B
  acc1 | Accumulator 1 input
  zero_acc1 | Zeroing mask for acc1
  sub_mul | Negation mask of multiplication result
  sub_acc1 | Negation mask of acc1

Returns
  Result of operation

## ◆ negmsc_4x8_8x8_conf() [2/8]

v32acc32 negmsc_4x8_8x8_conf | ( | v64int8 | a,
|  | int | sgn_x,
|  | v64uint8 | b,
|  | int | sgn_y,
|  | v32acc32 | acc1,
|  | int | zero_acc1,
|  | int | sub_mul,
|  | int | sub_acc1 )

Parameters

  a | Matrix A
  sgn_x | Sign mask for matrix A
  b | Matrix B
  sgn_y | Sign mask for matrix B
  acc1 | Accumulator 1 input
  zero_acc1 | Zeroing mask for acc1
  sub_mul | Negation mask of multiplication result
  sub_acc1 | Negation mask of acc1

Returns
  Result of operation

## ◆ negmsc_4x8_8x8_conf() [3/8]

v32acc32 negmsc_4x8_8x8_conf | ( | v64int8 | a,
|  | v64int8 | b,
|  | v32acc32 | acc1,
|  | int | zero_acc1,
|  | int | sub_mul,
|  | int | sub_acc1 )

Parameters

  a | Matrix A
  b | Matrix B
  acc1 | Accumulator 1 input
  zero_acc1 | Zeroing mask for acc1
  sub_mul | Negation mask of multiplication result
  sub_acc1 | Negation mask of acc1. If a bit is set the corresponding accumulator lane of acc1 is negated.

Returns
  Result of operation

## ◆ negmsc_4x8_8x8_conf() [4/8]

v32acc32 negmsc_4x8_8x8_conf | ( | v64int8 | a,
|  | v64uint8 | b,
|  | v32acc32 | acc1,
|  | int | zero_acc1,
|  | int | sub_mul,
|  | int | sub_acc1 )

Parameters

  a | Matrix A
  b | Matrix B
  acc1 | Accumulator 1 input
  zero_acc1 | Zeroing mask for acc1
  sub_mul | Negation mask of multiplication result
  sub_acc1 | Negation mask of acc1. If a bit is set the corresponding accumulator lane of acc1 is negated.

Returns
  Result of operation

## ◆ negmsc_4x8_8x8_conf() [5/8]

v32acc32 negmsc_4x8_8x8_conf | ( | v64uint8 | a,
|  | int | sgn_x,
|  | v64int8 | b,
|  | int | sgn_y,
|  | v32acc32 | acc1,
|  | int | zero_acc1,
|  | int | sub_mul,
|  | int | sub_acc1 )

Parameters

  a | Matrix A
  sgn_x | Sign mask for matrix A
  b | Matrix B
  sgn_y | Sign mask for matrix B
  acc1 | Accumulator 1 input
  zero_acc1 | Zeroing mask for acc1
  sub_mul | Negation mask of multiplication result
  sub_acc1 | Negation mask of acc1

Returns
  Result of operation

## ◆ negmsc_4x8_8x8_conf() [6/8]

v32acc32 negmsc_4x8_8x8_conf | ( | v64uint8 | a,
|  | int | sgn_x,
|  | v64uint8 | b,
|  | int | sgn_y,
|  | v32acc32 | acc1,
|  | int | zero_acc1,
|  | int | sub_mul,
|  | int | sub_acc1 )

Parameters

  a | Matrix A
  sgn_x | Sign mask for matrix A
  b | Matrix B
  sgn_y | Sign mask for matrix B
  acc1 | Accumulator 1 input
  zero_acc1 | Zeroing mask for acc1
  sub_mul | Negation mask of multiplication result
  sub_acc1 | Negation mask of acc1

Returns
  Result of operation

## ◆ negmsc_4x8_8x8_conf() [7/8]

v32acc32 negmsc_4x8_8x8_conf | ( | v64uint8 | a,
|  | v64int8 | b,
|  | v32acc32 | acc1,
|  | int | zero_acc1,
|  | int | sub_mul,
|  | int | sub_acc1 )

Parameters

  a | Matrix A
  b | Matrix B
  acc1 | Accumulator 1 input
  zero_acc1 | Zeroing mask for acc1
  sub_mul | Negation mask of multiplication result
  sub_acc1 | Negation mask of acc1. If a bit is set the corresponding accumulator lane of acc1 is negated.

Returns
  Result of operation

## ◆ negmsc_4x8_8x8_conf() [8/8]

v32acc32 negmsc_4x8_8x8_conf | ( | v64uint8 | a,
|  | v64uint8 | b,
|  | v32acc32 | acc1,
|  | int | zero_acc1,
|  | int | sub_mul,
|  | int | sub_acc1 )

Parameters

  a | Matrix A
  b | Matrix B
  acc1 | Accumulator 1 input
  zero_acc1 | Zeroing mask for acc1
  sub_mul | Negation mask of multiplication result
  sub_acc1 | Negation mask of acc1. If a bit is set the corresponding accumulator lane of acc1 is negated.

Returns
  Result of operation

## ◆ negmsc_conv_32x8() [1/8]

v32acc32 negmsc_conv_32x8 | ( | v64int8 | a,
|  | int | sgn_x,
|  | v64int8 | b,
|  | int | sgn_y,
|  | v32acc32 | acc1 )

Parameters

  a | Matrix A
  sgn_x | Sign mask for matrix A
  b | Matrix B
  sgn_y | Sign mask for matrix B
  acc1 | Accumulator 1 input

Returns
  Result of operation

## ◆ negmsc_conv_32x8() [2/8]

v32acc32 negmsc_conv_32x8 | ( | v64int8 | a,
|  | int | sgn_x,
|  | v64uint8 | b,
|  | int | sgn_y,
|  | v32acc32 | acc1 )

Parameters

  a | Matrix A
  sgn_x | Sign mask for matrix A
  b | Matrix B
  sgn_y | Sign mask for matrix B
  acc1 | Accumulator 1 input

Returns
  Result of operation

## ◆ negmsc_conv_32x8() [3/8]

v32acc32 negmsc_conv_32x8 | ( | v64int8 | a,
|  | v64int8 | b,
|  | v32acc32 | acc1 )

Parameters

  a | Matrix A
  b | Matrix B
  acc1 | Accumulator 1 input

Returns
  Result of operation

## ◆ negmsc_conv_32x8() [4/8]

v32acc32 negmsc_conv_32x8 | ( | v64int8 | a,
|  | v64uint8 | b,
|  | v32acc32 | acc1 )

Parameters

  a | Matrix A
  b | Matrix B
  acc1 | Accumulator 1 input

Returns
  Result of operation

## ◆ negmsc_conv_32x8() [5/8]

v32acc32 negmsc_conv_32x8 | ( | v64uint8 | a,
|  | int | sgn_x,
|  | v64int8 | b,
|  | int | sgn_y,
|  | v32acc32 | acc1 )

Parameters

  a | Matrix A
  sgn_x | Sign mask for matrix A
  b | Matrix B
  sgn_y | Sign mask for matrix B
  acc1 | Accumulator 1 input

Returns
  Result of operation

## ◆ negmsc_conv_32x8() [6/8]

v32acc32 negmsc_conv_32x8 | ( | v64uint8 | a,
|  | int | sgn_x,
|  | v64uint8 | b,
|  | int | sgn_y,
|  | v32acc32 | acc1 )

Parameters

  a | Matrix A
  sgn_x | Sign mask for matrix A
  b | Matrix B
  sgn_y | Sign mask for matrix B
  acc1 | Accumulator 1 input

Returns
  Result of operation

## ◆ negmsc_conv_32x8() [7/8]

v32acc32 negmsc_conv_32x8 | ( | v64uint8 | a,
|  | v64int8 | b,
|  | v32acc32 | acc1 )

Parameters

  a | Matrix A
  b | Matrix B
  acc1 | Accumulator 1 input

Returns
  Result of operation

## ◆ negmsc_conv_32x8() [8/8]

v32acc32 negmsc_conv_32x8 | ( | v64uint8 | a,
|  | v64uint8 | b,
|  | v32acc32 | acc1 )

Parameters

  a | Matrix A
  b | Matrix B
  acc1 | Accumulator 1 input

Returns
  Result of operation

## ◆ negmsc_conv_32x8_conf() [1/8]

v32acc32 negmsc_conv_32x8_conf | ( | v64int8 | a,
|  | int | sgn_x,
|  | v64int8 | b,
|  | int | sgn_y,
|  | v32acc32 | acc1,
|  | int | zero_acc1,
|  | int | sub_mul,
|  | int | sub_acc1 )

Parameters

  a | Matrix A
  sgn_x | Sign mask for matrix A
  b | Matrix B
  sgn_y | Sign mask for matrix B
  acc1 | Accumulator 1 input
  zero_acc1 | Zeroing mask for acc1
  sub_mul | Negation mask of multiplication result
  sub_acc1 | Negation mask of acc1

Returns
  Result of operation

## ◆ negmsc_conv_32x8_conf() [2/8]

v32acc32 negmsc_conv_32x8_conf | ( | v64int8 | a,
|  | int | sgn_x,
|  | v64uint8 | b,
|  | int | sgn_y,
|  | v32acc32 | acc1,
|  | int | zero_acc1,
|  | int | sub_mul,
|  | int | sub_acc1 )

Parameters

  a | Matrix A
  sgn_x | Sign mask for matrix A
  b | Matrix B
  sgn_y | Sign mask for matrix B
  acc1 | Accumulator 1 input
  zero_acc1 | Zeroing mask for acc1
  sub_mul | Negation mask of multiplication result
  sub_acc1 | Negation mask of acc1

Returns
  Result of operation

## ◆ negmsc_conv_32x8_conf() [3/8]

v32acc32 negmsc_conv_32x8_conf | ( | v64int8 | a,
|  | v64int8 | b,
|  | v32acc32 | acc1,
|  | int | zero_acc1,
|  | int | sub_mul,
|  | int | sub_acc1 )

Parameters

  a | Matrix A
  b | Matrix B
  acc1 | Accumulator 1 input
  zero_acc1 | Zeroing mask for acc1
  sub_mul | Negation mask of multiplication result
  sub_acc1 | Negation mask of acc1. If a bit is set the corresponding accumulator lane of acc1 is negated.

Returns
  Result of operation

## ◆ negmsc_conv_32x8_conf() [4/8]

v32acc32 negmsc_conv_32x8_conf | ( | v64int8 | a,
|  | v64uint8 | b,
|  | v32acc32 | acc1,
|  | int | zero_acc1,
|  | int | sub_mul,
|  | int | sub_acc1 )

Parameters

  a | Matrix A
  b | Matrix B
  acc1 | Accumulator 1 input
  zero_acc1 | Zeroing mask for acc1
  sub_mul | Negation mask of multiplication result
  sub_acc1 | Negation mask of acc1. If a bit is set the corresponding accumulator lane of acc1 is negated.

Returns
  Result of operation

## ◆ negmsc_conv_32x8_conf() [5/8]

v32acc32 negmsc_conv_32x8_conf | ( | v64uint8 | a,
|  | int | sgn_x,
|  | v64int8 | b,
|  | int | sgn_y,
|  | v32acc32 | acc1,
|  | int | zero_acc1,
|  | int | sub_mul,
|  | int | sub_acc1 )

Parameters

  a | Matrix A
  sgn_x | Sign mask for matrix A
  b | Matrix B
  sgn_y | Sign mask for matrix B
  acc1 | Accumulator 1 input
  zero_acc1 | Zeroing mask for acc1
  sub_mul | Negation mask of multiplication result
  sub_acc1 | Negation mask of acc1

Returns
  Result of operation

## ◆ negmsc_conv_32x8_conf() [6/8]

v32acc32 negmsc_conv_32x8_conf | ( | v64uint8 | a,
|  | int | sgn_x,
|  | v64uint8 | b,
|  | int | sgn_y,
|  | v32acc32 | acc1,
|  | int | zero_acc1,
|  | int | sub_mul,
|  | int | sub_acc1 )

Parameters

  a | Matrix A
  sgn_x | Sign mask for matrix A
  b | Matrix B
  sgn_y | Sign mask for matrix B
  acc1 | Accumulator 1 input
  zero_acc1 | Zeroing mask for acc1
  sub_mul | Negation mask of multiplication result
  sub_acc1 | Negation mask of acc1

Returns
  Result of operation

## ◆ negmsc_conv_32x8_conf() [7/8]

v32acc32 negmsc_conv_32x8_conf | ( | v64uint8 | a,
|  | v64int8 | b,
|  | v32acc32 | acc1,
|  | int | zero_acc1,
|  | int | sub_mul,
|  | int | sub_acc1 )

Parameters

  a | Matrix A
  b | Matrix B
  acc1 | Accumulator 1 input
  zero_acc1 | Zeroing mask for acc1
  sub_mul | Negation mask of multiplication result
  sub_acc1 | Negation mask of acc1. If a bit is set the corresponding accumulator lane of acc1 is negated.

Returns
  Result of operation

## ◆ negmsc_conv_32x8_conf() [8/8]

v32acc32 negmsc_conv_32x8_conf | ( | v64uint8 | a,
|  | v64uint8 | b,
|  | v32acc32 | acc1,
|  | int | zero_acc1,
|  | int | sub_mul,
|  | int | sub_acc1 )

Parameters

  a | Matrix A
  b | Matrix B
  acc1 | Accumulator 1 input
  zero_acc1 | Zeroing mask for acc1
  sub_mul | Negation mask of multiplication result
  sub_acc1 | Negation mask of acc1. If a bit is set the corresponding accumulator lane of acc1 is negated.

Returns
  Result of operation

## ◆ negmsc_conv_4x4_8ch() [1/8]

v32acc32 negmsc_conv_4x4_8ch | ( | v64int8 | a,
|  | int | sgn_x,
|  | v64int8 | b,
|  | int | sgn_y,
|  | v32acc32 | acc1 )

Parameters

  a | Matrix A
  sgn_x | Sign mask for matrix A
  b | Matrix B
  sgn_y | Sign mask for matrix B
  acc1 | Accumulator 1 input

Returns
  Result of operation

## ◆ negmsc_conv_4x4_8ch() [2/8]

v32acc32 negmsc_conv_4x4_8ch | ( | v64int8 | a,
|  | int | sgn_x,
|  | v64uint8 | b,
|  | int | sgn_y,
|  | v32acc32 | acc1 )

Parameters

  a | Matrix A
  sgn_x | Sign mask for matrix A
  b | Matrix B
  sgn_y | Sign mask for matrix B
  acc1 | Accumulator 1 input

Returns
  Result of operation

## ◆ negmsc_conv_4x4_8ch() [3/8]

v32acc32 negmsc_conv_4x4_8ch | ( | v64int8 | a,
|  | v64int8 | b,
|  | v32acc32 | acc1 )

Parameters

  a | Matrix A
  b | Matrix B
  acc1 | Accumulator 1 input

Returns
  Result of operation

## ◆ negmsc_conv_4x4_8ch() [4/8]

v32acc32 negmsc_conv_4x4_8ch | ( | v64int8 | a,
|  | v64uint8 | b,
|  | v32acc32 | acc1 )

Parameters

  a | Matrix A
  b | Matrix B
  acc1 | Accumulator 1 input

Returns
  Result of operation

## ◆ negmsc_conv_4x4_8ch() [5/8]

v32acc32 negmsc_conv_4x4_8ch | ( | v64uint8 | a,
|  | int | sgn_x,
|  | v64int8 | b,
|  | int | sgn_y,
|  | v32acc32 | acc1 )

Parameters

  a | Matrix A
  sgn_x | Sign mask for matrix A
  b | Matrix B
  sgn_y | Sign mask for matrix B
  acc1 | Accumulator 1 input

Returns
  Result of operation

## ◆ negmsc_conv_4x4_8ch() [6/8]

v32acc32 negmsc_conv_4x4_8ch | ( | v64uint8 | a,
|  | int | sgn_x,
|  | v64uint8 | b,
|  | int | sgn_y,
|  | v32acc32 | acc1 )

Parameters

  a | Matrix A
  sgn_x | Sign mask for matrix A
  b | Matrix B
  sgn_y | Sign mask for matrix B
  acc1 | Accumulator 1 input

Returns
  Result of operation

## ◆ negmsc_conv_4x4_8ch() [7/8]

v32acc32 negmsc_conv_4x4_8ch | ( | v64uint8 | a,
|  | v64int8 | b,
|  | v32acc32 | acc1 )

Parameters

  a | Matrix A
  b | Matrix B
  acc1 | Accumulator 1 input

Returns
  Result of operation

## ◆ negmsc_conv_4x4_8ch() [8/8]

v32acc32 negmsc_conv_4x4_8ch | ( | v64uint8 | a,
|  | v64uint8 | b,
|  | v32acc32 | acc1 )

Parameters

  a | Matrix A
  b | Matrix B
  acc1 | Accumulator 1 input

Returns
  Result of operation

## ◆ negmsc_conv_4x4_8ch_conf() [1/8]

v32acc32 negmsc_conv_4x4_8ch_conf | ( | v64int8 | a,
|  | int | sgn_x,
|  | v64int8 | b,
|  | int | sgn_y,
|  | v32acc32 | acc1,
|  | int | zero_acc1,
|  | int | sub_mul,
|  | int | sub_acc1 )

Parameters

  a | Matrix A
  sgn_x | Sign mask for matrix A
  b | Matrix B
  sgn_y | Sign mask for matrix B
  acc1 | Accumulator 1 input
  zero_acc1 | Zeroing mask for acc1
  sub_mul | Negation mask of multiplication result
  sub_acc1 | Negation mask of acc1

Returns
  Result of operation

## ◆ negmsc_conv_4x4_8ch_conf() [2/8]

v32acc32 negmsc_conv_4x4_8ch_conf | ( | v64int8 | a,
|  | int | sgn_x,
|  | v64uint8 | b,
|  | int | sgn_y,
|  | v32acc32 | acc1,
|  | int | zero_acc1,
|  | int | sub_mul,
|  | int | sub_acc1 )

Parameters

  a | Matrix A
  sgn_x | Sign mask for matrix A
  b | Matrix B
  sgn_y | Sign mask for matrix B
  acc1 | Accumulator 1 input
  zero_acc1 | Zeroing mask for acc1
  sub_mul | Negation mask of multiplication result
  sub_acc1 | Negation mask of acc1

Returns
  Result of operation

## ◆ negmsc_conv_4x4_8ch_conf() [3/8]

v32acc32 negmsc_conv_4x4_8ch_conf | ( | v64int8 | a,
|  | v64int8 | b,
|  | v32acc32 | acc1,
|  | int | zero_acc1,
|  | int | sub_mul,
|  | int | sub_acc1 )

Parameters

  a | Matrix A
  b | Matrix B
  acc1 | Accumulator 1 input
  zero_acc1 | Zeroing mask for acc1
  sub_mul | Negation mask of multiplication result
  sub_acc1 | Negation mask of acc1. If a bit is set the corresponding accumulator lane of acc1 is negated.

Returns
  Result of operation

## ◆ negmsc_conv_4x4_8ch_conf() [4/8]

v32acc32 negmsc_conv_4x4_8ch_conf | ( | v64int8 | a,
|  | v64uint8 | b,
|  | v32acc32 | acc1,
|  | int | zero_acc1,
|  | int | sub_mul,
|  | int | sub_acc1 )

Parameters

  a | Matrix A
  b | Matrix B
  acc1 | Accumulator 1 input
  zero_acc1 | Zeroing mask for acc1
  sub_mul | Negation mask of multiplication result
  sub_acc1 | Negation mask of acc1. If a bit is set the corresponding accumulator lane of acc1 is negated.

Returns
  Result of operation

## ◆ negmsc_conv_4x4_8ch_conf() [5/8]

v32acc32 negmsc_conv_4x4_8ch_conf | ( | v64uint8 | a,
|  | int | sgn_x,
|  | v64int8 | b,
|  | int | sgn_y,
|  | v32acc32 | acc1,
|  | int | zero_acc1,
|  | int | sub_mul,
|  | int | sub_acc1 )

Parameters

  a | Matrix A
  sgn_x | Sign mask for matrix A
  b | Matrix B
  sgn_y | Sign mask for matrix B
  acc1 | Accumulator 1 input
  zero_acc1 | Zeroing mask for acc1
  sub_mul | Negation mask of multiplication result
  sub_acc1 | Negation mask of acc1

Returns
  Result of operation

## ◆ negmsc_conv_4x4_8ch_conf() [6/8]

v32acc32 negmsc_conv_4x4_8ch_conf | ( | v64uint8 | a,
|  | int | sgn_x,
|  | v64uint8 | b,
|  | int | sgn_y,
|  | v32acc32 | acc1,
|  | int | zero_acc1,
|  | int | sub_mul,
|  | int | sub_acc1 )

Parameters

  a | Matrix A
  sgn_x | Sign mask for matrix A
  b | Matrix B
  sgn_y | Sign mask for matrix B
  acc1 | Accumulator 1 input
  zero_acc1 | Zeroing mask for acc1
  sub_mul | Negation mask of multiplication result
  sub_acc1 | Negation mask of acc1

Returns
  Result of operation

## ◆ negmsc_conv_4x4_8ch_conf() [7/8]

v32acc32 negmsc_conv_4x4_8ch_conf | ( | v64uint8 | a,
|  | v64int8 | b,
|  | v32acc32 | acc1,
|  | int | zero_acc1,
|  | int | sub_mul,
|  | int | sub_acc1 )

Parameters

  a | Matrix A
  b | Matrix B
  acc1 | Accumulator 1 input
  zero_acc1 | Zeroing mask for acc1
  sub_mul | Negation mask of multiplication result
  sub_acc1 | Negation mask of acc1. If a bit is set the corresponding accumulator lane of acc1 is negated.

Returns
  Result of operation

## ◆ negmsc_conv_4x4_8ch_conf() [8/8]

v32acc32 negmsc_conv_4x4_8ch_conf | ( | v64uint8 | a,
|  | v64uint8 | b,
|  | v32acc32 | acc1,
|  | int | zero_acc1,
|  | int | sub_mul,
|  | int | sub_acc1 )

Parameters

  a | Matrix A
  b | Matrix B
  acc1 | Accumulator 1 input
  zero_acc1 | Zeroing mask for acc1
  sub_mul | Negation mask of multiplication result
  sub_acc1 | Negation mask of acc1. If a bit is set the corresponding accumulator lane of acc1 is negated.

Returns
  Result of operation

## ◆ negmsc_conv_8x8_4ch() [1/8]

v32acc32 negmsc_conv_8x8_4ch | ( | v64int8 | a,
|  | int | sgn_x,
|  | v64int8 | b,
|  | int | sgn_y,
|  | v32acc32 | acc1 )

Parameters

  a | Matrix A
  sgn_x | Sign mask for matrix A
  b | Matrix B
  sgn_y | Sign mask for matrix B
  acc1 | Accumulator 1 input

Returns
  Result of operation

## ◆ negmsc_conv_8x8_4ch() [2/8]

v32acc32 negmsc_conv_8x8_4ch | ( | v64int8 | a,
|  | int | sgn_x,
|  | v64uint8 | b,
|  | int | sgn_y,
|  | v32acc32 | acc1 )

Parameters

  a | Matrix A
  sgn_x | Sign mask for matrix A
  b | Matrix B
  sgn_y | Sign mask for matrix B
  acc1 | Accumulator 1 input

Returns
  Result of operation

## ◆ negmsc_conv_8x8_4ch() [3/8]

v32acc32 negmsc_conv_8x8_4ch | ( | v64int8 | a,
|  | v64int8 | b,
|  | v32acc32 | acc1 )

Parameters

  a | Matrix A
  b | Matrix B
  acc1 | Accumulator 1 input

Returns
  Result of operation

## ◆ negmsc_conv_8x8_4ch() [4/8]

v32acc32 negmsc_conv_8x8_4ch | ( | v64int8 | a,
|  | v64uint8 | b,
|  | v32acc32 | acc1 )

Parameters

  a | Matrix A
  b | Matrix B
  acc1 | Accumulator 1 input

Returns
  Result of operation

## ◆ negmsc_conv_8x8_4ch() [5/8]

v32acc32 negmsc_conv_8x8_4ch | ( | v64uint8 | a,
|  | int | sgn_x,
|  | v64int8 | b,
|  | int | sgn_y,
|  | v32acc32 | acc1 )

Parameters

  a | Matrix A
  sgn_x | Sign mask for matrix A
  b | Matrix B
  sgn_y | Sign mask for matrix B
  acc1 | Accumulator 1 input

Returns
  Result of operation

## ◆ negmsc_conv_8x8_4ch() [6/8]

v32acc32 negmsc_conv_8x8_4ch | ( | v64uint8 | a,
|  | int | sgn_x,
|  | v64uint8 | b,
|  | int | sgn_y,
|  | v32acc32 | acc1 )

Parameters

  a | Matrix A
  sgn_x | Sign mask for matrix A
  b | Matrix B
  sgn_y | Sign mask for matrix B
  acc1 | Accumulator 1 input

Returns
  Result of operation

## ◆ negmsc_conv_8x8_4ch() [7/8]

v32acc32 negmsc_conv_8x8_4ch | ( | v64uint8 | a,
|  | v64int8 | b,
|  | v32acc32 | acc1 )

Parameters

  a | Matrix A
  b | Matrix B
  acc1 | Accumulator 1 input

Returns
  Result of operation

## ◆ negmsc_conv_8x8_4ch() [8/8]

v32acc32 negmsc_conv_8x8_4ch | ( | v64uint8 | a,
|  | v64uint8 | b,
|  | v32acc32 | acc1 )

Parameters

  a | Matrix A
  b | Matrix B
  acc1 | Accumulator 1 input

Returns
  Result of operation

## ◆ negmsc_conv_8x8_4ch_conf() [1/8]

v32acc32 negmsc_conv_8x8_4ch_conf | ( | v64int8 | a,
|  | int | sgn_x,
|  | v64int8 | b,
|  | int | sgn_y,
|  | v32acc32 | acc1,
|  | int | zero_acc1,
|  | int | sub_mul,
|  | int | sub_acc1 )

Parameters

  a | Matrix A
  sgn_x | Sign mask for matrix A
  b | Matrix B
  sgn_y | Sign mask for matrix B
  acc1 | Accumulator 1 input
  zero_acc1 | Zeroing mask for acc1
  sub_mul | Negation mask of multiplication result
  sub_acc1 | Negation mask of acc1

Returns
  Result of operation

## ◆ negmsc_conv_8x8_4ch_conf() [2/8]

v32acc32 negmsc_conv_8x8_4ch_conf | ( | v64int8 | a,
|  | int | sgn_x,
|  | v64uint8 | b,
|  | int | sgn_y,
|  | v32acc32 | acc1,
|  | int | zero_acc1,
|  | int | sub_mul,
|  | int | sub_acc1 )

Parameters

  a | Matrix A
  sgn_x | Sign mask for matrix A
  b | Matrix B
  sgn_y | Sign mask for matrix B
  acc1 | Accumulator 1 input
  zero_acc1 | Zeroing mask for acc1
  sub_mul | Negation mask of multiplication result
  sub_acc1 | Negation mask of acc1

Returns
  Result of operation

## ◆ negmsc_conv_8x8_4ch_conf() [3/8]

v32acc32 negmsc_conv_8x8_4ch_conf | ( | v64int8 | a,
|  | v64int8 | b,
|  | v32acc32 | acc1,
|  | int | zero_acc1,
|  | int | sub_mul,
|  | int | sub_acc1 )

Parameters

  a | Matrix A
  b | Matrix B
  acc1 | Accumulator 1 input
  zero_acc1 | Zeroing mask for acc1
  sub_mul | Negation mask of multiplication result
  sub_acc1 | Negation mask of acc1. If a bit is set the corresponding accumulator lane of acc1 is negated.

Returns
  Result of operation

## ◆ negmsc_conv_8x8_4ch_conf() [4/8]

v32acc32 negmsc_conv_8x8_4ch_conf | ( | v64int8 | a,
|  | v64uint8 | b,
|  | v32acc32 | acc1,
|  | int | zero_acc1,
|  | int | sub_mul,
|  | int | sub_acc1 )

Parameters

  a | Matrix A
  b | Matrix B
  acc1 | Accumulator 1 input
  zero_acc1 | Zeroing mask for acc1
  sub_mul | Negation mask of multiplication result
  sub_acc1 | Negation mask of acc1. If a bit is set the corresponding accumulator lane of acc1 is negated.

Returns
  Result of operation

## ◆ negmsc_conv_8x8_4ch_conf() [5/8]

v32acc32 negmsc_conv_8x8_4ch_conf | ( | v64uint8 | a,
|  | int | sgn_x,
|  | v64int8 | b,
|  | int | sgn_y,
|  | v32acc32 | acc1,
|  | int | zero_acc1,
|  | int | sub_mul,
|  | int | sub_acc1 )

Parameters

  a | Matrix A
  sgn_x | Sign mask for matrix A
  b | Matrix B
  sgn_y | Sign mask for matrix B
  acc1 | Accumulator 1 input
  zero_acc1 | Zeroing mask for acc1
  sub_mul | Negation mask of multiplication result
  sub_acc1 | Negation mask of acc1

Returns
  Result of operation

## ◆ negmsc_conv_8x8_4ch_conf() [6/8]

v32acc32 negmsc_conv_8x8_4ch_conf | ( | v64uint8 | a,
|  | int | sgn_x,
|  | v64uint8 | b,
|  | int | sgn_y,
|  | v32acc32 | acc1,
|  | int | zero_acc1,
|  | int | sub_mul,
|  | int | sub_acc1 )

Parameters

  a | Matrix A
  sgn_x | Sign mask for matrix A
  b | Matrix B
  sgn_y | Sign mask for matrix B
  acc1 | Accumulator 1 input
  zero_acc1 | Zeroing mask for acc1
  sub_mul | Negation mask of multiplication result
  sub_acc1 | Negation mask of acc1

Returns
  Result of operation

## ◆ negmsc_conv_8x8_4ch_conf() [7/8]

v32acc32 negmsc_conv_8x8_4ch_conf | ( | v64uint8 | a,
|  | v64int8 | b,
|  | v32acc32 | acc1,
|  | int | zero_acc1,
|  | int | sub_mul,
|  | int | sub_acc1 )

Parameters

  a | Matrix A
  b | Matrix B
  acc1 | Accumulator 1 input
  zero_acc1 | Zeroing mask for acc1
  sub_mul | Negation mask of multiplication result
  sub_acc1 | Negation mask of acc1. If a bit is set the corresponding accumulator lane of acc1 is negated.

Returns
  Result of operation

## ◆ negmsc_conv_8x8_4ch_conf() [8/8]

v32acc32 negmsc_conv_8x8_4ch_conf | ( | v64uint8 | a,
|  | v64uint8 | b,
|  | v32acc32 | acc1,
|  | int | zero_acc1,
|  | int | sub_mul,
|  | int | sub_acc1 )

Parameters

  a | Matrix A
  b | Matrix B
  acc1 | Accumulator 1 input
  zero_acc1 | Zeroing mask for acc1
  sub_mul | Negation mask of multiplication result
  sub_acc1 | Negation mask of acc1. If a bit is set the corresponding accumulator lane of acc1 is negated.

Returns
  Result of operation

## ◆ negmsc_elem_32_2() [1/8]

v32acc32 negmsc_elem_32_2 | ( | v64int8 | a,
|  | int | sgn_x,
|  | v64int8 | b,
|  | int | sgn_y,
|  | v32acc32 | acc1 )

Parameters

  a | Matrix A
  sgn_x | Sign mask for matrix A
  b | Matrix B
  sgn_y | Sign mask for matrix B
  acc1 | Accumulator 1 input

Returns
  Result of operation

## ◆ negmsc_elem_32_2() [2/8]

v32acc32 negmsc_elem_32_2 | ( | v64int8 | a,
|  | int | sgn_x,
|  | v64uint8 | b,
|  | int | sgn_y,
|  | v32acc32 | acc1 )

Parameters

  a | Matrix A
  sgn_x | Sign mask for matrix A
  b | Matrix B
  sgn_y | Sign mask for matrix B
  acc1 | Accumulator 1 input

Returns
  Result of operation

## ◆ negmsc_elem_32_2() [3/8]

v32acc32 negmsc_elem_32_2 | ( | v64int8 | a,
|  | v64int8 | b,
|  | v32acc32 | acc1 )

Parameters

  a | Matrix A
  b | Matrix B
  acc1 | Accumulator 1 input

Returns
  Result of operation

## ◆ negmsc_elem_32_2() [4/8]

v32acc32 negmsc_elem_32_2 | ( | v64int8 | a,
|  | v64uint8 | b,
|  | v32acc32 | acc1 )

Parameters

  a | Matrix A
  b | Matrix B
  acc1 | Accumulator 1 input

Returns
  Result of operation

## ◆ negmsc_elem_32_2() [5/8]

v32acc32 negmsc_elem_32_2 | ( | v64uint8 | a,
|  | int | sgn_x,
|  | v64int8 | b,
|  | int | sgn_y,
|  | v32acc32 | acc1 )

Parameters

  a | Matrix A
  sgn_x | Sign mask for matrix A
  b | Matrix B
  sgn_y | Sign mask for matrix B
  acc1 | Accumulator 1 input

Returns
  Result of operation

## ◆ negmsc_elem_32_2() [6/8]

v32acc32 negmsc_elem_32_2 | ( | v64uint8 | a,
|  | int | sgn_x,
|  | v64uint8 | b,
|  | int | sgn_y,
|  | v32acc32 | acc1 )

Parameters

  a | Matrix A
  sgn_x | Sign mask for matrix A
  b | Matrix B
  sgn_y | Sign mask for matrix B
  acc1 | Accumulator 1 input

Returns
  Result of operation

## ◆ negmsc_elem_32_2() [7/8]

v32acc32 negmsc_elem_32_2 | ( | v64uint8 | a,
|  | v64int8 | b,
|  | v32acc32 | acc1 )

Parameters

  a | Matrix A
  b | Matrix B
  acc1 | Accumulator 1 input

Returns
  Result of operation

## ◆ negmsc_elem_32_2() [8/8]

v32acc32 negmsc_elem_32_2 | ( | v64uint8 | a,
|  | v64uint8 | b,
|  | v32acc32 | acc1 )

Parameters

  a | Matrix A
  b | Matrix B
  acc1 | Accumulator 1 input

Returns
  Result of operation

## ◆ negmsc_elem_32_2_conf() [1/8]

v32acc32 negmsc_elem_32_2_conf | ( | v64int8 | a,
|  | int | sgn_x,
|  | v64int8 | b,
|  | int | sgn_y,
|  | v32acc32 | acc1,
|  | int | zero_acc1,
|  | int | sub_mul,
|  | int | sub_acc1 )

Parameters

  a | Matrix A
  sgn_x | Sign mask for matrix A
  b | Matrix B
  sgn_y | Sign mask for matrix B
  acc1 | Accumulator 1 input
  zero_acc1 | Zeroing mask for acc1
  sub_mul | Negation mask of multiplication result
  sub_acc1 | Negation mask of acc1

Returns
  Result of operation

## ◆ negmsc_elem_32_2_conf() [2/8]

v32acc32 negmsc_elem_32_2_conf | ( | v64int8 | a,
|  | int | sgn_x,
|  | v64uint8 | b,
|  | int | sgn_y,
|  | v32acc32 | acc1,
|  | int | zero_acc1,
|  | int | sub_mul,
|  | int | sub_acc1 )

Parameters

  a | Matrix A
  sgn_x | Sign mask for matrix A
  b | Matrix B
  sgn_y | Sign mask for matrix B
  acc1 | Accumulator 1 input
  zero_acc1 | Zeroing mask for acc1
  sub_mul | Negation mask of multiplication result
  sub_acc1 | Negation mask of acc1

Returns
  Result of operation

## ◆ negmsc_elem_32_2_conf() [3/8]

v32acc32 negmsc_elem_32_2_conf | ( | v64int8 | a,
|  | v64int8 | b,
|  | v32acc32 | acc1,
|  | int | zero_acc1,
|  | int | sub_mul,
|  | int | sub_acc1 )

Parameters

  a | Matrix A
  b | Matrix B
  acc1 | Accumulator 1 input
  zero_acc1 | Zeroing mask for acc1
  sub_mul | Negation mask of multiplication result
  sub_acc1 | Negation mask of acc1. If a bit is set the corresponding accumulator lane of acc1 is negated.

Returns
  Result of operation

## ◆ negmsc_elem_32_2_conf() [4/8]

v32acc32 negmsc_elem_32_2_conf | ( | v64int8 | a,
|  | v64uint8 | b,
|  | v32acc32 | acc1,
|  | int | zero_acc1,
|  | int | sub_mul,
|  | int | sub_acc1 )

Parameters

  a | Matrix A
  b | Matrix B
  acc1 | Accumulator 1 input
  zero_acc1 | Zeroing mask for acc1
  sub_mul | Negation mask of multiplication result
  sub_acc1 | Negation mask of acc1. If a bit is set the corresponding accumulator lane of acc1 is negated.

Returns
  Result of operation

## ◆ negmsc_elem_32_2_conf() [5/8]

v32acc32 negmsc_elem_32_2_conf | ( | v64uint8 | a,
|  | int | sgn_x,
|  | v64int8 | b,
|  | int | sgn_y,
|  | v32acc32 | acc1,
|  | int | zero_acc1,
|  | int | sub_mul,
|  | int | sub_acc1 )

Parameters

  a | Matrix A
  sgn_x | Sign mask for matrix A
  b | Matrix B
  sgn_y | Sign mask for matrix B
  acc1 | Accumulator 1 input
  zero_acc1 | Zeroing mask for acc1
  sub_mul | Negation mask of multiplication result
  sub_acc1 | Negation mask of acc1

Returns
  Result of operation

## ◆ negmsc_elem_32_2_conf() [6/8]

v32acc32 negmsc_elem_32_2_conf | ( | v64uint8 | a,
|  | int | sgn_x,
|  | v64uint8 | b,
|  | int | sgn_y,
|  | v32acc32 | acc1,
|  | int | zero_acc1,
|  | int | sub_mul,
|  | int | sub_acc1 )

Parameters

  a | Matrix A
  sgn_x | Sign mask for matrix A
  b | Matrix B
  sgn_y | Sign mask for matrix B
  acc1 | Accumulator 1 input
  zero_acc1 | Zeroing mask for acc1
  sub_mul | Negation mask of multiplication result
  sub_acc1 | Negation mask of acc1

Returns
  Result of operation

## ◆ negmsc_elem_32_2_conf() [7/8]

v32acc32 negmsc_elem_32_2_conf | ( | v64uint8 | a,
|  | v64int8 | b,
|  | v32acc32 | acc1,
|  | int | zero_acc1,
|  | int | sub_mul,
|  | int | sub_acc1 )

Parameters

  a | Matrix A
  b | Matrix B
  acc1 | Accumulator 1 input
  zero_acc1 | Zeroing mask for acc1
  sub_mul | Negation mask of multiplication result
  sub_acc1 | Negation mask of acc1. If a bit is set the corresponding accumulator lane of acc1 is negated.

Returns
  Result of operation

## ◆ negmsc_elem_32_2_conf() [8/8]

v32acc32 negmsc_elem_32_2_conf | ( | v64uint8 | a,
|  | v64uint8 | b,
|  | v32acc32 | acc1,
|  | int | zero_acc1,
|  | int | sub_mul,
|  | int | sub_acc1 )

Parameters

  a | Matrix A
  b | Matrix B
  acc1 | Accumulator 1 input
  zero_acc1 | Zeroing mask for acc1
  sub_mul | Negation mask of multiplication result
  sub_acc1 | Negation mask of acc1. If a bit is set the corresponding accumulator lane of acc1 is negated.

Returns
  Result of operation

## ◆ negmul_4x8_8x8() [1/8]

v32acc32 negmul_4x8_8x8 | ( | v64int8 | a,
|  | int | sgn_x,
|  | v64int8 | b,
|  | int | sgn_y )

Parameters

  a | Matrix A
  sgn_x | Sign mask for matrix A
  b | Matrix B
  sgn_y | Sign mask for matrix B

Returns
  Result of operation

## ◆ negmul_4x8_8x8() [2/8]

v32acc32 negmul_4x8_8x8 | ( | v64int8 | a,
|  | int | sgn_x,
|  | v64uint8 | b,
|  | int | sgn_y )

Parameters

  a | Matrix A
  sgn_x | Sign mask for matrix A
  b | Matrix B
  sgn_y | Sign mask for matrix B

Returns
  Result of operation

## ◆ negmul_4x8_8x8() [3/8]

v32acc32 negmul_4x8_8x8 | ( | v64int8 | a,
|  | v64int8 | b )

Parameters

  a | Matrix A
  b | Matrix B

Returns
  Result of operation

## ◆ negmul_4x8_8x8() [4/8]

v32acc32 negmul_4x8_8x8 | ( | v64int8 | a,
|  | v64uint8 | b )

Parameters

  a | Matrix A
  b | Matrix B

Returns
  Result of operation

## ◆ negmul_4x8_8x8() [5/8]

v32acc32 negmul_4x8_8x8 | ( | v64uint8 | a,
|  | int | sgn_x,
|  | v64int8 | b,
|  | int | sgn_y )

Parameters

  a | Matrix A
  sgn_x | Sign mask for matrix A
  b | Matrix B
  sgn_y | Sign mask for matrix B

Returns
  Result of operation

## ◆ negmul_4x8_8x8() [6/8]

v32acc32 negmul_4x8_8x8 | ( | v64uint8 | a,
|  | int | sgn_x,
|  | v64uint8 | b,
|  | int | sgn_y )

Parameters

  a | Matrix A
  sgn_x | Sign mask for matrix A
  b | Matrix B
  sgn_y | Sign mask for matrix B

Returns
  Result of operation

## ◆ negmul_4x8_8x8() [7/8]

v32acc32 negmul_4x8_8x8 | ( | v64uint8 | a,
|  | v64int8 | b )

Parameters

  a | Matrix A
  b | Matrix B

Returns
  Result of operation

## ◆ negmul_4x8_8x8() [8/8]

v32acc32 negmul_4x8_8x8 | ( | v64uint8 | a,
|  | v64uint8 | b )

Parameters

  a | Matrix A
  b | Matrix B

Returns
  Result of operation

## ◆ negmul_4x8_8x8_conf() [1/8]

v32acc32 negmul_4x8_8x8_conf | ( | v64int8 | a,
|  | int | sgn_x,
|  | v64int8 | b,
|  | int | sgn_y,
|  | int | sub_mul )

Parameters

  a | Matrix A
  sgn_x | Sign mask for matrix A
  b | Matrix B
  sgn_y | Sign mask for matrix B
  sub_mul | Negation mask of multiplication result

Returns
  Result of operation

## ◆ negmul_4x8_8x8_conf() [2/8]

v32acc32 negmul_4x8_8x8_conf | ( | v64int8 | a,
|  | int | sgn_x,
|  | v64uint8 | b,
|  | int | sgn_y,
|  | int | sub_mul )

Parameters

  a | Matrix A
  sgn_x | Sign mask for matrix A
  b | Matrix B
  sgn_y | Sign mask for matrix B
  sub_mul | Negation mask of multiplication result

Returns
  Result of operation

## ◆ negmul_4x8_8x8_conf() [3/8]

v32acc32 negmul_4x8_8x8_conf | ( | v64int8 | a,
|  | v64int8 | b,
|  | int | sub_mul )

Parameters

  a | Matrix A
  b | Matrix B
  sub_mul | Negation mask for multiplication result. If a bit of sub_mul is set the corresponding vector lane of the output accumulator will be negated.

Returns
  Result of operation

## ◆ negmul_4x8_8x8_conf() [4/8]

v32acc32 negmul_4x8_8x8_conf | ( | v64int8 | a,
|  | v64uint8 | b,
|  | int | sub_mul )

Parameters

  a | Matrix A
  b | Matrix B
  sub_mul | Negation mask for multiplication result. If a bit of sub_mul is set the corresponding vector lane of the output accumulator will be negated.

Returns
  Result of operation

## ◆ negmul_4x8_8x8_conf() [5/8]

v32acc32 negmul_4x8_8x8_conf | ( | v64uint8 | a,
|  | int | sgn_x,
|  | v64int8 | b,
|  | int | sgn_y,
|  | int | sub_mul )

Parameters

  a | Matrix A
  sgn_x | Sign mask for matrix A
  b | Matrix B
  sgn_y | Sign mask for matrix B
  sub_mul | Negation mask of multiplication result

Returns
  Result of operation

## ◆ negmul_4x8_8x8_conf() [6/8]

v32acc32 negmul_4x8_8x8_conf | ( | v64uint8 | a,
|  | int | sgn_x,
|  | v64uint8 | b,
|  | int | sgn_y,
|  | int | sub_mul )

Parameters

  a | Matrix A
  sgn_x | Sign mask for matrix A
  b | Matrix B
  sgn_y | Sign mask for matrix B
  sub_mul | Negation mask of multiplication result

Returns
  Result of operation

## ◆ negmul_4x8_8x8_conf() [7/8]

v32acc32 negmul_4x8_8x8_conf | ( | v64uint8 | a,
|  | v64int8 | b,
|  | int | sub_mul )

Parameters

  a | Matrix A
  b | Matrix B
  sub_mul | Negation mask for multiplication result. If a bit of sub_mul is set the corresponding vector lane of the output accumulator will be negated.

Returns
  Result of operation

## ◆ negmul_4x8_8x8_conf() [8/8]

v32acc32 negmul_4x8_8x8_conf | ( | v64uint8 | a,
|  | v64uint8 | b,
|  | int | sub_mul )

Parameters

  a | Matrix A
  b | Matrix B
  sub_mul | Negation mask for multiplication result. If a bit of sub_mul is set the corresponding vector lane of the output accumulator will be negated.

Returns
  Result of operation

## ◆ negmul_conv_32x8() [1/8]

v32acc32 negmul_conv_32x8 | ( | v64int8 | a,
|  | int | sgn_x,
|  | v64int8 | b,
|  | int | sgn_y )

Parameters

  a | Matrix A
  sgn_x | Sign mask for matrix A
  b | Matrix B
  sgn_y | Sign mask for matrix B

Returns
  Result of operation

## ◆ negmul_conv_32x8() [2/8]

v32acc32 negmul_conv_32x8 | ( | v64int8 | a,
|  | int | sgn_x,
|  | v64uint8 | b,
|  | int | sgn_y )

Parameters

  a | Matrix A
  sgn_x | Sign mask for matrix A
  b | Matrix B
  sgn_y | Sign mask for matrix B

Returns
  Result of operation

## ◆ negmul_conv_32x8() [3/8]

v32acc32 negmul_conv_32x8 | ( | v64int8 | a,
|  | v64int8 | b )

Parameters

  a | Matrix A
  b | Matrix B

Returns
  Result of operation

## ◆ negmul_conv_32x8() [4/8]

v32acc32 negmul_conv_32x8 | ( | v64int8 | a,
|  | v64uint8 | b )

Parameters

  a | Matrix A
  b | Matrix B

Returns
  Result of operation

## ◆ negmul_conv_32x8() [5/8]

v32acc32 negmul_conv_32x8 | ( | v64uint8 | a,
|  | int | sgn_x,
|  | v64int8 | b,
|  | int | sgn_y )

Parameters

  a | Matrix A
  sgn_x | Sign mask for matrix A
  b | Matrix B
  sgn_y | Sign mask for matrix B

Returns
  Result of operation

## ◆ negmul_conv_32x8() [6/8]

v32acc32 negmul_conv_32x8 | ( | v64uint8 | a,
|  | int | sgn_x,
|  | v64uint8 | b,
|  | int | sgn_y )

Parameters

  a | Matrix A
  sgn_x | Sign mask for matrix A
  b | Matrix B
  sgn_y | Sign mask for matrix B

Returns
  Result of operation

## ◆ negmul_conv_32x8() [7/8]

v32acc32 negmul_conv_32x8 | ( | v64uint8 | a,
|  | v64int8 | b )

Parameters

  a | Matrix A
  b | Matrix B

Returns
  Result of operation

## ◆ negmul_conv_32x8() [8/8]

v32acc32 negmul_conv_32x8 | ( | v64uint8 | a,
|  | v64uint8 | b )

Parameters

  a | Matrix A
  b | Matrix B

Returns
  Result of operation

## ◆ negmul_conv_32x8_conf() [1/8]

v32acc32 negmul_conv_32x8_conf | ( | v64int8 | a,
|  | int | sgn_x,
|  | v64int8 | b,
|  | int | sgn_y,
|  | int | sub_mul )

Parameters

  a | Matrix A
  sgn_x | Sign mask for matrix A
  b | Matrix B
  sgn_y | Sign mask for matrix B
  sub_mul | Negation mask of multiplication result

Returns
  Result of operation

## ◆ negmul_conv_32x8_conf() [2/8]

v32acc32 negmul_conv_32x8_conf | ( | v64int8 | a,
|  | int | sgn_x,
|  | v64uint8 | b,
|  | int | sgn_y,
|  | int | sub_mul )

Parameters

  a | Matrix A
  sgn_x | Sign mask for matrix A
  b | Matrix B
  sgn_y | Sign mask for matrix B
  sub_mul | Negation mask of multiplication result

Returns
  Result of operation

## ◆ negmul_conv_32x8_conf() [3/8]

v32acc32 negmul_conv_32x8_conf | ( | v64int8 | a,
|  | v64int8 | b,
|  | int | sub_mul )

Parameters

  a | Matrix A
  b | Matrix B
  sub_mul | Negation mask for multiplication result. If a bit of sub_mul is set the corresponding vector lane of the output accumulator will be negated.

Returns
  Result of operation

## ◆ negmul_conv_32x8_conf() [4/8]

v32acc32 negmul_conv_32x8_conf | ( | v64int8 | a,
|  | v64uint8 | b,
|  | int | sub_mul )

Parameters

  a | Matrix A
  b | Matrix B
  sub_mul | Negation mask for multiplication result. If a bit of sub_mul is set the corresponding vector lane of the output accumulator will be negated.

Returns
  Result of operation

## ◆ negmul_conv_32x8_conf() [5/8]

v32acc32 negmul_conv_32x8_conf | ( | v64uint8 | a,
|  | int | sgn_x,
|  | v64int8 | b,
|  | int | sgn_y,
|  | int | sub_mul )

Parameters

  a | Matrix A
  sgn_x | Sign mask for matrix A
  b | Matrix B
  sgn_y | Sign mask for matrix B
  sub_mul | Negation mask of multiplication result

Returns
  Result of operation

## ◆ negmul_conv_32x8_conf() [6/8]

v32acc32 negmul_conv_32x8_conf | ( | v64uint8 | a,
|  | int | sgn_x,
|  | v64uint8 | b,
|  | int | sgn_y,
|  | int | sub_mul )

Parameters

  a | Matrix A
  sgn_x | Sign mask for matrix A
  b | Matrix B
  sgn_y | Sign mask for matrix B
  sub_mul | Negation mask of multiplication result

Returns
  Result of operation

## ◆ negmul_conv_32x8_conf() [7/8]

v32acc32 negmul_conv_32x8_conf | ( | v64uint8 | a,
|  | v64int8 | b,
|  | int | sub_mul )

Parameters

  a | Matrix A
  b | Matrix B
  sub_mul | Negation mask for multiplication result. If a bit of sub_mul is set the corresponding vector lane of the output accumulator will be negated.

Returns
  Result of operation

## ◆ negmul_conv_32x8_conf() [8/8]

v32acc32 negmul_conv_32x8_conf | ( | v64uint8 | a,
|  | v64uint8 | b,
|  | int | sub_mul )

Parameters

  a | Matrix A
  b | Matrix B
  sub_mul | Negation mask for multiplication result. If a bit of sub_mul is set the corresponding vector lane of the output accumulator will be negated.

Returns
  Result of operation

## ◆ negmul_conv_4x4_8ch() [1/8]

v32acc32 negmul_conv_4x4_8ch | ( | v64int8 | a,
|  | int | sgn_x,
|  | v64int8 | b,
|  | int | sgn_y )

Parameters

  a | Matrix A
  sgn_x | Sign mask for matrix A
  b | Matrix B
  sgn_y | Sign mask for matrix B

Returns
  Result of operation

## ◆ negmul_conv_4x4_8ch() [2/8]

v32acc32 negmul_conv_4x4_8ch | ( | v64int8 | a,
|  | int | sgn_x,
|  | v64uint8 | b,
|  | int | sgn_y )

Parameters

  a | Matrix A
  sgn_x | Sign mask for matrix A
  b | Matrix B
  sgn_y | Sign mask for matrix B

Returns
  Result of operation

## ◆ negmul_conv_4x4_8ch() [3/8]

v32acc32 negmul_conv_4x4_8ch | ( | v64int8 | a,
|  | v64int8 | b )

Parameters

  a | Matrix A
  b | Matrix B

Returns
  Result of operation

## ◆ negmul_conv_4x4_8ch() [4/8]

v32acc32 negmul_conv_4x4_8ch | ( | v64int8 | a,
|  | v64uint8 | b )

Parameters

  a | Matrix A
  b | Matrix B

Returns
  Result of operation

## ◆ negmul_conv_4x4_8ch() [5/8]

v32acc32 negmul_conv_4x4_8ch | ( | v64uint8 | a,
|  | int | sgn_x,
|  | v64int8 | b,
|  | int | sgn_y )

Parameters

  a | Matrix A
  sgn_x | Sign mask for matrix A
  b | Matrix B
  sgn_y | Sign mask for matrix B

Returns
  Result of operation

## ◆ negmul_conv_4x4_8ch() [6/8]

v32acc32 negmul_conv_4x4_8ch | ( | v64uint8 | a,
|  | int | sgn_x,
|  | v64uint8 | b,
|  | int | sgn_y )

Parameters

  a | Matrix A
  sgn_x | Sign mask for matrix A
  b | Matrix B
  sgn_y | Sign mask for matrix B

Returns
  Result of operation

## ◆ negmul_conv_4x4_8ch() [7/8]

v32acc32 negmul_conv_4x4_8ch | ( | v64uint8 | a,
|  | v64int8 | b )

Parameters

  a | Matrix A
  b | Matrix B

Returns
  Result of operation

## ◆ negmul_conv_4x4_8ch() [8/8]

v32acc32 negmul_conv_4x4_8ch | ( | v64uint8 | a,
|  | v64uint8 | b )

Parameters

  a | Matrix A
  b | Matrix B

Returns
  Result of operation

## ◆ negmul_conv_4x4_8ch_conf() [1/8]

v32acc32 negmul_conv_4x4_8ch_conf | ( | v64int8 | a,
|  | int | sgn_x,
|  | v64int8 | b,
|  | int | sgn_y,
|  | int | sub_mul )

Parameters

  a | Matrix A
  sgn_x | Sign mask for matrix A
  b | Matrix B
  sgn_y | Sign mask for matrix B
  sub_mul | Negation mask of multiplication result

Returns
  Result of operation

## ◆ negmul_conv_4x4_8ch_conf() [2/8]

v32acc32 negmul_conv_4x4_8ch_conf | ( | v64int8 | a,
|  | int | sgn_x,
|  | v64uint8 | b,
|  | int | sgn_y,
|  | int | sub_mul )

Parameters

  a | Matrix A
  sgn_x | Sign mask for matrix A
  b | Matrix B
  sgn_y | Sign mask for matrix B
  sub_mul | Negation mask of multiplication result

Returns
  Result of operation

## ◆ negmul_conv_4x4_8ch_conf() [3/8]

v32acc32 negmul_conv_4x4_8ch_conf | ( | v64int8 | a,
|  | v64int8 | b,
|  | int | sub_mul )

Parameters

  a | Matrix A
  b | Matrix B
  sub_mul | Negation mask for multiplication result. If a bit of sub_mul is set the corresponding vector lane of the output accumulator will be negated.

Returns
  Result of operation

## ◆ negmul_conv_4x4_8ch_conf() [4/8]

v32acc32 negmul_conv_4x4_8ch_conf | ( | v64int8 | a,
|  | v64uint8 | b,
|  | int | sub_mul )

Parameters

  a | Matrix A
  b | Matrix B
  sub_mul | Negation mask for multiplication result. If a bit of sub_mul is set the corresponding vector lane of the output accumulator will be negated.

Returns
  Result of operation

## ◆ negmul_conv_4x4_8ch_conf() [5/8]

v32acc32 negmul_conv_4x4_8ch_conf | ( | v64uint8 | a,
|  | int | sgn_x,
|  | v64int8 | b,
|  | int | sgn_y,
|  | int | sub_mul )

Parameters

  a | Matrix A
  sgn_x | Sign mask for matrix A
  b | Matrix B
  sgn_y | Sign mask for matrix B
  sub_mul | Negation mask of multiplication result

Returns
  Result of operation

## ◆ negmul_conv_4x4_8ch_conf() [6/8]

v32acc32 negmul_conv_4x4_8ch_conf | ( | v64uint8 | a,
|  | int | sgn_x,
|  | v64uint8 | b,
|  | int | sgn_y,
|  | int | sub_mul )

Parameters

  a | Matrix A
  sgn_x | Sign mask for matrix A
  b | Matrix B
  sgn_y | Sign mask for matrix B
  sub_mul | Negation mask of multiplication result

Returns
  Result of operation

## ◆ negmul_conv_4x4_8ch_conf() [7/8]

v32acc32 negmul_conv_4x4_8ch_conf | ( | v64uint8 | a,
|  | v64int8 | b,
|  | int | sub_mul )

Parameters

  a | Matrix A
  b | Matrix B
  sub_mul | Negation mask for multiplication result. If a bit of sub_mul is set the corresponding vector lane of the output accumulator will be negated.

Returns
  Result of operation

## ◆ negmul_conv_4x4_8ch_conf() [8/8]

v32acc32 negmul_conv_4x4_8ch_conf | ( | v64uint8 | a,
|  | v64uint8 | b,
|  | int | sub_mul )

Parameters

  a | Matrix A
  b | Matrix B
  sub_mul | Negation mask for multiplication result. If a bit of sub_mul is set the corresponding vector lane of the output accumulator will be negated.

Returns
  Result of operation

## ◆ negmul_conv_8x8_4ch() [1/8]

v32acc32 negmul_conv_8x8_4ch | ( | v64int8 | a,
|  | int | sgn_x,
|  | v64int8 | b,
|  | int | sgn_y )

Parameters

  a | Matrix A
  sgn_x | Sign mask for matrix A
  b | Matrix B
  sgn_y | Sign mask for matrix B

Returns
  Result of operation

## ◆ negmul_conv_8x8_4ch() [2/8]

v32acc32 negmul_conv_8x8_4ch | ( | v64int8 | a,
|  | int | sgn_x,
|  | v64uint8 | b,
|  | int | sgn_y )

Parameters

  a | Matrix A
  sgn_x | Sign mask for matrix A
  b | Matrix B
  sgn_y | Sign mask for matrix B

Returns
  Result of operation

## ◆ negmul_conv_8x8_4ch() [3/8]

v32acc32 negmul_conv_8x8_4ch | ( | v64int8 | a,
|  | v64int8 | b )

Parameters

  a | Matrix A
  b | Matrix B

Returns
  Result of operation

## ◆ negmul_conv_8x8_4ch() [4/8]

v32acc32 negmul_conv_8x8_4ch | ( | v64int8 | a,
|  | v64uint8 | b )

Parameters

  a | Matrix A
  b | Matrix B

Returns
  Result of operation

## ◆ negmul_conv_8x8_4ch() [5/8]

v32acc32 negmul_conv_8x8_4ch | ( | v64uint8 | a,
|  | int | sgn_x,
|  | v64int8 | b,
|  | int | sgn_y )

Parameters

  a | Matrix A
  sgn_x | Sign mask for matrix A
  b | Matrix B
  sgn_y | Sign mask for matrix B

Returns
  Result of operation

## ◆ negmul_conv_8x8_4ch() [6/8]

v32acc32 negmul_conv_8x8_4ch | ( | v64uint8 | a,
|  | int | sgn_x,
|  | v64uint8 | b,
|  | int | sgn_y )

Parameters

  a | Matrix A
  sgn_x | Sign mask for matrix A
  b | Matrix B
  sgn_y | Sign mask for matrix B

Returns
  Result of operation

## ◆ negmul_conv_8x8_4ch() [7/8]

v32acc32 negmul_conv_8x8_4ch | ( | v64uint8 | a,
|  | v64int8 | b )

Parameters

  a | Matrix A
  b | Matrix B

Returns
  Result of operation

## ◆ negmul_conv_8x8_4ch() [8/8]

v32acc32 negmul_conv_8x8_4ch | ( | v64uint8 | a,
|  | v64uint8 | b )

Parameters

  a | Matrix A
  b | Matrix B

Returns
  Result of operation

## ◆ negmul_conv_8x8_4ch_conf() [1/8]

v32acc32 negmul_conv_8x8_4ch_conf | ( | v64int8 | a,
|  | int | sgn_x,
|  | v64int8 | b,
|  | int | sgn_y,
|  | int | sub_mul )

Parameters

  a | Matrix A
  sgn_x | Sign mask for matrix A
  b | Matrix B
  sgn_y | Sign mask for matrix B
  sub_mul | Negation mask of multiplication result

Returns
  Result of operation

## ◆ negmul_conv_8x8_4ch_conf() [2/8]

v32acc32 negmul_conv_8x8_4ch_conf | ( | v64int8 | a,
|  | int | sgn_x,
|  | v64uint8 | b,
|  | int | sgn_y,
|  | int | sub_mul )

Parameters

  a | Matrix A
  sgn_x | Sign mask for matrix A
  b | Matrix B
  sgn_y | Sign mask for matrix B
  sub_mul | Negation mask of multiplication result

Returns
  Result of operation

## ◆ negmul_conv_8x8_4ch_conf() [3/8]

v32acc32 negmul_conv_8x8_4ch_conf | ( | v64int8 | a,
|  | v64int8 | b,
|  | int | sub_mul )

Parameters

  a | Matrix A
  b | Matrix B
  sub_mul | Negation mask for multiplication result. If a bit of sub_mul is set the corresponding vector lane of the output accumulator will be negated.

Returns
  Result of operation

## ◆ negmul_conv_8x8_4ch_conf() [4/8]

v32acc32 negmul_conv_8x8_4ch_conf | ( | v64int8 | a,
|  | v64uint8 | b,
|  | int | sub_mul )

Parameters

  a | Matrix A
  b | Matrix B
  sub_mul | Negation mask for multiplication result. If a bit of sub_mul is set the corresponding vector lane of the output accumulator will be negated.

Returns
  Result of operation

## ◆ negmul_conv_8x8_4ch_conf() [5/8]

v32acc32 negmul_conv_8x8_4ch_conf | ( | v64uint8 | a,
|  | int | sgn_x,
|  | v64int8 | b,
|  | int | sgn_y,
|  | int | sub_mul )

Parameters

  a | Matrix A
  sgn_x | Sign mask for matrix A
  b | Matrix B
  sgn_y | Sign mask for matrix B
  sub_mul | Negation mask of multiplication result

Returns
  Result of operation

## ◆ negmul_conv_8x8_4ch_conf() [6/8]

v32acc32 negmul_conv_8x8_4ch_conf | ( | v64uint8 | a,
|  | int | sgn_x,
|  | v64uint8 | b,
|  | int | sgn_y,
|  | int | sub_mul )

Parameters

  a | Matrix A
  sgn_x | Sign mask for matrix A
  b | Matrix B
  sgn_y | Sign mask for matrix B
  sub_mul | Negation mask of multiplication result

Returns
  Result of operation

## ◆ negmul_conv_8x8_4ch_conf() [7/8]

v32acc32 negmul_conv_8x8_4ch_conf | ( | v64uint8 | a,
|  | v64int8 | b,
|  | int | sub_mul )

Parameters

  a | Matrix A
  b | Matrix B
  sub_mul | Negation mask for multiplication result. If a bit of sub_mul is set the corresponding vector lane of the output accumulator will be negated.

Returns
  Result of operation

## ◆ negmul_conv_8x8_4ch_conf() [8/8]

v32acc32 negmul_conv_8x8_4ch_conf | ( | v64uint8 | a,
|  | v64uint8 | b,
|  | int | sub_mul )

Parameters

  a | Matrix A
  b | Matrix B
  sub_mul | Negation mask for multiplication result. If a bit of sub_mul is set the corresponding vector lane of the output accumulator will be negated.

Returns
  Result of operation

## ◆ negmul_elem_32_2() [1/8]

v32acc32 negmul_elem_32_2 | ( | v64int8 | a,
|  | int | sgn_x,
|  | v64int8 | b,
|  | int | sgn_y )

Parameters

  a | Matrix A
  sgn_x | Sign mask for matrix A
  b | Matrix B
  sgn_y | Sign mask for matrix B

Returns
  Result of operation

## ◆ negmul_elem_32_2() [2/8]

v32acc32 negmul_elem_32_2 | ( | v64int8 | a,
|  | int | sgn_x,
|  | v64uint8 | b,
|  | int | sgn_y )

Parameters

  a | Matrix A
  sgn_x | Sign mask for matrix A
  b | Matrix B
  sgn_y | Sign mask for matrix B

Returns
  Result of operation

## ◆ negmul_elem_32_2() [3/8]

v32acc32 negmul_elem_32_2 | ( | v64int8 | a,
|  | v64int8 | b )

Parameters

  a | Matrix A
  b | Matrix B

Returns
  Result of operation

## ◆ negmul_elem_32_2() [4/8]

v32acc32 negmul_elem_32_2 | ( | v64int8 | a,
|  | v64uint8 | b )

Parameters

  a | Matrix A
  b | Matrix B

Returns
  Result of operation

## ◆ negmul_elem_32_2() [5/8]

v32acc32 negmul_elem_32_2 | ( | v64uint8 | a,
|  | int | sgn_x,
|  | v64int8 | b,
|  | int | sgn_y )

Parameters

  a | Matrix A
  sgn_x | Sign mask for matrix A
  b | Matrix B
  sgn_y | Sign mask for matrix B

Returns
  Result of operation

## ◆ negmul_elem_32_2() [6/8]

v32acc32 negmul_elem_32_2 | ( | v64uint8 | a,
|  | int | sgn_x,
|  | v64uint8 | b,
|  | int | sgn_y )

Parameters

  a | Matrix A
  sgn_x | Sign mask for matrix A
  b | Matrix B
  sgn_y | Sign mask for matrix B

Returns
  Result of operation

## ◆ negmul_elem_32_2() [7/8]

v32acc32 negmul_elem_32_2 | ( | v64uint8 | a,
|  | v64int8 | b )

Parameters

  a | Matrix A
  b | Matrix B

Returns
  Result of operation

## ◆ negmul_elem_32_2() [8/8]

v32acc32 negmul_elem_32_2 | ( | v64uint8 | a,
|  | v64uint8 | b )

Parameters

  a | Matrix A
  b | Matrix B

Returns
  Result of operation

## ◆ negmul_elem_32_2_conf() [1/8]

v32acc32 negmul_elem_32_2_conf | ( | v64int8 | a,
|  | int | sgn_x,
|  | v64int8 | b,
|  | int | sgn_y,
|  | int | sub_mul )

Parameters

  a | Matrix A
  sgn_x | Sign mask for matrix A
  b | Matrix B
  sgn_y | Sign mask for matrix B
  sub_mul | Negation mask of multiplication result

Returns
  Result of operation

## ◆ negmul_elem_32_2_conf() [2/8]

v32acc32 negmul_elem_32_2_conf | ( | v64int8 | a,
|  | int | sgn_x,
|  | v64uint8 | b,
|  | int | sgn_y,
|  | int | sub_mul )

Parameters

  a | Matrix A
  sgn_x | Sign mask for matrix A
  b | Matrix B
  sgn_y | Sign mask for matrix B
  sub_mul | Negation mask of multiplication result

Returns
  Result of operation

## ◆ negmul_elem_32_2_conf() [3/8]

v32acc32 negmul_elem_32_2_conf | ( | v64int8 | a,
|  | v64int8 | b,
|  | int | sub_mul )

Parameters

  a | Matrix A
  b | Matrix B
  sub_mul | Negation mask for multiplication result. If a bit of sub_mul is set the corresponding vector lane of the output accumulator will be negated.

Returns
  Result of operation

## ◆ negmul_elem_32_2_conf() [4/8]

v32acc32 negmul_elem_32_2_conf | ( | v64int8 | a,
|  | v64uint8 | b,
|  | int | sub_mul )

Parameters

  a | Matrix A
  b | Matrix B
  sub_mul | Negation mask for multiplication result. If a bit of sub_mul is set the corresponding vector lane of the output accumulator will be negated.

Returns
  Result of operation

## ◆ negmul_elem_32_2_conf() [5/8]

v32acc32 negmul_elem_32_2_conf | ( | v64uint8 | a,
|  | int | sgn_x,
|  | v64int8 | b,
|  | int | sgn_y,
|  | int | sub_mul )

Parameters

  a | Matrix A
  sgn_x | Sign mask for matrix A
  b | Matrix B
  sgn_y | Sign mask for matrix B
  sub_mul | Negation mask of multiplication result

Returns
  Result of operation

## ◆ negmul_elem_32_2_conf() [6/8]

v32acc32 negmul_elem_32_2_conf | ( | v64uint8 | a,
|  | int | sgn_x,
|  | v64uint8 | b,
|  | int | sgn_y,
|  | int | sub_mul )

Parameters

  a | Matrix A
  sgn_x | Sign mask for matrix A
  b | Matrix B
  sgn_y | Sign mask for matrix B
  sub_mul | Negation mask of multiplication result

Returns
  Result of operation

## ◆ negmul_elem_32_2_conf() [7/8]

v32acc32 negmul_elem_32_2_conf | ( | v64uint8 | a,
|  | v64int8 | b,
|  | int | sub_mul )

Parameters

  a | Matrix A
  b | Matrix B
  sub_mul | Negation mask for multiplication result. If a bit of sub_mul is set the corresponding vector lane of the output accumulator will be negated.

Returns
  Result of operation

## ◆ negmul_elem_32_2_conf() [8/8]

v32acc32 negmul_elem_32_2_conf | ( | v64uint8 | a,
|  | v64uint8 | b,
|  | int | sub_mul )

Parameters

  a | Matrix A
  b | Matrix B
  sub_mul | Negation mask for multiplication result. If a bit of sub_mul is set the corresponding vector lane of the output accumulator will be negated.

Returns
  Result of operation

## ◆ submac_4x8_8x8() [1/8]

v32acc32 submac_4x8_8x8 | ( | v64int8 | a,
|  | int | sgn_x,
|  | v64int8 | b,
|  | int | sgn_y,
|  | v32acc32 | acc1,
|  | v32acc32 | acc2 )

Parameters

  a | Matrix A
  sgn_x | Sign mask for matrix A
  b | Matrix B
  sgn_y | Sign mask for matrix B
  acc1 | Accumulator 1 input
  acc2 | Accumulator 2 input

Returns
  Result of operation

## ◆ submac_4x8_8x8() [2/8]

v32acc32 submac_4x8_8x8 | ( | v64int8 | a,
|  | int | sgn_x,
|  | v64uint8 | b,
|  | int | sgn_y,
|  | v32acc32 | acc1,
|  | v32acc32 | acc2 )

Parameters

  a | Matrix A
  sgn_x | Sign mask for matrix A
  b | Matrix B
  sgn_y | Sign mask for matrix B
  acc1 | Accumulator 1 input
  acc2 | Accumulator 2 input

Returns
  Result of operation

## ◆ submac_4x8_8x8() [3/8]

v32acc32 submac_4x8_8x8 | ( | v64int8 | a,
|  | v64int8 | b,
|  | v32acc32 | acc1,
|  | v32acc32 | acc2 )

Parameters

  a | Matrix A
  b | Matrix B
  acc1 | Accumulator 1 input
  acc2 | Accumulator 2 input

Returns
  Result of operation

## ◆ submac_4x8_8x8() [4/8]

v32acc32 submac_4x8_8x8 | ( | v64int8 | a,
|  | v64uint8 | b,
|  | v32acc32 | acc1,
|  | v32acc32 | acc2 )

Parameters

  a | Matrix A
  b | Matrix B
  acc1 | Accumulator 1 input
  acc2 | Accumulator 2 input

Returns
  Result of operation

## ◆ submac_4x8_8x8() [5/8]

v32acc32 submac_4x8_8x8 | ( | v64uint8 | a,
|  | int | sgn_x,
|  | v64int8 | b,
|  | int | sgn_y,
|  | v32acc32 | acc1,
|  | v32acc32 | acc2 )

Parameters

  a | Matrix A
  sgn_x | Sign mask for matrix A
  b | Matrix B
  sgn_y | Sign mask for matrix B
  acc1 | Accumulator 1 input
  acc2 | Accumulator 2 input

Returns
  Result of operation

## ◆ submac_4x8_8x8() [6/8]

v32acc32 submac_4x8_8x8 | ( | v64uint8 | a,
|  | int | sgn_x,
|  | v64uint8 | b,
|  | int | sgn_y,
|  | v32acc32 | acc1,
|  | v32acc32 | acc2 )

Parameters

  a | Matrix A
  sgn_x | Sign mask for matrix A
  b | Matrix B
  sgn_y | Sign mask for matrix B
  acc1 | Accumulator 1 input
  acc2 | Accumulator 2 input

Returns
  Result of operation

## ◆ submac_4x8_8x8() [7/8]

v32acc32 submac_4x8_8x8 | ( | v64uint8 | a,
|  | v64int8 | b,
|  | v32acc32 | acc1,
|  | v32acc32 | acc2 )

Parameters

  a | Matrix A
  b | Matrix B
  acc1 | Accumulator 1 input
  acc2 | Accumulator 2 input

Returns
  Result of operation

## ◆ submac_4x8_8x8() [8/8]

v32acc32 submac_4x8_8x8 | ( | v64uint8 | a,
|  | v64uint8 | b,
|  | v32acc32 | acc1,
|  | v32acc32 | acc2 )

Parameters

  a | Matrix A
  b | Matrix B
  acc1 | Accumulator 1 input
  acc2 | Accumulator 2 input

Returns
  Result of operation

## ◆ submac_4x8_8x8_conf() [1/8]

v32acc32 submac_4x8_8x8_conf | ( | v64int8 | a,
|  | int | sgn_x,
|  | v64int8 | b,
|  | int | sgn_y,
|  | v32acc32 | acc1,
|  | v32acc32 | acc2,
|  | int | zero_acc1,
|  | int | sub_mul,
|  | int | sub_acc1,
|  | int | sub_acc2 )

Parameters

  a | Matrix A
  sgn_x | Sign mask for matrix A
  b | Matrix B
  sgn_y | Sign mask for matrix B
  acc1 | Accumulator 1 input
  acc2 | Accumulator 2 input
  zero_acc1 | Zeroing mask for acc1
  sub_mul | Negation mask of multiplication result
  sub_acc1 | Negation mask of acc1
  sub_acc2 | Negation mask of acc2

Returns
  Result of operation

## ◆ submac_4x8_8x8_conf() [2/8]

v32acc32 submac_4x8_8x8_conf | ( | v64int8 | a,
|  | int | sgn_x,
|  | v64uint8 | b,
|  | int | sgn_y,
|  | v32acc32 | acc1,
|  | v32acc32 | acc2,
|  | int | zero_acc1,
|  | int | sub_mul,
|  | int | sub_acc1,
|  | int | sub_acc2 )

Parameters

  a | Matrix A
  sgn_x | Sign mask for matrix A
  b | Matrix B
  sgn_y | Sign mask for matrix B
  acc1 | Accumulator 1 input
  acc2 | Accumulator 2 input
  zero_acc1 | Zeroing mask for acc1
  sub_mul | Negation mask of multiplication result
  sub_acc1 | Negation mask of acc1
  sub_acc2 | Negation mask of acc2

Returns
  Result of operation

## ◆ submac_4x8_8x8_conf() [3/8]

v32acc32 submac_4x8_8x8_conf | ( | v64int8 | a,
|  | v64int8 | b,
|  | v32acc32 | acc1,
|  | v32acc32 | acc2,
|  | int | zero_acc1,
|  | int | sub_mul,
|  | int | sub_acc1,
|  | int | sub_acc2 )

Parameters

  a | Matrix A
  b | Matrix B
  acc1 | Accumulator 1 input
  acc2 | Accumulator 2 input
  zero_acc1 | Zeroing mask for acc1
  sub_mul | Negation mask of multiplication result
  sub_acc1 | Negation mask of acc1
  sub_acc2 | Negation mask of acc2

Returns
  Result of operation

## ◆ submac_4x8_8x8_conf() [4/8]

v32acc32 submac_4x8_8x8_conf | ( | v64int8 | a,
|  | v64uint8 | b,
|  | v32acc32 | acc1,
|  | v32acc32 | acc2,
|  | int | zero_acc1,
|  | int | sub_mul,
|  | int | sub_acc1,
|  | int | sub_acc2 )

Parameters

  a | Matrix A
  b | Matrix B
  acc1 | Accumulator 1 input
  acc2 | Accumulator 2 input
  zero_acc1 | Zeroing mask for acc1
  sub_mul | Negation mask of multiplication result
  sub_acc1 | Negation mask of acc1
  sub_acc2 | Negation mask of acc2

Returns
  Result of operation

## ◆ submac_4x8_8x8_conf() [5/8]

v32acc32 submac_4x8_8x8_conf | ( | v64uint8 | a,
|  | int | sgn_x,
|  | v64int8 | b,
|  | int | sgn_y,
|  | v32acc32 | acc1,
|  | v32acc32 | acc2,
|  | int | zero_acc1,
|  | int | sub_mul,
|  | int | sub_acc1,
|  | int | sub_acc2 )

Parameters

  a | Matrix A
  sgn_x | Sign mask for matrix A
  b | Matrix B
  sgn_y | Sign mask for matrix B
  acc1 | Accumulator 1 input
  acc2 | Accumulator 2 input
  zero_acc1 | Zeroing mask for acc1
  sub_mul | Negation mask of multiplication result
  sub_acc1 | Negation mask of acc1
  sub_acc2 | Negation mask of acc2

Returns
  Result of operation

## ◆ submac_4x8_8x8_conf() [6/8]

v32acc32 submac_4x8_8x8_conf | ( | v64uint8 | a,
|  | int | sgn_x,
|  | v64uint8 | b,
|  | int | sgn_y,
|  | v32acc32 | acc1,
|  | v32acc32 | acc2,
|  | int | zero_acc1,
|  | int | sub_mul,
|  | int | sub_acc1,
|  | int | sub_acc2 )

Parameters

  a | Matrix A
  sgn_x | Sign mask for matrix A
  b | Matrix B
  sgn_y | Sign mask for matrix B
  acc1 | Accumulator 1 input
  acc2 | Accumulator 2 input
  zero_acc1 | Zeroing mask for acc1
  sub_mul | Negation mask of multiplication result
  sub_acc1 | Negation mask of acc1
  sub_acc2 | Negation mask of acc2

Returns
  Result of operation

## ◆ submac_4x8_8x8_conf() [7/8]

v32acc32 submac_4x8_8x8_conf | ( | v64uint8 | a,
|  | v64int8 | b,
|  | v32acc32 | acc1,
|  | v32acc32 | acc2,
|  | int | zero_acc1,
|  | int | sub_mul,
|  | int | sub_acc1,
|  | int | sub_acc2 )

Parameters

  a | Matrix A
  b | Matrix B
  acc1 | Accumulator 1 input
  acc2 | Accumulator 2 input
  zero_acc1 | Zeroing mask for acc1
  sub_mul | Negation mask of multiplication result
  sub_acc1 | Negation mask of acc1
  sub_acc2 | Negation mask of acc2

Returns
  Result of operation

## ◆ submac_4x8_8x8_conf() [8/8]

v32acc32 submac_4x8_8x8_conf | ( | v64uint8 | a,
|  | v64uint8 | b,
|  | v32acc32 | acc1,
|  | v32acc32 | acc2,
|  | int | zero_acc1,
|  | int | sub_mul,
|  | int | sub_acc1,
|  | int | sub_acc2 )

Parameters

  a | Matrix A
  b | Matrix B
  acc1 | Accumulator 1 input
  acc2 | Accumulator 2 input
  zero_acc1 | Zeroing mask for acc1
  sub_mul | Negation mask of multiplication result
  sub_acc1 | Negation mask of acc1
  sub_acc2 | Negation mask of acc2

Returns
  Result of operation

## ◆ submac_conv_32x8() [1/8]

v32acc32 submac_conv_32x8 | ( | v64int8 | a,
|  | int | sgn_x,
|  | v64int8 | b,
|  | int | sgn_y,
|  | v32acc32 | acc1,
|  | v32acc32 | acc2 )

Parameters

  a | Matrix A
  sgn_x | Sign mask for matrix A
  b | Matrix B
  sgn_y | Sign mask for matrix B
  acc1 | Accumulator 1 input
  acc2 | Accumulator 2 input

Returns
  Result of operation

## ◆ submac_conv_32x8() [2/8]

v32acc32 submac_conv_32x8 | ( | v64int8 | a,
|  | int | sgn_x,
|  | v64uint8 | b,
|  | int | sgn_y,
|  | v32acc32 | acc1,
|  | v32acc32 | acc2 )

Parameters

  a | Matrix A
  sgn_x | Sign mask for matrix A
  b | Matrix B
  sgn_y | Sign mask for matrix B
  acc1 | Accumulator 1 input
  acc2 | Accumulator 2 input

Returns
  Result of operation

## ◆ submac_conv_32x8() [3/8]

v32acc32 submac_conv_32x8 | ( | v64int8 | a,
|  | v64int8 | b,
|  | v32acc32 | acc1,
|  | v32acc32 | acc2 )

Parameters

  a | Matrix A
  b | Matrix B
  acc1 | Accumulator 1 input
  acc2 | Accumulator 2 input

Returns
  Result of operation

## ◆ submac_conv_32x8() [4/8]

v32acc32 submac_conv_32x8 | ( | v64int8 | a,
|  | v64uint8 | b,
|  | v32acc32 | acc1,
|  | v32acc32 | acc2 )

Parameters

  a | Matrix A
  b | Matrix B
  acc1 | Accumulator 1 input
  acc2 | Accumulator 2 input

Returns
  Result of operation

## ◆ submac_conv_32x8() [5/8]

v32acc32 submac_conv_32x8 | ( | v64uint8 | a,
|  | int | sgn_x,
|  | v64int8 | b,
|  | int | sgn_y,
|  | v32acc32 | acc1,
|  | v32acc32 | acc2 )

Parameters

  a | Matrix A
  sgn_x | Sign mask for matrix A
  b | Matrix B
  sgn_y | Sign mask for matrix B
  acc1 | Accumulator 1 input
  acc2 | Accumulator 2 input

Returns
  Result of operation

## ◆ submac_conv_32x8() [6/8]

v32acc32 submac_conv_32x8 | ( | v64uint8 | a,
|  | int | sgn_x,
|  | v64uint8 | b,
|  | int | sgn_y,
|  | v32acc32 | acc1,
|  | v32acc32 | acc2 )

Parameters

  a | Matrix A
  sgn_x | Sign mask for matrix A
  b | Matrix B
  sgn_y | Sign mask for matrix B
  acc1 | Accumulator 1 input
  acc2 | Accumulator 2 input

Returns
  Result of operation

## ◆ submac_conv_32x8() [7/8]

v32acc32 submac_conv_32x8 | ( | v64uint8 | a,
|  | v64int8 | b,
|  | v32acc32 | acc1,
|  | v32acc32 | acc2 )

Parameters

  a | Matrix A
  b | Matrix B
  acc1 | Accumulator 1 input
  acc2 | Accumulator 2 input

Returns
  Result of operation

## ◆ submac_conv_32x8() [8/8]

v32acc32 submac_conv_32x8 | ( | v64uint8 | a,
|  | v64uint8 | b,
|  | v32acc32 | acc1,
|  | v32acc32 | acc2 )

Parameters

  a | Matrix A
  b | Matrix B
  acc1 | Accumulator 1 input
  acc2 | Accumulator 2 input

Returns
  Result of operation

## ◆ submac_conv_32x8_conf() [1/8]

v32acc32 submac_conv_32x8_conf | ( | v64int8 | a,
|  | int | sgn_x,
|  | v64int8 | b,
|  | int | sgn_y,
|  | v32acc32 | acc1,
|  | v32acc32 | acc2,
|  | int | zero_acc1,
|  | int | sub_mul,
|  | int | sub_acc1,
|  | int | sub_acc2 )

Parameters

  a | Matrix A
  sgn_x | Sign mask for matrix A
  b | Matrix B
  sgn_y | Sign mask for matrix B
  acc1 | Accumulator 1 input
  acc2 | Accumulator 2 input
  zero_acc1 | Zeroing mask for acc1
  sub_mul | Negation mask of multiplication result
  sub_acc1 | Negation mask of acc1
  sub_acc2 | Negation mask of acc2

Returns
  Result of operation

## ◆ submac_conv_32x8_conf() [2/8]

v32acc32 submac_conv_32x8_conf | ( | v64int8 | a,
|  | int | sgn_x,
|  | v64uint8 | b,
|  | int | sgn_y,
|  | v32acc32 | acc1,
|  | v32acc32 | acc2,
|  | int | zero_acc1,
|  | int | sub_mul,
|  | int | sub_acc1,
|  | int | sub_acc2 )

Parameters

  a | Matrix A
  sgn_x | Sign mask for matrix A
  b | Matrix B
  sgn_y | Sign mask for matrix B
  acc1 | Accumulator 1 input
  acc2 | Accumulator 2 input
  zero_acc1 | Zeroing mask for acc1
  sub_mul | Negation mask of multiplication result
  sub_acc1 | Negation mask of acc1
  sub_acc2 | Negation mask of acc2

Returns
  Result of operation

## ◆ submac_conv_32x8_conf() [3/8]

v32acc32 submac_conv_32x8_conf | ( | v64int8 | a,
|  | v64int8 | b,
|  | v32acc32 | acc1,
|  | v32acc32 | acc2,
|  | int | zero_acc1,
|  | int | sub_mul,
|  | int | sub_acc1,
|  | int | sub_acc2 )

Parameters

  a | Matrix A
  b | Matrix B
  acc1 | Accumulator 1 input
  acc2 | Accumulator 2 input
  zero_acc1 | Zeroing mask for acc1
  sub_mul | Negation mask of multiplication result
  sub_acc1 | Negation mask of acc1
  sub_acc2 | Negation mask of acc2

Returns
  Result of operation

## ◆ submac_conv_32x8_conf() [4/8]

v32acc32 submac_conv_32x8_conf | ( | v64int8 | a,
|  | v64uint8 | b,
|  | v32acc32 | acc1,
|  | v32acc32 | acc2,
|  | int | zero_acc1,
|  | int | sub_mul,
|  | int | sub_acc1,
|  | int | sub_acc2 )

Parameters

  a | Matrix A
  b | Matrix B
  acc1 | Accumulator 1 input
  acc2 | Accumulator 2 input
  zero_acc1 | Zeroing mask for acc1
  sub_mul | Negation mask of multiplication result
  sub_acc1 | Negation mask of acc1
  sub_acc2 | Negation mask of acc2

Returns
  Result of operation

## ◆ submac_conv_32x8_conf() [5/8]

v32acc32 submac_conv_32x8_conf | ( | v64uint8 | a,
|  | int | sgn_x,
|  | v64int8 | b,
|  | int | sgn_y,
|  | v32acc32 | acc1,
|  | v32acc32 | acc2,
|  | int | zero_acc1,
|  | int | sub_mul,
|  | int | sub_acc1,
|  | int | sub_acc2 )

Parameters

  a | Matrix A
  sgn_x | Sign mask for matrix A
  b | Matrix B
  sgn_y | Sign mask for matrix B
  acc1 | Accumulator 1 input
  acc2 | Accumulator 2 input
  zero_acc1 | Zeroing mask for acc1
  sub_mul | Negation mask of multiplication result
  sub_acc1 | Negation mask of acc1
  sub_acc2 | Negation mask of acc2

Returns
  Result of operation

## ◆ submac_conv_32x8_conf() [6/8]

v32acc32 submac_conv_32x8_conf | ( | v64uint8 | a,
|  | int | sgn_x,
|  | v64uint8 | b,
|  | int | sgn_y,
|  | v32acc32 | acc1,
|  | v32acc32 | acc2,
|  | int | zero_acc1,
|  | int | sub_mul,
|  | int | sub_acc1,
|  | int | sub_acc2 )

Parameters

  a | Matrix A
  sgn_x | Sign mask for matrix A
  b | Matrix B
  sgn_y | Sign mask for matrix B
  acc1 | Accumulator 1 input
  acc2 | Accumulator 2 input
  zero_acc1 | Zeroing mask for acc1
  sub_mul | Negation mask of multiplication result
  sub_acc1 | Negation mask of acc1
  sub_acc2 | Negation mask of acc2

Returns
  Result of operation

## ◆ submac_conv_32x8_conf() [7/8]

v32acc32 submac_conv_32x8_conf | ( | v64uint8 | a,
|  | v64int8 | b,
|  | v32acc32 | acc1,
|  | v32acc32 | acc2,
|  | int | zero_acc1,
|  | int | sub_mul,
|  | int | sub_acc1,
|  | int | sub_acc2 )

Parameters

  a | Matrix A
  b | Matrix B
  acc1 | Accumulator 1 input
  acc2 | Accumulator 2 input
  zero_acc1 | Zeroing mask for acc1
  sub_mul | Negation mask of multiplication result
  sub_acc1 | Negation mask of acc1
  sub_acc2 | Negation mask of acc2

Returns
  Result of operation

## ◆ submac_conv_32x8_conf() [8/8]

v32acc32 submac_conv_32x8_conf | ( | v64uint8 | a,
|  | v64uint8 | b,
|  | v32acc32 | acc1,
|  | v32acc32 | acc2,
|  | int | zero_acc1,
|  | int | sub_mul,
|  | int | sub_acc1,
|  | int | sub_acc2 )

Parameters

  a | Matrix A
  b | Matrix B
  acc1 | Accumulator 1 input
  acc2 | Accumulator 2 input
  zero_acc1 | Zeroing mask for acc1
  sub_mul | Negation mask of multiplication result
  sub_acc1 | Negation mask of acc1
  sub_acc2 | Negation mask of acc2

Returns
  Result of operation

## ◆ submac_conv_4x4_8ch() [1/8]

v32acc32 submac_conv_4x4_8ch | ( | v64int8 | a,
|  | int | sgn_x,
|  | v64int8 | b,
|  | int | sgn_y,
|  | v32acc32 | acc1,
|  | v32acc32 | acc2 )

Parameters

  a | Matrix A
  sgn_x | Sign mask for matrix A
  b | Matrix B
  sgn_y | Sign mask for matrix B
  acc1 | Accumulator 1 input
  acc2 | Accumulator 2 input

Returns
  Result of operation

## ◆ submac_conv_4x4_8ch() [2/8]

v32acc32 submac_conv_4x4_8ch | ( | v64int8 | a,
|  | int | sgn_x,
|  | v64uint8 | b,
|  | int | sgn_y,
|  | v32acc32 | acc1,
|  | v32acc32 | acc2 )

Parameters

  a | Matrix A
  sgn_x | Sign mask for matrix A
  b | Matrix B
  sgn_y | Sign mask for matrix B
  acc1 | Accumulator 1 input
  acc2 | Accumulator 2 input

Returns
  Result of operation

## ◆ submac_conv_4x4_8ch() [3/8]

v32acc32 submac_conv_4x4_8ch | ( | v64int8 | a,
|  | v64int8 | b,
|  | v32acc32 | acc1,
|  | v32acc32 | acc2 )

Parameters

  a | Matrix A
  b | Matrix B
  acc1 | Accumulator 1 input
  acc2 | Accumulator 2 input

Returns
  Result of operation

## ◆ submac_conv_4x4_8ch() [4/8]

v32acc32 submac_conv_4x4_8ch | ( | v64int8 | a,
|  | v64uint8 | b,
|  | v32acc32 | acc1,
|  | v32acc32 | acc2 )

Parameters

  a | Matrix A
  b | Matrix B
  acc1 | Accumulator 1 input
  acc2 | Accumulator 2 input

Returns
  Result of operation

## ◆ submac_conv_4x4_8ch() [5/8]

v32acc32 submac_conv_4x4_8ch | ( | v64uint8 | a,
|  | int | sgn_x,
|  | v64int8 | b,
|  | int | sgn_y,
|  | v32acc32 | acc1,
|  | v32acc32 | acc2 )

Parameters

  a | Matrix A
  sgn_x | Sign mask for matrix A
  b | Matrix B
  sgn_y | Sign mask for matrix B
  acc1 | Accumulator 1 input
  acc2 | Accumulator 2 input

Returns
  Result of operation

## ◆ submac_conv_4x4_8ch() [6/8]

v32acc32 submac_conv_4x4_8ch | ( | v64uint8 | a,
|  | int | sgn_x,
|  | v64uint8 | b,
|  | int | sgn_y,
|  | v32acc32 | acc1,
|  | v32acc32 | acc2 )

Parameters

  a | Matrix A
  sgn_x | Sign mask for matrix A
  b | Matrix B
  sgn_y | Sign mask for matrix B
  acc1 | Accumulator 1 input
  acc2 | Accumulator 2 input

Returns
  Result of operation

## ◆ submac_conv_4x4_8ch() [7/8]

v32acc32 submac_conv_4x4_8ch | ( | v64uint8 | a,
|  | v64int8 | b,
|  | v32acc32 | acc1,
|  | v32acc32 | acc2 )

Parameters

  a | Matrix A
  b | Matrix B
  acc1 | Accumulator 1 input
  acc2 | Accumulator 2 input

Returns
  Result of operation

## ◆ submac_conv_4x4_8ch() [8/8]

v32acc32 submac_conv_4x4_8ch | ( | v64uint8 | a,
|  | v64uint8 | b,
|  | v32acc32 | acc1,
|  | v32acc32 | acc2 )

Parameters

  a | Matrix A
  b | Matrix B
  acc1 | Accumulator 1 input
  acc2 | Accumulator 2 input

Returns
  Result of operation

## ◆ submac_conv_4x4_8ch_conf() [1/8]

v32acc32 submac_conv_4x4_8ch_conf | ( | v64int8 | a,
|  | int | sgn_x,
|  | v64int8 | b,
|  | int | sgn_y,
|  | v32acc32 | acc1,
|  | v32acc32 | acc2,
|  | int | zero_acc1,
|  | int | sub_mul,
|  | int | sub_acc1,
|  | int | sub_acc2 )

Parameters

  a | Matrix A
  sgn_x | Sign mask for matrix A
  b | Matrix B
  sgn_y | Sign mask for matrix B
  acc1 | Accumulator 1 input
  acc2 | Accumulator 2 input
  zero_acc1 | Zeroing mask for acc1
  sub_mul | Negation mask of multiplication result
  sub_acc1 | Negation mask of acc1
  sub_acc2 | Negation mask of acc2

Returns
  Result of operation

## ◆ submac_conv_4x4_8ch_conf() [2/8]

v32acc32 submac_conv_4x4_8ch_conf | ( | v64int8 | a,
|  | int | sgn_x,
|  | v64uint8 | b,
|  | int | sgn_y,
|  | v32acc32 | acc1,
|  | v32acc32 | acc2,
|  | int | zero_acc1,
|  | int | sub_mul,
|  | int | sub_acc1,
|  | int | sub_acc2 )

Parameters

  a | Matrix A
  sgn_x | Sign mask for matrix A
  b | Matrix B
  sgn_y | Sign mask for matrix B
  acc1 | Accumulator 1 input
  acc2 | Accumulator 2 input
  zero_acc1 | Zeroing mask for acc1
  sub_mul | Negation mask of multiplication result
  sub_acc1 | Negation mask of acc1
  sub_acc2 | Negation mask of acc2

Returns
  Result of operation

## ◆ submac_conv_4x4_8ch_conf() [3/8]

v32acc32 submac_conv_4x4_8ch_conf | ( | v64int8 | a,
|  | v64int8 | b,
|  | v32acc32 | acc1,
|  | v32acc32 | acc2,
|  | int | zero_acc1,
|  | int | sub_mul,
|  | int | sub_acc1,
|  | int | sub_acc2 )

Parameters

  a | Matrix A
  b | Matrix B
  acc1 | Accumulator 1 input
  acc2 | Accumulator 2 input
  zero_acc1 | Zeroing mask for acc1
  sub_mul | Negation mask of multiplication result
  sub_acc1 | Negation mask of acc1
  sub_acc2 | Negation mask of acc2

Returns
  Result of operation

## ◆ submac_conv_4x4_8ch_conf() [4/8]

v32acc32 submac_conv_4x4_8ch_conf | ( | v64int8 | a,
|  | v64uint8 | b,
|  | v32acc32 | acc1,
|  | v32acc32 | acc2,
|  | int | zero_acc1,
|  | int | sub_mul,
|  | int | sub_acc1,
|  | int | sub_acc2 )

Parameters

  a | Matrix A
  b | Matrix B
  acc1 | Accumulator 1 input
  acc2 | Accumulator 2 input
  zero_acc1 | Zeroing mask for acc1
  sub_mul | Negation mask of multiplication result
  sub_acc1 | Negation mask of acc1
  sub_acc2 | Negation mask of acc2

Returns
  Result of operation

## ◆ submac_conv_4x4_8ch_conf() [5/8]

v32acc32 submac_conv_4x4_8ch_conf | ( | v64uint8 | a,
|  | int | sgn_x,
|  | v64int8 | b,
|  | int | sgn_y,
|  | v32acc32 | acc1,
|  | v32acc32 | acc2,
|  | int | zero_acc1,
|  | int | sub_mul,
|  | int | sub_acc1,
|  | int | sub_acc2 )

Parameters

  a | Matrix A
  sgn_x | Sign mask for matrix A
  b | Matrix B
  sgn_y | Sign mask for matrix B
  acc1 | Accumulator 1 input
  acc2 | Accumulator 2 input
  zero_acc1 | Zeroing mask for acc1
  sub_mul | Negation mask of multiplication result
  sub_acc1 | Negation mask of acc1
  sub_acc2 | Negation mask of acc2

Returns
  Result of operation

## ◆ submac_conv_4x4_8ch_conf() [6/8]

v32acc32 submac_conv_4x4_8ch_conf | ( | v64uint8 | a,
|  | int | sgn_x,
|  | v64uint8 | b,
|  | int | sgn_y,
|  | v32acc32 | acc1,
|  | v32acc32 | acc2,
|  | int | zero_acc1,
|  | int | sub_mul,
|  | int | sub_acc1,
|  | int | sub_acc2 )

Parameters

  a | Matrix A
  sgn_x | Sign mask for matrix A
  b | Matrix B
  sgn_y | Sign mask for matrix B
  acc1 | Accumulator 1 input
  acc2 | Accumulator 2 input
  zero_acc1 | Zeroing mask for acc1
  sub_mul | Negation mask of multiplication result
  sub_acc1 | Negation mask of acc1
  sub_acc2 | Negation mask of acc2

Returns
  Result of operation

## ◆ submac_conv_4x4_8ch_conf() [7/8]

v32acc32 submac_conv_4x4_8ch_conf | ( | v64uint8 | a,
|  | v64int8 | b,
|  | v32acc32 | acc1,
|  | v32acc32 | acc2,
|  | int | zero_acc1,
|  | int | sub_mul,
|  | int | sub_acc1,
|  | int | sub_acc2 )

Parameters

  a | Matrix A
  b | Matrix B
  acc1 | Accumulator 1 input
  acc2 | Accumulator 2 input
  zero_acc1 | Zeroing mask for acc1
  sub_mul | Negation mask of multiplication result
  sub_acc1 | Negation mask of acc1
  sub_acc2 | Negation mask of acc2

Returns
  Result of operation

## ◆ submac_conv_4x4_8ch_conf() [8/8]

v32acc32 submac_conv_4x4_8ch_conf | ( | v64uint8 | a,
|  | v64uint8 | b,
|  | v32acc32 | acc1,
|  | v32acc32 | acc2,
|  | int | zero_acc1,
|  | int | sub_mul,
|  | int | sub_acc1,
|  | int | sub_acc2 )

Parameters

  a | Matrix A
  b | Matrix B
  acc1 | Accumulator 1 input
  acc2 | Accumulator 2 input
  zero_acc1 | Zeroing mask for acc1
  sub_mul | Negation mask of multiplication result
  sub_acc1 | Negation mask of acc1
  sub_acc2 | Negation mask of acc2

Returns
  Result of operation

## ◆ submac_conv_8x8_4ch() [1/8]

v32acc32 submac_conv_8x8_4ch | ( | v64int8 | a,
|  | int | sgn_x,
|  | v64int8 | b,
|  | int | sgn_y,
|  | v32acc32 | acc1,
|  | v32acc32 | acc2 )

Parameters

  a | Matrix A
  sgn_x | Sign mask for matrix A
  b | Matrix B
  sgn_y | Sign mask for matrix B
  acc1 | Accumulator 1 input
  acc2 | Accumulator 2 input

Returns
  Result of operation

## ◆ submac_conv_8x8_4ch() [2/8]

v32acc32 submac_conv_8x8_4ch | ( | v64int8 | a,
|  | int | sgn_x,
|  | v64uint8 | b,
|  | int | sgn_y,
|  | v32acc32 | acc1,
|  | v32acc32 | acc2 )

Parameters

  a | Matrix A
  sgn_x | Sign mask for matrix A
  b | Matrix B
  sgn_y | Sign mask for matrix B
  acc1 | Accumulator 1 input
  acc2 | Accumulator 2 input

Returns
  Result of operation

## ◆ submac_conv_8x8_4ch() [3/8]

v32acc32 submac_conv_8x8_4ch | ( | v64int8 | a,
|  | v64int8 | b,
|  | v32acc32 | acc1,
|  | v32acc32 | acc2 )

Parameters

  a | Matrix A
  b | Matrix B
  acc1 | Accumulator 1 input
  acc2 | Accumulator 2 input

Returns
  Result of operation

## ◆ submac_conv_8x8_4ch() [4/8]

v32acc32 submac_conv_8x8_4ch | ( | v64int8 | a,
|  | v64uint8 | b,
|  | v32acc32 | acc1,
|  | v32acc32 | acc2 )

Parameters

  a | Matrix A
  b | Matrix B
  acc1 | Accumulator 1 input
  acc2 | Accumulator 2 input

Returns
  Result of operation

## ◆ submac_conv_8x8_4ch() [5/8]

v32acc32 submac_conv_8x8_4ch | ( | v64uint8 | a,
|  | int | sgn_x,
|  | v64int8 | b,
|  | int | sgn_y,
|  | v32acc32 | acc1,
|  | v32acc32 | acc2 )

Parameters

  a | Matrix A
  sgn_x | Sign mask for matrix A
  b | Matrix B
  sgn_y | Sign mask for matrix B
  acc1 | Accumulator 1 input
  acc2 | Accumulator 2 input

Returns
  Result of operation

## ◆ submac_conv_8x8_4ch() [6/8]

v32acc32 submac_conv_8x8_4ch | ( | v64uint8 | a,
|  | int | sgn_x,
|  | v64uint8 | b,
|  | int | sgn_y,
|  | v32acc32 | acc1,
|  | v32acc32 | acc2 )

Parameters

  a | Matrix A
  sgn_x | Sign mask for matrix A
  b | Matrix B
  sgn_y | Sign mask for matrix B
  acc1 | Accumulator 1 input
  acc2 | Accumulator 2 input

Returns
  Result of operation

## ◆ submac_conv_8x8_4ch() [7/8]

v32acc32 submac_conv_8x8_4ch | ( | v64uint8 | a,
|  | v64int8 | b,
|  | v32acc32 | acc1,
|  | v32acc32 | acc2 )

Parameters

  a | Matrix A
  b | Matrix B
  acc1 | Accumulator 1 input
  acc2 | Accumulator 2 input

Returns
  Result of operation

## ◆ submac_conv_8x8_4ch() [8/8]

v32acc32 submac_conv_8x8_4ch | ( | v64uint8 | a,
|  | v64uint8 | b,
|  | v32acc32 | acc1,
|  | v32acc32 | acc2 )

Parameters

  a | Matrix A
  b | Matrix B
  acc1 | Accumulator 1 input
  acc2 | Accumulator 2 input

Returns
  Result of operation

## ◆ submac_conv_8x8_4ch_conf() [1/8]

v32acc32 submac_conv_8x8_4ch_conf | ( | v64int8 | a,
|  | int | sgn_x,
|  | v64int8 | b,
|  | int | sgn_y,
|  | v32acc32 | acc1,
|  | v32acc32 | acc2,
|  | int | zero_acc1,
|  | int | sub_mul,
|  | int | sub_acc1,
|  | int | sub_acc2 )

Parameters

  a | Matrix A
  sgn_x | Sign mask for matrix A
  b | Matrix B
  sgn_y | Sign mask for matrix B
  acc1 | Accumulator 1 input
  acc2 | Accumulator 2 input
  zero_acc1 | Zeroing mask for acc1
  sub_mul | Negation mask of multiplication result
  sub_acc1 | Negation mask of acc1
  sub_acc2 | Negation mask of acc2

Returns
  Result of operation

## ◆ submac_conv_8x8_4ch_conf() [2/8]

v32acc32 submac_conv_8x8_4ch_conf | ( | v64int8 | a,
|  | int | sgn_x,
|  | v64uint8 | b,
|  | int | sgn_y,
|  | v32acc32 | acc1,
|  | v32acc32 | acc2,
|  | int | zero_acc1,
|  | int | sub_mul,
|  | int | sub_acc1,
|  | int | sub_acc2 )

Parameters

  a | Matrix A
  sgn_x | Sign mask for matrix A
  b | Matrix B
  sgn_y | Sign mask for matrix B
  acc1 | Accumulator 1 input
  acc2 | Accumulator 2 input
  zero_acc1 | Zeroing mask for acc1
  sub_mul | Negation mask of multiplication result
  sub_acc1 | Negation mask of acc1
  sub_acc2 | Negation mask of acc2

Returns
  Result of operation

## ◆ submac_conv_8x8_4ch_conf() [3/8]

v32acc32 submac_conv_8x8_4ch_conf | ( | v64int8 | a,
|  | v64int8 | b,
|  | v32acc32 | acc1,
|  | v32acc32 | acc2,
|  | int | zero_acc1,
|  | int | sub_mul,
|  | int | sub_acc1,
|  | int | sub_acc2 )

Parameters

  a | Matrix A
  b | Matrix B
  acc1 | Accumulator 1 input
  acc2 | Accumulator 2 input
  zero_acc1 | Zeroing mask for acc1
  sub_mul | Negation mask of multiplication result
  sub_acc1 | Negation mask of acc1
  sub_acc2 | Negation mask of acc2

Returns
  Result of operation

## ◆ submac_conv_8x8_4ch_conf() [4/8]

v32acc32 submac_conv_8x8_4ch_conf | ( | v64int8 | a,
|  | v64uint8 | b,
|  | v32acc32 | acc1,
|  | v32acc32 | acc2,
|  | int | zero_acc1,
|  | int | sub_mul,
|  | int | sub_acc1,
|  | int | sub_acc2 )

Parameters

  a | Matrix A
  b | Matrix B
  acc1 | Accumulator 1 input
  acc2 | Accumulator 2 input
  zero_acc1 | Zeroing mask for acc1
  sub_mul | Negation mask of multiplication result
  sub_acc1 | Negation mask of acc1
  sub_acc2 | Negation mask of acc2

Returns
  Result of operation

## ◆ submac_conv_8x8_4ch_conf() [5/8]

v32acc32 submac_conv_8x8_4ch_conf | ( | v64uint8 | a,
|  | int | sgn_x,
|  | v64int8 | b,
|  | int | sgn_y,
|  | v32acc32 | acc1,
|  | v32acc32 | acc2,
|  | int | zero_acc1,
|  | int | sub_mul,
|  | int | sub_acc1,
|  | int | sub_acc2 )

Parameters

  a | Matrix A
  sgn_x | Sign mask for matrix A
  b | Matrix B
  sgn_y | Sign mask for matrix B
  acc1 | Accumulator 1 input
  acc2 | Accumulator 2 input
  zero_acc1 | Zeroing mask for acc1
  sub_mul | Negation mask of multiplication result
  sub_acc1 | Negation mask of acc1
  sub_acc2 | Negation mask of acc2

Returns
  Result of operation

## ◆ submac_conv_8x8_4ch_conf() [6/8]

v32acc32 submac_conv_8x8_4ch_conf | ( | v64uint8 | a,
|  | int | sgn_x,
|  | v64uint8 | b,
|  | int | sgn_y,
|  | v32acc32 | acc1,
|  | v32acc32 | acc2,
|  | int | zero_acc1,
|  | int | sub_mul,
|  | int | sub_acc1,
|  | int | sub_acc2 )

Parameters

  a | Matrix A
  sgn_x | Sign mask for matrix A
  b | Matrix B
  sgn_y | Sign mask for matrix B
  acc1 | Accumulator 1 input
  acc2 | Accumulator 2 input
  zero_acc1 | Zeroing mask for acc1
  sub_mul | Negation mask of multiplication result
  sub_acc1 | Negation mask of acc1
  sub_acc2 | Negation mask of acc2

Returns
  Result of operation

## ◆ submac_conv_8x8_4ch_conf() [7/8]

v32acc32 submac_conv_8x8_4ch_conf | ( | v64uint8 | a,
|  | v64int8 | b,
|  | v32acc32 | acc1,
|  | v32acc32 | acc2,
|  | int | zero_acc1,
|  | int | sub_mul,
|  | int | sub_acc1,
|  | int | sub_acc2 )

Parameters

  a | Matrix A
  b | Matrix B
  acc1 | Accumulator 1 input
  acc2 | Accumulator 2 input
  zero_acc1 | Zeroing mask for acc1
  sub_mul | Negation mask of multiplication result
  sub_acc1 | Negation mask of acc1
  sub_acc2 | Negation mask of acc2

Returns
  Result of operation

## ◆ submac_conv_8x8_4ch_conf() [8/8]

v32acc32 submac_conv_8x8_4ch_conf | ( | v64uint8 | a,
|  | v64uint8 | b,
|  | v32acc32 | acc1,
|  | v32acc32 | acc2,
|  | int | zero_acc1,
|  | int | sub_mul,
|  | int | sub_acc1,
|  | int | sub_acc2 )

Parameters

  a | Matrix A
  b | Matrix B
  acc1 | Accumulator 1 input
  acc2 | Accumulator 2 input
  zero_acc1 | Zeroing mask for acc1
  sub_mul | Negation mask of multiplication result
  sub_acc1 | Negation mask of acc1
  sub_acc2 | Negation mask of acc2

Returns
  Result of operation

## ◆ submac_elem_32_2() [1/8]

v32acc32 submac_elem_32_2 | ( | v64int8 | a,
|  | int | sgn_x,
|  | v64int8 | b,
|  | int | sgn_y,
|  | v32acc32 | acc1,
|  | v32acc32 | acc2 )

Parameters

  a | Matrix A
  sgn_x | Sign mask for matrix A
  b | Matrix B
  sgn_y | Sign mask for matrix B
  acc1 | Accumulator 1 input
  acc2 | Accumulator 2 input

Returns
  Result of operation

## ◆ submac_elem_32_2() [2/8]

v32acc32 submac_elem_32_2 | ( | v64int8 | a,
|  | int | sgn_x,
|  | v64uint8 | b,
|  | int | sgn_y,
|  | v32acc32 | acc1,
|  | v32acc32 | acc2 )

Parameters

  a | Matrix A
  sgn_x | Sign mask for matrix A
  b | Matrix B
  sgn_y | Sign mask for matrix B
  acc1 | Accumulator 1 input
  acc2 | Accumulator 2 input

Returns
  Result of operation

## ◆ submac_elem_32_2() [3/8]

v32acc32 submac_elem_32_2 | ( | v64int8 | a,
|  | v64int8 | b,
|  | v32acc32 | acc1,
|  | v32acc32 | acc2 )

Parameters

  a | Matrix A
  b | Matrix B
  acc1 | Accumulator 1 input
  acc2 | Accumulator 2 input

Returns
  Result of operation

## ◆ submac_elem_32_2() [4/8]

v32acc32 submac_elem_32_2 | ( | v64int8 | a,
|  | v64uint8 | b,
|  | v32acc32 | acc1,
|  | v32acc32 | acc2 )

Parameters

  a | Matrix A
  b | Matrix B
  acc1 | Accumulator 1 input
  acc2 | Accumulator 2 input

Returns
  Result of operation

## ◆ submac_elem_32_2() [5/8]

v32acc32 submac_elem_32_2 | ( | v64uint8 | a,
|  | int | sgn_x,
|  | v64int8 | b,
|  | int | sgn_y,
|  | v32acc32 | acc1,
|  | v32acc32 | acc2 )

Parameters

  a | Matrix A
  sgn_x | Sign mask for matrix A
  b | Matrix B
  sgn_y | Sign mask for matrix B
  acc1 | Accumulator 1 input
  acc2 | Accumulator 2 input

Returns
  Result of operation

## ◆ submac_elem_32_2() [6/8]

v32acc32 submac_elem_32_2 | ( | v64uint8 | a,
|  | int | sgn_x,
|  | v64uint8 | b,
|  | int | sgn_y,
|  | v32acc32 | acc1,
|  | v32acc32 | acc2 )

Parameters

  a | Matrix A
  sgn_x | Sign mask for matrix A
  b | Matrix B
  sgn_y | Sign mask for matrix B
  acc1 | Accumulator 1 input
  acc2 | Accumulator 2 input

Returns
  Result of operation

## ◆ submac_elem_32_2() [7/8]

v32acc32 submac_elem_32_2 | ( | v64uint8 | a,
|  | v64int8 | b,
|  | v32acc32 | acc1,
|  | v32acc32 | acc2 )

Parameters

  a | Matrix A
  b | Matrix B
  acc1 | Accumulator 1 input
  acc2 | Accumulator 2 input

Returns
  Result of operation

## ◆ submac_elem_32_2() [8/8]

v32acc32 submac_elem_32_2 | ( | v64uint8 | a,
|  | v64uint8 | b,
|  | v32acc32 | acc1,
|  | v32acc32 | acc2 )

Parameters

  a | Matrix A
  b | Matrix B
  acc1 | Accumulator 1 input
  acc2 | Accumulator 2 input

Returns
  Result of operation

## ◆ submac_elem_32_2_conf() [1/8]

v32acc32 submac_elem_32_2_conf | ( | v64int8 | a,
|  | int | sgn_x,
|  | v64int8 | b,
|  | int | sgn_y,
|  | v32acc32 | acc1,
|  | v32acc32 | acc2,
|  | int | zero_acc1,
|  | int | sub_mul,
|  | int | sub_acc1,
|  | int | sub_acc2 )

Parameters

  a | Matrix A
  sgn_x | Sign mask for matrix A
  b | Matrix B
  sgn_y | Sign mask for matrix B
  acc1 | Accumulator 1 input
  acc2 | Accumulator 2 input
  zero_acc1 | Zeroing mask for acc1
  sub_mul | Negation mask of multiplication result
  sub_acc1 | Negation mask of acc1
  sub_acc2 | Negation mask of acc2

Returns
  Result of operation

## ◆ submac_elem_32_2_conf() [2/8]

v32acc32 submac_elem_32_2_conf | ( | v64int8 | a,
|  | int | sgn_x,
|  | v64uint8 | b,
|  | int | sgn_y,
|  | v32acc32 | acc1,
|  | v32acc32 | acc2,
|  | int | zero_acc1,
|  | int | sub_mul,
|  | int | sub_acc1,
|  | int | sub_acc2 )

Parameters

  a | Matrix A
  sgn_x | Sign mask for matrix A
  b | Matrix B
  sgn_y | Sign mask for matrix B
  acc1 | Accumulator 1 input
  acc2 | Accumulator 2 input
  zero_acc1 | Zeroing mask for acc1
  sub_mul | Negation mask of multiplication result
  sub_acc1 | Negation mask of acc1
  sub_acc2 | Negation mask of acc2

Returns
  Result of operation

## ◆ submac_elem_32_2_conf() [3/8]

v32acc32 submac_elem_32_2_conf | ( | v64int8 | a,
|  | v64int8 | b,
|  | v32acc32 | acc1,
|  | v32acc32 | acc2,
|  | int | zero_acc1,
|  | int | sub_mul,
|  | int | sub_acc1,
|  | int | sub_acc2 )

Parameters

  a | Matrix A
  b | Matrix B
  acc1 | Accumulator 1 input
  acc2 | Accumulator 2 input
  zero_acc1 | Zeroing mask for acc1
  sub_mul | Negation mask of multiplication result
  sub_acc1 | Negation mask of acc1
  sub_acc2 | Negation mask of acc2

Returns
  Result of operation

## ◆ submac_elem_32_2_conf() [4/8]

v32acc32 submac_elem_32_2_conf | ( | v64int8 | a,
|  | v64uint8 | b,
|  | v32acc32 | acc1,
|  | v32acc32 | acc2,
|  | int | zero_acc1,
|  | int | sub_mul,
|  | int | sub_acc1,
|  | int | sub_acc2 )

Parameters

  a | Matrix A
  b | Matrix B
  acc1 | Accumulator 1 input
  acc2 | Accumulator 2 input
  zero_acc1 | Zeroing mask for acc1
  sub_mul | Negation mask of multiplication result
  sub_acc1 | Negation mask of acc1
  sub_acc2 | Negation mask of acc2

Returns
  Result of operation

## ◆ submac_elem_32_2_conf() [5/8]

v32acc32 submac_elem_32_2_conf | ( | v64uint8 | a,
|  | int | sgn_x,
|  | v64int8 | b,
|  | int | sgn_y,
|  | v32acc32 | acc1,
|  | v32acc32 | acc2,
|  | int | zero_acc1,
|  | int | sub_mul,
|  | int | sub_acc1,
|  | int | sub_acc2 )

Parameters

  a | Matrix A
  sgn_x | Sign mask for matrix A
  b | Matrix B
  sgn_y | Sign mask for matrix B
  acc1 | Accumulator 1 input
  acc2 | Accumulator 2 input
  zero_acc1 | Zeroing mask for acc1
  sub_mul | Negation mask of multiplication result
  sub_acc1 | Negation mask of acc1
  sub_acc2 | Negation mask of acc2

Returns
  Result of operation

## ◆ submac_elem_32_2_conf() [6/8]

v32acc32 submac_elem_32_2_conf | ( | v64uint8 | a,
|  | int | sgn_x,
|  | v64uint8 | b,
|  | int | sgn_y,
|  | v32acc32 | acc1,
|  | v32acc32 | acc2,
|  | int | zero_acc1,
|  | int | sub_mul,
|  | int | sub_acc1,
|  | int | sub_acc2 )

Parameters

  a | Matrix A
  sgn_x | Sign mask for matrix A
  b | Matrix B
  sgn_y | Sign mask for matrix B
  acc1 | Accumulator 1 input
  acc2 | Accumulator 2 input
  zero_acc1 | Zeroing mask for acc1
  sub_mul | Negation mask of multiplication result
  sub_acc1 | Negation mask of acc1
  sub_acc2 | Negation mask of acc2

Returns
  Result of operation

## ◆ submac_elem_32_2_conf() [7/8]

v32acc32 submac_elem_32_2_conf | ( | v64uint8 | a,
|  | v64int8 | b,
|  | v32acc32 | acc1,
|  | v32acc32 | acc2,
|  | int | zero_acc1,
|  | int | sub_mul,
|  | int | sub_acc1,
|  | int | sub_acc2 )

Parameters

  a | Matrix A
  b | Matrix B
  acc1 | Accumulator 1 input
  acc2 | Accumulator 2 input
  zero_acc1 | Zeroing mask for acc1
  sub_mul | Negation mask of multiplication result
  sub_acc1 | Negation mask of acc1
  sub_acc2 | Negation mask of acc2

Returns
  Result of operation

## ◆ submac_elem_32_2_conf() [8/8]

v32acc32 submac_elem_32_2_conf | ( | v64uint8 | a,
|  | v64uint8 | b,
|  | v32acc32 | acc1,
|  | v32acc32 | acc2,
|  | int | zero_acc1,
|  | int | sub_mul,
|  | int | sub_acc1,
|  | int | sub_acc2 )

Parameters

  a | Matrix A
  b | Matrix B
  acc1 | Accumulator 1 input
  acc2 | Accumulator 2 input
  zero_acc1 | Zeroing mask for acc1
  sub_mul | Negation mask of multiplication result
  sub_acc1 | Negation mask of acc1
  sub_acc2 | Negation mask of acc2

Returns
  Result of operation

## ◆ submsc_4x8_8x8() [1/8]

v32acc32 submsc_4x8_8x8 | ( | v64int8 | a,
|  | int | sgn_x,
|  | v64int8 | b,
|  | int | sgn_y,
|  | v32acc32 | acc1,
|  | v32acc32 | acc2 )

Parameters

  a | Matrix A
  sgn_x | Sign mask for matrix A
  b | Matrix B
  sgn_y | Sign mask for matrix B
  acc1 | Accumulator 1 input
  acc2 | Accumulator 2 input

Returns
  Result of operation

## ◆ submsc_4x8_8x8() [2/8]

v32acc32 submsc_4x8_8x8 | ( | v64int8 | a,
|  | int | sgn_x,
|  | v64uint8 | b,
|  | int | sgn_y,
|  | v32acc32 | acc1,
|  | v32acc32 | acc2 )

Parameters

  a | Matrix A
  sgn_x | Sign mask for matrix A
  b | Matrix B
  sgn_y | Sign mask for matrix B
  acc1 | Accumulator 1 input
  acc2 | Accumulator 2 input

Returns
  Result of operation

## ◆ submsc_4x8_8x8() [3/8]

v32acc32 submsc_4x8_8x8 | ( | v64int8 | a,
|  | v64int8 | b,
|  | v32acc32 | acc1,
|  | v32acc32 | acc2 )

Parameters

  a | Matrix A
  b | Matrix B
  acc1 | Accumulator 1 input
  acc2 | Accumulator 2 input

Returns
  Result of operation

## ◆ submsc_4x8_8x8() [4/8]

v32acc32 submsc_4x8_8x8 | ( | v64int8 | a,
|  | v64uint8 | b,
|  | v32acc32 | acc1,
|  | v32acc32 | acc2 )

Parameters

  a | Matrix A
  b | Matrix B
  acc1 | Accumulator 1 input
  acc2 | Accumulator 2 input

Returns
  Result of operation

## ◆ submsc_4x8_8x8() [5/8]

v32acc32 submsc_4x8_8x8 | ( | v64uint8 | a,
|  | int | sgn_x,
|  | v64int8 | b,
|  | int | sgn_y,
|  | v32acc32 | acc1,
|  | v32acc32 | acc2 )

Parameters

  a | Matrix A
  sgn_x | Sign mask for matrix A
  b | Matrix B
  sgn_y | Sign mask for matrix B
  acc1 | Accumulator 1 input
  acc2 | Accumulator 2 input

Returns
  Result of operation

## ◆ submsc_4x8_8x8() [6/8]

v32acc32 submsc_4x8_8x8 | ( | v64uint8 | a,
|  | int | sgn_x,
|  | v64uint8 | b,
|  | int | sgn_y,
|  | v32acc32 | acc1,
|  | v32acc32 | acc2 )

Parameters

  a | Matrix A
  sgn_x | Sign mask for matrix A
  b | Matrix B
  sgn_y | Sign mask for matrix B
  acc1 | Accumulator 1 input
  acc2 | Accumulator 2 input

Returns
  Result of operation

## ◆ submsc_4x8_8x8() [7/8]

v32acc32 submsc_4x8_8x8 | ( | v64uint8 | a,
|  | v64int8 | b,
|  | v32acc32 | acc1,
|  | v32acc32 | acc2 )

Parameters

  a | Matrix A
  b | Matrix B
  acc1 | Accumulator 1 input
  acc2 | Accumulator 2 input

Returns
  Result of operation

## ◆ submsc_4x8_8x8() [8/8]

v32acc32 submsc_4x8_8x8 | ( | v64uint8 | a,
|  | v64uint8 | b,
|  | v32acc32 | acc1,
|  | v32acc32 | acc2 )

Parameters

  a | Matrix A
  b | Matrix B
  acc1 | Accumulator 1 input
  acc2 | Accumulator 2 input

Returns
  Result of operation

## ◆ submsc_4x8_8x8_conf() [1/8]

v32acc32 submsc_4x8_8x8_conf | ( | v64int8 | a,
|  | int | sgn_x,
|  | v64int8 | b,
|  | int | sgn_y,
|  | v32acc32 | acc1,
|  | v32acc32 | acc2,
|  | int | zero_acc1,
|  | int | sub_mul,
|  | int | sub_acc1,
|  | int | sub_acc2 )

Parameters

  a | Matrix A
  sgn_x | Sign mask for matrix A
  b | Matrix B
  sgn_y | Sign mask for matrix B
  acc1 | Accumulator 1 input
  acc2 | Accumulator 2 input
  zero_acc1 | Zeroing mask for acc1
  sub_mul | Negation mask of multiplication result.
  sub_acc1 | Negation mask of acc1
  sub_acc2 | Negation mask of acc2

Returns
  Result of operation

## ◆ submsc_4x8_8x8_conf() [2/8]

v32acc32 submsc_4x8_8x8_conf | ( | v64int8 | a,
|  | int | sgn_x,
|  | v64uint8 | b,
|  | int | sgn_y,
|  | v32acc32 | acc1,
|  | v32acc32 | acc2,
|  | int | zero_acc1,
|  | int | sub_mul,
|  | int | sub_acc1,
|  | int | sub_acc2 )

Parameters

  a | Matrix A
  sgn_x | Sign mask for matrix A
  b | Matrix B
  sgn_y | Sign mask for matrix B
  acc1 | Accumulator 1 input
  acc2 | Accumulator 2 input
  zero_acc1 | Zeroing mask for acc1
  sub_mul | Negation mask of multiplication result.
  sub_acc1 | Negation mask of acc1
  sub_acc2 | Negation mask of acc2

Returns
  Result of operation

## ◆ submsc_4x8_8x8_conf() [3/8]

v32acc32 submsc_4x8_8x8_conf | ( | v64int8 | a,
|  | v64int8 | b,
|  | v32acc32 | acc1,
|  | v32acc32 | acc2,
|  | int | zero_acc1,
|  | int | sub_mul,
|  | int | sub_acc1,
|  | int | sub_acc2 )

Parameters

  a | Matrix A
  b | Matrix B
  acc1 | Accumulator 1 input
  acc2 | Accumulator 2 input
  zero_acc1 | Zeroing mask for acc1
  sub_mul | Negation mask of multiplication result
  sub_acc1 | Negation mask of acc1
  sub_acc2 | Negation mask of acc2

Returns
  Result of operation

## ◆ submsc_4x8_8x8_conf() [4/8]

v32acc32 submsc_4x8_8x8_conf | ( | v64int8 | a,
|  | v64uint8 | b,
|  | v32acc32 | acc1,
|  | v32acc32 | acc2,
|  | int | zero_acc1,
|  | int | sub_mul,
|  | int | sub_acc1,
|  | int | sub_acc2 )

Parameters

  a | Matrix A
  b | Matrix B
  acc1 | Accumulator 1 input
  acc2 | Accumulator 2 input
  zero_acc1 | Zeroing mask for acc1
  sub_mul | Negation mask of multiplication result
  sub_acc1 | Negation mask of acc1
  sub_acc2 | Negation mask of acc2

Returns
  Result of operation

## ◆ submsc_4x8_8x8_conf() [5/8]

v32acc32 submsc_4x8_8x8_conf | ( | v64uint8 | a,
|  | int | sgn_x,
|  | v64int8 | b,
|  | int | sgn_y,
|  | v32acc32 | acc1,
|  | v32acc32 | acc2,
|  | int | zero_acc1,
|  | int | sub_mul,
|  | int | sub_acc1,
|  | int | sub_acc2 )

Parameters

  a | Matrix A
  sgn_x | Sign mask for matrix A
  b | Matrix B
  sgn_y | Sign mask for matrix B
  acc1 | Accumulator 1 input
  acc2 | Accumulator 2 input
  zero_acc1 | Zeroing mask for acc1
  sub_mul | Negation mask of multiplication result.
  sub_acc1 | Negation mask of acc1
  sub_acc2 | Negation mask of acc2

Returns
  Result of operation

## ◆ submsc_4x8_8x8_conf() [6/8]

v32acc32 submsc_4x8_8x8_conf | ( | v64uint8 | a,
|  | int | sgn_x,
|  | v64uint8 | b,
|  | int | sgn_y,
|  | v32acc32 | acc1,
|  | v32acc32 | acc2,
|  | int | zero_acc1,
|  | int | sub_mul,
|  | int | sub_acc1,
|  | int | sub_acc2 )

Parameters

  a | Matrix A
  sgn_x | Sign mask for matrix A
  b | Matrix B
  sgn_y | Sign mask for matrix B
  acc1 | Accumulator 1 input
  acc2 | Accumulator 2 input
  zero_acc1 | Zeroing mask for acc1
  sub_mul | Negation mask of multiplication result.
  sub_acc1 | Negation mask of acc1
  sub_acc2 | Negation mask of acc2

Returns
  Result of operation

## ◆ submsc_4x8_8x8_conf() [7/8]

v32acc32 submsc_4x8_8x8_conf | ( | v64uint8 | a,
|  | v64int8 | b,
|  | v32acc32 | acc1,
|  | v32acc32 | acc2,
|  | int | zero_acc1,
|  | int | sub_mul,
|  | int | sub_acc1,
|  | int | sub_acc2 )

Parameters

  a | Matrix A
  b | Matrix B
  acc1 | Accumulator 1 input
  acc2 | Accumulator 2 input
  zero_acc1 | Zeroing mask for acc1
  sub_mul | Negation mask of multiplication result
  sub_acc1 | Negation mask of acc1
  sub_acc2 | Negation mask of acc2

Returns
  Result of operation

## ◆ submsc_4x8_8x8_conf() [8/8]

v32acc32 submsc_4x8_8x8_conf | ( | v64uint8 | a,
|  | v64uint8 | b,
|  | v32acc32 | acc1,
|  | v32acc32 | acc2,
|  | int | zero_acc1,
|  | int | sub_mul,
|  | int | sub_acc1,
|  | int | sub_acc2 )

Parameters

  a | Matrix A
  b | Matrix B
  acc1 | Accumulator 1 input
  acc2 | Accumulator 2 input
  zero_acc1 | Zeroing mask for acc1
  sub_mul | Negation mask of multiplication result
  sub_acc1 | Negation mask of acc1
  sub_acc2 | Negation mask of acc2

Returns
  Result of operation

## ◆ submsc_conv_32x8() [1/8]

v32acc32 submsc_conv_32x8 | ( | v64int8 | a,
|  | int | sgn_x,
|  | v64int8 | b,
|  | int | sgn_y,
|  | v32acc32 | acc1,
|  | v32acc32 | acc2 )

Parameters

  a | Matrix A
  sgn_x | Sign mask for matrix A
  b | Matrix B
  sgn_y | Sign mask for matrix B
  acc1 | Accumulator 1 input
  acc2 | Accumulator 2 input

Returns
  Result of operation

## ◆ submsc_conv_32x8() [2/8]

v32acc32 submsc_conv_32x8 | ( | v64int8 | a,
|  | int | sgn_x,
|  | v64uint8 | b,
|  | int | sgn_y,
|  | v32acc32 | acc1,
|  | v32acc32 | acc2 )

Parameters

  a | Matrix A
  sgn_x | Sign mask for matrix A
  b | Matrix B
  sgn_y | Sign mask for matrix B
  acc1 | Accumulator 1 input
  acc2 | Accumulator 2 input

Returns
  Result of operation

## ◆ submsc_conv_32x8() [3/8]

v32acc32 submsc_conv_32x8 | ( | v64int8 | a,
|  | v64int8 | b,
|  | v32acc32 | acc1,
|  | v32acc32 | acc2 )

Parameters

  a | Matrix A
  b | Matrix B
  acc1 | Accumulator 1 input
  acc2 | Accumulator 2 input

Returns
  Result of operation

## ◆ submsc_conv_32x8() [4/8]

v32acc32 submsc_conv_32x8 | ( | v64int8 | a,
|  | v64uint8 | b,
|  | v32acc32 | acc1,
|  | v32acc32 | acc2 )

Parameters

  a | Matrix A
  b | Matrix B
  acc1 | Accumulator 1 input
  acc2 | Accumulator 2 input

Returns
  Result of operation

## ◆ submsc_conv_32x8() [5/8]

v32acc32 submsc_conv_32x8 | ( | v64uint8 | a,
|  | int | sgn_x,
|  | v64int8 | b,
|  | int | sgn_y,
|  | v32acc32 | acc1,
|  | v32acc32 | acc2 )

Parameters

  a | Matrix A
  sgn_x | Sign mask for matrix A
  b | Matrix B
  sgn_y | Sign mask for matrix B
  acc1 | Accumulator 1 input
  acc2 | Accumulator 2 input

Returns
  Result of operation

## ◆ submsc_conv_32x8() [6/8]

v32acc32 submsc_conv_32x8 | ( | v64uint8 | a,
|  | int | sgn_x,
|  | v64uint8 | b,
|  | int | sgn_y,
|  | v32acc32 | acc1,
|  | v32acc32 | acc2 )

Parameters

  a | Matrix A
  sgn_x | Sign mask for matrix A
  b | Matrix B
  sgn_y | Sign mask for matrix B
  acc1 | Accumulator 1 input
  acc2 | Accumulator 2 input

Returns
  Result of operation

## ◆ submsc_conv_32x8() [7/8]

v32acc32 submsc_conv_32x8 | ( | v64uint8 | a,
|  | v64int8 | b,
|  | v32acc32 | acc1,
|  | v32acc32 | acc2 )

Parameters

  a | Matrix A
  b | Matrix B
  acc1 | Accumulator 1 input
  acc2 | Accumulator 2 input

Returns
  Result of operation

## ◆ submsc_conv_32x8() [8/8]

v32acc32 submsc_conv_32x8 | ( | v64uint8 | a,
|  | v64uint8 | b,
|  | v32acc32 | acc1,
|  | v32acc32 | acc2 )

Parameters

  a | Matrix A
  b | Matrix B
  acc1 | Accumulator 1 input
  acc2 | Accumulator 2 input

Returns
  Result of operation

## ◆ submsc_conv_32x8_conf() [1/8]

v32acc32 submsc_conv_32x8_conf | ( | v64int8 | a,
|  | int | sgn_x,
|  | v64int8 | b,
|  | int | sgn_y,
|  | v32acc32 | acc1,
|  | v32acc32 | acc2,
|  | int | zero_acc1,
|  | int | sub_mul,
|  | int | sub_acc1,
|  | int | sub_acc2 )

Parameters

  a | Matrix A
  sgn_x | Sign mask for matrix A
  b | Matrix B
  sgn_y | Sign mask for matrix B
  acc1 | Accumulator 1 input
  acc2 | Accumulator 2 input
  zero_acc1 | Zeroing mask for acc1
  sub_mul | Negation mask of multiplication result.
  sub_acc1 | Negation mask of acc1
  sub_acc2 | Negation mask of acc2

Returns
  Result of operation

## ◆ submsc_conv_32x8_conf() [2/8]

v32acc32 submsc_conv_32x8_conf | ( | v64int8 | a,
|  | int | sgn_x,
|  | v64uint8 | b,
|  | int | sgn_y,
|  | v32acc32 | acc1,
|  | v32acc32 | acc2,
|  | int | zero_acc1,
|  | int | sub_mul,
|  | int | sub_acc1,
|  | int | sub_acc2 )

Parameters

  a | Matrix A
  sgn_x | Sign mask for matrix A
  b | Matrix B
  sgn_y | Sign mask for matrix B
  acc1 | Accumulator 1 input
  acc2 | Accumulator 2 input
  zero_acc1 | Zeroing mask for acc1
  sub_mul | Negation mask of multiplication result.
  sub_acc1 | Negation mask of acc1
  sub_acc2 | Negation mask of acc2

Returns
  Result of operation

## ◆ submsc_conv_32x8_conf() [3/8]

v32acc32 submsc_conv_32x8_conf | ( | v64int8 | a,
|  | v64int8 | b,
|  | v32acc32 | acc1,
|  | v32acc32 | acc2,
|  | int | zero_acc1,
|  | int | sub_mul,
|  | int | sub_acc1,
|  | int | sub_acc2 )

Parameters

  a | Matrix A
  b | Matrix B
  acc1 | Accumulator 1 input
  acc2 | Accumulator 2 input
  zero_acc1 | Zeroing mask for acc1
  sub_mul | Negation mask of multiplication result
  sub_acc1 | Negation mask of acc1
  sub_acc2 | Negation mask of acc2

Returns
  Result of operation

## ◆ submsc_conv_32x8_conf() [4/8]

v32acc32 submsc_conv_32x8_conf | ( | v64int8 | a,
|  | v64uint8 | b,
|  | v32acc32 | acc1,
|  | v32acc32 | acc2,
|  | int | zero_acc1,
|  | int | sub_mul,
|  | int | sub_acc1,
|  | int | sub_acc2 )

Parameters

  a | Matrix A
  b | Matrix B
  acc1 | Accumulator 1 input
  acc2 | Accumulator 2 input
  zero_acc1 | Zeroing mask for acc1
  sub_mul | Negation mask of multiplication result
  sub_acc1 | Negation mask of acc1
  sub_acc2 | Negation mask of acc2

Returns
  Result of operation

## ◆ submsc_conv_32x8_conf() [5/8]

v32acc32 submsc_conv_32x8_conf | ( | v64uint8 | a,
|  | int | sgn_x,
|  | v64int8 | b,
|  | int | sgn_y,
|  | v32acc32 | acc1,
|  | v32acc32 | acc2,
|  | int | zero_acc1,
|  | int | sub_mul,
|  | int | sub_acc1,
|  | int | sub_acc2 )

Parameters

  a | Matrix A
  sgn_x | Sign mask for matrix A
  b | Matrix B
  sgn_y | Sign mask for matrix B
  acc1 | Accumulator 1 input
  acc2 | Accumulator 2 input
  zero_acc1 | Zeroing mask for acc1
  sub_mul | Negation mask of multiplication result.
  sub_acc1 | Negation mask of acc1
  sub_acc2 | Negation mask of acc2

Returns
  Result of operation

## ◆ submsc_conv_32x8_conf() [6/8]

v32acc32 submsc_conv_32x8_conf | ( | v64uint8 | a,
|  | int | sgn_x,
|  | v64uint8 | b,
|  | int | sgn_y,
|  | v32acc32 | acc1,
|  | v32acc32 | acc2,
|  | int | zero_acc1,
|  | int | sub_mul,
|  | int | sub_acc1,
|  | int | sub_acc2 )

Parameters

  a | Matrix A
  sgn_x | Sign mask for matrix A
  b | Matrix B
  sgn_y | Sign mask for matrix B
  acc1 | Accumulator 1 input
  acc2 | Accumulator 2 input
  zero_acc1 | Zeroing mask for acc1
  sub_mul | Negation mask of multiplication result.
  sub_acc1 | Negation mask of acc1
  sub_acc2 | Negation mask of acc2

Returns
  Result of operation

## ◆ submsc_conv_32x8_conf() [7/8]

v32acc32 submsc_conv_32x8_conf | ( | v64uint8 | a,
|  | v64int8 | b,
|  | v32acc32 | acc1,
|  | v32acc32 | acc2,
|  | int | zero_acc1,
|  | int | sub_mul,
|  | int | sub_acc1,
|  | int | sub_acc2 )

Parameters

  a | Matrix A
  b | Matrix B
  acc1 | Accumulator 1 input
  acc2 | Accumulator 2 input
  zero_acc1 | Zeroing mask for acc1
  sub_mul | Negation mask of multiplication result
  sub_acc1 | Negation mask of acc1
  sub_acc2 | Negation mask of acc2

Returns
  Result of operation

## ◆ submsc_conv_32x8_conf() [8/8]

v32acc32 submsc_conv_32x8_conf | ( | v64uint8 | a,
|  | v64uint8 | b,
|  | v32acc32 | acc1,
|  | v32acc32 | acc2,
|  | int | zero_acc1,
|  | int | sub_mul,
|  | int | sub_acc1,
|  | int | sub_acc2 )

Parameters

  a | Matrix A
  b | Matrix B
  acc1 | Accumulator 1 input
  acc2 | Accumulator 2 input
  zero_acc1 | Zeroing mask for acc1
  sub_mul | Negation mask of multiplication result
  sub_acc1 | Negation mask of acc1
  sub_acc2 | Negation mask of acc2

Returns
  Result of operation

## ◆ submsc_conv_4x4_8ch() [1/8]

v32acc32 submsc_conv_4x4_8ch | ( | v64int8 | a,
|  | int | sgn_x,
|  | v64int8 | b,
|  | int | sgn_y,
|  | v32acc32 | acc1,
|  | v32acc32 | acc2 )

Parameters

  a | Matrix A
  sgn_x | Sign mask for matrix A
  b | Matrix B
  sgn_y | Sign mask for matrix B
  acc1 | Accumulator 1 input
  acc2 | Accumulator 2 input

Returns
  Result of operation

## ◆ submsc_conv_4x4_8ch() [2/8]

v32acc32 submsc_conv_4x4_8ch | ( | v64int8 | a,
|  | int | sgn_x,
|  | v64uint8 | b,
|  | int | sgn_y,
|  | v32acc32 | acc1,
|  | v32acc32 | acc2 )

Parameters

  a | Matrix A
  sgn_x | Sign mask for matrix A
  b | Matrix B
  sgn_y | Sign mask for matrix B
  acc1 | Accumulator 1 input
  acc2 | Accumulator 2 input

Returns
  Result of operation

## ◆ submsc_conv_4x4_8ch() [3/8]

v32acc32 submsc_conv_4x4_8ch | ( | v64int8 | a,
|  | v64int8 | b,
|  | v32acc32 | acc1,
|  | v32acc32 | acc2 )

Parameters

  a | Matrix A
  b | Matrix B
  acc1 | Accumulator 1 input
  acc2 | Accumulator 2 input

Returns
  Result of operation

## ◆ submsc_conv_4x4_8ch() [4/8]

v32acc32 submsc_conv_4x4_8ch | ( | v64int8 | a,
|  | v64uint8 | b,
|  | v32acc32 | acc1,
|  | v32acc32 | acc2 )

Parameters

  a | Matrix A
  b | Matrix B
  acc1 | Accumulator 1 input
  acc2 | Accumulator 2 input

Returns
  Result of operation

## ◆ submsc_conv_4x4_8ch() [5/8]

v32acc32 submsc_conv_4x4_8ch | ( | v64uint8 | a,
|  | int | sgn_x,
|  | v64int8 | b,
|  | int | sgn_y,
|  | v32acc32 | acc1,
|  | v32acc32 | acc2 )

Parameters

  a | Matrix A
  sgn_x | Sign mask for matrix A
  b | Matrix B
  sgn_y | Sign mask for matrix B
  acc1 | Accumulator 1 input
  acc2 | Accumulator 2 input

Returns
  Result of operation

## ◆ submsc_conv_4x4_8ch() [6/8]

v32acc32 submsc_conv_4x4_8ch | ( | v64uint8 | a,
|  | int | sgn_x,
|  | v64uint8 | b,
|  | int | sgn_y,
|  | v32acc32 | acc1,
|  | v32acc32 | acc2 )

Parameters

  a | Matrix A
  sgn_x | Sign mask for matrix A
  b | Matrix B
  sgn_y | Sign mask for matrix B
  acc1 | Accumulator 1 input
  acc2 | Accumulator 2 input

Returns
  Result of operation

## ◆ submsc_conv_4x4_8ch() [7/8]

v32acc32 submsc_conv_4x4_8ch | ( | v64uint8 | a,
|  | v64int8 | b,
|  | v32acc32 | acc1,
|  | v32acc32 | acc2 )

Parameters

  a | Matrix A
  b | Matrix B
  acc1 | Accumulator 1 input
  acc2 | Accumulator 2 input

Returns
  Result of operation

## ◆ submsc_conv_4x4_8ch() [8/8]

v32acc32 submsc_conv_4x4_8ch | ( | v64uint8 | a,
|  | v64uint8 | b,
|  | v32acc32 | acc1,
|  | v32acc32 | acc2 )

Parameters

  a | Matrix A
  b | Matrix B
  acc1 | Accumulator 1 input
  acc2 | Accumulator 2 input

Returns
  Result of operation

## ◆ submsc_conv_4x4_8ch_conf() [1/8]

v32acc32 submsc_conv_4x4_8ch_conf | ( | v64int8 | a,
|  | int | sgn_x,
|  | v64int8 | b,
|  | int | sgn_y,
|  | v32acc32 | acc1,
|  | v32acc32 | acc2,
|  | int | zero_acc1,
|  | int | sub_mul,
|  | int | sub_acc1,
|  | int | sub_acc2 )

Parameters

  a | Matrix A
  sgn_x | Sign mask for matrix A
  b | Matrix B
  sgn_y | Sign mask for matrix B
  acc1 | Accumulator 1 input
  acc2 | Accumulator 2 input
  zero_acc1 | Zeroing mask for acc1
  sub_mul | Negation mask of multiplication result.
  sub_acc1 | Negation mask of acc1
  sub_acc2 | Negation mask of acc2

Returns
  Result of operation

## ◆ submsc_conv_4x4_8ch_conf() [2/8]

v32acc32 submsc_conv_4x4_8ch_conf | ( | v64int8 | a,
|  | int | sgn_x,
|  | v64uint8 | b,
|  | int | sgn_y,
|  | v32acc32 | acc1,
|  | v32acc32 | acc2,
|  | int | zero_acc1,
|  | int | sub_mul,
|  | int | sub_acc1,
|  | int | sub_acc2 )

Parameters

  a | Matrix A
  sgn_x | Sign mask for matrix A
  b | Matrix B
  sgn_y | Sign mask for matrix B
  acc1 | Accumulator 1 input
  acc2 | Accumulator 2 input
  zero_acc1 | Zeroing mask for acc1
  sub_mul | Negation mask of multiplication result.
  sub_acc1 | Negation mask of acc1
  sub_acc2 | Negation mask of acc2

Returns
  Result of operation

## ◆ submsc_conv_4x4_8ch_conf() [3/8]

v32acc32 submsc_conv_4x4_8ch_conf | ( | v64int8 | a,
|  | v64int8 | b,
|  | v32acc32 | acc1,
|  | v32acc32 | acc2,
|  | int | zero_acc1,
|  | int | sub_mul,
|  | int | sub_acc1,
|  | int | sub_acc2 )

Parameters

  a | Matrix A
  b | Matrix B
  acc1 | Accumulator 1 input
  acc2 | Accumulator 2 input
  zero_acc1 | Zeroing mask for acc1
  sub_mul | Negation mask of multiplication result
  sub_acc1 | Negation mask of acc1
  sub_acc2 | Negation mask of acc2

Returns
  Result of operation

## ◆ submsc_conv_4x4_8ch_conf() [4/8]

v32acc32 submsc_conv_4x4_8ch_conf | ( | v64int8 | a,
|  | v64uint8 | b,
|  | v32acc32 | acc1,
|  | v32acc32 | acc2,
|  | int | zero_acc1,
|  | int | sub_mul,
|  | int | sub_acc1,
|  | int | sub_acc2 )

Parameters

  a | Matrix A
  b | Matrix B
  acc1 | Accumulator 1 input
  acc2 | Accumulator 2 input
  zero_acc1 | Zeroing mask for acc1
  sub_mul | Negation mask of multiplication result
  sub_acc1 | Negation mask of acc1
  sub_acc2 | Negation mask of acc2

Returns
  Result of operation

## ◆ submsc_conv_4x4_8ch_conf() [5/8]

v32acc32 submsc_conv_4x4_8ch_conf | ( | v64uint8 | a,
|  | int | sgn_x,
|  | v64int8 | b,
|  | int | sgn_y,
|  | v32acc32 | acc1,
|  | v32acc32 | acc2,
|  | int | zero_acc1,
|  | int | sub_mul,
|  | int | sub_acc1,
|  | int | sub_acc2 )

Parameters

  a | Matrix A
  sgn_x | Sign mask for matrix A
  b | Matrix B
  sgn_y | Sign mask for matrix B
  acc1 | Accumulator 1 input
  acc2 | Accumulator 2 input
  zero_acc1 | Zeroing mask for acc1
  sub_mul | Negation mask of multiplication result.
  sub_acc1 | Negation mask of acc1
  sub_acc2 | Negation mask of acc2

Returns
  Result of operation

## ◆ submsc_conv_4x4_8ch_conf() [6/8]

v32acc32 submsc_conv_4x4_8ch_conf | ( | v64uint8 | a,
|  | int | sgn_x,
|  | v64uint8 | b,
|  | int | sgn_y,
|  | v32acc32 | acc1,
|  | v32acc32 | acc2,
|  | int | zero_acc1,
|  | int | sub_mul,
|  | int | sub_acc1,
|  | int | sub_acc2 )

Parameters

  a | Matrix A
  sgn_x | Sign mask for matrix A
  b | Matrix B
  sgn_y | Sign mask for matrix B
  acc1 | Accumulator 1 input
  acc2 | Accumulator 2 input
  zero_acc1 | Zeroing mask for acc1
  sub_mul | Negation mask of multiplication result.
  sub_acc1 | Negation mask of acc1
  sub_acc2 | Negation mask of acc2

Returns
  Result of operation

## ◆ submsc_conv_4x4_8ch_conf() [7/8]

v32acc32 submsc_conv_4x4_8ch_conf | ( | v64uint8 | a,
|  | v64int8 | b,
|  | v32acc32 | acc1,
|  | v32acc32 | acc2,
|  | int | zero_acc1,
|  | int | sub_mul,
|  | int | sub_acc1,
|  | int | sub_acc2 )

Parameters

  a | Matrix A
  b | Matrix B
  acc1 | Accumulator 1 input
  acc2 | Accumulator 2 input
  zero_acc1 | Zeroing mask for acc1
  sub_mul | Negation mask of multiplication result
  sub_acc1 | Negation mask of acc1
  sub_acc2 | Negation mask of acc2

Returns
  Result of operation

## ◆ submsc_conv_4x4_8ch_conf() [8/8]

v32acc32 submsc_conv_4x4_8ch_conf | ( | v64uint8 | a,
|  | v64uint8 | b,
|  | v32acc32 | acc1,
|  | v32acc32 | acc2,
|  | int | zero_acc1,
|  | int | sub_mul,
|  | int | sub_acc1,
|  | int | sub_acc2 )

Parameters

  a | Matrix A
  b | Matrix B
  acc1 | Accumulator 1 input
  acc2 | Accumulator 2 input
  zero_acc1 | Zeroing mask for acc1
  sub_mul | Negation mask of multiplication result
  sub_acc1 | Negation mask of acc1
  sub_acc2 | Negation mask of acc2

Returns
  Result of operation

## ◆ submsc_conv_8x8_4ch() [1/8]

v32acc32 submsc_conv_8x8_4ch | ( | v64int8 | a,
|  | int | sgn_x,
|  | v64int8 | b,
|  | int | sgn_y,
|  | v32acc32 | acc1,
|  | v32acc32 | acc2 )

Parameters

  a | Matrix A
  sgn_x | Sign mask for matrix A
  b | Matrix B
  sgn_y | Sign mask for matrix B
  acc1 | Accumulator 1 input
  acc2 | Accumulator 2 input

Returns
  Result of operation

## ◆ submsc_conv_8x8_4ch() [2/8]

v32acc32 submsc_conv_8x8_4ch | ( | v64int8 | a,
|  | int | sgn_x,
|  | v64uint8 | b,
|  | int | sgn_y,
|  | v32acc32 | acc1,
|  | v32acc32 | acc2 )

Parameters

  a | Matrix A
  sgn_x | Sign mask for matrix A
  b | Matrix B
  sgn_y | Sign mask for matrix B
  acc1 | Accumulator 1 input
  acc2 | Accumulator 2 input

Returns
  Result of operation

## ◆ submsc_conv_8x8_4ch() [3/8]

v32acc32 submsc_conv_8x8_4ch | ( | v64int8 | a,
|  | v64int8 | b,
|  | v32acc32 | acc1,
|  | v32acc32 | acc2 )

Parameters

  a | Matrix A
  b | Matrix B
  acc1 | Accumulator 1 input
  acc2 | Accumulator 2 input

Returns
  Result of operation

## ◆ submsc_conv_8x8_4ch() [4/8]

v32acc32 submsc_conv_8x8_4ch | ( | v64int8 | a,
|  | v64uint8 | b,
|  | v32acc32 | acc1,
|  | v32acc32 | acc2 )

Parameters

  a | Matrix A
  b | Matrix B
  acc1 | Accumulator 1 input
  acc2 | Accumulator 2 input

Returns
  Result of operation

## ◆ submsc_conv_8x8_4ch() [5/8]

v32acc32 submsc_conv_8x8_4ch | ( | v64uint8 | a,
|  | int | sgn_x,
|  | v64int8 | b,
|  | int | sgn_y,
|  | v32acc32 | acc1,
|  | v32acc32 | acc2 )

Parameters

  a | Matrix A
  sgn_x | Sign mask for matrix A
  b | Matrix B
  sgn_y | Sign mask for matrix B
  acc1 | Accumulator 1 input
  acc2 | Accumulator 2 input

Returns
  Result of operation

## ◆ submsc_conv_8x8_4ch() [6/8]

v32acc32 submsc_conv_8x8_4ch | ( | v64uint8 | a,
|  | int | sgn_x,
|  | v64uint8 | b,
|  | int | sgn_y,
|  | v32acc32 | acc1,
|  | v32acc32 | acc2 )

Parameters

  a | Matrix A
  sgn_x | Sign mask for matrix A
  b | Matrix B
  sgn_y | Sign mask for matrix B
  acc1 | Accumulator 1 input
  acc2 | Accumulator 2 input

Returns
  Result of operation

## ◆ submsc_conv_8x8_4ch() [7/8]

v32acc32 submsc_conv_8x8_4ch | ( | v64uint8 | a,
|  | v64int8 | b,
|  | v32acc32 | acc1,
|  | v32acc32 | acc2 )

Parameters

  a | Matrix A
  b | Matrix B
  acc1 | Accumulator 1 input
  acc2 | Accumulator 2 input

Returns
  Result of operation

## ◆ submsc_conv_8x8_4ch() [8/8]

v32acc32 submsc_conv_8x8_4ch | ( | v64uint8 | a,
|  | v64uint8 | b,
|  | v32acc32 | acc1,
|  | v32acc32 | acc2 )

Parameters

  a | Matrix A
  b | Matrix B
  acc1 | Accumulator 1 input
  acc2 | Accumulator 2 input

Returns
  Result of operation

## ◆ submsc_conv_8x8_4ch_conf() [1/8]

v32acc32 submsc_conv_8x8_4ch_conf | ( | v64int8 | a,
|  | int | sgn_x,
|  | v64int8 | b,
|  | int | sgn_y,
|  | v32acc32 | acc1,
|  | v32acc32 | acc2,
|  | int | zero_acc1,
|  | int | sub_mul,
|  | int | sub_acc1,
|  | int | sub_acc2 )

Parameters

  a | Matrix A
  sgn_x | Sign mask for matrix A
  b | Matrix B
  sgn_y | Sign mask for matrix B
  acc1 | Accumulator 1 input
  acc2 | Accumulator 2 input
  zero_acc1 | Zeroing mask for acc1
  sub_mul | Negation mask of multiplication result.
  sub_acc1 | Negation mask of acc1
  sub_acc2 | Negation mask of acc2

Returns
  Result of operation

## ◆ submsc_conv_8x8_4ch_conf() [2/8]

v32acc32 submsc_conv_8x8_4ch_conf | ( | v64int8 | a,
|  | int | sgn_x,
|  | v64uint8 | b,
|  | int | sgn_y,
|  | v32acc32 | acc1,
|  | v32acc32 | acc2,
|  | int | zero_acc1,
|  | int | sub_mul,
|  | int | sub_acc1,
|  | int | sub_acc2 )

Parameters

  a | Matrix A
  sgn_x | Sign mask for matrix A
  b | Matrix B
  sgn_y | Sign mask for matrix B
  acc1 | Accumulator 1 input
  acc2 | Accumulator 2 input
  zero_acc1 | Zeroing mask for acc1
  sub_mul | Negation mask of multiplication result.
  sub_acc1 | Negation mask of acc1
  sub_acc2 | Negation mask of acc2

Returns
  Result of operation

## ◆ submsc_conv_8x8_4ch_conf() [3/8]

v32acc32 submsc_conv_8x8_4ch_conf | ( | v64int8 | a,
|  | v64int8 | b,
|  | v32acc32 | acc1,
|  | v32acc32 | acc2,
|  | int | zero_acc1,
|  | int | sub_mul,
|  | int | sub_acc1,
|  | int | sub_acc2 )

Parameters

  a | Matrix A
  b | Matrix B
  acc1 | Accumulator 1 input
  acc2 | Accumulator 2 input
  zero_acc1 | Zeroing mask for acc1
  sub_mul | Negation mask of multiplication result
  sub_acc1 | Negation mask of acc1
  sub_acc2 | Negation mask of acc2

Returns
  Result of operation

## ◆ submsc_conv_8x8_4ch_conf() [4/8]

v32acc32 submsc_conv_8x8_4ch_conf | ( | v64int8 | a,
|  | v64uint8 | b,
|  | v32acc32 | acc1,
|  | v32acc32 | acc2,
|  | int | zero_acc1,
|  | int | sub_mul,
|  | int | sub_acc1,
|  | int | sub_acc2 )

Parameters

  a | Matrix A
  b | Matrix B
  acc1 | Accumulator 1 input
  acc2 | Accumulator 2 input
  zero_acc1 | Zeroing mask for acc1
  sub_mul | Negation mask of multiplication result
  sub_acc1 | Negation mask of acc1
  sub_acc2 | Negation mask of acc2

Returns
  Result of operation

## ◆ submsc_conv_8x8_4ch_conf() [5/8]

v32acc32 submsc_conv_8x8_4ch_conf | ( | v64uint8 | a,
|  | int | sgn_x,
|  | v64int8 | b,
|  | int | sgn_y,
|  | v32acc32 | acc1,
|  | v32acc32 | acc2,
|  | int | zero_acc1,
|  | int | sub_mul,
|  | int | sub_acc1,
|  | int | sub_acc2 )

Parameters

  a | Matrix A
  sgn_x | Sign mask for matrix A
  b | Matrix B
  sgn_y | Sign mask for matrix B
  acc1 | Accumulator 1 input
  acc2 | Accumulator 2 input
  zero_acc1 | Zeroing mask for acc1
  sub_mul | Negation mask of multiplication result.
  sub_acc1 | Negation mask of acc1
  sub_acc2 | Negation mask of acc2

Returns
  Result of operation

## ◆ submsc_conv_8x8_4ch_conf() [6/8]

v32acc32 submsc_conv_8x8_4ch_conf | ( | v64uint8 | a,
|  | int | sgn_x,
|  | v64uint8 | b,
|  | int | sgn_y,
|  | v32acc32 | acc1,
|  | v32acc32 | acc2,
|  | int | zero_acc1,
|  | int | sub_mul,
|  | int | sub_acc1,
|  | int | sub_acc2 )

Parameters

  a | Matrix A
  sgn_x | Sign mask for matrix A
  b | Matrix B
  sgn_y | Sign mask for matrix B
  acc1 | Accumulator 1 input
  acc2 | Accumulator 2 input
  zero_acc1 | Zeroing mask for acc1
  sub_mul | Negation mask of multiplication result.
  sub_acc1 | Negation mask of acc1
  sub_acc2 | Negation mask of acc2

Returns
  Result of operation

## ◆ submsc_conv_8x8_4ch_conf() [7/8]

v32acc32 submsc_conv_8x8_4ch_conf | ( | v64uint8 | a,
|  | v64int8 | b,
|  | v32acc32 | acc1,
|  | v32acc32 | acc2,
|  | int | zero_acc1,
|  | int | sub_mul,
|  | int | sub_acc1,
|  | int | sub_acc2 )

Parameters

  a | Matrix A
  b | Matrix B
  acc1 | Accumulator 1 input
  acc2 | Accumulator 2 input
  zero_acc1 | Zeroing mask for acc1
  sub_mul | Negation mask of multiplication result
  sub_acc1 | Negation mask of acc1
  sub_acc2 | Negation mask of acc2

Returns
  Result of operation

## ◆ submsc_conv_8x8_4ch_conf() [8/8]

v32acc32 submsc_conv_8x8_4ch_conf | ( | v64uint8 | a,
|  | v64uint8 | b,
|  | v32acc32 | acc1,
|  | v32acc32 | acc2,
|  | int | zero_acc1,
|  | int | sub_mul,
|  | int | sub_acc1,
|  | int | sub_acc2 )

Parameters

  a | Matrix A
  b | Matrix B
  acc1 | Accumulator 1 input
  acc2 | Accumulator 2 input
  zero_acc1 | Zeroing mask for acc1
  sub_mul | Negation mask of multiplication result
  sub_acc1 | Negation mask of acc1
  sub_acc2 | Negation mask of acc2

Returns
  Result of operation

## ◆ submsc_elem_32_2() [1/8]

v32acc32 submsc_elem_32_2 | ( | v64int8 | a,
|  | int | sgn_x,
|  | v64int8 | b,
|  | int | sgn_y,
|  | v32acc32 | acc1,
|  | v32acc32 | acc2 )

Parameters

  a | Matrix A
  sgn_x | Sign mask for matrix A
  b | Matrix B
  sgn_y | Sign mask for matrix B
  acc1 | Accumulator 1 input
  acc2 | Accumulator 2 input

Returns
  Result of operation

## ◆ submsc_elem_32_2() [2/8]

v32acc32 submsc_elem_32_2 | ( | v64int8 | a,
|  | int | sgn_x,
|  | v64uint8 | b,
|  | int | sgn_y,
|  | v32acc32 | acc1,
|  | v32acc32 | acc2 )

Parameters

  a | Matrix A
  sgn_x | Sign mask for matrix A
  b | Matrix B
  sgn_y | Sign mask for matrix B
  acc1 | Accumulator 1 input
  acc2 | Accumulator 2 input

Returns
  Result of operation

## ◆ submsc_elem_32_2() [3/8]

v32acc32 submsc_elem_32_2 | ( | v64int8 | a,
|  | v64int8 | b,
|  | v32acc32 | acc1,
|  | v32acc32 | acc2 )

Parameters

  a | Matrix A
  b | Matrix B
  acc1 | Accumulator 1 input
  acc2 | Accumulator 2 input

Returns
  Result of operation

## ◆ submsc_elem_32_2() [4/8]

v32acc32 submsc_elem_32_2 | ( | v64int8 | a,
|  | v64uint8 | b,
|  | v32acc32 | acc1,
|  | v32acc32 | acc2 )

Parameters

  a | Matrix A
  b | Matrix B
  acc1 | Accumulator 1 input
  acc2 | Accumulator 2 input

Returns
  Result of operation

## ◆ submsc_elem_32_2() [5/8]

v32acc32 submsc_elem_32_2 | ( | v64uint8 | a,
|  | int | sgn_x,
|  | v64int8 | b,
|  | int | sgn_y,
|  | v32acc32 | acc1,
|  | v32acc32 | acc2 )

Parameters

  a | Matrix A
  sgn_x | Sign mask for matrix A
  b | Matrix B
  sgn_y | Sign mask for matrix B
  acc1 | Accumulator 1 input
  acc2 | Accumulator 2 input

Returns
  Result of operation

## ◆ submsc_elem_32_2() [6/8]

v32acc32 submsc_elem_32_2 | ( | v64uint8 | a,
|  | int | sgn_x,
|  | v64uint8 | b,
|  | int | sgn_y,
|  | v32acc32 | acc1,
|  | v32acc32 | acc2 )

Parameters

  a | Matrix A
  sgn_x | Sign mask for matrix A
  b | Matrix B
  sgn_y | Sign mask for matrix B
  acc1 | Accumulator 1 input
  acc2 | Accumulator 2 input

Returns
  Result of operation

## ◆ submsc_elem_32_2() [7/8]

v32acc32 submsc_elem_32_2 | ( | v64uint8 | a,
|  | v64int8 | b,
|  | v32acc32 | acc1,
|  | v32acc32 | acc2 )

Parameters

  a | Matrix A
  b | Matrix B
  acc1 | Accumulator 1 input
  acc2 | Accumulator 2 input

Returns
  Result of operation

## ◆ submsc_elem_32_2() [8/8]

v32acc32 submsc_elem_32_2 | ( | v64uint8 | a,
|  | v64uint8 | b,
|  | v32acc32 | acc1,
|  | v32acc32 | acc2 )

Parameters

  a | Matrix A
  b | Matrix B
  acc1 | Accumulator 1 input
  acc2 | Accumulator 2 input

Returns
  Result of operation

## ◆ submsc_elem_32_2_conf() [1/8]

v32acc32 submsc_elem_32_2_conf | ( | v64int8 | a,
|  | int | sgn_x,
|  | v64int8 | b,
|  | int | sgn_y,
|  | v32acc32 | acc1,
|  | v32acc32 | acc2,
|  | int | zero_acc1,
|  | int | sub_mul,
|  | int | sub_acc1,
|  | int | sub_acc2 )

Parameters

  a | Matrix A
  sgn_x | Sign mask for matrix A
  b | Matrix B
  sgn_y | Sign mask for matrix B
  acc1 | Accumulator 1 input
  acc2 | Accumulator 2 input
  zero_acc1 | Zeroing mask for acc1
  sub_mul | Negation mask of multiplication result.
  sub_acc1 | Negation mask of acc1
  sub_acc2 | Negation mask of acc2

Returns
  Result of operation

## ◆ submsc_elem_32_2_conf() [2/8]

v32acc32 submsc_elem_32_2_conf | ( | v64int8 | a,
|  | int | sgn_x,
|  | v64uint8 | b,
|  | int | sgn_y,
|  | v32acc32 | acc1,
|  | v32acc32 | acc2,
|  | int | zero_acc1,
|  | int | sub_mul,
|  | int | sub_acc1,
|  | int | sub_acc2 )

Parameters

  a | Matrix A
  sgn_x | Sign mask for matrix A
  b | Matrix B
  sgn_y | Sign mask for matrix B
  acc1 | Accumulator 1 input
  acc2 | Accumulator 2 input
  zero_acc1 | Zeroing mask for acc1
  sub_mul | Negation mask of multiplication result.
  sub_acc1 | Negation mask of acc1
  sub_acc2 | Negation mask of acc2

Returns
  Result of operation

## ◆ submsc_elem_32_2_conf() [3/8]

v32acc32 submsc_elem_32_2_conf | ( | v64int8 | a,
|  | v64int8 | b,
|  | v32acc32 | acc1,
|  | v32acc32 | acc2,
|  | int | zero_acc1,
|  | int | sub_mul,
|  | int | sub_acc1,
|  | int | sub_acc2 )

Parameters

  a | Matrix A
  b | Matrix B
  acc1 | Accumulator 1 input
  acc2 | Accumulator 2 input
  zero_acc1 | Zeroing mask for acc1
  sub_mul | Negation mask of multiplication result
  sub_acc1 | Negation mask of acc1
  sub_acc2 | Negation mask of acc2

Returns
  Result of operation

## ◆ submsc_elem_32_2_conf() [4/8]

v32acc32 submsc_elem_32_2_conf | ( | v64int8 | a,
|  | v64uint8 | b,
|  | v32acc32 | acc1,
|  | v32acc32 | acc2,
|  | int | zero_acc1,
|  | int | sub_mul,
|  | int | sub_acc1,
|  | int | sub_acc2 )

Parameters

  a | Matrix A
  b | Matrix B
  acc1 | Accumulator 1 input
  acc2 | Accumulator 2 input
  zero_acc1 | Zeroing mask for acc1
  sub_mul | Negation mask of multiplication result
  sub_acc1 | Negation mask of acc1
  sub_acc2 | Negation mask of acc2

Returns
  Result of operation

## ◆ submsc_elem_32_2_conf() [5/8]

v32acc32 submsc_elem_32_2_conf | ( | v64uint8 | a,
|  | int | sgn_x,
|  | v64int8 | b,
|  | int | sgn_y,
|  | v32acc32 | acc1,
|  | v32acc32 | acc2,
|  | int | zero_acc1,
|  | int | sub_mul,
|  | int | sub_acc1,
|  | int | sub_acc2 )

Parameters

  a | Matrix A
  sgn_x | Sign mask for matrix A
  b | Matrix B
  sgn_y | Sign mask for matrix B
  acc1 | Accumulator 1 input
  acc2 | Accumulator 2 input
  zero_acc1 | Zeroing mask for acc1
  sub_mul | Negation mask of multiplication result.
  sub_acc1 | Negation mask of acc1
  sub_acc2 | Negation mask of acc2

Returns
  Result of operation

## ◆ submsc_elem_32_2_conf() [6/8]

v32acc32 submsc_elem_32_2_conf | ( | v64uint8 | a,
|  | int | sgn_x,
|  | v64uint8 | b,
|  | int | sgn_y,
|  | v32acc32 | acc1,
|  | v32acc32 | acc2,
|  | int | zero_acc1,
|  | int | sub_mul,
|  | int | sub_acc1,
|  | int | sub_acc2 )

Parameters

  a | Matrix A
  sgn_x | Sign mask for matrix A
  b | Matrix B
  sgn_y | Sign mask for matrix B
  acc1 | Accumulator 1 input
  acc2 | Accumulator 2 input
  zero_acc1 | Zeroing mask for acc1
  sub_mul | Negation mask of multiplication result.
  sub_acc1 | Negation mask of acc1
  sub_acc2 | Negation mask of acc2

Returns
  Result of operation

## ◆ submsc_elem_32_2_conf() [7/8]

v32acc32 submsc_elem_32_2_conf | ( | v64uint8 | a,
|  | v64int8 | b,
|  | v32acc32 | acc1,
|  | v32acc32 | acc2,
|  | int | zero_acc1,
|  | int | sub_mul,
|  | int | sub_acc1,
|  | int | sub_acc2 )

Parameters

  a | Matrix A
  b | Matrix B
  acc1 | Accumulator 1 input
  acc2 | Accumulator 2 input
  zero_acc1 | Zeroing mask for acc1
  sub_mul | Negation mask of multiplication result
  sub_acc1 | Negation mask of acc1
  sub_acc2 | Negation mask of acc2

Returns
  Result of operation

## ◆ submsc_elem_32_2_conf() [8/8]

v32acc32 submsc_elem_32_2_conf | ( | v64uint8 | a,
|  | v64uint8 | b,
|  | v32acc32 | acc1,
|  | v32acc32 | acc2,
|  | int | zero_acc1,
|  | int | sub_mul,
|  | int | sub_acc1,
|  | int | sub_acc2 )

Parameters

  a | Matrix A
  b | Matrix B
  acc1 | Accumulator 1 input
  acc2 | Accumulator 2 input
  zero_acc1 | Zeroing mask for acc1
  sub_mul | Negation mask of multiplication result
  sub_acc1 | Negation mask of acc1
  sub_acc2 | Negation mask of acc2

Returns
  Result of operation