| AI Engine-ML Intrinsics User Guide (v2025.2)

Loading...
Searching...
No Matches
Multiply-accumulate of 8b x 4b datatypes
Vector Operations » Multiply Accumulate

## Overview

Matrix multiplications in which matrix A has data elements of 8 bit and matrix B has data elements of 4 bit. These operations are emulated on top of int8 x int8.

For an explanation how these operations works see Multiply Accumulate.

## 4x16_16x8
v32acc32 | mul_4x16_16x8 (v64int8 a, v128int4 b)
v32acc32 | negmul_4x16_16x8 (v64int8 a, v128int4 b)
v32acc32 | mac_4x16_16x8 (v64int8 a, v128int4 b, v32acc32 acc)
v32acc32 | msc_4x16_16x8 (v64int8 a, v128int4 b, v32acc32 acc)
v32acc32 | negmac_4x16_16x8 (v64int8 a, v128int4 b, v32acc32 acc)
v32acc32 | negmsc_4x16_16x8 (v64int8 a, v128int4 b, v32acc32 acc)
v32acc32 | addmac_4x16_16x8 (v64int8 a, v128int4 b, v32acc32 acc1, v32acc32 acc2)
v32acc32 | addmsc_4x16_16x8 (v64int8 a, v128int4 b, v32acc32 acc1, v32acc32 acc2)
v32acc32 | submac_4x16_16x8 (v64int8 a, v128int4 b, v32acc32 acc1, v32acc32 acc2)
v32acc32 | submsc_4x16_16x8 (v64int8 a, v128int4 b, v32acc32 acc1, v32acc32 acc2)
v32acc32 | mul_4x16_16x8 (v64int8 a, v128uint4 b)
v32acc32 | negmul_4x16_16x8 (v64int8 a, v128uint4 b)
v32acc32 | mac_4x16_16x8 (v64int8 a, v128uint4 b, v32acc32 acc)
v32acc32 | msc_4x16_16x8 (v64int8 a, v128uint4 b, v32acc32 acc)
v32acc32 | negmac_4x16_16x8 (v64int8 a, v128uint4 b, v32acc32 acc)
v32acc32 | negmsc_4x16_16x8 (v64int8 a, v128uint4 b, v32acc32 acc)
v32acc32 | addmac_4x16_16x8 (v64int8 a, v128uint4 b, v32acc32 acc1, v32acc32 acc2)
v32acc32 | addmsc_4x16_16x8 (v64int8 a, v128uint4 b, v32acc32 acc1, v32acc32 acc2)
v32acc32 | submac_4x16_16x8 (v64int8 a, v128uint4 b, v32acc32 acc1, v32acc32 acc2)
v32acc32 | submsc_4x16_16x8 (v64int8 a, v128uint4 b, v32acc32 acc1, v32acc32 acc2)
v32acc32 | mul_4x16_16x8 (v64uint8 a, v128uint4 b)
v32acc32 | negmul_4x16_16x8 (v64uint8 a, v128uint4 b)
v32acc32 | mac_4x16_16x8 (v64uint8 a, v128uint4 b, v32acc32 acc)
v32acc32 | msc_4x16_16x8 (v64uint8 a, v128uint4 b, v32acc32 acc)
v32acc32 | negmac_4x16_16x8 (v64uint8 a, v128uint4 b, v32acc32 acc)
v32acc32 | negmsc_4x16_16x8 (v64uint8 a, v128uint4 b, v32acc32 acc)
v32acc32 | addmac_4x16_16x8 (v64uint8 a, v128uint4 b, v32acc32 acc1, v32acc32 acc2)
v32acc32 | addmsc_4x16_16x8 (v64uint8 a, v128uint4 b, v32acc32 acc1, v32acc32 acc2)
v32acc32 | submac_4x16_16x8 (v64uint8 a, v128uint4 b, v32acc32 acc1, v32acc32 acc2)
v32acc32 | submsc_4x16_16x8 (v64uint8 a, v128uint4 b, v32acc32 acc1, v32acc32 acc2)
v32acc32 | mul_4x16_16x8 (v64uint8 a, v128int4 b)
v32acc32 | negmul_4x16_16x8 (v64uint8 a, v128int4 b)
v32acc32 | mac_4x16_16x8 (v64uint8 a, v128int4 b, v32acc32 acc)
v32acc32 | msc_4x16_16x8 (v64uint8 a, v128int4 b, v32acc32 acc)
v32acc32 | negmac_4x16_16x8 (v64uint8 a, v128int4 b, v32acc32 acc)
v32acc32 | negmsc_4x16_16x8 (v64uint8 a, v128int4 b, v32acc32 acc)
v32acc32 | addmac_4x16_16x8 (v64uint8 a, v128int4 b, v32acc32 acc1, v32acc32 acc2)
v32acc32 | addmsc_4x16_16x8 (v64uint8 a, v128int4 b, v32acc32 acc1, v32acc32 acc2)
v32acc32 | submac_4x16_16x8 (v64uint8 a, v128int4 b, v32acc32 acc1, v32acc32 acc2)
v32acc32 | submsc_4x16_16x8 (v64uint8 a, v128int4 b, v32acc32 acc1, v32acc32 acc2)

## 4x16_16x8 with dynamic sign
v32acc32 | mul_4x16_16x8 (v64int8 a, int sgn_x, v128int4 b, int sgn_y)
v32acc32 | negmul_4x16_16x8 (v64int8 a, int sgn_x, v128int4 b, int sgn_y)
v32acc32 | mac_4x16_16x8 (v64int8 a, int sgn_x, v128int4 b, int sgn_y, v32acc32 acc)
v32acc32 | msc_4x16_16x8 (v64int8 a, int sgn_x, v128int4 b, int sgn_y, v32acc32 acc)
v32acc32 | negmac_4x16_16x8 (v64int8 a, int sgn_x, v128int4 b, int sgn_y, v32acc32 acc)
v32acc32 | negmsc_4x16_16x8 (v64int8 a, int sgn_x, v128int4 b, int sgn_y, v32acc32 acc)
v32acc32 | addmac_4x16_16x8 (v64int8 a, int sgn_x, v128int4 b, int sgn_y, v32acc32 acc1, v32acc32 acc2)
v32acc32 | addmsc_4x16_16x8 (v64int8 a, int sgn_x, v128int4 b, int sgn_y, v32acc32 acc1, v32acc32 acc2)
v32acc32 | submac_4x16_16x8 (v64int8 a, int sgn_x, v128int4 b, int sgn_y, v32acc32 acc1, v32acc32 acc2)
v32acc32 | submsc_4x16_16x8 (v64int8 a, int sgn_x, v128int4 b, int sgn_y, v32acc32 acc1, v32acc32 acc2)
v32acc32 | mul_4x16_16x8 (v64int8 a, int sgn_x, v128uint4 b, int sgn_y)
v32acc32 | negmul_4x16_16x8 (v64int8 a, int sgn_x, v128uint4 b, int sgn_y)
v32acc32 | mac_4x16_16x8 (v64int8 a, int sgn_x, v128uint4 b, int sgn_y, v32acc32 acc)
v32acc32 | msc_4x16_16x8 (v64int8 a, int sgn_x, v128uint4 b, int sgn_y, v32acc32 acc)
v32acc32 | negmac_4x16_16x8 (v64int8 a, int sgn_x, v128uint4 b, int sgn_y, v32acc32 acc)
v32acc32 | negmsc_4x16_16x8 (v64int8 a, int sgn_x, v128uint4 b, int sgn_y, v32acc32 acc)
v32acc32 | addmac_4x16_16x8 (v64int8 a, int sgn_x, v128uint4 b, int sgn_y, v32acc32 acc1, v32acc32 acc2)
v32acc32 | addmsc_4x16_16x8 (v64int8 a, int sgn_x, v128uint4 b, int sgn_y, v32acc32 acc1, v32acc32 acc2)
v32acc32 | submac_4x16_16x8 (v64int8 a, int sgn_x, v128uint4 b, int sgn_y, v32acc32 acc1, v32acc32 acc2)
v32acc32 | submsc_4x16_16x8 (v64int8 a, int sgn_x, v128uint4 b, int sgn_y, v32acc32 acc1, v32acc32 acc2)
v32acc32 | mul_4x16_16x8 (v64uint8 a, int sgn_x, v128uint4 b, int sgn_y)
v32acc32 | negmul_4x16_16x8 (v64uint8 a, int sgn_x, v128uint4 b, int sgn_y)
v32acc32 | mac_4x16_16x8 (v64uint8 a, int sgn_x, v128uint4 b, int sgn_y, v32acc32 acc)
v32acc32 | msc_4x16_16x8 (v64uint8 a, int sgn_x, v128uint4 b, int sgn_y, v32acc32 acc)
v32acc32 | negmac_4x16_16x8 (v64uint8 a, int sgn_x, v128uint4 b, int sgn_y, v32acc32 acc)
v32acc32 | negmsc_4x16_16x8 (v64uint8 a, int sgn_x, v128uint4 b, int sgn_y, v32acc32 acc)
v32acc32 | addmac_4x16_16x8 (v64uint8 a, int sgn_x, v128uint4 b, int sgn_y, v32acc32 acc1, v32acc32 acc2)
v32acc32 | addmsc_4x16_16x8 (v64uint8 a, int sgn_x, v128uint4 b, int sgn_y, v32acc32 acc1, v32acc32 acc2)
v32acc32 | submac_4x16_16x8 (v64uint8 a, int sgn_x, v128uint4 b, int sgn_y, v32acc32 acc1, v32acc32 acc2)
v32acc32 | submsc_4x16_16x8 (v64uint8 a, int sgn_x, v128uint4 b, int sgn_y, v32acc32 acc1, v32acc32 acc2)
v32acc32 | mul_4x16_16x8 (v64uint8 a, int sgn_x, v128int4 b, int sgn_y)
v32acc32 | negmul_4x16_16x8 (v64uint8 a, int sgn_x, v128int4 b, int sgn_y)
v32acc32 | mac_4x16_16x8 (v64uint8 a, int sgn_x, v128int4 b, int sgn_y, v32acc32 acc)
v32acc32 | msc_4x16_16x8 (v64uint8 a, int sgn_x, v128int4 b, int sgn_y, v32acc32 acc)
v32acc32 | negmac_4x16_16x8 (v64uint8 a, int sgn_x, v128int4 b, int sgn_y, v32acc32 acc)
v32acc32 | negmsc_4x16_16x8 (v64uint8 a, int sgn_x, v128int4 b, int sgn_y, v32acc32 acc)
v32acc32 | addmac_4x16_16x8 (v64uint8 a, int sgn_x, v128int4 b, int sgn_y, v32acc32 acc1, v32acc32 acc2)
v32acc32 | addmsc_4x16_16x8 (v64uint8 a, int sgn_x, v128int4 b, int sgn_y, v32acc32 acc1, v32acc32 acc2)
v32acc32 | submac_4x16_16x8 (v64uint8 a, int sgn_x, v128int4 b, int sgn_y, v32acc32 acc1, v32acc32 acc2)
v32acc32 | submsc_4x16_16x8 (v64uint8 a, int sgn_x, v128int4 b, int sgn_y, v32acc32 acc1, v32acc32 acc2)

## 4x16_16x8 with dynamic negation of multiplication result
v32acc32 | mul_4x16_16x8_conf (v64int8 a, v128int4 b, int sub_mul)
v32acc32 | negmul_4x16_16x8_conf (v64int8 a, v128int4 b, int sub_mul)
v32acc32 | mul_4x16_16x8_conf (v64int8 a, v128uint4 b, int sub_mul)
v32acc32 | negmul_4x16_16x8_conf (v64int8 a, v128uint4 b, int sub_mul)
v32acc32 | mul_4x16_16x8_conf (v64uint8 a, v128uint4 b, int sub_mul)
v32acc32 | negmul_4x16_16x8_conf (v64uint8 a, v128uint4 b, int sub_mul)
v32acc32 | mul_4x16_16x8_conf (v64uint8 a, v128int4 b, int sub_mul)
v32acc32 | negmul_4x16_16x8_conf (v64uint8 a, v128int4 b, int sub_mul)

## 4x16_16x8 with dynamic negation of multiplication result, zeroing of acc1, negation of acc1
v32acc32 | mac_4x16_16x8_conf (v64int8 a, v128int4 b, v32acc32 acc, int zero_acc, int shift16, int sub_mul, int sub_acc1)
v32acc32 | msc_4x16_16x8_conf (v64int8 a, v128int4 b, v32acc32 acc, int zero_acc, int shift16, int sub_mul, int sub_acc1)
v32acc32 | negmsc_4x16_16x8_conf (v64int8 a, v128int4 b, v32acc32 acc, int zero_acc, int sub_mul, int sub_acc1)
v32acc32 | negmac_4x16_16x8_conf (v64int8 a, v128int4 b, v32acc32 acc, int zero_acc, int sub_mul, int sub_acc1)
v32acc32 | addmac_4x16_16x8_conf (v64int8 a, v128int4 b, v32acc32 acc1, v32acc32 acc2, int zero_acc1, int shift16, int sub_mul, int sub_acc1, int sub_acc2)
v32acc32 | addmsc_4x16_16x8_conf (v64int8 a, v128int4 b, v32acc32 acc1, v32acc32 acc2, int zero_acc1, int shift16, int sub_mul, int sub_acc1, int sub_acc2)
v32acc32 | submac_4x16_16x8_conf (v64int8 a, v128int4 b, v32acc32 acc1, v32acc32 acc2, int zero_acc1, int sub_mul, int sub_acc1, int sub_acc2)
v32acc32 | submsc_4x16_16x8_conf (v64int8 a, v128int4 b, v32acc32 acc1, v32acc32 acc2, int zero_acc1, int sub_mul, int sub_acc1, int sub_acc2)
v32acc32 | mac_4x16_16x8_conf (v64int8 a, v128uint4 b, v32acc32 acc, int zero_acc, int shift16, int sub_mul, int sub_acc1)
v32acc32 | msc_4x16_16x8_conf (v64int8 a, v128uint4 b, v32acc32 acc, int zero_acc, int shift16, int sub_mul, int sub_acc1)
v32acc32 | negmsc_4x16_16x8_conf (v64int8 a, v128uint4 b, v32acc32 acc, int zero_acc, int sub_mul, int sub_acc1)
v32acc32 | negmac_4x16_16x8_conf (v64int8 a, v128uint4 b, v32acc32 acc, int zero_acc, int sub_mul, int sub_acc1)
v32acc32 | addmac_4x16_16x8_conf (v64int8 a, v128uint4 b, v32acc32 acc1, v32acc32 acc2, int zero_acc1, int shift16, int sub_mul, int sub_acc1, int sub_acc2)
v32acc32 | addmsc_4x16_16x8_conf (v64int8 a, v128uint4 b, v32acc32 acc1, v32acc32 acc2, int zero_acc1, int shift16, int sub_mul, int sub_acc1, int sub_acc2)
v32acc32 | submac_4x16_16x8_conf (v64int8 a, v128uint4 b, v32acc32 acc1, v32acc32 acc2, int zero_acc1, int sub_mul, int sub_acc1, int sub_acc2)
v32acc32 | submsc_4x16_16x8_conf (v64int8 a, v128uint4 b, v32acc32 acc1, v32acc32 acc2, int zero_acc1, int sub_mul, int sub_acc1, int sub_acc2)
v32acc32 | mac_4x16_16x8_conf (v64uint8 a, v128uint4 b, v32acc32 acc, int zero_acc, int shift16, int sub_mul, int sub_acc1)
v32acc32 | msc_4x16_16x8_conf (v64uint8 a, v128uint4 b, v32acc32 acc, int zero_acc, int shift16, int sub_mul, int sub_acc1)
v32acc32 | negmsc_4x16_16x8_conf (v64uint8 a, v128uint4 b, v32acc32 acc, int zero_acc, int sub_mul, int sub_acc1)
v32acc32 | negmac_4x16_16x8_conf (v64uint8 a, v128uint4 b, v32acc32 acc, int zero_acc, int sub_mul, int sub_acc1)
v32acc32 | addmac_4x16_16x8_conf (v64uint8 a, v128uint4 b, v32acc32 acc1, v32acc32 acc2, int zero_acc1, int shift16, int sub_mul, int sub_acc1, int sub_acc2)
v32acc32 | addmsc_4x16_16x8_conf (v64uint8 a, v128uint4 b, v32acc32 acc1, v32acc32 acc2, int zero_acc1, int shift16, int sub_mul, int sub_acc1, int sub_acc2)
v32acc32 | submac_4x16_16x8_conf (v64uint8 a, v128uint4 b, v32acc32 acc1, v32acc32 acc2, int zero_acc1, int sub_mul, int sub_acc1, int sub_acc2)
v32acc32 | submsc_4x16_16x8_conf (v64uint8 a, v128uint4 b, v32acc32 acc1, v32acc32 acc2, int zero_acc1, int sub_mul, int sub_acc1, int sub_acc2)
v32acc32 | mac_4x16_16x8_conf (v64uint8 a, v128int4 b, v32acc32 acc, int zero_acc, int shift16, int sub_mul, int sub_acc1)
v32acc32 | msc_4x16_16x8_conf (v64uint8 a, v128int4 b, v32acc32 acc, int zero_acc, int shift16, int sub_mul, int sub_acc1)
v32acc32 | negmsc_4x16_16x8_conf (v64uint8 a, v128int4 b, v32acc32 acc, int zero_acc, int sub_mul, int sub_acc1)
v32acc32 | negmac_4x16_16x8_conf (v64uint8 a, v128int4 b, v32acc32 acc, int zero_acc, int sub_mul, int sub_acc1)
v32acc32 | addmac_4x16_16x8_conf (v64uint8 a, v128int4 b, v32acc32 acc1, v32acc32 acc2, int zero_acc1, int shift16, int sub_mul, int sub_acc1, int sub_acc2)
v32acc32 | addmsc_4x16_16x8_conf (v64uint8 a, v128int4 b, v32acc32 acc1, v32acc32 acc2, int zero_acc1, int shift16, int sub_mul, int sub_acc1, int sub_acc2)
v32acc32 | submac_4x16_16x8_conf (v64uint8 a, v128int4 b, v32acc32 acc1, v32acc32 acc2, int zero_acc1, int sub_mul, int sub_acc1, int sub_acc2)
v32acc32 | submsc_4x16_16x8_conf (v64uint8 a, v128int4 b, v32acc32 acc1, v32acc32 acc2, int zero_acc1, int sub_mul, int sub_acc1, int sub_acc2)

## 4x16_16x8 with dynamic sign and dynamic negation of multiplication result
v32acc32 | mac_4x16_16x8_conf (v64int8 a, int sgn_x, v128int4 b, int sgn_y, v32acc32 acc, int zero_acc, int shift16, int sub_mul, int sub_acc1)
v32acc32 | mul_4x16_16x8_conf (v64int8 a, int sgn_x, v128int4 b, int sgn_y, int sub_mul)
v32acc32 | negmul_4x16_16x8_conf (v64int8 a, int sgn_x, v128int4 b, int sgn_y, int sub_mul)
v32acc32 | msc_4x16_16x8_conf (v64int8 a, int sgn_x, v128int4 b, int sgn_y, v32acc32 acc, int zero_acc, int shift16, int sub_mul, int sub_acc1)
v32acc32 | negmsc_4x16_16x8_conf (v64int8 a, int sgn_x, v128int4 b, int sgn_y, v32acc32 acc, int zero_acc, int sub_mul, int sub_acc1)
v32acc32 | negmac_4x16_16x8_conf (v64int8 a, int sgn_x, v128int4 b, int sgn_y, v32acc32 acc, int zero_acc, int sub_mul, int sub_acc1)
v32acc32 | addmac_4x16_16x8_conf (v64int8 a, int sgn_x, v128int4 b, int sgn_y, v32acc32 acc1, v32acc32 acc2, int zero_acc1, int shift16, int sub_mul, int sub_acc1, int sub_acc2)
v32acc32 | addmsc_4x16_16x8_conf (v64int8 a, int sgn_x, v128int4 b, int sgn_y, v32acc32 acc1, v32acc32 acc2, int zero_acc1, int shift16, int sub_mul, int sub_acc1, int sub_acc2)
v32acc32 | submac_4x16_16x8_conf (v64int8 a, int sgn_x, v128int4 b, int sgn_y, v32acc32 acc1, v32acc32 acc2, int zero_acc1, int sub_mul, int sub_acc1, int sub_acc2)
v32acc32 | submsc_4x16_16x8_conf (v64int8 a, int sgn_x, v128int4 b, int sgn_y, v32acc32 acc1, v32acc32 acc2, int zero_acc1, int sub_mul, int sub_acc1, int sub_acc2)
v32acc32 | mac_4x16_16x8_conf (v64int8 a, int sgn_x, v128uint4 b, int sgn_y, v32acc32 acc, int zero_acc, int shift16, int sub_mul, int sub_acc1)
v32acc32 | mul_4x16_16x8_conf (v64int8 a, int sgn_x, v128uint4 b, int sgn_y, int sub_mul)
v32acc32 | negmul_4x16_16x8_conf (v64int8 a, int sgn_x, v128uint4 b, int sgn_y, int sub_mul)
v32acc32 | msc_4x16_16x8_conf (v64int8 a, int sgn_x, v128uint4 b, int sgn_y, v32acc32 acc, int zero_acc, int shift16, int sub_mul, int sub_acc1)
v32acc32 | negmsc_4x16_16x8_conf (v64int8 a, int sgn_x, v128uint4 b, int sgn_y, v32acc32 acc, int zero_acc, int sub_mul, int sub_acc1)
v32acc32 | negmac_4x16_16x8_conf (v64int8 a, int sgn_x, v128uint4 b, int sgn_y, v32acc32 acc, int zero_acc, int sub_mul, int sub_acc1)
v32acc32 | addmac_4x16_16x8_conf (v64int8 a, int sgn_x, v128uint4 b, int sgn_y, v32acc32 acc1, v32acc32 acc2, int zero_acc1, int shift16, int sub_mul, int sub_acc1, int sub_acc2)
v32acc32 | addmsc_4x16_16x8_conf (v64int8 a, int sgn_x, v128uint4 b, int sgn_y, v32acc32 acc1, v32acc32 acc2, int zero_acc1, int shift16, int sub_mul, int sub_acc1, int sub_acc2)
v32acc32 | submac_4x16_16x8_conf (v64int8 a, int sgn_x, v128uint4 b, int sgn_y, v32acc32 acc1, v32acc32 acc2, int zero_acc1, int sub_mul, int sub_acc1, int sub_acc2)
v32acc32 | submsc_4x16_16x8_conf (v64int8 a, int sgn_x, v128uint4 b, int sgn_y, v32acc32 acc1, v32acc32 acc2, int zero_acc1, int sub_mul, int sub_acc1, int sub_acc2)
v32acc32 | mac_4x16_16x8_conf (v64uint8 a, int sgn_x, v128uint4 b, int sgn_y, v32acc32 acc, int zero_acc, int shift16, int sub_mul, int sub_acc1)
v32acc32 | mul_4x16_16x8_conf (v64uint8 a, int sgn_x, v128uint4 b, int sgn_y, int sub_mul)
v32acc32 | negmul_4x16_16x8_conf (v64uint8 a, int sgn_x, v128uint4 b, int sgn_y, int sub_mul)
v32acc32 | msc_4x16_16x8_conf (v64uint8 a, int sgn_x, v128uint4 b, int sgn_y, v32acc32 acc, int zero_acc, int shift16, int sub_mul, int sub_acc1)
v32acc32 | negmsc_4x16_16x8_conf (v64uint8 a, int sgn_x, v128uint4 b, int sgn_y, v32acc32 acc, int zero_acc, int sub_mul, int sub_acc1)
v32acc32 | negmac_4x16_16x8_conf (v64uint8 a, int sgn_x, v128uint4 b, int sgn_y, v32acc32 acc, int zero_acc, int sub_mul, int sub_acc1)
v32acc32 | addmac_4x16_16x8_conf (v64uint8 a, int sgn_x, v128uint4 b, int sgn_y, v32acc32 acc1, v32acc32 acc2, int zero_acc1, int shift16, int sub_mul, int sub_acc1, int sub_acc2)
v32acc32 | addmsc_4x16_16x8_conf (v64uint8 a, int sgn_x, v128uint4 b, int sgn_y, v32acc32 acc1, v32acc32 acc2, int zero_acc1, int shift16, int sub_mul, int sub_acc1, int sub_acc2)
v32acc32 | submac_4x16_16x8_conf (v64uint8 a, int sgn_x, v128uint4 b, int sgn_y, v32acc32 acc1, v32acc32 acc2, int zero_acc1, int sub_mul, int sub_acc1, int sub_acc2)
v32acc32 | submsc_4x16_16x8_conf (v64uint8 a, int sgn_x, v128uint4 b, int sgn_y, v32acc32 acc1, v32acc32 acc2, int zero_acc1, int sub_mul, int sub_acc1, int sub_acc2)
v32acc32 | mac_4x16_16x8_conf (v64uint8 a, int sgn_x, v128int4 b, int sgn_y, v32acc32 acc, int zero_acc, int shift16, int sub_mul, int sub_acc1)
v32acc32 | mul_4x16_16x8_conf (v64uint8 a, int sgn_x, v128int4 b, int sgn_y, int sub_mul)
v32acc32 | negmul_4x16_16x8_conf (v64uint8 a, int sgn_x, v128int4 b, int sgn_y, int sub_mul)
v32acc32 | msc_4x16_16x8_conf (v64uint8 a, int sgn_x, v128int4 b, int sgn_y, v32acc32 acc, int zero_acc, int shift16, int sub_mul, int sub_acc1)
v32acc32 | negmsc_4x16_16x8_conf (v64uint8 a, int sgn_x, v128int4 b, int sgn_y, v32acc32 acc, int zero_acc, int sub_mul, int sub_acc1)
v32acc32 | negmac_4x16_16x8_conf (v64uint8 a, int sgn_x, v128int4 b, int sgn_y, v32acc32 acc, int zero_acc, int sub_mul, int sub_acc1)
v32acc32 | addmac_4x16_16x8_conf (v64uint8 a, int sgn_x, v128int4 b, int sgn_y, v32acc32 acc1, v32acc32 acc2, int zero_acc1, int shift16, int sub_mul, int sub_acc1, int sub_acc2)
v32acc32 | addmsc_4x16_16x8_conf (v64uint8 a, int sgn_x, v128int4 b, int sgn_y, v32acc32 acc1, v32acc32 acc2, int zero_acc1, int shift16, int sub_mul, int sub_acc1, int sub_acc2)
v32acc32 | submac_4x16_16x8_conf (v64uint8 a, int sgn_x, v128int4 b, int sgn_y, v32acc32 acc1, v32acc32 acc2, int zero_acc1, int sub_mul, int sub_acc1, int sub_acc2)
v32acc32 | submsc_4x16_16x8_conf (v64uint8 a, int sgn_x, v128int4 b, int sgn_y, v32acc32 acc1, v32acc32 acc2, int zero_acc1, int sub_mul, int sub_acc1, int sub_acc2)

## Function Documentation

## ◆ addmac_4x16_16x8() [1/8]

v32acc32 addmac_4x16_16x8 | ( | v64int8 | a,
|  | int | sgn_x,
|  | v128int4 | b,
|  | int | sgn_y,
|  | v32acc32 | acc1,
|  | v32acc32 | acc2 )

Parameters

  a | Matrix A
  sgn_x | Sign mask for matrix A
  b | Matrix B
  sgn_y | Sign mask for matrix B
  acc1 | Input accumulator 1
  acc2 | Input accumulator 2

Returns
  Result of operation

## ◆ addmac_4x16_16x8() [2/8]

v32acc32 addmac_4x16_16x8 | ( | v64int8 | a,
|  | int | sgn_x,
|  | v128uint4 | b,
|  | int | sgn_y,
|  | v32acc32 | acc1,
|  | v32acc32 | acc2 )

Parameters

  a | Matrix A
  sgn_x | Sign mask for matrix A
  b | Matrix B
  sgn_y | Sign mask for matrix B
  acc1 | Input accumulator 1
  acc2 | Input accumulator 2

Returns
  Result of operation

## ◆ addmac_4x16_16x8() [3/8]

v32acc32 addmac_4x16_16x8 | ( | v64int8 | a,
|  | v128int4 | b,
|  | v32acc32 | acc1,
|  | v32acc32 | acc2 )

Parameters

  a | Matrix A
  b | Matrix B
  acc1 | Input accumulator 1
  acc2 | Input accumulator 2

Returns
  Result of operation

## ◆ addmac_4x16_16x8() [4/8]

v32acc32 addmac_4x16_16x8 | ( | v64int8 | a,
|  | v128uint4 | b,
|  | v32acc32 | acc1,
|  | v32acc32 | acc2 )

Parameters

  a | Matrix A
  b | Matrix B
  acc1 | Input accumulator 1
  acc2 | Input accumulator 2

Returns
  Result of operation

## ◆ addmac_4x16_16x8() [5/8]

v32acc32 addmac_4x16_16x8 | ( | v64uint8 | a,
|  | int | sgn_x,
|  | v128int4 | b,
|  | int | sgn_y,
|  | v32acc32 | acc1,
|  | v32acc32 | acc2 )

Parameters

  a | Matrix A
  sgn_x | Sign mask for matrix A
  b | Matrix B
  sgn_y | Sign mask for matrix B
  acc1 | Input accumulator 1
  acc2 | Input accumulator 2

Returns
  Result of operation

## ◆ addmac_4x16_16x8() [6/8]

v32acc32 addmac_4x16_16x8 | ( | v64uint8 | a,
|  | int | sgn_x,
|  | v128uint4 | b,
|  | int | sgn_y,
|  | v32acc32 | acc1,
|  | v32acc32 | acc2 )

Parameters

  a | Matrix A
  sgn_x | Sign mask for matrix A
  b | Matrix B
  sgn_y | Sign mask for matrix B
  acc1 | Input accumulator 1
  acc2 | Input accumulator 2

Returns
  Result of operation

## ◆ addmac_4x16_16x8() [7/8]

v32acc32 addmac_4x16_16x8 | ( | v64uint8 | a,
|  | v128int4 | b,
|  | v32acc32 | acc1,
|  | v32acc32 | acc2 )

Parameters

  a | Matrix A
  b | Matrix B
  acc1 | Input accumulator 1
  acc2 | Input accumulator 2

Returns
  Result of operation

## ◆ addmac_4x16_16x8() [8/8]

v32acc32 addmac_4x16_16x8 | ( | v64uint8 | a,
|  | v128uint4 | b,
|  | v32acc32 | acc1,
|  | v32acc32 | acc2 )

Parameters

  a | Matrix A
  b | Matrix B
  acc1 | Input accumulator 1
  acc2 | Input accumulator 2

Returns
  Result of operation

## ◆ addmac_4x16_16x8_conf() [1/8]

v32acc32 addmac_4x16_16x8_conf | ( | v64int8 | a,
|  | int | sgn_x,
|  | v128int4 | b,
|  | int | sgn_y,
|  | v32acc32 | acc1,
|  | v32acc32 | acc2,
|  | int | zero_acc1,
|  | int | shift16,
|  | int | sub_mul,
|  | int | sub_acc1,
|  | int | sub_acc2 )

Parameters

  a | Matrix A
  sgn_x | Sign mask for matrix A
  b | Matrix B
  sgn_y | Sign mask for matrix B
  acc1 | Input accumulator 1
  acc2 | Input accumulator 2
  zero_acc1 | Zeroing mask for acc1
  shift16 | Shift mask of input accumulator acc1
  sub_mul | Negation mask of multiplication result
  sub_acc1 | Negation mask of acc1

Returns
  Result of operation

## ◆ addmac_4x16_16x8_conf() [2/8]

v32acc32 addmac_4x16_16x8_conf | ( | v64int8 | a,
|  | int | sgn_x,
|  | v128uint4 | b,
|  | int | sgn_y,
|  | v32acc32 | acc1,
|  | v32acc32 | acc2,
|  | int | zero_acc1,
|  | int | shift16,
|  | int | sub_mul,
|  | int | sub_acc1,
|  | int | sub_acc2 )

Parameters

  a | Matrix A
  sgn_x | Sign mask for matrix A
  b | Matrix B
  sgn_y | Sign mask for matrix B
  acc1 | Input accumulator 1
  acc2 | Input accumulator 2
  zero_acc1 | Zeroing mask for acc1
  shift16 | Shift mask of input accumulator acc1
  sub_mul | Negation mask of multiplication result
  sub_acc1 | Negation mask of acc1

Returns
  Result of operation

## ◆ addmac_4x16_16x8_conf() [3/8]

v32acc32 addmac_4x16_16x8_conf | ( | v64int8 | a,
|  | v128int4 | b,
|  | v32acc32 | acc1,
|  | v32acc32 | acc2,
|  | int | zero_acc1,
|  | int | shift16,
|  | int | sub_mul,
|  | int | sub_acc1,
|  | int | sub_acc2 )

Parameters

  a | Matrix A
  b | Matrix B
  acc1 | Input accumulator 1
  acc2 | Input accumulator 2
  zero_acc1 | Zeroing mask for acc1
  shift16 | Shift mask of input accumulator acc1
  sub_mul | Negation mask of multiplication result
  sub_acc1 | Negation mask of acc1

Returns
  Result of operation

## ◆ addmac_4x16_16x8_conf() [4/8]

v32acc32 addmac_4x16_16x8_conf | ( | v64int8 | a,
|  | v128uint4 | b,
|  | v32acc32 | acc1,
|  | v32acc32 | acc2,
|  | int | zero_acc1,
|  | int | shift16,
|  | int | sub_mul,
|  | int | sub_acc1,
|  | int | sub_acc2 )

Parameters

  a | Matrix A
  b | Matrix B
  acc1 | Input accumulator 1
  acc2 | Input accumulator 2
  zero_acc1 | Zeroing mask for acc1
  shift16 | Shift mask of input accumulator acc1
  sub_mul | Negation mask of multiplication result
  sub_acc1 | Negation mask of acc1

Returns
  Result of operation

## ◆ addmac_4x16_16x8_conf() [5/8]

v32acc32 addmac_4x16_16x8_conf | ( | v64uint8 | a,
|  | int | sgn_x,
|  | v128int4 | b,
|  | int | sgn_y,
|  | v32acc32 | acc1,
|  | v32acc32 | acc2,
|  | int | zero_acc1,
|  | int | shift16,
|  | int | sub_mul,
|  | int | sub_acc1,
|  | int | sub_acc2 )

Parameters

  a | Matrix A
  sgn_x | Sign mask for matrix A
  b | Matrix B
  sgn_y | Sign mask for matrix B
  acc1 | Input accumulator 1
  acc2 | Input accumulator 2
  zero_acc1 | Zeroing mask for acc1
  shift16 | Shift mask of input accumulator acc1
  sub_mul | Negation mask of multiplication result
  sub_acc1 | Negation mask of acc1

Returns
  Result of operation

## ◆ addmac_4x16_16x8_conf() [6/8]

v32acc32 addmac_4x16_16x8_conf | ( | v64uint8 | a,
|  | int | sgn_x,
|  | v128uint4 | b,
|  | int | sgn_y,
|  | v32acc32 | acc1,
|  | v32acc32 | acc2,
|  | int | zero_acc1,
|  | int | shift16,
|  | int | sub_mul,
|  | int | sub_acc1,
|  | int | sub_acc2 )

Parameters

  a | Matrix A
  sgn_x | Sign mask for matrix A
  b | Matrix B
  sgn_y | Sign mask for matrix B
  acc1 | Input accumulator 1
  acc2 | Input accumulator 2
  zero_acc1 | Zeroing mask for acc1
  shift16 | Shift mask of input accumulator acc1
  sub_mul | Negation mask of multiplication result
  sub_acc1 | Negation mask of acc1

Returns
  Result of operation

## ◆ addmac_4x16_16x8_conf() [7/8]

v32acc32 addmac_4x16_16x8_conf | ( | v64uint8 | a,
|  | v128int4 | b,
|  | v32acc32 | acc1,
|  | v32acc32 | acc2,
|  | int | zero_acc1,
|  | int | shift16,
|  | int | sub_mul,
|  | int | sub_acc1,
|  | int | sub_acc2 )

Parameters

  a | Matrix A
  b | Matrix B
  acc1 | Input accumulator 1
  acc2 | Input accumulator 2
  zero_acc1 | Zeroing mask for acc1
  shift16 | Shift mask of input accumulator acc1
  sub_mul | Negation mask of multiplication result
  sub_acc1 | Negation mask of acc1

Returns
  Result of operation

## ◆ addmac_4x16_16x8_conf() [8/8]

v32acc32 addmac_4x16_16x8_conf | ( | v64uint8 | a,
|  | v128uint4 | b,
|  | v32acc32 | acc1,
|  | v32acc32 | acc2,
|  | int | zero_acc1,
|  | int | shift16,
|  | int | sub_mul,
|  | int | sub_acc1,
|  | int | sub_acc2 )

Parameters

  a | Matrix A
  b | Matrix B
  acc1 | Input accumulator 1
  acc2 | Input accumulator 2
  zero_acc1 | Zeroing mask for acc1
  shift16 | Shift mask of input accumulator acc1
  sub_mul | Negation mask of multiplication result
  sub_acc1 | Negation mask of acc1

Returns
  Result of operation

## ◆ addmsc_4x16_16x8() [1/8]

v32acc32 addmsc_4x16_16x8 | ( | v64int8 | a,
|  | int | sgn_x,
|  | v128int4 | b,
|  | int | sgn_y,
|  | v32acc32 | acc1,
|  | v32acc32 | acc2 )

Parameters

  a | Matrix A
  sgn_x | Sign mask for matrix A
  b | Matrix B
  sgn_y | Sign mask for matrix B
  acc1 | Input accumulator 1
  acc2 | Input accumulator 2

Returns
  Result of operation

## ◆ addmsc_4x16_16x8() [2/8]

v32acc32 addmsc_4x16_16x8 | ( | v64int8 | a,
|  | int | sgn_x,
|  | v128uint4 | b,
|  | int | sgn_y,
|  | v32acc32 | acc1,
|  | v32acc32 | acc2 )

Parameters

  a | Matrix A
  sgn_x | Sign mask for matrix A
  b | Matrix B
  sgn_y | Sign mask for matrix B
  acc1 | Input accumulator 1
  acc2 | Input accumulator 2

Returns
  Result of operation

## ◆ addmsc_4x16_16x8() [3/8]

v32acc32 addmsc_4x16_16x8 | ( | v64int8 | a,
|  | v128int4 | b,
|  | v32acc32 | acc1,
|  | v32acc32 | acc2 )

Parameters

  a | Matrix A
  b | Matrix B
  acc1 | Input accumulator 1
  acc2 | Input accumulator 2

Returns
  Result of operation

## ◆ addmsc_4x16_16x8() [4/8]

v32acc32 addmsc_4x16_16x8 | ( | v64int8 | a,
|  | v128uint4 | b,
|  | v32acc32 | acc1,
|  | v32acc32 | acc2 )

Parameters

  a | Matrix A
  b | Matrix B
  acc1 | Input accumulator 1
  acc2 | Input accumulator 2

Returns
  Result of operation

## ◆ addmsc_4x16_16x8() [5/8]

v32acc32 addmsc_4x16_16x8 | ( | v64uint8 | a,
|  | int | sgn_x,
|  | v128int4 | b,
|  | int | sgn_y,
|  | v32acc32 | acc1,
|  | v32acc32 | acc2 )

Parameters

  a | Matrix A
  sgn_x | Sign mask for matrix A
  b | Matrix B
  sgn_y | Sign mask for matrix B
  acc1 | Input accumulator 1
  acc2 | Input accumulator 2

Returns
  Result of operation

## ◆ addmsc_4x16_16x8() [6/8]

v32acc32 addmsc_4x16_16x8 | ( | v64uint8 | a,
|  | int | sgn_x,
|  | v128uint4 | b,
|  | int | sgn_y,
|  | v32acc32 | acc1,
|  | v32acc32 | acc2 )

Parameters

  a | Matrix A
  sgn_x | Sign mask for matrix A
  b | Matrix B
  sgn_y | Sign mask for matrix B
  acc1 | Input accumulator 1
  acc2 | Input accumulator 2

Returns
  Result of operation

## ◆ addmsc_4x16_16x8() [7/8]

v32acc32 addmsc_4x16_16x8 | ( | v64uint8 | a,
|  | v128int4 | b,
|  | v32acc32 | acc1,
|  | v32acc32 | acc2 )

Parameters

  a | Matrix A
  b | Matrix B
  acc1 | Input accumulator 1
  acc2 | Input accumulator 2

Returns
  Result of operation

## ◆ addmsc_4x16_16x8() [8/8]

v32acc32 addmsc_4x16_16x8 | ( | v64uint8 | a,
|  | v128uint4 | b,
|  | v32acc32 | acc1,
|  | v32acc32 | acc2 )

Parameters

  a | Matrix A
  b | Matrix B
  acc1 | Input accumulator 1
  acc2 | Input accumulator 2

Returns
  Result of operation

## ◆ addmsc_4x16_16x8_conf() [1/8]

v32acc32 addmsc_4x16_16x8_conf | ( | v64int8 | a,
|  | int | sgn_x,
|  | v128int4 | b,
|  | int | sgn_y,
|  | v32acc32 | acc1,
|  | v32acc32 | acc2,
|  | int | zero_acc1,
|  | int | shift16,
|  | int | sub_mul,
|  | int | sub_acc1,
|  | int | sub_acc2 )

Parameters

  a | Matrix A
  sgn_x | Sign mask for matrix A
  b | Matrix B
  sgn_y | Sign mask for matrix B
  acc1 | Input accumulator 1
  acc2 | Input accumulator 2
  zero_acc1 | Zeroing mask for acc1
  shift16 | Shift mask of input accumulator acc1
  sub_mul | Negation mask of multiplication result
  sub_acc1 | Negation mask of acc1

Returns
  Result of operation

## ◆ addmsc_4x16_16x8_conf() [2/8]

v32acc32 addmsc_4x16_16x8_conf | ( | v64int8 | a,
|  | int | sgn_x,
|  | v128uint4 | b,
|  | int | sgn_y,
|  | v32acc32 | acc1,
|  | v32acc32 | acc2,
|  | int | zero_acc1,
|  | int | shift16,
|  | int | sub_mul,
|  | int | sub_acc1,
|  | int | sub_acc2 )

Parameters

  a | Matrix A
  sgn_x | Sign mask for matrix A
  b | Matrix B
  sgn_y | Sign mask for matrix B
  acc1 | Input accumulator 1
  acc2 | Input accumulator 2
  zero_acc1 | Zeroing mask for acc1
  shift16 | Shift mask of input accumulator acc1
  sub_mul | Negation mask of multiplication result
  sub_acc1 | Negation mask of acc1

Returns
  Result of operation

## ◆ addmsc_4x16_16x8_conf() [3/8]

v32acc32 addmsc_4x16_16x8_conf | ( | v64int8 | a,
|  | v128int4 | b,
|  | v32acc32 | acc1,
|  | v32acc32 | acc2,
|  | int | zero_acc1,
|  | int | shift16,
|  | int | sub_mul,
|  | int | sub_acc1,
|  | int | sub_acc2 )

Parameters

  a | Matrix A
  b | Matrix B
  acc1 | Input accumulator 1
  acc2 | Input accumulator 2
  zero_acc1 | Zeroing mask for acc1
  shift16 | Shift mask of input accumulator acc1
  sub_mul | Negation mask of multiplication result
  sub_acc1 | Negation mask of acc1

Returns
  Result of operation

## ◆ addmsc_4x16_16x8_conf() [4/8]

v32acc32 addmsc_4x16_16x8_conf | ( | v64int8 | a,
|  | v128uint4 | b,
|  | v32acc32 | acc1,
|  | v32acc32 | acc2,
|  | int | zero_acc1,
|  | int | shift16,
|  | int | sub_mul,
|  | int | sub_acc1,
|  | int | sub_acc2 )

Parameters

  a | Matrix A
  b | Matrix B
  acc1 | Input accumulator 1
  acc2 | Input accumulator 2
  zero_acc1 | Zeroing mask for acc1
  shift16 | Shift mask of input accumulator acc1
  sub_mul | Negation mask of multiplication result
  sub_acc1 | Negation mask of acc1

Returns
  Result of operation

## ◆ addmsc_4x16_16x8_conf() [5/8]

v32acc32 addmsc_4x16_16x8_conf | ( | v64uint8 | a,
|  | int | sgn_x,
|  | v128int4 | b,
|  | int | sgn_y,
|  | v32acc32 | acc1,
|  | v32acc32 | acc2,
|  | int | zero_acc1,
|  | int | shift16,
|  | int | sub_mul,
|  | int | sub_acc1,
|  | int | sub_acc2 )

Parameters

  a | Matrix A
  sgn_x | Sign mask for matrix A
  b | Matrix B
  sgn_y | Sign mask for matrix B
  acc1 | Input accumulator 1
  acc2 | Input accumulator 2
  zero_acc1 | Zeroing mask for acc1
  shift16 | Shift mask of input accumulator acc1
  sub_mul | Negation mask of multiplication result
  sub_acc1 | Negation mask of acc1

Returns
  Result of operation

## ◆ addmsc_4x16_16x8_conf() [6/8]

v32acc32 addmsc_4x16_16x8_conf | ( | v64uint8 | a,
|  | int | sgn_x,
|  | v128uint4 | b,
|  | int | sgn_y,
|  | v32acc32 | acc1,
|  | v32acc32 | acc2,
|  | int | zero_acc1,
|  | int | shift16,
|  | int | sub_mul,
|  | int | sub_acc1,
|  | int | sub_acc2 )

Parameters

  a | Matrix A
  sgn_x | Sign mask for matrix A
  b | Matrix B
  sgn_y | Sign mask for matrix B
  acc1 | Input accumulator 1
  acc2 | Input accumulator 2
  zero_acc1 | Zeroing mask for acc1
  shift16 | Shift mask of input accumulator acc1
  sub_mul | Negation mask of multiplication result
  sub_acc1 | Negation mask of acc1

Returns
  Result of operation

## ◆ addmsc_4x16_16x8_conf() [7/8]

v32acc32 addmsc_4x16_16x8_conf | ( | v64uint8 | a,
|  | v128int4 | b,
|  | v32acc32 | acc1,
|  | v32acc32 | acc2,
|  | int | zero_acc1,
|  | int | shift16,
|  | int | sub_mul,
|  | int | sub_acc1,
|  | int | sub_acc2 )

Parameters

  a | Matrix A
  b | Matrix B
  acc1 | Input accumulator 1
  acc2 | Input accumulator 2
  zero_acc1 | Zeroing mask for acc1
  shift16 | Shift mask of input accumulator acc1
  sub_mul | Negation mask of multiplication result
  sub_acc1 | Negation mask of acc1

Returns
  Result of operation

## ◆ addmsc_4x16_16x8_conf() [8/8]

v32acc32 addmsc_4x16_16x8_conf | ( | v64uint8 | a,
|  | v128uint4 | b,
|  | v32acc32 | acc1,
|  | v32acc32 | acc2,
|  | int | zero_acc1,
|  | int | shift16,
|  | int | sub_mul,
|  | int | sub_acc1,
|  | int | sub_acc2 )

Parameters

  a | Matrix A
  b | Matrix B
  acc1 | Input accumulator 1
  acc2 | Input accumulator 2
  zero_acc1 | Zeroing mask for acc1
  shift16 | Shift mask of input accumulator acc1
  sub_mul | Negation mask of multiplication result
  sub_acc1 | Negation mask of acc1

Returns
  Result of operation

## ◆ mac_4x16_16x8() [1/8]

v32acc32 mac_4x16_16x8 | ( | v64int8 | a,
|  | int | sgn_x,
|  | v128int4 | b,
|  | int | sgn_y,
|  | v32acc32 | acc )

Parameters

  a | Matrix A
  sgn_x | Sign mask for matrix A
  b | Matrix B
  sgn_y | Sign mask for matrix B
  acc | Input accumulator

Returns
  Result of operation

## ◆ mac_4x16_16x8() [2/8]

v32acc32 mac_4x16_16x8 | ( | v64int8 | a,
|  | int | sgn_x,
|  | v128uint4 | b,
|  | int | sgn_y,
|  | v32acc32 | acc )

Parameters

  a | Matrix A
  sgn_x | Sign mask for matrix A
  b | Matrix B
  sgn_y | Sign mask for matrix B
  acc | Input accumulator

Returns
  Result of operation

## ◆ mac_4x16_16x8() [3/8]

v32acc32 mac_4x16_16x8 | ( | v64int8 | a,
|  | v128int4 | b,
|  | v32acc32 | acc )

Parameters

  a | Matrix A
  b | Matrix B
  acc | Accumulator

Returns
  Result of operation

## ◆ mac_4x16_16x8() [4/8]

v32acc32 mac_4x16_16x8 | ( | v64int8 | a,
|  | v128uint4 | b,
|  | v32acc32 | acc )

Parameters

  a | Matrix A
  b | Matrix B
  acc | Accumulator

Returns
  Result of operation

## ◆ mac_4x16_16x8() [5/8]

v32acc32 mac_4x16_16x8 | ( | v64uint8 | a,
|  | int | sgn_x,
|  | v128int4 | b,
|  | int | sgn_y,
|  | v32acc32 | acc )

Parameters

  a | Matrix A
  sgn_x | Sign mask for matrix A
  b | Matrix B
  sgn_y | Sign mask for matrix B
  acc | Input accumulator

Returns
  Result of operation

## ◆ mac_4x16_16x8() [6/8]

v32acc32 mac_4x16_16x8 | ( | v64uint8 | a,
|  | int | sgn_x,
|  | v128uint4 | b,
|  | int | sgn_y,
|  | v32acc32 | acc )

Parameters

  a | Matrix A
  sgn_x | Sign mask for matrix A
  b | Matrix B
  sgn_y | Sign mask for matrix B
  acc | Input accumulator

Returns
  Result of operation

## ◆ mac_4x16_16x8() [7/8]

v32acc32 mac_4x16_16x8 | ( | v64uint8 | a,
|  | v128int4 | b,
|  | v32acc32 | acc )

Parameters

  a | Matrix A
  b | Matrix B
  acc | Accumulator

Returns
  Result of operation

## ◆ mac_4x16_16x8() [8/8]

v32acc32 mac_4x16_16x8 | ( | v64uint8 | a,
|  | v128uint4 | b,
|  | v32acc32 | acc )

Parameters

  a | Matrix A
  b | Matrix B
  acc | Accumulator

Returns
  Result of operation

## ◆ mac_4x16_16x8_conf() [1/8]

v32acc32 mac_4x16_16x8_conf | ( | v64int8 | a,
|  | int | sgn_x,
|  | v128int4 | b,
|  | int | sgn_y,
|  | v32acc32 | acc,
|  | int | zero_acc,
|  | int | shift16,
|  | int | sub_mul,
|  | int | sub_acc1 )

Parameters

  a | Matrix A
  sgn_x | Sign mask for matrix A
  b | Matrix B
  sgn_y | Sign mask for matrix B
  acc | Input accumulator
  zero_acc | Zeroing mask for acc1
  shift16 | Shift mask of input accumulator acc1
  sub_mul | Negation mask of multiplication result
  sub_acc1 | Negation mask of acc1

Returns
  Result of operation

## ◆ mac_4x16_16x8_conf() [2/8]

v32acc32 mac_4x16_16x8_conf | ( | v64int8 | a,
|  | int | sgn_x,
|  | v128uint4 | b,
|  | int | sgn_y,
|  | v32acc32 | acc,
|  | int | zero_acc,
|  | int | shift16,
|  | int | sub_mul,
|  | int | sub_acc1 )

Parameters

  a | Matrix A
  sgn_x | Sign mask for matrix A
  b | Matrix B
  sgn_y | Sign mask for matrix B
  acc | Input accumulator
  zero_acc | Zeroing mask for acc1
  shift16 | Shift mask of input accumulator acc1
  sub_mul | Negation mask of multiplication result
  sub_acc1 | Negation mask of acc1

Returns
  Result of operation

## ◆ mac_4x16_16x8_conf() [3/8]

v32acc32 mac_4x16_16x8_conf | ( | v64int8 | a,
|  | v128int4 | b,
|  | v32acc32 | acc,
|  | int | zero_acc,
|  | int | shift16,
|  | int | sub_mul,
|  | int | sub_acc1 )

Parameters

  a | Matrix A
  b | Matrix B
  acc | Input accumulator
  zero_acc | Zeroing mask for acc1
  shift16 | Shift mask of input accumulator acc1
  sub_mul | Negation mask of multiplication result
  sub_acc1 | Negation mask of acc1

Returns
  Result of operation

## ◆ mac_4x16_16x8_conf() [4/8]

v32acc32 mac_4x16_16x8_conf | ( | v64int8 | a,
|  | v128uint4 | b,
|  | v32acc32 | acc,
|  | int | zero_acc,
|  | int | shift16,
|  | int | sub_mul,
|  | int | sub_acc1 )

Parameters

  a | Matrix A
  b | Matrix B
  acc | Input accumulator
  zero_acc | Zeroing mask for acc1
  shift16 | Shift mask of input accumulator acc1
  sub_mul | Negation mask of multiplication result
  sub_acc1 | Negation mask of acc1

Returns
  Result of operation

## ◆ mac_4x16_16x8_conf() [5/8]

v32acc32 mac_4x16_16x8_conf | ( | v64uint8 | a,
|  | int | sgn_x,
|  | v128int4 | b,
|  | int | sgn_y,
|  | v32acc32 | acc,
|  | int | zero_acc,
|  | int | shift16,
|  | int | sub_mul,
|  | int | sub_acc1 )

Parameters

  a | Matrix A
  sgn_x | Sign mask for matrix A
  b | Matrix B
  sgn_y | Sign mask for matrix B
  acc | Input accumulator
  zero_acc | Zeroing mask for acc1
  shift16 | Shift mask of input accumulator acc1
  sub_mul | Negation mask of multiplication result
  sub_acc1 | Negation mask of acc1

Returns
  Result of operation

## ◆ mac_4x16_16x8_conf() [6/8]

v32acc32 mac_4x16_16x8_conf | ( | v64uint8 | a,
|  | int | sgn_x,
|  | v128uint4 | b,
|  | int | sgn_y,
|  | v32acc32 | acc,
|  | int | zero_acc,
|  | int | shift16,
|  | int | sub_mul,
|  | int | sub_acc1 )

Parameters

  a | Matrix A
  sgn_x | Sign mask for matrix A
  b | Matrix B
  sgn_y | Sign mask for matrix B
  acc | Input accumulator
  zero_acc | Zeroing mask for acc1
  shift16 | Shift mask of input accumulator acc1
  sub_mul | Negation mask of multiplication result
  sub_acc1 | Negation mask of acc1

Returns
  Result of operation

## ◆ mac_4x16_16x8_conf() [7/8]

v32acc32 mac_4x16_16x8_conf | ( | v64uint8 | a,
|  | v128int4 | b,
|  | v32acc32 | acc,
|  | int | zero_acc,
|  | int | shift16,
|  | int | sub_mul,
|  | int | sub_acc1 )

Parameters

  a | Matrix A
  b | Matrix B
  acc | Input accumulator
  zero_acc | Zeroing mask for acc1
  shift16 | Shift mask of input accumulator acc1
  sub_mul | Negation mask of multiplication result
  sub_acc1 | Negation mask of acc1

Returns
  Result of operation

## ◆ mac_4x16_16x8_conf() [8/8]

v32acc32 mac_4x16_16x8_conf | ( | v64uint8 | a,
|  | v128uint4 | b,
|  | v32acc32 | acc,
|  | int | zero_acc,
|  | int | shift16,
|  | int | sub_mul,
|  | int | sub_acc1 )

Parameters

  a | Matrix A
  b | Matrix B
  acc | Input accumulator
  zero_acc | Zeroing mask for acc1
  shift16 | Shift mask of input accumulator acc1
  sub_mul | Negation mask of multiplication result
  sub_acc1 | Negation mask of acc1

Returns
  Result of operation

## ◆ msc_4x16_16x8() [1/8]

v32acc32 msc_4x16_16x8 | ( | v64int8 | a,
|  | int | sgn_x,
|  | v128int4 | b,
|  | int | sgn_y,
|  | v32acc32 | acc )

Parameters

  a | Matrix A
  sgn_x | Sign mask for matrix A
  b | Matrix B
  sgn_y | Sign mask for matrix B
  acc | Input accumulator

Returns
  Result of operation

## ◆ msc_4x16_16x8() [2/8]

v32acc32 msc_4x16_16x8 | ( | v64int8 | a,
|  | int | sgn_x,
|  | v128uint4 | b,
|  | int | sgn_y,
|  | v32acc32 | acc )

Parameters

  a | Matrix A
  sgn_x | Sign mask for matrix A
  b | Matrix B
  sgn_y | Sign mask for matrix B
  acc | Input accumulator

Returns
  Result of operation

## ◆ msc_4x16_16x8() [3/8]

v32acc32 msc_4x16_16x8 | ( | v64int8 | a,
|  | v128int4 | b,
|  | v32acc32 | acc )

Parameters

  a | Matrix A
  b | Matrix B
  acc | Accumulator

Returns
  Result of operation

## ◆ msc_4x16_16x8() [4/8]

v32acc32 msc_4x16_16x8 | ( | v64int8 | a,
|  | v128uint4 | b,
|  | v32acc32 | acc )

Parameters

  a | Matrix A
  b | Matrix B
  acc | Accumulator

Returns
  Result of operation

## ◆ msc_4x16_16x8() [5/8]

v32acc32 msc_4x16_16x8 | ( | v64uint8 | a,
|  | int | sgn_x,
|  | v128int4 | b,
|  | int | sgn_y,
|  | v32acc32 | acc )

Parameters

  a | Matrix A
  sgn_x | Sign mask for matrix A
  b | Matrix B
  sgn_y | Sign mask for matrix B
  acc | Input accumulator

Returns
  Result of operation

## ◆ msc_4x16_16x8() [6/8]

v32acc32 msc_4x16_16x8 | ( | v64uint8 | a,
|  | int | sgn_x,
|  | v128uint4 | b,
|  | int | sgn_y,
|  | v32acc32 | acc )

Parameters

  a | Matrix A
  sgn_x | Sign mask for matrix A
  b | Matrix B
  sgn_y | Sign mask for matrix B
  acc | Input accumulator

Returns
  Result of operation

## ◆ msc_4x16_16x8() [7/8]

v32acc32 msc_4x16_16x8 | ( | v64uint8 | a,
|  | v128int4 | b,
|  | v32acc32 | acc )

Parameters

  a | Matrix A
  b | Matrix B
  acc | Accumulator

Returns
  Result of operation

## ◆ msc_4x16_16x8() [8/8]

v32acc32 msc_4x16_16x8 | ( | v64uint8 | a,
|  | v128uint4 | b,
|  | v32acc32 | acc )

Parameters

  a | Matrix A
  b | Matrix B
  acc | Accumulator

Returns
  Result of operation

## ◆ msc_4x16_16x8_conf() [1/8]

v32acc32 msc_4x16_16x8_conf | ( | v64int8 | a,
|  | int | sgn_x,
|  | v128int4 | b,
|  | int | sgn_y,
|  | v32acc32 | acc,
|  | int | zero_acc,
|  | int | shift16,
|  | int | sub_mul,
|  | int | sub_acc1 )

Parameters

  a | Matrix A
  sgn_x | Sign mask for matrix A
  b | Matrix B
  sgn_y | Sign mask for matrix B
  acc | Input accumulator
  zero_acc | Zeroing mask for acc1
  shift16 | Shift mask of input accumulator acc1
  sub_mul | Negation mask of multiplication result
  sub_acc1 | Negation mask of acc1

Returns
  Result of operation

## ◆ msc_4x16_16x8_conf() [2/8]

v32acc32 msc_4x16_16x8_conf | ( | v64int8 | a,
|  | int | sgn_x,
|  | v128uint4 | b,
|  | int | sgn_y,
|  | v32acc32 | acc,
|  | int | zero_acc,
|  | int | shift16,
|  | int | sub_mul,
|  | int | sub_acc1 )

Parameters

  a | Matrix A
  sgn_x | Sign mask for matrix A
  b | Matrix B
  sgn_y | Sign mask for matrix B
  acc | Input accumulator
  zero_acc | Zeroing mask for acc1
  shift16 | Shift mask of input accumulator acc1
  sub_mul | Negation mask of multiplication result
  sub_acc1 | Negation mask of acc1

Returns
  Result of operation

## ◆ msc_4x16_16x8_conf() [3/8]

v32acc32 msc_4x16_16x8_conf | ( | v64int8 | a,
|  | v128int4 | b,
|  | v32acc32 | acc,
|  | int | zero_acc,
|  | int | shift16,
|  | int | sub_mul,
|  | int | sub_acc1 )

Parameters

  a | Matrix A
  b | Matrix B
  acc | Input accumulator
  zero_acc | Zeroing mask for acc1
  shift16 | Shift mask of input accumulator acc1
  sub_mul | Negation mask of multiplication result
  sub_acc1 | Negation mask of acc1

Returns
  Result of operation

## ◆ msc_4x16_16x8_conf() [4/8]

v32acc32 msc_4x16_16x8_conf | ( | v64int8 | a,
|  | v128uint4 | b,
|  | v32acc32 | acc,
|  | int | zero_acc,
|  | int | shift16,
|  | int | sub_mul,
|  | int | sub_acc1 )

Parameters

  a | Matrix A
  b | Matrix B
  acc | Input accumulator
  zero_acc | Zeroing mask for acc1
  shift16 | Shift mask of input accumulator acc1
  sub_mul | Negation mask of multiplication result
  sub_acc1 | Negation mask of acc1

Returns
  Result of operation

## ◆ msc_4x16_16x8_conf() [5/8]

v32acc32 msc_4x16_16x8_conf | ( | v64uint8 | a,
|  | int | sgn_x,
|  | v128int4 | b,
|  | int | sgn_y,
|  | v32acc32 | acc,
|  | int | zero_acc,
|  | int | shift16,
|  | int | sub_mul,
|  | int | sub_acc1 )

Parameters

  a | Matrix A
  sgn_x | Sign mask for matrix A
  b | Matrix B
  sgn_y | Sign mask for matrix B
  acc | Input accumulator
  zero_acc | Zeroing mask for acc1
  shift16 | Shift mask of input accumulator acc1
  sub_mul | Negation mask of multiplication result
  sub_acc1 | Negation mask of acc1

Returns
  Result of operation

## ◆ msc_4x16_16x8_conf() [6/8]

v32acc32 msc_4x16_16x8_conf | ( | v64uint8 | a,
|  | int | sgn_x,
|  | v128uint4 | b,
|  | int | sgn_y,
|  | v32acc32 | acc,
|  | int | zero_acc,
|  | int | shift16,
|  | int | sub_mul,
|  | int | sub_acc1 )

Parameters

  a | Matrix A
  sgn_x | Sign mask for matrix A
  b | Matrix B
  sgn_y | Sign mask for matrix B
  acc | Input accumulator
  zero_acc | Zeroing mask for acc1
  shift16 | Shift mask of input accumulator acc1
  sub_mul | Negation mask of multiplication result
  sub_acc1 | Negation mask of acc1

Returns
  Result of operation

## ◆ msc_4x16_16x8_conf() [7/8]

v32acc32 msc_4x16_16x8_conf | ( | v64uint8 | a,
|  | v128int4 | b,
|  | v32acc32 | acc,
|  | int | zero_acc,
|  | int | shift16,
|  | int | sub_mul,
|  | int | sub_acc1 )

Parameters

  a | Matrix A
  b | Matrix B
  acc | Input accumulator
  zero_acc | Zeroing mask for acc1
  shift16 | Shift mask of input accumulator acc1
  sub_mul | Negation mask of multiplication result
  sub_acc1 | Negation mask of acc1

Returns
  Result of operation

## ◆ msc_4x16_16x8_conf() [8/8]

v32acc32 msc_4x16_16x8_conf | ( | v64uint8 | a,
|  | v128uint4 | b,
|  | v32acc32 | acc,
|  | int | zero_acc,
|  | int | shift16,
|  | int | sub_mul,
|  | int | sub_acc1 )

Parameters

  a | Matrix A
  b | Matrix B
  acc | Input accumulator
  zero_acc | Zeroing mask for acc1
  shift16 | Shift mask of input accumulator acc1
  sub_mul | Negation mask of multiplication result
  sub_acc1 | Negation mask of acc1

Returns
  Result of operation

## ◆ mul_4x16_16x8() [1/8]

v32acc32 mul_4x16_16x8 | ( | v64int8 | a,
|  | int | sgn_x,
|  | v128int4 | b,
|  | int | sgn_y )

Parameters

  a | Matrix A
  sgn_x | Sign mask for matrix A
  b | Matrix B
  sgn_y | Sign mask for matrix B

Returns
  Result of operation

## ◆ mul_4x16_16x8() [2/8]

v32acc32 mul_4x16_16x8 | ( | v64int8 | a,
|  | int | sgn_x,
|  | v128uint4 | b,
|  | int | sgn_y )

Parameters

  a | Matrix A
  sgn_x | Sign mask for matrix A
  b | Matrix B
  sgn_y | Sign mask for matrix B

Returns
  Result of operation

## ◆ mul_4x16_16x8() [3/8]

v32acc32 mul_4x16_16x8 | ( | v64int8 | a,
|  | v128int4 | b )

Parameters

  a | Matrix A
  b | Matrix B

Returns
  Result of operation

## ◆ mul_4x16_16x8() [4/8]

v32acc32 mul_4x16_16x8 | ( | v64int8 | a,
|  | v128uint4 | b )

Parameters

  a | Matrix A
  b | Matrix B

Returns
  Result of operation

## ◆ mul_4x16_16x8() [5/8]

v32acc32 mul_4x16_16x8 | ( | v64uint8 | a,
|  | int | sgn_x,
|  | v128int4 | b,
|  | int | sgn_y )

Parameters

  a | Matrix A
  sgn_x | Sign mask for matrix A
  b | Matrix B
  sgn_y | Sign mask for matrix B

Returns
  Result of operation

## ◆ mul_4x16_16x8() [6/8]

v32acc32 mul_4x16_16x8 | ( | v64uint8 | a,
|  | int | sgn_x,
|  | v128uint4 | b,
|  | int | sgn_y )

Parameters

  a | Matrix A
  sgn_x | Sign mask for matrix A
  b | Matrix B
  sgn_y | Sign mask for matrix B

Returns
  Result of operation

## ◆ mul_4x16_16x8() [7/8]

v32acc32 mul_4x16_16x8 | ( | v64uint8 | a,
|  | v128int4 | b )

Parameters

  a | Matrix A
  b | Matrix B

Returns
  Result of operation

## ◆ mul_4x16_16x8() [8/8]

v32acc32 mul_4x16_16x8 | ( | v64uint8 | a,
|  | v128uint4 | b )

Parameters

  a | Matrix A
  b | Matrix B

Returns
  Result of operation

## ◆ mul_4x16_16x8_conf() [1/8]

v32acc32 mul_4x16_16x8_conf | ( | v64int8 | a,
|  | int | sgn_x,
|  | v128int4 | b,
|  | int | sgn_y,
|  | int | sub_mul )

Parameters

  a | Matrix A
  sgn_x | Sign mask for matrix A
  b | Matrix B
  sgn_y | Sign mask for matrix B
  sub_mul | Negation mask of multiplication result

Returns
  Result of operation

## ◆ mul_4x16_16x8_conf() [2/8]

v32acc32 mul_4x16_16x8_conf | ( | v64int8 | a,
|  | int | sgn_x,
|  | v128uint4 | b,
|  | int | sgn_y,
|  | int | sub_mul )

Parameters

  a | Matrix A
  sgn_x | Sign mask for matrix A
  b | Matrix B
  sgn_y | Sign mask for matrix B
  sub_mul | Negation mask of multiplication result

Returns
  Result of operation

## ◆ mul_4x16_16x8_conf() [3/8]

v32acc32 mul_4x16_16x8_conf | ( | v64int8 | a,
|  | v128int4 | b,
|  | int | sub_mul )

Parameters

  a | Matrix A
  b | Matrix B
  sub_mul | Negation mask for multiplication result. If a bit of sub_mul is set the corresponding vector lane of the output accumulator will be negated.

Returns
  Result of operation

## ◆ mul_4x16_16x8_conf() [4/8]

v32acc32 mul_4x16_16x8_conf | ( | v64int8 | a,
|  | v128uint4 | b,
|  | int | sub_mul )

Parameters

  a | Matrix A
  b | Matrix B
  sub_mul | Negation mask for multiplication result. If a bit of sub_mul is set the corresponding vector lane of the output accumulator will be negated.

Returns
  Result of operation

## ◆ mul_4x16_16x8_conf() [5/8]

v32acc32 mul_4x16_16x8_conf | ( | v64uint8 | a,
|  | int | sgn_x,
|  | v128int4 | b,
|  | int | sgn_y,
|  | int | sub_mul )

Parameters

  a | Matrix A
  sgn_x | Sign mask for matrix A
  b | Matrix B
  sgn_y | Sign mask for matrix B
  sub_mul | Negation mask of multiplication result

Returns
  Result of operation

## ◆ mul_4x16_16x8_conf() [6/8]

v32acc32 mul_4x16_16x8_conf | ( | v64uint8 | a,
|  | int | sgn_x,
|  | v128uint4 | b,
|  | int | sgn_y,
|  | int | sub_mul )

Parameters

  a | Matrix A
  sgn_x | Sign mask for matrix A
  b | Matrix B
  sgn_y | Sign mask for matrix B
  sub_mul | Negation mask of multiplication result

Returns
  Result of operation

## ◆ mul_4x16_16x8_conf() [7/8]

v32acc32 mul_4x16_16x8_conf | ( | v64uint8 | a,
|  | v128int4 | b,
|  | int | sub_mul )

Parameters

  a | Matrix A
  b | Matrix B
  sub_mul | Negation mask for multiplication result. If a bit of sub_mul is set the corresponding vector lane of the output accumulator will be negated.

Returns
  Result of operation

## ◆ mul_4x16_16x8_conf() [8/8]

v32acc32 mul_4x16_16x8_conf | ( | v64uint8 | a,
|  | v128uint4 | b,
|  | int | sub_mul )

Parameters

  a | Matrix A
  b | Matrix B
  sub_mul | Negation mask for multiplication result. If a bit of sub_mul is set the corresponding vector lane of the output accumulator will be negated.

Returns
  Result of operation

## ◆ negmac_4x16_16x8() [1/8]

v32acc32 negmac_4x16_16x8 | ( | v64int8 | a,
|  | int | sgn_x,
|  | v128int4 | b,
|  | int | sgn_y,
|  | v32acc32 | acc )

Parameters

  a | Matrix A
  sgn_x | Sign mask for matrix A
  b | Matrix B
  sgn_y | Sign mask for matrix B
  acc | Input accumulator

Returns
  Result of operation

## ◆ negmac_4x16_16x8() [2/8]

v32acc32 negmac_4x16_16x8 | ( | v64int8 | a,
|  | int | sgn_x,
|  | v128uint4 | b,
|  | int | sgn_y,
|  | v32acc32 | acc )

Parameters

  a | Matrix A
  sgn_x | Sign mask for matrix A
  b | Matrix B
  sgn_y | Sign mask for matrix B
  acc | Input accumulator

Returns
  Result of operation

## ◆ negmac_4x16_16x8() [3/8]

v32acc32 negmac_4x16_16x8 | ( | v64int8 | a,
|  | v128int4 | b,
|  | v32acc32 | acc )

Parameters

  a | Matrix A
  b | Matrix B
  acc | Accumulator

Returns
  Result of operation

## ◆ negmac_4x16_16x8() [4/8]

v32acc32 negmac_4x16_16x8 | ( | v64int8 | a,
|  | v128uint4 | b,
|  | v32acc32 | acc )

Parameters

  a | Matrix A
  b | Matrix B
  acc | Accumulator

Returns
  Result of operation

## ◆ negmac_4x16_16x8() [5/8]

v32acc32 negmac_4x16_16x8 | ( | v64uint8 | a,
|  | int | sgn_x,
|  | v128int4 | b,
|  | int | sgn_y,
|  | v32acc32 | acc )

Parameters

  a | Matrix A
  sgn_x | Sign mask for matrix A
  b | Matrix B
  sgn_y | Sign mask for matrix B
  acc | Input accumulator

Returns
  Result of operation

## ◆ negmac_4x16_16x8() [6/8]

v32acc32 negmac_4x16_16x8 | ( | v64uint8 | a,
|  | int | sgn_x,
|  | v128uint4 | b,
|  | int | sgn_y,
|  | v32acc32 | acc )

Parameters

  a | Matrix A
  sgn_x | Sign mask for matrix A
  b | Matrix B
  sgn_y | Sign mask for matrix B
  acc | Input accumulator

Returns
  Result of operation

## ◆ negmac_4x16_16x8() [7/8]

v32acc32 negmac_4x16_16x8 | ( | v64uint8 | a,
|  | v128int4 | b,
|  | v32acc32 | acc )

Parameters

  a | Matrix A
  b | Matrix B
  acc | Accumulator

Returns
  Result of operation

## ◆ negmac_4x16_16x8() [8/8]

v32acc32 negmac_4x16_16x8 | ( | v64uint8 | a,
|  | v128uint4 | b,
|  | v32acc32 | acc )

Parameters

  a | Matrix A
  b | Matrix B
  acc | Accumulator

Returns
  Result of operation

## ◆ negmac_4x16_16x8_conf() [1/8]

v32acc32 negmac_4x16_16x8_conf | ( | v64int8 | a,
|  | int | sgn_x,
|  | v128int4 | b,
|  | int | sgn_y,
|  | v32acc32 | acc,
|  | int | zero_acc,
|  | int | sub_mul,
|  | int | sub_acc1 )

Parameters

  a | Matrix A
  sgn_x | Sign mask for matrix A
  b | Matrix B
  sgn_y | Sign mask for matrix B
  acc | Input accumulator
  zero_acc | Zeroing mask for acc1
  sub_mul | Negation mask of multiplication result
  sub_acc1 | Negation mask of acc1

Returns
  Result of operation

## ◆ negmac_4x16_16x8_conf() [2/8]

v32acc32 negmac_4x16_16x8_conf | ( | v64int8 | a,
|  | int | sgn_x,
|  | v128uint4 | b,
|  | int | sgn_y,
|  | v32acc32 | acc,
|  | int | zero_acc,
|  | int | sub_mul,
|  | int | sub_acc1 )

Parameters

  a | Matrix A
  sgn_x | Sign mask for matrix A
  b | Matrix B
  sgn_y | Sign mask for matrix B
  acc | Input accumulator
  zero_acc | Zeroing mask for acc1
  sub_mul | Negation mask of multiplication result
  sub_acc1 | Negation mask of acc1

Returns
  Result of operation

## ◆ negmac_4x16_16x8_conf() [3/8]

v32acc32 negmac_4x16_16x8_conf | ( | v64int8 | a,
|  | v128int4 | b,
|  | v32acc32 | acc,
|  | int | zero_acc,
|  | int | sub_mul,
|  | int | sub_acc1 )

Parameters

  a | Matrix A
  b | Matrix B
  acc | Input accumulator
  zero_acc | Zeroing mask for acc1
  sub_mul | Negation mask of multiplication result
  sub_acc1 | Negation mask of acc1

Returns
  Result of operation

## ◆ negmac_4x16_16x8_conf() [4/8]

v32acc32 negmac_4x16_16x8_conf | ( | v64int8 | a,
|  | v128uint4 | b,
|  | v32acc32 | acc,
|  | int | zero_acc,
|  | int | sub_mul,
|  | int | sub_acc1 )

Parameters

  a | Matrix A
  b | Matrix B
  acc | Input accumulator
  zero_acc | Zeroing mask for acc1
  sub_mul | Negation mask of multiplication result
  sub_acc1 | Negation mask of acc1

Returns
  Result of operation

## ◆ negmac_4x16_16x8_conf() [5/8]

v32acc32 negmac_4x16_16x8_conf | ( | v64uint8 | a,
|  | int | sgn_x,
|  | v128int4 | b,
|  | int | sgn_y,
|  | v32acc32 | acc,
|  | int | zero_acc,
|  | int | sub_mul,
|  | int | sub_acc1 )

Parameters

  a | Matrix A
  sgn_x | Sign mask for matrix A
  b | Matrix B
  sgn_y | Sign mask for matrix B
  acc | Input accumulator
  zero_acc | Zeroing mask for acc1
  sub_mul | Negation mask of multiplication result
  sub_acc1 | Negation mask of acc1

Returns
  Result of operation

## ◆ negmac_4x16_16x8_conf() [6/8]

v32acc32 negmac_4x16_16x8_conf | ( | v64uint8 | a,
|  | int | sgn_x,
|  | v128uint4 | b,
|  | int | sgn_y,
|  | v32acc32 | acc,
|  | int | zero_acc,
|  | int | sub_mul,
|  | int | sub_acc1 )

Parameters

  a | Matrix A
  sgn_x | Sign mask for matrix A
  b | Matrix B
  sgn_y | Sign mask for matrix B
  acc | Input accumulator
  zero_acc | Zeroing mask for acc1
  sub_mul | Negation mask of multiplication result
  sub_acc1 | Negation mask of acc1

Returns
  Result of operation

## ◆ negmac_4x16_16x8_conf() [7/8]

v32acc32 negmac_4x16_16x8_conf | ( | v64uint8 | a,
|  | v128int4 | b,
|  | v32acc32 | acc,
|  | int | zero_acc,
|  | int | sub_mul,
|  | int | sub_acc1 )

Parameters

  a | Matrix A
  b | Matrix B
  acc | Input accumulator
  zero_acc | Zeroing mask for acc1
  sub_mul | Negation mask of multiplication result
  sub_acc1 | Negation mask of acc1

Returns
  Result of operation

## ◆ negmac_4x16_16x8_conf() [8/8]

v32acc32 negmac_4x16_16x8_conf | ( | v64uint8 | a,
|  | v128uint4 | b,
|  | v32acc32 | acc,
|  | int | zero_acc,
|  | int | sub_mul,
|  | int | sub_acc1 )

Parameters

  a | Matrix A
  b | Matrix B
  acc | Input accumulator
  zero_acc | Zeroing mask for acc1
  sub_mul | Negation mask of multiplication result
  sub_acc1 | Negation mask of acc1

Returns
  Result of operation

## ◆ negmsc_4x16_16x8() [1/8]

v32acc32 negmsc_4x16_16x8 | ( | v64int8 | a,
|  | int | sgn_x,
|  | v128int4 | b,
|  | int | sgn_y,
|  | v32acc32 | acc )

Parameters

  a | Matrix A
  sgn_x | Sign mask for matrix A
  b | Matrix B
  sgn_y | Sign mask for matrix B
  acc | Input accumulator

Returns
  Result of operation

## ◆ negmsc_4x16_16x8() [2/8]

v32acc32 negmsc_4x16_16x8 | ( | v64int8 | a,
|  | int | sgn_x,
|  | v128uint4 | b,
|  | int | sgn_y,
|  | v32acc32 | acc )

Parameters

  a | Matrix A
  sgn_x | Sign mask for matrix A
  b | Matrix B
  sgn_y | Sign mask for matrix B
  acc | Input accumulator

Returns
  Result of operation

## ◆ negmsc_4x16_16x8() [3/8]

v32acc32 negmsc_4x16_16x8 | ( | v64int8 | a,
|  | v128int4 | b,
|  | v32acc32 | acc )

Parameters

  a | Matrix A
  b | Matrix B
  acc | Accumulator

Returns
  Result of operation

## ◆ negmsc_4x16_16x8() [4/8]

v32acc32 negmsc_4x16_16x8 | ( | v64int8 | a,
|  | v128uint4 | b,
|  | v32acc32 | acc )

Parameters

  a | Matrix A
  b | Matrix B
  acc | Accumulator

Returns
  Result of operation

## ◆ negmsc_4x16_16x8() [5/8]

v32acc32 negmsc_4x16_16x8 | ( | v64uint8 | a,
|  | int | sgn_x,
|  | v128int4 | b,
|  | int | sgn_y,
|  | v32acc32 | acc )

Parameters

  a | Matrix A
  sgn_x | Sign mask for matrix A
  b | Matrix B
  sgn_y | Sign mask for matrix B
  acc | Input accumulator

Returns
  Result of operation

## ◆ negmsc_4x16_16x8() [6/8]

v32acc32 negmsc_4x16_16x8 | ( | v64uint8 | a,
|  | int | sgn_x,
|  | v128uint4 | b,
|  | int | sgn_y,
|  | v32acc32 | acc )

Parameters

  a | Matrix A
  sgn_x | Sign mask for matrix A
  b | Matrix B
  sgn_y | Sign mask for matrix B
  acc | Input accumulator

Returns
  Result of operation

## ◆ negmsc_4x16_16x8() [7/8]

v32acc32 negmsc_4x16_16x8 | ( | v64uint8 | a,
|  | v128int4 | b,
|  | v32acc32 | acc )

Parameters

  a | Matrix A
  b | Matrix B
  acc | Accumulator

Returns
  Result of operation

## ◆ negmsc_4x16_16x8() [8/8]

v32acc32 negmsc_4x16_16x8 | ( | v64uint8 | a,
|  | v128uint4 | b,
|  | v32acc32 | acc )

Parameters

  a | Matrix A
  b | Matrix B
  acc | Accumulator

Returns
  Result of operation

## ◆ negmsc_4x16_16x8_conf() [1/8]

v32acc32 negmsc_4x16_16x8_conf | ( | v64int8 | a,
|  | int | sgn_x,
|  | v128int4 | b,
|  | int | sgn_y,
|  | v32acc32 | acc,
|  | int | zero_acc,
|  | int | sub_mul,
|  | int | sub_acc1 )

Parameters

  a | Matrix A
  sgn_x | Sign mask for matrix A
  b | Matrix B
  sgn_y | Sign mask for matrix B
  acc | Input accumulator
  zero_acc | Zeroing mask for acc1
  sub_mul | Negation mask of multiplication result
  sub_acc1 | Negation mask of acc1

Returns
  Result of operation

## ◆ negmsc_4x16_16x8_conf() [2/8]

v32acc32 negmsc_4x16_16x8_conf | ( | v64int8 | a,
|  | int | sgn_x,
|  | v128uint4 | b,
|  | int | sgn_y,
|  | v32acc32 | acc,
|  | int | zero_acc,
|  | int | sub_mul,
|  | int | sub_acc1 )

Parameters

  a | Matrix A
  sgn_x | Sign mask for matrix A
  b | Matrix B
  sgn_y | Sign mask for matrix B
  acc | Input accumulator
  zero_acc | Zeroing mask for acc1
  sub_mul | Negation mask of multiplication result
  sub_acc1 | Negation mask of acc1

Returns
  Result of operation

## ◆ negmsc_4x16_16x8_conf() [3/8]

v32acc32 negmsc_4x16_16x8_conf | ( | v64int8 | a,
|  | v128int4 | b,
|  | v32acc32 | acc,
|  | int | zero_acc,
|  | int | sub_mul,
|  | int | sub_acc1 )

Parameters

  a | Matrix A
  b | Matrix B
  acc | Input accumulator
  zero_acc | Zeroing mask for acc1
  sub_mul | Negation mask of multiplication result
  sub_acc1 | Negation mask of acc1

Returns
  Result of operation

## ◆ negmsc_4x16_16x8_conf() [4/8]

v32acc32 negmsc_4x16_16x8_conf | ( | v64int8 | a,
|  | v128uint4 | b,
|  | v32acc32 | acc,
|  | int | zero_acc,
|  | int | sub_mul,
|  | int | sub_acc1 )

Parameters

  a | Matrix A
  b | Matrix B
  acc | Input accumulator
  zero_acc | Zeroing mask for acc1
  sub_mul | Negation mask of multiplication result
  sub_acc1 | Negation mask of acc1

Returns
  Result of operation

## ◆ negmsc_4x16_16x8_conf() [5/8]

v32acc32 negmsc_4x16_16x8_conf | ( | v64uint8 | a,
|  | int | sgn_x,
|  | v128int4 | b,
|  | int | sgn_y,
|  | v32acc32 | acc,
|  | int | zero_acc,
|  | int | sub_mul,
|  | int | sub_acc1 )

Parameters

  a | Matrix A
  sgn_x | Sign mask for matrix A
  b | Matrix B
  sgn_y | Sign mask for matrix B
  acc | Input accumulator
  zero_acc | Zeroing mask for acc1
  sub_mul | Negation mask of multiplication result
  sub_acc1 | Negation mask of acc1

Returns
  Result of operation

## ◆ negmsc_4x16_16x8_conf() [6/8]

v32acc32 negmsc_4x16_16x8_conf | ( | v64uint8 | a,
|  | int | sgn_x,
|  | v128uint4 | b,
|  | int | sgn_y,
|  | v32acc32 | acc,
|  | int | zero_acc,
|  | int | sub_mul,
|  | int | sub_acc1 )

Parameters

  a | Matrix A
  sgn_x | Sign mask for matrix A
  b | Matrix B
  sgn_y | Sign mask for matrix B
  acc | Input accumulator
  zero_acc | Zeroing mask for acc1
  sub_mul | Negation mask of multiplication result
  sub_acc1 | Negation mask of acc1

Returns
  Result of operation

## ◆ negmsc_4x16_16x8_conf() [7/8]

v32acc32 negmsc_4x16_16x8_conf | ( | v64uint8 | a,
|  | v128int4 | b,
|  | v32acc32 | acc,
|  | int | zero_acc,
|  | int | sub_mul,
|  | int | sub_acc1 )

Parameters

  a | Matrix A
  b | Matrix B
  acc | Input accumulator
  zero_acc | Zeroing mask for acc1
  sub_mul | Negation mask of multiplication result
  sub_acc1 | Negation mask of acc1

Returns
  Result of operation

## ◆ negmsc_4x16_16x8_conf() [8/8]

v32acc32 negmsc_4x16_16x8_conf | ( | v64uint8 | a,
|  | v128uint4 | b,
|  | v32acc32 | acc,
|  | int | zero_acc,
|  | int | sub_mul,
|  | int | sub_acc1 )

Parameters

  a | Matrix A
  b | Matrix B
  acc | Input accumulator
  zero_acc | Zeroing mask for acc1
  sub_mul | Negation mask of multiplication result
  sub_acc1 | Negation mask of acc1

Returns
  Result of operation

## ◆ negmul_4x16_16x8() [1/8]

v32acc32 negmul_4x16_16x8 | ( | v64int8 | a,
|  | int | sgn_x,
|  | v128int4 | b,
|  | int | sgn_y )

Parameters

  a | Matrix A
  sgn_x | Sign mask for matrix A
  b | Matrix B
  sgn_y | Sign mask for matrix B

Returns
  Result of operation

## ◆ negmul_4x16_16x8() [2/8]

v32acc32 negmul_4x16_16x8 | ( | v64int8 | a,
|  | int | sgn_x,
|  | v128uint4 | b,
|  | int | sgn_y )

Parameters

  a | Matrix A
  sgn_x | Sign mask for matrix A
  b | Matrix B
  sgn_y | Sign mask for matrix B

Returns
  Result of operation

## ◆ negmul_4x16_16x8() [3/8]

v32acc32 negmul_4x16_16x8 | ( | v64int8 | a,
|  | v128int4 | b )

Parameters

  a | Matrix A
  b | Matrix B

Returns
  Result of operation

## ◆ negmul_4x16_16x8() [4/8]

v32acc32 negmul_4x16_16x8 | ( | v64int8 | a,
|  | v128uint4 | b )

Parameters

  a | Matrix A
  b | Matrix B

Returns
  Result of operation

## ◆ negmul_4x16_16x8() [5/8]

v32acc32 negmul_4x16_16x8 | ( | v64uint8 | a,
|  | int | sgn_x,
|  | v128int4 | b,
|  | int | sgn_y )

Parameters

  a | Matrix A
  sgn_x | Sign mask for matrix A
  b | Matrix B
  sgn_y | Sign mask for matrix B

Returns
  Result of operation

## ◆ negmul_4x16_16x8() [6/8]

v32acc32 negmul_4x16_16x8 | ( | v64uint8 | a,
|  | int | sgn_x,
|  | v128uint4 | b,
|  | int | sgn_y )

Parameters

  a | Matrix A
  sgn_x | Sign mask for matrix A
  b | Matrix B
  sgn_y | Sign mask for matrix B

Returns
  Result of operation

## ◆ negmul_4x16_16x8() [7/8]

v32acc32 negmul_4x16_16x8 | ( | v64uint8 | a,
|  | v128int4 | b )

Parameters

  a | Matrix A
  b | Matrix B

Returns
  Result of operation

## ◆ negmul_4x16_16x8() [8/8]

v32acc32 negmul_4x16_16x8 | ( | v64uint8 | a,
|  | v128uint4 | b )

Parameters

  a | Matrix A
  b | Matrix B

Returns
  Result of operation

## ◆ negmul_4x16_16x8_conf() [1/8]

v32acc32 negmul_4x16_16x8_conf | ( | v64int8 | a,
|  | int | sgn_x,
|  | v128int4 | b,
|  | int | sgn_y,
|  | int | sub_mul )

Parameters

  a | Matrix A
  sgn_x | Sign mask for matrix A
  b | Matrix B
  sgn_y | Sign mask for matrix B
  sub_mul | Negation mask of multiplication result

Returns
  Result of operation

## ◆ negmul_4x16_16x8_conf() [2/8]

v32acc32 negmul_4x16_16x8_conf | ( | v64int8 | a,
|  | int | sgn_x,
|  | v128uint4 | b,
|  | int | sgn_y,
|  | int | sub_mul )

Parameters

  a | Matrix A
  sgn_x | Sign mask for matrix A
  b | Matrix B
  sgn_y | Sign mask for matrix B
  sub_mul | Negation mask of multiplication result

Returns
  Result of operation

## ◆ negmul_4x16_16x8_conf() [3/8]

v32acc32 negmul_4x16_16x8_conf | ( | v64int8 | a,
|  | v128int4 | b,
|  | int | sub_mul )

Parameters

  a | Matrix A
  b | Matrix B
  sub_mul | Negation mask for multiplication result. If a bit of sub_mul is set the corresponding vector lane of the output accumulator will be negated.

Returns
  Result of operation

## ◆ negmul_4x16_16x8_conf() [4/8]

v32acc32 negmul_4x16_16x8_conf | ( | v64int8 | a,
|  | v128uint4 | b,
|  | int | sub_mul )

Parameters

  a | Matrix A
  b | Matrix B
  sub_mul | Negation mask for multiplication result. If a bit of sub_mul is set the corresponding vector lane of the output accumulator will be negated.

Returns
  Result of operation

## ◆ negmul_4x16_16x8_conf() [5/8]

v32acc32 negmul_4x16_16x8_conf | ( | v64uint8 | a,
|  | int | sgn_x,
|  | v128int4 | b,
|  | int | sgn_y,
|  | int | sub_mul )

Parameters

  a | Matrix A
  sgn_x | Sign mask for matrix A
  b | Matrix B
  sgn_y | Sign mask for matrix B
  sub_mul | Negation mask of multiplication result

Returns
  Result of operation

## ◆ negmul_4x16_16x8_conf() [6/8]

v32acc32 negmul_4x16_16x8_conf | ( | v64uint8 | a,
|  | int | sgn_x,
|  | v128uint4 | b,
|  | int | sgn_y,
|  | int | sub_mul )

Parameters

  a | Matrix A
  sgn_x | Sign mask for matrix A
  b | Matrix B
  sgn_y | Sign mask for matrix B
  sub_mul | Negation mask of multiplication result

Returns
  Result of operation

## ◆ negmul_4x16_16x8_conf() [7/8]

v32acc32 negmul_4x16_16x8_conf | ( | v64uint8 | a,
|  | v128int4 | b,
|  | int | sub_mul )

Parameters

  a | Matrix A
  b | Matrix B
  sub_mul | Negation mask for multiplication result. If a bit of sub_mul is set the corresponding vector lane of the output accumulator will be negated.

Returns
  Result of operation

## ◆ negmul_4x16_16x8_conf() [8/8]

v32acc32 negmul_4x16_16x8_conf | ( | v64uint8 | a,
|  | v128uint4 | b,
|  | int | sub_mul )

Parameters

  a | Matrix A
  b | Matrix B
  sub_mul | Negation mask for multiplication result. If a bit of sub_mul is set the corresponding vector lane of the output accumulator will be negated.

Returns
  Result of operation

## ◆ submac_4x16_16x8() [1/8]

v32acc32 submac_4x16_16x8 | ( | v64int8 | a,
|  | int | sgn_x,
|  | v128int4 | b,
|  | int | sgn_y,
|  | v32acc32 | acc1,
|  | v32acc32 | acc2 )

Parameters

  a | Matrix A
  sgn_x | Sign mask for matrix A
  b | Matrix B
  sgn_y | Sign mask for matrix B
  acc1 | Input accumulator 1
  acc2 | Input accumulator 2

Returns
  Result of operation

## ◆ submac_4x16_16x8() [2/8]

v32acc32 submac_4x16_16x8 | ( | v64int8 | a,
|  | int | sgn_x,
|  | v128uint4 | b,
|  | int | sgn_y,
|  | v32acc32 | acc1,
|  | v32acc32 | acc2 )

Parameters

  a | Matrix A
  sgn_x | Sign mask for matrix A
  b | Matrix B
  sgn_y | Sign mask for matrix B
  acc1 | Input accumulator 1
  acc2 | Input accumulator 2

Returns
  Result of operation

## ◆ submac_4x16_16x8() [3/8]

v32acc32 submac_4x16_16x8 | ( | v64int8 | a,
|  | v128int4 | b,
|  | v32acc32 | acc1,
|  | v32acc32 | acc2 )

Parameters

  a | Matrix A
  b | Matrix B
  acc1 | Input accumulator 1
  acc2 | Input accumulator 2

Returns
  Result of operation

## ◆ submac_4x16_16x8() [4/8]

v32acc32 submac_4x16_16x8 | ( | v64int8 | a,
|  | v128uint4 | b,
|  | v32acc32 | acc1,
|  | v32acc32 | acc2 )

Parameters

  a | Matrix A
  b | Matrix B
  acc1 | Input accumulator 1
  acc2 | Input accumulator 2

Returns
  Result of operation

## ◆ submac_4x16_16x8() [5/8]

v32acc32 submac_4x16_16x8 | ( | v64uint8 | a,
|  | int | sgn_x,
|  | v128int4 | b,
|  | int | sgn_y,
|  | v32acc32 | acc1,
|  | v32acc32 | acc2 )

Parameters

  a | Matrix A
  sgn_x | Sign mask for matrix A
  b | Matrix B
  sgn_y | Sign mask for matrix B
  acc1 | Input accumulator 1
  acc2 | Input accumulator 2

Returns
  Result of operation

## ◆ submac_4x16_16x8() [6/8]

v32acc32 submac_4x16_16x8 | ( | v64uint8 | a,
|  | int | sgn_x,
|  | v128uint4 | b,
|  | int | sgn_y,
|  | v32acc32 | acc1,
|  | v32acc32 | acc2 )

Parameters

  a | Matrix A
  sgn_x | Sign mask for matrix A
  b | Matrix B
  sgn_y | Sign mask for matrix B
  acc1 | Input accumulator 1
  acc2 | Input accumulator 2

Returns
  Result of operation

## ◆ submac_4x16_16x8() [7/8]

v32acc32 submac_4x16_16x8 | ( | v64uint8 | a,
|  | v128int4 | b,
|  | v32acc32 | acc1,
|  | v32acc32 | acc2 )

Parameters

  a | Matrix A
  b | Matrix B
  acc1 | Input accumulator 1
  acc2 | Input accumulator 2

Returns
  Result of operation

## ◆ submac_4x16_16x8() [8/8]

v32acc32 submac_4x16_16x8 | ( | v64uint8 | a,
|  | v128uint4 | b,
|  | v32acc32 | acc1,
|  | v32acc32 | acc2 )

Parameters

  a | Matrix A
  b | Matrix B
  acc1 | Input accumulator 1
  acc2 | Input accumulator 2

Returns
  Result of operation

## ◆ submac_4x16_16x8_conf() [1/8]

v32acc32 submac_4x16_16x8_conf | ( | v64int8 | a,
|  | int | sgn_x,
|  | v128int4 | b,
|  | int | sgn_y,
|  | v32acc32 | acc1,
|  | v32acc32 | acc2,
|  | int | zero_acc1,
|  | int | sub_mul,
|  | int | sub_acc1,
|  | int | sub_acc2 )

Parameters

  a | Matrix A
  sgn_x | Sign mask for matrix A
  b | Matrix B
  sgn_y | Sign mask for matrix B
  acc1 | Input accumulator 1
  acc2 | Input accumulator 2
  zero_acc1 | Zeroing mask for acc1
  sub_mul | Negation mask of multiplication result
  sub_acc1 | Negation mask of acc1

Returns
  Result of operation

## ◆ submac_4x16_16x8_conf() [2/8]

v32acc32 submac_4x16_16x8_conf | ( | v64int8 | a,
|  | int | sgn_x,
|  | v128uint4 | b,
|  | int | sgn_y,
|  | v32acc32 | acc1,
|  | v32acc32 | acc2,
|  | int | zero_acc1,
|  | int | sub_mul,
|  | int | sub_acc1,
|  | int | sub_acc2 )

Parameters

  a | Matrix A
  sgn_x | Sign mask for matrix A
  b | Matrix B
  sgn_y | Sign mask for matrix B
  acc1 | Input accumulator 1
  acc2 | Input accumulator 2
  zero_acc1 | Zeroing mask for acc1
  sub_mul | Negation mask of multiplication result
  sub_acc1 | Negation mask of acc1

Returns
  Result of operation

## ◆ submac_4x16_16x8_conf() [3/8]

v32acc32 submac_4x16_16x8_conf | ( | v64int8 | a,
|  | v128int4 | b,
|  | v32acc32 | acc1,
|  | v32acc32 | acc2,
|  | int | zero_acc1,
|  | int | sub_mul,
|  | int | sub_acc1,
|  | int | sub_acc2 )

Parameters

  a | Matrix A
  b | Matrix B
  acc1 | Input accumulator 1
  acc2 | Input accumulator 2
  zero_acc1 | Zeroing mask for acc1
  sub_mul | Negation mask of multiplication result
  sub_acc1 | Negation mask of acc1

Returns
  Result of operation

## ◆ submac_4x16_16x8_conf() [4/8]

v32acc32 submac_4x16_16x8_conf | ( | v64int8 | a,
|  | v128uint4 | b,
|  | v32acc32 | acc1,
|  | v32acc32 | acc2,
|  | int | zero_acc1,
|  | int | sub_mul,
|  | int | sub_acc1,
|  | int | sub_acc2 )

Parameters

  a | Matrix A
  b | Matrix B
  acc1 | Input accumulator 1
  acc2 | Input accumulator 2
  zero_acc1 | Zeroing mask for acc1
  sub_mul | Negation mask of multiplication result
  sub_acc1 | Negation mask of acc1

Returns
  Result of operation

## ◆ submac_4x16_16x8_conf() [5/8]

v32acc32 submac_4x16_16x8_conf | ( | v64uint8 | a,
|  | int | sgn_x,
|  | v128int4 | b,
|  | int | sgn_y,
|  | v32acc32 | acc1,
|  | v32acc32 | acc2,
|  | int | zero_acc1,
|  | int | sub_mul,
|  | int | sub_acc1,
|  | int | sub_acc2 )

Parameters

  a | Matrix A
  sgn_x | Sign mask for matrix A
  b | Matrix B
  sgn_y | Sign mask for matrix B
  acc1 | Input accumulator 1
  acc2 | Input accumulator 2
  zero_acc1 | Zeroing mask for acc1
  sub_mul | Negation mask of multiplication result
  sub_acc1 | Negation mask of acc1

Returns
  Result of operation

## ◆ submac_4x16_16x8_conf() [6/8]

v32acc32 submac_4x16_16x8_conf | ( | v64uint8 | a,
|  | int | sgn_x,
|  | v128uint4 | b,
|  | int | sgn_y,
|  | v32acc32 | acc1,
|  | v32acc32 | acc2,
|  | int | zero_acc1,
|  | int | sub_mul,
|  | int | sub_acc1,
|  | int | sub_acc2 )

Parameters

  a | Matrix A
  sgn_x | Sign mask for matrix A
  b | Matrix B
  sgn_y | Sign mask for matrix B
  acc1 | Input accumulator 1
  acc2 | Input accumulator 2
  zero_acc1 | Zeroing mask for acc1
  sub_mul | Negation mask of multiplication result
  sub_acc1 | Negation mask of acc1

Returns
  Result of operation

## ◆ submac_4x16_16x8_conf() [7/8]

v32acc32 submac_4x16_16x8_conf | ( | v64uint8 | a,
|  | v128int4 | b,
|  | v32acc32 | acc1,
|  | v32acc32 | acc2,
|  | int | zero_acc1,
|  | int | sub_mul,
|  | int | sub_acc1,
|  | int | sub_acc2 )

Parameters

  a | Matrix A
  b | Matrix B
  acc1 | Input accumulator 1
  acc2 | Input accumulator 2
  zero_acc1 | Zeroing mask for acc1
  sub_mul | Negation mask of multiplication result
  sub_acc1 | Negation mask of acc1

Returns
  Result of operation

## ◆ submac_4x16_16x8_conf() [8/8]

v32acc32 submac_4x16_16x8_conf | ( | v64uint8 | a,
|  | v128uint4 | b,
|  | v32acc32 | acc1,
|  | v32acc32 | acc2,
|  | int | zero_acc1,
|  | int | sub_mul,
|  | int | sub_acc1,
|  | int | sub_acc2 )

Parameters

  a | Matrix A
  b | Matrix B
  acc1 | Input accumulator 1
  acc2 | Input accumulator 2
  zero_acc1 | Zeroing mask for acc1
  sub_mul | Negation mask of multiplication result
  sub_acc1 | Negation mask of acc1

Returns
  Result of operation

## ◆ submsc_4x16_16x8() [1/8]

v32acc32 submsc_4x16_16x8 | ( | v64int8 | a,
|  | int | sgn_x,
|  | v128int4 | b,
|  | int | sgn_y,
|  | v32acc32 | acc1,
|  | v32acc32 | acc2 )

Parameters

  a | Matrix A
  sgn_x | Sign mask for matrix A
  b | Matrix B
  sgn_y | Sign mask for matrix B
  acc1 | Input accumulator 1
  acc2 | Input accumulator 2

Returns
  Result of operation

## ◆ submsc_4x16_16x8() [2/8]

v32acc32 submsc_4x16_16x8 | ( | v64int8 | a,
|  | int | sgn_x,
|  | v128uint4 | b,
|  | int | sgn_y,
|  | v32acc32 | acc1,
|  | v32acc32 | acc2 )

Parameters

  a | Matrix A
  sgn_x | Sign mask for matrix A
  b | Matrix B
  sgn_y | Sign mask for matrix B
  acc1 | Input accumulator 1
  acc2 | Input accumulator 2

Returns
  Result of operation

## ◆ submsc_4x16_16x8() [3/8]

v32acc32 submsc_4x16_16x8 | ( | v64int8 | a,
|  | v128int4 | b,
|  | v32acc32 | acc1,
|  | v32acc32 | acc2 )

Parameters

  a | Matrix A
  b | Matrix B
  acc1 | Input accumulator 1
  acc2 | Input accumulator 2

Returns
  Result of operation

## ◆ submsc_4x16_16x8() [4/8]

v32acc32 submsc_4x16_16x8 | ( | v64int8 | a,
|  | v128uint4 | b,
|  | v32acc32 | acc1,
|  | v32acc32 | acc2 )

Parameters

  a | Matrix A
  b | Matrix B
  acc1 | Input accumulator 1
  acc2 | Input accumulator 2

Returns
  Result of operation

## ◆ submsc_4x16_16x8() [5/8]

v32acc32 submsc_4x16_16x8 | ( | v64uint8 | a,
|  | int | sgn_x,
|  | v128int4 | b,
|  | int | sgn_y,
|  | v32acc32 | acc1,
|  | v32acc32 | acc2 )

Parameters

  a | Matrix A
  sgn_x | Sign mask for matrix A
  b | Matrix B
  sgn_y | Sign mask for matrix B
  acc1 | Input accumulator 1
  acc2 | Input accumulator 2

Returns
  Result of operation

## ◆ submsc_4x16_16x8() [6/8]

v32acc32 submsc_4x16_16x8 | ( | v64uint8 | a,
|  | int | sgn_x,
|  | v128uint4 | b,
|  | int | sgn_y,
|  | v32acc32 | acc1,
|  | v32acc32 | acc2 )

Parameters

  a | Matrix A
  sgn_x | Sign mask for matrix A
  b | Matrix B
  sgn_y | Sign mask for matrix B
  acc1 | Input accumulator 1
  acc2 | Input accumulator 2

Returns
  Result of operation

## ◆ submsc_4x16_16x8() [7/8]

v32acc32 submsc_4x16_16x8 | ( | v64uint8 | a,
|  | v128int4 | b,
|  | v32acc32 | acc1,
|  | v32acc32 | acc2 )

Parameters

  a | Matrix A
  b | Matrix B
  acc1 | Input accumulator 1
  acc2 | Input accumulator 2

Returns
  Result of operation

## ◆ submsc_4x16_16x8() [8/8]

v32acc32 submsc_4x16_16x8 | ( | v64uint8 | a,
|  | v128uint4 | b,
|  | v32acc32 | acc1,
|  | v32acc32 | acc2 )

Parameters

  a | Matrix A
  b | Matrix B
  acc1 | Input accumulator 1
  acc2 | Input accumulator 2

Returns
  Result of operation

## ◆ submsc_4x16_16x8_conf() [1/8]

v32acc32 submsc_4x16_16x8_conf | ( | v64int8 | a,
|  | int | sgn_x,
|  | v128int4 | b,
|  | int | sgn_y,
|  | v32acc32 | acc1,
|  | v32acc32 | acc2,
|  | int | zero_acc1,
|  | int | sub_mul,
|  | int | sub_acc1,
|  | int | sub_acc2 )

Parameters

  a | Matrix A
  sgn_x | Sign mask for matrix A
  b | Matrix B
  sgn_y | Sign mask for matrix B
  acc1 | Input accumulator 1
  acc2 | Input accumulator 2
  zero_acc1 | Zeroing mask for acc1
  sub_mul | Negation mask of multiplication result
  sub_acc1 | Negation mask of acc1

Returns
  Result of operation

## ◆ submsc_4x16_16x8_conf() [2/8]

v32acc32 submsc_4x16_16x8_conf | ( | v64int8 | a,
|  | int | sgn_x,
|  | v128uint4 | b,
|  | int | sgn_y,
|  | v32acc32 | acc1,
|  | v32acc32 | acc2,
|  | int | zero_acc1,
|  | int | sub_mul,
|  | int | sub_acc1,
|  | int | sub_acc2 )

Parameters

  a | Matrix A
  sgn_x | Sign mask for matrix A
  b | Matrix B
  sgn_y | Sign mask for matrix B
  acc1 | Input accumulator 1
  acc2 | Input accumulator 2
  zero_acc1 | Zeroing mask for acc1
  sub_mul | Negation mask of multiplication result
  sub_acc1 | Negation mask of acc1

Returns
  Result of operation

## ◆ submsc_4x16_16x8_conf() [3/8]

v32acc32 submsc_4x16_16x8_conf | ( | v64int8 | a,
|  | v128int4 | b,
|  | v32acc32 | acc1,
|  | v32acc32 | acc2,
|  | int | zero_acc1,
|  | int | sub_mul,
|  | int | sub_acc1,
|  | int | sub_acc2 )

Parameters

  a | Matrix A
  b | Matrix B
  acc1 | Input accumulator 1
  acc2 | Input accumulator 2
  zero_acc1 | Zeroing mask for acc1
  sub_mul | Negation mask of multiplication result
  sub_acc1 | Negation mask of acc1

Returns
  Result of operation

## ◆ submsc_4x16_16x8_conf() [4/8]

v32acc32 submsc_4x16_16x8_conf | ( | v64int8 | a,
|  | v128uint4 | b,
|  | v32acc32 | acc1,
|  | v32acc32 | acc2,
|  | int | zero_acc1,
|  | int | sub_mul,
|  | int | sub_acc1,
|  | int | sub_acc2 )

Parameters

  a | Matrix A
  b | Matrix B
  acc1 | Input accumulator 1
  acc2 | Input accumulator 2
  zero_acc1 | Zeroing mask for acc1
  sub_mul | Negation mask of multiplication result
  sub_acc1 | Negation mask of acc1

Returns
  Result of operation

## ◆ submsc_4x16_16x8_conf() [5/8]

v32acc32 submsc_4x16_16x8_conf | ( | v64uint8 | a,
|  | int | sgn_x,
|  | v128int4 | b,
|  | int | sgn_y,
|  | v32acc32 | acc1,
|  | v32acc32 | acc2,
|  | int | zero_acc1,
|  | int | sub_mul,
|  | int | sub_acc1,
|  | int | sub_acc2 )

Parameters

  a | Matrix A
  sgn_x | Sign mask for matrix A
  b | Matrix B
  sgn_y | Sign mask for matrix B
  acc1 | Input accumulator 1
  acc2 | Input accumulator 2
  zero_acc1 | Zeroing mask for acc1
  sub_mul | Negation mask of multiplication result
  sub_acc1 | Negation mask of acc1

Returns
  Result of operation

## ◆ submsc_4x16_16x8_conf() [6/8]

v32acc32 submsc_4x16_16x8_conf | ( | v64uint8 | a,
|  | int | sgn_x,
|  | v128uint4 | b,
|  | int | sgn_y,
|  | v32acc32 | acc1,
|  | v32acc32 | acc2,
|  | int | zero_acc1,
|  | int | sub_mul,
|  | int | sub_acc1,
|  | int | sub_acc2 )

Parameters

  a | Matrix A
  sgn_x | Sign mask for matrix A
  b | Matrix B
  sgn_y | Sign mask for matrix B
  acc1 | Input accumulator 1
  acc2 | Input accumulator 2
  zero_acc1 | Zeroing mask for acc1
  sub_mul | Negation mask of multiplication result
  sub_acc1 | Negation mask of acc1

Returns
  Result of operation

## ◆ submsc_4x16_16x8_conf() [7/8]

v32acc32 submsc_4x16_16x8_conf | ( | v64uint8 | a,
|  | v128int4 | b,
|  | v32acc32 | acc1,
|  | v32acc32 | acc2,
|  | int | zero_acc1,
|  | int | sub_mul,
|  | int | sub_acc1,
|  | int | sub_acc2 )

Parameters

  a | Matrix A
  b | Matrix B
  acc1 | Input accumulator 1
  acc2 | Input accumulator 2
  zero_acc1 | Zeroing mask for acc1
  sub_mul | Negation mask of multiplication result
  sub_acc1 | Negation mask of acc1

Returns
  Result of operation

## ◆ submsc_4x16_16x8_conf() [8/8]

v32acc32 submsc_4x16_16x8_conf | ( | v64uint8 | a,
|  | v128uint4 | b,
|  | v32acc32 | acc1,
|  | v32acc32 | acc2,
|  | int | zero_acc1,
|  | int | sub_mul,
|  | int | sub_acc1,
|  | int | sub_acc2 )

Parameters

  a | Matrix A
  b | Matrix B
  acc1 | Input accumulator 1
  acc2 | Input accumulator 2
  zero_acc1 | Zeroing mask for acc1
  sub_mul | Negation mask of multiplication result
  sub_acc1 | Negation mask of acc1

Returns
  Result of operation