| AI Engine-ML v2 Intrinsics User Guide v2025.2

Loading...
Searching...
No Matches
Emulated Multiply-accumulate of 32b x 16b datatypes
Vector Operations » Multiply Accumulate

Matrix multiplications in which matrix A has data elements of 32 bit and matrix B has data elements of 16 bit. These operations are emulated on top of Multiply-accumulate of 16b x 16b integer datatypes and might not have optimal performance. More...

## Emulated Multiplication of (8x2) with (2x8) Matrices (32b * 16b)
v64acc32 | mul_8x2_2x8 (v16uint32 a0, v32uint16 b)
v64acc32 | negmul_8x2_2x8 (v16uint32 a0, v32uint16 b)
v64acc32 | mac_8x2_2x8 (v16uint32 a0, v32uint16 b, v64acc32 acc1)
v64acc32 | msc_8x2_2x8 (v16uint32 a0, v32uint16 b, v64acc32 acc1)
v64acc32 | mul_8x2_2x8 (v16uint32 a0, v32int16 b)
v64acc32 | negmul_8x2_2x8 (v16uint32 a0, v32int16 b)
v64acc32 | mac_8x2_2x8 (v16uint32 a0, v32int16 b, v64acc32 acc1)
v64acc32 | msc_8x2_2x8 (v16uint32 a0, v32int16 b, v64acc32 acc1)
v64acc32 | mul_8x2_2x8 (v16int32 a0, v32uint16 b)
v64acc32 | negmul_8x2_2x8 (v16int32 a0, v32uint16 b)
v64acc32 | mac_8x2_2x8 (v16int32 a0, v32uint16 b, v64acc32 acc1)
v64acc32 | msc_8x2_2x8 (v16int32 a0, v32uint16 b, v64acc32 acc1)
v64acc32 | mul_8x2_2x8 (v16int32 a0, v32int16 b)
v64acc32 | negmul_8x2_2x8 (v16int32 a0, v32int16 b)
v64acc32 | mac_8x2_2x8 (v16int32 a0, v32int16 b, v64acc32 acc1)
v64acc32 | msc_8x2_2x8 (v16int32 a0, v32int16 b, v64acc32 acc1)

## Emulated Multiplication of (8x2) with (2x8) Matrices (32b * 16b) with dynamic sign
v64acc32 | mul_8x2_2x8 (v16uint32 a0, int sgn_x, v32uint16 b, int sgn_y)
v64acc32 | negmul_8x2_2x8 (v16uint32 a0, int sgn_x, v32uint16 b, int sgn_y)
v64acc32 | mac_8x2_2x8 (v16uint32 a0, int sgn_x, v32uint16 b, int sgn_y, v64acc32 acc1)
v64acc32 | msc_8x2_2x8 (v16uint32 a0, int sgn_x, v32uint16 b, int sgn_y, v64acc32 acc1)
v64acc32 | mul_8x2_2x8 (v16uint32 a0, int sgn_x, v32int16 b, int sgn_y)
v64acc32 | negmul_8x2_2x8 (v16uint32 a0, int sgn_x, v32int16 b, int sgn_y)
v64acc32 | mac_8x2_2x8 (v16uint32 a0, int sgn_x, v32int16 b, int sgn_y, v64acc32 acc1)
v64acc32 | msc_8x2_2x8 (v16uint32 a0, int sgn_x, v32int16 b, int sgn_y, v64acc32 acc1)
v64acc32 | mul_8x2_2x8 (v16int32 a0, int sgn_x, v32uint16 b, int sgn_y)
v64acc32 | negmul_8x2_2x8 (v16int32 a0, int sgn_x, v32uint16 b, int sgn_y)
v64acc32 | mac_8x2_2x8 (v16int32 a0, int sgn_x, v32uint16 b, int sgn_y, v64acc32 acc1)
v64acc32 | msc_8x2_2x8 (v16int32 a0, int sgn_x, v32uint16 b, int sgn_y, v64acc32 acc1)
v64acc32 | mul_8x2_2x8 (v16int32 a0, int sgn_x, v32int16 b, int sgn_y)
v64acc32 | negmul_8x2_2x8 (v16int32 a0, int sgn_x, v32int16 b, int sgn_y)
v64acc32 | mac_8x2_2x8 (v16int32 a0, int sgn_x, v32int16 b, int sgn_y, v64acc32 acc1)
v64acc32 | msc_8x2_2x8 (v16int32 a0, int sgn_x, v32int16 b, int sgn_y, v64acc32 acc1)

## Emulated Multiplication of (8x2) with (2x8) Matrices (32b * 16b) with dynamic negation of multiplication result
v64acc32 | mul_8x2_2x8_conf (v16uint32 a0, v32uint16 b, int sub_mul)
v64acc32 | negmul_8x2_2x8_conf (v16uint32 a0, v32uint16 b, int sub_mul)
v64acc32 | mul_8x2_2x8_conf (v16uint32 a0, v32int16 b, int sub_mul)
v64acc32 | negmul_8x2_2x8_conf (v16uint32 a0, v32int16 b, int sub_mul)
v64acc32 | mul_8x2_2x8_conf (v16int32 a0, v32uint16 b, int sub_mul)
v64acc32 | negmul_8x2_2x8_conf (v16int32 a0, v32uint16 b, int sub_mul)
v64acc32 | mul_8x2_2x8_conf (v16int32 a0, v32int16 b, int sub_mul)
v64acc32 | negmul_8x2_2x8_conf (v16int32 a0, v32int16 b, int sub_mul)

## Emulated Multiplication of (8x2) with (2x8) Matrices (32b * 16b) with dynamic negation of multiplication result, negation of acc1
v64acc32 | mac_8x2_2x8_conf (v16uint32 a0, v32uint16 b, v64acc32 acc1, int sub_mul, int sub_acc1)
v64acc32 | msc_8x2_2x8_conf (v16uint32 a0, v32uint16 b, v64acc32 acc1, int sub_mul, int sub_acc1)
v64acc32 | mac_8x2_2x8_conf (v16uint32 a0, v32int16 b, v64acc32 acc1, int sub_mul, int sub_acc1)
v64acc32 | msc_8x2_2x8_conf (v16uint32 a0, v32int16 b, v64acc32 acc1, int sub_mul, int sub_acc1)
v64acc32 | mac_8x2_2x8_conf (v16int32 a0, v32uint16 b, v64acc32 acc1, int sub_mul, int sub_acc1)
v64acc32 | msc_8x2_2x8_conf (v16int32 a0, v32uint16 b, v64acc32 acc1, int sub_mul, int sub_acc1)
v64acc32 | mac_8x2_2x8_conf (v16int32 a0, v32int16 b, v64acc32 acc1, int sub_mul, int sub_acc1)
v64acc32 | msc_8x2_2x8_conf (v16int32 a0, v32int16 b, v64acc32 acc1, int sub_mul, int sub_acc1)

## Emulated Multiplication of (8x2) with (2x8) Matrices (32b * 16b) with dynamic sign and dynamic negation of multiplication result
v64acc32 | mul_8x2_2x8_conf (v16uint32 a0, int sgn_x, v32uint16 b, int sgn_y, int sub_mul)
v64acc32 | negmul_8x2_2x8_conf (v16uint32 a0, int sgn_x, v32uint16 b, int sgn_y, int sub_mul)
v64acc32 | mac_8x2_2x8_conf (v16uint32 a0, int sgn_x, v32uint16 b, int sgn_y, v64acc32 acc1, int sub_mul, int sub_acc1)
v64acc32 | msc_8x2_2x8_conf (v16uint32 a0, int sgn_x, v32uint16 b, int sgn_y, v64acc32 acc1, int sub_mul, int sub_acc1)
v64acc32 | mul_8x2_2x8_conf (v16uint32 a0, int sgn_x, v32int16 b, int sgn_y, int sub_mul)
v64acc32 | negmul_8x2_2x8_conf (v16uint32 a0, int sgn_x, v32int16 b, int sgn_y, int sub_mul)
v64acc32 | mac_8x2_2x8_conf (v16uint32 a0, int sgn_x, v32int16 b, int sgn_y, v64acc32 acc1, int sub_mul, int sub_acc1)
v64acc32 | msc_8x2_2x8_conf (v16uint32 a0, int sgn_x, v32int16 b, int sgn_y, v64acc32 acc1, int sub_mul, int sub_acc1)
v64acc32 | mul_8x2_2x8_conf (v16int32 a0, int sgn_x, v32uint16 b, int sgn_y, int sub_mul)
v64acc32 | negmul_8x2_2x8_conf (v16int32 a0, int sgn_x, v32uint16 b, int sgn_y, int sub_mul)
v64acc32 | mac_8x2_2x8_conf (v16int32 a0, int sgn_x, v32uint16 b, int sgn_y, v64acc32 acc1, int sub_mul, int sub_acc1)
v64acc32 | msc_8x2_2x8_conf (v16int32 a0, int sgn_x, v32uint16 b, int sgn_y, v64acc32 acc1, int sub_mul, int sub_acc1)
v64acc32 | mul_8x2_2x8_conf (v16int32 a0, int sgn_x, v32int16 b, int sgn_y, int sub_mul)
v64acc32 | negmul_8x2_2x8_conf (v16int32 a0, int sgn_x, v32int16 b, int sgn_y, int sub_mul)
v64acc32 | mac_8x2_2x8_conf (v16int32 a0, int sgn_x, v32int16 b, int sgn_y, v64acc32 acc1, int sub_mul, int sub_acc1)
v64acc32 | msc_8x2_2x8_conf (v16int32 a0, int sgn_x, v32int16 b, int sgn_y, v64acc32 acc1, int sub_mul, int sub_acc1)

## Emulated Multiplication of (8x2) with (2x8) Matrices (32b * 16b) with dynamic negation of multiplication result, negation of acc1 and zeroing of acc1
v64acc32 | mac_8x2_2x8_conf (v16uint32 a0, v32uint16 b, v64acc32 acc1, int zero_acc1, int sub_mul, int sub_acc1)
v64acc32 | msc_8x2_2x8_conf (v16uint32 a0, v32uint16 b, v64acc32 acc1, int zero_acc1, int sub_mul, int sub_acc1)
v64acc32 | mac_8x2_2x8_conf (v16uint32 a0, v32int16 b, v64acc32 acc1, int zero_acc1, int sub_mul, int sub_acc1)
v64acc32 | msc_8x2_2x8_conf (v16uint32 a0, v32int16 b, v64acc32 acc1, int zero_acc1, int sub_mul, int sub_acc1)
v64acc32 | mac_8x2_2x8_conf (v16int32 a0, v32uint16 b, v64acc32 acc1, int zero_acc1, int sub_mul, int sub_acc1)
v64acc32 | msc_8x2_2x8_conf (v16int32 a0, v32uint16 b, v64acc32 acc1, int zero_acc1, int sub_mul, int sub_acc1)
v64acc32 | mac_8x2_2x8_conf (v16int32 a0, v32int16 b, v64acc32 acc1, int zero_acc1, int sub_mul, int sub_acc1)
v64acc32 | msc_8x2_2x8_conf (v16int32 a0, v32int16 b, v64acc32 acc1, int zero_acc1, int sub_mul, int sub_acc1)

## Emulated Multiplication of (8x2) with (2x8) Matrices (32b * 16b) with dynamic sign, zeroing of acc1 and dynamic negation of multiplication result
v64acc32 | mac_8x2_2x8_conf (v16uint32 a0, int sgn_x, v32uint16 b, int sgn_y, v64acc32 acc1, int zero_acc1, int sub_mul, int sub_acc1)
v64acc32 | msc_8x2_2x8_conf (v16uint32 a0, int sgn_x, v32uint16 b, int sgn_y, v64acc32 acc1, int zero_acc1, int sub_mul, int sub_acc1)
v64acc32 | mac_8x2_2x8_conf (v16uint32 a0, int sgn_x, v32int16 b, int sgn_y, v64acc32 acc1, int zero_acc1, int sub_mul, int sub_acc1)
v64acc32 | msc_8x2_2x8_conf (v16uint32 a0, int sgn_x, v32int16 b, int sgn_y, v64acc32 acc1, int zero_acc1, int sub_mul, int sub_acc1)
v64acc32 | mac_8x2_2x8_conf (v16int32 a0, int sgn_x, v32uint16 b, int sgn_y, v64acc32 acc1, int zero_acc1, int sub_mul, int sub_acc1)
v64acc32 | msc_8x2_2x8_conf (v16int32 a0, int sgn_x, v32uint16 b, int sgn_y, v64acc32 acc1, int zero_acc1, int sub_mul, int sub_acc1)
v64acc32 | mac_8x2_2x8_conf (v16int32 a0, int sgn_x, v32int16 b, int sgn_y, v64acc32 acc1, int zero_acc1, int sub_mul, int sub_acc1)
v64acc32 | msc_8x2_2x8_conf (v16int32 a0, int sgn_x, v32int16 b, int sgn_y, v64acc32 acc1, int zero_acc1, int sub_mul, int sub_acc1)

## Emulated Channel by channel multiplication of (1x1) with (1x1) (32b * 16b)
v32acc64 | mul_4x4_4x8 (v16uint32 a0, v32uint16 b)
v32acc64 | negmul_4x4_4x8 (v16uint32 a0, v32uint16 b)
v32acc64 | mac_4x4_4x8 (v16uint32 a0, v32uint16 b, v32acc64 acc1)
v32acc64 | msc_4x4_4x8 (v16uint32 a0, v32uint16 b, v32acc64 acc1)
v32acc64 | mul_4x4_4x8 (v16uint32 a0, v32int16 b)
v32acc64 | negmul_4x4_4x8 (v16uint32 a0, v32int16 b)
v32acc64 | mac_4x4_4x8 (v16uint32 a0, v32int16 b, v32acc64 acc1)
v32acc64 | msc_4x4_4x8 (v16uint32 a0, v32int16 b, v32acc64 acc1)
v32acc64 | mul_4x4_4x8 (v16int32 a0, v32uint16 b)
v32acc64 | negmul_4x4_4x8 (v16int32 a0, v32uint16 b)
v32acc64 | mac_4x4_4x8 (v16int32 a0, v32uint16 b, v32acc64 acc1)
v32acc64 | msc_4x4_4x8 (v16int32 a0, v32uint16 b, v32acc64 acc1)
v32acc64 | mul_4x4_4x8 (v16int32 a0, v32int16 b)
v32acc64 | negmul_4x4_4x8 (v16int32 a0, v32int16 b)
v32acc64 | mac_4x4_4x8 (v16int32 a0, v32int16 b, v32acc64 acc1)
v32acc64 | msc_4x4_4x8 (v16int32 a0, v32int16 b, v32acc64 acc1)
v32acc64 | mul_elem_32 (v16uint32 a0, v16uint32 a1, v32uint16 b)
v32acc64 | negmul_elem_32 (v16uint32 a0, v16uint32 a1, v32uint16 b)
v32acc64 | mac_elem_32 (v16uint32 a0, v16uint32 a1, v32uint16 b, v32acc64 acc1)
v32acc64 | msc_elem_32 (v16uint32 a0, v16uint32 a1, v32uint16 b, v32acc64 acc1)
v32acc64 | mul_elem_32 (v16uint32 a0, v16uint32 a1, v32int16 b)
v32acc64 | negmul_elem_32 (v16uint32 a0, v16uint32 a1, v32int16 b)
v32acc64 | mac_elem_32 (v16uint32 a0, v16uint32 a1, v32int16 b, v32acc64 acc1)
v32acc64 | msc_elem_32 (v16uint32 a0, v16uint32 a1, v32int16 b, v32acc64 acc1)
v32acc64 | mul_elem_32 (v16int32 a0, v16int32 a1, v32uint16 b)
v32acc64 | negmul_elem_32 (v16int32 a0, v16int32 a1, v32uint16 b)
v32acc64 | mac_elem_32 (v16int32 a0, v16int32 a1, v32uint16 b, v32acc64 acc1)
v32acc64 | msc_elem_32 (v16int32 a0, v16int32 a1, v32uint16 b, v32acc64 acc1)
v32acc64 | mul_elem_32 (v16int32 a0, v16int32 a1, v32int16 b)
v32acc64 | negmul_elem_32 (v16int32 a0, v16int32 a1, v32int16 b)
v32acc64 | mac_elem_32 (v16int32 a0, v16int32 a1, v32int16 b, v32acc64 acc1)
v32acc64 | msc_elem_32 (v16int32 a0, v16int32 a1, v32int16 b, v32acc64 acc1)
v32acc64 | mul_conv_4x4_8ch (v32uint32 a0, v32uint32 a1, v32uint16 b)
v32acc64 | negmul_conv_4x4_8ch (v32uint32 a0, v32uint32 a1, v32uint16 b)
v32acc64 | mac_conv_4x4_8ch (v32uint32 a0, v32uint32 a1, v32uint16 b, v32acc64 acc1)
v32acc64 | msc_conv_4x4_8ch (v32uint32 a0, v32uint32 a1, v32uint16 b, v32acc64 acc1)
v32acc64 | mul_conv_4x4_8ch (v32uint32 a0, v32uint32 a1, v32int16 b)
v32acc64 | negmul_conv_4x4_8ch (v32uint32 a0, v32uint32 a1, v32int16 b)
v32acc64 | mac_conv_4x4_8ch (v32uint32 a0, v32uint32 a1, v32int16 b, v32acc64 acc1)
v32acc64 | msc_conv_4x4_8ch (v32uint32 a0, v32uint32 a1, v32int16 b, v32acc64 acc1)
v32acc64 | mul_conv_4x4_8ch (v32int32 a0, v32int32 a1, v32uint16 b)
v32acc64 | negmul_conv_4x4_8ch (v32int32 a0, v32int32 a1, v32uint16 b)
v32acc64 | mac_conv_4x4_8ch (v32int32 a0, v32int32 a1, v32uint16 b, v32acc64 acc1)
v32acc64 | msc_conv_4x4_8ch (v32int32 a0, v32int32 a1, v32uint16 b, v32acc64 acc1)
v32acc64 | mul_conv_4x4_8ch (v32int32 a0, v32int32 a1, v32int16 b)
v32acc64 | negmul_conv_4x4_8ch (v32int32 a0, v32int32 a1, v32int16 b)
v32acc64 | mac_conv_4x4_8ch (v32int32 a0, v32int32 a1, v32int16 b, v32acc64 acc1)
v32acc64 | msc_conv_4x4_8ch (v32int32 a0, v32int32 a1, v32int16 b, v32acc64 acc1)

## Emulated Channel by channel multiplication of (1x1) with (1x1) (32b * 16b) with dynamic sign
v32acc64 | mul_4x4_4x8 (v16uint32 a0, int sgn_x, v32uint16 b, int sgn_y)
v32acc64 | negmul_4x4_4x8 (v16uint32 a0, int sgn_x, v32uint16 b, int sgn_y)
v32acc64 | mac_4x4_4x8 (v16uint32 a0, int sgn_x, v32uint16 b, int sgn_y, v32acc64 acc1)
v32acc64 | msc_4x4_4x8 (v16uint32 a0, int sgn_x, v32uint16 b, int sgn_y, v32acc64 acc1)
v32acc64 | mul_4x4_4x8 (v16uint32 a0, int sgn_x, v32int16 b, int sgn_y)
v32acc64 | negmul_4x4_4x8 (v16uint32 a0, int sgn_x, v32int16 b, int sgn_y)
v32acc64 | mac_4x4_4x8 (v16uint32 a0, int sgn_x, v32int16 b, int sgn_y, v32acc64 acc1)
v32acc64 | msc_4x4_4x8 (v16uint32 a0, int sgn_x, v32int16 b, int sgn_y, v32acc64 acc1)
v32acc64 | mul_4x4_4x8 (v16int32 a0, int sgn_x, v32uint16 b, int sgn_y)
v32acc64 | negmul_4x4_4x8 (v16int32 a0, int sgn_x, v32uint16 b, int sgn_y)
v32acc64 | mac_4x4_4x8 (v16int32 a0, int sgn_x, v32uint16 b, int sgn_y, v32acc64 acc1)
v32acc64 | msc_4x4_4x8 (v16int32 a0, int sgn_x, v32uint16 b, int sgn_y, v32acc64 acc1)
v32acc64 | mul_4x4_4x8 (v16int32 a0, int sgn_x, v32int16 b, int sgn_y)
v32acc64 | negmul_4x4_4x8 (v16int32 a0, int sgn_x, v32int16 b, int sgn_y)
v32acc64 | mac_4x4_4x8 (v16int32 a0, int sgn_x, v32int16 b, int sgn_y, v32acc64 acc1)
v32acc64 | msc_4x4_4x8 (v16int32 a0, int sgn_x, v32int16 b, int sgn_y, v32acc64 acc1)
v32acc64 | mul_elem_32 (v16uint32 a0, v16uint32 a1, int sgn_x, v32uint16 b, int sgn_y)
v32acc64 | negmul_elem_32 (v16uint32 a0, v16uint32 a1, int sgn_x, v32uint16 b, int sgn_y)
v32acc64 | mac_elem_32 (v16uint32 a0, v16uint32 a1, int sgn_x, v32uint16 b, int sgn_y, v32acc64 acc1)
v32acc64 | msc_elem_32 (v16uint32 a0, v16uint32 a1, int sgn_x, v32uint16 b, int sgn_y, v32acc64 acc1)
v32acc64 | mul_elem_32 (v16uint32 a0, v16uint32 a1, int sgn_x, v32int16 b, int sgn_y)
v32acc64 | negmul_elem_32 (v16uint32 a0, v16uint32 a1, int sgn_x, v32int16 b, int sgn_y)
v32acc64 | mac_elem_32 (v16uint32 a0, v16uint32 a1, int sgn_x, v32int16 b, int sgn_y, v32acc64 acc1)
v32acc64 | msc_elem_32 (v16uint32 a0, v16uint32 a1, int sgn_x, v32int16 b, int sgn_y, v32acc64 acc1)
v32acc64 | mul_elem_32 (v16int32 a0, v16int32 a1, int sgn_x, v32uint16 b, int sgn_y)
v32acc64 | negmul_elem_32 (v16int32 a0, v16int32 a1, int sgn_x, v32uint16 b, int sgn_y)
v32acc64 | mac_elem_32 (v16int32 a0, v16int32 a1, int sgn_x, v32uint16 b, int sgn_y, v32acc64 acc1)
v32acc64 | msc_elem_32 (v16int32 a0, v16int32 a1, int sgn_x, v32uint16 b, int sgn_y, v32acc64 acc1)
v32acc64 | mul_elem_32 (v16int32 a0, v16int32 a1, int sgn_x, v32int16 b, int sgn_y)
v32acc64 | negmul_elem_32 (v16int32 a0, v16int32 a1, int sgn_x, v32int16 b, int sgn_y)
v32acc64 | mac_elem_32 (v16int32 a0, v16int32 a1, int sgn_x, v32int16 b, int sgn_y, v32acc64 acc1)
v32acc64 | msc_elem_32 (v16int32 a0, v16int32 a1, int sgn_x, v32int16 b, int sgn_y, v32acc64 acc1)
v32acc64 | mul_conv_4x4_8ch (v32uint32 a0, v32uint32 a1, int sgn_x, v32uint16 b, int sgn_y)
v32acc64 | negmul_conv_4x4_8ch (v32uint32 a0, v32uint32 a1, int sgn_x, v32uint16 b, int sgn_y)
v32acc64 | mac_conv_4x4_8ch (v32uint32 a0, v32uint32 a1, int sgn_x, v32uint16 b, int sgn_y, v32acc64 acc1)
v32acc64 | msc_conv_4x4_8ch (v32uint32 a0, v32uint32 a1, int sgn_x, v32uint16 b, int sgn_y, v32acc64 acc1)
v32acc64 | mul_conv_4x4_8ch (v32uint32 a0, v32uint32 a1, int sgn_x, v32int16 b, int sgn_y)
v32acc64 | negmul_conv_4x4_8ch (v32uint32 a0, v32uint32 a1, int sgn_x, v32int16 b, int sgn_y)
v32acc64 | mac_conv_4x4_8ch (v32uint32 a0, v32uint32 a1, int sgn_x, v32int16 b, int sgn_y, v32acc64 acc1)
v32acc64 | msc_conv_4x4_8ch (v32uint32 a0, v32uint32 a1, int sgn_x, v32int16 b, int sgn_y, v32acc64 acc1)
v32acc64 | mul_conv_4x4_8ch (v32int32 a0, v32int32 a1, int sgn_x, v32uint16 b, int sgn_y)
v32acc64 | negmul_conv_4x4_8ch (v32int32 a0, v32int32 a1, int sgn_x, v32uint16 b, int sgn_y)
v32acc64 | mac_conv_4x4_8ch (v32int32 a0, v32int32 a1, int sgn_x, v32uint16 b, int sgn_y, v32acc64 acc1)
v32acc64 | msc_conv_4x4_8ch (v32int32 a0, v32int32 a1, int sgn_x, v32uint16 b, int sgn_y, v32acc64 acc1)
v32acc64 | mul_conv_4x4_8ch (v32int32 a0, v32int32 a1, int sgn_x, v32int16 b, int sgn_y)
v32acc64 | negmul_conv_4x4_8ch (v32int32 a0, v32int32 a1, int sgn_x, v32int16 b, int sgn_y)
v32acc64 | mac_conv_4x4_8ch (v32int32 a0, v32int32 a1, int sgn_x, v32int16 b, int sgn_y, v32acc64 acc1)
v32acc64 | msc_conv_4x4_8ch (v32int32 a0, v32int32 a1, int sgn_x, v32int16 b, int sgn_y, v32acc64 acc1)

## Emulated Channel by channel multiplication of (1x1) with (1x1) (32b * 16b) with dynamic negation of multiplication result
v32acc64 | mul_4x4_4x8_conf (v16uint32 a0, v32uint16 b, int sub_mul)
v32acc64 | negmul_4x4_4x8_conf (v16uint32 a0, v32uint16 b, int sub_mul)
v32acc64 | mul_4x4_4x8_conf (v16uint32 a0, v32int16 b, int sub_mul)
v32acc64 | negmul_4x4_4x8_conf (v16uint32 a0, v32int16 b, int sub_mul)
v32acc64 | mul_4x4_4x8_conf (v16int32 a0, v32uint16 b, int sub_mul)
v32acc64 | negmul_4x4_4x8_conf (v16int32 a0, v32uint16 b, int sub_mul)
v32acc64 | mul_4x4_4x8_conf (v16int32 a0, v32int16 b, int sub_mul)
v32acc64 | negmul_4x4_4x8_conf (v16int32 a0, v32int16 b, int sub_mul)
v32acc64 | mul_elem_32_conf (v16uint32 a0, v16uint32 a1, v32uint16 b, int sub_mul)
v32acc64 | negmul_elem_32_conf (v16uint32 a0, v16uint32 a1, v32uint16 b, int sub_mul)
v32acc64 | mul_elem_32_conf (v16uint32 a0, v16uint32 a1, v32int16 b, int sub_mul)
v32acc64 | negmul_elem_32_conf (v16uint32 a0, v16uint32 a1, v32int16 b, int sub_mul)
v32acc64 | mul_elem_32_conf (v16int32 a0, v16int32 a1, v32uint16 b, int sub_mul)
v32acc64 | negmul_elem_32_conf (v16int32 a0, v16int32 a1, v32uint16 b, int sub_mul)
v32acc64 | mul_elem_32_conf (v16int32 a0, v16int32 a1, v32int16 b, int sub_mul)
v32acc64 | negmul_elem_32_conf (v16int32 a0, v16int32 a1, v32int16 b, int sub_mul)
v32acc64 | mul_conv_4x4_8ch_conf (v32uint32 a0, v32uint32 a1, v32uint16 b, int sub_mul)
v32acc64 | negmul_conv_4x4_8ch_conf (v32uint32 a0, v32uint32 a1, v32uint16 b, int sub_mul)
v32acc64 | mul_conv_4x4_8ch_conf (v32uint32 a0, v32uint32 a1, v32int16 b, int sub_mul)
v32acc64 | negmul_conv_4x4_8ch_conf (v32uint32 a0, v32uint32 a1, v32int16 b, int sub_mul)
v32acc64 | mul_conv_4x4_8ch_conf (v32int32 a0, v32int32 a1, v32uint16 b, int sub_mul)
v32acc64 | negmul_conv_4x4_8ch_conf (v32int32 a0, v32int32 a1, v32uint16 b, int sub_mul)
v32acc64 | mul_conv_4x4_8ch_conf (v32int32 a0, v32int32 a1, v32int16 b, int sub_mul)
v32acc64 | negmul_conv_4x4_8ch_conf (v32int32 a0, v32int32 a1, v32int16 b, int sub_mul)

## Emulated Channel by channel multiplication of (1x1) with (1x1) (32b * 16b) with dynamic negation of multiplication result, negation of acc1
v32acc64 | mac_4x4_4x8_conf (v16uint32 a0, v32uint16 b, v32acc64 acc1, int sub_mul, int sub_acc1)
v32acc64 | msc_4x4_4x8_conf (v16uint32 a0, v32uint16 b, v32acc64 acc1, int sub_mul, int sub_acc1)
v32acc64 | mac_4x4_4x8_conf (v16uint32 a0, v32int16 b, v32acc64 acc1, int sub_mul, int sub_acc1)
v32acc64 | msc_4x4_4x8_conf (v16uint32 a0, v32int16 b, v32acc64 acc1, int sub_mul, int sub_acc1)
v32acc64 | mac_4x4_4x8_conf (v16int32 a0, v32uint16 b, v32acc64 acc1, int sub_mul, int sub_acc1)
v32acc64 | msc_4x4_4x8_conf (v16int32 a0, v32uint16 b, v32acc64 acc1, int sub_mul, int sub_acc1)
v32acc64 | mac_4x4_4x8_conf (v16int32 a0, v32int16 b, v32acc64 acc1, int sub_mul, int sub_acc1)
v32acc64 | msc_4x4_4x8_conf (v16int32 a0, v32int16 b, v32acc64 acc1, int sub_mul, int sub_acc1)
v32acc64 | mac_elem_32_conf (v16uint32 a0, v16uint32 a1, v32uint16 b, v32acc64 acc1, int sub_mul, int sub_acc1)
v32acc64 | msc_elem_32_conf (v16uint32 a0, v16uint32 a1, v32uint16 b, v32acc64 acc1, int sub_mul, int sub_acc1)
v32acc64 | mac_elem_32_conf (v16uint32 a0, v16uint32 a1, v32int16 b, v32acc64 acc1, int sub_mul, int sub_acc1)
v32acc64 | msc_elem_32_conf (v16uint32 a0, v16uint32 a1, v32int16 b, v32acc64 acc1, int sub_mul, int sub_acc1)
v32acc64 | mac_elem_32_conf (v16int32 a0, v16int32 a1, v32uint16 b, v32acc64 acc1, int sub_mul, int sub_acc1)
v32acc64 | msc_elem_32_conf (v16int32 a0, v16int32 a1, v32uint16 b, v32acc64 acc1, int sub_mul, int sub_acc1)
v32acc64 | mac_elem_32_conf (v16int32 a0, v16int32 a1, v32int16 b, v32acc64 acc1, int sub_mul, int sub_acc1)
v32acc64 | msc_elem_32_conf (v16int32 a0, v16int32 a1, v32int16 b, v32acc64 acc1, int sub_mul, int sub_acc1)
v32acc64 | mac_conv_4x4_8ch_conf (v32uint32 a0, v32uint32 a1, v32uint16 b, v32acc64 acc1, int sub_mul, int sub_acc1)
v32acc64 | msc_conv_4x4_8ch_conf (v32uint32 a0, v32uint32 a1, v32uint16 b, v32acc64 acc1, int sub_mul, int sub_acc1)
v32acc64 | mac_conv_4x4_8ch_conf (v32uint32 a0, v32uint32 a1, v32int16 b, v32acc64 acc1, int sub_mul, int sub_acc1)
v32acc64 | msc_conv_4x4_8ch_conf (v32uint32 a0, v32uint32 a1, v32int16 b, v32acc64 acc1, int sub_mul, int sub_acc1)
v32acc64 | mac_conv_4x4_8ch_conf (v32int32 a0, v32int32 a1, v32uint16 b, v32acc64 acc1, int sub_mul, int sub_acc1)
v32acc64 | msc_conv_4x4_8ch_conf (v32int32 a0, v32int32 a1, v32uint16 b, v32acc64 acc1, int sub_mul, int sub_acc1)
v32acc64 | mac_conv_4x4_8ch_conf (v32int32 a0, v32int32 a1, v32int16 b, v32acc64 acc1, int sub_mul, int sub_acc1)
v32acc64 | msc_conv_4x4_8ch_conf (v32int32 a0, v32int32 a1, v32int16 b, v32acc64 acc1, int sub_mul, int sub_acc1)

## Emulated Channel by channel multiplication of (1x1) with (1x1) (32b * 16b) with dynamic sign and dynamic negation of multiplication result
v32acc64 | mul_4x4_4x8_conf (v16uint32 a0, int sgn_x, v32uint16 b, int sgn_y, int sub_mul)
v32acc64 | negmul_4x4_4x8_conf (v16uint32 a0, int sgn_x, v32uint16 b, int sgn_y, int sub_mul)
v32acc64 | mac_4x4_4x8_conf (v16uint32 a0, int sgn_x, v32uint16 b, int sgn_y, v32acc64 acc1, int sub_mul, int sub_acc1)
v32acc64 | msc_4x4_4x8_conf (v16uint32 a0, int sgn_x, v32uint16 b, int sgn_y, v32acc64 acc1, int sub_mul, int sub_acc1)
v32acc64 | mul_4x4_4x8_conf (v16uint32 a0, int sgn_x, v32int16 b, int sgn_y, int sub_mul)
v32acc64 | negmul_4x4_4x8_conf (v16uint32 a0, int sgn_x, v32int16 b, int sgn_y, int sub_mul)
v32acc64 | mac_4x4_4x8_conf (v16uint32 a0, int sgn_x, v32int16 b, int sgn_y, v32acc64 acc1, int sub_mul, int sub_acc1)
v32acc64 | msc_4x4_4x8_conf (v16uint32 a0, int sgn_x, v32int16 b, int sgn_y, v32acc64 acc1, int sub_mul, int sub_acc1)
v32acc64 | mul_4x4_4x8_conf (v16int32 a0, int sgn_x, v32uint16 b, int sgn_y, int sub_mul)
v32acc64 | negmul_4x4_4x8_conf (v16int32 a0, int sgn_x, v32uint16 b, int sgn_y, int sub_mul)
v32acc64 | mac_4x4_4x8_conf (v16int32 a0, int sgn_x, v32uint16 b, int sgn_y, v32acc64 acc1, int sub_mul, int sub_acc1)
v32acc64 | msc_4x4_4x8_conf (v16int32 a0, int sgn_x, v32uint16 b, int sgn_y, v32acc64 acc1, int sub_mul, int sub_acc1)
v32acc64 | mul_4x4_4x8_conf (v16int32 a0, int sgn_x, v32int16 b, int sgn_y, int sub_mul)
v32acc64 | negmul_4x4_4x8_conf (v16int32 a0, int sgn_x, v32int16 b, int sgn_y, int sub_mul)
v32acc64 | mac_4x4_4x8_conf (v16int32 a0, int sgn_x, v32int16 b, int sgn_y, v32acc64 acc1, int sub_mul, int sub_acc1)
v32acc64 | msc_4x4_4x8_conf (v16int32 a0, int sgn_x, v32int16 b, int sgn_y, v32acc64 acc1, int sub_mul, int sub_acc1)
v32acc64 | mul_elem_32_conf (v16uint32 a0, v16uint32 a1, int sgn_x, v32uint16 b, int sgn_y, int sub_mul)
v32acc64 | negmul_elem_32_conf (v16uint32 a0, v16uint32 a1, int sgn_x, v32uint16 b, int sgn_y, int sub_mul)
v32acc64 | mac_elem_32_conf (v16uint32 a0, v16uint32 a1, int sgn_x, v32uint16 b, int sgn_y, v32acc64 acc1, int sub_mul, int sub_acc1)
v32acc64 | msc_elem_32_conf (v16uint32 a0, v16uint32 a1, int sgn_x, v32uint16 b, int sgn_y, v32acc64 acc1, int sub_mul, int sub_acc1)
v32acc64 | mul_elem_32_conf (v16uint32 a0, v16uint32 a1, int sgn_x, v32int16 b, int sgn_y, int sub_mul)
v32acc64 | negmul_elem_32_conf (v16uint32 a0, v16uint32 a1, int sgn_x, v32int16 b, int sgn_y, int sub_mul)
v32acc64 | mac_elem_32_conf (v16uint32 a0, v16uint32 a1, int sgn_x, v32int16 b, int sgn_y, v32acc64 acc1, int sub_mul, int sub_acc1)
v32acc64 | msc_elem_32_conf (v16uint32 a0, v16uint32 a1, int sgn_x, v32int16 b, int sgn_y, v32acc64 acc1, int sub_mul, int sub_acc1)
v32acc64 | mul_elem_32_conf (v16int32 a0, v16int32 a1, int sgn_x, v32uint16 b, int sgn_y, int sub_mul)
v32acc64 | negmul_elem_32_conf (v16int32 a0, v16int32 a1, int sgn_x, v32uint16 b, int sgn_y, int sub_mul)
v32acc64 | mac_elem_32_conf (v16int32 a0, v16int32 a1, int sgn_x, v32uint16 b, int sgn_y, v32acc64 acc1, int sub_mul, int sub_acc1)
v32acc64 | msc_elem_32_conf (v16int32 a0, v16int32 a1, int sgn_x, v32uint16 b, int sgn_y, v32acc64 acc1, int sub_mul, int sub_acc1)
v32acc64 | mul_elem_32_conf (v16int32 a0, v16int32 a1, int sgn_x, v32int16 b, int sgn_y, int sub_mul)
v32acc64 | negmul_elem_32_conf (v16int32 a0, v16int32 a1, int sgn_x, v32int16 b, int sgn_y, int sub_mul)
v32acc64 | mac_elem_32_conf (v16int32 a0, v16int32 a1, int sgn_x, v32int16 b, int sgn_y, v32acc64 acc1, int sub_mul, int sub_acc1)
v32acc64 | msc_elem_32_conf (v16int32 a0, v16int32 a1, int sgn_x, v32int16 b, int sgn_y, v32acc64 acc1, int sub_mul, int sub_acc1)
v32acc64 | mul_conv_4x4_8ch_conf (v32uint32 a0, v32uint32 a1, int sgn_x, v32uint16 b, int sgn_y, int sub_mul)
v32acc64 | negmul_conv_4x4_8ch_conf (v32uint32 a0, v32uint32 a1, int sgn_x, v32uint16 b, int sgn_y, int sub_mul)
v32acc64 | mac_conv_4x4_8ch_conf (v32uint32 a0, v32uint32 a1, int sgn_x, v32uint16 b, int sgn_y, v32acc64 acc1, int sub_mul, int sub_acc1)
v32acc64 | msc_conv_4x4_8ch_conf (v32uint32 a0, v32uint32 a1, int sgn_x, v32uint16 b, int sgn_y, v32acc64 acc1, int sub_mul, int sub_acc1)
v32acc64 | mul_conv_4x4_8ch_conf (v32uint32 a0, v32uint32 a1, int sgn_x, v32int16 b, int sgn_y, int sub_mul)
v32acc64 | negmul_conv_4x4_8ch_conf (v32uint32 a0, v32uint32 a1, int sgn_x, v32int16 b, int sgn_y, int sub_mul)
v32acc64 | mac_conv_4x4_8ch_conf (v32uint32 a0, v32uint32 a1, int sgn_x, v32int16 b, int sgn_y, v32acc64 acc1, int sub_mul, int sub_acc1)
v32acc64 | msc_conv_4x4_8ch_conf (v32uint32 a0, v32uint32 a1, int sgn_x, v32int16 b, int sgn_y, v32acc64 acc1, int sub_mul, int sub_acc1)
v32acc64 | mul_conv_4x4_8ch_conf (v32int32 a0, v32int32 a1, int sgn_x, v32uint16 b, int sgn_y, int sub_mul)
v32acc64 | negmul_conv_4x4_8ch_conf (v32int32 a0, v32int32 a1, int sgn_x, v32uint16 b, int sgn_y, int sub_mul)
v32acc64 | mac_conv_4x4_8ch_conf (v32int32 a0, v32int32 a1, int sgn_x, v32uint16 b, int sgn_y, v32acc64 acc1, int sub_mul, int sub_acc1)
v32acc64 | msc_conv_4x4_8ch_conf (v32int32 a0, v32int32 a1, int sgn_x, v32uint16 b, int sgn_y, v32acc64 acc1, int sub_mul, int sub_acc1)
v32acc64 | mul_conv_4x4_8ch_conf (v32int32 a0, v32int32 a1, int sgn_x, v32int16 b, int sgn_y, int sub_mul)
v32acc64 | negmul_conv_4x4_8ch_conf (v32int32 a0, v32int32 a1, int sgn_x, v32int16 b, int sgn_y, int sub_mul)
v32acc64 | mac_conv_4x4_8ch_conf (v32int32 a0, v32int32 a1, int sgn_x, v32int16 b, int sgn_y, v32acc64 acc1, int sub_mul, int sub_acc1)
v32acc64 | msc_conv_4x4_8ch_conf (v32int32 a0, v32int32 a1, int sgn_x, v32int16 b, int sgn_y, v32acc64 acc1, int sub_mul, int sub_acc1)

## Emulated Channel by channel multiplication of (1x1) with (1x1) (32b * 16b) with dynamic negation of multiplication result, negation of acc1 and zeroing of acc1
v32acc64 | mac_4x4_4x8_conf (v16uint32 a0, v32uint16 b, v32acc64 acc1, int zero_acc1, int sub_mul, int sub_acc1)
v32acc64 | msc_4x4_4x8_conf (v16uint32 a0, v32uint16 b, v32acc64 acc1, int zero_acc1, int sub_mul, int sub_acc1)
v32acc64 | mac_4x4_4x8_conf (v16uint32 a0, v32int16 b, v32acc64 acc1, int zero_acc1, int sub_mul, int sub_acc1)
v32acc64 | msc_4x4_4x8_conf (v16uint32 a0, v32int16 b, v32acc64 acc1, int zero_acc1, int sub_mul, int sub_acc1)
v32acc64 | mac_4x4_4x8_conf (v16int32 a0, v32uint16 b, v32acc64 acc1, int zero_acc1, int sub_mul, int sub_acc1)
v32acc64 | msc_4x4_4x8_conf (v16int32 a0, v32uint16 b, v32acc64 acc1, int zero_acc1, int sub_mul, int sub_acc1)
v32acc64 | mac_4x4_4x8_conf (v16int32 a0, v32int16 b, v32acc64 acc1, int zero_acc1, int sub_mul, int sub_acc1)
v32acc64 | msc_4x4_4x8_conf (v16int32 a0, v32int16 b, v32acc64 acc1, int zero_acc1, int sub_mul, int sub_acc1)
v32acc64 | mac_elem_32_conf (v16uint32 a0, v16uint32 a1, v32uint16 b, v32acc64 acc1, int zero_acc1, int sub_mul, int sub_acc1)
v32acc64 | msc_elem_32_conf (v16uint32 a0, v16uint32 a1, v32uint16 b, v32acc64 acc1, int zero_acc1, int sub_mul, int sub_acc1)
v32acc64 | mac_elem_32_conf (v16uint32 a0, v16uint32 a1, v32int16 b, v32acc64 acc1, int zero_acc1, int sub_mul, int sub_acc1)
v32acc64 | msc_elem_32_conf (v16uint32 a0, v16uint32 a1, v32int16 b, v32acc64 acc1, int zero_acc1, int sub_mul, int sub_acc1)
v32acc64 | mac_elem_32_conf (v16int32 a0, v16int32 a1, v32uint16 b, v32acc64 acc1, int zero_acc1, int sub_mul, int sub_acc1)
v32acc64 | msc_elem_32_conf (v16int32 a0, v16int32 a1, v32uint16 b, v32acc64 acc1, int zero_acc1, int sub_mul, int sub_acc1)
v32acc64 | mac_elem_32_conf (v16int32 a0, v16int32 a1, v32int16 b, v32acc64 acc1, int zero_acc1, int sub_mul, int sub_acc1)
v32acc64 | msc_elem_32_conf (v16int32 a0, v16int32 a1, v32int16 b, v32acc64 acc1, int zero_acc1, int sub_mul, int sub_acc1)
v32acc64 | mac_conv_4x4_8ch_conf (v32uint32 a0, v32uint32 a1, v32uint16 b, v32acc64 acc1, int zero_acc1, int sub_mul, int sub_acc1)
v32acc64 | msc_conv_4x4_8ch_conf (v32uint32 a0, v32uint32 a1, v32uint16 b, v32acc64 acc1, int zero_acc1, int sub_mul, int sub_acc1)
v32acc64 | mac_conv_4x4_8ch_conf (v32uint32 a0, v32uint32 a1, v32int16 b, v32acc64 acc1, int zero_acc1, int sub_mul, int sub_acc1)
v32acc64 | msc_conv_4x4_8ch_conf (v32uint32 a0, v32uint32 a1, v32int16 b, v32acc64 acc1, int zero_acc1, int sub_mul, int sub_acc1)
v32acc64 | mac_conv_4x4_8ch_conf (v32int32 a0, v32int32 a1, v32uint16 b, v32acc64 acc1, int zero_acc1, int sub_mul, int sub_acc1)
v32acc64 | msc_conv_4x4_8ch_conf (v32int32 a0, v32int32 a1, v32uint16 b, v32acc64 acc1, int zero_acc1, int sub_mul, int sub_acc1)
v32acc64 | mac_conv_4x4_8ch_conf (v32int32 a0, v32int32 a1, v32int16 b, v32acc64 acc1, int zero_acc1, int sub_mul, int sub_acc1)
v32acc64 | msc_conv_4x4_8ch_conf (v32int32 a0, v32int32 a1, v32int16 b, v32acc64 acc1, int zero_acc1, int sub_mul, int sub_acc1)

## Emulated Channel by channel multiplication of (1x1) with (1x1) (32b * 16b) with dynamic sign, zeroing of acc1 and dynamic negation of multiplication result
v32acc64 | mac_4x4_4x8_conf (v16uint32 a0, int sgn_x, v32uint16 b, int sgn_y, v32acc64 acc1, int zero_acc1, int sub_mul, int sub_acc1)
v32acc64 | msc_4x4_4x8_conf (v16uint32 a0, int sgn_x, v32uint16 b, int sgn_y, v32acc64 acc1, int zero_acc1, int sub_mul, int sub_acc1)
v32acc64 | mac_4x4_4x8_conf (v16uint32 a0, int sgn_x, v32int16 b, int sgn_y, v32acc64 acc1, int zero_acc1, int sub_mul, int sub_acc1)
v32acc64 | msc_4x4_4x8_conf (v16uint32 a0, int sgn_x, v32int16 b, int sgn_y, v32acc64 acc1, int zero_acc1, int sub_mul, int sub_acc1)
v32acc64 | mac_4x4_4x8_conf (v16int32 a0, int sgn_x, v32uint16 b, int sgn_y, v32acc64 acc1, int zero_acc1, int sub_mul, int sub_acc1)
v32acc64 | msc_4x4_4x8_conf (v16int32 a0, int sgn_x, v32uint16 b, int sgn_y, v32acc64 acc1, int zero_acc1, int sub_mul, int sub_acc1)
v32acc64 | mac_4x4_4x8_conf (v16int32 a0, int sgn_x, v32int16 b, int sgn_y, v32acc64 acc1, int zero_acc1, int sub_mul, int sub_acc1)
v32acc64 | msc_4x4_4x8_conf (v16int32 a0, int sgn_x, v32int16 b, int sgn_y, v32acc64 acc1, int zero_acc1, int sub_mul, int sub_acc1)
v32acc64 | mac_elem_32_conf (v16uint32 a0, v16uint32 a1, int sgn_x, v32uint16 b, int sgn_y, v32acc64 acc1, int zero_acc1, int sub_mul, int sub_acc1)
v32acc64 | msc_elem_32_conf (v16uint32 a0, v16uint32 a1, int sgn_x, v32uint16 b, int sgn_y, v32acc64 acc1, int zero_acc1, int sub_mul, int sub_acc1)
v32acc64 | mac_elem_32_conf (v16uint32 a0, v16uint32 a1, int sgn_x, v32int16 b, int sgn_y, v32acc64 acc1, int zero_acc1, int sub_mul, int sub_acc1)
v32acc64 | msc_elem_32_conf (v16uint32 a0, v16uint32 a1, int sgn_x, v32int16 b, int sgn_y, v32acc64 acc1, int zero_acc1, int sub_mul, int sub_acc1)
v32acc64 | mac_elem_32_conf (v16int32 a0, v16int32 a1, int sgn_x, v32uint16 b, int sgn_y, v32acc64 acc1, int zero_acc1, int sub_mul, int sub_acc1)
v32acc64 | msc_elem_32_conf (v16int32 a0, v16int32 a1, int sgn_x, v32uint16 b, int sgn_y, v32acc64 acc1, int zero_acc1, int sub_mul, int sub_acc1)
v32acc64 | mac_elem_32_conf (v16int32 a0, v16int32 a1, int sgn_x, v32int16 b, int sgn_y, v32acc64 acc1, int zero_acc1, int sub_mul, int sub_acc1)
v32acc64 | msc_elem_32_conf (v16int32 a0, v16int32 a1, int sgn_x, v32int16 b, int sgn_y, v32acc64 acc1, int zero_acc1, int sub_mul, int sub_acc1)
v32acc64 | mac_conv_4x4_8ch_conf (v32uint32 a0, v32uint32 a1, int sgn_x, v32uint16 b, int sgn_y, v32acc64 acc1, int zero_acc1, int sub_mul, int sub_acc1)
v32acc64 | msc_conv_4x4_8ch_conf (v32uint32 a0, v32uint32 a1, int sgn_x, v32uint16 b, int sgn_y, v32acc64 acc1, int zero_acc1, int sub_mul, int sub_acc1)
v32acc64 | mac_conv_4x4_8ch_conf (v32uint32 a0, v32uint32 a1, int sgn_x, v32int16 b, int sgn_y, v32acc64 acc1, int zero_acc1, int sub_mul, int sub_acc1)
v32acc64 | msc_conv_4x4_8ch_conf (v32uint32 a0, v32uint32 a1, int sgn_x, v32int16 b, int sgn_y, v32acc64 acc1, int zero_acc1, int sub_mul, int sub_acc1)
v32acc64 | mac_conv_4x4_8ch_conf (v32int32 a0, v32int32 a1, int sgn_x, v32uint16 b, int sgn_y, v32acc64 acc1, int zero_acc1, int sub_mul, int sub_acc1)
v32acc64 | msc_conv_4x4_8ch_conf (v32int32 a0, v32int32 a1, int sgn_x, v32uint16 b, int sgn_y, v32acc64 acc1, int zero_acc1, int sub_mul, int sub_acc1)
v32acc64 | mac_conv_4x4_8ch_conf (v32int32 a0, v32int32 a1, int sgn_x, v32int16 b, int sgn_y, v32acc64 acc1, int zero_acc1, int sub_mul, int sub_acc1)
v32acc64 | msc_conv_4x4_8ch_conf (v32int32 a0, v32int32 a1, int sgn_x, v32int16 b, int sgn_y, v32acc64 acc1, int zero_acc1, int sub_mul, int sub_acc1)

## Emulated Channel by channel multiplication of (1x2) with (2x1) (32b * 16b)
v32acc64 | mul_elem_32_2 (v32uint32 a0, v32uint32 a1, v64uint16 b)
v32acc64 | negmul_elem_32_2 (v32uint32 a0, v32uint32 a1, v64uint16 b)
v32acc64 | mac_elem_32_2 (v32uint32 a0, v32uint32 a1, v64uint16 b, v32acc64 acc1)
v32acc64 | msc_elem_32_2 (v32uint32 a0, v32uint32 a1, v64uint16 b, v32acc64 acc1)
v32acc64 | mul_elem_32_2 (v32uint32 a0, v32uint32 a1, v64int16 b)
v32acc64 | negmul_elem_32_2 (v32uint32 a0, v32uint32 a1, v64int16 b)
v32acc64 | mac_elem_32_2 (v32uint32 a0, v32uint32 a1, v64int16 b, v32acc64 acc1)
v32acc64 | msc_elem_32_2 (v32uint32 a0, v32uint32 a1, v64int16 b, v32acc64 acc1)
v32acc64 | mul_elem_32_2 (v32int32 a0, v32int32 a1, v64uint16 b)
v32acc64 | negmul_elem_32_2 (v32int32 a0, v32int32 a1, v64uint16 b)
v32acc64 | mac_elem_32_2 (v32int32 a0, v32int32 a1, v64uint16 b, v32acc64 acc1)
v32acc64 | msc_elem_32_2 (v32int32 a0, v32int32 a1, v64uint16 b, v32acc64 acc1)
v32acc64 | mul_elem_32_2 (v32int32 a0, v32int32 a1, v64int16 b)
v32acc64 | negmul_elem_32_2 (v32int32 a0, v32int32 a1, v64int16 b)
v32acc64 | mac_elem_32_2 (v32int32 a0, v32int32 a1, v64int16 b, v32acc64 acc1)
v32acc64 | msc_elem_32_2 (v32int32 a0, v32int32 a1, v64int16 b, v32acc64 acc1)

## Emulated Channel by channel multiplication of (1x2) with (2x1) (32b * 16b) with dynamic sign
v32acc64 | mul_elem_32_2 (v32uint32 a0, v32uint32 a1, int sgn_x, v64uint16 b, int sgn_y)
v32acc64 | negmul_elem_32_2 (v32uint32 a0, v32uint32 a1, int sgn_x, v64uint16 b, int sgn_y)
v32acc64 | mac_elem_32_2 (v32uint32 a0, v32uint32 a1, int sgn_x, v64uint16 b, int sgn_y, v32acc64 acc1)
v32acc64 | msc_elem_32_2 (v32uint32 a0, v32uint32 a1, int sgn_x, v64uint16 b, int sgn_y, v32acc64 acc1)
v32acc64 | mul_elem_32_2 (v32uint32 a0, v32uint32 a1, int sgn_x, v64int16 b, int sgn_y)
v32acc64 | negmul_elem_32_2 (v32uint32 a0, v32uint32 a1, int sgn_x, v64int16 b, int sgn_y)
v32acc64 | mac_elem_32_2 (v32uint32 a0, v32uint32 a1, int sgn_x, v64int16 b, int sgn_y, v32acc64 acc1)
v32acc64 | msc_elem_32_2 (v32uint32 a0, v32uint32 a1, int sgn_x, v64int16 b, int sgn_y, v32acc64 acc1)
v32acc64 | mul_elem_32_2 (v32int32 a0, v32int32 a1, int sgn_x, v64uint16 b, int sgn_y)
v32acc64 | negmul_elem_32_2 (v32int32 a0, v32int32 a1, int sgn_x, v64uint16 b, int sgn_y)
v32acc64 | mac_elem_32_2 (v32int32 a0, v32int32 a1, int sgn_x, v64uint16 b, int sgn_y, v32acc64 acc1)
v32acc64 | msc_elem_32_2 (v32int32 a0, v32int32 a1, int sgn_x, v64uint16 b, int sgn_y, v32acc64 acc1)
v32acc64 | mul_elem_32_2 (v32int32 a0, v32int32 a1, int sgn_x, v64int16 b, int sgn_y)
v32acc64 | negmul_elem_32_2 (v32int32 a0, v32int32 a1, int sgn_x, v64int16 b, int sgn_y)
v32acc64 | mac_elem_32_2 (v32int32 a0, v32int32 a1, int sgn_x, v64int16 b, int sgn_y, v32acc64 acc1)
v32acc64 | msc_elem_32_2 (v32int32 a0, v32int32 a1, int sgn_x, v64int16 b, int sgn_y, v32acc64 acc1)

## Emulated Channel by channel multiplication of (1x2) with (2x1) (32b * 16b) with dynamic negation of multiplication result
v32acc64 | mul_elem_32_2_conf (v32uint32 a0, v32uint32 a1, v64uint16 b, int sub_mul)
v32acc64 | negmul_elem_32_2_conf (v32uint32 a0, v32uint32 a1, v64uint16 b, int sub_mul)
v32acc64 | mul_elem_32_2_conf (v32uint32 a0, v32uint32 a1, v64int16 b, int sub_mul)
v32acc64 | negmul_elem_32_2_conf (v32uint32 a0, v32uint32 a1, v64int16 b, int sub_mul)
v32acc64 | mul_elem_32_2_conf (v32int32 a0, v32int32 a1, v64uint16 b, int sub_mul)
v32acc64 | negmul_elem_32_2_conf (v32int32 a0, v32int32 a1, v64uint16 b, int sub_mul)
v32acc64 | mul_elem_32_2_conf (v32int32 a0, v32int32 a1, v64int16 b, int sub_mul)
v32acc64 | negmul_elem_32_2_conf (v32int32 a0, v32int32 a1, v64int16 b, int sub_mul)

## Emulated Channel by channel multiplication of (1x2) with (2x1) (32b * 16b) with dynamic negation of multiplication result, negation of acc1
v32acc64 | mac_elem_32_2_conf (v32uint32 a0, v32uint32 a1, v64uint16 b, v32acc64 acc1, int sub_mul, int sub_acc1)
v32acc64 | msc_elem_32_2_conf (v32uint32 a0, v32uint32 a1, v64uint16 b, v32acc64 acc1, int sub_mul, int sub_acc1)
v32acc64 | mac_elem_32_2_conf (v32uint32 a0, v32uint32 a1, v64int16 b, v32acc64 acc1, int sub_mul, int sub_acc1)
v32acc64 | msc_elem_32_2_conf (v32uint32 a0, v32uint32 a1, v64int16 b, v32acc64 acc1, int sub_mul, int sub_acc1)
v32acc64 | mac_elem_32_2_conf (v32int32 a0, v32int32 a1, v64uint16 b, v32acc64 acc1, int sub_mul, int sub_acc1)
v32acc64 | msc_elem_32_2_conf (v32int32 a0, v32int32 a1, v64uint16 b, v32acc64 acc1, int sub_mul, int sub_acc1)
v32acc64 | mac_elem_32_2_conf (v32int32 a0, v32int32 a1, v64int16 b, v32acc64 acc1, int sub_mul, int sub_acc1)
v32acc64 | msc_elem_32_2_conf (v32int32 a0, v32int32 a1, v64int16 b, v32acc64 acc1, int sub_mul, int sub_acc1)

## Emulated Channel by channel multiplication of (1x2) with (2x1) (32b * 16b) with dynamic sign and dynamic negation of multiplication result
v32acc64 | mul_elem_32_2_conf (v32uint32 a0, v32uint32 a1, int sgn_x, v64uint16 b, int sgn_y, int sub_mul)
v32acc64 | negmul_elem_32_2_conf (v32uint32 a0, v32uint32 a1, int sgn_x, v64uint16 b, int sgn_y, int sub_mul)
v32acc64 | mac_elem_32_2_conf (v32uint32 a0, v32uint32 a1, int sgn_x, v64uint16 b, int sgn_y, v32acc64 acc1, int sub_mul, int sub_acc1)
v32acc64 | msc_elem_32_2_conf (v32uint32 a0, v32uint32 a1, int sgn_x, v64uint16 b, int sgn_y, v32acc64 acc1, int sub_mul, int sub_acc1)
v32acc64 | mul_elem_32_2_conf (v32uint32 a0, v32uint32 a1, int sgn_x, v64int16 b, int sgn_y, int sub_mul)
v32acc64 | negmul_elem_32_2_conf (v32uint32 a0, v32uint32 a1, int sgn_x, v64int16 b, int sgn_y, int sub_mul)
v32acc64 | mac_elem_32_2_conf (v32uint32 a0, v32uint32 a1, int sgn_x, v64int16 b, int sgn_y, v32acc64 acc1, int sub_mul, int sub_acc1)
v32acc64 | msc_elem_32_2_conf (v32uint32 a0, v32uint32 a1, int sgn_x, v64int16 b, int sgn_y, v32acc64 acc1, int sub_mul, int sub_acc1)
v32acc64 | mul_elem_32_2_conf (v32int32 a0, v32int32 a1, int sgn_x, v64uint16 b, int sgn_y, int sub_mul)
v32acc64 | negmul_elem_32_2_conf (v32int32 a0, v32int32 a1, int sgn_x, v64uint16 b, int sgn_y, int sub_mul)
v32acc64 | mac_elem_32_2_conf (v32int32 a0, v32int32 a1, int sgn_x, v64uint16 b, int sgn_y, v32acc64 acc1, int sub_mul, int sub_acc1)
v32acc64 | msc_elem_32_2_conf (v32int32 a0, v32int32 a1, int sgn_x, v64uint16 b, int sgn_y, v32acc64 acc1, int sub_mul, int sub_acc1)
v32acc64 | mul_elem_32_2_conf (v32int32 a0, v32int32 a1, int sgn_x, v64int16 b, int sgn_y, int sub_mul)
v32acc64 | negmul_elem_32_2_conf (v32int32 a0, v32int32 a1, int sgn_x, v64int16 b, int sgn_y, int sub_mul)
v32acc64 | mac_elem_32_2_conf (v32int32 a0, v32int32 a1, int sgn_x, v64int16 b, int sgn_y, v32acc64 acc1, int sub_mul, int sub_acc1)
v32acc64 | msc_elem_32_2_conf (v32int32 a0, v32int32 a1, int sgn_x, v64int16 b, int sgn_y, v32acc64 acc1, int sub_mul, int sub_acc1)

## Emulated Channel by channel multiplication of (1x2) with (2x1) (32b * 16b) with dynamic negation of multiplication result, negation of acc1 and zeroing of acc1
v32acc64 | mac_elem_32_2_conf (v32uint32 a0, v32uint32 a1, v64uint16 b, v32acc64 acc1, int zero_acc1, int sub_mul, int sub_acc1)
v32acc64 | msc_elem_32_2_conf (v32uint32 a0, v32uint32 a1, v64uint16 b, v32acc64 acc1, int zero_acc1, int sub_mul, int sub_acc1)
v32acc64 | mac_elem_32_2_conf (v32uint32 a0, v32uint32 a1, v64int16 b, v32acc64 acc1, int zero_acc1, int sub_mul, int sub_acc1)
v32acc64 | msc_elem_32_2_conf (v32uint32 a0, v32uint32 a1, v64int16 b, v32acc64 acc1, int zero_acc1, int sub_mul, int sub_acc1)
v32acc64 | mac_elem_32_2_conf (v32int32 a0, v32int32 a1, v64uint16 b, v32acc64 acc1, int zero_acc1, int sub_mul, int sub_acc1)
v32acc64 | msc_elem_32_2_conf (v32int32 a0, v32int32 a1, v64uint16 b, v32acc64 acc1, int zero_acc1, int sub_mul, int sub_acc1)
v32acc64 | mac_elem_32_2_conf (v32int32 a0, v32int32 a1, v64int16 b, v32acc64 acc1, int zero_acc1, int sub_mul, int sub_acc1)
v32acc64 | msc_elem_32_2_conf (v32int32 a0, v32int32 a1, v64int16 b, v32acc64 acc1, int zero_acc1, int sub_mul, int sub_acc1)

## Emulated Channel by channel multiplication of (1x2) with (2x1) (32b * 16b) with dynamic sign, zeroing of acc1 and dynamic negation of multiplication result
v32acc64 | mac_elem_32_2_conf (v32uint32 a0, v32uint32 a1, int sgn_x, v64uint16 b, int sgn_y, v32acc64 acc1, int zero_acc1, int sub_mul, int sub_acc1)
v32acc64 | msc_elem_32_2_conf (v32uint32 a0, v32uint32 a1, int sgn_x, v64uint16 b, int sgn_y, v32acc64 acc1, int zero_acc1, int sub_mul, int sub_acc1)
v32acc64 | mac_elem_32_2_conf (v32uint32 a0, v32uint32 a1, int sgn_x, v64int16 b, int sgn_y, v32acc64 acc1, int zero_acc1, int sub_mul, int sub_acc1)
v32acc64 | msc_elem_32_2_conf (v32uint32 a0, v32uint32 a1, int sgn_x, v64int16 b, int sgn_y, v32acc64 acc1, int zero_acc1, int sub_mul, int sub_acc1)
v32acc64 | mac_elem_32_2_conf (v32int32 a0, v32int32 a1, int sgn_x, v64uint16 b, int sgn_y, v32acc64 acc1, int zero_acc1, int sub_mul, int sub_acc1)
v32acc64 | msc_elem_32_2_conf (v32int32 a0, v32int32 a1, int sgn_x, v64uint16 b, int sgn_y, v32acc64 acc1, int zero_acc1, int sub_mul, int sub_acc1)
v32acc64 | mac_elem_32_2_conf (v32int32 a0, v32int32 a1, int sgn_x, v64int16 b, int sgn_y, v32acc64 acc1, int zero_acc1, int sub_mul, int sub_acc1)
v32acc64 | msc_elem_32_2_conf (v32int32 a0, v32int32 a1, int sgn_x, v64int16 b, int sgn_y, v32acc64 acc1, int zero_acc1, int sub_mul, int sub_acc1)

## Detailed Description

Matrix multiplications in which matrix A has data elements of 32 bit and matrix B has data elements of 16 bit. These operations are emulated on top of Multiply-accumulate of 16b x 16b integer datatypes and might not have optimal performance.

For an explanation how these operations works see Multiply Accumulate.

## Function Documentation

## ◆ mac_4x4_4x8() [1/8]

v32acc64 mac_4x4_4x8 | ( | v16int32 | a0,
|  | int | sgn_x,
|  | v32int16 | b,
|  | int | sgn_y,
|  | v32acc64 | acc1 )

Parameters

  a0 | Matrix A
  sgn_x | Sign mask for matrix A
  b | Matrix B
  sgn_y | Sign mask for matrix B
  acc1 | Accumulator 1 input

Returns
  Result of operation

## ◆ mac_4x4_4x8() [2/8]

v32acc64 mac_4x4_4x8 | ( | v16int32 | a0,
|  | int | sgn_x,
|  | v32uint16 | b,
|  | int | sgn_y,
|  | v32acc64 | acc1 )

Parameters

  a0 | Matrix A
  sgn_x | Sign mask for matrix A
  b | Matrix B
  sgn_y | Sign mask for matrix B
  acc1 | Accumulator 1 input

Returns
  Result of operation

## ◆ mac_4x4_4x8() [3/8]

v32acc64 mac_4x4_4x8 | ( | v16int32 | a0,
|  | v32int16 | b,
|  | v32acc64 | acc1 )

Parameters

  a0 | Matrix A
  b | Matrix B
  acc1 | Accumulator 1 input

Returns
  Result of operation

## ◆ mac_4x4_4x8() [4/8]

v32acc64 mac_4x4_4x8 | ( | v16int32 | a0,
|  | v32uint16 | b,
|  | v32acc64 | acc1 )

Parameters

  a0 | Matrix A
  b | Matrix B
  acc1 | Accumulator 1 input

Returns
  Result of operation

## ◆ mac_4x4_4x8() [5/8]

v32acc64 mac_4x4_4x8 | ( | v16uint32 | a0,
|  | int | sgn_x,
|  | v32int16 | b,
|  | int | sgn_y,
|  | v32acc64 | acc1 )

Parameters

  a0 | Matrix A
  sgn_x | Sign mask for matrix A
  b | Matrix B
  sgn_y | Sign mask for matrix B
  acc1 | Accumulator 1 input

Returns
  Result of operation

## ◆ mac_4x4_4x8() [6/8]

v32acc64 mac_4x4_4x8 | ( | v16uint32 | a0,
|  | int | sgn_x,
|  | v32uint16 | b,
|  | int | sgn_y,
|  | v32acc64 | acc1 )

Parameters

  a0 | Matrix A
  sgn_x | Sign mask for matrix A
  b | Matrix B
  sgn_y | Sign mask for matrix B
  acc1 | Accumulator 1 input

Returns
  Result of operation

## ◆ mac_4x4_4x8() [7/8]

v32acc64 mac_4x4_4x8 | ( | v16uint32 | a0,
|  | v32int16 | b,
|  | v32acc64 | acc1 )

Parameters

  a0 | Matrix A
  b | Matrix B
  acc1 | Accumulator 1 input

Returns
  Result of operation

## ◆ mac_4x4_4x8() [8/8]

v32acc64 mac_4x4_4x8 | ( | v16uint32 | a0,
|  | v32uint16 | b,
|  | v32acc64 | acc1 )

Parameters

  a0 | Matrix A
  b | Matrix B
  acc1 | Accumulator 1 input

Returns
  Result of operation

## ◆ mac_4x4_4x8_conf() [1/16]

v32acc64 mac_4x4_4x8_conf | ( | v16int32 | a0,
|  | int | sgn_x,
|  | v32int16 | b,
|  | int | sgn_y,
|  | v32acc64 | acc1,
|  | int | sub_mul,
|  | int | sub_acc1 )

Parameters

  a0 | Matrix A
  sgn_x | Sign mask for matrix A
  b | Matrix B
  sgn_y | Sign mask for matrix B
  acc1 | Accumulator 1 input
  sub_mul | Negation mask of multiplication result
  sub_acc1 | Negation mask of acc1

Returns
  Result of operation

## ◆ mac_4x4_4x8_conf() [2/16]

v32acc64 mac_4x4_4x8_conf | ( | v16int32 | a0,
|  | int | sgn_x,
|  | v32int16 | b,
|  | int | sgn_y,
|  | v32acc64 | acc1,
|  | int | zero_acc1,
|  | int | sub_mul,
|  | int | sub_acc1 )

Parameters

  a0 | Matrix A
  sgn_x | Sign mask for matrix A
  b | Matrix B
  sgn_y | Sign mask for matrix B
  acc1 | Accumulator 1 input
  zero_acc1 | Zeroing mask for acc1
  sub_mul | Negation mask of multiplication result
  sub_acc1 | Negation mask of acc1

Returns
  Result of operation

## ◆ mac_4x4_4x8_conf() [3/16]

v32acc64 mac_4x4_4x8_conf | ( | v16int32 | a0,
|  | int | sgn_x,
|  | v32uint16 | b,
|  | int | sgn_y,
|  | v32acc64 | acc1,
|  | int | sub_mul,
|  | int | sub_acc1 )

Parameters

  a0 | Matrix A
  sgn_x | Sign mask for matrix A
  b | Matrix B
  sgn_y | Sign mask for matrix B
  acc1 | Accumulator 1 input
  sub_mul | Negation mask of multiplication result
  sub_acc1 | Negation mask of acc1

Returns
  Result of operation

## ◆ mac_4x4_4x8_conf() [4/16]

v32acc64 mac_4x4_4x8_conf | ( | v16int32 | a0,
|  | int | sgn_x,
|  | v32uint16 | b,
|  | int | sgn_y,
|  | v32acc64 | acc1,
|  | int | zero_acc1,
|  | int | sub_mul,
|  | int | sub_acc1 )

Parameters

  a0 | Matrix A
  sgn_x | Sign mask for matrix A
  b | Matrix B
  sgn_y | Sign mask for matrix B
  acc1 | Accumulator 1 input
  zero_acc1 | Zeroing mask for acc1
  sub_mul | Negation mask of multiplication result
  sub_acc1 | Negation mask of acc1

Returns
  Result of operation

## ◆ mac_4x4_4x8_conf() [5/16]

v32acc64 mac_4x4_4x8_conf | ( | v16int32 | a0,
|  | v32int16 | b,
|  | v32acc64 | acc1,
|  | int | sub_mul,
|  | int | sub_acc1 )

Parameters

  a0 | Matrix A
  b | Matrix B
  acc1 | Accumulator 1 input
  sub_mul | Negation mask of multiplication result
  sub_acc1 | Negation mask of acc1

Returns
  Result of operation

## ◆ mac_4x4_4x8_conf() [6/16]

v32acc64 mac_4x4_4x8_conf | ( | v16int32 | a0,
|  | v32int16 | b,
|  | v32acc64 | acc1,
|  | int | zero_acc1,
|  | int | sub_mul,
|  | int | sub_acc1 )

Parameters

  a0 | Matrix A
  b | Matrix B
  acc1 | Accumulator 1 input
  zero_acc1 | Zeroing mask for acc1
  sub_mul | Negation mask of multiplication result
  sub_acc1 | Negation mask of acc1

Returns
  Result of operation

## ◆ mac_4x4_4x8_conf() [7/16]

v32acc64 mac_4x4_4x8_conf | ( | v16int32 | a0,
|  | v32uint16 | b,
|  | v32acc64 | acc1,
|  | int | sub_mul,
|  | int | sub_acc1 )

Parameters

  a0 | Matrix A
  b | Matrix B
  acc1 | Accumulator 1 input
  sub_mul | Negation mask of multiplication result
  sub_acc1 | Negation mask of acc1

Returns
  Result of operation

## ◆ mac_4x4_4x8_conf() [8/16]

v32acc64 mac_4x4_4x8_conf | ( | v16int32 | a0,
|  | v32uint16 | b,
|  | v32acc64 | acc1,
|  | int | zero_acc1,
|  | int | sub_mul,
|  | int | sub_acc1 )

Parameters

  a0 | Matrix A
  b | Matrix B
  acc1 | Accumulator 1 input
  zero_acc1 | Zeroing mask for acc1
  sub_mul | Negation mask of multiplication result
  sub_acc1 | Negation mask of acc1

Returns
  Result of operation

## ◆ mac_4x4_4x8_conf() [9/16]

v32acc64 mac_4x4_4x8_conf | ( | v16uint32 | a0,
|  | int | sgn_x,
|  | v32int16 | b,
|  | int | sgn_y,
|  | v32acc64 | acc1,
|  | int | sub_mul,
|  | int | sub_acc1 )

Parameters

  a0 | Matrix A
  sgn_x | Sign mask for matrix A
  b | Matrix B
  sgn_y | Sign mask for matrix B
  acc1 | Accumulator 1 input
  sub_mul | Negation mask of multiplication result
  sub_acc1 | Negation mask of acc1

Returns
  Result of operation

## ◆ mac_4x4_4x8_conf() [10/16]

v32acc64 mac_4x4_4x8_conf | ( | v16uint32 | a0,
|  | int | sgn_x,
|  | v32int16 | b,
|  | int | sgn_y,
|  | v32acc64 | acc1,
|  | int | zero_acc1,
|  | int | sub_mul,
|  | int | sub_acc1 )

Parameters

  a0 | Matrix A
  sgn_x | Sign mask for matrix A
  b | Matrix B
  sgn_y | Sign mask for matrix B
  acc1 | Accumulator 1 input
  zero_acc1 | Zeroing mask for acc1
  sub_mul | Negation mask of multiplication result
  sub_acc1 | Negation mask of acc1

Returns
  Result of operation

## ◆ mac_4x4_4x8_conf() [11/16]

v32acc64 mac_4x4_4x8_conf | ( | v16uint32 | a0,
|  | int | sgn_x,
|  | v32uint16 | b,
|  | int | sgn_y,
|  | v32acc64 | acc1,
|  | int | sub_mul,
|  | int | sub_acc1 )

Parameters

  a0 | Matrix A
  sgn_x | Sign mask for matrix A
  b | Matrix B
  sgn_y | Sign mask for matrix B
  acc1 | Accumulator 1 input
  sub_mul | Negation mask of multiplication result
  sub_acc1 | Negation mask of acc1

Returns
  Result of operation

## ◆ mac_4x4_4x8_conf() [12/16]

v32acc64 mac_4x4_4x8_conf | ( | v16uint32 | a0,
|  | int | sgn_x,
|  | v32uint16 | b,
|  | int | sgn_y,
|  | v32acc64 | acc1,
|  | int | zero_acc1,
|  | int | sub_mul,
|  | int | sub_acc1 )

Parameters

  a0 | Matrix A
  sgn_x | Sign mask for matrix A
  b | Matrix B
  sgn_y | Sign mask for matrix B
  acc1 | Accumulator 1 input
  zero_acc1 | Zeroing mask for acc1
  sub_mul | Negation mask of multiplication result
  sub_acc1 | Negation mask of acc1

Returns
  Result of operation

## ◆ mac_4x4_4x8_conf() [13/16]

v32acc64 mac_4x4_4x8_conf | ( | v16uint32 | a0,
|  | v32int16 | b,
|  | v32acc64 | acc1,
|  | int | sub_mul,
|  | int | sub_acc1 )

Parameters

  a0 | Matrix A
  b | Matrix B
  acc1 | Accumulator 1 input
  sub_mul | Negation mask of multiplication result
  sub_acc1 | Negation mask of acc1

Returns
  Result of operation

## ◆ mac_4x4_4x8_conf() [14/16]

v32acc64 mac_4x4_4x8_conf | ( | v16uint32 | a0,
|  | v32int16 | b,
|  | v32acc64 | acc1,
|  | int | zero_acc1,
|  | int | sub_mul,
|  | int | sub_acc1 )

Parameters

  a0 | Matrix A
  b | Matrix B
  acc1 | Accumulator 1 input
  zero_acc1 | Zeroing mask for acc1
  sub_mul | Negation mask of multiplication result
  sub_acc1 | Negation mask of acc1

Returns
  Result of operation

## ◆ mac_4x4_4x8_conf() [15/16]

v32acc64 mac_4x4_4x8_conf | ( | v16uint32 | a0,
|  | v32uint16 | b,
|  | v32acc64 | acc1,
|  | int | sub_mul,
|  | int | sub_acc1 )

Parameters

  a0 | Matrix A
  b | Matrix B
  acc1 | Accumulator 1 input
  sub_mul | Negation mask of multiplication result
  sub_acc1 | Negation mask of acc1

Returns
  Result of operation

## ◆ mac_4x4_4x8_conf() [16/16]

v32acc64 mac_4x4_4x8_conf | ( | v16uint32 | a0,
|  | v32uint16 | b,
|  | v32acc64 | acc1,
|  | int | zero_acc1,
|  | int | sub_mul,
|  | int | sub_acc1 )

Parameters

  a0 | Matrix A
  b | Matrix B
  acc1 | Accumulator 1 input
  zero_acc1 | Zeroing mask for acc1
  sub_mul | Negation mask of multiplication result
  sub_acc1 | Negation mask of acc1

Returns
  Result of operation

## ◆ mac_8x2_2x8() [1/8]

v64acc32 mac_8x2_2x8 | ( | v16int32 | a0,
|  | int | sgn_x,
|  | v32int16 | b,
|  | int | sgn_y,
|  | v64acc32 | acc1 )

Parameters

  a0 | Matrix A
  sgn_x | Sign mask for matrix A
  b | Matrix B
  sgn_y | Sign mask for matrix B
  acc1 | Accumulator 1 input

Returns
  Result of operation

## ◆ mac_8x2_2x8() [2/8]

v64acc32 mac_8x2_2x8 | ( | v16int32 | a0,
|  | int | sgn_x,
|  | v32uint16 | b,
|  | int | sgn_y,
|  | v64acc32 | acc1 )

Parameters

  a0 | Matrix A
  sgn_x | Sign mask for matrix A
  b | Matrix B
  sgn_y | Sign mask for matrix B
  acc1 | Accumulator 1 input

Returns
  Result of operation

## ◆ mac_8x2_2x8() [3/8]

v64acc32 mac_8x2_2x8 | ( | v16int32 | a0,
|  | v32int16 | b,
|  | v64acc32 | acc1 )

Parameters

  a0 | Matrix A
  b | Matrix B
  acc1 | Accumulator 1 input

Returns
  Result of operation

## ◆ mac_8x2_2x8() [4/8]

v64acc32 mac_8x2_2x8 | ( | v16int32 | a0,
|  | v32uint16 | b,
|  | v64acc32 | acc1 )

Parameters

  a0 | Matrix A
  b | Matrix B
  acc1 | Accumulator 1 input

Returns
  Result of operation

## ◆ mac_8x2_2x8() [5/8]

v64acc32 mac_8x2_2x8 | ( | v16uint32 | a0,
|  | int | sgn_x,
|  | v32int16 | b,
|  | int | sgn_y,
|  | v64acc32 | acc1 )

Parameters

  a0 | Matrix A
  sgn_x | Sign mask for matrix A
  b | Matrix B
  sgn_y | Sign mask for matrix B
  acc1 | Accumulator 1 input

Returns
  Result of operation

## ◆ mac_8x2_2x8() [6/8]

v64acc32 mac_8x2_2x8 | ( | v16uint32 | a0,
|  | int | sgn_x,
|  | v32uint16 | b,
|  | int | sgn_y,
|  | v64acc32 | acc1 )

Parameters

  a0 | Matrix A
  sgn_x | Sign mask for matrix A
  b | Matrix B
  sgn_y | Sign mask for matrix B
  acc1 | Accumulator 1 input

Returns
  Result of operation

## ◆ mac_8x2_2x8() [7/8]

v64acc32 mac_8x2_2x8 | ( | v16uint32 | a0,
|  | v32int16 | b,
|  | v64acc32 | acc1 )

Parameters

  a0 | Matrix A
  b | Matrix B
  acc1 | Accumulator 1 input

Returns
  Result of operation

## ◆ mac_8x2_2x8() [8/8]

v64acc32 mac_8x2_2x8 | ( | v16uint32 | a0,
|  | v32uint16 | b,
|  | v64acc32 | acc1 )

Parameters

  a0 | Matrix A
  b | Matrix B
  acc1 | Accumulator 1 input

Returns
  Result of operation

## ◆ mac_8x2_2x8_conf() [1/16]

v64acc32 mac_8x2_2x8_conf | ( | v16int32 | a0,
|  | int | sgn_x,
|  | v32int16 | b,
|  | int | sgn_y,
|  | v64acc32 | acc1,
|  | int | sub_mul,
|  | int | sub_acc1 )

Parameters

  a0 | Matrix A
  sgn_x | Sign mask for matrix A
  b | Matrix B
  sgn_y | Sign mask for matrix B
  acc1 | Accumulator 1 input
  sub_mul | Negation mask of multiplication result
  sub_acc1 | Negation mask of acc1

Returns
  Result of operation

## ◆ mac_8x2_2x8_conf() [2/16]

v64acc32 mac_8x2_2x8_conf | ( | v16int32 | a0,
|  | int | sgn_x,
|  | v32int16 | b,
|  | int | sgn_y,
|  | v64acc32 | acc1,
|  | int | zero_acc1,
|  | int | sub_mul,
|  | int | sub_acc1 )

Parameters

  a0 | Matrix A
  sgn_x | Sign mask for matrix A
  b | Matrix B
  sgn_y | Sign mask for matrix B
  acc1 | Accumulator 1 input
  zero_acc1 | Zeroing mask for acc1
  sub_mul | Negation mask of multiplication result
  sub_acc1 | Negation mask of acc1

Returns
  Result of operation

## ◆ mac_8x2_2x8_conf() [3/16]

v64acc32 mac_8x2_2x8_conf | ( | v16int32 | a0,
|  | int | sgn_x,
|  | v32uint16 | b,
|  | int | sgn_y,
|  | v64acc32 | acc1,
|  | int | sub_mul,
|  | int | sub_acc1 )

Parameters

  a0 | Matrix A
  sgn_x | Sign mask for matrix A
  b | Matrix B
  sgn_y | Sign mask for matrix B
  acc1 | Accumulator 1 input
  sub_mul | Negation mask of multiplication result
  sub_acc1 | Negation mask of acc1

Returns
  Result of operation

## ◆ mac_8x2_2x8_conf() [4/16]

v64acc32 mac_8x2_2x8_conf | ( | v16int32 | a0,
|  | int | sgn_x,
|  | v32uint16 | b,
|  | int | sgn_y,
|  | v64acc32 | acc1,
|  | int | zero_acc1,
|  | int | sub_mul,
|  | int | sub_acc1 )

Parameters

  a0 | Matrix A
  sgn_x | Sign mask for matrix A
  b | Matrix B
  sgn_y | Sign mask for matrix B
  acc1 | Accumulator 1 input
  zero_acc1 | Zeroing mask for acc1
  sub_mul | Negation mask of multiplication result
  sub_acc1 | Negation mask of acc1

Returns
  Result of operation

## ◆ mac_8x2_2x8_conf() [5/16]

v64acc32 mac_8x2_2x8_conf | ( | v16int32 | a0,
|  | v32int16 | b,
|  | v64acc32 | acc1,
|  | int | sub_mul,
|  | int | sub_acc1 )

Parameters

  a0 | Matrix A
  b | Matrix B
  acc1 | Accumulator 1 input
  sub_mul | Negation mask of multiplication result
  sub_acc1 | Negation mask of acc1

Returns
  Result of operation

## ◆ mac_8x2_2x8_conf() [6/16]

v64acc32 mac_8x2_2x8_conf | ( | v16int32 | a0,
|  | v32int16 | b,
|  | v64acc32 | acc1,
|  | int | zero_acc1,
|  | int | sub_mul,
|  | int | sub_acc1 )

Parameters

  a0 | Matrix A
  b | Matrix B
  acc1 | Accumulator 1 input
  zero_acc1 | Zeroing mask for acc1
  sub_mul | Negation mask of multiplication result
  sub_acc1 | Negation mask of acc1

Returns
  Result of operation

## ◆ mac_8x2_2x8_conf() [7/16]

v64acc32 mac_8x2_2x8_conf | ( | v16int32 | a0,
|  | v32uint16 | b,
|  | v64acc32 | acc1,
|  | int | sub_mul,
|  | int | sub_acc1 )

Parameters

  a0 | Matrix A
  b | Matrix B
  acc1 | Accumulator 1 input
  sub_mul | Negation mask of multiplication result
  sub_acc1 | Negation mask of acc1

Returns
  Result of operation

## ◆ mac_8x2_2x8_conf() [8/16]

v64acc32 mac_8x2_2x8_conf | ( | v16int32 | a0,
|  | v32uint16 | b,
|  | v64acc32 | acc1,
|  | int | zero_acc1,
|  | int | sub_mul,
|  | int | sub_acc1 )

Parameters

  a0 | Matrix A
  b | Matrix B
  acc1 | Accumulator 1 input
  zero_acc1 | Zeroing mask for acc1
  sub_mul | Negation mask of multiplication result
  sub_acc1 | Negation mask of acc1

Returns
  Result of operation

## ◆ mac_8x2_2x8_conf() [9/16]

v64acc32 mac_8x2_2x8_conf | ( | v16uint32 | a0,
|  | int | sgn_x,
|  | v32int16 | b,
|  | int | sgn_y,
|  | v64acc32 | acc1,
|  | int | sub_mul,
|  | int | sub_acc1 )

Parameters

  a0 | Matrix A
  sgn_x | Sign mask for matrix A
  b | Matrix B
  sgn_y | Sign mask for matrix B
  acc1 | Accumulator 1 input
  sub_mul | Negation mask of multiplication result
  sub_acc1 | Negation mask of acc1

Returns
  Result of operation

## ◆ mac_8x2_2x8_conf() [10/16]

v64acc32 mac_8x2_2x8_conf | ( | v16uint32 | a0,
|  | int | sgn_x,
|  | v32int16 | b,
|  | int | sgn_y,
|  | v64acc32 | acc1,
|  | int | zero_acc1,
|  | int | sub_mul,
|  | int | sub_acc1 )

Parameters

  a0 | Matrix A
  sgn_x | Sign mask for matrix A
  b | Matrix B
  sgn_y | Sign mask for matrix B
  acc1 | Accumulator 1 input
  zero_acc1 | Zeroing mask for acc1
  sub_mul | Negation mask of multiplication result
  sub_acc1 | Negation mask of acc1

Returns
  Result of operation

## ◆ mac_8x2_2x8_conf() [11/16]

v64acc32 mac_8x2_2x8_conf | ( | v16uint32 | a0,
|  | int | sgn_x,
|  | v32uint16 | b,
|  | int | sgn_y,
|  | v64acc32 | acc1,
|  | int | sub_mul,
|  | int | sub_acc1 )

Parameters

  a0 | Matrix A
  sgn_x | Sign mask for matrix A
  b | Matrix B
  sgn_y | Sign mask for matrix B
  acc1 | Accumulator 1 input
  sub_mul | Negation mask of multiplication result
  sub_acc1 | Negation mask of acc1

Returns
  Result of operation

## ◆ mac_8x2_2x8_conf() [12/16]

v64acc32 mac_8x2_2x8_conf | ( | v16uint32 | a0,
|  | int | sgn_x,
|  | v32uint16 | b,
|  | int | sgn_y,
|  | v64acc32 | acc1,
|  | int | zero_acc1,
|  | int | sub_mul,
|  | int | sub_acc1 )

Parameters

  a0 | Matrix A
  sgn_x | Sign mask for matrix A
  b | Matrix B
  sgn_y | Sign mask for matrix B
  acc1 | Accumulator 1 input
  zero_acc1 | Zeroing mask for acc1
  sub_mul | Negation mask of multiplication result
  sub_acc1 | Negation mask of acc1

Returns
  Result of operation

## ◆ mac_8x2_2x8_conf() [13/16]

v64acc32 mac_8x2_2x8_conf | ( | v16uint32 | a0,
|  | v32int16 | b,
|  | v64acc32 | acc1,
|  | int | sub_mul,
|  | int | sub_acc1 )

Parameters

  a0 | Matrix A
  b | Matrix B
  acc1 | Accumulator 1 input
  sub_mul | Negation mask of multiplication result
  sub_acc1 | Negation mask of acc1

Returns
  Result of operation

## ◆ mac_8x2_2x8_conf() [14/16]

v64acc32 mac_8x2_2x8_conf | ( | v16uint32 | a0,
|  | v32int16 | b,
|  | v64acc32 | acc1,
|  | int | zero_acc1,
|  | int | sub_mul,
|  | int | sub_acc1 )

Parameters

  a0 | Matrix A
  b | Matrix B
  acc1 | Accumulator 1 input
  zero_acc1 | Zeroing mask for acc1
  sub_mul | Negation mask of multiplication result
  sub_acc1 | Negation mask of acc1

Returns
  Result of operation

## ◆ mac_8x2_2x8_conf() [15/16]

v64acc32 mac_8x2_2x8_conf | ( | v16uint32 | a0,
|  | v32uint16 | b,
|  | v64acc32 | acc1,
|  | int | sub_mul,
|  | int | sub_acc1 )

Parameters

  a0 | Matrix A
  b | Matrix B
  acc1 | Accumulator 1 input
  sub_mul | Negation mask of multiplication result
  sub_acc1 | Negation mask of acc1

Returns
  Result of operation

## ◆ mac_8x2_2x8_conf() [16/16]

v64acc32 mac_8x2_2x8_conf | ( | v16uint32 | a0,
|  | v32uint16 | b,
|  | v64acc32 | acc1,
|  | int | zero_acc1,
|  | int | sub_mul,
|  | int | sub_acc1 )

Parameters

  a0 | Matrix A
  b | Matrix B
  acc1 | Accumulator 1 input
  zero_acc1 | Zeroing mask for acc1
  sub_mul | Negation mask of multiplication result
  sub_acc1 | Negation mask of acc1

Returns
  Result of operation

## ◆ mac_conv_4x4_8ch() [1/8]

v32acc64 mac_conv_4x4_8ch | ( | v32int32 | a0,
|  | v32int32 | a1,
|  | int | sgn_x,
|  | v32int16 | b,
|  | int | sgn_y,
|  | v32acc64 | acc1 )

Parameters

  a0 | Matrix A
  sgn_x | Sign mask for matrix A
  b | Matrix B
  sgn_y | Sign mask for matrix B
  acc1 | Accumulator 1 input

Returns
  Result of operation

## ◆ mac_conv_4x4_8ch() [2/8]

v32acc64 mac_conv_4x4_8ch | ( | v32int32 | a0,
|  | v32int32 | a1,
|  | int | sgn_x,
|  | v32uint16 | b,
|  | int | sgn_y,
|  | v32acc64 | acc1 )

Parameters

  a0 | Matrix A
  sgn_x | Sign mask for matrix A
  b | Matrix B
  sgn_y | Sign mask for matrix B
  acc1 | Accumulator 1 input

Returns
  Result of operation

## ◆ mac_conv_4x4_8ch() [3/8]

v32acc64 mac_conv_4x4_8ch | ( | v32int32 | a0,
|  | v32int32 | a1,
|  | v32int16 | b,
|  | v32acc64 | acc1 )

Parameters

  a0 | Matrix A
  b | Matrix B
  acc1 | Accumulator 1 input

Returns
  Result of operation

## ◆ mac_conv_4x4_8ch() [4/8]

v32acc64 mac_conv_4x4_8ch | ( | v32int32 | a0,
|  | v32int32 | a1,
|  | v32uint16 | b,
|  | v32acc64 | acc1 )

Parameters

  a0 | Matrix A
  b | Matrix B
  acc1 | Accumulator 1 input

Returns
  Result of operation

## ◆ mac_conv_4x4_8ch() [5/8]

v32acc64 mac_conv_4x4_8ch | ( | v32uint32 | a0,
|  | v32uint32 | a1,
|  | int | sgn_x,
|  | v32int16 | b,
|  | int | sgn_y,
|  | v32acc64 | acc1 )

Parameters

  a0 | Matrix A
  sgn_x | Sign mask for matrix A
  b | Matrix B
  sgn_y | Sign mask for matrix B
  acc1 | Accumulator 1 input

Returns
  Result of operation

## ◆ mac_conv_4x4_8ch() [6/8]

v32acc64 mac_conv_4x4_8ch | ( | v32uint32 | a0,
|  | v32uint32 | a1,
|  | int | sgn_x,
|  | v32uint16 | b,
|  | int | sgn_y,
|  | v32acc64 | acc1 )

Parameters

  a0 | Matrix A
  sgn_x | Sign mask for matrix A
  b | Matrix B
  sgn_y | Sign mask for matrix B
  acc1 | Accumulator 1 input

Returns
  Result of operation

## ◆ mac_conv_4x4_8ch() [7/8]

v32acc64 mac_conv_4x4_8ch | ( | v32uint32 | a0,
|  | v32uint32 | a1,
|  | v32int16 | b,
|  | v32acc64 | acc1 )

Parameters

  a0 | Matrix A
  b | Matrix B
  acc1 | Accumulator 1 input

Returns
  Result of operation

## ◆ mac_conv_4x4_8ch() [8/8]

v32acc64 mac_conv_4x4_8ch | ( | v32uint32 | a0,
|  | v32uint32 | a1,
|  | v32uint16 | b,
|  | v32acc64 | acc1 )

Parameters

  a0 | Matrix A
  b | Matrix B
  acc1 | Accumulator 1 input

Returns
  Result of operation

## ◆ mac_conv_4x4_8ch_conf() [1/16]

v32acc64 mac_conv_4x4_8ch_conf | ( | v32int32 | a0,
|  | v32int32 | a1,
|  | int | sgn_x,
|  | v32int16 | b,
|  | int | sgn_y,
|  | v32acc64 | acc1,
|  | int | sub_mul,
|  | int | sub_acc1 )

Parameters

  a0 | Matrix A
  sgn_x | Sign mask for matrix A
  b | Matrix B
  sgn_y | Sign mask for matrix B
  acc1 | Accumulator 1 input
  sub_mul | Negation mask of multiplication result
  sub_acc1 | Negation mask of acc1

Returns
  Result of operation

## ◆ mac_conv_4x4_8ch_conf() [2/16]

v32acc64 mac_conv_4x4_8ch_conf | ( | v32int32 | a0,
|  | v32int32 | a1,
|  | int | sgn_x,
|  | v32int16 | b,
|  | int | sgn_y,
|  | v32acc64 | acc1,
|  | int | zero_acc1,
|  | int | sub_mul,
|  | int | sub_acc1 )

Parameters

  a0 | Matrix A
  sgn_x | Sign mask for matrix A
  b | Matrix B
  sgn_y | Sign mask for matrix B
  acc1 | Accumulator 1 input
  zero_acc1 | Zeroing mask for acc1
  sub_mul | Negation mask of multiplication result
  sub_acc1 | Negation mask of acc1

Returns
  Result of operation

## ◆ mac_conv_4x4_8ch_conf() [3/16]

v32acc64 mac_conv_4x4_8ch_conf | ( | v32int32 | a0,
|  | v32int32 | a1,
|  | int | sgn_x,
|  | v32uint16 | b,
|  | int | sgn_y,
|  | v32acc64 | acc1,
|  | int | sub_mul,
|  | int | sub_acc1 )

Parameters

  a0 | Matrix A
  sgn_x | Sign mask for matrix A
  b | Matrix B
  sgn_y | Sign mask for matrix B
  acc1 | Accumulator 1 input
  sub_mul | Negation mask of multiplication result
  sub_acc1 | Negation mask of acc1

Returns
  Result of operation

## ◆ mac_conv_4x4_8ch_conf() [4/16]

v32acc64 mac_conv_4x4_8ch_conf | ( | v32int32 | a0,
|  | v32int32 | a1,
|  | int | sgn_x,
|  | v32uint16 | b,
|  | int | sgn_y,
|  | v32acc64 | acc1,
|  | int | zero_acc1,
|  | int | sub_mul,
|  | int | sub_acc1 )

Parameters

  a0 | Matrix A
  sgn_x | Sign mask for matrix A
  b | Matrix B
  sgn_y | Sign mask for matrix B
  acc1 | Accumulator 1 input
  zero_acc1 | Zeroing mask for acc1
  sub_mul | Negation mask of multiplication result
  sub_acc1 | Negation mask of acc1

Returns
  Result of operation

## ◆ mac_conv_4x4_8ch_conf() [5/16]

v32acc64 mac_conv_4x4_8ch_conf | ( | v32int32 | a0,
|  | v32int32 | a1,
|  | v32int16 | b,
|  | v32acc64 | acc1,
|  | int | sub_mul,
|  | int | sub_acc1 )

Parameters

  a0 | Matrix A
  b | Matrix B
  acc1 | Accumulator 1 input
  sub_mul | Negation mask of multiplication result
  sub_acc1 | Negation mask of acc1

Returns
  Result of operation

## ◆ mac_conv_4x4_8ch_conf() [6/16]

v32acc64 mac_conv_4x4_8ch_conf | ( | v32int32 | a0,
|  | v32int32 | a1,
|  | v32int16 | b,
|  | v32acc64 | acc1,
|  | int | zero_acc1,
|  | int | sub_mul,
|  | int | sub_acc1 )

Parameters

  a0 | Matrix A
  b | Matrix B
  acc1 | Accumulator 1 input
  zero_acc1 | Zeroing mask for acc1
  sub_mul | Negation mask of multiplication result
  sub_acc1 | Negation mask of acc1

Returns
  Result of operation

## ◆ mac_conv_4x4_8ch_conf() [7/16]

v32acc64 mac_conv_4x4_8ch_conf | ( | v32int32 | a0,
|  | v32int32 | a1,
|  | v32uint16 | b,
|  | v32acc64 | acc1,
|  | int | sub_mul,
|  | int | sub_acc1 )

Parameters

  a0 | Matrix A
  b | Matrix B
  acc1 | Accumulator 1 input
  sub_mul | Negation mask of multiplication result
  sub_acc1 | Negation mask of acc1

Returns
  Result of operation

## ◆ mac_conv_4x4_8ch_conf() [8/16]

v32acc64 mac_conv_4x4_8ch_conf | ( | v32int32 | a0,
|  | v32int32 | a1,
|  | v32uint16 | b,
|  | v32acc64 | acc1,
|  | int | zero_acc1,
|  | int | sub_mul,
|  | int | sub_acc1 )

Parameters

  a0 | Matrix A
  b | Matrix B
  acc1 | Accumulator 1 input
  zero_acc1 | Zeroing mask for acc1
  sub_mul | Negation mask of multiplication result
  sub_acc1 | Negation mask of acc1

Returns
  Result of operation

## ◆ mac_conv_4x4_8ch_conf() [9/16]

v32acc64 mac_conv_4x4_8ch_conf | ( | v32uint32 | a0,
|  | v32uint32 | a1,
|  | int | sgn_x,
|  | v32int16 | b,
|  | int | sgn_y,
|  | v32acc64 | acc1,
|  | int | sub_mul,
|  | int | sub_acc1 )

Parameters

  a0 | Matrix A
  sgn_x | Sign mask for matrix A
  b | Matrix B
  sgn_y | Sign mask for matrix B
  acc1 | Accumulator 1 input
  sub_mul | Negation mask of multiplication result
  sub_acc1 | Negation mask of acc1

Returns
  Result of operation

## ◆ mac_conv_4x4_8ch_conf() [10/16]

v32acc64 mac_conv_4x4_8ch_conf | ( | v32uint32 | a0,
|  | v32uint32 | a1,
|  | int | sgn_x,
|  | v32int16 | b,
|  | int | sgn_y,
|  | v32acc64 | acc1,
|  | int | zero_acc1,
|  | int | sub_mul,
|  | int | sub_acc1 )

Parameters

  a0 | Matrix A
  sgn_x | Sign mask for matrix A
  b | Matrix B
  sgn_y | Sign mask for matrix B
  acc1 | Accumulator 1 input
  zero_acc1 | Zeroing mask for acc1
  sub_mul | Negation mask of multiplication result
  sub_acc1 | Negation mask of acc1

Returns
  Result of operation

## ◆ mac_conv_4x4_8ch_conf() [11/16]

v32acc64 mac_conv_4x4_8ch_conf | ( | v32uint32 | a0,
|  | v32uint32 | a1,
|  | int | sgn_x,
|  | v32uint16 | b,
|  | int | sgn_y,
|  | v32acc64 | acc1,
|  | int | sub_mul,
|  | int | sub_acc1 )

Parameters

  a0 | Matrix A
  sgn_x | Sign mask for matrix A
  b | Matrix B
  sgn_y | Sign mask for matrix B
  acc1 | Accumulator 1 input
  sub_mul | Negation mask of multiplication result
  sub_acc1 | Negation mask of acc1

Returns
  Result of operation

## ◆ mac_conv_4x4_8ch_conf() [12/16]

v32acc64 mac_conv_4x4_8ch_conf | ( | v32uint32 | a0,
|  | v32uint32 | a1,
|  | int | sgn_x,
|  | v32uint16 | b,
|  | int | sgn_y,
|  | v32acc64 | acc1,
|  | int | zero_acc1,
|  | int | sub_mul,
|  | int | sub_acc1 )

Parameters

  a0 | Matrix A
  sgn_x | Sign mask for matrix A
  b | Matrix B
  sgn_y | Sign mask for matrix B
  acc1 | Accumulator 1 input
  zero_acc1 | Zeroing mask for acc1
  sub_mul | Negation mask of multiplication result
  sub_acc1 | Negation mask of acc1

Returns
  Result of operation

## ◆ mac_conv_4x4_8ch_conf() [13/16]

v32acc64 mac_conv_4x4_8ch_conf | ( | v32uint32 | a0,
|  | v32uint32 | a1,
|  | v32int16 | b,
|  | v32acc64 | acc1,
|  | int | sub_mul,
|  | int | sub_acc1 )

Parameters

  a0 | Matrix A
  b | Matrix B
  acc1 | Accumulator 1 input
  sub_mul | Negation mask of multiplication result
  sub_acc1 | Negation mask of acc1

Returns
  Result of operation

## ◆ mac_conv_4x4_8ch_conf() [14/16]

v32acc64 mac_conv_4x4_8ch_conf | ( | v32uint32 | a0,
|  | v32uint32 | a1,
|  | v32int16 | b,
|  | v32acc64 | acc1,
|  | int | zero_acc1,
|  | int | sub_mul,
|  | int | sub_acc1 )

Parameters

  a0 | Matrix A
  b | Matrix B
  acc1 | Accumulator 1 input
  zero_acc1 | Zeroing mask for acc1
  sub_mul | Negation mask of multiplication result
  sub_acc1 | Negation mask of acc1

Returns
  Result of operation

## ◆ mac_conv_4x4_8ch_conf() [15/16]

v32acc64 mac_conv_4x4_8ch_conf | ( | v32uint32 | a0,
|  | v32uint32 | a1,
|  | v32uint16 | b,
|  | v32acc64 | acc1,
|  | int | sub_mul,
|  | int | sub_acc1 )

Parameters

  a0 | Matrix A
  b | Matrix B
  acc1 | Accumulator 1 input
  sub_mul | Negation mask of multiplication result
  sub_acc1 | Negation mask of acc1

Returns
  Result of operation

## ◆ mac_conv_4x4_8ch_conf() [16/16]

v32acc64 mac_conv_4x4_8ch_conf | ( | v32uint32 | a0,
|  | v32uint32 | a1,
|  | v32uint16 | b,
|  | v32acc64 | acc1,
|  | int | zero_acc1,
|  | int | sub_mul,
|  | int | sub_acc1 )

Parameters

  a0 | Matrix A
  b | Matrix B
  acc1 | Accumulator 1 input
  zero_acc1 | Zeroing mask for acc1
  sub_mul | Negation mask of multiplication result
  sub_acc1 | Negation mask of acc1

Returns
  Result of operation

## ◆ mac_elem_32() [1/8]

v32acc64 mac_elem_32 | ( | v16int32 | a0,
|  | v16int32 | a1,
|  | int | sgn_x,
|  | v32int16 | b,
|  | int | sgn_y,
|  | v32acc64 | acc1 )

Parameters

  a0 | Matrix A
  sgn_x | Sign mask for matrix A
  b | Matrix B
  sgn_y | Sign mask for matrix B
  acc1 | Accumulator 1 input

Returns
  Result of operation

## ◆ mac_elem_32() [2/8]

v32acc64 mac_elem_32 | ( | v16int32 | a0,
|  | v16int32 | a1,
|  | int | sgn_x,
|  | v32uint16 | b,
|  | int | sgn_y,
|  | v32acc64 | acc1 )

Parameters

  a0 | Matrix A
  sgn_x | Sign mask for matrix A
  b | Matrix B
  sgn_y | Sign mask for matrix B
  acc1 | Accumulator 1 input

Returns
  Result of operation

## ◆ mac_elem_32() [3/8]

v32acc64 mac_elem_32 | ( | v16int32 | a0,
|  | v16int32 | a1,
|  | v32int16 | b,
|  | v32acc64 | acc1 )

Parameters

  a0 | Matrix A
  b | Matrix B
  acc1 | Accumulator 1 input

Returns
  Result of operation

## ◆ mac_elem_32() [4/8]

v32acc64 mac_elem_32 | ( | v16int32 | a0,
|  | v16int32 | a1,
|  | v32uint16 | b,
|  | v32acc64 | acc1 )

Parameters

  a0 | Matrix A
  b | Matrix B
  acc1 | Accumulator 1 input

Returns
  Result of operation

## ◆ mac_elem_32() [5/8]

v32acc64 mac_elem_32 | ( | v16uint32 | a0,
|  | v16uint32 | a1,
|  | int | sgn_x,
|  | v32int16 | b,
|  | int | sgn_y,
|  | v32acc64 | acc1 )

Parameters

  a0 | Matrix A
  sgn_x | Sign mask for matrix A
  b | Matrix B
  sgn_y | Sign mask for matrix B
  acc1 | Accumulator 1 input

Returns
  Result of operation

## ◆ mac_elem_32() [6/8]

v32acc64 mac_elem_32 | ( | v16uint32 | a0,
|  | v16uint32 | a1,
|  | int | sgn_x,
|  | v32uint16 | b,
|  | int | sgn_y,
|  | v32acc64 | acc1 )

Parameters

  a0 | Matrix A
  sgn_x | Sign mask for matrix A
  b | Matrix B
  sgn_y | Sign mask for matrix B
  acc1 | Accumulator 1 input

Returns
  Result of operation

## ◆ mac_elem_32() [7/8]

v32acc64 mac_elem_32 | ( | v16uint32 | a0,
|  | v16uint32 | a1,
|  | v32int16 | b,
|  | v32acc64 | acc1 )

Parameters

  a0 | Matrix A
  b | Matrix B
  acc1 | Accumulator 1 input

Returns
  Result of operation

## ◆ mac_elem_32() [8/8]

v32acc64 mac_elem_32 | ( | v16uint32 | a0,
|  | v16uint32 | a1,
|  | v32uint16 | b,
|  | v32acc64 | acc1 )

Parameters

  a0 | Matrix A
  b | Matrix B
  acc1 | Accumulator 1 input

Returns
  Result of operation

## ◆ mac_elem_32_2() [1/8]

v32acc64 mac_elem_32_2 | ( | v32int32 | a0,
|  | v32int32 | a1,
|  | int | sgn_x,
|  | v64int16 | b,
|  | int | sgn_y,
|  | v32acc64 | acc1 )

Parameters

  a0 | Matrix A
  sgn_x | Sign mask for matrix A
  b | Matrix B
  sgn_y | Sign mask for matrix B
  acc1 | Accumulator 1 input

Returns
  Result of operation

## ◆ mac_elem_32_2() [2/8]

v32acc64 mac_elem_32_2 | ( | v32int32 | a0,
|  | v32int32 | a1,
|  | int | sgn_x,
|  | v64uint16 | b,
|  | int | sgn_y,
|  | v32acc64 | acc1 )

Parameters

  a0 | Matrix A
  sgn_x | Sign mask for matrix A
  b | Matrix B
  sgn_y | Sign mask for matrix B
  acc1 | Accumulator 1 input

Returns
  Result of operation

## ◆ mac_elem_32_2() [3/8]

v32acc64 mac_elem_32_2 | ( | v32int32 | a0,
|  | v32int32 | a1,
|  | v64int16 | b,
|  | v32acc64 | acc1 )

Parameters

  a0 | Matrix A
  b | Matrix B
  acc1 | Accumulator 1 input

Returns
  Result of operation

## ◆ mac_elem_32_2() [4/8]

v32acc64 mac_elem_32_2 | ( | v32int32 | a0,
|  | v32int32 | a1,
|  | v64uint16 | b,
|  | v32acc64 | acc1 )

Parameters

  a0 | Matrix A
  b | Matrix B
  acc1 | Accumulator 1 input

Returns
  Result of operation

## ◆ mac_elem_32_2() [5/8]

v32acc64 mac_elem_32_2 | ( | v32uint32 | a0,
|  | v32uint32 | a1,
|  | int | sgn_x,
|  | v64int16 | b,
|  | int | sgn_y,
|  | v32acc64 | acc1 )

Parameters

  a0 | Matrix A
  sgn_x | Sign mask for matrix A
  b | Matrix B
  sgn_y | Sign mask for matrix B
  acc1 | Accumulator 1 input

Returns
  Result of operation

## ◆ mac_elem_32_2() [6/8]

v32acc64 mac_elem_32_2 | ( | v32uint32 | a0,
|  | v32uint32 | a1,
|  | int | sgn_x,
|  | v64uint16 | b,
|  | int | sgn_y,
|  | v32acc64 | acc1 )

Parameters

  a0 | Matrix A
  sgn_x | Sign mask for matrix A
  b | Matrix B
  sgn_y | Sign mask for matrix B
  acc1 | Accumulator 1 input

Returns
  Result of operation

## ◆ mac_elem_32_2() [7/8]

v32acc64 mac_elem_32_2 | ( | v32uint32 | a0,
|  | v32uint32 | a1,
|  | v64int16 | b,
|  | v32acc64 | acc1 )

Parameters

  a0 | Matrix A
  b | Matrix B
  acc1 | Accumulator 1 input

Returns
  Result of operation

## ◆ mac_elem_32_2() [8/8]

v32acc64 mac_elem_32_2 | ( | v32uint32 | a0,
|  | v32uint32 | a1,
|  | v64uint16 | b,
|  | v32acc64 | acc1 )

Parameters

  a0 | Matrix A
  b | Matrix B
  acc1 | Accumulator 1 input

Returns
  Result of operation

## ◆ mac_elem_32_2_conf() [1/16]

v32acc64 mac_elem_32_2_conf | ( | v32int32 | a0,
|  | v32int32 | a1,
|  | int | sgn_x,
|  | v64int16 | b,
|  | int | sgn_y,
|  | v32acc64 | acc1,
|  | int | sub_mul,
|  | int | sub_acc1 )

Parameters

  a0 | Matrix A
  sgn_x | Sign mask for matrix A
  b | Matrix B
  sgn_y | Sign mask for matrix B
  acc1 | Accumulator 1 input
  sub_mul | Negation mask of multiplication result
  sub_acc1 | Negation mask of acc1

Returns
  Result of operation

## ◆ mac_elem_32_2_conf() [2/16]

v32acc64 mac_elem_32_2_conf | ( | v32int32 | a0,
|  | v32int32 | a1,
|  | int | sgn_x,
|  | v64int16 | b,
|  | int | sgn_y,
|  | v32acc64 | acc1,
|  | int | zero_acc1,
|  | int | sub_mul,
|  | int | sub_acc1 )

Parameters

  a0 | Matrix A
  sgn_x | Sign mask for matrix A
  b | Matrix B
  sgn_y | Sign mask for matrix B
  acc1 | Accumulator 1 input
  zero_acc1 | Zeroing mask for acc1
  sub_mul | Negation mask of multiplication result
  sub_acc1 | Negation mask of acc1

Returns
  Result of operation

## ◆ mac_elem_32_2_conf() [3/16]

v32acc64 mac_elem_32_2_conf | ( | v32int32 | a0,
|  | v32int32 | a1,
|  | int | sgn_x,
|  | v64uint16 | b,
|  | int | sgn_y,
|  | v32acc64 | acc1,
|  | int | sub_mul,
|  | int | sub_acc1 )

Parameters

  a0 | Matrix A
  sgn_x | Sign mask for matrix A
  b | Matrix B
  sgn_y | Sign mask for matrix B
  acc1 | Accumulator 1 input
  sub_mul | Negation mask of multiplication result
  sub_acc1 | Negation mask of acc1

Returns
  Result of operation

## ◆ mac_elem_32_2_conf() [4/16]

v32acc64 mac_elem_32_2_conf | ( | v32int32 | a0,
|  | v32int32 | a1,
|  | int | sgn_x,
|  | v64uint16 | b,
|  | int | sgn_y,
|  | v32acc64 | acc1,
|  | int | zero_acc1,
|  | int | sub_mul,
|  | int | sub_acc1 )

Parameters

  a0 | Matrix A
  sgn_x | Sign mask for matrix A
  b | Matrix B
  sgn_y | Sign mask for matrix B
  acc1 | Accumulator 1 input
  zero_acc1 | Zeroing mask for acc1
  sub_mul | Negation mask of multiplication result
  sub_acc1 | Negation mask of acc1

Returns
  Result of operation

## ◆ mac_elem_32_2_conf() [5/16]

v32acc64 mac_elem_32_2_conf | ( | v32int32 | a0,
|  | v32int32 | a1,
|  | v64int16 | b,
|  | v32acc64 | acc1,
|  | int | sub_mul,
|  | int | sub_acc1 )

Parameters

  a0 | Matrix A
  b | Matrix B
  acc1 | Accumulator 1 input
  sub_mul | Negation mask of multiplication result
  sub_acc1 | Negation mask of acc1

Returns
  Result of operation

## ◆ mac_elem_32_2_conf() [6/16]

v32acc64 mac_elem_32_2_conf | ( | v32int32 | a0,
|  | v32int32 | a1,
|  | v64int16 | b,
|  | v32acc64 | acc1,
|  | int | zero_acc1,
|  | int | sub_mul,
|  | int | sub_acc1 )

Parameters

  a0 | Matrix A
  b | Matrix B
  acc1 | Accumulator 1 input
  zero_acc1 | Zeroing mask for acc1
  sub_mul | Negation mask of multiplication result
  sub_acc1 | Negation mask of acc1

Returns
  Result of operation

## ◆ mac_elem_32_2_conf() [7/16]

v32acc64 mac_elem_32_2_conf | ( | v32int32 | a0,
|  | v32int32 | a1,
|  | v64uint16 | b,
|  | v32acc64 | acc1,
|  | int | sub_mul,
|  | int | sub_acc1 )

Parameters

  a0 | Matrix A
  b | Matrix B
  acc1 | Accumulator 1 input
  sub_mul | Negation mask of multiplication result
  sub_acc1 | Negation mask of acc1

Returns
  Result of operation

## ◆ mac_elem_32_2_conf() [8/16]

v32acc64 mac_elem_32_2_conf | ( | v32int32 | a0,
|  | v32int32 | a1,
|  | v64uint16 | b,
|  | v32acc64 | acc1,
|  | int | zero_acc1,
|  | int | sub_mul,
|  | int | sub_acc1 )

Parameters

  a0 | Matrix A
  b | Matrix B
  acc1 | Accumulator 1 input
  zero_acc1 | Zeroing mask for acc1
  sub_mul | Negation mask of multiplication result
  sub_acc1 | Negation mask of acc1

Returns
  Result of operation

## ◆ mac_elem_32_2_conf() [9/16]

v32acc64 mac_elem_32_2_conf | ( | v32uint32 | a0,
|  | v32uint32 | a1,
|  | int | sgn_x,
|  | v64int16 | b,
|  | int | sgn_y,
|  | v32acc64 | acc1,
|  | int | sub_mul,
|  | int | sub_acc1 )

Parameters

  a0 | Matrix A
  sgn_x | Sign mask for matrix A
  b | Matrix B
  sgn_y | Sign mask for matrix B
  acc1 | Accumulator 1 input
  sub_mul | Negation mask of multiplication result
  sub_acc1 | Negation mask of acc1

Returns
  Result of operation

## ◆ mac_elem_32_2_conf() [10/16]

v32acc64 mac_elem_32_2_conf | ( | v32uint32 | a0,
|  | v32uint32 | a1,
|  | int | sgn_x,
|  | v64int16 | b,
|  | int | sgn_y,
|  | v32acc64 | acc1,
|  | int | zero_acc1,
|  | int | sub_mul,
|  | int | sub_acc1 )

Parameters

  a0 | Matrix A
  sgn_x | Sign mask for matrix A
  b | Matrix B
  sgn_y | Sign mask for matrix B
  acc1 | Accumulator 1 input
  zero_acc1 | Zeroing mask for acc1
  sub_mul | Negation mask of multiplication result
  sub_acc1 | Negation mask of acc1

Returns
  Result of operation

## ◆ mac_elem_32_2_conf() [11/16]

v32acc64 mac_elem_32_2_conf | ( | v32uint32 | a0,
|  | v32uint32 | a1,
|  | int | sgn_x,
|  | v64uint16 | b,
|  | int | sgn_y,
|  | v32acc64 | acc1,
|  | int | sub_mul,
|  | int | sub_acc1 )

Parameters

  a0 | Matrix A
  sgn_x | Sign mask for matrix A
  b | Matrix B
  sgn_y | Sign mask for matrix B
  acc1 | Accumulator 1 input
  sub_mul | Negation mask of multiplication result
  sub_acc1 | Negation mask of acc1

Returns
  Result of operation

## ◆ mac_elem_32_2_conf() [12/16]

v32acc64 mac_elem_32_2_conf | ( | v32uint32 | a0,
|  | v32uint32 | a1,
|  | int | sgn_x,
|  | v64uint16 | b,
|  | int | sgn_y,
|  | v32acc64 | acc1,
|  | int | zero_acc1,
|  | int | sub_mul,
|  | int | sub_acc1 )

Parameters

  a0 | Matrix A
  sgn_x | Sign mask for matrix A
  b | Matrix B
  sgn_y | Sign mask for matrix B
  acc1 | Accumulator 1 input
  zero_acc1 | Zeroing mask for acc1
  sub_mul | Negation mask of multiplication result
  sub_acc1 | Negation mask of acc1

Returns
  Result of operation

## ◆ mac_elem_32_2_conf() [13/16]

v32acc64 mac_elem_32_2_conf | ( | v32uint32 | a0,
|  | v32uint32 | a1,
|  | v64int16 | b,
|  | v32acc64 | acc1,
|  | int | sub_mul,
|  | int | sub_acc1 )

Parameters

  a0 | Matrix A
  b | Matrix B
  acc1 | Accumulator 1 input
  sub_mul | Negation mask of multiplication result
  sub_acc1 | Negation mask of acc1

Returns
  Result of operation

## ◆ mac_elem_32_2_conf() [14/16]

v32acc64 mac_elem_32_2_conf | ( | v32uint32 | a0,
|  | v32uint32 | a1,
|  | v64int16 | b,
|  | v32acc64 | acc1,
|  | int | zero_acc1,
|  | int | sub_mul,
|  | int | sub_acc1 )

Parameters

  a0 | Matrix A
  b | Matrix B
  acc1 | Accumulator 1 input
  zero_acc1 | Zeroing mask for acc1
  sub_mul | Negation mask of multiplication result
  sub_acc1 | Negation mask of acc1

Returns
  Result of operation

## ◆ mac_elem_32_2_conf() [15/16]

v32acc64 mac_elem_32_2_conf | ( | v32uint32 | a0,
|  | v32uint32 | a1,
|  | v64uint16 | b,
|  | v32acc64 | acc1,
|  | int | sub_mul,
|  | int | sub_acc1 )

Parameters

  a0 | Matrix A
  b | Matrix B
  acc1 | Accumulator 1 input
  sub_mul | Negation mask of multiplication result
  sub_acc1 | Negation mask of acc1

Returns
  Result of operation

## ◆ mac_elem_32_2_conf() [16/16]

v32acc64 mac_elem_32_2_conf | ( | v32uint32 | a0,
|  | v32uint32 | a1,
|  | v64uint16 | b,
|  | v32acc64 | acc1,
|  | int | zero_acc1,
|  | int | sub_mul,
|  | int | sub_acc1 )

Parameters

  a0 | Matrix A
  b | Matrix B
  acc1 | Accumulator 1 input
  zero_acc1 | Zeroing mask for acc1
  sub_mul | Negation mask of multiplication result
  sub_acc1 | Negation mask of acc1

Returns
  Result of operation

## ◆ mac_elem_32_conf() [1/16]

v32acc64 mac_elem_32_conf | ( | v16int32 | a0,
|  | v16int32 | a1,
|  | int | sgn_x,
|  | v32int16 | b,
|  | int | sgn_y,
|  | v32acc64 | acc1,
|  | int | sub_mul,
|  | int | sub_acc1 )

Parameters

  a0 | Matrix A
  sgn_x | Sign mask for matrix A
  b | Matrix B
  sgn_y | Sign mask for matrix B
  acc1 | Accumulator 1 input
  sub_mul | Negation mask of multiplication result
  sub_acc1 | Negation mask of acc1

Returns
  Result of operation

## ◆ mac_elem_32_conf() [2/16]

v32acc64 mac_elem_32_conf | ( | v16int32 | a0,
|  | v16int32 | a1,
|  | int | sgn_x,
|  | v32int16 | b,
|  | int | sgn_y,
|  | v32acc64 | acc1,
|  | int | zero_acc1,
|  | int | sub_mul,
|  | int | sub_acc1 )

Parameters

  a0 | Matrix A
  sgn_x | Sign mask for matrix A
  b | Matrix B
  sgn_y | Sign mask for matrix B
  acc1 | Accumulator 1 input
  zero_acc1 | Zeroing mask for acc1
  sub_mul | Negation mask of multiplication result
  sub_acc1 | Negation mask of acc1

Returns
  Result of operation

## ◆ mac_elem_32_conf() [3/16]

v32acc64 mac_elem_32_conf | ( | v16int32 | a0,
|  | v16int32 | a1,
|  | int | sgn_x,
|  | v32uint16 | b,
|  | int | sgn_y,
|  | v32acc64 | acc1,
|  | int | sub_mul,
|  | int | sub_acc1 )

Parameters

  a0 | Matrix A
  sgn_x | Sign mask for matrix A
  b | Matrix B
  sgn_y | Sign mask for matrix B
  acc1 | Accumulator 1 input
  sub_mul | Negation mask of multiplication result
  sub_acc1 | Negation mask of acc1

Returns
  Result of operation

## ◆ mac_elem_32_conf() [4/16]

v32acc64 mac_elem_32_conf | ( | v16int32 | a0,
|  | v16int32 | a1,
|  | int | sgn_x,
|  | v32uint16 | b,
|  | int | sgn_y,
|  | v32acc64 | acc1,
|  | int | zero_acc1,
|  | int | sub_mul,
|  | int | sub_acc1 )

Parameters

  a0 | Matrix A
  sgn_x | Sign mask for matrix A
  b | Matrix B
  sgn_y | Sign mask for matrix B
  acc1 | Accumulator 1 input
  zero_acc1 | Zeroing mask for acc1
  sub_mul | Negation mask of multiplication result
  sub_acc1 | Negation mask of acc1

Returns
  Result of operation

## ◆ mac_elem_32_conf() [5/16]

v32acc64 mac_elem_32_conf | ( | v16int32 | a0,
|  | v16int32 | a1,
|  | v32int16 | b,
|  | v32acc64 | acc1,
|  | int | sub_mul,
|  | int | sub_acc1 )

Parameters

  a0 | Matrix A
  b | Matrix B
  acc1 | Accumulator 1 input
  sub_mul | Negation mask of multiplication result
  sub_acc1 | Negation mask of acc1

Returns
  Result of operation

## ◆ mac_elem_32_conf() [6/16]

v32acc64 mac_elem_32_conf | ( | v16int32 | a0,
|  | v16int32 | a1,
|  | v32int16 | b,
|  | v32acc64 | acc1,
|  | int | zero_acc1,
|  | int | sub_mul,
|  | int | sub_acc1 )

Parameters

  a0 | Matrix A
  b | Matrix B
  acc1 | Accumulator 1 input
  zero_acc1 | Zeroing mask for acc1
  sub_mul | Negation mask of multiplication result
  sub_acc1 | Negation mask of acc1

Returns
  Result of operation

## ◆ mac_elem_32_conf() [7/16]

v32acc64 mac_elem_32_conf | ( | v16int32 | a0,
|  | v16int32 | a1,
|  | v32uint16 | b,
|  | v32acc64 | acc1,
|  | int | sub_mul,
|  | int | sub_acc1 )

Parameters

  a0 | Matrix A
  b | Matrix B
  acc1 | Accumulator 1 input
  sub_mul | Negation mask of multiplication result
  sub_acc1 | Negation mask of acc1

Returns
  Result of operation

## ◆ mac_elem_32_conf() [8/16]

v32acc64 mac_elem_32_conf | ( | v16int32 | a0,
|  | v16int32 | a1,
|  | v32uint16 | b,
|  | v32acc64 | acc1,
|  | int | zero_acc1,
|  | int | sub_mul,
|  | int | sub_acc1 )

Parameters

  a0 | Matrix A
  b | Matrix B
  acc1 | Accumulator 1 input
  zero_acc1 | Zeroing mask for acc1
  sub_mul | Negation mask of multiplication result
  sub_acc1 | Negation mask of acc1

Returns
  Result of operation

## ◆ mac_elem_32_conf() [9/16]

v32acc64 mac_elem_32_conf | ( | v16uint32 | a0,
|  | v16uint32 | a1,
|  | int | sgn_x,
|  | v32int16 | b,
|  | int | sgn_y,
|  | v32acc64 | acc1,
|  | int | sub_mul,
|  | int | sub_acc1 )

Parameters

  a0 | Matrix A
  sgn_x | Sign mask for matrix A
  b | Matrix B
  sgn_y | Sign mask for matrix B
  acc1 | Accumulator 1 input
  sub_mul | Negation mask of multiplication result
  sub_acc1 | Negation mask of acc1

Returns
  Result of operation

## ◆ mac_elem_32_conf() [10/16]

v32acc64 mac_elem_32_conf | ( | v16uint32 | a0,
|  | v16uint32 | a1,
|  | int | sgn_x,
|  | v32int16 | b,
|  | int | sgn_y,
|  | v32acc64 | acc1,
|  | int | zero_acc1,
|  | int | sub_mul,
|  | int | sub_acc1 )

Parameters

  a0 | Matrix A
  sgn_x | Sign mask for matrix A
  b | Matrix B
  sgn_y | Sign mask for matrix B
  acc1 | Accumulator 1 input
  zero_acc1 | Zeroing mask for acc1
  sub_mul | Negation mask of multiplication result
  sub_acc1 | Negation mask of acc1

Returns
  Result of operation

## ◆ mac_elem_32_conf() [11/16]

v32acc64 mac_elem_32_conf | ( | v16uint32 | a0,
|  | v16uint32 | a1,
|  | int | sgn_x,
|  | v32uint16 | b,
|  | int | sgn_y,
|  | v32acc64 | acc1,
|  | int | sub_mul,
|  | int | sub_acc1 )

Parameters

  a0 | Matrix A
  sgn_x | Sign mask for matrix A
  b | Matrix B
  sgn_y | Sign mask for matrix B
  acc1 | Accumulator 1 input
  sub_mul | Negation mask of multiplication result
  sub_acc1 | Negation mask of acc1

Returns
  Result of operation

## ◆ mac_elem_32_conf() [12/16]

v32acc64 mac_elem_32_conf | ( | v16uint32 | a0,
|  | v16uint32 | a1,
|  | int | sgn_x,
|  | v32uint16 | b,
|  | int | sgn_y,
|  | v32acc64 | acc1,
|  | int | zero_acc1,
|  | int | sub_mul,
|  | int | sub_acc1 )

Parameters

  a0 | Matrix A
  sgn_x | Sign mask for matrix A
  b | Matrix B
  sgn_y | Sign mask for matrix B
  acc1 | Accumulator 1 input
  zero_acc1 | Zeroing mask for acc1
  sub_mul | Negation mask of multiplication result
  sub_acc1 | Negation mask of acc1

Returns
  Result of operation

## ◆ mac_elem_32_conf() [13/16]

v32acc64 mac_elem_32_conf | ( | v16uint32 | a0,
|  | v16uint32 | a1,
|  | v32int16 | b,
|  | v32acc64 | acc1,
|  | int | sub_mul,
|  | int | sub_acc1 )

Parameters

  a0 | Matrix A
  b | Matrix B
  acc1 | Accumulator 1 input
  sub_mul | Negation mask of multiplication result
  sub_acc1 | Negation mask of acc1

Returns
  Result of operation

## ◆ mac_elem_32_conf() [14/16]

v32acc64 mac_elem_32_conf | ( | v16uint32 | a0,
|  | v16uint32 | a1,
|  | v32int16 | b,
|  | v32acc64 | acc1,
|  | int | zero_acc1,
|  | int | sub_mul,
|  | int | sub_acc1 )

Parameters

  a0 | Matrix A
  b | Matrix B
  acc1 | Accumulator 1 input
  zero_acc1 | Zeroing mask for acc1
  sub_mul | Negation mask of multiplication result
  sub_acc1 | Negation mask of acc1

Returns
  Result of operation

## ◆ mac_elem_32_conf() [15/16]

v32acc64 mac_elem_32_conf | ( | v16uint32 | a0,
|  | v16uint32 | a1,
|  | v32uint16 | b,
|  | v32acc64 | acc1,
|  | int | sub_mul,
|  | int | sub_acc1 )

Parameters

  a0 | Matrix A
  b | Matrix B
  acc1 | Accumulator 1 input
  sub_mul | Negation mask of multiplication result
  sub_acc1 | Negation mask of acc1

Returns
  Result of operation

## ◆ mac_elem_32_conf() [16/16]

v32acc64 mac_elem_32_conf | ( | v16uint32 | a0,
|  | v16uint32 | a1,
|  | v32uint16 | b,
|  | v32acc64 | acc1,
|  | int | zero_acc1,
|  | int | sub_mul,
|  | int | sub_acc1 )

Parameters

  a0 | Matrix A
  b | Matrix B
  acc1 | Accumulator 1 input
  zero_acc1 | Zeroing mask for acc1
  sub_mul | Negation mask of multiplication result
  sub_acc1 | Negation mask of acc1

Returns
  Result of operation

## ◆ msc_4x4_4x8() [1/8]

v32acc64 msc_4x4_4x8 | ( | v16int32 | a0,
|  | int | sgn_x,
|  | v32int16 | b,
|  | int | sgn_y,
|  | v32acc64 | acc1 )

Parameters

  a0 | Matrix A
  sgn_x | Sign mask for matrix A
  b | Matrix B
  sgn_y | Sign mask for matrix B
  acc1 | Accumulator 1 input

Returns
  Result of operation

## ◆ msc_4x4_4x8() [2/8]

v32acc64 msc_4x4_4x8 | ( | v16int32 | a0,
|  | int | sgn_x,
|  | v32uint16 | b,
|  | int | sgn_y,
|  | v32acc64 | acc1 )

Parameters

  a0 | Matrix A
  sgn_x | Sign mask for matrix A
  b | Matrix B
  sgn_y | Sign mask for matrix B
  acc1 | Accumulator 1 input

Returns
  Result of operation

## ◆ msc_4x4_4x8() [3/8]

v32acc64 msc_4x4_4x8 | ( | v16int32 | a0,
|  | v32int16 | b,
|  | v32acc64 | acc1 )

Parameters

  a0 | Matrix A
  b | Matrix B
  acc1 | Accumulator 1 input

Returns
  Result of operation

## ◆ msc_4x4_4x8() [4/8]

v32acc64 msc_4x4_4x8 | ( | v16int32 | a0,
|  | v32uint16 | b,
|  | v32acc64 | acc1 )

Parameters

  a0 | Matrix A
  b | Matrix B
  acc1 | Accumulator 1 input

Returns
  Result of operation

## ◆ msc_4x4_4x8() [5/8]

v32acc64 msc_4x4_4x8 | ( | v16uint32 | a0,
|  | int | sgn_x,
|  | v32int16 | b,
|  | int | sgn_y,
|  | v32acc64 | acc1 )

Parameters

  a0 | Matrix A
  sgn_x | Sign mask for matrix A
  b | Matrix B
  sgn_y | Sign mask for matrix B
  acc1 | Accumulator 1 input

Returns
  Result of operation

## ◆ msc_4x4_4x8() [6/8]

v32acc64 msc_4x4_4x8 | ( | v16uint32 | a0,
|  | int | sgn_x,
|  | v32uint16 | b,
|  | int | sgn_y,
|  | v32acc64 | acc1 )

Parameters

  a0 | Matrix A
  sgn_x | Sign mask for matrix A
  b | Matrix B
  sgn_y | Sign mask for matrix B
  acc1 | Accumulator 1 input

Returns
  Result of operation

## ◆ msc_4x4_4x8() [7/8]

v32acc64 msc_4x4_4x8 | ( | v16uint32 | a0,
|  | v32int16 | b,
|  | v32acc64 | acc1 )

Parameters

  a0 | Matrix A
  b | Matrix B
  acc1 | Accumulator 1 input

Returns
  Result of operation

## ◆ msc_4x4_4x8() [8/8]

v32acc64 msc_4x4_4x8 | ( | v16uint32 | a0,
|  | v32uint16 | b,
|  | v32acc64 | acc1 )

Parameters

  a0 | Matrix A
  b | Matrix B
  acc1 | Accumulator 1 input

Returns
  Result of operation

## ◆ msc_4x4_4x8_conf() [1/16]

v32acc64 msc_4x4_4x8_conf | ( | v16int32 | a0,
|  | int | sgn_x,
|  | v32int16 | b,
|  | int | sgn_y,
|  | v32acc64 | acc1,
|  | int | sub_mul,
|  | int | sub_acc1 )

Parameters

  a0 | Matrix A
  sgn_x | Sign mask for matrix A
  b | Matrix B
  sgn_y | Sign mask for matrix B
  acc1 | Accumulator 1 input
  sub_mul | Negation mask of multiplication result. If a bit is set the corresponding output accumulator lane is negated.
  sub_acc1 | Negation mask of acc1. If a bit is set the corresponding accumulator lane of acc1 is negated.

Returns
  Result of operation

## ◆ msc_4x4_4x8_conf() [2/16]

v32acc64 msc_4x4_4x8_conf | ( | v16int32 | a0,
|  | int | sgn_x,
|  | v32int16 | b,
|  | int | sgn_y,
|  | v32acc64 | acc1,
|  | int | zero_acc1,
|  | int | sub_mul,
|  | int | sub_acc1 )

Parameters

  a0 | Matrix A
  sgn_x | Sign mask for matrix A
  b | Matrix B
  sgn_y | Sign mask for matrix B
  acc1 | Accumulator 1 input
  zero_acc1 | Zeroing mask for acc1
  sub_mul | Negation mask of multiplication result. If a bit is set the corresponding output accumulator lane is negated.
  sub_acc1 | Negation mask of acc1. If a bit is set the corresponding accumulator lane of acc1 is negated.

Returns
  Result of operation

## ◆ msc_4x4_4x8_conf() [3/16]

v32acc64 msc_4x4_4x8_conf | ( | v16int32 | a0,
|  | int | sgn_x,
|  | v32uint16 | b,
|  | int | sgn_y,
|  | v32acc64 | acc1,
|  | int | sub_mul,
|  | int | sub_acc1 )

Parameters

  a0 | Matrix A
  sgn_x | Sign mask for matrix A
  b | Matrix B
  sgn_y | Sign mask for matrix B
  acc1 | Accumulator 1 input
  sub_mul | Negation mask of multiplication result. If a bit is set the corresponding output accumulator lane is negated.
  sub_acc1 | Negation mask of acc1. If a bit is set the corresponding accumulator lane of acc1 is negated.

Returns
  Result of operation

## ◆ msc_4x4_4x8_conf() [4/16]

v32acc64 msc_4x4_4x8_conf | ( | v16int32 | a0,
|  | int | sgn_x,
|  | v32uint16 | b,
|  | int | sgn_y,
|  | v32acc64 | acc1,
|  | int | zero_acc1,
|  | int | sub_mul,
|  | int | sub_acc1 )

Parameters

  a0 | Matrix A
  sgn_x | Sign mask for matrix A
  b | Matrix B
  sgn_y | Sign mask for matrix B
  acc1 | Accumulator 1 input
  zero_acc1 | Zeroing mask for acc1
  sub_mul | Negation mask of multiplication result. If a bit is set the corresponding output accumulator lane is negated.
  sub_acc1 | Negation mask of acc1. If a bit is set the corresponding accumulator lane of acc1 is negated.

Returns
  Result of operation

## ◆ msc_4x4_4x8_conf() [5/16]

v32acc64 msc_4x4_4x8_conf | ( | v16int32 | a0,
|  | v32int16 | b,
|  | v32acc64 | acc1,
|  | int | sub_mul,
|  | int | sub_acc1 )

Parameters

  a0 | Matrix A
  b | Matrix B
  acc1 | Accumulator 1 input
  sub_mul | Negation mask of multiplication result
  sub_acc1 | Negation mask of acc1

Returns
  Result of operation

## ◆ msc_4x4_4x8_conf() [6/16]

v32acc64 msc_4x4_4x8_conf | ( | v16int32 | a0,
|  | v32int16 | b,
|  | v32acc64 | acc1,
|  | int | zero_acc1,
|  | int | sub_mul,
|  | int | sub_acc1 )

Parameters

  a0 | Matrix A
  b | Matrix B
  acc1 | Accumulator 1 input
  zero_acc1 | Zeroing mask for acc1
  sub_mul | Negation mask of multiplication result
  sub_acc1 | Negation mask of acc1

Returns
  Result of operation

## ◆ msc_4x4_4x8_conf() [7/16]

v32acc64 msc_4x4_4x8_conf | ( | v16int32 | a0,
|  | v32uint16 | b,
|  | v32acc64 | acc1,
|  | int | sub_mul,
|  | int | sub_acc1 )

Parameters

  a0 | Matrix A
  b | Matrix B
  acc1 | Accumulator 1 input
  sub_mul | Negation mask of multiplication result
  sub_acc1 | Negation mask of acc1

Returns
  Result of operation

## ◆ msc_4x4_4x8_conf() [8/16]

v32acc64 msc_4x4_4x8_conf | ( | v16int32 | a0,
|  | v32uint16 | b,
|  | v32acc64 | acc1,
|  | int | zero_acc1,
|  | int | sub_mul,
|  | int | sub_acc1 )

Parameters

  a0 | Matrix A
  b | Matrix B
  acc1 | Accumulator 1 input
  zero_acc1 | Zeroing mask for acc1
  sub_mul | Negation mask of multiplication result
  sub_acc1 | Negation mask of acc1

Returns
  Result of operation

## ◆ msc_4x4_4x8_conf() [9/16]

v32acc64 msc_4x4_4x8_conf | ( | v16uint32 | a0,
|  | int | sgn_x,
|  | v32int16 | b,
|  | int | sgn_y,
|  | v32acc64 | acc1,
|  | int | sub_mul,
|  | int | sub_acc1 )

Parameters

  a0 | Matrix A
  sgn_x | Sign mask for matrix A
  b | Matrix B
  sgn_y | Sign mask for matrix B
  acc1 | Accumulator 1 input
  sub_mul | Negation mask of multiplication result. If a bit is set the corresponding output accumulator lane is negated.
  sub_acc1 | Negation mask of acc1. If a bit is set the corresponding accumulator lane of acc1 is negated.

Returns
  Result of operation

## ◆ msc_4x4_4x8_conf() [10/16]

v32acc64 msc_4x4_4x8_conf | ( | v16uint32 | a0,
|  | int | sgn_x,
|  | v32int16 | b,
|  | int | sgn_y,
|  | v32acc64 | acc1,
|  | int | zero_acc1,
|  | int | sub_mul,
|  | int | sub_acc1 )

Parameters

  a0 | Matrix A
  sgn_x | Sign mask for matrix A
  b | Matrix B
  sgn_y | Sign mask for matrix B
  acc1 | Accumulator 1 input
  zero_acc1 | Zeroing mask for acc1
  sub_mul | Negation mask of multiplication result. If a bit is set the corresponding output accumulator lane is negated.
  sub_acc1 | Negation mask of acc1. If a bit is set the corresponding accumulator lane of acc1 is negated.

Returns
  Result of operation

## ◆ msc_4x4_4x8_conf() [11/16]

v32acc64 msc_4x4_4x8_conf | ( | v16uint32 | a0,
|  | int | sgn_x,
|  | v32uint16 | b,
|  | int | sgn_y,
|  | v32acc64 | acc1,
|  | int | sub_mul,
|  | int | sub_acc1 )

Parameters

  a0 | Matrix A
  sgn_x | Sign mask for matrix A
  b | Matrix B
  sgn_y | Sign mask for matrix B
  acc1 | Accumulator 1 input
  sub_mul | Negation mask of multiplication result. If a bit is set the corresponding output accumulator lane is negated.
  sub_acc1 | Negation mask of acc1. If a bit is set the corresponding accumulator lane of acc1 is negated.

Returns
  Result of operation

## ◆ msc_4x4_4x8_conf() [12/16]

v32acc64 msc_4x4_4x8_conf | ( | v16uint32 | a0,
|  | int | sgn_x,
|  | v32uint16 | b,
|  | int | sgn_y,
|  | v32acc64 | acc1,
|  | int | zero_acc1,
|  | int | sub_mul,
|  | int | sub_acc1 )

Parameters

  a0 | Matrix A
  sgn_x | Sign mask for matrix A
  b | Matrix B
  sgn_y | Sign mask for matrix B
  acc1 | Accumulator 1 input
  zero_acc1 | Zeroing mask for acc1
  sub_mul | Negation mask of multiplication result. If a bit is set the corresponding output accumulator lane is negated.
  sub_acc1 | Negation mask of acc1. If a bit is set the corresponding accumulator lane of acc1 is negated.

Returns
  Result of operation

## ◆ msc_4x4_4x8_conf() [13/16]

v32acc64 msc_4x4_4x8_conf | ( | v16uint32 | a0,
|  | v32int16 | b,
|  | v32acc64 | acc1,
|  | int | sub_mul,
|  | int | sub_acc1 )

Parameters

  a0 | Matrix A
  b | Matrix B
  acc1 | Accumulator 1 input
  sub_mul | Negation mask of multiplication result
  sub_acc1 | Negation mask of acc1

Returns
  Result of operation

## ◆ msc_4x4_4x8_conf() [14/16]

v32acc64 msc_4x4_4x8_conf | ( | v16uint32 | a0,
|  | v32int16 | b,
|  | v32acc64 | acc1,
|  | int | zero_acc1,
|  | int | sub_mul,
|  | int | sub_acc1 )

Parameters

  a0 | Matrix A
  b | Matrix B
  acc1 | Accumulator 1 input
  zero_acc1 | Zeroing mask for acc1
  sub_mul | Negation mask of multiplication result
  sub_acc1 | Negation mask of acc1

Returns
  Result of operation

## ◆ msc_4x4_4x8_conf() [15/16]

v32acc64 msc_4x4_4x8_conf | ( | v16uint32 | a0,
|  | v32uint16 | b,
|  | v32acc64 | acc1,
|  | int | sub_mul,
|  | int | sub_acc1 )

Parameters

  a0 | Matrix A
  b | Matrix B
  acc1 | Accumulator 1 input
  sub_mul | Negation mask of multiplication result
  sub_acc1 | Negation mask of acc1

Returns
  Result of operation

## ◆ msc_4x4_4x8_conf() [16/16]

v32acc64 msc_4x4_4x8_conf | ( | v16uint32 | a0,
|  | v32uint16 | b,
|  | v32acc64 | acc1,
|  | int | zero_acc1,
|  | int | sub_mul,
|  | int | sub_acc1 )

Parameters

  a0 | Matrix A
  b | Matrix B
  acc1 | Accumulator 1 input
  zero_acc1 | Zeroing mask for acc1
  sub_mul | Negation mask of multiplication result
  sub_acc1 | Negation mask of acc1

Returns
  Result of operation

## ◆ msc_8x2_2x8() [1/8]

v64acc32 msc_8x2_2x8 | ( | v16int32 | a0,
|  | int | sgn_x,
|  | v32int16 | b,
|  | int | sgn_y,
|  | v64acc32 | acc1 )

Parameters

  a0 | Matrix A
  sgn_x | Sign mask for matrix A
  b | Matrix B
  sgn_y | Sign mask for matrix B
  acc1 | Accumulator 1 input

Returns
  Result of operation

## ◆ msc_8x2_2x8() [2/8]

v64acc32 msc_8x2_2x8 | ( | v16int32 | a0,
|  | int | sgn_x,
|  | v32uint16 | b,
|  | int | sgn_y,
|  | v64acc32 | acc1 )

Parameters

  a0 | Matrix A
  sgn_x | Sign mask for matrix A
  b | Matrix B
  sgn_y | Sign mask for matrix B
  acc1 | Accumulator 1 input

Returns
  Result of operation

## ◆ msc_8x2_2x8() [3/8]

v64acc32 msc_8x2_2x8 | ( | v16int32 | a0,
|  | v32int16 | b,
|  | v64acc32 | acc1 )

Parameters

  a0 | Matrix A
  b | Matrix B
  acc1 | Accumulator 1 input

Returns
  Result of operation

## ◆ msc_8x2_2x8() [4/8]

v64acc32 msc_8x2_2x8 | ( | v16int32 | a0,
|  | v32uint16 | b,
|  | v64acc32 | acc1 )

Parameters

  a0 | Matrix A
  b | Matrix B
  acc1 | Accumulator 1 input

Returns
  Result of operation

## ◆ msc_8x2_2x8() [5/8]

v64acc32 msc_8x2_2x8 | ( | v16uint32 | a0,
|  | int | sgn_x,
|  | v32int16 | b,
|  | int | sgn_y,
|  | v64acc32 | acc1 )

Parameters

  a0 | Matrix A
  sgn_x | Sign mask for matrix A
  b | Matrix B
  sgn_y | Sign mask for matrix B
  acc1 | Accumulator 1 input

Returns
  Result of operation

## ◆ msc_8x2_2x8() [6/8]

v64acc32 msc_8x2_2x8 | ( | v16uint32 | a0,
|  | int | sgn_x,
|  | v32uint16 | b,
|  | int | sgn_y,
|  | v64acc32 | acc1 )

Parameters

  a0 | Matrix A
  sgn_x | Sign mask for matrix A
  b | Matrix B
  sgn_y | Sign mask for matrix B
  acc1 | Accumulator 1 input

Returns
  Result of operation

## ◆ msc_8x2_2x8() [7/8]

v64acc32 msc_8x2_2x8 | ( | v16uint32 | a0,
|  | v32int16 | b,
|  | v64acc32 | acc1 )

Parameters

  a0 | Matrix A
  b | Matrix B
  acc1 | Accumulator 1 input

Returns
  Result of operation

## ◆ msc_8x2_2x8() [8/8]

v64acc32 msc_8x2_2x8 | ( | v16uint32 | a0,
|  | v32uint16 | b,
|  | v64acc32 | acc1 )

Parameters

  a0 | Matrix A
  b | Matrix B
  acc1 | Accumulator 1 input

Returns
  Result of operation

## ◆ msc_8x2_2x8_conf() [1/16]

v64acc32 msc_8x2_2x8_conf | ( | v16int32 | a0,
|  | int | sgn_x,
|  | v32int16 | b,
|  | int | sgn_y,
|  | v64acc32 | acc1,
|  | int | sub_mul,
|  | int | sub_acc1 )

Parameters

  a0 | Matrix A
  sgn_x | Sign mask for matrix A
  b | Matrix B
  sgn_y | Sign mask for matrix B
  acc1 | Accumulator 1 input
  sub_mul | Negation mask of multiplication result. If a bit is set the corresponding output accumulator lane is negated.
  sub_acc1 | Negation mask of acc1. If a bit is set the corresponding accumulator lane of acc1 is negated.

Returns
  Result of operation

## ◆ msc_8x2_2x8_conf() [2/16]

v64acc32 msc_8x2_2x8_conf | ( | v16int32 | a0,
|  | int | sgn_x,
|  | v32int16 | b,
|  | int | sgn_y,
|  | v64acc32 | acc1,
|  | int | zero_acc1,
|  | int | sub_mul,
|  | int | sub_acc1 )

Parameters

  a0 | Matrix A
  sgn_x | Sign mask for matrix A
  b | Matrix B
  sgn_y | Sign mask for matrix B
  acc1 | Accumulator 1 input
  zero_acc1 | Zeroing mask for acc1
  sub_mul | Negation mask of multiplication result. If a bit is set the corresponding output accumulator lane is negated.
  sub_acc1 | Negation mask of acc1. If a bit is set the corresponding accumulator lane of acc1 is negated.

Returns
  Result of operation

## ◆ msc_8x2_2x8_conf() [3/16]

v64acc32 msc_8x2_2x8_conf | ( | v16int32 | a0,
|  | int | sgn_x,
|  | v32uint16 | b,
|  | int | sgn_y,
|  | v64acc32 | acc1,
|  | int | sub_mul,
|  | int | sub_acc1 )

Parameters

  a0 | Matrix A
  sgn_x | Sign mask for matrix A
  b | Matrix B
  sgn_y | Sign mask for matrix B
  acc1 | Accumulator 1 input
  sub_mul | Negation mask of multiplication result. If a bit is set the corresponding output accumulator lane is negated.
  sub_acc1 | Negation mask of acc1. If a bit is set the corresponding accumulator lane of acc1 is negated.

Returns
  Result of operation

## ◆ msc_8x2_2x8_conf() [4/16]

v64acc32 msc_8x2_2x8_conf | ( | v16int32 | a0,
|  | int | sgn_x,
|  | v32uint16 | b,
|  | int | sgn_y,
|  | v64acc32 | acc1,
|  | int | zero_acc1,
|  | int | sub_mul,
|  | int | sub_acc1 )

Parameters

  a0 | Matrix A
  sgn_x | Sign mask for matrix A
  b | Matrix B
  sgn_y | Sign mask for matrix B
  acc1 | Accumulator 1 input
  zero_acc1 | Zeroing mask for acc1
  sub_mul | Negation mask of multiplication result. If a bit is set the corresponding output accumulator lane is negated.
  sub_acc1 | Negation mask of acc1. If a bit is set the corresponding accumulator lane of acc1 is negated.

Returns
  Result of operation

## ◆ msc_8x2_2x8_conf() [5/16]

v64acc32 msc_8x2_2x8_conf | ( | v16int32 | a0,
|  | v32int16 | b,
|  | v64acc32 | acc1,
|  | int | sub_mul,
|  | int | sub_acc1 )

Parameters

  a0 | Matrix A
  b | Matrix B
  acc1 | Accumulator 1 input
  sub_mul | Negation mask of multiplication result
  sub_acc1 | Negation mask of acc1

Returns
  Result of operation

## ◆ msc_8x2_2x8_conf() [6/16]

v64acc32 msc_8x2_2x8_conf | ( | v16int32 | a0,
|  | v32int16 | b,
|  | v64acc32 | acc1,
|  | int | zero_acc1,
|  | int | sub_mul,
|  | int | sub_acc1 )

Parameters

  a0 | Matrix A
  b | Matrix B
  acc1 | Accumulator 1 input
  zero_acc1 | Zeroing mask for acc1
  sub_mul | Negation mask of multiplication result
  sub_acc1 | Negation mask of acc1

Returns
  Result of operation

## ◆ msc_8x2_2x8_conf() [7/16]

v64acc32 msc_8x2_2x8_conf | ( | v16int32 | a0,
|  | v32uint16 | b,
|  | v64acc32 | acc1,
|  | int | sub_mul,
|  | int | sub_acc1 )

Parameters

  a0 | Matrix A
  b | Matrix B
  acc1 | Accumulator 1 input
  sub_mul | Negation mask of multiplication result
  sub_acc1 | Negation mask of acc1

Returns
  Result of operation

## ◆ msc_8x2_2x8_conf() [8/16]

v64acc32 msc_8x2_2x8_conf | ( | v16int32 | a0,
|  | v32uint16 | b,
|  | v64acc32 | acc1,
|  | int | zero_acc1,
|  | int | sub_mul,
|  | int | sub_acc1 )

Parameters

  a0 | Matrix A
  b | Matrix B
  acc1 | Accumulator 1 input
  zero_acc1 | Zeroing mask for acc1
  sub_mul | Negation mask of multiplication result
  sub_acc1 | Negation mask of acc1

Returns
  Result of operation

## ◆ msc_8x2_2x8_conf() [9/16]

v64acc32 msc_8x2_2x8_conf | ( | v16uint32 | a0,
|  | int | sgn_x,
|  | v32int16 | b,
|  | int | sgn_y,
|  | v64acc32 | acc1,
|  | int | sub_mul,
|  | int | sub_acc1 )

Parameters

  a0 | Matrix A
  sgn_x | Sign mask for matrix A
  b | Matrix B
  sgn_y | Sign mask for matrix B
  acc1 | Accumulator 1 input
  sub_mul | Negation mask of multiplication result. If a bit is set the corresponding output accumulator lane is negated.
  sub_acc1 | Negation mask of acc1. If a bit is set the corresponding accumulator lane of acc1 is negated.

Returns
  Result of operation

## ◆ msc_8x2_2x8_conf() [10/16]

v64acc32 msc_8x2_2x8_conf | ( | v16uint32 | a0,
|  | int | sgn_x,
|  | v32int16 | b,
|  | int | sgn_y,
|  | v64acc32 | acc1,
|  | int | zero_acc1,
|  | int | sub_mul,
|  | int | sub_acc1 )

Parameters

  a0 | Matrix A
  sgn_x | Sign mask for matrix A
  b | Matrix B
  sgn_y | Sign mask for matrix B
  acc1 | Accumulator 1 input
  zero_acc1 | Zeroing mask for acc1
  sub_mul | Negation mask of multiplication result. If a bit is set the corresponding output accumulator lane is negated.
  sub_acc1 | Negation mask of acc1. If a bit is set the corresponding accumulator lane of acc1 is negated.

Returns
  Result of operation

## ◆ msc_8x2_2x8_conf() [11/16]

v64acc32 msc_8x2_2x8_conf | ( | v16uint32 | a0,
|  | int | sgn_x,
|  | v32uint16 | b,
|  | int | sgn_y,
|  | v64acc32 | acc1,
|  | int | sub_mul,
|  | int | sub_acc1 )

Parameters

  a0 | Matrix A
  sgn_x | Sign mask for matrix A
  b | Matrix B
  sgn_y | Sign mask for matrix B
  acc1 | Accumulator 1 input
  sub_mul | Negation mask of multiplication result. If a bit is set the corresponding output accumulator lane is negated.
  sub_acc1 | Negation mask of acc1. If a bit is set the corresponding accumulator lane of acc1 is negated.

Returns
  Result of operation

## ◆ msc_8x2_2x8_conf() [12/16]

v64acc32 msc_8x2_2x8_conf | ( | v16uint32 | a0,
|  | int | sgn_x,
|  | v32uint16 | b,
|  | int | sgn_y,
|  | v64acc32 | acc1,
|  | int | zero_acc1,
|  | int | sub_mul,
|  | int | sub_acc1 )

Parameters

  a0 | Matrix A
  sgn_x | Sign mask for matrix A
  b | Matrix B
  sgn_y | Sign mask for matrix B
  acc1 | Accumulator 1 input
  zero_acc1 | Zeroing mask for acc1
  sub_mul | Negation mask of multiplication result. If a bit is set the corresponding output accumulator lane is negated.
  sub_acc1 | Negation mask of acc1. If a bit is set the corresponding accumulator lane of acc1 is negated.

Returns
  Result of operation

## ◆ msc_8x2_2x8_conf() [13/16]

v64acc32 msc_8x2_2x8_conf | ( | v16uint32 | a0,
|  | v32int16 | b,
|  | v64acc32 | acc1,
|  | int | sub_mul,
|  | int | sub_acc1 )

Parameters

  a0 | Matrix A
  b | Matrix B
  acc1 | Accumulator 1 input
  sub_mul | Negation mask of multiplication result
  sub_acc1 | Negation mask of acc1

Returns
  Result of operation

## ◆ msc_8x2_2x8_conf() [14/16]

v64acc32 msc_8x2_2x8_conf | ( | v16uint32 | a0,
|  | v32int16 | b,
|  | v64acc32 | acc1,
|  | int | zero_acc1,
|  | int | sub_mul,
|  | int | sub_acc1 )

Parameters

  a0 | Matrix A
  b | Matrix B
  acc1 | Accumulator 1 input
  zero_acc1 | Zeroing mask for acc1
  sub_mul | Negation mask of multiplication result
  sub_acc1 | Negation mask of acc1

Returns
  Result of operation

## ◆ msc_8x2_2x8_conf() [15/16]

v64acc32 msc_8x2_2x8_conf | ( | v16uint32 | a0,
|  | v32uint16 | b,
|  | v64acc32 | acc1,
|  | int | sub_mul,
|  | int | sub_acc1 )

Parameters

  a0 | Matrix A
  b | Matrix B
  acc1 | Accumulator 1 input
  sub_mul | Negation mask of multiplication result
  sub_acc1 | Negation mask of acc1

Returns
  Result of operation

## ◆ msc_8x2_2x8_conf() [16/16]

v64acc32 msc_8x2_2x8_conf | ( | v16uint32 | a0,
|  | v32uint16 | b,
|  | v64acc32 | acc1,
|  | int | zero_acc1,
|  | int | sub_mul,
|  | int | sub_acc1 )

Parameters

  a0 | Matrix A
  b | Matrix B
  acc1 | Accumulator 1 input
  zero_acc1 | Zeroing mask for acc1
  sub_mul | Negation mask of multiplication result
  sub_acc1 | Negation mask of acc1

Returns
  Result of operation

## ◆ msc_conv_4x4_8ch() [1/8]

v32acc64 msc_conv_4x4_8ch | ( | v32int32 | a0,
|  | v32int32 | a1,
|  | int | sgn_x,
|  | v32int16 | b,
|  | int | sgn_y,
|  | v32acc64 | acc1 )

Parameters

  a0 | Matrix A
  sgn_x | Sign mask for matrix A
  b | Matrix B
  sgn_y | Sign mask for matrix B
  acc1 | Accumulator 1 input

Returns
  Result of operation

## ◆ msc_conv_4x4_8ch() [2/8]

v32acc64 msc_conv_4x4_8ch | ( | v32int32 | a0,
|  | v32int32 | a1,
|  | int | sgn_x,
|  | v32uint16 | b,
|  | int | sgn_y,
|  | v32acc64 | acc1 )

Parameters

  a0 | Matrix A
  sgn_x | Sign mask for matrix A
  b | Matrix B
  sgn_y | Sign mask for matrix B
  acc1 | Accumulator 1 input

Returns
  Result of operation

## ◆ msc_conv_4x4_8ch() [3/8]

v32acc64 msc_conv_4x4_8ch | ( | v32int32 | a0,
|  | v32int32 | a1,
|  | v32int16 | b,
|  | v32acc64 | acc1 )

Parameters

  a0 | Matrix A
  b | Matrix B
  acc1 | Accumulator 1 input

Returns
  Result of operation

## ◆ msc_conv_4x4_8ch() [4/8]

v32acc64 msc_conv_4x4_8ch | ( | v32int32 | a0,
|  | v32int32 | a1,
|  | v32uint16 | b,
|  | v32acc64 | acc1 )

Parameters

  a0 | Matrix A
  b | Matrix B
  acc1 | Accumulator 1 input

Returns
  Result of operation

## ◆ msc_conv_4x4_8ch() [5/8]

v32acc64 msc_conv_4x4_8ch | ( | v32uint32 | a0,
|  | v32uint32 | a1,
|  | int | sgn_x,
|  | v32int16 | b,
|  | int | sgn_y,
|  | v32acc64 | acc1 )

Parameters

  a0 | Matrix A
  sgn_x | Sign mask for matrix A
  b | Matrix B
  sgn_y | Sign mask for matrix B
  acc1 | Accumulator 1 input

Returns
  Result of operation

## ◆ msc_conv_4x4_8ch() [6/8]

v32acc64 msc_conv_4x4_8ch | ( | v32uint32 | a0,
|  | v32uint32 | a1,
|  | int | sgn_x,
|  | v32uint16 | b,
|  | int | sgn_y,
|  | v32acc64 | acc1 )

Parameters

  a0 | Matrix A
  sgn_x | Sign mask for matrix A
  b | Matrix B
  sgn_y | Sign mask for matrix B
  acc1 | Accumulator 1 input

Returns
  Result of operation

## ◆ msc_conv_4x4_8ch() [7/8]

v32acc64 msc_conv_4x4_8ch | ( | v32uint32 | a0,
|  | v32uint32 | a1,
|  | v32int16 | b,
|  | v32acc64 | acc1 )

Parameters

  a0 | Matrix A
  b | Matrix B
  acc1 | Accumulator 1 input

Returns
  Result of operation

## ◆ msc_conv_4x4_8ch() [8/8]

v32acc64 msc_conv_4x4_8ch | ( | v32uint32 | a0,
|  | v32uint32 | a1,
|  | v32uint16 | b,
|  | v32acc64 | acc1 )

Parameters

  a0 | Matrix A
  b | Matrix B
  acc1 | Accumulator 1 input

Returns
  Result of operation

## ◆ msc_conv_4x4_8ch_conf() [1/16]

v32acc64 msc_conv_4x4_8ch_conf | ( | v32int32 | a0,
|  | v32int32 | a1,
|  | int | sgn_x,
|  | v32int16 | b,
|  | int | sgn_y,
|  | v32acc64 | acc1,
|  | int | sub_mul,
|  | int | sub_acc1 )

Parameters

  a0 | Matrix A
  sgn_x | Sign mask for matrix A
  b | Matrix B
  sgn_y | Sign mask for matrix B
  acc1 | Accumulator 1 input
  sub_mul | Negation mask of multiplication result. If a bit is set the corresponding output accumulator lane is negated.
  sub_acc1 | Negation mask of acc1. If a bit is set the corresponding accumulator lane of acc1 is negated.

Returns
  Result of operation

## ◆ msc_conv_4x4_8ch_conf() [2/16]

v32acc64 msc_conv_4x4_8ch_conf | ( | v32int32 | a0,
|  | v32int32 | a1,
|  | int | sgn_x,
|  | v32int16 | b,
|  | int | sgn_y,
|  | v32acc64 | acc1,
|  | int | zero_acc1,
|  | int | sub_mul,
|  | int | sub_acc1 )

Parameters

  a0 | Matrix A
  sgn_x | Sign mask for matrix A
  b | Matrix B
  sgn_y | Sign mask for matrix B
  acc1 | Accumulator 1 input
  zero_acc1 | Zeroing mask for acc1
  sub_mul | Negation mask of multiplication result. If a bit is set the corresponding output accumulator lane is negated.
  sub_acc1 | Negation mask of acc1. If a bit is set the corresponding accumulator lane of acc1 is negated.

Returns
  Result of operation

## ◆ msc_conv_4x4_8ch_conf() [3/16]

v32acc64 msc_conv_4x4_8ch_conf | ( | v32int32 | a0,
|  | v32int32 | a1,
|  | int | sgn_x,
|  | v32uint16 | b,
|  | int | sgn_y,
|  | v32acc64 | acc1,
|  | int | sub_mul,
|  | int | sub_acc1 )

Parameters

  a0 | Matrix A
  sgn_x | Sign mask for matrix A
  b | Matrix B
  sgn_y | Sign mask for matrix B
  acc1 | Accumulator 1 input
  sub_mul | Negation mask of multiplication result. If a bit is set the corresponding output accumulator lane is negated.
  sub_acc1 | Negation mask of acc1. If a bit is set the corresponding accumulator lane of acc1 is negated.

Returns
  Result of operation

## ◆ msc_conv_4x4_8ch_conf() [4/16]

v32acc64 msc_conv_4x4_8ch_conf | ( | v32int32 | a0,
|  | v32int32 | a1,
|  | int | sgn_x,
|  | v32uint16 | b,
|  | int | sgn_y,
|  | v32acc64 | acc1,
|  | int | zero_acc1,
|  | int | sub_mul,
|  | int | sub_acc1 )

Parameters

  a0 | Matrix A
  sgn_x | Sign mask for matrix A
  b | Matrix B
  sgn_y | Sign mask for matrix B
  acc1 | Accumulator 1 input
  zero_acc1 | Zeroing mask for acc1
  sub_mul | Negation mask of multiplication result. If a bit is set the corresponding output accumulator lane is negated.
  sub_acc1 | Negation mask of acc1. If a bit is set the corresponding accumulator lane of acc1 is negated.

Returns
  Result of operation

## ◆ msc_conv_4x4_8ch_conf() [5/16]

v32acc64 msc_conv_4x4_8ch_conf | ( | v32int32 | a0,
|  | v32int32 | a1,
|  | v32int16 | b,
|  | v32acc64 | acc1,
|  | int | sub_mul,
|  | int | sub_acc1 )

Parameters

  a0 | Matrix A
  b | Matrix B
  acc1 | Accumulator 1 input
  sub_mul | Negation mask of multiplication result
  sub_acc1 | Negation mask of acc1

Returns
  Result of operation

## ◆ msc_conv_4x4_8ch_conf() [6/16]

v32acc64 msc_conv_4x4_8ch_conf | ( | v32int32 | a0,
|  | v32int32 | a1,
|  | v32int16 | b,
|  | v32acc64 | acc1,
|  | int | zero_acc1,
|  | int | sub_mul,
|  | int | sub_acc1 )

Parameters

  a0 | Matrix A
  b | Matrix B
  acc1 | Accumulator 1 input
  zero_acc1 | Zeroing mask for acc1
  sub_mul | Negation mask of multiplication result
  sub_acc1 | Negation mask of acc1

Returns
  Result of operation

## ◆ msc_conv_4x4_8ch_conf() [7/16]

v32acc64 msc_conv_4x4_8ch_conf | ( | v32int32 | a0,
|  | v32int32 | a1,
|  | v32uint16 | b,
|  | v32acc64 | acc1,
|  | int | sub_mul,
|  | int | sub_acc1 )

Parameters

  a0 | Matrix A
  b | Matrix B
  acc1 | Accumulator 1 input
  sub_mul | Negation mask of multiplication result
  sub_acc1 | Negation mask of acc1

Returns
  Result of operation

## ◆ msc_conv_4x4_8ch_conf() [8/16]

v32acc64 msc_conv_4x4_8ch_conf | ( | v32int32 | a0,
|  | v32int32 | a1,
|  | v32uint16 | b,
|  | v32acc64 | acc1,
|  | int | zero_acc1,
|  | int | sub_mul,
|  | int | sub_acc1 )

Parameters

  a0 | Matrix A
  b | Matrix B
  acc1 | Accumulator 1 input
  zero_acc1 | Zeroing mask for acc1
  sub_mul | Negation mask of multiplication result
  sub_acc1 | Negation mask of acc1

Returns
  Result of operation

## ◆ msc_conv_4x4_8ch_conf() [9/16]

v32acc64 msc_conv_4x4_8ch_conf | ( | v32uint32 | a0,
|  | v32uint32 | a1,
|  | int | sgn_x,
|  | v32int16 | b,
|  | int | sgn_y,
|  | v32acc64 | acc1,
|  | int | sub_mul,
|  | int | sub_acc1 )

Parameters

  a0 | Matrix A
  sgn_x | Sign mask for matrix A
  b | Matrix B
  sgn_y | Sign mask for matrix B
  acc1 | Accumulator 1 input
  sub_mul | Negation mask of multiplication result. If a bit is set the corresponding output accumulator lane is negated.
  sub_acc1 | Negation mask of acc1. If a bit is set the corresponding accumulator lane of acc1 is negated.

Returns
  Result of operation

## ◆ msc_conv_4x4_8ch_conf() [10/16]

v32acc64 msc_conv_4x4_8ch_conf | ( | v32uint32 | a0,
|  | v32uint32 | a1,
|  | int | sgn_x,
|  | v32int16 | b,
|  | int | sgn_y,
|  | v32acc64 | acc1,
|  | int | zero_acc1,
|  | int | sub_mul,
|  | int | sub_acc1 )

Parameters

  a0 | Matrix A
  sgn_x | Sign mask for matrix A
  b | Matrix B
  sgn_y | Sign mask for matrix B
  acc1 | Accumulator 1 input
  zero_acc1 | Zeroing mask for acc1
  sub_mul | Negation mask of multiplication result. If a bit is set the corresponding output accumulator lane is negated.
  sub_acc1 | Negation mask of acc1. If a bit is set the corresponding accumulator lane of acc1 is negated.

Returns
  Result of operation

## ◆ msc_conv_4x4_8ch_conf() [11/16]

v32acc64 msc_conv_4x4_8ch_conf | ( | v32uint32 | a0,
|  | v32uint32 | a1,
|  | int | sgn_x,
|  | v32uint16 | b,
|  | int | sgn_y,
|  | v32acc64 | acc1,
|  | int | sub_mul,
|  | int | sub_acc1 )

Parameters

  a0 | Matrix A
  sgn_x | Sign mask for matrix A
  b | Matrix B
  sgn_y | Sign mask for matrix B
  acc1 | Accumulator 1 input
  sub_mul | Negation mask of multiplication result. If a bit is set the corresponding output accumulator lane is negated.
  sub_acc1 | Negation mask of acc1. If a bit is set the corresponding accumulator lane of acc1 is negated.

Returns
  Result of operation

## ◆ msc_conv_4x4_8ch_conf() [12/16]

v32acc64 msc_conv_4x4_8ch_conf | ( | v32uint32 | a0,
|  | v32uint32 | a1,
|  | int | sgn_x,
|  | v32uint16 | b,
|  | int | sgn_y,
|  | v32acc64 | acc1,
|  | int | zero_acc1,
|  | int | sub_mul,
|  | int | sub_acc1 )

Parameters

  a0 | Matrix A
  sgn_x | Sign mask for matrix A
  b | Matrix B
  sgn_y | Sign mask for matrix B
  acc1 | Accumulator 1 input
  zero_acc1 | Zeroing mask for acc1
  sub_mul | Negation mask of multiplication result. If a bit is set the corresponding output accumulator lane is negated.
  sub_acc1 | Negation mask of acc1. If a bit is set the corresponding accumulator lane of acc1 is negated.

Returns
  Result of operation

## ◆ msc_conv_4x4_8ch_conf() [13/16]

v32acc64 msc_conv_4x4_8ch_conf | ( | v32uint32 | a0,
|  | v32uint32 | a1,
|  | v32int16 | b,
|  | v32acc64 | acc1,
|  | int | sub_mul,
|  | int | sub_acc1 )

Parameters

  a0 | Matrix A
  b | Matrix B
  acc1 | Accumulator 1 input
  sub_mul | Negation mask of multiplication result
  sub_acc1 | Negation mask of acc1

Returns
  Result of operation

## ◆ msc_conv_4x4_8ch_conf() [14/16]

v32acc64 msc_conv_4x4_8ch_conf | ( | v32uint32 | a0,
|  | v32uint32 | a1,
|  | v32int16 | b,
|  | v32acc64 | acc1,
|  | int | zero_acc1,
|  | int | sub_mul,
|  | int | sub_acc1 )

Parameters

  a0 | Matrix A
  b | Matrix B
  acc1 | Accumulator 1 input
  zero_acc1 | Zeroing mask for acc1
  sub_mul | Negation mask of multiplication result
  sub_acc1 | Negation mask of acc1

Returns
  Result of operation

## ◆ msc_conv_4x4_8ch_conf() [15/16]

v32acc64 msc_conv_4x4_8ch_conf | ( | v32uint32 | a0,
|  | v32uint32 | a1,
|  | v32uint16 | b,
|  | v32acc64 | acc1,
|  | int | sub_mul,
|  | int | sub_acc1 )

Parameters

  a0 | Matrix A
  b | Matrix B
  acc1 | Accumulator 1 input
  sub_mul | Negation mask of multiplication result
  sub_acc1 | Negation mask of acc1

Returns
  Result of operation

## ◆ msc_conv_4x4_8ch_conf() [16/16]

v32acc64 msc_conv_4x4_8ch_conf | ( | v32uint32 | a0,
|  | v32uint32 | a1,
|  | v32uint16 | b,
|  | v32acc64 | acc1,
|  | int | zero_acc1,
|  | int | sub_mul,
|  | int | sub_acc1 )

Parameters

  a0 | Matrix A
  b | Matrix B
  acc1 | Accumulator 1 input
  zero_acc1 | Zeroing mask for acc1
  sub_mul | Negation mask of multiplication result
  sub_acc1 | Negation mask of acc1

Returns
  Result of operation

## ◆ msc_elem_32() [1/8]

v32acc64 msc_elem_32 | ( | v16int32 | a0,
|  | v16int32 | a1,
|  | int | sgn_x,
|  | v32int16 | b,
|  | int | sgn_y,
|  | v32acc64 | acc1 )

Parameters

  a0 | Matrix A
  sgn_x | Sign mask for matrix A
  b | Matrix B
  sgn_y | Sign mask for matrix B
  acc1 | Accumulator 1 input

Returns
  Result of operation

## ◆ msc_elem_32() [2/8]

v32acc64 msc_elem_32 | ( | v16int32 | a0,
|  | v16int32 | a1,
|  | int | sgn_x,
|  | v32uint16 | b,
|  | int | sgn_y,
|  | v32acc64 | acc1 )

Parameters

  a0 | Matrix A
  sgn_x | Sign mask for matrix A
  b | Matrix B
  sgn_y | Sign mask for matrix B
  acc1 | Accumulator 1 input

Returns
  Result of operation

## ◆ msc_elem_32() [3/8]

v32acc64 msc_elem_32 | ( | v16int32 | a0,
|  | v16int32 | a1,
|  | v32int16 | b,
|  | v32acc64 | acc1 )

Parameters

  a0 | Matrix A
  b | Matrix B
  acc1 | Accumulator 1 input

Returns
  Result of operation

## ◆ msc_elem_32() [4/8]

v32acc64 msc_elem_32 | ( | v16int32 | a0,
|  | v16int32 | a1,
|  | v32uint16 | b,
|  | v32acc64 | acc1 )

Parameters

  a0 | Matrix A
  b | Matrix B
  acc1 | Accumulator 1 input

Returns
  Result of operation

## ◆ msc_elem_32() [5/8]

v32acc64 msc_elem_32 | ( | v16uint32 | a0,
|  | v16uint32 | a1,
|  | int | sgn_x,
|  | v32int16 | b,
|  | int | sgn_y,
|  | v32acc64 | acc1 )

Parameters

  a0 | Matrix A
  sgn_x | Sign mask for matrix A
  b | Matrix B
  sgn_y | Sign mask for matrix B
  acc1 | Accumulator 1 input

Returns
  Result of operation

## ◆ msc_elem_32() [6/8]

v32acc64 msc_elem_32 | ( | v16uint32 | a0,
|  | v16uint32 | a1,
|  | int | sgn_x,
|  | v32uint16 | b,
|  | int | sgn_y,
|  | v32acc64 | acc1 )

Parameters

  a0 | Matrix A
  sgn_x | Sign mask for matrix A
  b | Matrix B
  sgn_y | Sign mask for matrix B
  acc1 | Accumulator 1 input

Returns
  Result of operation

## ◆ msc_elem_32() [7/8]

v32acc64 msc_elem_32 | ( | v16uint32 | a0,
|  | v16uint32 | a1,
|  | v32int16 | b,
|  | v32acc64 | acc1 )

Parameters

  a0 | Matrix A
  b | Matrix B
  acc1 | Accumulator 1 input

Returns
  Result of operation

## ◆ msc_elem_32() [8/8]

v32acc64 msc_elem_32 | ( | v16uint32 | a0,
|  | v16uint32 | a1,
|  | v32uint16 | b,
|  | v32acc64 | acc1 )

Parameters

  a0 | Matrix A
  b | Matrix B
  acc1 | Accumulator 1 input

Returns
  Result of operation

## ◆ msc_elem_32_2() [1/8]

v32acc64 msc_elem_32_2 | ( | v32int32 | a0,
|  | v32int32 | a1,
|  | int | sgn_x,
|  | v64int16 | b,
|  | int | sgn_y,
|  | v32acc64 | acc1 )

Parameters

  a0 | Matrix A
  sgn_x | Sign mask for matrix A
  b | Matrix B
  sgn_y | Sign mask for matrix B
  acc1 | Accumulator 1 input

Returns
  Result of operation

## ◆ msc_elem_32_2() [2/8]

v32acc64 msc_elem_32_2 | ( | v32int32 | a0,
|  | v32int32 | a1,
|  | int | sgn_x,
|  | v64uint16 | b,
|  | int | sgn_y,
|  | v32acc64 | acc1 )

Parameters

  a0 | Matrix A
  sgn_x | Sign mask for matrix A
  b | Matrix B
  sgn_y | Sign mask for matrix B
  acc1 | Accumulator 1 input

Returns
  Result of operation

## ◆ msc_elem_32_2() [3/8]

v32acc64 msc_elem_32_2 | ( | v32int32 | a0,
|  | v32int32 | a1,
|  | v64int16 | b,
|  | v32acc64 | acc1 )

Parameters

  a0 | Matrix A
  b | Matrix B
  acc1 | Accumulator 1 input

Returns
  Result of operation

## ◆ msc_elem_32_2() [4/8]

v32acc64 msc_elem_32_2 | ( | v32int32 | a0,
|  | v32int32 | a1,
|  | v64uint16 | b,
|  | v32acc64 | acc1 )

Parameters

  a0 | Matrix A
  b | Matrix B
  acc1 | Accumulator 1 input

Returns
  Result of operation

## ◆ msc_elem_32_2() [5/8]

v32acc64 msc_elem_32_2 | ( | v32uint32 | a0,
|  | v32uint32 | a1,
|  | int | sgn_x,
|  | v64int16 | b,
|  | int | sgn_y,
|  | v32acc64 | acc1 )

Parameters

  a0 | Matrix A
  sgn_x | Sign mask for matrix A
  b | Matrix B
  sgn_y | Sign mask for matrix B
  acc1 | Accumulator 1 input

Returns
  Result of operation

## ◆ msc_elem_32_2() [6/8]

v32acc64 msc_elem_32_2 | ( | v32uint32 | a0,
|  | v32uint32 | a1,
|  | int | sgn_x,
|  | v64uint16 | b,
|  | int | sgn_y,
|  | v32acc64 | acc1 )

Parameters

  a0 | Matrix A
  sgn_x | Sign mask for matrix A
  b | Matrix B
  sgn_y | Sign mask for matrix B
  acc1 | Accumulator 1 input

Returns
  Result of operation

## ◆ msc_elem_32_2() [7/8]

v32acc64 msc_elem_32_2 | ( | v32uint32 | a0,
|  | v32uint32 | a1,
|  | v64int16 | b,
|  | v32acc64 | acc1 )

Parameters

  a0 | Matrix A
  b | Matrix B
  acc1 | Accumulator 1 input

Returns
  Result of operation

## ◆ msc_elem_32_2() [8/8]

v32acc64 msc_elem_32_2 | ( | v32uint32 | a0,
|  | v32uint32 | a1,
|  | v64uint16 | b,
|  | v32acc64 | acc1 )

Parameters

  a0 | Matrix A
  b | Matrix B
  acc1 | Accumulator 1 input

Returns
  Result of operation

## ◆ msc_elem_32_2_conf() [1/16]

v32acc64 msc_elem_32_2_conf | ( | v32int32 | a0,
|  | v32int32 | a1,
|  | int | sgn_x,
|  | v64int16 | b,
|  | int | sgn_y,
|  | v32acc64 | acc1,
|  | int | sub_mul,
|  | int | sub_acc1 )

Parameters

  a0 | Matrix A
  sgn_x | Sign mask for matrix A
  b | Matrix B
  sgn_y | Sign mask for matrix B
  acc1 | Accumulator 1 input
  sub_mul | Negation mask of multiplication result. If a bit is set the corresponding output accumulator lane is negated.
  sub_acc1 | Negation mask of acc1. If a bit is set the corresponding accumulator lane of acc1 is negated.

Returns
  Result of operation

## ◆ msc_elem_32_2_conf() [2/16]

v32acc64 msc_elem_32_2_conf | ( | v32int32 | a0,
|  | v32int32 | a1,
|  | int | sgn_x,
|  | v64int16 | b,
|  | int | sgn_y,
|  | v32acc64 | acc1,
|  | int | zero_acc1,
|  | int | sub_mul,
|  | int | sub_acc1 )

Parameters

  a0 | Matrix A
  sgn_x | Sign mask for matrix A
  b | Matrix B
  sgn_y | Sign mask for matrix B
  acc1 | Accumulator 1 input
  zero_acc1 | Zeroing mask for acc1
  sub_mul | Negation mask of multiplication result. If a bit is set the corresponding output accumulator lane is negated.
  sub_acc1 | Negation mask of acc1. If a bit is set the corresponding accumulator lane of acc1 is negated.

Returns
  Result of operation

## ◆ msc_elem_32_2_conf() [3/16]

v32acc64 msc_elem_32_2_conf | ( | v32int32 | a0,
|  | v32int32 | a1,
|  | int | sgn_x,
|  | v64uint16 | b,
|  | int | sgn_y,
|  | v32acc64 | acc1,
|  | int | sub_mul,
|  | int | sub_acc1 )

Parameters

  a0 | Matrix A
  sgn_x | Sign mask for matrix A
  b | Matrix B
  sgn_y | Sign mask for matrix B
  acc1 | Accumulator 1 input
  sub_mul | Negation mask of multiplication result. If a bit is set the corresponding output accumulator lane is negated.
  sub_acc1 | Negation mask of acc1. If a bit is set the corresponding accumulator lane of acc1 is negated.

Returns
  Result of operation

## ◆ msc_elem_32_2_conf() [4/16]

v32acc64 msc_elem_32_2_conf | ( | v32int32 | a0,
|  | v32int32 | a1,
|  | int | sgn_x,
|  | v64uint16 | b,
|  | int | sgn_y,
|  | v32acc64 | acc1,
|  | int | zero_acc1,
|  | int | sub_mul,
|  | int | sub_acc1 )

Parameters

  a0 | Matrix A
  sgn_x | Sign mask for matrix A
  b | Matrix B
  sgn_y | Sign mask for matrix B
  acc1 | Accumulator 1 input
  zero_acc1 | Zeroing mask for acc1
  sub_mul | Negation mask of multiplication result. If a bit is set the corresponding output accumulator lane is negated.
  sub_acc1 | Negation mask of acc1. If a bit is set the corresponding accumulator lane of acc1 is negated.

Returns
  Result of operation

## ◆ msc_elem_32_2_conf() [5/16]

v32acc64 msc_elem_32_2_conf | ( | v32int32 | a0,
|  | v32int32 | a1,
|  | v64int16 | b,
|  | v32acc64 | acc1,
|  | int | sub_mul,
|  | int | sub_acc1 )

Parameters

  a0 | Matrix A
  b | Matrix B
  acc1 | Accumulator 1 input
  sub_mul | Negation mask of multiplication result
  sub_acc1 | Negation mask of acc1

Returns
  Result of operation

## ◆ msc_elem_32_2_conf() [6/16]

v32acc64 msc_elem_32_2_conf | ( | v32int32 | a0,
|  | v32int32 | a1,
|  | v64int16 | b,
|  | v32acc64 | acc1,
|  | int | zero_acc1,
|  | int | sub_mul,
|  | int | sub_acc1 )

Parameters

  a0 | Matrix A
  b | Matrix B
  acc1 | Accumulator 1 input
  zero_acc1 | Zeroing mask for acc1
  sub_mul | Negation mask of multiplication result
  sub_acc1 | Negation mask of acc1

Returns
  Result of operation

## ◆ msc_elem_32_2_conf() [7/16]

v32acc64 msc_elem_32_2_conf | ( | v32int32 | a0,
|  | v32int32 | a1,
|  | v64uint16 | b,
|  | v32acc64 | acc1,
|  | int | sub_mul,
|  | int | sub_acc1 )

Parameters

  a0 | Matrix A
  b | Matrix B
  acc1 | Accumulator 1 input
  sub_mul | Negation mask of multiplication result
  sub_acc1 | Negation mask of acc1

Returns
  Result of operation

## ◆ msc_elem_32_2_conf() [8/16]

v32acc64 msc_elem_32_2_conf | ( | v32int32 | a0,
|  | v32int32 | a1,
|  | v64uint16 | b,
|  | v32acc64 | acc1,
|  | int | zero_acc1,
|  | int | sub_mul,
|  | int | sub_acc1 )

Parameters

  a0 | Matrix A
  b | Matrix B
  acc1 | Accumulator 1 input
  zero_acc1 | Zeroing mask for acc1
  sub_mul | Negation mask of multiplication result
  sub_acc1 | Negation mask of acc1

Returns
  Result of operation

## ◆ msc_elem_32_2_conf() [9/16]

v32acc64 msc_elem_32_2_conf | ( | v32uint32 | a0,
|  | v32uint32 | a1,
|  | int | sgn_x,
|  | v64int16 | b,
|  | int | sgn_y,
|  | v32acc64 | acc1,
|  | int | sub_mul,
|  | int | sub_acc1 )

Parameters

  a0 | Matrix A
  sgn_x | Sign mask for matrix A
  b | Matrix B
  sgn_y | Sign mask for matrix B
  acc1 | Accumulator 1 input
  sub_mul | Negation mask of multiplication result. If a bit is set the corresponding output accumulator lane is negated.
  sub_acc1 | Negation mask of acc1. If a bit is set the corresponding accumulator lane of acc1 is negated.

Returns
  Result of operation

## ◆ msc_elem_32_2_conf() [10/16]

v32acc64 msc_elem_32_2_conf | ( | v32uint32 | a0,
|  | v32uint32 | a1,
|  | int | sgn_x,
|  | v64int16 | b,
|  | int | sgn_y,
|  | v32acc64 | acc1,
|  | int | zero_acc1,
|  | int | sub_mul,
|  | int | sub_acc1 )

Parameters

  a0 | Matrix A
  sgn_x | Sign mask for matrix A
  b | Matrix B
  sgn_y | Sign mask for matrix B
  acc1 | Accumulator 1 input
  zero_acc1 | Zeroing mask for acc1
  sub_mul | Negation mask of multiplication result. If a bit is set the corresponding output accumulator lane is negated.
  sub_acc1 | Negation mask of acc1. If a bit is set the corresponding accumulator lane of acc1 is negated.

Returns
  Result of operation

## ◆ msc_elem_32_2_conf() [11/16]

v32acc64 msc_elem_32_2_conf | ( | v32uint32 | a0,
|  | v32uint32 | a1,
|  | int | sgn_x,
|  | v64uint16 | b,
|  | int | sgn_y,
|  | v32acc64 | acc1,
|  | int | sub_mul,
|  | int | sub_acc1 )

Parameters

  a0 | Matrix A
  sgn_x | Sign mask for matrix A
  b | Matrix B
  sgn_y | Sign mask for matrix B
  acc1 | Accumulator 1 input
  sub_mul | Negation mask of multiplication result. If a bit is set the corresponding output accumulator lane is negated.
  sub_acc1 | Negation mask of acc1. If a bit is set the corresponding accumulator lane of acc1 is negated.

Returns
  Result of operation

## ◆ msc_elem_32_2_conf() [12/16]

v32acc64 msc_elem_32_2_conf | ( | v32uint32 | a0,
|  | v32uint32 | a1,
|  | int | sgn_x,
|  | v64uint16 | b,
|  | int | sgn_y,
|  | v32acc64 | acc1,
|  | int | zero_acc1,
|  | int | sub_mul,
|  | int | sub_acc1 )

Parameters

  a0 | Matrix A
  sgn_x | Sign mask for matrix A
  b | Matrix B
  sgn_y | Sign mask for matrix B
  acc1 | Accumulator 1 input
  zero_acc1 | Zeroing mask for acc1
  sub_mul | Negation mask of multiplication result. If a bit is set the corresponding output accumulator lane is negated.
  sub_acc1 | Negation mask of acc1. If a bit is set the corresponding accumulator lane of acc1 is negated.

Returns
  Result of operation

## ◆ msc_elem_32_2_conf() [13/16]

v32acc64 msc_elem_32_2_conf | ( | v32uint32 | a0,
|  | v32uint32 | a1,
|  | v64int16 | b,
|  | v32acc64 | acc1,
|  | int | sub_mul,
|  | int | sub_acc1 )

Parameters

  a0 | Matrix A
  b | Matrix B
  acc1 | Accumulator 1 input
  sub_mul | Negation mask of multiplication result
  sub_acc1 | Negation mask of acc1

Returns
  Result of operation

## ◆ msc_elem_32_2_conf() [14/16]

v32acc64 msc_elem_32_2_conf | ( | v32uint32 | a0,
|  | v32uint32 | a1,
|  | v64int16 | b,
|  | v32acc64 | acc1,
|  | int | zero_acc1,
|  | int | sub_mul,
|  | int | sub_acc1 )

Parameters

  a0 | Matrix A
  b | Matrix B
  acc1 | Accumulator 1 input
  zero_acc1 | Zeroing mask for acc1
  sub_mul | Negation mask of multiplication result
  sub_acc1 | Negation mask of acc1

Returns
  Result of operation

## ◆ msc_elem_32_2_conf() [15/16]

v32acc64 msc_elem_32_2_conf | ( | v32uint32 | a0,
|  | v32uint32 | a1,
|  | v64uint16 | b,
|  | v32acc64 | acc1,
|  | int | sub_mul,
|  | int | sub_acc1 )

Parameters

  a0 | Matrix A
  b | Matrix B
  acc1 | Accumulator 1 input
  sub_mul | Negation mask of multiplication result
  sub_acc1 | Negation mask of acc1

Returns
  Result of operation

## ◆ msc_elem_32_2_conf() [16/16]

v32acc64 msc_elem_32_2_conf | ( | v32uint32 | a0,
|  | v32uint32 | a1,
|  | v64uint16 | b,
|  | v32acc64 | acc1,
|  | int | zero_acc1,
|  | int | sub_mul,
|  | int | sub_acc1 )

Parameters

  a0 | Matrix A
  b | Matrix B
  acc1 | Accumulator 1 input
  zero_acc1 | Zeroing mask for acc1
  sub_mul | Negation mask of multiplication result
  sub_acc1 | Negation mask of acc1

Returns
  Result of operation

## ◆ msc_elem_32_conf() [1/16]

v32acc64 msc_elem_32_conf | ( | v16int32 | a0,
|  | v16int32 | a1,
|  | int | sgn_x,
|  | v32int16 | b,
|  | int | sgn_y,
|  | v32acc64 | acc1,
|  | int | sub_mul,
|  | int | sub_acc1 )

Parameters

  a0 | Matrix A
  sgn_x | Sign mask for matrix A
  b | Matrix B
  sgn_y | Sign mask for matrix B
  acc1 | Accumulator 1 input
  sub_mul | Negation mask of multiplication result. If a bit is set the corresponding output accumulator lane is negated.
  sub_acc1 | Negation mask of acc1. If a bit is set the corresponding accumulator lane of acc1 is negated.

Returns
  Result of operation

## ◆ msc_elem_32_conf() [2/16]

v32acc64 msc_elem_32_conf | ( | v16int32 | a0,
|  | v16int32 | a1,
|  | int | sgn_x,
|  | v32int16 | b,
|  | int | sgn_y,
|  | v32acc64 | acc1,
|  | int | zero_acc1,
|  | int | sub_mul,
|  | int | sub_acc1 )

Parameters

  a0 | Matrix A
  sgn_x | Sign mask for matrix A
  b | Matrix B
  sgn_y | Sign mask for matrix B
  acc1 | Accumulator 1 input
  zero_acc1 | Zeroing mask for acc1
  sub_mul | Negation mask of multiplication result. If a bit is set the corresponding output accumulator lane is negated.
  sub_acc1 | Negation mask of acc1. If a bit is set the corresponding accumulator lane of acc1 is negated.

Returns
  Result of operation

## ◆ msc_elem_32_conf() [3/16]

v32acc64 msc_elem_32_conf | ( | v16int32 | a0,
|  | v16int32 | a1,
|  | int | sgn_x,
|  | v32uint16 | b,
|  | int | sgn_y,
|  | v32acc64 | acc1,
|  | int | sub_mul,
|  | int | sub_acc1 )

Parameters

  a0 | Matrix A
  sgn_x | Sign mask for matrix A
  b | Matrix B
  sgn_y | Sign mask for matrix B
  acc1 | Accumulator 1 input
  sub_mul | Negation mask of multiplication result. If a bit is set the corresponding output accumulator lane is negated.
  sub_acc1 | Negation mask of acc1. If a bit is set the corresponding accumulator lane of acc1 is negated.

Returns
  Result of operation

## ◆ msc_elem_32_conf() [4/16]

v32acc64 msc_elem_32_conf | ( | v16int32 | a0,
|  | v16int32 | a1,
|  | int | sgn_x,
|  | v32uint16 | b,
|  | int | sgn_y,
|  | v32acc64 | acc1,
|  | int | zero_acc1,
|  | int | sub_mul,
|  | int | sub_acc1 )

Parameters

  a0 | Matrix A
  sgn_x | Sign mask for matrix A
  b | Matrix B
  sgn_y | Sign mask for matrix B
  acc1 | Accumulator 1 input
  zero_acc1 | Zeroing mask for acc1
  sub_mul | Negation mask of multiplication result. If a bit is set the corresponding output accumulator lane is negated.
  sub_acc1 | Negation mask of acc1. If a bit is set the corresponding accumulator lane of acc1 is negated.

Returns
  Result of operation

## ◆ msc_elem_32_conf() [5/16]

v32acc64 msc_elem_32_conf | ( | v16int32 | a0,
|  | v16int32 | a1,
|  | v32int16 | b,
|  | v32acc64 | acc1,
|  | int | sub_mul,
|  | int | sub_acc1 )

Parameters

  a0 | Matrix A
  b | Matrix B
  acc1 | Accumulator 1 input
  sub_mul | Negation mask of multiplication result
  sub_acc1 | Negation mask of acc1

Returns
  Result of operation

## ◆ msc_elem_32_conf() [6/16]

v32acc64 msc_elem_32_conf | ( | v16int32 | a0,
|  | v16int32 | a1,
|  | v32int16 | b,
|  | v32acc64 | acc1,
|  | int | zero_acc1,
|  | int | sub_mul,
|  | int | sub_acc1 )

Parameters

  a0 | Matrix A
  b | Matrix B
  acc1 | Accumulator 1 input
  zero_acc1 | Zeroing mask for acc1
  sub_mul | Negation mask of multiplication result
  sub_acc1 | Negation mask of acc1

Returns
  Result of operation

## ◆ msc_elem_32_conf() [7/16]

v32acc64 msc_elem_32_conf | ( | v16int32 | a0,
|  | v16int32 | a1,
|  | v32uint16 | b,
|  | v32acc64 | acc1,
|  | int | sub_mul,
|  | int | sub_acc1 )

Parameters

  a0 | Matrix A
  b | Matrix B
  acc1 | Accumulator 1 input
  sub_mul | Negation mask of multiplication result
  sub_acc1 | Negation mask of acc1

Returns
  Result of operation

## ◆ msc_elem_32_conf() [8/16]

v32acc64 msc_elem_32_conf | ( | v16int32 | a0,
|  | v16int32 | a1,
|  | v32uint16 | b,
|  | v32acc64 | acc1,
|  | int | zero_acc1,
|  | int | sub_mul,
|  | int | sub_acc1 )

Parameters

  a0 | Matrix A
  b | Matrix B
  acc1 | Accumulator 1 input
  zero_acc1 | Zeroing mask for acc1
  sub_mul | Negation mask of multiplication result
  sub_acc1 | Negation mask of acc1

Returns
  Result of operation

## ◆ msc_elem_32_conf() [9/16]

v32acc64 msc_elem_32_conf | ( | v16uint32 | a0,
|  | v16uint32 | a1,
|  | int | sgn_x,
|  | v32int16 | b,
|  | int | sgn_y,
|  | v32acc64 | acc1,
|  | int | sub_mul,
|  | int | sub_acc1 )

Parameters

  a0 | Matrix A
  sgn_x | Sign mask for matrix A
  b | Matrix B
  sgn_y | Sign mask for matrix B
  acc1 | Accumulator 1 input
  sub_mul | Negation mask of multiplication result. If a bit is set the corresponding output accumulator lane is negated.
  sub_acc1 | Negation mask of acc1. If a bit is set the corresponding accumulator lane of acc1 is negated.

Returns
  Result of operation

## ◆ msc_elem_32_conf() [10/16]

v32acc64 msc_elem_32_conf | ( | v16uint32 | a0,
|  | v16uint32 | a1,
|  | int | sgn_x,
|  | v32int16 | b,
|  | int | sgn_y,
|  | v32acc64 | acc1,
|  | int | zero_acc1,
|  | int | sub_mul,
|  | int | sub_acc1 )

Parameters

  a0 | Matrix A
  sgn_x | Sign mask for matrix A
  b | Matrix B
  sgn_y | Sign mask for matrix B
  acc1 | Accumulator 1 input
  zero_acc1 | Zeroing mask for acc1
  sub_mul | Negation mask of multiplication result. If a bit is set the corresponding output accumulator lane is negated.
  sub_acc1 | Negation mask of acc1. If a bit is set the corresponding accumulator lane of acc1 is negated.

Returns
  Result of operation

## ◆ msc_elem_32_conf() [11/16]

v32acc64 msc_elem_32_conf | ( | v16uint32 | a0,
|  | v16uint32 | a1,
|  | int | sgn_x,
|  | v32uint16 | b,
|  | int | sgn_y,
|  | v32acc64 | acc1,
|  | int | sub_mul,
|  | int | sub_acc1 )

Parameters

  a0 | Matrix A
  sgn_x | Sign mask for matrix A
  b | Matrix B
  sgn_y | Sign mask for matrix B
  acc1 | Accumulator 1 input
  sub_mul | Negation mask of multiplication result. If a bit is set the corresponding output accumulator lane is negated.
  sub_acc1 | Negation mask of acc1. If a bit is set the corresponding accumulator lane of acc1 is negated.

Returns
  Result of operation

## ◆ msc_elem_32_conf() [12/16]

v32acc64 msc_elem_32_conf | ( | v16uint32 | a0,
|  | v16uint32 | a1,
|  | int | sgn_x,
|  | v32uint16 | b,
|  | int | sgn_y,
|  | v32acc64 | acc1,
|  | int | zero_acc1,
|  | int | sub_mul,
|  | int | sub_acc1 )

Parameters

  a0 | Matrix A
  sgn_x | Sign mask for matrix A
  b | Matrix B
  sgn_y | Sign mask for matrix B
  acc1 | Accumulator 1 input
  zero_acc1 | Zeroing mask for acc1
  sub_mul | Negation mask of multiplication result. If a bit is set the corresponding output accumulator lane is negated.
  sub_acc1 | Negation mask of acc1. If a bit is set the corresponding accumulator lane of acc1 is negated.

Returns
  Result of operation

## ◆ msc_elem_32_conf() [13/16]

v32acc64 msc_elem_32_conf | ( | v16uint32 | a0,
|  | v16uint32 | a1,
|  | v32int16 | b,
|  | v32acc64 | acc1,
|  | int | sub_mul,
|  | int | sub_acc1 )

Parameters

  a0 | Matrix A
  b | Matrix B
  acc1 | Accumulator 1 input
  sub_mul | Negation mask of multiplication result
  sub_acc1 | Negation mask of acc1

Returns
  Result of operation

## ◆ msc_elem_32_conf() [14/16]

v32acc64 msc_elem_32_conf | ( | v16uint32 | a0,
|  | v16uint32 | a1,
|  | v32int16 | b,
|  | v32acc64 | acc1,
|  | int | zero_acc1,
|  | int | sub_mul,
|  | int | sub_acc1 )

Parameters

  a0 | Matrix A
  b | Matrix B
  acc1 | Accumulator 1 input
  zero_acc1 | Zeroing mask for acc1
  sub_mul | Negation mask of multiplication result
  sub_acc1 | Negation mask of acc1

Returns
  Result of operation

## ◆ msc_elem_32_conf() [15/16]

v32acc64 msc_elem_32_conf | ( | v16uint32 | a0,
|  | v16uint32 | a1,
|  | v32uint16 | b,
|  | v32acc64 | acc1,
|  | int | sub_mul,
|  | int | sub_acc1 )

Parameters

  a0 | Matrix A
  b | Matrix B
  acc1 | Accumulator 1 input
  sub_mul | Negation mask of multiplication result
  sub_acc1 | Negation mask of acc1

Returns
  Result of operation

## ◆ msc_elem_32_conf() [16/16]

v32acc64 msc_elem_32_conf | ( | v16uint32 | a0,
|  | v16uint32 | a1,
|  | v32uint16 | b,
|  | v32acc64 | acc1,
|  | int | zero_acc1,
|  | int | sub_mul,
|  | int | sub_acc1 )

Parameters

  a0 | Matrix A
  b | Matrix B
  acc1 | Accumulator 1 input
  zero_acc1 | Zeroing mask for acc1
  sub_mul | Negation mask of multiplication result
  sub_acc1 | Negation mask of acc1

Returns
  Result of operation

## ◆ mul_4x4_4x8() [1/8]

v32acc64 mul_4x4_4x8 | ( | v16int32 | a0,
|  | int | sgn_x,
|  | v32int16 | b,
|  | int | sgn_y )

Parameters

  a0 | Matrix A
  sgn_x | Sign mask for matrix A
  b | Matrix B
  sgn_y | Sign mask for matrix B

Returns
  Result of operation

## ◆ mul_4x4_4x8() [2/8]

v32acc64 mul_4x4_4x8 | ( | v16int32 | a0,
|  | int | sgn_x,
|  | v32uint16 | b,
|  | int | sgn_y )

Parameters

  a0 | Matrix A
  sgn_x | Sign mask for matrix A
  b | Matrix B
  sgn_y | Sign mask for matrix B

Returns
  Result of operation

## ◆ mul_4x4_4x8() [3/8]

v32acc64 mul_4x4_4x8 | ( | v16int32 | a0,
|  | v32int16 | b )

Parameters

  a0 | Matrix A
  b | Matrix B

Returns
  Result of operation

## ◆ mul_4x4_4x8() [4/8]

v32acc64 mul_4x4_4x8 | ( | v16int32 | a0,
|  | v32uint16 | b )

Parameters

  a0 | Matrix A
  b | Matrix B

Returns
  Result of operation

## ◆ mul_4x4_4x8() [5/8]

v32acc64 mul_4x4_4x8 | ( | v16uint32 | a0,
|  | int | sgn_x,
|  | v32int16 | b,
|  | int | sgn_y )

Parameters

  a0 | Matrix A
  sgn_x | Sign mask for matrix A
  b | Matrix B
  sgn_y | Sign mask for matrix B

Returns
  Result of operation

## ◆ mul_4x4_4x8() [6/8]

v32acc64 mul_4x4_4x8 | ( | v16uint32 | a0,
|  | int | sgn_x,
|  | v32uint16 | b,
|  | int | sgn_y )

Parameters

  a0 | Matrix A
  sgn_x | Sign mask for matrix A
  b | Matrix B
  sgn_y | Sign mask for matrix B

Returns
  Result of operation

## ◆ mul_4x4_4x8() [7/8]

v32acc64 mul_4x4_4x8 | ( | v16uint32 | a0,
|  | v32int16 | b )

Parameters

  a0 | Matrix A
  b | Matrix B

Returns
  Result of operation

## ◆ mul_4x4_4x8() [8/8]

v32acc64 mul_4x4_4x8 | ( | v16uint32 | a0,
|  | v32uint16 | b )

Parameters

  a0 | Matrix A
  b | Matrix B

Returns
  Result of operation

## ◆ mul_4x4_4x8_conf() [1/8]

v32acc64 mul_4x4_4x8_conf | ( | v16int32 | a0,
|  | int | sgn_x,
|  | v32int16 | b,
|  | int | sgn_y,
|  | int | sub_mul )

Parameters

  a0 | Matrix A
  sgn_x | Sign mask for matrix A
  b | Matrix B
  sgn_y | Sign mask for matrix B
  sub_mul | Negation mask of multiplication result. If a bit is set the corresponding output accumulator lane is negated.

Returns
  Result of operation

## ◆ mul_4x4_4x8_conf() [2/8]

v32acc64 mul_4x4_4x8_conf | ( | v16int32 | a0,
|  | int | sgn_x,
|  | v32uint16 | b,
|  | int | sgn_y,
|  | int | sub_mul )

Parameters

  a0 | Matrix A
  sgn_x | Sign mask for matrix A
  b | Matrix B
  sgn_y | Sign mask for matrix B
  sub_mul | Negation mask of multiplication result. If a bit is set the corresponding output accumulator lane is negated.

Returns
  Result of operation

## ◆ mul_4x4_4x8_conf() [3/8]

v32acc64 mul_4x4_4x8_conf | ( | v16int32 | a0,
|  | v32int16 | b,
|  | int | sub_mul )

Parameters

  a0 | Matrix A
  b | Matrix B
  sub_mul | Negation mask for multiplication result

Returns
  Result of operation

## ◆ mul_4x4_4x8_conf() [4/8]

v32acc64 mul_4x4_4x8_conf | ( | v16int32 | a0,
|  | v32uint16 | b,
|  | int | sub_mul )

Parameters

  a0 | Matrix A
  b | Matrix B
  sub_mul | Negation mask for multiplication result

Returns
  Result of operation

## ◆ mul_4x4_4x8_conf() [5/8]

v32acc64 mul_4x4_4x8_conf | ( | v16uint32 | a0,
|  | int | sgn_x,
|  | v32int16 | b,
|  | int | sgn_y,
|  | int | sub_mul )

Parameters

  a0 | Matrix A
  sgn_x | Sign mask for matrix A
  b | Matrix B
  sgn_y | Sign mask for matrix B
  sub_mul | Negation mask of multiplication result. If a bit is set the corresponding output accumulator lane is negated.

Returns
  Result of operation

## ◆ mul_4x4_4x8_conf() [6/8]

v32acc64 mul_4x4_4x8_conf | ( | v16uint32 | a0,
|  | int | sgn_x,
|  | v32uint16 | b,
|  | int | sgn_y,
|  | int | sub_mul )

Parameters

  a0 | Matrix A
  sgn_x | Sign mask for matrix A
  b | Matrix B
  sgn_y | Sign mask for matrix B
  sub_mul | Negation mask of multiplication result. If a bit is set the corresponding output accumulator lane is negated.

Returns
  Result of operation

## ◆ mul_4x4_4x8_conf() [7/8]

v32acc64 mul_4x4_4x8_conf | ( | v16uint32 | a0,
|  | v32int16 | b,
|  | int | sub_mul )

Parameters

  a0 | Matrix A
  b | Matrix B
  sub_mul | Negation mask for multiplication result

Returns
  Result of operation

## ◆ mul_4x4_4x8_conf() [8/8]

v32acc64 mul_4x4_4x8_conf | ( | v16uint32 | a0,
|  | v32uint16 | b,
|  | int | sub_mul )

Parameters

  a0 | Matrix A
  b | Matrix B
  sub_mul | Negation mask for multiplication result

Returns
  Result of operation

## ◆ mul_8x2_2x8() [1/8]

v64acc32 mul_8x2_2x8 | ( | v16int32 | a0,
|  | int | sgn_x,
|  | v32int16 | b,
|  | int | sgn_y )

Parameters

  a0 | Matrix A
  sgn_x | Sign mask for matrix A
  b | Matrix B
  sgn_y | Sign mask for matrix B

Returns
  Result of operation

## ◆ mul_8x2_2x8() [2/8]

v64acc32 mul_8x2_2x8 | ( | v16int32 | a0,
|  | int | sgn_x,
|  | v32uint16 | b,
|  | int | sgn_y )

Parameters

  a0 | Matrix A
  sgn_x | Sign mask for matrix A
  b | Matrix B
  sgn_y | Sign mask for matrix B

Returns
  Result of operation

## ◆ mul_8x2_2x8() [3/8]

v64acc32 mul_8x2_2x8 | ( | v16int32 | a0,
|  | v32int16 | b )

Parameters

  a0 | Matrix A
  b | Matrix B

Returns
  Result of operation

## ◆ mul_8x2_2x8() [4/8]

v64acc32 mul_8x2_2x8 | ( | v16int32 | a0,
|  | v32uint16 | b )

Parameters

  a0 | Matrix A
  b | Matrix B

Returns
  Result of operation

## ◆ mul_8x2_2x8() [5/8]

v64acc32 mul_8x2_2x8 | ( | v16uint32 | a0,
|  | int | sgn_x,
|  | v32int16 | b,
|  | int | sgn_y )

Parameters

  a0 | Matrix A
  sgn_x | Sign mask for matrix A
  b | Matrix B
  sgn_y | Sign mask for matrix B

Returns
  Result of operation

## ◆ mul_8x2_2x8() [6/8]

v64acc32 mul_8x2_2x8 | ( | v16uint32 | a0,
|  | int | sgn_x,
|  | v32uint16 | b,
|  | int | sgn_y )

Parameters

  a0 | Matrix A
  sgn_x | Sign mask for matrix A
  b | Matrix B
  sgn_y | Sign mask for matrix B

Returns
  Result of operation

## ◆ mul_8x2_2x8() [7/8]

v64acc32 mul_8x2_2x8 | ( | v16uint32 | a0,
|  | v32int16 | b )

Parameters

  a0 | Matrix A
  b | Matrix B

Returns
  Result of operation

## ◆ mul_8x2_2x8() [8/8]

v64acc32 mul_8x2_2x8 | ( | v16uint32 | a0,
|  | v32uint16 | b )

Parameters

  a0 | Matrix A
  b | Matrix B

Returns
  Result of operation

## ◆ mul_8x2_2x8_conf() [1/8]

v64acc32 mul_8x2_2x8_conf | ( | v16int32 | a0,
|  | int | sgn_x,
|  | v32int16 | b,
|  | int | sgn_y,
|  | int | sub_mul )

Parameters

  a0 | Matrix A
  sgn_x | Sign mask for matrix A
  b | Matrix B
  sgn_y | Sign mask for matrix B
  sub_mul | Negation mask of multiplication result. If a bit is set the corresponding output accumulator lane is negated.

Returns
  Result of operation

## ◆ mul_8x2_2x8_conf() [2/8]

v64acc32 mul_8x2_2x8_conf | ( | v16int32 | a0,
|  | int | sgn_x,
|  | v32uint16 | b,
|  | int | sgn_y,
|  | int | sub_mul )

Parameters

  a0 | Matrix A
  sgn_x | Sign mask for matrix A
  b | Matrix B
  sgn_y | Sign mask for matrix B
  sub_mul | Negation mask of multiplication result. If a bit is set the corresponding output accumulator lane is negated.

Returns
  Result of operation

## ◆ mul_8x2_2x8_conf() [3/8]

v64acc32 mul_8x2_2x8_conf | ( | v16int32 | a0,
|  | v32int16 | b,
|  | int | sub_mul )

Parameters

  a0 | Matrix A
  b | Matrix B
  sub_mul | Negation mask for multiplication result

Returns
  Result of operation

## ◆ mul_8x2_2x8_conf() [4/8]

v64acc32 mul_8x2_2x8_conf | ( | v16int32 | a0,
|  | v32uint16 | b,
|  | int | sub_mul )

Parameters

  a0 | Matrix A
  b | Matrix B
  sub_mul | Negation mask for multiplication result

Returns
  Result of operation

## ◆ mul_8x2_2x8_conf() [5/8]

v64acc32 mul_8x2_2x8_conf | ( | v16uint32 | a0,
|  | int | sgn_x,
|  | v32int16 | b,
|  | int | sgn_y,
|  | int | sub_mul )

Parameters

  a0 | Matrix A
  sgn_x | Sign mask for matrix A
  b | Matrix B
  sgn_y | Sign mask for matrix B
  sub_mul | Negation mask of multiplication result. If a bit is set the corresponding output accumulator lane is negated.

Returns
  Result of operation

## ◆ mul_8x2_2x8_conf() [6/8]

v64acc32 mul_8x2_2x8_conf | ( | v16uint32 | a0,
|  | int | sgn_x,
|  | v32uint16 | b,
|  | int | sgn_y,
|  | int | sub_mul )

Parameters

  a0 | Matrix A
  sgn_x | Sign mask for matrix A
  b | Matrix B
  sgn_y | Sign mask for matrix B
  sub_mul | Negation mask of multiplication result. If a bit is set the corresponding output accumulator lane is negated.

Returns
  Result of operation

## ◆ mul_8x2_2x8_conf() [7/8]

v64acc32 mul_8x2_2x8_conf | ( | v16uint32 | a0,
|  | v32int16 | b,
|  | int | sub_mul )

Parameters

  a0 | Matrix A
  b | Matrix B
  sub_mul | Negation mask for multiplication result

Returns
  Result of operation

## ◆ mul_8x2_2x8_conf() [8/8]

v64acc32 mul_8x2_2x8_conf | ( | v16uint32 | a0,
|  | v32uint16 | b,
|  | int | sub_mul )

Parameters

  a0 | Matrix A
  b | Matrix B
  sub_mul | Negation mask for multiplication result

Returns
  Result of operation

## ◆ mul_conv_4x4_8ch() [1/8]

v32acc64 mul_conv_4x4_8ch | ( | v32int32 | a0,
|  | v32int32 | a1,
|  | int | sgn_x,
|  | v32int16 | b,
|  | int | sgn_y )

Parameters

  a0 | Matrix A
  sgn_x | Sign mask for matrix A
  b | Matrix B
  sgn_y | Sign mask for matrix B

Returns
  Result of operation

## ◆ mul_conv_4x4_8ch() [2/8]

v32acc64 mul_conv_4x4_8ch | ( | v32int32 | a0,
|  | v32int32 | a1,
|  | int | sgn_x,
|  | v32uint16 | b,
|  | int | sgn_y )

Parameters

  a0 | Matrix A
  sgn_x | Sign mask for matrix A
  b | Matrix B
  sgn_y | Sign mask for matrix B

Returns
  Result of operation

## ◆ mul_conv_4x4_8ch() [3/8]

v32acc64 mul_conv_4x4_8ch | ( | v32int32 | a0,
|  | v32int32 | a1,
|  | v32int16 | b )

Parameters

  a0 | Matrix A
  b | Matrix B

Returns
  Result of operation

## ◆ mul_conv_4x4_8ch() [4/8]

v32acc64 mul_conv_4x4_8ch | ( | v32int32 | a0,
|  | v32int32 | a1,
|  | v32uint16 | b )

Parameters

  a0 | Matrix A
  b | Matrix B

Returns
  Result of operation

## ◆ mul_conv_4x4_8ch() [5/8]

v32acc64 mul_conv_4x4_8ch | ( | v32uint32 | a0,
|  | v32uint32 | a1,
|  | int | sgn_x,
|  | v32int16 | b,
|  | int | sgn_y )

Parameters

  a0 | Matrix A
  sgn_x | Sign mask for matrix A
  b | Matrix B
  sgn_y | Sign mask for matrix B

Returns
  Result of operation

## ◆ mul_conv_4x4_8ch() [6/8]

v32acc64 mul_conv_4x4_8ch | ( | v32uint32 | a0,
|  | v32uint32 | a1,
|  | int | sgn_x,
|  | v32uint16 | b,
|  | int | sgn_y )

Parameters

  a0 | Matrix A
  sgn_x | Sign mask for matrix A
  b | Matrix B
  sgn_y | Sign mask for matrix B

Returns
  Result of operation

## ◆ mul_conv_4x4_8ch() [7/8]

v32acc64 mul_conv_4x4_8ch | ( | v32uint32 | a0,
|  | v32uint32 | a1,
|  | v32int16 | b )

Parameters

  a0 | Matrix A
  b | Matrix B

Returns
  Result of operation

## ◆ mul_conv_4x4_8ch() [8/8]

v32acc64 mul_conv_4x4_8ch | ( | v32uint32 | a0,
|  | v32uint32 | a1,
|  | v32uint16 | b )

Parameters

  a0 | Matrix A
  b | Matrix B

Returns
  Result of operation

## ◆ mul_conv_4x4_8ch_conf() [1/8]

v32acc64 mul_conv_4x4_8ch_conf | ( | v32int32 | a0,
|  | v32int32 | a1,
|  | int | sgn_x,
|  | v32int16 | b,
|  | int | sgn_y,
|  | int | sub_mul )

Parameters

  a0 | Matrix A
  sgn_x | Sign mask for matrix A
  b | Matrix B
  sgn_y | Sign mask for matrix B
  sub_mul | Negation mask of multiplication result. If a bit is set the corresponding output accumulator lane is negated.

Returns
  Result of operation

## ◆ mul_conv_4x4_8ch_conf() [2/8]

v32acc64 mul_conv_4x4_8ch_conf | ( | v32int32 | a0,
|  | v32int32 | a1,
|  | int | sgn_x,
|  | v32uint16 | b,
|  | int | sgn_y,
|  | int | sub_mul )

Parameters

  a0 | Matrix A
  sgn_x | Sign mask for matrix A
  b | Matrix B
  sgn_y | Sign mask for matrix B
  sub_mul | Negation mask of multiplication result. If a bit is set the corresponding output accumulator lane is negated.

Returns
  Result of operation

## ◆ mul_conv_4x4_8ch_conf() [3/8]

v32acc64 mul_conv_4x4_8ch_conf | ( | v32int32 | a0,
|  | v32int32 | a1,
|  | v32int16 | b,
|  | int | sub_mul )

Parameters

  a0 | Matrix A
  b | Matrix B
  sub_mul | Negation mask for multiplication result

Returns
  Result of operation

## ◆ mul_conv_4x4_8ch_conf() [4/8]

v32acc64 mul_conv_4x4_8ch_conf | ( | v32int32 | a0,
|  | v32int32 | a1,
|  | v32uint16 | b,
|  | int | sub_mul )

Parameters

  a0 | Matrix A
  b | Matrix B
  sub_mul | Negation mask for multiplication result

Returns
  Result of operation

## ◆ mul_conv_4x4_8ch_conf() [5/8]

v32acc64 mul_conv_4x4_8ch_conf | ( | v32uint32 | a0,
|  | v32uint32 | a1,
|  | int | sgn_x,
|  | v32int16 | b,
|  | int | sgn_y,
|  | int | sub_mul )

Parameters

  a0 | Matrix A
  sgn_x | Sign mask for matrix A
  b | Matrix B
  sgn_y | Sign mask for matrix B
  sub_mul | Negation mask of multiplication result. If a bit is set the corresponding output accumulator lane is negated.

Returns
  Result of operation

## ◆ mul_conv_4x4_8ch_conf() [6/8]

v32acc64 mul_conv_4x4_8ch_conf | ( | v32uint32 | a0,
|  | v32uint32 | a1,
|  | int | sgn_x,
|  | v32uint16 | b,
|  | int | sgn_y,
|  | int | sub_mul )

Parameters

  a0 | Matrix A
  sgn_x | Sign mask for matrix A
  b | Matrix B
  sgn_y | Sign mask for matrix B
  sub_mul | Negation mask of multiplication result. If a bit is set the corresponding output accumulator lane is negated.

Returns
  Result of operation

## ◆ mul_conv_4x4_8ch_conf() [7/8]

v32acc64 mul_conv_4x4_8ch_conf | ( | v32uint32 | a0,
|  | v32uint32 | a1,
|  | v32int16 | b,
|  | int | sub_mul )

Parameters

  a0 | Matrix A
  b | Matrix B
  sub_mul | Negation mask for multiplication result

Returns
  Result of operation

## ◆ mul_conv_4x4_8ch_conf() [8/8]

v32acc64 mul_conv_4x4_8ch_conf | ( | v32uint32 | a0,
|  | v32uint32 | a1,
|  | v32uint16 | b,
|  | int | sub_mul )

Parameters

  a0 | Matrix A
  b | Matrix B
  sub_mul | Negation mask for multiplication result

Returns
  Result of operation

## ◆ mul_elem_32() [1/8]

v32acc64 mul_elem_32 | ( | v16int32 | a0,
|  | v16int32 | a1,
|  | int | sgn_x,
|  | v32int16 | b,
|  | int | sgn_y )

Parameters

  a0 | Matrix A
  sgn_x | Sign mask for matrix A
  b | Matrix B
  sgn_y | Sign mask for matrix B

Returns
  Result of operation

## ◆ mul_elem_32() [2/8]

v32acc64 mul_elem_32 | ( | v16int32 | a0,
|  | v16int32 | a1,
|  | int | sgn_x,
|  | v32uint16 | b,
|  | int | sgn_y )

Parameters

  a0 | Matrix A
  sgn_x | Sign mask for matrix A
  b | Matrix B
  sgn_y | Sign mask for matrix B

Returns
  Result of operation

## ◆ mul_elem_32() [3/8]

v32acc64 mul_elem_32 | ( | v16int32 | a0,
|  | v16int32 | a1,
|  | v32int16 | b )

Parameters

  a0 | Matrix A
  b | Matrix B

Returns
  Result of operation

## ◆ mul_elem_32() [4/8]

v32acc64 mul_elem_32 | ( | v16int32 | a0,
|  | v16int32 | a1,
|  | v32uint16 | b )

Parameters

  a0 | Matrix A
  b | Matrix B

Returns
  Result of operation

## ◆ mul_elem_32() [5/8]

v32acc64 mul_elem_32 | ( | v16uint32 | a0,
|  | v16uint32 | a1,
|  | int | sgn_x,
|  | v32int16 | b,
|  | int | sgn_y )

Parameters

  a0 | Matrix A
  sgn_x | Sign mask for matrix A
  b | Matrix B
  sgn_y | Sign mask for matrix B

Returns
  Result of operation

## ◆ mul_elem_32() [6/8]

v32acc64 mul_elem_32 | ( | v16uint32 | a0,
|  | v16uint32 | a1,
|  | int | sgn_x,
|  | v32uint16 | b,
|  | int | sgn_y )

Parameters

  a0 | Matrix A
  sgn_x | Sign mask for matrix A
  b | Matrix B
  sgn_y | Sign mask for matrix B

Returns
  Result of operation

## ◆ mul_elem_32() [7/8]

v32acc64 mul_elem_32 | ( | v16uint32 | a0,
|  | v16uint32 | a1,
|  | v32int16 | b )

Parameters

  a0 | Matrix A
  b | Matrix B

Returns
  Result of operation

## ◆ mul_elem_32() [8/8]

v32acc64 mul_elem_32 | ( | v16uint32 | a0,
|  | v16uint32 | a1,
|  | v32uint16 | b )

Parameters

  a0 | Matrix A
  b | Matrix B

Returns
  Result of operation

## ◆ mul_elem_32_2() [1/8]

v32acc64 mul_elem_32_2 | ( | v32int32 | a0,
|  | v32int32 | a1,
|  | int | sgn_x,
|  | v64int16 | b,
|  | int | sgn_y )

Parameters

  a0 | Matrix A
  sgn_x | Sign mask for matrix A
  b | Matrix B
  sgn_y | Sign mask for matrix B

Returns
  Result of operation

## ◆ mul_elem_32_2() [2/8]

v32acc64 mul_elem_32_2 | ( | v32int32 | a0,
|  | v32int32 | a1,
|  | int | sgn_x,
|  | v64uint16 | b,
|  | int | sgn_y )

Parameters

  a0 | Matrix A
  sgn_x | Sign mask for matrix A
  b | Matrix B
  sgn_y | Sign mask for matrix B

Returns
  Result of operation

## ◆ mul_elem_32_2() [3/8]

v32acc64 mul_elem_32_2 | ( | v32int32 | a0,
|  | v32int32 | a1,
|  | v64int16 | b )

Parameters

  a0 | Matrix A
  b | Matrix B

Returns
  Result of operation

## ◆ mul_elem_32_2() [4/8]

v32acc64 mul_elem_32_2 | ( | v32int32 | a0,
|  | v32int32 | a1,
|  | v64uint16 | b )

Parameters

  a0 | Matrix A
  b | Matrix B

Returns
  Result of operation

## ◆ mul_elem_32_2() [5/8]

v32acc64 mul_elem_32_2 | ( | v32uint32 | a0,
|  | v32uint32 | a1,
|  | int | sgn_x,
|  | v64int16 | b,
|  | int | sgn_y )

Parameters

  a0 | Matrix A
  sgn_x | Sign mask for matrix A
  b | Matrix B
  sgn_y | Sign mask for matrix B

Returns
  Result of operation

## ◆ mul_elem_32_2() [6/8]

v32acc64 mul_elem_32_2 | ( | v32uint32 | a0,
|  | v32uint32 | a1,
|  | int | sgn_x,
|  | v64uint16 | b,
|  | int | sgn_y )

Parameters

  a0 | Matrix A
  sgn_x | Sign mask for matrix A
  b | Matrix B
  sgn_y | Sign mask for matrix B

Returns
  Result of operation

## ◆ mul_elem_32_2() [7/8]

v32acc64 mul_elem_32_2 | ( | v32uint32 | a0,
|  | v32uint32 | a1,
|  | v64int16 | b )

Parameters

  a0 | Matrix A
  b | Matrix B

Returns
  Result of operation

## ◆ mul_elem_32_2() [8/8]

v32acc64 mul_elem_32_2 | ( | v32uint32 | a0,
|  | v32uint32 | a1,
|  | v64uint16 | b )

Parameters

  a0 | Matrix A
  b | Matrix B

Returns
  Result of operation

## ◆ mul_elem_32_2_conf() [1/8]

v32acc64 mul_elem_32_2_conf | ( | v32int32 | a0,
|  | v32int32 | a1,
|  | int | sgn_x,
|  | v64int16 | b,
|  | int | sgn_y,
|  | int | sub_mul )

Parameters

  a0 | Matrix A
  sgn_x | Sign mask for matrix A
  b | Matrix B
  sgn_y | Sign mask for matrix B
  sub_mul | Negation mask of multiplication result. If a bit is set the corresponding output accumulator lane is negated.

Returns
  Result of operation

## ◆ mul_elem_32_2_conf() [2/8]

v32acc64 mul_elem_32_2_conf | ( | v32int32 | a0,
|  | v32int32 | a1,
|  | int | sgn_x,
|  | v64uint16 | b,
|  | int | sgn_y,
|  | int | sub_mul )

Parameters

  a0 | Matrix A
  sgn_x | Sign mask for matrix A
  b | Matrix B
  sgn_y | Sign mask for matrix B
  sub_mul | Negation mask of multiplication result. If a bit is set the corresponding output accumulator lane is negated.

Returns
  Result of operation

## ◆ mul_elem_32_2_conf() [3/8]

v32acc64 mul_elem_32_2_conf | ( | v32int32 | a0,
|  | v32int32 | a1,
|  | v64int16 | b,
|  | int | sub_mul )

Parameters

  a0 | Matrix A
  b | Matrix B
  sub_mul | Negation mask for multiplication result

Returns
  Result of operation

## ◆ mul_elem_32_2_conf() [4/8]

v32acc64 mul_elem_32_2_conf | ( | v32int32 | a0,
|  | v32int32 | a1,
|  | v64uint16 | b,
|  | int | sub_mul )

Parameters

  a0 | Matrix A
  b | Matrix B
  sub_mul | Negation mask for multiplication result

Returns
  Result of operation

## ◆ mul_elem_32_2_conf() [5/8]

v32acc64 mul_elem_32_2_conf | ( | v32uint32 | a0,
|  | v32uint32 | a1,
|  | int | sgn_x,
|  | v64int16 | b,
|  | int | sgn_y,
|  | int | sub_mul )

Parameters

  a0 | Matrix A
  sgn_x | Sign mask for matrix A
  b | Matrix B
  sgn_y | Sign mask for matrix B
  sub_mul | Negation mask of multiplication result. If a bit is set the corresponding output accumulator lane is negated.

Returns
  Result of operation

## ◆ mul_elem_32_2_conf() [6/8]

v32acc64 mul_elem_32_2_conf | ( | v32uint32 | a0,
|  | v32uint32 | a1,
|  | int | sgn_x,
|  | v64uint16 | b,
|  | int | sgn_y,
|  | int | sub_mul )

Parameters

  a0 | Matrix A
  sgn_x | Sign mask for matrix A
  b | Matrix B
  sgn_y | Sign mask for matrix B
  sub_mul | Negation mask of multiplication result. If a bit is set the corresponding output accumulator lane is negated.

Returns
  Result of operation

## ◆ mul_elem_32_2_conf() [7/8]

v32acc64 mul_elem_32_2_conf | ( | v32uint32 | a0,
|  | v32uint32 | a1,
|  | v64int16 | b,
|  | int | sub_mul )

Parameters

  a0 | Matrix A
  b | Matrix B
  sub_mul | Negation mask for multiplication result

Returns
  Result of operation

## ◆ mul_elem_32_2_conf() [8/8]

v32acc64 mul_elem_32_2_conf | ( | v32uint32 | a0,
|  | v32uint32 | a1,
|  | v64uint16 | b,
|  | int | sub_mul )

Parameters

  a0 | Matrix A
  b | Matrix B
  sub_mul | Negation mask for multiplication result

Returns
  Result of operation

## ◆ mul_elem_32_conf() [1/8]

v32acc64 mul_elem_32_conf | ( | v16int32 | a0,
|  | v16int32 | a1,
|  | int | sgn_x,
|  | v32int16 | b,
|  | int | sgn_y,
|  | int | sub_mul )

Parameters

  a0 | Matrix A
  sgn_x | Sign mask for matrix A
  b | Matrix B
  sgn_y | Sign mask for matrix B
  sub_mul | Negation mask of multiplication result. If a bit is set the corresponding output accumulator lane is negated.

Returns
  Result of operation

## ◆ mul_elem_32_conf() [2/8]

v32acc64 mul_elem_32_conf | ( | v16int32 | a0,
|  | v16int32 | a1,
|  | int | sgn_x,
|  | v32uint16 | b,
|  | int | sgn_y,
|  | int | sub_mul )

Parameters

  a0 | Matrix A
  sgn_x | Sign mask for matrix A
  b | Matrix B
  sgn_y | Sign mask for matrix B
  sub_mul | Negation mask of multiplication result. If a bit is set the corresponding output accumulator lane is negated.

Returns
  Result of operation

## ◆ mul_elem_32_conf() [3/8]

v32acc64 mul_elem_32_conf | ( | v16int32 | a0,
|  | v16int32 | a1,
|  | v32int16 | b,
|  | int | sub_mul )

Parameters

  a0 | Matrix A
  b | Matrix B
  sub_mul | Negation mask for multiplication result

Returns
  Result of operation

## ◆ mul_elem_32_conf() [4/8]

v32acc64 mul_elem_32_conf | ( | v16int32 | a0,
|  | v16int32 | a1,
|  | v32uint16 | b,
|  | int | sub_mul )

Parameters

  a0 | Matrix A
  b | Matrix B
  sub_mul | Negation mask for multiplication result

Returns
  Result of operation

## ◆ mul_elem_32_conf() [5/8]

v32acc64 mul_elem_32_conf | ( | v16uint32 | a0,
|  | v16uint32 | a1,
|  | int | sgn_x,
|  | v32int16 | b,
|  | int | sgn_y,
|  | int | sub_mul )

Parameters

  a0 | Matrix A
  sgn_x | Sign mask for matrix A
  b | Matrix B
  sgn_y | Sign mask for matrix B
  sub_mul | Negation mask of multiplication result. If a bit is set the corresponding output accumulator lane is negated.

Returns
  Result of operation

## ◆ mul_elem_32_conf() [6/8]

v32acc64 mul_elem_32_conf | ( | v16uint32 | a0,
|  | v16uint32 | a1,
|  | int | sgn_x,
|  | v32uint16 | b,
|  | int | sgn_y,
|  | int | sub_mul )

Parameters

  a0 | Matrix A
  sgn_x | Sign mask for matrix A
  b | Matrix B
  sgn_y | Sign mask for matrix B
  sub_mul | Negation mask of multiplication result. If a bit is set the corresponding output accumulator lane is negated.

Returns
  Result of operation

## ◆ mul_elem_32_conf() [7/8]

v32acc64 mul_elem_32_conf | ( | v16uint32 | a0,
|  | v16uint32 | a1,
|  | v32int16 | b,
|  | int | sub_mul )

Parameters

  a0 | Matrix A
  b | Matrix B
  sub_mul | Negation mask for multiplication result

Returns
  Result of operation

## ◆ mul_elem_32_conf() [8/8]

v32acc64 mul_elem_32_conf | ( | v16uint32 | a0,
|  | v16uint32 | a1,
|  | v32uint16 | b,
|  | int | sub_mul )

Parameters

  a0 | Matrix A
  b | Matrix B
  sub_mul | Negation mask for multiplication result

Returns
  Result of operation

## ◆ negmul_4x4_4x8() [1/8]

v32acc64 negmul_4x4_4x8 | ( | v16int32 | a0,
|  | int | sgn_x,
|  | v32int16 | b,
|  | int | sgn_y )

Parameters

  a0 | Matrix A
  sgn_x | Sign mask for matrix A
  b | Matrix B
  sgn_y | Sign mask for matrix B

Returns
  Result of operation

## ◆ negmul_4x4_4x8() [2/8]

v32acc64 negmul_4x4_4x8 | ( | v16int32 | a0,
|  | int | sgn_x,
|  | v32uint16 | b,
|  | int | sgn_y )

Parameters

  a0 | Matrix A
  sgn_x | Sign mask for matrix A
  b | Matrix B
  sgn_y | Sign mask for matrix B

Returns
  Result of operation

## ◆ negmul_4x4_4x8() [3/8]

v32acc64 negmul_4x4_4x8 | ( | v16int32 | a0,
|  | v32int16 | b )

Parameters

  a0 | Matrix A
  b | Matrix B

Returns
  Result of operation

## ◆ negmul_4x4_4x8() [4/8]

v32acc64 negmul_4x4_4x8 | ( | v16int32 | a0,
|  | v32uint16 | b )

Parameters

  a0 | Matrix A
  b | Matrix B

Returns
  Result of operation

## ◆ negmul_4x4_4x8() [5/8]

v32acc64 negmul_4x4_4x8 | ( | v16uint32 | a0,
|  | int | sgn_x,
|  | v32int16 | b,
|  | int | sgn_y )

Parameters

  a0 | Matrix A
  sgn_x | Sign mask for matrix A
  b | Matrix B
  sgn_y | Sign mask for matrix B

Returns
  Result of operation

## ◆ negmul_4x4_4x8() [6/8]

v32acc64 negmul_4x4_4x8 | ( | v16uint32 | a0,
|  | int | sgn_x,
|  | v32uint16 | b,
|  | int | sgn_y )

Parameters

  a0 | Matrix A
  sgn_x | Sign mask for matrix A
  b | Matrix B
  sgn_y | Sign mask for matrix B

Returns
  Result of operation

## ◆ negmul_4x4_4x8() [7/8]

v32acc64 negmul_4x4_4x8 | ( | v16uint32 | a0,
|  | v32int16 | b )

Parameters

  a0 | Matrix A
  b | Matrix B

Returns
  Result of operation

## ◆ negmul_4x4_4x8() [8/8]

v32acc64 negmul_4x4_4x8 | ( | v16uint32 | a0,
|  | v32uint16 | b )

Parameters

  a0 | Matrix A
  b | Matrix B

Returns
  Result of operation

## ◆ negmul_4x4_4x8_conf() [1/8]

v32acc64 negmul_4x4_4x8_conf | ( | v16int32 | a0,
|  | int | sgn_x,
|  | v32int16 | b,
|  | int | sgn_y,
|  | int | sub_mul )

Parameters

  a0 | Matrix A
  sgn_x | Sign mask for matrix A
  b | Matrix B
  sgn_y | Sign mask for matrix B
  sub_mul | Negation mask of multiplication result

Returns
  Result of operation

## ◆ negmul_4x4_4x8_conf() [2/8]

v32acc64 negmul_4x4_4x8_conf | ( | v16int32 | a0,
|  | int | sgn_x,
|  | v32uint16 | b,
|  | int | sgn_y,
|  | int | sub_mul )

Parameters

  a0 | Matrix A
  sgn_x | Sign mask for matrix A
  b | Matrix B
  sgn_y | Sign mask for matrix B
  sub_mul | Negation mask of multiplication result

Returns
  Result of operation

## ◆ negmul_4x4_4x8_conf() [3/8]

v32acc64 negmul_4x4_4x8_conf | ( | v16int32 | a0,
|  | v32int16 | b,
|  | int | sub_mul )

Parameters

  a0 | Matrix A
  b | Matrix B
  sub_mul | Negation mask for multiplication result. If a bit of sub_mul is set the corresponding vector lane of the output accumulator will be negated.

Returns
  Result of operation

## ◆ negmul_4x4_4x8_conf() [4/8]

v32acc64 negmul_4x4_4x8_conf | ( | v16int32 | a0,
|  | v32uint16 | b,
|  | int | sub_mul )

Parameters

  a0 | Matrix A
  b | Matrix B
  sub_mul | Negation mask for multiplication result. If a bit of sub_mul is set the corresponding vector lane of the output accumulator will be negated.

Returns
  Result of operation

## ◆ negmul_4x4_4x8_conf() [5/8]

v32acc64 negmul_4x4_4x8_conf | ( | v16uint32 | a0,
|  | int | sgn_x,
|  | v32int16 | b,
|  | int | sgn_y,
|  | int | sub_mul )

Parameters

  a0 | Matrix A
  sgn_x | Sign mask for matrix A
  b | Matrix B
  sgn_y | Sign mask for matrix B
  sub_mul | Negation mask of multiplication result

Returns
  Result of operation

## ◆ negmul_4x4_4x8_conf() [6/8]

v32acc64 negmul_4x4_4x8_conf | ( | v16uint32 | a0,
|  | int | sgn_x,
|  | v32uint16 | b,
|  | int | sgn_y,
|  | int | sub_mul )

Parameters

  a0 | Matrix A
  sgn_x | Sign mask for matrix A
  b | Matrix B
  sgn_y | Sign mask for matrix B
  sub_mul | Negation mask of multiplication result

Returns
  Result of operation

## ◆ negmul_4x4_4x8_conf() [7/8]

v32acc64 negmul_4x4_4x8_conf | ( | v16uint32 | a0,
|  | v32int16 | b,
|  | int | sub_mul )

Parameters

  a0 | Matrix A
  b | Matrix B
  sub_mul | Negation mask for multiplication result. If a bit of sub_mul is set the corresponding vector lane of the output accumulator will be negated.

Returns
  Result of operation

## ◆ negmul_4x4_4x8_conf() [8/8]

v32acc64 negmul_4x4_4x8_conf | ( | v16uint32 | a0,
|  | v32uint16 | b,
|  | int | sub_mul )

Parameters

  a0 | Matrix A
  b | Matrix B
  sub_mul | Negation mask for multiplication result. If a bit of sub_mul is set the corresponding vector lane of the output accumulator will be negated.

Returns
  Result of operation

## ◆ negmul_8x2_2x8() [1/8]

v64acc32 negmul_8x2_2x8 | ( | v16int32 | a0,
|  | int | sgn_x,
|  | v32int16 | b,
|  | int | sgn_y )

Parameters

  a0 | Matrix A
  sgn_x | Sign mask for matrix A
  b | Matrix B
  sgn_y | Sign mask for matrix B

Returns
  Result of operation

## ◆ negmul_8x2_2x8() [2/8]

v64acc32 negmul_8x2_2x8 | ( | v16int32 | a0,
|  | int | sgn_x,
|  | v32uint16 | b,
|  | int | sgn_y )

Parameters

  a0 | Matrix A
  sgn_x | Sign mask for matrix A
  b | Matrix B
  sgn_y | Sign mask for matrix B

Returns
  Result of operation

## ◆ negmul_8x2_2x8() [3/8]

v64acc32 negmul_8x2_2x8 | ( | v16int32 | a0,
|  | v32int16 | b )

Parameters

  a0 | Matrix A
  b | Matrix B

Returns
  Result of operation

## ◆ negmul_8x2_2x8() [4/8]

v64acc32 negmul_8x2_2x8 | ( | v16int32 | a0,
|  | v32uint16 | b )

Parameters

  a0 | Matrix A
  b | Matrix B

Returns
  Result of operation

## ◆ negmul_8x2_2x8() [5/8]

v64acc32 negmul_8x2_2x8 | ( | v16uint32 | a0,
|  | int | sgn_x,
|  | v32int16 | b,
|  | int | sgn_y )

Parameters

  a0 | Matrix A
  sgn_x | Sign mask for matrix A
  b | Matrix B
  sgn_y | Sign mask for matrix B

Returns
  Result of operation

## ◆ negmul_8x2_2x8() [6/8]

v64acc32 negmul_8x2_2x8 | ( | v16uint32 | a0,
|  | int | sgn_x,
|  | v32uint16 | b,
|  | int | sgn_y )

Parameters

  a0 | Matrix A
  sgn_x | Sign mask for matrix A
  b | Matrix B
  sgn_y | Sign mask for matrix B

Returns
  Result of operation

## ◆ negmul_8x2_2x8() [7/8]

v64acc32 negmul_8x2_2x8 | ( | v16uint32 | a0,
|  | v32int16 | b )

Parameters

  a0 | Matrix A
  b | Matrix B

Returns
  Result of operation

## ◆ negmul_8x2_2x8() [8/8]

v64acc32 negmul_8x2_2x8 | ( | v16uint32 | a0,
|  | v32uint16 | b )

Parameters

  a0 | Matrix A
  b | Matrix B

Returns
  Result of operation

## ◆ negmul_8x2_2x8_conf() [1/8]

v64acc32 negmul_8x2_2x8_conf | ( | v16int32 | a0,
|  | int | sgn_x,
|  | v32int16 | b,
|  | int | sgn_y,
|  | int | sub_mul )

Parameters

  a0 | Matrix A
  sgn_x | Sign mask for matrix A
  b | Matrix B
  sgn_y | Sign mask for matrix B
  sub_mul | Negation mask of multiplication result

Returns
  Result of operation

## ◆ negmul_8x2_2x8_conf() [2/8]

v64acc32 negmul_8x2_2x8_conf | ( | v16int32 | a0,
|  | int | sgn_x,
|  | v32uint16 | b,
|  | int | sgn_y,
|  | int | sub_mul )

Parameters

  a0 | Matrix A
  sgn_x | Sign mask for matrix A
  b | Matrix B
  sgn_y | Sign mask for matrix B
  sub_mul | Negation mask of multiplication result

Returns
  Result of operation

## ◆ negmul_8x2_2x8_conf() [3/8]

v64acc32 negmul_8x2_2x8_conf | ( | v16int32 | a0,
|  | v32int16 | b,
|  | int | sub_mul )

Parameters

  a0 | Matrix A
  b | Matrix B
  sub_mul | Negation mask for multiplication result. If a bit of sub_mul is set the corresponding vector lane of the output accumulator will be negated.

Returns
  Result of operation

## ◆ negmul_8x2_2x8_conf() [4/8]

v64acc32 negmul_8x2_2x8_conf | ( | v16int32 | a0,
|  | v32uint16 | b,
|  | int | sub_mul )

Parameters

  a0 | Matrix A
  b | Matrix B
  sub_mul | Negation mask for multiplication result. If a bit of sub_mul is set the corresponding vector lane of the output accumulator will be negated.

Returns
  Result of operation

## ◆ negmul_8x2_2x8_conf() [5/8]

v64acc32 negmul_8x2_2x8_conf | ( | v16uint32 | a0,
|  | int | sgn_x,
|  | v32int16 | b,
|  | int | sgn_y,
|  | int | sub_mul )

Parameters

  a0 | Matrix A
  sgn_x | Sign mask for matrix A
  b | Matrix B
  sgn_y | Sign mask for matrix B
  sub_mul | Negation mask of multiplication result

Returns
  Result of operation

## ◆ negmul_8x2_2x8_conf() [6/8]

v64acc32 negmul_8x2_2x8_conf | ( | v16uint32 | a0,
|  | int | sgn_x,
|  | v32uint16 | b,
|  | int | sgn_y,
|  | int | sub_mul )

Parameters

  a0 | Matrix A
  sgn_x | Sign mask for matrix A
  b | Matrix B
  sgn_y | Sign mask for matrix B
  sub_mul | Negation mask of multiplication result

Returns
  Result of operation

## ◆ negmul_8x2_2x8_conf() [7/8]

v64acc32 negmul_8x2_2x8_conf | ( | v16uint32 | a0,
|  | v32int16 | b,
|  | int | sub_mul )

Parameters

  a0 | Matrix A
  b | Matrix B
  sub_mul | Negation mask for multiplication result. If a bit of sub_mul is set the corresponding vector lane of the output accumulator will be negated.

Returns
  Result of operation

## ◆ negmul_8x2_2x8_conf() [8/8]

v64acc32 negmul_8x2_2x8_conf | ( | v16uint32 | a0,
|  | v32uint16 | b,
|  | int | sub_mul )

Parameters

  a0 | Matrix A
  b | Matrix B
  sub_mul | Negation mask for multiplication result. If a bit of sub_mul is set the corresponding vector lane of the output accumulator will be negated.

Returns
  Result of operation

## ◆ negmul_conv_4x4_8ch() [1/8]

v32acc64 negmul_conv_4x4_8ch | ( | v32int32 | a0,
|  | v32int32 | a1,
|  | int | sgn_x,
|  | v32int16 | b,
|  | int | sgn_y )

Parameters

  a0 | Matrix A
  sgn_x | Sign mask for matrix A
  b | Matrix B
  sgn_y | Sign mask for matrix B

Returns
  Result of operation

## ◆ negmul_conv_4x4_8ch() [2/8]

v32acc64 negmul_conv_4x4_8ch | ( | v32int32 | a0,
|  | v32int32 | a1,
|  | int | sgn_x,
|  | v32uint16 | b,
|  | int | sgn_y )

Parameters

  a0 | Matrix A
  sgn_x | Sign mask for matrix A
  b | Matrix B
  sgn_y | Sign mask for matrix B

Returns
  Result of operation

## ◆ negmul_conv_4x4_8ch() [3/8]

v32acc64 negmul_conv_4x4_8ch | ( | v32int32 | a0,
|  | v32int32 | a1,
|  | v32int16 | b )

Parameters

  a0 | Matrix A
  b | Matrix B

Returns
  Result of operation

## ◆ negmul_conv_4x4_8ch() [4/8]

v32acc64 negmul_conv_4x4_8ch | ( | v32int32 | a0,
|  | v32int32 | a1,
|  | v32uint16 | b )

Parameters

  a0 | Matrix A
  b | Matrix B

Returns
  Result of operation

## ◆ negmul_conv_4x4_8ch() [5/8]

v32acc64 negmul_conv_4x4_8ch | ( | v32uint32 | a0,
|  | v32uint32 | a1,
|  | int | sgn_x,
|  | v32int16 | b,
|  | int | sgn_y )

Parameters

  a0 | Matrix A
  sgn_x | Sign mask for matrix A
  b | Matrix B
  sgn_y | Sign mask for matrix B

Returns
  Result of operation

## ◆ negmul_conv_4x4_8ch() [6/8]

v32acc64 negmul_conv_4x4_8ch | ( | v32uint32 | a0,
|  | v32uint32 | a1,
|  | int | sgn_x,
|  | v32uint16 | b,
|  | int | sgn_y )

Parameters

  a0 | Matrix A
  sgn_x | Sign mask for matrix A
  b | Matrix B
  sgn_y | Sign mask for matrix B

Returns
  Result of operation

## ◆ negmul_conv_4x4_8ch() [7/8]

v32acc64 negmul_conv_4x4_8ch | ( | v32uint32 | a0,
|  | v32uint32 | a1,
|  | v32int16 | b )

Parameters

  a0 | Matrix A
  b | Matrix B

Returns
  Result of operation

## ◆ negmul_conv_4x4_8ch() [8/8]

v32acc64 negmul_conv_4x4_8ch | ( | v32uint32 | a0,
|  | v32uint32 | a1,
|  | v32uint16 | b )

Parameters

  a0 | Matrix A
  b | Matrix B

Returns
  Result of operation

## ◆ negmul_conv_4x4_8ch_conf() [1/8]

v32acc64 negmul_conv_4x4_8ch_conf | ( | v32int32 | a0,
|  | v32int32 | a1,
|  | int | sgn_x,
|  | v32int16 | b,
|  | int | sgn_y,
|  | int | sub_mul )

Parameters

  a0 | Matrix A
  sgn_x | Sign mask for matrix A
  b | Matrix B
  sgn_y | Sign mask for matrix B
  sub_mul | Negation mask of multiplication result

Returns
  Result of operation

## ◆ negmul_conv_4x4_8ch_conf() [2/8]

v32acc64 negmul_conv_4x4_8ch_conf | ( | v32int32 | a0,
|  | v32int32 | a1,
|  | int | sgn_x,
|  | v32uint16 | b,
|  | int | sgn_y,
|  | int | sub_mul )

Parameters

  a0 | Matrix A
  sgn_x | Sign mask for matrix A
  b | Matrix B
  sgn_y | Sign mask for matrix B
  sub_mul | Negation mask of multiplication result

Returns
  Result of operation

## ◆ negmul_conv_4x4_8ch_conf() [3/8]

v32acc64 negmul_conv_4x4_8ch_conf | ( | v32int32 | a0,
|  | v32int32 | a1,
|  | v32int16 | b,
|  | int | sub_mul )

Parameters

  a0 | Matrix A
  b | Matrix B
  sub_mul | Negation mask for multiplication result. If a bit of sub_mul is set the corresponding vector lane of the output accumulator will be negated.

Returns
  Result of operation

## ◆ negmul_conv_4x4_8ch_conf() [4/8]

v32acc64 negmul_conv_4x4_8ch_conf | ( | v32int32 | a0,
|  | v32int32 | a1,
|  | v32uint16 | b,
|  | int | sub_mul )

Parameters

  a0 | Matrix A
  b | Matrix B
  sub_mul | Negation mask for multiplication result. If a bit of sub_mul is set the corresponding vector lane of the output accumulator will be negated.

Returns
  Result of operation

## ◆ negmul_conv_4x4_8ch_conf() [5/8]

v32acc64 negmul_conv_4x4_8ch_conf | ( | v32uint32 | a0,
|  | v32uint32 | a1,
|  | int | sgn_x,
|  | v32int16 | b,
|  | int | sgn_y,
|  | int | sub_mul )

Parameters

  a0 | Matrix A
  sgn_x | Sign mask for matrix A
  b | Matrix B
  sgn_y | Sign mask for matrix B
  sub_mul | Negation mask of multiplication result

Returns
  Result of operation

## ◆ negmul_conv_4x4_8ch_conf() [6/8]

v32acc64 negmul_conv_4x4_8ch_conf | ( | v32uint32 | a0,
|  | v32uint32 | a1,
|  | int | sgn_x,
|  | v32uint16 | b,
|  | int | sgn_y,
|  | int | sub_mul )

Parameters

  a0 | Matrix A
  sgn_x | Sign mask for matrix A
  b | Matrix B
  sgn_y | Sign mask for matrix B
  sub_mul | Negation mask of multiplication result

Returns
  Result of operation

## ◆ negmul_conv_4x4_8ch_conf() [7/8]

v32acc64 negmul_conv_4x4_8ch_conf | ( | v32uint32 | a0,
|  | v32uint32 | a1,
|  | v32int16 | b,
|  | int | sub_mul )

Parameters

  a0 | Matrix A
  b | Matrix B
  sub_mul | Negation mask for multiplication result. If a bit of sub_mul is set the corresponding vector lane of the output accumulator will be negated.

Returns
  Result of operation

## ◆ negmul_conv_4x4_8ch_conf() [8/8]

v32acc64 negmul_conv_4x4_8ch_conf | ( | v32uint32 | a0,
|  | v32uint32 | a1,
|  | v32uint16 | b,
|  | int | sub_mul )

Parameters

  a0 | Matrix A
  b | Matrix B
  sub_mul | Negation mask for multiplication result. If a bit of sub_mul is set the corresponding vector lane of the output accumulator will be negated.

Returns
  Result of operation

## ◆ negmul_elem_32() [1/8]

v32acc64 negmul_elem_32 | ( | v16int32 | a0,
|  | v16int32 | a1,
|  | int | sgn_x,
|  | v32int16 | b,
|  | int | sgn_y )

Parameters

  a0 | Matrix A
  sgn_x | Sign mask for matrix A
  b | Matrix B
  sgn_y | Sign mask for matrix B

Returns
  Result of operation

## ◆ negmul_elem_32() [2/8]

v32acc64 negmul_elem_32 | ( | v16int32 | a0,
|  | v16int32 | a1,
|  | int | sgn_x,
|  | v32uint16 | b,
|  | int | sgn_y )

Parameters

  a0 | Matrix A
  sgn_x | Sign mask for matrix A
  b | Matrix B
  sgn_y | Sign mask for matrix B

Returns
  Result of operation

## ◆ negmul_elem_32() [3/8]

v32acc64 negmul_elem_32 | ( | v16int32 | a0,
|  | v16int32 | a1,
|  | v32int16 | b )

Parameters

  a0 | Matrix A
  b | Matrix B

Returns
  Result of operation

## ◆ negmul_elem_32() [4/8]

v32acc64 negmul_elem_32 | ( | v16int32 | a0,
|  | v16int32 | a1,
|  | v32uint16 | b )

Parameters

  a0 | Matrix A
  b | Matrix B

Returns
  Result of operation

## ◆ negmul_elem_32() [5/8]

v32acc64 negmul_elem_32 | ( | v16uint32 | a0,
|  | v16uint32 | a1,
|  | int | sgn_x,
|  | v32int16 | b,
|  | int | sgn_y )

Parameters

  a0 | Matrix A
  sgn_x | Sign mask for matrix A
  b | Matrix B
  sgn_y | Sign mask for matrix B

Returns
  Result of operation

## ◆ negmul_elem_32() [6/8]

v32acc64 negmul_elem_32 | ( | v16uint32 | a0,
|  | v16uint32 | a1,
|  | int | sgn_x,
|  | v32uint16 | b,
|  | int | sgn_y )

Parameters

  a0 | Matrix A
  sgn_x | Sign mask for matrix A
  b | Matrix B
  sgn_y | Sign mask for matrix B

Returns
  Result of operation

## ◆ negmul_elem_32() [7/8]

v32acc64 negmul_elem_32 | ( | v16uint32 | a0,
|  | v16uint32 | a1,
|  | v32int16 | b )

Parameters

  a0 | Matrix A
  b | Matrix B

Returns
  Result of operation

## ◆ negmul_elem_32() [8/8]

v32acc64 negmul_elem_32 | ( | v16uint32 | a0,
|  | v16uint32 | a1,
|  | v32uint16 | b )

Parameters

  a0 | Matrix A
  b | Matrix B

Returns
  Result of operation

## ◆ negmul_elem_32_2() [1/8]

v32acc64 negmul_elem_32_2 | ( | v32int32 | a0,
|  | v32int32 | a1,
|  | int | sgn_x,
|  | v64int16 | b,
|  | int | sgn_y )

Parameters

  a0 | Matrix A
  sgn_x | Sign mask for matrix A
  b | Matrix B
  sgn_y | Sign mask for matrix B

Returns
  Result of operation

## ◆ negmul_elem_32_2() [2/8]

v32acc64 negmul_elem_32_2 | ( | v32int32 | a0,
|  | v32int32 | a1,
|  | int | sgn_x,
|  | v64uint16 | b,
|  | int | sgn_y )

Parameters

  a0 | Matrix A
  sgn_x | Sign mask for matrix A
  b | Matrix B
  sgn_y | Sign mask for matrix B

Returns
  Result of operation

## ◆ negmul_elem_32_2() [3/8]

v32acc64 negmul_elem_32_2 | ( | v32int32 | a0,
|  | v32int32 | a1,
|  | v64int16 | b )

Parameters

  a0 | Matrix A
  b | Matrix B

Returns
  Result of operation

## ◆ negmul_elem_32_2() [4/8]

v32acc64 negmul_elem_32_2 | ( | v32int32 | a0,
|  | v32int32 | a1,
|  | v64uint16 | b )

Parameters

  a0 | Matrix A
  b | Matrix B

Returns
  Result of operation

## ◆ negmul_elem_32_2() [5/8]

v32acc64 negmul_elem_32_2 | ( | v32uint32 | a0,
|  | v32uint32 | a1,
|  | int | sgn_x,
|  | v64int16 | b,
|  | int | sgn_y )

Parameters

  a0 | Matrix A
  sgn_x | Sign mask for matrix A
  b | Matrix B
  sgn_y | Sign mask for matrix B

Returns
  Result of operation

## ◆ negmul_elem_32_2() [6/8]

v32acc64 negmul_elem_32_2 | ( | v32uint32 | a0,
|  | v32uint32 | a1,
|  | int | sgn_x,
|  | v64uint16 | b,
|  | int | sgn_y )

Parameters

  a0 | Matrix A
  sgn_x | Sign mask for matrix A
  b | Matrix B
  sgn_y | Sign mask for matrix B

Returns
  Result of operation

## ◆ negmul_elem_32_2() [7/8]

v32acc64 negmul_elem_32_2 | ( | v32uint32 | a0,
|  | v32uint32 | a1,
|  | v64int16 | b )

Parameters

  a0 | Matrix A
  b | Matrix B

Returns
  Result of operation

## ◆ negmul_elem_32_2() [8/8]

v32acc64 negmul_elem_32_2 | ( | v32uint32 | a0,
|  | v32uint32 | a1,
|  | v64uint16 | b )

Parameters

  a0 | Matrix A
  b | Matrix B

Returns
  Result of operation

## ◆ negmul_elem_32_2_conf() [1/8]

v32acc64 negmul_elem_32_2_conf | ( | v32int32 | a0,
|  | v32int32 | a1,
|  | int | sgn_x,
|  | v64int16 | b,
|  | int | sgn_y,
|  | int | sub_mul )

Parameters

  a0 | Matrix A
  sgn_x | Sign mask for matrix A
  b | Matrix B
  sgn_y | Sign mask for matrix B
  sub_mul | Negation mask of multiplication result

Returns
  Result of operation

## ◆ negmul_elem_32_2_conf() [2/8]

v32acc64 negmul_elem_32_2_conf | ( | v32int32 | a0,
|  | v32int32 | a1,
|  | int | sgn_x,
|  | v64uint16 | b,
|  | int | sgn_y,
|  | int | sub_mul )

Parameters

  a0 | Matrix A
  sgn_x | Sign mask for matrix A
  b | Matrix B
  sgn_y | Sign mask for matrix B
  sub_mul | Negation mask of multiplication result

Returns
  Result of operation

## ◆ negmul_elem_32_2_conf() [3/8]

v32acc64 negmul_elem_32_2_conf | ( | v32int32 | a0,
|  | v32int32 | a1,
|  | v64int16 | b,
|  | int | sub_mul )

Parameters

  a0 | Matrix A
  b | Matrix B
  sub_mul | Negation mask for multiplication result. If a bit of sub_mul is set the corresponding vector lane of the output accumulator will be negated.

Returns
  Result of operation

## ◆ negmul_elem_32_2_conf() [4/8]

v32acc64 negmul_elem_32_2_conf | ( | v32int32 | a0,
|  | v32int32 | a1,
|  | v64uint16 | b,
|  | int | sub_mul )

Parameters

  a0 | Matrix A
  b | Matrix B
  sub_mul | Negation mask for multiplication result. If a bit of sub_mul is set the corresponding vector lane of the output accumulator will be negated.

Returns
  Result of operation

## ◆ negmul_elem_32_2_conf() [5/8]

v32acc64 negmul_elem_32_2_conf | ( | v32uint32 | a0,
|  | v32uint32 | a1,
|  | int | sgn_x,
|  | v64int16 | b,
|  | int | sgn_y,
|  | int | sub_mul )

Parameters

  a0 | Matrix A
  sgn_x | Sign mask for matrix A
  b | Matrix B
  sgn_y | Sign mask for matrix B
  sub_mul | Negation mask of multiplication result

Returns
  Result of operation

## ◆ negmul_elem_32_2_conf() [6/8]

v32acc64 negmul_elem_32_2_conf | ( | v32uint32 | a0,
|  | v32uint32 | a1,
|  | int | sgn_x,
|  | v64uint16 | b,
|  | int | sgn_y,
|  | int | sub_mul )

Parameters

  a0 | Matrix A
  sgn_x | Sign mask for matrix A
  b | Matrix B
  sgn_y | Sign mask for matrix B
  sub_mul | Negation mask of multiplication result

Returns
  Result of operation

## ◆ negmul_elem_32_2_conf() [7/8]

v32acc64 negmul_elem_32_2_conf | ( | v32uint32 | a0,
|  | v32uint32 | a1,
|  | v64int16 | b,
|  | int | sub_mul )

Parameters

  a0 | Matrix A
  b | Matrix B
  sub_mul | Negation mask for multiplication result. If a bit of sub_mul is set the corresponding vector lane of the output accumulator will be negated.

Returns
  Result of operation

## ◆ negmul_elem_32_2_conf() [8/8]

v32acc64 negmul_elem_32_2_conf | ( | v32uint32 | a0,
|  | v32uint32 | a1,
|  | v64uint16 | b,
|  | int | sub_mul )

Parameters

  a0 | Matrix A
  b | Matrix B
  sub_mul | Negation mask for multiplication result. If a bit of sub_mul is set the corresponding vector lane of the output accumulator will be negated.

Returns
  Result of operation

## ◆ negmul_elem_32_conf() [1/8]

v32acc64 negmul_elem_32_conf | ( | v16int32 | a0,
|  | v16int32 | a1,
|  | int | sgn_x,
|  | v32int16 | b,
|  | int | sgn_y,
|  | int | sub_mul )

Parameters

  a0 | Matrix A
  sgn_x | Sign mask for matrix A
  b | Matrix B
  sgn_y | Sign mask for matrix B
  sub_mul | Negation mask of multiplication result

Returns
  Result of operation

## ◆ negmul_elem_32_conf() [2/8]

v32acc64 negmul_elem_32_conf | ( | v16int32 | a0,
|  | v16int32 | a1,
|  | int | sgn_x,
|  | v32uint16 | b,
|  | int | sgn_y,
|  | int | sub_mul )

Parameters

  a0 | Matrix A
  sgn_x | Sign mask for matrix A
  b | Matrix B
  sgn_y | Sign mask for matrix B
  sub_mul | Negation mask of multiplication result

Returns
  Result of operation

## ◆ negmul_elem_32_conf() [3/8]

v32acc64 negmul_elem_32_conf | ( | v16int32 | a0,
|  | v16int32 | a1,
|  | v32int16 | b,
|  | int | sub_mul )

Parameters

  a0 | Matrix A
  b | Matrix B
  sub_mul | Negation mask for multiplication result. If a bit of sub_mul is set the corresponding vector lane of the output accumulator will be negated.

Returns
  Result of operation

## ◆ negmul_elem_32_conf() [4/8]

v32acc64 negmul_elem_32_conf | ( | v16int32 | a0,
|  | v16int32 | a1,
|  | v32uint16 | b,
|  | int | sub_mul )

Parameters

  a0 | Matrix A
  b | Matrix B
  sub_mul | Negation mask for multiplication result. If a bit of sub_mul is set the corresponding vector lane of the output accumulator will be negated.

Returns
  Result of operation

## ◆ negmul_elem_32_conf() [5/8]

v32acc64 negmul_elem_32_conf | ( | v16uint32 | a0,
|  | v16uint32 | a1,
|  | int | sgn_x,
|  | v32int16 | b,
|  | int | sgn_y,
|  | int | sub_mul )

Parameters

  a0 | Matrix A
  sgn_x | Sign mask for matrix A
  b | Matrix B
  sgn_y | Sign mask for matrix B
  sub_mul | Negation mask of multiplication result

Returns
  Result of operation

## ◆ negmul_elem_32_conf() [6/8]

v32acc64 negmul_elem_32_conf | ( | v16uint32 | a0,
|  | v16uint32 | a1,
|  | int | sgn_x,
|  | v32uint16 | b,
|  | int | sgn_y,
|  | int | sub_mul )

Parameters

  a0 | Matrix A
  sgn_x | Sign mask for matrix A
  b | Matrix B
  sgn_y | Sign mask for matrix B
  sub_mul | Negation mask of multiplication result

Returns
  Result of operation

## ◆ negmul_elem_32_conf() [7/8]

v32acc64 negmul_elem_32_conf | ( | v16uint32 | a0,
|  | v16uint32 | a1,
|  | v32int16 | b,
|  | int | sub_mul )

Parameters

  a0 | Matrix A
  b | Matrix B
  sub_mul | Negation mask for multiplication result. If a bit of sub_mul is set the corresponding vector lane of the output accumulator will be negated.

Returns
  Result of operation

## ◆ negmul_elem_32_conf() [8/8]

v32acc64 negmul_elem_32_conf | ( | v16uint32 | a0,
|  | v16uint32 | a1,
|  | v32uint16 | b,
|  | int | sub_mul )

Parameters

  a0 | Matrix A
  b | Matrix B
  sub_mul | Negation mask for multiplication result. If a bit of sub_mul is set the corresponding vector lane of the output accumulator will be negated.

Returns
  Result of operation