| AI Engine Intrinsics User Guide (v2026.1)

Loading...
Searching...
No Matches
Functions
No conjugation
Intrinsics » Vector Operations » MAC intrinsics » Multiplication » Advanced » Integer » Vector MAC combined with vector comparisons » 16 bit x 16 bit » 16 bit Real x 16 bit Complex

## Overview

16 bit real by 16 bit complex using no conjugation

## Functions
v4cacc48 | mac4_abs (v4cacc48 acc, v32int16 xbuff, int xstart, unsigned int xoffsets, int xstep, v8cint16 zbuff, int zstart, unsigned int zoffsets, int zstep)
| Complex multiply-accumulate intrinsic function after computing the absolute value in the selected lanes from the input buffer using small X input buffer.
v4cacc48 | mac4_abs (v4cacc48 acc, v64int16 xbuff, int xstart, unsigned int xoffsets, int xstep, v8cint16 zbuff, int zstart, unsigned int zoffsets, int zstep)
| Complex multiply-accumulate intrinsic function after computing the absolute value in the selected lanes from the input buffer .
v4cacc48 | mac4_max (v4cacc48 acc, v32int16 xbuff, int xstart, unsigned int xoffsets, int xstep, int ystart, v8cint16 zbuff, int zstart, unsigned int zoffsets, int zstep)
| Complex multiply-accumulate intrinsic function after computing the maximum between the selected lanes from the input buffer using small X input buffer.
v4cacc48 | mac4_max (v4cacc48 acc, v32int16 xbuff, int xstart, unsigned int xoffsets, int xstep, v32int16 ybuff, int ystart, v8cint16 zbuff, int zstart, unsigned int zoffsets, int zstep)
| Complex multiply-accumulate intrinsic function after computing the maximum between the selected lanes from the input buffer using small X input buffer.
v4cacc48 | mac4_max (v4cacc48 acc, v64int16 xbuff, int xstart, unsigned int xoffsets, int xstep, int ystart, v8cint16 zbuff, int zstart, unsigned int zoffsets, int zstep)
| Complex multiply-accumulate intrinsic function after computing the maximum between the selected lanes from the input buffer .
v4cacc48 | mac4_maxdiff (v4cacc48 acc, v32int16 xbuff, int xstart, unsigned int xoffsets, int xstep, int ystart, v8cint16 zbuff, int zstart, unsigned int zoffsets, int zstep)
| Complex multiply-accumulate intrinsic function after computing the maximum difference between the selected lanes from the input buffer using small X input buffer.
v4cacc48 | mac4_maxdiff (v4cacc48 acc, v32int16 xbuff, int xstart, unsigned int xoffsets, int xstep, v32int16 ybuff, int ystart, v8cint16 zbuff, int zstart, unsigned int zoffsets, int zstep)
| Complex multiply-accumulate intrinsic function after computing the maximum difference between the selected lanes from the input buffer using small X input buffer.
v4cacc48 | mac4_maxdiff (v4cacc48 acc, v64int16 xbuff, int xstart, unsigned int xoffsets, int xstep, int ystart, v8cint16 zbuff, int zstart, unsigned int zoffsets, int zstep)
| Complex multiply-accumulate intrinsic function after computing the maximum difference between the selected lanes from the input buffer .
v4cacc48 | mac4_min (v4cacc48 acc, v32int16 xbuff, int xstart, unsigned int xoffsets, int xstep, int ystart, v8cint16 zbuff, int zstart, unsigned int zoffsets, int zstep)
| Complex multiply-accumulate intrinsic function after computing the minimum between the selected lanes from the input buffer using small X input buffer.
v4cacc48 | mac4_min (v4cacc48 acc, v32int16 xbuff, int xstart, unsigned int xoffsets, int xstep, v32int16 ybuff, int ystart, v8cint16 zbuff, int zstart, unsigned int zoffsets, int zstep)
| Complex multiply-accumulate intrinsic function after computing the minimum between the selected lanes from the input buffer using small X input buffer.
v4cacc48 | mac4_min (v4cacc48 acc, v64int16 xbuff, int xstart, unsigned int xoffsets, int xstep, int ystart, v8cint16 zbuff, int zstart, unsigned int zoffsets, int zstep)
| Complex multiply-accumulate intrinsic function after computing the minimum between the selected lanes from the input buffer .
v8cacc48 | mac8_abs (v8cacc48 acc, v32int16 xbuff, int xstart, unsigned int xoffsets, int xstep, v8cint16 zbuff, int zstart, unsigned int zoffsets, int zstep)
| Complex multiply-accumulate intrinsic function after computing the absolute value in the selected lanes from the input buffer using small X input buffer.
v8cacc48 | mac8_abs (v8cacc48 acc, v64int16 xbuff, int xstart, unsigned int xoffsets, int xstep, v8cint16 zbuff, int zstart, unsigned int zoffsets, int zstep)
| Complex multiply-accumulate intrinsic function after computing the absolute value in the selected lanes from the input buffer .
v8cacc48 | mac8_max (v8cacc48 acc, v32int16 xbuff, int xstart, unsigned int xoffsets, int xstep, int ystart, v8cint16 zbuff, int zstart, unsigned int zoffsets, int zstep)
| Complex multiply-accumulate intrinsic function after computing the maximum between the selected lanes from the input buffer using small X input buffer.
v8cacc48 | mac8_max (v8cacc48 acc, v32int16 xbuff, int xstart, unsigned int xoffsets, int xstep, v32int16 ybuff, int ystart, v8cint16 zbuff, int zstart, unsigned int zoffsets, int zstep)
| Complex multiply-accumulate intrinsic function after computing the maximum between the selected lanes from the input buffer using small X input buffer.
v8cacc48 | mac8_max (v8cacc48 acc, v64int16 xbuff, int xstart, unsigned int xoffsets, int xstep, int ystart, v8cint16 zbuff, int zstart, unsigned int zoffsets, int zstep)
| Complex multiply-accumulate intrinsic function after computing the maximum between the selected lanes from the input buffer .
v8cacc48 | mac8_maxdiff (v8cacc48 acc, v32int16 xbuff, int xstart, unsigned int xoffsets, int xstep, int ystart, v8cint16 zbuff, int zstart, unsigned int zoffsets, int zstep)
| Complex multiply-accumulate intrinsic function after computing the maximum difference between the selected lanes from the input buffer using small X input buffer.
v8cacc48 | mac8_maxdiff (v8cacc48 acc, v32int16 xbuff, int xstart, unsigned int xoffsets, int xstep, v32int16 ybuff, int ystart, v8cint16 zbuff, int zstart, unsigned int zoffsets, int zstep)
| Complex multiply-accumulate intrinsic function after computing the maximum difference between the selected lanes from the input buffer using small X input buffer.
v8cacc48 | mac8_maxdiff (v8cacc48 acc, v64int16 xbuff, int xstart, unsigned int xoffsets, int xstep, int ystart, v8cint16 zbuff, int zstart, unsigned int zoffsets, int zstep)
| Complex multiply-accumulate intrinsic function after computing the maximum difference between the selected lanes from the input buffer .
v8cacc48 | mac8_min (v8cacc48 acc, v32int16 xbuff, int xstart, unsigned int xoffsets, int xstep, int ystart, v8cint16 zbuff, int zstart, unsigned int zoffsets, int zstep)
| Complex multiply-accumulate intrinsic function after computing the minimum between the selected lanes from the input buffer using small X input buffer.
v8cacc48 | mac8_min (v8cacc48 acc, v32int16 xbuff, int xstart, unsigned int xoffsets, int xstep, v32int16 ybuff, int ystart, v8cint16 zbuff, int zstart, unsigned int zoffsets, int zstep)
| Complex multiply-accumulate intrinsic function after computing the minimum between the selected lanes from the input buffer using small X input buffer.
v8cacc48 | mac8_min (v8cacc48 acc, v64int16 xbuff, int xstart, unsigned int xoffsets, int xstep, int ystart, v8cint16 zbuff, int zstart, unsigned int zoffsets, int zstep)
| Complex multiply-accumulate intrinsic function after computing the minimum between the selected lanes from the input buffer .
v4cacc48 | msc4_abs (v4cacc48 acc, v32int16 xbuff, int xstart, unsigned int xoffsets, int xstep, v8cint16 zbuff, int zstart, unsigned int zoffsets, int zstep)
| Complex multiply-subtract intrinsic function after computing the absolute value in the selected lanes from the input buffer using small X input buffer.
v4cacc48 | msc4_abs (v4cacc48 acc, v64int16 xbuff, int xstart, unsigned int xoffsets, int xstep, v8cint16 zbuff, int zstart, unsigned int zoffsets, int zstep)
| Complex multiply-subtract intrinsic function after computing the absolute value in the selected lanes from the input buffer .
v4cacc48 | msc4_max (v4cacc48 acc, v32int16 xbuff, int xstart, unsigned int xoffsets, int xstep, int ystart, v8cint16 zbuff, int zstart, unsigned int zoffsets, int zstep)
| Complex multiply-subtract intrinsic function after computing the maximum between the selected lanes from the input buffer using small X input buffer.
v4cacc48 | msc4_max (v4cacc48 acc, v32int16 xbuff, int xstart, unsigned int xoffsets, int xstep, v32int16 ybuff, int ystart, v8cint16 zbuff, int zstart, unsigned int zoffsets, int zstep)
| Complex multiply-subtract intrinsic function after computing the maximum between the selected lanes from the input buffer using small X input buffer.
v4cacc48 | msc4_max (v4cacc48 acc, v64int16 xbuff, int xstart, unsigned int xoffsets, int xstep, int ystart, v8cint16 zbuff, int zstart, unsigned int zoffsets, int zstep)
| Complex multiply-subtract intrinsic function after computing the maximum between the selected lanes from the input buffer .
v4cacc48 | msc4_maxdiff (v4cacc48 acc, v32int16 xbuff, int xstart, unsigned int xoffsets, int xstep, int ystart, v8cint16 zbuff, int zstart, unsigned int zoffsets, int zstep)
| Complex multiply-subtract intrinsic function after computing the maximum difference between the selected lanes from the input buffer using small X input buffer.
v4cacc48 | msc4_maxdiff (v4cacc48 acc, v32int16 xbuff, int xstart, unsigned int xoffsets, int xstep, v32int16 ybuff, int ystart, v8cint16 zbuff, int zstart, unsigned int zoffsets, int zstep)
| Complex multiply-subtract intrinsic function after computing the maximum difference between the selected lanes from the input buffer using small X input buffer.
v4cacc48 | msc4_maxdiff (v4cacc48 acc, v64int16 xbuff, int xstart, unsigned int xoffsets, int xstep, int ystart, v8cint16 zbuff, int zstart, unsigned int zoffsets, int zstep)
| Complex multiply-subtract intrinsic function after computing the maximum difference between the selected lanes from the input buffer .
v4cacc48 | msc4_min (v4cacc48 acc, v32int16 xbuff, int xstart, unsigned int xoffsets, int xstep, int ystart, v8cint16 zbuff, int zstart, unsigned int zoffsets, int zstep)
| Complex multiply-subtract intrinsic function after computing the minimum between the selected lanes from the input buffer using small X input buffer.
v4cacc48 | msc4_min (v4cacc48 acc, v32int16 xbuff, int xstart, unsigned int xoffsets, int xstep, v32int16 ybuff, int ystart, v8cint16 zbuff, int zstart, unsigned int zoffsets, int zstep)
| Complex multiply-subtract intrinsic function after computing the minimum between the selected lanes from the input buffer using small X input buffer.
v4cacc48 | msc4_min (v4cacc48 acc, v64int16 xbuff, int xstart, unsigned int xoffsets, int xstep, int ystart, v8cint16 zbuff, int zstart, unsigned int zoffsets, int zstep)
| Complex multiply-subtract intrinsic function after computing the minimum between the selected lanes from the input buffer .
v8cacc48 | msc8_abs (v8cacc48 acc, v32int16 xbuff, int xstart, unsigned int xoffsets, int xstep, v8cint16 zbuff, int zstart, unsigned int zoffsets, int zstep)
| Complex multiply-subtract intrinsic function after computing the absolute value in the selected lanes from the input buffer using small X input buffer.
v8cacc48 | msc8_abs (v8cacc48 acc, v64int16 xbuff, int xstart, unsigned int xoffsets, int xstep, v8cint16 zbuff, int zstart, unsigned int zoffsets, int zstep)
| Complex multiply-subtract intrinsic function after computing the absolute value in the selected lanes from the input buffer .
v8cacc48 | msc8_max (v8cacc48 acc, v32int16 xbuff, int xstart, unsigned int xoffsets, int xstep, int ystart, v8cint16 zbuff, int zstart, unsigned int zoffsets, int zstep)
| Complex multiply-subtract intrinsic function after computing the maximum between the selected lanes from the input buffer using small X input buffer.
v8cacc48 | msc8_max (v8cacc48 acc, v32int16 xbuff, int xstart, unsigned int xoffsets, int xstep, v32int16 ybuff, int ystart, v8cint16 zbuff, int zstart, unsigned int zoffsets, int zstep)
| Complex multiply-subtract intrinsic function after computing the maximum between the selected lanes from the input buffer using small X input buffer.
v8cacc48 | msc8_max (v8cacc48 acc, v64int16 xbuff, int xstart, unsigned int xoffsets, int xstep, int ystart, v8cint16 zbuff, int zstart, unsigned int zoffsets, int zstep)
| Complex multiply-subtract intrinsic function after computing the maximum between the selected lanes from the input buffer .
v8cacc48 | msc8_maxdiff (v8cacc48 acc, v32int16 xbuff, int xstart, unsigned int xoffsets, int xstep, int ystart, v8cint16 zbuff, int zstart, unsigned int zoffsets, int zstep)
| Complex multiply-subtract intrinsic function after computing the maximum difference between the selected lanes from the input buffer using small X input buffer.
v8cacc48 | msc8_maxdiff (v8cacc48 acc, v32int16 xbuff, int xstart, unsigned int xoffsets, int xstep, v32int16 ybuff, int ystart, v8cint16 zbuff, int zstart, unsigned int zoffsets, int zstep)
| Complex multiply-subtract intrinsic function after computing the maximum difference between the selected lanes from the input buffer using small X input buffer.
v8cacc48 | msc8_maxdiff (v8cacc48 acc, v64int16 xbuff, int xstart, unsigned int xoffsets, int xstep, int ystart, v8cint16 zbuff, int zstart, unsigned int zoffsets, int zstep)
| Complex multiply-subtract intrinsic function after computing the maximum difference between the selected lanes from the input buffer .
v8cacc48 | msc8_min (v8cacc48 acc, v32int16 xbuff, int xstart, unsigned int xoffsets, int xstep, int ystart, v8cint16 zbuff, int zstart, unsigned int zoffsets, int zstep)
| Complex multiply-subtract intrinsic function after computing the minimum between the selected lanes from the input buffer using small X input buffer.
v8cacc48 | msc8_min (v8cacc48 acc, v32int16 xbuff, int xstart, unsigned int xoffsets, int xstep, v32int16 ybuff, int ystart, v8cint16 zbuff, int zstart, unsigned int zoffsets, int zstep)
| Complex multiply-subtract intrinsic function after computing the minimum between the selected lanes from the input buffer using small X input buffer.
v8cacc48 | msc8_min (v8cacc48 acc, v64int16 xbuff, int xstart, unsigned int xoffsets, int xstep, int ystart, v8cint16 zbuff, int zstart, unsigned int zoffsets, int zstep)
| Complex multiply-subtract intrinsic function after computing the minimum between the selected lanes from the input buffer .
v4cacc48 | mul4_abs (v32int16 xbuff, int xstart, unsigned int xoffsets, int xstep, v8cint16 zbuff, int zstart, unsigned int zoffsets, int zstep)
| Complex multiply intrinsic function after computing the absolute value in the selected lanes from the input buffer using small X input buffer.
v4cacc48 | mul4_abs (v64int16 xbuff, int xstart, unsigned int xoffsets, int xstep, v8cint16 zbuff, int zstart, unsigned int zoffsets, int zstep)
| Complex multiply intrinsic function after computing the absolute value in the selected lanes from the input buffer .
v4cacc48 | mul4_max (v32int16 xbuff, int xstart, unsigned int xoffsets, int xstep, int ystart, v8cint16 zbuff, int zstart, unsigned int zoffsets, int zstep)
| Complex multiply intrinsic function after computing the maximum between the selected lanes from the input buffer using small X input buffer.
v4cacc48 | mul4_max (v32int16 xbuff, int xstart, unsigned int xoffsets, int xstep, v32int16 ybuff, int ystart, v8cint16 zbuff, int zstart, unsigned int zoffsets, int zstep)
| Complex multiply intrinsic function after computing the maximum between the selected lanes from the input buffer using small X input buffer.
v4cacc48 | mul4_max (v64int16 xbuff, int xstart, unsigned int xoffsets, int xstep, int ystart, v8cint16 zbuff, int zstart, unsigned int zoffsets, int zstep)
| Complex multiply intrinsic function after computing the maximum between the selected lanes from the input buffer .
v4cacc48 | mul4_maxdiff (v32int16 xbuff, int xstart, unsigned int xoffsets, int xstep, int ystart, v8cint16 zbuff, int zstart, unsigned int zoffsets, int zstep)
| Complex multiply intrinsic function after computing the maximum difference between the selected lanes from the input buffer using small X input buffer.
v4cacc48 | mul4_maxdiff (v32int16 xbuff, int xstart, unsigned int xoffsets, int xstep, v32int16 ybuff, int ystart, v8cint16 zbuff, int zstart, unsigned int zoffsets, int zstep)
| Complex multiply intrinsic function after computing the maximum difference between the selected lanes from the input buffer using small X input buffer.
v4cacc48 | mul4_maxdiff (v64int16 xbuff, int xstart, unsigned int xoffsets, int xstep, int ystart, v8cint16 zbuff, int zstart, unsigned int zoffsets, int zstep)
| Complex multiply intrinsic function after computing the maximum difference between the selected lanes from the input buffer .
v4cacc48 | mul4_min (v32int16 xbuff, int xstart, unsigned int xoffsets, int xstep, int ystart, v8cint16 zbuff, int zstart, unsigned int zoffsets, int zstep)
| Complex multiply intrinsic function after computing the minimum between the selected lanes from the input buffer using small X input buffer.
v4cacc48 | mul4_min (v32int16 xbuff, int xstart, unsigned int xoffsets, int xstep, v32int16 ybuff, int ystart, v8cint16 zbuff, int zstart, unsigned int zoffsets, int zstep)
| Complex multiply intrinsic function after computing the minimum between the selected lanes from the input buffer using small X input buffer.
v4cacc48 | mul4_min (v64int16 xbuff, int xstart, unsigned int xoffsets, int xstep, int ystart, v8cint16 zbuff, int zstart, unsigned int zoffsets, int zstep)
| Complex multiply intrinsic function after computing the minimum between the selected lanes from the input buffer .
v8cacc48 | mul8_abs (v32int16 xbuff, int xstart, unsigned int xoffsets, int xstep, v8cint16 zbuff, int zstart, unsigned int zoffsets, int zstep)
| Complex multiply intrinsic function after computing the absolute value in the selected lanes from the input buffer using small X input buffer.
v8cacc48 | mul8_abs (v64int16 xbuff, int xstart, unsigned int xoffsets, int xstep, v8cint16 zbuff, int zstart, unsigned int zoffsets, int zstep)
| Complex multiply intrinsic function after computing the absolute value in the selected lanes from the input buffer .
v8cacc48 | mul8_max (v32int16 xbuff, int xstart, unsigned int xoffsets, int xstep, int ystart, v8cint16 zbuff, int zstart, unsigned int zoffsets, int zstep)
| Complex multiply intrinsic function after computing the maximum between the selected lanes from the input buffer using small X input buffer.
v8cacc48 | mul8_max (v32int16 xbuff, int xstart, unsigned int xoffsets, int xstep, v32int16 ybuff, int ystart, v8cint16 zbuff, int zstart, unsigned int zoffsets, int zstep)
| Complex multiply intrinsic function after computing the maximum between the selected lanes from the input buffer using small X input buffer.
v8cacc48 | mul8_max (v64int16 xbuff, int xstart, unsigned int xoffsets, int xstep, int ystart, v8cint16 zbuff, int zstart, unsigned int zoffsets, int zstep)
| Complex multiply intrinsic function after computing the maximum between the selected lanes from the input buffer .
v8cacc48 | mul8_maxdiff (v32int16 xbuff, int xstart, unsigned int xoffsets, int xstep, int ystart, v8cint16 zbuff, int zstart, unsigned int zoffsets, int zstep)
| Complex multiply intrinsic function after computing the maximum difference between the selected lanes from the input buffer using small X input buffer.
v8cacc48 | mul8_maxdiff (v32int16 xbuff, int xstart, unsigned int xoffsets, int xstep, v32int16 ybuff, int ystart, v8cint16 zbuff, int zstart, unsigned int zoffsets, int zstep)
| Complex multiply intrinsic function after computing the maximum difference between the selected lanes from the input buffer using small X input buffer.
v8cacc48 | mul8_maxdiff (v64int16 xbuff, int xstart, unsigned int xoffsets, int xstep, int ystart, v8cint16 zbuff, int zstart, unsigned int zoffsets, int zstep)
| Complex multiply intrinsic function after computing the maximum difference between the selected lanes from the input buffer .
v8cacc48 | mul8_min (v32int16 xbuff, int xstart, unsigned int xoffsets, int xstep, int ystart, v8cint16 zbuff, int zstart, unsigned int zoffsets, int zstep)
| Complex multiply intrinsic function after computing the minimum between the selected lanes from the input buffer using small X input buffer.
v8cacc48 | mul8_min (v32int16 xbuff, int xstart, unsigned int xoffsets, int xstep, v32int16 ybuff, int ystart, v8cint16 zbuff, int zstart, unsigned int zoffsets, int zstep)
| Complex multiply intrinsic function after computing the minimum between the selected lanes from the input buffer using small X input buffer.
v8cacc48 | mul8_min (v64int16 xbuff, int xstart, unsigned int xoffsets, int xstep, int ystart, v8cint16 zbuff, int zstart, unsigned int zoffsets, int zstep)
| Complex multiply intrinsic function after computing the minimum between the selected lanes from the input buffer .
v4cacc48 | negmul4_abs (v32int16 xbuff, int xstart, unsigned int xoffsets, int xstep, v8cint16 zbuff, int zstart, unsigned int zoffsets, int zstep)
| Complex multiply-negate intrinsic function after computing the absolute value in the selected lanes from the input buffer using small X input buffer.
v4cacc48 | negmul4_abs (v64int16 xbuff, int xstart, unsigned int xoffsets, int xstep, v8cint16 zbuff, int zstart, unsigned int zoffsets, int zstep)
| Complex multiply-negate intrinsic function after computing the absolute value in the selected lanes from the input buffer .
v4cacc48 | negmul4_max (v32int16 xbuff, int xstart, unsigned int xoffsets, int xstep, int ystart, v8cint16 zbuff, int zstart, unsigned int zoffsets, int zstep)
| Complex multiply-negate intrinsic function after computing the maximum between the selected lanes from the input buffer using small X input buffer.
v4cacc48 | negmul4_max (v32int16 xbuff, int xstart, unsigned int xoffsets, int xstep, v32int16 ybuff, int ystart, v8cint16 zbuff, int zstart, unsigned int zoffsets, int zstep)
| Complex multiply-negate intrinsic function after computing the maximum between the selected lanes from the input buffer using small X input buffer.
v4cacc48 | negmul4_max (v64int16 xbuff, int xstart, unsigned int xoffsets, int xstep, int ystart, v8cint16 zbuff, int zstart, unsigned int zoffsets, int zstep)
| Complex multiply-negate intrinsic function after computing the maximum between the selected lanes from the input buffer .
v4cacc48 | negmul4_maxdiff (v32int16 xbuff, int xstart, unsigned int xoffsets, int xstep, int ystart, v8cint16 zbuff, int zstart, unsigned int zoffsets, int zstep)
| Complex multiply-negate intrinsic function after computing the maximum difference between the selected lanes from the input buffer using small X input buffer.
v4cacc48 | negmul4_maxdiff (v32int16 xbuff, int xstart, unsigned int xoffsets, int xstep, v32int16 ybuff, int ystart, v8cint16 zbuff, int zstart, unsigned int zoffsets, int zstep)
| Complex multiply-negate intrinsic function after computing the maximum difference between the selected lanes from the input buffer using small X input buffer.
v4cacc48 | negmul4_maxdiff (v64int16 xbuff, int xstart, unsigned int xoffsets, int xstep, int ystart, v8cint16 zbuff, int zstart, unsigned int zoffsets, int zstep)
| Complex multiply-negate intrinsic function after computing the maximum difference between the selected lanes from the input buffer .
v4cacc48 | negmul4_min (v32int16 xbuff, int xstart, unsigned int xoffsets, int xstep, int ystart, v8cint16 zbuff, int zstart, unsigned int zoffsets, int zstep)
| Complex multiply-negate intrinsic function after computing the minimum between the selected lanes from the input buffer using small X input buffer.
v4cacc48 | negmul4_min (v32int16 xbuff, int xstart, unsigned int xoffsets, int xstep, v32int16 ybuff, int ystart, v8cint16 zbuff, int zstart, unsigned int zoffsets, int zstep)
| Complex multiply-negate intrinsic function after computing the minimum between the selected lanes from the input buffer using small X input buffer.
v4cacc48 | negmul4_min (v64int16 xbuff, int xstart, unsigned int xoffsets, int xstep, int ystart, v8cint16 zbuff, int zstart, unsigned int zoffsets, int zstep)
| Complex multiply-negate intrinsic function after computing the minimum between the selected lanes from the input buffer .
v8cacc48 | negmul8_abs (v32int16 xbuff, int xstart, unsigned int xoffsets, int xstep, v8cint16 zbuff, int zstart, unsigned int zoffsets, int zstep)
| Complex multiply-negate intrinsic function after computing the absolute value in the selected lanes from the input buffer using small X input buffer.
v8cacc48 | negmul8_abs (v64int16 xbuff, int xstart, unsigned int xoffsets, int xstep, v8cint16 zbuff, int zstart, unsigned int zoffsets, int zstep)
| Complex multiply-negate intrinsic function after computing the absolute value in the selected lanes from the input buffer .
v8cacc48 | negmul8_max (v32int16 xbuff, int xstart, unsigned int xoffsets, int xstep, int ystart, v8cint16 zbuff, int zstart, unsigned int zoffsets, int zstep)
| Complex multiply-negate intrinsic function after computing the maximum between the selected lanes from the input buffer using small X input buffer.
v8cacc48 | negmul8_max (v32int16 xbuff, int xstart, unsigned int xoffsets, int xstep, v32int16 ybuff, int ystart, v8cint16 zbuff, int zstart, unsigned int zoffsets, int zstep)
| Complex multiply-negate intrinsic function after computing the maximum between the selected lanes from the input buffer using small X input buffer.
v8cacc48 | negmul8_max (v64int16 xbuff, int xstart, unsigned int xoffsets, int xstep, int ystart, v8cint16 zbuff, int zstart, unsigned int zoffsets, int zstep)
| Complex multiply-negate intrinsic function after computing the maximum between the selected lanes from the input buffer .
v8cacc48 | negmul8_maxdiff (v32int16 xbuff, int xstart, unsigned int xoffsets, int xstep, int ystart, v8cint16 zbuff, int zstart, unsigned int zoffsets, int zstep)
| Complex multiply-negate intrinsic function after computing the maximum difference between the selected lanes from the input buffer using small X input buffer.
v8cacc48 | negmul8_maxdiff (v32int16 xbuff, int xstart, unsigned int xoffsets, int xstep, v32int16 ybuff, int ystart, v8cint16 zbuff, int zstart, unsigned int zoffsets, int zstep)
| Complex multiply-negate intrinsic function after computing the maximum difference between the selected lanes from the input buffer using small X input buffer.
v8cacc48 | negmul8_maxdiff (v64int16 xbuff, int xstart, unsigned int xoffsets, int xstep, int ystart, v8cint16 zbuff, int zstart, unsigned int zoffsets, int zstep)
| Complex multiply-negate intrinsic function after computing the maximum difference between the selected lanes from the input buffer .
v8cacc48 | negmul8_min (v32int16 xbuff, int xstart, unsigned int xoffsets, int xstep, int ystart, v8cint16 zbuff, int zstart, unsigned int zoffsets, int zstep)
| Complex multiply-negate intrinsic function after computing the minimum between the selected lanes from the input buffer using small X input buffer.
v8cacc48 | negmul8_min (v32int16 xbuff, int xstart, unsigned int xoffsets, int xstep, v32int16 ybuff, int ystart, v8cint16 zbuff, int zstart, unsigned int zoffsets, int zstep)
| Complex multiply-negate intrinsic function after computing the minimum between the selected lanes from the input buffer using small X input buffer.
v8cacc48 | negmul8_min (v64int16 xbuff, int xstart, unsigned int xoffsets, int xstep, int ystart, v8cint16 zbuff, int zstart, unsigned int zoffsets, int zstep)
| Complex multiply-negate intrinsic function after computing the minimum between the selected lanes from the input buffer .

## Function Documentation

## ◆ mac4_abs() [1/2]

v4cacc48 mac4_abs | ( | v4cacc48 | acc,
|  | v32int16 | xbuff,
|  | int | xstart,
|  | unsigned int | xoffsets,
|  | int | xstep,
|  | v8cint16 | zbuff,
|  | int | zstart,
|  | unsigned int | zoffsets,
|  | int | zstep )

Complex multiply-accumulate intrinsic function after computing the absolute value in the selected lanes from the input buffer using small X input buffer.

acc0 += z00*abs(x00) + z01*abs(x01) + z02*abs(x02) + z03*abs(x03)
acc1 += z10*abs(x10) + z11*abs(x11) + z12*abs(x12) + z13*abs(x13)
acc2 += z20*abs(x20) + z21*abs(x21) + z22*abs(x22) + z23*abs(x23)
acc3 += z30*abs(x30) + z31*abs(x31) + z32*abs(x32) + z33*abs(x33)

Returns
  Returned accumulation vector (4 x cint48 lanes)

Parameters

  acc | Incoming accumulation vector (4 x cint48 lanes)
  xbuff | Input buffer of 32 elements of type int16
  xstart | Starting position offset applied to all lanes of input from X buffer.
  xoffsets | 4b offset for each lane, applied to the x buffer. LSB apply to first lane
  xstep | Step between each column for selection in the xbuffer.
  zbuff | Input buffer of 8 elements of type cint16
  zstart | Starting position offset applied to all lanes for input from Z buffer. This must be a compile time constant. Only the 4 LSB of the argument are used.
  zoffsets | 4b offset for each lane, applied to input from Z buffer. LSB apply to first lane
  zstep | Step between each column for selection in the zbuffer.

Note
  - For more information on how data selection works from the buffers go here. The data buffer and coefficient buffer in this intrinsic use the general scheme.
  - Parameter 'zstart' must be a compile time constant.

## ◆ mac4_abs() [2/2]

v4cacc48 mac4_abs | ( | v4cacc48 | acc,
|  | v64int16 | xbuff,
|  | int | xstart,
|  | unsigned int | xoffsets,
|  | int | xstep,
|  | v8cint16 | zbuff,
|  | int | zstart,
|  | unsigned int | zoffsets,
|  | int | zstep )

Complex multiply-accumulate intrinsic function after computing the absolute value in the selected lanes from the input buffer .

acc0 += z00*abs(x00) + z01*abs(x01) + z02*abs(x02) + z03*abs(x03)
acc1 += z10*abs(x10) + z11*abs(x11) + z12*abs(x12) + z13*abs(x13)
acc2 += z20*abs(x20) + z21*abs(x21) + z22*abs(x22) + z23*abs(x23)
acc3 += z30*abs(x30) + z31*abs(x31) + z32*abs(x32) + z33*abs(x33)

Returns
  Returned accumulation vector (4 x cint48 lanes)

Parameters

  acc | Incoming accumulation vector (4 x cint48 lanes)
  xbuff | Input buffer of 64 elements of type int16
  xstart | Starting position offset applied to all lanes of input from X buffer.
  xoffsets | 4b offset for each lane, applied to the x buffer. LSB apply to first lane
  xstep | Step between each column for selection in the xbuffer.
  zbuff | Input buffer of 8 elements of type cint16
  zstart | Starting position offset applied to all lanes for input from Z buffer. This must be a compile time constant. Only the 4 LSB of the argument are used.
  zoffsets | 4b offset for each lane, applied to input from Z buffer. LSB apply to first lane
  zstep | Step between each column for selection in the zbuffer.

Note
  - For more information on how data selection works from the buffers go here. The data buffer and coefficient buffer in this intrinsic use the general scheme.
  - Parameter 'zstart' must be a compile time constant.

## ◆ mac4_max() [1/3]

v4cacc48 mac4_max | ( | v4cacc48 | acc,
|  | v32int16 | xbuff,
|  | int | xstart,
|  | unsigned int | xoffsets,
|  | int | xstep,
|  | int | ystart,
|  | v8cint16 | zbuff,
|  | int | zstart,
|  | unsigned int | zoffsets,
|  | int | zstep )

Complex multiply-accumulate intrinsic function after computing the maximum between the selected lanes from the input buffer using small X input buffer.

acc0 += z00*(max(x00 , y00)) + z01*(max(x01 , y01)) + z02*(max(x02 , y02)) + z03*(max(x03 , y03))
acc1 += z10*(max(x10 , y10)) + z11*(max(x11 , y11)) + z12*(max(x12 , y12)) + z13*(max(x13 , y13))
acc2 += z20*(max(x20 , y20)) + z21*(max(x21 , y21)) + z22*(max(x22 , y22)) + z23*(max(x23 , y23))
acc3 += z30*(max(x30 , y30)) + z31*(max(x31 , y31)) + z32*(max(x32 , y32)) + z33*(max(x33 , y33))

Returns
  Returned accumulation vector (4 x cint48 lanes)

Parameters

  acc | Incoming accumulation vector (4 x cint48 lanes)
  xbuff | Input buffer of 32 elements of type int16
  xstart | Starting position offset applied to all lanes of input from X buffer.
  xoffsets | 4b offset for each lane, applied to both x and y buffers. LSB apply to first lane
  xstep | Step between each column for selection in the x and y buffers. Ystep is symmetric to xstep (ystep advances by -xstep).
  ystart | Starting position offset applied to all lanes for input from Y buffer.
  zbuff | Input buffer of 8 elements of type cint16
  zstart | Starting position offset applied to all lanes for input from Z buffer. This must be a compile time constant. Only the 4 LSB of the argument are used.
  zoffsets | 4b offset for each lane, applied to input from Z buffer. LSB apply to first lane
  zstep | Step between each column for selection in the zbuffer.

Note
  - For more information on how data selection works from the buffers go here. The data buffer and coefficient buffer in this intrinsic use the general scheme.
  - Parameter 'zstart' must be a compile time constant.

## ◆ mac4_max() [2/3]

v4cacc48 mac4_max | ( | v4cacc48 | acc,
|  | v32int16 | xbuff,
|  | int | xstart,
|  | unsigned int | xoffsets,
|  | int | xstep,
|  | v32int16 | ybuff,
|  | int | ystart,
|  | v8cint16 | zbuff,
|  | int | zstart,
|  | unsigned int | zoffsets,
|  | int | zstep )

Complex multiply-accumulate intrinsic function after computing the maximum between the selected lanes from the input buffer using small X input buffer.

acc0 += z00*(max(x00 , y00)) + z01*(max(x01 , y01)) + z02*(max(x02 , y02)) + z03*(max(x03 , y03))
acc1 += z10*(max(x10 , y10)) + z11*(max(x11 , y11)) + z12*(max(x12 , y12)) + z13*(max(x13 , y13))
acc2 += z20*(max(x20 , y20)) + z21*(max(x21 , y21)) + z22*(max(x22 , y22)) + z23*(max(x23 , y23))
acc3 += z30*(max(x30 , y30)) + z31*(max(x31 , y31)) + z32*(max(x32 , y32)) + z33*(max(x33 , y33))

Returns
  Returned accumulation vector (4 x cint48 lanes)

Parameters

  acc | Incoming accumulation vector (4 x cint48 lanes)
  xbuff | Input buffer of 32 elements of type int16
  xstart | Starting position offset applied to all lanes of input from X buffer.
  xoffsets | 4b offset for each lane, applied to both x and y buffers. LSB apply to first lane
  xstep | Step between each column for selection in the x and y buffers. Ystep is symmetric to xstep (ystep advances by -xstep).
  ybuff | Right input buffer of 32 elements of type int16
  ystart | Starting position offset applied to all lanes for input from Y buffer.
  zbuff | Input buffer of 8 elements of type cint16
  zstart | Starting position offset applied to all lanes for input from Z buffer. This must be a compile time constant. Only the 4 LSB of the argument are used.
  zoffsets | 4b offset for each lane, applied to input from Z buffer. LSB apply to first lane
  zstep | Step between each column for selection in the zbuffer.

Note
  - For more information on how data selection works from the buffers go here. The data buffer and coefficient buffer in this intrinsic use the general scheme.
  - Parameter 'zstart' must be a compile time constant.

## ◆ mac4_max() [3/3]

v4cacc48 mac4_max | ( | v4cacc48 | acc,
|  | v64int16 | xbuff,
|  | int | xstart,
|  | unsigned int | xoffsets,
|  | int | xstep,
|  | int | ystart,
|  | v8cint16 | zbuff,
|  | int | zstart,
|  | unsigned int | zoffsets,
|  | int | zstep )

Complex multiply-accumulate intrinsic function after computing the maximum between the selected lanes from the input buffer .

acc0 += z00*(max(x00 , y00)) + z01*(max(x01 , y01)) + z02*(max(x02 , y02)) + z03*(max(x03 , y03))
acc1 += z10*(max(x10 , y10)) + z11*(max(x11 , y11)) + z12*(max(x12 , y12)) + z13*(max(x13 , y13))
acc2 += z20*(max(x20 , y20)) + z21*(max(x21 , y21)) + z22*(max(x22 , y22)) + z23*(max(x23 , y23))
acc3 += z30*(max(x30 , y30)) + z31*(max(x31 , y31)) + z32*(max(x32 , y32)) + z33*(max(x33 , y33))

Returns
  Returned accumulation vector (4 x cint48 lanes)

Parameters

  acc | Incoming accumulation vector (4 x cint48 lanes)
  xbuff | Input buffer of 64 elements of type int16
  xstart | Starting position offset applied to all lanes of input from X buffer.
  xoffsets | 4b offset for each lane, applied to both x and y buffers. LSB apply to first lane
  xstep | Step between each column for selection in the x and y buffers. Ystep is symmetric to xstep (ystep advances by -xstep).
  ystart | Starting position offset applied to all lanes for input from Y buffer.
  zbuff | Input buffer of 8 elements of type cint16
  zstart | Starting position offset applied to all lanes for input from Z buffer. This must be a compile time constant. Only the 4 LSB of the argument are used.
  zoffsets | 4b offset for each lane, applied to input from Z buffer. LSB apply to first lane
  zstep | Step between each column for selection in the zbuffer.

Note
  - For more information on how data selection works from the buffers go here. The data buffer and coefficient buffer in this intrinsic use the general scheme.
  - Parameter 'zstart' must be a compile time constant.

## ◆ mac4_maxdiff() [1/3]

v4cacc48 mac4_maxdiff | ( | v4cacc48 | acc,
|  | v32int16 | xbuff,
|  | int | xstart,
|  | unsigned int | xoffsets,
|  | int | xstep,
|  | int | ystart,
|  | v8cint16 | zbuff,
|  | int | zstart,
|  | unsigned int | zoffsets,
|  | int | zstep )

Complex multiply-accumulate intrinsic function after computing the maximum difference between the selected lanes from the input buffer using small X input buffer.

acc0 += z00*((x00 - y00 > 0) ? (x00 - y00):0) + z01*((x01 - y01 > 0) ? (x01 - y01):0) + z02*((x02 - y02 > 0) ? (x02 - y02):0) + z03*((x03 - y03 > 0) ? (x03 - y03):0)
acc1 += z10*((x10 - y10 > 0) ? (x10 - y10):0) + z11*((x11 - y11 > 0) ? (x11 - y11):0) + z12*((x12 - y12 > 0) ? (x12 - y12):0) + z13*((x13 - y13 > 0) ? (x13 - y13):0)
acc2 += z20*((x20 - y20 > 0) ? (x20 - y20):0) + z21*((x21 - y21 > 0) ? (x21 - y21):0) + z22*((x22 - y22 > 0) ? (x22 - y22):0) + z23*((x23 - y23 > 0) ? (x23 - y23):0)
acc3 += z30*((x30 - y30 > 0) ? (x30 - y30):0) + z31*((x31 - y31 > 0) ? (x31 - y31):0) + z32*((x32 - y32 > 0) ? (x32 - y32):0) + z33*((x33 - y33 > 0) ? (x33 - y33):0)

Returns
  Returned accumulation vector (4 x cint48 lanes)

Parameters

  acc | Incoming accumulation vector (4 x cint48 lanes)
  xbuff | Input buffer of 32 elements of type int16
  xstart | Starting position offset applied to all lanes of input from X buffer.
  xoffsets | 4b offset for each lane, applied to both x and y buffers. LSB apply to first lane
  xstep | Step between each column for selection in the x and y buffers. Ystep is symmetric to xstep (ystep advances by -xstep).
  ystart | Starting position offset applied to all lanes for input from Y buffer.
  zbuff | Input buffer of 8 elements of type cint16
  zstart | Starting position offset applied to all lanes for input from Z buffer. This must be a compile time constant. Only the 4 LSB of the argument are used.
  zoffsets | 4b offset for each lane, applied to input from Z buffer. LSB apply to first lane
  zstep | Step between each column for selection in the zbuffer.

Note
  - For more information on how data selection works from the buffers go here. The data buffer and coefficient buffer in this intrinsic use the general scheme.
  - Parameter 'zstart' must be a compile time constant.

## ◆ mac4_maxdiff() [2/3]

v4cacc48 mac4_maxdiff | ( | v4cacc48 | acc,
|  | v32int16 | xbuff,
|  | int | xstart,
|  | unsigned int | xoffsets,
|  | int | xstep,
|  | v32int16 | ybuff,
|  | int | ystart,
|  | v8cint16 | zbuff,
|  | int | zstart,
|  | unsigned int | zoffsets,
|  | int | zstep )

Complex multiply-accumulate intrinsic function after computing the maximum difference between the selected lanes from the input buffer using small X input buffer.

acc0 += z00*((x00 - y00 > 0) ? (x00 - y00):0) + z01*((x01 - y01 > 0) ? (x01 - y01):0) + z02*((x02 - y02 > 0) ? (x02 - y02):0) + z03*((x03 - y03 > 0) ? (x03 - y03):0)
acc1 += z10*((x10 - y10 > 0) ? (x10 - y10):0) + z11*((x11 - y11 > 0) ? (x11 - y11):0) + z12*((x12 - y12 > 0) ? (x12 - y12):0) + z13*((x13 - y13 > 0) ? (x13 - y13):0)
acc2 += z20*((x20 - y20 > 0) ? (x20 - y20):0) + z21*((x21 - y21 > 0) ? (x21 - y21):0) + z22*((x22 - y22 > 0) ? (x22 - y22):0) + z23*((x23 - y23 > 0) ? (x23 - y23):0)
acc3 += z30*((x30 - y30 > 0) ? (x30 - y30):0) + z31*((x31 - y31 > 0) ? (x31 - y31):0) + z32*((x32 - y32 > 0) ? (x32 - y32):0) + z33*((x33 - y33 > 0) ? (x33 - y33):0)

Returns
  Returned accumulation vector (4 x cint48 lanes)

Parameters

  acc | Incoming accumulation vector (4 x cint48 lanes)
  xbuff | Input buffer of 32 elements of type int16
  xstart | Starting position offset applied to all lanes of input from X buffer.
  xoffsets | 4b offset for each lane, applied to both x and y buffers. LSB apply to first lane
  xstep | Step between each column for selection in the x and y buffers. Ystep is symmetric to xstep (ystep advances by -xstep).
  ybuff | Right input buffer of 32 elements of type int16
  ystart | Starting position offset applied to all lanes for input from Y buffer.
  zbuff | Input buffer of 8 elements of type cint16
  zstart | Starting position offset applied to all lanes for input from Z buffer. This must be a compile time constant. Only the 4 LSB of the argument are used.
  zoffsets | 4b offset for each lane, applied to input from Z buffer. LSB apply to first lane
  zstep | Step between each column for selection in the zbuffer.

Note
  - For more information on how data selection works from the buffers go here. The data buffer and coefficient buffer in this intrinsic use the general scheme.
  - Parameter 'zstart' must be a compile time constant.

## ◆ mac4_maxdiff() [3/3]

v4cacc48 mac4_maxdiff | ( | v4cacc48 | acc,
|  | v64int16 | xbuff,
|  | int | xstart,
|  | unsigned int | xoffsets,
|  | int | xstep,
|  | int | ystart,
|  | v8cint16 | zbuff,
|  | int | zstart,
|  | unsigned int | zoffsets,
|  | int | zstep )

Complex multiply-accumulate intrinsic function after computing the maximum difference between the selected lanes from the input buffer .

acc0 += z00*((x00 - y00 > 0) ? (x00 - y00):0) + z01*((x01 - y01 > 0) ? (x01 - y01):0) + z02*((x02 - y02 > 0) ? (x02 - y02):0) + z03*((x03 - y03 > 0) ? (x03 - y03):0)
acc1 += z10*((x10 - y10 > 0) ? (x10 - y10):0) + z11*((x11 - y11 > 0) ? (x11 - y11):0) + z12*((x12 - y12 > 0) ? (x12 - y12):0) + z13*((x13 - y13 > 0) ? (x13 - y13):0)
acc2 += z20*((x20 - y20 > 0) ? (x20 - y20):0) + z21*((x21 - y21 > 0) ? (x21 - y21):0) + z22*((x22 - y22 > 0) ? (x22 - y22):0) + z23*((x23 - y23 > 0) ? (x23 - y23):0)
acc3 += z30*((x30 - y30 > 0) ? (x30 - y30):0) + z31*((x31 - y31 > 0) ? (x31 - y31):0) + z32*((x32 - y32 > 0) ? (x32 - y32):0) + z33*((x33 - y33 > 0) ? (x33 - y33):0)

Returns
  Returned accumulation vector (4 x cint48 lanes)

Parameters

  acc | Incoming accumulation vector (4 x cint48 lanes)
  xbuff | Input buffer of 64 elements of type int16
  xstart | Starting position offset applied to all lanes of input from X buffer.
  xoffsets | 4b offset for each lane, applied to both x and y buffers. LSB apply to first lane
  xstep | Step between each column for selection in the x and y buffers. Ystep is symmetric to xstep (ystep advances by -xstep).
  ystart | Starting position offset applied to all lanes for input from Y buffer.
  zbuff | Input buffer of 8 elements of type cint16
  zstart | Starting position offset applied to all lanes for input from Z buffer. This must be a compile time constant. Only the 4 LSB of the argument are used.
  zoffsets | 4b offset for each lane, applied to input from Z buffer. LSB apply to first lane
  zstep | Step between each column for selection in the zbuffer.

Note
  - For more information on how data selection works from the buffers go here. The data buffer and coefficient buffer in this intrinsic use the general scheme.
  - Parameter 'zstart' must be a compile time constant.

## ◆ mac4_min() [1/3]

v4cacc48 mac4_min | ( | v4cacc48 | acc,
|  | v32int16 | xbuff,
|  | int | xstart,
|  | unsigned int | xoffsets,
|  | int | xstep,
|  | int | ystart,
|  | v8cint16 | zbuff,
|  | int | zstart,
|  | unsigned int | zoffsets,
|  | int | zstep )

Complex multiply-accumulate intrinsic function after computing the minimum between the selected lanes from the input buffer using small X input buffer.

acc0 += z00*(min(x00 , y00)) + z01*(min(x01 , y01)) + z02*(min(x02 , y02)) + z03*(min(x03 , y03))
acc1 += z10*(min(x10 , y10)) + z11*(min(x11 , y11)) + z12*(min(x12 , y12)) + z13*(min(x13 , y13))
acc2 += z20*(min(x20 , y20)) + z21*(min(x21 , y21)) + z22*(min(x22 , y22)) + z23*(min(x23 , y23))
acc3 += z30*(min(x30 , y30)) + z31*(min(x31 , y31)) + z32*(min(x32 , y32)) + z33*(min(x33 , y33))

Returns
  Returned accumulation vector (4 x cint48 lanes)

Parameters

  acc | Incoming accumulation vector (4 x cint48 lanes)
  xbuff | Input buffer of 32 elements of type int16
  xstart | Starting position offset applied to all lanes of input from X buffer.
  xoffsets | 4b offset for each lane, applied to both x and y buffers. LSB apply to first lane
  xstep | Step between each column for selection in the x and y buffers. Ystep is symmetric to xstep (ystep advances by -xstep).
  ystart | Starting position offset applied to all lanes for input from Y buffer.
  zbuff | Input buffer of 8 elements of type cint16
  zstart | Starting position offset applied to all lanes for input from Z buffer. This must be a compile time constant. Only the 4 LSB of the argument are used.
  zoffsets | 4b offset for each lane, applied to input from Z buffer. LSB apply to first lane
  zstep | Step between each column for selection in the zbuffer.

Note
  - For more information on how data selection works from the buffers go here. The data buffer and coefficient buffer in this intrinsic use the general scheme.
  - Parameter 'zstart' must be a compile time constant.

## ◆ mac4_min() [2/3]

v4cacc48 mac4_min | ( | v4cacc48 | acc,
|  | v32int16 | xbuff,
|  | int | xstart,
|  | unsigned int | xoffsets,
|  | int | xstep,
|  | v32int16 | ybuff,
|  | int | ystart,
|  | v8cint16 | zbuff,
|  | int | zstart,
|  | unsigned int | zoffsets,
|  | int | zstep )

Complex multiply-accumulate intrinsic function after computing the minimum between the selected lanes from the input buffer using small X input buffer.

acc0 += z00*(min(x00 , y00)) + z01*(min(x01 , y01)) + z02*(min(x02 , y02)) + z03*(min(x03 , y03))
acc1 += z10*(min(x10 , y10)) + z11*(min(x11 , y11)) + z12*(min(x12 , y12)) + z13*(min(x13 , y13))
acc2 += z20*(min(x20 , y20)) + z21*(min(x21 , y21)) + z22*(min(x22 , y22)) + z23*(min(x23 , y23))
acc3 += z30*(min(x30 , y30)) + z31*(min(x31 , y31)) + z32*(min(x32 , y32)) + z33*(min(x33 , y33))

Returns
  Returned accumulation vector (4 x cint48 lanes)

Parameters

  acc | Incoming accumulation vector (4 x cint48 lanes)
  xbuff | Input buffer of 32 elements of type int16
  xstart | Starting position offset applied to all lanes of input from X buffer.
  xoffsets | 4b offset for each lane, applied to both x and y buffers. LSB apply to first lane
  xstep | Step between each column for selection in the x and y buffers. Ystep is symmetric to xstep (ystep advances by -xstep).
  ybuff | Right input buffer of 32 elements of type int16
  ystart | Starting position offset applied to all lanes for input from Y buffer.
  zbuff | Input buffer of 8 elements of type cint16
  zstart | Starting position offset applied to all lanes for input from Z buffer. This must be a compile time constant. Only the 4 LSB of the argument are used.
  zoffsets | 4b offset for each lane, applied to input from Z buffer. LSB apply to first lane
  zstep | Step between each column for selection in the zbuffer.

Note
  - For more information on how data selection works from the buffers go here. The data buffer and coefficient buffer in this intrinsic use the general scheme.
  - Parameter 'zstart' must be a compile time constant.

## ◆ mac4_min() [3/3]

v4cacc48 mac4_min | ( | v4cacc48 | acc,
|  | v64int16 | xbuff,
|  | int | xstart,
|  | unsigned int | xoffsets,
|  | int | xstep,
|  | int | ystart,
|  | v8cint16 | zbuff,
|  | int | zstart,
|  | unsigned int | zoffsets,
|  | int | zstep )

Complex multiply-accumulate intrinsic function after computing the minimum between the selected lanes from the input buffer .

acc0 += z00*(min(x00 , y00)) + z01*(min(x01 , y01)) + z02*(min(x02 , y02)) + z03*(min(x03 , y03))
acc1 += z10*(min(x10 , y10)) + z11*(min(x11 , y11)) + z12*(min(x12 , y12)) + z13*(min(x13 , y13))
acc2 += z20*(min(x20 , y20)) + z21*(min(x21 , y21)) + z22*(min(x22 , y22)) + z23*(min(x23 , y23))
acc3 += z30*(min(x30 , y30)) + z31*(min(x31 , y31)) + z32*(min(x32 , y32)) + z33*(min(x33 , y33))

Returns
  Returned accumulation vector (4 x cint48 lanes)

Parameters

  acc | Incoming accumulation vector (4 x cint48 lanes)
  xbuff | Input buffer of 64 elements of type int16
  xstart | Starting position offset applied to all lanes of input from X buffer.
  xoffsets | 4b offset for each lane, applied to both x and y buffers. LSB apply to first lane
  xstep | Step between each column for selection in the x and y buffers. Ystep is symmetric to xstep (ystep advances by -xstep).
  ystart | Starting position offset applied to all lanes for input from Y buffer.
  zbuff | Input buffer of 8 elements of type cint16
  zstart | Starting position offset applied to all lanes for input from Z buffer. This must be a compile time constant. Only the 4 LSB of the argument are used.
  zoffsets | 4b offset for each lane, applied to input from Z buffer. LSB apply to first lane
  zstep | Step between each column for selection in the zbuffer.

Note
  - For more information on how data selection works from the buffers go here. The data buffer and coefficient buffer in this intrinsic use the general scheme.
  - Parameter 'zstart' must be a compile time constant.

## ◆ mac8_abs() [1/2]

v8cacc48 mac8_abs | ( | v8cacc48 | acc,
|  | v32int16 | xbuff,
|  | int | xstart,
|  | unsigned int | xoffsets,
|  | int | xstep,
|  | v8cint16 | zbuff,
|  | int | zstart,
|  | unsigned int | zoffsets,
|  | int | zstep )

Complex multiply-accumulate intrinsic function after computing the absolute value in the selected lanes from the input buffer using small X input buffer.

acc0 += z00*abs(x00) + z01*abs(x01)
acc1 += z10*abs(x10) + z11*abs(x11)
acc2 += z20*abs(x20) + z21*abs(x21)
acc3 += z30*abs(x30) + z31*abs(x31)
acc4 += z40*abs(x40) + z41*abs(x41)
acc5 += z50*abs(x50) + z51*abs(x51)
acc6 += z60*abs(x60) + z61*abs(x61)
acc7 += z70*abs(x70) + z71*abs(x71)

Returns
  Returned accumulation vector (8 x cint48 lanes)

Parameters

  acc | Incoming accumulation vector (8 x cint48 lanes)
  xbuff | Input buffer of 32 elements of type int16
  xstart | Starting position offset applied to all lanes of input from X buffer.
  xoffsets | 4b offset for each lane, applied to the x buffer. LSB apply to first lane
  xstep | Step between each column for selection in the xbuffer.
  zbuff | Input buffer of 8 elements of type cint16
  zstart | Starting position offset applied to all lanes for input from Z buffer. This must be a compile time constant. Only the 4 LSB of the argument are used.
  zoffsets | 4b offset for each lane, applied to input from Z buffer. LSB apply to first lane
  zstep | Step between each column for selection in the zbuffer.

Note
  - For more information on how data selection works from the buffers go here. The data buffer and coefficient buffer in this intrinsic use the general scheme.
  - Parameter 'zstart' must be a compile time constant.

## ◆ mac8_abs() [2/2]

v8cacc48 mac8_abs | ( | v8cacc48 | acc,
|  | v64int16 | xbuff,
|  | int | xstart,
|  | unsigned int | xoffsets,
|  | int | xstep,
|  | v8cint16 | zbuff,
|  | int | zstart,
|  | unsigned int | zoffsets,
|  | int | zstep )

Complex multiply-accumulate intrinsic function after computing the absolute value in the selected lanes from the input buffer .

acc0 += z00*abs(x00) + z01*abs(x01)
acc1 += z10*abs(x10) + z11*abs(x11)
acc2 += z20*abs(x20) + z21*abs(x21)
acc3 += z30*abs(x30) + z31*abs(x31)
acc4 += z40*abs(x40) + z41*abs(x41)
acc5 += z50*abs(x50) + z51*abs(x51)
acc6 += z60*abs(x60) + z61*abs(x61)
acc7 += z70*abs(x70) + z71*abs(x71)

Returns
  Returned accumulation vector (8 x cint48 lanes)

Parameters

  acc | Incoming accumulation vector (8 x cint48 lanes)
  xbuff | Input buffer of 64 elements of type int16
  xstart | Starting position offset applied to all lanes of input from X buffer.
  xoffsets | 4b offset for each lane, applied to the x buffer. LSB apply to first lane
  xstep | Step between each column for selection in the xbuffer.
  zbuff | Input buffer of 8 elements of type cint16
  zstart | Starting position offset applied to all lanes for input from Z buffer. This must be a compile time constant. Only the 4 LSB of the argument are used.
  zoffsets | 4b offset for each lane, applied to input from Z buffer. LSB apply to first lane
  zstep | Step between each column for selection in the zbuffer.

Note
  - For more information on how data selection works from the buffers go here. The data buffer and coefficient buffer in this intrinsic use the general scheme.
  - Parameter 'zstart' must be a compile time constant.

## ◆ mac8_max() [1/3]

v8cacc48 mac8_max | ( | v8cacc48 | acc,
|  | v32int16 | xbuff,
|  | int | xstart,
|  | unsigned int | xoffsets,
|  | int | xstep,
|  | int | ystart,
|  | v8cint16 | zbuff,
|  | int | zstart,
|  | unsigned int | zoffsets,
|  | int | zstep )

Complex multiply-accumulate intrinsic function after computing the maximum between the selected lanes from the input buffer using small X input buffer.

acc0 += z00*(max(x00 , y00)) + z01*(max(x01 , y01))
acc1 += z10*(max(x10 , y10)) + z11*(max(x11 , y11))
acc2 += z20*(max(x20 , y20)) + z21*(max(x21 , y21))
acc3 += z30*(max(x30 , y30)) + z31*(max(x31 , y31))
acc4 += z40*(max(x40 , y40)) + z41*(max(x41 , y41))
acc5 += z50*(max(x50 , y50)) + z51*(max(x51 , y51))
acc6 += z60*(max(x60 , y60)) + z61*(max(x61 , y61))
acc7 += z70*(max(x70 , y70)) + z71*(max(x71 , y71))

Returns
  Returned accumulation vector (8 x cint48 lanes)

Parameters

  acc | Incoming accumulation vector (8 x cint48 lanes)
  xbuff | Input buffer of 32 elements of type int16
  xstart | Starting position offset applied to all lanes of input from X buffer.
  xoffsets | 4b offset for each lane, applied to both x and y buffers. LSB apply to first lane
  xstep | Step between each column for selection in the x and y buffers. Ystep is symmetric to xstep (ystep advances by -xstep).
  ystart | Starting position offset applied to all lanes for input from Y buffer.
  zbuff | Input buffer of 8 elements of type cint16
  zstart | Starting position offset applied to all lanes for input from Z buffer. This must be a compile time constant. Only the 4 LSB of the argument are used.
  zoffsets | 4b offset for each lane, applied to input from Z buffer. LSB apply to first lane
  zstep | Step between each column for selection in the zbuffer.

Note
  - For more information on how data selection works from the buffers go here. The data buffer and coefficient buffer in this intrinsic use the general scheme.
  - Parameter 'zstart' must be a compile time constant.

## ◆ mac8_max() [2/3]

v8cacc48 mac8_max | ( | v8cacc48 | acc,
|  | v32int16 | xbuff,
|  | int | xstart,
|  | unsigned int | xoffsets,
|  | int | xstep,
|  | v32int16 | ybuff,
|  | int | ystart,
|  | v8cint16 | zbuff,
|  | int | zstart,
|  | unsigned int | zoffsets,
|  | int | zstep )

Complex multiply-accumulate intrinsic function after computing the maximum between the selected lanes from the input buffer using small X input buffer.

acc0 += z00*(max(x00 , y00)) + z01*(max(x01 , y01))
acc1 += z10*(max(x10 , y10)) + z11*(max(x11 , y11))
acc2 += z20*(max(x20 , y20)) + z21*(max(x21 , y21))
acc3 += z30*(max(x30 , y30)) + z31*(max(x31 , y31))
acc4 += z40*(max(x40 , y40)) + z41*(max(x41 , y41))
acc5 += z50*(max(x50 , y50)) + z51*(max(x51 , y51))
acc6 += z60*(max(x60 , y60)) + z61*(max(x61 , y61))
acc7 += z70*(max(x70 , y70)) + z71*(max(x71 , y71))

Returns
  Returned accumulation vector (8 x cint48 lanes)

Parameters

  acc | Incoming accumulation vector (8 x cint48 lanes)
  xbuff | Input buffer of 32 elements of type int16
  xstart | Starting position offset applied to all lanes of input from X buffer.
  xoffsets | 4b offset for each lane, applied to both x and y buffers. LSB apply to first lane
  xstep | Step between each column for selection in the x and y buffers. Ystep is symmetric to xstep (ystep advances by -xstep).
  ybuff | Right input buffer of 32 elements of type int16
  ystart | Starting position offset applied to all lanes for input from Y buffer.
  zbuff | Input buffer of 8 elements of type cint16
  zstart | Starting position offset applied to all lanes for input from Z buffer. This must be a compile time constant. Only the 4 LSB of the argument are used.
  zoffsets | 4b offset for each lane, applied to input from Z buffer. LSB apply to first lane
  zstep | Step between each column for selection in the zbuffer.

Note
  - For more information on how data selection works from the buffers go here. The data buffer and coefficient buffer in this intrinsic use the general scheme.
  - Parameter 'zstart' must be a compile time constant.

## ◆ mac8_max() [3/3]

v8cacc48 mac8_max | ( | v8cacc48 | acc,
|  | v64int16 | xbuff,
|  | int | xstart,
|  | unsigned int | xoffsets,
|  | int | xstep,
|  | int | ystart,
|  | v8cint16 | zbuff,
|  | int | zstart,
|  | unsigned int | zoffsets,
|  | int | zstep )

Complex multiply-accumulate intrinsic function after computing the maximum between the selected lanes from the input buffer .

acc0 += z00*(max(x00 , y00)) + z01*(max(x01 , y01))
acc1 += z10*(max(x10 , y10)) + z11*(max(x11 , y11))
acc2 += z20*(max(x20 , y20)) + z21*(max(x21 , y21))
acc3 += z30*(max(x30 , y30)) + z31*(max(x31 , y31))
acc4 += z40*(max(x40 , y40)) + z41*(max(x41 , y41))
acc5 += z50*(max(x50 , y50)) + z51*(max(x51 , y51))
acc6 += z60*(max(x60 , y60)) + z61*(max(x61 , y61))
acc7 += z70*(max(x70 , y70)) + z71*(max(x71 , y71))

Returns
  Returned accumulation vector (8 x cint48 lanes)

Parameters

  acc | Incoming accumulation vector (8 x cint48 lanes)
  xbuff | Input buffer of 64 elements of type int16
  xstart | Starting position offset applied to all lanes of input from X buffer.
  xoffsets | 4b offset for each lane, applied to both x and y buffers. LSB apply to first lane
  xstep | Step between each column for selection in the x and y buffers. Ystep is symmetric to xstep (ystep advances by -xstep).
  ystart | Starting position offset applied to all lanes for input from Y buffer.
  zbuff | Input buffer of 8 elements of type cint16
  zstart | Starting position offset applied to all lanes for input from Z buffer. This must be a compile time constant. Only the 4 LSB of the argument are used.
  zoffsets | 4b offset for each lane, applied to input from Z buffer. LSB apply to first lane
  zstep | Step between each column for selection in the zbuffer.

Note
  - For more information on how data selection works from the buffers go here. The data buffer and coefficient buffer in this intrinsic use the general scheme.
  - Parameter 'zstart' must be a compile time constant.

## ◆ mac8_maxdiff() [1/3]

v8cacc48 mac8_maxdiff | ( | v8cacc48 | acc,
|  | v32int16 | xbuff,
|  | int | xstart,
|  | unsigned int | xoffsets,
|  | int | xstep,
|  | int | ystart,
|  | v8cint16 | zbuff,
|  | int | zstart,
|  | unsigned int | zoffsets,
|  | int | zstep )

Complex multiply-accumulate intrinsic function after computing the maximum difference between the selected lanes from the input buffer using small X input buffer.

acc0 += z00*((x00 - y00 > 0) ? (x00 - y00):0) + z01*((x01 - y01 > 0) ? (x01 - y01):0)
acc1 += z10*((x10 - y10 > 0) ? (x10 - y10):0) + z11*((x11 - y11 > 0) ? (x11 - y11):0)
acc2 += z20*((x20 - y20 > 0) ? (x20 - y20):0) + z21*((x21 - y21 > 0) ? (x21 - y21):0)
acc3 += z30*((x30 - y30 > 0) ? (x30 - y30):0) + z31*((x31 - y31 > 0) ? (x31 - y31):0)
acc4 += z40*((x40 - y40 > 0) ? (x40 - y40):0) + z41*((x41 - y41 > 0) ? (x41 - y41):0)
acc5 += z50*((x50 - y50 > 0) ? (x50 - y50):0) + z51*((x51 - y51 > 0) ? (x51 - y51):0)
acc6 += z60*((x60 - y60 > 0) ? (x60 - y60):0) + z61*((x61 - y61 > 0) ? (x61 - y61):0)
acc7 += z70*((x70 - y70 > 0) ? (x70 - y70):0) + z71*((x71 - y71 > 0) ? (x71 - y71):0)

Returns
  Returned accumulation vector (8 x cint48 lanes)

Parameters

  acc | Incoming accumulation vector (8 x cint48 lanes)
  xbuff | Input buffer of 32 elements of type int16
  xstart | Starting position offset applied to all lanes of input from X buffer.
  xoffsets | 4b offset for each lane, applied to both x and y buffers. LSB apply to first lane
  xstep | Step between each column for selection in the x and y buffers. Ystep is symmetric to xstep (ystep advances by -xstep).
  ystart | Starting position offset applied to all lanes for input from Y buffer.
  zbuff | Input buffer of 8 elements of type cint16
  zstart | Starting position offset applied to all lanes for input from Z buffer. This must be a compile time constant. Only the 4 LSB of the argument are used.
  zoffsets | 4b offset for each lane, applied to input from Z buffer. LSB apply to first lane
  zstep | Step between each column for selection in the zbuffer.

Note
  - For more information on how data selection works from the buffers go here. The data buffer and coefficient buffer in this intrinsic use the general scheme.
  - Parameter 'zstart' must be a compile time constant.

## ◆ mac8_maxdiff() [2/3]

v8cacc48 mac8_maxdiff | ( | v8cacc48 | acc,
|  | v32int16 | xbuff,
|  | int | xstart,
|  | unsigned int | xoffsets,
|  | int | xstep,
|  | v32int16 | ybuff,
|  | int | ystart,
|  | v8cint16 | zbuff,
|  | int | zstart,
|  | unsigned int | zoffsets,
|  | int | zstep )

Complex multiply-accumulate intrinsic function after computing the maximum difference between the selected lanes from the input buffer using small X input buffer.

acc0 += z00*((x00 - y00 > 0) ? (x00 - y00):0) + z01*((x01 - y01 > 0) ? (x01 - y01):0)
acc1 += z10*((x10 - y10 > 0) ? (x10 - y10):0) + z11*((x11 - y11 > 0) ? (x11 - y11):0)
acc2 += z20*((x20 - y20 > 0) ? (x20 - y20):0) + z21*((x21 - y21 > 0) ? (x21 - y21):0)
acc3 += z30*((x30 - y30 > 0) ? (x30 - y30):0) + z31*((x31 - y31 > 0) ? (x31 - y31):0)
acc4 += z40*((x40 - y40 > 0) ? (x40 - y40):0) + z41*((x41 - y41 > 0) ? (x41 - y41):0)
acc5 += z50*((x50 - y50 > 0) ? (x50 - y50):0) + z51*((x51 - y51 > 0) ? (x51 - y51):0)
acc6 += z60*((x60 - y60 > 0) ? (x60 - y60):0) + z61*((x61 - y61 > 0) ? (x61 - y61):0)
acc7 += z70*((x70 - y70 > 0) ? (x70 - y70):0) + z71*((x71 - y71 > 0) ? (x71 - y71):0)

Returns
  Returned accumulation vector (8 x cint48 lanes)

Parameters

  acc | Incoming accumulation vector (8 x cint48 lanes)
  xbuff | Input buffer of 32 elements of type int16
  xstart | Starting position offset applied to all lanes of input from X buffer.
  xoffsets | 4b offset for each lane, applied to both x and y buffers. LSB apply to first lane
  xstep | Step between each column for selection in the x and y buffers. Ystep is symmetric to xstep (ystep advances by -xstep).
  ybuff | Right input buffer of 32 elements of type int16
  ystart | Starting position offset applied to all lanes for input from Y buffer.
  zbuff | Input buffer of 8 elements of type cint16
  zstart | Starting position offset applied to all lanes for input from Z buffer. This must be a compile time constant. Only the 4 LSB of the argument are used.
  zoffsets | 4b offset for each lane, applied to input from Z buffer. LSB apply to first lane
  zstep | Step between each column for selection in the zbuffer.

Note
  - For more information on how data selection works from the buffers go here. The data buffer and coefficient buffer in this intrinsic use the general scheme.
  - Parameter 'zstart' must be a compile time constant.

## ◆ mac8_maxdiff() [3/3]

v8cacc48 mac8_maxdiff | ( | v8cacc48 | acc,
|  | v64int16 | xbuff,
|  | int | xstart,
|  | unsigned int | xoffsets,
|  | int | xstep,
|  | int | ystart,
|  | v8cint16 | zbuff,
|  | int | zstart,
|  | unsigned int | zoffsets,
|  | int | zstep )

Complex multiply-accumulate intrinsic function after computing the maximum difference between the selected lanes from the input buffer .

acc0 += z00*((x00 - y00 > 0) ? (x00 - y00):0) + z01*((x01 - y01 > 0) ? (x01 - y01):0)
acc1 += z10*((x10 - y10 > 0) ? (x10 - y10):0) + z11*((x11 - y11 > 0) ? (x11 - y11):0)
acc2 += z20*((x20 - y20 > 0) ? (x20 - y20):0) + z21*((x21 - y21 > 0) ? (x21 - y21):0)
acc3 += z30*((x30 - y30 > 0) ? (x30 - y30):0) + z31*((x31 - y31 > 0) ? (x31 - y31):0)
acc4 += z40*((x40 - y40 > 0) ? (x40 - y40):0) + z41*((x41 - y41 > 0) ? (x41 - y41):0)
acc5 += z50*((x50 - y50 > 0) ? (x50 - y50):0) + z51*((x51 - y51 > 0) ? (x51 - y51):0)
acc6 += z60*((x60 - y60 > 0) ? (x60 - y60):0) + z61*((x61 - y61 > 0) ? (x61 - y61):0)
acc7 += z70*((x70 - y70 > 0) ? (x70 - y70):0) + z71*((x71 - y71 > 0) ? (x71 - y71):0)

Returns
  Returned accumulation vector (8 x cint48 lanes)

Parameters

  acc | Incoming accumulation vector (8 x cint48 lanes)
  xbuff | Input buffer of 64 elements of type int16
  xstart | Starting position offset applied to all lanes of input from X buffer.
  xoffsets | 4b offset for each lane, applied to both x and y buffers. LSB apply to first lane
  xstep | Step between each column for selection in the x and y buffers. Ystep is symmetric to xstep (ystep advances by -xstep).
  ystart | Starting position offset applied to all lanes for input from Y buffer.
  zbuff | Input buffer of 8 elements of type cint16
  zstart | Starting position offset applied to all lanes for input from Z buffer. This must be a compile time constant. Only the 4 LSB of the argument are used.
  zoffsets | 4b offset for each lane, applied to input from Z buffer. LSB apply to first lane
  zstep | Step between each column for selection in the zbuffer.

Note
  - For more information on how data selection works from the buffers go here. The data buffer and coefficient buffer in this intrinsic use the general scheme.
  - Parameter 'zstart' must be a compile time constant.

## ◆ mac8_min() [1/3]

v8cacc48 mac8_min | ( | v8cacc48 | acc,
|  | v32int16 | xbuff,
|  | int | xstart,
|  | unsigned int | xoffsets,
|  | int | xstep,
|  | int | ystart,
|  | v8cint16 | zbuff,
|  | int | zstart,
|  | unsigned int | zoffsets,
|  | int | zstep )

Complex multiply-accumulate intrinsic function after computing the minimum between the selected lanes from the input buffer using small X input buffer.

acc0 += z00*(min(x00 , y00)) + z01*(min(x01 , y01))
acc1 += z10*(min(x10 , y10)) + z11*(min(x11 , y11))
acc2 += z20*(min(x20 , y20)) + z21*(min(x21 , y21))
acc3 += z30*(min(x30 , y30)) + z31*(min(x31 , y31))
acc4 += z40*(min(x40 , y40)) + z41*(min(x41 , y41))
acc5 += z50*(min(x50 , y50)) + z51*(min(x51 , y51))
acc6 += z60*(min(x60 , y60)) + z61*(min(x61 , y61))
acc7 += z70*(min(x70 , y70)) + z71*(min(x71 , y71))

Returns
  Returned accumulation vector (8 x cint48 lanes)

Parameters

  acc | Incoming accumulation vector (8 x cint48 lanes)
  xbuff | Input buffer of 32 elements of type int16
  xstart | Starting position offset applied to all lanes of input from X buffer.
  xoffsets | 4b offset for each lane, applied to both x and y buffers. LSB apply to first lane
  xstep | Step between each column for selection in the x and y buffers. Ystep is symmetric to xstep (ystep advances by -xstep).
  ystart | Starting position offset applied to all lanes for input from Y buffer.
  zbuff | Input buffer of 8 elements of type cint16
  zstart | Starting position offset applied to all lanes for input from Z buffer. This must be a compile time constant. Only the 4 LSB of the argument are used.
  zoffsets | 4b offset for each lane, applied to input from Z buffer. LSB apply to first lane
  zstep | Step between each column for selection in the zbuffer.

Note
  - For more information on how data selection works from the buffers go here. The data buffer and coefficient buffer in this intrinsic use the general scheme.
  - Parameter 'zstart' must be a compile time constant.

## ◆ mac8_min() [2/3]

v8cacc48 mac8_min | ( | v8cacc48 | acc,
|  | v32int16 | xbuff,
|  | int | xstart,
|  | unsigned int | xoffsets,
|  | int | xstep,
|  | v32int16 | ybuff,
|  | int | ystart,
|  | v8cint16 | zbuff,
|  | int | zstart,
|  | unsigned int | zoffsets,
|  | int | zstep )

Complex multiply-accumulate intrinsic function after computing the minimum between the selected lanes from the input buffer using small X input buffer.

acc0 += z00*(min(x00 , y00)) + z01*(min(x01 , y01))
acc1 += z10*(min(x10 , y10)) + z11*(min(x11 , y11))
acc2 += z20*(min(x20 , y20)) + z21*(min(x21 , y21))
acc3 += z30*(min(x30 , y30)) + z31*(min(x31 , y31))
acc4 += z40*(min(x40 , y40)) + z41*(min(x41 , y41))
acc5 += z50*(min(x50 , y50)) + z51*(min(x51 , y51))
acc6 += z60*(min(x60 , y60)) + z61*(min(x61 , y61))
acc7 += z70*(min(x70 , y70)) + z71*(min(x71 , y71))

Returns
  Returned accumulation vector (8 x cint48 lanes)

Parameters

  acc | Incoming accumulation vector (8 x cint48 lanes)
  xbuff | Input buffer of 32 elements of type int16
  xstart | Starting position offset applied to all lanes of input from X buffer.
  xoffsets | 4b offset for each lane, applied to both x and y buffers. LSB apply to first lane
  xstep | Step between each column for selection in the x and y buffers. Ystep is symmetric to xstep (ystep advances by -xstep).
  ybuff | Right input buffer of 32 elements of type int16
  ystart | Starting position offset applied to all lanes for input from Y buffer.
  zbuff | Input buffer of 8 elements of type cint16
  zstart | Starting position offset applied to all lanes for input from Z buffer. This must be a compile time constant. Only the 4 LSB of the argument are used.
  zoffsets | 4b offset for each lane, applied to input from Z buffer. LSB apply to first lane
  zstep | Step between each column for selection in the zbuffer.

Note
  - For more information on how data selection works from the buffers go here. The data buffer and coefficient buffer in this intrinsic use the general scheme.
  - Parameter 'zstart' must be a compile time constant.

## ◆ mac8_min() [3/3]

v8cacc48 mac8_min | ( | v8cacc48 | acc,
|  | v64int16 | xbuff,
|  | int | xstart,
|  | unsigned int | xoffsets,
|  | int | xstep,
|  | int | ystart,
|  | v8cint16 | zbuff,
|  | int | zstart,
|  | unsigned int | zoffsets,
|  | int | zstep )

Complex multiply-accumulate intrinsic function after computing the minimum between the selected lanes from the input buffer .

acc0 += z00*(min(x00 , y00)) + z01*(min(x01 , y01))
acc1 += z10*(min(x10 , y10)) + z11*(min(x11 , y11))
acc2 += z20*(min(x20 , y20)) + z21*(min(x21 , y21))
acc3 += z30*(min(x30 , y30)) + z31*(min(x31 , y31))
acc4 += z40*(min(x40 , y40)) + z41*(min(x41 , y41))
acc5 += z50*(min(x50 , y50)) + z51*(min(x51 , y51))
acc6 += z60*(min(x60 , y60)) + z61*(min(x61 , y61))
acc7 += z70*(min(x70 , y70)) + z71*(min(x71 , y71))

Returns
  Returned accumulation vector (8 x cint48 lanes)

Parameters

  acc | Incoming accumulation vector (8 x cint48 lanes)
  xbuff | Input buffer of 64 elements of type int16
  xstart | Starting position offset applied to all lanes of input from X buffer.
  xoffsets | 4b offset for each lane, applied to both x and y buffers. LSB apply to first lane
  xstep | Step between each column for selection in the x and y buffers. Ystep is symmetric to xstep (ystep advances by -xstep).
  ystart | Starting position offset applied to all lanes for input from Y buffer.
  zbuff | Input buffer of 8 elements of type cint16
  zstart | Starting position offset applied to all lanes for input from Z buffer. This must be a compile time constant. Only the 4 LSB of the argument are used.
  zoffsets | 4b offset for each lane, applied to input from Z buffer. LSB apply to first lane
  zstep | Step between each column for selection in the zbuffer.

Note
  - For more information on how data selection works from the buffers go here. The data buffer and coefficient buffer in this intrinsic use the general scheme.
  - Parameter 'zstart' must be a compile time constant.

## ◆ msc4_abs() [1/2]

v4cacc48 msc4_abs | ( | v4cacc48 | acc,
|  | v32int16 | xbuff,
|  | int | xstart,
|  | unsigned int | xoffsets,
|  | int | xstep,
|  | v8cint16 | zbuff,
|  | int | zstart,
|  | unsigned int | zoffsets,
|  | int | zstep )

Complex multiply-subtract intrinsic function after computing the absolute value in the selected lanes from the input buffer using small X input buffer.

acc0 -= z00*abs(x00) + z01*abs(x01) + z02*abs(x02) + z03*abs(x03)
acc1 -= z10*abs(x10) + z11*abs(x11) + z12*abs(x12) + z13*abs(x13)
acc2 -= z20*abs(x20) + z21*abs(x21) + z22*abs(x22) + z23*abs(x23)
acc3 -= z30*abs(x30) + z31*abs(x31) + z32*abs(x32) + z33*abs(x33)

Returns
  Returned accumulation vector (4 x cint48 lanes)

Parameters

  acc | Incoming accumulation vector (4 x cint48 lanes)
  xbuff | Input buffer of 32 elements of type int16
  xstart | Starting position offset applied to all lanes of input from X buffer.
  xoffsets | 4b offset for each lane, applied to the x buffer. LSB apply to first lane
  xstep | Step between each column for selection in the xbuffer.
  zbuff | Input buffer of 8 elements of type cint16
  zstart | Starting position offset applied to all lanes for input from Z buffer. This must be a compile time constant. Only the 4 LSB of the argument are used.
  zoffsets | 4b offset for each lane, applied to input from Z buffer. LSB apply to first lane
  zstep | Step between each column for selection in the zbuffer.

Note
  - For more information on how data selection works from the buffers go here. The data buffer and coefficient buffer in this intrinsic use the general scheme.
  - Parameter 'zstart' must be a compile time constant.

## ◆ msc4_abs() [2/2]

v4cacc48 msc4_abs | ( | v4cacc48 | acc,
|  | v64int16 | xbuff,
|  | int | xstart,
|  | unsigned int | xoffsets,
|  | int | xstep,
|  | v8cint16 | zbuff,
|  | int | zstart,
|  | unsigned int | zoffsets,
|  | int | zstep )

Complex multiply-subtract intrinsic function after computing the absolute value in the selected lanes from the input buffer .

acc0 -= z00*abs(x00) + z01*abs(x01) + z02*abs(x02) + z03*abs(x03)
acc1 -= z10*abs(x10) + z11*abs(x11) + z12*abs(x12) + z13*abs(x13)
acc2 -= z20*abs(x20) + z21*abs(x21) + z22*abs(x22) + z23*abs(x23)
acc3 -= z30*abs(x30) + z31*abs(x31) + z32*abs(x32) + z33*abs(x33)

Returns
  Returned accumulation vector (4 x cint48 lanes)

Parameters

  acc | Incoming accumulation vector (4 x cint48 lanes)
  xbuff | Input buffer of 64 elements of type int16
  xstart | Starting position offset applied to all lanes of input from X buffer.
  xoffsets | 4b offset for each lane, applied to the x buffer. LSB apply to first lane
  xstep | Step between each column for selection in the xbuffer.
  zbuff | Input buffer of 8 elements of type cint16
  zstart | Starting position offset applied to all lanes for input from Z buffer. This must be a compile time constant. Only the 4 LSB of the argument are used.
  zoffsets | 4b offset for each lane, applied to input from Z buffer. LSB apply to first lane
  zstep | Step between each column for selection in the zbuffer.

Note
  - For more information on how data selection works from the buffers go here. The data buffer and coefficient buffer in this intrinsic use the general scheme.
  - Parameter 'zstart' must be a compile time constant.

## ◆ msc4_max() [1/3]

v4cacc48 msc4_max | ( | v4cacc48 | acc,
|  | v32int16 | xbuff,
|  | int | xstart,
|  | unsigned int | xoffsets,
|  | int | xstep,
|  | int | ystart,
|  | v8cint16 | zbuff,
|  | int | zstart,
|  | unsigned int | zoffsets,
|  | int | zstep )

Complex multiply-subtract intrinsic function after computing the maximum between the selected lanes from the input buffer using small X input buffer.

acc0 -= z00*(max(x00 , y00)) + z01*(max(x01 , y01)) + z02*(max(x02 , y02)) + z03*(max(x03 , y03))
acc1 -= z10*(max(x10 , y10)) + z11*(max(x11 , y11)) + z12*(max(x12 , y12)) + z13*(max(x13 , y13))
acc2 -= z20*(max(x20 , y20)) + z21*(max(x21 , y21)) + z22*(max(x22 , y22)) + z23*(max(x23 , y23))
acc3 -= z30*(max(x30 , y30)) + z31*(max(x31 , y31)) + z32*(max(x32 , y32)) + z33*(max(x33 , y33))

Returns
  Returned accumulation vector (4 x cint48 lanes)

Parameters

  acc | Incoming accumulation vector (4 x cint48 lanes)
  xbuff | Input buffer of 32 elements of type int16
  xstart | Starting position offset applied to all lanes of input from X buffer.
  xoffsets | 4b offset for each lane, applied to both x and y buffers. LSB apply to first lane
  xstep | Step between each column for selection in the x and y buffers. Ystep is symmetric to xstep (ystep advances by -xstep).
  ystart | Starting position offset applied to all lanes for input from Y buffer.
  zbuff | Input buffer of 8 elements of type cint16
  zstart | Starting position offset applied to all lanes for input from Z buffer. This must be a compile time constant. Only the 4 LSB of the argument are used.
  zoffsets | 4b offset for each lane, applied to input from Z buffer. LSB apply to first lane
  zstep | Step between each column for selection in the zbuffer.

Note
  - For more information on how data selection works from the buffers go here. The data buffer and coefficient buffer in this intrinsic use the general scheme.
  - Parameter 'zstart' must be a compile time constant.

## ◆ msc4_max() [2/3]

v4cacc48 msc4_max | ( | v4cacc48 | acc,
|  | v32int16 | xbuff,
|  | int | xstart,
|  | unsigned int | xoffsets,
|  | int | xstep,
|  | v32int16 | ybuff,
|  | int | ystart,
|  | v8cint16 | zbuff,
|  | int | zstart,
|  | unsigned int | zoffsets,
|  | int | zstep )

Complex multiply-subtract intrinsic function after computing the maximum between the selected lanes from the input buffer using small X input buffer.

acc0 -= z00*(max(x00 , y00)) + z01*(max(x01 , y01)) + z02*(max(x02 , y02)) + z03*(max(x03 , y03))
acc1 -= z10*(max(x10 , y10)) + z11*(max(x11 , y11)) + z12*(max(x12 , y12)) + z13*(max(x13 , y13))
acc2 -= z20*(max(x20 , y20)) + z21*(max(x21 , y21)) + z22*(max(x22 , y22)) + z23*(max(x23 , y23))
acc3 -= z30*(max(x30 , y30)) + z31*(max(x31 , y31)) + z32*(max(x32 , y32)) + z33*(max(x33 , y33))

Returns
  Returned accumulation vector (4 x cint48 lanes)

Parameters

  acc | Incoming accumulation vector (4 x cint48 lanes)
  xbuff | Input buffer of 32 elements of type int16
  xstart | Starting position offset applied to all lanes of input from X buffer.
  xoffsets | 4b offset for each lane, applied to both x and y buffers. LSB apply to first lane
  xstep | Step between each column for selection in the x and y buffers. Ystep is symmetric to xstep (ystep advances by -xstep).
  ybuff | Right input buffer of 32 elements of type int16
  ystart | Starting position offset applied to all lanes for input from Y buffer.
  zbuff | Input buffer of 8 elements of type cint16
  zstart | Starting position offset applied to all lanes for input from Z buffer. This must be a compile time constant. Only the 4 LSB of the argument are used.
  zoffsets | 4b offset for each lane, applied to input from Z buffer. LSB apply to first lane
  zstep | Step between each column for selection in the zbuffer.

Note
  - For more information on how data selection works from the buffers go here. The data buffer and coefficient buffer in this intrinsic use the general scheme.
  - Parameter 'zstart' must be a compile time constant.

## ◆ msc4_max() [3/3]

v4cacc48 msc4_max | ( | v4cacc48 | acc,
|  | v64int16 | xbuff,
|  | int | xstart,
|  | unsigned int | xoffsets,
|  | int | xstep,
|  | int | ystart,
|  | v8cint16 | zbuff,
|  | int | zstart,
|  | unsigned int | zoffsets,
|  | int | zstep )

Complex multiply-subtract intrinsic function after computing the maximum between the selected lanes from the input buffer .

acc0 -= z00*(max(x00 , y00)) + z01*(max(x01 , y01)) + z02*(max(x02 , y02)) + z03*(max(x03 , y03))
acc1 -= z10*(max(x10 , y10)) + z11*(max(x11 , y11)) + z12*(max(x12 , y12)) + z13*(max(x13 , y13))
acc2 -= z20*(max(x20 , y20)) + z21*(max(x21 , y21)) + z22*(max(x22 , y22)) + z23*(max(x23 , y23))
acc3 -= z30*(max(x30 , y30)) + z31*(max(x31 , y31)) + z32*(max(x32 , y32)) + z33*(max(x33 , y33))

Returns
  Returned accumulation vector (4 x cint48 lanes)

Parameters

  acc | Incoming accumulation vector (4 x cint48 lanes)
  xbuff | Input buffer of 64 elements of type int16
  xstart | Starting position offset applied to all lanes of input from X buffer.
  xoffsets | 4b offset for each lane, applied to both x and y buffers. LSB apply to first lane
  xstep | Step between each column for selection in the x and y buffers. Ystep is symmetric to xstep (ystep advances by -xstep).
  ystart | Starting position offset applied to all lanes for input from Y buffer.
  zbuff | Input buffer of 8 elements of type cint16
  zstart | Starting position offset applied to all lanes for input from Z buffer. This must be a compile time constant. Only the 4 LSB of the argument are used.
  zoffsets | 4b offset for each lane, applied to input from Z buffer. LSB apply to first lane
  zstep | Step between each column for selection in the zbuffer.

Note
  - For more information on how data selection works from the buffers go here. The data buffer and coefficient buffer in this intrinsic use the general scheme.
  - Parameter 'zstart' must be a compile time constant.

## ◆ msc4_maxdiff() [1/3]

v4cacc48 msc4_maxdiff | ( | v4cacc48 | acc,
|  | v32int16 | xbuff,
|  | int | xstart,
|  | unsigned int | xoffsets,
|  | int | xstep,
|  | int | ystart,
|  | v8cint16 | zbuff,
|  | int | zstart,
|  | unsigned int | zoffsets,
|  | int | zstep )

Complex multiply-subtract intrinsic function after computing the maximum difference between the selected lanes from the input buffer using small X input buffer.

acc0 -= z00*((x00 - y00 > 0) ? (x00 - y00):0) + z01*((x01 - y01 > 0) ? (x01 - y01):0) + z02*((x02 - y02 > 0) ? (x02 - y02):0) + z03*((x03 - y03 > 0) ? (x03 - y03):0)
acc1 -= z10*((x10 - y10 > 0) ? (x10 - y10):0) + z11*((x11 - y11 > 0) ? (x11 - y11):0) + z12*((x12 - y12 > 0) ? (x12 - y12):0) + z13*((x13 - y13 > 0) ? (x13 - y13):0)
acc2 -= z20*((x20 - y20 > 0) ? (x20 - y20):0) + z21*((x21 - y21 > 0) ? (x21 - y21):0) + z22*((x22 - y22 > 0) ? (x22 - y22):0) + z23*((x23 - y23 > 0) ? (x23 - y23):0)
acc3 -= z30*((x30 - y30 > 0) ? (x30 - y30):0) + z31*((x31 - y31 > 0) ? (x31 - y31):0) + z32*((x32 - y32 > 0) ? (x32 - y32):0) + z33*((x33 - y33 > 0) ? (x33 - y33):0)

Returns
  Returned accumulation vector (4 x cint48 lanes)

Parameters

  acc | Incoming accumulation vector (4 x cint48 lanes)
  xbuff | Input buffer of 32 elements of type int16
  xstart | Starting position offset applied to all lanes of input from X buffer.
  xoffsets | 4b offset for each lane, applied to both x and y buffers. LSB apply to first lane
  xstep | Step between each column for selection in the x and y buffers. Ystep is symmetric to xstep (ystep advances by -xstep).
  ystart | Starting position offset applied to all lanes for input from Y buffer.
  zbuff | Input buffer of 8 elements of type cint16
  zstart | Starting position offset applied to all lanes for input from Z buffer. This must be a compile time constant. Only the 4 LSB of the argument are used.
  zoffsets | 4b offset for each lane, applied to input from Z buffer. LSB apply to first lane
  zstep | Step between each column for selection in the zbuffer.

Note
  - For more information on how data selection works from the buffers go here. The data buffer and coefficient buffer in this intrinsic use the general scheme.
  - Parameter 'zstart' must be a compile time constant.

## ◆ msc4_maxdiff() [2/3]

v4cacc48 msc4_maxdiff | ( | v4cacc48 | acc,
|  | v32int16 | xbuff,
|  | int | xstart,
|  | unsigned int | xoffsets,
|  | int | xstep,
|  | v32int16 | ybuff,
|  | int | ystart,
|  | v8cint16 | zbuff,
|  | int | zstart,
|  | unsigned int | zoffsets,
|  | int | zstep )

Complex multiply-subtract intrinsic function after computing the maximum difference between the selected lanes from the input buffer using small X input buffer.

acc0 -= z00*((x00 - y00 > 0) ? (x00 - y00):0) + z01*((x01 - y01 > 0) ? (x01 - y01):0) + z02*((x02 - y02 > 0) ? (x02 - y02):0) + z03*((x03 - y03 > 0) ? (x03 - y03):0)
acc1 -= z10*((x10 - y10 > 0) ? (x10 - y10):0) + z11*((x11 - y11 > 0) ? (x11 - y11):0) + z12*((x12 - y12 > 0) ? (x12 - y12):0) + z13*((x13 - y13 > 0) ? (x13 - y13):0)
acc2 -= z20*((x20 - y20 > 0) ? (x20 - y20):0) + z21*((x21 - y21 > 0) ? (x21 - y21):0) + z22*((x22 - y22 > 0) ? (x22 - y22):0) + z23*((x23 - y23 > 0) ? (x23 - y23):0)
acc3 -= z30*((x30 - y30 > 0) ? (x30 - y30):0) + z31*((x31 - y31 > 0) ? (x31 - y31):0) + z32*((x32 - y32 > 0) ? (x32 - y32):0) + z33*((x33 - y33 > 0) ? (x33 - y33):0)

Returns
  Returned accumulation vector (4 x cint48 lanes)

Parameters

  acc | Incoming accumulation vector (4 x cint48 lanes)
  xbuff | Input buffer of 32 elements of type int16
  xstart | Starting position offset applied to all lanes of input from X buffer.
  xoffsets | 4b offset for each lane, applied to both x and y buffers. LSB apply to first lane
  xstep | Step between each column for selection in the x and y buffers. Ystep is symmetric to xstep (ystep advances by -xstep).
  ybuff | Right input buffer of 32 elements of type int16
  ystart | Starting position offset applied to all lanes for input from Y buffer.
  zbuff | Input buffer of 8 elements of type cint16
  zstart | Starting position offset applied to all lanes for input from Z buffer. This must be a compile time constant. Only the 4 LSB of the argument are used.
  zoffsets | 4b offset for each lane, applied to input from Z buffer. LSB apply to first lane
  zstep | Step between each column for selection in the zbuffer.

Note
  - For more information on how data selection works from the buffers go here. The data buffer and coefficient buffer in this intrinsic use the general scheme.
  - Parameter 'zstart' must be a compile time constant.

## ◆ msc4_maxdiff() [3/3]

v4cacc48 msc4_maxdiff | ( | v4cacc48 | acc,
|  | v64int16 | xbuff,
|  | int | xstart,
|  | unsigned int | xoffsets,
|  | int | xstep,
|  | int | ystart,
|  | v8cint16 | zbuff,
|  | int | zstart,
|  | unsigned int | zoffsets,
|  | int | zstep )

Complex multiply-subtract intrinsic function after computing the maximum difference between the selected lanes from the input buffer .

acc0 -= z00*((x00 - y00 > 0) ? (x00 - y00):0) + z01*((x01 - y01 > 0) ? (x01 - y01):0) + z02*((x02 - y02 > 0) ? (x02 - y02):0) + z03*((x03 - y03 > 0) ? (x03 - y03):0)
acc1 -= z10*((x10 - y10 > 0) ? (x10 - y10):0) + z11*((x11 - y11 > 0) ? (x11 - y11):0) + z12*((x12 - y12 > 0) ? (x12 - y12):0) + z13*((x13 - y13 > 0) ? (x13 - y13):0)
acc2 -= z20*((x20 - y20 > 0) ? (x20 - y20):0) + z21*((x21 - y21 > 0) ? (x21 - y21):0) + z22*((x22 - y22 > 0) ? (x22 - y22):0) + z23*((x23 - y23 > 0) ? (x23 - y23):0)
acc3 -= z30*((x30 - y30 > 0) ? (x30 - y30):0) + z31*((x31 - y31 > 0) ? (x31 - y31):0) + z32*((x32 - y32 > 0) ? (x32 - y32):0) + z33*((x33 - y33 > 0) ? (x33 - y33):0)

Returns
  Returned accumulation vector (4 x cint48 lanes)

Parameters

  acc | Incoming accumulation vector (4 x cint48 lanes)
  xbuff | Input buffer of 64 elements of type int16
  xstart | Starting position offset applied to all lanes of input from X buffer.
  xoffsets | 4b offset for each lane, applied to both x and y buffers. LSB apply to first lane
  xstep | Step between each column for selection in the x and y buffers. Ystep is symmetric to xstep (ystep advances by -xstep).
  ystart | Starting position offset applied to all lanes for input from Y buffer.
  zbuff | Input buffer of 8 elements of type cint16
  zstart | Starting position offset applied to all lanes for input from Z buffer. This must be a compile time constant. Only the 4 LSB of the argument are used.
  zoffsets | 4b offset for each lane, applied to input from Z buffer. LSB apply to first lane
  zstep | Step between each column for selection in the zbuffer.

Note
  - For more information on how data selection works from the buffers go here. The data buffer and coefficient buffer in this intrinsic use the general scheme.
  - Parameter 'zstart' must be a compile time constant.

## ◆ msc4_min() [1/3]

v4cacc48 msc4_min | ( | v4cacc48 | acc,
|  | v32int16 | xbuff,
|  | int | xstart,
|  | unsigned int | xoffsets,
|  | int | xstep,
|  | int | ystart,
|  | v8cint16 | zbuff,
|  | int | zstart,
|  | unsigned int | zoffsets,
|  | int | zstep )

Complex multiply-subtract intrinsic function after computing the minimum between the selected lanes from the input buffer using small X input buffer.

acc0 -= z00*(min(x00 , y00)) + z01*(min(x01 , y01)) + z02*(min(x02 , y02)) + z03*(min(x03 , y03))
acc1 -= z10*(min(x10 , y10)) + z11*(min(x11 , y11)) + z12*(min(x12 , y12)) + z13*(min(x13 , y13))
acc2 -= z20*(min(x20 , y20)) + z21*(min(x21 , y21)) + z22*(min(x22 , y22)) + z23*(min(x23 , y23))
acc3 -= z30*(min(x30 , y30)) + z31*(min(x31 , y31)) + z32*(min(x32 , y32)) + z33*(min(x33 , y33))

Returns
  Returned accumulation vector (4 x cint48 lanes)

Parameters

  acc | Incoming accumulation vector (4 x cint48 lanes)
  xbuff | Input buffer of 32 elements of type int16
  xstart | Starting position offset applied to all lanes of input from X buffer.
  xoffsets | 4b offset for each lane, applied to both x and y buffers. LSB apply to first lane
  xstep | Step between each column for selection in the x and y buffers. Ystep is symmetric to xstep (ystep advances by -xstep).
  ystart | Starting position offset applied to all lanes for input from Y buffer.
  zbuff | Input buffer of 8 elements of type cint16
  zstart | Starting position offset applied to all lanes for input from Z buffer. This must be a compile time constant. Only the 4 LSB of the argument are used.
  zoffsets | 4b offset for each lane, applied to input from Z buffer. LSB apply to first lane
  zstep | Step between each column for selection in the zbuffer.

Note
  - For more information on how data selection works from the buffers go here. The data buffer and coefficient buffer in this intrinsic use the general scheme.
  - Parameter 'zstart' must be a compile time constant.

## ◆ msc4_min() [2/3]

v4cacc48 msc4_min | ( | v4cacc48 | acc,
|  | v32int16 | xbuff,
|  | int | xstart,
|  | unsigned int | xoffsets,
|  | int | xstep,
|  | v32int16 | ybuff,
|  | int | ystart,
|  | v8cint16 | zbuff,
|  | int | zstart,
|  | unsigned int | zoffsets,
|  | int | zstep )

Complex multiply-subtract intrinsic function after computing the minimum between the selected lanes from the input buffer using small X input buffer.

acc0 -= z00*(min(x00 , y00)) + z01*(min(x01 , y01)) + z02*(min(x02 , y02)) + z03*(min(x03 , y03))
acc1 -= z10*(min(x10 , y10)) + z11*(min(x11 , y11)) + z12*(min(x12 , y12)) + z13*(min(x13 , y13))
acc2 -= z20*(min(x20 , y20)) + z21*(min(x21 , y21)) + z22*(min(x22 , y22)) + z23*(min(x23 , y23))
acc3 -= z30*(min(x30 , y30)) + z31*(min(x31 , y31)) + z32*(min(x32 , y32)) + z33*(min(x33 , y33))

Returns
  Returned accumulation vector (4 x cint48 lanes)

Parameters

  acc | Incoming accumulation vector (4 x cint48 lanes)
  xbuff | Input buffer of 32 elements of type int16
  xstart | Starting position offset applied to all lanes of input from X buffer.
  xoffsets | 4b offset for each lane, applied to both x and y buffers. LSB apply to first lane
  xstep | Step between each column for selection in the x and y buffers. Ystep is symmetric to xstep (ystep advances by -xstep).
  ybuff | Right input buffer of 32 elements of type int16
  ystart | Starting position offset applied to all lanes for input from Y buffer.
  zbuff | Input buffer of 8 elements of type cint16
  zstart | Starting position offset applied to all lanes for input from Z buffer. This must be a compile time constant. Only the 4 LSB of the argument are used.
  zoffsets | 4b offset for each lane, applied to input from Z buffer. LSB apply to first lane
  zstep | Step between each column for selection in the zbuffer.

Note
  - For more information on how data selection works from the buffers go here. The data buffer and coefficient buffer in this intrinsic use the general scheme.
  - Parameter 'zstart' must be a compile time constant.

## ◆ msc4_min() [3/3]

v4cacc48 msc4_min | ( | v4cacc48 | acc,
|  | v64int16 | xbuff,
|  | int | xstart,
|  | unsigned int | xoffsets,
|  | int | xstep,
|  | int | ystart,
|  | v8cint16 | zbuff,
|  | int | zstart,
|  | unsigned int | zoffsets,
|  | int | zstep )

Complex multiply-subtract intrinsic function after computing the minimum between the selected lanes from the input buffer .

acc0 -= z00*(min(x00 , y00)) + z01*(min(x01 , y01)) + z02*(min(x02 , y02)) + z03*(min(x03 , y03))
acc1 -= z10*(min(x10 , y10)) + z11*(min(x11 , y11)) + z12*(min(x12 , y12)) + z13*(min(x13 , y13))
acc2 -= z20*(min(x20 , y20)) + z21*(min(x21 , y21)) + z22*(min(x22 , y22)) + z23*(min(x23 , y23))
acc3 -= z30*(min(x30 , y30)) + z31*(min(x31 , y31)) + z32*(min(x32 , y32)) + z33*(min(x33 , y33))

Returns
  Returned accumulation vector (4 x cint48 lanes)

Parameters

  acc | Incoming accumulation vector (4 x cint48 lanes)
  xbuff | Input buffer of 64 elements of type int16
  xstart | Starting position offset applied to all lanes of input from X buffer.
  xoffsets | 4b offset for each lane, applied to both x and y buffers. LSB apply to first lane
  xstep | Step between each column for selection in the x and y buffers. Ystep is symmetric to xstep (ystep advances by -xstep).
  ystart | Starting position offset applied to all lanes for input from Y buffer.
  zbuff | Input buffer of 8 elements of type cint16
  zstart | Starting position offset applied to all lanes for input from Z buffer. This must be a compile time constant. Only the 4 LSB of the argument are used.
  zoffsets | 4b offset for each lane, applied to input from Z buffer. LSB apply to first lane
  zstep | Step between each column for selection in the zbuffer.

Note
  - For more information on how data selection works from the buffers go here. The data buffer and coefficient buffer in this intrinsic use the general scheme.
  - Parameter 'zstart' must be a compile time constant.

## ◆ msc8_abs() [1/2]

v8cacc48 msc8_abs | ( | v8cacc48 | acc,
|  | v32int16 | xbuff,
|  | int | xstart,
|  | unsigned int | xoffsets,
|  | int | xstep,
|  | v8cint16 | zbuff,
|  | int | zstart,
|  | unsigned int | zoffsets,
|  | int | zstep )

Complex multiply-subtract intrinsic function after computing the absolute value in the selected lanes from the input buffer using small X input buffer.

acc0 -= z00*abs(x00) + z01*abs(x01)
acc1 -= z10*abs(x10) + z11*abs(x11)
acc2 -= z20*abs(x20) + z21*abs(x21)
acc3 -= z30*abs(x30) + z31*abs(x31)
acc4 -= z40*abs(x40) + z41*abs(x41)
acc5 -= z50*abs(x50) + z51*abs(x51)
acc6 -= z60*abs(x60) + z61*abs(x61)
acc7 -= z70*abs(x70) + z71*abs(x71)

Returns
  Returned accumulation vector (8 x cint48 lanes)

Parameters

  acc | Incoming accumulation vector (8 x cint48 lanes)
  xbuff | Input buffer of 32 elements of type int16
  xstart | Starting position offset applied to all lanes of input from X buffer.
  xoffsets | 4b offset for each lane, applied to the x buffer. LSB apply to first lane
  xstep | Step between each column for selection in the xbuffer.
  zbuff | Input buffer of 8 elements of type cint16
  zstart | Starting position offset applied to all lanes for input from Z buffer. This must be a compile time constant. Only the 4 LSB of the argument are used.
  zoffsets | 4b offset for each lane, applied to input from Z buffer. LSB apply to first lane
  zstep | Step between each column for selection in the zbuffer.

Note
  - For more information on how data selection works from the buffers go here. The data buffer and coefficient buffer in this intrinsic use the general scheme.
  - Parameter 'zstart' must be a compile time constant.

## ◆ msc8_abs() [2/2]

v8cacc48 msc8_abs | ( | v8cacc48 | acc,
|  | v64int16 | xbuff,
|  | int | xstart,
|  | unsigned int | xoffsets,
|  | int | xstep,
|  | v8cint16 | zbuff,
|  | int | zstart,
|  | unsigned int | zoffsets,
|  | int | zstep )

Complex multiply-subtract intrinsic function after computing the absolute value in the selected lanes from the input buffer .

acc0 -= z00*abs(x00) + z01*abs(x01)
acc1 -= z10*abs(x10) + z11*abs(x11)
acc2 -= z20*abs(x20) + z21*abs(x21)
acc3 -= z30*abs(x30) + z31*abs(x31)
acc4 -= z40*abs(x40) + z41*abs(x41)
acc5 -= z50*abs(x50) + z51*abs(x51)
acc6 -= z60*abs(x60) + z61*abs(x61)
acc7 -= z70*abs(x70) + z71*abs(x71)

Returns
  Returned accumulation vector (8 x cint48 lanes)

Parameters

  acc | Incoming accumulation vector (8 x cint48 lanes)
  xbuff | Input buffer of 64 elements of type int16
  xstart | Starting position offset applied to all lanes of input from X buffer.
  xoffsets | 4b offset for each lane, applied to the x buffer. LSB apply to first lane
  xstep | Step between each column for selection in the xbuffer.
  zbuff | Input buffer of 8 elements of type cint16
  zstart | Starting position offset applied to all lanes for input from Z buffer. This must be a compile time constant. Only the 4 LSB of the argument are used.
  zoffsets | 4b offset for each lane, applied to input from Z buffer. LSB apply to first lane
  zstep | Step between each column for selection in the zbuffer.

Note
  - For more information on how data selection works from the buffers go here. The data buffer and coefficient buffer in this intrinsic use the general scheme.
  - Parameter 'zstart' must be a compile time constant.

## ◆ msc8_max() [1/3]

v8cacc48 msc8_max | ( | v8cacc48 | acc,
|  | v32int16 | xbuff,
|  | int | xstart,
|  | unsigned int | xoffsets,
|  | int | xstep,
|  | int | ystart,
|  | v8cint16 | zbuff,
|  | int | zstart,
|  | unsigned int | zoffsets,
|  | int | zstep )

Complex multiply-subtract intrinsic function after computing the maximum between the selected lanes from the input buffer using small X input buffer.

acc0 -= z00*(max(x00 , y00)) + z01*(max(x01 , y01))
acc1 -= z10*(max(x10 , y10)) + z11*(max(x11 , y11))
acc2 -= z20*(max(x20 , y20)) + z21*(max(x21 , y21))
acc3 -= z30*(max(x30 , y30)) + z31*(max(x31 , y31))
acc4 -= z40*(max(x40 , y40)) + z41*(max(x41 , y41))
acc5 -= z50*(max(x50 , y50)) + z51*(max(x51 , y51))
acc6 -= z60*(max(x60 , y60)) + z61*(max(x61 , y61))
acc7 -= z70*(max(x70 , y70)) + z71*(max(x71 , y71))

Returns
  Returned accumulation vector (8 x cint48 lanes)

Parameters

  acc | Incoming accumulation vector (8 x cint48 lanes)
  xbuff | Input buffer of 32 elements of type int16
  xstart | Starting position offset applied to all lanes of input from X buffer.
  xoffsets | 4b offset for each lane, applied to both x and y buffers. LSB apply to first lane
  xstep | Step between each column for selection in the x and y buffers. Ystep is symmetric to xstep (ystep advances by -xstep).
  ystart | Starting position offset applied to all lanes for input from Y buffer.
  zbuff | Input buffer of 8 elements of type cint16
  zstart | Starting position offset applied to all lanes for input from Z buffer. This must be a compile time constant. Only the 4 LSB of the argument are used.
  zoffsets | 4b offset for each lane, applied to input from Z buffer. LSB apply to first lane
  zstep | Step between each column for selection in the zbuffer.

Note
  - For more information on how data selection works from the buffers go here. The data buffer and coefficient buffer in this intrinsic use the general scheme.
  - Parameter 'zstart' must be a compile time constant.

## ◆ msc8_max() [2/3]

v8cacc48 msc8_max | ( | v8cacc48 | acc,
|  | v32int16 | xbuff,
|  | int | xstart,
|  | unsigned int | xoffsets,
|  | int | xstep,
|  | v32int16 | ybuff,
|  | int | ystart,
|  | v8cint16 | zbuff,
|  | int | zstart,
|  | unsigned int | zoffsets,
|  | int | zstep )

Complex multiply-subtract intrinsic function after computing the maximum between the selected lanes from the input buffer using small X input buffer.

acc0 -= z00*(max(x00 , y00)) + z01*(max(x01 , y01))
acc1 -= z10*(max(x10 , y10)) + z11*(max(x11 , y11))
acc2 -= z20*(max(x20 , y20)) + z21*(max(x21 , y21))
acc3 -= z30*(max(x30 , y30)) + z31*(max(x31 , y31))
acc4 -= z40*(max(x40 , y40)) + z41*(max(x41 , y41))
acc5 -= z50*(max(x50 , y50)) + z51*(max(x51 , y51))
acc6 -= z60*(max(x60 , y60)) + z61*(max(x61 , y61))
acc7 -= z70*(max(x70 , y70)) + z71*(max(x71 , y71))

Returns
  Returned accumulation vector (8 x cint48 lanes)

Parameters

  acc | Incoming accumulation vector (8 x cint48 lanes)
  xbuff | Input buffer of 32 elements of type int16
  xstart | Starting position offset applied to all lanes of input from X buffer.
  xoffsets | 4b offset for each lane, applied to both x and y buffers. LSB apply to first lane
  xstep | Step between each column for selection in the x and y buffers. Ystep is symmetric to xstep (ystep advances by -xstep).
  ybuff | Right input buffer of 32 elements of type int16
  ystart | Starting position offset applied to all lanes for input from Y buffer.
  zbuff | Input buffer of 8 elements of type cint16
  zstart | Starting position offset applied to all lanes for input from Z buffer. This must be a compile time constant. Only the 4 LSB of the argument are used.
  zoffsets | 4b offset for each lane, applied to input from Z buffer. LSB apply to first lane
  zstep | Step between each column for selection in the zbuffer.

Note
  - For more information on how data selection works from the buffers go here. The data buffer and coefficient buffer in this intrinsic use the general scheme.
  - Parameter 'zstart' must be a compile time constant.

## ◆ msc8_max() [3/3]

v8cacc48 msc8_max | ( | v8cacc48 | acc,
|  | v64int16 | xbuff,
|  | int | xstart,
|  | unsigned int | xoffsets,
|  | int | xstep,
|  | int | ystart,
|  | v8cint16 | zbuff,
|  | int | zstart,
|  | unsigned int | zoffsets,
|  | int | zstep )

Complex multiply-subtract intrinsic function after computing the maximum between the selected lanes from the input buffer .

acc0 -= z00*(max(x00 , y00)) + z01*(max(x01 , y01))
acc1 -= z10*(max(x10 , y10)) + z11*(max(x11 , y11))
acc2 -= z20*(max(x20 , y20)) + z21*(max(x21 , y21))
acc3 -= z30*(max(x30 , y30)) + z31*(max(x31 , y31))
acc4 -= z40*(max(x40 , y40)) + z41*(max(x41 , y41))
acc5 -= z50*(max(x50 , y50)) + z51*(max(x51 , y51))
acc6 -= z60*(max(x60 , y60)) + z61*(max(x61 , y61))
acc7 -= z70*(max(x70 , y70)) + z71*(max(x71 , y71))

Returns
  Returned accumulation vector (8 x cint48 lanes)

Parameters

  acc | Incoming accumulation vector (8 x cint48 lanes)
  xbuff | Input buffer of 64 elements of type int16
  xstart | Starting position offset applied to all lanes of input from X buffer.
  xoffsets | 4b offset for each lane, applied to both x and y buffers. LSB apply to first lane
  xstep | Step between each column for selection in the x and y buffers. Ystep is symmetric to xstep (ystep advances by -xstep).
  ystart | Starting position offset applied to all lanes for input from Y buffer.
  zbuff | Input buffer of 8 elements of type cint16
  zstart | Starting position offset applied to all lanes for input from Z buffer. This must be a compile time constant. Only the 4 LSB of the argument are used.
  zoffsets | 4b offset for each lane, applied to input from Z buffer. LSB apply to first lane
  zstep | Step between each column for selection in the zbuffer.

Note
  - For more information on how data selection works from the buffers go here. The data buffer and coefficient buffer in this intrinsic use the general scheme.
  - Parameter 'zstart' must be a compile time constant.

## ◆ msc8_maxdiff() [1/3]

v8cacc48 msc8_maxdiff | ( | v8cacc48 | acc,
|  | v32int16 | xbuff,
|  | int | xstart,
|  | unsigned int | xoffsets,
|  | int | xstep,
|  | int | ystart,
|  | v8cint16 | zbuff,
|  | int | zstart,
|  | unsigned int | zoffsets,
|  | int | zstep )

Complex multiply-subtract intrinsic function after computing the maximum difference between the selected lanes from the input buffer using small X input buffer.

acc0 -= z00*((x00 - y00 > 0) ? (x00 - y00):0) + z01*((x01 - y01 > 0) ? (x01 - y01):0)
acc1 -= z10*((x10 - y10 > 0) ? (x10 - y10):0) + z11*((x11 - y11 > 0) ? (x11 - y11):0)
acc2 -= z20*((x20 - y20 > 0) ? (x20 - y20):0) + z21*((x21 - y21 > 0) ? (x21 - y21):0)
acc3 -= z30*((x30 - y30 > 0) ? (x30 - y30):0) + z31*((x31 - y31 > 0) ? (x31 - y31):0)
acc4 -= z40*((x40 - y40 > 0) ? (x40 - y40):0) + z41*((x41 - y41 > 0) ? (x41 - y41):0)
acc5 -= z50*((x50 - y50 > 0) ? (x50 - y50):0) + z51*((x51 - y51 > 0) ? (x51 - y51):0)
acc6 -= z60*((x60 - y60 > 0) ? (x60 - y60):0) + z61*((x61 - y61 > 0) ? (x61 - y61):0)
acc7 -= z70*((x70 - y70 > 0) ? (x70 - y70):0) + z71*((x71 - y71 > 0) ? (x71 - y71):0)

Returns
  Returned accumulation vector (8 x cint48 lanes)

Parameters

  acc | Incoming accumulation vector (8 x cint48 lanes)
  xbuff | Input buffer of 32 elements of type int16
  xstart | Starting position offset applied to all lanes of input from X buffer.
  xoffsets | 4b offset for each lane, applied to both x and y buffers. LSB apply to first lane
  xstep | Step between each column for selection in the x and y buffers. Ystep is symmetric to xstep (ystep advances by -xstep).
  ystart | Starting position offset applied to all lanes for input from Y buffer.
  zbuff | Input buffer of 8 elements of type cint16
  zstart | Starting position offset applied to all lanes for input from Z buffer. This must be a compile time constant. Only the 4 LSB of the argument are used.
  zoffsets | 4b offset for each lane, applied to input from Z buffer. LSB apply to first lane
  zstep | Step between each column for selection in the zbuffer.

Note
  - For more information on how data selection works from the buffers go here. The data buffer and coefficient buffer in this intrinsic use the general scheme.
  - Parameter 'zstart' must be a compile time constant.

## ◆ msc8_maxdiff() [2/3]

v8cacc48 msc8_maxdiff | ( | v8cacc48 | acc,
|  | v32int16 | xbuff,
|  | int | xstart,
|  | unsigned int | xoffsets,
|  | int | xstep,
|  | v32int16 | ybuff,
|  | int | ystart,
|  | v8cint16 | zbuff,
|  | int | zstart,
|  | unsigned int | zoffsets,
|  | int | zstep )

Complex multiply-subtract intrinsic function after computing the maximum difference between the selected lanes from the input buffer using small X input buffer.

acc0 -= z00*((x00 - y00 > 0) ? (x00 - y00):0) + z01*((x01 - y01 > 0) ? (x01 - y01):0)
acc1 -= z10*((x10 - y10 > 0) ? (x10 - y10):0) + z11*((x11 - y11 > 0) ? (x11 - y11):0)
acc2 -= z20*((x20 - y20 > 0) ? (x20 - y20):0) + z21*((x21 - y21 > 0) ? (x21 - y21):0)
acc3 -= z30*((x30 - y30 > 0) ? (x30 - y30):0) + z31*((x31 - y31 > 0) ? (x31 - y31):0)
acc4 -= z40*((x40 - y40 > 0) ? (x40 - y40):0) + z41*((x41 - y41 > 0) ? (x41 - y41):0)
acc5 -= z50*((x50 - y50 > 0) ? (x50 - y50):0) + z51*((x51 - y51 > 0) ? (x51 - y51):0)
acc6 -= z60*((x60 - y60 > 0) ? (x60 - y60):0) + z61*((x61 - y61 > 0) ? (x61 - y61):0)
acc7 -= z70*((x70 - y70 > 0) ? (x70 - y70):0) + z71*((x71 - y71 > 0) ? (x71 - y71):0)

Returns
  Returned accumulation vector (8 x cint48 lanes)

Parameters

  acc | Incoming accumulation vector (8 x cint48 lanes)
  xbuff | Input buffer of 32 elements of type int16
  xstart | Starting position offset applied to all lanes of input from X buffer.
  xoffsets | 4b offset for each lane, applied to both x and y buffers. LSB apply to first lane
  xstep | Step between each column for selection in the x and y buffers. Ystep is symmetric to xstep (ystep advances by -xstep).
  ybuff | Right input buffer of 32 elements of type int16
  ystart | Starting position offset applied to all lanes for input from Y buffer.
  zbuff | Input buffer of 8 elements of type cint16
  zstart | Starting position offset applied to all lanes for input from Z buffer. This must be a compile time constant. Only the 4 LSB of the argument are used.
  zoffsets | 4b offset for each lane, applied to input from Z buffer. LSB apply to first lane
  zstep | Step between each column for selection in the zbuffer.

Note
  - For more information on how data selection works from the buffers go here. The data buffer and coefficient buffer in this intrinsic use the general scheme.
  - Parameter 'zstart' must be a compile time constant.

## ◆ msc8_maxdiff() [3/3]

v8cacc48 msc8_maxdiff | ( | v8cacc48 | acc,
|  | v64int16 | xbuff,
|  | int | xstart,
|  | unsigned int | xoffsets,
|  | int | xstep,
|  | int | ystart,
|  | v8cint16 | zbuff,
|  | int | zstart,
|  | unsigned int | zoffsets,
|  | int | zstep )

Complex multiply-subtract intrinsic function after computing the maximum difference between the selected lanes from the input buffer .

acc0 -= z00*((x00 - y00 > 0) ? (x00 - y00):0) + z01*((x01 - y01 > 0) ? (x01 - y01):0)
acc1 -= z10*((x10 - y10 > 0) ? (x10 - y10):0) + z11*((x11 - y11 > 0) ? (x11 - y11):0)
acc2 -= z20*((x20 - y20 > 0) ? (x20 - y20):0) + z21*((x21 - y21 > 0) ? (x21 - y21):0)
acc3 -= z30*((x30 - y30 > 0) ? (x30 - y30):0) + z31*((x31 - y31 > 0) ? (x31 - y31):0)
acc4 -= z40*((x40 - y40 > 0) ? (x40 - y40):0) + z41*((x41 - y41 > 0) ? (x41 - y41):0)
acc5 -= z50*((x50 - y50 > 0) ? (x50 - y50):0) + z51*((x51 - y51 > 0) ? (x51 - y51):0)
acc6 -= z60*((x60 - y60 > 0) ? (x60 - y60):0) + z61*((x61 - y61 > 0) ? (x61 - y61):0)
acc7 -= z70*((x70 - y70 > 0) ? (x70 - y70):0) + z71*((x71 - y71 > 0) ? (x71 - y71):0)

Returns
  Returned accumulation vector (8 x cint48 lanes)

Parameters

  acc | Incoming accumulation vector (8 x cint48 lanes)
  xbuff | Input buffer of 64 elements of type int16
  xstart | Starting position offset applied to all lanes of input from X buffer.
  xoffsets | 4b offset for each lane, applied to both x and y buffers. LSB apply to first lane
  xstep | Step between each column for selection in the x and y buffers. Ystep is symmetric to xstep (ystep advances by -xstep).
  ystart | Starting position offset applied to all lanes for input from Y buffer.
  zbuff | Input buffer of 8 elements of type cint16
  zstart | Starting position offset applied to all lanes for input from Z buffer. This must be a compile time constant. Only the 4 LSB of the argument are used.
  zoffsets | 4b offset for each lane, applied to input from Z buffer. LSB apply to first lane
  zstep | Step between each column for selection in the zbuffer.

Note
  - For more information on how data selection works from the buffers go here. The data buffer and coefficient buffer in this intrinsic use the general scheme.
  - Parameter 'zstart' must be a compile time constant.

## ◆ msc8_min() [1/3]

v8cacc48 msc8_min | ( | v8cacc48 | acc,
|  | v32int16 | xbuff,
|  | int | xstart,
|  | unsigned int | xoffsets,
|  | int | xstep,
|  | int | ystart,
|  | v8cint16 | zbuff,
|  | int | zstart,
|  | unsigned int | zoffsets,
|  | int | zstep )

Complex multiply-subtract intrinsic function after computing the minimum between the selected lanes from the input buffer using small X input buffer.

acc0 -= z00*(min(x00 , y00)) + z01*(min(x01 , y01))
acc1 -= z10*(min(x10 , y10)) + z11*(min(x11 , y11))
acc2 -= z20*(min(x20 , y20)) + z21*(min(x21 , y21))
acc3 -= z30*(min(x30 , y30)) + z31*(min(x31 , y31))
acc4 -= z40*(min(x40 , y40)) + z41*(min(x41 , y41))
acc5 -= z50*(min(x50 , y50)) + z51*(min(x51 , y51))
acc6 -= z60*(min(x60 , y60)) + z61*(min(x61 , y61))
acc7 -= z70*(min(x70 , y70)) + z71*(min(x71 , y71))

Returns
  Returned accumulation vector (8 x cint48 lanes)

Parameters

  acc | Incoming accumulation vector (8 x cint48 lanes)
  xbuff | Input buffer of 32 elements of type int16
  xstart | Starting position offset applied to all lanes of input from X buffer.
  xoffsets | 4b offset for each lane, applied to both x and y buffers. LSB apply to first lane
  xstep | Step between each column for selection in the x and y buffers. Ystep is symmetric to xstep (ystep advances by -xstep).
  ystart | Starting position offset applied to all lanes for input from Y buffer.
  zbuff | Input buffer of 8 elements of type cint16
  zstart | Starting position offset applied to all lanes for input from Z buffer. This must be a compile time constant. Only the 4 LSB of the argument are used.
  zoffsets | 4b offset for each lane, applied to input from Z buffer. LSB apply to first lane
  zstep | Step between each column for selection in the zbuffer.

Note
  - For more information on how data selection works from the buffers go here. The data buffer and coefficient buffer in this intrinsic use the general scheme.
  - Parameter 'zstart' must be a compile time constant.

## ◆ msc8_min() [2/3]

v8cacc48 msc8_min | ( | v8cacc48 | acc,
|  | v32int16 | xbuff,
|  | int | xstart,
|  | unsigned int | xoffsets,
|  | int | xstep,
|  | v32int16 | ybuff,
|  | int | ystart,
|  | v8cint16 | zbuff,
|  | int | zstart,
|  | unsigned int | zoffsets,
|  | int | zstep )

Complex multiply-subtract intrinsic function after computing the minimum between the selected lanes from the input buffer using small X input buffer.

acc0 -= z00*(min(x00 , y00)) + z01*(min(x01 , y01))
acc1 -= z10*(min(x10 , y10)) + z11*(min(x11 , y11))
acc2 -= z20*(min(x20 , y20)) + z21*(min(x21 , y21))
acc3 -= z30*(min(x30 , y30)) + z31*(min(x31 , y31))
acc4 -= z40*(min(x40 , y40)) + z41*(min(x41 , y41))
acc5 -= z50*(min(x50 , y50)) + z51*(min(x51 , y51))
acc6 -= z60*(min(x60 , y60)) + z61*(min(x61 , y61))
acc7 -= z70*(min(x70 , y70)) + z71*(min(x71 , y71))

Returns
  Returned accumulation vector (8 x cint48 lanes)

Parameters

  acc | Incoming accumulation vector (8 x cint48 lanes)
  xbuff | Input buffer of 32 elements of type int16
  xstart | Starting position offset applied to all lanes of input from X buffer.
  xoffsets | 4b offset for each lane, applied to both x and y buffers. LSB apply to first lane
  xstep | Step between each column for selection in the x and y buffers. Ystep is symmetric to xstep (ystep advances by -xstep).
  ybuff | Right input buffer of 32 elements of type int16
  ystart | Starting position offset applied to all lanes for input from Y buffer.
  zbuff | Input buffer of 8 elements of type cint16
  zstart | Starting position offset applied to all lanes for input from Z buffer. This must be a compile time constant. Only the 4 LSB of the argument are used.
  zoffsets | 4b offset for each lane, applied to input from Z buffer. LSB apply to first lane
  zstep | Step between each column for selection in the zbuffer.

Note
  - For more information on how data selection works from the buffers go here. The data buffer and coefficient buffer in this intrinsic use the general scheme.
  - Parameter 'zstart' must be a compile time constant.

## ◆ msc8_min() [3/3]

v8cacc48 msc8_min | ( | v8cacc48 | acc,
|  | v64int16 | xbuff,
|  | int | xstart,
|  | unsigned int | xoffsets,
|  | int | xstep,
|  | int | ystart,
|  | v8cint16 | zbuff,
|  | int | zstart,
|  | unsigned int | zoffsets,
|  | int | zstep )

Complex multiply-subtract intrinsic function after computing the minimum between the selected lanes from the input buffer .

acc0 -= z00*(min(x00 , y00)) + z01*(min(x01 , y01))
acc1 -= z10*(min(x10 , y10)) + z11*(min(x11 , y11))
acc2 -= z20*(min(x20 , y20)) + z21*(min(x21 , y21))
acc3 -= z30*(min(x30 , y30)) + z31*(min(x31 , y31))
acc4 -= z40*(min(x40 , y40)) + z41*(min(x41 , y41))
acc5 -= z50*(min(x50 , y50)) + z51*(min(x51 , y51))
acc6 -= z60*(min(x60 , y60)) + z61*(min(x61 , y61))
acc7 -= z70*(min(x70 , y70)) + z71*(min(x71 , y71))

Returns
  Returned accumulation vector (8 x cint48 lanes)

Parameters

  acc | Incoming accumulation vector (8 x cint48 lanes)
  xbuff | Input buffer of 64 elements of type int16
  xstart | Starting position offset applied to all lanes of input from X buffer.
  xoffsets | 4b offset for each lane, applied to both x and y buffers. LSB apply to first lane
  xstep | Step between each column for selection in the x and y buffers. Ystep is symmetric to xstep (ystep advances by -xstep).
  ystart | Starting position offset applied to all lanes for input from Y buffer.
  zbuff | Input buffer of 8 elements of type cint16
  zstart | Starting position offset applied to all lanes for input from Z buffer. This must be a compile time constant. Only the 4 LSB of the argument are used.
  zoffsets | 4b offset for each lane, applied to input from Z buffer. LSB apply to first lane
  zstep | Step between each column for selection in the zbuffer.

Note
  - For more information on how data selection works from the buffers go here. The data buffer and coefficient buffer in this intrinsic use the general scheme.
  - Parameter 'zstart' must be a compile time constant.

## ◆ mul4_abs() [1/2]

v4cacc48 mul4_abs | ( | v32int16 | xbuff,
|  | int | xstart,
|  | unsigned int | xoffsets,
|  | int | xstep,
|  | v8cint16 | zbuff,
|  | int | zstart,
|  | unsigned int | zoffsets,
|  | int | zstep )

Complex multiply intrinsic function after computing the absolute value in the selected lanes from the input buffer using small X input buffer.

acc0 = z00*abs(x00) + z01*abs(x01) + z02*abs(x02) + z03*abs(x03)
acc1 = z10*abs(x10) + z11*abs(x11) + z12*abs(x12) + z13*abs(x13)
acc2 = z20*abs(x20) + z21*abs(x21) + z22*abs(x22) + z23*abs(x23)
acc3 = z30*abs(x30) + z31*abs(x31) + z32*abs(x32) + z33*abs(x33)

Returns
  Returned accumulation vector (4 x cint48 lanes)

Parameters

  xbuff | Input buffer of 32 elements of type int16
  xstart | Starting position offset applied to all lanes of input from X buffer.
  xoffsets | 4b offset for each lane, applied to the x buffer. LSB apply to first lane
  xstep | Step between each column for selection in the xbuffer.
  zbuff | Input buffer of 8 elements of type cint16
  zstart | Starting position offset applied to all lanes for input from Z buffer. This must be a compile time constant. Only the 4 LSB of the argument are used.
  zoffsets | 4b offset for each lane, applied to input from Z buffer. LSB apply to first lane
  zstep | Step between each column for selection in the zbuffer.

Note
  - For more information on how data selection works from the buffers go here. The data buffer and coefficient buffer in this intrinsic use the general scheme.
  - Parameter 'zstart' must be a compile time constant.

## ◆ mul4_abs() [2/2]

v4cacc48 mul4_abs | ( | v64int16 | xbuff,
|  | int | xstart,
|  | unsigned int | xoffsets,
|  | int | xstep,
|  | v8cint16 | zbuff,
|  | int | zstart,
|  | unsigned int | zoffsets,
|  | int | zstep )

Complex multiply intrinsic function after computing the absolute value in the selected lanes from the input buffer .

acc0 = z00*abs(x00) + z01*abs(x01) + z02*abs(x02) + z03*abs(x03)
acc1 = z10*abs(x10) + z11*abs(x11) + z12*abs(x12) + z13*abs(x13)
acc2 = z20*abs(x20) + z21*abs(x21) + z22*abs(x22) + z23*abs(x23)
acc3 = z30*abs(x30) + z31*abs(x31) + z32*abs(x32) + z33*abs(x33)

Returns
  Returned accumulation vector (4 x cint48 lanes)

Parameters

  xbuff | Input buffer of 64 elements of type int16
  xstart | Starting position offset applied to all lanes of input from X buffer.
  xoffsets | 4b offset for each lane, applied to the x buffer. LSB apply to first lane
  xstep | Step between each column for selection in the xbuffer.
  zbuff | Input buffer of 8 elements of type cint16
  zstart | Starting position offset applied to all lanes for input from Z buffer. This must be a compile time constant. Only the 4 LSB of the argument are used.
  zoffsets | 4b offset for each lane, applied to input from Z buffer. LSB apply to first lane
  zstep | Step between each column for selection in the zbuffer.

Note
  - For more information on how data selection works from the buffers go here. The data buffer and coefficient buffer in this intrinsic use the general scheme.
  - Parameter 'zstart' must be a compile time constant.

## ◆ mul4_max() [1/3]

v4cacc48 mul4_max | ( | v32int16 | xbuff,
|  | int | xstart,
|  | unsigned int | xoffsets,
|  | int | xstep,
|  | int | ystart,
|  | v8cint16 | zbuff,
|  | int | zstart,
|  | unsigned int | zoffsets,
|  | int | zstep )

Complex multiply intrinsic function after computing the maximum between the selected lanes from the input buffer using small X input buffer.

acc0 = z00*(max(x00 , y00)) + z01*(max(x01 , y01)) + z02*(max(x02 , y02)) + z03*(max(x03 , y03))
acc1 = z10*(max(x10 , y10)) + z11*(max(x11 , y11)) + z12*(max(x12 , y12)) + z13*(max(x13 , y13))
acc2 = z20*(max(x20 , y20)) + z21*(max(x21 , y21)) + z22*(max(x22 , y22)) + z23*(max(x23 , y23))
acc3 = z30*(max(x30 , y30)) + z31*(max(x31 , y31)) + z32*(max(x32 , y32)) + z33*(max(x33 , y33))

Returns
  Returned accumulation vector (4 x cint48 lanes)

Parameters

  xbuff | Input buffer of 32 elements of type int16
  xstart | Starting position offset applied to all lanes of input from X buffer.
  xoffsets | 4b offset for each lane, applied to both x and y buffers. LSB apply to first lane
  xstep | Step between each column for selection in the x and y buffers. Ystep is symmetric to xstep (ystep advances by -xstep).
  ystart | Starting position offset applied to all lanes for input from Y buffer.
  zbuff | Input buffer of 8 elements of type cint16
  zstart | Starting position offset applied to all lanes for input from Z buffer. This must be a compile time constant. Only the 4 LSB of the argument are used.
  zoffsets | 4b offset for each lane, applied to input from Z buffer. LSB apply to first lane
  zstep | Step between each column for selection in the zbuffer.

Note
  - For more information on how data selection works from the buffers go here. The data buffer and coefficient buffer in this intrinsic use the general scheme.
  - Parameter 'zstart' must be a compile time constant.

## ◆ mul4_max() [2/3]

v4cacc48 mul4_max | ( | v32int16 | xbuff,
|  | int | xstart,
|  | unsigned int | xoffsets,
|  | int | xstep,
|  | v32int16 | ybuff,
|  | int | ystart,
|  | v8cint16 | zbuff,
|  | int | zstart,
|  | unsigned int | zoffsets,
|  | int | zstep )

Complex multiply intrinsic function after computing the maximum between the selected lanes from the input buffer using small X input buffer.

acc0 = z00*(max(x00 , y00)) + z01*(max(x01 , y01)) + z02*(max(x02 , y02)) + z03*(max(x03 , y03))
acc1 = z10*(max(x10 , y10)) + z11*(max(x11 , y11)) + z12*(max(x12 , y12)) + z13*(max(x13 , y13))
acc2 = z20*(max(x20 , y20)) + z21*(max(x21 , y21)) + z22*(max(x22 , y22)) + z23*(max(x23 , y23))
acc3 = z30*(max(x30 , y30)) + z31*(max(x31 , y31)) + z32*(max(x32 , y32)) + z33*(max(x33 , y33))

Returns
  Returned accumulation vector (4 x cint48 lanes)

Parameters

  xbuff | Input buffer of 32 elements of type int16
  xstart | Starting position offset applied to all lanes of input from X buffer.
  xoffsets | 4b offset for each lane, applied to both x and y buffers. LSB apply to first lane
  xstep | Step between each column for selection in the x and y buffers. Ystep is symmetric to xstep (ystep advances by -xstep).
  ybuff | Right input buffer of 32 elements of type int16
  ystart | Starting position offset applied to all lanes for input from Y buffer.
  zbuff | Input buffer of 8 elements of type cint16
  zstart | Starting position offset applied to all lanes for input from Z buffer. This must be a compile time constant. Only the 4 LSB of the argument are used.
  zoffsets | 4b offset for each lane, applied to input from Z buffer. LSB apply to first lane
  zstep | Step between each column for selection in the zbuffer.

Note
  - For more information on how data selection works from the buffers go here. The data buffer and coefficient buffer in this intrinsic use the general scheme.
  - Parameter 'zstart' must be a compile time constant.

## ◆ mul4_max() [3/3]

v4cacc48 mul4_max | ( | v64int16 | xbuff,
|  | int | xstart,
|  | unsigned int | xoffsets,
|  | int | xstep,
|  | int | ystart,
|  | v8cint16 | zbuff,
|  | int | zstart,
|  | unsigned int | zoffsets,
|  | int | zstep )

Complex multiply intrinsic function after computing the maximum between the selected lanes from the input buffer .

acc0 = z00*(max(x00 , y00)) + z01*(max(x01 , y01)) + z02*(max(x02 , y02)) + z03*(max(x03 , y03))
acc1 = z10*(max(x10 , y10)) + z11*(max(x11 , y11)) + z12*(max(x12 , y12)) + z13*(max(x13 , y13))
acc2 = z20*(max(x20 , y20)) + z21*(max(x21 , y21)) + z22*(max(x22 , y22)) + z23*(max(x23 , y23))
acc3 = z30*(max(x30 , y30)) + z31*(max(x31 , y31)) + z32*(max(x32 , y32)) + z33*(max(x33 , y33))

Returns
  Returned accumulation vector (4 x cint48 lanes)

Parameters

  xbuff | Input buffer of 64 elements of type int16
  xstart | Starting position offset applied to all lanes of input from X buffer.
  xoffsets | 4b offset for each lane, applied to both x and y buffers. LSB apply to first lane
  xstep | Step between each column for selection in the x and y buffers. Ystep is symmetric to xstep (ystep advances by -xstep).
  ystart | Starting position offset applied to all lanes for input from Y buffer.
  zbuff | Input buffer of 8 elements of type cint16
  zstart | Starting position offset applied to all lanes for input from Z buffer. This must be a compile time constant. Only the 4 LSB of the argument are used.
  zoffsets | 4b offset for each lane, applied to input from Z buffer. LSB apply to first lane
  zstep | Step between each column for selection in the zbuffer.

Note
  - For more information on how data selection works from the buffers go here. The data buffer and coefficient buffer in this intrinsic use the general scheme.
  - Parameter 'zstart' must be a compile time constant.

## ◆ mul4_maxdiff() [1/3]

v4cacc48 mul4_maxdiff | ( | v32int16 | xbuff,
|  | int | xstart,
|  | unsigned int | xoffsets,
|  | int | xstep,
|  | int | ystart,
|  | v8cint16 | zbuff,
|  | int | zstart,
|  | unsigned int | zoffsets,
|  | int | zstep )

Complex multiply intrinsic function after computing the maximum difference between the selected lanes from the input buffer using small X input buffer.

acc0 = z00*((x00 - y00 > 0) ? (x00 - y00):0) + z01*((x01 - y01 > 0) ? (x01 - y01):0) + z02*((x02 - y02 > 0) ? (x02 - y02):0) + z03*((x03 - y03 > 0) ? (x03 - y03):0)
acc1 = z10*((x10 - y10 > 0) ? (x10 - y10):0) + z11*((x11 - y11 > 0) ? (x11 - y11):0) + z12*((x12 - y12 > 0) ? (x12 - y12):0) + z13*((x13 - y13 > 0) ? (x13 - y13):0)
acc2 = z20*((x20 - y20 > 0) ? (x20 - y20):0) + z21*((x21 - y21 > 0) ? (x21 - y21):0) + z22*((x22 - y22 > 0) ? (x22 - y22):0) + z23*((x23 - y23 > 0) ? (x23 - y23):0)
acc3 = z30*((x30 - y30 > 0) ? (x30 - y30):0) + z31*((x31 - y31 > 0) ? (x31 - y31):0) + z32*((x32 - y32 > 0) ? (x32 - y32):0) + z33*((x33 - y33 > 0) ? (x33 - y33):0)

Returns
  Returned accumulation vector (4 x cint48 lanes)

Parameters

  xbuff | Input buffer of 32 elements of type int16
  xstart | Starting position offset applied to all lanes of input from X buffer.
  xoffsets | 4b offset for each lane, applied to both x and y buffers. LSB apply to first lane
  xstep | Step between each column for selection in the x and y buffers. Ystep is symmetric to xstep (ystep advances by -xstep).
  ystart | Starting position offset applied to all lanes for input from Y buffer.
  zbuff | Input buffer of 8 elements of type cint16
  zstart | Starting position offset applied to all lanes for input from Z buffer. This must be a compile time constant. Only the 4 LSB of the argument are used.
  zoffsets | 4b offset for each lane, applied to input from Z buffer. LSB apply to first lane
  zstep | Step between each column for selection in the zbuffer.

Note
  - For more information on how data selection works from the buffers go here. The data buffer and coefficient buffer in this intrinsic use the general scheme.
  - Parameter 'zstart' must be a compile time constant.

## ◆ mul4_maxdiff() [2/3]

v4cacc48 mul4_maxdiff | ( | v32int16 | xbuff,
|  | int | xstart,
|  | unsigned int | xoffsets,
|  | int | xstep,
|  | v32int16 | ybuff,
|  | int | ystart,
|  | v8cint16 | zbuff,
|  | int | zstart,
|  | unsigned int | zoffsets,
|  | int | zstep )

Complex multiply intrinsic function after computing the maximum difference between the selected lanes from the input buffer using small X input buffer.

acc0 = z00*((x00 - y00 > 0) ? (x00 - y00):0) + z01*((x01 - y01 > 0) ? (x01 - y01):0) + z02*((x02 - y02 > 0) ? (x02 - y02):0) + z03*((x03 - y03 > 0) ? (x03 - y03):0)
acc1 = z10*((x10 - y10 > 0) ? (x10 - y10):0) + z11*((x11 - y11 > 0) ? (x11 - y11):0) + z12*((x12 - y12 > 0) ? (x12 - y12):0) + z13*((x13 - y13 > 0) ? (x13 - y13):0)
acc2 = z20*((x20 - y20 > 0) ? (x20 - y20):0) + z21*((x21 - y21 > 0) ? (x21 - y21):0) + z22*((x22 - y22 > 0) ? (x22 - y22):0) + z23*((x23 - y23 > 0) ? (x23 - y23):0)
acc3 = z30*((x30 - y30 > 0) ? (x30 - y30):0) + z31*((x31 - y31 > 0) ? (x31 - y31):0) + z32*((x32 - y32 > 0) ? (x32 - y32):0) + z33*((x33 - y33 > 0) ? (x33 - y33):0)

Returns
  Returned accumulation vector (4 x cint48 lanes)

Parameters

  xbuff | Input buffer of 32 elements of type int16
  xstart | Starting position offset applied to all lanes of input from X buffer.
  xoffsets | 4b offset for each lane, applied to both x and y buffers. LSB apply to first lane
  xstep | Step between each column for selection in the x and y buffers. Ystep is symmetric to xstep (ystep advances by -xstep).
  ybuff | Right input buffer of 32 elements of type int16
  ystart | Starting position offset applied to all lanes for input from Y buffer.
  zbuff | Input buffer of 8 elements of type cint16
  zstart | Starting position offset applied to all lanes for input from Z buffer. This must be a compile time constant. Only the 4 LSB of the argument are used.
  zoffsets | 4b offset for each lane, applied to input from Z buffer. LSB apply to first lane
  zstep | Step between each column for selection in the zbuffer.

Note
  - For more information on how data selection works from the buffers go here. The data buffer and coefficient buffer in this intrinsic use the general scheme.
  - Parameter 'zstart' must be a compile time constant.

## ◆ mul4_maxdiff() [3/3]

v4cacc48 mul4_maxdiff | ( | v64int16 | xbuff,
|  | int | xstart,
|  | unsigned int | xoffsets,
|  | int | xstep,
|  | int | ystart,
|  | v8cint16 | zbuff,
|  | int | zstart,
|  | unsigned int | zoffsets,
|  | int | zstep )

Complex multiply intrinsic function after computing the maximum difference between the selected lanes from the input buffer .

acc0 = z00*((x00 - y00 > 0) ? (x00 - y00):0) + z01*((x01 - y01 > 0) ? (x01 - y01):0) + z02*((x02 - y02 > 0) ? (x02 - y02):0) + z03*((x03 - y03 > 0) ? (x03 - y03):0)
acc1 = z10*((x10 - y10 > 0) ? (x10 - y10):0) + z11*((x11 - y11 > 0) ? (x11 - y11):0) + z12*((x12 - y12 > 0) ? (x12 - y12):0) + z13*((x13 - y13 > 0) ? (x13 - y13):0)
acc2 = z20*((x20 - y20 > 0) ? (x20 - y20):0) + z21*((x21 - y21 > 0) ? (x21 - y21):0) + z22*((x22 - y22 > 0) ? (x22 - y22):0) + z23*((x23 - y23 > 0) ? (x23 - y23):0)
acc3 = z30*((x30 - y30 > 0) ? (x30 - y30):0) + z31*((x31 - y31 > 0) ? (x31 - y31):0) + z32*((x32 - y32 > 0) ? (x32 - y32):0) + z33*((x33 - y33 > 0) ? (x33 - y33):0)

Returns
  Returned accumulation vector (4 x cint48 lanes)

Parameters

  xbuff | Input buffer of 64 elements of type int16
  xstart | Starting position offset applied to all lanes of input from X buffer.
  xoffsets | 4b offset for each lane, applied to both x and y buffers. LSB apply to first lane
  xstep | Step between each column for selection in the x and y buffers. Ystep is symmetric to xstep (ystep advances by -xstep).
  ystart | Starting position offset applied to all lanes for input from Y buffer.
  zbuff | Input buffer of 8 elements of type cint16
  zstart | Starting position offset applied to all lanes for input from Z buffer. This must be a compile time constant. Only the 4 LSB of the argument are used.
  zoffsets | 4b offset for each lane, applied to input from Z buffer. LSB apply to first lane
  zstep | Step between each column for selection in the zbuffer.

Note
  - For more information on how data selection works from the buffers go here. The data buffer and coefficient buffer in this intrinsic use the general scheme.
  - Parameter 'zstart' must be a compile time constant.

## ◆ mul4_min() [1/3]

v4cacc48 mul4_min | ( | v32int16 | xbuff,
|  | int | xstart,
|  | unsigned int | xoffsets,
|  | int | xstep,
|  | int | ystart,
|  | v8cint16 | zbuff,
|  | int | zstart,
|  | unsigned int | zoffsets,
|  | int | zstep )

Complex multiply intrinsic function after computing the minimum between the selected lanes from the input buffer using small X input buffer.

acc0 = z00*(min(x00 , y00)) + z01*(min(x01 , y01)) + z02*(min(x02 , y02)) + z03*(min(x03 , y03))
acc1 = z10*(min(x10 , y10)) + z11*(min(x11 , y11)) + z12*(min(x12 , y12)) + z13*(min(x13 , y13))
acc2 = z20*(min(x20 , y20)) + z21*(min(x21 , y21)) + z22*(min(x22 , y22)) + z23*(min(x23 , y23))
acc3 = z30*(min(x30 , y30)) + z31*(min(x31 , y31)) + z32*(min(x32 , y32)) + z33*(min(x33 , y33))

Returns
  Returned accumulation vector (4 x cint48 lanes)

Parameters

  xbuff | Input buffer of 32 elements of type int16
  xstart | Starting position offset applied to all lanes of input from X buffer.
  xoffsets | 4b offset for each lane, applied to both x and y buffers. LSB apply to first lane
  xstep | Step between each column for selection in the x and y buffers. Ystep is symmetric to xstep (ystep advances by -xstep).
  ystart | Starting position offset applied to all lanes for input from Y buffer.
  zbuff | Input buffer of 8 elements of type cint16
  zstart | Starting position offset applied to all lanes for input from Z buffer. This must be a compile time constant. Only the 4 LSB of the argument are used.
  zoffsets | 4b offset for each lane, applied to input from Z buffer. LSB apply to first lane
  zstep | Step between each column for selection in the zbuffer.

Note
  - For more information on how data selection works from the buffers go here. The data buffer and coefficient buffer in this intrinsic use the general scheme.
  - Parameter 'zstart' must be a compile time constant.

## ◆ mul4_min() [2/3]

v4cacc48 mul4_min | ( | v32int16 | xbuff,
|  | int | xstart,
|  | unsigned int | xoffsets,
|  | int | xstep,
|  | v32int16 | ybuff,
|  | int | ystart,
|  | v8cint16 | zbuff,
|  | int | zstart,
|  | unsigned int | zoffsets,
|  | int | zstep )

Complex multiply intrinsic function after computing the minimum between the selected lanes from the input buffer using small X input buffer.

acc0 = z00*(min(x00 , y00)) + z01*(min(x01 , y01)) + z02*(min(x02 , y02)) + z03*(min(x03 , y03))
acc1 = z10*(min(x10 , y10)) + z11*(min(x11 , y11)) + z12*(min(x12 , y12)) + z13*(min(x13 , y13))
acc2 = z20*(min(x20 , y20)) + z21*(min(x21 , y21)) + z22*(min(x22 , y22)) + z23*(min(x23 , y23))
acc3 = z30*(min(x30 , y30)) + z31*(min(x31 , y31)) + z32*(min(x32 , y32)) + z33*(min(x33 , y33))

Returns
  Returned accumulation vector (4 x cint48 lanes)

Parameters

  xbuff | Input buffer of 32 elements of type int16
  xstart | Starting position offset applied to all lanes of input from X buffer.
  xoffsets | 4b offset for each lane, applied to both x and y buffers. LSB apply to first lane
  xstep | Step between each column for selection in the x and y buffers. Ystep is symmetric to xstep (ystep advances by -xstep).
  ybuff | Right input buffer of 32 elements of type int16
  ystart | Starting position offset applied to all lanes for input from Y buffer.
  zbuff | Input buffer of 8 elements of type cint16
  zstart | Starting position offset applied to all lanes for input from Z buffer. This must be a compile time constant. Only the 4 LSB of the argument are used.
  zoffsets | 4b offset for each lane, applied to input from Z buffer. LSB apply to first lane
  zstep | Step between each column for selection in the zbuffer.

Note
  - For more information on how data selection works from the buffers go here. The data buffer and coefficient buffer in this intrinsic use the general scheme.
  - Parameter 'zstart' must be a compile time constant.

## ◆ mul4_min() [3/3]

v4cacc48 mul4_min | ( | v64int16 | xbuff,
|  | int | xstart,
|  | unsigned int | xoffsets,
|  | int | xstep,
|  | int | ystart,
|  | v8cint16 | zbuff,
|  | int | zstart,
|  | unsigned int | zoffsets,
|  | int | zstep )

Complex multiply intrinsic function after computing the minimum between the selected lanes from the input buffer .

acc0 = z00*(min(x00 , y00)) + z01*(min(x01 , y01)) + z02*(min(x02 , y02)) + z03*(min(x03 , y03))
acc1 = z10*(min(x10 , y10)) + z11*(min(x11 , y11)) + z12*(min(x12 , y12)) + z13*(min(x13 , y13))
acc2 = z20*(min(x20 , y20)) + z21*(min(x21 , y21)) + z22*(min(x22 , y22)) + z23*(min(x23 , y23))
acc3 = z30*(min(x30 , y30)) + z31*(min(x31 , y31)) + z32*(min(x32 , y32)) + z33*(min(x33 , y33))

Returns
  Returned accumulation vector (4 x cint48 lanes)

Parameters

  xbuff | Input buffer of 64 elements of type int16
  xstart | Starting position offset applied to all lanes of input from X buffer.
  xoffsets | 4b offset for each lane, applied to both x and y buffers. LSB apply to first lane
  xstep | Step between each column for selection in the x and y buffers. Ystep is symmetric to xstep (ystep advances by -xstep).
  ystart | Starting position offset applied to all lanes for input from Y buffer.
  zbuff | Input buffer of 8 elements of type cint16
  zstart | Starting position offset applied to all lanes for input from Z buffer. This must be a compile time constant. Only the 4 LSB of the argument are used.
  zoffsets | 4b offset for each lane, applied to input from Z buffer. LSB apply to first lane
  zstep | Step between each column for selection in the zbuffer.

Note
  - For more information on how data selection works from the buffers go here. The data buffer and coefficient buffer in this intrinsic use the general scheme.
  - Parameter 'zstart' must be a compile time constant.

## ◆ mul8_abs() [1/2]

v8cacc48 mul8_abs | ( | v32int16 | xbuff,
|  | int | xstart,
|  | unsigned int | xoffsets,
|  | int | xstep,
|  | v8cint16 | zbuff,
|  | int | zstart,
|  | unsigned int | zoffsets,
|  | int | zstep )

Complex multiply intrinsic function after computing the absolute value in the selected lanes from the input buffer using small X input buffer.

acc0 = z00*abs(x00) + z01*abs(x01)
acc1 = z10*abs(x10) + z11*abs(x11)
acc2 = z20*abs(x20) + z21*abs(x21)
acc3 = z30*abs(x30) + z31*abs(x31)
acc4 = z40*abs(x40) + z41*abs(x41)
acc5 = z50*abs(x50) + z51*abs(x51)
acc6 = z60*abs(x60) + z61*abs(x61)
acc7 = z70*abs(x70) + z71*abs(x71)

Returns
  Returned accumulation vector (8 x cint48 lanes)

Parameters

  xbuff | Input buffer of 32 elements of type int16
  xstart | Starting position offset applied to all lanes of input from X buffer.
  xoffsets | 4b offset for each lane, applied to the x buffer. LSB apply to first lane
  xstep | Step between each column for selection in the xbuffer.
  zbuff | Input buffer of 8 elements of type cint16
  zstart | Starting position offset applied to all lanes for input from Z buffer. This must be a compile time constant. Only the 4 LSB of the argument are used.
  zoffsets | 4b offset for each lane, applied to input from Z buffer. LSB apply to first lane
  zstep | Step between each column for selection in the zbuffer.

Note
  - For more information on how data selection works from the buffers go here. The data buffer and coefficient buffer in this intrinsic use the general scheme.
  - Parameter 'zstart' must be a compile time constant.

## ◆ mul8_abs() [2/2]

v8cacc48 mul8_abs | ( | v64int16 | xbuff,
|  | int | xstart,
|  | unsigned int | xoffsets,
|  | int | xstep,
|  | v8cint16 | zbuff,
|  | int | zstart,
|  | unsigned int | zoffsets,
|  | int | zstep )

Complex multiply intrinsic function after computing the absolute value in the selected lanes from the input buffer .

acc0 = z00*abs(x00) + z01*abs(x01)
acc1 = z10*abs(x10) + z11*abs(x11)
acc2 = z20*abs(x20) + z21*abs(x21)
acc3 = z30*abs(x30) + z31*abs(x31)
acc4 = z40*abs(x40) + z41*abs(x41)
acc5 = z50*abs(x50) + z51*abs(x51)
acc6 = z60*abs(x60) + z61*abs(x61)
acc7 = z70*abs(x70) + z71*abs(x71)

Returns
  Returned accumulation vector (8 x cint48 lanes)

Parameters

  xbuff | Input buffer of 64 elements of type int16
  xstart | Starting position offset applied to all lanes of input from X buffer.
  xoffsets | 4b offset for each lane, applied to the x buffer. LSB apply to first lane
  xstep | Step between each column for selection in the xbuffer.
  zbuff | Input buffer of 8 elements of type cint16
  zstart | Starting position offset applied to all lanes for input from Z buffer. This must be a compile time constant. Only the 4 LSB of the argument are used.
  zoffsets | 4b offset for each lane, applied to input from Z buffer. LSB apply to first lane
  zstep | Step between each column for selection in the zbuffer.

Note
  - For more information on how data selection works from the buffers go here. The data buffer and coefficient buffer in this intrinsic use the general scheme.
  - Parameter 'zstart' must be a compile time constant.

## ◆ mul8_max() [1/3]

v8cacc48 mul8_max | ( | v32int16 | xbuff,
|  | int | xstart,
|  | unsigned int | xoffsets,
|  | int | xstep,
|  | int | ystart,
|  | v8cint16 | zbuff,
|  | int | zstart,
|  | unsigned int | zoffsets,
|  | int | zstep )

Complex multiply intrinsic function after computing the maximum between the selected lanes from the input buffer using small X input buffer.

acc0 = z00*(max(x00 , y00)) + z01*(max(x01 , y01))
acc1 = z10*(max(x10 , y10)) + z11*(max(x11 , y11))
acc2 = z20*(max(x20 , y20)) + z21*(max(x21 , y21))
acc3 = z30*(max(x30 , y30)) + z31*(max(x31 , y31))
acc4 = z40*(max(x40 , y40)) + z41*(max(x41 , y41))
acc5 = z50*(max(x50 , y50)) + z51*(max(x51 , y51))
acc6 = z60*(max(x60 , y60)) + z61*(max(x61 , y61))
acc7 = z70*(max(x70 , y70)) + z71*(max(x71 , y71))

Returns
  Returned accumulation vector (8 x cint48 lanes)

Parameters

  xbuff | Input buffer of 32 elements of type int16
  xstart | Starting position offset applied to all lanes of input from X buffer.
  xoffsets | 4b offset for each lane, applied to both x and y buffers. LSB apply to first lane
  xstep | Step between each column for selection in the x and y buffers. Ystep is symmetric to xstep (ystep advances by -xstep).
  ystart | Starting position offset applied to all lanes for input from Y buffer.
  zbuff | Input buffer of 8 elements of type cint16
  zstart | Starting position offset applied to all lanes for input from Z buffer. This must be a compile time constant. Only the 4 LSB of the argument are used.
  zoffsets | 4b offset for each lane, applied to input from Z buffer. LSB apply to first lane
  zstep | Step between each column for selection in the zbuffer.

Note
  - For more information on how data selection works from the buffers go here. The data buffer and coefficient buffer in this intrinsic use the general scheme.
  - Parameter 'zstart' must be a compile time constant.

## ◆ mul8_max() [2/3]

v8cacc48 mul8_max | ( | v32int16 | xbuff,
|  | int | xstart,
|  | unsigned int | xoffsets,
|  | int | xstep,
|  | v32int16 | ybuff,
|  | int | ystart,
|  | v8cint16 | zbuff,
|  | int | zstart,
|  | unsigned int | zoffsets,
|  | int | zstep )

Complex multiply intrinsic function after computing the maximum between the selected lanes from the input buffer using small X input buffer.

acc0 = z00*(max(x00 , y00)) + z01*(max(x01 , y01))
acc1 = z10*(max(x10 , y10)) + z11*(max(x11 , y11))
acc2 = z20*(max(x20 , y20)) + z21*(max(x21 , y21))
acc3 = z30*(max(x30 , y30)) + z31*(max(x31 , y31))
acc4 = z40*(max(x40 , y40)) + z41*(max(x41 , y41))
acc5 = z50*(max(x50 , y50)) + z51*(max(x51 , y51))
acc6 = z60*(max(x60 , y60)) + z61*(max(x61 , y61))
acc7 = z70*(max(x70 , y70)) + z71*(max(x71 , y71))

Returns
  Returned accumulation vector (8 x cint48 lanes)

Parameters

  xbuff | Input buffer of 32 elements of type int16
  xstart | Starting position offset applied to all lanes of input from X buffer.
  xoffsets | 4b offset for each lane, applied to both x and y buffers. LSB apply to first lane
  xstep | Step between each column for selection in the x and y buffers. Ystep is symmetric to xstep (ystep advances by -xstep).
  ybuff | Right input buffer of 32 elements of type int16
  ystart | Starting position offset applied to all lanes for input from Y buffer.
  zbuff | Input buffer of 8 elements of type cint16
  zstart | Starting position offset applied to all lanes for input from Z buffer. This must be a compile time constant. Only the 4 LSB of the argument are used.
  zoffsets | 4b offset for each lane, applied to input from Z buffer. LSB apply to first lane
  zstep | Step between each column for selection in the zbuffer.

Note
  - For more information on how data selection works from the buffers go here. The data buffer and coefficient buffer in this intrinsic use the general scheme.
  - Parameter 'zstart' must be a compile time constant.

## ◆ mul8_max() [3/3]

v8cacc48 mul8_max | ( | v64int16 | xbuff,
|  | int | xstart,
|  | unsigned int | xoffsets,
|  | int | xstep,
|  | int | ystart,
|  | v8cint16 | zbuff,
|  | int | zstart,
|  | unsigned int | zoffsets,
|  | int | zstep )

Complex multiply intrinsic function after computing the maximum between the selected lanes from the input buffer .

acc0 = z00*(max(x00 , y00)) + z01*(max(x01 , y01))
acc1 = z10*(max(x10 , y10)) + z11*(max(x11 , y11))
acc2 = z20*(max(x20 , y20)) + z21*(max(x21 , y21))
acc3 = z30*(max(x30 , y30)) + z31*(max(x31 , y31))
acc4 = z40*(max(x40 , y40)) + z41*(max(x41 , y41))
acc5 = z50*(max(x50 , y50)) + z51*(max(x51 , y51))
acc6 = z60*(max(x60 , y60)) + z61*(max(x61 , y61))
acc7 = z70*(max(x70 , y70)) + z71*(max(x71 , y71))

Returns
  Returned accumulation vector (8 x cint48 lanes)

Parameters

  xbuff | Input buffer of 64 elements of type int16
  xstart | Starting position offset applied to all lanes of input from X buffer.
  xoffsets | 4b offset for each lane, applied to both x and y buffers. LSB apply to first lane
  xstep | Step between each column for selection in the x and y buffers. Ystep is symmetric to xstep (ystep advances by -xstep).
  ystart | Starting position offset applied to all lanes for input from Y buffer.
  zbuff | Input buffer of 8 elements of type cint16
  zstart | Starting position offset applied to all lanes for input from Z buffer. This must be a compile time constant. Only the 4 LSB of the argument are used.
  zoffsets | 4b offset for each lane, applied to input from Z buffer. LSB apply to first lane
  zstep | Step between each column for selection in the zbuffer.

Note
  - For more information on how data selection works from the buffers go here. The data buffer and coefficient buffer in this intrinsic use the general scheme.
  - Parameter 'zstart' must be a compile time constant.

## ◆ mul8_maxdiff() [1/3]

v8cacc48 mul8_maxdiff | ( | v32int16 | xbuff,
|  | int | xstart,
|  | unsigned int | xoffsets,
|  | int | xstep,
|  | int | ystart,
|  | v8cint16 | zbuff,
|  | int | zstart,
|  | unsigned int | zoffsets,
|  | int | zstep )

Complex multiply intrinsic function after computing the maximum difference between the selected lanes from the input buffer using small X input buffer.

acc0 = z00*((x00 - y00 > 0) ? (x00 - y00):0) + z01*((x01 - y01 > 0) ? (x01 - y01):0)
acc1 = z10*((x10 - y10 > 0) ? (x10 - y10):0) + z11*((x11 - y11 > 0) ? (x11 - y11):0)
acc2 = z20*((x20 - y20 > 0) ? (x20 - y20):0) + z21*((x21 - y21 > 0) ? (x21 - y21):0)
acc3 = z30*((x30 - y30 > 0) ? (x30 - y30):0) + z31*((x31 - y31 > 0) ? (x31 - y31):0)
acc4 = z40*((x40 - y40 > 0) ? (x40 - y40):0) + z41*((x41 - y41 > 0) ? (x41 - y41):0)
acc5 = z50*((x50 - y50 > 0) ? (x50 - y50):0) + z51*((x51 - y51 > 0) ? (x51 - y51):0)
acc6 = z60*((x60 - y60 > 0) ? (x60 - y60):0) + z61*((x61 - y61 > 0) ? (x61 - y61):0)
acc7 = z70*((x70 - y70 > 0) ? (x70 - y70):0) + z71*((x71 - y71 > 0) ? (x71 - y71):0)

Returns
  Returned accumulation vector (8 x cint48 lanes)

Parameters

  xbuff | Input buffer of 32 elements of type int16
  xstart | Starting position offset applied to all lanes of input from X buffer.
  xoffsets | 4b offset for each lane, applied to both x and y buffers. LSB apply to first lane
  xstep | Step between each column for selection in the x and y buffers. Ystep is symmetric to xstep (ystep advances by -xstep).
  ystart | Starting position offset applied to all lanes for input from Y buffer.
  zbuff | Input buffer of 8 elements of type cint16
  zstart | Starting position offset applied to all lanes for input from Z buffer. This must be a compile time constant. Only the 4 LSB of the argument are used.
  zoffsets | 4b offset for each lane, applied to input from Z buffer. LSB apply to first lane
  zstep | Step between each column for selection in the zbuffer.

Note
  - For more information on how data selection works from the buffers go here. The data buffer and coefficient buffer in this intrinsic use the general scheme.
  - Parameter 'zstart' must be a compile time constant.

## ◆ mul8_maxdiff() [2/3]

v8cacc48 mul8_maxdiff | ( | v32int16 | xbuff,
|  | int | xstart,
|  | unsigned int | xoffsets,
|  | int | xstep,
|  | v32int16 | ybuff,
|  | int | ystart,
|  | v8cint16 | zbuff,
|  | int | zstart,
|  | unsigned int | zoffsets,
|  | int | zstep )

Complex multiply intrinsic function after computing the maximum difference between the selected lanes from the input buffer using small X input buffer.

acc0 = z00*((x00 - y00 > 0) ? (x00 - y00):0) + z01*((x01 - y01 > 0) ? (x01 - y01):0)
acc1 = z10*((x10 - y10 > 0) ? (x10 - y10):0) + z11*((x11 - y11 > 0) ? (x11 - y11):0)
acc2 = z20*((x20 - y20 > 0) ? (x20 - y20):0) + z21*((x21 - y21 > 0) ? (x21 - y21):0)
acc3 = z30*((x30 - y30 > 0) ? (x30 - y30):0) + z31*((x31 - y31 > 0) ? (x31 - y31):0)
acc4 = z40*((x40 - y40 > 0) ? (x40 - y40):0) + z41*((x41 - y41 > 0) ? (x41 - y41):0)
acc5 = z50*((x50 - y50 > 0) ? (x50 - y50):0) + z51*((x51 - y51 > 0) ? (x51 - y51):0)
acc6 = z60*((x60 - y60 > 0) ? (x60 - y60):0) + z61*((x61 - y61 > 0) ? (x61 - y61):0)
acc7 = z70*((x70 - y70 > 0) ? (x70 - y70):0) + z71*((x71 - y71 > 0) ? (x71 - y71):0)

Returns
  Returned accumulation vector (8 x cint48 lanes)

Parameters

  xbuff | Input buffer of 32 elements of type int16
  xstart | Starting position offset applied to all lanes of input from X buffer.
  xoffsets | 4b offset for each lane, applied to both x and y buffers. LSB apply to first lane
  xstep | Step between each column for selection in the x and y buffers. Ystep is symmetric to xstep (ystep advances by -xstep).
  ybuff | Right input buffer of 32 elements of type int16
  ystart | Starting position offset applied to all lanes for input from Y buffer.
  zbuff | Input buffer of 8 elements of type cint16
  zstart | Starting position offset applied to all lanes for input from Z buffer. This must be a compile time constant. Only the 4 LSB of the argument are used.
  zoffsets | 4b offset for each lane, applied to input from Z buffer. LSB apply to first lane
  zstep | Step between each column for selection in the zbuffer.

Note
  - For more information on how data selection works from the buffers go here. The data buffer and coefficient buffer in this intrinsic use the general scheme.
  - Parameter 'zstart' must be a compile time constant.

## ◆ mul8_maxdiff() [3/3]

v8cacc48 mul8_maxdiff | ( | v64int16 | xbuff,
|  | int | xstart,
|  | unsigned int | xoffsets,
|  | int | xstep,
|  | int | ystart,
|  | v8cint16 | zbuff,
|  | int | zstart,
|  | unsigned int | zoffsets,
|  | int | zstep )

Complex multiply intrinsic function after computing the maximum difference between the selected lanes from the input buffer .

acc0 = z00*((x00 - y00 > 0) ? (x00 - y00):0) + z01*((x01 - y01 > 0) ? (x01 - y01):0)
acc1 = z10*((x10 - y10 > 0) ? (x10 - y10):0) + z11*((x11 - y11 > 0) ? (x11 - y11):0)
acc2 = z20*((x20 - y20 > 0) ? (x20 - y20):0) + z21*((x21 - y21 > 0) ? (x21 - y21):0)
acc3 = z30*((x30 - y30 > 0) ? (x30 - y30):0) + z31*((x31 - y31 > 0) ? (x31 - y31):0)
acc4 = z40*((x40 - y40 > 0) ? (x40 - y40):0) + z41*((x41 - y41 > 0) ? (x41 - y41):0)
acc5 = z50*((x50 - y50 > 0) ? (x50 - y50):0) + z51*((x51 - y51 > 0) ? (x51 - y51):0)
acc6 = z60*((x60 - y60 > 0) ? (x60 - y60):0) + z61*((x61 - y61 > 0) ? (x61 - y61):0)
acc7 = z70*((x70 - y70 > 0) ? (x70 - y70):0) + z71*((x71 - y71 > 0) ? (x71 - y71):0)

Returns
  Returned accumulation vector (8 x cint48 lanes)

Parameters

  xbuff | Input buffer of 64 elements of type int16
  xstart | Starting position offset applied to all lanes of input from X buffer.
  xoffsets | 4b offset for each lane, applied to both x and y buffers. LSB apply to first lane
  xstep | Step between each column for selection in the x and y buffers. Ystep is symmetric to xstep (ystep advances by -xstep).
  ystart | Starting position offset applied to all lanes for input from Y buffer.
  zbuff | Input buffer of 8 elements of type cint16
  zstart | Starting position offset applied to all lanes for input from Z buffer. This must be a compile time constant. Only the 4 LSB of the argument are used.
  zoffsets | 4b offset for each lane, applied to input from Z buffer. LSB apply to first lane
  zstep | Step between each column for selection in the zbuffer.

Note
  - For more information on how data selection works from the buffers go here. The data buffer and coefficient buffer in this intrinsic use the general scheme.
  - Parameter 'zstart' must be a compile time constant.

## ◆ mul8_min() [1/3]

v8cacc48 mul8_min | ( | v32int16 | xbuff,
|  | int | xstart,
|  | unsigned int | xoffsets,
|  | int | xstep,
|  | int | ystart,
|  | v8cint16 | zbuff,
|  | int | zstart,
|  | unsigned int | zoffsets,
|  | int | zstep )

Complex multiply intrinsic function after computing the minimum between the selected lanes from the input buffer using small X input buffer.

acc0 = z00*(min(x00 , y00)) + z01*(min(x01 , y01))
acc1 = z10*(min(x10 , y10)) + z11*(min(x11 , y11))
acc2 = z20*(min(x20 , y20)) + z21*(min(x21 , y21))
acc3 = z30*(min(x30 , y30)) + z31*(min(x31 , y31))
acc4 = z40*(min(x40 , y40)) + z41*(min(x41 , y41))
acc5 = z50*(min(x50 , y50)) + z51*(min(x51 , y51))
acc6 = z60*(min(x60 , y60)) + z61*(min(x61 , y61))
acc7 = z70*(min(x70 , y70)) + z71*(min(x71 , y71))

Returns
  Returned accumulation vector (8 x cint48 lanes)

Parameters

  xbuff | Input buffer of 32 elements of type int16
  xstart | Starting position offset applied to all lanes of input from X buffer.
  xoffsets | 4b offset for each lane, applied to both x and y buffers. LSB apply to first lane
  xstep | Step between each column for selection in the x and y buffers. Ystep is symmetric to xstep (ystep advances by -xstep).
  ystart | Starting position offset applied to all lanes for input from Y buffer.
  zbuff | Input buffer of 8 elements of type cint16
  zstart | Starting position offset applied to all lanes for input from Z buffer. This must be a compile time constant. Only the 4 LSB of the argument are used.
  zoffsets | 4b offset for each lane, applied to input from Z buffer. LSB apply to first lane
  zstep | Step between each column for selection in the zbuffer.

Note
  - For more information on how data selection works from the buffers go here. The data buffer and coefficient buffer in this intrinsic use the general scheme.
  - Parameter 'zstart' must be a compile time constant.

## ◆ mul8_min() [2/3]

v8cacc48 mul8_min | ( | v32int16 | xbuff,
|  | int | xstart,
|  | unsigned int | xoffsets,
|  | int | xstep,
|  | v32int16 | ybuff,
|  | int | ystart,
|  | v8cint16 | zbuff,
|  | int | zstart,
|  | unsigned int | zoffsets,
|  | int | zstep )

Complex multiply intrinsic function after computing the minimum between the selected lanes from the input buffer using small X input buffer.

acc0 = z00*(min(x00 , y00)) + z01*(min(x01 , y01))
acc1 = z10*(min(x10 , y10)) + z11*(min(x11 , y11))
acc2 = z20*(min(x20 , y20)) + z21*(min(x21 , y21))
acc3 = z30*(min(x30 , y30)) + z31*(min(x31 , y31))
acc4 = z40*(min(x40 , y40)) + z41*(min(x41 , y41))
acc5 = z50*(min(x50 , y50)) + z51*(min(x51 , y51))
acc6 = z60*(min(x60 , y60)) + z61*(min(x61 , y61))
acc7 = z70*(min(x70 , y70)) + z71*(min(x71 , y71))

Returns
  Returned accumulation vector (8 x cint48 lanes)

Parameters

  xbuff | Input buffer of 32 elements of type int16
  xstart | Starting position offset applied to all lanes of input from X buffer.
  xoffsets | 4b offset for each lane, applied to both x and y buffers. LSB apply to first lane
  xstep | Step between each column for selection in the x and y buffers. Ystep is symmetric to xstep (ystep advances by -xstep).
  ybuff | Right input buffer of 32 elements of type int16
  ystart | Starting position offset applied to all lanes for input from Y buffer.
  zbuff | Input buffer of 8 elements of type cint16
  zstart | Starting position offset applied to all lanes for input from Z buffer. This must be a compile time constant. Only the 4 LSB of the argument are used.
  zoffsets | 4b offset for each lane, applied to input from Z buffer. LSB apply to first lane
  zstep | Step between each column for selection in the zbuffer.

Note
  - For more information on how data selection works from the buffers go here. The data buffer and coefficient buffer in this intrinsic use the general scheme.
  - Parameter 'zstart' must be a compile time constant.

## ◆ mul8_min() [3/3]

v8cacc48 mul8_min | ( | v64int16 | xbuff,
|  | int | xstart,
|  | unsigned int | xoffsets,
|  | int | xstep,
|  | int | ystart,
|  | v8cint16 | zbuff,
|  | int | zstart,
|  | unsigned int | zoffsets,
|  | int | zstep )

Complex multiply intrinsic function after computing the minimum between the selected lanes from the input buffer .

acc0 = z00*(min(x00 , y00)) + z01*(min(x01 , y01))
acc1 = z10*(min(x10 , y10)) + z11*(min(x11 , y11))
acc2 = z20*(min(x20 , y20)) + z21*(min(x21 , y21))
acc3 = z30*(min(x30 , y30)) + z31*(min(x31 , y31))
acc4 = z40*(min(x40 , y40)) + z41*(min(x41 , y41))
acc5 = z50*(min(x50 , y50)) + z51*(min(x51 , y51))
acc6 = z60*(min(x60 , y60)) + z61*(min(x61 , y61))
acc7 = z70*(min(x70 , y70)) + z71*(min(x71 , y71))

Returns
  Returned accumulation vector (8 x cint48 lanes)

Parameters

  xbuff | Input buffer of 64 elements of type int16
  xstart | Starting position offset applied to all lanes of input from X buffer.
  xoffsets | 4b offset for each lane, applied to both x and y buffers. LSB apply to first lane
  xstep | Step between each column for selection in the x and y buffers. Ystep is symmetric to xstep (ystep advances by -xstep).
  ystart | Starting position offset applied to all lanes for input from Y buffer.
  zbuff | Input buffer of 8 elements of type cint16
  zstart | Starting position offset applied to all lanes for input from Z buffer. This must be a compile time constant. Only the 4 LSB of the argument are used.
  zoffsets | 4b offset for each lane, applied to input from Z buffer. LSB apply to first lane
  zstep | Step between each column for selection in the zbuffer.

Note
  - For more information on how data selection works from the buffers go here. The data buffer and coefficient buffer in this intrinsic use the general scheme.
  - Parameter 'zstart' must be a compile time constant.

## ◆ negmul4_abs() [1/2]

v4cacc48 negmul4_abs | ( | v32int16 | xbuff,
|  | int | xstart,
|  | unsigned int | xoffsets,
|  | int | xstep,
|  | v8cint16 | zbuff,
|  | int | zstart,
|  | unsigned int | zoffsets,
|  | int | zstep )

Complex multiply-negate intrinsic function after computing the absolute value in the selected lanes from the input buffer using small X input buffer.

acc0 = -( z00*abs(x00) + z01*abs(x01) + z02*abs(x02) + z03*abs(x03) )
acc1 = -( z10*abs(x10) + z11*abs(x11) + z12*abs(x12) + z13*abs(x13) )
acc2 = -( z20*abs(x20) + z21*abs(x21) + z22*abs(x22) + z23*abs(x23) )
acc3 = -( z30*abs(x30) + z31*abs(x31) + z32*abs(x32) + z33*abs(x33) )

Returns
  Returned accumulation vector (4 x cint48 lanes)

Parameters

  xbuff | Input buffer of 32 elements of type int16
  xstart | Starting position offset applied to all lanes of input from X buffer.
  xoffsets | 4b offset for each lane, applied to the x buffer. LSB apply to first lane
  xstep | Step between each column for selection in the xbuffer.
  zbuff | Input buffer of 8 elements of type cint16
  zstart | Starting position offset applied to all lanes for input from Z buffer. This must be a compile time constant. Only the 4 LSB of the argument are used.
  zoffsets | 4b offset for each lane, applied to input from Z buffer. LSB apply to first lane
  zstep | Step between each column for selection in the zbuffer.

Note
  - For more information on how data selection works from the buffers go here. The data buffer and coefficient buffer in this intrinsic use the general scheme.
  - Parameter 'zstart' must be a compile time constant.

## ◆ negmul4_abs() [2/2]

v4cacc48 negmul4_abs | ( | v64int16 | xbuff,
|  | int | xstart,
|  | unsigned int | xoffsets,
|  | int | xstep,
|  | v8cint16 | zbuff,
|  | int | zstart,
|  | unsigned int | zoffsets,
|  | int | zstep )

Complex multiply-negate intrinsic function after computing the absolute value in the selected lanes from the input buffer .

acc0 = -( z00*abs(x00) + z01*abs(x01) + z02*abs(x02) + z03*abs(x03) )
acc1 = -( z10*abs(x10) + z11*abs(x11) + z12*abs(x12) + z13*abs(x13) )
acc2 = -( z20*abs(x20) + z21*abs(x21) + z22*abs(x22) + z23*abs(x23) )
acc3 = -( z30*abs(x30) + z31*abs(x31) + z32*abs(x32) + z33*abs(x33) )

Returns
  Returned accumulation vector (4 x cint48 lanes)

Parameters

  xbuff | Input buffer of 64 elements of type int16
  xstart | Starting position offset applied to all lanes of input from X buffer.
  xoffsets | 4b offset for each lane, applied to the x buffer. LSB apply to first lane
  xstep | Step between each column for selection in the xbuffer.
  zbuff | Input buffer of 8 elements of type cint16
  zstart | Starting position offset applied to all lanes for input from Z buffer. This must be a compile time constant. Only the 4 LSB of the argument are used.
  zoffsets | 4b offset for each lane, applied to input from Z buffer. LSB apply to first lane
  zstep | Step between each column for selection in the zbuffer.

Note
  - For more information on how data selection works from the buffers go here. The data buffer and coefficient buffer in this intrinsic use the general scheme.
  - Parameter 'zstart' must be a compile time constant.

## ◆ negmul4_max() [1/3]

v4cacc48 negmul4_max | ( | v32int16 | xbuff,
|  | int | xstart,
|  | unsigned int | xoffsets,
|  | int | xstep,
|  | int | ystart,
|  | v8cint16 | zbuff,
|  | int | zstart,
|  | unsigned int | zoffsets,
|  | int | zstep )

Complex multiply-negate intrinsic function after computing the maximum between the selected lanes from the input buffer using small X input buffer.

acc0 = -( z00*(max(x00 , y00)) + z01*(max(x01 , y01)) + z02*(max(x02 , y02)) + z03*(max(x03 , y03)) )
acc1 = -( z10*(max(x10 , y10)) + z11*(max(x11 , y11)) + z12*(max(x12 , y12)) + z13*(max(x13 , y13)) )
acc2 = -( z20*(max(x20 , y20)) + z21*(max(x21 , y21)) + z22*(max(x22 , y22)) + z23*(max(x23 , y23)) )
acc3 = -( z30*(max(x30 , y30)) + z31*(max(x31 , y31)) + z32*(max(x32 , y32)) + z33*(max(x33 , y33)) )

Returns
  Returned accumulation vector (4 x cint48 lanes)

Parameters

  xbuff | Input buffer of 32 elements of type int16
  xstart | Starting position offset applied to all lanes of input from X buffer.
  xoffsets | 4b offset for each lane, applied to both x and y buffers. LSB apply to first lane
  xstep | Step between each column for selection in the x and y buffers. Ystep is symmetric to xstep (ystep advances by -xstep).
  ystart | Starting position offset applied to all lanes for input from Y buffer.
  zbuff | Input buffer of 8 elements of type cint16
  zstart | Starting position offset applied to all lanes for input from Z buffer. This must be a compile time constant. Only the 4 LSB of the argument are used.
  zoffsets | 4b offset for each lane, applied to input from Z buffer. LSB apply to first lane
  zstep | Step between each column for selection in the zbuffer.

Note
  - For more information on how data selection works from the buffers go here. The data buffer and coefficient buffer in this intrinsic use the general scheme.
  - Parameter 'zstart' must be a compile time constant.

## ◆ negmul4_max() [2/3]

v4cacc48 negmul4_max | ( | v32int16 | xbuff,
|  | int | xstart,
|  | unsigned int | xoffsets,
|  | int | xstep,
|  | v32int16 | ybuff,
|  | int | ystart,
|  | v8cint16 | zbuff,
|  | int | zstart,
|  | unsigned int | zoffsets,
|  | int | zstep )

Complex multiply-negate intrinsic function after computing the maximum between the selected lanes from the input buffer using small X input buffer.

acc0 = -( z00*(max(x00 , y00)) + z01*(max(x01 , y01)) + z02*(max(x02 , y02)) + z03*(max(x03 , y03)) )
acc1 = -( z10*(max(x10 , y10)) + z11*(max(x11 , y11)) + z12*(max(x12 , y12)) + z13*(max(x13 , y13)) )
acc2 = -( z20*(max(x20 , y20)) + z21*(max(x21 , y21)) + z22*(max(x22 , y22)) + z23*(max(x23 , y23)) )
acc3 = -( z30*(max(x30 , y30)) + z31*(max(x31 , y31)) + z32*(max(x32 , y32)) + z33*(max(x33 , y33)) )

Returns
  Returned accumulation vector (4 x cint48 lanes)

Parameters

  xbuff | Input buffer of 32 elements of type int16
  xstart | Starting position offset applied to all lanes of input from X buffer.
  xoffsets | 4b offset for each lane, applied to both x and y buffers. LSB apply to first lane
  xstep | Step between each column for selection in the x and y buffers. Ystep is symmetric to xstep (ystep advances by -xstep).
  ybuff | Right input buffer of 32 elements of type int16
  ystart | Starting position offset applied to all lanes for input from Y buffer.
  zbuff | Input buffer of 8 elements of type cint16
  zstart | Starting position offset applied to all lanes for input from Z buffer. This must be a compile time constant. Only the 4 LSB of the argument are used.
  zoffsets | 4b offset for each lane, applied to input from Z buffer. LSB apply to first lane
  zstep | Step between each column for selection in the zbuffer.

Note
  - For more information on how data selection works from the buffers go here. The data buffer and coefficient buffer in this intrinsic use the general scheme.
  - Parameter 'zstart' must be a compile time constant.

## ◆ negmul4_max() [3/3]

v4cacc48 negmul4_max | ( | v64int16 | xbuff,
|  | int | xstart,
|  | unsigned int | xoffsets,
|  | int | xstep,
|  | int | ystart,
|  | v8cint16 | zbuff,
|  | int | zstart,
|  | unsigned int | zoffsets,
|  | int | zstep )

Complex multiply-negate intrinsic function after computing the maximum between the selected lanes from the input buffer .

acc0 = -( z00*(max(x00 , y00)) + z01*(max(x01 , y01)) + z02*(max(x02 , y02)) + z03*(max(x03 , y03)) )
acc1 = -( z10*(max(x10 , y10)) + z11*(max(x11 , y11)) + z12*(max(x12 , y12)) + z13*(max(x13 , y13)) )
acc2 = -( z20*(max(x20 , y20)) + z21*(max(x21 , y21)) + z22*(max(x22 , y22)) + z23*(max(x23 , y23)) )
acc3 = -( z30*(max(x30 , y30)) + z31*(max(x31 , y31)) + z32*(max(x32 , y32)) + z33*(max(x33 , y33)) )

Returns
  Returned accumulation vector (4 x cint48 lanes)

Parameters

  xbuff | Input buffer of 64 elements of type int16
  xstart | Starting position offset applied to all lanes of input from X buffer.
  xoffsets | 4b offset for each lane, applied to both x and y buffers. LSB apply to first lane
  xstep | Step between each column for selection in the x and y buffers. Ystep is symmetric to xstep (ystep advances by -xstep).
  ystart | Starting position offset applied to all lanes for input from Y buffer.
  zbuff | Input buffer of 8 elements of type cint16
  zstart | Starting position offset applied to all lanes for input from Z buffer. This must be a compile time constant. Only the 4 LSB of the argument are used.
  zoffsets | 4b offset for each lane, applied to input from Z buffer. LSB apply to first lane
  zstep | Step between each column for selection in the zbuffer.

Note
  - For more information on how data selection works from the buffers go here. The data buffer and coefficient buffer in this intrinsic use the general scheme.
  - Parameter 'zstart' must be a compile time constant.

## ◆ negmul4_maxdiff() [1/3]

v4cacc48 negmul4_maxdiff | ( | v32int16 | xbuff,
|  | int | xstart,
|  | unsigned int | xoffsets,
|  | int | xstep,
|  | int | ystart,
|  | v8cint16 | zbuff,
|  | int | zstart,
|  | unsigned int | zoffsets,
|  | int | zstep )

Complex multiply-negate intrinsic function after computing the maximum difference between the selected lanes from the input buffer using small X input buffer.

acc0 = -( z00*((x00 - y00 > 0) ? (x00 - y00):0) + z01*((x01 - y01 > 0) ? (x01 - y01):0) + z02*((x02 - y02 > 0) ? (x02 - y02):0) + z03*((x03 - y03 > 0) ? (x03 - y03):0) )
acc1 = -( z10*((x10 - y10 > 0) ? (x10 - y10):0) + z11*((x11 - y11 > 0) ? (x11 - y11):0) + z12*((x12 - y12 > 0) ? (x12 - y12):0) + z13*((x13 - y13 > 0) ? (x13 - y13):0) )
acc2 = -( z20*((x20 - y20 > 0) ? (x20 - y20):0) + z21*((x21 - y21 > 0) ? (x21 - y21):0) + z22*((x22 - y22 > 0) ? (x22 - y22):0) + z23*((x23 - y23 > 0) ? (x23 - y23):0) )
acc3 = -( z30*((x30 - y30 > 0) ? (x30 - y30):0) + z31*((x31 - y31 > 0) ? (x31 - y31):0) + z32*((x32 - y32 > 0) ? (x32 - y32):0) + z33*((x33 - y33 > 0) ? (x33 - y33):0) )

Returns
  Returned accumulation vector (4 x cint48 lanes)

Parameters

  xbuff | Input buffer of 32 elements of type int16
  xstart | Starting position offset applied to all lanes of input from X buffer.
  xoffsets | 4b offset for each lane, applied to both x and y buffers. LSB apply to first lane
  xstep | Step between each column for selection in the x and y buffers. Ystep is symmetric to xstep (ystep advances by -xstep).
  ystart | Starting position offset applied to all lanes for input from Y buffer.
  zbuff | Input buffer of 8 elements of type cint16
  zstart | Starting position offset applied to all lanes for input from Z buffer. This must be a compile time constant. Only the 4 LSB of the argument are used.
  zoffsets | 4b offset for each lane, applied to input from Z buffer. LSB apply to first lane
  zstep | Step between each column for selection in the zbuffer.

Note
  - For more information on how data selection works from the buffers go here. The data buffer and coefficient buffer in this intrinsic use the general scheme.
  - Parameter 'zstart' must be a compile time constant.

## ◆ negmul4_maxdiff() [2/3]

v4cacc48 negmul4_maxdiff | ( | v32int16 | xbuff,
|  | int | xstart,
|  | unsigned int | xoffsets,
|  | int | xstep,
|  | v32int16 | ybuff,
|  | int | ystart,
|  | v8cint16 | zbuff,
|  | int | zstart,
|  | unsigned int | zoffsets,
|  | int | zstep )

Complex multiply-negate intrinsic function after computing the maximum difference between the selected lanes from the input buffer using small X input buffer.

acc0 = -( z00*((x00 - y00 > 0) ? (x00 - y00):0) + z01*((x01 - y01 > 0) ? (x01 - y01):0) + z02*((x02 - y02 > 0) ? (x02 - y02):0) + z03*((x03 - y03 > 0) ? (x03 - y03):0) )
acc1 = -( z10*((x10 - y10 > 0) ? (x10 - y10):0) + z11*((x11 - y11 > 0) ? (x11 - y11):0) + z12*((x12 - y12 > 0) ? (x12 - y12):0) + z13*((x13 - y13 > 0) ? (x13 - y13):0) )
acc2 = -( z20*((x20 - y20 > 0) ? (x20 - y20):0) + z21*((x21 - y21 > 0) ? (x21 - y21):0) + z22*((x22 - y22 > 0) ? (x22 - y22):0) + z23*((x23 - y23 > 0) ? (x23 - y23):0) )
acc3 = -( z30*((x30 - y30 > 0) ? (x30 - y30):0) + z31*((x31 - y31 > 0) ? (x31 - y31):0) + z32*((x32 - y32 > 0) ? (x32 - y32):0) + z33*((x33 - y33 > 0) ? (x33 - y33):0) )

Returns
  Returned accumulation vector (4 x cint48 lanes)

Parameters

  xbuff | Input buffer of 32 elements of type int16
  xstart | Starting position offset applied to all lanes of input from X buffer.
  xoffsets | 4b offset for each lane, applied to both x and y buffers. LSB apply to first lane
  xstep | Step between each column for selection in the x and y buffers. Ystep is symmetric to xstep (ystep advances by -xstep).
  ybuff | Right input buffer of 32 elements of type int16
  ystart | Starting position offset applied to all lanes for input from Y buffer.
  zbuff | Input buffer of 8 elements of type cint16
  zstart | Starting position offset applied to all lanes for input from Z buffer. This must be a compile time constant. Only the 4 LSB of the argument are used.
  zoffsets | 4b offset for each lane, applied to input from Z buffer. LSB apply to first lane
  zstep | Step between each column for selection in the zbuffer.

Note
  - For more information on how data selection works from the buffers go here. The data buffer and coefficient buffer in this intrinsic use the general scheme.
  - Parameter 'zstart' must be a compile time constant.

## ◆ negmul4_maxdiff() [3/3]

v4cacc48 negmul4_maxdiff | ( | v64int16 | xbuff,
|  | int | xstart,
|  | unsigned int | xoffsets,
|  | int | xstep,
|  | int | ystart,
|  | v8cint16 | zbuff,
|  | int | zstart,
|  | unsigned int | zoffsets,
|  | int | zstep )

Complex multiply-negate intrinsic function after computing the maximum difference between the selected lanes from the input buffer .

acc0 = -( z00*((x00 - y00 > 0) ? (x00 - y00):0) + z01*((x01 - y01 > 0) ? (x01 - y01):0) + z02*((x02 - y02 > 0) ? (x02 - y02):0) + z03*((x03 - y03 > 0) ? (x03 - y03):0) )
acc1 = -( z10*((x10 - y10 > 0) ? (x10 - y10):0) + z11*((x11 - y11 > 0) ? (x11 - y11):0) + z12*((x12 - y12 > 0) ? (x12 - y12):0) + z13*((x13 - y13 > 0) ? (x13 - y13):0) )
acc2 = -( z20*((x20 - y20 > 0) ? (x20 - y20):0) + z21*((x21 - y21 > 0) ? (x21 - y21):0) + z22*((x22 - y22 > 0) ? (x22 - y22):0) + z23*((x23 - y23 > 0) ? (x23 - y23):0) )
acc3 = -( z30*((x30 - y30 > 0) ? (x30 - y30):0) + z31*((x31 - y31 > 0) ? (x31 - y31):0) + z32*((x32 - y32 > 0) ? (x32 - y32):0) + z33*((x33 - y33 > 0) ? (x33 - y33):0) )

Returns
  Returned accumulation vector (4 x cint48 lanes)

Parameters

  xbuff | Input buffer of 64 elements of type int16
  xstart | Starting position offset applied to all lanes of input from X buffer.
  xoffsets | 4b offset for each lane, applied to both x and y buffers. LSB apply to first lane
  xstep | Step between each column for selection in the x and y buffers. Ystep is symmetric to xstep (ystep advances by -xstep).
  ystart | Starting position offset applied to all lanes for input from Y buffer.
  zbuff | Input buffer of 8 elements of type cint16
  zstart | Starting position offset applied to all lanes for input from Z buffer. This must be a compile time constant. Only the 4 LSB of the argument are used.
  zoffsets | 4b offset for each lane, applied to input from Z buffer. LSB apply to first lane
  zstep | Step between each column for selection in the zbuffer.

Note
  - For more information on how data selection works from the buffers go here. The data buffer and coefficient buffer in this intrinsic use the general scheme.
  - Parameter 'zstart' must be a compile time constant.

## ◆ negmul4_min() [1/3]

v4cacc48 negmul4_min | ( | v32int16 | xbuff,
|  | int | xstart,
|  | unsigned int | xoffsets,
|  | int | xstep,
|  | int | ystart,
|  | v8cint16 | zbuff,
|  | int | zstart,
|  | unsigned int | zoffsets,
|  | int | zstep )

Complex multiply-negate intrinsic function after computing the minimum between the selected lanes from the input buffer using small X input buffer.

acc0 = -( z00*(min(x00 , y00)) + z01*(min(x01 , y01)) + z02*(min(x02 , y02)) + z03*(min(x03 , y03)) )
acc1 = -( z10*(min(x10 , y10)) + z11*(min(x11 , y11)) + z12*(min(x12 , y12)) + z13*(min(x13 , y13)) )
acc2 = -( z20*(min(x20 , y20)) + z21*(min(x21 , y21)) + z22*(min(x22 , y22)) + z23*(min(x23 , y23)) )
acc3 = -( z30*(min(x30 , y30)) + z31*(min(x31 , y31)) + z32*(min(x32 , y32)) + z33*(min(x33 , y33)) )

Returns
  Returned accumulation vector (4 x cint48 lanes)

Parameters

  xbuff | Input buffer of 32 elements of type int16
  xstart | Starting position offset applied to all lanes of input from X buffer.
  xoffsets | 4b offset for each lane, applied to both x and y buffers. LSB apply to first lane
  xstep | Step between each column for selection in the x and y buffers. Ystep is symmetric to xstep (ystep advances by -xstep).
  ystart | Starting position offset applied to all lanes for input from Y buffer.
  zbuff | Input buffer of 8 elements of type cint16
  zstart | Starting position offset applied to all lanes for input from Z buffer. This must be a compile time constant. Only the 4 LSB of the argument are used.
  zoffsets | 4b offset for each lane, applied to input from Z buffer. LSB apply to first lane
  zstep | Step between each column for selection in the zbuffer.

Note
  - For more information on how data selection works from the buffers go here. The data buffer and coefficient buffer in this intrinsic use the general scheme.
  - Parameter 'zstart' must be a compile time constant.

## ◆ negmul4_min() [2/3]

v4cacc48 negmul4_min | ( | v32int16 | xbuff,
|  | int | xstart,
|  | unsigned int | xoffsets,
|  | int | xstep,
|  | v32int16 | ybuff,
|  | int | ystart,
|  | v8cint16 | zbuff,
|  | int | zstart,
|  | unsigned int | zoffsets,
|  | int | zstep )

Complex multiply-negate intrinsic function after computing the minimum between the selected lanes from the input buffer using small X input buffer.

acc0 = -( z00*(min(x00 , y00)) + z01*(min(x01 , y01)) + z02*(min(x02 , y02)) + z03*(min(x03 , y03)) )
acc1 = -( z10*(min(x10 , y10)) + z11*(min(x11 , y11)) + z12*(min(x12 , y12)) + z13*(min(x13 , y13)) )
acc2 = -( z20*(min(x20 , y20)) + z21*(min(x21 , y21)) + z22*(min(x22 , y22)) + z23*(min(x23 , y23)) )
acc3 = -( z30*(min(x30 , y30)) + z31*(min(x31 , y31)) + z32*(min(x32 , y32)) + z33*(min(x33 , y33)) )

Returns
  Returned accumulation vector (4 x cint48 lanes)

Parameters

  xbuff | Input buffer of 32 elements of type int16
  xstart | Starting position offset applied to all lanes of input from X buffer.
  xoffsets | 4b offset for each lane, applied to both x and y buffers. LSB apply to first lane
  xstep | Step between each column for selection in the x and y buffers. Ystep is symmetric to xstep (ystep advances by -xstep).
  ybuff | Right input buffer of 32 elements of type int16
  ystart | Starting position offset applied to all lanes for input from Y buffer.
  zbuff | Input buffer of 8 elements of type cint16
  zstart | Starting position offset applied to all lanes for input from Z buffer. This must be a compile time constant. Only the 4 LSB of the argument are used.
  zoffsets | 4b offset for each lane, applied to input from Z buffer. LSB apply to first lane
  zstep | Step between each column for selection in the zbuffer.

Note
  - For more information on how data selection works from the buffers go here. The data buffer and coefficient buffer in this intrinsic use the general scheme.
  - Parameter 'zstart' must be a compile time constant.

## ◆ negmul4_min() [3/3]

v4cacc48 negmul4_min | ( | v64int16 | xbuff,
|  | int | xstart,
|  | unsigned int | xoffsets,
|  | int | xstep,
|  | int | ystart,
|  | v8cint16 | zbuff,
|  | int | zstart,
|  | unsigned int | zoffsets,
|  | int | zstep )

Complex multiply-negate intrinsic function after computing the minimum between the selected lanes from the input buffer .

acc0 = -( z00*(min(x00 , y00)) + z01*(min(x01 , y01)) + z02*(min(x02 , y02)) + z03*(min(x03 , y03)) )
acc1 = -( z10*(min(x10 , y10)) + z11*(min(x11 , y11)) + z12*(min(x12 , y12)) + z13*(min(x13 , y13)) )
acc2 = -( z20*(min(x20 , y20)) + z21*(min(x21 , y21)) + z22*(min(x22 , y22)) + z23*(min(x23 , y23)) )
acc3 = -( z30*(min(x30 , y30)) + z31*(min(x31 , y31)) + z32*(min(x32 , y32)) + z33*(min(x33 , y33)) )

Returns
  Returned accumulation vector (4 x cint48 lanes)

Parameters

  xbuff | Input buffer of 64 elements of type int16
  xstart | Starting position offset applied to all lanes of input from X buffer.
  xoffsets | 4b offset for each lane, applied to both x and y buffers. LSB apply to first lane
  xstep | Step between each column for selection in the x and y buffers. Ystep is symmetric to xstep (ystep advances by -xstep).
  ystart | Starting position offset applied to all lanes for input from Y buffer.
  zbuff | Input buffer of 8 elements of type cint16
  zstart | Starting position offset applied to all lanes for input from Z buffer. This must be a compile time constant. Only the 4 LSB of the argument are used.
  zoffsets | 4b offset for each lane, applied to input from Z buffer. LSB apply to first lane
  zstep | Step between each column for selection in the zbuffer.

Note
  - For more information on how data selection works from the buffers go here. The data buffer and coefficient buffer in this intrinsic use the general scheme.
  - Parameter 'zstart' must be a compile time constant.

## ◆ negmul8_abs() [1/2]

v8cacc48 negmul8_abs | ( | v32int16 | xbuff,
|  | int | xstart,
|  | unsigned int | xoffsets,
|  | int | xstep,
|  | v8cint16 | zbuff,
|  | int | zstart,
|  | unsigned int | zoffsets,
|  | int | zstep )

Complex multiply-negate intrinsic function after computing the absolute value in the selected lanes from the input buffer using small X input buffer.

acc0 = -( z00*abs(x00) + z01*abs(x01) )
acc1 = -( z10*abs(x10) + z11*abs(x11) )
acc2 = -( z20*abs(x20) + z21*abs(x21) )
acc3 = -( z30*abs(x30) + z31*abs(x31) )
acc4 = -( z40*abs(x40) + z41*abs(x41) )
acc5 = -( z50*abs(x50) + z51*abs(x51) )
acc6 = -( z60*abs(x60) + z61*abs(x61) )
acc7 = -( z70*abs(x70) + z71*abs(x71) )

Returns
  Returned accumulation vector (8 x cint48 lanes)

Parameters

  xbuff | Input buffer of 32 elements of type int16
  xstart | Starting position offset applied to all lanes of input from X buffer.
  xoffsets | 4b offset for each lane, applied to the x buffer. LSB apply to first lane
  xstep | Step between each column for selection in the xbuffer.
  zbuff | Input buffer of 8 elements of type cint16
  zstart | Starting position offset applied to all lanes for input from Z buffer. This must be a compile time constant. Only the 4 LSB of the argument are used.
  zoffsets | 4b offset for each lane, applied to input from Z buffer. LSB apply to first lane
  zstep | Step between each column for selection in the zbuffer.

Note
  - For more information on how data selection works from the buffers go here. The data buffer and coefficient buffer in this intrinsic use the general scheme.
  - Parameter 'zstart' must be a compile time constant.

## ◆ negmul8_abs() [2/2]

v8cacc48 negmul8_abs | ( | v64int16 | xbuff,
|  | int | xstart,
|  | unsigned int | xoffsets,
|  | int | xstep,
|  | v8cint16 | zbuff,
|  | int | zstart,
|  | unsigned int | zoffsets,
|  | int | zstep )

Complex multiply-negate intrinsic function after computing the absolute value in the selected lanes from the input buffer .

acc0 = -( z00*abs(x00) + z01*abs(x01) )
acc1 = -( z10*abs(x10) + z11*abs(x11) )
acc2 = -( z20*abs(x20) + z21*abs(x21) )
acc3 = -( z30*abs(x30) + z31*abs(x31) )
acc4 = -( z40*abs(x40) + z41*abs(x41) )
acc5 = -( z50*abs(x50) + z51*abs(x51) )
acc6 = -( z60*abs(x60) + z61*abs(x61) )
acc7 = -( z70*abs(x70) + z71*abs(x71) )

Returns
  Returned accumulation vector (8 x cint48 lanes)

Parameters

  xbuff | Input buffer of 64 elements of type int16
  xstart | Starting position offset applied to all lanes of input from X buffer.
  xoffsets | 4b offset for each lane, applied to the x buffer. LSB apply to first lane
  xstep | Step between each column for selection in the xbuffer.
  zbuff | Input buffer of 8 elements of type cint16
  zstart | Starting position offset applied to all lanes for input from Z buffer. This must be a compile time constant. Only the 4 LSB of the argument are used.
  zoffsets | 4b offset for each lane, applied to input from Z buffer. LSB apply to first lane
  zstep | Step between each column for selection in the zbuffer.

Note
  - For more information on how data selection works from the buffers go here. The data buffer and coefficient buffer in this intrinsic use the general scheme.
  - Parameter 'zstart' must be a compile time constant.

## ◆ negmul8_max() [1/3]

v8cacc48 negmul8_max | ( | v32int16 | xbuff,
|  | int | xstart,
|  | unsigned int | xoffsets,
|  | int | xstep,
|  | int | ystart,
|  | v8cint16 | zbuff,
|  | int | zstart,
|  | unsigned int | zoffsets,
|  | int | zstep )

Complex multiply-negate intrinsic function after computing the maximum between the selected lanes from the input buffer using small X input buffer.

acc0 = -( z00*(max(x00 , y00)) + z01*(max(x01 , y01)) )
acc1 = -( z10*(max(x10 , y10)) + z11*(max(x11 , y11)) )
acc2 = -( z20*(max(x20 , y20)) + z21*(max(x21 , y21)) )
acc3 = -( z30*(max(x30 , y30)) + z31*(max(x31 , y31)) )
acc4 = -( z40*(max(x40 , y40)) + z41*(max(x41 , y41)) )
acc5 = -( z50*(max(x50 , y50)) + z51*(max(x51 , y51)) )
acc6 = -( z60*(max(x60 , y60)) + z61*(max(x61 , y61)) )
acc7 = -( z70*(max(x70 , y70)) + z71*(max(x71 , y71)) )

Returns
  Returned accumulation vector (8 x cint48 lanes)

Parameters

  xbuff | Input buffer of 32 elements of type int16
  xstart | Starting position offset applied to all lanes of input from X buffer.
  xoffsets | 4b offset for each lane, applied to both x and y buffers. LSB apply to first lane
  xstep | Step between each column for selection in the x and y buffers. Ystep is symmetric to xstep (ystep advances by -xstep).
  ystart | Starting position offset applied to all lanes for input from Y buffer.
  zbuff | Input buffer of 8 elements of type cint16
  zstart | Starting position offset applied to all lanes for input from Z buffer. This must be a compile time constant. Only the 4 LSB of the argument are used.
  zoffsets | 4b offset for each lane, applied to input from Z buffer. LSB apply to first lane
  zstep | Step between each column for selection in the zbuffer.

Note
  - For more information on how data selection works from the buffers go here. The data buffer and coefficient buffer in this intrinsic use the general scheme.
  - Parameter 'zstart' must be a compile time constant.

## ◆ negmul8_max() [2/3]

v8cacc48 negmul8_max | ( | v32int16 | xbuff,
|  | int | xstart,
|  | unsigned int | xoffsets,
|  | int | xstep,
|  | v32int16 | ybuff,
|  | int | ystart,
|  | v8cint16 | zbuff,
|  | int | zstart,
|  | unsigned int | zoffsets,
|  | int | zstep )

Complex multiply-negate intrinsic function after computing the maximum between the selected lanes from the input buffer using small X input buffer.

acc0 = -( z00*(max(x00 , y00)) + z01*(max(x01 , y01)) )
acc1 = -( z10*(max(x10 , y10)) + z11*(max(x11 , y11)) )
acc2 = -( z20*(max(x20 , y20)) + z21*(max(x21 , y21)) )
acc3 = -( z30*(max(x30 , y30)) + z31*(max(x31 , y31)) )
acc4 = -( z40*(max(x40 , y40)) + z41*(max(x41 , y41)) )
acc5 = -( z50*(max(x50 , y50)) + z51*(max(x51 , y51)) )
acc6 = -( z60*(max(x60 , y60)) + z61*(max(x61 , y61)) )
acc7 = -( z70*(max(x70 , y70)) + z71*(max(x71 , y71)) )

Returns
  Returned accumulation vector (8 x cint48 lanes)

Parameters

  xbuff | Input buffer of 32 elements of type int16
  xstart | Starting position offset applied to all lanes of input from X buffer.
  xoffsets | 4b offset for each lane, applied to both x and y buffers. LSB apply to first lane
  xstep | Step between each column for selection in the x and y buffers. Ystep is symmetric to xstep (ystep advances by -xstep).
  ybuff | Right input buffer of 32 elements of type int16
  ystart | Starting position offset applied to all lanes for input from Y buffer.
  zbuff | Input buffer of 8 elements of type cint16
  zstart | Starting position offset applied to all lanes for input from Z buffer. This must be a compile time constant. Only the 4 LSB of the argument are used.
  zoffsets | 4b offset for each lane, applied to input from Z buffer. LSB apply to first lane
  zstep | Step between each column for selection in the zbuffer.

Note
  - For more information on how data selection works from the buffers go here. The data buffer and coefficient buffer in this intrinsic use the general scheme.
  - Parameter 'zstart' must be a compile time constant.

## ◆ negmul8_max() [3/3]

v8cacc48 negmul8_max | ( | v64int16 | xbuff,
|  | int | xstart,
|  | unsigned int | xoffsets,
|  | int | xstep,
|  | int | ystart,
|  | v8cint16 | zbuff,
|  | int | zstart,
|  | unsigned int | zoffsets,
|  | int | zstep )

Complex multiply-negate intrinsic function after computing the maximum between the selected lanes from the input buffer .

acc0 = -( z00*(max(x00 , y00)) + z01*(max(x01 , y01)) )
acc1 = -( z10*(max(x10 , y10)) + z11*(max(x11 , y11)) )
acc2 = -( z20*(max(x20 , y20)) + z21*(max(x21 , y21)) )
acc3 = -( z30*(max(x30 , y30)) + z31*(max(x31 , y31)) )
acc4 = -( z40*(max(x40 , y40)) + z41*(max(x41 , y41)) )
acc5 = -( z50*(max(x50 , y50)) + z51*(max(x51 , y51)) )
acc6 = -( z60*(max(x60 , y60)) + z61*(max(x61 , y61)) )
acc7 = -( z70*(max(x70 , y70)) + z71*(max(x71 , y71)) )

Returns
  Returned accumulation vector (8 x cint48 lanes)

Parameters

  xbuff | Input buffer of 64 elements of type int16
  xstart | Starting position offset applied to all lanes of input from X buffer.
  xoffsets | 4b offset for each lane, applied to both x and y buffers. LSB apply to first lane
  xstep | Step between each column for selection in the x and y buffers. Ystep is symmetric to xstep (ystep advances by -xstep).
  ystart | Starting position offset applied to all lanes for input from Y buffer.
  zbuff | Input buffer of 8 elements of type cint16
  zstart | Starting position offset applied to all lanes for input from Z buffer. This must be a compile time constant. Only the 4 LSB of the argument are used.
  zoffsets | 4b offset for each lane, applied to input from Z buffer. LSB apply to first lane
  zstep | Step between each column for selection in the zbuffer.

Note
  - For more information on how data selection works from the buffers go here. The data buffer and coefficient buffer in this intrinsic use the general scheme.
  - Parameter 'zstart' must be a compile time constant.

## ◆ negmul8_maxdiff() [1/3]

v8cacc48 negmul8_maxdiff | ( | v32int16 | xbuff,
|  | int | xstart,
|  | unsigned int | xoffsets,
|  | int | xstep,
|  | int | ystart,
|  | v8cint16 | zbuff,
|  | int | zstart,
|  | unsigned int | zoffsets,
|  | int | zstep )

Complex multiply-negate intrinsic function after computing the maximum difference between the selected lanes from the input buffer using small X input buffer.

acc0 = -( z00*((x00 - y00 > 0) ? (x00 - y00):0) + z01*((x01 - y01 > 0) ? (x01 - y01):0) )
acc1 = -( z10*((x10 - y10 > 0) ? (x10 - y10):0) + z11*((x11 - y11 > 0) ? (x11 - y11):0) )
acc2 = -( z20*((x20 - y20 > 0) ? (x20 - y20):0) + z21*((x21 - y21 > 0) ? (x21 - y21):0) )
acc3 = -( z30*((x30 - y30 > 0) ? (x30 - y30):0) + z31*((x31 - y31 > 0) ? (x31 - y31):0) )
acc4 = -( z40*((x40 - y40 > 0) ? (x40 - y40):0) + z41*((x41 - y41 > 0) ? (x41 - y41):0) )
acc5 = -( z50*((x50 - y50 > 0) ? (x50 - y50):0) + z51*((x51 - y51 > 0) ? (x51 - y51):0) )
acc6 = -( z60*((x60 - y60 > 0) ? (x60 - y60):0) + z61*((x61 - y61 > 0) ? (x61 - y61):0) )
acc7 = -( z70*((x70 - y70 > 0) ? (x70 - y70):0) + z71*((x71 - y71 > 0) ? (x71 - y71):0) )

Returns
  Returned accumulation vector (8 x cint48 lanes)

Parameters

  xbuff | Input buffer of 32 elements of type int16
  xstart | Starting position offset applied to all lanes of input from X buffer.
  xoffsets | 4b offset for each lane, applied to both x and y buffers. LSB apply to first lane
  xstep | Step between each column for selection in the x and y buffers. Ystep is symmetric to xstep (ystep advances by -xstep).
  ystart | Starting position offset applied to all lanes for input from Y buffer.
  zbuff | Input buffer of 8 elements of type cint16
  zstart | Starting position offset applied to all lanes for input from Z buffer. This must be a compile time constant. Only the 4 LSB of the argument are used.
  zoffsets | 4b offset for each lane, applied to input from Z buffer. LSB apply to first lane
  zstep | Step between each column for selection in the zbuffer.

Note
  - For more information on how data selection works from the buffers go here. The data buffer and coefficient buffer in this intrinsic use the general scheme.
  - Parameter 'zstart' must be a compile time constant.

## ◆ negmul8_maxdiff() [2/3]

v8cacc48 negmul8_maxdiff | ( | v32int16 | xbuff,
|  | int | xstart,
|  | unsigned int | xoffsets,
|  | int | xstep,
|  | v32int16 | ybuff,
|  | int | ystart,
|  | v8cint16 | zbuff,
|  | int | zstart,
|  | unsigned int | zoffsets,
|  | int | zstep )

Complex multiply-negate intrinsic function after computing the maximum difference between the selected lanes from the input buffer using small X input buffer.

acc0 = -( z00*((x00 - y00 > 0) ? (x00 - y00):0) + z01*((x01 - y01 > 0) ? (x01 - y01):0) )
acc1 = -( z10*((x10 - y10 > 0) ? (x10 - y10):0) + z11*((x11 - y11 > 0) ? (x11 - y11):0) )
acc2 = -( z20*((x20 - y20 > 0) ? (x20 - y20):0) + z21*((x21 - y21 > 0) ? (x21 - y21):0) )
acc3 = -( z30*((x30 - y30 > 0) ? (x30 - y30):0) + z31*((x31 - y31 > 0) ? (x31 - y31):0) )
acc4 = -( z40*((x40 - y40 > 0) ? (x40 - y40):0) + z41*((x41 - y41 > 0) ? (x41 - y41):0) )
acc5 = -( z50*((x50 - y50 > 0) ? (x50 - y50):0) + z51*((x51 - y51 > 0) ? (x51 - y51):0) )
acc6 = -( z60*((x60 - y60 > 0) ? (x60 - y60):0) + z61*((x61 - y61 > 0) ? (x61 - y61):0) )
acc7 = -( z70*((x70 - y70 > 0) ? (x70 - y70):0) + z71*((x71 - y71 > 0) ? (x71 - y71):0) )

Returns
  Returned accumulation vector (8 x cint48 lanes)

Parameters

  xbuff | Input buffer of 32 elements of type int16
  xstart | Starting position offset applied to all lanes of input from X buffer.
  xoffsets | 4b offset for each lane, applied to both x and y buffers. LSB apply to first lane
  xstep | Step between each column for selection in the x and y buffers. Ystep is symmetric to xstep (ystep advances by -xstep).
  ybuff | Right input buffer of 32 elements of type int16
  ystart | Starting position offset applied to all lanes for input from Y buffer.
  zbuff | Input buffer of 8 elements of type cint16
  zstart | Starting position offset applied to all lanes for input from Z buffer. This must be a compile time constant. Only the 4 LSB of the argument are used.
  zoffsets | 4b offset for each lane, applied to input from Z buffer. LSB apply to first lane
  zstep | Step between each column for selection in the zbuffer.

Note
  - For more information on how data selection works from the buffers go here. The data buffer and coefficient buffer in this intrinsic use the general scheme.
  - Parameter 'zstart' must be a compile time constant.

## ◆ negmul8_maxdiff() [3/3]

v8cacc48 negmul8_maxdiff | ( | v64int16 | xbuff,
|  | int | xstart,
|  | unsigned int | xoffsets,
|  | int | xstep,
|  | int | ystart,
|  | v8cint16 | zbuff,
|  | int | zstart,
|  | unsigned int | zoffsets,
|  | int | zstep )

Complex multiply-negate intrinsic function after computing the maximum difference between the selected lanes from the input buffer .

acc0 = -( z00*((x00 - y00 > 0) ? (x00 - y00):0) + z01*((x01 - y01 > 0) ? (x01 - y01):0) )
acc1 = -( z10*((x10 - y10 > 0) ? (x10 - y10):0) + z11*((x11 - y11 > 0) ? (x11 - y11):0) )
acc2 = -( z20*((x20 - y20 > 0) ? (x20 - y20):0) + z21*((x21 - y21 > 0) ? (x21 - y21):0) )
acc3 = -( z30*((x30 - y30 > 0) ? (x30 - y30):0) + z31*((x31 - y31 > 0) ? (x31 - y31):0) )
acc4 = -( z40*((x40 - y40 > 0) ? (x40 - y40):0) + z41*((x41 - y41 > 0) ? (x41 - y41):0) )
acc5 = -( z50*((x50 - y50 > 0) ? (x50 - y50):0) + z51*((x51 - y51 > 0) ? (x51 - y51):0) )
acc6 = -( z60*((x60 - y60 > 0) ? (x60 - y60):0) + z61*((x61 - y61 > 0) ? (x61 - y61):0) )
acc7 = -( z70*((x70 - y70 > 0) ? (x70 - y70):0) + z71*((x71 - y71 > 0) ? (x71 - y71):0) )

Returns
  Returned accumulation vector (8 x cint48 lanes)

Parameters

  xbuff | Input buffer of 64 elements of type int16
  xstart | Starting position offset applied to all lanes of input from X buffer.
  xoffsets | 4b offset for each lane, applied to both x and y buffers. LSB apply to first lane
  xstep | Step between each column for selection in the x and y buffers. Ystep is symmetric to xstep (ystep advances by -xstep).
  ystart | Starting position offset applied to all lanes for input from Y buffer.
  zbuff | Input buffer of 8 elements of type cint16
  zstart | Starting position offset applied to all lanes for input from Z buffer. This must be a compile time constant. Only the 4 LSB of the argument are used.
  zoffsets | 4b offset for each lane, applied to input from Z buffer. LSB apply to first lane
  zstep | Step between each column for selection in the zbuffer.

Note
  - For more information on how data selection works from the buffers go here. The data buffer and coefficient buffer in this intrinsic use the general scheme.
  - Parameter 'zstart' must be a compile time constant.

## ◆ negmul8_min() [1/3]

v8cacc48 negmul8_min | ( | v32int16 | xbuff,
|  | int | xstart,
|  | unsigned int | xoffsets,
|  | int | xstep,
|  | int | ystart,
|  | v8cint16 | zbuff,
|  | int | zstart,
|  | unsigned int | zoffsets,
|  | int | zstep )

Complex multiply-negate intrinsic function after computing the minimum between the selected lanes from the input buffer using small X input buffer.

acc0 = -( z00*(min(x00 , y00)) + z01*(min(x01 , y01)) )
acc1 = -( z10*(min(x10 , y10)) + z11*(min(x11 , y11)) )
acc2 = -( z20*(min(x20 , y20)) + z21*(min(x21 , y21)) )
acc3 = -( z30*(min(x30 , y30)) + z31*(min(x31 , y31)) )
acc4 = -( z40*(min(x40 , y40)) + z41*(min(x41 , y41)) )
acc5 = -( z50*(min(x50 , y50)) + z51*(min(x51 , y51)) )
acc6 = -( z60*(min(x60 , y60)) + z61*(min(x61 , y61)) )
acc7 = -( z70*(min(x70 , y70)) + z71*(min(x71 , y71)) )

Returns
  Returned accumulation vector (8 x cint48 lanes)

Parameters

  xbuff | Input buffer of 32 elements of type int16
  xstart | Starting position offset applied to all lanes of input from X buffer.
  xoffsets | 4b offset for each lane, applied to both x and y buffers. LSB apply to first lane
  xstep | Step between each column for selection in the x and y buffers. Ystep is symmetric to xstep (ystep advances by -xstep).
  ystart | Starting position offset applied to all lanes for input from Y buffer.
  zbuff | Input buffer of 8 elements of type cint16
  zstart | Starting position offset applied to all lanes for input from Z buffer. This must be a compile time constant. Only the 4 LSB of the argument are used.
  zoffsets | 4b offset for each lane, applied to input from Z buffer. LSB apply to first lane
  zstep | Step between each column for selection in the zbuffer.

Note
  - For more information on how data selection works from the buffers go here. The data buffer and coefficient buffer in this intrinsic use the general scheme.
  - Parameter 'zstart' must be a compile time constant.

## ◆ negmul8_min() [2/3]

v8cacc48 negmul8_min | ( | v32int16 | xbuff,
|  | int | xstart,
|  | unsigned int | xoffsets,
|  | int | xstep,
|  | v32int16 | ybuff,
|  | int | ystart,
|  | v8cint16 | zbuff,
|  | int | zstart,
|  | unsigned int | zoffsets,
|  | int | zstep )

Complex multiply-negate intrinsic function after computing the minimum between the selected lanes from the input buffer using small X input buffer.

acc0 = -( z00*(min(x00 , y00)) + z01*(min(x01 , y01)) )
acc1 = -( z10*(min(x10 , y10)) + z11*(min(x11 , y11)) )
acc2 = -( z20*(min(x20 , y20)) + z21*(min(x21 , y21)) )
acc3 = -( z30*(min(x30 , y30)) + z31*(min(x31 , y31)) )
acc4 = -( z40*(min(x40 , y40)) + z41*(min(x41 , y41)) )
acc5 = -( z50*(min(x50 , y50)) + z51*(min(x51 , y51)) )
acc6 = -( z60*(min(x60 , y60)) + z61*(min(x61 , y61)) )
acc7 = -( z70*(min(x70 , y70)) + z71*(min(x71 , y71)) )

Returns
  Returned accumulation vector (8 x cint48 lanes)

Parameters

  xbuff | Input buffer of 32 elements of type int16
  xstart | Starting position offset applied to all lanes of input from X buffer.
  xoffsets | 4b offset for each lane, applied to both x and y buffers. LSB apply to first lane
  xstep | Step between each column for selection in the x and y buffers. Ystep is symmetric to xstep (ystep advances by -xstep).
  ybuff | Right input buffer of 32 elements of type int16
  ystart | Starting position offset applied to all lanes for input from Y buffer.
  zbuff | Input buffer of 8 elements of type cint16
  zstart | Starting position offset applied to all lanes for input from Z buffer. This must be a compile time constant. Only the 4 LSB of the argument are used.
  zoffsets | 4b offset for each lane, applied to input from Z buffer. LSB apply to first lane
  zstep | Step between each column for selection in the zbuffer.

Note
  - For more information on how data selection works from the buffers go here. The data buffer and coefficient buffer in this intrinsic use the general scheme.
  - Parameter 'zstart' must be a compile time constant.

## ◆ negmul8_min() [3/3]

v8cacc48 negmul8_min | ( | v64int16 | xbuff,
|  | int | xstart,
|  | unsigned int | xoffsets,
|  | int | xstep,
|  | int | ystart,
|  | v8cint16 | zbuff,
|  | int | zstart,
|  | unsigned int | zoffsets,
|  | int | zstep )

Complex multiply-negate intrinsic function after computing the minimum between the selected lanes from the input buffer .

acc0 = -( z00*(min(x00 , y00)) + z01*(min(x01 , y01)) )
acc1 = -( z10*(min(x10 , y10)) + z11*(min(x11 , y11)) )
acc2 = -( z20*(min(x20 , y20)) + z21*(min(x21 , y21)) )
acc3 = -( z30*(min(x30 , y30)) + z31*(min(x31 , y31)) )
acc4 = -( z40*(min(x40 , y40)) + z41*(min(x41 , y41)) )
acc5 = -( z50*(min(x50 , y50)) + z51*(min(x51 , y51)) )
acc6 = -( z60*(min(x60 , y60)) + z61*(min(x61 , y61)) )
acc7 = -( z70*(min(x70 , y70)) + z71*(min(x71 , y71)) )

Returns
  Returned accumulation vector (8 x cint48 lanes)

Parameters

  xbuff | Input buffer of 64 elements of type int16
  xstart | Starting position offset applied to all lanes of input from X buffer.
  xoffsets | 4b offset for each lane, applied to both x and y buffers. LSB apply to first lane
  xstep | Step between each column for selection in the x and y buffers. Ystep is symmetric to xstep (ystep advances by -xstep).
  ystart | Starting position offset applied to all lanes for input from Y buffer.
  zbuff | Input buffer of 8 elements of type cint16
  zstart | Starting position offset applied to all lanes for input from Z buffer. This must be a compile time constant. Only the 4 LSB of the argument are used.
  zoffsets | 4b offset for each lane, applied to input from Z buffer. LSB apply to first lane
  zstep | Step between each column for selection in the zbuffer.

Note
  - For more information on how data selection works from the buffers go here. The data buffer and coefficient buffer in this intrinsic use the general scheme.
  - Parameter 'zstart' must be a compile time constant.