| AI Engine-ML v2 Intrinsics User Guide (v2026.1)

Loading...
Searching...
No Matches
Stream write
Load/Store Operations » Streams

## Packet headers
These intrinsics are designed to facilitate the headers creation. They write directly to a stream
void | put_ms_packet_header (int tlast, unsigned dstID, unsigned pcktType)
| Generate a packet header and write to it to the output stream port.
void | put_ms_packet_header (unsigned dstID, unsigned pcktType)
| Generate a packet header and write to it to the output stream port.
void | put_ms_nb_packet_header (int tlast, unsigned dstID, unsigned pcktType, bool &success)
| Generate a packet header and write to it to the output stream port.
void | put_ms_nb_packet_header (unsigned dstID, unsigned pcktType, bool &success)
| Generate a packet header and write to it to the output stream port.
void | put_ms_ctrl_packet_header (int tlast, unsigned Addr, unsigned n_words, unsigned op_type, unsigned rspID)
| Generate a control packet header and write it to the output stream port.
void | put_ms_ctrl_packet_header (unsigned Addr, unsigned n_words, unsigned op_type, unsigned rspID)
| Generate a control packet header and write it to the output stream port.
void | put_ms_nb_ctrl_packet_header (int tlast, unsigned Addr, unsigned n_words, unsigned op_type, unsigned rspID, bool &success)
| Generate a control packet header and write it to the output stream port.
void | put_ms_nb_ctrl_packet_header (unsigned Addr, unsigned n_words, unsigned op_type, unsigned rspID, bool &success)
| Generate a control packet header and write it to the output stream port.

## Packet headers (deprecated)
These intrinsics are designed to facilitate the headers creation. They do not write directly to a stream and should always be combined with a "put_ms" call.
unsigned int | packet_header (unsigned dstID, unsigned pcktType)
| Generate a packet header.
unsigned int | ctrl_packet_header (unsigned Addr, unsigned n_words, unsigned op_type, unsigned rspID)
| Generate a control packet header.

## Write Single word to 32-bit streams
void | put_ms (int val)
| Write a 32-bit value to the output stream port.
void | put_ms (int val, int tlast)
| Write a 32-bit value to the output stream port. Non-blocking read.
void | put_ms_nb (int val, int tlast, bool &success)
| Write a 32-bit value to the output stream port. Non-blocking read.
void | put_ms_nb (int val, bool &success)
| Write a 32-bit value to the output stream port. Non-blocking read.
void | put_ms (int val, int en, int tlast)
| Write a 32-bit value to the output stream port.
void | put_ms (unsigned int val)
| Write a 32-bit value to the output stream port.
void | put_ms (unsigned int val, int tlast)
| Write a 32-bit value to the output stream port. Non-blocking read.
void | put_ms_nb (unsigned int val, int tlast, bool &success)
| Write a 32-bit value to the output stream port. Non-blocking read.
void | put_ms_nb (unsigned int val, bool &success)
| Write a 32-bit value to the output stream port. Non-blocking read.
void | put_ms (unsigned int val, int en, int tlast)
| Write a 32-bit value to the output stream port.
void | put_ms (float val)
| Write a 32-bit value to the output stream port.
void | put_ms (float val, int tlast)
| Write a 32-bit value to the output stream port. Non-blocking read.
void | put_ms_nb (float val, int tlast, bool &success)
| Write a 32-bit value to the output stream port. Non-blocking read.
void | put_ms_nb (float val, bool &success)
| Write a 32-bit value to the output stream port. Non-blocking read.
void | put_ms (float val, int en, int tlast)
| Write a 32-bit value to the output stream port.
void | put_ms (v8int4 val)
| Write a 32-bit value to the output stream port.
void | put_ms (v8int4 val, int tlast)
| Write a 32-bit value to the output stream port. Non-blocking read.
void | put_ms_nb (v8int4 val, int tlast, bool &success)
| Write a 32-bit value to the output stream port. Non-blocking read.
void | put_ms_nb (v8int4 val, bool &success)
| Write a 32-bit value to the output stream port. Non-blocking read.
void | put_ms (v8int4 val, int en, int tlast)
| Write a 32-bit value to the output stream port.
void | put_ms (v8uint4 val)
| Write a 32-bit value to the output stream port.
void | put_ms (v8uint4 val, int tlast)
| Write a 32-bit value to the output stream port. Non-blocking read.
void | put_ms_nb (v8uint4 val, int tlast, bool &success)
| Write a 32-bit value to the output stream port. Non-blocking read.
void | put_ms_nb (v8uint4 val, bool &success)
| Write a 32-bit value to the output stream port. Non-blocking read.
void | put_ms (v8uint4 val, int en, int tlast)
| Write a 32-bit value to the output stream port.
void | put_ms (v4int8 val)
| Write a 32-bit value to the output stream port.
void | put_ms (v4int8 val, int tlast)
| Write a 32-bit value to the output stream port. Non-blocking read.
void | put_ms_nb (v4int8 val, int tlast, bool &success)
| Write a 32-bit value to the output stream port. Non-blocking read.
void | put_ms_nb (v4int8 val, bool &success)
| Write a 32-bit value to the output stream port. Non-blocking read.
void | put_ms (v4int8 val, int en, int tlast)
| Write a 32-bit value to the output stream port.
void | put_ms (v4uint8 val)
| Write a 32-bit value to the output stream port.
void | put_ms (v4uint8 val, int tlast)
| Write a 32-bit value to the output stream port. Non-blocking read.
void | put_ms_nb (v4uint8 val, int tlast, bool &success)
| Write a 32-bit value to the output stream port. Non-blocking read.
void | put_ms_nb (v4uint8 val, bool &success)
| Write a 32-bit value to the output stream port. Non-blocking read.
void | put_ms (v4uint8 val, int en, int tlast)
| Write a 32-bit value to the output stream port.
void | put_ms (v2int16 val)
| Write a 32-bit value to the output stream port.
void | put_ms (v2int16 val, int tlast)
| Write a 32-bit value to the output stream port. Non-blocking read.
void | put_ms_nb (v2int16 val, int tlast, bool &success)
| Write a 32-bit value to the output stream port. Non-blocking read.
void | put_ms_nb (v2int16 val, bool &success)
| Write a 32-bit value to the output stream port. Non-blocking read.
void | put_ms (v2int16 val, int en, int tlast)
| Write a 32-bit value to the output stream port.
void | put_ms (v2uint16 val)
| Write a 32-bit value to the output stream port.
void | put_ms (v2uint16 val, int tlast)
| Write a 32-bit value to the output stream port. Non-blocking read.
void | put_ms_nb (v2uint16 val, int tlast, bool &success)
| Write a 32-bit value to the output stream port. Non-blocking read.
void | put_ms_nb (v2uint16 val, bool &success)
| Write a 32-bit value to the output stream port. Non-blocking read.
void | put_ms (v2uint16 val, int en, int tlast)
| Write a 32-bit value to the output stream port.
void | put_ms (cint16 val)
| Write a 32-bit value to the output stream port.
void | put_ms (cint16 val, int tlast)
| Write a 32-bit value to the output stream port. Non-blocking read.
void | put_ms_nb (cint16 val, int tlast, bool &success)
| Write a 32-bit value to the output stream port. Non-blocking read.
void | put_ms_nb (cint16 val, bool &success)
| Write a 32-bit value to the output stream port. Non-blocking read.
void | put_ms (cint16 val, int en, int tlast)
| Write a 32-bit value to the output stream port.
void | put_ms (v2bfloat16 val)
| Write a 32-bit value to the output stream port.
void | put_ms (v2bfloat16 val, int tlast)
| Write a 32-bit value to the output stream port. Non-blocking read.
void | put_ms_nb (v2bfloat16 val, int tlast, bool &success)
| Write a 32-bit value to the output stream port. Non-blocking read.
void | put_ms_nb (v2bfloat16 val, bool &success)
| Write a 32-bit value to the output stream port. Non-blocking read.
void | put_ms (v2bfloat16 val, int en, int tlast)
| Write a 32-bit value to the output stream port.
void | put_ms (v2float16 val)
| Write a 32-bit value to the output stream port.
void | put_ms (v2float16 val, int tlast)
| Write a 32-bit value to the output stream port. Non-blocking read.
void | put_ms_nb (v2float16 val, int tlast, bool &success)
| Write a 32-bit value to the output stream port. Non-blocking read.
void | put_ms_nb (v2float16 val, bool &success)
| Write a 32-bit value to the output stream port. Non-blocking read.
void | put_ms (v2float16 val, int en, int tlast)
| Write a 32-bit value to the output stream port.

## Write 128-bit vector to 32-bit streams
void | put_ms (v4int32 a, int tlast)
| Write a 128-bit vector value to the output stream port.
void | put_ms (v4int32 a, int en, int tlast)
| Write a 128-bit vector value to the output stream port.
void | put_ms (v32int4 a, int tlast)
| Write a 128-bit vector value to the output stream port.
void | put_ms (v32int4 a, int en, int tlast)
| Write a 128-bit vector value to the output stream port.
void | put_ms (v32uint4 a, int tlast)
| Write a 128-bit vector value to the output stream port.
void | put_ms (v32uint4 a, int en, int tlast)
| Write a 128-bit vector value to the output stream port.
void | put_ms (v16int8 a, int tlast)
| Write a 128-bit vector value to the output stream port.
void | put_ms (v16int8 a, int en, int tlast)
| Write a 128-bit vector value to the output stream port.
void | put_ms (v16uint8 a, int tlast)
| Write a 128-bit vector value to the output stream port.
void | put_ms (v16uint8 a, int en, int tlast)
| Write a 128-bit vector value to the output stream port.
void | put_ms (v8int16 a, int tlast)
| Write a 128-bit vector value to the output stream port.
void | put_ms (v8int16 a, int en, int tlast)
| Write a 128-bit vector value to the output stream port.
void | put_ms (v8uint16 a, int tlast)
| Write a 128-bit vector value to the output stream port.
void | put_ms (v8uint16 a, int en, int tlast)
| Write a 128-bit vector value to the output stream port.
void | put_ms (v4cint16 a, int tlast)
| Write a 128-bit vector value to the output stream port.
void | put_ms (v4cint16 a, int en, int tlast)
| Write a 128-bit vector value to the output stream port.
void | put_ms (v4uint32 a, int tlast)
| Write a 128-bit vector value to the output stream port.
void | put_ms (v4uint32 a, int en, int tlast)
| Write a 128-bit vector value to the output stream port.
void | put_ms (v2cint32 a, int tlast)
| Write a 128-bit vector value to the output stream port.
void | put_ms (v2cint32 a, int en, int tlast)
| Write a 128-bit vector value to the output stream port.
void | put_ms (v2cfloat a, int tlast)
| Write a 128-bit vector value to the output stream port.
void | put_ms (v2cfloat a, int en, int tlast)
| Write a 128-bit vector value to the output stream port.
void | put_ms (v4cbfloat16 a, int tlast)
| Write a 128-bit vector value to the output stream port.
void | put_ms (v4cbfloat16 a, int en, int tlast)
| Write a 128-bit vector value to the output stream port.
void | put_ms (v8bfloat16 a, int tlast)
| Write a 128-bit vector value to the output stream port.
void | put_ms (v8bfloat16 a, int en, int tlast)
| Write a 128-bit vector value to the output stream port.
void | put_ms (v8float16 a, int tlast)
| Write a 128-bit vector value to the output stream port.
void | put_ms (v8float16 a, int en, int tlast)
| Write a 128-bit vector value to the output stream port.
void | put_ms (v4float a, int tlast)
| Write a 128-bit vector value to the output stream port.
void | put_ms (v4float a, int en, int tlast)
| Write a 128-bit vector value to the output stream port.

## Write 256-bit vector to 32-bit streams
void | put_ms (v8int32 a, int tlast)
| Write a 256-bit vector value to the output stream port.
void | put_ms (v8int32 a, int en, int tlast)
| Write a 256-bit vector value to the output stream port.
void | put_ms (v64int4 a, int tlast)
| Write a 256-bit vector value to the output stream port.
void | put_ms (v64int4 a, int en, int tlast)
| Write a 256-bit vector value to the output stream port.
void | put_ms (v64uint4 a, int tlast)
| Write a 256-bit vector value to the output stream port.
void | put_ms (v64uint4 a, int en, int tlast)
| Write a 256-bit vector value to the output stream port.
void | put_ms (v32int8 a, int tlast)
| Write a 256-bit vector value to the output stream port.
void | put_ms (v32int8 a, int en, int tlast)
| Write a 256-bit vector value to the output stream port.
void | put_ms (v32uint8 a, int tlast)
| Write a 256-bit vector value to the output stream port.
void | put_ms (v32uint8 a, int en, int tlast)
| Write a 256-bit vector value to the output stream port.
void | put_ms (v16int16 a, int tlast)
| Write a 256-bit vector value to the output stream port.
void | put_ms (v16int16 a, int en, int tlast)
| Write a 256-bit vector value to the output stream port.
void | put_ms (v16uint16 a, int tlast)
| Write a 256-bit vector value to the output stream port.
void | put_ms (v16uint16 a, int en, int tlast)
| Write a 256-bit vector value to the output stream port.
void | put_ms (v8cint16 a, int tlast)
| Write a 256-bit vector value to the output stream port.
void | put_ms (v8cint16 a, int en, int tlast)
| Write a 256-bit vector value to the output stream port.
void | put_ms (v8uint32 a, int tlast)
| Write a 256-bit vector value to the output stream port.
void | put_ms (v8uint32 a, int en, int tlast)
| Write a 256-bit vector value to the output stream port.
void | put_ms (v4cint32 a, int tlast)
| Write a 256-bit vector value to the output stream port.
void | put_ms (v4cint32 a, int en, int tlast)
| Write a 256-bit vector value to the output stream port.
void | put_ms (v4cfloat a, int tlast)
| Write a 256-bit vector value to the output stream port.
void | put_ms (v4cfloat a, int en, int tlast)
| Write a 256-bit vector value to the output stream port.
void | put_ms (v8cbfloat16 a, int tlast)
| Write a 256-bit vector value to the output stream port.
void | put_ms (v8cbfloat16 a, int en, int tlast)
| Write a 256-bit vector value to the output stream port.
void | put_ms (v16bfloat16 a, int tlast)
| Write a 256-bit vector value to the output stream port.
void | put_ms (v16bfloat16 a, int en, int tlast)
| Write a 256-bit vector value to the output stream port.
void | put_ms (v16float16 a, int tlast)
| Write a 256-bit vector value to the output stream port.
void | put_ms (v16float16 a, int en, int tlast)
| Write a 256-bit vector value to the output stream port.
void | put_ms (v8float a, int tlast)
| Write a 256-bit vector value to the output stream port.
void | put_ms (v8float a, int en, int tlast)
| Write a 256-bit vector value to the output stream port.

## Write 512-bit vector to 32-bit streams
void | put_ms (v16int32 a, int tlast)
| Write a 512-bit vector value to the output stream port.
void | put_ms (v16int32 a, int en, int tlast)
| Write a 512-bit vector value to the output stream port.
void | put_ms (v128int4 a, int tlast)
| Write a 512-bit vector value to the output stream port.
void | put_ms (v128int4 a, int en, int tlast)
| Write a 512-bit vector value to the output stream port.
void | put_ms (v128uint4 a, int tlast)
| Write a 512-bit vector value to the output stream port.
void | put_ms (v128uint4 a, int en, int tlast)
| Write a 512-bit vector value to the output stream port.
void | put_ms (v64int8 a, int tlast)
| Write a 512-bit vector value to the output stream port.
void | put_ms (v64int8 a, int en, int tlast)
| Write a 512-bit vector value to the output stream port.
void | put_ms (v64uint8 a, int tlast)
| Write a 512-bit vector value to the output stream port.
void | put_ms (v64uint8 a, int en, int tlast)
| Write a 512-bit vector value to the output stream port.
void | put_ms (v32int16 a, int tlast)
| Write a 512-bit vector value to the output stream port.
void | put_ms (v32int16 a, int en, int tlast)
| Write a 512-bit vector value to the output stream port.
void | put_ms (v32uint16 a, int tlast)
| Write a 512-bit vector value to the output stream port.
void | put_ms (v32uint16 a, int en, int tlast)
| Write a 512-bit vector value to the output stream port.
void | put_ms (v16cint16 a, int tlast)
| Write a 512-bit vector value to the output stream port.
void | put_ms (v16cint16 a, int en, int tlast)
| Write a 512-bit vector value to the output stream port.
void | put_ms (v16uint32 a, int tlast)
| Write a 512-bit vector value to the output stream port.
void | put_ms (v16uint32 a, int en, int tlast)
| Write a 512-bit vector value to the output stream port.
void | put_ms (v8cint32 a, int tlast)
| Write a 512-bit vector value to the output stream port.
void | put_ms (v8cint32 a, int en, int tlast)
| Write a 512-bit vector value to the output stream port.
void | put_ms (v8cfloat a, int tlast)
| Write a 512-bit vector value to the output stream port.
void | put_ms (v8cfloat a, int en, int tlast)
| Write a 512-bit vector value to the output stream port.
void | put_ms (v16cbfloat16 a, int tlast)
| Write a 512-bit vector value to the output stream port.
void | put_ms (v16cbfloat16 a, int en, int tlast)
| Write a 512-bit vector value to the output stream port.
void | put_ms (v32bfloat16 a, int tlast)
| Write a 512-bit vector value to the output stream port.
void | put_ms (v32bfloat16 a, int en, int tlast)
| Write a 512-bit vector value to the output stream port.
void | put_ms (v32float16 a, int tlast)
| Write a 512-bit vector value to the output stream port.
void | put_ms (v32float16 a, int en, int tlast)
| Write a 512-bit vector value to the output stream port.
void | put_ms (v16float a, int tlast)
| Write a 512-bit vector value to the output stream port.
void | put_ms (v16float a, int en, int tlast)
| Write a 512-bit vector value to the output stream port.

## Write 1024-bit vector to 32-bit streams
void | put_ms (v32int32 a, int tlast)
| Write a 1024-bit vector value to the output stream port.
void | put_ms (v32int32 a, int en, int tlast)
| Write a 1024-bit vector value to the output stream port.
void | put_ms (v256int4 a, int tlast)
| Write a 1024-bit vector value to the output stream port.
void | put_ms (v256int4 a, int en, int tlast)
| Write a 1024-bit vector value to the output stream port.
void | put_ms (v256uint4 a, int tlast)
| Write a 1024-bit vector value to the output stream port.
void | put_ms (v256uint4 a, int en, int tlast)
| Write a 1024-bit vector value to the output stream port.
void | put_ms (v128int8 a, int tlast)
| Write a 1024-bit vector value to the output stream port.
void | put_ms (v128int8 a, int en, int tlast)
| Write a 1024-bit vector value to the output stream port.
void | put_ms (v128uint8 a, int tlast)
| Write a 1024-bit vector value to the output stream port.
void | put_ms (v128uint8 a, int en, int tlast)
| Write a 1024-bit vector value to the output stream port.
void | put_ms (v64int16 a, int tlast)
| Write a 1024-bit vector value to the output stream port.
void | put_ms (v64int16 a, int en, int tlast)
| Write a 1024-bit vector value to the output stream port.
void | put_ms (v64uint16 a, int tlast)
| Write a 1024-bit vector value to the output stream port.
void | put_ms (v64uint16 a, int en, int tlast)
| Write a 1024-bit vector value to the output stream port.
void | put_ms (v32cint16 a, int tlast)
| Write a 1024-bit vector value to the output stream port.
void | put_ms (v32cint16 a, int en, int tlast)
| Write a 1024-bit vector value to the output stream port.
void | put_ms (v32uint32 a, int tlast)
| Write a 1024-bit vector value to the output stream port.
void | put_ms (v32uint32 a, int en, int tlast)
| Write a 1024-bit vector value to the output stream port.
void | put_ms (v16cint32 a, int tlast)
| Write a 1024-bit vector value to the output stream port.
void | put_ms (v16cint32 a, int en, int tlast)
| Write a 1024-bit vector value to the output stream port.
void | put_ms (v16cfloat a, int tlast)
| Write a 1024-bit vector value to the output stream port.
void | put_ms (v16cfloat a, int en, int tlast)
| Write a 1024-bit vector value to the output stream port.
void | put_ms (v32cbfloat16 a, int tlast)
| Write a 1024-bit vector value to the output stream port.
void | put_ms (v32cbfloat16 a, int en, int tlast)
| Write a 1024-bit vector value to the output stream port.
void | put_ms (v64bfloat16 a, int tlast)
| Write a 1024-bit vector value to the output stream port.
void | put_ms (v64bfloat16 a, int en, int tlast)
| Write a 1024-bit vector value to the output stream port.
void | put_ms (v64float16 a, int tlast)
| Write a 1024-bit vector value to the output stream port.
void | put_ms (v64float16 a, int en, int tlast)
| Write a 1024-bit vector value to the output stream port.
void | put_ms (v32float a, int tlast)
| Write a 1024-bit vector value to the output stream port.
void | put_ms (v32float a, int en, int tlast)
| Write a 1024-bit vector value to the output stream port.

## Detailed Description

## Function Documentation

## ◆ ctrl_packet_header()

unsigned int ctrl_packet_header | ( | unsigned | Addr,
|  | unsigned | n_words,
|  | unsigned | op_type,
|  | unsigned | rspID )

Generate a control packet header.

Parameters

  Addr | unsigned Local Byte Address (two LSB not used). Accesses are 128 bit aligned.
  n_words | unsigned 2 bits. 1 to 4 words of 32 bit data to follow. This must be a compile time constant.
  op_type | unsigned Operation modes - 2 bit (LSB). 3 modes. 0 - Write without return, 1 - Read with return, 2 - Write with return. The response to a read will be a packet switched stream header and 1 to 4 32 bit word data. The response to a write will be a packet switched stream header. This must be a compile time constant.
  rspID | unsigned Response ID: 5 bit (LSB). Identifies the return destination for operation modes with a return. (The return packet's header's 'dstID' is set to this).

This intrinsic takes an address, number of words, operation type and response ID and returns a control packet header.

Note
  Parameters 'n_words' and 'op_type' must be compile time constants.

Deprecated
  Please use one variant of 'put_ms_ctrl_packet_header' instead

## ◆ packet_header()

unsigned int packet_header | ( | unsigned | dstID,
|  | unsigned | pcktType )

Generate a packet header.

Parameters

  dstID | unsigned 5 bit (LSB). Identifies the destination of the packet. Should be unique amongst all streams it shares ports with. Can be 32 destinations or more with nested headers.
  pcktType | unsigned 3 bit (LSB). Can be used to distinguish packets with the same source and destination. Control packets set this to 7 if there is an error. This must be a compile time constant.

This intrinsic takes a destination ID and a packet type and returns a packet header.

Note
  Parameter 'pcktType' must be a compile time constant.
  A packet with nested headers has a number of headers at the beginning (instead of the usual single header). For every level of header nesting, the number of possible destinations is multiplied by 32, thus for a two-nested header approach, the number of destinations is already 1024.

Deprecated
  Please use one variant of put_ms_packet_header instead

## ◆ put_ms() [1/156]

void put_ms | ( | cint16 | val | ) |

Write a 32-bit value to the output stream port.

## ◆ put_ms() [2/156]

void put_ms | ( | cint16 | val,
|  | int | en,
|  | int | tlast )

Write a 32-bit value to the output stream port.

Deprecated
  Please use 'void put_ms(cint16 val, int tlast)' instead.

Parameters

  val | 32-bit value datatype
  en | Enable input
  tlast | Success of transfer.

## ◆ put_ms() [3/156]

void put_ms | ( | cint16 | val,
|  | int | tlast )

Write a 32-bit value to the output stream port. Non-blocking read.

Parameters

  val | 32-bit value datatype
  tlast | Last word in a packet and the default is fals

## ◆ put_ms() [4/156]

void put_ms | ( | float | val | ) |

Write a 32-bit value to the output stream port.

## ◆ put_ms() [5/156]

void put_ms | ( | float | val,
|  | int | en,
|  | int | tlast )

Write a 32-bit value to the output stream port.

Deprecated
  Please use 'void put_ms(float val, int tlast)' instead.

Parameters

  val | 32-bit value datatype
  en | Enable input
  tlast | Success of transfer.

## ◆ put_ms() [6/156]

void put_ms | ( | float | val,
|  | int | tlast )

Write a 32-bit value to the output stream port. Non-blocking read.

Parameters

  val | 32-bit value datatype
  tlast | Last word in a packet and the default is fals

## ◆ put_ms() [7/156]

void put_ms | ( | int | val | ) |

Write a 32-bit value to the output stream port.

## ◆ put_ms() [8/156]

void put_ms | ( | int | val,
|  | int | en,
|  | int | tlast )

Write a 32-bit value to the output stream port.

Deprecated
  Please use 'void put_ms(int val, int tlast)' instead.

Parameters

  val | 32-bit value datatype
  en | Enable input
  tlast | Success of transfer.

## ◆ put_ms() [9/156]

void put_ms | ( | int | val,
|  | int | tlast )

Write a 32-bit value to the output stream port. Non-blocking read.

Parameters

  val | 32-bit value datatype
  tlast | Last word in a packet and the default is fals

## ◆ put_ms() [10/156]

void put_ms | ( | unsigned int | val | ) |

Write a 32-bit value to the output stream port.

## ◆ put_ms() [11/156]

void put_ms | ( | unsigned int | val,
|  | int | en,
|  | int | tlast )

Write a 32-bit value to the output stream port.

Deprecated
  Please use 'void put_ms(unsigned int val, int tlast)' instead.

Parameters

  val | 32-bit value datatype
  en | Enable input
  tlast | Success of transfer.

## ◆ put_ms() [12/156]

void put_ms | ( | unsigned int | val,
|  | int | tlast )

Write a 32-bit value to the output stream port. Non-blocking read.

Parameters

  val | 32-bit value datatype
  tlast | Last word in a packet and the default is fals

## ◆ put_ms() [13/156]

void put_ms | ( | v128int4 | a,
|  | int | en,
|  | int | tlast )

Write a 512-bit vector value to the output stream port.

Deprecated
  Please use 'void put_ms(v128int4 val, int tlast)' instead.

Parameters

  a | 512-bit vector
  en | Enable input
  tlast | Last word in a packet and the default is false.

## ◆ put_ms() [14/156]

void put_ms | ( | v128int4 | a,
|  | int | tlast )

Write a 512-bit vector value to the output stream port.

Parameters

  a | 512-bit vector
  tlast | Last word in a packet and the default is false.

## ◆ put_ms() [15/156]

void put_ms | ( | v128int8 | a,
|  | int | en,
|  | int | tlast )

Write a 1024-bit vector value to the output stream port.

Deprecated
  Please use 'void put_ms(v128int8 val, int tlast)' instead.

Parameters

  a | 1024-bit vector
  en | Enable input
  tlast | Last word in a packet and the default is false.

## ◆ put_ms() [16/156]

void put_ms | ( | v128int8 | a,
|  | int | tlast )

Write a 1024-bit vector value to the output stream port.

Parameters

  a | 1024-bit vector
  tlast | Last word in a packet and the default is false.

## ◆ put_ms() [17/156]

void put_ms | ( | v128uint4 | a,
|  | int | en,
|  | int | tlast )

Write a 512-bit vector value to the output stream port.

Deprecated
  Please use 'void put_ms(v128uint4 val, int tlast)' instead.

Parameters

  a | 512-bit vector
  en | Enable input
  tlast | Last word in a packet and the default is false.

## ◆ put_ms() [18/156]

void put_ms | ( | v128uint4 | a,
|  | int | tlast )

Write a 512-bit vector value to the output stream port.

Parameters

  a | 512-bit vector
  tlast | Last word in a packet and the default is false.

## ◆ put_ms() [19/156]

void put_ms | ( | v128uint8 | a,
|  | int | en,
|  | int | tlast )

Write a 1024-bit vector value to the output stream port.

Deprecated
  Please use 'void put_ms(v128uint8 val, int tlast)' instead.

Parameters

  a | 1024-bit vector
  en | Enable input
  tlast | Last word in a packet and the default is false.

## ◆ put_ms() [20/156]

void put_ms | ( | v128uint8 | a,
|  | int | tlast )

Write a 1024-bit vector value to the output stream port.

Parameters

  a | 1024-bit vector
  tlast | Last word in a packet and the default is false.

## ◆ put_ms() [21/156]

void put_ms | ( | v16bfloat16 | a,
|  | int | en,
|  | int | tlast )

Write a 256-bit vector value to the output stream port.

Deprecated
  Please use 'void put_ms(v16bfloat16 val, int tlast)' instead.

Parameters

  a | 256-bit vector
  en | Enable input
  tlast | Last word in a packet and the default is false.

## ◆ put_ms() [22/156]

void put_ms | ( | v16bfloat16 | a,
|  | int | tlast )

Write a 256-bit vector value to the output stream port.

Parameters

  a | 256-bit vector
  tlast | Last word in a packet and the default is false.

## ◆ put_ms() [23/156]

void put_ms | ( | v16cbfloat16 | a,
|  | int | en,
|  | int | tlast )

Write a 512-bit vector value to the output stream port.

Deprecated
  Please use 'void put_ms(v16cbfloat16 val, int tlast)' instead.

Parameters

  a | 512-bit vector
  en | Enable input
  tlast | Last word in a packet and the default is false.

## ◆ put_ms() [24/156]

void put_ms | ( | v16cbfloat16 | a,
|  | int | tlast )

Write a 512-bit vector value to the output stream port.

Parameters

  a | 512-bit vector
  tlast | Last word in a packet and the default is false.

## ◆ put_ms() [25/156]

void put_ms | ( | v16cfloat | a,
|  | int | en,
|  | int | tlast )

Write a 1024-bit vector value to the output stream port.

Deprecated
  Please use 'void put_ms(v16cfloat val, int tlast)' instead.

Parameters

  a | 1024-bit vector
  en | Enable input
  tlast | Last word in a packet and the default is false.

## ◆ put_ms() [26/156]

void put_ms | ( | v16cfloat | a,
|  | int | tlast )

Write a 1024-bit vector value to the output stream port.

Parameters

  a | 1024-bit vector
  tlast | Last word in a packet and the default is false.

## ◆ put_ms() [27/156]

void put_ms | ( | v16cint16 | a,
|  | int | en,
|  | int | tlast )

Write a 512-bit vector value to the output stream port.

Deprecated
  Please use 'void put_ms(v16cint16 val, int tlast)' instead.

Parameters

  a | 512-bit vector
  en | Enable input
  tlast | Last word in a packet and the default is false.

## ◆ put_ms() [28/156]

void put_ms | ( | v16cint16 | a,
|  | int | tlast )

Write a 512-bit vector value to the output stream port.

Parameters

  a | 512-bit vector
  tlast | Last word in a packet and the default is false.

## ◆ put_ms() [29/156]

void put_ms | ( | v16cint32 | a,
|  | int | en,
|  | int | tlast )

Write a 1024-bit vector value to the output stream port.

Deprecated
  Please use 'void put_ms(v16cint32 val, int tlast)' instead.

Parameters

  a | 1024-bit vector
  en | Enable input
  tlast | Last word in a packet and the default is false.

## ◆ put_ms() [30/156]

void put_ms | ( | v16cint32 | a,
|  | int | tlast )

Write a 1024-bit vector value to the output stream port.

Parameters

  a | 1024-bit vector
  tlast | Last word in a packet and the default is false.

## ◆ put_ms() [31/156]

void put_ms | ( | v16float | a,
|  | int | en,
|  | int | tlast )

Write a 512-bit vector value to the output stream port.

Deprecated
  Please use 'void put_ms(v16float val, int tlast)' instead.

Parameters

  a | 512-bit vector
  en | Enable input
  tlast | Last word in a packet and the default is false.

## ◆ put_ms() [32/156]

void put_ms | ( | v16float | a,
|  | int | tlast )

Write a 512-bit vector value to the output stream port.

Parameters

  a | 512-bit vector
  tlast | Last word in a packet and the default is false.

## ◆ put_ms() [33/156]

void put_ms | ( | v16float16 | a,
|  | int | en,
|  | int | tlast )

Write a 256-bit vector value to the output stream port.

Deprecated
  Please use 'void put_ms(v16float16 val, int tlast)' instead.

Parameters

  a | 256-bit vector
  en | Enable input
  tlast | Last word in a packet and the default is false.

## ◆ put_ms() [34/156]

void put_ms | ( | v16float16 | a,
|  | int | tlast )

Write a 256-bit vector value to the output stream port.

Parameters

  a | 256-bit vector
  tlast | Last word in a packet and the default is false.

## ◆ put_ms() [35/156]

void put_ms | ( | v16int16 | a,
|  | int | en,
|  | int | tlast )

Write a 256-bit vector value to the output stream port.

Deprecated
  Please use 'void put_ms(v16int16 val, int tlast)' instead.

Parameters

  a | 256-bit vector
  en | Enable input
  tlast | Last word in a packet and the default is false.

## ◆ put_ms() [36/156]

void put_ms | ( | v16int16 | a,
|  | int | tlast )

Write a 256-bit vector value to the output stream port.

Parameters

  a | 256-bit vector
  tlast | Last word in a packet and the default is false.

## ◆ put_ms() [37/156]

void put_ms | ( | v16int32 | a,
|  | int | en,
|  | int | tlast )

Write a 512-bit vector value to the output stream port.

Deprecated
  Please use 'void put_ms(v16int32 val, int tlast)' instead.

Parameters

  a | 512-bit vector
  en | Enable input
  tlast | Last word in a packet and the default is false.

## ◆ put_ms() [38/156]

void put_ms | ( | v16int32 | a,
|  | int | tlast )

Write a 512-bit vector value to the output stream port.

Parameters

  a | 512-bit vector
  tlast | Last word in a packet and the default is false.

## ◆ put_ms() [39/156]

void put_ms | ( | v16int8 | a,
|  | int | en,
|  | int | tlast )

Write a 128-bit vector value to the output stream port.

Deprecated
  Please use 'void put_ms(v16int8 val, int tlast)' instead.

Parameters

  a | 128-bit vector
  en | Enable input
  tlast | Last word in a packet and the default is false.

## ◆ put_ms() [40/156]

void put_ms | ( | v16int8 | a,
|  | int | tlast )

Write a 128-bit vector value to the output stream port.

Parameters

  a | 128-bit vector
  tlast | Last word in a packet and the default is false.

## ◆ put_ms() [41/156]

void put_ms | ( | v16uint16 | a,
|  | int | en,
|  | int | tlast )

Write a 256-bit vector value to the output stream port.

Deprecated
  Please use 'void put_ms(v16uint16 val, int tlast)' instead.

Parameters

  a | 256-bit vector
  en | Enable input
  tlast | Last word in a packet and the default is false.

## ◆ put_ms() [42/156]

void put_ms | ( | v16uint16 | a,
|  | int | tlast )

Write a 256-bit vector value to the output stream port.

Parameters

  a | 256-bit vector
  tlast | Last word in a packet and the default is false.

## ◆ put_ms() [43/156]

void put_ms | ( | v16uint32 | a,
|  | int | en,
|  | int | tlast )

Write a 512-bit vector value to the output stream port.

Deprecated
  Please use 'void put_ms(v16uint32 val, int tlast)' instead.

Parameters

  a | 512-bit vector
  en | Enable input
  tlast | Last word in a packet and the default is false.

## ◆ put_ms() [44/156]

void put_ms | ( | v16uint32 | a,
|  | int | tlast )

Write a 512-bit vector value to the output stream port.

Parameters

  a | 512-bit vector
  tlast | Last word in a packet and the default is false.

## ◆ put_ms() [45/156]

void put_ms | ( | v16uint8 | a,
|  | int | en,
|  | int | tlast )

Write a 128-bit vector value to the output stream port.

Deprecated
  Please use 'void put_ms(v16uint8 val, int tlast)' instead.

Parameters

  a | 128-bit vector
  en | Enable input
  tlast | Last word in a packet and the default is false.

## ◆ put_ms() [46/156]

void put_ms | ( | v16uint8 | a,
|  | int | tlast )

Write a 128-bit vector value to the output stream port.

Parameters

  a | 128-bit vector
  tlast | Last word in a packet and the default is false.

## ◆ put_ms() [47/156]

void put_ms | ( | v256int4 | a,
|  | int | en,
|  | int | tlast )

Write a 1024-bit vector value to the output stream port.

Deprecated
  Please use 'void put_ms(v256int4 val, int tlast)' instead.

Parameters

  a | 1024-bit vector
  en | Enable input
  tlast | Last word in a packet and the default is false.

## ◆ put_ms() [48/156]

void put_ms | ( | v256int4 | a,
|  | int | tlast )

Write a 1024-bit vector value to the output stream port.

Parameters

  a | 1024-bit vector
  tlast | Last word in a packet and the default is false.

## ◆ put_ms() [49/156]

void put_ms | ( | v256uint4 | a,
|  | int | en,
|  | int | tlast )

Write a 1024-bit vector value to the output stream port.

Deprecated
  Please use 'void put_ms(v256uint4 val, int tlast)' instead.

Parameters

  a | 1024-bit vector
  en | Enable input
  tlast | Last word in a packet and the default is false.

## ◆ put_ms() [50/156]

void put_ms | ( | v256uint4 | a,
|  | int | tlast )

Write a 1024-bit vector value to the output stream port.

Parameters

  a | 1024-bit vector
  tlast | Last word in a packet and the default is false.

## ◆ put_ms() [51/156]

void put_ms | ( | v2bfloat16 | val | ) |

Write a 32-bit value to the output stream port.

## ◆ put_ms() [52/156]

void put_ms | ( | v2bfloat16 | val,
|  | int | en,
|  | int | tlast )

Write a 32-bit value to the output stream port.

Deprecated
  Please use 'void put_ms(v2bfloat16 val, int tlast)' instead.

Parameters

  val | 32-bit value datatype
  en | Enable input
  tlast | Success of transfer.

## ◆ put_ms() [53/156]

void put_ms | ( | v2bfloat16 | val,
|  | int | tlast )

Write a 32-bit value to the output stream port. Non-blocking read.

Parameters

  val | 32-bit value datatype
  tlast | Last word in a packet and the default is fals

## ◆ put_ms() [54/156]

void put_ms | ( | v2cfloat | a,
|  | int | en,
|  | int | tlast )

Write a 128-bit vector value to the output stream port.

Deprecated
  Please use 'void put_ms(v2cfloat val, int tlast)' instead.

Parameters

  a | 128-bit vector
  en | Enable input
  tlast | Last word in a packet and the default is false.

## ◆ put_ms() [55/156]

void put_ms | ( | v2cfloat | a,
|  | int | tlast )

Write a 128-bit vector value to the output stream port.

Parameters

  a | 128-bit vector
  tlast | Last word in a packet and the default is false.

## ◆ put_ms() [56/156]

void put_ms | ( | v2cint32 | a,
|  | int | en,
|  | int | tlast )

Write a 128-bit vector value to the output stream port.

Deprecated
  Please use 'void put_ms(v2cint32 val, int tlast)' instead.

Parameters

  a | 128-bit vector
  en | Enable input
  tlast | Last word in a packet and the default is false.

## ◆ put_ms() [57/156]

void put_ms | ( | v2cint32 | a,
|  | int | tlast )

Write a 128-bit vector value to the output stream port.

Parameters

  a | 128-bit vector
  tlast | Last word in a packet and the default is false.

## ◆ put_ms() [58/156]

void put_ms | ( | v2float16 | val | ) |

Write a 32-bit value to the output stream port.

## ◆ put_ms() [59/156]

void put_ms | ( | v2float16 | val,
|  | int | en,
|  | int | tlast )

Write a 32-bit value to the output stream port.

Deprecated
  Please use 'void put_ms(v2float16 val, int tlast)' instead.

Parameters

  val | 32-bit value datatype
  en | Enable input
  tlast | Success of transfer.

## ◆ put_ms() [60/156]

void put_ms | ( | v2float16 | val,
|  | int | tlast )

Write a 32-bit value to the output stream port. Non-blocking read.

Parameters

  val | 32-bit value datatype
  tlast | Last word in a packet and the default is fals

## ◆ put_ms() [61/156]

void put_ms | ( | v2int16 | val | ) |

Write a 32-bit value to the output stream port.

## ◆ put_ms() [62/156]

void put_ms | ( | v2int16 | val,
|  | int | en,
|  | int | tlast )

Write a 32-bit value to the output stream port.

Deprecated
  Please use 'void put_ms(v2int16 val, int tlast)' instead.

Parameters

  val | 32-bit value datatype
  en | Enable input
  tlast | Success of transfer.

## ◆ put_ms() [63/156]

void put_ms | ( | v2int16 | val,
|  | int | tlast )

Write a 32-bit value to the output stream port. Non-blocking read.

Parameters

  val | 32-bit value datatype
  tlast | Last word in a packet and the default is fals

## ◆ put_ms() [64/156]

void put_ms | ( | v2uint16 | val | ) |

Write a 32-bit value to the output stream port.

## ◆ put_ms() [65/156]

void put_ms | ( | v2uint16 | val,
|  | int | en,
|  | int | tlast )

Write a 32-bit value to the output stream port.

Deprecated
  Please use 'void put_ms(v2uint16 val, int tlast)' instead.

Parameters

  val | 32-bit value datatype
  en | Enable input
  tlast | Success of transfer.

## ◆ put_ms() [66/156]

void put_ms | ( | v2uint16 | val,
|  | int | tlast )

Write a 32-bit value to the output stream port. Non-blocking read.

Parameters

  val | 32-bit value datatype
  tlast | Last word in a packet and the default is fals

## ◆ put_ms() [67/156]

void put_ms | ( | v32bfloat16 | a,
|  | int | en,
|  | int | tlast )

Write a 512-bit vector value to the output stream port.

Deprecated
  Please use 'void put_ms(v32bfloat16 val, int tlast)' instead.

Parameters

  a | 512-bit vector
  en | Enable input
  tlast | Last word in a packet and the default is false.

## ◆ put_ms() [68/156]

void put_ms | ( | v32bfloat16 | a,
|  | int | tlast )

Write a 512-bit vector value to the output stream port.

Parameters

  a | 512-bit vector
  tlast | Last word in a packet and the default is false.

## ◆ put_ms() [69/156]

void put_ms | ( | v32cbfloat16 | a,
|  | int | en,
|  | int | tlast )

Write a 1024-bit vector value to the output stream port.

Deprecated
  Please use 'void put_ms(v32cbfloat16 val, int tlast)' instead.

Parameters

  a | 1024-bit vector
  en | Enable input
  tlast | Last word in a packet and the default is false.

## ◆ put_ms() [70/156]

void put_ms | ( | v32cbfloat16 | a,
|  | int | tlast )

Write a 1024-bit vector value to the output stream port.

Parameters

  a | 1024-bit vector
  tlast | Last word in a packet and the default is false.

## ◆ put_ms() [71/156]

void put_ms | ( | v32cint16 | a,
|  | int | en,
|  | int | tlast )

Write a 1024-bit vector value to the output stream port.

Deprecated
  Please use 'void put_ms(v32cint16 val, int tlast)' instead.

Parameters

  a | 1024-bit vector
  en | Enable input
  tlast | Last word in a packet and the default is false.

## ◆ put_ms() [72/156]

void put_ms | ( | v32cint16 | a,
|  | int | tlast )

Write a 1024-bit vector value to the output stream port.

Parameters

  a | 1024-bit vector
  tlast | Last word in a packet and the default is false.

## ◆ put_ms() [73/156]

void put_ms | ( | v32float | a,
|  | int | en,
|  | int | tlast )

Write a 1024-bit vector value to the output stream port.

Deprecated
  Please use 'void put_ms(v32float val, int tlast)' instead.

Parameters

  a | 1024-bit vector
  en | Enable input
  tlast | Last word in a packet and the default is false.

## ◆ put_ms() [74/156]

void put_ms | ( | v32float | a,
|  | int | tlast )

Write a 1024-bit vector value to the output stream port.

Parameters

  a | 1024-bit vector
  tlast | Last word in a packet and the default is false.

## ◆ put_ms() [75/156]

void put_ms | ( | v32float16 | a,
|  | int | en,
|  | int | tlast )

Write a 512-bit vector value to the output stream port.

Deprecated
  Please use 'void put_ms(v32float16 val, int tlast)' instead.

Parameters

  a | 512-bit vector
  en | Enable input
  tlast | Last word in a packet and the default is false.

## ◆ put_ms() [76/156]

void put_ms | ( | v32float16 | a,
|  | int | tlast )

Write a 512-bit vector value to the output stream port.

Parameters

  a | 512-bit vector
  tlast | Last word in a packet and the default is false.

## ◆ put_ms() [77/156]

void put_ms | ( | v32int16 | a,
|  | int | en,
|  | int | tlast )

Write a 512-bit vector value to the output stream port.

Deprecated
  Please use 'void put_ms(v32int16 val, int tlast)' instead.

Parameters

  a | 512-bit vector
  en | Enable input
  tlast | Last word in a packet and the default is false.

## ◆ put_ms() [78/156]

void put_ms | ( | v32int16 | a,
|  | int | tlast )

Write a 512-bit vector value to the output stream port.

Parameters

  a | 512-bit vector
  tlast | Last word in a packet and the default is false.

## ◆ put_ms() [79/156]

void put_ms | ( | v32int32 | a,
|  | int | en,
|  | int | tlast )

Write a 1024-bit vector value to the output stream port.

Deprecated
  Please use 'void put_ms(v32int32 val, int tlast)' instead.

Parameters

  a | 1024-bit vector
  en | Enable input
  tlast | Last word in a packet and the default is false.

## ◆ put_ms() [80/156]

void put_ms | ( | v32int32 | a,
|  | int | tlast )

Write a 1024-bit vector value to the output stream port.

Parameters

  a | 1024-bit vector
  tlast | Last word in a packet and the default is false.

## ◆ put_ms() [81/156]

void put_ms | ( | v32int4 | a,
|  | int | en,
|  | int | tlast )

Write a 128-bit vector value to the output stream port.

Deprecated
  Please use 'void put_ms(v32int4 val, int tlast)' instead.

Parameters

  a | 128-bit vector
  en | Enable input
  tlast | Last word in a packet and the default is false.

## ◆ put_ms() [82/156]

void put_ms | ( | v32int4 | a,
|  | int | tlast )

Write a 128-bit vector value to the output stream port.

Parameters

  a | 128-bit vector
  tlast | Last word in a packet and the default is false.

## ◆ put_ms() [83/156]

void put_ms | ( | v32int8 | a,
|  | int | en,
|  | int | tlast )

Write a 256-bit vector value to the output stream port.

Deprecated
  Please use 'void put_ms(v32int8 val, int tlast)' instead.

Parameters

  a | 256-bit vector
  en | Enable input
  tlast | Last word in a packet and the default is false.

## ◆ put_ms() [84/156]

void put_ms | ( | v32int8 | a,
|  | int | tlast )

Write a 256-bit vector value to the output stream port.

Parameters

  a | 256-bit vector
  tlast | Last word in a packet and the default is false.

## ◆ put_ms() [85/156]

void put_ms | ( | v32uint16 | a,
|  | int | en,
|  | int | tlast )

Write a 512-bit vector value to the output stream port.

Deprecated
  Please use 'void put_ms(v32uint16 val, int tlast)' instead.

Parameters

  a | 512-bit vector
  en | Enable input
  tlast | Last word in a packet and the default is false.

## ◆ put_ms() [86/156]

void put_ms | ( | v32uint16 | a,
|  | int | tlast )

Write a 512-bit vector value to the output stream port.

Parameters

  a | 512-bit vector
  tlast | Last word in a packet and the default is false.

## ◆ put_ms() [87/156]

void put_ms | ( | v32uint32 | a,
|  | int | en,
|  | int | tlast )

Write a 1024-bit vector value to the output stream port.

Deprecated
  Please use 'void put_ms(v32uint32 val, int tlast)' instead.

Parameters

  a | 1024-bit vector
  en | Enable input
  tlast | Last word in a packet and the default is false.

## ◆ put_ms() [88/156]

void put_ms | ( | v32uint32 | a,
|  | int | tlast )

Write a 1024-bit vector value to the output stream port.

Parameters

  a | 1024-bit vector
  tlast | Last word in a packet and the default is false.

## ◆ put_ms() [89/156]

void put_ms | ( | v32uint4 | a,
|  | int | en,
|  | int | tlast )

Write a 128-bit vector value to the output stream port.

Deprecated
  Please use 'void put_ms(v32uint4 val, int tlast)' instead.

Parameters

  a | 128-bit vector
  en | Enable input
  tlast | Last word in a packet and the default is false.

## ◆ put_ms() [90/156]

void put_ms | ( | v32uint4 | a,
|  | int | tlast )

Write a 128-bit vector value to the output stream port.

Parameters

  a | 128-bit vector
  tlast | Last word in a packet and the default is false.

## ◆ put_ms() [91/156]

void put_ms | ( | v32uint8 | a,
|  | int | en,
|  | int | tlast )

Write a 256-bit vector value to the output stream port.

Deprecated
  Please use 'void put_ms(v32uint8 val, int tlast)' instead.

Parameters

  a | 256-bit vector
  en | Enable input
  tlast | Last word in a packet and the default is false.

## ◆ put_ms() [92/156]

void put_ms | ( | v32uint8 | a,
|  | int | tlast )

Write a 256-bit vector value to the output stream port.

Parameters

  a | 256-bit vector
  tlast | Last word in a packet and the default is false.

## ◆ put_ms() [93/156]

void put_ms | ( | v4cbfloat16 | a,
|  | int | en,
|  | int | tlast )

Write a 128-bit vector value to the output stream port.

Deprecated
  Please use 'void put_ms(v4cbfloat16 val, int tlast)' instead.

Parameters

  a | 128-bit vector
  en | Enable input
  tlast | Last word in a packet and the default is false.

## ◆ put_ms() [94/156]

void put_ms | ( | v4cbfloat16 | a,
|  | int | tlast )

Write a 128-bit vector value to the output stream port.

Parameters

  a | 128-bit vector
  tlast | Last word in a packet and the default is false.

## ◆ put_ms() [95/156]

void put_ms | ( | v4cfloat | a,
|  | int | en,
|  | int | tlast )

Write a 256-bit vector value to the output stream port.

Deprecated
  Please use 'void put_ms(v4cfloat val, int tlast)' instead.

Parameters

  a | 256-bit vector
  en | Enable input
  tlast | Last word in a packet and the default is false.

## ◆ put_ms() [96/156]

void put_ms | ( | v4cfloat | a,
|  | int | tlast )

Write a 256-bit vector value to the output stream port.

Parameters

  a | 256-bit vector
  tlast | Last word in a packet and the default is false.

## ◆ put_ms() [97/156]

void put_ms | ( | v4cint16 | a,
|  | int | en,
|  | int | tlast )

Write a 128-bit vector value to the output stream port.

Deprecated
  Please use 'void put_ms(v4cint16 val, int tlast)' instead.

Parameters

  a | 128-bit vector
  en | Enable input
  tlast | Last word in a packet and the default is false.

## ◆ put_ms() [98/156]

void put_ms | ( | v4cint16 | a,
|  | int | tlast )

Write a 128-bit vector value to the output stream port.

Parameters

  a | 128-bit vector
  tlast | Last word in a packet and the default is false.

## ◆ put_ms() [99/156]

void put_ms | ( | v4cint32 | a,
|  | int | en,
|  | int | tlast )

Write a 256-bit vector value to the output stream port.

Deprecated
  Please use 'void put_ms(v4cint32 val, int tlast)' instead.

Parameters

  a | 256-bit vector
  en | Enable input
  tlast | Last word in a packet and the default is false.

## ◆ put_ms() [100/156]

void put_ms | ( | v4cint32 | a,
|  | int | tlast )

Write a 256-bit vector value to the output stream port.

Parameters

  a | 256-bit vector
  tlast | Last word in a packet and the default is false.

## ◆ put_ms() [101/156]

void put_ms | ( | v4float | a,
|  | int | en,
|  | int | tlast )

Write a 128-bit vector value to the output stream port.

Deprecated
  Please use 'void put_ms(v4float val, int tlast)' instead.

Parameters

  a | 128-bit vector
  en | Enable input
  tlast | Last word in a packet and the default is false.

## ◆ put_ms() [102/156]

void put_ms | ( | v4float | a,
|  | int | tlast )

Write a 128-bit vector value to the output stream port.

Parameters

  a | 128-bit vector
  tlast | Last word in a packet and the default is false.

## ◆ put_ms() [103/156]

void put_ms | ( | v4int32 | a,
|  | int | en,
|  | int | tlast )

Write a 128-bit vector value to the output stream port.

Deprecated
  Please use 'void put_ms(v4int32 val, int tlast)' instead.

Parameters

  a | 128-bit vector
  en | Enable input
  tlast | Last word in a packet and the default is false.

## ◆ put_ms() [104/156]

void put_ms | ( | v4int32 | a,
|  | int | tlast )

Write a 128-bit vector value to the output stream port.

Parameters

  a | 128-bit vector
  tlast | Last word in a packet and the default is false.

## ◆ put_ms() [105/156]

void put_ms | ( | v4int8 | val | ) |

Write a 32-bit value to the output stream port.

## ◆ put_ms() [106/156]

void put_ms | ( | v4int8 | val,
|  | int | en,
|  | int | tlast )

Write a 32-bit value to the output stream port.

Deprecated
  Please use 'void put_ms(v4int8 val, int tlast)' instead.

Parameters

  val | 32-bit value datatype
  en | Enable input
  tlast | Success of transfer.

## ◆ put_ms() [107/156]

void put_ms | ( | v4int8 | val,
|  | int | tlast )

Write a 32-bit value to the output stream port. Non-blocking read.

Parameters

  val | 32-bit value datatype
  tlast | Last word in a packet and the default is fals

## ◆ put_ms() [108/156]

void put_ms | ( | v4uint32 | a,
|  | int | en,
|  | int | tlast )

Write a 128-bit vector value to the output stream port.

Deprecated
  Please use 'void put_ms(v4uint32 val, int tlast)' instead.

Parameters

  a | 128-bit vector
  en | Enable input
  tlast | Last word in a packet and the default is false.

## ◆ put_ms() [109/156]

void put_ms | ( | v4uint32 | a,
|  | int | tlast )

Write a 128-bit vector value to the output stream port.

Parameters

  a | 128-bit vector
  tlast | Last word in a packet and the default is false.

## ◆ put_ms() [110/156]

void put_ms | ( | v4uint8 | val | ) |

Write a 32-bit value to the output stream port.

## ◆ put_ms() [111/156]

void put_ms | ( | v4uint8 | val,
|  | int | en,
|  | int | tlast )

Write a 32-bit value to the output stream port.

Deprecated
  Please use 'void put_ms(v4uint8 val, int tlast)' instead.

Parameters

  val | 32-bit value datatype
  en | Enable input
  tlast | Success of transfer.

## ◆ put_ms() [112/156]

void put_ms | ( | v4uint8 | val,
|  | int | tlast )

Write a 32-bit value to the output stream port. Non-blocking read.

Parameters

  val | 32-bit value datatype
  tlast | Last word in a packet and the default is fals

## ◆ put_ms() [113/156]

void put_ms | ( | v64bfloat16 | a,
|  | int | en,
|  | int | tlast )

Write a 1024-bit vector value to the output stream port.

Deprecated
  Please use 'void put_ms(v64bfloat16 val, int tlast)' instead.

Parameters

  a | 1024-bit vector
  en | Enable input
  tlast | Last word in a packet and the default is false.

## ◆ put_ms() [114/156]

void put_ms | ( | v64bfloat16 | a,
|  | int | tlast )

Write a 1024-bit vector value to the output stream port.

Parameters

  a | 1024-bit vector
  tlast | Last word in a packet and the default is false.

## ◆ put_ms() [115/156]

void put_ms | ( | v64float16 | a,
|  | int | en,
|  | int | tlast )

Write a 1024-bit vector value to the output stream port.

Deprecated
  Please use 'void put_ms(v64float16 val, int tlast)' instead.

Parameters

  a | 1024-bit vector
  en | Enable input
  tlast | Last word in a packet and the default is false.

## ◆ put_ms() [116/156]

void put_ms | ( | v64float16 | a,
|  | int | tlast )

Write a 1024-bit vector value to the output stream port.

Parameters

  a | 1024-bit vector
  tlast | Last word in a packet and the default is false.

## ◆ put_ms() [117/156]

void put_ms | ( | v64int16 | a,
|  | int | en,
|  | int | tlast )

Write a 1024-bit vector value to the output stream port.

Deprecated
  Please use 'void put_ms(v64int16 val, int tlast)' instead.

Parameters

  a | 1024-bit vector
  en | Enable input
  tlast | Last word in a packet and the default is false.

## ◆ put_ms() [118/156]

void put_ms | ( | v64int16 | a,
|  | int | tlast )

Write a 1024-bit vector value to the output stream port.

Parameters

  a | 1024-bit vector
  tlast | Last word in a packet and the default is false.

## ◆ put_ms() [119/156]

void put_ms | ( | v64int4 | a,
|  | int | en,
|  | int | tlast )

Write a 256-bit vector value to the output stream port.

Deprecated
  Please use 'void put_ms(v64int4 val, int tlast)' instead.

Parameters

  a | 256-bit vector
  en | Enable input
  tlast | Last word in a packet and the default is false.

## ◆ put_ms() [120/156]

void put_ms | ( | v64int4 | a,
|  | int | tlast )

Write a 256-bit vector value to the output stream port.

Parameters

  a | 256-bit vector
  tlast | Last word in a packet and the default is false.

## ◆ put_ms() [121/156]

void put_ms | ( | v64int8 | a,
|  | int | en,
|  | int | tlast )

Write a 512-bit vector value to the output stream port.

Deprecated
  Please use 'void put_ms(v64int8 val, int tlast)' instead.

Parameters

  a | 512-bit vector
  en | Enable input
  tlast | Last word in a packet and the default is false.

## ◆ put_ms() [122/156]

void put_ms | ( | v64int8 | a,
|  | int | tlast )

Write a 512-bit vector value to the output stream port.

Parameters

  a | 512-bit vector
  tlast | Last word in a packet and the default is false.

## ◆ put_ms() [123/156]

void put_ms | ( | v64uint16 | a,
|  | int | en,
|  | int | tlast )

Write a 1024-bit vector value to the output stream port.

Deprecated
  Please use 'void put_ms(v64uint16 val, int tlast)' instead.

Parameters

  a | 1024-bit vector
  en | Enable input
  tlast | Last word in a packet and the default is false.

## ◆ put_ms() [124/156]

void put_ms | ( | v64uint16 | a,
|  | int | tlast )

Write a 1024-bit vector value to the output stream port.

Parameters

  a | 1024-bit vector
  tlast | Last word in a packet and the default is false.

## ◆ put_ms() [125/156]

void put_ms | ( | v64uint4 | a,
|  | int | en,
|  | int | tlast )

Write a 256-bit vector value to the output stream port.

Deprecated
  Please use 'void put_ms(v64uint4 val, int tlast)' instead.

Parameters

  a | 256-bit vector
  en | Enable input
  tlast | Last word in a packet and the default is false.

## ◆ put_ms() [126/156]

void put_ms | ( | v64uint4 | a,
|  | int | tlast )

Write a 256-bit vector value to the output stream port.

Parameters

  a | 256-bit vector
  tlast | Last word in a packet and the default is false.

## ◆ put_ms() [127/156]

void put_ms | ( | v64uint8 | a,
|  | int | en,
|  | int | tlast )

Write a 512-bit vector value to the output stream port.

Deprecated
  Please use 'void put_ms(v64uint8 val, int tlast)' instead.

Parameters

  a | 512-bit vector
  en | Enable input
  tlast | Last word in a packet and the default is false.

## ◆ put_ms() [128/156]

void put_ms | ( | v64uint8 | a,
|  | int | tlast )

Write a 512-bit vector value to the output stream port.

Parameters

  a | 512-bit vector
  tlast | Last word in a packet and the default is false.

## ◆ put_ms() [129/156]

void put_ms | ( | v8bfloat16 | a,
|  | int | en,
|  | int | tlast )

Write a 128-bit vector value to the output stream port.

Deprecated
  Please use 'void put_ms(v8bfloat16 val, int tlast)' instead.

Parameters

  a | 128-bit vector
  en | Enable input
  tlast | Last word in a packet and the default is false.

## ◆ put_ms() [130/156]

void put_ms | ( | v8bfloat16 | a,
|  | int | tlast )

Write a 128-bit vector value to the output stream port.

Parameters

  a | 128-bit vector
  tlast | Last word in a packet and the default is false.

## ◆ put_ms() [131/156]

void put_ms | ( | v8cbfloat16 | a,
|  | int | en,
|  | int | tlast )

Write a 256-bit vector value to the output stream port.

Deprecated
  Please use 'void put_ms(v8cbfloat16 val, int tlast)' instead.

Parameters

  a | 256-bit vector
  en | Enable input
  tlast | Last word in a packet and the default is false.

## ◆ put_ms() [132/156]

void put_ms | ( | v8cbfloat16 | a,
|  | int | tlast )

Write a 256-bit vector value to the output stream port.

Parameters

  a | 256-bit vector
  tlast | Last word in a packet and the default is false.

## ◆ put_ms() [133/156]

void put_ms | ( | v8cfloat | a,
|  | int | en,
|  | int | tlast )

Write a 512-bit vector value to the output stream port.

Deprecated
  Please use 'void put_ms(v8cfloat val, int tlast)' instead.

Parameters

  a | 512-bit vector
  en | Enable input
  tlast | Last word in a packet and the default is false.

## ◆ put_ms() [134/156]

void put_ms | ( | v8cfloat | a,
|  | int | tlast )

Write a 512-bit vector value to the output stream port.

Parameters

  a | 512-bit vector
  tlast | Last word in a packet and the default is false.

## ◆ put_ms() [135/156]

void put_ms | ( | v8cint16 | a,
|  | int | en,
|  | int | tlast )

Write a 256-bit vector value to the output stream port.

Deprecated
  Please use 'void put_ms(v8cint16 val, int tlast)' instead.

Parameters

  a | 256-bit vector
  en | Enable input
  tlast | Last word in a packet and the default is false.

## ◆ put_ms() [136/156]

void put_ms | ( | v8cint16 | a,
|  | int | tlast )

Write a 256-bit vector value to the output stream port.

Parameters

  a | 256-bit vector
  tlast | Last word in a packet and the default is false.

## ◆ put_ms() [137/156]

void put_ms | ( | v8cint32 | a,
|  | int | en,
|  | int | tlast )

Write a 512-bit vector value to the output stream port.

Deprecated
  Please use 'void put_ms(v8cint32 val, int tlast)' instead.

Parameters

  a | 512-bit vector
  en | Enable input
  tlast | Last word in a packet and the default is false.

## ◆ put_ms() [138/156]

void put_ms | ( | v8cint32 | a,
|  | int | tlast )

Write a 512-bit vector value to the output stream port.

Parameters

  a | 512-bit vector
  tlast | Last word in a packet and the default is false.

## ◆ put_ms() [139/156]

void put_ms | ( | v8float | a,
|  | int | en,
|  | int | tlast )

Write a 256-bit vector value to the output stream port.

Deprecated
  Please use 'void put_ms(v8float val, int tlast)' instead.

Parameters

  a | 256-bit vector
  en | Enable input
  tlast | Last word in a packet and the default is false.

## ◆ put_ms() [140/156]

void put_ms | ( | v8float | a,
|  | int | tlast )

Write a 256-bit vector value to the output stream port.

Parameters

  a | 256-bit vector
  tlast | Last word in a packet and the default is false.

## ◆ put_ms() [141/156]

void put_ms | ( | v8float16 | a,
|  | int | en,
|  | int | tlast )

Write a 128-bit vector value to the output stream port.

Deprecated
  Please use 'void put_ms(v8float16 val, int tlast)' instead.

Parameters

  a | 128-bit vector
  en | Enable input
  tlast | Last word in a packet and the default is false.

## ◆ put_ms() [142/156]

void put_ms | ( | v8float16 | a,
|  | int | tlast )

Write a 128-bit vector value to the output stream port.

Parameters

  a | 128-bit vector
  tlast | Last word in a packet and the default is false.

## ◆ put_ms() [143/156]

void put_ms | ( | v8int16 | a,
|  | int | en,
|  | int | tlast )

Write a 128-bit vector value to the output stream port.

Deprecated
  Please use 'void put_ms(v8int16 val, int tlast)' instead.

Parameters

  a | 128-bit vector
  en | Enable input
  tlast | Last word in a packet and the default is false.

## ◆ put_ms() [144/156]

void put_ms | ( | v8int16 | a,
|  | int | tlast )

Write a 128-bit vector value to the output stream port.

Parameters

  a | 128-bit vector
  tlast | Last word in a packet and the default is false.

## ◆ put_ms() [145/156]

void put_ms | ( | v8int32 | a,
|  | int | en,
|  | int | tlast )

Write a 256-bit vector value to the output stream port.

Deprecated
  Please use 'void put_ms(v8int32 val, int tlast)' instead.

Parameters

  a | 256-bit vector
  en | Enable input
  tlast | Last word in a packet and the default is false.

## ◆ put_ms() [146/156]

void put_ms | ( | v8int32 | a,
|  | int | tlast )

Write a 256-bit vector value to the output stream port.

Parameters

  a | 256-bit vector
  tlast | Last word in a packet and the default is false.

## ◆ put_ms() [147/156]

void put_ms | ( | v8int4 | val | ) |

Write a 32-bit value to the output stream port.

## ◆ put_ms() [148/156]

void put_ms | ( | v8int4 | val,
|  | int | en,
|  | int | tlast )

Write a 32-bit value to the output stream port.

Deprecated
  Please use 'void put_ms(v8int4 val, int tlast)' instead.

Parameters

  val | 32-bit value datatype
  en | Enable input
  tlast | Success of transfer.

## ◆ put_ms() [149/156]

void put_ms | ( | v8int4 | val,
|  | int | tlast )

Write a 32-bit value to the output stream port. Non-blocking read.

Parameters

  val | 32-bit value datatype
  tlast | Last word in a packet and the default is fals

## ◆ put_ms() [150/156]

void put_ms | ( | v8uint16 | a,
|  | int | en,
|  | int | tlast )

Write a 128-bit vector value to the output stream port.

Deprecated
  Please use 'void put_ms(v8uint16 val, int tlast)' instead.

Parameters

  a | 128-bit vector
  en | Enable input
  tlast | Last word in a packet and the default is false.

## ◆ put_ms() [151/156]

void put_ms | ( | v8uint16 | a,
|  | int | tlast )

Write a 128-bit vector value to the output stream port.

Parameters

  a | 128-bit vector
  tlast | Last word in a packet and the default is false.

## ◆ put_ms() [152/156]

void put_ms | ( | v8uint32 | a,
|  | int | en,
|  | int | tlast )

Write a 256-bit vector value to the output stream port.

Deprecated
  Please use 'void put_ms(v8uint32 val, int tlast)' instead.

Parameters

  a | 256-bit vector
  en | Enable input
  tlast | Last word in a packet and the default is false.

## ◆ put_ms() [153/156]

void put_ms | ( | v8uint32 | a,
|  | int | tlast )

Write a 256-bit vector value to the output stream port.

Parameters

  a | 256-bit vector
  tlast | Last word in a packet and the default is false.

## ◆ put_ms() [154/156]

void put_ms | ( | v8uint4 | val | ) |

Write a 32-bit value to the output stream port.

## ◆ put_ms() [155/156]

void put_ms | ( | v8uint4 | val,
|  | int | en,
|  | int | tlast )

Write a 32-bit value to the output stream port.

Deprecated
  Please use 'void put_ms(v8uint4 val, int tlast)' instead.

Parameters

  val | 32-bit value datatype
  en | Enable input
  tlast | Success of transfer.

## ◆ put_ms() [156/156]

void put_ms | ( | v8uint4 | val,
|  | int | tlast )

Write a 32-bit value to the output stream port. Non-blocking read.

Parameters

  val | 32-bit value datatype
  tlast | Last word in a packet and the default is fals

## ◆ put_ms_ctrl_packet_header() [1/2]

void put_ms_ctrl_packet_header | ( | int | tlast,
|  | unsigned | Addr,
|  | unsigned | n_words,
|  | unsigned | op_type,
|  | unsigned | rspID )

Generate a control packet header and write it to the output stream port.

Parameters

  tlast | tlast
  Addr | unsigned Local Byte Address (two LSB not used). Accesses are 128 bit aligned.
  n_words | unsigned 2 bits. 1 to 4 words of 32 bit data to follow. This must be a compile time constant.
  op_type | unsigned Operation modes - 2 bit (LSB). 3 modes. 0 - Write without return, 1 - Read with return, 2 - Write with return. The response to a read will be a packet switched stream header and 1 to 4 32 bit word data. The response to a write will be a packet switched stream header. This must be a compile time constant.
  rspID | unsigned Response ID: 5 bit (LSB). Identifies the return destination for operation modes with a return. (The return packet's header's 'dstID' is set to this).

This intrinsic takes an address, number of words, operation type and response ID and returns a control packet header.

Note
  Parameters 'n_words' and 'op_type' must be compile time constants.

## ◆ put_ms_ctrl_packet_header() [2/2]

void put_ms_ctrl_packet_header | ( | unsigned | Addr,
|  | unsigned | n_words,
|  | unsigned | op_type,
|  | unsigned | rspID )

Generate a control packet header and write it to the output stream port.

Parameters

  Addr | unsigned Local Byte Address (two LSB not used). Accesses are 128 bit aligned.
  n_words | unsigned 2 bits. 1 to 4 words of 32 bit data to follow. This must be a compile time constant.
  op_type | unsigned Operation modes - 2 bit (LSB). 3 modes. 0 - Write without return, 1 - Read with return, 2 - Write with return. The response to a read will be a packet switched stream header and 1 to 4 32 bit word data. The response to a write will be a packet switched stream header. This must be a compile time constant.
  rspID | unsigned Response ID: 5 bit (LSB). Identifies the return destination for operation modes with a return. (The return packet's header's 'dstID' is set to this).

This intrinsic takes an address, number of words, operation type and response ID and returns a control packet header.

Note
  Parameters 'n_words' and 'op_type' must be compile time constants.

## ◆ put_ms_nb() [1/24]

void put_ms_nb | ( | cint16 | val,
|  | bool & | success )

Write a 32-bit value to the output stream port. Non-blocking read.

Parameters

  val | 32-bit value datatype
  success | Success of transfer.

## ◆ put_ms_nb() [2/24]

void put_ms_nb | ( | cint16 | val,
|  | int | tlast,
|  | bool & | success )

Write a 32-bit value to the output stream port. Non-blocking read.

Parameters

  val | 32-bit value datatype
  tlast | last word in a packet and the default is fals
  success | Success of transfer.

## ◆ put_ms_nb() [3/24]

void put_ms_nb | ( | float | val,
|  | bool & | success )

Write a 32-bit value to the output stream port. Non-blocking read.

Parameters

  val | 32-bit value datatype
  success | Success of transfer.

## ◆ put_ms_nb() [4/24]

void put_ms_nb | ( | float | val,
|  | int | tlast,
|  | bool & | success )

Write a 32-bit value to the output stream port. Non-blocking read.

Parameters

  val | 32-bit value datatype
  tlast | last word in a packet and the default is fals
  success | Success of transfer.

## ◆ put_ms_nb() [5/24]

void put_ms_nb | ( | int | val,
|  | bool & | success )

Write a 32-bit value to the output stream port. Non-blocking read.

Parameters

  val | 32-bit value datatype
  success | Success of transfer.

## ◆ put_ms_nb() [6/24]

void put_ms_nb | ( | int | val,
|  | int | tlast,
|  | bool & | success )

Write a 32-bit value to the output stream port. Non-blocking read.

Parameters

  val | 32-bit value datatype
  tlast | last word in a packet and the default is fals
  success | Success of transfer.

## ◆ put_ms_nb() [7/24]

void put_ms_nb | ( | unsigned int | val,
|  | bool & | success )

Write a 32-bit value to the output stream port. Non-blocking read.

Parameters

  val | 32-bit value datatype
  success | Success of transfer.

## ◆ put_ms_nb() [8/24]

void put_ms_nb | ( | unsigned int | val,
|  | int | tlast,
|  | bool & | success )

Write a 32-bit value to the output stream port. Non-blocking read.

Parameters

  val | 32-bit value datatype
  tlast | last word in a packet and the default is fals
  success | Success of transfer.

## ◆ put_ms_nb() [9/24]

void put_ms_nb | ( | v2bfloat16 | val,
|  | bool & | success )

Write a 32-bit value to the output stream port. Non-blocking read.

Parameters

  val | 32-bit value datatype
  success | Success of transfer.

## ◆ put_ms_nb() [10/24]

void put_ms_nb | ( | v2bfloat16 | val,
|  | int | tlast,
|  | bool & | success )

Write a 32-bit value to the output stream port. Non-blocking read.

Parameters

  val | 32-bit value datatype
  tlast | last word in a packet and the default is fals
  success | Success of transfer.

## ◆ put_ms_nb() [11/24]

void put_ms_nb | ( | v2float16 | val,
|  | bool & | success )

Write a 32-bit value to the output stream port. Non-blocking read.

Parameters

  val | 32-bit value datatype
  success | Success of transfer.

## ◆ put_ms_nb() [12/24]

void put_ms_nb | ( | v2float16 | val,
|  | int | tlast,
|  | bool & | success )

Write a 32-bit value to the output stream port. Non-blocking read.

Parameters

  val | 32-bit value datatype
  tlast | last word in a packet and the default is fals
  success | Success of transfer.

## ◆ put_ms_nb() [13/24]

void put_ms_nb | ( | v2int16 | val,
|  | bool & | success )

Write a 32-bit value to the output stream port. Non-blocking read.

Parameters

  val | 32-bit value datatype
  success | Success of transfer.

## ◆ put_ms_nb() [14/24]

void put_ms_nb | ( | v2int16 | val,
|  | int | tlast,
|  | bool & | success )

Write a 32-bit value to the output stream port. Non-blocking read.

Parameters

  val | 32-bit value datatype
  tlast | last word in a packet and the default is fals
  success | Success of transfer.

## ◆ put_ms_nb() [15/24]

void put_ms_nb | ( | v2uint16 | val,
|  | bool & | success )

Write a 32-bit value to the output stream port. Non-blocking read.

Parameters

  val | 32-bit value datatype
  success | Success of transfer.

## ◆ put_ms_nb() [16/24]

void put_ms_nb | ( | v2uint16 | val,
|  | int | tlast,
|  | bool & | success )

Write a 32-bit value to the output stream port. Non-blocking read.

Parameters

  val | 32-bit value datatype
  tlast | last word in a packet and the default is fals
  success | Success of transfer.

## ◆ put_ms_nb() [17/24]

void put_ms_nb | ( | v4int8 | val,
|  | bool & | success )

Write a 32-bit value to the output stream port. Non-blocking read.

Parameters

  val | 32-bit value datatype
  success | Success of transfer.

## ◆ put_ms_nb() [18/24]

void put_ms_nb | ( | v4int8 | val,
|  | int | tlast,
|  | bool & | success )

Write a 32-bit value to the output stream port. Non-blocking read.

Parameters

  val | 32-bit value datatype
  tlast | last word in a packet and the default is fals
  success | Success of transfer.

## ◆ put_ms_nb() [19/24]

void put_ms_nb | ( | v4uint8 | val,
|  | bool & | success )

Write a 32-bit value to the output stream port. Non-blocking read.

Parameters

  val | 32-bit value datatype
  success | Success of transfer.

## ◆ put_ms_nb() [20/24]

void put_ms_nb | ( | v4uint8 | val,
|  | int | tlast,
|  | bool & | success )

Write a 32-bit value to the output stream port. Non-blocking read.

Parameters

  val | 32-bit value datatype
  tlast | last word in a packet and the default is fals
  success | Success of transfer.

## ◆ put_ms_nb() [21/24]

void put_ms_nb | ( | v8int4 | val,
|  | bool & | success )

Write a 32-bit value to the output stream port. Non-blocking read.

Parameters

  val | 32-bit value datatype
  success | Success of transfer.

## ◆ put_ms_nb() [22/24]

void put_ms_nb | ( | v8int4 | val,
|  | int | tlast,
|  | bool & | success )

Write a 32-bit value to the output stream port. Non-blocking read.

Parameters

  val | 32-bit value datatype
  tlast | last word in a packet and the default is fals
  success | Success of transfer.

## ◆ put_ms_nb() [23/24]

void put_ms_nb | ( | v8uint4 | val,
|  | bool & | success )

Write a 32-bit value to the output stream port. Non-blocking read.

Parameters

  val | 32-bit value datatype
  success | Success of transfer.

## ◆ put_ms_nb() [24/24]

void put_ms_nb | ( | v8uint4 | val,
|  | int | tlast,
|  | bool & | success )

Write a 32-bit value to the output stream port. Non-blocking read.

Parameters

  val | 32-bit value datatype
  tlast | last word in a packet and the default is fals
  success | Success of transfer.

## ◆ put_ms_nb_ctrl_packet_header() [1/2]

void put_ms_nb_ctrl_packet_header | ( | int | tlast,
|  | unsigned | Addr,
|  | unsigned | n_words,
|  | unsigned | op_type,
|  | unsigned | rspID,
|  | bool & | success )

Generate a control packet header and write it to the output stream port.

Parameters

  tlast | tlast
  Addr | unsigned Local Byte Address (two LSB not used). Accesses are 128 bit aligned.
  n_words | unsigned 2 bits. 1 to 4 words of 32 bit data to follow. This must be a compile time constant.
  op_type | unsigned Operation modes - 2 bit (LSB). 3 modes. 0 - Write without return, 1 - Read with return, 2 - Write with return. The response to a read will be a packet switched stream header and 1 to 4 32 bit word data. The response to a write will be a packet switched stream header. This must be a compile time constant.
  rspID | unsigned Response ID: 5 bit (LSB). Identifies the return destination for operation modes with a return. (The return packet's header's 'dstID' is set to this).
  success | success of transfer

This intrinsic takes an address, number of words, operation type and response ID and returns a control packet header.

Note
  Parameters 'n_words' and 'op_type' must be compile time constants.

## ◆ put_ms_nb_ctrl_packet_header() [2/2]

void put_ms_nb_ctrl_packet_header | ( | unsigned | Addr,
|  | unsigned | n_words,
|  | unsigned | op_type,
|  | unsigned | rspID,
|  | bool & | success )

Generate a control packet header and write it to the output stream port.

Parameters

  Addr | unsigned Local Byte Address (two LSB not used). Accesses are 128 bit aligned.
  n_words | unsigned 2 bits. 1 to 4 words of 32 bit data to follow. This must be a compile time constant.
  op_type | unsigned Operation modes - 2 bit (LSB). 3 modes. 0 - Write without return, 1 - Read with return, 2 - Write with return. The response to a read will be a packet switched stream header and 1 to 4 32 bit word data. The response to a write will be a packet switched stream header. This must be a compile time constant.
  rspID | unsigned Response ID: 5 bit (LSB). Identifies the return destination for operation modes with a return. (The return packet's header's 'dstID' is set to this).
  success | success of transfer

This intrinsic takes an address, number of words, operation type and response ID and returns a control packet header.

Note
  Parameters 'n_words' and 'op_type' must be compile time constants.

## ◆ put_ms_nb_packet_header() [1/2]

void put_ms_nb_packet_header | ( | int | tlast,
|  | unsigned | dstID,
|  | unsigned | pcktType,
|  | bool & | success )

Generate a packet header and write to it to the output stream port.

Parameters

  tlast | tlast
  dstID | unsigned 5 bit (LSB). Identifies the destination of the packet. Should be unique amongst all streams it shares ports with. Can be 32 destinations or more with nested headers.
  pcktType | unsigned 3 bit (LSB). Can be used to distinguish packets with the same source and destination. Control packets set this to 7 if there is an error. This must be a compile time constant.
  success | success of transfer

This intrinsic takes a destination ID and a packet type and returns a packet header.

Note
  Parameter 'pcktType' must be a compile time constant.
  A packet with nested headers has a number of headers at the beginning (instead of the usual single header). For every level of header nesting, the number of possible destinations is multiplied by 32, thus for a two-nested header approach, the number of destinations is already 1024.

## ◆ put_ms_nb_packet_header() [2/2]

void put_ms_nb_packet_header | ( | unsigned | dstID,
|  | unsigned | pcktType,
|  | bool & | success )

Generate a packet header and write to it to the output stream port.

Parameters

  dstID | unsigned 5 bit (LSB). Identifies the destination of the packet. Should be unique amongst all streams it shares ports with. Can be 32 destinations or more with nested headers.
  pcktType | unsigned 3 bit (LSB). Can be used to distinguish packets with the same source and destination. Control packets set this to 7 if there is an error. This must be a compile time constant.
  success | success of transfer

This intrinsic takes a destination ID and a packet type and returns a packet header.

Note
  Parameter 'pcktType' must be a compile time constant.
  A packet with nested headers has a number of headers at the beginning (instead of the usual single header). For every level of header nesting, the number of possible destinations is multiplied by 32, thus for a two-nested header approach, the number of destinations is already 1024.

## ◆ put_ms_packet_header() [1/2]

void put_ms_packet_header | ( | int | tlast,
|  | unsigned | dstID,
|  | unsigned | pcktType )

Generate a packet header and write to it to the output stream port.

Parameters

  tlast | tlast
  dstID | unsigned 5 bit (LSB). Identifies the destination of the packet. Should be unique amongst all streams it shares ports with. Can be 32 destinations or more with nested headers.
  pcktType | unsigned 3 bit (LSB). Can be used to distinguish packets with the same source and destination. Control packets set this to 7 if there is an error. This must be a compile time constant.

This intrinsic takes a destination ID and a packet type and returns a packet header.

Note
  Parameter 'pcktType' must be a compile time constant.
  A packet with nested headers has a number of headers at the beginning (instead of the usual single header). For every level of header nesting, the number of possible destinations is multiplied by 32, thus for a two-nested header approach, the number of destinations is already 1024.

## ◆ put_ms_packet_header() [2/2]

void put_ms_packet_header | ( | unsigned | dstID,
|  | unsigned | pcktType )

Generate a packet header and write to it to the output stream port.

Parameters

  dstID | unsigned 5 bit (LSB). Identifies the destination of the packet. Should be unique amongst all streams it shares ports with. Can be 32 destinations or more with nested headers.
  pcktType | unsigned 3 bit (LSB). Can be used to distinguish packets with the same source and destination. Control packets set this to 7 if there is an error. This must be a compile time constant.

This intrinsic takes a destination ID and a packet type and returns a packet header.

Note
  Parameter 'pcktType' must be a compile time constant.
  A packet with nested headers has a number of headers at the beginning (instead of the usual single header). For every level of header nesting, the number of possible destinations is multiplied by 32, thus for a two-nested header approach, the number of destinations is already 1024.