| AI Engine Intrinsics User Guide (AIE) v2025.2

Loading...
Searching...
No Matches
Modules
Vector MAC with pre-adding and upshifting
Intrinsics » Vector Operations » MAC intrinsics » Multiplication » Advanced » Integer

## Overview

Vector MAC operations allowing pre-addition from within the X buffer, or between the X and Y buffers. The result is then multiplied with data from the Z buffer to generate four lanes. The next four lanes are a column of data seperately selected from the Y buffer which is upshifted.

For general information on all vector MAC intrinsics go here.

## Modules
| 16 bit x 16 bit
| 16 bit x 32 bit