| AI Engine-ML Intrinsics User Guide (v2025.2)

Loading...
Searching...
No Matches
Functions
Broadcast from scalar
Vector Conversions » Broadcast

## Overview

Broadcasts input value to all vector lanes (alternative syntax to broadcast to vector)

## Functions
v32bfloat16 | broadcast_bfloat16 (bfloat16 b)
v16cint16 | broadcast_c16 (cint16 b)
v8cint32 | broadcast_c32 (cint32 b)
v16float | broadcast_float (float b)
v32int16 | broadcast_s16 (int b)
v16int32 | broadcast_s32 (int b)
v16int32 | broadcast_s64 (long long b)
v64int8 | broadcast_s8 (int b)
v32uint16 | broadcast_u16 (unsigned int b)
v16uint32 | broadcast_u32 (unsigned int b)
v16uint32 | broadcast_u64 (unsigned long long b)
v64uint8 | broadcast_u8 (unsigned int b)
v16int32 | broadcast_v2s32 (v2int32 b)
v16uint32 | broadcast_v2u32 (v2uint32 b)

## Function Documentation

## ◆ broadcast_bfloat16()

v32bfloat16 broadcast_bfloat16 | ( | bfloat16 | b | ) |

## ◆ broadcast_c16()

v16cint16 broadcast_c16 | ( | cint16 | b | ) |

## ◆ broadcast_c32()

v8cint32 broadcast_c32 | ( | cint32 | b | ) |

## ◆ broadcast_float()

v16float broadcast_float | ( | float | b | ) |

## ◆ broadcast_s16()

v32int16 broadcast_s16 | ( | int | b | ) |

## ◆ broadcast_s32()

v16int32 broadcast_s32 | ( | int | b | ) |

## ◆ broadcast_s64()

v16int32 broadcast_s64 | ( | long long | b | ) |

## ◆ broadcast_s8()

v64int8 broadcast_s8 | ( | int | b | ) |

## ◆ broadcast_u16()

v32uint16 broadcast_u16 | ( | unsigned int | b | ) |

## ◆ broadcast_u32()

v16uint32 broadcast_u32 | ( | unsigned int | b | ) |

## ◆ broadcast_u64()

v16uint32 broadcast_u64 | ( | unsigned long long | b | ) |

## ◆ broadcast_u8()

v64uint8 broadcast_u8 | ( | unsigned int | b | ) |

## ◆ broadcast_v2s32()

v16int32 broadcast_v2s32 | ( | v2int32 | b | ) |

## ◆ broadcast_v2u32()

v16uint32 broadcast_v2u32 | ( | v2uint32 | b | ) |