| AI Engine-ML v2 Intrinsics User Guide v2025.2

Loading...
Searching...
No Matches
Emulated Multiply-accumulate of Complex Float and Float datatypes
Vector Operations » Multiply Accumulate

Elementwise operations based on the already emulated FP32 operations (see Emulated Multiply-accumulate of 32-bit Floating-Point). These operations might not have optimal performance. More...

## Emulated vector complex float operations
v16caccfloat | mul_elem_16 (v16float v1, v16cfloat v2)
v16caccfloat | negmul_elem_16 (v16float v1, v16cfloat v2)
v16caccfloat | mac_elem_16 (v16float v1, v16cfloat v2, v16caccfloat acc)
v16caccfloat | msc_elem_16 (v16float v1, v16cfloat v2, v16caccfloat acc)
v16caccfloat | mul_elem_16_conf (v16float v1, v16cfloat v2, int sub_mask, int sub_mul)
v16caccfloat | negmul_elem_16_conf (v16float v1, v16cfloat v2, int sub_mask, int sub_mul)
v16caccfloat | mac_elem_16_conf (v16float v1, v16cfloat v2, v16caccfloat acc, int zero_acc, int sub_mask, int sub_mul, int sub_acc1)
v16caccfloat | msc_elem_16_conf (v16float v1, v16cfloat v2, v16caccfloat acc, int zero_acc, int sub_mask, int sub_mul, int sub_acc1)
v16caccfloat | mul_elem_16 (v16cfloat v1, v16float v2)
v16caccfloat | negmul_elem_16 (v16cfloat v1, v16float v2)
v16caccfloat | mac_elem_16 (v16cfloat v1, v16float v2, v16caccfloat acc)
v16caccfloat | msc_elem_16 (v16cfloat v1, v16float v2, v16caccfloat acc)
v16caccfloat | mul_elem_16_conf (v16cfloat v1, v16float v2, int sub_mask, int sub_mul)
v16caccfloat | negmul_elem_16_conf (v16cfloat v1, v16float v2, int sub_mask, int sub_mul)
v16caccfloat | mac_elem_16_conf (v16cfloat v1, v16float v2, v16caccfloat acc, int zero_acc, int sub_mask, int sub_mul, int sub_acc1)
v16caccfloat | msc_elem_16_conf (v16cfloat v1, v16float v2, v16caccfloat acc, int zero_acc, int sub_mask, int sub_mul, int sub_acc1)
v16caccfloat | mul_elem_16 (v16cfloat v1, v16cfloat v2)
v16caccfloat | negmul_elem_16 (v16cfloat v1, v16cfloat v2)
v16caccfloat | mac_elem_16 (v16cfloat v1, v16cfloat v2, v16caccfloat acc)
v16caccfloat | msc_elem_16 (v16cfloat v1, v16cfloat v2, v16caccfloat acc)
v16caccfloat | mul_elem_16_conf (v16cfloat v1, v16cfloat v2, int sub_mask, int sub_mul)
v16caccfloat | negmul_elem_16_conf (v16cfloat v1, v16cfloat v2, int sub_mask, int sub_mul)
v16caccfloat | mac_elem_16_conf (v16cfloat v1, v16cfloat v2, v16caccfloat acc, int zero_acc, int sub_mask, int sub_mul, int sub_acc1)
v16caccfloat | msc_elem_16_conf (v16cfloat v1, v16cfloat v2, v16caccfloat acc, int zero_acc, int sub_mask, int sub_mul, int sub_acc1)
v32caccfloat | mul_elem_32 (v32float v1, v32cfloat v2)
v32caccfloat | negmul_elem_32 (v32float v1, v32cfloat v2)
v32caccfloat | mac_elem_32 (v32float v1, v32cfloat v2, v32caccfloat acc)
v32caccfloat | msc_elem_32 (v32float v1, v32cfloat v2, v32caccfloat acc)
v32caccfloat | mul_elem_32_conf (v32float v1, v32cfloat v2, int sub_mask, int sub_mul)
v32caccfloat | negmul_elem_32_conf (v32float v1, v32cfloat v2, int sub_mask, int sub_mul)
v32caccfloat | mac_elem_32_conf (v32float v1, v32cfloat v2, v32caccfloat acc, int zero_acc, int sub_mask, int sub_mul, int sub_acc1)
v32caccfloat | msc_elem_32_conf (v32float v1, v32cfloat v2, v32caccfloat acc, int zero_acc, int sub_mask, int sub_mul, int sub_acc1)
v32caccfloat | mul_elem_32 (v32cfloat v1, v32float v2)
v32caccfloat | negmul_elem_32 (v32cfloat v1, v32float v2)
v32caccfloat | mac_elem_32 (v32cfloat v1, v32float v2, v32caccfloat acc)
v32caccfloat | msc_elem_32 (v32cfloat v1, v32float v2, v32caccfloat acc)
v32caccfloat | mul_elem_32_conf (v32cfloat v1, v32float v2, int sub_mask, int sub_mul)
v32caccfloat | negmul_elem_32_conf (v32cfloat v1, v32float v2, int sub_mask, int sub_mul)
v32caccfloat | mac_elem_32_conf (v32cfloat v1, v32float v2, v32caccfloat acc, int zero_acc, int sub_mask, int sub_mul, int sub_acc1)
v32caccfloat | msc_elem_32_conf (v32cfloat v1, v32float v2, v32caccfloat acc, int zero_acc, int sub_mask, int sub_mul, int sub_acc1)
v32caccfloat | mul_elem_32 (v32cfloat v1, v32cfloat v2)
v32caccfloat | negmul_elem_32 (v32cfloat v1, v32cfloat v2)
v32caccfloat | mac_elem_32 (v32cfloat v1, v32cfloat v2, v32caccfloat acc)
v32caccfloat | msc_elem_32 (v32cfloat v1, v32cfloat v2, v32caccfloat acc)
v32caccfloat | mul_elem_32_conf (v32cfloat v1, v32cfloat v2, int sub_mask, int sub_mul)
v32caccfloat | negmul_elem_32_conf (v32cfloat v1, v32cfloat v2, int sub_mask, int sub_mul)
v32caccfloat | mac_elem_32_conf (v32cfloat v1, v32cfloat v2, v32caccfloat acc, int zero_acc, int sub_mask, int sub_mul, int sub_acc1)
v32caccfloat | msc_elem_32_conf (v32cfloat v1, v32cfloat v2, v32caccfloat acc, int zero_acc, int sub_mask, int sub_mul, int sub_acc1)
v8caccfloat | mul_2x8_8x4 (v16float v1, v32cfloat v2)
v8caccfloat | negmul_2x8_8x4 (v16float v1, v32cfloat v2)
v8caccfloat | mac_2x8_8x4 (v16float v1, v32cfloat v2, v8caccfloat acc)
v8caccfloat | msc_2x8_8x4 (v16float v1, v32cfloat v2, v8caccfloat acc)
v8caccfloat | mul_2x8_8x4_conf (v16float v1, v32cfloat v2, int sub_mask, int sub_mul)
v8caccfloat | negmul_2x8_8x4_conf (v16float v1, v32cfloat v2, int sub_mask, int sub_mul)
v8caccfloat | mac_2x8_8x4_conf (v16float v1, v32cfloat v2, v8caccfloat acc, int zero_acc, int sub_mask, int sub_mul, int sub_acc1)
v8caccfloat | msc_2x8_8x4_conf (v16float v1, v32cfloat v2, v8caccfloat acc, int zero_acc, int sub_mask, int sub_mul, int sub_acc1)
v8caccfloat | mul_2x8_8x4 (v16cfloat v1, v32float v2)
v8caccfloat | negmul_2x8_8x4 (v16cfloat v1, v32float v2)
v8caccfloat | mac_2x8_8x4 (v16cfloat v1, v32float v2, v8caccfloat acc)
v8caccfloat | msc_2x8_8x4 (v16cfloat v1, v32float v2, v8caccfloat acc)
v8caccfloat | mul_2x8_8x4_conf (v16cfloat v1, v32float v2, int sub_mask, int sub_mul)
v8caccfloat | negmul_2x8_8x4_conf (v16cfloat v1, v32float v2, int sub_mask, int sub_mul)
v8caccfloat | mac_2x8_8x4_conf (v16cfloat v1, v32float v2, v8caccfloat acc, int zero_acc, int sub_mask, int sub_mul, int sub_acc1)
v8caccfloat | msc_2x8_8x4_conf (v16cfloat v1, v32float v2, v8caccfloat acc, int zero_acc, int sub_mask, int sub_mul, int sub_acc1)
v8caccfloat | mul_2x8_8x4 (v16cfloat v1, v32cfloat v2)
v8caccfloat | negmul_2x8_8x4 (v16cfloat v1, v32cfloat v2)
v8caccfloat | mac_2x8_8x4 (v16cfloat v1, v32cfloat v2, v8caccfloat acc)
v8caccfloat | msc_2x8_8x4 (v16cfloat v1, v32cfloat v2, v8caccfloat acc)
v8caccfloat | mul_2x8_8x4_conf (v16cfloat v1, v32cfloat v2, int sub_mask, int sub_mul)
v8caccfloat | negmul_2x8_8x4_conf (v16cfloat v1, v32cfloat v2, int sub_mask, int sub_mul)
v8caccfloat | mac_2x8_8x4_conf (v16cfloat v1, v32cfloat v2, v8caccfloat acc, int zero_acc, int sub_mask, int sub_mul, int sub_acc1)
v8caccfloat | msc_2x8_8x4_conf (v16cfloat v1, v32cfloat v2, v8caccfloat acc, int zero_acc, int sub_mask, int sub_mul, int sub_acc1)

## Detailed Description

Elementwise operations based on the already emulated FP32 operations (see Emulated Multiply-accumulate of 32-bit Floating-Point). These operations might not have optimal performance.

For an explanation how these operations works and the different accuracies provided, please refer to Multiply Accumulate.

## Function Documentation

## ◆ mac_2x8_8x4() [1/3]

v8caccfloat mac_2x8_8x4 | ( | v16cfloat | v1,
|  | v32cfloat | v2,
|  | v8caccfloat | acc )

Parameters

  v1 | Matrix A
  v2 | Matrix B
  acc | Accumulator 1 input

Returns
  Result of operation

## ◆ mac_2x8_8x4() [2/3]

v8caccfloat mac_2x8_8x4 | ( | v16cfloat | v1,
|  | v32float | v2,
|  | v8caccfloat | acc )

Parameters

  v1 | Matrix A
  v2 | Matrix B
  acc | Accumulator 1 input

Returns
  Result of operation

## ◆ mac_2x8_8x4() [3/3]

v8caccfloat mac_2x8_8x4 | ( | v16float | v1,
|  | v32cfloat | v2,
|  | v8caccfloat | acc )

Parameters

  v1 | Matrix A
  v2 | Matrix B
  acc | Accumulator 1 input

Returns
  Result of operation

## ◆ mac_2x8_8x4_conf() [1/3]

v8caccfloat mac_2x8_8x4_conf | ( | v16cfloat | v1,
|  | v32cfloat | v2,
|  | v8caccfloat | acc,
|  | int | zero_acc,
|  | int | sub_mask,
|  | int | sub_mul,
|  | int | sub_acc1 )

Parameters

  v1 | Matrix A
  v2 | Matrix B
  acc | Accumulator 1 input

Returns
  Result of operation

## ◆ mac_2x8_8x4_conf() [2/3]

v8caccfloat mac_2x8_8x4_conf | ( | v16cfloat | v1,
|  | v32float | v2,
|  | v8caccfloat | acc,
|  | int | zero_acc,
|  | int | sub_mask,
|  | int | sub_mul,
|  | int | sub_acc1 )

Parameters

  v1 | Matrix A
  v2 | Matrix B
  acc | Accumulator 1 input

Returns
  Result of operation

## ◆ mac_2x8_8x4_conf() [3/3]

v8caccfloat mac_2x8_8x4_conf | ( | v16float | v1,
|  | v32cfloat | v2,
|  | v8caccfloat | acc,
|  | int | zero_acc,
|  | int | sub_mask,
|  | int | sub_mul,
|  | int | sub_acc1 )

Parameters

  v1 | Matrix A
  v2 | Matrix B
  acc | Accumulator 1 input

Returns
  Result of operation

## ◆ mac_elem_16() [1/3]

v16caccfloat mac_elem_16 | ( | v16cfloat | v1,
|  | v16cfloat | v2,
|  | v16caccfloat | acc )

Parameters

  v1 | Matrix A
  v2 | Matrix B
  acc | Accumulator 1 input

Returns
  Result of operation

## ◆ mac_elem_16() [2/3]

v16caccfloat mac_elem_16 | ( | v16cfloat | v1,
|  | v16float | v2,
|  | v16caccfloat | acc )

Parameters

  v1 | Matrix A
  v2 | Matrix B
  acc | Accumulator 1 input

Returns
  Result of operation

## ◆ mac_elem_16() [3/3]

v16caccfloat mac_elem_16 | ( | v16float | v1,
|  | v16cfloat | v2,
|  | v16caccfloat | acc )

Parameters

  v1 | Matrix A
  v2 | Matrix B
  acc | Accumulator 1 input

Returns
  Result of operation

## ◆ mac_elem_16_conf() [1/3]

v16caccfloat mac_elem_16_conf | ( | v16cfloat | v1,
|  | v16cfloat | v2,
|  | v16caccfloat | acc,
|  | int | zero_acc,
|  | int | sub_mask,
|  | int | sub_mul,
|  | int | sub_acc1 )

Parameters

  v1 | Matrix A
  v2 | Matrix B
  acc | Accumulator 1 input

Returns
  Result of operation

## ◆ mac_elem_16_conf() [2/3]

v16caccfloat mac_elem_16_conf | ( | v16cfloat | v1,
|  | v16float | v2,
|  | v16caccfloat | acc,
|  | int | zero_acc,
|  | int | sub_mask,
|  | int | sub_mul,
|  | int | sub_acc1 )

Parameters

  v1 | Matrix A
  v2 | Matrix B
  acc | Accumulator 1 input

Returns
  Result of operation

## ◆ mac_elem_16_conf() [3/3]

v16caccfloat mac_elem_16_conf | ( | v16float | v1,
|  | v16cfloat | v2,
|  | v16caccfloat | acc,
|  | int | zero_acc,
|  | int | sub_mask,
|  | int | sub_mul,
|  | int | sub_acc1 )

Parameters

  v1 | Matrix A
  v2 | Matrix B
  acc | Accumulator 1 input

Returns
  Result of operation

## ◆ mac_elem_32() [1/3]

v32caccfloat mac_elem_32 | ( | v32cfloat | v1,
|  | v32cfloat | v2,
|  | v32caccfloat | acc )

Parameters

  v1 | Matrix A
  v2 | Matrix B
  acc | Accumulator 1 input

Returns
  Result of operation

## ◆ mac_elem_32() [2/3]

v32caccfloat mac_elem_32 | ( | v32cfloat | v1,
|  | v32float | v2,
|  | v32caccfloat | acc )

Parameters

  v1 | Matrix A
  v2 | Matrix B
  acc | Accumulator 1 input

Returns
  Result of operation

## ◆ mac_elem_32() [3/3]

v32caccfloat mac_elem_32 | ( | v32float | v1,
|  | v32cfloat | v2,
|  | v32caccfloat | acc )

Parameters

  v1 | Matrix A
  v2 | Matrix B
  acc | Accumulator 1 input

Returns
  Result of operation

## ◆ mac_elem_32_conf() [1/3]

v32caccfloat mac_elem_32_conf | ( | v32cfloat | v1,
|  | v32cfloat | v2,
|  | v32caccfloat | acc,
|  | int | zero_acc,
|  | int | sub_mask,
|  | int | sub_mul,
|  | int | sub_acc1 )

Parameters

  v1 | Matrix A
  v2 | Matrix B
  acc | Accumulator 1 input

Returns
  Result of operation

## ◆ mac_elem_32_conf() [2/3]

v32caccfloat mac_elem_32_conf | ( | v32cfloat | v1,
|  | v32float | v2,
|  | v32caccfloat | acc,
|  | int | zero_acc,
|  | int | sub_mask,
|  | int | sub_mul,
|  | int | sub_acc1 )

Parameters

  v1 | Matrix A
  v2 | Matrix B
  acc | Accumulator 1 input

Returns
  Result of operation

## ◆ mac_elem_32_conf() [3/3]

v32caccfloat mac_elem_32_conf | ( | v32float | v1,
|  | v32cfloat | v2,
|  | v32caccfloat | acc,
|  | int | zero_acc,
|  | int | sub_mask,
|  | int | sub_mul,
|  | int | sub_acc1 )

Parameters

  v1 | Matrix A
  v2 | Matrix B
  acc | Accumulator 1 input

Returns
  Result of operation

## ◆ msc_2x8_8x4() [1/3]

v8caccfloat msc_2x8_8x4 | ( | v16cfloat | v1,
|  | v32cfloat | v2,
|  | v8caccfloat | acc )

Parameters

  v1 | Matrix A
  v2 | Matrix B
  acc | Accumulator 1 input

Returns
  Result of operation

## ◆ msc_2x8_8x4() [2/3]

v8caccfloat msc_2x8_8x4 | ( | v16cfloat | v1,
|  | v32float | v2,
|  | v8caccfloat | acc )

Parameters

  v1 | Matrix A
  v2 | Matrix B
  acc | Accumulator 1 input

Returns
  Result of operation

## ◆ msc_2x8_8x4() [3/3]

v8caccfloat msc_2x8_8x4 | ( | v16float | v1,
|  | v32cfloat | v2,
|  | v8caccfloat | acc )

Parameters

  v1 | Matrix A
  v2 | Matrix B
  acc | Accumulator 1 input

Returns
  Result of operation

## ◆ msc_2x8_8x4_conf() [1/3]

v8caccfloat msc_2x8_8x4_conf | ( | v16cfloat | v1,
|  | v32cfloat | v2,
|  | v8caccfloat | acc,
|  | int | zero_acc,
|  | int | sub_mask,
|  | int | sub_mul,
|  | int | sub_acc1 )

Parameters

  v1 | Matrix A
  v2 | Matrix B
  acc | Accumulator 1 input

Returns
  Result of operation

## ◆ msc_2x8_8x4_conf() [2/3]

v8caccfloat msc_2x8_8x4_conf | ( | v16cfloat | v1,
|  | v32float | v2,
|  | v8caccfloat | acc,
|  | int | zero_acc,
|  | int | sub_mask,
|  | int | sub_mul,
|  | int | sub_acc1 )

Parameters

  v1 | Matrix A
  v2 | Matrix B
  acc | Accumulator 1 input

Returns
  Result of operation

## ◆ msc_2x8_8x4_conf() [3/3]

v8caccfloat msc_2x8_8x4_conf | ( | v16float | v1,
|  | v32cfloat | v2,
|  | v8caccfloat | acc,
|  | int | zero_acc,
|  | int | sub_mask,
|  | int | sub_mul,
|  | int | sub_acc1 )

Parameters

  v1 | Matrix A
  v2 | Matrix B
  acc | Accumulator 1 input

Returns
  Result of operation

## ◆ msc_elem_16() [1/3]

v16caccfloat msc_elem_16 | ( | v16cfloat | v1,
|  | v16cfloat | v2,
|  | v16caccfloat | acc )

Parameters

  v1 | Matrix A
  v2 | Matrix B
  acc | Accumulator 1 input

Returns
  Result of operation

## ◆ msc_elem_16() [2/3]

v16caccfloat msc_elem_16 | ( | v16cfloat | v1,
|  | v16float | v2,
|  | v16caccfloat | acc )

Parameters

  v1 | Matrix A
  v2 | Matrix B
  acc | Accumulator 1 input

Returns
  Result of operation

## ◆ msc_elem_16() [3/3]

v16caccfloat msc_elem_16 | ( | v16float | v1,
|  | v16cfloat | v2,
|  | v16caccfloat | acc )

Parameters

  v1 | Matrix A
  v2 | Matrix B
  acc | Accumulator 1 input

Returns
  Result of operation

## ◆ msc_elem_16_conf() [1/3]

v16caccfloat msc_elem_16_conf | ( | v16cfloat | v1,
|  | v16cfloat | v2,
|  | v16caccfloat | acc,
|  | int | zero_acc,
|  | int | sub_mask,
|  | int | sub_mul,
|  | int | sub_acc1 )

Parameters

  v1 | Matrix A
  v2 | Matrix B
  acc | Accumulator 1 input

Returns
  Result of operation

## ◆ msc_elem_16_conf() [2/3]

v16caccfloat msc_elem_16_conf | ( | v16cfloat | v1,
|  | v16float | v2,
|  | v16caccfloat | acc,
|  | int | zero_acc,
|  | int | sub_mask,
|  | int | sub_mul,
|  | int | sub_acc1 )

Parameters

  v1 | Matrix A
  v2 | Matrix B
  acc | Accumulator 1 input

Returns
  Result of operation

## ◆ msc_elem_16_conf() [3/3]

v16caccfloat msc_elem_16_conf | ( | v16float | v1,
|  | v16cfloat | v2,
|  | v16caccfloat | acc,
|  | int | zero_acc,
|  | int | sub_mask,
|  | int | sub_mul,
|  | int | sub_acc1 )

Parameters

  v1 | Matrix A
  v2 | Matrix B
  acc | Accumulator 1 input

Returns
  Result of operation

## ◆ msc_elem_32() [1/3]

v32caccfloat msc_elem_32 | ( | v32cfloat | v1,
|  | v32cfloat | v2,
|  | v32caccfloat | acc )

Parameters

  v1 | Matrix A
  v2 | Matrix B
  acc | Accumulator 1 input

Returns
  Result of operation

## ◆ msc_elem_32() [2/3]

v32caccfloat msc_elem_32 | ( | v32cfloat | v1,
|  | v32float | v2,
|  | v32caccfloat | acc )

Parameters

  v1 | Matrix A
  v2 | Matrix B
  acc | Accumulator 1 input

Returns
  Result of operation

## ◆ msc_elem_32() [3/3]

v32caccfloat msc_elem_32 | ( | v32float | v1,
|  | v32cfloat | v2,
|  | v32caccfloat | acc )

Parameters

  v1 | Matrix A
  v2 | Matrix B
  acc | Accumulator 1 input

Returns
  Result of operation

## ◆ msc_elem_32_conf() [1/3]

v32caccfloat msc_elem_32_conf | ( | v32cfloat | v1,
|  | v32cfloat | v2,
|  | v32caccfloat | acc,
|  | int | zero_acc,
|  | int | sub_mask,
|  | int | sub_mul,
|  | int | sub_acc1 )

Parameters

  v1 | Matrix A
  v2 | Matrix B
  acc | Accumulator 1 input

Returns
  Result of operation

## ◆ msc_elem_32_conf() [2/3]

v32caccfloat msc_elem_32_conf | ( | v32cfloat | v1,
|  | v32float | v2,
|  | v32caccfloat | acc,
|  | int | zero_acc,
|  | int | sub_mask,
|  | int | sub_mul,
|  | int | sub_acc1 )

Parameters

  v1 | Matrix A
  v2 | Matrix B
  acc | Accumulator 1 input

Returns
  Result of operation

## ◆ msc_elem_32_conf() [3/3]

v32caccfloat msc_elem_32_conf | ( | v32float | v1,
|  | v32cfloat | v2,
|  | v32caccfloat | acc,
|  | int | zero_acc,
|  | int | sub_mask,
|  | int | sub_mul,
|  | int | sub_acc1 )

Parameters

  v1 | Matrix A
  v2 | Matrix B
  acc | Accumulator 1 input

Returns
  Result of operation

## ◆ mul_2x8_8x4() [1/3]

v8caccfloat mul_2x8_8x4 | ( | v16cfloat | v1,
|  | v32cfloat | v2 )

Parameters

  v1 | Matrix A
  v2 | Matrix B

Returns
  Result of operation

## ◆ mul_2x8_8x4() [2/3]

v8caccfloat mul_2x8_8x4 | ( | v16cfloat | v1,
|  | v32float | v2 )

Parameters

  v1 | Matrix A
  v2 | Matrix B

Returns
  Result of operation

## ◆ mul_2x8_8x4() [3/3]

v8caccfloat mul_2x8_8x4 | ( | v16float | v1,
|  | v32cfloat | v2 )

Parameters

  v1 | Matrix A
  v2 | Matrix B

Returns
  Result of operation

## ◆ mul_2x8_8x4_conf() [1/3]

v8caccfloat mul_2x8_8x4_conf | ( | v16cfloat | v1,
|  | v32cfloat | v2,
|  | int | sub_mask,
|  | int | sub_mul )

Parameters

  v1 | Matrix A
  v2 | Matrix B

Returns
  Result of operation

## ◆ mul_2x8_8x4_conf() [2/3]

v8caccfloat mul_2x8_8x4_conf | ( | v16cfloat | v1,
|  | v32float | v2,
|  | int | sub_mask,
|  | int | sub_mul )

Parameters

  v1 | Matrix A
  v2 | Matrix B

Returns
  Result of operation

## ◆ mul_2x8_8x4_conf() [3/3]

v8caccfloat mul_2x8_8x4_conf | ( | v16float | v1,
|  | v32cfloat | v2,
|  | int | sub_mask,
|  | int | sub_mul )

Parameters

  v1 | Matrix A
  v2 | Matrix B

Returns
  Result of operation

## ◆ mul_elem_16() [1/3]

v16caccfloat mul_elem_16 | ( | v16cfloat | v1,
|  | v16cfloat | v2 )

Parameters

  v1 | Matrix A
  v2 | Matrix B

Returns
  Result of operation

## ◆ mul_elem_16() [2/3]

v16caccfloat mul_elem_16 | ( | v16cfloat | v1,
|  | v16float | v2 )

Parameters

  v1 | Matrix A
  v2 | Matrix B

Returns
  Result of operation

## ◆ mul_elem_16() [3/3]

v16caccfloat mul_elem_16 | ( | v16float | v1,
|  | v16cfloat | v2 )

Parameters

  v1 | Matrix A
  v2 | Matrix B

Returns
  Result of operation

## ◆ mul_elem_16_conf() [1/3]

v16caccfloat mul_elem_16_conf | ( | v16cfloat | v1,
|  | v16cfloat | v2,
|  | int | sub_mask,
|  | int | sub_mul )

Parameters

  v1 | Matrix A
  v2 | Matrix B

Returns
  Result of operation

## ◆ mul_elem_16_conf() [2/3]

v16caccfloat mul_elem_16_conf | ( | v16cfloat | v1,
|  | v16float | v2,
|  | int | sub_mask,
|  | int | sub_mul )

Parameters

  v1 | Matrix A
  v2 | Matrix B

Returns
  Result of operation

## ◆ mul_elem_16_conf() [3/3]

v16caccfloat mul_elem_16_conf | ( | v16float | v1,
|  | v16cfloat | v2,
|  | int | sub_mask,
|  | int | sub_mul )

Parameters

  v1 | Matrix A
  v2 | Matrix B

Returns
  Result of operation

## ◆ mul_elem_32() [1/3]

v32caccfloat mul_elem_32 | ( | v32cfloat | v1,
|  | v32cfloat | v2 )

Parameters

  v1 | Matrix A
  v2 | Matrix B

Returns
  Result of operation

## ◆ mul_elem_32() [2/3]

v32caccfloat mul_elem_32 | ( | v32cfloat | v1,
|  | v32float | v2 )

Parameters

  v1 | Matrix A
  v2 | Matrix B

Returns
  Result of operation

## ◆ mul_elem_32() [3/3]

v32caccfloat mul_elem_32 | ( | v32float | v1,
|  | v32cfloat | v2 )

Parameters

  v1 | Matrix A
  v2 | Matrix B

Returns
  Result of operation

## ◆ mul_elem_32_conf() [1/3]

v32caccfloat mul_elem_32_conf | ( | v32cfloat | v1,
|  | v32cfloat | v2,
|  | int | sub_mask,
|  | int | sub_mul )

Parameters

  v1 | Matrix A
  v2 | Matrix B

Returns
  Result of operation

## ◆ mul_elem_32_conf() [2/3]

v32caccfloat mul_elem_32_conf | ( | v32cfloat | v1,
|  | v32float | v2,
|  | int | sub_mask,
|  | int | sub_mul )

Parameters

  v1 | Matrix A
  v2 | Matrix B

Returns
  Result of operation

## ◆ mul_elem_32_conf() [3/3]

v32caccfloat mul_elem_32_conf | ( | v32float | v1,
|  | v32cfloat | v2,
|  | int | sub_mask,
|  | int | sub_mul )

Parameters

  v1 | Matrix A
  v2 | Matrix B

Returns
  Result of operation

## ◆ negmul_2x8_8x4() [1/3]

v8caccfloat negmul_2x8_8x4 | ( | v16cfloat | v1,
|  | v32cfloat | v2 )

Parameters

  v1 | Matrix A
  v2 | Matrix B

Returns
  Result of operation

## ◆ negmul_2x8_8x4() [2/3]

v8caccfloat negmul_2x8_8x4 | ( | v16cfloat | v1,
|  | v32float | v2 )

Parameters

  v1 | Matrix A
  v2 | Matrix B

Returns
  Result of operation

## ◆ negmul_2x8_8x4() [3/3]

v8caccfloat negmul_2x8_8x4 | ( | v16float | v1,
|  | v32cfloat | v2 )

Parameters

  v1 | Matrix A
  v2 | Matrix B

Returns
  Result of operation

## ◆ negmul_2x8_8x4_conf() [1/3]

v8caccfloat negmul_2x8_8x4_conf | ( | v16cfloat | v1,
|  | v32cfloat | v2,
|  | int | sub_mask,
|  | int | sub_mul )

Parameters

  v1 | Matrix A
  v2 | Matrix B

Returns
  Result of operation

## ◆ negmul_2x8_8x4_conf() [2/3]

v8caccfloat negmul_2x8_8x4_conf | ( | v16cfloat | v1,
|  | v32float | v2,
|  | int | sub_mask,
|  | int | sub_mul )

Parameters

  v1 | Matrix A
  v2 | Matrix B

Returns
  Result of operation

## ◆ negmul_2x8_8x4_conf() [3/3]

v8caccfloat negmul_2x8_8x4_conf | ( | v16float | v1,
|  | v32cfloat | v2,
|  | int | sub_mask,
|  | int | sub_mul )

Parameters

  v1 | Matrix A
  v2 | Matrix B

Returns
  Result of operation

## ◆ negmul_elem_16() [1/3]

v16caccfloat negmul_elem_16 | ( | v16cfloat | v1,
|  | v16cfloat | v2 )

Parameters

  v1 | Matrix A
  v2 | Matrix B

Returns
  Result of operation

## ◆ negmul_elem_16() [2/3]

v16caccfloat negmul_elem_16 | ( | v16cfloat | v1,
|  | v16float | v2 )

Parameters

  v1 | Matrix A
  v2 | Matrix B

Returns
  Result of operation

## ◆ negmul_elem_16() [3/3]

v16caccfloat negmul_elem_16 | ( | v16float | v1,
|  | v16cfloat | v2 )

Parameters

  v1 | Matrix A
  v2 | Matrix B

Returns
  Result of operation

## ◆ negmul_elem_16_conf() [1/3]

v16caccfloat negmul_elem_16_conf | ( | v16cfloat | v1,
|  | v16cfloat | v2,
|  | int | sub_mask,
|  | int | sub_mul )

Parameters

  v1 | Matrix A
  v2 | Matrix B

Returns
  Result of operation

## ◆ negmul_elem_16_conf() [2/3]

v16caccfloat negmul_elem_16_conf | ( | v16cfloat | v1,
|  | v16float | v2,
|  | int | sub_mask,
|  | int | sub_mul )

Parameters

  v1 | Matrix A
  v2 | Matrix B

Returns
  Result of operation

## ◆ negmul_elem_16_conf() [3/3]

v16caccfloat negmul_elem_16_conf | ( | v16float | v1,
|  | v16cfloat | v2,
|  | int | sub_mask,
|  | int | sub_mul )

Parameters

  v1 | Matrix A
  v2 | Matrix B

Returns
  Result of operation

## ◆ negmul_elem_32() [1/3]

v32caccfloat negmul_elem_32 | ( | v32cfloat | v1,
|  | v32cfloat | v2 )

Parameters

  v1 | Matrix A
  v2 | Matrix B

Returns
  Result of operation

## ◆ negmul_elem_32() [2/3]

v32caccfloat negmul_elem_32 | ( | v32cfloat | v1,
|  | v32float | v2 )

Parameters

  v1 | Matrix A
  v2 | Matrix B

Returns
  Result of operation

## ◆ negmul_elem_32() [3/3]

v32caccfloat negmul_elem_32 | ( | v32float | v1,
|  | v32cfloat | v2 )

Parameters

  v1 | Matrix A
  v2 | Matrix B

Returns
  Result of operation

## ◆ negmul_elem_32_conf() [1/3]

v32caccfloat negmul_elem_32_conf | ( | v32cfloat | v1,
|  | v32cfloat | v2,
|  | int | sub_mask,
|  | int | sub_mul )

Parameters

  v1 | Matrix A
  v2 | Matrix B

Returns
  Result of operation

## ◆ negmul_elem_32_conf() [2/3]

v32caccfloat negmul_elem_32_conf | ( | v32cfloat | v1,
|  | v32float | v2,
|  | int | sub_mask,
|  | int | sub_mul )

Parameters

  v1 | Matrix A
  v2 | Matrix B

Returns
  Result of operation

## ◆ negmul_elem_32_conf() [3/3]

v32caccfloat negmul_elem_32_conf | ( | v32float | v1,
|  | v32cfloat | v2,
|  | int | sub_mask,
|  | int | sub_mul )

Parameters

  v1 | Matrix A
  v2 | Matrix B

Returns
  Result of operation