| AI Engine-ML v2 Intrinsics User Guide v2025.2

Loading...
Searching...
No Matches
Load/store to FIFO registers

## FIFO loads from memory to vector v128int4
void | fifo_ld_reset (v128int4 *&p, fifo_state_t &s)
void | fifo_ld_fill (v128int4 *&p, fifo_state_t &s)
v128int4 | fifo_ld_pop (v128int4 *&p, fifo_state_t &s)
v128int4 | fifo_ld_pop_1d_byte (v128int4 *&p, fifo_state_t &s, int off)
v128int4 | fifo_ld_pop_2d_byte (v128int4 *&p, fifo_state_t &s, int off, int size1, addr_t &count1, int inc1)
v128int4 | fifo_ld_pop_3d_byte (v128int4 *&p, fifo_state_t &s, int off, int size1, addr_t &count1, int inc1, int size2, addr_t &count2, int inc2)

## FIFO loads from memory to vector v128int4 with extra register
v128int4 | fifo_ld_popx (v128int4 *&p, fifo_state_t &s)
v128int4 | fifo_ld_popx (v128int4 *&p, fifo_state_t &s, int step, int mask)

## FIFO loads from memory to vector v128uint4
void | fifo_ld_reset (v128uint4 *&p, fifo_state_t &s)
void | fifo_ld_fill (v128uint4 *&p, fifo_state_t &s)
v128uint4 | fifo_ld_pop (v128uint4 *&p, fifo_state_t &s)
v128uint4 | fifo_ld_pop_1d_byte (v128uint4 *&p, fifo_state_t &s, int off)
v128uint4 | fifo_ld_pop_2d_byte (v128uint4 *&p, fifo_state_t &s, int off, int size1, addr_t &count1, int inc1)
v128uint4 | fifo_ld_pop_3d_byte (v128uint4 *&p, fifo_state_t &s, int off, int size1, addr_t &count1, int inc1, int size2, addr_t &count2, int inc2)

## FIFO loads from memory to vector v128uint4 with extra register
v128uint4 | fifo_ld_popx (v128uint4 *&p, fifo_state_t &s)
v128uint4 | fifo_ld_popx (v128uint4 *&p, fifo_state_t &s, int step, int mask)

## FIFO loads from memory to vector v64int8
void | fifo_ld_reset (v64int8 *&p, fifo_state_t &s)
void | fifo_ld_fill (v64int8 *&p, fifo_state_t &s)
v64int8 | fifo_ld_pop (v64int8 *&p, fifo_state_t &s)
v64int8 | fifo_ld_pop_1d_byte (v64int8 *&p, fifo_state_t &s, int off)
v64int8 | fifo_ld_pop_2d_byte (v64int8 *&p, fifo_state_t &s, int off, int size1, addr_t &count1, int inc1)
v64int8 | fifo_ld_pop_3d_byte (v64int8 *&p, fifo_state_t &s, int off, int size1, addr_t &count1, int inc1, int size2, addr_t &count2, int inc2)

## FIFO loads from memory to vector v64int8 with extra register
v64int8 | fifo_ld_popx (v64int8 *&p, fifo_state_t &s)
v64int8 | fifo_ld_popx (v64int8 *&p, fifo_state_t &s, int step, int mask)

## FIFO loads from memory to vector v64uint8
void | fifo_ld_reset (v64uint8 *&p, fifo_state_t &s)
void | fifo_ld_fill (v64uint8 *&p, fifo_state_t &s)
v64uint8 | fifo_ld_pop (v64uint8 *&p, fifo_state_t &s)
v64uint8 | fifo_ld_pop_1d_byte (v64uint8 *&p, fifo_state_t &s, int off)
v64uint8 | fifo_ld_pop_2d_byte (v64uint8 *&p, fifo_state_t &s, int off, int size1, addr_t &count1, int inc1)
v64uint8 | fifo_ld_pop_3d_byte (v64uint8 *&p, fifo_state_t &s, int off, int size1, addr_t &count1, int inc1, int size2, addr_t &count2, int inc2)

## FIFO loads from memory to vector v64uint8 with extra register
v64uint8 | fifo_ld_popx (v64uint8 *&p, fifo_state_t &s)
v64uint8 | fifo_ld_popx (v64uint8 *&p, fifo_state_t &s, int step, int mask)

## FIFO loads from memory to vector v32int16
void | fifo_ld_reset (v32int16 *&p, fifo_state_t &s)
void | fifo_ld_fill (v32int16 *&p, fifo_state_t &s)
v32int16 | fifo_ld_pop (v32int16 *&p, fifo_state_t &s)
v32int16 | fifo_ld_pop_1d_byte (v32int16 *&p, fifo_state_t &s, int off)
v32int16 | fifo_ld_pop_2d_byte (v32int16 *&p, fifo_state_t &s, int off, int size1, addr_t &count1, int inc1)
v32int16 | fifo_ld_pop_3d_byte (v32int16 *&p, fifo_state_t &s, int off, int size1, addr_t &count1, int inc1, int size2, addr_t &count2, int inc2)

## FIFO loads from memory to vector v32int16 with extra register
v32int16 | fifo_ld_popx (v32int16 *&p, fifo_state_t &s)
v32int16 | fifo_ld_popx (v32int16 *&p, fifo_state_t &s, int step, int mask)

## FIFO loads from memory to vector v32uint16
void | fifo_ld_reset (v32uint16 *&p, fifo_state_t &s)
void | fifo_ld_fill (v32uint16 *&p, fifo_state_t &s)
v32uint16 | fifo_ld_pop (v32uint16 *&p, fifo_state_t &s)
v32uint16 | fifo_ld_pop_1d_byte (v32uint16 *&p, fifo_state_t &s, int off)
v32uint16 | fifo_ld_pop_2d_byte (v32uint16 *&p, fifo_state_t &s, int off, int size1, addr_t &count1, int inc1)
v32uint16 | fifo_ld_pop_3d_byte (v32uint16 *&p, fifo_state_t &s, int off, int size1, addr_t &count1, int inc1, int size2, addr_t &count2, int inc2)

## FIFO loads from memory to vector v32uint16 with extra register
v32uint16 | fifo_ld_popx (v32uint16 *&p, fifo_state_t &s)
v32uint16 | fifo_ld_popx (v32uint16 *&p, fifo_state_t &s, int step, int mask)

## FIFO loads from memory to vector v16int32
void | fifo_ld_reset (v16int32 *&p, fifo_state_t &s)
void | fifo_ld_fill (v16int32 *&p, fifo_state_t &s)
v16int32 | fifo_ld_pop (v16int32 *&p, fifo_state_t &s)
v16int32 | fifo_ld_pop_1d_byte (v16int32 *&p, fifo_state_t &s, int off)
v16int32 | fifo_ld_pop_2d_byte (v16int32 *&p, fifo_state_t &s, int off, int size1, addr_t &count1, int inc1)
v16int32 | fifo_ld_pop_3d_byte (v16int32 *&p, fifo_state_t &s, int off, int size1, addr_t &count1, int inc1, int size2, addr_t &count2, int inc2)

## FIFO loads from memory to vector v16int32 with extra register
v16int32 | fifo_ld_popx (v16int32 *&p, fifo_state_t &s)
v16int32 | fifo_ld_popx (v16int32 *&p, fifo_state_t &s, int step, int mask)

## FIFO loads from memory to vector v16uint32
void | fifo_ld_reset (v16uint32 *&p, fifo_state_t &s)
void | fifo_ld_fill (v16uint32 *&p, fifo_state_t &s)
v16uint32 | fifo_ld_pop (v16uint32 *&p, fifo_state_t &s)
v16uint32 | fifo_ld_pop_1d_byte (v16uint32 *&p, fifo_state_t &s, int off)
v16uint32 | fifo_ld_pop_2d_byte (v16uint32 *&p, fifo_state_t &s, int off, int size1, addr_t &count1, int inc1)
v16uint32 | fifo_ld_pop_3d_byte (v16uint32 *&p, fifo_state_t &s, int off, int size1, addr_t &count1, int inc1, int size2, addr_t &count2, int inc2)

## FIFO loads from memory to vector v16uint32 with extra register
v16uint32 | fifo_ld_popx (v16uint32 *&p, fifo_state_t &s)
v16uint32 | fifo_ld_popx (v16uint32 *&p, fifo_state_t &s, int step, int mask)

## FIFO loads from memory to vector v64bfloat8
void | fifo_ld_reset (v64bfloat8 *&p, fifo_state_t &s)
void | fifo_ld_fill (v64bfloat8 *&p, fifo_state_t &s)
v64bfloat8 | fifo_ld_pop (v64bfloat8 *&p, fifo_state_t &s)
v64bfloat8 | fifo_ld_pop_1d_byte (v64bfloat8 *&p, fifo_state_t &s, int off)
v64bfloat8 | fifo_ld_pop_2d_byte (v64bfloat8 *&p, fifo_state_t &s, int off, int size1, addr_t &count1, int inc1)
v64bfloat8 | fifo_ld_pop_3d_byte (v64bfloat8 *&p, fifo_state_t &s, int off, int size1, addr_t &count1, int inc1, int size2, addr_t &count2, int inc2)

## FIFO loads from memory to vector v64bfloat8 with extra register
v64bfloat8 | fifo_ld_popx (v64bfloat8 *&p, fifo_state_t &s)
v64bfloat8 | fifo_ld_popx (v64bfloat8 *&p, fifo_state_t &s, int step, int mask)

## FIFO loads from memory to vector v64float8
void | fifo_ld_reset (v64float8 *&p, fifo_state_t &s)
void | fifo_ld_fill (v64float8 *&p, fifo_state_t &s)
v64float8 | fifo_ld_pop (v64float8 *&p, fifo_state_t &s)
v64float8 | fifo_ld_pop_1d_byte (v64float8 *&p, fifo_state_t &s, int off)
v64float8 | fifo_ld_pop_2d_byte (v64float8 *&p, fifo_state_t &s, int off, int size1, addr_t &count1, int inc1)
v64float8 | fifo_ld_pop_3d_byte (v64float8 *&p, fifo_state_t &s, int off, int size1, addr_t &count1, int inc1, int size2, addr_t &count2, int inc2)

## FIFO loads from memory to vector v64float8 with extra register
v64float8 | fifo_ld_popx (v64float8 *&p, fifo_state_t &s)
v64float8 | fifo_ld_popx (v64float8 *&p, fifo_state_t &s, int step, int mask)

## FIFO loads from memory to vector v16cint16
void | fifo_ld_reset (v16cint16 *&p, fifo_state_t &s)
void | fifo_ld_fill (v16cint16 *&p, fifo_state_t &s)
v16cint16 | fifo_ld_pop (v16cint16 *&p, fifo_state_t &s)
v16cint16 | fifo_ld_pop_1d_byte (v16cint16 *&p, fifo_state_t &s, int off)
v16cint16 | fifo_ld_pop_2d_byte (v16cint16 *&p, fifo_state_t &s, int off, int size1, addr_t &count1, int inc1)
v16cint16 | fifo_ld_pop_3d_byte (v16cint16 *&p, fifo_state_t &s, int off, int size1, addr_t &count1, int inc1, int size2, addr_t &count2, int inc2)

## FIFO loads from memory to vector v16cint16 with extra register
v16cint16 | fifo_ld_popx (v16cint16 *&p, fifo_state_t &s)
v16cint16 | fifo_ld_popx (v16cint16 *&p, fifo_state_t &s, int step, int mask)

## FIFO loads from memory to vector v8cint32
void | fifo_ld_reset (v8cint32 *&p, fifo_state_t &s)
void | fifo_ld_fill (v8cint32 *&p, fifo_state_t &s)
v8cint32 | fifo_ld_pop (v8cint32 *&p, fifo_state_t &s)
v8cint32 | fifo_ld_pop_1d_byte (v8cint32 *&p, fifo_state_t &s, int off)
v8cint32 | fifo_ld_pop_2d_byte (v8cint32 *&p, fifo_state_t &s, int off, int size1, addr_t &count1, int inc1)
v8cint32 | fifo_ld_pop_3d_byte (v8cint32 *&p, fifo_state_t &s, int off, int size1, addr_t &count1, int inc1, int size2, addr_t &count2, int inc2)

## FIFO loads from memory to vector v8cint32 with extra register
v8cint32 | fifo_ld_popx (v8cint32 *&p, fifo_state_t &s)
v8cint32 | fifo_ld_popx (v8cint32 *&p, fifo_state_t &s, int step, int mask)

## FIFO loads from memory to vector v32float16
void | fifo_ld_reset (v32float16 *&p, fifo_state_t &s)
void | fifo_ld_fill (v32float16 *&p, fifo_state_t &s)
v32float16 | fifo_ld_pop (v32float16 *&p, fifo_state_t &s)
v32float16 | fifo_ld_pop_1d_byte (v32float16 *&p, fifo_state_t &s, int off)
v32float16 | fifo_ld_pop_2d_byte (v32float16 *&p, fifo_state_t &s, int off, int size1, addr_t &count1, int inc1)
v32float16 | fifo_ld_pop_3d_byte (v32float16 *&p, fifo_state_t &s, int off, int size1, addr_t &count1, int inc1, int size2, addr_t &count2, int inc2)

## FIFO loads from memory to vector v32float16 with extra register
v32float16 | fifo_ld_popx (v32float16 *&p, fifo_state_t &s)
v32float16 | fifo_ld_popx (v32float16 *&p, fifo_state_t &s, int step, int mask)

## FIFO loads from memory to vector v32bfloat16
void | fifo_ld_reset (v32bfloat16 *&p, fifo_state_t &s)
void | fifo_ld_fill (v32bfloat16 *&p, fifo_state_t &s)
v32bfloat16 | fifo_ld_pop (v32bfloat16 *&p, fifo_state_t &s)
v32bfloat16 | fifo_ld_pop_1d_byte (v32bfloat16 *&p, fifo_state_t &s, int off)
v32bfloat16 | fifo_ld_pop_2d_byte (v32bfloat16 *&p, fifo_state_t &s, int off, int size1, addr_t &count1, int inc1)
v32bfloat16 | fifo_ld_pop_3d_byte (v32bfloat16 *&p, fifo_state_t &s, int off, int size1, addr_t &count1, int inc1, int size2, addr_t &count2, int inc2)

## FIFO loads from memory to vector v32bfloat16 with extra register
v32bfloat16 | fifo_ld_popx (v32bfloat16 *&p, fifo_state_t &s)
v32bfloat16 | fifo_ld_popx (v32bfloat16 *&p, fifo_state_t &s, int step, int mask)

## FIFO loads from memory to vector v16float
void | fifo_ld_reset (v16float *&p, fifo_state_t &s)
void | fifo_ld_fill (v16float *&p, fifo_state_t &s)
v16float | fifo_ld_pop (v16float *&p, fifo_state_t &s)
v16float | fifo_ld_pop_1d_byte (v16float *&p, fifo_state_t &s, int off)
v16float | fifo_ld_pop_2d_byte (v16float *&p, fifo_state_t &s, int off, int size1, addr_t &count1, int inc1)
v16float | fifo_ld_pop_3d_byte (v16float *&p, fifo_state_t &s, int off, int size1, addr_t &count1, int inc1, int size2, addr_t &count2, int inc2)

## FIFO loads from memory to vector v16float with extra register
v16float | fifo_ld_popx (v16float *&p, fifo_state_t &s)
v16float | fifo_ld_popx (v16float *&p, fifo_state_t &s, int step, int mask)

## FIFO loads from memory to vector v8cfloat
void | fifo_ld_reset (v8cfloat *&p, fifo_state_t &s)
void | fifo_ld_fill (v8cfloat *&p, fifo_state_t &s)
v8cfloat | fifo_ld_pop (v8cfloat *&p, fifo_state_t &s)
v8cfloat | fifo_ld_pop_1d_byte (v8cfloat *&p, fifo_state_t &s, int off)
v8cfloat | fifo_ld_pop_2d_byte (v8cfloat *&p, fifo_state_t &s, int off, int size1, addr_t &count1, int inc1)
v8cfloat | fifo_ld_pop_3d_byte (v8cfloat *&p, fifo_state_t &s, int off, int size1, addr_t &count1, int inc1, int size2, addr_t &count2, int inc2)

## FIFO loads from memory to vector v8cfloat with extra register
v8cfloat | fifo_ld_popx (v8cfloat *&p, fifo_state_t &s)
v8cfloat | fifo_ld_popx (v8cfloat *&p, fifo_state_t &s, int step, int mask)

## FIFO loads from memory to vector v16cbfloat16
void | fifo_ld_reset (v16cbfloat16 *&p, fifo_state_t &s)
void | fifo_ld_fill (v16cbfloat16 *&p, fifo_state_t &s)
v16cbfloat16 | fifo_ld_pop (v16cbfloat16 *&p, fifo_state_t &s)
v16cbfloat16 | fifo_ld_pop_1d_byte (v16cbfloat16 *&p, fifo_state_t &s, int off)
v16cbfloat16 | fifo_ld_pop_2d_byte (v16cbfloat16 *&p, fifo_state_t &s, int off, int size1, addr_t &count1, int inc1)
v16cbfloat16 | fifo_ld_pop_3d_byte (v16cbfloat16 *&p, fifo_state_t &s, int off, int size1, addr_t &count1, int inc1, int size2, addr_t &count2, int inc2)

## FIFO loads from memory to vector v16cbfloat16 with extra register
v16cbfloat16 | fifo_ld_popx (v16cbfloat16 *&p, fifo_state_t &s)
v16cbfloat16 | fifo_ld_popx (v16cbfloat16 *&p, fifo_state_t &s, int step, int mask)

## FIFO loads from memory to vector v256uint4_sparse
void | fifo_ld_reset (v256uint4_sparse_unaligned *&p, fifo_state_t &s)
void | fifo_ld_fill (v256uint4_sparse_unaligned *&p, fifo_state_t &s)
v256uint4_sparse | fifo_ld_pop (v256uint4_sparse_unaligned *&p, fifo_state_t &s)
v256uint4_sparse | fifo_ld_pop_1d_byte (v256uint4_sparse_unaligned *&p, fifo_state_t &s, int off)
v256uint4_sparse | fifo_ld_pop_2d_byte (v256uint4_sparse_unaligned *&p, fifo_state_t &s, int off, int size1, addr_t &count1, int inc1)
v256uint4_sparse | fifo_ld_pop_3d_byte (v256uint4_sparse_unaligned *&p, fifo_state_t &s, int off, int size1, addr_t &count1, int inc1, int size2, addr_t &count2, int inc2)

## FIFO loads from memory to vector v128uint8_sparse
void | fifo_ld_reset (v128uint8_sparse_unaligned *&p, fifo_state_t &s)
void | fifo_ld_fill (v128uint8_sparse_unaligned *&p, fifo_state_t &s)
v128uint8_sparse | fifo_ld_pop (v128uint8_sparse_unaligned *&p, fifo_state_t &s)
v128uint8_sparse | fifo_ld_pop_1d_byte (v128uint8_sparse_unaligned *&p, fifo_state_t &s, int off)
v128uint8_sparse | fifo_ld_pop_2d_byte (v128uint8_sparse_unaligned *&p, fifo_state_t &s, int off, int size1, addr_t &count1, int inc1)
v128uint8_sparse | fifo_ld_pop_3d_byte (v128uint8_sparse_unaligned *&p, fifo_state_t &s, int off, int size1, addr_t &count1, int inc1, int size2, addr_t &count2, int inc2)

## FIFO loads from memory to vector v64uint16_sparse
void | fifo_ld_reset (v64uint16_sparse_unaligned *&p, fifo_state_t &s)
void | fifo_ld_fill (v64uint16_sparse_unaligned *&p, fifo_state_t &s)
v64uint16_sparse | fifo_ld_pop (v64uint16_sparse_unaligned *&p, fifo_state_t &s)
v64uint16_sparse | fifo_ld_pop_1d_byte (v64uint16_sparse_unaligned *&p, fifo_state_t &s, int off)
v64uint16_sparse | fifo_ld_pop_2d_byte (v64uint16_sparse_unaligned *&p, fifo_state_t &s, int off, int size1, addr_t &count1, int inc1)
v64uint16_sparse | fifo_ld_pop_3d_byte (v64uint16_sparse_unaligned *&p, fifo_state_t &s, int off, int size1, addr_t &count1, int inc1, int size2, addr_t &count2, int inc2)

## FIFO loads from memory to vector v256int4_sparse
void | fifo_ld_reset (v256int4_sparse_unaligned *&p, fifo_state_t &s)
void | fifo_ld_fill (v256int4_sparse_unaligned *&p, fifo_state_t &s)
v256int4_sparse | fifo_ld_pop (v256int4_sparse_unaligned *&p, fifo_state_t &s)
v256int4_sparse | fifo_ld_pop_1d_byte (v256int4_sparse_unaligned *&p, fifo_state_t &s, int off)
v256int4_sparse | fifo_ld_pop_2d_byte (v256int4_sparse_unaligned *&p, fifo_state_t &s, int off, int size1, addr_t &count1, int inc1)
v256int4_sparse | fifo_ld_pop_3d_byte (v256int4_sparse_unaligned *&p, fifo_state_t &s, int off, int size1, addr_t &count1, int inc1, int size2, addr_t &count2, int inc2)

## FIFO loads from memory to vector v128int8_sparse
void | fifo_ld_reset (v128int8_sparse_unaligned *&p, fifo_state_t &s)
void | fifo_ld_fill (v128int8_sparse_unaligned *&p, fifo_state_t &s)
v128int8_sparse | fifo_ld_pop (v128int8_sparse_unaligned *&p, fifo_state_t &s)
v128int8_sparse | fifo_ld_pop_1d_byte (v128int8_sparse_unaligned *&p, fifo_state_t &s, int off)
v128int8_sparse | fifo_ld_pop_2d_byte (v128int8_sparse_unaligned *&p, fifo_state_t &s, int off, int size1, addr_t &count1, int inc1)
v128int8_sparse | fifo_ld_pop_3d_byte (v128int8_sparse_unaligned *&p, fifo_state_t &s, int off, int size1, addr_t &count1, int inc1, int size2, addr_t &count2, int inc2)

## FIFO loads from memory to vector v64int16_sparse
void | fifo_ld_reset (v64int16_sparse_unaligned *&p, fifo_state_t &s)
void | fifo_ld_fill (v64int16_sparse_unaligned *&p, fifo_state_t &s)
v64int16_sparse | fifo_ld_pop (v64int16_sparse_unaligned *&p, fifo_state_t &s)
v64int16_sparse | fifo_ld_pop_1d_byte (v64int16_sparse_unaligned *&p, fifo_state_t &s, int off)
v64int16_sparse | fifo_ld_pop_2d_byte (v64int16_sparse_unaligned *&p, fifo_state_t &s, int off, int size1, addr_t &count1, int inc1)
v64int16_sparse | fifo_ld_pop_3d_byte (v64int16_sparse_unaligned *&p, fifo_state_t &s, int off, int size1, addr_t &count1, int inc1, int size2, addr_t &count2, int inc2)

## FIFO loads from memory to vector v64bfloat16_sparse
void | fifo_ld_reset (v64bfloat16_sparse_unaligned *&p, fifo_state_t &s)
void | fifo_ld_fill (v64bfloat16_sparse_unaligned *&p, fifo_state_t &s)
v64bfloat16_sparse | fifo_ld_pop (v64bfloat16_sparse_unaligned *&p, fifo_state_t &s)
v64bfloat16_sparse | fifo_ld_pop_1d_byte (v64bfloat16_sparse_unaligned *&p, fifo_state_t &s, int off)
v64bfloat16_sparse | fifo_ld_pop_2d_byte (v64bfloat16_sparse_unaligned *&p, fifo_state_t &s, int off, int size1, addr_t &count1, int inc1)
v64bfloat16_sparse | fifo_ld_pop_3d_byte (v64bfloat16_sparse_unaligned *&p, fifo_state_t &s, int off, int size1, addr_t &count1, int inc1, int size2, addr_t &count2, int inc2)

## FIFO loads from memory to vector v64float16_sparse
void | fifo_ld_reset (v64float16_sparse_unaligned *&p, fifo_state_t &s)
void | fifo_ld_fill (v64float16_sparse_unaligned *&p, fifo_state_t &s)
v64float16_sparse | fifo_ld_pop (v64float16_sparse_unaligned *&p, fifo_state_t &s)
v64float16_sparse | fifo_ld_pop_1d_byte (v64float16_sparse_unaligned *&p, fifo_state_t &s, int off)
v64float16_sparse | fifo_ld_pop_2d_byte (v64float16_sparse_unaligned *&p, fifo_state_t &s, int off, int size1, addr_t &count1, int inc1)
v64float16_sparse | fifo_ld_pop_3d_byte (v64float16_sparse_unaligned *&p, fifo_state_t &s, int off, int size1, addr_t &count1, int inc1, int size2, addr_t &count2, int inc2)

## FIFO loads from memory to vector v128bfloat8_sparse
void | fifo_ld_reset (v128bfloat8_sparse_unaligned *&p, fifo_state_t &s)
void | fifo_ld_fill (v128bfloat8_sparse_unaligned *&p, fifo_state_t &s)
v128bfloat8_sparse | fifo_ld_pop (v128bfloat8_sparse_unaligned *&p, fifo_state_t &s)
v128bfloat8_sparse | fifo_ld_pop_1d_byte (v128bfloat8_sparse_unaligned *&p, fifo_state_t &s, int off)
v128bfloat8_sparse | fifo_ld_pop_2d_byte (v128bfloat8_sparse_unaligned *&p, fifo_state_t &s, int off, int size1, addr_t &count1, int inc1)
v128bfloat8_sparse | fifo_ld_pop_3d_byte (v128bfloat8_sparse_unaligned *&p, fifo_state_t &s, int off, int size1, addr_t &count1, int inc1, int size2, addr_t &count2, int inc2)

## FIFO loads from memory to vector v128float8_sparse
void | fifo_ld_reset (v128float8_sparse_unaligned *&p, fifo_state_t &s)
void | fifo_ld_fill (v128float8_sparse_unaligned *&p, fifo_state_t &s)
v128float8_sparse | fifo_ld_pop (v128float8_sparse_unaligned *&p, fifo_state_t &s)
v128float8_sparse | fifo_ld_pop_1d_byte (v128float8_sparse_unaligned *&p, fifo_state_t &s, int off)
v128float8_sparse | fifo_ld_pop_2d_byte (v128float8_sparse_unaligned *&p, fifo_state_t &s, int off, int size1, addr_t &count1, int inc1)
v128float8_sparse | fifo_ld_pop_3d_byte (v128float8_sparse_unaligned *&p, fifo_state_t &s, int off, int size1, addr_t &count1, int inc1, int size2, addr_t &count2, int inc2)

## FIFO loads from memory to vector v64mx9
void | fifo_ld_reset (v64mx9_unaligned *&p, fifo_state_t &s)
void | fifo_ld_fill (v64mx9_unaligned *&p, fifo_state_t &s)
v64mx9 | fifo_ld_pop (v64mx9_unaligned *&p, fifo_state_t &s)
v64mx9 | fifo_ld_pop_1d_byte (v64mx9_unaligned *&p, fifo_state_t &s, int off)
v64mx9 | fifo_ld_pop_2d_byte (v64mx9_unaligned *&p, fifo_state_t &s, int off, int size1, addr_t &count1, int inc1)
v64mx9 | fifo_ld_pop_3d_byte (v64mx9_unaligned *&p, fifo_state_t &s, int off, int size1, addr_t &count1, int inc1, int size2, addr_t &count2, int inc2)

## FIFO loads from memory to vector v64mx9 with extra register
void | fifo_ld_fillx (v64mx9_unaligned *&p, fifo_state_t &s)
void | fifo_ld_fillx (v64mx9_unaligned *&p, fifo_state_t &s, int step, int mask)

## FIFO loads from memory to vector v128mx6
void | fifo_ld_reset (v128mx6_unaligned *&p, fifo_state_t &s)
void | fifo_ld_fill (v128mx6_unaligned *&p, fifo_state_t &s)
v128mx6 | fifo_ld_pop (v128mx6_unaligned *&p, fifo_state_t &s)
v128mx6 | fifo_ld_pop_1d_byte (v128mx6_unaligned *&p, fifo_state_t &s, int off)
v128mx6 | fifo_ld_pop_2d_byte (v128mx6_unaligned *&p, fifo_state_t &s, int off, int size1, addr_t &count1, int inc1)
v128mx6 | fifo_ld_pop_3d_byte (v128mx6_unaligned *&p, fifo_state_t &s, int off, int size1, addr_t &count1, int inc1, int size2, addr_t &count2, int inc2)

## FIFO loads from memory to vector v128mx6 with extra register
void | fifo_ld_fillx (v128mx6_unaligned *&p, fifo_state_t &s)
void | fifo_ld_fillx (v128mx6_unaligned *&p, fifo_state_t &s, int step, int mask)

## FIFO loads from memory to vector v128mx4
void | fifo_ld_reset (v128mx4_unaligned *&p, fifo_state_t &s)
void | fifo_ld_fill (v128mx4_unaligned *&p, fifo_state_t &s)
v128mx4 | fifo_ld_pop (v128mx4_unaligned *&p, fifo_state_t &s)
v128mx4 | fifo_ld_pop_1d_byte (v128mx4_unaligned *&p, fifo_state_t &s, int off)
v128mx4 | fifo_ld_pop_2d_byte (v128mx4_unaligned *&p, fifo_state_t &s, int off, int size1, addr_t &count1, int inc1)
v128mx4 | fifo_ld_pop_3d_byte (v128mx4_unaligned *&p, fifo_state_t &s, int off, int size1, addr_t &count1, int inc1, int size2, addr_t &count2, int inc2)

## FIFO loads from memory to vector v128mx4 with extra register
void | fifo_ld_fillx (v128mx4_unaligned *&p, fifo_state_t &s)
void | fifo_ld_fillx (v128mx4_unaligned *&p, fifo_state_t &s, int step, int mask)

## FIFO loads from memory to vector v512uint4_sparse
void | fifo_ld_reset (v512uint4_sparse_unaligned *&p, fifo_state_t &fifo)
void | fifo_ld_fill (v512uint4_sparse_unaligned *&p, fifo_state_t &fifo)
v512uint4_sparse | fifo_ld_pop (v512uint4_sparse_unaligned *&p, fifo_state_t &fifo)

## FIFO loads from memory to vector v256uint8_sparse
void | fifo_ld_reset (v256uint8_sparse_unaligned *&p, fifo_state_t &fifo)
void | fifo_ld_fill (v256uint8_sparse_unaligned *&p, fifo_state_t &fifo)
v256uint8_sparse | fifo_ld_pop (v256uint8_sparse_unaligned *&p, fifo_state_t &fifo)

## FIFO loads from memory to vector v128uint16_sparse
void | fifo_ld_reset (v128uint16_sparse_unaligned *&p, fifo_state_t &fifo)
void | fifo_ld_fill (v128uint16_sparse_unaligned *&p, fifo_state_t &fifo)
v128uint16_sparse | fifo_ld_pop (v128uint16_sparse_unaligned *&p, fifo_state_t &fifo)

## FIFO loads from memory to vector v512int4_sparse
void | fifo_ld_reset (v512int4_sparse_unaligned *&p, fifo_state_t &fifo)
void | fifo_ld_fill (v512int4_sparse_unaligned *&p, fifo_state_t &fifo)
v512int4_sparse | fifo_ld_pop (v512int4_sparse_unaligned *&p, fifo_state_t &fifo)

## FIFO loads from memory to vector v256int8_sparse
void | fifo_ld_reset (v256int8_sparse_unaligned *&p, fifo_state_t &fifo)
void | fifo_ld_fill (v256int8_sparse_unaligned *&p, fifo_state_t &fifo)
v256int8_sparse | fifo_ld_pop (v256int8_sparse_unaligned *&p, fifo_state_t &fifo)

## FIFO loads from memory to vector v128int16_sparse
void | fifo_ld_reset (v128int16_sparse_unaligned *&p, fifo_state_t &fifo)
void | fifo_ld_fill (v128int16_sparse_unaligned *&p, fifo_state_t &fifo)
v128int16_sparse | fifo_ld_pop (v128int16_sparse_unaligned *&p, fifo_state_t &fifo)

## FIFO loads from memory to vector v128bfloat16_sparse
void | fifo_ld_reset (v128bfloat16_sparse_unaligned *&p, fifo_state_t &fifo)
void | fifo_ld_fill (v128bfloat16_sparse_unaligned *&p, fifo_state_t &fifo)
v128bfloat16_sparse | fifo_ld_pop (v128bfloat16_sparse_unaligned *&p, fifo_state_t &fifo)

## FIFO loads from memory to vector v128float16_sparse
void | fifo_ld_reset (v128float16_sparse_unaligned *&p, fifo_state_t &fifo)
void | fifo_ld_fill (v128float16_sparse_unaligned *&p, fifo_state_t &fifo)
v128float16_sparse | fifo_ld_pop (v128float16_sparse_unaligned *&p, fifo_state_t &fifo)

## FIFO loads from memory to vector v256bfloat8_sparse
void | fifo_ld_reset (v256bfloat8_sparse_unaligned *&p, fifo_state_t &fifo)
void | fifo_ld_fill (v256bfloat8_sparse_unaligned *&p, fifo_state_t &fifo)
v256bfloat8_sparse | fifo_ld_pop (v256bfloat8_sparse_unaligned *&p, fifo_state_t &fifo)

## FIFO loads from memory to vector v256float8_sparse
void | fifo_ld_reset (v256float8_sparse_unaligned *&p, fifo_state_t &fifo)
void | fifo_ld_fill (v256float8_sparse_unaligned *&p, fifo_state_t &fifo)
v256float8_sparse | fifo_ld_pop (v256float8_sparse_unaligned *&p, fifo_state_t &fifo)

## FIFO loads from memory to vector v256mx6
void | fifo_ld_reset (v256mx6_unaligned *&p, fifo_state_t &fifo)
void | fifo_ld_fill (v256mx6_unaligned *&p, fifo_state_t &fifo)
v256mx6 | fifo_ld_pop (v256mx6_unaligned *&p, fifo_state_t &fifo)

## FIFO loads from memory to vector v256mx4
void | fifo_ld_reset (v256mx4_unaligned *&p, fifo_state_t &fifo)
void | fifo_ld_fill (v256mx4_unaligned *&p, fifo_state_t &fifo)
v256mx4 | fifo_ld_pop (v256mx4_unaligned *&p, fifo_state_t &fifo)

## FIFO stores to memory from register v128int4
void | fifo_st_reset (v128int4 *p, v128int4 v, v128int4 *&p_o, sparse_fifo_t &fifo_o, int &pos_o)
void | fifo_st_reset (v128int4 *&p, v128int4 v, fifo_state_t &s)
void | fifo_st_push (v128int4 *&p, v128int4 v, fifo_state_t &s)
void | fifo_st_flush (v128int4 *&p, fifo_state_t &s)
void | fifo_st_flush_1d_byte (v128int4 *&p, fifo_state_t &s, int off)
void | fifo_st_flush_2d_byte (v128int4 *&p, fifo_state_t &s, int off, int size1, addr_t &count1, int inc1)
void | fifo_st_flush_3d_byte (v128int4 *&p, fifo_state_t &s, int off, int size1, addr_t &count1, int inc1, int size2, addr_t &count2, int inc2)
void | fifo_st_flush_bare (v128int4 *&p, fifo_state_t &s)
void | fifo_st_flush_bare_1d_byte (v128int4 *&p, fifo_state_t &s, int off)
void | fifo_st_flush_bare_2d_byte (v128int4 *&p, fifo_state_t &s, int off, int size1, addr_t &count1, int inc1)
void | fifo_st_flush_bare_3d_byte (v128int4 *&p, fifo_state_t &s, int off, int size1, addr_t &count1, int inc1, int size2, addr_t &count2, int inc2)
void | fifo_st_flush_conv (v128int4 *&p, fifo_state_t &s)
void | fifo_st_flush_conv_1d_byte (v128int4 *&p, fifo_state_t &s, int off)
void | fifo_st_flush_conv_2d_byte (v128int4 *&p, fifo_state_t &s, int off, int size1, addr_t &count1, int inc1)
void | fifo_st_flush_conv_3d_byte (v128int4 *&p, fifo_state_t &s, int off, int size1, addr_t &count1, int inc1, int size2, addr_t &count2, int inc2)

## FIFO stores to memory from register v128uint4
void | fifo_st_reset (v128uint4 *p, v128uint4 v, v128uint4 *&p_o, sparse_fifo_t &fifo_o, int &pos_o)
void | fifo_st_reset (v128uint4 *&p, v128uint4 v, fifo_state_t &s)
void | fifo_st_push (v128uint4 *&p, v128uint4 v, fifo_state_t &s)
void | fifo_st_flush (v128uint4 *&p, fifo_state_t &s)
void | fifo_st_flush_1d_byte (v128uint4 *&p, fifo_state_t &s, int off)
void | fifo_st_flush_2d_byte (v128uint4 *&p, fifo_state_t &s, int off, int size1, addr_t &count1, int inc1)
void | fifo_st_flush_3d_byte (v128uint4 *&p, fifo_state_t &s, int off, int size1, addr_t &count1, int inc1, int size2, addr_t &count2, int inc2)
void | fifo_st_flush_bare (v128uint4 *&p, fifo_state_t &s)
void | fifo_st_flush_bare_1d_byte (v128uint4 *&p, fifo_state_t &s, int off)
void | fifo_st_flush_bare_2d_byte (v128uint4 *&p, fifo_state_t &s, int off, int size1, addr_t &count1, int inc1)
void | fifo_st_flush_bare_3d_byte (v128uint4 *&p, fifo_state_t &s, int off, int size1, addr_t &count1, int inc1, int size2, addr_t &count2, int inc2)
void | fifo_st_flush_conv (v128uint4 *&p, fifo_state_t &s)
void | fifo_st_flush_conv_1d_byte (v128uint4 *&p, fifo_state_t &s, int off)
void | fifo_st_flush_conv_2d_byte (v128uint4 *&p, fifo_state_t &s, int off, int size1, addr_t &count1, int inc1)
void | fifo_st_flush_conv_3d_byte (v128uint4 *&p, fifo_state_t &s, int off, int size1, addr_t &count1, int inc1, int size2, addr_t &count2, int inc2)

## FIFO stores to memory from register v64int8
void | fifo_st_reset (v64int8 *p, v64int8 v, v64int8 *&p_o, sparse_fifo_t &fifo_o, int &pos_o)
void | fifo_st_reset (v64int8 *&p, v64int8 v, fifo_state_t &s)
void | fifo_st_push (v64int8 *&p, v64int8 v, fifo_state_t &s)
void | fifo_st_flush (v64int8 *&p, fifo_state_t &s)
void | fifo_st_flush_1d_byte (v64int8 *&p, fifo_state_t &s, int off)
void | fifo_st_flush_2d_byte (v64int8 *&p, fifo_state_t &s, int off, int size1, addr_t &count1, int inc1)
void | fifo_st_flush_3d_byte (v64int8 *&p, fifo_state_t &s, int off, int size1, addr_t &count1, int inc1, int size2, addr_t &count2, int inc2)
void | fifo_st_flush_bare (v64int8 *&p, fifo_state_t &s)
void | fifo_st_flush_bare_1d_byte (v64int8 *&p, fifo_state_t &s, int off)
void | fifo_st_flush_bare_2d_byte (v64int8 *&p, fifo_state_t &s, int off, int size1, addr_t &count1, int inc1)
void | fifo_st_flush_bare_3d_byte (v64int8 *&p, fifo_state_t &s, int off, int size1, addr_t &count1, int inc1, int size2, addr_t &count2, int inc2)
void | fifo_st_flush_conv (v64int8 *&p, fifo_state_t &s)
void | fifo_st_flush_conv_1d_byte (v64int8 *&p, fifo_state_t &s, int off)
void | fifo_st_flush_conv_2d_byte (v64int8 *&p, fifo_state_t &s, int off, int size1, addr_t &count1, int inc1)
void | fifo_st_flush_conv_3d_byte (v64int8 *&p, fifo_state_t &s, int off, int size1, addr_t &count1, int inc1, int size2, addr_t &count2, int inc2)

## FIFO stores to memory from register v64uint8
void | fifo_st_reset (v64uint8 *p, v64uint8 v, v64uint8 *&p_o, sparse_fifo_t &fifo_o, int &pos_o)
void | fifo_st_reset (v64uint8 *&p, v64uint8 v, fifo_state_t &s)
void | fifo_st_push (v64uint8 *&p, v64uint8 v, fifo_state_t &s)
void | fifo_st_flush (v64uint8 *&p, fifo_state_t &s)
void | fifo_st_flush_1d_byte (v64uint8 *&p, fifo_state_t &s, int off)
void | fifo_st_flush_2d_byte (v64uint8 *&p, fifo_state_t &s, int off, int size1, addr_t &count1, int inc1)
void | fifo_st_flush_3d_byte (v64uint8 *&p, fifo_state_t &s, int off, int size1, addr_t &count1, int inc1, int size2, addr_t &count2, int inc2)
void | fifo_st_flush_bare (v64uint8 *&p, fifo_state_t &s)
void | fifo_st_flush_bare_1d_byte (v64uint8 *&p, fifo_state_t &s, int off)
void | fifo_st_flush_bare_2d_byte (v64uint8 *&p, fifo_state_t &s, int off, int size1, addr_t &count1, int inc1)
void | fifo_st_flush_bare_3d_byte (v64uint8 *&p, fifo_state_t &s, int off, int size1, addr_t &count1, int inc1, int size2, addr_t &count2, int inc2)
void | fifo_st_flush_conv (v64uint8 *&p, fifo_state_t &s)
void | fifo_st_flush_conv_1d_byte (v64uint8 *&p, fifo_state_t &s, int off)
void | fifo_st_flush_conv_2d_byte (v64uint8 *&p, fifo_state_t &s, int off, int size1, addr_t &count1, int inc1)
void | fifo_st_flush_conv_3d_byte (v64uint8 *&p, fifo_state_t &s, int off, int size1, addr_t &count1, int inc1, int size2, addr_t &count2, int inc2)

## FIFO stores to memory from register v32int16
void | fifo_st_reset (v32int16 *p, v32int16 v, v32int16 *&p_o, sparse_fifo_t &fifo_o, int &pos_o)
void | fifo_st_reset (v32int16 *&p, v32int16 v, fifo_state_t &s)
void | fifo_st_push (v32int16 *&p, v32int16 v, fifo_state_t &s)
void | fifo_st_flush (v32int16 *&p, fifo_state_t &s)
void | fifo_st_flush_1d_byte (v32int16 *&p, fifo_state_t &s, int off)
void | fifo_st_flush_2d_byte (v32int16 *&p, fifo_state_t &s, int off, int size1, addr_t &count1, int inc1)
void | fifo_st_flush_3d_byte (v32int16 *&p, fifo_state_t &s, int off, int size1, addr_t &count1, int inc1, int size2, addr_t &count2, int inc2)
void | fifo_st_flush_bare (v32int16 *&p, fifo_state_t &s)
void | fifo_st_flush_bare_1d_byte (v32int16 *&p, fifo_state_t &s, int off)
void | fifo_st_flush_bare_2d_byte (v32int16 *&p, fifo_state_t &s, int off, int size1, addr_t &count1, int inc1)
void | fifo_st_flush_bare_3d_byte (v32int16 *&p, fifo_state_t &s, int off, int size1, addr_t &count1, int inc1, int size2, addr_t &count2, int inc2)
void | fifo_st_flush_conv (v32int16 *&p, fifo_state_t &s)
void | fifo_st_flush_conv_1d_byte (v32int16 *&p, fifo_state_t &s, int off)
void | fifo_st_flush_conv_2d_byte (v32int16 *&p, fifo_state_t &s, int off, int size1, addr_t &count1, int inc1)
void | fifo_st_flush_conv_3d_byte (v32int16 *&p, fifo_state_t &s, int off, int size1, addr_t &count1, int inc1, int size2, addr_t &count2, int inc2)

## FIFO stores to memory from register v32uint16
void | fifo_st_reset (v32uint16 *p, v32uint16 v, v32uint16 *&p_o, sparse_fifo_t &fifo_o, int &pos_o)
void | fifo_st_reset (v32uint16 *&p, v32uint16 v, fifo_state_t &s)
void | fifo_st_push (v32uint16 *&p, v32uint16 v, fifo_state_t &s)
void | fifo_st_flush (v32uint16 *&p, fifo_state_t &s)
void | fifo_st_flush_1d_byte (v32uint16 *&p, fifo_state_t &s, int off)
void | fifo_st_flush_2d_byte (v32uint16 *&p, fifo_state_t &s, int off, int size1, addr_t &count1, int inc1)
void | fifo_st_flush_3d_byte (v32uint16 *&p, fifo_state_t &s, int off, int size1, addr_t &count1, int inc1, int size2, addr_t &count2, int inc2)
void | fifo_st_flush_bare (v32uint16 *&p, fifo_state_t &s)
void | fifo_st_flush_bare_1d_byte (v32uint16 *&p, fifo_state_t &s, int off)
void | fifo_st_flush_bare_2d_byte (v32uint16 *&p, fifo_state_t &s, int off, int size1, addr_t &count1, int inc1)
void | fifo_st_flush_bare_3d_byte (v32uint16 *&p, fifo_state_t &s, int off, int size1, addr_t &count1, int inc1, int size2, addr_t &count2, int inc2)
void | fifo_st_flush_conv (v32uint16 *&p, fifo_state_t &s)
void | fifo_st_flush_conv_1d_byte (v32uint16 *&p, fifo_state_t &s, int off)
void | fifo_st_flush_conv_2d_byte (v32uint16 *&p, fifo_state_t &s, int off, int size1, addr_t &count1, int inc1)
void | fifo_st_flush_conv_3d_byte (v32uint16 *&p, fifo_state_t &s, int off, int size1, addr_t &count1, int inc1, int size2, addr_t &count2, int inc2)

## FIFO stores to memory from register v16int32
void | fifo_st_reset (v16int32 *p, v16int32 v, v16int32 *&p_o, sparse_fifo_t &fifo_o, int &pos_o)
void | fifo_st_reset (v16int32 *&p, v16int32 v, fifo_state_t &s)
void | fifo_st_push (v16int32 *&p, v16int32 v, fifo_state_t &s)
void | fifo_st_flush (v16int32 *&p, fifo_state_t &s)
void | fifo_st_flush_1d_byte (v16int32 *&p, fifo_state_t &s, int off)
void | fifo_st_flush_2d_byte (v16int32 *&p, fifo_state_t &s, int off, int size1, addr_t &count1, int inc1)
void | fifo_st_flush_3d_byte (v16int32 *&p, fifo_state_t &s, int off, int size1, addr_t &count1, int inc1, int size2, addr_t &count2, int inc2)
void | fifo_st_flush_bare (v16int32 *&p, fifo_state_t &s)
void | fifo_st_flush_bare_1d_byte (v16int32 *&p, fifo_state_t &s, int off)
void | fifo_st_flush_bare_2d_byte (v16int32 *&p, fifo_state_t &s, int off, int size1, addr_t &count1, int inc1)
void | fifo_st_flush_bare_3d_byte (v16int32 *&p, fifo_state_t &s, int off, int size1, addr_t &count1, int inc1, int size2, addr_t &count2, int inc2)
void | fifo_st_flush_conv (v16int32 *&p, fifo_state_t &s)
void | fifo_st_flush_conv_1d_byte (v16int32 *&p, fifo_state_t &s, int off)
void | fifo_st_flush_conv_2d_byte (v16int32 *&p, fifo_state_t &s, int off, int size1, addr_t &count1, int inc1)
void | fifo_st_flush_conv_3d_byte (v16int32 *&p, fifo_state_t &s, int off, int size1, addr_t &count1, int inc1, int size2, addr_t &count2, int inc2)

## FIFO stores to memory from register v16uint32
void | fifo_st_reset (v16uint32 *p, v16uint32 v, v16uint32 *&p_o, sparse_fifo_t &fifo_o, int &pos_o)
void | fifo_st_reset (v16uint32 *&p, v16uint32 v, fifo_state_t &s)
void | fifo_st_push (v16uint32 *&p, v16uint32 v, fifo_state_t &s)
void | fifo_st_flush (v16uint32 *&p, fifo_state_t &s)
void | fifo_st_flush_1d_byte (v16uint32 *&p, fifo_state_t &s, int off)
void | fifo_st_flush_2d_byte (v16uint32 *&p, fifo_state_t &s, int off, int size1, addr_t &count1, int inc1)
void | fifo_st_flush_3d_byte (v16uint32 *&p, fifo_state_t &s, int off, int size1, addr_t &count1, int inc1, int size2, addr_t &count2, int inc2)
void | fifo_st_flush_bare (v16uint32 *&p, fifo_state_t &s)
void | fifo_st_flush_bare_1d_byte (v16uint32 *&p, fifo_state_t &s, int off)
void | fifo_st_flush_bare_2d_byte (v16uint32 *&p, fifo_state_t &s, int off, int size1, addr_t &count1, int inc1)
void | fifo_st_flush_bare_3d_byte (v16uint32 *&p, fifo_state_t &s, int off, int size1, addr_t &count1, int inc1, int size2, addr_t &count2, int inc2)
void | fifo_st_flush_conv (v16uint32 *&p, fifo_state_t &s)
void | fifo_st_flush_conv_1d_byte (v16uint32 *&p, fifo_state_t &s, int off)
void | fifo_st_flush_conv_2d_byte (v16uint32 *&p, fifo_state_t &s, int off, int size1, addr_t &count1, int inc1)
void | fifo_st_flush_conv_3d_byte (v16uint32 *&p, fifo_state_t &s, int off, int size1, addr_t &count1, int inc1, int size2, addr_t &count2, int inc2)

## FIFO stores to memory from register v64bfloat8
void | fifo_st_reset (v64bfloat8 *p, v64bfloat8 v, v64bfloat8 *&p_o, sparse_fifo_t &fifo_o, int &pos_o)
void | fifo_st_reset (v64bfloat8 *&p, v64bfloat8 v, fifo_state_t &s)
void | fifo_st_push (v64bfloat8 *&p, v64bfloat8 v, fifo_state_t &s)
void | fifo_st_flush (v64bfloat8 *&p, fifo_state_t &s)
void | fifo_st_flush_1d_byte (v64bfloat8 *&p, fifo_state_t &s, int off)
void | fifo_st_flush_2d_byte (v64bfloat8 *&p, fifo_state_t &s, int off, int size1, addr_t &count1, int inc1)
void | fifo_st_flush_3d_byte (v64bfloat8 *&p, fifo_state_t &s, int off, int size1, addr_t &count1, int inc1, int size2, addr_t &count2, int inc2)
void | fifo_st_flush_bare (v64bfloat8 *&p, fifo_state_t &s)
void | fifo_st_flush_bare_1d_byte (v64bfloat8 *&p, fifo_state_t &s, int off)
void | fifo_st_flush_bare_2d_byte (v64bfloat8 *&p, fifo_state_t &s, int off, int size1, addr_t &count1, int inc1)
void | fifo_st_flush_bare_3d_byte (v64bfloat8 *&p, fifo_state_t &s, int off, int size1, addr_t &count1, int inc1, int size2, addr_t &count2, int inc2)
void | fifo_st_flush_conv (v64bfloat8 *&p, fifo_state_t &s)
void | fifo_st_flush_conv_1d_byte (v64bfloat8 *&p, fifo_state_t &s, int off)
void | fifo_st_flush_conv_2d_byte (v64bfloat8 *&p, fifo_state_t &s, int off, int size1, addr_t &count1, int inc1)
void | fifo_st_flush_conv_3d_byte (v64bfloat8 *&p, fifo_state_t &s, int off, int size1, addr_t &count1, int inc1, int size2, addr_t &count2, int inc2)

## FIFO stores to memory from register v64float8
void | fifo_st_reset (v64float8 *p, v64float8 v, v64float8 *&p_o, sparse_fifo_t &fifo_o, int &pos_o)
void | fifo_st_reset (v64float8 *&p, v64float8 v, fifo_state_t &s)
void | fifo_st_push (v64float8 *&p, v64float8 v, fifo_state_t &s)
void | fifo_st_flush (v64float8 *&p, fifo_state_t &s)
void | fifo_st_flush_1d_byte (v64float8 *&p, fifo_state_t &s, int off)
void | fifo_st_flush_2d_byte (v64float8 *&p, fifo_state_t &s, int off, int size1, addr_t &count1, int inc1)
void | fifo_st_flush_3d_byte (v64float8 *&p, fifo_state_t &s, int off, int size1, addr_t &count1, int inc1, int size2, addr_t &count2, int inc2)
void | fifo_st_flush_bare (v64float8 *&p, fifo_state_t &s)
void | fifo_st_flush_bare_1d_byte (v64float8 *&p, fifo_state_t &s, int off)
void | fifo_st_flush_bare_2d_byte (v64float8 *&p, fifo_state_t &s, int off, int size1, addr_t &count1, int inc1)
void | fifo_st_flush_bare_3d_byte (v64float8 *&p, fifo_state_t &s, int off, int size1, addr_t &count1, int inc1, int size2, addr_t &count2, int inc2)
void | fifo_st_flush_conv (v64float8 *&p, fifo_state_t &s)
void | fifo_st_flush_conv_1d_byte (v64float8 *&p, fifo_state_t &s, int off)
void | fifo_st_flush_conv_2d_byte (v64float8 *&p, fifo_state_t &s, int off, int size1, addr_t &count1, int inc1)
void | fifo_st_flush_conv_3d_byte (v64float8 *&p, fifo_state_t &s, int off, int size1, addr_t &count1, int inc1, int size2, addr_t &count2, int inc2)

## FIFO stores to memory from register v16cint16
void | fifo_st_reset (v16cint16 *p, v16cint16 v, v16cint16 *&p_o, sparse_fifo_t &fifo_o, int &pos_o)
void | fifo_st_reset (v16cint16 *&p, v16cint16 v, fifo_state_t &s)
void | fifo_st_push (v16cint16 *&p, v16cint16 v, fifo_state_t &s)
void | fifo_st_flush (v16cint16 *&p, fifo_state_t &s)
void | fifo_st_flush_1d_byte (v16cint16 *&p, fifo_state_t &s, int off)
void | fifo_st_flush_2d_byte (v16cint16 *&p, fifo_state_t &s, int off, int size1, addr_t &count1, int inc1)
void | fifo_st_flush_3d_byte (v16cint16 *&p, fifo_state_t &s, int off, int size1, addr_t &count1, int inc1, int size2, addr_t &count2, int inc2)
void | fifo_st_flush_bare (v16cint16 *&p, fifo_state_t &s)
void | fifo_st_flush_bare_1d_byte (v16cint16 *&p, fifo_state_t &s, int off)
void | fifo_st_flush_bare_2d_byte (v16cint16 *&p, fifo_state_t &s, int off, int size1, addr_t &count1, int inc1)
void | fifo_st_flush_bare_3d_byte (v16cint16 *&p, fifo_state_t &s, int off, int size1, addr_t &count1, int inc1, int size2, addr_t &count2, int inc2)
void | fifo_st_flush_conv (v16cint16 *&p, fifo_state_t &s)
void | fifo_st_flush_conv_1d_byte (v16cint16 *&p, fifo_state_t &s, int off)
void | fifo_st_flush_conv_2d_byte (v16cint16 *&p, fifo_state_t &s, int off, int size1, addr_t &count1, int inc1)
void | fifo_st_flush_conv_3d_byte (v16cint16 *&p, fifo_state_t &s, int off, int size1, addr_t &count1, int inc1, int size2, addr_t &count2, int inc2)

## FIFO stores to memory from register v8cint32
void | fifo_st_reset (v8cint32 *p, v8cint32 v, v8cint32 *&p_o, sparse_fifo_t &fifo_o, int &pos_o)
void | fifo_st_reset (v8cint32 *&p, v8cint32 v, fifo_state_t &s)
void | fifo_st_push (v8cint32 *&p, v8cint32 v, fifo_state_t &s)
void | fifo_st_flush (v8cint32 *&p, fifo_state_t &s)
void | fifo_st_flush_1d_byte (v8cint32 *&p, fifo_state_t &s, int off)
void | fifo_st_flush_2d_byte (v8cint32 *&p, fifo_state_t &s, int off, int size1, addr_t &count1, int inc1)
void | fifo_st_flush_3d_byte (v8cint32 *&p, fifo_state_t &s, int off, int size1, addr_t &count1, int inc1, int size2, addr_t &count2, int inc2)
void | fifo_st_flush_bare (v8cint32 *&p, fifo_state_t &s)
void | fifo_st_flush_bare_1d_byte (v8cint32 *&p, fifo_state_t &s, int off)
void | fifo_st_flush_bare_2d_byte (v8cint32 *&p, fifo_state_t &s, int off, int size1, addr_t &count1, int inc1)
void | fifo_st_flush_bare_3d_byte (v8cint32 *&p, fifo_state_t &s, int off, int size1, addr_t &count1, int inc1, int size2, addr_t &count2, int inc2)
void | fifo_st_flush_conv (v8cint32 *&p, fifo_state_t &s)
void | fifo_st_flush_conv_1d_byte (v8cint32 *&p, fifo_state_t &s, int off)
void | fifo_st_flush_conv_2d_byte (v8cint32 *&p, fifo_state_t &s, int off, int size1, addr_t &count1, int inc1)
void | fifo_st_flush_conv_3d_byte (v8cint32 *&p, fifo_state_t &s, int off, int size1, addr_t &count1, int inc1, int size2, addr_t &count2, int inc2)

## FIFO stores to memory from register v8cfloat
void | fifo_st_reset (v8cfloat *p, v8cfloat v, v8cfloat *&p_o, sparse_fifo_t &fifo_o, int &pos_o)
void | fifo_st_reset (v8cfloat *&p, v8cfloat v, fifo_state_t &s)
void | fifo_st_push (v8cfloat *&p, v8cfloat v, fifo_state_t &s)
void | fifo_st_flush (v8cfloat *&p, fifo_state_t &s)
void | fifo_st_flush_1d_byte (v8cfloat *&p, fifo_state_t &s, int off)
void | fifo_st_flush_2d_byte (v8cfloat *&p, fifo_state_t &s, int off, int size1, addr_t &count1, int inc1)
void | fifo_st_flush_3d_byte (v8cfloat *&p, fifo_state_t &s, int off, int size1, addr_t &count1, int inc1, int size2, addr_t &count2, int inc2)
void | fifo_st_flush_bare (v8cfloat *&p, fifo_state_t &s)
void | fifo_st_flush_bare_1d_byte (v8cfloat *&p, fifo_state_t &s, int off)
void | fifo_st_flush_bare_2d_byte (v8cfloat *&p, fifo_state_t &s, int off, int size1, addr_t &count1, int inc1)
void | fifo_st_flush_bare_3d_byte (v8cfloat *&p, fifo_state_t &s, int off, int size1, addr_t &count1, int inc1, int size2, addr_t &count2, int inc2)
void | fifo_st_flush_conv (v8cfloat *&p, fifo_state_t &s)
void | fifo_st_flush_conv_1d_byte (v8cfloat *&p, fifo_state_t &s, int off)
void | fifo_st_flush_conv_2d_byte (v8cfloat *&p, fifo_state_t &s, int off, int size1, addr_t &count1, int inc1)
void | fifo_st_flush_conv_3d_byte (v8cfloat *&p, fifo_state_t &s, int off, int size1, addr_t &count1, int inc1, int size2, addr_t &count2, int inc2)

## FIFO stores to memory from register v16cbfloat16
void | fifo_st_reset (v16cbfloat16 *p, v16cbfloat16 v, v16cbfloat16 *&p_o, sparse_fifo_t &fifo_o, int &pos_o)
void | fifo_st_reset (v16cbfloat16 *&p, v16cbfloat16 v, fifo_state_t &s)
void | fifo_st_push (v16cbfloat16 *&p, v16cbfloat16 v, fifo_state_t &s)
void | fifo_st_flush (v16cbfloat16 *&p, fifo_state_t &s)
void | fifo_st_flush_1d_byte (v16cbfloat16 *&p, fifo_state_t &s, int off)
void | fifo_st_flush_2d_byte (v16cbfloat16 *&p, fifo_state_t &s, int off, int size1, addr_t &count1, int inc1)
void | fifo_st_flush_3d_byte (v16cbfloat16 *&p, fifo_state_t &s, int off, int size1, addr_t &count1, int inc1, int size2, addr_t &count2, int inc2)
void | fifo_st_flush_bare (v16cbfloat16 *&p, fifo_state_t &s)
void | fifo_st_flush_bare_1d_byte (v16cbfloat16 *&p, fifo_state_t &s, int off)
void | fifo_st_flush_bare_2d_byte (v16cbfloat16 *&p, fifo_state_t &s, int off, int size1, addr_t &count1, int inc1)
void | fifo_st_flush_bare_3d_byte (v16cbfloat16 *&p, fifo_state_t &s, int off, int size1, addr_t &count1, int inc1, int size2, addr_t &count2, int inc2)
void | fifo_st_flush_conv (v16cbfloat16 *&p, fifo_state_t &s)
void | fifo_st_flush_conv_1d_byte (v16cbfloat16 *&p, fifo_state_t &s, int off)
void | fifo_st_flush_conv_2d_byte (v16cbfloat16 *&p, fifo_state_t &s, int off, int size1, addr_t &count1, int inc1)
void | fifo_st_flush_conv_3d_byte (v16cbfloat16 *&p, fifo_state_t &s, int off, int size1, addr_t &count1, int inc1, int size2, addr_t &count2, int inc2)

## FIFO stores to memory from register v32float16
void | fifo_st_reset (v32float16 *p, v32float16 v, v32float16 *&p_o, sparse_fifo_t &fifo_o, int &pos_o)
void | fifo_st_reset (v32float16 *&p, v32float16 v, fifo_state_t &s)
void | fifo_st_push (v32float16 *&p, v32float16 v, fifo_state_t &s)
void | fifo_st_flush (v32float16 *&p, fifo_state_t &s)
void | fifo_st_flush_1d_byte (v32float16 *&p, fifo_state_t &s, int off)
void | fifo_st_flush_2d_byte (v32float16 *&p, fifo_state_t &s, int off, int size1, addr_t &count1, int inc1)
void | fifo_st_flush_3d_byte (v32float16 *&p, fifo_state_t &s, int off, int size1, addr_t &count1, int inc1, int size2, addr_t &count2, int inc2)
void | fifo_st_flush_bare (v32float16 *&p, fifo_state_t &s)
void | fifo_st_flush_bare_1d_byte (v32float16 *&p, fifo_state_t &s, int off)
void | fifo_st_flush_bare_2d_byte (v32float16 *&p, fifo_state_t &s, int off, int size1, addr_t &count1, int inc1)
void | fifo_st_flush_bare_3d_byte (v32float16 *&p, fifo_state_t &s, int off, int size1, addr_t &count1, int inc1, int size2, addr_t &count2, int inc2)
void | fifo_st_flush_conv (v32float16 *&p, fifo_state_t &s)
void | fifo_st_flush_conv_1d_byte (v32float16 *&p, fifo_state_t &s, int off)
void | fifo_st_flush_conv_2d_byte (v32float16 *&p, fifo_state_t &s, int off, int size1, addr_t &count1, int inc1)
void | fifo_st_flush_conv_3d_byte (v32float16 *&p, fifo_state_t &s, int off, int size1, addr_t &count1, int inc1, int size2, addr_t &count2, int inc2)

## FIFO stores to memory from register v32bfloat16
void | fifo_st_reset (v32bfloat16 *p, v32bfloat16 v, v32bfloat16 *&p_o, sparse_fifo_t &fifo_o, int &pos_o)
void | fifo_st_reset (v32bfloat16 *&p, v32bfloat16 v, fifo_state_t &s)
void | fifo_st_push (v32bfloat16 *&p, v32bfloat16 v, fifo_state_t &s)
void | fifo_st_flush (v32bfloat16 *&p, fifo_state_t &s)
void | fifo_st_flush_1d_byte (v32bfloat16 *&p, fifo_state_t &s, int off)
void | fifo_st_flush_2d_byte (v32bfloat16 *&p, fifo_state_t &s, int off, int size1, addr_t &count1, int inc1)
void | fifo_st_flush_3d_byte (v32bfloat16 *&p, fifo_state_t &s, int off, int size1, addr_t &count1, int inc1, int size2, addr_t &count2, int inc2)
void | fifo_st_flush_bare (v32bfloat16 *&p, fifo_state_t &s)
void | fifo_st_flush_bare_1d_byte (v32bfloat16 *&p, fifo_state_t &s, int off)
void | fifo_st_flush_bare_2d_byte (v32bfloat16 *&p, fifo_state_t &s, int off, int size1, addr_t &count1, int inc1)
void | fifo_st_flush_bare_3d_byte (v32bfloat16 *&p, fifo_state_t &s, int off, int size1, addr_t &count1, int inc1, int size2, addr_t &count2, int inc2)
void | fifo_st_flush_conv (v32bfloat16 *&p, fifo_state_t &s)
void | fifo_st_flush_conv_1d_byte (v32bfloat16 *&p, fifo_state_t &s, int off)
void | fifo_st_flush_conv_2d_byte (v32bfloat16 *&p, fifo_state_t &s, int off, int size1, addr_t &count1, int inc1)
void | fifo_st_flush_conv_3d_byte (v32bfloat16 *&p, fifo_state_t &s, int off, int size1, addr_t &count1, int inc1, int size2, addr_t &count2, int inc2)

## FIFO stores to memory from register v16float
void | fifo_st_reset (v16float *p, v16float v, v16float *&p_o, sparse_fifo_t &fifo_o, int &pos_o)
void | fifo_st_reset (v16float *&p, v16float v, fifo_state_t &s)
void | fifo_st_push (v16float *&p, v16float v, fifo_state_t &s)
void | fifo_st_flush (v16float *&p, fifo_state_t &s)
void | fifo_st_flush_1d_byte (v16float *&p, fifo_state_t &s, int off)
void | fifo_st_flush_2d_byte (v16float *&p, fifo_state_t &s, int off, int size1, addr_t &count1, int inc1)
void | fifo_st_flush_3d_byte (v16float *&p, fifo_state_t &s, int off, int size1, addr_t &count1, int inc1, int size2, addr_t &count2, int inc2)
void | fifo_st_flush_bare (v16float *&p, fifo_state_t &s)
void | fifo_st_flush_bare_1d_byte (v16float *&p, fifo_state_t &s, int off)
void | fifo_st_flush_bare_2d_byte (v16float *&p, fifo_state_t &s, int off, int size1, addr_t &count1, int inc1)
void | fifo_st_flush_bare_3d_byte (v16float *&p, fifo_state_t &s, int off, int size1, addr_t &count1, int inc1, int size2, addr_t &count2, int inc2)
void | fifo_st_flush_conv (v16float *&p, fifo_state_t &s)
void | fifo_st_flush_conv_1d_byte (v16float *&p, fifo_state_t &s, int off)
void | fifo_st_flush_conv_2d_byte (v16float *&p, fifo_state_t &s, int off, int size1, addr_t &count1, int inc1)
void | fifo_st_flush_conv_3d_byte (v16float *&p, fifo_state_t &s, int off, int size1, addr_t &count1, int inc1, int size2, addr_t &count2, int inc2)

## FIFO stores to memory from register v64mx9
void | fifo_st_reset (v64mx9_unaligned *p, v64mx9 v, v64mx9_unaligned *&p_o, sparse_fifo_t &fifo_o, int &pos_o)
void | fifo_st_reset (v64mx9_unaligned *&p, v64mx9 v, fifo_state_t &s)
void | fifo_st_push (v64mx9_unaligned *&p, v64mx9 v, fifo_state_t &s)
void | fifo_st_flush (v64mx9_unaligned *&p, fifo_state_t &s)
void | fifo_st_flush_1d_byte (v64mx9_unaligned *&p, fifo_state_t &s, int off)
void | fifo_st_flush_2d_byte (v64mx9_unaligned *&p, fifo_state_t &s, int off, int size1, addr_t &count1, int inc1)
void | fifo_st_flush_3d_byte (v64mx9_unaligned *&p, fifo_state_t &s, int off, int size1, addr_t &count1, int inc1, int size2, addr_t &count2, int inc2)
void | fifo_st_flush_bare (v64mx9_unaligned *&p, fifo_state_t &s)
void | fifo_st_flush_bare_1d_byte (v64mx9_unaligned *&p, fifo_state_t &s, int off)
void | fifo_st_flush_bare_2d_byte (v64mx9_unaligned *&p, fifo_state_t &s, int off, int size1, addr_t &count1, int inc1)
void | fifo_st_flush_bare_3d_byte (v64mx9_unaligned *&p, fifo_state_t &s, int off, int size1, addr_t &count1, int inc1, int size2, addr_t &count2, int inc2)
void | fifo_st_flush_conv (v64mx9_unaligned *&p, fifo_state_t &s)
void | fifo_st_flush_conv_1d_byte (v64mx9_unaligned *&p, fifo_state_t &s, int off)
void | fifo_st_flush_conv_2d_byte (v64mx9_unaligned *&p, fifo_state_t &s, int off, int size1, addr_t &count1, int inc1)
void | fifo_st_flush_conv_3d_byte (v64mx9_unaligned *&p, fifo_state_t &s, int off, int size1, addr_t &count1, int inc1, int size2, addr_t &count2, int inc2)

## FIFO stores to memory from register v128mx6
void | fifo_st_reset (v128mx6_unaligned *p, v128mx6 v, v128mx6_unaligned *&p_o, sparse_fifo_t &fifo_o, int &pos_o)
void | fifo_st_reset (v128mx6_unaligned *&p, v128mx6 v, fifo_state_t &s)
void | fifo_st_push (v128mx6_unaligned *&p, v128mx6 v, fifo_state_t &s)
void | fifo_st_flush (v128mx6_unaligned *&p, fifo_state_t &s)
void | fifo_st_flush_1d_byte (v128mx6_unaligned *&p, fifo_state_t &s, int off)
void | fifo_st_flush_2d_byte (v128mx6_unaligned *&p, fifo_state_t &s, int off, int size1, addr_t &count1, int inc1)
void | fifo_st_flush_3d_byte (v128mx6_unaligned *&p, fifo_state_t &s, int off, int size1, addr_t &count1, int inc1, int size2, addr_t &count2, int inc2)
void | fifo_st_flush_bare (v128mx6_unaligned *&p, fifo_state_t &s)
void | fifo_st_flush_bare_1d_byte (v128mx6_unaligned *&p, fifo_state_t &s, int off)
void | fifo_st_flush_bare_2d_byte (v128mx6_unaligned *&p, fifo_state_t &s, int off, int size1, addr_t &count1, int inc1)
void | fifo_st_flush_bare_3d_byte (v128mx6_unaligned *&p, fifo_state_t &s, int off, int size1, addr_t &count1, int inc1, int size2, addr_t &count2, int inc2)
void | fifo_st_flush_conv (v128mx6_unaligned *&p, fifo_state_t &s)
void | fifo_st_flush_conv_1d_byte (v128mx6_unaligned *&p, fifo_state_t &s, int off)
void | fifo_st_flush_conv_2d_byte (v128mx6_unaligned *&p, fifo_state_t &s, int off, int size1, addr_t &count1, int inc1)
void | fifo_st_flush_conv_3d_byte (v128mx6_unaligned *&p, fifo_state_t &s, int off, int size1, addr_t &count1, int inc1, int size2, addr_t &count2, int inc2)

## FIFO stores to memory from register v64mx6
void | fifo_st_reset (v64mx6_unaligned *p, v64mx6 v, v64mx6_unaligned *&p_o, sparse_fifo_t &fifo_o, int &pos_o)
void | fifo_st_reset (v64mx6_unaligned *&p, v64mx6 v, fifo_state_t &s)
void | fifo_st_push (v64mx6_unaligned *&p, v64mx6 v, fifo_state_t &s)
void | fifo_st_flush (v64mx6_unaligned *&p, fifo_state_t &s)
void | fifo_st_flush_1d_byte (v64mx6_unaligned *&p, fifo_state_t &s, int off)
void | fifo_st_flush_2d_byte (v64mx6_unaligned *&p, fifo_state_t &s, int off, int size1, addr_t &count1, int inc1)
void | fifo_st_flush_3d_byte (v64mx6_unaligned *&p, fifo_state_t &s, int off, int size1, addr_t &count1, int inc1, int size2, addr_t &count2, int inc2)
void | fifo_st_flush_bare (v64mx6_unaligned *&p, fifo_state_t &s)
void | fifo_st_flush_bare_1d_byte (v64mx6_unaligned *&p, fifo_state_t &s, int off)
void | fifo_st_flush_bare_2d_byte (v64mx6_unaligned *&p, fifo_state_t &s, int off, int size1, addr_t &count1, int inc1)
void | fifo_st_flush_bare_3d_byte (v64mx6_unaligned *&p, fifo_state_t &s, int off, int size1, addr_t &count1, int inc1, int size2, addr_t &count2, int inc2)
void | fifo_st_flush_conv (v64mx6_unaligned *&p, fifo_state_t &s)
void | fifo_st_flush_conv_1d_byte (v64mx6_unaligned *&p, fifo_state_t &s, int off)
void | fifo_st_flush_conv_2d_byte (v64mx6_unaligned *&p, fifo_state_t &s, int off, int size1, addr_t &count1, int inc1)
void | fifo_st_flush_conv_3d_byte (v64mx6_unaligned *&p, fifo_state_t &s, int off, int size1, addr_t &count1, int inc1, int size2, addr_t &count2, int inc2)

## FIFO stores to memory from register v128mx4
void | fifo_st_reset (v128mx4_unaligned *p, v128mx4 v, v128mx4_unaligned *&p_o, sparse_fifo_t &fifo_o, int &pos_o)
void | fifo_st_reset (v128mx4_unaligned *&p, v128mx4 v, fifo_state_t &s)
void | fifo_st_push (v128mx4_unaligned *&p, v128mx4 v, fifo_state_t &s)
void | fifo_st_flush (v128mx4_unaligned *&p, fifo_state_t &s)
void | fifo_st_flush_1d_byte (v128mx4_unaligned *&p, fifo_state_t &s, int off)
void | fifo_st_flush_2d_byte (v128mx4_unaligned *&p, fifo_state_t &s, int off, int size1, addr_t &count1, int inc1)
void | fifo_st_flush_3d_byte (v128mx4_unaligned *&p, fifo_state_t &s, int off, int size1, addr_t &count1, int inc1, int size2, addr_t &count2, int inc2)
void | fifo_st_flush_bare (v128mx4_unaligned *&p, fifo_state_t &s)
void | fifo_st_flush_bare_1d_byte (v128mx4_unaligned *&p, fifo_state_t &s, int off)
void | fifo_st_flush_bare_2d_byte (v128mx4_unaligned *&p, fifo_state_t &s, int off, int size1, addr_t &count1, int inc1)
void | fifo_st_flush_bare_3d_byte (v128mx4_unaligned *&p, fifo_state_t &s, int off, int size1, addr_t &count1, int inc1, int size2, addr_t &count2, int inc2)
void | fifo_st_flush_conv (v128mx4_unaligned *&p, fifo_state_t &s)
void | fifo_st_flush_conv_1d_byte (v128mx4_unaligned *&p, fifo_state_t &s, int off)
void | fifo_st_flush_conv_2d_byte (v128mx4_unaligned *&p, fifo_state_t &s, int off, int size1, addr_t &count1, int inc1)
void | fifo_st_flush_conv_3d_byte (v128mx4_unaligned *&p, fifo_state_t &s, int off, int size1, addr_t &count1, int inc1, int size2, addr_t &count2, int inc2)

## FIFO stores to memory from register v64mx4
void | fifo_st_reset (v64mx4_unaligned *p, v64mx4 v, v64mx4_unaligned *&p_o, sparse_fifo_t &fifo_o, int &pos_o)
void | fifo_st_reset (v64mx4_unaligned *&p, v64mx4 v, fifo_state_t &s)
void | fifo_st_push (v64mx4_unaligned *&p, v64mx4 v, fifo_state_t &s)
void | fifo_st_flush (v64mx4_unaligned *&p, fifo_state_t &s)
void | fifo_st_flush_1d_byte (v64mx4_unaligned *&p, fifo_state_t &s, int off)
void | fifo_st_flush_2d_byte (v64mx4_unaligned *&p, fifo_state_t &s, int off, int size1, addr_t &count1, int inc1)
void | fifo_st_flush_3d_byte (v64mx4_unaligned *&p, fifo_state_t &s, int off, int size1, addr_t &count1, int inc1, int size2, addr_t &count2, int inc2)
void | fifo_st_flush_bare (v64mx4_unaligned *&p, fifo_state_t &s)
void | fifo_st_flush_bare_1d_byte (v64mx4_unaligned *&p, fifo_state_t &s, int off)
void | fifo_st_flush_bare_2d_byte (v64mx4_unaligned *&p, fifo_state_t &s, int off, int size1, addr_t &count1, int inc1)
void | fifo_st_flush_bare_3d_byte (v64mx4_unaligned *&p, fifo_state_t &s, int off, int size1, addr_t &count1, int inc1, int size2, addr_t &count2, int inc2)
void | fifo_st_flush_conv (v64mx4_unaligned *&p, fifo_state_t &s)
void | fifo_st_flush_conv_1d_byte (v64mx4_unaligned *&p, fifo_state_t &s, int off)
void | fifo_st_flush_conv_2d_byte (v64mx4_unaligned *&p, fifo_state_t &s, int off, int size1, addr_t &count1, int inc1)
void | fifo_st_flush_conv_3d_byte (v64mx4_unaligned *&p, fifo_state_t &s, int off, int size1, addr_t &count1, int inc1, int size2, addr_t &count2, int inc2)

## Detailed Description

## Function Documentation

## ◆ fifo_ld_fill() [1/42]

void fifo_ld_fill | ( | v128bfloat16_sparse_unaligned *& | p,
|  | fifo_state_t & | fifo )

## ◆ fifo_ld_fill() [2/42]

void fifo_ld_fill | ( | v128bfloat8_sparse_unaligned *& | p,
|  | fifo_state_t & | s )

## ◆ fifo_ld_fill() [3/42]

void fifo_ld_fill | ( | v128float16_sparse_unaligned *& | p,
|  | fifo_state_t & | fifo )

## ◆ fifo_ld_fill() [4/42]

void fifo_ld_fill | ( | v128float8_sparse_unaligned *& | p,
|  | fifo_state_t & | s )

## ◆ fifo_ld_fill() [5/42]

void fifo_ld_fill | ( | v128int16_sparse_unaligned *& | p,
|  | fifo_state_t & | fifo )

## ◆ fifo_ld_fill() [6/42]

void fifo_ld_fill | ( | v128int4 *& | p,
|  | fifo_state_t & | s )

## ◆ fifo_ld_fill() [7/42]

void fifo_ld_fill | ( | v128int8_sparse_unaligned *& | p,
|  | fifo_state_t & | s )

## ◆ fifo_ld_fill() [8/42]

void fifo_ld_fill | ( | v128mx4_unaligned *& | p,
|  | fifo_state_t & | s )

## ◆ fifo_ld_fill() [9/42]

void fifo_ld_fill | ( | v128mx6_unaligned *& | p,
|  | fifo_state_t & | s )

## ◆ fifo_ld_fill() [10/42]

void fifo_ld_fill | ( | v128uint16_sparse_unaligned *& | p,
|  | fifo_state_t & | fifo )

## ◆ fifo_ld_fill() [11/42]

void fifo_ld_fill | ( | v128uint4 *& | p,
|  | fifo_state_t & | s )

## ◆ fifo_ld_fill() [12/42]

void fifo_ld_fill | ( | v128uint8_sparse_unaligned *& | p,
|  | fifo_state_t & | s )

## ◆ fifo_ld_fill() [13/42]

void fifo_ld_fill | ( | v16cbfloat16 *& | p,
|  | fifo_state_t & | s )

## ◆ fifo_ld_fill() [14/42]

void fifo_ld_fill | ( | v16cint16 *& | p,
|  | fifo_state_t & | s )

## ◆ fifo_ld_fill() [15/42]

void fifo_ld_fill | ( | v16float *& | p,
|  | fifo_state_t & | s )

## ◆ fifo_ld_fill() [16/42]

void fifo_ld_fill | ( | v16int32 *& | p,
|  | fifo_state_t & | s )

## ◆ fifo_ld_fill() [17/42]

void fifo_ld_fill | ( | v16uint32 *& | p,
|  | fifo_state_t & | s )

## ◆ fifo_ld_fill() [18/42]

void fifo_ld_fill | ( | v256bfloat8_sparse_unaligned *& | p,
|  | fifo_state_t & | fifo )

## ◆ fifo_ld_fill() [19/42]

void fifo_ld_fill | ( | v256float8_sparse_unaligned *& | p,
|  | fifo_state_t & | fifo )

## ◆ fifo_ld_fill() [20/42]

void fifo_ld_fill | ( | v256int4_sparse_unaligned *& | p,
|  | fifo_state_t & | s )

## ◆ fifo_ld_fill() [21/42]

void fifo_ld_fill | ( | v256int8_sparse_unaligned *& | p,
|  | fifo_state_t & | fifo )

## ◆ fifo_ld_fill() [22/42]

void fifo_ld_fill | ( | v256mx4_unaligned *& | p,
|  | fifo_state_t & | fifo )

## ◆ fifo_ld_fill() [23/42]

void fifo_ld_fill | ( | v256mx6_unaligned *& | p,
|  | fifo_state_t & | fifo )

## ◆ fifo_ld_fill() [24/42]

void fifo_ld_fill | ( | v256uint4_sparse_unaligned *& | p,
|  | fifo_state_t & | s )

## ◆ fifo_ld_fill() [25/42]

void fifo_ld_fill | ( | v256uint8_sparse_unaligned *& | p,
|  | fifo_state_t & | fifo )

## ◆ fifo_ld_fill() [26/42]

void fifo_ld_fill | ( | v32bfloat16 *& | p,
|  | fifo_state_t & | s )

## ◆ fifo_ld_fill() [27/42]

void fifo_ld_fill | ( | v32float16 *& | p,
|  | fifo_state_t & | s )

## ◆ fifo_ld_fill() [28/42]

void fifo_ld_fill | ( | v32int16 *& | p,
|  | fifo_state_t & | s )

## ◆ fifo_ld_fill() [29/42]

void fifo_ld_fill | ( | v32uint16 *& | p,
|  | fifo_state_t & | s )

## ◆ fifo_ld_fill() [30/42]

void fifo_ld_fill | ( | v512int4_sparse_unaligned *& | p,
|  | fifo_state_t & | fifo )

## ◆ fifo_ld_fill() [31/42]

void fifo_ld_fill | ( | v512uint4_sparse_unaligned *& | p,
|  | fifo_state_t & | fifo )

## ◆ fifo_ld_fill() [32/42]

void fifo_ld_fill | ( | v64bfloat16_sparse_unaligned *& | p,
|  | fifo_state_t & | s )

## ◆ fifo_ld_fill() [33/42]

void fifo_ld_fill | ( | v64bfloat8 *& | p,
|  | fifo_state_t & | s )

## ◆ fifo_ld_fill() [34/42]

void fifo_ld_fill | ( | v64float16_sparse_unaligned *& | p,
|  | fifo_state_t & | s )

## ◆ fifo_ld_fill() [35/42]

void fifo_ld_fill | ( | v64float8 *& | p,
|  | fifo_state_t & | s )

## ◆ fifo_ld_fill() [36/42]

void fifo_ld_fill | ( | v64int16_sparse_unaligned *& | p,
|  | fifo_state_t & | s )

## ◆ fifo_ld_fill() [37/42]

void fifo_ld_fill | ( | v64int8 *& | p,
|  | fifo_state_t & | s )

## ◆ fifo_ld_fill() [38/42]

void fifo_ld_fill | ( | v64mx9_unaligned *& | p,
|  | fifo_state_t & | s )

## ◆ fifo_ld_fill() [39/42]

void fifo_ld_fill | ( | v64uint16_sparse_unaligned *& | p,
|  | fifo_state_t & | s )

## ◆ fifo_ld_fill() [40/42]

void fifo_ld_fill | ( | v64uint8 *& | p,
|  | fifo_state_t & | s )

## ◆ fifo_ld_fill() [41/42]

void fifo_ld_fill | ( | v8cfloat *& | p,
|  | fifo_state_t & | s )

## ◆ fifo_ld_fill() [42/42]

void fifo_ld_fill | ( | v8cint32 *& | p,
|  | fifo_state_t & | s )

## ◆ fifo_ld_fillx() [1/6]

void fifo_ld_fillx | ( | v128mx4_unaligned *& | p,
|  | fifo_state_t & | s )

## ◆ fifo_ld_fillx() [2/6]

void fifo_ld_fillx | ( | v128mx4_unaligned *& | p,
|  | fifo_state_t & | s,
|  | int | step,
|  | int | mask )

## ◆ fifo_ld_fillx() [3/6]

void fifo_ld_fillx | ( | v128mx6_unaligned *& | p,
|  | fifo_state_t & | s )

## ◆ fifo_ld_fillx() [4/6]

void fifo_ld_fillx | ( | v128mx6_unaligned *& | p,
|  | fifo_state_t & | s,
|  | int | step,
|  | int | mask )

## ◆ fifo_ld_fillx() [5/6]

void fifo_ld_fillx | ( | v64mx9_unaligned *& | p,
|  | fifo_state_t & | s )

## ◆ fifo_ld_fillx() [6/6]

void fifo_ld_fillx | ( | v64mx9_unaligned *& | p,
|  | fifo_state_t & | s,
|  | int | step,
|  | int | mask )

## ◆ fifo_ld_pop() [1/42]

v128bfloat16_sparse fifo_ld_pop | ( | v128bfloat16_sparse_unaligned *& | p,
|  | fifo_state_t & | fifo )

## ◆ fifo_ld_pop() [2/42]

v128bfloat8_sparse fifo_ld_pop | ( | v128bfloat8_sparse_unaligned *& | p,
|  | fifo_state_t & | s )

## ◆ fifo_ld_pop() [3/42]

v128float16_sparse fifo_ld_pop | ( | v128float16_sparse_unaligned *& | p,
|  | fifo_state_t & | fifo )

## ◆ fifo_ld_pop() [4/42]

v128float8_sparse fifo_ld_pop | ( | v128float8_sparse_unaligned *& | p,
|  | fifo_state_t & | s )

## ◆ fifo_ld_pop() [5/42]

v128int16_sparse fifo_ld_pop | ( | v128int16_sparse_unaligned *& | p,
|  | fifo_state_t & | fifo )

## ◆ fifo_ld_pop() [6/42]

v128int4 fifo_ld_pop | ( | v128int4 *& | p,
|  | fifo_state_t & | s )

## ◆ fifo_ld_pop() [7/42]

v128int8_sparse fifo_ld_pop | ( | v128int8_sparse_unaligned *& | p,
|  | fifo_state_t & | s )

## ◆ fifo_ld_pop() [8/42]

v128mx4 fifo_ld_pop | ( | v128mx4_unaligned *& | p,
|  | fifo_state_t & | s )

## ◆ fifo_ld_pop() [9/42]

v128mx6 fifo_ld_pop | ( | v128mx6_unaligned *& | p,
|  | fifo_state_t & | s )

## ◆ fifo_ld_pop() [10/42]

v128uint16_sparse fifo_ld_pop | ( | v128uint16_sparse_unaligned *& | p,
|  | fifo_state_t & | fifo )

## ◆ fifo_ld_pop() [11/42]

v128uint4 fifo_ld_pop | ( | v128uint4 *& | p,
|  | fifo_state_t & | s )

## ◆ fifo_ld_pop() [12/42]

v128uint8_sparse fifo_ld_pop | ( | v128uint8_sparse_unaligned *& | p,
|  | fifo_state_t & | s )

## ◆ fifo_ld_pop() [13/42]

v16cbfloat16 fifo_ld_pop | ( | v16cbfloat16 *& | p,
|  | fifo_state_t & | s )

## ◆ fifo_ld_pop() [14/42]

v16cint16 fifo_ld_pop | ( | v16cint16 *& | p,
|  | fifo_state_t & | s )

## ◆ fifo_ld_pop() [15/42]

v16float fifo_ld_pop | ( | v16float *& | p,
|  | fifo_state_t & | s )

## ◆ fifo_ld_pop() [16/42]

v16int32 fifo_ld_pop | ( | v16int32 *& | p,
|  | fifo_state_t & | s )

## ◆ fifo_ld_pop() [17/42]

v16uint32 fifo_ld_pop | ( | v16uint32 *& | p,
|  | fifo_state_t & | s )

## ◆ fifo_ld_pop() [18/42]

v256bfloat8_sparse fifo_ld_pop | ( | v256bfloat8_sparse_unaligned *& | p,
|  | fifo_state_t & | fifo )

## ◆ fifo_ld_pop() [19/42]

v256float8_sparse fifo_ld_pop | ( | v256float8_sparse_unaligned *& | p,
|  | fifo_state_t & | fifo )

## ◆ fifo_ld_pop() [20/42]

v256int4_sparse fifo_ld_pop | ( | v256int4_sparse_unaligned *& | p,
|  | fifo_state_t & | s )

## ◆ fifo_ld_pop() [21/42]

v256int8_sparse fifo_ld_pop | ( | v256int8_sparse_unaligned *& | p,
|  | fifo_state_t & | fifo )

## ◆ fifo_ld_pop() [22/42]

v256mx4 fifo_ld_pop | ( | v256mx4_unaligned *& | p,
|  | fifo_state_t & | fifo )

## ◆ fifo_ld_pop() [23/42]

v256mx6 fifo_ld_pop | ( | v256mx6_unaligned *& | p,
|  | fifo_state_t & | fifo )

## ◆ fifo_ld_pop() [24/42]

v256uint4_sparse fifo_ld_pop | ( | v256uint4_sparse_unaligned *& | p,
|  | fifo_state_t & | s )

## ◆ fifo_ld_pop() [25/42]

v256uint8_sparse fifo_ld_pop | ( | v256uint8_sparse_unaligned *& | p,
|  | fifo_state_t & | fifo )

## ◆ fifo_ld_pop() [26/42]

v32bfloat16 fifo_ld_pop | ( | v32bfloat16 *& | p,
|  | fifo_state_t & | s )

## ◆ fifo_ld_pop() [27/42]

v32float16 fifo_ld_pop | ( | v32float16 *& | p,
|  | fifo_state_t & | s )

## ◆ fifo_ld_pop() [28/42]

v32int16 fifo_ld_pop | ( | v32int16 *& | p,
|  | fifo_state_t & | s )

## ◆ fifo_ld_pop() [29/42]

v32uint16 fifo_ld_pop | ( | v32uint16 *& | p,
|  | fifo_state_t & | s )

## ◆ fifo_ld_pop() [30/42]

v512int4_sparse fifo_ld_pop | ( | v512int4_sparse_unaligned *& | p,
|  | fifo_state_t & | fifo )

## ◆ fifo_ld_pop() [31/42]

v512uint4_sparse fifo_ld_pop | ( | v512uint4_sparse_unaligned *& | p,
|  | fifo_state_t & | fifo )

## ◆ fifo_ld_pop() [32/42]

v64bfloat16_sparse fifo_ld_pop | ( | v64bfloat16_sparse_unaligned *& | p,
|  | fifo_state_t & | s )

## ◆ fifo_ld_pop() [33/42]

v64bfloat8 fifo_ld_pop | ( | v64bfloat8 *& | p,
|  | fifo_state_t & | s )

## ◆ fifo_ld_pop() [34/42]

v64float16_sparse fifo_ld_pop | ( | v64float16_sparse_unaligned *& | p,
|  | fifo_state_t & | s )

## ◆ fifo_ld_pop() [35/42]

v64float8 fifo_ld_pop | ( | v64float8 *& | p,
|  | fifo_state_t & | s )

## ◆ fifo_ld_pop() [36/42]

v64int16_sparse fifo_ld_pop | ( | v64int16_sparse_unaligned *& | p,
|  | fifo_state_t & | s )

## ◆ fifo_ld_pop() [37/42]

v64int8 fifo_ld_pop | ( | v64int8 *& | p,
|  | fifo_state_t & | s )

## ◆ fifo_ld_pop() [38/42]

v64mx9 fifo_ld_pop | ( | v64mx9_unaligned *& | p,
|  | fifo_state_t & | s )

## ◆ fifo_ld_pop() [39/42]

v64uint16_sparse fifo_ld_pop | ( | v64uint16_sparse_unaligned *& | p,
|  | fifo_state_t & | s )

## ◆ fifo_ld_pop() [40/42]

v64uint8 fifo_ld_pop | ( | v64uint8 *& | p,
|  | fifo_state_t & | s )

## ◆ fifo_ld_pop() [41/42]

v8cfloat fifo_ld_pop | ( | v8cfloat *& | p,
|  | fifo_state_t & | s )

## ◆ fifo_ld_pop() [42/42]

v8cint32 fifo_ld_pop | ( | v8cint32 *& | p,
|  | fifo_state_t & | s )

## ◆ fifo_ld_pop_1d_byte() [1/30]

v128bfloat8_sparse fifo_ld_pop_1d_byte | ( | v128bfloat8_sparse_unaligned *& | p,
|  | fifo_state_t & | s,
|  | int | off )

## ◆ fifo_ld_pop_1d_byte() [2/30]

v128float8_sparse fifo_ld_pop_1d_byte | ( | v128float8_sparse_unaligned *& | p,
|  | fifo_state_t & | s,
|  | int | off )

## ◆ fifo_ld_pop_1d_byte() [3/30]

v128int4 fifo_ld_pop_1d_byte | ( | v128int4 *& | p,
|  | fifo_state_t & | s,
|  | int | off )

## ◆ fifo_ld_pop_1d_byte() [4/30]

v128int8_sparse fifo_ld_pop_1d_byte | ( | v128int8_sparse_unaligned *& | p,
|  | fifo_state_t & | s,
|  | int | off )

## ◆ fifo_ld_pop_1d_byte() [5/30]

v128mx4 fifo_ld_pop_1d_byte | ( | v128mx4_unaligned *& | p,
|  | fifo_state_t & | s,
|  | int | off )

## ◆ fifo_ld_pop_1d_byte() [6/30]

v128mx6 fifo_ld_pop_1d_byte | ( | v128mx6_unaligned *& | p,
|  | fifo_state_t & | s,
|  | int | off )

## ◆ fifo_ld_pop_1d_byte() [7/30]

v128uint4 fifo_ld_pop_1d_byte | ( | v128uint4 *& | p,
|  | fifo_state_t & | s,
|  | int | off )

## ◆ fifo_ld_pop_1d_byte() [8/30]

v128uint8_sparse fifo_ld_pop_1d_byte | ( | v128uint8_sparse_unaligned *& | p,
|  | fifo_state_t & | s,
|  | int | off )

## ◆ fifo_ld_pop_1d_byte() [9/30]

v16cbfloat16 fifo_ld_pop_1d_byte | ( | v16cbfloat16 *& | p,
|  | fifo_state_t & | s,
|  | int | off )

## ◆ fifo_ld_pop_1d_byte() [10/30]

v16cint16 fifo_ld_pop_1d_byte | ( | v16cint16 *& | p,
|  | fifo_state_t & | s,
|  | int | off )

## ◆ fifo_ld_pop_1d_byte() [11/30]

v16float fifo_ld_pop_1d_byte | ( | v16float *& | p,
|  | fifo_state_t & | s,
|  | int | off )

## ◆ fifo_ld_pop_1d_byte() [12/30]

v16int32 fifo_ld_pop_1d_byte | ( | v16int32 *& | p,
|  | fifo_state_t & | s,
|  | int | off )

## ◆ fifo_ld_pop_1d_byte() [13/30]

v16uint32 fifo_ld_pop_1d_byte | ( | v16uint32 *& | p,
|  | fifo_state_t & | s,
|  | int | off )

## ◆ fifo_ld_pop_1d_byte() [14/30]

v256int4_sparse fifo_ld_pop_1d_byte | ( | v256int4_sparse_unaligned *& | p,
|  | fifo_state_t & | s,
|  | int | off )

## ◆ fifo_ld_pop_1d_byte() [15/30]

v256uint4_sparse fifo_ld_pop_1d_byte | ( | v256uint4_sparse_unaligned *& | p,
|  | fifo_state_t & | s,
|  | int | off )

## ◆ fifo_ld_pop_1d_byte() [16/30]

v32bfloat16 fifo_ld_pop_1d_byte | ( | v32bfloat16 *& | p,
|  | fifo_state_t & | s,
|  | int | off )

## ◆ fifo_ld_pop_1d_byte() [17/30]

v32float16 fifo_ld_pop_1d_byte | ( | v32float16 *& | p,
|  | fifo_state_t & | s,
|  | int | off )

## ◆ fifo_ld_pop_1d_byte() [18/30]

v32int16 fifo_ld_pop_1d_byte | ( | v32int16 *& | p,
|  | fifo_state_t & | s,
|  | int | off )

## ◆ fifo_ld_pop_1d_byte() [19/30]

v32uint16 fifo_ld_pop_1d_byte | ( | v32uint16 *& | p,
|  | fifo_state_t & | s,
|  | int | off )

## ◆ fifo_ld_pop_1d_byte() [20/30]

v64bfloat16_sparse fifo_ld_pop_1d_byte | ( | v64bfloat16_sparse_unaligned *& | p,
|  | fifo_state_t & | s,
|  | int | off )

## ◆ fifo_ld_pop_1d_byte() [21/30]

v64bfloat8 fifo_ld_pop_1d_byte | ( | v64bfloat8 *& | p,
|  | fifo_state_t & | s,
|  | int | off )

## ◆ fifo_ld_pop_1d_byte() [22/30]

v64float16_sparse fifo_ld_pop_1d_byte | ( | v64float16_sparse_unaligned *& | p,
|  | fifo_state_t & | s,
|  | int | off )

## ◆ fifo_ld_pop_1d_byte() [23/30]

v64float8 fifo_ld_pop_1d_byte | ( | v64float8 *& | p,
|  | fifo_state_t & | s,
|  | int | off )

## ◆ fifo_ld_pop_1d_byte() [24/30]

v64int16_sparse fifo_ld_pop_1d_byte | ( | v64int16_sparse_unaligned *& | p,
|  | fifo_state_t & | s,
|  | int | off )

## ◆ fifo_ld_pop_1d_byte() [25/30]

v64int8 fifo_ld_pop_1d_byte | ( | v64int8 *& | p,
|  | fifo_state_t & | s,
|  | int | off )

## ◆ fifo_ld_pop_1d_byte() [26/30]

v64mx9 fifo_ld_pop_1d_byte | ( | v64mx9_unaligned *& | p,
|  | fifo_state_t & | s,
|  | int | off )

## ◆ fifo_ld_pop_1d_byte() [27/30]

v64uint16_sparse fifo_ld_pop_1d_byte | ( | v64uint16_sparse_unaligned *& | p,
|  | fifo_state_t & | s,
|  | int | off )

## ◆ fifo_ld_pop_1d_byte() [28/30]

v64uint8 fifo_ld_pop_1d_byte | ( | v64uint8 *& | p,
|  | fifo_state_t & | s,
|  | int | off )

## ◆ fifo_ld_pop_1d_byte() [29/30]

v8cfloat fifo_ld_pop_1d_byte | ( | v8cfloat *& | p,
|  | fifo_state_t & | s,
|  | int | off )

## ◆ fifo_ld_pop_1d_byte() [30/30]

v8cint32 fifo_ld_pop_1d_byte | ( | v8cint32 *& | p,
|  | fifo_state_t & | s,
|  | int | off )

## ◆ fifo_ld_pop_2d_byte() [1/30]

v128bfloat8_sparse fifo_ld_pop_2d_byte | ( | v128bfloat8_sparse_unaligned *& | p,
|  | fifo_state_t & | s,
|  | int | off,
|  | int | size1,
|  | addr_t & | count1,
|  | int | inc1 )

## ◆ fifo_ld_pop_2d_byte() [2/30]

v128float8_sparse fifo_ld_pop_2d_byte | ( | v128float8_sparse_unaligned *& | p,
|  | fifo_state_t & | s,
|  | int | off,
|  | int | size1,
|  | addr_t & | count1,
|  | int | inc1 )

## ◆ fifo_ld_pop_2d_byte() [3/30]

v128int4 fifo_ld_pop_2d_byte | ( | v128int4 *& | p,
|  | fifo_state_t & | s,
|  | int | off,
|  | int | size1,
|  | addr_t & | count1,
|  | int | inc1 )

## ◆ fifo_ld_pop_2d_byte() [4/30]

v128int8_sparse fifo_ld_pop_2d_byte | ( | v128int8_sparse_unaligned *& | p,
|  | fifo_state_t & | s,
|  | int | off,
|  | int | size1,
|  | addr_t & | count1,
|  | int | inc1 )

## ◆ fifo_ld_pop_2d_byte() [5/30]

v128mx4 fifo_ld_pop_2d_byte | ( | v128mx4_unaligned *& | p,
|  | fifo_state_t & | s,
|  | int | off,
|  | int | size1,
|  | addr_t & | count1,
|  | int | inc1 )

## ◆ fifo_ld_pop_2d_byte() [6/30]

v128mx6 fifo_ld_pop_2d_byte | ( | v128mx6_unaligned *& | p,
|  | fifo_state_t & | s,
|  | int | off,
|  | int | size1,
|  | addr_t & | count1,
|  | int | inc1 )

## ◆ fifo_ld_pop_2d_byte() [7/30]

v128uint4 fifo_ld_pop_2d_byte | ( | v128uint4 *& | p,
|  | fifo_state_t & | s,
|  | int | off,
|  | int | size1,
|  | addr_t & | count1,
|  | int | inc1 )

## ◆ fifo_ld_pop_2d_byte() [8/30]

v128uint8_sparse fifo_ld_pop_2d_byte | ( | v128uint8_sparse_unaligned *& | p,
|  | fifo_state_t & | s,
|  | int | off,
|  | int | size1,
|  | addr_t & | count1,
|  | int | inc1 )

## ◆ fifo_ld_pop_2d_byte() [9/30]

v16cbfloat16 fifo_ld_pop_2d_byte | ( | v16cbfloat16 *& | p,
|  | fifo_state_t & | s,
|  | int | off,
|  | int | size1,
|  | addr_t & | count1,
|  | int | inc1 )

## ◆ fifo_ld_pop_2d_byte() [10/30]

v16cint16 fifo_ld_pop_2d_byte | ( | v16cint16 *& | p,
|  | fifo_state_t & | s,
|  | int | off,
|  | int | size1,
|  | addr_t & | count1,
|  | int | inc1 )

## ◆ fifo_ld_pop_2d_byte() [11/30]

v16float fifo_ld_pop_2d_byte | ( | v16float *& | p,
|  | fifo_state_t & | s,
|  | int | off,
|  | int | size1,
|  | addr_t & | count1,
|  | int | inc1 )

## ◆ fifo_ld_pop_2d_byte() [12/30]

v16int32 fifo_ld_pop_2d_byte | ( | v16int32 *& | p,
|  | fifo_state_t & | s,
|  | int | off,
|  | int | size1,
|  | addr_t & | count1,
|  | int | inc1 )

## ◆ fifo_ld_pop_2d_byte() [13/30]

v16uint32 fifo_ld_pop_2d_byte | ( | v16uint32 *& | p,
|  | fifo_state_t & | s,
|  | int | off,
|  | int | size1,
|  | addr_t & | count1,
|  | int | inc1 )

## ◆ fifo_ld_pop_2d_byte() [14/30]

v256int4_sparse fifo_ld_pop_2d_byte | ( | v256int4_sparse_unaligned *& | p,
|  | fifo_state_t & | s,
|  | int | off,
|  | int | size1,
|  | addr_t & | count1,
|  | int | inc1 )

## ◆ fifo_ld_pop_2d_byte() [15/30]

v256uint4_sparse fifo_ld_pop_2d_byte | ( | v256uint4_sparse_unaligned *& | p,
|  | fifo_state_t & | s,
|  | int | off,
|  | int | size1,
|  | addr_t & | count1,
|  | int | inc1 )

## ◆ fifo_ld_pop_2d_byte() [16/30]

v32bfloat16 fifo_ld_pop_2d_byte | ( | v32bfloat16 *& | p,
|  | fifo_state_t & | s,
|  | int | off,
|  | int | size1,
|  | addr_t & | count1,
|  | int | inc1 )

## ◆ fifo_ld_pop_2d_byte() [17/30]

v32float16 fifo_ld_pop_2d_byte | ( | v32float16 *& | p,
|  | fifo_state_t & | s,
|  | int | off,
|  | int | size1,
|  | addr_t & | count1,
|  | int | inc1 )

## ◆ fifo_ld_pop_2d_byte() [18/30]

v32int16 fifo_ld_pop_2d_byte | ( | v32int16 *& | p,
|  | fifo_state_t & | s,
|  | int | off,
|  | int | size1,
|  | addr_t & | count1,
|  | int | inc1 )

## ◆ fifo_ld_pop_2d_byte() [19/30]

v32uint16 fifo_ld_pop_2d_byte | ( | v32uint16 *& | p,
|  | fifo_state_t & | s,
|  | int | off,
|  | int | size1,
|  | addr_t & | count1,
|  | int | inc1 )

## ◆ fifo_ld_pop_2d_byte() [20/30]

v64bfloat16_sparse fifo_ld_pop_2d_byte | ( | v64bfloat16_sparse_unaligned *& | p,
|  | fifo_state_t & | s,
|  | int | off,
|  | int | size1,
|  | addr_t & | count1,
|  | int | inc1 )

## ◆ fifo_ld_pop_2d_byte() [21/30]

v64bfloat8 fifo_ld_pop_2d_byte | ( | v64bfloat8 *& | p,
|  | fifo_state_t & | s,
|  | int | off,
|  | int | size1,
|  | addr_t & | count1,
|  | int | inc1 )

## ◆ fifo_ld_pop_2d_byte() [22/30]

v64float16_sparse fifo_ld_pop_2d_byte | ( | v64float16_sparse_unaligned *& | p,
|  | fifo_state_t & | s,
|  | int | off,
|  | int | size1,
|  | addr_t & | count1,
|  | int | inc1 )

## ◆ fifo_ld_pop_2d_byte() [23/30]

v64float8 fifo_ld_pop_2d_byte | ( | v64float8 *& | p,
|  | fifo_state_t & | s,
|  | int | off,
|  | int | size1,
|  | addr_t & | count1,
|  | int | inc1 )

## ◆ fifo_ld_pop_2d_byte() [24/30]

v64int16_sparse fifo_ld_pop_2d_byte | ( | v64int16_sparse_unaligned *& | p,
|  | fifo_state_t & | s,
|  | int | off,
|  | int | size1,
|  | addr_t & | count1,
|  | int | inc1 )

## ◆ fifo_ld_pop_2d_byte() [25/30]

v64int8 fifo_ld_pop_2d_byte | ( | v64int8 *& | p,
|  | fifo_state_t & | s,
|  | int | off,
|  | int | size1,
|  | addr_t & | count1,
|  | int | inc1 )

## ◆ fifo_ld_pop_2d_byte() [26/30]

v64mx9 fifo_ld_pop_2d_byte | ( | v64mx9_unaligned *& | p,
|  | fifo_state_t & | s,
|  | int | off,
|  | int | size1,
|  | addr_t & | count1,
|  | int | inc1 )

## ◆ fifo_ld_pop_2d_byte() [27/30]

v64uint16_sparse fifo_ld_pop_2d_byte | ( | v64uint16_sparse_unaligned *& | p,
|  | fifo_state_t & | s,
|  | int | off,
|  | int | size1,
|  | addr_t & | count1,
|  | int | inc1 )

## ◆ fifo_ld_pop_2d_byte() [28/30]

v64uint8 fifo_ld_pop_2d_byte | ( | v64uint8 *& | p,
|  | fifo_state_t & | s,
|  | int | off,
|  | int | size1,
|  | addr_t & | count1,
|  | int | inc1 )

## ◆ fifo_ld_pop_2d_byte() [29/30]

v8cfloat fifo_ld_pop_2d_byte | ( | v8cfloat *& | p,
|  | fifo_state_t & | s,
|  | int | off,
|  | int | size1,
|  | addr_t & | count1,
|  | int | inc1 )

## ◆ fifo_ld_pop_2d_byte() [30/30]

v8cint32 fifo_ld_pop_2d_byte | ( | v8cint32 *& | p,
|  | fifo_state_t & | s,
|  | int | off,
|  | int | size1,
|  | addr_t & | count1,
|  | int | inc1 )

## ◆ fifo_ld_pop_3d_byte() [1/30]

v128bfloat8_sparse fifo_ld_pop_3d_byte | ( | v128bfloat8_sparse_unaligned *& | p,
|  | fifo_state_t & | s,
|  | int | off,
|  | int | size1,
|  | addr_t & | count1,
|  | int | inc1,
|  | int | size2,
|  | addr_t & | count2,
|  | int | inc2 )

## ◆ fifo_ld_pop_3d_byte() [2/30]

v128float8_sparse fifo_ld_pop_3d_byte | ( | v128float8_sparse_unaligned *& | p,
|  | fifo_state_t & | s,
|  | int | off,
|  | int | size1,
|  | addr_t & | count1,
|  | int | inc1,
|  | int | size2,
|  | addr_t & | count2,
|  | int | inc2 )

## ◆ fifo_ld_pop_3d_byte() [3/30]

v128int4 fifo_ld_pop_3d_byte | ( | v128int4 *& | p,
|  | fifo_state_t & | s,
|  | int | off,
|  | int | size1,
|  | addr_t & | count1,
|  | int | inc1,
|  | int | size2,
|  | addr_t & | count2,
|  | int | inc2 )

## ◆ fifo_ld_pop_3d_byte() [4/30]

v128int8_sparse fifo_ld_pop_3d_byte | ( | v128int8_sparse_unaligned *& | p,
|  | fifo_state_t & | s,
|  | int | off,
|  | int | size1,
|  | addr_t & | count1,
|  | int | inc1,
|  | int | size2,
|  | addr_t & | count2,
|  | int | inc2 )

## ◆ fifo_ld_pop_3d_byte() [5/30]

v128mx4 fifo_ld_pop_3d_byte | ( | v128mx4_unaligned *& | p,
|  | fifo_state_t & | s,
|  | int | off,
|  | int | size1,
|  | addr_t & | count1,
|  | int | inc1,
|  | int | size2,
|  | addr_t & | count2,
|  | int | inc2 )

## ◆ fifo_ld_pop_3d_byte() [6/30]

v128mx6 fifo_ld_pop_3d_byte | ( | v128mx6_unaligned *& | p,
|  | fifo_state_t & | s,
|  | int | off,
|  | int | size1,
|  | addr_t & | count1,
|  | int | inc1,
|  | int | size2,
|  | addr_t & | count2,
|  | int | inc2 )

## ◆ fifo_ld_pop_3d_byte() [7/30]

v128uint4 fifo_ld_pop_3d_byte | ( | v128uint4 *& | p,
|  | fifo_state_t & | s,
|  | int | off,
|  | int | size1,
|  | addr_t & | count1,
|  | int | inc1,
|  | int | size2,
|  | addr_t & | count2,
|  | int | inc2 )

## ◆ fifo_ld_pop_3d_byte() [8/30]

v128uint8_sparse fifo_ld_pop_3d_byte | ( | v128uint8_sparse_unaligned *& | p,
|  | fifo_state_t & | s,
|  | int | off,
|  | int | size1,
|  | addr_t & | count1,
|  | int | inc1,
|  | int | size2,
|  | addr_t & | count2,
|  | int | inc2 )

## ◆ fifo_ld_pop_3d_byte() [9/30]

v16cbfloat16 fifo_ld_pop_3d_byte | ( | v16cbfloat16 *& | p,
|  | fifo_state_t & | s,
|  | int | off,
|  | int | size1,
|  | addr_t & | count1,
|  | int | inc1,
|  | int | size2,
|  | addr_t & | count2,
|  | int | inc2 )

## ◆ fifo_ld_pop_3d_byte() [10/30]

v16cint16 fifo_ld_pop_3d_byte | ( | v16cint16 *& | p,
|  | fifo_state_t & | s,
|  | int | off,
|  | int | size1,
|  | addr_t & | count1,
|  | int | inc1,
|  | int | size2,
|  | addr_t & | count2,
|  | int | inc2 )

## ◆ fifo_ld_pop_3d_byte() [11/30]

v16float fifo_ld_pop_3d_byte | ( | v16float *& | p,
|  | fifo_state_t & | s,
|  | int | off,
|  | int | size1,
|  | addr_t & | count1,
|  | int | inc1,
|  | int | size2,
|  | addr_t & | count2,
|  | int | inc2 )

## ◆ fifo_ld_pop_3d_byte() [12/30]

v16int32 fifo_ld_pop_3d_byte | ( | v16int32 *& | p,
|  | fifo_state_t & | s,
|  | int | off,
|  | int | size1,
|  | addr_t & | count1,
|  | int | inc1,
|  | int | size2,
|  | addr_t & | count2,
|  | int | inc2 )

## ◆ fifo_ld_pop_3d_byte() [13/30]

v16uint32 fifo_ld_pop_3d_byte | ( | v16uint32 *& | p,
|  | fifo_state_t & | s,
|  | int | off,
|  | int | size1,
|  | addr_t & | count1,
|  | int | inc1,
|  | int | size2,
|  | addr_t & | count2,
|  | int | inc2 )

## ◆ fifo_ld_pop_3d_byte() [14/30]

v256int4_sparse fifo_ld_pop_3d_byte | ( | v256int4_sparse_unaligned *& | p,
|  | fifo_state_t & | s,
|  | int | off,
|  | int | size1,
|  | addr_t & | count1,
|  | int | inc1,
|  | int | size2,
|  | addr_t & | count2,
|  | int | inc2 )

## ◆ fifo_ld_pop_3d_byte() [15/30]

v256uint4_sparse fifo_ld_pop_3d_byte | ( | v256uint4_sparse_unaligned *& | p,
|  | fifo_state_t & | s,
|  | int | off,
|  | int | size1,
|  | addr_t & | count1,
|  | int | inc1,
|  | int | size2,
|  | addr_t & | count2,
|  | int | inc2 )

## ◆ fifo_ld_pop_3d_byte() [16/30]

v32bfloat16 fifo_ld_pop_3d_byte | ( | v32bfloat16 *& | p,
|  | fifo_state_t & | s,
|  | int | off,
|  | int | size1,
|  | addr_t & | count1,
|  | int | inc1,
|  | int | size2,
|  | addr_t & | count2,
|  | int | inc2 )

## ◆ fifo_ld_pop_3d_byte() [17/30]

v32float16 fifo_ld_pop_3d_byte | ( | v32float16 *& | p,
|  | fifo_state_t & | s,
|  | int | off,
|  | int | size1,
|  | addr_t & | count1,
|  | int | inc1,
|  | int | size2,
|  | addr_t & | count2,
|  | int | inc2 )

## ◆ fifo_ld_pop_3d_byte() [18/30]

v32int16 fifo_ld_pop_3d_byte | ( | v32int16 *& | p,
|  | fifo_state_t & | s,
|  | int | off,
|  | int | size1,
|  | addr_t & | count1,
|  | int | inc1,
|  | int | size2,
|  | addr_t & | count2,
|  | int | inc2 )

## ◆ fifo_ld_pop_3d_byte() [19/30]

v32uint16 fifo_ld_pop_3d_byte | ( | v32uint16 *& | p,
|  | fifo_state_t & | s,
|  | int | off,
|  | int | size1,
|  | addr_t & | count1,
|  | int | inc1,
|  | int | size2,
|  | addr_t & | count2,
|  | int | inc2 )

## ◆ fifo_ld_pop_3d_byte() [20/30]

v64bfloat16_sparse fifo_ld_pop_3d_byte | ( | v64bfloat16_sparse_unaligned *& | p,
|  | fifo_state_t & | s,
|  | int | off,
|  | int | size1,
|  | addr_t & | count1,
|  | int | inc1,
|  | int | size2,
|  | addr_t & | count2,
|  | int | inc2 )

## ◆ fifo_ld_pop_3d_byte() [21/30]

v64bfloat8 fifo_ld_pop_3d_byte | ( | v64bfloat8 *& | p,
|  | fifo_state_t & | s,
|  | int | off,
|  | int | size1,
|  | addr_t & | count1,
|  | int | inc1,
|  | int | size2,
|  | addr_t & | count2,
|  | int | inc2 )

## ◆ fifo_ld_pop_3d_byte() [22/30]

v64float16_sparse fifo_ld_pop_3d_byte | ( | v64float16_sparse_unaligned *& | p,
|  | fifo_state_t & | s,
|  | int | off,
|  | int | size1,
|  | addr_t & | count1,
|  | int | inc1,
|  | int | size2,
|  | addr_t & | count2,
|  | int | inc2 )

## ◆ fifo_ld_pop_3d_byte() [23/30]

v64float8 fifo_ld_pop_3d_byte | ( | v64float8 *& | p,
|  | fifo_state_t & | s,
|  | int | off,
|  | int | size1,
|  | addr_t & | count1,
|  | int | inc1,
|  | int | size2,
|  | addr_t & | count2,
|  | int | inc2 )

## ◆ fifo_ld_pop_3d_byte() [24/30]

v64int16_sparse fifo_ld_pop_3d_byte | ( | v64int16_sparse_unaligned *& | p,
|  | fifo_state_t & | s,
|  | int | off,
|  | int | size1,
|  | addr_t & | count1,
|  | int | inc1,
|  | int | size2,
|  | addr_t & | count2,
|  | int | inc2 )

## ◆ fifo_ld_pop_3d_byte() [25/30]

v64int8 fifo_ld_pop_3d_byte | ( | v64int8 *& | p,
|  | fifo_state_t & | s,
|  | int | off,
|  | int | size1,
|  | addr_t & | count1,
|  | int | inc1,
|  | int | size2,
|  | addr_t & | count2,
|  | int | inc2 )

## ◆ fifo_ld_pop_3d_byte() [26/30]

v64mx9 fifo_ld_pop_3d_byte | ( | v64mx9_unaligned *& | p,
|  | fifo_state_t & | s,
|  | int | off,
|  | int | size1,
|  | addr_t & | count1,
|  | int | inc1,
|  | int | size2,
|  | addr_t & | count2,
|  | int | inc2 )

## ◆ fifo_ld_pop_3d_byte() [27/30]

v64uint16_sparse fifo_ld_pop_3d_byte | ( | v64uint16_sparse_unaligned *& | p,
|  | fifo_state_t & | s,
|  | int | off,
|  | int | size1,
|  | addr_t & | count1,
|  | int | inc1,
|  | int | size2,
|  | addr_t & | count2,
|  | int | inc2 )

## ◆ fifo_ld_pop_3d_byte() [28/30]

v64uint8 fifo_ld_pop_3d_byte | ( | v64uint8 *& | p,
|  | fifo_state_t & | s,
|  | int | off,
|  | int | size1,
|  | addr_t & | count1,
|  | int | inc1,
|  | int | size2,
|  | addr_t & | count2,
|  | int | inc2 )

## ◆ fifo_ld_pop_3d_byte() [29/30]

v8cfloat fifo_ld_pop_3d_byte | ( | v8cfloat *& | p,
|  | fifo_state_t & | s,
|  | int | off,
|  | int | size1,
|  | addr_t & | count1,
|  | int | inc1,
|  | int | size2,
|  | addr_t & | count2,
|  | int | inc2 )

## ◆ fifo_ld_pop_3d_byte() [30/30]

v8cint32 fifo_ld_pop_3d_byte | ( | v8cint32 *& | p,
|  | fifo_state_t & | s,
|  | int | off,
|  | int | size1,
|  | addr_t & | count1,
|  | int | inc1,
|  | int | size2,
|  | addr_t & | count2,
|  | int | inc2 )

## ◆ fifo_ld_popx() [1/34]

v128int4 fifo_ld_popx | ( | v128int4 *& | p,
|  | fifo_state_t & | s )

## ◆ fifo_ld_popx() [2/34]

v128int4 fifo_ld_popx | ( | v128int4 *& | p,
|  | fifo_state_t & | s,
|  | int | step,
|  | int | mask )

## ◆ fifo_ld_popx() [3/34]

v128uint4 fifo_ld_popx | ( | v128uint4 *& | p,
|  | fifo_state_t & | s )

## ◆ fifo_ld_popx() [4/34]

v128uint4 fifo_ld_popx | ( | v128uint4 *& | p,
|  | fifo_state_t & | s,
|  | int | step,
|  | int | mask )

## ◆ fifo_ld_popx() [5/34]

v16cbfloat16 fifo_ld_popx | ( | v16cbfloat16 *& | p,
|  | fifo_state_t & | s )

## ◆ fifo_ld_popx() [6/34]

v16cbfloat16 fifo_ld_popx | ( | v16cbfloat16 *& | p,
|  | fifo_state_t & | s,
|  | int | step,
|  | int | mask )

## ◆ fifo_ld_popx() [7/34]

v16cint16 fifo_ld_popx | ( | v16cint16 *& | p,
|  | fifo_state_t & | s )

## ◆ fifo_ld_popx() [8/34]

v16cint16 fifo_ld_popx | ( | v16cint16 *& | p,
|  | fifo_state_t & | s,
|  | int | step,
|  | int | mask )

## ◆ fifo_ld_popx() [9/34]

v16float fifo_ld_popx | ( | v16float *& | p,
|  | fifo_state_t & | s )

## ◆ fifo_ld_popx() [10/34]

v16float fifo_ld_popx | ( | v16float *& | p,
|  | fifo_state_t & | s,
|  | int | step,
|  | int | mask )

## ◆ fifo_ld_popx() [11/34]

v16int32 fifo_ld_popx | ( | v16int32 *& | p,
|  | fifo_state_t & | s )

## ◆ fifo_ld_popx() [12/34]

v16int32 fifo_ld_popx | ( | v16int32 *& | p,
|  | fifo_state_t & | s,
|  | int | step,
|  | int | mask )

## ◆ fifo_ld_popx() [13/34]

v16uint32 fifo_ld_popx | ( | v16uint32 *& | p,
|  | fifo_state_t & | s )

## ◆ fifo_ld_popx() [14/34]

v16uint32 fifo_ld_popx | ( | v16uint32 *& | p,
|  | fifo_state_t & | s,
|  | int | step,
|  | int | mask )

## ◆ fifo_ld_popx() [15/34]

v32bfloat16 fifo_ld_popx | ( | v32bfloat16 *& | p,
|  | fifo_state_t & | s )

## ◆ fifo_ld_popx() [16/34]

v32bfloat16 fifo_ld_popx | ( | v32bfloat16 *& | p,
|  | fifo_state_t & | s,
|  | int | step,
|  | int | mask )

## ◆ fifo_ld_popx() [17/34]

v32float16 fifo_ld_popx | ( | v32float16 *& | p,
|  | fifo_state_t & | s )

## ◆ fifo_ld_popx() [18/34]

v32float16 fifo_ld_popx | ( | v32float16 *& | p,
|  | fifo_state_t & | s,
|  | int | step,
|  | int | mask )

## ◆ fifo_ld_popx() [19/34]

v32int16 fifo_ld_popx | ( | v32int16 *& | p,
|  | fifo_state_t & | s )

## ◆ fifo_ld_popx() [20/34]

v32int16 fifo_ld_popx | ( | v32int16 *& | p,
|  | fifo_state_t & | s,
|  | int | step,
|  | int | mask )

## ◆ fifo_ld_popx() [21/34]

v32uint16 fifo_ld_popx | ( | v32uint16 *& | p,
|  | fifo_state_t & | s )

## ◆ fifo_ld_popx() [22/34]

v32uint16 fifo_ld_popx | ( | v32uint16 *& | p,
|  | fifo_state_t & | s,
|  | int | step,
|  | int | mask )

## ◆ fifo_ld_popx() [23/34]

v64bfloat8 fifo_ld_popx | ( | v64bfloat8 *& | p,
|  | fifo_state_t & | s )

## ◆ fifo_ld_popx() [24/34]

v64bfloat8 fifo_ld_popx | ( | v64bfloat8 *& | p,
|  | fifo_state_t & | s,
|  | int | step,
|  | int | mask )

## ◆ fifo_ld_popx() [25/34]

v64float8 fifo_ld_popx | ( | v64float8 *& | p,
|  | fifo_state_t & | s )

## ◆ fifo_ld_popx() [26/34]

v64float8 fifo_ld_popx | ( | v64float8 *& | p,
|  | fifo_state_t & | s,
|  | int | step,
|  | int | mask )

## ◆ fifo_ld_popx() [27/34]

v64int8 fifo_ld_popx | ( | v64int8 *& | p,
|  | fifo_state_t & | s )

## ◆ fifo_ld_popx() [28/34]

v64int8 fifo_ld_popx | ( | v64int8 *& | p,
|  | fifo_state_t & | s,
|  | int | step,
|  | int | mask )

## ◆ fifo_ld_popx() [29/34]

v64uint8 fifo_ld_popx | ( | v64uint8 *& | p,
|  | fifo_state_t & | s )

## ◆ fifo_ld_popx() [30/34]

v64uint8 fifo_ld_popx | ( | v64uint8 *& | p,
|  | fifo_state_t & | s,
|  | int | step,
|  | int | mask )

## ◆ fifo_ld_popx() [31/34]

v8cfloat fifo_ld_popx | ( | v8cfloat *& | p,
|  | fifo_state_t & | s )

## ◆ fifo_ld_popx() [32/34]

v8cfloat fifo_ld_popx | ( | v8cfloat *& | p,
|  | fifo_state_t & | s,
|  | int | step,
|  | int | mask )

## ◆ fifo_ld_popx() [33/34]

v8cint32 fifo_ld_popx | ( | v8cint32 *& | p,
|  | fifo_state_t & | s )

## ◆ fifo_ld_popx() [34/34]

v8cint32 fifo_ld_popx | ( | v8cint32 *& | p,
|  | fifo_state_t & | s,
|  | int | step,
|  | int | mask )

## ◆ fifo_ld_reset() [1/42]

void fifo_ld_reset | ( | v128bfloat16_sparse_unaligned *& | p,
|  | fifo_state_t & | fifo )

## ◆ fifo_ld_reset() [2/42]

void fifo_ld_reset | ( | v128bfloat8_sparse_unaligned *& | p,
|  | fifo_state_t & | s )

## ◆ fifo_ld_reset() [3/42]

void fifo_ld_reset | ( | v128float16_sparse_unaligned *& | p,
|  | fifo_state_t & | fifo )

## ◆ fifo_ld_reset() [4/42]

void fifo_ld_reset | ( | v128float8_sparse_unaligned *& | p,
|  | fifo_state_t & | s )

## ◆ fifo_ld_reset() [5/42]

void fifo_ld_reset | ( | v128int16_sparse_unaligned *& | p,
|  | fifo_state_t & | fifo )

## ◆ fifo_ld_reset() [6/42]

void fifo_ld_reset | ( | v128int4 *& | p,
|  | fifo_state_t & | s )

## ◆ fifo_ld_reset() [7/42]

void fifo_ld_reset | ( | v128int8_sparse_unaligned *& | p,
|  | fifo_state_t & | s )

## ◆ fifo_ld_reset() [8/42]

void fifo_ld_reset | ( | v128mx4_unaligned *& | p,
|  | fifo_state_t & | s )

## ◆ fifo_ld_reset() [9/42]

void fifo_ld_reset | ( | v128mx6_unaligned *& | p,
|  | fifo_state_t & | s )

## ◆ fifo_ld_reset() [10/42]

void fifo_ld_reset | ( | v128uint16_sparse_unaligned *& | p,
|  | fifo_state_t & | fifo )

## ◆ fifo_ld_reset() [11/42]

void fifo_ld_reset | ( | v128uint4 *& | p,
|  | fifo_state_t & | s )

## ◆ fifo_ld_reset() [12/42]

void fifo_ld_reset | ( | v128uint8_sparse_unaligned *& | p,
|  | fifo_state_t & | s )

## ◆ fifo_ld_reset() [13/42]

void fifo_ld_reset | ( | v16cbfloat16 *& | p,
|  | fifo_state_t & | s )

## ◆ fifo_ld_reset() [14/42]

void fifo_ld_reset | ( | v16cint16 *& | p,
|  | fifo_state_t & | s )

## ◆ fifo_ld_reset() [15/42]

void fifo_ld_reset | ( | v16float *& | p,
|  | fifo_state_t & | s )

## ◆ fifo_ld_reset() [16/42]

void fifo_ld_reset | ( | v16int32 *& | p,
|  | fifo_state_t & | s )

## ◆ fifo_ld_reset() [17/42]

void fifo_ld_reset | ( | v16uint32 *& | p,
|  | fifo_state_t & | s )

## ◆ fifo_ld_reset() [18/42]

void fifo_ld_reset | ( | v256bfloat8_sparse_unaligned *& | p,
|  | fifo_state_t & | fifo )

## ◆ fifo_ld_reset() [19/42]

void fifo_ld_reset | ( | v256float8_sparse_unaligned *& | p,
|  | fifo_state_t & | fifo )

## ◆ fifo_ld_reset() [20/42]

void fifo_ld_reset | ( | v256int4_sparse_unaligned *& | p,
|  | fifo_state_t & | s )

## ◆ fifo_ld_reset() [21/42]

void fifo_ld_reset | ( | v256int8_sparse_unaligned *& | p,
|  | fifo_state_t & | fifo )

## ◆ fifo_ld_reset() [22/42]

void fifo_ld_reset | ( | v256mx4_unaligned *& | p,
|  | fifo_state_t & | fifo )

## ◆ fifo_ld_reset() [23/42]

void fifo_ld_reset | ( | v256mx6_unaligned *& | p,
|  | fifo_state_t & | fifo )

## ◆ fifo_ld_reset() [24/42]

void fifo_ld_reset | ( | v256uint4_sparse_unaligned *& | p,
|  | fifo_state_t & | s )

## ◆ fifo_ld_reset() [25/42]

void fifo_ld_reset | ( | v256uint8_sparse_unaligned *& | p,
|  | fifo_state_t & | fifo )

## ◆ fifo_ld_reset() [26/42]

void fifo_ld_reset | ( | v32bfloat16 *& | p,
|  | fifo_state_t & | s )

## ◆ fifo_ld_reset() [27/42]

void fifo_ld_reset | ( | v32float16 *& | p,
|  | fifo_state_t & | s )

## ◆ fifo_ld_reset() [28/42]

void fifo_ld_reset | ( | v32int16 *& | p,
|  | fifo_state_t & | s )

## ◆ fifo_ld_reset() [29/42]

void fifo_ld_reset | ( | v32uint16 *& | p,
|  | fifo_state_t & | s )

## ◆ fifo_ld_reset() [30/42]

void fifo_ld_reset | ( | v512int4_sparse_unaligned *& | p,
|  | fifo_state_t & | fifo )

## ◆ fifo_ld_reset() [31/42]

void fifo_ld_reset | ( | v512uint4_sparse_unaligned *& | p,
|  | fifo_state_t & | fifo )

## ◆ fifo_ld_reset() [32/42]

void fifo_ld_reset | ( | v64bfloat16_sparse_unaligned *& | p,
|  | fifo_state_t & | s )

## ◆ fifo_ld_reset() [33/42]

void fifo_ld_reset | ( | v64bfloat8 *& | p,
|  | fifo_state_t & | s )

## ◆ fifo_ld_reset() [34/42]

void fifo_ld_reset | ( | v64float16_sparse_unaligned *& | p,
|  | fifo_state_t & | s )

## ◆ fifo_ld_reset() [35/42]

void fifo_ld_reset | ( | v64float8 *& | p,
|  | fifo_state_t & | s )

## ◆ fifo_ld_reset() [36/42]

void fifo_ld_reset | ( | v64int16_sparse_unaligned *& | p,
|  | fifo_state_t & | s )

## ◆ fifo_ld_reset() [37/42]

void fifo_ld_reset | ( | v64int8 *& | p,
|  | fifo_state_t & | s )

## ◆ fifo_ld_reset() [38/42]

void fifo_ld_reset | ( | v64mx9_unaligned *& | p,
|  | fifo_state_t & | s )

## ◆ fifo_ld_reset() [39/42]

void fifo_ld_reset | ( | v64uint16_sparse_unaligned *& | p,
|  | fifo_state_t & | s )

## ◆ fifo_ld_reset() [40/42]

void fifo_ld_reset | ( | v64uint8 *& | p,
|  | fifo_state_t & | s )

## ◆ fifo_ld_reset() [41/42]

void fifo_ld_reset | ( | v8cfloat *& | p,
|  | fifo_state_t & | s )

## ◆ fifo_ld_reset() [42/42]

void fifo_ld_reset | ( | v8cint32 *& | p,
|  | fifo_state_t & | s )

## ◆ fifo_st_flush() [1/22]

void fifo_st_flush | ( | v128int4 *& | p,
|  | fifo_state_t & | s )

## ◆ fifo_st_flush() [2/22]

void fifo_st_flush | ( | v128mx4_unaligned *& | p,
|  | fifo_state_t & | s )

## ◆ fifo_st_flush() [3/22]

void fifo_st_flush | ( | v128mx6_unaligned *& | p,
|  | fifo_state_t & | s )

## ◆ fifo_st_flush() [4/22]

void fifo_st_flush | ( | v128uint4 *& | p,
|  | fifo_state_t & | s )

## ◆ fifo_st_flush() [5/22]

void fifo_st_flush | ( | v16cbfloat16 *& | p,
|  | fifo_state_t & | s )

## ◆ fifo_st_flush() [6/22]

void fifo_st_flush | ( | v16cint16 *& | p,
|  | fifo_state_t & | s )

## ◆ fifo_st_flush() [7/22]

void fifo_st_flush | ( | v16float *& | p,
|  | fifo_state_t & | s )

## ◆ fifo_st_flush() [8/22]

void fifo_st_flush | ( | v16int32 *& | p,
|  | fifo_state_t & | s )

## ◆ fifo_st_flush() [9/22]

void fifo_st_flush | ( | v16uint32 *& | p,
|  | fifo_state_t & | s )

## ◆ fifo_st_flush() [10/22]

void fifo_st_flush | ( | v32bfloat16 *& | p,
|  | fifo_state_t & | s )

## ◆ fifo_st_flush() [11/22]

void fifo_st_flush | ( | v32float16 *& | p,
|  | fifo_state_t & | s )

## ◆ fifo_st_flush() [12/22]

void fifo_st_flush | ( | v32int16 *& | p,
|  | fifo_state_t & | s )

## ◆ fifo_st_flush() [13/22]

void fifo_st_flush | ( | v32uint16 *& | p,
|  | fifo_state_t & | s )

## ◆ fifo_st_flush() [14/22]

void fifo_st_flush | ( | v64bfloat8 *& | p,
|  | fifo_state_t & | s )

## ◆ fifo_st_flush() [15/22]

void fifo_st_flush | ( | v64float8 *& | p,
|  | fifo_state_t & | s )

## ◆ fifo_st_flush() [16/22]

void fifo_st_flush | ( | v64int8 *& | p,
|  | fifo_state_t & | s )

## ◆ fifo_st_flush() [17/22]

void fifo_st_flush | ( | v64mx4_unaligned *& | p,
|  | fifo_state_t & | s )

## ◆ fifo_st_flush() [18/22]

void fifo_st_flush | ( | v64mx6_unaligned *& | p,
|  | fifo_state_t & | s )

## ◆ fifo_st_flush() [19/22]

void fifo_st_flush | ( | v64mx9_unaligned *& | p,
|  | fifo_state_t & | s )

## ◆ fifo_st_flush() [20/22]

void fifo_st_flush | ( | v64uint8 *& | p,
|  | fifo_state_t & | s )

## ◆ fifo_st_flush() [21/22]

void fifo_st_flush | ( | v8cfloat *& | p,
|  | fifo_state_t & | s )

## ◆ fifo_st_flush() [22/22]

void fifo_st_flush | ( | v8cint32 *& | p,
|  | fifo_state_t & | s )

## ◆ fifo_st_flush_1d_byte() [1/22]

void fifo_st_flush_1d_byte | ( | v128int4 *& | p,
|  | fifo_state_t & | s,
|  | int | off )

## ◆ fifo_st_flush_1d_byte() [2/22]

void fifo_st_flush_1d_byte | ( | v128mx4_unaligned *& | p,
|  | fifo_state_t & | s,
|  | int | off )

## ◆ fifo_st_flush_1d_byte() [3/22]

void fifo_st_flush_1d_byte | ( | v128mx6_unaligned *& | p,
|  | fifo_state_t & | s,
|  | int | off )

## ◆ fifo_st_flush_1d_byte() [4/22]

void fifo_st_flush_1d_byte | ( | v128uint4 *& | p,
|  | fifo_state_t & | s,
|  | int | off )

## ◆ fifo_st_flush_1d_byte() [5/22]

void fifo_st_flush_1d_byte | ( | v16cbfloat16 *& | p,
|  | fifo_state_t & | s,
|  | int | off )

## ◆ fifo_st_flush_1d_byte() [6/22]

void fifo_st_flush_1d_byte | ( | v16cint16 *& | p,
|  | fifo_state_t & | s,
|  | int | off )

## ◆ fifo_st_flush_1d_byte() [7/22]

void fifo_st_flush_1d_byte | ( | v16float *& | p,
|  | fifo_state_t & | s,
|  | int | off )

## ◆ fifo_st_flush_1d_byte() [8/22]

void fifo_st_flush_1d_byte | ( | v16int32 *& | p,
|  | fifo_state_t & | s,
|  | int | off )

## ◆ fifo_st_flush_1d_byte() [9/22]

void fifo_st_flush_1d_byte | ( | v16uint32 *& | p,
|  | fifo_state_t & | s,
|  | int | off )

## ◆ fifo_st_flush_1d_byte() [10/22]

void fifo_st_flush_1d_byte | ( | v32bfloat16 *& | p,
|  | fifo_state_t & | s,
|  | int | off )

## ◆ fifo_st_flush_1d_byte() [11/22]

void fifo_st_flush_1d_byte | ( | v32float16 *& | p,
|  | fifo_state_t & | s,
|  | int | off )

## ◆ fifo_st_flush_1d_byte() [12/22]

void fifo_st_flush_1d_byte | ( | v32int16 *& | p,
|  | fifo_state_t & | s,
|  | int | off )

## ◆ fifo_st_flush_1d_byte() [13/22]

void fifo_st_flush_1d_byte | ( | v32uint16 *& | p,
|  | fifo_state_t & | s,
|  | int | off )

## ◆ fifo_st_flush_1d_byte() [14/22]

void fifo_st_flush_1d_byte | ( | v64bfloat8 *& | p,
|  | fifo_state_t & | s,
|  | int | off )

## ◆ fifo_st_flush_1d_byte() [15/22]

void fifo_st_flush_1d_byte | ( | v64float8 *& | p,
|  | fifo_state_t & | s,
|  | int | off )

## ◆ fifo_st_flush_1d_byte() [16/22]

void fifo_st_flush_1d_byte | ( | v64int8 *& | p,
|  | fifo_state_t & | s,
|  | int | off )

## ◆ fifo_st_flush_1d_byte() [17/22]

void fifo_st_flush_1d_byte | ( | v64mx4_unaligned *& | p,
|  | fifo_state_t & | s,
|  | int | off )

## ◆ fifo_st_flush_1d_byte() [18/22]

void fifo_st_flush_1d_byte | ( | v64mx6_unaligned *& | p,
|  | fifo_state_t & | s,
|  | int | off )

## ◆ fifo_st_flush_1d_byte() [19/22]

void fifo_st_flush_1d_byte | ( | v64mx9_unaligned *& | p,
|  | fifo_state_t & | s,
|  | int | off )

## ◆ fifo_st_flush_1d_byte() [20/22]

void fifo_st_flush_1d_byte | ( | v64uint8 *& | p,
|  | fifo_state_t & | s,
|  | int | off )

## ◆ fifo_st_flush_1d_byte() [21/22]

void fifo_st_flush_1d_byte | ( | v8cfloat *& | p,
|  | fifo_state_t & | s,
|  | int | off )

## ◆ fifo_st_flush_1d_byte() [22/22]

void fifo_st_flush_1d_byte | ( | v8cint32 *& | p,
|  | fifo_state_t & | s,
|  | int | off )

## ◆ fifo_st_flush_2d_byte() [1/22]

void fifo_st_flush_2d_byte | ( | v128int4 *& | p,
|  | fifo_state_t & | s,
|  | int | off,
|  | int | size1,
|  | addr_t & | count1,
|  | int | inc1 )

## ◆ fifo_st_flush_2d_byte() [2/22]

void fifo_st_flush_2d_byte | ( | v128mx4_unaligned *& | p,
|  | fifo_state_t & | s,
|  | int | off,
|  | int | size1,
|  | addr_t & | count1,
|  | int | inc1 )

## ◆ fifo_st_flush_2d_byte() [3/22]

void fifo_st_flush_2d_byte | ( | v128mx6_unaligned *& | p,
|  | fifo_state_t & | s,
|  | int | off,
|  | int | size1,
|  | addr_t & | count1,
|  | int | inc1 )

## ◆ fifo_st_flush_2d_byte() [4/22]

void fifo_st_flush_2d_byte | ( | v128uint4 *& | p,
|  | fifo_state_t & | s,
|  | int | off,
|  | int | size1,
|  | addr_t & | count1,
|  | int | inc1 )

## ◆ fifo_st_flush_2d_byte() [5/22]

void fifo_st_flush_2d_byte | ( | v16cbfloat16 *& | p,
|  | fifo_state_t & | s,
|  | int | off,
|  | int | size1,
|  | addr_t & | count1,
|  | int | inc1 )

## ◆ fifo_st_flush_2d_byte() [6/22]

void fifo_st_flush_2d_byte | ( | v16cint16 *& | p,
|  | fifo_state_t & | s,
|  | int | off,
|  | int | size1,
|  | addr_t & | count1,
|  | int | inc1 )

## ◆ fifo_st_flush_2d_byte() [7/22]

void fifo_st_flush_2d_byte | ( | v16float *& | p,
|  | fifo_state_t & | s,
|  | int | off,
|  | int | size1,
|  | addr_t & | count1,
|  | int | inc1 )

## ◆ fifo_st_flush_2d_byte() [8/22]

void fifo_st_flush_2d_byte | ( | v16int32 *& | p,
|  | fifo_state_t & | s,
|  | int | off,
|  | int | size1,
|  | addr_t & | count1,
|  | int | inc1 )

## ◆ fifo_st_flush_2d_byte() [9/22]

void fifo_st_flush_2d_byte | ( | v16uint32 *& | p,
|  | fifo_state_t & | s,
|  | int | off,
|  | int | size1,
|  | addr_t & | count1,
|  | int | inc1 )

## ◆ fifo_st_flush_2d_byte() [10/22]

void fifo_st_flush_2d_byte | ( | v32bfloat16 *& | p,
|  | fifo_state_t & | s,
|  | int | off,
|  | int | size1,
|  | addr_t & | count1,
|  | int | inc1 )

## ◆ fifo_st_flush_2d_byte() [11/22]

void fifo_st_flush_2d_byte | ( | v32float16 *& | p,
|  | fifo_state_t & | s,
|  | int | off,
|  | int | size1,
|  | addr_t & | count1,
|  | int | inc1 )

## ◆ fifo_st_flush_2d_byte() [12/22]

void fifo_st_flush_2d_byte | ( | v32int16 *& | p,
|  | fifo_state_t & | s,
|  | int | off,
|  | int | size1,
|  | addr_t & | count1,
|  | int | inc1 )

## ◆ fifo_st_flush_2d_byte() [13/22]

void fifo_st_flush_2d_byte | ( | v32uint16 *& | p,
|  | fifo_state_t & | s,
|  | int | off,
|  | int | size1,
|  | addr_t & | count1,
|  | int | inc1 )

## ◆ fifo_st_flush_2d_byte() [14/22]

void fifo_st_flush_2d_byte | ( | v64bfloat8 *& | p,
|  | fifo_state_t & | s,
|  | int | off,
|  | int | size1,
|  | addr_t & | count1,
|  | int | inc1 )

## ◆ fifo_st_flush_2d_byte() [15/22]

void fifo_st_flush_2d_byte | ( | v64float8 *& | p,
|  | fifo_state_t & | s,
|  | int | off,
|  | int | size1,
|  | addr_t & | count1,
|  | int | inc1 )

## ◆ fifo_st_flush_2d_byte() [16/22]

void fifo_st_flush_2d_byte | ( | v64int8 *& | p,
|  | fifo_state_t & | s,
|  | int | off,
|  | int | size1,
|  | addr_t & | count1,
|  | int | inc1 )

## ◆ fifo_st_flush_2d_byte() [17/22]

void fifo_st_flush_2d_byte | ( | v64mx4_unaligned *& | p,
|  | fifo_state_t & | s,
|  | int | off,
|  | int | size1,
|  | addr_t & | count1,
|  | int | inc1 )

## ◆ fifo_st_flush_2d_byte() [18/22]

void fifo_st_flush_2d_byte | ( | v64mx6_unaligned *& | p,
|  | fifo_state_t & | s,
|  | int | off,
|  | int | size1,
|  | addr_t & | count1,
|  | int | inc1 )

## ◆ fifo_st_flush_2d_byte() [19/22]

void fifo_st_flush_2d_byte | ( | v64mx9_unaligned *& | p,
|  | fifo_state_t & | s,
|  | int | off,
|  | int | size1,
|  | addr_t & | count1,
|  | int | inc1 )

## ◆ fifo_st_flush_2d_byte() [20/22]

void fifo_st_flush_2d_byte | ( | v64uint8 *& | p,
|  | fifo_state_t & | s,
|  | int | off,
|  | int | size1,
|  | addr_t & | count1,
|  | int | inc1 )

## ◆ fifo_st_flush_2d_byte() [21/22]

void fifo_st_flush_2d_byte | ( | v8cfloat *& | p,
|  | fifo_state_t & | s,
|  | int | off,
|  | int | size1,
|  | addr_t & | count1,
|  | int | inc1 )

## ◆ fifo_st_flush_2d_byte() [22/22]

void fifo_st_flush_2d_byte | ( | v8cint32 *& | p,
|  | fifo_state_t & | s,
|  | int | off,
|  | int | size1,
|  | addr_t & | count1,
|  | int | inc1 )

## ◆ fifo_st_flush_3d_byte() [1/22]

void fifo_st_flush_3d_byte | ( | v128int4 *& | p,
|  | fifo_state_t & | s,
|  | int | off,
|  | int | size1,
|  | addr_t & | count1,
|  | int | inc1,
|  | int | size2,
|  | addr_t & | count2,
|  | int | inc2 )

## ◆ fifo_st_flush_3d_byte() [2/22]

void fifo_st_flush_3d_byte | ( | v128mx4_unaligned *& | p,
|  | fifo_state_t & | s,
|  | int | off,
|  | int | size1,
|  | addr_t & | count1,
|  | int | inc1,
|  | int | size2,
|  | addr_t & | count2,
|  | int | inc2 )

## ◆ fifo_st_flush_3d_byte() [3/22]

void fifo_st_flush_3d_byte | ( | v128mx6_unaligned *& | p,
|  | fifo_state_t & | s,
|  | int | off,
|  | int | size1,
|  | addr_t & | count1,
|  | int | inc1,
|  | int | size2,
|  | addr_t & | count2,
|  | int | inc2 )

## ◆ fifo_st_flush_3d_byte() [4/22]

void fifo_st_flush_3d_byte | ( | v128uint4 *& | p,
|  | fifo_state_t & | s,
|  | int | off,
|  | int | size1,
|  | addr_t & | count1,
|  | int | inc1,
|  | int | size2,
|  | addr_t & | count2,
|  | int | inc2 )

## ◆ fifo_st_flush_3d_byte() [5/22]

void fifo_st_flush_3d_byte | ( | v16cbfloat16 *& | p,
|  | fifo_state_t & | s,
|  | int | off,
|  | int | size1,
|  | addr_t & | count1,
|  | int | inc1,
|  | int | size2,
|  | addr_t & | count2,
|  | int | inc2 )

## ◆ fifo_st_flush_3d_byte() [6/22]

void fifo_st_flush_3d_byte | ( | v16cint16 *& | p,
|  | fifo_state_t & | s,
|  | int | off,
|  | int | size1,
|  | addr_t & | count1,
|  | int | inc1,
|  | int | size2,
|  | addr_t & | count2,
|  | int | inc2 )

## ◆ fifo_st_flush_3d_byte() [7/22]

void fifo_st_flush_3d_byte | ( | v16float *& | p,
|  | fifo_state_t & | s,
|  | int | off,
|  | int | size1,
|  | addr_t & | count1,
|  | int | inc1,
|  | int | size2,
|  | addr_t & | count2,
|  | int | inc2 )

## ◆ fifo_st_flush_3d_byte() [8/22]

void fifo_st_flush_3d_byte | ( | v16int32 *& | p,
|  | fifo_state_t & | s,
|  | int | off,
|  | int | size1,
|  | addr_t & | count1,
|  | int | inc1,
|  | int | size2,
|  | addr_t & | count2,
|  | int | inc2 )

## ◆ fifo_st_flush_3d_byte() [9/22]

void fifo_st_flush_3d_byte | ( | v16uint32 *& | p,
|  | fifo_state_t & | s,
|  | int | off,
|  | int | size1,
|  | addr_t & | count1,
|  | int | inc1,
|  | int | size2,
|  | addr_t & | count2,
|  | int | inc2 )

## ◆ fifo_st_flush_3d_byte() [10/22]

void fifo_st_flush_3d_byte | ( | v32bfloat16 *& | p,
|  | fifo_state_t & | s,
|  | int | off,
|  | int | size1,
|  | addr_t & | count1,
|  | int | inc1,
|  | int | size2,
|  | addr_t & | count2,
|  | int | inc2 )

## ◆ fifo_st_flush_3d_byte() [11/22]

void fifo_st_flush_3d_byte | ( | v32float16 *& | p,
|  | fifo_state_t & | s,
|  | int | off,
|  | int | size1,
|  | addr_t & | count1,
|  | int | inc1,
|  | int | size2,
|  | addr_t & | count2,
|  | int | inc2 )

## ◆ fifo_st_flush_3d_byte() [12/22]

void fifo_st_flush_3d_byte | ( | v32int16 *& | p,
|  | fifo_state_t & | s,
|  | int | off,
|  | int | size1,
|  | addr_t & | count1,
|  | int | inc1,
|  | int | size2,
|  | addr_t & | count2,
|  | int | inc2 )

## ◆ fifo_st_flush_3d_byte() [13/22]

void fifo_st_flush_3d_byte | ( | v32uint16 *& | p,
|  | fifo_state_t & | s,
|  | int | off,
|  | int | size1,
|  | addr_t & | count1,
|  | int | inc1,
|  | int | size2,
|  | addr_t & | count2,
|  | int | inc2 )

## ◆ fifo_st_flush_3d_byte() [14/22]

void fifo_st_flush_3d_byte | ( | v64bfloat8 *& | p,
|  | fifo_state_t & | s,
|  | int | off,
|  | int | size1,
|  | addr_t & | count1,
|  | int | inc1,
|  | int | size2,
|  | addr_t & | count2,
|  | int | inc2 )

## ◆ fifo_st_flush_3d_byte() [15/22]

void fifo_st_flush_3d_byte | ( | v64float8 *& | p,
|  | fifo_state_t & | s,
|  | int | off,
|  | int | size1,
|  | addr_t & | count1,
|  | int | inc1,
|  | int | size2,
|  | addr_t & | count2,
|  | int | inc2 )

## ◆ fifo_st_flush_3d_byte() [16/22]

void fifo_st_flush_3d_byte | ( | v64int8 *& | p,
|  | fifo_state_t & | s,
|  | int | off,
|  | int | size1,
|  | addr_t & | count1,
|  | int | inc1,
|  | int | size2,
|  | addr_t & | count2,
|  | int | inc2 )

## ◆ fifo_st_flush_3d_byte() [17/22]

void fifo_st_flush_3d_byte | ( | v64mx4_unaligned *& | p,
|  | fifo_state_t & | s,
|  | int | off,
|  | int | size1,
|  | addr_t & | count1,
|  | int | inc1,
|  | int | size2,
|  | addr_t & | count2,
|  | int | inc2 )

## ◆ fifo_st_flush_3d_byte() [18/22]

void fifo_st_flush_3d_byte | ( | v64mx6_unaligned *& | p,
|  | fifo_state_t & | s,
|  | int | off,
|  | int | size1,
|  | addr_t & | count1,
|  | int | inc1,
|  | int | size2,
|  | addr_t & | count2,
|  | int | inc2 )

## ◆ fifo_st_flush_3d_byte() [19/22]

void fifo_st_flush_3d_byte | ( | v64mx9_unaligned *& | p,
|  | fifo_state_t & | s,
|  | int | off,
|  | int | size1,
|  | addr_t & | count1,
|  | int | inc1,
|  | int | size2,
|  | addr_t & | count2,
|  | int | inc2 )

## ◆ fifo_st_flush_3d_byte() [20/22]

void fifo_st_flush_3d_byte | ( | v64uint8 *& | p,
|  | fifo_state_t & | s,
|  | int | off,
|  | int | size1,
|  | addr_t & | count1,
|  | int | inc1,
|  | int | size2,
|  | addr_t & | count2,
|  | int | inc2 )

## ◆ fifo_st_flush_3d_byte() [21/22]

void fifo_st_flush_3d_byte | ( | v8cfloat *& | p,
|  | fifo_state_t & | s,
|  | int | off,
|  | int | size1,
|  | addr_t & | count1,
|  | int | inc1,
|  | int | size2,
|  | addr_t & | count2,
|  | int | inc2 )

## ◆ fifo_st_flush_3d_byte() [22/22]

void fifo_st_flush_3d_byte | ( | v8cint32 *& | p,
|  | fifo_state_t & | s,
|  | int | off,
|  | int | size1,
|  | addr_t & | count1,
|  | int | inc1,
|  | int | size2,
|  | addr_t & | count2,
|  | int | inc2 )

## ◆ fifo_st_flush_bare() [1/22]

void fifo_st_flush_bare | ( | v128int4 *& | p,
|  | fifo_state_t & | s )

## ◆ fifo_st_flush_bare() [2/22]

void fifo_st_flush_bare | ( | v128mx4_unaligned *& | p,
|  | fifo_state_t & | s )

## ◆ fifo_st_flush_bare() [3/22]

void fifo_st_flush_bare | ( | v128mx6_unaligned *& | p,
|  | fifo_state_t & | s )

## ◆ fifo_st_flush_bare() [4/22]

void fifo_st_flush_bare | ( | v128uint4 *& | p,
|  | fifo_state_t & | s )

## ◆ fifo_st_flush_bare() [5/22]

void fifo_st_flush_bare | ( | v16cbfloat16 *& | p,
|  | fifo_state_t & | s )

## ◆ fifo_st_flush_bare() [6/22]

void fifo_st_flush_bare | ( | v16cint16 *& | p,
|  | fifo_state_t & | s )

## ◆ fifo_st_flush_bare() [7/22]

void fifo_st_flush_bare | ( | v16float *& | p,
|  | fifo_state_t & | s )

## ◆ fifo_st_flush_bare() [8/22]

void fifo_st_flush_bare | ( | v16int32 *& | p,
|  | fifo_state_t & | s )

## ◆ fifo_st_flush_bare() [9/22]

void fifo_st_flush_bare | ( | v16uint32 *& | p,
|  | fifo_state_t & | s )

## ◆ fifo_st_flush_bare() [10/22]

void fifo_st_flush_bare | ( | v32bfloat16 *& | p,
|  | fifo_state_t & | s )

## ◆ fifo_st_flush_bare() [11/22]

void fifo_st_flush_bare | ( | v32float16 *& | p,
|  | fifo_state_t & | s )

## ◆ fifo_st_flush_bare() [12/22]

void fifo_st_flush_bare | ( | v32int16 *& | p,
|  | fifo_state_t & | s )

## ◆ fifo_st_flush_bare() [13/22]

void fifo_st_flush_bare | ( | v32uint16 *& | p,
|  | fifo_state_t & | s )

## ◆ fifo_st_flush_bare() [14/22]

void fifo_st_flush_bare | ( | v64bfloat8 *& | p,
|  | fifo_state_t & | s )

## ◆ fifo_st_flush_bare() [15/22]

void fifo_st_flush_bare | ( | v64float8 *& | p,
|  | fifo_state_t & | s )

## ◆ fifo_st_flush_bare() [16/22]

void fifo_st_flush_bare | ( | v64int8 *& | p,
|  | fifo_state_t & | s )

## ◆ fifo_st_flush_bare() [17/22]

void fifo_st_flush_bare | ( | v64mx4_unaligned *& | p,
|  | fifo_state_t & | s )

## ◆ fifo_st_flush_bare() [18/22]

void fifo_st_flush_bare | ( | v64mx6_unaligned *& | p,
|  | fifo_state_t & | s )

## ◆ fifo_st_flush_bare() [19/22]

void fifo_st_flush_bare | ( | v64mx9_unaligned *& | p,
|  | fifo_state_t & | s )

## ◆ fifo_st_flush_bare() [20/22]

void fifo_st_flush_bare | ( | v64uint8 *& | p,
|  | fifo_state_t & | s )

## ◆ fifo_st_flush_bare() [21/22]

void fifo_st_flush_bare | ( | v8cfloat *& | p,
|  | fifo_state_t & | s )

## ◆ fifo_st_flush_bare() [22/22]

void fifo_st_flush_bare | ( | v8cint32 *& | p,
|  | fifo_state_t & | s )

## ◆ fifo_st_flush_bare_1d_byte() [1/22]

void fifo_st_flush_bare_1d_byte | ( | v128int4 *& | p,
|  | fifo_state_t & | s,
|  | int | off )

## ◆ fifo_st_flush_bare_1d_byte() [2/22]

void fifo_st_flush_bare_1d_byte | ( | v128mx4_unaligned *& | p,
|  | fifo_state_t & | s,
|  | int | off )

## ◆ fifo_st_flush_bare_1d_byte() [3/22]

void fifo_st_flush_bare_1d_byte | ( | v128mx6_unaligned *& | p,
|  | fifo_state_t & | s,
|  | int | off )

## ◆ fifo_st_flush_bare_1d_byte() [4/22]

void fifo_st_flush_bare_1d_byte | ( | v128uint4 *& | p,
|  | fifo_state_t & | s,
|  | int | off )

## ◆ fifo_st_flush_bare_1d_byte() [5/22]

void fifo_st_flush_bare_1d_byte | ( | v16cbfloat16 *& | p,
|  | fifo_state_t & | s,
|  | int | off )

## ◆ fifo_st_flush_bare_1d_byte() [6/22]

void fifo_st_flush_bare_1d_byte | ( | v16cint16 *& | p,
|  | fifo_state_t & | s,
|  | int | off )

## ◆ fifo_st_flush_bare_1d_byte() [7/22]

void fifo_st_flush_bare_1d_byte | ( | v16float *& | p,
|  | fifo_state_t & | s,
|  | int | off )

## ◆ fifo_st_flush_bare_1d_byte() [8/22]

void fifo_st_flush_bare_1d_byte | ( | v16int32 *& | p,
|  | fifo_state_t & | s,
|  | int | off )

## ◆ fifo_st_flush_bare_1d_byte() [9/22]

void fifo_st_flush_bare_1d_byte | ( | v16uint32 *& | p,
|  | fifo_state_t & | s,
|  | int | off )

## ◆ fifo_st_flush_bare_1d_byte() [10/22]

void fifo_st_flush_bare_1d_byte | ( | v32bfloat16 *& | p,
|  | fifo_state_t & | s,
|  | int | off )

## ◆ fifo_st_flush_bare_1d_byte() [11/22]

void fifo_st_flush_bare_1d_byte | ( | v32float16 *& | p,
|  | fifo_state_t & | s,
|  | int | off )

## ◆ fifo_st_flush_bare_1d_byte() [12/22]

void fifo_st_flush_bare_1d_byte | ( | v32int16 *& | p,
|  | fifo_state_t & | s,
|  | int | off )

## ◆ fifo_st_flush_bare_1d_byte() [13/22]

void fifo_st_flush_bare_1d_byte | ( | v32uint16 *& | p,
|  | fifo_state_t & | s,
|  | int | off )

## ◆ fifo_st_flush_bare_1d_byte() [14/22]

void fifo_st_flush_bare_1d_byte | ( | v64bfloat8 *& | p,
|  | fifo_state_t & | s,
|  | int | off )

## ◆ fifo_st_flush_bare_1d_byte() [15/22]

void fifo_st_flush_bare_1d_byte | ( | v64float8 *& | p,
|  | fifo_state_t & | s,
|  | int | off )

## ◆ fifo_st_flush_bare_1d_byte() [16/22]

void fifo_st_flush_bare_1d_byte | ( | v64int8 *& | p,
|  | fifo_state_t & | s,
|  | int | off )

## ◆ fifo_st_flush_bare_1d_byte() [17/22]

void fifo_st_flush_bare_1d_byte | ( | v64mx4_unaligned *& | p,
|  | fifo_state_t & | s,
|  | int | off )

## ◆ fifo_st_flush_bare_1d_byte() [18/22]

void fifo_st_flush_bare_1d_byte | ( | v64mx6_unaligned *& | p,
|  | fifo_state_t & | s,
|  | int | off )

## ◆ fifo_st_flush_bare_1d_byte() [19/22]

void fifo_st_flush_bare_1d_byte | ( | v64mx9_unaligned *& | p,
|  | fifo_state_t & | s,
|  | int | off )

## ◆ fifo_st_flush_bare_1d_byte() [20/22]

void fifo_st_flush_bare_1d_byte | ( | v64uint8 *& | p,
|  | fifo_state_t & | s,
|  | int | off )

## ◆ fifo_st_flush_bare_1d_byte() [21/22]

void fifo_st_flush_bare_1d_byte | ( | v8cfloat *& | p,
|  | fifo_state_t & | s,
|  | int | off )

## ◆ fifo_st_flush_bare_1d_byte() [22/22]

void fifo_st_flush_bare_1d_byte | ( | v8cint32 *& | p,
|  | fifo_state_t & | s,
|  | int | off )

## ◆ fifo_st_flush_bare_2d_byte() [1/22]

void fifo_st_flush_bare_2d_byte | ( | v128int4 *& | p,
|  | fifo_state_t & | s,
|  | int | off,
|  | int | size1,
|  | addr_t & | count1,
|  | int | inc1 )

## ◆ fifo_st_flush_bare_2d_byte() [2/22]

void fifo_st_flush_bare_2d_byte | ( | v128mx4_unaligned *& | p,
|  | fifo_state_t & | s,
|  | int | off,
|  | int | size1,
|  | addr_t & | count1,
|  | int | inc1 )

## ◆ fifo_st_flush_bare_2d_byte() [3/22]

void fifo_st_flush_bare_2d_byte | ( | v128mx6_unaligned *& | p,
|  | fifo_state_t & | s,
|  | int | off,
|  | int | size1,
|  | addr_t & | count1,
|  | int | inc1 )

## ◆ fifo_st_flush_bare_2d_byte() [4/22]

void fifo_st_flush_bare_2d_byte | ( | v128uint4 *& | p,
|  | fifo_state_t & | s,
|  | int | off,
|  | int | size1,
|  | addr_t & | count1,
|  | int | inc1 )

## ◆ fifo_st_flush_bare_2d_byte() [5/22]

void fifo_st_flush_bare_2d_byte | ( | v16cbfloat16 *& | p,
|  | fifo_state_t & | s,
|  | int | off,
|  | int | size1,
|  | addr_t & | count1,
|  | int | inc1 )

## ◆ fifo_st_flush_bare_2d_byte() [6/22]

void fifo_st_flush_bare_2d_byte | ( | v16cint16 *& | p,
|  | fifo_state_t & | s,
|  | int | off,
|  | int | size1,
|  | addr_t & | count1,
|  | int | inc1 )

## ◆ fifo_st_flush_bare_2d_byte() [7/22]

void fifo_st_flush_bare_2d_byte | ( | v16float *& | p,
|  | fifo_state_t & | s,
|  | int | off,
|  | int | size1,
|  | addr_t & | count1,
|  | int | inc1 )

## ◆ fifo_st_flush_bare_2d_byte() [8/22]

void fifo_st_flush_bare_2d_byte | ( | v16int32 *& | p,
|  | fifo_state_t & | s,
|  | int | off,
|  | int | size1,
|  | addr_t & | count1,
|  | int | inc1 )

## ◆ fifo_st_flush_bare_2d_byte() [9/22]

void fifo_st_flush_bare_2d_byte | ( | v16uint32 *& | p,
|  | fifo_state_t & | s,
|  | int | off,
|  | int | size1,
|  | addr_t & | count1,
|  | int | inc1 )

## ◆ fifo_st_flush_bare_2d_byte() [10/22]

void fifo_st_flush_bare_2d_byte | ( | v32bfloat16 *& | p,
|  | fifo_state_t & | s,
|  | int | off,
|  | int | size1,
|  | addr_t & | count1,
|  | int | inc1 )

## ◆ fifo_st_flush_bare_2d_byte() [11/22]

void fifo_st_flush_bare_2d_byte | ( | v32float16 *& | p,
|  | fifo_state_t & | s,
|  | int | off,
|  | int | size1,
|  | addr_t & | count1,
|  | int | inc1 )

## ◆ fifo_st_flush_bare_2d_byte() [12/22]

void fifo_st_flush_bare_2d_byte | ( | v32int16 *& | p,
|  | fifo_state_t & | s,
|  | int | off,
|  | int | size1,
|  | addr_t & | count1,
|  | int | inc1 )

## ◆ fifo_st_flush_bare_2d_byte() [13/22]

void fifo_st_flush_bare_2d_byte | ( | v32uint16 *& | p,
|  | fifo_state_t & | s,
|  | int | off,
|  | int | size1,
|  | addr_t & | count1,
|  | int | inc1 )

## ◆ fifo_st_flush_bare_2d_byte() [14/22]

void fifo_st_flush_bare_2d_byte | ( | v64bfloat8 *& | p,
|  | fifo_state_t & | s,
|  | int | off,
|  | int | size1,
|  | addr_t & | count1,
|  | int | inc1 )

## ◆ fifo_st_flush_bare_2d_byte() [15/22]

void fifo_st_flush_bare_2d_byte | ( | v64float8 *& | p,
|  | fifo_state_t & | s,
|  | int | off,
|  | int | size1,
|  | addr_t & | count1,
|  | int | inc1 )

## ◆ fifo_st_flush_bare_2d_byte() [16/22]

void fifo_st_flush_bare_2d_byte | ( | v64int8 *& | p,
|  | fifo_state_t & | s,
|  | int | off,
|  | int | size1,
|  | addr_t & | count1,
|  | int | inc1 )

## ◆ fifo_st_flush_bare_2d_byte() [17/22]

void fifo_st_flush_bare_2d_byte | ( | v64mx4_unaligned *& | p,
|  | fifo_state_t & | s,
|  | int | off,
|  | int | size1,
|  | addr_t & | count1,
|  | int | inc1 )

## ◆ fifo_st_flush_bare_2d_byte() [18/22]

void fifo_st_flush_bare_2d_byte | ( | v64mx6_unaligned *& | p,
|  | fifo_state_t & | s,
|  | int | off,
|  | int | size1,
|  | addr_t & | count1,
|  | int | inc1 )

## ◆ fifo_st_flush_bare_2d_byte() [19/22]

void fifo_st_flush_bare_2d_byte | ( | v64mx9_unaligned *& | p,
|  | fifo_state_t & | s,
|  | int | off,
|  | int | size1,
|  | addr_t & | count1,
|  | int | inc1 )

## ◆ fifo_st_flush_bare_2d_byte() [20/22]

void fifo_st_flush_bare_2d_byte | ( | v64uint8 *& | p,
|  | fifo_state_t & | s,
|  | int | off,
|  | int | size1,
|  | addr_t & | count1,
|  | int | inc1 )

## ◆ fifo_st_flush_bare_2d_byte() [21/22]

void fifo_st_flush_bare_2d_byte | ( | v8cfloat *& | p,
|  | fifo_state_t & | s,
|  | int | off,
|  | int | size1,
|  | addr_t & | count1,
|  | int | inc1 )

## ◆ fifo_st_flush_bare_2d_byte() [22/22]

void fifo_st_flush_bare_2d_byte | ( | v8cint32 *& | p,
|  | fifo_state_t & | s,
|  | int | off,
|  | int | size1,
|  | addr_t & | count1,
|  | int | inc1 )

## ◆ fifo_st_flush_bare_3d_byte() [1/22]

void fifo_st_flush_bare_3d_byte | ( | v128int4 *& | p,
|  | fifo_state_t & | s,
|  | int | off,
|  | int | size1,
|  | addr_t & | count1,
|  | int | inc1,
|  | int | size2,
|  | addr_t & | count2,
|  | int | inc2 )

## ◆ fifo_st_flush_bare_3d_byte() [2/22]

void fifo_st_flush_bare_3d_byte | ( | v128mx4_unaligned *& | p,
|  | fifo_state_t & | s,
|  | int | off,
|  | int | size1,
|  | addr_t & | count1,
|  | int | inc1,
|  | int | size2,
|  | addr_t & | count2,
|  | int | inc2 )

## ◆ fifo_st_flush_bare_3d_byte() [3/22]

void fifo_st_flush_bare_3d_byte | ( | v128mx6_unaligned *& | p,
|  | fifo_state_t & | s,
|  | int | off,
|  | int | size1,
|  | addr_t & | count1,
|  | int | inc1,
|  | int | size2,
|  | addr_t & | count2,
|  | int | inc2 )

## ◆ fifo_st_flush_bare_3d_byte() [4/22]

void fifo_st_flush_bare_3d_byte | ( | v128uint4 *& | p,
|  | fifo_state_t & | s,
|  | int | off,
|  | int | size1,
|  | addr_t & | count1,
|  | int | inc1,
|  | int | size2,
|  | addr_t & | count2,
|  | int | inc2 )

## ◆ fifo_st_flush_bare_3d_byte() [5/22]

void fifo_st_flush_bare_3d_byte | ( | v16cbfloat16 *& | p,
|  | fifo_state_t & | s,
|  | int | off,
|  | int | size1,
|  | addr_t & | count1,
|  | int | inc1,
|  | int | size2,
|  | addr_t & | count2,
|  | int | inc2 )

## ◆ fifo_st_flush_bare_3d_byte() [6/22]

void fifo_st_flush_bare_3d_byte | ( | v16cint16 *& | p,
|  | fifo_state_t & | s,
|  | int | off,
|  | int | size1,
|  | addr_t & | count1,
|  | int | inc1,
|  | int | size2,
|  | addr_t & | count2,
|  | int | inc2 )

## ◆ fifo_st_flush_bare_3d_byte() [7/22]

void fifo_st_flush_bare_3d_byte | ( | v16float *& | p,
|  | fifo_state_t & | s,
|  | int | off,
|  | int | size1,
|  | addr_t & | count1,
|  | int | inc1,
|  | int | size2,
|  | addr_t & | count2,
|  | int | inc2 )

## ◆ fifo_st_flush_bare_3d_byte() [8/22]

void fifo_st_flush_bare_3d_byte | ( | v16int32 *& | p,
|  | fifo_state_t & | s,
|  | int | off,
|  | int | size1,
|  | addr_t & | count1,
|  | int | inc1,
|  | int | size2,
|  | addr_t & | count2,
|  | int | inc2 )

## ◆ fifo_st_flush_bare_3d_byte() [9/22]

void fifo_st_flush_bare_3d_byte | ( | v16uint32 *& | p,
|  | fifo_state_t & | s,
|  | int | off,
|  | int | size1,
|  | addr_t & | count1,
|  | int | inc1,
|  | int | size2,
|  | addr_t & | count2,
|  | int | inc2 )

## ◆ fifo_st_flush_bare_3d_byte() [10/22]

void fifo_st_flush_bare_3d_byte | ( | v32bfloat16 *& | p,
|  | fifo_state_t & | s,
|  | int | off,
|  | int | size1,
|  | addr_t & | count1,
|  | int | inc1,
|  | int | size2,
|  | addr_t & | count2,
|  | int | inc2 )

## ◆ fifo_st_flush_bare_3d_byte() [11/22]

void fifo_st_flush_bare_3d_byte | ( | v32float16 *& | p,
|  | fifo_state_t & | s,
|  | int | off,
|  | int | size1,
|  | addr_t & | count1,
|  | int | inc1,
|  | int | size2,
|  | addr_t & | count2,
|  | int | inc2 )

## ◆ fifo_st_flush_bare_3d_byte() [12/22]

void fifo_st_flush_bare_3d_byte | ( | v32int16 *& | p,
|  | fifo_state_t & | s,
|  | int | off,
|  | int | size1,
|  | addr_t & | count1,
|  | int | inc1,
|  | int | size2,
|  | addr_t & | count2,
|  | int | inc2 )

## ◆ fifo_st_flush_bare_3d_byte() [13/22]

void fifo_st_flush_bare_3d_byte | ( | v32uint16 *& | p,
|  | fifo_state_t & | s,
|  | int | off,
|  | int | size1,
|  | addr_t & | count1,
|  | int | inc1,
|  | int | size2,
|  | addr_t & | count2,
|  | int | inc2 )

## ◆ fifo_st_flush_bare_3d_byte() [14/22]

void fifo_st_flush_bare_3d_byte | ( | v64bfloat8 *& | p,
|  | fifo_state_t & | s,
|  | int | off,
|  | int | size1,
|  | addr_t & | count1,
|  | int | inc1,
|  | int | size2,
|  | addr_t & | count2,
|  | int | inc2 )

## ◆ fifo_st_flush_bare_3d_byte() [15/22]

void fifo_st_flush_bare_3d_byte | ( | v64float8 *& | p,
|  | fifo_state_t & | s,
|  | int | off,
|  | int | size1,
|  | addr_t & | count1,
|  | int | inc1,
|  | int | size2,
|  | addr_t & | count2,
|  | int | inc2 )

## ◆ fifo_st_flush_bare_3d_byte() [16/22]

void fifo_st_flush_bare_3d_byte | ( | v64int8 *& | p,
|  | fifo_state_t & | s,
|  | int | off,
|  | int | size1,
|  | addr_t & | count1,
|  | int | inc1,
|  | int | size2,
|  | addr_t & | count2,
|  | int | inc2 )

## ◆ fifo_st_flush_bare_3d_byte() [17/22]

void fifo_st_flush_bare_3d_byte | ( | v64mx4_unaligned *& | p,
|  | fifo_state_t & | s,
|  | int | off,
|  | int | size1,
|  | addr_t & | count1,
|  | int | inc1,
|  | int | size2,
|  | addr_t & | count2,
|  | int | inc2 )

## ◆ fifo_st_flush_bare_3d_byte() [18/22]

void fifo_st_flush_bare_3d_byte | ( | v64mx6_unaligned *& | p,
|  | fifo_state_t & | s,
|  | int | off,
|  | int | size1,
|  | addr_t & | count1,
|  | int | inc1,
|  | int | size2,
|  | addr_t & | count2,
|  | int | inc2 )

## ◆ fifo_st_flush_bare_3d_byte() [19/22]

void fifo_st_flush_bare_3d_byte | ( | v64mx9_unaligned *& | p,
|  | fifo_state_t & | s,
|  | int | off,
|  | int | size1,
|  | addr_t & | count1,
|  | int | inc1,
|  | int | size2,
|  | addr_t & | count2,
|  | int | inc2 )

## ◆ fifo_st_flush_bare_3d_byte() [20/22]

void fifo_st_flush_bare_3d_byte | ( | v64uint8 *& | p,
|  | fifo_state_t & | s,
|  | int | off,
|  | int | size1,
|  | addr_t & | count1,
|  | int | inc1,
|  | int | size2,
|  | addr_t & | count2,
|  | int | inc2 )

## ◆ fifo_st_flush_bare_3d_byte() [21/22]

void fifo_st_flush_bare_3d_byte | ( | v8cfloat *& | p,
|  | fifo_state_t & | s,
|  | int | off,
|  | int | size1,
|  | addr_t & | count1,
|  | int | inc1,
|  | int | size2,
|  | addr_t & | count2,
|  | int | inc2 )

## ◆ fifo_st_flush_bare_3d_byte() [22/22]

void fifo_st_flush_bare_3d_byte | ( | v8cint32 *& | p,
|  | fifo_state_t & | s,
|  | int | off,
|  | int | size1,
|  | addr_t & | count1,
|  | int | inc1,
|  | int | size2,
|  | addr_t & | count2,
|  | int | inc2 )

## ◆ fifo_st_flush_conv() [1/22]

void fifo_st_flush_conv | ( | v128int4 *& | p,
|  | fifo_state_t & | s )

## ◆ fifo_st_flush_conv() [2/22]

void fifo_st_flush_conv | ( | v128mx4_unaligned *& | p,
|  | fifo_state_t & | s )

## ◆ fifo_st_flush_conv() [3/22]

void fifo_st_flush_conv | ( | v128mx6_unaligned *& | p,
|  | fifo_state_t & | s )

## ◆ fifo_st_flush_conv() [4/22]

void fifo_st_flush_conv | ( | v128uint4 *& | p,
|  | fifo_state_t & | s )

## ◆ fifo_st_flush_conv() [5/22]

void fifo_st_flush_conv | ( | v16cbfloat16 *& | p,
|  | fifo_state_t & | s )

## ◆ fifo_st_flush_conv() [6/22]

void fifo_st_flush_conv | ( | v16cint16 *& | p,
|  | fifo_state_t & | s )

## ◆ fifo_st_flush_conv() [7/22]

void fifo_st_flush_conv | ( | v16float *& | p,
|  | fifo_state_t & | s )

## ◆ fifo_st_flush_conv() [8/22]

void fifo_st_flush_conv | ( | v16int32 *& | p,
|  | fifo_state_t & | s )

## ◆ fifo_st_flush_conv() [9/22]

void fifo_st_flush_conv | ( | v16uint32 *& | p,
|  | fifo_state_t & | s )

## ◆ fifo_st_flush_conv() [10/22]

void fifo_st_flush_conv | ( | v32bfloat16 *& | p,
|  | fifo_state_t & | s )

## ◆ fifo_st_flush_conv() [11/22]

void fifo_st_flush_conv | ( | v32float16 *& | p,
|  | fifo_state_t & | s )

## ◆ fifo_st_flush_conv() [12/22]

void fifo_st_flush_conv | ( | v32int16 *& | p,
|  | fifo_state_t & | s )

## ◆ fifo_st_flush_conv() [13/22]

void fifo_st_flush_conv | ( | v32uint16 *& | p,
|  | fifo_state_t & | s )

## ◆ fifo_st_flush_conv() [14/22]

void fifo_st_flush_conv | ( | v64bfloat8 *& | p,
|  | fifo_state_t & | s )

## ◆ fifo_st_flush_conv() [15/22]

void fifo_st_flush_conv | ( | v64float8 *& | p,
|  | fifo_state_t & | s )

## ◆ fifo_st_flush_conv() [16/22]

void fifo_st_flush_conv | ( | v64int8 *& | p,
|  | fifo_state_t & | s )

## ◆ fifo_st_flush_conv() [17/22]

void fifo_st_flush_conv | ( | v64mx4_unaligned *& | p,
|  | fifo_state_t & | s )

## ◆ fifo_st_flush_conv() [18/22]

void fifo_st_flush_conv | ( | v64mx6_unaligned *& | p,
|  | fifo_state_t & | s )

## ◆ fifo_st_flush_conv() [19/22]

void fifo_st_flush_conv | ( | v64mx9_unaligned *& | p,
|  | fifo_state_t & | s )

## ◆ fifo_st_flush_conv() [20/22]

void fifo_st_flush_conv | ( | v64uint8 *& | p,
|  | fifo_state_t & | s )

## ◆ fifo_st_flush_conv() [21/22]

void fifo_st_flush_conv | ( | v8cfloat *& | p,
|  | fifo_state_t & | s )

## ◆ fifo_st_flush_conv() [22/22]

void fifo_st_flush_conv | ( | v8cint32 *& | p,
|  | fifo_state_t & | s )

## ◆ fifo_st_flush_conv_1d_byte() [1/22]

void fifo_st_flush_conv_1d_byte | ( | v128int4 *& | p,
|  | fifo_state_t & | s,
|  | int | off )

## ◆ fifo_st_flush_conv_1d_byte() [2/22]

void fifo_st_flush_conv_1d_byte | ( | v128mx4_unaligned *& | p,
|  | fifo_state_t & | s,
|  | int | off )

## ◆ fifo_st_flush_conv_1d_byte() [3/22]

void fifo_st_flush_conv_1d_byte | ( | v128mx6_unaligned *& | p,
|  | fifo_state_t & | s,
|  | int | off )

## ◆ fifo_st_flush_conv_1d_byte() [4/22]

void fifo_st_flush_conv_1d_byte | ( | v128uint4 *& | p,
|  | fifo_state_t & | s,
|  | int | off )

## ◆ fifo_st_flush_conv_1d_byte() [5/22]

void fifo_st_flush_conv_1d_byte | ( | v16cbfloat16 *& | p,
|  | fifo_state_t & | s,
|  | int | off )

## ◆ fifo_st_flush_conv_1d_byte() [6/22]

void fifo_st_flush_conv_1d_byte | ( | v16cint16 *& | p,
|  | fifo_state_t & | s,
|  | int | off )

## ◆ fifo_st_flush_conv_1d_byte() [7/22]

void fifo_st_flush_conv_1d_byte | ( | v16float *& | p,
|  | fifo_state_t & | s,
|  | int | off )

## ◆ fifo_st_flush_conv_1d_byte() [8/22]

void fifo_st_flush_conv_1d_byte | ( | v16int32 *& | p,
|  | fifo_state_t & | s,
|  | int | off )

## ◆ fifo_st_flush_conv_1d_byte() [9/22]

void fifo_st_flush_conv_1d_byte | ( | v16uint32 *& | p,
|  | fifo_state_t & | s,
|  | int | off )

## ◆ fifo_st_flush_conv_1d_byte() [10/22]

void fifo_st_flush_conv_1d_byte | ( | v32bfloat16 *& | p,
|  | fifo_state_t & | s,
|  | int | off )

## ◆ fifo_st_flush_conv_1d_byte() [11/22]

void fifo_st_flush_conv_1d_byte | ( | v32float16 *& | p,
|  | fifo_state_t & | s,
|  | int | off )

## ◆ fifo_st_flush_conv_1d_byte() [12/22]

void fifo_st_flush_conv_1d_byte | ( | v32int16 *& | p,
|  | fifo_state_t & | s,
|  | int | off )

## ◆ fifo_st_flush_conv_1d_byte() [13/22]

void fifo_st_flush_conv_1d_byte | ( | v32uint16 *& | p,
|  | fifo_state_t & | s,
|  | int | off )

## ◆ fifo_st_flush_conv_1d_byte() [14/22]

void fifo_st_flush_conv_1d_byte | ( | v64bfloat8 *& | p,
|  | fifo_state_t & | s,
|  | int | off )

## ◆ fifo_st_flush_conv_1d_byte() [15/22]

void fifo_st_flush_conv_1d_byte | ( | v64float8 *& | p,
|  | fifo_state_t & | s,
|  | int | off )

## ◆ fifo_st_flush_conv_1d_byte() [16/22]

void fifo_st_flush_conv_1d_byte | ( | v64int8 *& | p,
|  | fifo_state_t & | s,
|  | int | off )

## ◆ fifo_st_flush_conv_1d_byte() [17/22]

void fifo_st_flush_conv_1d_byte | ( | v64mx4_unaligned *& | p,
|  | fifo_state_t & | s,
|  | int | off )

## ◆ fifo_st_flush_conv_1d_byte() [18/22]

void fifo_st_flush_conv_1d_byte | ( | v64mx6_unaligned *& | p,
|  | fifo_state_t & | s,
|  | int | off )

## ◆ fifo_st_flush_conv_1d_byte() [19/22]

void fifo_st_flush_conv_1d_byte | ( | v64mx9_unaligned *& | p,
|  | fifo_state_t & | s,
|  | int | off )

## ◆ fifo_st_flush_conv_1d_byte() [20/22]

void fifo_st_flush_conv_1d_byte | ( | v64uint8 *& | p,
|  | fifo_state_t & | s,
|  | int | off )

## ◆ fifo_st_flush_conv_1d_byte() [21/22]

void fifo_st_flush_conv_1d_byte | ( | v8cfloat *& | p,
|  | fifo_state_t & | s,
|  | int | off )

## ◆ fifo_st_flush_conv_1d_byte() [22/22]

void fifo_st_flush_conv_1d_byte | ( | v8cint32 *& | p,
|  | fifo_state_t & | s,
|  | int | off )

## ◆ fifo_st_flush_conv_2d_byte() [1/22]

void fifo_st_flush_conv_2d_byte | ( | v128int4 *& | p,
|  | fifo_state_t & | s,
|  | int | off,
|  | int | size1,
|  | addr_t & | count1,
|  | int | inc1 )

## ◆ fifo_st_flush_conv_2d_byte() [2/22]

void fifo_st_flush_conv_2d_byte | ( | v128mx4_unaligned *& | p,
|  | fifo_state_t & | s,
|  | int | off,
|  | int | size1,
|  | addr_t & | count1,
|  | int | inc1 )

## ◆ fifo_st_flush_conv_2d_byte() [3/22]

void fifo_st_flush_conv_2d_byte | ( | v128mx6_unaligned *& | p,
|  | fifo_state_t & | s,
|  | int | off,
|  | int | size1,
|  | addr_t & | count1,
|  | int | inc1 )

## ◆ fifo_st_flush_conv_2d_byte() [4/22]

void fifo_st_flush_conv_2d_byte | ( | v128uint4 *& | p,
|  | fifo_state_t & | s,
|  | int | off,
|  | int | size1,
|  | addr_t & | count1,
|  | int | inc1 )

## ◆ fifo_st_flush_conv_2d_byte() [5/22]

void fifo_st_flush_conv_2d_byte | ( | v16cbfloat16 *& | p,
|  | fifo_state_t & | s,
|  | int | off,
|  | int | size1,
|  | addr_t & | count1,
|  | int | inc1 )

## ◆ fifo_st_flush_conv_2d_byte() [6/22]

void fifo_st_flush_conv_2d_byte | ( | v16cint16 *& | p,
|  | fifo_state_t & | s,
|  | int | off,
|  | int | size1,
|  | addr_t & | count1,
|  | int | inc1 )

## ◆ fifo_st_flush_conv_2d_byte() [7/22]

void fifo_st_flush_conv_2d_byte | ( | v16float *& | p,
|  | fifo_state_t & | s,
|  | int | off,
|  | int | size1,
|  | addr_t & | count1,
|  | int | inc1 )

## ◆ fifo_st_flush_conv_2d_byte() [8/22]

void fifo_st_flush_conv_2d_byte | ( | v16int32 *& | p,
|  | fifo_state_t & | s,
|  | int | off,
|  | int | size1,
|  | addr_t & | count1,
|  | int | inc1 )

## ◆ fifo_st_flush_conv_2d_byte() [9/22]

void fifo_st_flush_conv_2d_byte | ( | v16uint32 *& | p,
|  | fifo_state_t & | s,
|  | int | off,
|  | int | size1,
|  | addr_t & | count1,
|  | int | inc1 )

## ◆ fifo_st_flush_conv_2d_byte() [10/22]

void fifo_st_flush_conv_2d_byte | ( | v32bfloat16 *& | p,
|  | fifo_state_t & | s,
|  | int | off,
|  | int | size1,
|  | addr_t & | count1,
|  | int | inc1 )

## ◆ fifo_st_flush_conv_2d_byte() [11/22]

void fifo_st_flush_conv_2d_byte | ( | v32float16 *& | p,
|  | fifo_state_t & | s,
|  | int | off,
|  | int | size1,
|  | addr_t & | count1,
|  | int | inc1 )

## ◆ fifo_st_flush_conv_2d_byte() [12/22]

void fifo_st_flush_conv_2d_byte | ( | v32int16 *& | p,
|  | fifo_state_t & | s,
|  | int | off,
|  | int | size1,
|  | addr_t & | count1,
|  | int | inc1 )

## ◆ fifo_st_flush_conv_2d_byte() [13/22]

void fifo_st_flush_conv_2d_byte | ( | v32uint16 *& | p,
|  | fifo_state_t & | s,
|  | int | off,
|  | int | size1,
|  | addr_t & | count1,
|  | int | inc1 )

## ◆ fifo_st_flush_conv_2d_byte() [14/22]

void fifo_st_flush_conv_2d_byte | ( | v64bfloat8 *& | p,
|  | fifo_state_t & | s,
|  | int | off,
|  | int | size1,
|  | addr_t & | count1,
|  | int | inc1 )

## ◆ fifo_st_flush_conv_2d_byte() [15/22]

void fifo_st_flush_conv_2d_byte | ( | v64float8 *& | p,
|  | fifo_state_t & | s,
|  | int | off,
|  | int | size1,
|  | addr_t & | count1,
|  | int | inc1 )

## ◆ fifo_st_flush_conv_2d_byte() [16/22]

void fifo_st_flush_conv_2d_byte | ( | v64int8 *& | p,
|  | fifo_state_t & | s,
|  | int | off,
|  | int | size1,
|  | addr_t & | count1,
|  | int | inc1 )

## ◆ fifo_st_flush_conv_2d_byte() [17/22]

void fifo_st_flush_conv_2d_byte | ( | v64mx4_unaligned *& | p,
|  | fifo_state_t & | s,
|  | int | off,
|  | int | size1,
|  | addr_t & | count1,
|  | int | inc1 )

## ◆ fifo_st_flush_conv_2d_byte() [18/22]

void fifo_st_flush_conv_2d_byte | ( | v64mx6_unaligned *& | p,
|  | fifo_state_t & | s,
|  | int | off,
|  | int | size1,
|  | addr_t & | count1,
|  | int | inc1 )

## ◆ fifo_st_flush_conv_2d_byte() [19/22]

void fifo_st_flush_conv_2d_byte | ( | v64mx9_unaligned *& | p,
|  | fifo_state_t & | s,
|  | int | off,
|  | int | size1,
|  | addr_t & | count1,
|  | int | inc1 )

## ◆ fifo_st_flush_conv_2d_byte() [20/22]

void fifo_st_flush_conv_2d_byte | ( | v64uint8 *& | p,
|  | fifo_state_t & | s,
|  | int | off,
|  | int | size1,
|  | addr_t & | count1,
|  | int | inc1 )

## ◆ fifo_st_flush_conv_2d_byte() [21/22]

void fifo_st_flush_conv_2d_byte | ( | v8cfloat *& | p,
|  | fifo_state_t & | s,
|  | int | off,
|  | int | size1,
|  | addr_t & | count1,
|  | int | inc1 )

## ◆ fifo_st_flush_conv_2d_byte() [22/22]

void fifo_st_flush_conv_2d_byte | ( | v8cint32 *& | p,
|  | fifo_state_t & | s,
|  | int | off,
|  | int | size1,
|  | addr_t & | count1,
|  | int | inc1 )

## ◆ fifo_st_flush_conv_3d_byte() [1/22]

void fifo_st_flush_conv_3d_byte | ( | v128int4 *& | p,
|  | fifo_state_t & | s,
|  | int | off,
|  | int | size1,
|  | addr_t & | count1,
|  | int | inc1,
|  | int | size2,
|  | addr_t & | count2,
|  | int | inc2 )

## ◆ fifo_st_flush_conv_3d_byte() [2/22]

void fifo_st_flush_conv_3d_byte | ( | v128mx4_unaligned *& | p,
|  | fifo_state_t & | s,
|  | int | off,
|  | int | size1,
|  | addr_t & | count1,
|  | int | inc1,
|  | int | size2,
|  | addr_t & | count2,
|  | int | inc2 )

## ◆ fifo_st_flush_conv_3d_byte() [3/22]

void fifo_st_flush_conv_3d_byte | ( | v128mx6_unaligned *& | p,
|  | fifo_state_t & | s,
|  | int | off,
|  | int | size1,
|  | addr_t & | count1,
|  | int | inc1,
|  | int | size2,
|  | addr_t & | count2,
|  | int | inc2 )

## ◆ fifo_st_flush_conv_3d_byte() [4/22]

void fifo_st_flush_conv_3d_byte | ( | v128uint4 *& | p,
|  | fifo_state_t & | s,
|  | int | off,
|  | int | size1,
|  | addr_t & | count1,
|  | int | inc1,
|  | int | size2,
|  | addr_t & | count2,
|  | int | inc2 )

## ◆ fifo_st_flush_conv_3d_byte() [5/22]

void fifo_st_flush_conv_3d_byte | ( | v16cbfloat16 *& | p,
|  | fifo_state_t & | s,
|  | int | off,
|  | int | size1,
|  | addr_t & | count1,
|  | int | inc1,
|  | int | size2,
|  | addr_t & | count2,
|  | int | inc2 )

## ◆ fifo_st_flush_conv_3d_byte() [6/22]

void fifo_st_flush_conv_3d_byte | ( | v16cint16 *& | p,
|  | fifo_state_t & | s,
|  | int | off,
|  | int | size1,
|  | addr_t & | count1,
|  | int | inc1,
|  | int | size2,
|  | addr_t & | count2,
|  | int | inc2 )

## ◆ fifo_st_flush_conv_3d_byte() [7/22]

void fifo_st_flush_conv_3d_byte | ( | v16float *& | p,
|  | fifo_state_t & | s,
|  | int | off,
|  | int | size1,
|  | addr_t & | count1,
|  | int | inc1,
|  | int | size2,
|  | addr_t & | count2,
|  | int | inc2 )

## ◆ fifo_st_flush_conv_3d_byte() [8/22]

void fifo_st_flush_conv_3d_byte | ( | v16int32 *& | p,
|  | fifo_state_t & | s,
|  | int | off,
|  | int | size1,
|  | addr_t & | count1,
|  | int | inc1,
|  | int | size2,
|  | addr_t & | count2,
|  | int | inc2 )

## ◆ fifo_st_flush_conv_3d_byte() [9/22]

void fifo_st_flush_conv_3d_byte | ( | v16uint32 *& | p,
|  | fifo_state_t & | s,
|  | int | off,
|  | int | size1,
|  | addr_t & | count1,
|  | int | inc1,
|  | int | size2,
|  | addr_t & | count2,
|  | int | inc2 )

## ◆ fifo_st_flush_conv_3d_byte() [10/22]

void fifo_st_flush_conv_3d_byte | ( | v32bfloat16 *& | p,
|  | fifo_state_t & | s,
|  | int | off,
|  | int | size1,
|  | addr_t & | count1,
|  | int | inc1,
|  | int | size2,
|  | addr_t & | count2,
|  | int | inc2 )

## ◆ fifo_st_flush_conv_3d_byte() [11/22]

void fifo_st_flush_conv_3d_byte | ( | v32float16 *& | p,
|  | fifo_state_t & | s,
|  | int | off,
|  | int | size1,
|  | addr_t & | count1,
|  | int | inc1,
|  | int | size2,
|  | addr_t & | count2,
|  | int | inc2 )

## ◆ fifo_st_flush_conv_3d_byte() [12/22]

void fifo_st_flush_conv_3d_byte | ( | v32int16 *& | p,
|  | fifo_state_t & | s,
|  | int | off,
|  | int | size1,
|  | addr_t & | count1,
|  | int | inc1,
|  | int | size2,
|  | addr_t & | count2,
|  | int | inc2 )

## ◆ fifo_st_flush_conv_3d_byte() [13/22]

void fifo_st_flush_conv_3d_byte | ( | v32uint16 *& | p,
|  | fifo_state_t & | s,
|  | int | off,
|  | int | size1,
|  | addr_t & | count1,
|  | int | inc1,
|  | int | size2,
|  | addr_t & | count2,
|  | int | inc2 )

## ◆ fifo_st_flush_conv_3d_byte() [14/22]

void fifo_st_flush_conv_3d_byte | ( | v64bfloat8 *& | p,
|  | fifo_state_t & | s,
|  | int | off,
|  | int | size1,
|  | addr_t & | count1,
|  | int | inc1,
|  | int | size2,
|  | addr_t & | count2,
|  | int | inc2 )

## ◆ fifo_st_flush_conv_3d_byte() [15/22]

void fifo_st_flush_conv_3d_byte | ( | v64float8 *& | p,
|  | fifo_state_t & | s,
|  | int | off,
|  | int | size1,
|  | addr_t & | count1,
|  | int | inc1,
|  | int | size2,
|  | addr_t & | count2,
|  | int | inc2 )

## ◆ fifo_st_flush_conv_3d_byte() [16/22]

void fifo_st_flush_conv_3d_byte | ( | v64int8 *& | p,
|  | fifo_state_t & | s,
|  | int | off,
|  | int | size1,
|  | addr_t & | count1,
|  | int | inc1,
|  | int | size2,
|  | addr_t & | count2,
|  | int | inc2 )

## ◆ fifo_st_flush_conv_3d_byte() [17/22]

void fifo_st_flush_conv_3d_byte | ( | v64mx4_unaligned *& | p,
|  | fifo_state_t & | s,
|  | int | off,
|  | int | size1,
|  | addr_t & | count1,
|  | int | inc1,
|  | int | size2,
|  | addr_t & | count2,
|  | int | inc2 )

## ◆ fifo_st_flush_conv_3d_byte() [18/22]

void fifo_st_flush_conv_3d_byte | ( | v64mx6_unaligned *& | p,
|  | fifo_state_t & | s,
|  | int | off,
|  | int | size1,
|  | addr_t & | count1,
|  | int | inc1,
|  | int | size2,
|  | addr_t & | count2,
|  | int | inc2 )

## ◆ fifo_st_flush_conv_3d_byte() [19/22]

void fifo_st_flush_conv_3d_byte | ( | v64mx9_unaligned *& | p,
|  | fifo_state_t & | s,
|  | int | off,
|  | int | size1,
|  | addr_t & | count1,
|  | int | inc1,
|  | int | size2,
|  | addr_t & | count2,
|  | int | inc2 )

## ◆ fifo_st_flush_conv_3d_byte() [20/22]

void fifo_st_flush_conv_3d_byte | ( | v64uint8 *& | p,
|  | fifo_state_t & | s,
|  | int | off,
|  | int | size1,
|  | addr_t & | count1,
|  | int | inc1,
|  | int | size2,
|  | addr_t & | count2,
|  | int | inc2 )

## ◆ fifo_st_flush_conv_3d_byte() [21/22]

void fifo_st_flush_conv_3d_byte | ( | v8cfloat *& | p,
|  | fifo_state_t & | s,
|  | int | off,
|  | int | size1,
|  | addr_t & | count1,
|  | int | inc1,
|  | int | size2,
|  | addr_t & | count2,
|  | int | inc2 )

## ◆ fifo_st_flush_conv_3d_byte() [22/22]

void fifo_st_flush_conv_3d_byte | ( | v8cint32 *& | p,
|  | fifo_state_t & | s,
|  | int | off,
|  | int | size1,
|  | addr_t & | count1,
|  | int | inc1,
|  | int | size2,
|  | addr_t & | count2,
|  | int | inc2 )

## ◆ fifo_st_push() [1/22]

void fifo_st_push | ( | v128int4 *& | p,
|  | v128int4 | v,
|  | fifo_state_t & | s )

## ◆ fifo_st_push() [2/22]

void fifo_st_push | ( | v128mx4_unaligned *& | p,
|  | v128mx4 | v,
|  | fifo_state_t & | s )

## ◆ fifo_st_push() [3/22]

void fifo_st_push | ( | v128mx6_unaligned *& | p,
|  | v128mx6 | v,
|  | fifo_state_t & | s )

## ◆ fifo_st_push() [4/22]

void fifo_st_push | ( | v128uint4 *& | p,
|  | v128uint4 | v,
|  | fifo_state_t & | s )

## ◆ fifo_st_push() [5/22]

void fifo_st_push | ( | v16cbfloat16 *& | p,
|  | v16cbfloat16 | v,
|  | fifo_state_t & | s )

## ◆ fifo_st_push() [6/22]

void fifo_st_push | ( | v16cint16 *& | p,
|  | v16cint16 | v,
|  | fifo_state_t & | s )

## ◆ fifo_st_push() [7/22]

void fifo_st_push | ( | v16float *& | p,
|  | v16float | v,
|  | fifo_state_t & | s )

## ◆ fifo_st_push() [8/22]

void fifo_st_push | ( | v16int32 *& | p,
|  | v16int32 | v,
|  | fifo_state_t & | s )

## ◆ fifo_st_push() [9/22]

void fifo_st_push | ( | v16uint32 *& | p,
|  | v16uint32 | v,
|  | fifo_state_t & | s )

## ◆ fifo_st_push() [10/22]

void fifo_st_push | ( | v32bfloat16 *& | p,
|  | v32bfloat16 | v,
|  | fifo_state_t & | s )

## ◆ fifo_st_push() [11/22]

void fifo_st_push | ( | v32float16 *& | p,
|  | v32float16 | v,
|  | fifo_state_t & | s )

## ◆ fifo_st_push() [12/22]

void fifo_st_push | ( | v32int16 *& | p,
|  | v32int16 | v,
|  | fifo_state_t & | s )

## ◆ fifo_st_push() [13/22]

void fifo_st_push | ( | v32uint16 *& | p,
|  | v32uint16 | v,
|  | fifo_state_t & | s )

## ◆ fifo_st_push() [14/22]

void fifo_st_push | ( | v64bfloat8 *& | p,
|  | v64bfloat8 | v,
|  | fifo_state_t & | s )

## ◆ fifo_st_push() [15/22]

void fifo_st_push | ( | v64float8 *& | p,
|  | v64float8 | v,
|  | fifo_state_t & | s )

## ◆ fifo_st_push() [16/22]

void fifo_st_push | ( | v64int8 *& | p,
|  | v64int8 | v,
|  | fifo_state_t & | s )

## ◆ fifo_st_push() [17/22]

void fifo_st_push | ( | v64mx4_unaligned *& | p,
|  | v64mx4 | v,
|  | fifo_state_t & | s )

## ◆ fifo_st_push() [18/22]

void fifo_st_push | ( | v64mx6_unaligned *& | p,
|  | v64mx6 | v,
|  | fifo_state_t & | s )

## ◆ fifo_st_push() [19/22]

void fifo_st_push | ( | v64mx9_unaligned *& | p,
|  | v64mx9 | v,
|  | fifo_state_t & | s )

## ◆ fifo_st_push() [20/22]

void fifo_st_push | ( | v64uint8 *& | p,
|  | v64uint8 | v,
|  | fifo_state_t & | s )

## ◆ fifo_st_push() [21/22]

void fifo_st_push | ( | v8cfloat *& | p,
|  | v8cfloat | v,
|  | fifo_state_t & | s )

## ◆ fifo_st_push() [22/22]

void fifo_st_push | ( | v8cint32 *& | p,
|  | v8cint32 | v,
|  | fifo_state_t & | s )

## ◆ fifo_st_reset() [1/44]

void fifo_st_reset | ( | v128int4 *& | p,
|  | v128int4 | v,
|  | fifo_state_t & | s )

## ◆ fifo_st_reset() [2/44]

void fifo_st_reset | ( | v128int4 * | p,
|  | v128int4 | v,
|  | v128int4 *& | p_o,
|  | sparse_fifo_t & | fifo_o,
|  | int & | pos_o )

## ◆ fifo_st_reset() [3/44]

void fifo_st_reset | ( | v128mx4_unaligned *& | p,
|  | v128mx4 | v,
|  | fifo_state_t & | s )

## ◆ fifo_st_reset() [4/44]

void fifo_st_reset | ( | v128mx4_unaligned * | p,
|  | v128mx4 | v,
|  | v128mx4_unaligned *& | p_o,
|  | sparse_fifo_t & | fifo_o,
|  | int & | pos_o )

## ◆ fifo_st_reset() [5/44]

void fifo_st_reset | ( | v128mx6_unaligned *& | p,
|  | v128mx6 | v,
|  | fifo_state_t & | s )

## ◆ fifo_st_reset() [6/44]

void fifo_st_reset | ( | v128mx6_unaligned * | p,
|  | v128mx6 | v,
|  | v128mx6_unaligned *& | p_o,
|  | sparse_fifo_t & | fifo_o,
|  | int & | pos_o )

## ◆ fifo_st_reset() [7/44]

void fifo_st_reset | ( | v128uint4 *& | p,
|  | v128uint4 | v,
|  | fifo_state_t & | s )

## ◆ fifo_st_reset() [8/44]

void fifo_st_reset | ( | v128uint4 * | p,
|  | v128uint4 | v,
|  | v128uint4 *& | p_o,
|  | sparse_fifo_t & | fifo_o,
|  | int & | pos_o )

## ◆ fifo_st_reset() [9/44]

void fifo_st_reset | ( | v16cbfloat16 *& | p,
|  | v16cbfloat16 | v,
|  | fifo_state_t & | s )

## ◆ fifo_st_reset() [10/44]

void fifo_st_reset | ( | v16cbfloat16 * | p,
|  | v16cbfloat16 | v,
|  | v16cbfloat16 *& | p_o,
|  | sparse_fifo_t & | fifo_o,
|  | int & | pos_o )

## ◆ fifo_st_reset() [11/44]

void fifo_st_reset | ( | v16cint16 *& | p,
|  | v16cint16 | v,
|  | fifo_state_t & | s )

## ◆ fifo_st_reset() [12/44]

void fifo_st_reset | ( | v16cint16 * | p,
|  | v16cint16 | v,
|  | v16cint16 *& | p_o,
|  | sparse_fifo_t & | fifo_o,
|  | int & | pos_o )

## ◆ fifo_st_reset() [13/44]

void fifo_st_reset | ( | v16float *& | p,
|  | v16float | v,
|  | fifo_state_t & | s )

## ◆ fifo_st_reset() [14/44]

void fifo_st_reset | ( | v16float * | p,
|  | v16float | v,
|  | v16float *& | p_o,
|  | sparse_fifo_t & | fifo_o,
|  | int & | pos_o )

## ◆ fifo_st_reset() [15/44]

void fifo_st_reset | ( | v16int32 *& | p,
|  | v16int32 | v,
|  | fifo_state_t & | s )

## ◆ fifo_st_reset() [16/44]

void fifo_st_reset | ( | v16int32 * | p,
|  | v16int32 | v,
|  | v16int32 *& | p_o,
|  | sparse_fifo_t & | fifo_o,
|  | int & | pos_o )

## ◆ fifo_st_reset() [17/44]

void fifo_st_reset | ( | v16uint32 *& | p,
|  | v16uint32 | v,
|  | fifo_state_t & | s )

## ◆ fifo_st_reset() [18/44]

void fifo_st_reset | ( | v16uint32 * | p,
|  | v16uint32 | v,
|  | v16uint32 *& | p_o,
|  | sparse_fifo_t & | fifo_o,
|  | int & | pos_o )

## ◆ fifo_st_reset() [19/44]

void fifo_st_reset | ( | v32bfloat16 *& | p,
|  | v32bfloat16 | v,
|  | fifo_state_t & | s )

## ◆ fifo_st_reset() [20/44]

void fifo_st_reset | ( | v32bfloat16 * | p,
|  | v32bfloat16 | v,
|  | v32bfloat16 *& | p_o,
|  | sparse_fifo_t & | fifo_o,
|  | int & | pos_o )

## ◆ fifo_st_reset() [21/44]

void fifo_st_reset | ( | v32float16 *& | p,
|  | v32float16 | v,
|  | fifo_state_t & | s )

## ◆ fifo_st_reset() [22/44]

void fifo_st_reset | ( | v32float16 * | p,
|  | v32float16 | v,
|  | v32float16 *& | p_o,
|  | sparse_fifo_t & | fifo_o,
|  | int & | pos_o )

## ◆ fifo_st_reset() [23/44]

void fifo_st_reset | ( | v32int16 *& | p,
|  | v32int16 | v,
|  | fifo_state_t & | s )

## ◆ fifo_st_reset() [24/44]

void fifo_st_reset | ( | v32int16 * | p,
|  | v32int16 | v,
|  | v32int16 *& | p_o,
|  | sparse_fifo_t & | fifo_o,
|  | int & | pos_o )

## ◆ fifo_st_reset() [25/44]

void fifo_st_reset | ( | v32uint16 *& | p,
|  | v32uint16 | v,
|  | fifo_state_t & | s )

## ◆ fifo_st_reset() [26/44]

void fifo_st_reset | ( | v32uint16 * | p,
|  | v32uint16 | v,
|  | v32uint16 *& | p_o,
|  | sparse_fifo_t & | fifo_o,
|  | int & | pos_o )

## ◆ fifo_st_reset() [27/44]

void fifo_st_reset | ( | v64bfloat8 *& | p,
|  | v64bfloat8 | v,
|  | fifo_state_t & | s )

## ◆ fifo_st_reset() [28/44]

void fifo_st_reset | ( | v64bfloat8 * | p,
|  | v64bfloat8 | v,
|  | v64bfloat8 *& | p_o,
|  | sparse_fifo_t & | fifo_o,
|  | int & | pos_o )

## ◆ fifo_st_reset() [29/44]

void fifo_st_reset | ( | v64float8 *& | p,
|  | v64float8 | v,
|  | fifo_state_t & | s )

## ◆ fifo_st_reset() [30/44]

void fifo_st_reset | ( | v64float8 * | p,
|  | v64float8 | v,
|  | v64float8 *& | p_o,
|  | sparse_fifo_t & | fifo_o,
|  | int & | pos_o )

## ◆ fifo_st_reset() [31/44]

void fifo_st_reset | ( | v64int8 *& | p,
|  | v64int8 | v,
|  | fifo_state_t & | s )

## ◆ fifo_st_reset() [32/44]

void fifo_st_reset | ( | v64int8 * | p,
|  | v64int8 | v,
|  | v64int8 *& | p_o,
|  | sparse_fifo_t & | fifo_o,
|  | int & | pos_o )

## ◆ fifo_st_reset() [33/44]

void fifo_st_reset | ( | v64mx4_unaligned *& | p,
|  | v64mx4 | v,
|  | fifo_state_t & | s )

## ◆ fifo_st_reset() [34/44]

void fifo_st_reset | ( | v64mx4_unaligned * | p,
|  | v64mx4 | v,
|  | v64mx4_unaligned *& | p_o,
|  | sparse_fifo_t & | fifo_o,
|  | int & | pos_o )

## ◆ fifo_st_reset() [35/44]

void fifo_st_reset | ( | v64mx6_unaligned *& | p,
|  | v64mx6 | v,
|  | fifo_state_t & | s )

## ◆ fifo_st_reset() [36/44]

void fifo_st_reset | ( | v64mx6_unaligned * | p,
|  | v64mx6 | v,
|  | v64mx6_unaligned *& | p_o,
|  | sparse_fifo_t & | fifo_o,
|  | int & | pos_o )

## ◆ fifo_st_reset() [37/44]

void fifo_st_reset | ( | v64mx9_unaligned *& | p,
|  | v64mx9 | v,
|  | fifo_state_t & | s )

## ◆ fifo_st_reset() [38/44]

void fifo_st_reset | ( | v64mx9_unaligned * | p,
|  | v64mx9 | v,
|  | v64mx9_unaligned *& | p_o,
|  | sparse_fifo_t & | fifo_o,
|  | int & | pos_o )

## ◆ fifo_st_reset() [39/44]

void fifo_st_reset | ( | v64uint8 *& | p,
|  | v64uint8 | v,
|  | fifo_state_t & | s )

## ◆ fifo_st_reset() [40/44]

void fifo_st_reset | ( | v64uint8 * | p,
|  | v64uint8 | v,
|  | v64uint8 *& | p_o,
|  | sparse_fifo_t & | fifo_o,
|  | int & | pos_o )

## ◆ fifo_st_reset() [41/44]

void fifo_st_reset | ( | v8cfloat *& | p,
|  | v8cfloat | v,
|  | fifo_state_t & | s )

## ◆ fifo_st_reset() [42/44]

void fifo_st_reset | ( | v8cfloat * | p,
|  | v8cfloat | v,
|  | v8cfloat *& | p_o,
|  | sparse_fifo_t & | fifo_o,
|  | int & | pos_o )

## ◆ fifo_st_reset() [43/44]

void fifo_st_reset | ( | v8cint32 *& | p,
|  | v8cint32 | v,
|  | fifo_state_t & | s )

## ◆ fifo_st_reset() [44/44]

void fifo_st_reset | ( | v8cint32 * | p,
|  | v8cint32 | v,
|  | v8cint32 *& | p_o,
|  | sparse_fifo_t & | fifo_o,
|  | int & | pos_o )