| AI Engine Intrinsics User Guide (v2026.1)

Loading...
Searching...
No Matches
Topics | Functions
Addressing Operations
Intrinsics » Scalar Operations

## Overview

Addressing mode intrinsics.

## Topics
| Cyclic Addressing
| FFT Addressing

## Functions
template<class T>
T * | byte_incr (T *p, int i)
| Increments input pointer by a number of bytes.

## Initialization functions for scalars
mod_t | undef_mod ()
umod_t | undef_umod ()
unsigned int | undef_uint ()
float | undef_float ()

## Function Documentation

## ◆ byte_incr()

template<class T>

T * byte_incr | ( | T * | p,
|  | int | i )

Increments input pointer by a number of bytes.

Parameters

  p | Input pointer.
  i | The amount of bytes to increment by.

Returns input pointer p incremented by i.

## ◆ undef_float()

float undef_float | ( |  | ) |

## ◆ undef_mod()

mod_t undef_mod | ( |  | ) |

## ◆ undef_uint()

unsigned int undef_uint | ( |  | ) |

## ◆ undef_umod()

umod_t undef_umod | ( |  | ) |