| AI Engine-ML v2 Intrinsics User Guide (v2026.1)

Loading...
Searching...
No Matches
Multiply-accumulate of 16b x 16b integer datatypes
Vector Operations » Multiply Accumulate

## 8x2_2x8
v64acc32 | mul_8x2_2x8 (v32uint16 a, v32uint16 b)
v64acc32 | negmul_8x2_2x8 (v32uint16 a, v32uint16 b)
v64acc32 | mac_8x2_2x8 (v32uint16 a, v32uint16 b, v64acc32 acc)
v64acc32 | msc_8x2_2x8 (v32uint16 a, v32uint16 b, v64acc32 acc)
v64acc32 | addmac_8x2_2x8 (v32uint16 a, v32uint16 b, v64acc32 acc1, v64acc32 acc2)
v64acc32 | addmsc_8x2_2x8 (v32uint16 a, v32uint16 b, v64acc32 acc1, v64acc32 acc2)
v64acc32 | mul_8x2_2x8 (v32uint16 a, v32int16 b)
v64acc32 | negmul_8x2_2x8 (v32uint16 a, v32int16 b)
v64acc32 | mac_8x2_2x8 (v32uint16 a, v32int16 b, v64acc32 acc)
v64acc32 | msc_8x2_2x8 (v32uint16 a, v32int16 b, v64acc32 acc)
v64acc32 | addmac_8x2_2x8 (v32uint16 a, v32int16 b, v64acc32 acc1, v64acc32 acc2)
v64acc32 | addmsc_8x2_2x8 (v32uint16 a, v32int16 b, v64acc32 acc1, v64acc32 acc2)
v64acc32 | mul_8x2_2x8 (v32int16 a, v32uint16 b)
v64acc32 | negmul_8x2_2x8 (v32int16 a, v32uint16 b)
v64acc32 | mac_8x2_2x8 (v32int16 a, v32uint16 b, v64acc32 acc)
v64acc32 | msc_8x2_2x8 (v32int16 a, v32uint16 b, v64acc32 acc)
v64acc32 | addmac_8x2_2x8 (v32int16 a, v32uint16 b, v64acc32 acc1, v64acc32 acc2)
v64acc32 | addmsc_8x2_2x8 (v32int16 a, v32uint16 b, v64acc32 acc1, v64acc32 acc2)
v64acc32 | mul_8x2_2x8 (v32int16 a, v32int16 b)
v64acc32 | negmul_8x2_2x8 (v32int16 a, v32int16 b)
v64acc32 | mac_8x2_2x8 (v32int16 a, v32int16 b, v64acc32 acc)
v64acc32 | msc_8x2_2x8 (v32int16 a, v32int16 b, v64acc32 acc)
v64acc32 | addmac_8x2_2x8 (v32int16 a, v32int16 b, v64acc32 acc1, v64acc32 acc2)
v64acc32 | addmsc_8x2_2x8 (v32int16 a, v32int16 b, v64acc32 acc1, v64acc32 acc2)

## 8x2_2x8 with dynamic sign
v64acc32 | mul_8x2_2x8 (v32uint16 a, int sgn_x, v32uint16 b, int sgn_y)
v64acc32 | negmul_8x2_2x8 (v32uint16 a, int sgn_x, v32uint16 b, int sgn_y)
v64acc32 | mac_8x2_2x8 (v32uint16 a, int sgn_x, v32uint16 b, int sgn_y, v64acc32 acc)
v64acc32 | msc_8x2_2x8 (v32uint16 a, int sgn_x, v32uint16 b, int sgn_y, v64acc32 acc)
v64acc32 | addmac_8x2_2x8 (v32uint16 a, int sgn_x, v32uint16 b, int sgn_y, v64acc32 acc1, v64acc32 acc2)
v64acc32 | addmsc_8x2_2x8 (v32uint16 a, int sgn_x, v32uint16 b, int sgn_y, v64acc32 acc1, v64acc32 acc2)
v64acc32 | mul_8x2_2x8 (v32uint16 a, int sgn_x, v32int16 b, int sgn_y)
v64acc32 | negmul_8x2_2x8 (v32uint16 a, int sgn_x, v32int16 b, int sgn_y)
v64acc32 | mac_8x2_2x8 (v32uint16 a, int sgn_x, v32int16 b, int sgn_y, v64acc32 acc)
v64acc32 | msc_8x2_2x8 (v32uint16 a, int sgn_x, v32int16 b, int sgn_y, v64acc32 acc)
v64acc32 | addmac_8x2_2x8 (v32uint16 a, int sgn_x, v32int16 b, int sgn_y, v64acc32 acc1, v64acc32 acc2)
v64acc32 | addmsc_8x2_2x8 (v32uint16 a, int sgn_x, v32int16 b, int sgn_y, v64acc32 acc1, v64acc32 acc2)
v64acc32 | mul_8x2_2x8 (v32int16 a, int sgn_x, v32uint16 b, int sgn_y)
v64acc32 | negmul_8x2_2x8 (v32int16 a, int sgn_x, v32uint16 b, int sgn_y)
v64acc32 | mac_8x2_2x8 (v32int16 a, int sgn_x, v32uint16 b, int sgn_y, v64acc32 acc)
v64acc32 | msc_8x2_2x8 (v32int16 a, int sgn_x, v32uint16 b, int sgn_y, v64acc32 acc)
v64acc32 | addmac_8x2_2x8 (v32int16 a, int sgn_x, v32uint16 b, int sgn_y, v64acc32 acc1, v64acc32 acc2)
v64acc32 | addmsc_8x2_2x8 (v32int16 a, int sgn_x, v32uint16 b, int sgn_y, v64acc32 acc1, v64acc32 acc2)
v64acc32 | mul_8x2_2x8 (v32int16 a, int sgn_x, v32int16 b, int sgn_y)
v64acc32 | negmul_8x2_2x8 (v32int16 a, int sgn_x, v32int16 b, int sgn_y)
v64acc32 | mac_8x2_2x8 (v32int16 a, int sgn_x, v32int16 b, int sgn_y, v64acc32 acc)
v64acc32 | msc_8x2_2x8 (v32int16 a, int sgn_x, v32int16 b, int sgn_y, v64acc32 acc)
v64acc32 | addmac_8x2_2x8 (v32int16 a, int sgn_x, v32int16 b, int sgn_y, v64acc32 acc1, v64acc32 acc2)
v64acc32 | addmsc_8x2_2x8 (v32int16 a, int sgn_x, v32int16 b, int sgn_y, v64acc32 acc1, v64acc32 acc2)

## 8x2_2x8 with dynamic negation of multiplication result
v64acc32 | mul_8x2_2x8_conf (v32uint16 a, v32uint16 b, int sub_mul)
v64acc32 | negmul_8x2_2x8_conf (v32uint16 a, v32uint16 b, int sub_mul)
v64acc32 | mul_8x2_2x8_conf (v32uint16 a, v32int16 b, int sub_mul)
v64acc32 | negmul_8x2_2x8_conf (v32uint16 a, v32int16 b, int sub_mul)
v64acc32 | mul_8x2_2x8_conf (v32int16 a, v32uint16 b, int sub_mul)
v64acc32 | negmul_8x2_2x8_conf (v32int16 a, v32uint16 b, int sub_mul)
v64acc32 | mul_8x2_2x8_conf (v32int16 a, v32int16 b, int sub_mul)
v64acc32 | negmul_8x2_2x8_conf (v32int16 a, v32int16 b, int sub_mul)

## 8x2_2x8 with dynamic negation of multiplication result, zeroing of acc1, negation of acc1
v64acc32 | mac_8x2_2x8_conf (v32uint16 a, v32uint16 b, v64acc32 acc, int zero_acc, int shift16, int sub_mul, int sub_acc1)
v64acc32 | msc_8x2_2x8_conf (v32uint16 a, v32uint16 b, v64acc32 acc, int zero_acc, int shift16, int sub_mul, int sub_acc1)
v64acc32 | addmac_8x2_2x8_conf (v32uint16 a, v32uint16 b, v64acc32 acc1, v64acc32 acc2, int zero_acc1, int shift16, int sub_mul, int sub_acc1, int sub_acc2)
v64acc32 | addmsc_8x2_2x8_conf (v32uint16 a, v32uint16 b, v64acc32 acc1, v64acc32 acc2, int zero_acc1, int shift16, int sub_mul, int sub_acc1, int sub_acc2)
v64acc32 | mac_8x2_2x8_conf (v32uint16 a, v32int16 b, v64acc32 acc, int zero_acc, int shift16, int sub_mul, int sub_acc1)
v64acc32 | msc_8x2_2x8_conf (v32uint16 a, v32int16 b, v64acc32 acc, int zero_acc, int shift16, int sub_mul, int sub_acc1)
v64acc32 | addmac_8x2_2x8_conf (v32uint16 a, v32int16 b, v64acc32 acc1, v64acc32 acc2, int zero_acc1, int shift16, int sub_mul, int sub_acc1, int sub_acc2)
v64acc32 | addmsc_8x2_2x8_conf (v32uint16 a, v32int16 b, v64acc32 acc1, v64acc32 acc2, int zero_acc1, int shift16, int sub_mul, int sub_acc1, int sub_acc2)
v64acc32 | mac_8x2_2x8_conf (v32int16 a, v32uint16 b, v64acc32 acc, int zero_acc, int shift16, int sub_mul, int sub_acc1)
v64acc32 | msc_8x2_2x8_conf (v32int16 a, v32uint16 b, v64acc32 acc, int zero_acc, int shift16, int sub_mul, int sub_acc1)
v64acc32 | addmac_8x2_2x8_conf (v32int16 a, v32uint16 b, v64acc32 acc1, v64acc32 acc2, int zero_acc1, int shift16, int sub_mul, int sub_acc1, int sub_acc2)
v64acc32 | addmsc_8x2_2x8_conf (v32int16 a, v32uint16 b, v64acc32 acc1, v64acc32 acc2, int zero_acc1, int shift16, int sub_mul, int sub_acc1, int sub_acc2)
v64acc32 | mac_8x2_2x8_conf (v32int16 a, v32int16 b, v64acc32 acc, int zero_acc, int shift16, int sub_mul, int sub_acc1)
v64acc32 | msc_8x2_2x8_conf (v32int16 a, v32int16 b, v64acc32 acc, int zero_acc, int shift16, int sub_mul, int sub_acc1)
v64acc32 | addmac_8x2_2x8_conf (v32int16 a, v32int16 b, v64acc32 acc1, v64acc32 acc2, int zero_acc1, int shift16, int sub_mul, int sub_acc1, int sub_acc2)
v64acc32 | addmsc_8x2_2x8_conf (v32int16 a, v32int16 b, v64acc32 acc1, v64acc32 acc2, int zero_acc1, int shift16, int sub_mul, int sub_acc1, int sub_acc2)

## 8x2_2x8 with dynamic sign and dynamic negation of multiplication result
v64acc32 | mul_8x2_2x8_conf (v32uint16 a, int sgn_x, v32uint16 b, int sgn_y, int sub_mul)
v64acc32 | negmul_8x2_2x8_conf (v32uint16 a, int sgn_x, v32uint16 b, int sgn_y, int sub_mul)
v64acc32 | mac_8x2_2x8_conf (v32uint16 a, int sgn_x, v32uint16 b, int sgn_y, v64acc32 acc, int zero_acc, int shift16, int sub_mul, int sub_acc1)
v64acc32 | msc_8x2_2x8_conf (v32uint16 a, int sgn_x, v32uint16 b, int sgn_y, v64acc32 acc, int zero_acc, int shift16, int sub_mul, int sub_acc1)
v64acc32 | addmac_8x2_2x8_conf (v32uint16 a, int sgn_x, v32uint16 b, int sgn_y, v64acc32 acc1, v64acc32 acc2, int zero_acc1, int shift16, int sub_mul, int sub_acc1, int sub_acc2)
v64acc32 | addmsc_8x2_2x8_conf (v32uint16 a, int sgn_x, v32uint16 b, int sgn_y, v64acc32 acc1, v64acc32 acc2, int zero_acc1, int shift16, int sub_mul, int sub_acc1, int sub_acc2)
v64acc32 | mul_8x2_2x8_conf (v32uint16 a, int sgn_x, v32int16 b, int sgn_y, int sub_mul)
v64acc32 | negmul_8x2_2x8_conf (v32uint16 a, int sgn_x, v32int16 b, int sgn_y, int sub_mul)
v64acc32 | mac_8x2_2x8_conf (v32uint16 a, int sgn_x, v32int16 b, int sgn_y, v64acc32 acc, int zero_acc, int shift16, int sub_mul, int sub_acc1)
v64acc32 | msc_8x2_2x8_conf (v32uint16 a, int sgn_x, v32int16 b, int sgn_y, v64acc32 acc, int zero_acc, int shift16, int sub_mul, int sub_acc1)
v64acc32 | addmac_8x2_2x8_conf (v32uint16 a, int sgn_x, v32int16 b, int sgn_y, v64acc32 acc1, v64acc32 acc2, int zero_acc1, int shift16, int sub_mul, int sub_acc1, int sub_acc2)
v64acc32 | addmsc_8x2_2x8_conf (v32uint16 a, int sgn_x, v32int16 b, int sgn_y, v64acc32 acc1, v64acc32 acc2, int zero_acc1, int shift16, int sub_mul, int sub_acc1, int sub_acc2)
v64acc32 | mul_8x2_2x8_conf (v32int16 a, int sgn_x, v32uint16 b, int sgn_y, int sub_mul)
v64acc32 | negmul_8x2_2x8_conf (v32int16 a, int sgn_x, v32uint16 b, int sgn_y, int sub_mul)
v64acc32 | mac_8x2_2x8_conf (v32int16 a, int sgn_x, v32uint16 b, int sgn_y, v64acc32 acc, int zero_acc, int shift16, int sub_mul, int sub_acc1)
v64acc32 | msc_8x2_2x8_conf (v32int16 a, int sgn_x, v32uint16 b, int sgn_y, v64acc32 acc, int zero_acc, int shift16, int sub_mul, int sub_acc1)
v64acc32 | addmac_8x2_2x8_conf (v32int16 a, int sgn_x, v32uint16 b, int sgn_y, v64acc32 acc1, v64acc32 acc2, int zero_acc1, int shift16, int sub_mul, int sub_acc1, int sub_acc2)
v64acc32 | addmsc_8x2_2x8_conf (v32int16 a, int sgn_x, v32uint16 b, int sgn_y, v64acc32 acc1, v64acc32 acc2, int zero_acc1, int shift16, int sub_mul, int sub_acc1, int sub_acc2)
v64acc32 | mul_8x2_2x8_conf (v32int16 a, int sgn_x, v32int16 b, int sgn_y, int sub_mul)
v64acc32 | negmul_8x2_2x8_conf (v32int16 a, int sgn_x, v32int16 b, int sgn_y, int sub_mul)
v64acc32 | mac_8x2_2x8_conf (v32int16 a, int sgn_x, v32int16 b, int sgn_y, v64acc32 acc, int zero_acc, int shift16, int sub_mul, int sub_acc1)
v64acc32 | msc_8x2_2x8_conf (v32int16 a, int sgn_x, v32int16 b, int sgn_y, v64acc32 acc, int zero_acc, int shift16, int sub_mul, int sub_acc1)
v64acc32 | addmac_8x2_2x8_conf (v32int16 a, int sgn_x, v32int16 b, int sgn_y, v64acc32 acc1, v64acc32 acc2, int zero_acc1, int shift16, int sub_mul, int sub_acc1, int sub_acc2)
v64acc32 | addmsc_8x2_2x8_conf (v32int16 a, int sgn_x, v32int16 b, int sgn_y, v64acc32 acc1, v64acc32 acc2, int zero_acc1, int shift16, int sub_mul, int sub_acc1, int sub_acc2)

## elem_64
v64acc32 | mul_elem_64 (v64uint16 a, v64uint16 b)
v64acc32 | negmul_elem_64 (v64uint16 a, v64uint16 b)
v64acc32 | mac_elem_64 (v64uint16 a, v64uint16 b, v64acc32 acc)
v64acc32 | msc_elem_64 (v64uint16 a, v64uint16 b, v64acc32 acc)
v64acc32 | addmac_elem_64 (v64uint16 a, v64uint16 b, v64acc32 acc1, v64acc32 acc2)
v64acc32 | addmsc_elem_64 (v64uint16 a, v64uint16 b, v64acc32 acc1, v64acc32 acc2)
v64acc32 | mul_elem_64 (v64uint16 a, v64int16 b)
v64acc32 | negmul_elem_64 (v64uint16 a, v64int16 b)
v64acc32 | mac_elem_64 (v64uint16 a, v64int16 b, v64acc32 acc)
v64acc32 | msc_elem_64 (v64uint16 a, v64int16 b, v64acc32 acc)
v64acc32 | addmac_elem_64 (v64uint16 a, v64int16 b, v64acc32 acc1, v64acc32 acc2)
v64acc32 | addmsc_elem_64 (v64uint16 a, v64int16 b, v64acc32 acc1, v64acc32 acc2)
v64acc32 | mul_elem_64 (v64int16 a, v64uint16 b)
v64acc32 | negmul_elem_64 (v64int16 a, v64uint16 b)
v64acc32 | mac_elem_64 (v64int16 a, v64uint16 b, v64acc32 acc)
v64acc32 | msc_elem_64 (v64int16 a, v64uint16 b, v64acc32 acc)
v64acc32 | addmac_elem_64 (v64int16 a, v64uint16 b, v64acc32 acc1, v64acc32 acc2)
v64acc32 | addmsc_elem_64 (v64int16 a, v64uint16 b, v64acc32 acc1, v64acc32 acc2)
v64acc32 | mul_elem_64 (v64int16 a, v64int16 b)
v64acc32 | negmul_elem_64 (v64int16 a, v64int16 b)
v64acc32 | mac_elem_64 (v64int16 a, v64int16 b, v64acc32 acc)
v64acc32 | msc_elem_64 (v64int16 a, v64int16 b, v64acc32 acc)
v64acc32 | addmac_elem_64 (v64int16 a, v64int16 b, v64acc32 acc1, v64acc32 acc2)
v64acc32 | addmsc_elem_64 (v64int16 a, v64int16 b, v64acc32 acc1, v64acc32 acc2)

## elem_64 with dynamic sign
v64acc32 | mul_elem_64 (v64uint16 a, int sgn_x, v64uint16 b, int sgn_y)
v64acc32 | negmul_elem_64 (v64uint16 a, int sgn_x, v64uint16 b, int sgn_y)
v64acc32 | mac_elem_64 (v64uint16 a, int sgn_x, v64uint16 b, int sgn_y, v64acc32 acc)
v64acc32 | msc_elem_64 (v64uint16 a, int sgn_x, v64uint16 b, int sgn_y, v64acc32 acc)
v64acc32 | addmac_elem_64 (v64uint16 a, int sgn_x, v64uint16 b, int sgn_y, v64acc32 acc1, v64acc32 acc2)
v64acc32 | addmsc_elem_64 (v64uint16 a, int sgn_x, v64uint16 b, int sgn_y, v64acc32 acc1, v64acc32 acc2)
v64acc32 | mul_elem_64 (v64uint16 a, int sgn_x, v64int16 b, int sgn_y)
v64acc32 | negmul_elem_64 (v64uint16 a, int sgn_x, v64int16 b, int sgn_y)
v64acc32 | mac_elem_64 (v64uint16 a, int sgn_x, v64int16 b, int sgn_y, v64acc32 acc)
v64acc32 | msc_elem_64 (v64uint16 a, int sgn_x, v64int16 b, int sgn_y, v64acc32 acc)
v64acc32 | addmac_elem_64 (v64uint16 a, int sgn_x, v64int16 b, int sgn_y, v64acc32 acc1, v64acc32 acc2)
v64acc32 | addmsc_elem_64 (v64uint16 a, int sgn_x, v64int16 b, int sgn_y, v64acc32 acc1, v64acc32 acc2)
v64acc32 | mul_elem_64 (v64int16 a, int sgn_x, v64uint16 b, int sgn_y)
v64acc32 | negmul_elem_64 (v64int16 a, int sgn_x, v64uint16 b, int sgn_y)
v64acc32 | mac_elem_64 (v64int16 a, int sgn_x, v64uint16 b, int sgn_y, v64acc32 acc)
v64acc32 | msc_elem_64 (v64int16 a, int sgn_x, v64uint16 b, int sgn_y, v64acc32 acc)
v64acc32 | addmac_elem_64 (v64int16 a, int sgn_x, v64uint16 b, int sgn_y, v64acc32 acc1, v64acc32 acc2)
v64acc32 | addmsc_elem_64 (v64int16 a, int sgn_x, v64uint16 b, int sgn_y, v64acc32 acc1, v64acc32 acc2)
v64acc32 | mul_elem_64 (v64int16 a, int sgn_x, v64int16 b, int sgn_y)
v64acc32 | negmul_elem_64 (v64int16 a, int sgn_x, v64int16 b, int sgn_y)
v64acc32 | mac_elem_64 (v64int16 a, int sgn_x, v64int16 b, int sgn_y, v64acc32 acc)
v64acc32 | msc_elem_64 (v64int16 a, int sgn_x, v64int16 b, int sgn_y, v64acc32 acc)
v64acc32 | addmac_elem_64 (v64int16 a, int sgn_x, v64int16 b, int sgn_y, v64acc32 acc1, v64acc32 acc2)
v64acc32 | addmsc_elem_64 (v64int16 a, int sgn_x, v64int16 b, int sgn_y, v64acc32 acc1, v64acc32 acc2)

## elem_64 with dynamic negation of multiplication result
v64acc32 | mul_elem_64_conf (v64uint16 a, v64uint16 b, int sub_mul)
v64acc32 | negmul_elem_64_conf (v64uint16 a, v64uint16 b, int sub_mul)
v64acc32 | mul_elem_64_conf (v64uint16 a, v64int16 b, int sub_mul)
v64acc32 | negmul_elem_64_conf (v64uint16 a, v64int16 b, int sub_mul)
v64acc32 | mul_elem_64_conf (v64int16 a, v64uint16 b, int sub_mul)
v64acc32 | negmul_elem_64_conf (v64int16 a, v64uint16 b, int sub_mul)
v64acc32 | mul_elem_64_conf (v64int16 a, v64int16 b, int sub_mul)
v64acc32 | negmul_elem_64_conf (v64int16 a, v64int16 b, int sub_mul)

## elem_64 with dynamic negation of multiplication result, zeroing of acc1, negation of acc1
v64acc32 | mac_elem_64_conf (v64uint16 a, v64uint16 b, v64acc32 acc, int zero_acc, int shift16, int sub_mul, int sub_acc1)
v64acc32 | msc_elem_64_conf (v64uint16 a, v64uint16 b, v64acc32 acc, int zero_acc, int shift16, int sub_mul, int sub_acc1)
v64acc32 | addmac_elem_64_conf (v64uint16 a, v64uint16 b, v64acc32 acc1, v64acc32 acc2, int zero_acc1, int shift16, int sub_mul, int sub_acc1, int sub_acc2)
v64acc32 | addmsc_elem_64_conf (v64uint16 a, v64uint16 b, v64acc32 acc1, v64acc32 acc2, int zero_acc1, int shift16, int sub_mul, int sub_acc1, int sub_acc2)
v64acc32 | mac_elem_64_conf (v64uint16 a, v64int16 b, v64acc32 acc, int zero_acc, int shift16, int sub_mul, int sub_acc1)
v64acc32 | msc_elem_64_conf (v64uint16 a, v64int16 b, v64acc32 acc, int zero_acc, int shift16, int sub_mul, int sub_acc1)
v64acc32 | addmac_elem_64_conf (v64uint16 a, v64int16 b, v64acc32 acc1, v64acc32 acc2, int zero_acc1, int shift16, int sub_mul, int sub_acc1, int sub_acc2)
v64acc32 | addmsc_elem_64_conf (v64uint16 a, v64int16 b, v64acc32 acc1, v64acc32 acc2, int zero_acc1, int shift16, int sub_mul, int sub_acc1, int sub_acc2)
v64acc32 | mac_elem_64_conf (v64int16 a, v64uint16 b, v64acc32 acc, int zero_acc, int shift16, int sub_mul, int sub_acc1)
v64acc32 | msc_elem_64_conf (v64int16 a, v64uint16 b, v64acc32 acc, int zero_acc, int shift16, int sub_mul, int sub_acc1)
v64acc32 | addmac_elem_64_conf (v64int16 a, v64uint16 b, v64acc32 acc1, v64acc32 acc2, int zero_acc1, int shift16, int sub_mul, int sub_acc1, int sub_acc2)
v64acc32 | addmsc_elem_64_conf (v64int16 a, v64uint16 b, v64acc32 acc1, v64acc32 acc2, int zero_acc1, int shift16, int sub_mul, int sub_acc1, int sub_acc2)
v64acc32 | mac_elem_64_conf (v64int16 a, v64int16 b, v64acc32 acc, int zero_acc, int shift16, int sub_mul, int sub_acc1)
v64acc32 | msc_elem_64_conf (v64int16 a, v64int16 b, v64acc32 acc, int zero_acc, int shift16, int sub_mul, int sub_acc1)
v64acc32 | addmac_elem_64_conf (v64int16 a, v64int16 b, v64acc32 acc1, v64acc32 acc2, int zero_acc1, int shift16, int sub_mul, int sub_acc1, int sub_acc2)
v64acc32 | addmsc_elem_64_conf (v64int16 a, v64int16 b, v64acc32 acc1, v64acc32 acc2, int zero_acc1, int shift16, int sub_mul, int sub_acc1, int sub_acc2)

## elem_64 with dynamic sign and dynamic negation of multiplication result
v64acc32 | mul_elem_64_conf (v64uint16 a, int sgn_x, v64uint16 b, int sgn_y, int sub_mul)
v64acc32 | negmul_elem_64_conf (v64uint16 a, int sgn_x, v64uint16 b, int sgn_y, int sub_mul)
v64acc32 | mac_elem_64_conf (v64uint16 a, int sgn_x, v64uint16 b, int sgn_y, v64acc32 acc, int zero_acc, int shift16, int sub_mul, int sub_acc1)
v64acc32 | msc_elem_64_conf (v64uint16 a, int sgn_x, v64uint16 b, int sgn_y, v64acc32 acc, int zero_acc, int shift16, int sub_mul, int sub_acc1)
v64acc32 | addmac_elem_64_conf (v64uint16 a, int sgn_x, v64uint16 b, int sgn_y, v64acc32 acc1, v64acc32 acc2, int zero_acc1, int shift16, int sub_mul, int sub_acc1, int sub_acc2)
v64acc32 | addmsc_elem_64_conf (v64uint16 a, int sgn_x, v64uint16 b, int sgn_y, v64acc32 acc1, v64acc32 acc2, int zero_acc1, int shift16, int sub_mul, int sub_acc1, int sub_acc2)
v64acc32 | mul_elem_64_conf (v64uint16 a, int sgn_x, v64int16 b, int sgn_y, int sub_mul)
v64acc32 | negmul_elem_64_conf (v64uint16 a, int sgn_x, v64int16 b, int sgn_y, int sub_mul)
v64acc32 | mac_elem_64_conf (v64uint16 a, int sgn_x, v64int16 b, int sgn_y, v64acc32 acc, int zero_acc, int shift16, int sub_mul, int sub_acc1)
v64acc32 | msc_elem_64_conf (v64uint16 a, int sgn_x, v64int16 b, int sgn_y, v64acc32 acc, int zero_acc, int shift16, int sub_mul, int sub_acc1)
v64acc32 | addmac_elem_64_conf (v64uint16 a, int sgn_x, v64int16 b, int sgn_y, v64acc32 acc1, v64acc32 acc2, int zero_acc1, int shift16, int sub_mul, int sub_acc1, int sub_acc2)
v64acc32 | addmsc_elem_64_conf (v64uint16 a, int sgn_x, v64int16 b, int sgn_y, v64acc32 acc1, v64acc32 acc2, int zero_acc1, int shift16, int sub_mul, int sub_acc1, int sub_acc2)
v64acc32 | mul_elem_64_conf (v64int16 a, int sgn_x, v64uint16 b, int sgn_y, int sub_mul)
v64acc32 | negmul_elem_64_conf (v64int16 a, int sgn_x, v64uint16 b, int sgn_y, int sub_mul)
v64acc32 | mac_elem_64_conf (v64int16 a, int sgn_x, v64uint16 b, int sgn_y, v64acc32 acc, int zero_acc, int shift16, int sub_mul, int sub_acc1)
v64acc32 | msc_elem_64_conf (v64int16 a, int sgn_x, v64uint16 b, int sgn_y, v64acc32 acc, int zero_acc, int shift16, int sub_mul, int sub_acc1)
v64acc32 | addmac_elem_64_conf (v64int16 a, int sgn_x, v64uint16 b, int sgn_y, v64acc32 acc1, v64acc32 acc2, int zero_acc1, int shift16, int sub_mul, int sub_acc1, int sub_acc2)
v64acc32 | addmsc_elem_64_conf (v64int16 a, int sgn_x, v64uint16 b, int sgn_y, v64acc32 acc1, v64acc32 acc2, int zero_acc1, int shift16, int sub_mul, int sub_acc1, int sub_acc2)
v64acc32 | mul_elem_64_conf (v64int16 a, int sgn_x, v64int16 b, int sgn_y, int sub_mul)
v64acc32 | negmul_elem_64_conf (v64int16 a, int sgn_x, v64int16 b, int sgn_y, int sub_mul)
v64acc32 | mac_elem_64_conf (v64int16 a, int sgn_x, v64int16 b, int sgn_y, v64acc32 acc, int zero_acc, int shift16, int sub_mul, int sub_acc1)
v64acc32 | msc_elem_64_conf (v64int16 a, int sgn_x, v64int16 b, int sgn_y, v64acc32 acc, int zero_acc, int shift16, int sub_mul, int sub_acc1)
v64acc32 | addmac_elem_64_conf (v64int16 a, int sgn_x, v64int16 b, int sgn_y, v64acc32 acc1, v64acc32 acc2, int zero_acc1, int shift16, int sub_mul, int sub_acc1, int sub_acc2)
v64acc32 | addmsc_elem_64_conf (v64int16 a, int sgn_x, v64int16 b, int sgn_y, v64acc32 acc1, v64acc32 acc2, int zero_acc1, int shift16, int sub_mul, int sub_acc1, int sub_acc2)

## elem_32_32b
v32acc32 | mul_elem_32_32b (v32uint16 a, v32uint16 b)
v32acc32 | negmul_elem_32_32b (v32uint16 a, v32uint16 b)
v32acc32 | mac_elem_32_32b (v32uint16 a, v32uint16 b, v32acc32 acc)
v32acc32 | msc_elem_32_32b (v32uint16 a, v32uint16 b, v32acc32 acc)
v32acc32 | addmac_elem_32_32b (v32uint16 a, v32uint16 b, v32acc32 acc1, v32acc32 acc2)
v32acc32 | addmsc_elem_32_32b (v32uint16 a, v32uint16 b, v32acc32 acc1, v32acc32 acc2)
v32acc32 | mul_elem_32_32b (v32uint16 a, v32int16 b)
v32acc32 | negmul_elem_32_32b (v32uint16 a, v32int16 b)
v32acc32 | mac_elem_32_32b (v32uint16 a, v32int16 b, v32acc32 acc)
v32acc32 | msc_elem_32_32b (v32uint16 a, v32int16 b, v32acc32 acc)
v32acc32 | addmac_elem_32_32b (v32uint16 a, v32int16 b, v32acc32 acc1, v32acc32 acc2)
v32acc32 | addmsc_elem_32_32b (v32uint16 a, v32int16 b, v32acc32 acc1, v32acc32 acc2)
v32acc32 | mul_elem_32_32b (v32int16 a, v32uint16 b)
v32acc32 | negmul_elem_32_32b (v32int16 a, v32uint16 b)
v32acc32 | mac_elem_32_32b (v32int16 a, v32uint16 b, v32acc32 acc)
v32acc32 | msc_elem_32_32b (v32int16 a, v32uint16 b, v32acc32 acc)
v32acc32 | addmac_elem_32_32b (v32int16 a, v32uint16 b, v32acc32 acc1, v32acc32 acc2)
v32acc32 | addmsc_elem_32_32b (v32int16 a, v32uint16 b, v32acc32 acc1, v32acc32 acc2)
v32acc32 | mul_elem_32_32b (v32int16 a, v32int16 b)
v32acc32 | negmul_elem_32_32b (v32int16 a, v32int16 b)
v32acc32 | mac_elem_32_32b (v32int16 a, v32int16 b, v32acc32 acc)
v32acc32 | msc_elem_32_32b (v32int16 a, v32int16 b, v32acc32 acc)
v32acc32 | addmac_elem_32_32b (v32int16 a, v32int16 b, v32acc32 acc1, v32acc32 acc2)
v32acc32 | addmsc_elem_32_32b (v32int16 a, v32int16 b, v32acc32 acc1, v32acc32 acc2)

## elem_32_32b with dynamic sign
v32acc32 | mul_elem_32_32b (v32uint16 a, int sgn_x, v32uint16 b, int sgn_y)
v32acc32 | negmul_elem_32_32b (v32uint16 a, int sgn_x, v32uint16 b, int sgn_y)
v32acc32 | mac_elem_32_32b (v32uint16 a, int sgn_x, v32uint16 b, int sgn_y, v32acc32 acc)
v32acc32 | msc_elem_32_32b (v32uint16 a, int sgn_x, v32uint16 b, int sgn_y, v32acc32 acc)
v32acc32 | addmac_elem_32_32b (v32uint16 a, int sgn_x, v32uint16 b, int sgn_y, v32acc32 acc1, v32acc32 acc2)
v32acc32 | addmsc_elem_32_32b (v32uint16 a, int sgn_x, v32uint16 b, int sgn_y, v32acc32 acc1, v32acc32 acc2)
v32acc32 | mul_elem_32_32b (v32uint16 a, int sgn_x, v32int16 b, int sgn_y)
v32acc32 | negmul_elem_32_32b (v32uint16 a, int sgn_x, v32int16 b, int sgn_y)
v32acc32 | mac_elem_32_32b (v32uint16 a, int sgn_x, v32int16 b, int sgn_y, v32acc32 acc)
v32acc32 | msc_elem_32_32b (v32uint16 a, int sgn_x, v32int16 b, int sgn_y, v32acc32 acc)
v32acc32 | addmac_elem_32_32b (v32uint16 a, int sgn_x, v32int16 b, int sgn_y, v32acc32 acc1, v32acc32 acc2)
v32acc32 | addmsc_elem_32_32b (v32uint16 a, int sgn_x, v32int16 b, int sgn_y, v32acc32 acc1, v32acc32 acc2)
v32acc32 | mul_elem_32_32b (v32int16 a, int sgn_x, v32uint16 b, int sgn_y)
v32acc32 | negmul_elem_32_32b (v32int16 a, int sgn_x, v32uint16 b, int sgn_y)
v32acc32 | mac_elem_32_32b (v32int16 a, int sgn_x, v32uint16 b, int sgn_y, v32acc32 acc)
v32acc32 | msc_elem_32_32b (v32int16 a, int sgn_x, v32uint16 b, int sgn_y, v32acc32 acc)
v32acc32 | addmac_elem_32_32b (v32int16 a, int sgn_x, v32uint16 b, int sgn_y, v32acc32 acc1, v32acc32 acc2)
v32acc32 | addmsc_elem_32_32b (v32int16 a, int sgn_x, v32uint16 b, int sgn_y, v32acc32 acc1, v32acc32 acc2)
v32acc32 | mul_elem_32_32b (v32int16 a, int sgn_x, v32int16 b, int sgn_y)
v32acc32 | negmul_elem_32_32b (v32int16 a, int sgn_x, v32int16 b, int sgn_y)
v32acc32 | mac_elem_32_32b (v32int16 a, int sgn_x, v32int16 b, int sgn_y, v32acc32 acc)
v32acc32 | msc_elem_32_32b (v32int16 a, int sgn_x, v32int16 b, int sgn_y, v32acc32 acc)
v32acc32 | addmac_elem_32_32b (v32int16 a, int sgn_x, v32int16 b, int sgn_y, v32acc32 acc1, v32acc32 acc2)
v32acc32 | addmsc_elem_32_32b (v32int16 a, int sgn_x, v32int16 b, int sgn_y, v32acc32 acc1, v32acc32 acc2)

## elem_32_32b with dynamic negation of multiplication result
v32acc32 | mul_elem_32_32b_conf (v32uint16 a, v32uint16 b, int sub_mul)
v32acc32 | negmul_elem_32_32b_conf (v32uint16 a, v32uint16 b, int sub_mul)
v32acc32 | mul_elem_32_32b_conf (v32uint16 a, v32int16 b, int sub_mul)
v32acc32 | negmul_elem_32_32b_conf (v32uint16 a, v32int16 b, int sub_mul)
v32acc32 | mul_elem_32_32b_conf (v32int16 a, v32uint16 b, int sub_mul)
v32acc32 | negmul_elem_32_32b_conf (v32int16 a, v32uint16 b, int sub_mul)
v32acc32 | mul_elem_32_32b_conf (v32int16 a, v32int16 b, int sub_mul)
v32acc32 | negmul_elem_32_32b_conf (v32int16 a, v32int16 b, int sub_mul)

## elem_32_32b with dynamic negation of multiplication result, zeroing of acc1, negation of acc1
v32acc32 | mac_elem_32_32b_conf (v32uint16 a, v32uint16 b, v32acc32 acc, int zero_acc, int shift16, int sub_mul, int sub_acc1)
v32acc32 | msc_elem_32_32b_conf (v32uint16 a, v32uint16 b, v32acc32 acc, int zero_acc, int shift16, int sub_mul, int sub_acc1)
v32acc32 | addmac_elem_32_32b_conf (v32uint16 a, v32uint16 b, v32acc32 acc1, v32acc32 acc2, int zero_acc1, int shift16, int sub_mul, int sub_acc1, int sub_acc2)
v32acc32 | addmsc_elem_32_32b_conf (v32uint16 a, v32uint16 b, v32acc32 acc1, v32acc32 acc2, int zero_acc1, int shift16, int sub_mul, int sub_acc1, int sub_acc2)
v32acc32 | mac_elem_32_32b_conf (v32uint16 a, v32int16 b, v32acc32 acc, int zero_acc, int shift16, int sub_mul, int sub_acc1)
v32acc32 | msc_elem_32_32b_conf (v32uint16 a, v32int16 b, v32acc32 acc, int zero_acc, int shift16, int sub_mul, int sub_acc1)
v32acc32 | addmac_elem_32_32b_conf (v32uint16 a, v32int16 b, v32acc32 acc1, v32acc32 acc2, int zero_acc1, int shift16, int sub_mul, int sub_acc1, int sub_acc2)
v32acc32 | addmsc_elem_32_32b_conf (v32uint16 a, v32int16 b, v32acc32 acc1, v32acc32 acc2, int zero_acc1, int shift16, int sub_mul, int sub_acc1, int sub_acc2)
v32acc32 | mac_elem_32_32b_conf (v32int16 a, v32uint16 b, v32acc32 acc, int zero_acc, int shift16, int sub_mul, int sub_acc1)
v32acc32 | msc_elem_32_32b_conf (v32int16 a, v32uint16 b, v32acc32 acc, int zero_acc, int shift16, int sub_mul, int sub_acc1)
v32acc32 | addmac_elem_32_32b_conf (v32int16 a, v32uint16 b, v32acc32 acc1, v32acc32 acc2, int zero_acc1, int shift16, int sub_mul, int sub_acc1, int sub_acc2)
v32acc32 | addmsc_elem_32_32b_conf (v32int16 a, v32uint16 b, v32acc32 acc1, v32acc32 acc2, int zero_acc1, int shift16, int sub_mul, int sub_acc1, int sub_acc2)
v32acc32 | mac_elem_32_32b_conf (v32int16 a, v32int16 b, v32acc32 acc, int zero_acc, int shift16, int sub_mul, int sub_acc1)
v32acc32 | msc_elem_32_32b_conf (v32int16 a, v32int16 b, v32acc32 acc, int zero_acc, int shift16, int sub_mul, int sub_acc1)
v32acc32 | addmac_elem_32_32b_conf (v32int16 a, v32int16 b, v32acc32 acc1, v32acc32 acc2, int zero_acc1, int shift16, int sub_mul, int sub_acc1, int sub_acc2)
v32acc32 | addmsc_elem_32_32b_conf (v32int16 a, v32int16 b, v32acc32 acc1, v32acc32 acc2, int zero_acc1, int shift16, int sub_mul, int sub_acc1, int sub_acc2)

## elem_32_32b with dynamic sign and dynamic negation of multiplication result
v32acc32 | mul_elem_32_32b_conf (v32uint16 a, int sgn_x, v32uint16 b, int sgn_y, int sub_mul)
v32acc32 | negmul_elem_32_32b_conf (v32uint16 a, int sgn_x, v32uint16 b, int sgn_y, int sub_mul)
v32acc32 | mac_elem_32_32b_conf (v32uint16 a, int sgn_x, v32uint16 b, int sgn_y, v32acc32 acc, int zero_acc, int shift16, int sub_mul, int sub_acc1)
v32acc32 | msc_elem_32_32b_conf (v32uint16 a, int sgn_x, v32uint16 b, int sgn_y, v32acc32 acc, int zero_acc, int shift16, int sub_mul, int sub_acc1)
v32acc32 | addmac_elem_32_32b_conf (v32uint16 a, int sgn_x, v32uint16 b, int sgn_y, v32acc32 acc1, v32acc32 acc2, int zero_acc1, int shift16, int sub_mul, int sub_acc1, int sub_acc2)
v32acc32 | addmsc_elem_32_32b_conf (v32uint16 a, int sgn_x, v32uint16 b, int sgn_y, v32acc32 acc1, v32acc32 acc2, int zero_acc1, int shift16, int sub_mul, int sub_acc1, int sub_acc2)
v32acc32 | mul_elem_32_32b_conf (v32uint16 a, int sgn_x, v32int16 b, int sgn_y, int sub_mul)
v32acc32 | negmul_elem_32_32b_conf (v32uint16 a, int sgn_x, v32int16 b, int sgn_y, int sub_mul)
v32acc32 | mac_elem_32_32b_conf (v32uint16 a, int sgn_x, v32int16 b, int sgn_y, v32acc32 acc, int zero_acc, int shift16, int sub_mul, int sub_acc1)
v32acc32 | msc_elem_32_32b_conf (v32uint16 a, int sgn_x, v32int16 b, int sgn_y, v32acc32 acc, int zero_acc, int shift16, int sub_mul, int sub_acc1)
v32acc32 | addmac_elem_32_32b_conf (v32uint16 a, int sgn_x, v32int16 b, int sgn_y, v32acc32 acc1, v32acc32 acc2, int zero_acc1, int shift16, int sub_mul, int sub_acc1, int sub_acc2)
v32acc32 | addmsc_elem_32_32b_conf (v32uint16 a, int sgn_x, v32int16 b, int sgn_y, v32acc32 acc1, v32acc32 acc2, int zero_acc1, int shift16, int sub_mul, int sub_acc1, int sub_acc2)
v32acc32 | mul_elem_32_32b_conf (v32int16 a, int sgn_x, v32uint16 b, int sgn_y, int sub_mul)
v32acc32 | negmul_elem_32_32b_conf (v32int16 a, int sgn_x, v32uint16 b, int sgn_y, int sub_mul)
v32acc32 | mac_elem_32_32b_conf (v32int16 a, int sgn_x, v32uint16 b, int sgn_y, v32acc32 acc, int zero_acc, int shift16, int sub_mul, int sub_acc1)
v32acc32 | msc_elem_32_32b_conf (v32int16 a, int sgn_x, v32uint16 b, int sgn_y, v32acc32 acc, int zero_acc, int shift16, int sub_mul, int sub_acc1)
v32acc32 | addmac_elem_32_32b_conf (v32int16 a, int sgn_x, v32uint16 b, int sgn_y, v32acc32 acc1, v32acc32 acc2, int zero_acc1, int shift16, int sub_mul, int sub_acc1, int sub_acc2)
v32acc32 | addmsc_elem_32_32b_conf (v32int16 a, int sgn_x, v32uint16 b, int sgn_y, v32acc32 acc1, v32acc32 acc2, int zero_acc1, int shift16, int sub_mul, int sub_acc1, int sub_acc2)
v32acc32 | mul_elem_32_32b_conf (v32int16 a, int sgn_x, v32int16 b, int sgn_y, int sub_mul)
v32acc32 | negmul_elem_32_32b_conf (v32int16 a, int sgn_x, v32int16 b, int sgn_y, int sub_mul)
v32acc32 | mac_elem_32_32b_conf (v32int16 a, int sgn_x, v32int16 b, int sgn_y, v32acc32 acc, int zero_acc, int shift16, int sub_mul, int sub_acc1)
v32acc32 | msc_elem_32_32b_conf (v32int16 a, int sgn_x, v32int16 b, int sgn_y, v32acc32 acc, int zero_acc, int shift16, int sub_mul, int sub_acc1)
v32acc32 | addmac_elem_32_32b_conf (v32int16 a, int sgn_x, v32int16 b, int sgn_y, v32acc32 acc1, v32acc32 acc2, int zero_acc1, int shift16, int sub_mul, int sub_acc1, int sub_acc2)
v32acc32 | addmsc_elem_32_32b_conf (v32int16 a, int sgn_x, v32int16 b, int sgn_y, v32acc32 acc1, v32acc32 acc2, int zero_acc1, int shift16, int sub_mul, int sub_acc1, int sub_acc2)

## 4x4_4x8
v32acc64 | mul_4x4_4x8 (v32uint16 a, v32uint16 b)
v32acc64 | negmul_4x4_4x8 (v32uint16 a, v32uint16 b)
v32acc64 | mac_4x4_4x8 (v32uint16 a, v32uint16 b, v32acc64 acc)
v32acc64 | msc_4x4_4x8 (v32uint16 a, v32uint16 b, v32acc64 acc)
v32acc64 | addmac_4x4_4x8 (v32uint16 a, v32uint16 b, v32acc64 acc1, v32acc64 acc2)
v32acc64 | addmsc_4x4_4x8 (v32uint16 a, v32uint16 b, v32acc64 acc1, v32acc64 acc2)
v32acc64 | mul_4x4_4x8 (v32uint16 a, v32int16 b)
v32acc64 | negmul_4x4_4x8 (v32uint16 a, v32int16 b)
v32acc64 | mac_4x4_4x8 (v32uint16 a, v32int16 b, v32acc64 acc)
v32acc64 | msc_4x4_4x8 (v32uint16 a, v32int16 b, v32acc64 acc)
v32acc64 | addmac_4x4_4x8 (v32uint16 a, v32int16 b, v32acc64 acc1, v32acc64 acc2)
v32acc64 | addmsc_4x4_4x8 (v32uint16 a, v32int16 b, v32acc64 acc1, v32acc64 acc2)
v32acc64 | mul_4x4_4x8 (v32int16 a, v32uint16 b)
v32acc64 | negmul_4x4_4x8 (v32int16 a, v32uint16 b)
v32acc64 | mac_4x4_4x8 (v32int16 a, v32uint16 b, v32acc64 acc)
v32acc64 | msc_4x4_4x8 (v32int16 a, v32uint16 b, v32acc64 acc)
v32acc64 | addmac_4x4_4x8 (v32int16 a, v32uint16 b, v32acc64 acc1, v32acc64 acc2)
v32acc64 | addmsc_4x4_4x8 (v32int16 a, v32uint16 b, v32acc64 acc1, v32acc64 acc2)
v32acc64 | mul_4x4_4x8 (v32int16 a, v32int16 b)
v32acc64 | negmul_4x4_4x8 (v32int16 a, v32int16 b)
v32acc64 | mac_4x4_4x8 (v32int16 a, v32int16 b, v32acc64 acc)
v32acc64 | msc_4x4_4x8 (v32int16 a, v32int16 b, v32acc64 acc)
v32acc64 | addmac_4x4_4x8 (v32int16 a, v32int16 b, v32acc64 acc1, v32acc64 acc2)
v32acc64 | addmsc_4x4_4x8 (v32int16 a, v32int16 b, v32acc64 acc1, v32acc64 acc2)

## 4x4_4x8 with dynamic sign
v32acc64 | mul_4x4_4x8 (v32uint16 a, int sgn_x, v32uint16 b, int sgn_y)
v32acc64 | negmul_4x4_4x8 (v32uint16 a, int sgn_x, v32uint16 b, int sgn_y)
v32acc64 | mac_4x4_4x8 (v32uint16 a, int sgn_x, v32uint16 b, int sgn_y, v32acc64 acc)
v32acc64 | msc_4x4_4x8 (v32uint16 a, int sgn_x, v32uint16 b, int sgn_y, v32acc64 acc)
v32acc64 | addmac_4x4_4x8 (v32uint16 a, int sgn_x, v32uint16 b, int sgn_y, v32acc64 acc1, v32acc64 acc2)
v32acc64 | addmsc_4x4_4x8 (v32uint16 a, int sgn_x, v32uint16 b, int sgn_y, v32acc64 acc1, v32acc64 acc2)
v32acc64 | mul_4x4_4x8 (v32uint16 a, int sgn_x, v32int16 b, int sgn_y)
v32acc64 | negmul_4x4_4x8 (v32uint16 a, int sgn_x, v32int16 b, int sgn_y)
v32acc64 | mac_4x4_4x8 (v32uint16 a, int sgn_x, v32int16 b, int sgn_y, v32acc64 acc)
v32acc64 | msc_4x4_4x8 (v32uint16 a, int sgn_x, v32int16 b, int sgn_y, v32acc64 acc)
v32acc64 | addmac_4x4_4x8 (v32uint16 a, int sgn_x, v32int16 b, int sgn_y, v32acc64 acc1, v32acc64 acc2)
v32acc64 | addmsc_4x4_4x8 (v32uint16 a, int sgn_x, v32int16 b, int sgn_y, v32acc64 acc1, v32acc64 acc2)
v32acc64 | mul_4x4_4x8 (v32int16 a, int sgn_x, v32uint16 b, int sgn_y)
v32acc64 | negmul_4x4_4x8 (v32int16 a, int sgn_x, v32uint16 b, int sgn_y)
v32acc64 | mac_4x4_4x8 (v32int16 a, int sgn_x, v32uint16 b, int sgn_y, v32acc64 acc)
v32acc64 | msc_4x4_4x8 (v32int16 a, int sgn_x, v32uint16 b, int sgn_y, v32acc64 acc)
v32acc64 | addmac_4x4_4x8 (v32int16 a, int sgn_x, v32uint16 b, int sgn_y, v32acc64 acc1, v32acc64 acc2)
v32acc64 | addmsc_4x4_4x8 (v32int16 a, int sgn_x, v32uint16 b, int sgn_y, v32acc64 acc1, v32acc64 acc2)
v32acc64 | mul_4x4_4x8 (v32int16 a, int sgn_x, v32int16 b, int sgn_y)
v32acc64 | negmul_4x4_4x8 (v32int16 a, int sgn_x, v32int16 b, int sgn_y)
v32acc64 | mac_4x4_4x8 (v32int16 a, int sgn_x, v32int16 b, int sgn_y, v32acc64 acc)
v32acc64 | msc_4x4_4x8 (v32int16 a, int sgn_x, v32int16 b, int sgn_y, v32acc64 acc)
v32acc64 | addmac_4x4_4x8 (v32int16 a, int sgn_x, v32int16 b, int sgn_y, v32acc64 acc1, v32acc64 acc2)
v32acc64 | addmsc_4x4_4x8 (v32int16 a, int sgn_x, v32int16 b, int sgn_y, v32acc64 acc1, v32acc64 acc2)

## 4x4_4x8 with dynamic negation of multiplication result
v32acc64 | mul_4x4_4x8_conf (v32uint16 a, v32uint16 b, int sub_mul)
v32acc64 | negmul_4x4_4x8_conf (v32uint16 a, v32uint16 b, int sub_mul)
v32acc64 | mul_4x4_4x8_conf (v32uint16 a, v32int16 b, int sub_mul)
v32acc64 | negmul_4x4_4x8_conf (v32uint16 a, v32int16 b, int sub_mul)
v32acc64 | mul_4x4_4x8_conf (v32int16 a, v32uint16 b, int sub_mul)
v32acc64 | negmul_4x4_4x8_conf (v32int16 a, v32uint16 b, int sub_mul)
v32acc64 | mul_4x4_4x8_conf (v32int16 a, v32int16 b, int sub_mul)
v32acc64 | negmul_4x4_4x8_conf (v32int16 a, v32int16 b, int sub_mul)

## 4x4_4x8 with dynamic negation of multiplication result, zeroing of acc1, negation of acc1
v32acc64 | mac_4x4_4x8_conf (v32uint16 a, v32uint16 b, v32acc64 acc, int zero_acc, int shift16, int sub_mul, int sub_acc1)
v32acc64 | msc_4x4_4x8_conf (v32uint16 a, v32uint16 b, v32acc64 acc, int zero_acc, int shift16, int sub_mul, int sub_acc1)
v32acc64 | addmac_4x4_4x8_conf (v32uint16 a, v32uint16 b, v32acc64 acc1, v32acc64 acc2, int zero_acc1, int shift16, int sub_mul, int sub_acc1, int sub_acc2)
v32acc64 | addmsc_4x4_4x8_conf (v32uint16 a, v32uint16 b, v32acc64 acc1, v32acc64 acc2, int zero_acc1, int shift16, int sub_mul, int sub_acc1, int sub_acc2)
v32acc64 | mac_4x4_4x8_conf (v32uint16 a, v32int16 b, v32acc64 acc, int zero_acc, int shift16, int sub_mul, int sub_acc1)
v32acc64 | msc_4x4_4x8_conf (v32uint16 a, v32int16 b, v32acc64 acc, int zero_acc, int shift16, int sub_mul, int sub_acc1)
v32acc64 | addmac_4x4_4x8_conf (v32uint16 a, v32int16 b, v32acc64 acc1, v32acc64 acc2, int zero_acc1, int shift16, int sub_mul, int sub_acc1, int sub_acc2)
v32acc64 | addmsc_4x4_4x8_conf (v32uint16 a, v32int16 b, v32acc64 acc1, v32acc64 acc2, int zero_acc1, int shift16, int sub_mul, int sub_acc1, int sub_acc2)
v32acc64 | mac_4x4_4x8_conf (v32int16 a, v32uint16 b, v32acc64 acc, int zero_acc, int shift16, int sub_mul, int sub_acc1)
v32acc64 | msc_4x4_4x8_conf (v32int16 a, v32uint16 b, v32acc64 acc, int zero_acc, int shift16, int sub_mul, int sub_acc1)
v32acc64 | addmac_4x4_4x8_conf (v32int16 a, v32uint16 b, v32acc64 acc1, v32acc64 acc2, int zero_acc1, int shift16, int sub_mul, int sub_acc1, int sub_acc2)
v32acc64 | addmsc_4x4_4x8_conf (v32int16 a, v32uint16 b, v32acc64 acc1, v32acc64 acc2, int zero_acc1, int shift16, int sub_mul, int sub_acc1, int sub_acc2)
v32acc64 | mac_4x4_4x8_conf (v32int16 a, v32int16 b, v32acc64 acc, int zero_acc, int shift16, int sub_mul, int sub_acc1)
v32acc64 | msc_4x4_4x8_conf (v32int16 a, v32int16 b, v32acc64 acc, int zero_acc, int shift16, int sub_mul, int sub_acc1)
v32acc64 | addmac_4x4_4x8_conf (v32int16 a, v32int16 b, v32acc64 acc1, v32acc64 acc2, int zero_acc1, int shift16, int sub_mul, int sub_acc1, int sub_acc2)
v32acc64 | addmsc_4x4_4x8_conf (v32int16 a, v32int16 b, v32acc64 acc1, v32acc64 acc2, int zero_acc1, int shift16, int sub_mul, int sub_acc1, int sub_acc2)

## 4x4_4x8 with dynamic sign and dynamic negation of multiplication result
v32acc64 | mul_4x4_4x8_conf (v32uint16 a, int sgn_x, v32uint16 b, int sgn_y, int sub_mul)
v32acc64 | negmul_4x4_4x8_conf (v32uint16 a, int sgn_x, v32uint16 b, int sgn_y, int sub_mul)
v32acc64 | mac_4x4_4x8_conf (v32uint16 a, int sgn_x, v32uint16 b, int sgn_y, v32acc64 acc, int zero_acc, int shift16, int sub_mul, int sub_acc1)
v32acc64 | msc_4x4_4x8_conf (v32uint16 a, int sgn_x, v32uint16 b, int sgn_y, v32acc64 acc, int zero_acc, int shift16, int sub_mul, int sub_acc1)
v32acc64 | addmac_4x4_4x8_conf (v32uint16 a, int sgn_x, v32uint16 b, int sgn_y, v32acc64 acc1, v32acc64 acc2, int zero_acc1, int shift16, int sub_mul, int sub_acc1, int sub_acc2)
v32acc64 | addmsc_4x4_4x8_conf (v32uint16 a, int sgn_x, v32uint16 b, int sgn_y, v32acc64 acc1, v32acc64 acc2, int zero_acc1, int shift16, int sub_mul, int sub_acc1, int sub_acc2)
v32acc64 | mul_4x4_4x8_conf (v32uint16 a, int sgn_x, v32int16 b, int sgn_y, int sub_mul)
v32acc64 | negmul_4x4_4x8_conf (v32uint16 a, int sgn_x, v32int16 b, int sgn_y, int sub_mul)
v32acc64 | mac_4x4_4x8_conf (v32uint16 a, int sgn_x, v32int16 b, int sgn_y, v32acc64 acc, int zero_acc, int shift16, int sub_mul, int sub_acc1)
v32acc64 | msc_4x4_4x8_conf (v32uint16 a, int sgn_x, v32int16 b, int sgn_y, v32acc64 acc, int zero_acc, int shift16, int sub_mul, int sub_acc1)
v32acc64 | addmac_4x4_4x8_conf (v32uint16 a, int sgn_x, v32int16 b, int sgn_y, v32acc64 acc1, v32acc64 acc2, int zero_acc1, int shift16, int sub_mul, int sub_acc1, int sub_acc2)
v32acc64 | addmsc_4x4_4x8_conf (v32uint16 a, int sgn_x, v32int16 b, int sgn_y, v32acc64 acc1, v32acc64 acc2, int zero_acc1, int shift16, int sub_mul, int sub_acc1, int sub_acc2)
v32acc64 | mul_4x4_4x8_conf (v32int16 a, int sgn_x, v32uint16 b, int sgn_y, int sub_mul)
v32acc64 | negmul_4x4_4x8_conf (v32int16 a, int sgn_x, v32uint16 b, int sgn_y, int sub_mul)
v32acc64 | mac_4x4_4x8_conf (v32int16 a, int sgn_x, v32uint16 b, int sgn_y, v32acc64 acc, int zero_acc, int shift16, int sub_mul, int sub_acc1)
v32acc64 | msc_4x4_4x8_conf (v32int16 a, int sgn_x, v32uint16 b, int sgn_y, v32acc64 acc, int zero_acc, int shift16, int sub_mul, int sub_acc1)
v32acc64 | addmac_4x4_4x8_conf (v32int16 a, int sgn_x, v32uint16 b, int sgn_y, v32acc64 acc1, v32acc64 acc2, int zero_acc1, int shift16, int sub_mul, int sub_acc1, int sub_acc2)
v32acc64 | addmsc_4x4_4x8_conf (v32int16 a, int sgn_x, v32uint16 b, int sgn_y, v32acc64 acc1, v32acc64 acc2, int zero_acc1, int shift16, int sub_mul, int sub_acc1, int sub_acc2)
v32acc64 | mul_4x4_4x8_conf (v32int16 a, int sgn_x, v32int16 b, int sgn_y, int sub_mul)
v32acc64 | negmul_4x4_4x8_conf (v32int16 a, int sgn_x, v32int16 b, int sgn_y, int sub_mul)
v32acc64 | mac_4x4_4x8_conf (v32int16 a, int sgn_x, v32int16 b, int sgn_y, v32acc64 acc, int zero_acc, int shift16, int sub_mul, int sub_acc1)
v32acc64 | msc_4x4_4x8_conf (v32int16 a, int sgn_x, v32int16 b, int sgn_y, v32acc64 acc, int zero_acc, int shift16, int sub_mul, int sub_acc1)
v32acc64 | addmac_4x4_4x8_conf (v32int16 a, int sgn_x, v32int16 b, int sgn_y, v32acc64 acc1, v32acc64 acc2, int zero_acc1, int shift16, int sub_mul, int sub_acc1, int sub_acc2)
v32acc64 | addmsc_4x4_4x8_conf (v32int16 a, int sgn_x, v32int16 b, int sgn_y, v32acc64 acc1, v32acc64 acc2, int zero_acc1, int shift16, int sub_mul, int sub_acc1, int sub_acc2)

## elem_32
v32acc64 | mul_elem_32 (v32uint16 a, v32uint16 b)
v32acc64 | negmul_elem_32 (v32uint16 a, v32uint16 b)
v32acc64 | mac_elem_32 (v32uint16 a, v32uint16 b, v32acc64 acc)
v32acc64 | msc_elem_32 (v32uint16 a, v32uint16 b, v32acc64 acc)
v32acc64 | addmac_elem_32 (v32uint16 a, v32uint16 b, v32acc64 acc1, v32acc64 acc2)
v32acc64 | addmsc_elem_32 (v32uint16 a, v32uint16 b, v32acc64 acc1, v32acc64 acc2)
v32acc64 | mul_elem_32 (v32uint16 a, v32int16 b)
v32acc64 | negmul_elem_32 (v32uint16 a, v32int16 b)
v32acc64 | mac_elem_32 (v32uint16 a, v32int16 b, v32acc64 acc)
v32acc64 | msc_elem_32 (v32uint16 a, v32int16 b, v32acc64 acc)
v32acc64 | addmac_elem_32 (v32uint16 a, v32int16 b, v32acc64 acc1, v32acc64 acc2)
v32acc64 | addmsc_elem_32 (v32uint16 a, v32int16 b, v32acc64 acc1, v32acc64 acc2)
v32acc64 | mul_elem_32 (v32int16 a, v32uint16 b)
v32acc64 | negmul_elem_32 (v32int16 a, v32uint16 b)
v32acc64 | mac_elem_32 (v32int16 a, v32uint16 b, v32acc64 acc)
v32acc64 | msc_elem_32 (v32int16 a, v32uint16 b, v32acc64 acc)
v32acc64 | addmac_elem_32 (v32int16 a, v32uint16 b, v32acc64 acc1, v32acc64 acc2)
v32acc64 | addmsc_elem_32 (v32int16 a, v32uint16 b, v32acc64 acc1, v32acc64 acc2)
v32acc64 | mul_elem_32 (v32int16 a, v32int16 b)
v32acc64 | negmul_elem_32 (v32int16 a, v32int16 b)
v32acc64 | mac_elem_32 (v32int16 a, v32int16 b, v32acc64 acc)
v32acc64 | msc_elem_32 (v32int16 a, v32int16 b, v32acc64 acc)
v32acc64 | addmac_elem_32 (v32int16 a, v32int16 b, v32acc64 acc1, v32acc64 acc2)
v32acc64 | addmsc_elem_32 (v32int16 a, v32int16 b, v32acc64 acc1, v32acc64 acc2)
v32acc64 | mul_elem_32 (v32uint16 a, unsigned short b)
v32acc64 | negmul_elem_32 (v32uint16 a, unsigned short b)
v32acc64 | mac_elem_32 (v32uint16 a, unsigned short b, v32acc64 acc)
v32acc64 | msc_elem_32 (v32uint16 a, unsigned short b, v32acc64 acc)
v32acc64 | addmac_elem_32 (v32uint16 a, unsigned short b, v32acc64 acc1, v32acc64 acc2)
v32acc64 | addmsc_elem_32 (v32uint16 a, unsigned short b, v32acc64 acc1, v32acc64 acc2)
v32acc64 | mul_elem_32 (v32uint16 a, signed short b)
v32acc64 | negmul_elem_32 (v32uint16 a, signed short b)
v32acc64 | mac_elem_32 (v32uint16 a, signed short b, v32acc64 acc)
v32acc64 | msc_elem_32 (v32uint16 a, signed short b, v32acc64 acc)
v32acc64 | addmac_elem_32 (v32uint16 a, signed short b, v32acc64 acc1, v32acc64 acc2)
v32acc64 | addmsc_elem_32 (v32uint16 a, signed short b, v32acc64 acc1, v32acc64 acc2)
v32acc64 | mul_elem_32 (v32int16 a, unsigned short b)
v32acc64 | negmul_elem_32 (v32int16 a, unsigned short b)
v32acc64 | mac_elem_32 (v32int16 a, unsigned short b, v32acc64 acc)
v32acc64 | msc_elem_32 (v32int16 a, unsigned short b, v32acc64 acc)
v32acc64 | addmac_elem_32 (v32int16 a, unsigned short b, v32acc64 acc1, v32acc64 acc2)
v32acc64 | addmsc_elem_32 (v32int16 a, unsigned short b, v32acc64 acc1, v32acc64 acc2)
v32acc64 | mul_elem_32 (v32int16 a, signed short b)
v32acc64 | negmul_elem_32 (v32int16 a, signed short b)
v32acc64 | mac_elem_32 (v32int16 a, signed short b, v32acc64 acc)
v32acc64 | msc_elem_32 (v32int16 a, signed short b, v32acc64 acc)
v32acc64 | addmac_elem_32 (v32int16 a, signed short b, v32acc64 acc1, v32acc64 acc2)
v32acc64 | addmsc_elem_32 (v32int16 a, signed short b, v32acc64 acc1, v32acc64 acc2)
v32accfloat | mul_elem_32 (v32bfloat16 a, v32bfloat16 b)
v32accfloat | negmul_elem_32 (v32bfloat16 a, v32bfloat16 b)
v32accfloat | mac_elem_32 (v32bfloat16 a, v32bfloat16 b, v32accfloat acc)
v32accfloat | msc_elem_32 (v32bfloat16 a, v32bfloat16 b, v32accfloat acc)
v32accfloat | addmac_elem_32 (v32bfloat16 a, v32bfloat16 b, v32accfloat acc1, v32accfloat acc2)
v32accfloat | addmsc_elem_32 (v32bfloat16 a, v32bfloat16 b, v32accfloat acc1, v32accfloat acc2)
v32accfloat | mul_elem_32 (v32bfloat16 a, v32float16 b)
v32accfloat | negmul_elem_32 (v32bfloat16 a, v32float16 b)
v32accfloat | mac_elem_32 (v32bfloat16 a, v32float16 b, v32accfloat acc)
v32accfloat | msc_elem_32 (v32bfloat16 a, v32float16 b, v32accfloat acc)
v32accfloat | addmac_elem_32 (v32bfloat16 a, v32float16 b, v32accfloat acc1, v32accfloat acc2)
v32accfloat | addmsc_elem_32 (v32bfloat16 a, v32float16 b, v32accfloat acc1, v32accfloat acc2)
v32accfloat | mul_elem_32 (v32float16 a, v32bfloat16 b)
v32accfloat | negmul_elem_32 (v32float16 a, v32bfloat16 b)
v32accfloat | mac_elem_32 (v32float16 a, v32bfloat16 b, v32accfloat acc)
v32accfloat | msc_elem_32 (v32float16 a, v32bfloat16 b, v32accfloat acc)
v32accfloat | addmac_elem_32 (v32float16 a, v32bfloat16 b, v32accfloat acc1, v32accfloat acc2)
v32accfloat | addmsc_elem_32 (v32float16 a, v32bfloat16 b, v32accfloat acc1, v32accfloat acc2)
v32accfloat | mul_elem_32 (v32float16 a, v32float16 b)
v32accfloat | negmul_elem_32 (v32float16 a, v32float16 b)
v32accfloat | mac_elem_32 (v32float16 a, v32float16 b, v32accfloat acc)
v32accfloat | msc_elem_32 (v32float16 a, v32float16 b, v32accfloat acc)
v32accfloat | addmac_elem_32 (v32float16 a, v32float16 b, v32accfloat acc1, v32accfloat acc2)
v32accfloat | addmsc_elem_32 (v32float16 a, v32float16 b, v32accfloat acc1, v32accfloat acc2)
v32accfloat | mul_elem_32 (v32bfloat16 a, bfloat16 b)
v32accfloat | negmul_elem_32 (v32bfloat16 a, bfloat16 b)
v32accfloat | mac_elem_32 (v32bfloat16 a, bfloat16 b, v32accfloat acc)
v32accfloat | msc_elem_32 (v32bfloat16 a, bfloat16 b, v32accfloat acc)
v32accfloat | addmac_elem_32 (v32bfloat16 a, bfloat16 b, v32accfloat acc1, v32accfloat acc2)
v32accfloat | addmsc_elem_32 (v32bfloat16 a, bfloat16 b, v32accfloat acc1, v32accfloat acc2)
v32accfloat | mul_elem_32 (v32bfloat16 a, float16 b)
v32accfloat | negmul_elem_32 (v32bfloat16 a, float16 b)
v32accfloat | mac_elem_32 (v32bfloat16 a, float16 b, v32accfloat acc)
v32accfloat | msc_elem_32 (v32bfloat16 a, float16 b, v32accfloat acc)
v32accfloat | addmac_elem_32 (v32bfloat16 a, float16 b, v32accfloat acc1, v32accfloat acc2)
v32accfloat | addmsc_elem_32 (v32bfloat16 a, float16 b, v32accfloat acc1, v32accfloat acc2)
v32accfloat | mul_elem_32 (v32float16 a, bfloat16 b)
v32accfloat | negmul_elem_32 (v32float16 a, bfloat16 b)
v32accfloat | mac_elem_32 (v32float16 a, bfloat16 b, v32accfloat acc)
v32accfloat | msc_elem_32 (v32float16 a, bfloat16 b, v32accfloat acc)
v32accfloat | addmac_elem_32 (v32float16 a, bfloat16 b, v32accfloat acc1, v32accfloat acc2)
v32accfloat | addmsc_elem_32 (v32float16 a, bfloat16 b, v32accfloat acc1, v32accfloat acc2)
v32accfloat | mul_elem_32 (v32float16 a, float16 b)
v32accfloat | negmul_elem_32 (v32float16 a, float16 b)
v32accfloat | mac_elem_32 (v32float16 a, float16 b, v32accfloat acc)
v32accfloat | msc_elem_32 (v32float16 a, float16 b, v32accfloat acc)
v32accfloat | addmac_elem_32 (v32float16 a, float16 b, v32accfloat acc1, v32accfloat acc2)
v32accfloat | addmsc_elem_32 (v32float16 a, float16 b, v32accfloat acc1, v32accfloat acc2)

## elem_32 with dynamic sign
v32acc64 | mul_elem_32 (v32uint16 a, int sgn_x, v32uint16 b, int sgn_y)
v32acc64 | negmul_elem_32 (v32uint16 a, int sgn_x, v32uint16 b, int sgn_y)
v32acc64 | mac_elem_32 (v32uint16 a, int sgn_x, v32uint16 b, int sgn_y, v32acc64 acc)
v32acc64 | msc_elem_32 (v32uint16 a, int sgn_x, v32uint16 b, int sgn_y, v32acc64 acc)
v32acc64 | addmac_elem_32 (v32uint16 a, int sgn_x, v32uint16 b, int sgn_y, v32acc64 acc1, v32acc64 acc2)
v32acc64 | addmsc_elem_32 (v32uint16 a, int sgn_x, v32uint16 b, int sgn_y, v32acc64 acc1, v32acc64 acc2)
v32acc64 | mul_elem_32 (v32uint16 a, int sgn_x, v32int16 b, int sgn_y)
v32acc64 | negmul_elem_32 (v32uint16 a, int sgn_x, v32int16 b, int sgn_y)
v32acc64 | mac_elem_32 (v32uint16 a, int sgn_x, v32int16 b, int sgn_y, v32acc64 acc)
v32acc64 | msc_elem_32 (v32uint16 a, int sgn_x, v32int16 b, int sgn_y, v32acc64 acc)
v32acc64 | addmac_elem_32 (v32uint16 a, int sgn_x, v32int16 b, int sgn_y, v32acc64 acc1, v32acc64 acc2)
v32acc64 | addmsc_elem_32 (v32uint16 a, int sgn_x, v32int16 b, int sgn_y, v32acc64 acc1, v32acc64 acc2)
v32acc64 | mul_elem_32 (v32int16 a, int sgn_x, v32uint16 b, int sgn_y)
v32acc64 | negmul_elem_32 (v32int16 a, int sgn_x, v32uint16 b, int sgn_y)
v32acc64 | mac_elem_32 (v32int16 a, int sgn_x, v32uint16 b, int sgn_y, v32acc64 acc)
v32acc64 | msc_elem_32 (v32int16 a, int sgn_x, v32uint16 b, int sgn_y, v32acc64 acc)
v32acc64 | addmac_elem_32 (v32int16 a, int sgn_x, v32uint16 b, int sgn_y, v32acc64 acc1, v32acc64 acc2)
v32acc64 | addmsc_elem_32 (v32int16 a, int sgn_x, v32uint16 b, int sgn_y, v32acc64 acc1, v32acc64 acc2)
v32acc64 | mul_elem_32 (v32int16 a, int sgn_x, v32int16 b, int sgn_y)
v32acc64 | negmul_elem_32 (v32int16 a, int sgn_x, v32int16 b, int sgn_y)
v32acc64 | mac_elem_32 (v32int16 a, int sgn_x, v32int16 b, int sgn_y, v32acc64 acc)
v32acc64 | msc_elem_32 (v32int16 a, int sgn_x, v32int16 b, int sgn_y, v32acc64 acc)
v32acc64 | addmac_elem_32 (v32int16 a, int sgn_x, v32int16 b, int sgn_y, v32acc64 acc1, v32acc64 acc2)
v32acc64 | addmsc_elem_32 (v32int16 a, int sgn_x, v32int16 b, int sgn_y, v32acc64 acc1, v32acc64 acc2)
v32acc64 | mul_elem_32 (v32uint16 a, int sgn_x, unsigned short b, int sgn_y)
v32acc64 | negmul_elem_32 (v32uint16 a, int sgn_x, unsigned short b, int sgn_y)
v32acc64 | mac_elem_32 (v32uint16 a, int sgn_x, unsigned short b, int sgn_y, v32acc64 acc)
v32acc64 | msc_elem_32 (v32uint16 a, int sgn_x, unsigned short b, int sgn_y, v32acc64 acc)
v32acc64 | addmac_elem_32 (v32uint16 a, int sgn_x, unsigned short b, int sgn_y, v32acc64 acc1, v32acc64 acc2)
v32acc64 | addmsc_elem_32 (v32uint16 a, int sgn_x, unsigned short b, int sgn_y, v32acc64 acc1, v32acc64 acc2)
v32acc64 | mul_elem_32 (v32uint16 a, int sgn_x, signed short b, int sgn_y)
v32acc64 | negmul_elem_32 (v32uint16 a, int sgn_x, signed short b, int sgn_y)
v32acc64 | mac_elem_32 (v32uint16 a, int sgn_x, signed short b, int sgn_y, v32acc64 acc)
v32acc64 | msc_elem_32 (v32uint16 a, int sgn_x, signed short b, int sgn_y, v32acc64 acc)
v32acc64 | addmac_elem_32 (v32uint16 a, int sgn_x, signed short b, int sgn_y, v32acc64 acc1, v32acc64 acc2)
v32acc64 | addmsc_elem_32 (v32uint16 a, int sgn_x, signed short b, int sgn_y, v32acc64 acc1, v32acc64 acc2)
v32acc64 | mul_elem_32 (v32int16 a, int sgn_x, unsigned short b, int sgn_y)
v32acc64 | negmul_elem_32 (v32int16 a, int sgn_x, unsigned short b, int sgn_y)
v32acc64 | mac_elem_32 (v32int16 a, int sgn_x, unsigned short b, int sgn_y, v32acc64 acc)
v32acc64 | msc_elem_32 (v32int16 a, int sgn_x, unsigned short b, int sgn_y, v32acc64 acc)
v32acc64 | addmac_elem_32 (v32int16 a, int sgn_x, unsigned short b, int sgn_y, v32acc64 acc1, v32acc64 acc2)
v32acc64 | addmsc_elem_32 (v32int16 a, int sgn_x, unsigned short b, int sgn_y, v32acc64 acc1, v32acc64 acc2)
v32acc64 | mul_elem_32 (v32int16 a, int sgn_x, signed short b, int sgn_y)
v32acc64 | negmul_elem_32 (v32int16 a, int sgn_x, signed short b, int sgn_y)
v32acc64 | mac_elem_32 (v32int16 a, int sgn_x, signed short b, int sgn_y, v32acc64 acc)
v32acc64 | msc_elem_32 (v32int16 a, int sgn_x, signed short b, int sgn_y, v32acc64 acc)
v32acc64 | addmac_elem_32 (v32int16 a, int sgn_x, signed short b, int sgn_y, v32acc64 acc1, v32acc64 acc2)
v32acc64 | addmsc_elem_32 (v32int16 a, int sgn_x, signed short b, int sgn_y, v32acc64 acc1, v32acc64 acc2)
v32accfloat | mul_elem_32 (v32bfloat16 a, int sgn_x, v32bfloat16 b, int sgn_y)
v32accfloat | negmul_elem_32 (v32bfloat16 a, int sgn_x, v32bfloat16 b, int sgn_y)
v32accfloat | mac_elem_32 (v32bfloat16 a, int sgn_x, v32bfloat16 b, int sgn_y, v32accfloat acc)
v32accfloat | msc_elem_32 (v32bfloat16 a, int sgn_x, v32bfloat16 b, int sgn_y, v32accfloat acc)
v32accfloat | addmac_elem_32 (v32bfloat16 a, int sgn_x, v32bfloat16 b, int sgn_y, v32accfloat acc1, v32accfloat acc2)
v32accfloat | addmsc_elem_32 (v32bfloat16 a, int sgn_x, v32bfloat16 b, int sgn_y, v32accfloat acc1, v32accfloat acc2)
v32accfloat | mul_elem_32 (v32bfloat16 a, int sgn_x, v32float16 b, int sgn_y)
v32accfloat | negmul_elem_32 (v32bfloat16 a, int sgn_x, v32float16 b, int sgn_y)
v32accfloat | mac_elem_32 (v32bfloat16 a, int sgn_x, v32float16 b, int sgn_y, v32accfloat acc)
v32accfloat | msc_elem_32 (v32bfloat16 a, int sgn_x, v32float16 b, int sgn_y, v32accfloat acc)
v32accfloat | addmac_elem_32 (v32bfloat16 a, int sgn_x, v32float16 b, int sgn_y, v32accfloat acc1, v32accfloat acc2)
v32accfloat | addmsc_elem_32 (v32bfloat16 a, int sgn_x, v32float16 b, int sgn_y, v32accfloat acc1, v32accfloat acc2)
v32accfloat | mul_elem_32 (v32float16 a, int sgn_x, v32bfloat16 b, int sgn_y)
v32accfloat | negmul_elem_32 (v32float16 a, int sgn_x, v32bfloat16 b, int sgn_y)
v32accfloat | mac_elem_32 (v32float16 a, int sgn_x, v32bfloat16 b, int sgn_y, v32accfloat acc)
v32accfloat | msc_elem_32 (v32float16 a, int sgn_x, v32bfloat16 b, int sgn_y, v32accfloat acc)
v32accfloat | addmac_elem_32 (v32float16 a, int sgn_x, v32bfloat16 b, int sgn_y, v32accfloat acc1, v32accfloat acc2)
v32accfloat | addmsc_elem_32 (v32float16 a, int sgn_x, v32bfloat16 b, int sgn_y, v32accfloat acc1, v32accfloat acc2)
v32accfloat | mul_elem_32 (v32float16 a, int sgn_x, v32float16 b, int sgn_y)
v32accfloat | negmul_elem_32 (v32float16 a, int sgn_x, v32float16 b, int sgn_y)
v32accfloat | mac_elem_32 (v32float16 a, int sgn_x, v32float16 b, int sgn_y, v32accfloat acc)
v32accfloat | msc_elem_32 (v32float16 a, int sgn_x, v32float16 b, int sgn_y, v32accfloat acc)
v32accfloat | addmac_elem_32 (v32float16 a, int sgn_x, v32float16 b, int sgn_y, v32accfloat acc1, v32accfloat acc2)
v32accfloat | addmsc_elem_32 (v32float16 a, int sgn_x, v32float16 b, int sgn_y, v32accfloat acc1, v32accfloat acc2)
v32accfloat | mul_elem_32 (v32bfloat16 a, int sgn_x, bfloat16 b, int sgn_y)
v32accfloat | negmul_elem_32 (v32bfloat16 a, int sgn_x, bfloat16 b, int sgn_y)
v32accfloat | mac_elem_32 (v32bfloat16 a, int sgn_x, bfloat16 b, int sgn_y, v32accfloat acc)
v32accfloat | msc_elem_32 (v32bfloat16 a, int sgn_x, bfloat16 b, int sgn_y, v32accfloat acc)
v32accfloat | addmac_elem_32 (v32bfloat16 a, int sgn_x, bfloat16 b, int sgn_y, v32accfloat acc1, v32accfloat acc2)
v32accfloat | addmsc_elem_32 (v32bfloat16 a, int sgn_x, bfloat16 b, int sgn_y, v32accfloat acc1, v32accfloat acc2)
v32accfloat | mul_elem_32 (v32bfloat16 a, int sgn_x, float16 b, int sgn_y)
v32accfloat | negmul_elem_32 (v32bfloat16 a, int sgn_x, float16 b, int sgn_y)
v32accfloat | mac_elem_32 (v32bfloat16 a, int sgn_x, float16 b, int sgn_y, v32accfloat acc)
v32accfloat | msc_elem_32 (v32bfloat16 a, int sgn_x, float16 b, int sgn_y, v32accfloat acc)
v32accfloat | addmac_elem_32 (v32bfloat16 a, int sgn_x, float16 b, int sgn_y, v32accfloat acc1, v32accfloat acc2)
v32accfloat | addmsc_elem_32 (v32bfloat16 a, int sgn_x, float16 b, int sgn_y, v32accfloat acc1, v32accfloat acc2)
v32accfloat | mul_elem_32 (v32float16 a, int sgn_x, bfloat16 b, int sgn_y)
v32accfloat | negmul_elem_32 (v32float16 a, int sgn_x, bfloat16 b, int sgn_y)
v32accfloat | mac_elem_32 (v32float16 a, int sgn_x, bfloat16 b, int sgn_y, v32accfloat acc)
v32accfloat | msc_elem_32 (v32float16 a, int sgn_x, bfloat16 b, int sgn_y, v32accfloat acc)
v32accfloat | addmac_elem_32 (v32float16 a, int sgn_x, bfloat16 b, int sgn_y, v32accfloat acc1, v32accfloat acc2)
v32accfloat | addmsc_elem_32 (v32float16 a, int sgn_x, bfloat16 b, int sgn_y, v32accfloat acc1, v32accfloat acc2)
v32accfloat | mul_elem_32 (v32float16 a, int sgn_x, float16 b, int sgn_y)
v32accfloat | negmul_elem_32 (v32float16 a, int sgn_x, float16 b, int sgn_y)
v32accfloat | mac_elem_32 (v32float16 a, int sgn_x, float16 b, int sgn_y, v32accfloat acc)
v32accfloat | msc_elem_32 (v32float16 a, int sgn_x, float16 b, int sgn_y, v32accfloat acc)
v32accfloat | addmac_elem_32 (v32float16 a, int sgn_x, float16 b, int sgn_y, v32accfloat acc1, v32accfloat acc2)
v32accfloat | addmsc_elem_32 (v32float16 a, int sgn_x, float16 b, int sgn_y, v32accfloat acc1, v32accfloat acc2)

## elem_32 with dynamic negation of multiplication result
v32acc64 | mul_elem_32_conf (v32uint16 a, v32uint16 b, int sub_mul)
v32acc64 | negmul_elem_32_conf (v32uint16 a, v32uint16 b, int sub_mul)
v32acc64 | mul_elem_32_conf (v32uint16 a, v32int16 b, int sub_mul)
v32acc64 | negmul_elem_32_conf (v32uint16 a, v32int16 b, int sub_mul)
v32acc64 | mul_elem_32_conf (v32int16 a, v32uint16 b, int sub_mul)
v32acc64 | negmul_elem_32_conf (v32int16 a, v32uint16 b, int sub_mul)
v32acc64 | mul_elem_32_conf (v32int16 a, v32int16 b, int sub_mul)
v32acc64 | negmul_elem_32_conf (v32int16 a, v32int16 b, int sub_mul)
v32acc64 | mul_elem_32_conf (v32uint16 a, unsigned short b, int sub_mul)
v32acc64 | negmul_elem_32_conf (v32uint16 a, unsigned short b, int sub_mul)
v32acc64 | mul_elem_32_conf (v32uint16 a, signed short b, int sub_mul)
v32acc64 | negmul_elem_32_conf (v32uint16 a, signed short b, int sub_mul)
v32acc64 | mul_elem_32_conf (v32int16 a, unsigned short b, int sub_mul)
v32acc64 | negmul_elem_32_conf (v32int16 a, unsigned short b, int sub_mul)
v32acc64 | mul_elem_32_conf (v32int16 a, signed short b, int sub_mul)
v32acc64 | negmul_elem_32_conf (v32int16 a, signed short b, int sub_mul)
v32accfloat | mul_elem_32_conf (v32bfloat16 a, v32bfloat16 b, int sub_mul)
v32accfloat | negmul_elem_32_conf (v32bfloat16 a, v32bfloat16 b, int sub_mul)
v32accfloat | mul_elem_32_conf (v32bfloat16 a, v32float16 b, int sub_mul)
v32accfloat | negmul_elem_32_conf (v32bfloat16 a, v32float16 b, int sub_mul)
v32accfloat | mul_elem_32_conf (v32float16 a, v32bfloat16 b, int sub_mul)
v32accfloat | negmul_elem_32_conf (v32float16 a, v32bfloat16 b, int sub_mul)
v32accfloat | mul_elem_32_conf (v32float16 a, v32float16 b, int sub_mul)
v32accfloat | negmul_elem_32_conf (v32float16 a, v32float16 b, int sub_mul)
v32accfloat | mul_elem_32_conf (v32bfloat16 a, bfloat16 b, int sub_mul)
v32accfloat | negmul_elem_32_conf (v32bfloat16 a, bfloat16 b, int sub_mul)
v32accfloat | mul_elem_32_conf (v32bfloat16 a, float16 b, int sub_mul)
v32accfloat | negmul_elem_32_conf (v32bfloat16 a, float16 b, int sub_mul)
v32accfloat | mul_elem_32_conf (v32float16 a, bfloat16 b, int sub_mul)
v32accfloat | negmul_elem_32_conf (v32float16 a, bfloat16 b, int sub_mul)
v32accfloat | mul_elem_32_conf (v32float16 a, float16 b, int sub_mul)
v32accfloat | negmul_elem_32_conf (v32float16 a, float16 b, int sub_mul)

## elem_32 with dynamic negation of multiplication result, zeroing of acc1, negation of acc1
v32acc64 | mac_elem_32_conf (v32uint16 a, v32uint16 b, v32acc64 acc, int zero_acc, int shift16, int sub_mul, int sub_acc1)
v32acc64 | msc_elem_32_conf (v32uint16 a, v32uint16 b, v32acc64 acc, int zero_acc, int shift16, int sub_mul, int sub_acc1)
v32acc64 | addmac_elem_32_conf (v32uint16 a, v32uint16 b, v32acc64 acc1, v32acc64 acc2, int zero_acc1, int shift16, int sub_mul, int sub_acc1, int sub_acc2)
v32acc64 | addmsc_elem_32_conf (v32uint16 a, v32uint16 b, v32acc64 acc1, v32acc64 acc2, int zero_acc1, int shift16, int sub_mul, int sub_acc1, int sub_acc2)
v32acc64 | mac_elem_32_conf (v32uint16 a, v32int16 b, v32acc64 acc, int zero_acc, int shift16, int sub_mul, int sub_acc1)
v32acc64 | msc_elem_32_conf (v32uint16 a, v32int16 b, v32acc64 acc, int zero_acc, int shift16, int sub_mul, int sub_acc1)
v32acc64 | addmac_elem_32_conf (v32uint16 a, v32int16 b, v32acc64 acc1, v32acc64 acc2, int zero_acc1, int shift16, int sub_mul, int sub_acc1, int sub_acc2)
v32acc64 | addmsc_elem_32_conf (v32uint16 a, v32int16 b, v32acc64 acc1, v32acc64 acc2, int zero_acc1, int shift16, int sub_mul, int sub_acc1, int sub_acc2)
v32acc64 | mac_elem_32_conf (v32int16 a, v32uint16 b, v32acc64 acc, int zero_acc, int shift16, int sub_mul, int sub_acc1)
v32acc64 | msc_elem_32_conf (v32int16 a, v32uint16 b, v32acc64 acc, int zero_acc, int shift16, int sub_mul, int sub_acc1)
v32acc64 | addmac_elem_32_conf (v32int16 a, v32uint16 b, v32acc64 acc1, v32acc64 acc2, int zero_acc1, int shift16, int sub_mul, int sub_acc1, int sub_acc2)
v32acc64 | addmsc_elem_32_conf (v32int16 a, v32uint16 b, v32acc64 acc1, v32acc64 acc2, int zero_acc1, int shift16, int sub_mul, int sub_acc1, int sub_acc2)
v32acc64 | mac_elem_32_conf (v32int16 a, v32int16 b, v32acc64 acc, int zero_acc, int shift16, int sub_mul, int sub_acc1)
v32acc64 | msc_elem_32_conf (v32int16 a, v32int16 b, v32acc64 acc, int zero_acc, int shift16, int sub_mul, int sub_acc1)
v32acc64 | addmac_elem_32_conf (v32int16 a, v32int16 b, v32acc64 acc1, v32acc64 acc2, int zero_acc1, int shift16, int sub_mul, int sub_acc1, int sub_acc2)
v32acc64 | addmsc_elem_32_conf (v32int16 a, v32int16 b, v32acc64 acc1, v32acc64 acc2, int zero_acc1, int shift16, int sub_mul, int sub_acc1, int sub_acc2)
v32acc64 | mac_elem_32_conf (v32uint16 a, unsigned short b, v32acc64 acc, int zero_acc, int shift16, int sub_mul, int sub_acc1)
v32acc64 | msc_elem_32_conf (v32uint16 a, unsigned short b, v32acc64 acc, int zero_acc, int shift16, int sub_mul, int sub_acc1)
v32acc64 | addmac_elem_32_conf (v32uint16 a, unsigned short b, v32acc64 acc1, v32acc64 acc2, int zero_acc1, int shift16, int sub_mul, int sub_acc1, int sub_acc2)
v32acc64 | addmsc_elem_32_conf (v32uint16 a, unsigned short b, v32acc64 acc1, v32acc64 acc2, int zero_acc1, int shift16, int sub_mul, int sub_acc1, int sub_acc2)
v32acc64 | mac_elem_32_conf (v32uint16 a, signed short b, v32acc64 acc, int zero_acc, int shift16, int sub_mul, int sub_acc1)
v32acc64 | msc_elem_32_conf (v32uint16 a, signed short b, v32acc64 acc, int zero_acc, int shift16, int sub_mul, int sub_acc1)
v32acc64 | addmac_elem_32_conf (v32uint16 a, signed short b, v32acc64 acc1, v32acc64 acc2, int zero_acc1, int shift16, int sub_mul, int sub_acc1, int sub_acc2)
v32acc64 | addmsc_elem_32_conf (v32uint16 a, signed short b, v32acc64 acc1, v32acc64 acc2, int zero_acc1, int shift16, int sub_mul, int sub_acc1, int sub_acc2)
v32acc64 | mac_elem_32_conf (v32int16 a, unsigned short b, v32acc64 acc, int zero_acc, int shift16, int sub_mul, int sub_acc1)
v32acc64 | msc_elem_32_conf (v32int16 a, unsigned short b, v32acc64 acc, int zero_acc, int shift16, int sub_mul, int sub_acc1)
v32acc64 | addmac_elem_32_conf (v32int16 a, unsigned short b, v32acc64 acc1, v32acc64 acc2, int zero_acc1, int shift16, int sub_mul, int sub_acc1, int sub_acc2)
v32acc64 | addmsc_elem_32_conf (v32int16 a, unsigned short b, v32acc64 acc1, v32acc64 acc2, int zero_acc1, int shift16, int sub_mul, int sub_acc1, int sub_acc2)
v32acc64 | mac_elem_32_conf (v32int16 a, signed short b, v32acc64 acc, int zero_acc, int shift16, int sub_mul, int sub_acc1)
v32acc64 | msc_elem_32_conf (v32int16 a, signed short b, v32acc64 acc, int zero_acc, int shift16, int sub_mul, int sub_acc1)
v32acc64 | addmac_elem_32_conf (v32int16 a, signed short b, v32acc64 acc1, v32acc64 acc2, int zero_acc1, int shift16, int sub_mul, int sub_acc1, int sub_acc2)
v32acc64 | addmsc_elem_32_conf (v32int16 a, signed short b, v32acc64 acc1, v32acc64 acc2, int zero_acc1, int shift16, int sub_mul, int sub_acc1, int sub_acc2)
v32accfloat | mac_elem_32_conf (v32bfloat16 a, v32bfloat16 b, v32accfloat acc, int zero_acc, int sub_mul, int sub_acc1)
v32accfloat | msc_elem_32_conf (v32bfloat16 a, v32bfloat16 b, v32accfloat acc, int zero_acc, int sub_mul, int sub_acc1)
v32accfloat | addmac_elem_32_conf (v32bfloat16 a, v32bfloat16 b, v32accfloat acc1, v32accfloat acc2, int zero_acc1, int sub_mul, int sub_acc1, int sub_acc2)
v32accfloat | addmsc_elem_32_conf (v32bfloat16 a, v32bfloat16 b, v32accfloat acc1, v32accfloat acc2, int zero_acc1, int sub_mul, int sub_acc1, int sub_acc2)
v32accfloat | mac_elem_32_conf (v32bfloat16 a, v32float16 b, v32accfloat acc, int zero_acc, int sub_mul, int sub_acc1)
v32accfloat | msc_elem_32_conf (v32bfloat16 a, v32float16 b, v32accfloat acc, int zero_acc, int sub_mul, int sub_acc1)
v32accfloat | addmac_elem_32_conf (v32bfloat16 a, v32float16 b, v32accfloat acc1, v32accfloat acc2, int zero_acc1, int sub_mul, int sub_acc1, int sub_acc2)
v32accfloat | addmsc_elem_32_conf (v32bfloat16 a, v32float16 b, v32accfloat acc1, v32accfloat acc2, int zero_acc1, int sub_mul, int sub_acc1, int sub_acc2)
v32accfloat | mac_elem_32_conf (v32float16 a, v32bfloat16 b, v32accfloat acc, int zero_acc, int sub_mul, int sub_acc1)
v32accfloat | msc_elem_32_conf (v32float16 a, v32bfloat16 b, v32accfloat acc, int zero_acc, int sub_mul, int sub_acc1)
v32accfloat | addmac_elem_32_conf (v32float16 a, v32bfloat16 b, v32accfloat acc1, v32accfloat acc2, int zero_acc1, int sub_mul, int sub_acc1, int sub_acc2)
v32accfloat | addmsc_elem_32_conf (v32float16 a, v32bfloat16 b, v32accfloat acc1, v32accfloat acc2, int zero_acc1, int sub_mul, int sub_acc1, int sub_acc2)
v32accfloat | mac_elem_32_conf (v32float16 a, v32float16 b, v32accfloat acc, int zero_acc, int sub_mul, int sub_acc1)
v32accfloat | msc_elem_32_conf (v32float16 a, v32float16 b, v32accfloat acc, int zero_acc, int sub_mul, int sub_acc1)
v32accfloat | addmac_elem_32_conf (v32float16 a, v32float16 b, v32accfloat acc1, v32accfloat acc2, int zero_acc1, int sub_mul, int sub_acc1, int sub_acc2)
v32accfloat | addmsc_elem_32_conf (v32float16 a, v32float16 b, v32accfloat acc1, v32accfloat acc2, int zero_acc1, int sub_mul, int sub_acc1, int sub_acc2)
v32accfloat | mac_elem_32_conf (v32bfloat16 a, bfloat16 b, v32accfloat acc, int zero_acc, int sub_mul, int sub_acc1)
v32accfloat | msc_elem_32_conf (v32bfloat16 a, bfloat16 b, v32accfloat acc, int zero_acc, int sub_mul, int sub_acc1)
v32accfloat | addmac_elem_32_conf (v32bfloat16 a, bfloat16 b, v32accfloat acc1, v32accfloat acc2, int zero_acc1, int sub_mul, int sub_acc1, int sub_acc2)
v32accfloat | addmsc_elem_32_conf (v32bfloat16 a, bfloat16 b, v32accfloat acc1, v32accfloat acc2, int zero_acc1, int sub_mul, int sub_acc1, int sub_acc2)
v32accfloat | mac_elem_32_conf (v32bfloat16 a, float16 b, v32accfloat acc, int zero_acc, int sub_mul, int sub_acc1)
v32accfloat | msc_elem_32_conf (v32bfloat16 a, float16 b, v32accfloat acc, int zero_acc, int sub_mul, int sub_acc1)
v32accfloat | addmac_elem_32_conf (v32bfloat16 a, float16 b, v32accfloat acc1, v32accfloat acc2, int zero_acc1, int sub_mul, int sub_acc1, int sub_acc2)
v32accfloat | addmsc_elem_32_conf (v32bfloat16 a, float16 b, v32accfloat acc1, v32accfloat acc2, int zero_acc1, int sub_mul, int sub_acc1, int sub_acc2)
v32accfloat | mac_elem_32_conf (v32float16 a, bfloat16 b, v32accfloat acc, int zero_acc, int sub_mul, int sub_acc1)
v32accfloat | msc_elem_32_conf (v32float16 a, bfloat16 b, v32accfloat acc, int zero_acc, int sub_mul, int sub_acc1)
v32accfloat | addmac_elem_32_conf (v32float16 a, bfloat16 b, v32accfloat acc1, v32accfloat acc2, int zero_acc1, int sub_mul, int sub_acc1, int sub_acc2)
v32accfloat | addmsc_elem_32_conf (v32float16 a, bfloat16 b, v32accfloat acc1, v32accfloat acc2, int zero_acc1, int sub_mul, int sub_acc1, int sub_acc2)
v32accfloat | mac_elem_32_conf (v32float16 a, float16 b, v32accfloat acc, int zero_acc, int sub_mul, int sub_acc1)
v32accfloat | msc_elem_32_conf (v32float16 a, float16 b, v32accfloat acc, int zero_acc, int sub_mul, int sub_acc1)
v32accfloat | addmac_elem_32_conf (v32float16 a, float16 b, v32accfloat acc1, v32accfloat acc2, int zero_acc1, int sub_mul, int sub_acc1, int sub_acc2)
v32accfloat | addmsc_elem_32_conf (v32float16 a, float16 b, v32accfloat acc1, v32accfloat acc2, int zero_acc1, int sub_mul, int sub_acc1, int sub_acc2)

## elem_32 with dynamic sign and dynamic negation of multiplication result
v32acc64 | mul_elem_32_conf (v32uint16 a, int sgn_x, v32uint16 b, int sgn_y, int sub_mul)
v32acc64 | negmul_elem_32_conf (v32uint16 a, int sgn_x, v32uint16 b, int sgn_y, int sub_mul)
v32acc64 | mac_elem_32_conf (v32uint16 a, int sgn_x, v32uint16 b, int sgn_y, v32acc64 acc, int zero_acc, int shift16, int sub_mul, int sub_acc1)
v32acc64 | msc_elem_32_conf (v32uint16 a, int sgn_x, v32uint16 b, int sgn_y, v32acc64 acc, int zero_acc, int shift16, int sub_mul, int sub_acc1)
v32acc64 | addmac_elem_32_conf (v32uint16 a, int sgn_x, v32uint16 b, int sgn_y, v32acc64 acc1, v32acc64 acc2, int zero_acc1, int shift16, int sub_mul, int sub_acc1, int sub_acc2)
v32acc64 | addmsc_elem_32_conf (v32uint16 a, int sgn_x, v32uint16 b, int sgn_y, v32acc64 acc1, v32acc64 acc2, int zero_acc1, int shift16, int sub_mul, int sub_acc1, int sub_acc2)
v32acc64 | mul_elem_32_conf (v32uint16 a, int sgn_x, v32int16 b, int sgn_y, int sub_mul)
v32acc64 | negmul_elem_32_conf (v32uint16 a, int sgn_x, v32int16 b, int sgn_y, int sub_mul)
v32acc64 | mac_elem_32_conf (v32uint16 a, int sgn_x, v32int16 b, int sgn_y, v32acc64 acc, int zero_acc, int shift16, int sub_mul, int sub_acc1)
v32acc64 | msc_elem_32_conf (v32uint16 a, int sgn_x, v32int16 b, int sgn_y, v32acc64 acc, int zero_acc, int shift16, int sub_mul, int sub_acc1)
v32acc64 | addmac_elem_32_conf (v32uint16 a, int sgn_x, v32int16 b, int sgn_y, v32acc64 acc1, v32acc64 acc2, int zero_acc1, int shift16, int sub_mul, int sub_acc1, int sub_acc2)
v32acc64 | addmsc_elem_32_conf (v32uint16 a, int sgn_x, v32int16 b, int sgn_y, v32acc64 acc1, v32acc64 acc2, int zero_acc1, int shift16, int sub_mul, int sub_acc1, int sub_acc2)
v32acc64 | mul_elem_32_conf (v32int16 a, int sgn_x, v32uint16 b, int sgn_y, int sub_mul)
v32acc64 | negmul_elem_32_conf (v32int16 a, int sgn_x, v32uint16 b, int sgn_y, int sub_mul)
v32acc64 | mac_elem_32_conf (v32int16 a, int sgn_x, v32uint16 b, int sgn_y, v32acc64 acc, int zero_acc, int shift16, int sub_mul, int sub_acc1)
v32acc64 | msc_elem_32_conf (v32int16 a, int sgn_x, v32uint16 b, int sgn_y, v32acc64 acc, int zero_acc, int shift16, int sub_mul, int sub_acc1)
v32acc64 | addmac_elem_32_conf (v32int16 a, int sgn_x, v32uint16 b, int sgn_y, v32acc64 acc1, v32acc64 acc2, int zero_acc1, int shift16, int sub_mul, int sub_acc1, int sub_acc2)
v32acc64 | addmsc_elem_32_conf (v32int16 a, int sgn_x, v32uint16 b, int sgn_y, v32acc64 acc1, v32acc64 acc2, int zero_acc1, int shift16, int sub_mul, int sub_acc1, int sub_acc2)
v32acc64 | mul_elem_32_conf (v32int16 a, int sgn_x, v32int16 b, int sgn_y, int sub_mul)
v32acc64 | negmul_elem_32_conf (v32int16 a, int sgn_x, v32int16 b, int sgn_y, int sub_mul)
v32acc64 | mac_elem_32_conf (v32int16 a, int sgn_x, v32int16 b, int sgn_y, v32acc64 acc, int zero_acc, int shift16, int sub_mul, int sub_acc1)
v32acc64 | msc_elem_32_conf (v32int16 a, int sgn_x, v32int16 b, int sgn_y, v32acc64 acc, int zero_acc, int shift16, int sub_mul, int sub_acc1)
v32acc64 | addmac_elem_32_conf (v32int16 a, int sgn_x, v32int16 b, int sgn_y, v32acc64 acc1, v32acc64 acc2, int zero_acc1, int shift16, int sub_mul, int sub_acc1, int sub_acc2)
v32acc64 | addmsc_elem_32_conf (v32int16 a, int sgn_x, v32int16 b, int sgn_y, v32acc64 acc1, v32acc64 acc2, int zero_acc1, int shift16, int sub_mul, int sub_acc1, int sub_acc2)
v32acc64 | mul_elem_32_conf (v32uint16 a, int sgn_x, unsigned short b, int sgn_y, int sub_mul)
v32acc64 | negmul_elem_32_conf (v32uint16 a, int sgn_x, unsigned short b, int sgn_y, int sub_mul)
v32acc64 | mac_elem_32_conf (v32uint16 a, int sgn_x, unsigned short b, int sgn_y, v32acc64 acc, int zero_acc, int shift16, int sub_mul, int sub_acc1)
v32acc64 | msc_elem_32_conf (v32uint16 a, int sgn_x, unsigned short b, int sgn_y, v32acc64 acc, int zero_acc, int shift16, int sub_mul, int sub_acc1)
v32acc64 | addmac_elem_32_conf (v32uint16 a, int sgn_x, unsigned short b, int sgn_y, v32acc64 acc1, v32acc64 acc2, int zero_acc1, int shift16, int sub_mul, int sub_acc1, int sub_acc2)
v32acc64 | addmsc_elem_32_conf (v32uint16 a, int sgn_x, unsigned short b, int sgn_y, v32acc64 acc1, v32acc64 acc2, int zero_acc1, int shift16, int sub_mul, int sub_acc1, int sub_acc2)
v32acc64 | mul_elem_32_conf (v32uint16 a, int sgn_x, signed short b, int sgn_y, int sub_mul)
v32acc64 | negmul_elem_32_conf (v32uint16 a, int sgn_x, signed short b, int sgn_y, int sub_mul)
v32acc64 | mac_elem_32_conf (v32uint16 a, int sgn_x, signed short b, int sgn_y, v32acc64 acc, int zero_acc, int shift16, int sub_mul, int sub_acc1)
v32acc64 | msc_elem_32_conf (v32uint16 a, int sgn_x, signed short b, int sgn_y, v32acc64 acc, int zero_acc, int shift16, int sub_mul, int sub_acc1)
v32acc64 | addmac_elem_32_conf (v32uint16 a, int sgn_x, signed short b, int sgn_y, v32acc64 acc1, v32acc64 acc2, int zero_acc1, int shift16, int sub_mul, int sub_acc1, int sub_acc2)
v32acc64 | addmsc_elem_32_conf (v32uint16 a, int sgn_x, signed short b, int sgn_y, v32acc64 acc1, v32acc64 acc2, int zero_acc1, int shift16, int sub_mul, int sub_acc1, int sub_acc2)
v32acc64 | mul_elem_32_conf (v32int16 a, int sgn_x, unsigned short b, int sgn_y, int sub_mul)
v32acc64 | negmul_elem_32_conf (v32int16 a, int sgn_x, unsigned short b, int sgn_y, int sub_mul)
v32acc64 | mac_elem_32_conf (v32int16 a, int sgn_x, unsigned short b, int sgn_y, v32acc64 acc, int zero_acc, int shift16, int sub_mul, int sub_acc1)
v32acc64 | msc_elem_32_conf (v32int16 a, int sgn_x, unsigned short b, int sgn_y, v32acc64 acc, int zero_acc, int shift16, int sub_mul, int sub_acc1)
v32acc64 | addmac_elem_32_conf (v32int16 a, int sgn_x, unsigned short b, int sgn_y, v32acc64 acc1, v32acc64 acc2, int zero_acc1, int shift16, int sub_mul, int sub_acc1, int sub_acc2)
v32acc64 | addmsc_elem_32_conf (v32int16 a, int sgn_x, unsigned short b, int sgn_y, v32acc64 acc1, v32acc64 acc2, int zero_acc1, int shift16, int sub_mul, int sub_acc1, int sub_acc2)
v32acc64 | mul_elem_32_conf (v32int16 a, int sgn_x, signed short b, int sgn_y, int sub_mul)
v32acc64 | negmul_elem_32_conf (v32int16 a, int sgn_x, signed short b, int sgn_y, int sub_mul)
v32acc64 | mac_elem_32_conf (v32int16 a, int sgn_x, signed short b, int sgn_y, v32acc64 acc, int zero_acc, int shift16, int sub_mul, int sub_acc1)
v32acc64 | msc_elem_32_conf (v32int16 a, int sgn_x, signed short b, int sgn_y, v32acc64 acc, int zero_acc, int shift16, int sub_mul, int sub_acc1)
v32acc64 | addmac_elem_32_conf (v32int16 a, int sgn_x, signed short b, int sgn_y, v32acc64 acc1, v32acc64 acc2, int zero_acc1, int shift16, int sub_mul, int sub_acc1, int sub_acc2)
v32acc64 | addmsc_elem_32_conf (v32int16 a, int sgn_x, signed short b, int sgn_y, v32acc64 acc1, v32acc64 acc2, int zero_acc1, int shift16, int sub_mul, int sub_acc1, int sub_acc2)
v32accfloat | mul_elem_32_conf (v32bfloat16 a, int sgn_x, v32bfloat16 b, int sgn_y, int sub_mul)
v32accfloat | negmul_elem_32_conf (v32bfloat16 a, int sgn_x, v32bfloat16 b, int sgn_y, int sub_mul)
v32accfloat | mac_elem_32_conf (v32bfloat16 a, int sgn_x, v32bfloat16 b, int sgn_y, v32accfloat acc, int zero_acc, int sub_mul, int sub_acc1)
v32accfloat | msc_elem_32_conf (v32bfloat16 a, int sgn_x, v32bfloat16 b, int sgn_y, v32accfloat acc, int zero_acc, int sub_mul, int sub_acc1)
v32accfloat | addmac_elem_32_conf (v32bfloat16 a, int sgn_x, v32bfloat16 b, int sgn_y, v32accfloat acc1, v32accfloat acc2, int zero_acc1, int sub_mul, int sub_acc1, int sub_acc2)
v32accfloat | addmsc_elem_32_conf (v32bfloat16 a, int sgn_x, v32bfloat16 b, int sgn_y, v32accfloat acc1, v32accfloat acc2, int zero_acc1, int sub_mul, int sub_acc1, int sub_acc2)
v32accfloat | mul_elem_32_conf (v32bfloat16 a, int sgn_x, v32float16 b, int sgn_y, int sub_mul)
v32accfloat | negmul_elem_32_conf (v32bfloat16 a, int sgn_x, v32float16 b, int sgn_y, int sub_mul)
v32accfloat | mac_elem_32_conf (v32bfloat16 a, int sgn_x, v32float16 b, int sgn_y, v32accfloat acc, int zero_acc, int sub_mul, int sub_acc1)
v32accfloat | msc_elem_32_conf (v32bfloat16 a, int sgn_x, v32float16 b, int sgn_y, v32accfloat acc, int zero_acc, int sub_mul, int sub_acc1)
v32accfloat | addmac_elem_32_conf (v32bfloat16 a, int sgn_x, v32float16 b, int sgn_y, v32accfloat acc1, v32accfloat acc2, int zero_acc1, int sub_mul, int sub_acc1, int sub_acc2)
v32accfloat | addmsc_elem_32_conf (v32bfloat16 a, int sgn_x, v32float16 b, int sgn_y, v32accfloat acc1, v32accfloat acc2, int zero_acc1, int sub_mul, int sub_acc1, int sub_acc2)
v32accfloat | mul_elem_32_conf (v32float16 a, int sgn_x, v32bfloat16 b, int sgn_y, int sub_mul)
v32accfloat | negmul_elem_32_conf (v32float16 a, int sgn_x, v32bfloat16 b, int sgn_y, int sub_mul)
v32accfloat | mac_elem_32_conf (v32float16 a, int sgn_x, v32bfloat16 b, int sgn_y, v32accfloat acc, int zero_acc, int sub_mul, int sub_acc1)
v32accfloat | msc_elem_32_conf (v32float16 a, int sgn_x, v32bfloat16 b, int sgn_y, v32accfloat acc, int zero_acc, int sub_mul, int sub_acc1)
v32accfloat | addmac_elem_32_conf (v32float16 a, int sgn_x, v32bfloat16 b, int sgn_y, v32accfloat acc1, v32accfloat acc2, int zero_acc1, int sub_mul, int sub_acc1, int sub_acc2)
v32accfloat | addmsc_elem_32_conf (v32float16 a, int sgn_x, v32bfloat16 b, int sgn_y, v32accfloat acc1, v32accfloat acc2, int zero_acc1, int sub_mul, int sub_acc1, int sub_acc2)
v32accfloat | mul_elem_32_conf (v32float16 a, int sgn_x, v32float16 b, int sgn_y, int sub_mul)
v32accfloat | negmul_elem_32_conf (v32float16 a, int sgn_x, v32float16 b, int sgn_y, int sub_mul)
v32accfloat | mac_elem_32_conf (v32float16 a, int sgn_x, v32float16 b, int sgn_y, v32accfloat acc, int zero_acc, int sub_mul, int sub_acc1)
v32accfloat | msc_elem_32_conf (v32float16 a, int sgn_x, v32float16 b, int sgn_y, v32accfloat acc, int zero_acc, int sub_mul, int sub_acc1)
v32accfloat | addmac_elem_32_conf (v32float16 a, int sgn_x, v32float16 b, int sgn_y, v32accfloat acc1, v32accfloat acc2, int zero_acc1, int sub_mul, int sub_acc1, int sub_acc2)
v32accfloat | addmsc_elem_32_conf (v32float16 a, int sgn_x, v32float16 b, int sgn_y, v32accfloat acc1, v32accfloat acc2, int zero_acc1, int sub_mul, int sub_acc1, int sub_acc2)
v32accfloat | mul_elem_32_conf (v32bfloat16 a, int sgn_x, bfloat16 b, int sgn_y, int sub_mul)
v32accfloat | negmul_elem_32_conf (v32bfloat16 a, int sgn_x, bfloat16 b, int sgn_y, int sub_mul)
v32accfloat | mac_elem_32_conf (v32bfloat16 a, int sgn_x, bfloat16 b, int sgn_y, v32accfloat acc, int zero_acc, int sub_mul, int sub_acc1)
v32accfloat | msc_elem_32_conf (v32bfloat16 a, int sgn_x, bfloat16 b, int sgn_y, v32accfloat acc, int zero_acc, int sub_mul, int sub_acc1)
v32accfloat | addmac_elem_32_conf (v32bfloat16 a, int sgn_x, bfloat16 b, int sgn_y, v32accfloat acc1, v32accfloat acc2, int zero_acc1, int sub_mul, int sub_acc1, int sub_acc2)
v32accfloat | addmsc_elem_32_conf (v32bfloat16 a, int sgn_x, bfloat16 b, int sgn_y, v32accfloat acc1, v32accfloat acc2, int zero_acc1, int sub_mul, int sub_acc1, int sub_acc2)
v32accfloat | mul_elem_32_conf (v32bfloat16 a, int sgn_x, float16 b, int sgn_y, int sub_mul)
v32accfloat | negmul_elem_32_conf (v32bfloat16 a, int sgn_x, float16 b, int sgn_y, int sub_mul)
v32accfloat | mac_elem_32_conf (v32bfloat16 a, int sgn_x, float16 b, int sgn_y, v32accfloat acc, int zero_acc, int sub_mul, int sub_acc1)
v32accfloat | msc_elem_32_conf (v32bfloat16 a, int sgn_x, float16 b, int sgn_y, v32accfloat acc, int zero_acc, int sub_mul, int sub_acc1)
v32accfloat | addmac_elem_32_conf (v32bfloat16 a, int sgn_x, float16 b, int sgn_y, v32accfloat acc1, v32accfloat acc2, int zero_acc1, int sub_mul, int sub_acc1, int sub_acc2)
v32accfloat | addmsc_elem_32_conf (v32bfloat16 a, int sgn_x, float16 b, int sgn_y, v32accfloat acc1, v32accfloat acc2, int zero_acc1, int sub_mul, int sub_acc1, int sub_acc2)
v32accfloat | mul_elem_32_conf (v32float16 a, int sgn_x, bfloat16 b, int sgn_y, int sub_mul)
v32accfloat | negmul_elem_32_conf (v32float16 a, int sgn_x, bfloat16 b, int sgn_y, int sub_mul)
v32accfloat | mac_elem_32_conf (v32float16 a, int sgn_x, bfloat16 b, int sgn_y, v32accfloat acc, int zero_acc, int sub_mul, int sub_acc1)
v32accfloat | msc_elem_32_conf (v32float16 a, int sgn_x, bfloat16 b, int sgn_y, v32accfloat acc, int zero_acc, int sub_mul, int sub_acc1)
v32accfloat | addmac_elem_32_conf (v32float16 a, int sgn_x, bfloat16 b, int sgn_y, v32accfloat acc1, v32accfloat acc2, int zero_acc1, int sub_mul, int sub_acc1, int sub_acc2)
v32accfloat | addmsc_elem_32_conf (v32float16 a, int sgn_x, bfloat16 b, int sgn_y, v32accfloat acc1, v32accfloat acc2, int zero_acc1, int sub_mul, int sub_acc1, int sub_acc2)
v32accfloat | mul_elem_32_conf (v32float16 a, int sgn_x, float16 b, int sgn_y, int sub_mul)
v32accfloat | negmul_elem_32_conf (v32float16 a, int sgn_x, float16 b, int sgn_y, int sub_mul)
v32accfloat | mac_elem_32_conf (v32float16 a, int sgn_x, float16 b, int sgn_y, v32accfloat acc, int zero_acc, int sub_mul, int sub_acc1)
v32accfloat | msc_elem_32_conf (v32float16 a, int sgn_x, float16 b, int sgn_y, v32accfloat acc, int zero_acc, int sub_mul, int sub_acc1)
v32accfloat | addmac_elem_32_conf (v32float16 a, int sgn_x, float16 b, int sgn_y, v32accfloat acc1, v32accfloat acc2, int zero_acc1, int sub_mul, int sub_acc1, int sub_acc2)
v32accfloat | addmsc_elem_32_conf (v32float16 a, int sgn_x, float16 b, int sgn_y, v32accfloat acc1, v32accfloat acc2, int zero_acc1, int sub_mul, int sub_acc1, int sub_acc2)

## elem_32_2
v32acc64 | mul_elem_32_2 (v64uint16 a, v64uint16 b)
v32acc64 | negmul_elem_32_2 (v64uint16 a, v64uint16 b)
v32acc64 | mac_elem_32_2 (v64uint16 a, v64uint16 b, v32acc64 acc)
v32acc64 | msc_elem_32_2 (v64uint16 a, v64uint16 b, v32acc64 acc)
v32acc64 | addmac_elem_32_2 (v64uint16 a, v64uint16 b, v32acc64 acc1, v32acc64 acc2)
v32acc64 | addmsc_elem_32_2 (v64uint16 a, v64uint16 b, v32acc64 acc1, v32acc64 acc2)
v32acc64 | mul_elem_32_2 (v64uint16 a, v64int16 b)
v32acc64 | negmul_elem_32_2 (v64uint16 a, v64int16 b)
v32acc64 | mac_elem_32_2 (v64uint16 a, v64int16 b, v32acc64 acc)
v32acc64 | msc_elem_32_2 (v64uint16 a, v64int16 b, v32acc64 acc)
v32acc64 | addmac_elem_32_2 (v64uint16 a, v64int16 b, v32acc64 acc1, v32acc64 acc2)
v32acc64 | addmsc_elem_32_2 (v64uint16 a, v64int16 b, v32acc64 acc1, v32acc64 acc2)
v32acc64 | mul_elem_32_2 (v64int16 a, v64uint16 b)
v32acc64 | negmul_elem_32_2 (v64int16 a, v64uint16 b)
v32acc64 | mac_elem_32_2 (v64int16 a, v64uint16 b, v32acc64 acc)
v32acc64 | msc_elem_32_2 (v64int16 a, v64uint16 b, v32acc64 acc)
v32acc64 | addmac_elem_32_2 (v64int16 a, v64uint16 b, v32acc64 acc1, v32acc64 acc2)
v32acc64 | addmsc_elem_32_2 (v64int16 a, v64uint16 b, v32acc64 acc1, v32acc64 acc2)
v32acc64 | mul_elem_32_2 (v64int16 a, v64int16 b)
v32acc64 | negmul_elem_32_2 (v64int16 a, v64int16 b)
v32acc64 | mac_elem_32_2 (v64int16 a, v64int16 b, v32acc64 acc)
v32acc64 | msc_elem_32_2 (v64int16 a, v64int16 b, v32acc64 acc)
v32acc64 | addmac_elem_32_2 (v64int16 a, v64int16 b, v32acc64 acc1, v32acc64 acc2)
v32acc64 | addmsc_elem_32_2 (v64int16 a, v64int16 b, v32acc64 acc1, v32acc64 acc2)

## elem_32_2 with dynamic sign
v32acc64 | mul_elem_32_2 (v64uint16 a, int sgn_x, v64uint16 b, int sgn_y)
v32acc64 | negmul_elem_32_2 (v64uint16 a, int sgn_x, v64uint16 b, int sgn_y)
v32acc64 | mac_elem_32_2 (v64uint16 a, int sgn_x, v64uint16 b, int sgn_y, v32acc64 acc)
v32acc64 | msc_elem_32_2 (v64uint16 a, int sgn_x, v64uint16 b, int sgn_y, v32acc64 acc)
v32acc64 | addmac_elem_32_2 (v64uint16 a, int sgn_x, v64uint16 b, int sgn_y, v32acc64 acc1, v32acc64 acc2)
v32acc64 | addmsc_elem_32_2 (v64uint16 a, int sgn_x, v64uint16 b, int sgn_y, v32acc64 acc1, v32acc64 acc2)
v32acc64 | mul_elem_32_2 (v64uint16 a, int sgn_x, v64int16 b, int sgn_y)
v32acc64 | negmul_elem_32_2 (v64uint16 a, int sgn_x, v64int16 b, int sgn_y)
v32acc64 | mac_elem_32_2 (v64uint16 a, int sgn_x, v64int16 b, int sgn_y, v32acc64 acc)
v32acc64 | msc_elem_32_2 (v64uint16 a, int sgn_x, v64int16 b, int sgn_y, v32acc64 acc)
v32acc64 | addmac_elem_32_2 (v64uint16 a, int sgn_x, v64int16 b, int sgn_y, v32acc64 acc1, v32acc64 acc2)
v32acc64 | addmsc_elem_32_2 (v64uint16 a, int sgn_x, v64int16 b, int sgn_y, v32acc64 acc1, v32acc64 acc2)
v32acc64 | mul_elem_32_2 (v64int16 a, int sgn_x, v64uint16 b, int sgn_y)
v32acc64 | negmul_elem_32_2 (v64int16 a, int sgn_x, v64uint16 b, int sgn_y)
v32acc64 | mac_elem_32_2 (v64int16 a, int sgn_x, v64uint16 b, int sgn_y, v32acc64 acc)
v32acc64 | msc_elem_32_2 (v64int16 a, int sgn_x, v64uint16 b, int sgn_y, v32acc64 acc)
v32acc64 | addmac_elem_32_2 (v64int16 a, int sgn_x, v64uint16 b, int sgn_y, v32acc64 acc1, v32acc64 acc2)
v32acc64 | addmsc_elem_32_2 (v64int16 a, int sgn_x, v64uint16 b, int sgn_y, v32acc64 acc1, v32acc64 acc2)
v32acc64 | mul_elem_32_2 (v64int16 a, int sgn_x, v64int16 b, int sgn_y)
v32acc64 | negmul_elem_32_2 (v64int16 a, int sgn_x, v64int16 b, int sgn_y)
v32acc64 | mac_elem_32_2 (v64int16 a, int sgn_x, v64int16 b, int sgn_y, v32acc64 acc)
v32acc64 | msc_elem_32_2 (v64int16 a, int sgn_x, v64int16 b, int sgn_y, v32acc64 acc)
v32acc64 | addmac_elem_32_2 (v64int16 a, int sgn_x, v64int16 b, int sgn_y, v32acc64 acc1, v32acc64 acc2)
v32acc64 | addmsc_elem_32_2 (v64int16 a, int sgn_x, v64int16 b, int sgn_y, v32acc64 acc1, v32acc64 acc2)

## elem_32_2 with dynamic negation of multiplication result
v32acc64 | mul_elem_32_2_conf (v64uint16 a, v64uint16 b, int sub_mul)
v32acc64 | negmul_elem_32_2_conf (v64uint16 a, v64uint16 b, int sub_mul)
v32acc64 | mul_elem_32_2_conf (v64uint16 a, v64int16 b, int sub_mul)
v32acc64 | negmul_elem_32_2_conf (v64uint16 a, v64int16 b, int sub_mul)
v32acc64 | mul_elem_32_2_conf (v64int16 a, v64uint16 b, int sub_mul)
v32acc64 | negmul_elem_32_2_conf (v64int16 a, v64uint16 b, int sub_mul)
v32acc64 | mul_elem_32_2_conf (v64int16 a, v64int16 b, int sub_mul)
v32acc64 | negmul_elem_32_2_conf (v64int16 a, v64int16 b, int sub_mul)

## elem_32_2 with dynamic negation of multiplication result, zeroing of acc1, negation of acc1
v32acc64 | mac_elem_32_2_conf (v64uint16 a, v64uint16 b, v32acc64 acc, int zero_acc, int shift16, int sub_mul, int sub_acc1)
v32acc64 | msc_elem_32_2_conf (v64uint16 a, v64uint16 b, v32acc64 acc, int zero_acc, int shift16, int sub_mul, int sub_acc1)
v32acc64 | addmac_elem_32_2_conf (v64uint16 a, v64uint16 b, v32acc64 acc1, v32acc64 acc2, int zero_acc1, int shift16, int sub_mul, int sub_acc1, int sub_acc2)
v32acc64 | addmsc_elem_32_2_conf (v64uint16 a, v64uint16 b, v32acc64 acc1, v32acc64 acc2, int zero_acc1, int shift16, int sub_mul, int sub_acc1, int sub_acc2)
v32acc64 | mac_elem_32_2_conf (v64uint16 a, v64int16 b, v32acc64 acc, int zero_acc, int shift16, int sub_mul, int sub_acc1)
v32acc64 | msc_elem_32_2_conf (v64uint16 a, v64int16 b, v32acc64 acc, int zero_acc, int shift16, int sub_mul, int sub_acc1)
v32acc64 | addmac_elem_32_2_conf (v64uint16 a, v64int16 b, v32acc64 acc1, v32acc64 acc2, int zero_acc1, int shift16, int sub_mul, int sub_acc1, int sub_acc2)
v32acc64 | addmsc_elem_32_2_conf (v64uint16 a, v64int16 b, v32acc64 acc1, v32acc64 acc2, int zero_acc1, int shift16, int sub_mul, int sub_acc1, int sub_acc2)
v32acc64 | mac_elem_32_2_conf (v64int16 a, v64uint16 b, v32acc64 acc, int zero_acc, int shift16, int sub_mul, int sub_acc1)
v32acc64 | msc_elem_32_2_conf (v64int16 a, v64uint16 b, v32acc64 acc, int zero_acc, int shift16, int sub_mul, int sub_acc1)
v32acc64 | addmac_elem_32_2_conf (v64int16 a, v64uint16 b, v32acc64 acc1, v32acc64 acc2, int zero_acc1, int shift16, int sub_mul, int sub_acc1, int sub_acc2)
v32acc64 | addmsc_elem_32_2_conf (v64int16 a, v64uint16 b, v32acc64 acc1, v32acc64 acc2, int zero_acc1, int shift16, int sub_mul, int sub_acc1, int sub_acc2)
v32acc64 | mac_elem_32_2_conf (v64int16 a, v64int16 b, v32acc64 acc, int zero_acc, int shift16, int sub_mul, int sub_acc1)
v32acc64 | msc_elem_32_2_conf (v64int16 a, v64int16 b, v32acc64 acc, int zero_acc, int shift16, int sub_mul, int sub_acc1)
v32acc64 | addmac_elem_32_2_conf (v64int16 a, v64int16 b, v32acc64 acc1, v32acc64 acc2, int zero_acc1, int shift16, int sub_mul, int sub_acc1, int sub_acc2)
v32acc64 | addmsc_elem_32_2_conf (v64int16 a, v64int16 b, v32acc64 acc1, v32acc64 acc2, int zero_acc1, int shift16, int sub_mul, int sub_acc1, int sub_acc2)

## elem_32_2 with dynamic sign and dynamic negation of multiplication result
v32acc64 | mul_elem_32_2_conf (v64uint16 a, int sgn_x, v64uint16 b, int sgn_y, int sub_mul)
v32acc64 | negmul_elem_32_2_conf (v64uint16 a, int sgn_x, v64uint16 b, int sgn_y, int sub_mul)
v32acc64 | mac_elem_32_2_conf (v64uint16 a, int sgn_x, v64uint16 b, int sgn_y, v32acc64 acc, int zero_acc, int shift16, int sub_mul, int sub_acc1)
v32acc64 | msc_elem_32_2_conf (v64uint16 a, int sgn_x, v64uint16 b, int sgn_y, v32acc64 acc, int zero_acc, int shift16, int sub_mul, int sub_acc1)
v32acc64 | addmac_elem_32_2_conf (v64uint16 a, int sgn_x, v64uint16 b, int sgn_y, v32acc64 acc1, v32acc64 acc2, int zero_acc1, int shift16, int sub_mul, int sub_acc1, int sub_acc2)
v32acc64 | addmsc_elem_32_2_conf (v64uint16 a, int sgn_x, v64uint16 b, int sgn_y, v32acc64 acc1, v32acc64 acc2, int zero_acc1, int shift16, int sub_mul, int sub_acc1, int sub_acc2)
v32acc64 | mul_elem_32_2_conf (v64uint16 a, int sgn_x, v64int16 b, int sgn_y, int sub_mul)
v32acc64 | negmul_elem_32_2_conf (v64uint16 a, int sgn_x, v64int16 b, int sgn_y, int sub_mul)
v32acc64 | mac_elem_32_2_conf (v64uint16 a, int sgn_x, v64int16 b, int sgn_y, v32acc64 acc, int zero_acc, int shift16, int sub_mul, int sub_acc1)
v32acc64 | msc_elem_32_2_conf (v64uint16 a, int sgn_x, v64int16 b, int sgn_y, v32acc64 acc, int zero_acc, int shift16, int sub_mul, int sub_acc1)
v32acc64 | addmac_elem_32_2_conf (v64uint16 a, int sgn_x, v64int16 b, int sgn_y, v32acc64 acc1, v32acc64 acc2, int zero_acc1, int shift16, int sub_mul, int sub_acc1, int sub_acc2)
v32acc64 | addmsc_elem_32_2_conf (v64uint16 a, int sgn_x, v64int16 b, int sgn_y, v32acc64 acc1, v32acc64 acc2, int zero_acc1, int shift16, int sub_mul, int sub_acc1, int sub_acc2)
v32acc64 | mul_elem_32_2_conf (v64int16 a, int sgn_x, v64uint16 b, int sgn_y, int sub_mul)
v32acc64 | negmul_elem_32_2_conf (v64int16 a, int sgn_x, v64uint16 b, int sgn_y, int sub_mul)
v32acc64 | mac_elem_32_2_conf (v64int16 a, int sgn_x, v64uint16 b, int sgn_y, v32acc64 acc, int zero_acc, int shift16, int sub_mul, int sub_acc1)
v32acc64 | msc_elem_32_2_conf (v64int16 a, int sgn_x, v64uint16 b, int sgn_y, v32acc64 acc, int zero_acc, int shift16, int sub_mul, int sub_acc1)
v32acc64 | addmac_elem_32_2_conf (v64int16 a, int sgn_x, v64uint16 b, int sgn_y, v32acc64 acc1, v32acc64 acc2, int zero_acc1, int shift16, int sub_mul, int sub_acc1, int sub_acc2)
v32acc64 | addmsc_elem_32_2_conf (v64int16 a, int sgn_x, v64uint16 b, int sgn_y, v32acc64 acc1, v32acc64 acc2, int zero_acc1, int shift16, int sub_mul, int sub_acc1, int sub_acc2)
v32acc64 | mul_elem_32_2_conf (v64int16 a, int sgn_x, v64int16 b, int sgn_y, int sub_mul)
v32acc64 | negmul_elem_32_2_conf (v64int16 a, int sgn_x, v64int16 b, int sgn_y, int sub_mul)
v32acc64 | mac_elem_32_2_conf (v64int16 a, int sgn_x, v64int16 b, int sgn_y, v32acc64 acc, int zero_acc, int shift16, int sub_mul, int sub_acc1)
v32acc64 | msc_elem_32_2_conf (v64int16 a, int sgn_x, v64int16 b, int sgn_y, v32acc64 acc, int zero_acc, int shift16, int sub_mul, int sub_acc1)
v32acc64 | addmac_elem_32_2_conf (v64int16 a, int sgn_x, v64int16 b, int sgn_y, v32acc64 acc1, v32acc64 acc2, int zero_acc1, int shift16, int sub_mul, int sub_acc1, int sub_acc2)
v32acc64 | addmsc_elem_32_2_conf (v64int16 a, int sgn_x, v64int16 b, int sgn_y, v32acc64 acc1, v32acc64 acc2, int zero_acc1, int shift16, int sub_mul, int sub_acc1, int sub_acc2)

## conv_32x4
v32acc64 | mul_conv_32x4 (v64uint16 a, v32uint16 b)
v32acc64 | negmul_conv_32x4 (v64uint16 a, v32uint16 b)
v32acc64 | mac_conv_32x4 (v64uint16 a, v32uint16 b, v32acc64 acc)
v32acc64 | msc_conv_32x4 (v64uint16 a, v32uint16 b, v32acc64 acc)
v32acc64 | addmac_conv_32x4 (v64uint16 a, v32uint16 b, v32acc64 acc1, v32acc64 acc2)
v32acc64 | addmsc_conv_32x4 (v64uint16 a, v32uint16 b, v32acc64 acc1, v32acc64 acc2)
v32acc64 | mul_conv_32x4 (v64uint16 a, v32int16 b)
v32acc64 | negmul_conv_32x4 (v64uint16 a, v32int16 b)
v32acc64 | mac_conv_32x4 (v64uint16 a, v32int16 b, v32acc64 acc)
v32acc64 | msc_conv_32x4 (v64uint16 a, v32int16 b, v32acc64 acc)
v32acc64 | addmac_conv_32x4 (v64uint16 a, v32int16 b, v32acc64 acc1, v32acc64 acc2)
v32acc64 | addmsc_conv_32x4 (v64uint16 a, v32int16 b, v32acc64 acc1, v32acc64 acc2)
v32acc64 | mul_conv_32x4 (v64int16 a, v32uint16 b)
v32acc64 | negmul_conv_32x4 (v64int16 a, v32uint16 b)
v32acc64 | mac_conv_32x4 (v64int16 a, v32uint16 b, v32acc64 acc)
v32acc64 | msc_conv_32x4 (v64int16 a, v32uint16 b, v32acc64 acc)
v32acc64 | addmac_conv_32x4 (v64int16 a, v32uint16 b, v32acc64 acc1, v32acc64 acc2)
v32acc64 | addmsc_conv_32x4 (v64int16 a, v32uint16 b, v32acc64 acc1, v32acc64 acc2)
v32acc64 | mul_conv_32x4 (v64int16 a, v32int16 b)
v32acc64 | negmul_conv_32x4 (v64int16 a, v32int16 b)
v32acc64 | mac_conv_32x4 (v64int16 a, v32int16 b, v32acc64 acc)
v32acc64 | msc_conv_32x4 (v64int16 a, v32int16 b, v32acc64 acc)
v32acc64 | addmac_conv_32x4 (v64int16 a, v32int16 b, v32acc64 acc1, v32acc64 acc2)
v32acc64 | addmsc_conv_32x4 (v64int16 a, v32int16 b, v32acc64 acc1, v32acc64 acc2)

## conv_32x4 with dynamic sign
v32acc64 | mul_conv_32x4 (v64uint16 a, int sgn_x, v32uint16 b, int sgn_y)
v32acc64 | negmul_conv_32x4 (v64uint16 a, int sgn_x, v32uint16 b, int sgn_y)
v32acc64 | mac_conv_32x4 (v64uint16 a, int sgn_x, v32uint16 b, int sgn_y, v32acc64 acc)
v32acc64 | msc_conv_32x4 (v64uint16 a, int sgn_x, v32uint16 b, int sgn_y, v32acc64 acc)
v32acc64 | addmac_conv_32x4 (v64uint16 a, int sgn_x, v32uint16 b, int sgn_y, v32acc64 acc1, v32acc64 acc2)
v32acc64 | addmsc_conv_32x4 (v64uint16 a, int sgn_x, v32uint16 b, int sgn_y, v32acc64 acc1, v32acc64 acc2)
v32acc64 | mul_conv_32x4 (v64uint16 a, int sgn_x, v32int16 b, int sgn_y)
v32acc64 | negmul_conv_32x4 (v64uint16 a, int sgn_x, v32int16 b, int sgn_y)
v32acc64 | mac_conv_32x4 (v64uint16 a, int sgn_x, v32int16 b, int sgn_y, v32acc64 acc)
v32acc64 | msc_conv_32x4 (v64uint16 a, int sgn_x, v32int16 b, int sgn_y, v32acc64 acc)
v32acc64 | addmac_conv_32x4 (v64uint16 a, int sgn_x, v32int16 b, int sgn_y, v32acc64 acc1, v32acc64 acc2)
v32acc64 | addmsc_conv_32x4 (v64uint16 a, int sgn_x, v32int16 b, int sgn_y, v32acc64 acc1, v32acc64 acc2)
v32acc64 | mul_conv_32x4 (v64int16 a, int sgn_x, v32uint16 b, int sgn_y)
v32acc64 | negmul_conv_32x4 (v64int16 a, int sgn_x, v32uint16 b, int sgn_y)
v32acc64 | mac_conv_32x4 (v64int16 a, int sgn_x, v32uint16 b, int sgn_y, v32acc64 acc)
v32acc64 | msc_conv_32x4 (v64int16 a, int sgn_x, v32uint16 b, int sgn_y, v32acc64 acc)
v32acc64 | addmac_conv_32x4 (v64int16 a, int sgn_x, v32uint16 b, int sgn_y, v32acc64 acc1, v32acc64 acc2)
v32acc64 | addmsc_conv_32x4 (v64int16 a, int sgn_x, v32uint16 b, int sgn_y, v32acc64 acc1, v32acc64 acc2)
v32acc64 | mul_conv_32x4 (v64int16 a, int sgn_x, v32int16 b, int sgn_y)
v32acc64 | negmul_conv_32x4 (v64int16 a, int sgn_x, v32int16 b, int sgn_y)
v32acc64 | mac_conv_32x4 (v64int16 a, int sgn_x, v32int16 b, int sgn_y, v32acc64 acc)
v32acc64 | msc_conv_32x4 (v64int16 a, int sgn_x, v32int16 b, int sgn_y, v32acc64 acc)
v32acc64 | addmac_conv_32x4 (v64int16 a, int sgn_x, v32int16 b, int sgn_y, v32acc64 acc1, v32acc64 acc2)
v32acc64 | addmsc_conv_32x4 (v64int16 a, int sgn_x, v32int16 b, int sgn_y, v32acc64 acc1, v32acc64 acc2)

## conv_32x4 with dynamic negation of multiplication result
v32acc64 | mul_conv_32x4_conf (v64uint16 a, v32uint16 b, int sub_mul)
v32acc64 | negmul_conv_32x4_conf (v64uint16 a, v32uint16 b, int sub_mul)
v32acc64 | mul_conv_32x4_conf (v64uint16 a, v32int16 b, int sub_mul)
v32acc64 | negmul_conv_32x4_conf (v64uint16 a, v32int16 b, int sub_mul)
v32acc64 | mul_conv_32x4_conf (v64int16 a, v32uint16 b, int sub_mul)
v32acc64 | negmul_conv_32x4_conf (v64int16 a, v32uint16 b, int sub_mul)
v32acc64 | mul_conv_32x4_conf (v64int16 a, v32int16 b, int sub_mul)
v32acc64 | negmul_conv_32x4_conf (v64int16 a, v32int16 b, int sub_mul)

## conv_32x4 with dynamic negation of multiplication result, zeroing of acc1, negation of acc1
v32acc64 | mac_conv_32x4_conf (v64uint16 a, v32uint16 b, v32acc64 acc, int zero_acc, int shift16, int sub_mul, int sub_acc1)
v32acc64 | msc_conv_32x4_conf (v64uint16 a, v32uint16 b, v32acc64 acc, int zero_acc, int shift16, int sub_mul, int sub_acc1)
v32acc64 | addmac_conv_32x4_conf (v64uint16 a, v32uint16 b, v32acc64 acc1, v32acc64 acc2, int zero_acc1, int shift16, int sub_mul, int sub_acc1, int sub_acc2)
v32acc64 | addmsc_conv_32x4_conf (v64uint16 a, v32uint16 b, v32acc64 acc1, v32acc64 acc2, int zero_acc1, int shift16, int sub_mul, int sub_acc1, int sub_acc2)
v32acc64 | mac_conv_32x4_conf (v64uint16 a, v32int16 b, v32acc64 acc, int zero_acc, int shift16, int sub_mul, int sub_acc1)
v32acc64 | msc_conv_32x4_conf (v64uint16 a, v32int16 b, v32acc64 acc, int zero_acc, int shift16, int sub_mul, int sub_acc1)
v32acc64 | addmac_conv_32x4_conf (v64uint16 a, v32int16 b, v32acc64 acc1, v32acc64 acc2, int zero_acc1, int shift16, int sub_mul, int sub_acc1, int sub_acc2)
v32acc64 | addmsc_conv_32x4_conf (v64uint16 a, v32int16 b, v32acc64 acc1, v32acc64 acc2, int zero_acc1, int shift16, int sub_mul, int sub_acc1, int sub_acc2)
v32acc64 | mac_conv_32x4_conf (v64int16 a, v32uint16 b, v32acc64 acc, int zero_acc, int shift16, int sub_mul, int sub_acc1)
v32acc64 | msc_conv_32x4_conf (v64int16 a, v32uint16 b, v32acc64 acc, int zero_acc, int shift16, int sub_mul, int sub_acc1)
v32acc64 | addmac_conv_32x4_conf (v64int16 a, v32uint16 b, v32acc64 acc1, v32acc64 acc2, int zero_acc1, int shift16, int sub_mul, int sub_acc1, int sub_acc2)
v32acc64 | addmsc_conv_32x4_conf (v64int16 a, v32uint16 b, v32acc64 acc1, v32acc64 acc2, int zero_acc1, int shift16, int sub_mul, int sub_acc1, int sub_acc2)
v32acc64 | mac_conv_32x4_conf (v64int16 a, v32int16 b, v32acc64 acc, int zero_acc, int shift16, int sub_mul, int sub_acc1)
v32acc64 | msc_conv_32x4_conf (v64int16 a, v32int16 b, v32acc64 acc, int zero_acc, int shift16, int sub_mul, int sub_acc1)
v32acc64 | addmac_conv_32x4_conf (v64int16 a, v32int16 b, v32acc64 acc1, v32acc64 acc2, int zero_acc1, int shift16, int sub_mul, int sub_acc1, int sub_acc2)
v32acc64 | addmsc_conv_32x4_conf (v64int16 a, v32int16 b, v32acc64 acc1, v32acc64 acc2, int zero_acc1, int shift16, int sub_mul, int sub_acc1, int sub_acc2)

## conv_32x4 with dynamic sign and dynamic negation of multiplication result
v32acc64 | mul_conv_32x4_conf (v64uint16 a, int sgn_x, v32uint16 b, int sgn_y, int sub_mul)
v32acc64 | negmul_conv_32x4_conf (v64uint16 a, int sgn_x, v32uint16 b, int sgn_y, int sub_mul)
v32acc64 | mac_conv_32x4_conf (v64uint16 a, int sgn_x, v32uint16 b, int sgn_y, v32acc64 acc, int zero_acc, int shift16, int sub_mul, int sub_acc1)
v32acc64 | msc_conv_32x4_conf (v64uint16 a, int sgn_x, v32uint16 b, int sgn_y, v32acc64 acc, int zero_acc, int shift16, int sub_mul, int sub_acc1)
v32acc64 | addmac_conv_32x4_conf (v64uint16 a, int sgn_x, v32uint16 b, int sgn_y, v32acc64 acc1, v32acc64 acc2, int zero_acc1, int shift16, int sub_mul, int sub_acc1, int sub_acc2)
v32acc64 | addmsc_conv_32x4_conf (v64uint16 a, int sgn_x, v32uint16 b, int sgn_y, v32acc64 acc1, v32acc64 acc2, int zero_acc1, int shift16, int sub_mul, int sub_acc1, int sub_acc2)
v32acc64 | mul_conv_32x4_conf (v64uint16 a, int sgn_x, v32int16 b, int sgn_y, int sub_mul)
v32acc64 | negmul_conv_32x4_conf (v64uint16 a, int sgn_x, v32int16 b, int sgn_y, int sub_mul)
v32acc64 | mac_conv_32x4_conf (v64uint16 a, int sgn_x, v32int16 b, int sgn_y, v32acc64 acc, int zero_acc, int shift16, int sub_mul, int sub_acc1)
v32acc64 | msc_conv_32x4_conf (v64uint16 a, int sgn_x, v32int16 b, int sgn_y, v32acc64 acc, int zero_acc, int shift16, int sub_mul, int sub_acc1)
v32acc64 | addmac_conv_32x4_conf (v64uint16 a, int sgn_x, v32int16 b, int sgn_y, v32acc64 acc1, v32acc64 acc2, int zero_acc1, int shift16, int sub_mul, int sub_acc1, int sub_acc2)
v32acc64 | addmsc_conv_32x4_conf (v64uint16 a, int sgn_x, v32int16 b, int sgn_y, v32acc64 acc1, v32acc64 acc2, int zero_acc1, int shift16, int sub_mul, int sub_acc1, int sub_acc2)
v32acc64 | mul_conv_32x4_conf (v64int16 a, int sgn_x, v32uint16 b, int sgn_y, int sub_mul)
v32acc64 | negmul_conv_32x4_conf (v64int16 a, int sgn_x, v32uint16 b, int sgn_y, int sub_mul)
v32acc64 | mac_conv_32x4_conf (v64int16 a, int sgn_x, v32uint16 b, int sgn_y, v32acc64 acc, int zero_acc, int shift16, int sub_mul, int sub_acc1)
v32acc64 | msc_conv_32x4_conf (v64int16 a, int sgn_x, v32uint16 b, int sgn_y, v32acc64 acc, int zero_acc, int shift16, int sub_mul, int sub_acc1)
v32acc64 | addmac_conv_32x4_conf (v64int16 a, int sgn_x, v32uint16 b, int sgn_y, v32acc64 acc1, v32acc64 acc2, int zero_acc1, int shift16, int sub_mul, int sub_acc1, int sub_acc2)
v32acc64 | addmsc_conv_32x4_conf (v64int16 a, int sgn_x, v32uint16 b, int sgn_y, v32acc64 acc1, v32acc64 acc2, int zero_acc1, int shift16, int sub_mul, int sub_acc1, int sub_acc2)
v32acc64 | mul_conv_32x4_conf (v64int16 a, int sgn_x, v32int16 b, int sgn_y, int sub_mul)
v32acc64 | negmul_conv_32x4_conf (v64int16 a, int sgn_x, v32int16 b, int sgn_y, int sub_mul)
v32acc64 | mac_conv_32x4_conf (v64int16 a, int sgn_x, v32int16 b, int sgn_y, v32acc64 acc, int zero_acc, int shift16, int sub_mul, int sub_acc1)
v32acc64 | msc_conv_32x4_conf (v64int16 a, int sgn_x, v32int16 b, int sgn_y, v32acc64 acc, int zero_acc, int shift16, int sub_mul, int sub_acc1)
v32acc64 | addmac_conv_32x4_conf (v64int16 a, int sgn_x, v32int16 b, int sgn_y, v32acc64 acc1, v32acc64 acc2, int zero_acc1, int shift16, int sub_mul, int sub_acc1, int sub_acc2)
v32acc64 | addmsc_conv_32x4_conf (v64int16 a, int sgn_x, v32int16 b, int sgn_y, v32acc64 acc1, v32acc64 acc2, int zero_acc1, int shift16, int sub_mul, int sub_acc1, int sub_acc2)

## conv_4x4_8ch
v32acc64 | mul_conv_4x4_8ch (v64uint16 a, v32uint16 b)
v32acc64 | negmul_conv_4x4_8ch (v64uint16 a, v32uint16 b)
v32acc64 | mac_conv_4x4_8ch (v64uint16 a, v32uint16 b, v32acc64 acc)
v32acc64 | msc_conv_4x4_8ch (v64uint16 a, v32uint16 b, v32acc64 acc)
v32acc64 | addmac_conv_4x4_8ch (v64uint16 a, v32uint16 b, v32acc64 acc1, v32acc64 acc2)
v32acc64 | addmsc_conv_4x4_8ch (v64uint16 a, v32uint16 b, v32acc64 acc1, v32acc64 acc2)
v32acc64 | mul_conv_4x4_8ch (v64uint16 a, v32int16 b)
v32acc64 | negmul_conv_4x4_8ch (v64uint16 a, v32int16 b)
v32acc64 | mac_conv_4x4_8ch (v64uint16 a, v32int16 b, v32acc64 acc)
v32acc64 | msc_conv_4x4_8ch (v64uint16 a, v32int16 b, v32acc64 acc)
v32acc64 | addmac_conv_4x4_8ch (v64uint16 a, v32int16 b, v32acc64 acc1, v32acc64 acc2)
v32acc64 | addmsc_conv_4x4_8ch (v64uint16 a, v32int16 b, v32acc64 acc1, v32acc64 acc2)
v32acc64 | mul_conv_4x4_8ch (v64int16 a, v32uint16 b)
v32acc64 | negmul_conv_4x4_8ch (v64int16 a, v32uint16 b)
v32acc64 | mac_conv_4x4_8ch (v64int16 a, v32uint16 b, v32acc64 acc)
v32acc64 | msc_conv_4x4_8ch (v64int16 a, v32uint16 b, v32acc64 acc)
v32acc64 | addmac_conv_4x4_8ch (v64int16 a, v32uint16 b, v32acc64 acc1, v32acc64 acc2)
v32acc64 | addmsc_conv_4x4_8ch (v64int16 a, v32uint16 b, v32acc64 acc1, v32acc64 acc2)
v32acc64 | mul_conv_4x4_8ch (v64int16 a, v32int16 b)
v32acc64 | negmul_conv_4x4_8ch (v64int16 a, v32int16 b)
v32acc64 | mac_conv_4x4_8ch (v64int16 a, v32int16 b, v32acc64 acc)
v32acc64 | msc_conv_4x4_8ch (v64int16 a, v32int16 b, v32acc64 acc)
v32acc64 | addmac_conv_4x4_8ch (v64int16 a, v32int16 b, v32acc64 acc1, v32acc64 acc2)
v32acc64 | addmsc_conv_4x4_8ch (v64int16 a, v32int16 b, v32acc64 acc1, v32acc64 acc2)

## conv_4x4_8ch with dynamic sign
v32acc64 | mul_conv_4x4_8ch (v64uint16 a, int sgn_x, v32uint16 b, int sgn_y)
v32acc64 | negmul_conv_4x4_8ch (v64uint16 a, int sgn_x, v32uint16 b, int sgn_y)
v32acc64 | mac_conv_4x4_8ch (v64uint16 a, int sgn_x, v32uint16 b, int sgn_y, v32acc64 acc)
v32acc64 | msc_conv_4x4_8ch (v64uint16 a, int sgn_x, v32uint16 b, int sgn_y, v32acc64 acc)
v32acc64 | addmac_conv_4x4_8ch (v64uint16 a, int sgn_x, v32uint16 b, int sgn_y, v32acc64 acc1, v32acc64 acc2)
v32acc64 | addmsc_conv_4x4_8ch (v64uint16 a, int sgn_x, v32uint16 b, int sgn_y, v32acc64 acc1, v32acc64 acc2)
v32acc64 | mul_conv_4x4_8ch (v64uint16 a, int sgn_x, v32int16 b, int sgn_y)
v32acc64 | negmul_conv_4x4_8ch (v64uint16 a, int sgn_x, v32int16 b, int sgn_y)
v32acc64 | mac_conv_4x4_8ch (v64uint16 a, int sgn_x, v32int16 b, int sgn_y, v32acc64 acc)
v32acc64 | msc_conv_4x4_8ch (v64uint16 a, int sgn_x, v32int16 b, int sgn_y, v32acc64 acc)
v32acc64 | addmac_conv_4x4_8ch (v64uint16 a, int sgn_x, v32int16 b, int sgn_y, v32acc64 acc1, v32acc64 acc2)
v32acc64 | addmsc_conv_4x4_8ch (v64uint16 a, int sgn_x, v32int16 b, int sgn_y, v32acc64 acc1, v32acc64 acc2)
v32acc64 | mul_conv_4x4_8ch (v64int16 a, int sgn_x, v32uint16 b, int sgn_y)
v32acc64 | negmul_conv_4x4_8ch (v64int16 a, int sgn_x, v32uint16 b, int sgn_y)
v32acc64 | mac_conv_4x4_8ch (v64int16 a, int sgn_x, v32uint16 b, int sgn_y, v32acc64 acc)
v32acc64 | msc_conv_4x4_8ch (v64int16 a, int sgn_x, v32uint16 b, int sgn_y, v32acc64 acc)
v32acc64 | addmac_conv_4x4_8ch (v64int16 a, int sgn_x, v32uint16 b, int sgn_y, v32acc64 acc1, v32acc64 acc2)
v32acc64 | addmsc_conv_4x4_8ch (v64int16 a, int sgn_x, v32uint16 b, int sgn_y, v32acc64 acc1, v32acc64 acc2)
v32acc64 | mul_conv_4x4_8ch (v64int16 a, int sgn_x, v32int16 b, int sgn_y)
v32acc64 | negmul_conv_4x4_8ch (v64int16 a, int sgn_x, v32int16 b, int sgn_y)
v32acc64 | mac_conv_4x4_8ch (v64int16 a, int sgn_x, v32int16 b, int sgn_y, v32acc64 acc)
v32acc64 | msc_conv_4x4_8ch (v64int16 a, int sgn_x, v32int16 b, int sgn_y, v32acc64 acc)
v32acc64 | addmac_conv_4x4_8ch (v64int16 a, int sgn_x, v32int16 b, int sgn_y, v32acc64 acc1, v32acc64 acc2)
v32acc64 | addmsc_conv_4x4_8ch (v64int16 a, int sgn_x, v32int16 b, int sgn_y, v32acc64 acc1, v32acc64 acc2)

## conv_4x4_8ch with dynamic negation of multiplication result
v32acc64 | mul_conv_4x4_8ch_conf (v64uint16 a, v32uint16 b, int sub_mul)
v32acc64 | negmul_conv_4x4_8ch_conf (v64uint16 a, v32uint16 b, int sub_mul)
v32acc64 | mul_conv_4x4_8ch_conf (v64uint16 a, v32int16 b, int sub_mul)
v32acc64 | negmul_conv_4x4_8ch_conf (v64uint16 a, v32int16 b, int sub_mul)
v32acc64 | mul_conv_4x4_8ch_conf (v64int16 a, v32uint16 b, int sub_mul)
v32acc64 | negmul_conv_4x4_8ch_conf (v64int16 a, v32uint16 b, int sub_mul)
v32acc64 | mul_conv_4x4_8ch_conf (v64int16 a, v32int16 b, int sub_mul)
v32acc64 | negmul_conv_4x4_8ch_conf (v64int16 a, v32int16 b, int sub_mul)

## conv_4x4_8ch with dynamic negation of multiplication result, zeroing of acc1, negation of acc1
v32acc64 | mac_conv_4x4_8ch_conf (v64uint16 a, v32uint16 b, v32acc64 acc, int zero_acc, int shift16, int sub_mul, int sub_acc1)
v32acc64 | msc_conv_4x4_8ch_conf (v64uint16 a, v32uint16 b, v32acc64 acc, int zero_acc, int shift16, int sub_mul, int sub_acc1)
v32acc64 | addmac_conv_4x4_8ch_conf (v64uint16 a, v32uint16 b, v32acc64 acc1, v32acc64 acc2, int zero_acc1, int shift16, int sub_mul, int sub_acc1, int sub_acc2)
v32acc64 | addmsc_conv_4x4_8ch_conf (v64uint16 a, v32uint16 b, v32acc64 acc1, v32acc64 acc2, int zero_acc1, int shift16, int sub_mul, int sub_acc1, int sub_acc2)
v32acc64 | mac_conv_4x4_8ch_conf (v64uint16 a, v32int16 b, v32acc64 acc, int zero_acc, int shift16, int sub_mul, int sub_acc1)
v32acc64 | msc_conv_4x4_8ch_conf (v64uint16 a, v32int16 b, v32acc64 acc, int zero_acc, int shift16, int sub_mul, int sub_acc1)
v32acc64 | addmac_conv_4x4_8ch_conf (v64uint16 a, v32int16 b, v32acc64 acc1, v32acc64 acc2, int zero_acc1, int shift16, int sub_mul, int sub_acc1, int sub_acc2)
v32acc64 | addmsc_conv_4x4_8ch_conf (v64uint16 a, v32int16 b, v32acc64 acc1, v32acc64 acc2, int zero_acc1, int shift16, int sub_mul, int sub_acc1, int sub_acc2)
v32acc64 | mac_conv_4x4_8ch_conf (v64int16 a, v32uint16 b, v32acc64 acc, int zero_acc, int shift16, int sub_mul, int sub_acc1)
v32acc64 | msc_conv_4x4_8ch_conf (v64int16 a, v32uint16 b, v32acc64 acc, int zero_acc, int shift16, int sub_mul, int sub_acc1)
v32acc64 | addmac_conv_4x4_8ch_conf (v64int16 a, v32uint16 b, v32acc64 acc1, v32acc64 acc2, int zero_acc1, int shift16, int sub_mul, int sub_acc1, int sub_acc2)
v32acc64 | addmsc_conv_4x4_8ch_conf (v64int16 a, v32uint16 b, v32acc64 acc1, v32acc64 acc2, int zero_acc1, int shift16, int sub_mul, int sub_acc1, int sub_acc2)
v32acc64 | mac_conv_4x4_8ch_conf (v64int16 a, v32int16 b, v32acc64 acc, int zero_acc, int shift16, int sub_mul, int sub_acc1)
v32acc64 | msc_conv_4x4_8ch_conf (v64int16 a, v32int16 b, v32acc64 acc, int zero_acc, int shift16, int sub_mul, int sub_acc1)
v32acc64 | addmac_conv_4x4_8ch_conf (v64int16 a, v32int16 b, v32acc64 acc1, v32acc64 acc2, int zero_acc1, int shift16, int sub_mul, int sub_acc1, int sub_acc2)
v32acc64 | addmsc_conv_4x4_8ch_conf (v64int16 a, v32int16 b, v32acc64 acc1, v32acc64 acc2, int zero_acc1, int shift16, int sub_mul, int sub_acc1, int sub_acc2)

## conv_4x4_8ch with dynamic sign and dynamic negation of multiplication result
v32acc64 | mul_conv_4x4_8ch_conf (v64uint16 a, int sgn_x, v32uint16 b, int sgn_y, int sub_mul)
v32acc64 | negmul_conv_4x4_8ch_conf (v64uint16 a, int sgn_x, v32uint16 b, int sgn_y, int sub_mul)
v32acc64 | mac_conv_4x4_8ch_conf (v64uint16 a, int sgn_x, v32uint16 b, int sgn_y, v32acc64 acc, int zero_acc, int shift16, int sub_mul, int sub_acc1)
v32acc64 | msc_conv_4x4_8ch_conf (v64uint16 a, int sgn_x, v32uint16 b, int sgn_y, v32acc64 acc, int zero_acc, int shift16, int sub_mul, int sub_acc1)
v32acc64 | addmac_conv_4x4_8ch_conf (v64uint16 a, int sgn_x, v32uint16 b, int sgn_y, v32acc64 acc1, v32acc64 acc2, int zero_acc1, int shift16, int sub_mul, int sub_acc1, int sub_acc2)
v32acc64 | addmsc_conv_4x4_8ch_conf (v64uint16 a, int sgn_x, v32uint16 b, int sgn_y, v32acc64 acc1, v32acc64 acc2, int zero_acc1, int shift16, int sub_mul, int sub_acc1, int sub_acc2)
v32acc64 | mul_conv_4x4_8ch_conf (v64uint16 a, int sgn_x, v32int16 b, int sgn_y, int sub_mul)
v32acc64 | negmul_conv_4x4_8ch_conf (v64uint16 a, int sgn_x, v32int16 b, int sgn_y, int sub_mul)
v32acc64 | mac_conv_4x4_8ch_conf (v64uint16 a, int sgn_x, v32int16 b, int sgn_y, v32acc64 acc, int zero_acc, int shift16, int sub_mul, int sub_acc1)
v32acc64 | msc_conv_4x4_8ch_conf (v64uint16 a, int sgn_x, v32int16 b, int sgn_y, v32acc64 acc, int zero_acc, int shift16, int sub_mul, int sub_acc1)
v32acc64 | addmac_conv_4x4_8ch_conf (v64uint16 a, int sgn_x, v32int16 b, int sgn_y, v32acc64 acc1, v32acc64 acc2, int zero_acc1, int shift16, int sub_mul, int sub_acc1, int sub_acc2)
v32acc64 | addmsc_conv_4x4_8ch_conf (v64uint16 a, int sgn_x, v32int16 b, int sgn_y, v32acc64 acc1, v32acc64 acc2, int zero_acc1, int shift16, int sub_mul, int sub_acc1, int sub_acc2)
v32acc64 | mul_conv_4x4_8ch_conf (v64int16 a, int sgn_x, v32uint16 b, int sgn_y, int sub_mul)
v32acc64 | negmul_conv_4x4_8ch_conf (v64int16 a, int sgn_x, v32uint16 b, int sgn_y, int sub_mul)
v32acc64 | mac_conv_4x4_8ch_conf (v64int16 a, int sgn_x, v32uint16 b, int sgn_y, v32acc64 acc, int zero_acc, int shift16, int sub_mul, int sub_acc1)
v32acc64 | msc_conv_4x4_8ch_conf (v64int16 a, int sgn_x, v32uint16 b, int sgn_y, v32acc64 acc, int zero_acc, int shift16, int sub_mul, int sub_acc1)
v32acc64 | addmac_conv_4x4_8ch_conf (v64int16 a, int sgn_x, v32uint16 b, int sgn_y, v32acc64 acc1, v32acc64 acc2, int zero_acc1, int shift16, int sub_mul, int sub_acc1, int sub_acc2)
v32acc64 | addmsc_conv_4x4_8ch_conf (v64int16 a, int sgn_x, v32uint16 b, int sgn_y, v32acc64 acc1, v32acc64 acc2, int zero_acc1, int shift16, int sub_mul, int sub_acc1, int sub_acc2)
v32acc64 | mul_conv_4x4_8ch_conf (v64int16 a, int sgn_x, v32int16 b, int sgn_y, int sub_mul)
v32acc64 | negmul_conv_4x4_8ch_conf (v64int16 a, int sgn_x, v32int16 b, int sgn_y, int sub_mul)
v32acc64 | mac_conv_4x4_8ch_conf (v64int16 a, int sgn_x, v32int16 b, int sgn_y, v32acc64 acc, int zero_acc, int shift16, int sub_mul, int sub_acc1)
v32acc64 | msc_conv_4x4_8ch_conf (v64int16 a, int sgn_x, v32int16 b, int sgn_y, v32acc64 acc, int zero_acc, int shift16, int sub_mul, int sub_acc1)
v32acc64 | addmac_conv_4x4_8ch_conf (v64int16 a, int sgn_x, v32int16 b, int sgn_y, v32acc64 acc1, v32acc64 acc2, int zero_acc1, int shift16, int sub_mul, int sub_acc1, int sub_acc2)
v32acc64 | addmsc_conv_4x4_8ch_conf (v64int16 a, int sgn_x, v32int16 b, int sgn_y, v32acc64 acc1, v32acc64 acc2, int zero_acc1, int shift16, int sub_mul, int sub_acc1, int sub_acc2)

## Detailed Description

## Function Documentation

## ◆ addmac_4x4_4x8() [1/8]

v32acc64 addmac_4x4_4x8 | ( | v32int16 | a,
|  | int | sgn_x,
|  | v32int16 | b,
|  | int | sgn_y,
|  | v32acc64 | acc1,
|  | v32acc64 | acc2 )

## ◆ addmac_4x4_4x8() [2/8]

v32acc64 addmac_4x4_4x8 | ( | v32int16 | a,
|  | int | sgn_x,
|  | v32uint16 | b,
|  | int | sgn_y,
|  | v32acc64 | acc1,
|  | v32acc64 | acc2 )

## ◆ addmac_4x4_4x8() [3/8]

v32acc64 addmac_4x4_4x8 | ( | v32int16 | a,
|  | v32int16 | b,
|  | v32acc64 | acc1,
|  | v32acc64 | acc2 )

## ◆ addmac_4x4_4x8() [4/8]

v32acc64 addmac_4x4_4x8 | ( | v32int16 | a,
|  | v32uint16 | b,
|  | v32acc64 | acc1,
|  | v32acc64 | acc2 )

## ◆ addmac_4x4_4x8() [5/8]

v32acc64 addmac_4x4_4x8 | ( | v32uint16 | a,
|  | int | sgn_x,
|  | v32int16 | b,
|  | int | sgn_y,
|  | v32acc64 | acc1,
|  | v32acc64 | acc2 )

## ◆ addmac_4x4_4x8() [6/8]

v32acc64 addmac_4x4_4x8 | ( | v32uint16 | a,
|  | int | sgn_x,
|  | v32uint16 | b,
|  | int | sgn_y,
|  | v32acc64 | acc1,
|  | v32acc64 | acc2 )

## ◆ addmac_4x4_4x8() [7/8]

v32acc64 addmac_4x4_4x8 | ( | v32uint16 | a,
|  | v32int16 | b,
|  | v32acc64 | acc1,
|  | v32acc64 | acc2 )

## ◆ addmac_4x4_4x8() [8/8]

v32acc64 addmac_4x4_4x8 | ( | v32uint16 | a,
|  | v32uint16 | b,
|  | v32acc64 | acc1,
|  | v32acc64 | acc2 )

## ◆ addmac_4x4_4x8_conf() [1/8]

v32acc64 addmac_4x4_4x8_conf | ( | v32int16 | a,
|  | int | sgn_x,
|  | v32int16 | b,
|  | int | sgn_y,
|  | v32acc64 | acc1,
|  | v32acc64 | acc2,
|  | int | zero_acc1,
|  | int | shift16,
|  | int | sub_mul,
|  | int | sub_acc1,
|  | int | sub_acc2 )

## ◆ addmac_4x4_4x8_conf() [2/8]

v32acc64 addmac_4x4_4x8_conf | ( | v32int16 | a,
|  | int | sgn_x,
|  | v32uint16 | b,
|  | int | sgn_y,
|  | v32acc64 | acc1,
|  | v32acc64 | acc2,
|  | int | zero_acc1,
|  | int | shift16,
|  | int | sub_mul,
|  | int | sub_acc1,
|  | int | sub_acc2 )

## ◆ addmac_4x4_4x8_conf() [3/8]

v32acc64 addmac_4x4_4x8_conf | ( | v32int16 | a,
|  | v32int16 | b,
|  | v32acc64 | acc1,
|  | v32acc64 | acc2,
|  | int | zero_acc1,
|  | int | shift16,
|  | int | sub_mul,
|  | int | sub_acc1,
|  | int | sub_acc2 )

## ◆ addmac_4x4_4x8_conf() [4/8]

v32acc64 addmac_4x4_4x8_conf | ( | v32int16 | a,
|  | v32uint16 | b,
|  | v32acc64 | acc1,
|  | v32acc64 | acc2,
|  | int | zero_acc1,
|  | int | shift16,
|  | int | sub_mul,
|  | int | sub_acc1,
|  | int | sub_acc2 )

## ◆ addmac_4x4_4x8_conf() [5/8]

v32acc64 addmac_4x4_4x8_conf | ( | v32uint16 | a,
|  | int | sgn_x,
|  | v32int16 | b,
|  | int | sgn_y,
|  | v32acc64 | acc1,
|  | v32acc64 | acc2,
|  | int | zero_acc1,
|  | int | shift16,
|  | int | sub_mul,
|  | int | sub_acc1,
|  | int | sub_acc2 )

## ◆ addmac_4x4_4x8_conf() [6/8]

v32acc64 addmac_4x4_4x8_conf | ( | v32uint16 | a,
|  | int | sgn_x,
|  | v32uint16 | b,
|  | int | sgn_y,
|  | v32acc64 | acc1,
|  | v32acc64 | acc2,
|  | int | zero_acc1,
|  | int | shift16,
|  | int | sub_mul,
|  | int | sub_acc1,
|  | int | sub_acc2 )

## ◆ addmac_4x4_4x8_conf() [7/8]

v32acc64 addmac_4x4_4x8_conf | ( | v32uint16 | a,
|  | v32int16 | b,
|  | v32acc64 | acc1,
|  | v32acc64 | acc2,
|  | int | zero_acc1,
|  | int | shift16,
|  | int | sub_mul,
|  | int | sub_acc1,
|  | int | sub_acc2 )

## ◆ addmac_4x4_4x8_conf() [8/8]

v32acc64 addmac_4x4_4x8_conf | ( | v32uint16 | a,
|  | v32uint16 | b,
|  | v32acc64 | acc1,
|  | v32acc64 | acc2,
|  | int | zero_acc1,
|  | int | shift16,
|  | int | sub_mul,
|  | int | sub_acc1,
|  | int | sub_acc2 )

## ◆ addmac_8x2_2x8() [1/8]

v64acc32 addmac_8x2_2x8 | ( | v32int16 | a,
|  | int | sgn_x,
|  | v32int16 | b,
|  | int | sgn_y,
|  | v64acc32 | acc1,
|  | v64acc32 | acc2 )

## ◆ addmac_8x2_2x8() [2/8]

v64acc32 addmac_8x2_2x8 | ( | v32int16 | a,
|  | int | sgn_x,
|  | v32uint16 | b,
|  | int | sgn_y,
|  | v64acc32 | acc1,
|  | v64acc32 | acc2 )

## ◆ addmac_8x2_2x8() [3/8]

v64acc32 addmac_8x2_2x8 | ( | v32int16 | a,
|  | v32int16 | b,
|  | v64acc32 | acc1,
|  | v64acc32 | acc2 )

## ◆ addmac_8x2_2x8() [4/8]

v64acc32 addmac_8x2_2x8 | ( | v32int16 | a,
|  | v32uint16 | b,
|  | v64acc32 | acc1,
|  | v64acc32 | acc2 )

## ◆ addmac_8x2_2x8() [5/8]

v64acc32 addmac_8x2_2x8 | ( | v32uint16 | a,
|  | int | sgn_x,
|  | v32int16 | b,
|  | int | sgn_y,
|  | v64acc32 | acc1,
|  | v64acc32 | acc2 )

## ◆ addmac_8x2_2x8() [6/8]

v64acc32 addmac_8x2_2x8 | ( | v32uint16 | a,
|  | int | sgn_x,
|  | v32uint16 | b,
|  | int | sgn_y,
|  | v64acc32 | acc1,
|  | v64acc32 | acc2 )

## ◆ addmac_8x2_2x8() [7/8]

v64acc32 addmac_8x2_2x8 | ( | v32uint16 | a,
|  | v32int16 | b,
|  | v64acc32 | acc1,
|  | v64acc32 | acc2 )

## ◆ addmac_8x2_2x8() [8/8]

v64acc32 addmac_8x2_2x8 | ( | v32uint16 | a,
|  | v32uint16 | b,
|  | v64acc32 | acc1,
|  | v64acc32 | acc2 )

## ◆ addmac_8x2_2x8_conf() [1/8]

v64acc32 addmac_8x2_2x8_conf | ( | v32int16 | a,
|  | int | sgn_x,
|  | v32int16 | b,
|  | int | sgn_y,
|  | v64acc32 | acc1,
|  | v64acc32 | acc2,
|  | int | zero_acc1,
|  | int | shift16,
|  | int | sub_mul,
|  | int | sub_acc1,
|  | int | sub_acc2 )

## ◆ addmac_8x2_2x8_conf() [2/8]

v64acc32 addmac_8x2_2x8_conf | ( | v32int16 | a,
|  | int | sgn_x,
|  | v32uint16 | b,
|  | int | sgn_y,
|  | v64acc32 | acc1,
|  | v64acc32 | acc2,
|  | int | zero_acc1,
|  | int | shift16,
|  | int | sub_mul,
|  | int | sub_acc1,
|  | int | sub_acc2 )

## ◆ addmac_8x2_2x8_conf() [3/8]

v64acc32 addmac_8x2_2x8_conf | ( | v32int16 | a,
|  | v32int16 | b,
|  | v64acc32 | acc1,
|  | v64acc32 | acc2,
|  | int | zero_acc1,
|  | int | shift16,
|  | int | sub_mul,
|  | int | sub_acc1,
|  | int | sub_acc2 )

## ◆ addmac_8x2_2x8_conf() [4/8]

v64acc32 addmac_8x2_2x8_conf | ( | v32int16 | a,
|  | v32uint16 | b,
|  | v64acc32 | acc1,
|  | v64acc32 | acc2,
|  | int | zero_acc1,
|  | int | shift16,
|  | int | sub_mul,
|  | int | sub_acc1,
|  | int | sub_acc2 )

## ◆ addmac_8x2_2x8_conf() [5/8]

v64acc32 addmac_8x2_2x8_conf | ( | v32uint16 | a,
|  | int | sgn_x,
|  | v32int16 | b,
|  | int | sgn_y,
|  | v64acc32 | acc1,
|  | v64acc32 | acc2,
|  | int | zero_acc1,
|  | int | shift16,
|  | int | sub_mul,
|  | int | sub_acc1,
|  | int | sub_acc2 )

## ◆ addmac_8x2_2x8_conf() [6/8]

v64acc32 addmac_8x2_2x8_conf | ( | v32uint16 | a,
|  | int | sgn_x,
|  | v32uint16 | b,
|  | int | sgn_y,
|  | v64acc32 | acc1,
|  | v64acc32 | acc2,
|  | int | zero_acc1,
|  | int | shift16,
|  | int | sub_mul,
|  | int | sub_acc1,
|  | int | sub_acc2 )

## ◆ addmac_8x2_2x8_conf() [7/8]

v64acc32 addmac_8x2_2x8_conf | ( | v32uint16 | a,
|  | v32int16 | b,
|  | v64acc32 | acc1,
|  | v64acc32 | acc2,
|  | int | zero_acc1,
|  | int | shift16,
|  | int | sub_mul,
|  | int | sub_acc1,
|  | int | sub_acc2 )

## ◆ addmac_8x2_2x8_conf() [8/8]

v64acc32 addmac_8x2_2x8_conf | ( | v32uint16 | a,
|  | v32uint16 | b,
|  | v64acc32 | acc1,
|  | v64acc32 | acc2,
|  | int | zero_acc1,
|  | int | shift16,
|  | int | sub_mul,
|  | int | sub_acc1,
|  | int | sub_acc2 )

## ◆ addmac_conv_32x4() [1/8]

v32acc64 addmac_conv_32x4 | ( | v64int16 | a,
|  | int | sgn_x,
|  | v32int16 | b,
|  | int | sgn_y,
|  | v32acc64 | acc1,
|  | v32acc64 | acc2 )

## ◆ addmac_conv_32x4() [2/8]

v32acc64 addmac_conv_32x4 | ( | v64int16 | a,
|  | int | sgn_x,
|  | v32uint16 | b,
|  | int | sgn_y,
|  | v32acc64 | acc1,
|  | v32acc64 | acc2 )

## ◆ addmac_conv_32x4() [3/8]

v32acc64 addmac_conv_32x4 | ( | v64int16 | a,
|  | v32int16 | b,
|  | v32acc64 | acc1,
|  | v32acc64 | acc2 )

## ◆ addmac_conv_32x4() [4/8]

v32acc64 addmac_conv_32x4 | ( | v64int16 | a,
|  | v32uint16 | b,
|  | v32acc64 | acc1,
|  | v32acc64 | acc2 )

## ◆ addmac_conv_32x4() [5/8]

v32acc64 addmac_conv_32x4 | ( | v64uint16 | a,
|  | int | sgn_x,
|  | v32int16 | b,
|  | int | sgn_y,
|  | v32acc64 | acc1,
|  | v32acc64 | acc2 )

## ◆ addmac_conv_32x4() [6/8]

v32acc64 addmac_conv_32x4 | ( | v64uint16 | a,
|  | int | sgn_x,
|  | v32uint16 | b,
|  | int | sgn_y,
|  | v32acc64 | acc1,
|  | v32acc64 | acc2 )

## ◆ addmac_conv_32x4() [7/8]

v32acc64 addmac_conv_32x4 | ( | v64uint16 | a,
|  | v32int16 | b,
|  | v32acc64 | acc1,
|  | v32acc64 | acc2 )

## ◆ addmac_conv_32x4() [8/8]

v32acc64 addmac_conv_32x4 | ( | v64uint16 | a,
|  | v32uint16 | b,
|  | v32acc64 | acc1,
|  | v32acc64 | acc2 )

## ◆ addmac_conv_32x4_conf() [1/8]

v32acc64 addmac_conv_32x4_conf | ( | v64int16 | a,
|  | int | sgn_x,
|  | v32int16 | b,
|  | int | sgn_y,
|  | v32acc64 | acc1,
|  | v32acc64 | acc2,
|  | int | zero_acc1,
|  | int | shift16,
|  | int | sub_mul,
|  | int | sub_acc1,
|  | int | sub_acc2 )

## ◆ addmac_conv_32x4_conf() [2/8]

v32acc64 addmac_conv_32x4_conf | ( | v64int16 | a,
|  | int | sgn_x,
|  | v32uint16 | b,
|  | int | sgn_y,
|  | v32acc64 | acc1,
|  | v32acc64 | acc2,
|  | int | zero_acc1,
|  | int | shift16,
|  | int | sub_mul,
|  | int | sub_acc1,
|  | int | sub_acc2 )

## ◆ addmac_conv_32x4_conf() [3/8]

v32acc64 addmac_conv_32x4_conf | ( | v64int16 | a,
|  | v32int16 | b,
|  | v32acc64 | acc1,
|  | v32acc64 | acc2,
|  | int | zero_acc1,
|  | int | shift16,
|  | int | sub_mul,
|  | int | sub_acc1,
|  | int | sub_acc2 )

## ◆ addmac_conv_32x4_conf() [4/8]

v32acc64 addmac_conv_32x4_conf | ( | v64int16 | a,
|  | v32uint16 | b,
|  | v32acc64 | acc1,
|  | v32acc64 | acc2,
|  | int | zero_acc1,
|  | int | shift16,
|  | int | sub_mul,
|  | int | sub_acc1,
|  | int | sub_acc2 )

## ◆ addmac_conv_32x4_conf() [5/8]

v32acc64 addmac_conv_32x4_conf | ( | v64uint16 | a,
|  | int | sgn_x,
|  | v32int16 | b,
|  | int | sgn_y,
|  | v32acc64 | acc1,
|  | v32acc64 | acc2,
|  | int | zero_acc1,
|  | int | shift16,
|  | int | sub_mul,
|  | int | sub_acc1,
|  | int | sub_acc2 )

## ◆ addmac_conv_32x4_conf() [6/8]

v32acc64 addmac_conv_32x4_conf | ( | v64uint16 | a,
|  | int | sgn_x,
|  | v32uint16 | b,
|  | int | sgn_y,
|  | v32acc64 | acc1,
|  | v32acc64 | acc2,
|  | int | zero_acc1,
|  | int | shift16,
|  | int | sub_mul,
|  | int | sub_acc1,
|  | int | sub_acc2 )

## ◆ addmac_conv_32x4_conf() [7/8]

v32acc64 addmac_conv_32x4_conf | ( | v64uint16 | a,
|  | v32int16 | b,
|  | v32acc64 | acc1,
|  | v32acc64 | acc2,
|  | int | zero_acc1,
|  | int | shift16,
|  | int | sub_mul,
|  | int | sub_acc1,
|  | int | sub_acc2 )

## ◆ addmac_conv_32x4_conf() [8/8]

v32acc64 addmac_conv_32x4_conf | ( | v64uint16 | a,
|  | v32uint16 | b,
|  | v32acc64 | acc1,
|  | v32acc64 | acc2,
|  | int | zero_acc1,
|  | int | shift16,
|  | int | sub_mul,
|  | int | sub_acc1,
|  | int | sub_acc2 )

## ◆ addmac_conv_4x4_8ch() [1/8]

v32acc64 addmac_conv_4x4_8ch | ( | v64int16 | a,
|  | int | sgn_x,
|  | v32int16 | b,
|  | int | sgn_y,
|  | v32acc64 | acc1,
|  | v32acc64 | acc2 )

## ◆ addmac_conv_4x4_8ch() [2/8]

v32acc64 addmac_conv_4x4_8ch | ( | v64int16 | a,
|  | int | sgn_x,
|  | v32uint16 | b,
|  | int | sgn_y,
|  | v32acc64 | acc1,
|  | v32acc64 | acc2 )

## ◆ addmac_conv_4x4_8ch() [3/8]

v32acc64 addmac_conv_4x4_8ch | ( | v64int16 | a,
|  | v32int16 | b,
|  | v32acc64 | acc1,
|  | v32acc64 | acc2 )

## ◆ addmac_conv_4x4_8ch() [4/8]

v32acc64 addmac_conv_4x4_8ch | ( | v64int16 | a,
|  | v32uint16 | b,
|  | v32acc64 | acc1,
|  | v32acc64 | acc2 )

## ◆ addmac_conv_4x4_8ch() [5/8]

v32acc64 addmac_conv_4x4_8ch | ( | v64uint16 | a,
|  | int | sgn_x,
|  | v32int16 | b,
|  | int | sgn_y,
|  | v32acc64 | acc1,
|  | v32acc64 | acc2 )

## ◆ addmac_conv_4x4_8ch() [6/8]

v32acc64 addmac_conv_4x4_8ch | ( | v64uint16 | a,
|  | int | sgn_x,
|  | v32uint16 | b,
|  | int | sgn_y,
|  | v32acc64 | acc1,
|  | v32acc64 | acc2 )

## ◆ addmac_conv_4x4_8ch() [7/8]

v32acc64 addmac_conv_4x4_8ch | ( | v64uint16 | a,
|  | v32int16 | b,
|  | v32acc64 | acc1,
|  | v32acc64 | acc2 )

## ◆ addmac_conv_4x4_8ch() [8/8]

v32acc64 addmac_conv_4x4_8ch | ( | v64uint16 | a,
|  | v32uint16 | b,
|  | v32acc64 | acc1,
|  | v32acc64 | acc2 )

## ◆ addmac_conv_4x4_8ch_conf() [1/8]

v32acc64 addmac_conv_4x4_8ch_conf | ( | v64int16 | a,
|  | int | sgn_x,
|  | v32int16 | b,
|  | int | sgn_y,
|  | v32acc64 | acc1,
|  | v32acc64 | acc2,
|  | int | zero_acc1,
|  | int | shift16,
|  | int | sub_mul,
|  | int | sub_acc1,
|  | int | sub_acc2 )

## ◆ addmac_conv_4x4_8ch_conf() [2/8]

v32acc64 addmac_conv_4x4_8ch_conf | ( | v64int16 | a,
|  | int | sgn_x,
|  | v32uint16 | b,
|  | int | sgn_y,
|  | v32acc64 | acc1,
|  | v32acc64 | acc2,
|  | int | zero_acc1,
|  | int | shift16,
|  | int | sub_mul,
|  | int | sub_acc1,
|  | int | sub_acc2 )

## ◆ addmac_conv_4x4_8ch_conf() [3/8]

v32acc64 addmac_conv_4x4_8ch_conf | ( | v64int16 | a,
|  | v32int16 | b,
|  | v32acc64 | acc1,
|  | v32acc64 | acc2,
|  | int | zero_acc1,
|  | int | shift16,
|  | int | sub_mul,
|  | int | sub_acc1,
|  | int | sub_acc2 )

## ◆ addmac_conv_4x4_8ch_conf() [4/8]

v32acc64 addmac_conv_4x4_8ch_conf | ( | v64int16 | a,
|  | v32uint16 | b,
|  | v32acc64 | acc1,
|  | v32acc64 | acc2,
|  | int | zero_acc1,
|  | int | shift16,
|  | int | sub_mul,
|  | int | sub_acc1,
|  | int | sub_acc2 )

## ◆ addmac_conv_4x4_8ch_conf() [5/8]

v32acc64 addmac_conv_4x4_8ch_conf | ( | v64uint16 | a,
|  | int | sgn_x,
|  | v32int16 | b,
|  | int | sgn_y,
|  | v32acc64 | acc1,
|  | v32acc64 | acc2,
|  | int | zero_acc1,
|  | int | shift16,
|  | int | sub_mul,
|  | int | sub_acc1,
|  | int | sub_acc2 )

## ◆ addmac_conv_4x4_8ch_conf() [6/8]

v32acc64 addmac_conv_4x4_8ch_conf | ( | v64uint16 | a,
|  | int | sgn_x,
|  | v32uint16 | b,
|  | int | sgn_y,
|  | v32acc64 | acc1,
|  | v32acc64 | acc2,
|  | int | zero_acc1,
|  | int | shift16,
|  | int | sub_mul,
|  | int | sub_acc1,
|  | int | sub_acc2 )

## ◆ addmac_conv_4x4_8ch_conf() [7/8]

v32acc64 addmac_conv_4x4_8ch_conf | ( | v64uint16 | a,
|  | v32int16 | b,
|  | v32acc64 | acc1,
|  | v32acc64 | acc2,
|  | int | zero_acc1,
|  | int | shift16,
|  | int | sub_mul,
|  | int | sub_acc1,
|  | int | sub_acc2 )

## ◆ addmac_conv_4x4_8ch_conf() [8/8]

v32acc64 addmac_conv_4x4_8ch_conf | ( | v64uint16 | a,
|  | v32uint16 | b,
|  | v32acc64 | acc1,
|  | v32acc64 | acc2,
|  | int | zero_acc1,
|  | int | shift16,
|  | int | sub_mul,
|  | int | sub_acc1,
|  | int | sub_acc2 )

## ◆ addmac_elem_32() [1/32]

v32accfloat addmac_elem_32 | ( | v32bfloat16 | a,
|  | bfloat16 | b,
|  | v32accfloat | acc1,
|  | v32accfloat | acc2 )

## ◆ addmac_elem_32() [2/32]

v32accfloat addmac_elem_32 | ( | v32bfloat16 | a,
|  | float16 | b,
|  | v32accfloat | acc1,
|  | v32accfloat | acc2 )

## ◆ addmac_elem_32() [3/32]

v32accfloat addmac_elem_32 | ( | v32bfloat16 | a,
|  | int | sgn_x,
|  | bfloat16 | b,
|  | int | sgn_y,
|  | v32accfloat | acc1,
|  | v32accfloat | acc2 )

## ◆ addmac_elem_32() [4/32]

v32accfloat addmac_elem_32 | ( | v32bfloat16 | a,
|  | int | sgn_x,
|  | float16 | b,
|  | int | sgn_y,
|  | v32accfloat | acc1,
|  | v32accfloat | acc2 )

## ◆ addmac_elem_32() [5/32]

v32accfloat addmac_elem_32 | ( | v32bfloat16 | a,
|  | int | sgn_x,
|  | v32bfloat16 | b,
|  | int | sgn_y,
|  | v32accfloat | acc1,
|  | v32accfloat | acc2 )

## ◆ addmac_elem_32() [6/32]

v32accfloat addmac_elem_32 | ( | v32bfloat16 | a,
|  | int | sgn_x,
|  | v32float16 | b,
|  | int | sgn_y,
|  | v32accfloat | acc1,
|  | v32accfloat | acc2 )

## ◆ addmac_elem_32() [7/32]

v32accfloat addmac_elem_32 | ( | v32bfloat16 | a,
|  | v32bfloat16 | b,
|  | v32accfloat | acc1,
|  | v32accfloat | acc2 )

## ◆ addmac_elem_32() [8/32]

v32accfloat addmac_elem_32 | ( | v32bfloat16 | a,
|  | v32float16 | b,
|  | v32accfloat | acc1,
|  | v32accfloat | acc2 )

## ◆ addmac_elem_32() [9/32]

v32accfloat addmac_elem_32 | ( | v32float16 | a,
|  | bfloat16 | b,
|  | v32accfloat | acc1,
|  | v32accfloat | acc2 )

## ◆ addmac_elem_32() [10/32]

v32accfloat addmac_elem_32 | ( | v32float16 | a,
|  | float16 | b,
|  | v32accfloat | acc1,
|  | v32accfloat | acc2 )

## ◆ addmac_elem_32() [11/32]

v32accfloat addmac_elem_32 | ( | v32float16 | a,
|  | int | sgn_x,
|  | bfloat16 | b,
|  | int | sgn_y,
|  | v32accfloat | acc1,
|  | v32accfloat | acc2 )

## ◆ addmac_elem_32() [12/32]

v32accfloat addmac_elem_32 | ( | v32float16 | a,
|  | int | sgn_x,
|  | float16 | b,
|  | int | sgn_y,
|  | v32accfloat | acc1,
|  | v32accfloat | acc2 )

## ◆ addmac_elem_32() [13/32]

v32accfloat addmac_elem_32 | ( | v32float16 | a,
|  | int | sgn_x,
|  | v32bfloat16 | b,
|  | int | sgn_y,
|  | v32accfloat | acc1,
|  | v32accfloat | acc2 )

## ◆ addmac_elem_32() [14/32]

v32accfloat addmac_elem_32 | ( | v32float16 | a,
|  | int | sgn_x,
|  | v32float16 | b,
|  | int | sgn_y,
|  | v32accfloat | acc1,
|  | v32accfloat | acc2 )

## ◆ addmac_elem_32() [15/32]

v32accfloat addmac_elem_32 | ( | v32float16 | a,
|  | v32bfloat16 | b,
|  | v32accfloat | acc1,
|  | v32accfloat | acc2 )

## ◆ addmac_elem_32() [16/32]

v32accfloat addmac_elem_32 | ( | v32float16 | a,
|  | v32float16 | b,
|  | v32accfloat | acc1,
|  | v32accfloat | acc2 )

## ◆ addmac_elem_32() [17/32]

v32acc64 addmac_elem_32 | ( | v32int16 | a,
|  | int | sgn_x,
|  | signed short | b,
|  | int | sgn_y,
|  | v32acc64 | acc1,
|  | v32acc64 | acc2 )

## ◆ addmac_elem_32() [18/32]

v32acc64 addmac_elem_32 | ( | v32int16 | a,
|  | int | sgn_x,
|  | unsigned short | b,
|  | int | sgn_y,
|  | v32acc64 | acc1,
|  | v32acc64 | acc2 )

## ◆ addmac_elem_32() [19/32]

v32acc64 addmac_elem_32 | ( | v32int16 | a,
|  | int | sgn_x,
|  | v32int16 | b,
|  | int | sgn_y,
|  | v32acc64 | acc1,
|  | v32acc64 | acc2 )

## ◆ addmac_elem_32() [20/32]

v32acc64 addmac_elem_32 | ( | v32int16 | a,
|  | int | sgn_x,
|  | v32uint16 | b,
|  | int | sgn_y,
|  | v32acc64 | acc1,
|  | v32acc64 | acc2 )

## ◆ addmac_elem_32() [21/32]

v32acc64 addmac_elem_32 | ( | v32int16 | a,
|  | signed short | b,
|  | v32acc64 | acc1,
|  | v32acc64 | acc2 )

## ◆ addmac_elem_32() [22/32]

v32acc64 addmac_elem_32 | ( | v32int16 | a,
|  | unsigned short | b,
|  | v32acc64 | acc1,
|  | v32acc64 | acc2 )

## ◆ addmac_elem_32() [23/32]

v32acc64 addmac_elem_32 | ( | v32int16 | a,
|  | v32int16 | b,
|  | v32acc64 | acc1,
|  | v32acc64 | acc2 )

## ◆ addmac_elem_32() [24/32]

v32acc64 addmac_elem_32 | ( | v32int16 | a,
|  | v32uint16 | b,
|  | v32acc64 | acc1,
|  | v32acc64 | acc2 )

## ◆ addmac_elem_32() [25/32]

v32acc64 addmac_elem_32 | ( | v32uint16 | a,
|  | int | sgn_x,
|  | signed short | b,
|  | int | sgn_y,
|  | v32acc64 | acc1,
|  | v32acc64 | acc2 )

## ◆ addmac_elem_32() [26/32]

v32acc64 addmac_elem_32 | ( | v32uint16 | a,
|  | int | sgn_x,
|  | unsigned short | b,
|  | int | sgn_y,
|  | v32acc64 | acc1,
|  | v32acc64 | acc2 )

## ◆ addmac_elem_32() [27/32]

v32acc64 addmac_elem_32 | ( | v32uint16 | a,
|  | int | sgn_x,
|  | v32int16 | b,
|  | int | sgn_y,
|  | v32acc64 | acc1,
|  | v32acc64 | acc2 )

## ◆ addmac_elem_32() [28/32]

v32acc64 addmac_elem_32 | ( | v32uint16 | a,
|  | int | sgn_x,
|  | v32uint16 | b,
|  | int | sgn_y,
|  | v32acc64 | acc1,
|  | v32acc64 | acc2 )

## ◆ addmac_elem_32() [29/32]

v32acc64 addmac_elem_32 | ( | v32uint16 | a,
|  | signed short | b,
|  | v32acc64 | acc1,
|  | v32acc64 | acc2 )

## ◆ addmac_elem_32() [30/32]

v32acc64 addmac_elem_32 | ( | v32uint16 | a,
|  | unsigned short | b,
|  | v32acc64 | acc1,
|  | v32acc64 | acc2 )

## ◆ addmac_elem_32() [31/32]

v32acc64 addmac_elem_32 | ( | v32uint16 | a,
|  | v32int16 | b,
|  | v32acc64 | acc1,
|  | v32acc64 | acc2 )

## ◆ addmac_elem_32() [32/32]

v32acc64 addmac_elem_32 | ( | v32uint16 | a,
|  | v32uint16 | b,
|  | v32acc64 | acc1,
|  | v32acc64 | acc2 )

## ◆ addmac_elem_32_2() [1/8]

v32acc64 addmac_elem_32_2 | ( | v64int16 | a,
|  | int | sgn_x,
|  | v64int16 | b,
|  | int | sgn_y,
|  | v32acc64 | acc1,
|  | v32acc64 | acc2 )

## ◆ addmac_elem_32_2() [2/8]

v32acc64 addmac_elem_32_2 | ( | v64int16 | a,
|  | int | sgn_x,
|  | v64uint16 | b,
|  | int | sgn_y,
|  | v32acc64 | acc1,
|  | v32acc64 | acc2 )

## ◆ addmac_elem_32_2() [3/8]

v32acc64 addmac_elem_32_2 | ( | v64int16 | a,
|  | v64int16 | b,
|  | v32acc64 | acc1,
|  | v32acc64 | acc2 )

## ◆ addmac_elem_32_2() [4/8]

v32acc64 addmac_elem_32_2 | ( | v64int16 | a,
|  | v64uint16 | b,
|  | v32acc64 | acc1,
|  | v32acc64 | acc2 )

## ◆ addmac_elem_32_2() [5/8]

v32acc64 addmac_elem_32_2 | ( | v64uint16 | a,
|  | int | sgn_x,
|  | v64int16 | b,
|  | int | sgn_y,
|  | v32acc64 | acc1,
|  | v32acc64 | acc2 )

## ◆ addmac_elem_32_2() [6/8]

v32acc64 addmac_elem_32_2 | ( | v64uint16 | a,
|  | int | sgn_x,
|  | v64uint16 | b,
|  | int | sgn_y,
|  | v32acc64 | acc1,
|  | v32acc64 | acc2 )

## ◆ addmac_elem_32_2() [7/8]

v32acc64 addmac_elem_32_2 | ( | v64uint16 | a,
|  | v64int16 | b,
|  | v32acc64 | acc1,
|  | v32acc64 | acc2 )

## ◆ addmac_elem_32_2() [8/8]

v32acc64 addmac_elem_32_2 | ( | v64uint16 | a,
|  | v64uint16 | b,
|  | v32acc64 | acc1,
|  | v32acc64 | acc2 )

## ◆ addmac_elem_32_2_conf() [1/8]

v32acc64 addmac_elem_32_2_conf | ( | v64int16 | a,
|  | int | sgn_x,
|  | v64int16 | b,
|  | int | sgn_y,
|  | v32acc64 | acc1,
|  | v32acc64 | acc2,
|  | int | zero_acc1,
|  | int | shift16,
|  | int | sub_mul,
|  | int | sub_acc1,
|  | int | sub_acc2 )

## ◆ addmac_elem_32_2_conf() [2/8]

v32acc64 addmac_elem_32_2_conf | ( | v64int16 | a,
|  | int | sgn_x,
|  | v64uint16 | b,
|  | int | sgn_y,
|  | v32acc64 | acc1,
|  | v32acc64 | acc2,
|  | int | zero_acc1,
|  | int | shift16,
|  | int | sub_mul,
|  | int | sub_acc1,
|  | int | sub_acc2 )

## ◆ addmac_elem_32_2_conf() [3/8]

v32acc64 addmac_elem_32_2_conf | ( | v64int16 | a,
|  | v64int16 | b,
|  | v32acc64 | acc1,
|  | v32acc64 | acc2,
|  | int | zero_acc1,
|  | int | shift16,
|  | int | sub_mul,
|  | int | sub_acc1,
|  | int | sub_acc2 )

## ◆ addmac_elem_32_2_conf() [4/8]

v32acc64 addmac_elem_32_2_conf | ( | v64int16 | a,
|  | v64uint16 | b,
|  | v32acc64 | acc1,
|  | v32acc64 | acc2,
|  | int | zero_acc1,
|  | int | shift16,
|  | int | sub_mul,
|  | int | sub_acc1,
|  | int | sub_acc2 )

## ◆ addmac_elem_32_2_conf() [5/8]

v32acc64 addmac_elem_32_2_conf | ( | v64uint16 | a,
|  | int | sgn_x,
|  | v64int16 | b,
|  | int | sgn_y,
|  | v32acc64 | acc1,
|  | v32acc64 | acc2,
|  | int | zero_acc1,
|  | int | shift16,
|  | int | sub_mul,
|  | int | sub_acc1,
|  | int | sub_acc2 )

## ◆ addmac_elem_32_2_conf() [6/8]

v32acc64 addmac_elem_32_2_conf | ( | v64uint16 | a,
|  | int | sgn_x,
|  | v64uint16 | b,
|  | int | sgn_y,
|  | v32acc64 | acc1,
|  | v32acc64 | acc2,
|  | int | zero_acc1,
|  | int | shift16,
|  | int | sub_mul,
|  | int | sub_acc1,
|  | int | sub_acc2 )

## ◆ addmac_elem_32_2_conf() [7/8]

v32acc64 addmac_elem_32_2_conf | ( | v64uint16 | a,
|  | v64int16 | b,
|  | v32acc64 | acc1,
|  | v32acc64 | acc2,
|  | int | zero_acc1,
|  | int | shift16,
|  | int | sub_mul,
|  | int | sub_acc1,
|  | int | sub_acc2 )

## ◆ addmac_elem_32_2_conf() [8/8]

v32acc64 addmac_elem_32_2_conf | ( | v64uint16 | a,
|  | v64uint16 | b,
|  | v32acc64 | acc1,
|  | v32acc64 | acc2,
|  | int | zero_acc1,
|  | int | shift16,
|  | int | sub_mul,
|  | int | sub_acc1,
|  | int | sub_acc2 )

## ◆ addmac_elem_32_32b() [1/8]

v32acc32 addmac_elem_32_32b | ( | v32int16 | a,
|  | int | sgn_x,
|  | v32int16 | b,
|  | int | sgn_y,
|  | v32acc32 | acc1,
|  | v32acc32 | acc2 )

## ◆ addmac_elem_32_32b() [2/8]

v32acc32 addmac_elem_32_32b | ( | v32int16 | a,
|  | int | sgn_x,
|  | v32uint16 | b,
|  | int | sgn_y,
|  | v32acc32 | acc1,
|  | v32acc32 | acc2 )

## ◆ addmac_elem_32_32b() [3/8]

v32acc32 addmac_elem_32_32b | ( | v32int16 | a,
|  | v32int16 | b,
|  | v32acc32 | acc1,
|  | v32acc32 | acc2 )

## ◆ addmac_elem_32_32b() [4/8]

v32acc32 addmac_elem_32_32b | ( | v32int16 | a,
|  | v32uint16 | b,
|  | v32acc32 | acc1,
|  | v32acc32 | acc2 )

## ◆ addmac_elem_32_32b() [5/8]

v32acc32 addmac_elem_32_32b | ( | v32uint16 | a,
|  | int | sgn_x,
|  | v32int16 | b,
|  | int | sgn_y,
|  | v32acc32 | acc1,
|  | v32acc32 | acc2 )

## ◆ addmac_elem_32_32b() [6/8]

v32acc32 addmac_elem_32_32b | ( | v32uint16 | a,
|  | int | sgn_x,
|  | v32uint16 | b,
|  | int | sgn_y,
|  | v32acc32 | acc1,
|  | v32acc32 | acc2 )

## ◆ addmac_elem_32_32b() [7/8]

v32acc32 addmac_elem_32_32b | ( | v32uint16 | a,
|  | v32int16 | b,
|  | v32acc32 | acc1,
|  | v32acc32 | acc2 )

## ◆ addmac_elem_32_32b() [8/8]

v32acc32 addmac_elem_32_32b | ( | v32uint16 | a,
|  | v32uint16 | b,
|  | v32acc32 | acc1,
|  | v32acc32 | acc2 )

## ◆ addmac_elem_32_32b_conf() [1/8]

v32acc32 addmac_elem_32_32b_conf | ( | v32int16 | a,
|  | int | sgn_x,
|  | v32int16 | b,
|  | int | sgn_y,
|  | v32acc32 | acc1,
|  | v32acc32 | acc2,
|  | int | zero_acc1,
|  | int | shift16,
|  | int | sub_mul,
|  | int | sub_acc1,
|  | int | sub_acc2 )

## ◆ addmac_elem_32_32b_conf() [2/8]

v32acc32 addmac_elem_32_32b_conf | ( | v32int16 | a,
|  | int | sgn_x,
|  | v32uint16 | b,
|  | int | sgn_y,
|  | v32acc32 | acc1,
|  | v32acc32 | acc2,
|  | int | zero_acc1,
|  | int | shift16,
|  | int | sub_mul,
|  | int | sub_acc1,
|  | int | sub_acc2 )

## ◆ addmac_elem_32_32b_conf() [3/8]

v32acc32 addmac_elem_32_32b_conf | ( | v32int16 | a,
|  | v32int16 | b,
|  | v32acc32 | acc1,
|  | v32acc32 | acc2,
|  | int | zero_acc1,
|  | int | shift16,
|  | int | sub_mul,
|  | int | sub_acc1,
|  | int | sub_acc2 )

## ◆ addmac_elem_32_32b_conf() [4/8]

v32acc32 addmac_elem_32_32b_conf | ( | v32int16 | a,
|  | v32uint16 | b,
|  | v32acc32 | acc1,
|  | v32acc32 | acc2,
|  | int | zero_acc1,
|  | int | shift16,
|  | int | sub_mul,
|  | int | sub_acc1,
|  | int | sub_acc2 )

## ◆ addmac_elem_32_32b_conf() [5/8]

v32acc32 addmac_elem_32_32b_conf | ( | v32uint16 | a,
|  | int | sgn_x,
|  | v32int16 | b,
|  | int | sgn_y,
|  | v32acc32 | acc1,
|  | v32acc32 | acc2,
|  | int | zero_acc1,
|  | int | shift16,
|  | int | sub_mul,
|  | int | sub_acc1,
|  | int | sub_acc2 )

## ◆ addmac_elem_32_32b_conf() [6/8]

v32acc32 addmac_elem_32_32b_conf | ( | v32uint16 | a,
|  | int | sgn_x,
|  | v32uint16 | b,
|  | int | sgn_y,
|  | v32acc32 | acc1,
|  | v32acc32 | acc2,
|  | int | zero_acc1,
|  | int | shift16,
|  | int | sub_mul,
|  | int | sub_acc1,
|  | int | sub_acc2 )

## ◆ addmac_elem_32_32b_conf() [7/8]

v32acc32 addmac_elem_32_32b_conf | ( | v32uint16 | a,
|  | v32int16 | b,
|  | v32acc32 | acc1,
|  | v32acc32 | acc2,
|  | int | zero_acc1,
|  | int | shift16,
|  | int | sub_mul,
|  | int | sub_acc1,
|  | int | sub_acc2 )

## ◆ addmac_elem_32_32b_conf() [8/8]

v32acc32 addmac_elem_32_32b_conf | ( | v32uint16 | a,
|  | v32uint16 | b,
|  | v32acc32 | acc1,
|  | v32acc32 | acc2,
|  | int | zero_acc1,
|  | int | shift16,
|  | int | sub_mul,
|  | int | sub_acc1,
|  | int | sub_acc2 )

## ◆ addmac_elem_32_conf() [1/32]

v32accfloat addmac_elem_32_conf | ( | v32bfloat16 | a,
|  | bfloat16 | b,
|  | v32accfloat | acc1,
|  | v32accfloat | acc2,
|  | int | zero_acc1,
|  | int | sub_mul,
|  | int | sub_acc1,
|  | int | sub_acc2 )

## ◆ addmac_elem_32_conf() [2/32]

v32accfloat addmac_elem_32_conf | ( | v32bfloat16 | a,
|  | float16 | b,
|  | v32accfloat | acc1,
|  | v32accfloat | acc2,
|  | int | zero_acc1,
|  | int | sub_mul,
|  | int | sub_acc1,
|  | int | sub_acc2 )

## ◆ addmac_elem_32_conf() [3/32]

v32accfloat addmac_elem_32_conf | ( | v32bfloat16 | a,
|  | int | sgn_x,
|  | bfloat16 | b,
|  | int | sgn_y,
|  | v32accfloat | acc1,
|  | v32accfloat | acc2,
|  | int | zero_acc1,
|  | int | sub_mul,
|  | int | sub_acc1,
|  | int | sub_acc2 )

## ◆ addmac_elem_32_conf() [4/32]

v32accfloat addmac_elem_32_conf | ( | v32bfloat16 | a,
|  | int | sgn_x,
|  | float16 | b,
|  | int | sgn_y,
|  | v32accfloat | acc1,
|  | v32accfloat | acc2,
|  | int | zero_acc1,
|  | int | sub_mul,
|  | int | sub_acc1,
|  | int | sub_acc2 )

## ◆ addmac_elem_32_conf() [5/32]

v32accfloat addmac_elem_32_conf | ( | v32bfloat16 | a,
|  | int | sgn_x,
|  | v32bfloat16 | b,
|  | int | sgn_y,
|  | v32accfloat | acc1,
|  | v32accfloat | acc2,
|  | int | zero_acc1,
|  | int | sub_mul,
|  | int | sub_acc1,
|  | int | sub_acc2 )

## ◆ addmac_elem_32_conf() [6/32]

v32accfloat addmac_elem_32_conf | ( | v32bfloat16 | a,
|  | int | sgn_x,
|  | v32float16 | b,
|  | int | sgn_y,
|  | v32accfloat | acc1,
|  | v32accfloat | acc2,
|  | int | zero_acc1,
|  | int | sub_mul,
|  | int | sub_acc1,
|  | int | sub_acc2 )

## ◆ addmac_elem_32_conf() [7/32]

v32accfloat addmac_elem_32_conf | ( | v32bfloat16 | a,
|  | v32bfloat16 | b,
|  | v32accfloat | acc1,
|  | v32accfloat | acc2,
|  | int | zero_acc1,
|  | int | sub_mul,
|  | int | sub_acc1,
|  | int | sub_acc2 )

## ◆ addmac_elem_32_conf() [8/32]

v32accfloat addmac_elem_32_conf | ( | v32bfloat16 | a,
|  | v32float16 | b,
|  | v32accfloat | acc1,
|  | v32accfloat | acc2,
|  | int | zero_acc1,
|  | int | sub_mul,
|  | int | sub_acc1,
|  | int | sub_acc2 )

## ◆ addmac_elem_32_conf() [9/32]

v32accfloat addmac_elem_32_conf | ( | v32float16 | a,
|  | bfloat16 | b,
|  | v32accfloat | acc1,
|  | v32accfloat | acc2,
|  | int | zero_acc1,
|  | int | sub_mul,
|  | int | sub_acc1,
|  | int | sub_acc2 )

## ◆ addmac_elem_32_conf() [10/32]

v32accfloat addmac_elem_32_conf | ( | v32float16 | a,
|  | float16 | b,
|  | v32accfloat | acc1,
|  | v32accfloat | acc2,
|  | int | zero_acc1,
|  | int | sub_mul,
|  | int | sub_acc1,
|  | int | sub_acc2 )

## ◆ addmac_elem_32_conf() [11/32]

v32accfloat addmac_elem_32_conf | ( | v32float16 | a,
|  | int | sgn_x,
|  | bfloat16 | b,
|  | int | sgn_y,
|  | v32accfloat | acc1,
|  | v32accfloat | acc2,
|  | int | zero_acc1,
|  | int | sub_mul,
|  | int | sub_acc1,
|  | int | sub_acc2 )

## ◆ addmac_elem_32_conf() [12/32]

v32accfloat addmac_elem_32_conf | ( | v32float16 | a,
|  | int | sgn_x,
|  | float16 | b,
|  | int | sgn_y,
|  | v32accfloat | acc1,
|  | v32accfloat | acc2,
|  | int | zero_acc1,
|  | int | sub_mul,
|  | int | sub_acc1,
|  | int | sub_acc2 )

## ◆ addmac_elem_32_conf() [13/32]

v32accfloat addmac_elem_32_conf | ( | v32float16 | a,
|  | int | sgn_x,
|  | v32bfloat16 | b,
|  | int | sgn_y,
|  | v32accfloat | acc1,
|  | v32accfloat | acc2,
|  | int | zero_acc1,
|  | int | sub_mul,
|  | int | sub_acc1,
|  | int | sub_acc2 )

## ◆ addmac_elem_32_conf() [14/32]

v32accfloat addmac_elem_32_conf | ( | v32float16 | a,
|  | int | sgn_x,
|  | v32float16 | b,
|  | int | sgn_y,
|  | v32accfloat | acc1,
|  | v32accfloat | acc2,
|  | int | zero_acc1,
|  | int | sub_mul,
|  | int | sub_acc1,
|  | int | sub_acc2 )

## ◆ addmac_elem_32_conf() [15/32]

v32accfloat addmac_elem_32_conf | ( | v32float16 | a,
|  | v32bfloat16 | b,
|  | v32accfloat | acc1,
|  | v32accfloat | acc2,
|  | int | zero_acc1,
|  | int | sub_mul,
|  | int | sub_acc1,
|  | int | sub_acc2 )

## ◆ addmac_elem_32_conf() [16/32]

v32accfloat addmac_elem_32_conf | ( | v32float16 | a,
|  | v32float16 | b,
|  | v32accfloat | acc1,
|  | v32accfloat | acc2,
|  | int | zero_acc1,
|  | int | sub_mul,
|  | int | sub_acc1,
|  | int | sub_acc2 )

## ◆ addmac_elem_32_conf() [17/32]

v32acc64 addmac_elem_32_conf | ( | v32int16 | a,
|  | int | sgn_x,
|  | signed short | b,
|  | int | sgn_y,
|  | v32acc64 | acc1,
|  | v32acc64 | acc2,
|  | int | zero_acc1,
|  | int | shift16,
|  | int | sub_mul,
|  | int | sub_acc1,
|  | int | sub_acc2 )

## ◆ addmac_elem_32_conf() [18/32]

v32acc64 addmac_elem_32_conf | ( | v32int16 | a,
|  | int | sgn_x,
|  | unsigned short | b,
|  | int | sgn_y,
|  | v32acc64 | acc1,
|  | v32acc64 | acc2,
|  | int | zero_acc1,
|  | int | shift16,
|  | int | sub_mul,
|  | int | sub_acc1,
|  | int | sub_acc2 )

## ◆ addmac_elem_32_conf() [19/32]

v32acc64 addmac_elem_32_conf | ( | v32int16 | a,
|  | int | sgn_x,
|  | v32int16 | b,
|  | int | sgn_y,
|  | v32acc64 | acc1,
|  | v32acc64 | acc2,
|  | int | zero_acc1,
|  | int | shift16,
|  | int | sub_mul,
|  | int | sub_acc1,
|  | int | sub_acc2 )

## ◆ addmac_elem_32_conf() [20/32]

v32acc64 addmac_elem_32_conf | ( | v32int16 | a,
|  | int | sgn_x,
|  | v32uint16 | b,
|  | int | sgn_y,
|  | v32acc64 | acc1,
|  | v32acc64 | acc2,
|  | int | zero_acc1,
|  | int | shift16,
|  | int | sub_mul,
|  | int | sub_acc1,
|  | int | sub_acc2 )

## ◆ addmac_elem_32_conf() [21/32]

v32acc64 addmac_elem_32_conf | ( | v32int16 | a,
|  | signed short | b,
|  | v32acc64 | acc1,
|  | v32acc64 | acc2,
|  | int | zero_acc1,
|  | int | shift16,
|  | int | sub_mul,
|  | int | sub_acc1,
|  | int | sub_acc2 )

## ◆ addmac_elem_32_conf() [22/32]

v32acc64 addmac_elem_32_conf | ( | v32int16 | a,
|  | unsigned short | b,
|  | v32acc64 | acc1,
|  | v32acc64 | acc2,
|  | int | zero_acc1,
|  | int | shift16,
|  | int | sub_mul,
|  | int | sub_acc1,
|  | int | sub_acc2 )

## ◆ addmac_elem_32_conf() [23/32]

v32acc64 addmac_elem_32_conf | ( | v32int16 | a,
|  | v32int16 | b,
|  | v32acc64 | acc1,
|  | v32acc64 | acc2,
|  | int | zero_acc1,
|  | int | shift16,
|  | int | sub_mul,
|  | int | sub_acc1,
|  | int | sub_acc2 )

## ◆ addmac_elem_32_conf() [24/32]

v32acc64 addmac_elem_32_conf | ( | v32int16 | a,
|  | v32uint16 | b,
|  | v32acc64 | acc1,
|  | v32acc64 | acc2,
|  | int | zero_acc1,
|  | int | shift16,
|  | int | sub_mul,
|  | int | sub_acc1,
|  | int | sub_acc2 )

## ◆ addmac_elem_32_conf() [25/32]

v32acc64 addmac_elem_32_conf | ( | v32uint16 | a,
|  | int | sgn_x,
|  | signed short | b,
|  | int | sgn_y,
|  | v32acc64 | acc1,
|  | v32acc64 | acc2,
|  | int | zero_acc1,
|  | int | shift16,
|  | int | sub_mul,
|  | int | sub_acc1,
|  | int | sub_acc2 )

## ◆ addmac_elem_32_conf() [26/32]

v32acc64 addmac_elem_32_conf | ( | v32uint16 | a,
|  | int | sgn_x,
|  | unsigned short | b,
|  | int | sgn_y,
|  | v32acc64 | acc1,
|  | v32acc64 | acc2,
|  | int | zero_acc1,
|  | int | shift16,
|  | int | sub_mul,
|  | int | sub_acc1,
|  | int | sub_acc2 )

## ◆ addmac_elem_32_conf() [27/32]

v32acc64 addmac_elem_32_conf | ( | v32uint16 | a,
|  | int | sgn_x,
|  | v32int16 | b,
|  | int | sgn_y,
|  | v32acc64 | acc1,
|  | v32acc64 | acc2,
|  | int | zero_acc1,
|  | int | shift16,
|  | int | sub_mul,
|  | int | sub_acc1,
|  | int | sub_acc2 )

## ◆ addmac_elem_32_conf() [28/32]

v32acc64 addmac_elem_32_conf | ( | v32uint16 | a,
|  | int | sgn_x,
|  | v32uint16 | b,
|  | int | sgn_y,
|  | v32acc64 | acc1,
|  | v32acc64 | acc2,
|  | int | zero_acc1,
|  | int | shift16,
|  | int | sub_mul,
|  | int | sub_acc1,
|  | int | sub_acc2 )

## ◆ addmac_elem_32_conf() [29/32]

v32acc64 addmac_elem_32_conf | ( | v32uint16 | a,
|  | signed short | b,
|  | v32acc64 | acc1,
|  | v32acc64 | acc2,
|  | int | zero_acc1,
|  | int | shift16,
|  | int | sub_mul,
|  | int | sub_acc1,
|  | int | sub_acc2 )

## ◆ addmac_elem_32_conf() [30/32]

v32acc64 addmac_elem_32_conf | ( | v32uint16 | a,
|  | unsigned short | b,
|  | v32acc64 | acc1,
|  | v32acc64 | acc2,
|  | int | zero_acc1,
|  | int | shift16,
|  | int | sub_mul,
|  | int | sub_acc1,
|  | int | sub_acc2 )

## ◆ addmac_elem_32_conf() [31/32]

v32acc64 addmac_elem_32_conf | ( | v32uint16 | a,
|  | v32int16 | b,
|  | v32acc64 | acc1,
|  | v32acc64 | acc2,
|  | int | zero_acc1,
|  | int | shift16,
|  | int | sub_mul,
|  | int | sub_acc1,
|  | int | sub_acc2 )

## ◆ addmac_elem_32_conf() [32/32]

v32acc64 addmac_elem_32_conf | ( | v32uint16 | a,
|  | v32uint16 | b,
|  | v32acc64 | acc1,
|  | v32acc64 | acc2,
|  | int | zero_acc1,
|  | int | shift16,
|  | int | sub_mul,
|  | int | sub_acc1,
|  | int | sub_acc2 )

## ◆ addmac_elem_64() [1/8]

v64acc32 addmac_elem_64 | ( | v64int16 | a,
|  | int | sgn_x,
|  | v64int16 | b,
|  | int | sgn_y,
|  | v64acc32 | acc1,
|  | v64acc32 | acc2 )

## ◆ addmac_elem_64() [2/8]

v64acc32 addmac_elem_64 | ( | v64int16 | a,
|  | int | sgn_x,
|  | v64uint16 | b,
|  | int | sgn_y,
|  | v64acc32 | acc1,
|  | v64acc32 | acc2 )

## ◆ addmac_elem_64() [3/8]

v64acc32 addmac_elem_64 | ( | v64int16 | a,
|  | v64int16 | b,
|  | v64acc32 | acc1,
|  | v64acc32 | acc2 )

## ◆ addmac_elem_64() [4/8]

v64acc32 addmac_elem_64 | ( | v64int16 | a,
|  | v64uint16 | b,
|  | v64acc32 | acc1,
|  | v64acc32 | acc2 )

## ◆ addmac_elem_64() [5/8]

v64acc32 addmac_elem_64 | ( | v64uint16 | a,
|  | int | sgn_x,
|  | v64int16 | b,
|  | int | sgn_y,
|  | v64acc32 | acc1,
|  | v64acc32 | acc2 )

## ◆ addmac_elem_64() [6/8]

v64acc32 addmac_elem_64 | ( | v64uint16 | a,
|  | int | sgn_x,
|  | v64uint16 | b,
|  | int | sgn_y,
|  | v64acc32 | acc1,
|  | v64acc32 | acc2 )

## ◆ addmac_elem_64() [7/8]

v64acc32 addmac_elem_64 | ( | v64uint16 | a,
|  | v64int16 | b,
|  | v64acc32 | acc1,
|  | v64acc32 | acc2 )

## ◆ addmac_elem_64() [8/8]

v64acc32 addmac_elem_64 | ( | v64uint16 | a,
|  | v64uint16 | b,
|  | v64acc32 | acc1,
|  | v64acc32 | acc2 )

## ◆ addmac_elem_64_conf() [1/8]

v64acc32 addmac_elem_64_conf | ( | v64int16 | a,
|  | int | sgn_x,
|  | v64int16 | b,
|  | int | sgn_y,
|  | v64acc32 | acc1,
|  | v64acc32 | acc2,
|  | int | zero_acc1,
|  | int | shift16,
|  | int | sub_mul,
|  | int | sub_acc1,
|  | int | sub_acc2 )

## ◆ addmac_elem_64_conf() [2/8]

v64acc32 addmac_elem_64_conf | ( | v64int16 | a,
|  | int | sgn_x,
|  | v64uint16 | b,
|  | int | sgn_y,
|  | v64acc32 | acc1,
|  | v64acc32 | acc2,
|  | int | zero_acc1,
|  | int | shift16,
|  | int | sub_mul,
|  | int | sub_acc1,
|  | int | sub_acc2 )

## ◆ addmac_elem_64_conf() [3/8]

v64acc32 addmac_elem_64_conf | ( | v64int16 | a,
|  | v64int16 | b,
|  | v64acc32 | acc1,
|  | v64acc32 | acc2,
|  | int | zero_acc1,
|  | int | shift16,
|  | int | sub_mul,
|  | int | sub_acc1,
|  | int | sub_acc2 )

## ◆ addmac_elem_64_conf() [4/8]

v64acc32 addmac_elem_64_conf | ( | v64int16 | a,
|  | v64uint16 | b,
|  | v64acc32 | acc1,
|  | v64acc32 | acc2,
|  | int | zero_acc1,
|  | int | shift16,
|  | int | sub_mul,
|  | int | sub_acc1,
|  | int | sub_acc2 )

## ◆ addmac_elem_64_conf() [5/8]

v64acc32 addmac_elem_64_conf | ( | v64uint16 | a,
|  | int | sgn_x,
|  | v64int16 | b,
|  | int | sgn_y,
|  | v64acc32 | acc1,
|  | v64acc32 | acc2,
|  | int | zero_acc1,
|  | int | shift16,
|  | int | sub_mul,
|  | int | sub_acc1,
|  | int | sub_acc2 )

## ◆ addmac_elem_64_conf() [6/8]

v64acc32 addmac_elem_64_conf | ( | v64uint16 | a,
|  | int | sgn_x,
|  | v64uint16 | b,
|  | int | sgn_y,
|  | v64acc32 | acc1,
|  | v64acc32 | acc2,
|  | int | zero_acc1,
|  | int | shift16,
|  | int | sub_mul,
|  | int | sub_acc1,
|  | int | sub_acc2 )

## ◆ addmac_elem_64_conf() [7/8]

v64acc32 addmac_elem_64_conf | ( | v64uint16 | a,
|  | v64int16 | b,
|  | v64acc32 | acc1,
|  | v64acc32 | acc2,
|  | int | zero_acc1,
|  | int | shift16,
|  | int | sub_mul,
|  | int | sub_acc1,
|  | int | sub_acc2 )

## ◆ addmac_elem_64_conf() [8/8]

v64acc32 addmac_elem_64_conf | ( | v64uint16 | a,
|  | v64uint16 | b,
|  | v64acc32 | acc1,
|  | v64acc32 | acc2,
|  | int | zero_acc1,
|  | int | shift16,
|  | int | sub_mul,
|  | int | sub_acc1,
|  | int | sub_acc2 )

## ◆ addmsc_4x4_4x8() [1/8]

v32acc64 addmsc_4x4_4x8 | ( | v32int16 | a,
|  | int | sgn_x,
|  | v32int16 | b,
|  | int | sgn_y,
|  | v32acc64 | acc1,
|  | v32acc64 | acc2 )

## ◆ addmsc_4x4_4x8() [2/8]

v32acc64 addmsc_4x4_4x8 | ( | v32int16 | a,
|  | int | sgn_x,
|  | v32uint16 | b,
|  | int | sgn_y,
|  | v32acc64 | acc1,
|  | v32acc64 | acc2 )

## ◆ addmsc_4x4_4x8() [3/8]

v32acc64 addmsc_4x4_4x8 | ( | v32int16 | a,
|  | v32int16 | b,
|  | v32acc64 | acc1,
|  | v32acc64 | acc2 )

## ◆ addmsc_4x4_4x8() [4/8]

v32acc64 addmsc_4x4_4x8 | ( | v32int16 | a,
|  | v32uint16 | b,
|  | v32acc64 | acc1,
|  | v32acc64 | acc2 )

## ◆ addmsc_4x4_4x8() [5/8]

v32acc64 addmsc_4x4_4x8 | ( | v32uint16 | a,
|  | int | sgn_x,
|  | v32int16 | b,
|  | int | sgn_y,
|  | v32acc64 | acc1,
|  | v32acc64 | acc2 )

## ◆ addmsc_4x4_4x8() [6/8]

v32acc64 addmsc_4x4_4x8 | ( | v32uint16 | a,
|  | int | sgn_x,
|  | v32uint16 | b,
|  | int | sgn_y,
|  | v32acc64 | acc1,
|  | v32acc64 | acc2 )

## ◆ addmsc_4x4_4x8() [7/8]

v32acc64 addmsc_4x4_4x8 | ( | v32uint16 | a,
|  | v32int16 | b,
|  | v32acc64 | acc1,
|  | v32acc64 | acc2 )

## ◆ addmsc_4x4_4x8() [8/8]

v32acc64 addmsc_4x4_4x8 | ( | v32uint16 | a,
|  | v32uint16 | b,
|  | v32acc64 | acc1,
|  | v32acc64 | acc2 )

## ◆ addmsc_4x4_4x8_conf() [1/8]

v32acc64 addmsc_4x4_4x8_conf | ( | v32int16 | a,
|  | int | sgn_x,
|  | v32int16 | b,
|  | int | sgn_y,
|  | v32acc64 | acc1,
|  | v32acc64 | acc2,
|  | int | zero_acc1,
|  | int | shift16,
|  | int | sub_mul,
|  | int | sub_acc1,
|  | int | sub_acc2 )

## ◆ addmsc_4x4_4x8_conf() [2/8]

v32acc64 addmsc_4x4_4x8_conf | ( | v32int16 | a,
|  | int | sgn_x,
|  | v32uint16 | b,
|  | int | sgn_y,
|  | v32acc64 | acc1,
|  | v32acc64 | acc2,
|  | int | zero_acc1,
|  | int | shift16,
|  | int | sub_mul,
|  | int | sub_acc1,
|  | int | sub_acc2 )

## ◆ addmsc_4x4_4x8_conf() [3/8]

v32acc64 addmsc_4x4_4x8_conf | ( | v32int16 | a,
|  | v32int16 | b,
|  | v32acc64 | acc1,
|  | v32acc64 | acc2,
|  | int | zero_acc1,
|  | int | shift16,
|  | int | sub_mul,
|  | int | sub_acc1,
|  | int | sub_acc2 )

## ◆ addmsc_4x4_4x8_conf() [4/8]

v32acc64 addmsc_4x4_4x8_conf | ( | v32int16 | a,
|  | v32uint16 | b,
|  | v32acc64 | acc1,
|  | v32acc64 | acc2,
|  | int | zero_acc1,
|  | int | shift16,
|  | int | sub_mul,
|  | int | sub_acc1,
|  | int | sub_acc2 )

## ◆ addmsc_4x4_4x8_conf() [5/8]

v32acc64 addmsc_4x4_4x8_conf | ( | v32uint16 | a,
|  | int | sgn_x,
|  | v32int16 | b,
|  | int | sgn_y,
|  | v32acc64 | acc1,
|  | v32acc64 | acc2,
|  | int | zero_acc1,
|  | int | shift16,
|  | int | sub_mul,
|  | int | sub_acc1,
|  | int | sub_acc2 )

## ◆ addmsc_4x4_4x8_conf() [6/8]

v32acc64 addmsc_4x4_4x8_conf | ( | v32uint16 | a,
|  | int | sgn_x,
|  | v32uint16 | b,
|  | int | sgn_y,
|  | v32acc64 | acc1,
|  | v32acc64 | acc2,
|  | int | zero_acc1,
|  | int | shift16,
|  | int | sub_mul,
|  | int | sub_acc1,
|  | int | sub_acc2 )

## ◆ addmsc_4x4_4x8_conf() [7/8]

v32acc64 addmsc_4x4_4x8_conf | ( | v32uint16 | a,
|  | v32int16 | b,
|  | v32acc64 | acc1,
|  | v32acc64 | acc2,
|  | int | zero_acc1,
|  | int | shift16,
|  | int | sub_mul,
|  | int | sub_acc1,
|  | int | sub_acc2 )

## ◆ addmsc_4x4_4x8_conf() [8/8]

v32acc64 addmsc_4x4_4x8_conf | ( | v32uint16 | a,
|  | v32uint16 | b,
|  | v32acc64 | acc1,
|  | v32acc64 | acc2,
|  | int | zero_acc1,
|  | int | shift16,
|  | int | sub_mul,
|  | int | sub_acc1,
|  | int | sub_acc2 )

## ◆ addmsc_8x2_2x8() [1/8]

v64acc32 addmsc_8x2_2x8 | ( | v32int16 | a,
|  | int | sgn_x,
|  | v32int16 | b,
|  | int | sgn_y,
|  | v64acc32 | acc1,
|  | v64acc32 | acc2 )

## ◆ addmsc_8x2_2x8() [2/8]

v64acc32 addmsc_8x2_2x8 | ( | v32int16 | a,
|  | int | sgn_x,
|  | v32uint16 | b,
|  | int | sgn_y,
|  | v64acc32 | acc1,
|  | v64acc32 | acc2 )

## ◆ addmsc_8x2_2x8() [3/8]

v64acc32 addmsc_8x2_2x8 | ( | v32int16 | a,
|  | v32int16 | b,
|  | v64acc32 | acc1,
|  | v64acc32 | acc2 )

## ◆ addmsc_8x2_2x8() [4/8]

v64acc32 addmsc_8x2_2x8 | ( | v32int16 | a,
|  | v32uint16 | b,
|  | v64acc32 | acc1,
|  | v64acc32 | acc2 )

## ◆ addmsc_8x2_2x8() [5/8]

v64acc32 addmsc_8x2_2x8 | ( | v32uint16 | a,
|  | int | sgn_x,
|  | v32int16 | b,
|  | int | sgn_y,
|  | v64acc32 | acc1,
|  | v64acc32 | acc2 )

## ◆ addmsc_8x2_2x8() [6/8]

v64acc32 addmsc_8x2_2x8 | ( | v32uint16 | a,
|  | int | sgn_x,
|  | v32uint16 | b,
|  | int | sgn_y,
|  | v64acc32 | acc1,
|  | v64acc32 | acc2 )

## ◆ addmsc_8x2_2x8() [7/8]

v64acc32 addmsc_8x2_2x8 | ( | v32uint16 | a,
|  | v32int16 | b,
|  | v64acc32 | acc1,
|  | v64acc32 | acc2 )

## ◆ addmsc_8x2_2x8() [8/8]

v64acc32 addmsc_8x2_2x8 | ( | v32uint16 | a,
|  | v32uint16 | b,
|  | v64acc32 | acc1,
|  | v64acc32 | acc2 )

## ◆ addmsc_8x2_2x8_conf() [1/8]

v64acc32 addmsc_8x2_2x8_conf | ( | v32int16 | a,
|  | int | sgn_x,
|  | v32int16 | b,
|  | int | sgn_y,
|  | v64acc32 | acc1,
|  | v64acc32 | acc2,
|  | int | zero_acc1,
|  | int | shift16,
|  | int | sub_mul,
|  | int | sub_acc1,
|  | int | sub_acc2 )

## ◆ addmsc_8x2_2x8_conf() [2/8]

v64acc32 addmsc_8x2_2x8_conf | ( | v32int16 | a,
|  | int | sgn_x,
|  | v32uint16 | b,
|  | int | sgn_y,
|  | v64acc32 | acc1,
|  | v64acc32 | acc2,
|  | int | zero_acc1,
|  | int | shift16,
|  | int | sub_mul,
|  | int | sub_acc1,
|  | int | sub_acc2 )

## ◆ addmsc_8x2_2x8_conf() [3/8]

v64acc32 addmsc_8x2_2x8_conf | ( | v32int16 | a,
|  | v32int16 | b,
|  | v64acc32 | acc1,
|  | v64acc32 | acc2,
|  | int | zero_acc1,
|  | int | shift16,
|  | int | sub_mul,
|  | int | sub_acc1,
|  | int | sub_acc2 )

## ◆ addmsc_8x2_2x8_conf() [4/8]

v64acc32 addmsc_8x2_2x8_conf | ( | v32int16 | a,
|  | v32uint16 | b,
|  | v64acc32 | acc1,
|  | v64acc32 | acc2,
|  | int | zero_acc1,
|  | int | shift16,
|  | int | sub_mul,
|  | int | sub_acc1,
|  | int | sub_acc2 )

## ◆ addmsc_8x2_2x8_conf() [5/8]

v64acc32 addmsc_8x2_2x8_conf | ( | v32uint16 | a,
|  | int | sgn_x,
|  | v32int16 | b,
|  | int | sgn_y,
|  | v64acc32 | acc1,
|  | v64acc32 | acc2,
|  | int | zero_acc1,
|  | int | shift16,
|  | int | sub_mul,
|  | int | sub_acc1,
|  | int | sub_acc2 )

## ◆ addmsc_8x2_2x8_conf() [6/8]

v64acc32 addmsc_8x2_2x8_conf | ( | v32uint16 | a,
|  | int | sgn_x,
|  | v32uint16 | b,
|  | int | sgn_y,
|  | v64acc32 | acc1,
|  | v64acc32 | acc2,
|  | int | zero_acc1,
|  | int | shift16,
|  | int | sub_mul,
|  | int | sub_acc1,
|  | int | sub_acc2 )

## ◆ addmsc_8x2_2x8_conf() [7/8]

v64acc32 addmsc_8x2_2x8_conf | ( | v32uint16 | a,
|  | v32int16 | b,
|  | v64acc32 | acc1,
|  | v64acc32 | acc2,
|  | int | zero_acc1,
|  | int | shift16,
|  | int | sub_mul,
|  | int | sub_acc1,
|  | int | sub_acc2 )

## ◆ addmsc_8x2_2x8_conf() [8/8]

v64acc32 addmsc_8x2_2x8_conf | ( | v32uint16 | a,
|  | v32uint16 | b,
|  | v64acc32 | acc1,
|  | v64acc32 | acc2,
|  | int | zero_acc1,
|  | int | shift16,
|  | int | sub_mul,
|  | int | sub_acc1,
|  | int | sub_acc2 )

## ◆ addmsc_conv_32x4() [1/8]

v32acc64 addmsc_conv_32x4 | ( | v64int16 | a,
|  | int | sgn_x,
|  | v32int16 | b,
|  | int | sgn_y,
|  | v32acc64 | acc1,
|  | v32acc64 | acc2 )

## ◆ addmsc_conv_32x4() [2/8]

v32acc64 addmsc_conv_32x4 | ( | v64int16 | a,
|  | int | sgn_x,
|  | v32uint16 | b,
|  | int | sgn_y,
|  | v32acc64 | acc1,
|  | v32acc64 | acc2 )

## ◆ addmsc_conv_32x4() [3/8]

v32acc64 addmsc_conv_32x4 | ( | v64int16 | a,
|  | v32int16 | b,
|  | v32acc64 | acc1,
|  | v32acc64 | acc2 )

## ◆ addmsc_conv_32x4() [4/8]

v32acc64 addmsc_conv_32x4 | ( | v64int16 | a,
|  | v32uint16 | b,
|  | v32acc64 | acc1,
|  | v32acc64 | acc2 )

## ◆ addmsc_conv_32x4() [5/8]

v32acc64 addmsc_conv_32x4 | ( | v64uint16 | a,
|  | int | sgn_x,
|  | v32int16 | b,
|  | int | sgn_y,
|  | v32acc64 | acc1,
|  | v32acc64 | acc2 )

## ◆ addmsc_conv_32x4() [6/8]

v32acc64 addmsc_conv_32x4 | ( | v64uint16 | a,
|  | int | sgn_x,
|  | v32uint16 | b,
|  | int | sgn_y,
|  | v32acc64 | acc1,
|  | v32acc64 | acc2 )

## ◆ addmsc_conv_32x4() [7/8]

v32acc64 addmsc_conv_32x4 | ( | v64uint16 | a,
|  | v32int16 | b,
|  | v32acc64 | acc1,
|  | v32acc64 | acc2 )

## ◆ addmsc_conv_32x4() [8/8]

v32acc64 addmsc_conv_32x4 | ( | v64uint16 | a,
|  | v32uint16 | b,
|  | v32acc64 | acc1,
|  | v32acc64 | acc2 )

## ◆ addmsc_conv_32x4_conf() [1/8]

v32acc64 addmsc_conv_32x4_conf | ( | v64int16 | a,
|  | int | sgn_x,
|  | v32int16 | b,
|  | int | sgn_y,
|  | v32acc64 | acc1,
|  | v32acc64 | acc2,
|  | int | zero_acc1,
|  | int | shift16,
|  | int | sub_mul,
|  | int | sub_acc1,
|  | int | sub_acc2 )

## ◆ addmsc_conv_32x4_conf() [2/8]

v32acc64 addmsc_conv_32x4_conf | ( | v64int16 | a,
|  | int | sgn_x,
|  | v32uint16 | b,
|  | int | sgn_y,
|  | v32acc64 | acc1,
|  | v32acc64 | acc2,
|  | int | zero_acc1,
|  | int | shift16,
|  | int | sub_mul,
|  | int | sub_acc1,
|  | int | sub_acc2 )

## ◆ addmsc_conv_32x4_conf() [3/8]

v32acc64 addmsc_conv_32x4_conf | ( | v64int16 | a,
|  | v32int16 | b,
|  | v32acc64 | acc1,
|  | v32acc64 | acc2,
|  | int | zero_acc1,
|  | int | shift16,
|  | int | sub_mul,
|  | int | sub_acc1,
|  | int | sub_acc2 )

## ◆ addmsc_conv_32x4_conf() [4/8]

v32acc64 addmsc_conv_32x4_conf | ( | v64int16 | a,
|  | v32uint16 | b,
|  | v32acc64 | acc1,
|  | v32acc64 | acc2,
|  | int | zero_acc1,
|  | int | shift16,
|  | int | sub_mul,
|  | int | sub_acc1,
|  | int | sub_acc2 )

## ◆ addmsc_conv_32x4_conf() [5/8]

v32acc64 addmsc_conv_32x4_conf | ( | v64uint16 | a,
|  | int | sgn_x,
|  | v32int16 | b,
|  | int | sgn_y,
|  | v32acc64 | acc1,
|  | v32acc64 | acc2,
|  | int | zero_acc1,
|  | int | shift16,
|  | int | sub_mul,
|  | int | sub_acc1,
|  | int | sub_acc2 )

## ◆ addmsc_conv_32x4_conf() [6/8]

v32acc64 addmsc_conv_32x4_conf | ( | v64uint16 | a,
|  | int | sgn_x,
|  | v32uint16 | b,
|  | int | sgn_y,
|  | v32acc64 | acc1,
|  | v32acc64 | acc2,
|  | int | zero_acc1,
|  | int | shift16,
|  | int | sub_mul,
|  | int | sub_acc1,
|  | int | sub_acc2 )

## ◆ addmsc_conv_32x4_conf() [7/8]

v32acc64 addmsc_conv_32x4_conf | ( | v64uint16 | a,
|  | v32int16 | b,
|  | v32acc64 | acc1,
|  | v32acc64 | acc2,
|  | int | zero_acc1,
|  | int | shift16,
|  | int | sub_mul,
|  | int | sub_acc1,
|  | int | sub_acc2 )

## ◆ addmsc_conv_32x4_conf() [8/8]

v32acc64 addmsc_conv_32x4_conf | ( | v64uint16 | a,
|  | v32uint16 | b,
|  | v32acc64 | acc1,
|  | v32acc64 | acc2,
|  | int | zero_acc1,
|  | int | shift16,
|  | int | sub_mul,
|  | int | sub_acc1,
|  | int | sub_acc2 )

## ◆ addmsc_conv_4x4_8ch() [1/8]

v32acc64 addmsc_conv_4x4_8ch | ( | v64int16 | a,
|  | int | sgn_x,
|  | v32int16 | b,
|  | int | sgn_y,
|  | v32acc64 | acc1,
|  | v32acc64 | acc2 )

## ◆ addmsc_conv_4x4_8ch() [2/8]

v32acc64 addmsc_conv_4x4_8ch | ( | v64int16 | a,
|  | int | sgn_x,
|  | v32uint16 | b,
|  | int | sgn_y,
|  | v32acc64 | acc1,
|  | v32acc64 | acc2 )

## ◆ addmsc_conv_4x4_8ch() [3/8]

v32acc64 addmsc_conv_4x4_8ch | ( | v64int16 | a,
|  | v32int16 | b,
|  | v32acc64 | acc1,
|  | v32acc64 | acc2 )

## ◆ addmsc_conv_4x4_8ch() [4/8]

v32acc64 addmsc_conv_4x4_8ch | ( | v64int16 | a,
|  | v32uint16 | b,
|  | v32acc64 | acc1,
|  | v32acc64 | acc2 )

## ◆ addmsc_conv_4x4_8ch() [5/8]

v32acc64 addmsc_conv_4x4_8ch | ( | v64uint16 | a,
|  | int | sgn_x,
|  | v32int16 | b,
|  | int | sgn_y,
|  | v32acc64 | acc1,
|  | v32acc64 | acc2 )

## ◆ addmsc_conv_4x4_8ch() [6/8]

v32acc64 addmsc_conv_4x4_8ch | ( | v64uint16 | a,
|  | int | sgn_x,
|  | v32uint16 | b,
|  | int | sgn_y,
|  | v32acc64 | acc1,
|  | v32acc64 | acc2 )

## ◆ addmsc_conv_4x4_8ch() [7/8]

v32acc64 addmsc_conv_4x4_8ch | ( | v64uint16 | a,
|  | v32int16 | b,
|  | v32acc64 | acc1,
|  | v32acc64 | acc2 )

## ◆ addmsc_conv_4x4_8ch() [8/8]

v32acc64 addmsc_conv_4x4_8ch | ( | v64uint16 | a,
|  | v32uint16 | b,
|  | v32acc64 | acc1,
|  | v32acc64 | acc2 )

## ◆ addmsc_conv_4x4_8ch_conf() [1/8]

v32acc64 addmsc_conv_4x4_8ch_conf | ( | v64int16 | a,
|  | int | sgn_x,
|  | v32int16 | b,
|  | int | sgn_y,
|  | v32acc64 | acc1,
|  | v32acc64 | acc2,
|  | int | zero_acc1,
|  | int | shift16,
|  | int | sub_mul,
|  | int | sub_acc1,
|  | int | sub_acc2 )

## ◆ addmsc_conv_4x4_8ch_conf() [2/8]

v32acc64 addmsc_conv_4x4_8ch_conf | ( | v64int16 | a,
|  | int | sgn_x,
|  | v32uint16 | b,
|  | int | sgn_y,
|  | v32acc64 | acc1,
|  | v32acc64 | acc2,
|  | int | zero_acc1,
|  | int | shift16,
|  | int | sub_mul,
|  | int | sub_acc1,
|  | int | sub_acc2 )

## ◆ addmsc_conv_4x4_8ch_conf() [3/8]

v32acc64 addmsc_conv_4x4_8ch_conf | ( | v64int16 | a,
|  | v32int16 | b,
|  | v32acc64 | acc1,
|  | v32acc64 | acc2,
|  | int | zero_acc1,
|  | int | shift16,
|  | int | sub_mul,
|  | int | sub_acc1,
|  | int | sub_acc2 )

## ◆ addmsc_conv_4x4_8ch_conf() [4/8]

v32acc64 addmsc_conv_4x4_8ch_conf | ( | v64int16 | a,
|  | v32uint16 | b,
|  | v32acc64 | acc1,
|  | v32acc64 | acc2,
|  | int | zero_acc1,
|  | int | shift16,
|  | int | sub_mul,
|  | int | sub_acc1,
|  | int | sub_acc2 )

## ◆ addmsc_conv_4x4_8ch_conf() [5/8]

v32acc64 addmsc_conv_4x4_8ch_conf | ( | v64uint16 | a,
|  | int | sgn_x,
|  | v32int16 | b,
|  | int | sgn_y,
|  | v32acc64 | acc1,
|  | v32acc64 | acc2,
|  | int | zero_acc1,
|  | int | shift16,
|  | int | sub_mul,
|  | int | sub_acc1,
|  | int | sub_acc2 )

## ◆ addmsc_conv_4x4_8ch_conf() [6/8]

v32acc64 addmsc_conv_4x4_8ch_conf | ( | v64uint16 | a,
|  | int | sgn_x,
|  | v32uint16 | b,
|  | int | sgn_y,
|  | v32acc64 | acc1,
|  | v32acc64 | acc2,
|  | int | zero_acc1,
|  | int | shift16,
|  | int | sub_mul,
|  | int | sub_acc1,
|  | int | sub_acc2 )

## ◆ addmsc_conv_4x4_8ch_conf() [7/8]

v32acc64 addmsc_conv_4x4_8ch_conf | ( | v64uint16 | a,
|  | v32int16 | b,
|  | v32acc64 | acc1,
|  | v32acc64 | acc2,
|  | int | zero_acc1,
|  | int | shift16,
|  | int | sub_mul,
|  | int | sub_acc1,
|  | int | sub_acc2 )

## ◆ addmsc_conv_4x4_8ch_conf() [8/8]

v32acc64 addmsc_conv_4x4_8ch_conf | ( | v64uint16 | a,
|  | v32uint16 | b,
|  | v32acc64 | acc1,
|  | v32acc64 | acc2,
|  | int | zero_acc1,
|  | int | shift16,
|  | int | sub_mul,
|  | int | sub_acc1,
|  | int | sub_acc2 )

## ◆ addmsc_elem_32() [1/32]

v32accfloat addmsc_elem_32 | ( | v32bfloat16 | a,
|  | bfloat16 | b,
|  | v32accfloat | acc1,
|  | v32accfloat | acc2 )

## ◆ addmsc_elem_32() [2/32]

v32accfloat addmsc_elem_32 | ( | v32bfloat16 | a,
|  | float16 | b,
|  | v32accfloat | acc1,
|  | v32accfloat | acc2 )

## ◆ addmsc_elem_32() [3/32]

v32accfloat addmsc_elem_32 | ( | v32bfloat16 | a,
|  | int | sgn_x,
|  | bfloat16 | b,
|  | int | sgn_y,
|  | v32accfloat | acc1,
|  | v32accfloat | acc2 )

## ◆ addmsc_elem_32() [4/32]

v32accfloat addmsc_elem_32 | ( | v32bfloat16 | a,
|  | int | sgn_x,
|  | float16 | b,
|  | int | sgn_y,
|  | v32accfloat | acc1,
|  | v32accfloat | acc2 )

## ◆ addmsc_elem_32() [5/32]

v32accfloat addmsc_elem_32 | ( | v32bfloat16 | a,
|  | int | sgn_x,
|  | v32bfloat16 | b,
|  | int | sgn_y,
|  | v32accfloat | acc1,
|  | v32accfloat | acc2 )

## ◆ addmsc_elem_32() [6/32]

v32accfloat addmsc_elem_32 | ( | v32bfloat16 | a,
|  | int | sgn_x,
|  | v32float16 | b,
|  | int | sgn_y,
|  | v32accfloat | acc1,
|  | v32accfloat | acc2 )

## ◆ addmsc_elem_32() [7/32]

v32accfloat addmsc_elem_32 | ( | v32bfloat16 | a,
|  | v32bfloat16 | b,
|  | v32accfloat | acc1,
|  | v32accfloat | acc2 )

## ◆ addmsc_elem_32() [8/32]

v32accfloat addmsc_elem_32 | ( | v32bfloat16 | a,
|  | v32float16 | b,
|  | v32accfloat | acc1,
|  | v32accfloat | acc2 )

## ◆ addmsc_elem_32() [9/32]

v32accfloat addmsc_elem_32 | ( | v32float16 | a,
|  | bfloat16 | b,
|  | v32accfloat | acc1,
|  | v32accfloat | acc2 )

## ◆ addmsc_elem_32() [10/32]

v32accfloat addmsc_elem_32 | ( | v32float16 | a,
|  | float16 | b,
|  | v32accfloat | acc1,
|  | v32accfloat | acc2 )

## ◆ addmsc_elem_32() [11/32]

v32accfloat addmsc_elem_32 | ( | v32float16 | a,
|  | int | sgn_x,
|  | bfloat16 | b,
|  | int | sgn_y,
|  | v32accfloat | acc1,
|  | v32accfloat | acc2 )

## ◆ addmsc_elem_32() [12/32]

v32accfloat addmsc_elem_32 | ( | v32float16 | a,
|  | int | sgn_x,
|  | float16 | b,
|  | int | sgn_y,
|  | v32accfloat | acc1,
|  | v32accfloat | acc2 )

## ◆ addmsc_elem_32() [13/32]

v32accfloat addmsc_elem_32 | ( | v32float16 | a,
|  | int | sgn_x,
|  | v32bfloat16 | b,
|  | int | sgn_y,
|  | v32accfloat | acc1,
|  | v32accfloat | acc2 )

## ◆ addmsc_elem_32() [14/32]

v32accfloat addmsc_elem_32 | ( | v32float16 | a,
|  | int | sgn_x,
|  | v32float16 | b,
|  | int | sgn_y,
|  | v32accfloat | acc1,
|  | v32accfloat | acc2 )

## ◆ addmsc_elem_32() [15/32]

v32accfloat addmsc_elem_32 | ( | v32float16 | a,
|  | v32bfloat16 | b,
|  | v32accfloat | acc1,
|  | v32accfloat | acc2 )

## ◆ addmsc_elem_32() [16/32]

v32accfloat addmsc_elem_32 | ( | v32float16 | a,
|  | v32float16 | b,
|  | v32accfloat | acc1,
|  | v32accfloat | acc2 )

## ◆ addmsc_elem_32() [17/32]

v32acc64 addmsc_elem_32 | ( | v32int16 | a,
|  | int | sgn_x,
|  | signed short | b,
|  | int | sgn_y,
|  | v32acc64 | acc1,
|  | v32acc64 | acc2 )

## ◆ addmsc_elem_32() [18/32]

v32acc64 addmsc_elem_32 | ( | v32int16 | a,
|  | int | sgn_x,
|  | unsigned short | b,
|  | int | sgn_y,
|  | v32acc64 | acc1,
|  | v32acc64 | acc2 )

## ◆ addmsc_elem_32() [19/32]

v32acc64 addmsc_elem_32 | ( | v32int16 | a,
|  | int | sgn_x,
|  | v32int16 | b,
|  | int | sgn_y,
|  | v32acc64 | acc1,
|  | v32acc64 | acc2 )

## ◆ addmsc_elem_32() [20/32]

v32acc64 addmsc_elem_32 | ( | v32int16 | a,
|  | int | sgn_x,
|  | v32uint16 | b,
|  | int | sgn_y,
|  | v32acc64 | acc1,
|  | v32acc64 | acc2 )

## ◆ addmsc_elem_32() [21/32]

v32acc64 addmsc_elem_32 | ( | v32int16 | a,
|  | signed short | b,
|  | v32acc64 | acc1,
|  | v32acc64 | acc2 )

## ◆ addmsc_elem_32() [22/32]

v32acc64 addmsc_elem_32 | ( | v32int16 | a,
|  | unsigned short | b,
|  | v32acc64 | acc1,
|  | v32acc64 | acc2 )

## ◆ addmsc_elem_32() [23/32]

v32acc64 addmsc_elem_32 | ( | v32int16 | a,
|  | v32int16 | b,
|  | v32acc64 | acc1,
|  | v32acc64 | acc2 )

## ◆ addmsc_elem_32() [24/32]

v32acc64 addmsc_elem_32 | ( | v32int16 | a,
|  | v32uint16 | b,
|  | v32acc64 | acc1,
|  | v32acc64 | acc2 )

## ◆ addmsc_elem_32() [25/32]

v32acc64 addmsc_elem_32 | ( | v32uint16 | a,
|  | int | sgn_x,
|  | signed short | b,
|  | int | sgn_y,
|  | v32acc64 | acc1,
|  | v32acc64 | acc2 )

## ◆ addmsc_elem_32() [26/32]

v32acc64 addmsc_elem_32 | ( | v32uint16 | a,
|  | int | sgn_x,
|  | unsigned short | b,
|  | int | sgn_y,
|  | v32acc64 | acc1,
|  | v32acc64 | acc2 )

## ◆ addmsc_elem_32() [27/32]

v32acc64 addmsc_elem_32 | ( | v32uint16 | a,
|  | int | sgn_x,
|  | v32int16 | b,
|  | int | sgn_y,
|  | v32acc64 | acc1,
|  | v32acc64 | acc2 )

## ◆ addmsc_elem_32() [28/32]

v32acc64 addmsc_elem_32 | ( | v32uint16 | a,
|  | int | sgn_x,
|  | v32uint16 | b,
|  | int | sgn_y,
|  | v32acc64 | acc1,
|  | v32acc64 | acc2 )

## ◆ addmsc_elem_32() [29/32]

v32acc64 addmsc_elem_32 | ( | v32uint16 | a,
|  | signed short | b,
|  | v32acc64 | acc1,
|  | v32acc64 | acc2 )

## ◆ addmsc_elem_32() [30/32]

v32acc64 addmsc_elem_32 | ( | v32uint16 | a,
|  | unsigned short | b,
|  | v32acc64 | acc1,
|  | v32acc64 | acc2 )

## ◆ addmsc_elem_32() [31/32]

v32acc64 addmsc_elem_32 | ( | v32uint16 | a,
|  | v32int16 | b,
|  | v32acc64 | acc1,
|  | v32acc64 | acc2 )

## ◆ addmsc_elem_32() [32/32]

v32acc64 addmsc_elem_32 | ( | v32uint16 | a,
|  | v32uint16 | b,
|  | v32acc64 | acc1,
|  | v32acc64 | acc2 )

## ◆ addmsc_elem_32_2() [1/8]

v32acc64 addmsc_elem_32_2 | ( | v64int16 | a,
|  | int | sgn_x,
|  | v64int16 | b,
|  | int | sgn_y,
|  | v32acc64 | acc1,
|  | v32acc64 | acc2 )

## ◆ addmsc_elem_32_2() [2/8]

v32acc64 addmsc_elem_32_2 | ( | v64int16 | a,
|  | int | sgn_x,
|  | v64uint16 | b,
|  | int | sgn_y,
|  | v32acc64 | acc1,
|  | v32acc64 | acc2 )

## ◆ addmsc_elem_32_2() [3/8]

v32acc64 addmsc_elem_32_2 | ( | v64int16 | a,
|  | v64int16 | b,
|  | v32acc64 | acc1,
|  | v32acc64 | acc2 )

## ◆ addmsc_elem_32_2() [4/8]

v32acc64 addmsc_elem_32_2 | ( | v64int16 | a,
|  | v64uint16 | b,
|  | v32acc64 | acc1,
|  | v32acc64 | acc2 )

## ◆ addmsc_elem_32_2() [5/8]

v32acc64 addmsc_elem_32_2 | ( | v64uint16 | a,
|  | int | sgn_x,
|  | v64int16 | b,
|  | int | sgn_y,
|  | v32acc64 | acc1,
|  | v32acc64 | acc2 )

## ◆ addmsc_elem_32_2() [6/8]

v32acc64 addmsc_elem_32_2 | ( | v64uint16 | a,
|  | int | sgn_x,
|  | v64uint16 | b,
|  | int | sgn_y,
|  | v32acc64 | acc1,
|  | v32acc64 | acc2 )

## ◆ addmsc_elem_32_2() [7/8]

v32acc64 addmsc_elem_32_2 | ( | v64uint16 | a,
|  | v64int16 | b,
|  | v32acc64 | acc1,
|  | v32acc64 | acc2 )

## ◆ addmsc_elem_32_2() [8/8]

v32acc64 addmsc_elem_32_2 | ( | v64uint16 | a,
|  | v64uint16 | b,
|  | v32acc64 | acc1,
|  | v32acc64 | acc2 )

## ◆ addmsc_elem_32_2_conf() [1/8]

v32acc64 addmsc_elem_32_2_conf | ( | v64int16 | a,
|  | int | sgn_x,
|  | v64int16 | b,
|  | int | sgn_y,
|  | v32acc64 | acc1,
|  | v32acc64 | acc2,
|  | int | zero_acc1,
|  | int | shift16,
|  | int | sub_mul,
|  | int | sub_acc1,
|  | int | sub_acc2 )

## ◆ addmsc_elem_32_2_conf() [2/8]

v32acc64 addmsc_elem_32_2_conf | ( | v64int16 | a,
|  | int | sgn_x,
|  | v64uint16 | b,
|  | int | sgn_y,
|  | v32acc64 | acc1,
|  | v32acc64 | acc2,
|  | int | zero_acc1,
|  | int | shift16,
|  | int | sub_mul,
|  | int | sub_acc1,
|  | int | sub_acc2 )

## ◆ addmsc_elem_32_2_conf() [3/8]

v32acc64 addmsc_elem_32_2_conf | ( | v64int16 | a,
|  | v64int16 | b,
|  | v32acc64 | acc1,
|  | v32acc64 | acc2,
|  | int | zero_acc1,
|  | int | shift16,
|  | int | sub_mul,
|  | int | sub_acc1,
|  | int | sub_acc2 )

## ◆ addmsc_elem_32_2_conf() [4/8]

v32acc64 addmsc_elem_32_2_conf | ( | v64int16 | a,
|  | v64uint16 | b,
|  | v32acc64 | acc1,
|  | v32acc64 | acc2,
|  | int | zero_acc1,
|  | int | shift16,
|  | int | sub_mul,
|  | int | sub_acc1,
|  | int | sub_acc2 )

## ◆ addmsc_elem_32_2_conf() [5/8]

v32acc64 addmsc_elem_32_2_conf | ( | v64uint16 | a,
|  | int | sgn_x,
|  | v64int16 | b,
|  | int | sgn_y,
|  | v32acc64 | acc1,
|  | v32acc64 | acc2,
|  | int | zero_acc1,
|  | int | shift16,
|  | int | sub_mul,
|  | int | sub_acc1,
|  | int | sub_acc2 )

## ◆ addmsc_elem_32_2_conf() [6/8]

v32acc64 addmsc_elem_32_2_conf | ( | v64uint16 | a,
|  | int | sgn_x,
|  | v64uint16 | b,
|  | int | sgn_y,
|  | v32acc64 | acc1,
|  | v32acc64 | acc2,
|  | int | zero_acc1,
|  | int | shift16,
|  | int | sub_mul,
|  | int | sub_acc1,
|  | int | sub_acc2 )

## ◆ addmsc_elem_32_2_conf() [7/8]

v32acc64 addmsc_elem_32_2_conf | ( | v64uint16 | a,
|  | v64int16 | b,
|  | v32acc64 | acc1,
|  | v32acc64 | acc2,
|  | int | zero_acc1,
|  | int | shift16,
|  | int | sub_mul,
|  | int | sub_acc1,
|  | int | sub_acc2 )

## ◆ addmsc_elem_32_2_conf() [8/8]

v32acc64 addmsc_elem_32_2_conf | ( | v64uint16 | a,
|  | v64uint16 | b,
|  | v32acc64 | acc1,
|  | v32acc64 | acc2,
|  | int | zero_acc1,
|  | int | shift16,
|  | int | sub_mul,
|  | int | sub_acc1,
|  | int | sub_acc2 )

## ◆ addmsc_elem_32_32b() [1/8]

v32acc32 addmsc_elem_32_32b | ( | v32int16 | a,
|  | int | sgn_x,
|  | v32int16 | b,
|  | int | sgn_y,
|  | v32acc32 | acc1,
|  | v32acc32 | acc2 )

## ◆ addmsc_elem_32_32b() [2/8]

v32acc32 addmsc_elem_32_32b | ( | v32int16 | a,
|  | int | sgn_x,
|  | v32uint16 | b,
|  | int | sgn_y,
|  | v32acc32 | acc1,
|  | v32acc32 | acc2 )

## ◆ addmsc_elem_32_32b() [3/8]

v32acc32 addmsc_elem_32_32b | ( | v32int16 | a,
|  | v32int16 | b,
|  | v32acc32 | acc1,
|  | v32acc32 | acc2 )

## ◆ addmsc_elem_32_32b() [4/8]

v32acc32 addmsc_elem_32_32b | ( | v32int16 | a,
|  | v32uint16 | b,
|  | v32acc32 | acc1,
|  | v32acc32 | acc2 )

## ◆ addmsc_elem_32_32b() [5/8]

v32acc32 addmsc_elem_32_32b | ( | v32uint16 | a,
|  | int | sgn_x,
|  | v32int16 | b,
|  | int | sgn_y,
|  | v32acc32 | acc1,
|  | v32acc32 | acc2 )

## ◆ addmsc_elem_32_32b() [6/8]

v32acc32 addmsc_elem_32_32b | ( | v32uint16 | a,
|  | int | sgn_x,
|  | v32uint16 | b,
|  | int | sgn_y,
|  | v32acc32 | acc1,
|  | v32acc32 | acc2 )

## ◆ addmsc_elem_32_32b() [7/8]

v32acc32 addmsc_elem_32_32b | ( | v32uint16 | a,
|  | v32int16 | b,
|  | v32acc32 | acc1,
|  | v32acc32 | acc2 )

## ◆ addmsc_elem_32_32b() [8/8]

v32acc32 addmsc_elem_32_32b | ( | v32uint16 | a,
|  | v32uint16 | b,
|  | v32acc32 | acc1,
|  | v32acc32 | acc2 )

## ◆ addmsc_elem_32_32b_conf() [1/8]

v32acc32 addmsc_elem_32_32b_conf | ( | v32int16 | a,
|  | int | sgn_x,
|  | v32int16 | b,
|  | int | sgn_y,
|  | v32acc32 | acc1,
|  | v32acc32 | acc2,
|  | int | zero_acc1,
|  | int | shift16,
|  | int | sub_mul,
|  | int | sub_acc1,
|  | int | sub_acc2 )

## ◆ addmsc_elem_32_32b_conf() [2/8]

v32acc32 addmsc_elem_32_32b_conf | ( | v32int16 | a,
|  | int | sgn_x,
|  | v32uint16 | b,
|  | int | sgn_y,
|  | v32acc32 | acc1,
|  | v32acc32 | acc2,
|  | int | zero_acc1,
|  | int | shift16,
|  | int | sub_mul,
|  | int | sub_acc1,
|  | int | sub_acc2 )

## ◆ addmsc_elem_32_32b_conf() [3/8]

v32acc32 addmsc_elem_32_32b_conf | ( | v32int16 | a,
|  | v32int16 | b,
|  | v32acc32 | acc1,
|  | v32acc32 | acc2,
|  | int | zero_acc1,
|  | int | shift16,
|  | int | sub_mul,
|  | int | sub_acc1,
|  | int | sub_acc2 )

## ◆ addmsc_elem_32_32b_conf() [4/8]

v32acc32 addmsc_elem_32_32b_conf | ( | v32int16 | a,
|  | v32uint16 | b,
|  | v32acc32 | acc1,
|  | v32acc32 | acc2,
|  | int | zero_acc1,
|  | int | shift16,
|  | int | sub_mul,
|  | int | sub_acc1,
|  | int | sub_acc2 )

## ◆ addmsc_elem_32_32b_conf() [5/8]

v32acc32 addmsc_elem_32_32b_conf | ( | v32uint16 | a,
|  | int | sgn_x,
|  | v32int16 | b,
|  | int | sgn_y,
|  | v32acc32 | acc1,
|  | v32acc32 | acc2,
|  | int | zero_acc1,
|  | int | shift16,
|  | int | sub_mul,
|  | int | sub_acc1,
|  | int | sub_acc2 )

## ◆ addmsc_elem_32_32b_conf() [6/8]

v32acc32 addmsc_elem_32_32b_conf | ( | v32uint16 | a,
|  | int | sgn_x,
|  | v32uint16 | b,
|  | int | sgn_y,
|  | v32acc32 | acc1,
|  | v32acc32 | acc2,
|  | int | zero_acc1,
|  | int | shift16,
|  | int | sub_mul,
|  | int | sub_acc1,
|  | int | sub_acc2 )

## ◆ addmsc_elem_32_32b_conf() [7/8]

v32acc32 addmsc_elem_32_32b_conf | ( | v32uint16 | a,
|  | v32int16 | b,
|  | v32acc32 | acc1,
|  | v32acc32 | acc2,
|  | int | zero_acc1,
|  | int | shift16,
|  | int | sub_mul,
|  | int | sub_acc1,
|  | int | sub_acc2 )

## ◆ addmsc_elem_32_32b_conf() [8/8]

v32acc32 addmsc_elem_32_32b_conf | ( | v32uint16 | a,
|  | v32uint16 | b,
|  | v32acc32 | acc1,
|  | v32acc32 | acc2,
|  | int | zero_acc1,
|  | int | shift16,
|  | int | sub_mul,
|  | int | sub_acc1,
|  | int | sub_acc2 )

## ◆ addmsc_elem_32_conf() [1/32]

v32accfloat addmsc_elem_32_conf | ( | v32bfloat16 | a,
|  | bfloat16 | b,
|  | v32accfloat | acc1,
|  | v32accfloat | acc2,
|  | int | zero_acc1,
|  | int | sub_mul,
|  | int | sub_acc1,
|  | int | sub_acc2 )

## ◆ addmsc_elem_32_conf() [2/32]

v32accfloat addmsc_elem_32_conf | ( | v32bfloat16 | a,
|  | float16 | b,
|  | v32accfloat | acc1,
|  | v32accfloat | acc2,
|  | int | zero_acc1,
|  | int | sub_mul,
|  | int | sub_acc1,
|  | int | sub_acc2 )

## ◆ addmsc_elem_32_conf() [3/32]

v32accfloat addmsc_elem_32_conf | ( | v32bfloat16 | a,
|  | int | sgn_x,
|  | bfloat16 | b,
|  | int | sgn_y,
|  | v32accfloat | acc1,
|  | v32accfloat | acc2,
|  | int | zero_acc1,
|  | int | sub_mul,
|  | int | sub_acc1,
|  | int | sub_acc2 )

## ◆ addmsc_elem_32_conf() [4/32]

v32accfloat addmsc_elem_32_conf | ( | v32bfloat16 | a,
|  | int | sgn_x,
|  | float16 | b,
|  | int | sgn_y,
|  | v32accfloat | acc1,
|  | v32accfloat | acc2,
|  | int | zero_acc1,
|  | int | sub_mul,
|  | int | sub_acc1,
|  | int | sub_acc2 )

## ◆ addmsc_elem_32_conf() [5/32]

v32accfloat addmsc_elem_32_conf | ( | v32bfloat16 | a,
|  | int | sgn_x,
|  | v32bfloat16 | b,
|  | int | sgn_y,
|  | v32accfloat | acc1,
|  | v32accfloat | acc2,
|  | int | zero_acc1,
|  | int | sub_mul,
|  | int | sub_acc1,
|  | int | sub_acc2 )

## ◆ addmsc_elem_32_conf() [6/32]

v32accfloat addmsc_elem_32_conf | ( | v32bfloat16 | a,
|  | int | sgn_x,
|  | v32float16 | b,
|  | int | sgn_y,
|  | v32accfloat | acc1,
|  | v32accfloat | acc2,
|  | int | zero_acc1,
|  | int | sub_mul,
|  | int | sub_acc1,
|  | int | sub_acc2 )

## ◆ addmsc_elem_32_conf() [7/32]

v32accfloat addmsc_elem_32_conf | ( | v32bfloat16 | a,
|  | v32bfloat16 | b,
|  | v32accfloat | acc1,
|  | v32accfloat | acc2,
|  | int | zero_acc1,
|  | int | sub_mul,
|  | int | sub_acc1,
|  | int | sub_acc2 )

## ◆ addmsc_elem_32_conf() [8/32]

v32accfloat addmsc_elem_32_conf | ( | v32bfloat16 | a,
|  | v32float16 | b,
|  | v32accfloat | acc1,
|  | v32accfloat | acc2,
|  | int | zero_acc1,
|  | int | sub_mul,
|  | int | sub_acc1,
|  | int | sub_acc2 )

## ◆ addmsc_elem_32_conf() [9/32]

v32accfloat addmsc_elem_32_conf | ( | v32float16 | a,
|  | bfloat16 | b,
|  | v32accfloat | acc1,
|  | v32accfloat | acc2,
|  | int | zero_acc1,
|  | int | sub_mul,
|  | int | sub_acc1,
|  | int | sub_acc2 )

## ◆ addmsc_elem_32_conf() [10/32]

v32accfloat addmsc_elem_32_conf | ( | v32float16 | a,
|  | float16 | b,
|  | v32accfloat | acc1,
|  | v32accfloat | acc2,
|  | int | zero_acc1,
|  | int | sub_mul,
|  | int | sub_acc1,
|  | int | sub_acc2 )

## ◆ addmsc_elem_32_conf() [11/32]

v32accfloat addmsc_elem_32_conf | ( | v32float16 | a,
|  | int | sgn_x,
|  | bfloat16 | b,
|  | int | sgn_y,
|  | v32accfloat | acc1,
|  | v32accfloat | acc2,
|  | int | zero_acc1,
|  | int | sub_mul,
|  | int | sub_acc1,
|  | int | sub_acc2 )

## ◆ addmsc_elem_32_conf() [12/32]

v32accfloat addmsc_elem_32_conf | ( | v32float16 | a,
|  | int | sgn_x,
|  | float16 | b,
|  | int | sgn_y,
|  | v32accfloat | acc1,
|  | v32accfloat | acc2,
|  | int | zero_acc1,
|  | int | sub_mul,
|  | int | sub_acc1,
|  | int | sub_acc2 )

## ◆ addmsc_elem_32_conf() [13/32]

v32accfloat addmsc_elem_32_conf | ( | v32float16 | a,
|  | int | sgn_x,
|  | v32bfloat16 | b,
|  | int | sgn_y,
|  | v32accfloat | acc1,
|  | v32accfloat | acc2,
|  | int | zero_acc1,
|  | int | sub_mul,
|  | int | sub_acc1,
|  | int | sub_acc2 )

## ◆ addmsc_elem_32_conf() [14/32]

v32accfloat addmsc_elem_32_conf | ( | v32float16 | a,
|  | int | sgn_x,
|  | v32float16 | b,
|  | int | sgn_y,
|  | v32accfloat | acc1,
|  | v32accfloat | acc2,
|  | int | zero_acc1,
|  | int | sub_mul,
|  | int | sub_acc1,
|  | int | sub_acc2 )

## ◆ addmsc_elem_32_conf() [15/32]

v32accfloat addmsc_elem_32_conf | ( | v32float16 | a,
|  | v32bfloat16 | b,
|  | v32accfloat | acc1,
|  | v32accfloat | acc2,
|  | int | zero_acc1,
|  | int | sub_mul,
|  | int | sub_acc1,
|  | int | sub_acc2 )

## ◆ addmsc_elem_32_conf() [16/32]

v32accfloat addmsc_elem_32_conf | ( | v32float16 | a,
|  | v32float16 | b,
|  | v32accfloat | acc1,
|  | v32accfloat | acc2,
|  | int | zero_acc1,
|  | int | sub_mul,
|  | int | sub_acc1,
|  | int | sub_acc2 )

## ◆ addmsc_elem_32_conf() [17/32]

v32acc64 addmsc_elem_32_conf | ( | v32int16 | a,
|  | int | sgn_x,
|  | signed short | b,
|  | int | sgn_y,
|  | v32acc64 | acc1,
|  | v32acc64 | acc2,
|  | int | zero_acc1,
|  | int | shift16,
|  | int | sub_mul,
|  | int | sub_acc1,
|  | int | sub_acc2 )

## ◆ addmsc_elem_32_conf() [18/32]

v32acc64 addmsc_elem_32_conf | ( | v32int16 | a,
|  | int | sgn_x,
|  | unsigned short | b,
|  | int | sgn_y,
|  | v32acc64 | acc1,
|  | v32acc64 | acc2,
|  | int | zero_acc1,
|  | int | shift16,
|  | int | sub_mul,
|  | int | sub_acc1,
|  | int | sub_acc2 )

## ◆ addmsc_elem_32_conf() [19/32]

v32acc64 addmsc_elem_32_conf | ( | v32int16 | a,
|  | int | sgn_x,
|  | v32int16 | b,
|  | int | sgn_y,
|  | v32acc64 | acc1,
|  | v32acc64 | acc2,
|  | int | zero_acc1,
|  | int | shift16,
|  | int | sub_mul,
|  | int | sub_acc1,
|  | int | sub_acc2 )

## ◆ addmsc_elem_32_conf() [20/32]

v32acc64 addmsc_elem_32_conf | ( | v32int16 | a,
|  | int | sgn_x,
|  | v32uint16 | b,
|  | int | sgn_y,
|  | v32acc64 | acc1,
|  | v32acc64 | acc2,
|  | int | zero_acc1,
|  | int | shift16,
|  | int | sub_mul,
|  | int | sub_acc1,
|  | int | sub_acc2 )

## ◆ addmsc_elem_32_conf() [21/32]

v32acc64 addmsc_elem_32_conf | ( | v32int16 | a,
|  | signed short | b,
|  | v32acc64 | acc1,
|  | v32acc64 | acc2,
|  | int | zero_acc1,
|  | int | shift16,
|  | int | sub_mul,
|  | int | sub_acc1,
|  | int | sub_acc2 )

## ◆ addmsc_elem_32_conf() [22/32]

v32acc64 addmsc_elem_32_conf | ( | v32int16 | a,
|  | unsigned short | b,
|  | v32acc64 | acc1,
|  | v32acc64 | acc2,
|  | int | zero_acc1,
|  | int | shift16,
|  | int | sub_mul,
|  | int | sub_acc1,
|  | int | sub_acc2 )

## ◆ addmsc_elem_32_conf() [23/32]

v32acc64 addmsc_elem_32_conf | ( | v32int16 | a,
|  | v32int16 | b,
|  | v32acc64 | acc1,
|  | v32acc64 | acc2,
|  | int | zero_acc1,
|  | int | shift16,
|  | int | sub_mul,
|  | int | sub_acc1,
|  | int | sub_acc2 )

## ◆ addmsc_elem_32_conf() [24/32]

v32acc64 addmsc_elem_32_conf | ( | v32int16 | a,
|  | v32uint16 | b,
|  | v32acc64 | acc1,
|  | v32acc64 | acc2,
|  | int | zero_acc1,
|  | int | shift16,
|  | int | sub_mul,
|  | int | sub_acc1,
|  | int | sub_acc2 )

## ◆ addmsc_elem_32_conf() [25/32]

v32acc64 addmsc_elem_32_conf | ( | v32uint16 | a,
|  | int | sgn_x,
|  | signed short | b,
|  | int | sgn_y,
|  | v32acc64 | acc1,
|  | v32acc64 | acc2,
|  | int | zero_acc1,
|  | int | shift16,
|  | int | sub_mul,
|  | int | sub_acc1,
|  | int | sub_acc2 )

## ◆ addmsc_elem_32_conf() [26/32]

v32acc64 addmsc_elem_32_conf | ( | v32uint16 | a,
|  | int | sgn_x,
|  | unsigned short | b,
|  | int | sgn_y,
|  | v32acc64 | acc1,
|  | v32acc64 | acc2,
|  | int | zero_acc1,
|  | int | shift16,
|  | int | sub_mul,
|  | int | sub_acc1,
|  | int | sub_acc2 )

## ◆ addmsc_elem_32_conf() [27/32]

v32acc64 addmsc_elem_32_conf | ( | v32uint16 | a,
|  | int | sgn_x,
|  | v32int16 | b,
|  | int | sgn_y,
|  | v32acc64 | acc1,
|  | v32acc64 | acc2,
|  | int | zero_acc1,
|  | int | shift16,
|  | int | sub_mul,
|  | int | sub_acc1,
|  | int | sub_acc2 )

## ◆ addmsc_elem_32_conf() [28/32]

v32acc64 addmsc_elem_32_conf | ( | v32uint16 | a,
|  | int | sgn_x,
|  | v32uint16 | b,
|  | int | sgn_y,
|  | v32acc64 | acc1,
|  | v32acc64 | acc2,
|  | int | zero_acc1,
|  | int | shift16,
|  | int | sub_mul,
|  | int | sub_acc1,
|  | int | sub_acc2 )

## ◆ addmsc_elem_32_conf() [29/32]

v32acc64 addmsc_elem_32_conf | ( | v32uint16 | a,
|  | signed short | b,
|  | v32acc64 | acc1,
|  | v32acc64 | acc2,
|  | int | zero_acc1,
|  | int | shift16,
|  | int | sub_mul,
|  | int | sub_acc1,
|  | int | sub_acc2 )

## ◆ addmsc_elem_32_conf() [30/32]

v32acc64 addmsc_elem_32_conf | ( | v32uint16 | a,
|  | unsigned short | b,
|  | v32acc64 | acc1,
|  | v32acc64 | acc2,
|  | int | zero_acc1,
|  | int | shift16,
|  | int | sub_mul,
|  | int | sub_acc1,
|  | int | sub_acc2 )

## ◆ addmsc_elem_32_conf() [31/32]

v32acc64 addmsc_elem_32_conf | ( | v32uint16 | a,
|  | v32int16 | b,
|  | v32acc64 | acc1,
|  | v32acc64 | acc2,
|  | int | zero_acc1,
|  | int | shift16,
|  | int | sub_mul,
|  | int | sub_acc1,
|  | int | sub_acc2 )

## ◆ addmsc_elem_32_conf() [32/32]

v32acc64 addmsc_elem_32_conf | ( | v32uint16 | a,
|  | v32uint16 | b,
|  | v32acc64 | acc1,
|  | v32acc64 | acc2,
|  | int | zero_acc1,
|  | int | shift16,
|  | int | sub_mul,
|  | int | sub_acc1,
|  | int | sub_acc2 )

## ◆ addmsc_elem_64() [1/8]

v64acc32 addmsc_elem_64 | ( | v64int16 | a,
|  | int | sgn_x,
|  | v64int16 | b,
|  | int | sgn_y,
|  | v64acc32 | acc1,
|  | v64acc32 | acc2 )

## ◆ addmsc_elem_64() [2/8]

v64acc32 addmsc_elem_64 | ( | v64int16 | a,
|  | int | sgn_x,
|  | v64uint16 | b,
|  | int | sgn_y,
|  | v64acc32 | acc1,
|  | v64acc32 | acc2 )

## ◆ addmsc_elem_64() [3/8]

v64acc32 addmsc_elem_64 | ( | v64int16 | a,
|  | v64int16 | b,
|  | v64acc32 | acc1,
|  | v64acc32 | acc2 )

## ◆ addmsc_elem_64() [4/8]

v64acc32 addmsc_elem_64 | ( | v64int16 | a,
|  | v64uint16 | b,
|  | v64acc32 | acc1,
|  | v64acc32 | acc2 )

## ◆ addmsc_elem_64() [5/8]

v64acc32 addmsc_elem_64 | ( | v64uint16 | a,
|  | int | sgn_x,
|  | v64int16 | b,
|  | int | sgn_y,
|  | v64acc32 | acc1,
|  | v64acc32 | acc2 )

## ◆ addmsc_elem_64() [6/8]

v64acc32 addmsc_elem_64 | ( | v64uint16 | a,
|  | int | sgn_x,
|  | v64uint16 | b,
|  | int | sgn_y,
|  | v64acc32 | acc1,
|  | v64acc32 | acc2 )

## ◆ addmsc_elem_64() [7/8]

v64acc32 addmsc_elem_64 | ( | v64uint16 | a,
|  | v64int16 | b,
|  | v64acc32 | acc1,
|  | v64acc32 | acc2 )

## ◆ addmsc_elem_64() [8/8]

v64acc32 addmsc_elem_64 | ( | v64uint16 | a,
|  | v64uint16 | b,
|  | v64acc32 | acc1,
|  | v64acc32 | acc2 )

## ◆ addmsc_elem_64_conf() [1/8]

v64acc32 addmsc_elem_64_conf | ( | v64int16 | a,
|  | int | sgn_x,
|  | v64int16 | b,
|  | int | sgn_y,
|  | v64acc32 | acc1,
|  | v64acc32 | acc2,
|  | int | zero_acc1,
|  | int | shift16,
|  | int | sub_mul,
|  | int | sub_acc1,
|  | int | sub_acc2 )

## ◆ addmsc_elem_64_conf() [2/8]

v64acc32 addmsc_elem_64_conf | ( | v64int16 | a,
|  | int | sgn_x,
|  | v64uint16 | b,
|  | int | sgn_y,
|  | v64acc32 | acc1,
|  | v64acc32 | acc2,
|  | int | zero_acc1,
|  | int | shift16,
|  | int | sub_mul,
|  | int | sub_acc1,
|  | int | sub_acc2 )

## ◆ addmsc_elem_64_conf() [3/8]

v64acc32 addmsc_elem_64_conf | ( | v64int16 | a,
|  | v64int16 | b,
|  | v64acc32 | acc1,
|  | v64acc32 | acc2,
|  | int | zero_acc1,
|  | int | shift16,
|  | int | sub_mul,
|  | int | sub_acc1,
|  | int | sub_acc2 )

## ◆ addmsc_elem_64_conf() [4/8]

v64acc32 addmsc_elem_64_conf | ( | v64int16 | a,
|  | v64uint16 | b,
|  | v64acc32 | acc1,
|  | v64acc32 | acc2,
|  | int | zero_acc1,
|  | int | shift16,
|  | int | sub_mul,
|  | int | sub_acc1,
|  | int | sub_acc2 )

## ◆ addmsc_elem_64_conf() [5/8]

v64acc32 addmsc_elem_64_conf | ( | v64uint16 | a,
|  | int | sgn_x,
|  | v64int16 | b,
|  | int | sgn_y,
|  | v64acc32 | acc1,
|  | v64acc32 | acc2,
|  | int | zero_acc1,
|  | int | shift16,
|  | int | sub_mul,
|  | int | sub_acc1,
|  | int | sub_acc2 )

## ◆ addmsc_elem_64_conf() [6/8]

v64acc32 addmsc_elem_64_conf | ( | v64uint16 | a,
|  | int | sgn_x,
|  | v64uint16 | b,
|  | int | sgn_y,
|  | v64acc32 | acc1,
|  | v64acc32 | acc2,
|  | int | zero_acc1,
|  | int | shift16,
|  | int | sub_mul,
|  | int | sub_acc1,
|  | int | sub_acc2 )

## ◆ addmsc_elem_64_conf() [7/8]

v64acc32 addmsc_elem_64_conf | ( | v64uint16 | a,
|  | v64int16 | b,
|  | v64acc32 | acc1,
|  | v64acc32 | acc2,
|  | int | zero_acc1,
|  | int | shift16,
|  | int | sub_mul,
|  | int | sub_acc1,
|  | int | sub_acc2 )

## ◆ addmsc_elem_64_conf() [8/8]

v64acc32 addmsc_elem_64_conf | ( | v64uint16 | a,
|  | v64uint16 | b,
|  | v64acc32 | acc1,
|  | v64acc32 | acc2,
|  | int | zero_acc1,
|  | int | shift16,
|  | int | sub_mul,
|  | int | sub_acc1,
|  | int | sub_acc2 )

## ◆ mac_4x4_4x8() [1/8]

v32acc64 mac_4x4_4x8 | ( | v32int16 | a,
|  | int | sgn_x,
|  | v32int16 | b,
|  | int | sgn_y,
|  | v32acc64 | acc )

## ◆ mac_4x4_4x8() [2/8]

v32acc64 mac_4x4_4x8 | ( | v32int16 | a,
|  | int | sgn_x,
|  | v32uint16 | b,
|  | int | sgn_y,
|  | v32acc64 | acc )

## ◆ mac_4x4_4x8() [3/8]

v32acc64 mac_4x4_4x8 | ( | v32int16 | a,
|  | v32int16 | b,
|  | v32acc64 | acc )

## ◆ mac_4x4_4x8() [4/8]

v32acc64 mac_4x4_4x8 | ( | v32int16 | a,
|  | v32uint16 | b,
|  | v32acc64 | acc )

## ◆ mac_4x4_4x8() [5/8]

v32acc64 mac_4x4_4x8 | ( | v32uint16 | a,
|  | int | sgn_x,
|  | v32int16 | b,
|  | int | sgn_y,
|  | v32acc64 | acc )

## ◆ mac_4x4_4x8() [6/8]

v32acc64 mac_4x4_4x8 | ( | v32uint16 | a,
|  | int | sgn_x,
|  | v32uint16 | b,
|  | int | sgn_y,
|  | v32acc64 | acc )

## ◆ mac_4x4_4x8() [7/8]

v32acc64 mac_4x4_4x8 | ( | v32uint16 | a,
|  | v32int16 | b,
|  | v32acc64 | acc )

## ◆ mac_4x4_4x8() [8/8]

v32acc64 mac_4x4_4x8 | ( | v32uint16 | a,
|  | v32uint16 | b,
|  | v32acc64 | acc )

## ◆ mac_4x4_4x8_conf() [1/8]

v32acc64 mac_4x4_4x8_conf | ( | v32int16 | a,
|  | int | sgn_x,
|  | v32int16 | b,
|  | int | sgn_y,
|  | v32acc64 | acc,
|  | int | zero_acc,
|  | int | shift16,
|  | int | sub_mul,
|  | int | sub_acc1 )

## ◆ mac_4x4_4x8_conf() [2/8]

v32acc64 mac_4x4_4x8_conf | ( | v32int16 | a,
|  | int | sgn_x,
|  | v32uint16 | b,
|  | int | sgn_y,
|  | v32acc64 | acc,
|  | int | zero_acc,
|  | int | shift16,
|  | int | sub_mul,
|  | int | sub_acc1 )

## ◆ mac_4x4_4x8_conf() [3/8]

v32acc64 mac_4x4_4x8_conf | ( | v32int16 | a,
|  | v32int16 | b,
|  | v32acc64 | acc,
|  | int | zero_acc,
|  | int | shift16,
|  | int | sub_mul,
|  | int | sub_acc1 )

## ◆ mac_4x4_4x8_conf() [4/8]

v32acc64 mac_4x4_4x8_conf | ( | v32int16 | a,
|  | v32uint16 | b,
|  | v32acc64 | acc,
|  | int | zero_acc,
|  | int | shift16,
|  | int | sub_mul,
|  | int | sub_acc1 )

## ◆ mac_4x4_4x8_conf() [5/8]

v32acc64 mac_4x4_4x8_conf | ( | v32uint16 | a,
|  | int | sgn_x,
|  | v32int16 | b,
|  | int | sgn_y,
|  | v32acc64 | acc,
|  | int | zero_acc,
|  | int | shift16,
|  | int | sub_mul,
|  | int | sub_acc1 )

## ◆ mac_4x4_4x8_conf() [6/8]

v32acc64 mac_4x4_4x8_conf | ( | v32uint16 | a,
|  | int | sgn_x,
|  | v32uint16 | b,
|  | int | sgn_y,
|  | v32acc64 | acc,
|  | int | zero_acc,
|  | int | shift16,
|  | int | sub_mul,
|  | int | sub_acc1 )

## ◆ mac_4x4_4x8_conf() [7/8]

v32acc64 mac_4x4_4x8_conf | ( | v32uint16 | a,
|  | v32int16 | b,
|  | v32acc64 | acc,
|  | int | zero_acc,
|  | int | shift16,
|  | int | sub_mul,
|  | int | sub_acc1 )

## ◆ mac_4x4_4x8_conf() [8/8]

v32acc64 mac_4x4_4x8_conf | ( | v32uint16 | a,
|  | v32uint16 | b,
|  | v32acc64 | acc,
|  | int | zero_acc,
|  | int | shift16,
|  | int | sub_mul,
|  | int | sub_acc1 )

## ◆ mac_8x2_2x8() [1/8]

v64acc32 mac_8x2_2x8 | ( | v32int16 | a,
|  | int | sgn_x,
|  | v32int16 | b,
|  | int | sgn_y,
|  | v64acc32 | acc )

## ◆ mac_8x2_2x8() [2/8]

v64acc32 mac_8x2_2x8 | ( | v32int16 | a,
|  | int | sgn_x,
|  | v32uint16 | b,
|  | int | sgn_y,
|  | v64acc32 | acc )

## ◆ mac_8x2_2x8() [3/8]

v64acc32 mac_8x2_2x8 | ( | v32int16 | a,
|  | v32int16 | b,
|  | v64acc32 | acc )

## ◆ mac_8x2_2x8() [4/8]

v64acc32 mac_8x2_2x8 | ( | v32int16 | a,
|  | v32uint16 | b,
|  | v64acc32 | acc )

## ◆ mac_8x2_2x8() [5/8]

v64acc32 mac_8x2_2x8 | ( | v32uint16 | a,
|  | int | sgn_x,
|  | v32int16 | b,
|  | int | sgn_y,
|  | v64acc32 | acc )

## ◆ mac_8x2_2x8() [6/8]

v64acc32 mac_8x2_2x8 | ( | v32uint16 | a,
|  | int | sgn_x,
|  | v32uint16 | b,
|  | int | sgn_y,
|  | v64acc32 | acc )

## ◆ mac_8x2_2x8() [7/8]

v64acc32 mac_8x2_2x8 | ( | v32uint16 | a,
|  | v32int16 | b,
|  | v64acc32 | acc )

## ◆ mac_8x2_2x8() [8/8]

v64acc32 mac_8x2_2x8 | ( | v32uint16 | a,
|  | v32uint16 | b,
|  | v64acc32 | acc )

## ◆ mac_8x2_2x8_conf() [1/8]

v64acc32 mac_8x2_2x8_conf | ( | v32int16 | a,
|  | int | sgn_x,
|  | v32int16 | b,
|  | int | sgn_y,
|  | v64acc32 | acc,
|  | int | zero_acc,
|  | int | shift16,
|  | int | sub_mul,
|  | int | sub_acc1 )

## ◆ mac_8x2_2x8_conf() [2/8]

v64acc32 mac_8x2_2x8_conf | ( | v32int16 | a,
|  | int | sgn_x,
|  | v32uint16 | b,
|  | int | sgn_y,
|  | v64acc32 | acc,
|  | int | zero_acc,
|  | int | shift16,
|  | int | sub_mul,
|  | int | sub_acc1 )

## ◆ mac_8x2_2x8_conf() [3/8]

v64acc32 mac_8x2_2x8_conf | ( | v32int16 | a,
|  | v32int16 | b,
|  | v64acc32 | acc,
|  | int | zero_acc,
|  | int | shift16,
|  | int | sub_mul,
|  | int | sub_acc1 )

## ◆ mac_8x2_2x8_conf() [4/8]

v64acc32 mac_8x2_2x8_conf | ( | v32int16 | a,
|  | v32uint16 | b,
|  | v64acc32 | acc,
|  | int | zero_acc,
|  | int | shift16,
|  | int | sub_mul,
|  | int | sub_acc1 )

## ◆ mac_8x2_2x8_conf() [5/8]

v64acc32 mac_8x2_2x8_conf | ( | v32uint16 | a,
|  | int | sgn_x,
|  | v32int16 | b,
|  | int | sgn_y,
|  | v64acc32 | acc,
|  | int | zero_acc,
|  | int | shift16,
|  | int | sub_mul,
|  | int | sub_acc1 )

## ◆ mac_8x2_2x8_conf() [6/8]

v64acc32 mac_8x2_2x8_conf | ( | v32uint16 | a,
|  | int | sgn_x,
|  | v32uint16 | b,
|  | int | sgn_y,
|  | v64acc32 | acc,
|  | int | zero_acc,
|  | int | shift16,
|  | int | sub_mul,
|  | int | sub_acc1 )

## ◆ mac_8x2_2x8_conf() [7/8]

v64acc32 mac_8x2_2x8_conf | ( | v32uint16 | a,
|  | v32int16 | b,
|  | v64acc32 | acc,
|  | int | zero_acc,
|  | int | shift16,
|  | int | sub_mul,
|  | int | sub_acc1 )

## ◆ mac_8x2_2x8_conf() [8/8]

v64acc32 mac_8x2_2x8_conf | ( | v32uint16 | a,
|  | v32uint16 | b,
|  | v64acc32 | acc,
|  | int | zero_acc,
|  | int | shift16,
|  | int | sub_mul,
|  | int | sub_acc1 )

## ◆ mac_conv_32x4() [1/8]

v32acc64 mac_conv_32x4 | ( | v64int16 | a,
|  | int | sgn_x,
|  | v32int16 | b,
|  | int | sgn_y,
|  | v32acc64 | acc )

## ◆ mac_conv_32x4() [2/8]

v32acc64 mac_conv_32x4 | ( | v64int16 | a,
|  | int | sgn_x,
|  | v32uint16 | b,
|  | int | sgn_y,
|  | v32acc64 | acc )

## ◆ mac_conv_32x4() [3/8]

v32acc64 mac_conv_32x4 | ( | v64int16 | a,
|  | v32int16 | b,
|  | v32acc64 | acc )

## ◆ mac_conv_32x4() [4/8]

v32acc64 mac_conv_32x4 | ( | v64int16 | a,
|  | v32uint16 | b,
|  | v32acc64 | acc )

## ◆ mac_conv_32x4() [5/8]

v32acc64 mac_conv_32x4 | ( | v64uint16 | a,
|  | int | sgn_x,
|  | v32int16 | b,
|  | int | sgn_y,
|  | v32acc64 | acc )

## ◆ mac_conv_32x4() [6/8]

v32acc64 mac_conv_32x4 | ( | v64uint16 | a,
|  | int | sgn_x,
|  | v32uint16 | b,
|  | int | sgn_y,
|  | v32acc64 | acc )

## ◆ mac_conv_32x4() [7/8]

v32acc64 mac_conv_32x4 | ( | v64uint16 | a,
|  | v32int16 | b,
|  | v32acc64 | acc )

## ◆ mac_conv_32x4() [8/8]

v32acc64 mac_conv_32x4 | ( | v64uint16 | a,
|  | v32uint16 | b,
|  | v32acc64 | acc )

## ◆ mac_conv_32x4_conf() [1/8]

v32acc64 mac_conv_32x4_conf | ( | v64int16 | a,
|  | int | sgn_x,
|  | v32int16 | b,
|  | int | sgn_y,
|  | v32acc64 | acc,
|  | int | zero_acc,
|  | int | shift16,
|  | int | sub_mul,
|  | int | sub_acc1 )

## ◆ mac_conv_32x4_conf() [2/8]

v32acc64 mac_conv_32x4_conf | ( | v64int16 | a,
|  | int | sgn_x,
|  | v32uint16 | b,
|  | int | sgn_y,
|  | v32acc64 | acc,
|  | int | zero_acc,
|  | int | shift16,
|  | int | sub_mul,
|  | int | sub_acc1 )

## ◆ mac_conv_32x4_conf() [3/8]

v32acc64 mac_conv_32x4_conf | ( | v64int16 | a,
|  | v32int16 | b,
|  | v32acc64 | acc,
|  | int | zero_acc,
|  | int | shift16,
|  | int | sub_mul,
|  | int | sub_acc1 )

## ◆ mac_conv_32x4_conf() [4/8]

v32acc64 mac_conv_32x4_conf | ( | v64int16 | a,
|  | v32uint16 | b,
|  | v32acc64 | acc,
|  | int | zero_acc,
|  | int | shift16,
|  | int | sub_mul,
|  | int | sub_acc1 )

## ◆ mac_conv_32x4_conf() [5/8]

v32acc64 mac_conv_32x4_conf | ( | v64uint16 | a,
|  | int | sgn_x,
|  | v32int16 | b,
|  | int | sgn_y,
|  | v32acc64 | acc,
|  | int | zero_acc,
|  | int | shift16,
|  | int | sub_mul,
|  | int | sub_acc1 )

## ◆ mac_conv_32x4_conf() [6/8]

v32acc64 mac_conv_32x4_conf | ( | v64uint16 | a,
|  | int | sgn_x,
|  | v32uint16 | b,
|  | int | sgn_y,
|  | v32acc64 | acc,
|  | int | zero_acc,
|  | int | shift16,
|  | int | sub_mul,
|  | int | sub_acc1 )

## ◆ mac_conv_32x4_conf() [7/8]

v32acc64 mac_conv_32x4_conf | ( | v64uint16 | a,
|  | v32int16 | b,
|  | v32acc64 | acc,
|  | int | zero_acc,
|  | int | shift16,
|  | int | sub_mul,
|  | int | sub_acc1 )

## ◆ mac_conv_32x4_conf() [8/8]

v32acc64 mac_conv_32x4_conf | ( | v64uint16 | a,
|  | v32uint16 | b,
|  | v32acc64 | acc,
|  | int | zero_acc,
|  | int | shift16,
|  | int | sub_mul,
|  | int | sub_acc1 )

## ◆ mac_conv_4x4_8ch() [1/8]

v32acc64 mac_conv_4x4_8ch | ( | v64int16 | a,
|  | int | sgn_x,
|  | v32int16 | b,
|  | int | sgn_y,
|  | v32acc64 | acc )

## ◆ mac_conv_4x4_8ch() [2/8]

v32acc64 mac_conv_4x4_8ch | ( | v64int16 | a,
|  | int | sgn_x,
|  | v32uint16 | b,
|  | int | sgn_y,
|  | v32acc64 | acc )

## ◆ mac_conv_4x4_8ch() [3/8]

v32acc64 mac_conv_4x4_8ch | ( | v64int16 | a,
|  | v32int16 | b,
|  | v32acc64 | acc )

## ◆ mac_conv_4x4_8ch() [4/8]

v32acc64 mac_conv_4x4_8ch | ( | v64int16 | a,
|  | v32uint16 | b,
|  | v32acc64 | acc )

## ◆ mac_conv_4x4_8ch() [5/8]

v32acc64 mac_conv_4x4_8ch | ( | v64uint16 | a,
|  | int | sgn_x,
|  | v32int16 | b,
|  | int | sgn_y,
|  | v32acc64 | acc )

## ◆ mac_conv_4x4_8ch() [6/8]

v32acc64 mac_conv_4x4_8ch | ( | v64uint16 | a,
|  | int | sgn_x,
|  | v32uint16 | b,
|  | int | sgn_y,
|  | v32acc64 | acc )

## ◆ mac_conv_4x4_8ch() [7/8]

v32acc64 mac_conv_4x4_8ch | ( | v64uint16 | a,
|  | v32int16 | b,
|  | v32acc64 | acc )

## ◆ mac_conv_4x4_8ch() [8/8]

v32acc64 mac_conv_4x4_8ch | ( | v64uint16 | a,
|  | v32uint16 | b,
|  | v32acc64 | acc )

## ◆ mac_conv_4x4_8ch_conf() [1/8]

v32acc64 mac_conv_4x4_8ch_conf | ( | v64int16 | a,
|  | int | sgn_x,
|  | v32int16 | b,
|  | int | sgn_y,
|  | v32acc64 | acc,
|  | int | zero_acc,
|  | int | shift16,
|  | int | sub_mul,
|  | int | sub_acc1 )

## ◆ mac_conv_4x4_8ch_conf() [2/8]

v32acc64 mac_conv_4x4_8ch_conf | ( | v64int16 | a,
|  | int | sgn_x,
|  | v32uint16 | b,
|  | int | sgn_y,
|  | v32acc64 | acc,
|  | int | zero_acc,
|  | int | shift16,
|  | int | sub_mul,
|  | int | sub_acc1 )

## ◆ mac_conv_4x4_8ch_conf() [3/8]

v32acc64 mac_conv_4x4_8ch_conf | ( | v64int16 | a,
|  | v32int16 | b,
|  | v32acc64 | acc,
|  | int | zero_acc,
|  | int | shift16,
|  | int | sub_mul,
|  | int | sub_acc1 )

## ◆ mac_conv_4x4_8ch_conf() [4/8]

v32acc64 mac_conv_4x4_8ch_conf | ( | v64int16 | a,
|  | v32uint16 | b,
|  | v32acc64 | acc,
|  | int | zero_acc,
|  | int | shift16,
|  | int | sub_mul,
|  | int | sub_acc1 )

## ◆ mac_conv_4x4_8ch_conf() [5/8]

v32acc64 mac_conv_4x4_8ch_conf | ( | v64uint16 | a,
|  | int | sgn_x,
|  | v32int16 | b,
|  | int | sgn_y,
|  | v32acc64 | acc,
|  | int | zero_acc,
|  | int | shift16,
|  | int | sub_mul,
|  | int | sub_acc1 )

## ◆ mac_conv_4x4_8ch_conf() [6/8]

v32acc64 mac_conv_4x4_8ch_conf | ( | v64uint16 | a,
|  | int | sgn_x,
|  | v32uint16 | b,
|  | int | sgn_y,
|  | v32acc64 | acc,
|  | int | zero_acc,
|  | int | shift16,
|  | int | sub_mul,
|  | int | sub_acc1 )

## ◆ mac_conv_4x4_8ch_conf() [7/8]

v32acc64 mac_conv_4x4_8ch_conf | ( | v64uint16 | a,
|  | v32int16 | b,
|  | v32acc64 | acc,
|  | int | zero_acc,
|  | int | shift16,
|  | int | sub_mul,
|  | int | sub_acc1 )

## ◆ mac_conv_4x4_8ch_conf() [8/8]

v32acc64 mac_conv_4x4_8ch_conf | ( | v64uint16 | a,
|  | v32uint16 | b,
|  | v32acc64 | acc,
|  | int | zero_acc,
|  | int | shift16,
|  | int | sub_mul,
|  | int | sub_acc1 )

## ◆ mac_elem_32() [1/32]

v32accfloat mac_elem_32 | ( | v32bfloat16 | a,
|  | bfloat16 | b,
|  | v32accfloat | acc )

## ◆ mac_elem_32() [2/32]

v32accfloat mac_elem_32 | ( | v32bfloat16 | a,
|  | float16 | b,
|  | v32accfloat | acc )

## ◆ mac_elem_32() [3/32]

v32accfloat mac_elem_32 | ( | v32bfloat16 | a,
|  | int | sgn_x,
|  | bfloat16 | b,
|  | int | sgn_y,
|  | v32accfloat | acc )

## ◆ mac_elem_32() [4/32]

v32accfloat mac_elem_32 | ( | v32bfloat16 | a,
|  | int | sgn_x,
|  | float16 | b,
|  | int | sgn_y,
|  | v32accfloat | acc )

## ◆ mac_elem_32() [5/32]

v32accfloat mac_elem_32 | ( | v32bfloat16 | a,
|  | int | sgn_x,
|  | v32bfloat16 | b,
|  | int | sgn_y,
|  | v32accfloat | acc )

## ◆ mac_elem_32() [6/32]

v32accfloat mac_elem_32 | ( | v32bfloat16 | a,
|  | int | sgn_x,
|  | v32float16 | b,
|  | int | sgn_y,
|  | v32accfloat | acc )

## ◆ mac_elem_32() [7/32]

v32accfloat mac_elem_32 | ( | v32bfloat16 | a,
|  | v32bfloat16 | b,
|  | v32accfloat | acc )

## ◆ mac_elem_32() [8/32]

v32accfloat mac_elem_32 | ( | v32bfloat16 | a,
|  | v32float16 | b,
|  | v32accfloat | acc )

## ◆ mac_elem_32() [9/32]

v32accfloat mac_elem_32 | ( | v32float16 | a,
|  | bfloat16 | b,
|  | v32accfloat | acc )

## ◆ mac_elem_32() [10/32]

v32accfloat mac_elem_32 | ( | v32float16 | a,
|  | float16 | b,
|  | v32accfloat | acc )

## ◆ mac_elem_32() [11/32]

v32accfloat mac_elem_32 | ( | v32float16 | a,
|  | int | sgn_x,
|  | bfloat16 | b,
|  | int | sgn_y,
|  | v32accfloat | acc )

## ◆ mac_elem_32() [12/32]

v32accfloat mac_elem_32 | ( | v32float16 | a,
|  | int | sgn_x,
|  | float16 | b,
|  | int | sgn_y,
|  | v32accfloat | acc )

## ◆ mac_elem_32() [13/32]

v32accfloat mac_elem_32 | ( | v32float16 | a,
|  | int | sgn_x,
|  | v32bfloat16 | b,
|  | int | sgn_y,
|  | v32accfloat | acc )

## ◆ mac_elem_32() [14/32]

v32accfloat mac_elem_32 | ( | v32float16 | a,
|  | int | sgn_x,
|  | v32float16 | b,
|  | int | sgn_y,
|  | v32accfloat | acc )

## ◆ mac_elem_32() [15/32]

v32accfloat mac_elem_32 | ( | v32float16 | a,
|  | v32bfloat16 | b,
|  | v32accfloat | acc )

## ◆ mac_elem_32() [16/32]

v32accfloat mac_elem_32 | ( | v32float16 | a,
|  | v32float16 | b,
|  | v32accfloat | acc )

## ◆ mac_elem_32() [17/32]

v32acc64 mac_elem_32 | ( | v32int16 | a,
|  | int | sgn_x,
|  | signed short | b,
|  | int | sgn_y,
|  | v32acc64 | acc )

## ◆ mac_elem_32() [18/32]

v32acc64 mac_elem_32 | ( | v32int16 | a,
|  | int | sgn_x,
|  | unsigned short | b,
|  | int | sgn_y,
|  | v32acc64 | acc )

## ◆ mac_elem_32() [19/32]

v32acc64 mac_elem_32 | ( | v32int16 | a,
|  | int | sgn_x,
|  | v32int16 | b,
|  | int | sgn_y,
|  | v32acc64 | acc )

## ◆ mac_elem_32() [20/32]

v32acc64 mac_elem_32 | ( | v32int16 | a,
|  | int | sgn_x,
|  | v32uint16 | b,
|  | int | sgn_y,
|  | v32acc64 | acc )

## ◆ mac_elem_32() [21/32]

v32acc64 mac_elem_32 | ( | v32int16 | a,
|  | signed short | b,
|  | v32acc64 | acc )

## ◆ mac_elem_32() [22/32]

v32acc64 mac_elem_32 | ( | v32int16 | a,
|  | unsigned short | b,
|  | v32acc64 | acc )

## ◆ mac_elem_32() [23/32]

v32acc64 mac_elem_32 | ( | v32int16 | a,
|  | v32int16 | b,
|  | v32acc64 | acc )

## ◆ mac_elem_32() [24/32]

v32acc64 mac_elem_32 | ( | v32int16 | a,
|  | v32uint16 | b,
|  | v32acc64 | acc )

## ◆ mac_elem_32() [25/32]

v32acc64 mac_elem_32 | ( | v32uint16 | a,
|  | int | sgn_x,
|  | signed short | b,
|  | int | sgn_y,
|  | v32acc64 | acc )

## ◆ mac_elem_32() [26/32]

v32acc64 mac_elem_32 | ( | v32uint16 | a,
|  | int | sgn_x,
|  | unsigned short | b,
|  | int | sgn_y,
|  | v32acc64 | acc )

## ◆ mac_elem_32() [27/32]

v32acc64 mac_elem_32 | ( | v32uint16 | a,
|  | int | sgn_x,
|  | v32int16 | b,
|  | int | sgn_y,
|  | v32acc64 | acc )

## ◆ mac_elem_32() [28/32]

v32acc64 mac_elem_32 | ( | v32uint16 | a,
|  | int | sgn_x,
|  | v32uint16 | b,
|  | int | sgn_y,
|  | v32acc64 | acc )

## ◆ mac_elem_32() [29/32]

v32acc64 mac_elem_32 | ( | v32uint16 | a,
|  | signed short | b,
|  | v32acc64 | acc )

## ◆ mac_elem_32() [30/32]

v32acc64 mac_elem_32 | ( | v32uint16 | a,
|  | unsigned short | b,
|  | v32acc64 | acc )

## ◆ mac_elem_32() [31/32]

v32acc64 mac_elem_32 | ( | v32uint16 | a,
|  | v32int16 | b,
|  | v32acc64 | acc )

## ◆ mac_elem_32() [32/32]

v32acc64 mac_elem_32 | ( | v32uint16 | a,
|  | v32uint16 | b,
|  | v32acc64 | acc )

## ◆ mac_elem_32_2() [1/8]

v32acc64 mac_elem_32_2 | ( | v64int16 | a,
|  | int | sgn_x,
|  | v64int16 | b,
|  | int | sgn_y,
|  | v32acc64 | acc )

## ◆ mac_elem_32_2() [2/8]

v32acc64 mac_elem_32_2 | ( | v64int16 | a,
|  | int | sgn_x,
|  | v64uint16 | b,
|  | int | sgn_y,
|  | v32acc64 | acc )

## ◆ mac_elem_32_2() [3/8]

v32acc64 mac_elem_32_2 | ( | v64int16 | a,
|  | v64int16 | b,
|  | v32acc64 | acc )

## ◆ mac_elem_32_2() [4/8]

v32acc64 mac_elem_32_2 | ( | v64int16 | a,
|  | v64uint16 | b,
|  | v32acc64 | acc )

## ◆ mac_elem_32_2() [5/8]

v32acc64 mac_elem_32_2 | ( | v64uint16 | a,
|  | int | sgn_x,
|  | v64int16 | b,
|  | int | sgn_y,
|  | v32acc64 | acc )

## ◆ mac_elem_32_2() [6/8]

v32acc64 mac_elem_32_2 | ( | v64uint16 | a,
|  | int | sgn_x,
|  | v64uint16 | b,
|  | int | sgn_y,
|  | v32acc64 | acc )

## ◆ mac_elem_32_2() [7/8]

v32acc64 mac_elem_32_2 | ( | v64uint16 | a,
|  | v64int16 | b,
|  | v32acc64 | acc )

## ◆ mac_elem_32_2() [8/8]

v32acc64 mac_elem_32_2 | ( | v64uint16 | a,
|  | v64uint16 | b,
|  | v32acc64 | acc )

## ◆ mac_elem_32_2_conf() [1/8]

v32acc64 mac_elem_32_2_conf | ( | v64int16 | a,
|  | int | sgn_x,
|  | v64int16 | b,
|  | int | sgn_y,
|  | v32acc64 | acc,
|  | int | zero_acc,
|  | int | shift16,
|  | int | sub_mul,
|  | int | sub_acc1 )

## ◆ mac_elem_32_2_conf() [2/8]

v32acc64 mac_elem_32_2_conf | ( | v64int16 | a,
|  | int | sgn_x,
|  | v64uint16 | b,
|  | int | sgn_y,
|  | v32acc64 | acc,
|  | int | zero_acc,
|  | int | shift16,
|  | int | sub_mul,
|  | int | sub_acc1 )

## ◆ mac_elem_32_2_conf() [3/8]

v32acc64 mac_elem_32_2_conf | ( | v64int16 | a,
|  | v64int16 | b,
|  | v32acc64 | acc,
|  | int | zero_acc,
|  | int | shift16,
|  | int | sub_mul,
|  | int | sub_acc1 )

## ◆ mac_elem_32_2_conf() [4/8]

v32acc64 mac_elem_32_2_conf | ( | v64int16 | a,
|  | v64uint16 | b,
|  | v32acc64 | acc,
|  | int | zero_acc,
|  | int | shift16,
|  | int | sub_mul,
|  | int | sub_acc1 )

## ◆ mac_elem_32_2_conf() [5/8]

v32acc64 mac_elem_32_2_conf | ( | v64uint16 | a,
|  | int | sgn_x,
|  | v64int16 | b,
|  | int | sgn_y,
|  | v32acc64 | acc,
|  | int | zero_acc,
|  | int | shift16,
|  | int | sub_mul,
|  | int | sub_acc1 )

## ◆ mac_elem_32_2_conf() [6/8]

v32acc64 mac_elem_32_2_conf | ( | v64uint16 | a,
|  | int | sgn_x,
|  | v64uint16 | b,
|  | int | sgn_y,
|  | v32acc64 | acc,
|  | int | zero_acc,
|  | int | shift16,
|  | int | sub_mul,
|  | int | sub_acc1 )

## ◆ mac_elem_32_2_conf() [7/8]

v32acc64 mac_elem_32_2_conf | ( | v64uint16 | a,
|  | v64int16 | b,
|  | v32acc64 | acc,
|  | int | zero_acc,
|  | int | shift16,
|  | int | sub_mul,
|  | int | sub_acc1 )

## ◆ mac_elem_32_2_conf() [8/8]

v32acc64 mac_elem_32_2_conf | ( | v64uint16 | a,
|  | v64uint16 | b,
|  | v32acc64 | acc,
|  | int | zero_acc,
|  | int | shift16,
|  | int | sub_mul,
|  | int | sub_acc1 )

## ◆ mac_elem_32_32b() [1/8]

v32acc32 mac_elem_32_32b | ( | v32int16 | a,
|  | int | sgn_x,
|  | v32int16 | b,
|  | int | sgn_y,
|  | v32acc32 | acc )

## ◆ mac_elem_32_32b() [2/8]

v32acc32 mac_elem_32_32b | ( | v32int16 | a,
|  | int | sgn_x,
|  | v32uint16 | b,
|  | int | sgn_y,
|  | v32acc32 | acc )

## ◆ mac_elem_32_32b() [3/8]

v32acc32 mac_elem_32_32b | ( | v32int16 | a,
|  | v32int16 | b,
|  | v32acc32 | acc )

## ◆ mac_elem_32_32b() [4/8]

v32acc32 mac_elem_32_32b | ( | v32int16 | a,
|  | v32uint16 | b,
|  | v32acc32 | acc )

## ◆ mac_elem_32_32b() [5/8]

v32acc32 mac_elem_32_32b | ( | v32uint16 | a,
|  | int | sgn_x,
|  | v32int16 | b,
|  | int | sgn_y,
|  | v32acc32 | acc )

## ◆ mac_elem_32_32b() [6/8]

v32acc32 mac_elem_32_32b | ( | v32uint16 | a,
|  | int | sgn_x,
|  | v32uint16 | b,
|  | int | sgn_y,
|  | v32acc32 | acc )

## ◆ mac_elem_32_32b() [7/8]

v32acc32 mac_elem_32_32b | ( | v32uint16 | a,
|  | v32int16 | b,
|  | v32acc32 | acc )

## ◆ mac_elem_32_32b() [8/8]

v32acc32 mac_elem_32_32b | ( | v32uint16 | a,
|  | v32uint16 | b,
|  | v32acc32 | acc )

## ◆ mac_elem_32_32b_conf() [1/8]

v32acc32 mac_elem_32_32b_conf | ( | v32int16 | a,
|  | int | sgn_x,
|  | v32int16 | b,
|  | int | sgn_y,
|  | v32acc32 | acc,
|  | int | zero_acc,
|  | int | shift16,
|  | int | sub_mul,
|  | int | sub_acc1 )

## ◆ mac_elem_32_32b_conf() [2/8]

v32acc32 mac_elem_32_32b_conf | ( | v32int16 | a,
|  | int | sgn_x,
|  | v32uint16 | b,
|  | int | sgn_y,
|  | v32acc32 | acc,
|  | int | zero_acc,
|  | int | shift16,
|  | int | sub_mul,
|  | int | sub_acc1 )

## ◆ mac_elem_32_32b_conf() [3/8]

v32acc32 mac_elem_32_32b_conf | ( | v32int16 | a,
|  | v32int16 | b,
|  | v32acc32 | acc,
|  | int | zero_acc,
|  | int | shift16,
|  | int | sub_mul,
|  | int | sub_acc1 )

## ◆ mac_elem_32_32b_conf() [4/8]

v32acc32 mac_elem_32_32b_conf | ( | v32int16 | a,
|  | v32uint16 | b,
|  | v32acc32 | acc,
|  | int | zero_acc,
|  | int | shift16,
|  | int | sub_mul,
|  | int | sub_acc1 )

## ◆ mac_elem_32_32b_conf() [5/8]

v32acc32 mac_elem_32_32b_conf | ( | v32uint16 | a,
|  | int | sgn_x,
|  | v32int16 | b,
|  | int | sgn_y,
|  | v32acc32 | acc,
|  | int | zero_acc,
|  | int | shift16,
|  | int | sub_mul,
|  | int | sub_acc1 )

## ◆ mac_elem_32_32b_conf() [6/8]

v32acc32 mac_elem_32_32b_conf | ( | v32uint16 | a,
|  | int | sgn_x,
|  | v32uint16 | b,
|  | int | sgn_y,
|  | v32acc32 | acc,
|  | int | zero_acc,
|  | int | shift16,
|  | int | sub_mul,
|  | int | sub_acc1 )

## ◆ mac_elem_32_32b_conf() [7/8]

v32acc32 mac_elem_32_32b_conf | ( | v32uint16 | a,
|  | v32int16 | b,
|  | v32acc32 | acc,
|  | int | zero_acc,
|  | int | shift16,
|  | int | sub_mul,
|  | int | sub_acc1 )

## ◆ mac_elem_32_32b_conf() [8/8]

v32acc32 mac_elem_32_32b_conf | ( | v32uint16 | a,
|  | v32uint16 | b,
|  | v32acc32 | acc,
|  | int | zero_acc,
|  | int | shift16,
|  | int | sub_mul,
|  | int | sub_acc1 )

## ◆ mac_elem_32_conf() [1/32]

v32accfloat mac_elem_32_conf | ( | v32bfloat16 | a,
|  | bfloat16 | b,
|  | v32accfloat | acc,
|  | int | zero_acc,
|  | int | sub_mul,
|  | int | sub_acc1 )

## ◆ mac_elem_32_conf() [2/32]

v32accfloat mac_elem_32_conf | ( | v32bfloat16 | a,
|  | float16 | b,
|  | v32accfloat | acc,
|  | int | zero_acc,
|  | int | sub_mul,
|  | int | sub_acc1 )

## ◆ mac_elem_32_conf() [3/32]

v32accfloat mac_elem_32_conf | ( | v32bfloat16 | a,
|  | int | sgn_x,
|  | bfloat16 | b,
|  | int | sgn_y,
|  | v32accfloat | acc,
|  | int | zero_acc,
|  | int | sub_mul,
|  | int | sub_acc1 )

## ◆ mac_elem_32_conf() [4/32]

v32accfloat mac_elem_32_conf | ( | v32bfloat16 | a,
|  | int | sgn_x,
|  | float16 | b,
|  | int | sgn_y,
|  | v32accfloat | acc,
|  | int | zero_acc,
|  | int | sub_mul,
|  | int | sub_acc1 )

## ◆ mac_elem_32_conf() [5/32]

v32accfloat mac_elem_32_conf | ( | v32bfloat16 | a,
|  | int | sgn_x,
|  | v32bfloat16 | b,
|  | int | sgn_y,
|  | v32accfloat | acc,
|  | int | zero_acc,
|  | int | sub_mul,
|  | int | sub_acc1 )

## ◆ mac_elem_32_conf() [6/32]

v32accfloat mac_elem_32_conf | ( | v32bfloat16 | a,
|  | int | sgn_x,
|  | v32float16 | b,
|  | int | sgn_y,
|  | v32accfloat | acc,
|  | int | zero_acc,
|  | int | sub_mul,
|  | int | sub_acc1 )

## ◆ mac_elem_32_conf() [7/32]

v32accfloat mac_elem_32_conf | ( | v32bfloat16 | a,
|  | v32bfloat16 | b,
|  | v32accfloat | acc,
|  | int | zero_acc,
|  | int | sub_mul,
|  | int | sub_acc1 )

## ◆ mac_elem_32_conf() [8/32]

v32accfloat mac_elem_32_conf | ( | v32bfloat16 | a,
|  | v32float16 | b,
|  | v32accfloat | acc,
|  | int | zero_acc,
|  | int | sub_mul,
|  | int | sub_acc1 )

## ◆ mac_elem_32_conf() [9/32]

v32accfloat mac_elem_32_conf | ( | v32float16 | a,
|  | bfloat16 | b,
|  | v32accfloat | acc,
|  | int | zero_acc,
|  | int | sub_mul,
|  | int | sub_acc1 )

## ◆ mac_elem_32_conf() [10/32]

v32accfloat mac_elem_32_conf | ( | v32float16 | a,
|  | float16 | b,
|  | v32accfloat | acc,
|  | int | zero_acc,
|  | int | sub_mul,
|  | int | sub_acc1 )

## ◆ mac_elem_32_conf() [11/32]

v32accfloat mac_elem_32_conf | ( | v32float16 | a,
|  | int | sgn_x,
|  | bfloat16 | b,
|  | int | sgn_y,
|  | v32accfloat | acc,
|  | int | zero_acc,
|  | int | sub_mul,
|  | int | sub_acc1 )

## ◆ mac_elem_32_conf() [12/32]

v32accfloat mac_elem_32_conf | ( | v32float16 | a,
|  | int | sgn_x,
|  | float16 | b,
|  | int | sgn_y,
|  | v32accfloat | acc,
|  | int | zero_acc,
|  | int | sub_mul,
|  | int | sub_acc1 )

## ◆ mac_elem_32_conf() [13/32]

v32accfloat mac_elem_32_conf | ( | v32float16 | a,
|  | int | sgn_x,
|  | v32bfloat16 | b,
|  | int | sgn_y,
|  | v32accfloat | acc,
|  | int | zero_acc,
|  | int | sub_mul,
|  | int | sub_acc1 )

## ◆ mac_elem_32_conf() [14/32]

v32accfloat mac_elem_32_conf | ( | v32float16 | a,
|  | int | sgn_x,
|  | v32float16 | b,
|  | int | sgn_y,
|  | v32accfloat | acc,
|  | int | zero_acc,
|  | int | sub_mul,
|  | int | sub_acc1 )

## ◆ mac_elem_32_conf() [15/32]

v32accfloat mac_elem_32_conf | ( | v32float16 | a,
|  | v32bfloat16 | b,
|  | v32accfloat | acc,
|  | int | zero_acc,
|  | int | sub_mul,
|  | int | sub_acc1 )

## ◆ mac_elem_32_conf() [16/32]

v32accfloat mac_elem_32_conf | ( | v32float16 | a,
|  | v32float16 | b,
|  | v32accfloat | acc,
|  | int | zero_acc,
|  | int | sub_mul,
|  | int | sub_acc1 )

## ◆ mac_elem_32_conf() [17/32]

v32acc64 mac_elem_32_conf | ( | v32int16 | a,
|  | int | sgn_x,
|  | signed short | b,
|  | int | sgn_y,
|  | v32acc64 | acc,
|  | int | zero_acc,
|  | int | shift16,
|  | int | sub_mul,
|  | int | sub_acc1 )

## ◆ mac_elem_32_conf() [18/32]

v32acc64 mac_elem_32_conf | ( | v32int16 | a,
|  | int | sgn_x,
|  | unsigned short | b,
|  | int | sgn_y,
|  | v32acc64 | acc,
|  | int | zero_acc,
|  | int | shift16,
|  | int | sub_mul,
|  | int | sub_acc1 )

## ◆ mac_elem_32_conf() [19/32]

v32acc64 mac_elem_32_conf | ( | v32int16 | a,
|  | int | sgn_x,
|  | v32int16 | b,
|  | int | sgn_y,
|  | v32acc64 | acc,
|  | int | zero_acc,
|  | int | shift16,
|  | int | sub_mul,
|  | int | sub_acc1 )

## ◆ mac_elem_32_conf() [20/32]

v32acc64 mac_elem_32_conf | ( | v32int16 | a,
|  | int | sgn_x,
|  | v32uint16 | b,
|  | int | sgn_y,
|  | v32acc64 | acc,
|  | int | zero_acc,
|  | int | shift16,
|  | int | sub_mul,
|  | int | sub_acc1 )

## ◆ mac_elem_32_conf() [21/32]

v32acc64 mac_elem_32_conf | ( | v32int16 | a,
|  | signed short | b,
|  | v32acc64 | acc,
|  | int | zero_acc,
|  | int | shift16,
|  | int | sub_mul,
|  | int | sub_acc1 )

## ◆ mac_elem_32_conf() [22/32]

v32acc64 mac_elem_32_conf | ( | v32int16 | a,
|  | unsigned short | b,
|  | v32acc64 | acc,
|  | int | zero_acc,
|  | int | shift16,
|  | int | sub_mul,
|  | int | sub_acc1 )

## ◆ mac_elem_32_conf() [23/32]

v32acc64 mac_elem_32_conf | ( | v32int16 | a,
|  | v32int16 | b,
|  | v32acc64 | acc,
|  | int | zero_acc,
|  | int | shift16,
|  | int | sub_mul,
|  | int | sub_acc1 )

## ◆ mac_elem_32_conf() [24/32]

v32acc64 mac_elem_32_conf | ( | v32int16 | a,
|  | v32uint16 | b,
|  | v32acc64 | acc,
|  | int | zero_acc,
|  | int | shift16,
|  | int | sub_mul,
|  | int | sub_acc1 )

## ◆ mac_elem_32_conf() [25/32]

v32acc64 mac_elem_32_conf | ( | v32uint16 | a,
|  | int | sgn_x,
|  | signed short | b,
|  | int | sgn_y,
|  | v32acc64 | acc,
|  | int | zero_acc,
|  | int | shift16,
|  | int | sub_mul,
|  | int | sub_acc1 )

## ◆ mac_elem_32_conf() [26/32]

v32acc64 mac_elem_32_conf | ( | v32uint16 | a,
|  | int | sgn_x,
|  | unsigned short | b,
|  | int | sgn_y,
|  | v32acc64 | acc,
|  | int | zero_acc,
|  | int | shift16,
|  | int | sub_mul,
|  | int | sub_acc1 )

## ◆ mac_elem_32_conf() [27/32]

v32acc64 mac_elem_32_conf | ( | v32uint16 | a,
|  | int | sgn_x,
|  | v32int16 | b,
|  | int | sgn_y,
|  | v32acc64 | acc,
|  | int | zero_acc,
|  | int | shift16,
|  | int | sub_mul,
|  | int | sub_acc1 )

## ◆ mac_elem_32_conf() [28/32]

v32acc64 mac_elem_32_conf | ( | v32uint16 | a,
|  | int | sgn_x,
|  | v32uint16 | b,
|  | int | sgn_y,
|  | v32acc64 | acc,
|  | int | zero_acc,
|  | int | shift16,
|  | int | sub_mul,
|  | int | sub_acc1 )

## ◆ mac_elem_32_conf() [29/32]

v32acc64 mac_elem_32_conf | ( | v32uint16 | a,
|  | signed short | b,
|  | v32acc64 | acc,
|  | int | zero_acc,
|  | int | shift16,
|  | int | sub_mul,
|  | int | sub_acc1 )

## ◆ mac_elem_32_conf() [30/32]

v32acc64 mac_elem_32_conf | ( | v32uint16 | a,
|  | unsigned short | b,
|  | v32acc64 | acc,
|  | int | zero_acc,
|  | int | shift16,
|  | int | sub_mul,
|  | int | sub_acc1 )

## ◆ mac_elem_32_conf() [31/32]

v32acc64 mac_elem_32_conf | ( | v32uint16 | a,
|  | v32int16 | b,
|  | v32acc64 | acc,
|  | int | zero_acc,
|  | int | shift16,
|  | int | sub_mul,
|  | int | sub_acc1 )

## ◆ mac_elem_32_conf() [32/32]

v32acc64 mac_elem_32_conf | ( | v32uint16 | a,
|  | v32uint16 | b,
|  | v32acc64 | acc,
|  | int | zero_acc,
|  | int | shift16,
|  | int | sub_mul,
|  | int | sub_acc1 )

## ◆ mac_elem_64() [1/8]

v64acc32 mac_elem_64 | ( | v64int16 | a,
|  | int | sgn_x,
|  | v64int16 | b,
|  | int | sgn_y,
|  | v64acc32 | acc )

## ◆ mac_elem_64() [2/8]

v64acc32 mac_elem_64 | ( | v64int16 | a,
|  | int | sgn_x,
|  | v64uint16 | b,
|  | int | sgn_y,
|  | v64acc32 | acc )

## ◆ mac_elem_64() [3/8]

v64acc32 mac_elem_64 | ( | v64int16 | a,
|  | v64int16 | b,
|  | v64acc32 | acc )

## ◆ mac_elem_64() [4/8]

v64acc32 mac_elem_64 | ( | v64int16 | a,
|  | v64uint16 | b,
|  | v64acc32 | acc )

## ◆ mac_elem_64() [5/8]

v64acc32 mac_elem_64 | ( | v64uint16 | a,
|  | int | sgn_x,
|  | v64int16 | b,
|  | int | sgn_y,
|  | v64acc32 | acc )

## ◆ mac_elem_64() [6/8]

v64acc32 mac_elem_64 | ( | v64uint16 | a,
|  | int | sgn_x,
|  | v64uint16 | b,
|  | int | sgn_y,
|  | v64acc32 | acc )

## ◆ mac_elem_64() [7/8]

v64acc32 mac_elem_64 | ( | v64uint16 | a,
|  | v64int16 | b,
|  | v64acc32 | acc )

## ◆ mac_elem_64() [8/8]

v64acc32 mac_elem_64 | ( | v64uint16 | a,
|  | v64uint16 | b,
|  | v64acc32 | acc )

## ◆ mac_elem_64_conf() [1/8]

v64acc32 mac_elem_64_conf | ( | v64int16 | a,
|  | int | sgn_x,
|  | v64int16 | b,
|  | int | sgn_y,
|  | v64acc32 | acc,
|  | int | zero_acc,
|  | int | shift16,
|  | int | sub_mul,
|  | int | sub_acc1 )

## ◆ mac_elem_64_conf() [2/8]

v64acc32 mac_elem_64_conf | ( | v64int16 | a,
|  | int | sgn_x,
|  | v64uint16 | b,
|  | int | sgn_y,
|  | v64acc32 | acc,
|  | int | zero_acc,
|  | int | shift16,
|  | int | sub_mul,
|  | int | sub_acc1 )

## ◆ mac_elem_64_conf() [3/8]

v64acc32 mac_elem_64_conf | ( | v64int16 | a,
|  | v64int16 | b,
|  | v64acc32 | acc,
|  | int | zero_acc,
|  | int | shift16,
|  | int | sub_mul,
|  | int | sub_acc1 )

## ◆ mac_elem_64_conf() [4/8]

v64acc32 mac_elem_64_conf | ( | v64int16 | a,
|  | v64uint16 | b,
|  | v64acc32 | acc,
|  | int | zero_acc,
|  | int | shift16,
|  | int | sub_mul,
|  | int | sub_acc1 )

## ◆ mac_elem_64_conf() [5/8]

v64acc32 mac_elem_64_conf | ( | v64uint16 | a,
|  | int | sgn_x,
|  | v64int16 | b,
|  | int | sgn_y,
|  | v64acc32 | acc,
|  | int | zero_acc,
|  | int | shift16,
|  | int | sub_mul,
|  | int | sub_acc1 )

## ◆ mac_elem_64_conf() [6/8]

v64acc32 mac_elem_64_conf | ( | v64uint16 | a,
|  | int | sgn_x,
|  | v64uint16 | b,
|  | int | sgn_y,
|  | v64acc32 | acc,
|  | int | zero_acc,
|  | int | shift16,
|  | int | sub_mul,
|  | int | sub_acc1 )

## ◆ mac_elem_64_conf() [7/8]

v64acc32 mac_elem_64_conf | ( | v64uint16 | a,
|  | v64int16 | b,
|  | v64acc32 | acc,
|  | int | zero_acc,
|  | int | shift16,
|  | int | sub_mul,
|  | int | sub_acc1 )

## ◆ mac_elem_64_conf() [8/8]

v64acc32 mac_elem_64_conf | ( | v64uint16 | a,
|  | v64uint16 | b,
|  | v64acc32 | acc,
|  | int | zero_acc,
|  | int | shift16,
|  | int | sub_mul,
|  | int | sub_acc1 )

## ◆ msc_4x4_4x8() [1/8]

v32acc64 msc_4x4_4x8 | ( | v32int16 | a,
|  | int | sgn_x,
|  | v32int16 | b,
|  | int | sgn_y,
|  | v32acc64 | acc )

## ◆ msc_4x4_4x8() [2/8]

v32acc64 msc_4x4_4x8 | ( | v32int16 | a,
|  | int | sgn_x,
|  | v32uint16 | b,
|  | int | sgn_y,
|  | v32acc64 | acc )

## ◆ msc_4x4_4x8() [3/8]

v32acc64 msc_4x4_4x8 | ( | v32int16 | a,
|  | v32int16 | b,
|  | v32acc64 | acc )

## ◆ msc_4x4_4x8() [4/8]

v32acc64 msc_4x4_4x8 | ( | v32int16 | a,
|  | v32uint16 | b,
|  | v32acc64 | acc )

## ◆ msc_4x4_4x8() [5/8]

v32acc64 msc_4x4_4x8 | ( | v32uint16 | a,
|  | int | sgn_x,
|  | v32int16 | b,
|  | int | sgn_y,
|  | v32acc64 | acc )

## ◆ msc_4x4_4x8() [6/8]

v32acc64 msc_4x4_4x8 | ( | v32uint16 | a,
|  | int | sgn_x,
|  | v32uint16 | b,
|  | int | sgn_y,
|  | v32acc64 | acc )

## ◆ msc_4x4_4x8() [7/8]

v32acc64 msc_4x4_4x8 | ( | v32uint16 | a,
|  | v32int16 | b,
|  | v32acc64 | acc )

## ◆ msc_4x4_4x8() [8/8]

v32acc64 msc_4x4_4x8 | ( | v32uint16 | a,
|  | v32uint16 | b,
|  | v32acc64 | acc )

## ◆ msc_4x4_4x8_conf() [1/8]

v32acc64 msc_4x4_4x8_conf | ( | v32int16 | a,
|  | int | sgn_x,
|  | v32int16 | b,
|  | int | sgn_y,
|  | v32acc64 | acc,
|  | int | zero_acc,
|  | int | shift16,
|  | int | sub_mul,
|  | int | sub_acc1 )

## ◆ msc_4x4_4x8_conf() [2/8]

v32acc64 msc_4x4_4x8_conf | ( | v32int16 | a,
|  | int | sgn_x,
|  | v32uint16 | b,
|  | int | sgn_y,
|  | v32acc64 | acc,
|  | int | zero_acc,
|  | int | shift16,
|  | int | sub_mul,
|  | int | sub_acc1 )

## ◆ msc_4x4_4x8_conf() [3/8]

v32acc64 msc_4x4_4x8_conf | ( | v32int16 | a,
|  | v32int16 | b,
|  | v32acc64 | acc,
|  | int | zero_acc,
|  | int | shift16,
|  | int | sub_mul,
|  | int | sub_acc1 )

## ◆ msc_4x4_4x8_conf() [4/8]

v32acc64 msc_4x4_4x8_conf | ( | v32int16 | a,
|  | v32uint16 | b,
|  | v32acc64 | acc,
|  | int | zero_acc,
|  | int | shift16,
|  | int | sub_mul,
|  | int | sub_acc1 )

## ◆ msc_4x4_4x8_conf() [5/8]

v32acc64 msc_4x4_4x8_conf | ( | v32uint16 | a,
|  | int | sgn_x,
|  | v32int16 | b,
|  | int | sgn_y,
|  | v32acc64 | acc,
|  | int | zero_acc,
|  | int | shift16,
|  | int | sub_mul,
|  | int | sub_acc1 )

## ◆ msc_4x4_4x8_conf() [6/8]

v32acc64 msc_4x4_4x8_conf | ( | v32uint16 | a,
|  | int | sgn_x,
|  | v32uint16 | b,
|  | int | sgn_y,
|  | v32acc64 | acc,
|  | int | zero_acc,
|  | int | shift16,
|  | int | sub_mul,
|  | int | sub_acc1 )

## ◆ msc_4x4_4x8_conf() [7/8]

v32acc64 msc_4x4_4x8_conf | ( | v32uint16 | a,
|  | v32int16 | b,
|  | v32acc64 | acc,
|  | int | zero_acc,
|  | int | shift16,
|  | int | sub_mul,
|  | int | sub_acc1 )

## ◆ msc_4x4_4x8_conf() [8/8]

v32acc64 msc_4x4_4x8_conf | ( | v32uint16 | a,
|  | v32uint16 | b,
|  | v32acc64 | acc,
|  | int | zero_acc,
|  | int | shift16,
|  | int | sub_mul,
|  | int | sub_acc1 )

## ◆ msc_8x2_2x8() [1/8]

v64acc32 msc_8x2_2x8 | ( | v32int16 | a,
|  | int | sgn_x,
|  | v32int16 | b,
|  | int | sgn_y,
|  | v64acc32 | acc )

## ◆ msc_8x2_2x8() [2/8]

v64acc32 msc_8x2_2x8 | ( | v32int16 | a,
|  | int | sgn_x,
|  | v32uint16 | b,
|  | int | sgn_y,
|  | v64acc32 | acc )

## ◆ msc_8x2_2x8() [3/8]

v64acc32 msc_8x2_2x8 | ( | v32int16 | a,
|  | v32int16 | b,
|  | v64acc32 | acc )

## ◆ msc_8x2_2x8() [4/8]

v64acc32 msc_8x2_2x8 | ( | v32int16 | a,
|  | v32uint16 | b,
|  | v64acc32 | acc )

## ◆ msc_8x2_2x8() [5/8]

v64acc32 msc_8x2_2x8 | ( | v32uint16 | a,
|  | int | sgn_x,
|  | v32int16 | b,
|  | int | sgn_y,
|  | v64acc32 | acc )

## ◆ msc_8x2_2x8() [6/8]

v64acc32 msc_8x2_2x8 | ( | v32uint16 | a,
|  | int | sgn_x,
|  | v32uint16 | b,
|  | int | sgn_y,
|  | v64acc32 | acc )

## ◆ msc_8x2_2x8() [7/8]

v64acc32 msc_8x2_2x8 | ( | v32uint16 | a,
|  | v32int16 | b,
|  | v64acc32 | acc )

## ◆ msc_8x2_2x8() [8/8]

v64acc32 msc_8x2_2x8 | ( | v32uint16 | a,
|  | v32uint16 | b,
|  | v64acc32 | acc )

## ◆ msc_8x2_2x8_conf() [1/8]

v64acc32 msc_8x2_2x8_conf | ( | v32int16 | a,
|  | int | sgn_x,
|  | v32int16 | b,
|  | int | sgn_y,
|  | v64acc32 | acc,
|  | int | zero_acc,
|  | int | shift16,
|  | int | sub_mul,
|  | int | sub_acc1 )

## ◆ msc_8x2_2x8_conf() [2/8]

v64acc32 msc_8x2_2x8_conf | ( | v32int16 | a,
|  | int | sgn_x,
|  | v32uint16 | b,
|  | int | sgn_y,
|  | v64acc32 | acc,
|  | int | zero_acc,
|  | int | shift16,
|  | int | sub_mul,
|  | int | sub_acc1 )

## ◆ msc_8x2_2x8_conf() [3/8]

v64acc32 msc_8x2_2x8_conf | ( | v32int16 | a,
|  | v32int16 | b,
|  | v64acc32 | acc,
|  | int | zero_acc,
|  | int | shift16,
|  | int | sub_mul,
|  | int | sub_acc1 )

## ◆ msc_8x2_2x8_conf() [4/8]

v64acc32 msc_8x2_2x8_conf | ( | v32int16 | a,
|  | v32uint16 | b,
|  | v64acc32 | acc,
|  | int | zero_acc,
|  | int | shift16,
|  | int | sub_mul,
|  | int | sub_acc1 )

## ◆ msc_8x2_2x8_conf() [5/8]

v64acc32 msc_8x2_2x8_conf | ( | v32uint16 | a,
|  | int | sgn_x,
|  | v32int16 | b,
|  | int | sgn_y,
|  | v64acc32 | acc,
|  | int | zero_acc,
|  | int | shift16,
|  | int | sub_mul,
|  | int | sub_acc1 )

## ◆ msc_8x2_2x8_conf() [6/8]

v64acc32 msc_8x2_2x8_conf | ( | v32uint16 | a,
|  | int | sgn_x,
|  | v32uint16 | b,
|  | int | sgn_y,
|  | v64acc32 | acc,
|  | int | zero_acc,
|  | int | shift16,
|  | int | sub_mul,
|  | int | sub_acc1 )

## ◆ msc_8x2_2x8_conf() [7/8]

v64acc32 msc_8x2_2x8_conf | ( | v32uint16 | a,
|  | v32int16 | b,
|  | v64acc32 | acc,
|  | int | zero_acc,
|  | int | shift16,
|  | int | sub_mul,
|  | int | sub_acc1 )

## ◆ msc_8x2_2x8_conf() [8/8]

v64acc32 msc_8x2_2x8_conf | ( | v32uint16 | a,
|  | v32uint16 | b,
|  | v64acc32 | acc,
|  | int | zero_acc,
|  | int | shift16,
|  | int | sub_mul,
|  | int | sub_acc1 )

## ◆ msc_conv_32x4() [1/8]

v32acc64 msc_conv_32x4 | ( | v64int16 | a,
|  | int | sgn_x,
|  | v32int16 | b,
|  | int | sgn_y,
|  | v32acc64 | acc )

## ◆ msc_conv_32x4() [2/8]

v32acc64 msc_conv_32x4 | ( | v64int16 | a,
|  | int | sgn_x,
|  | v32uint16 | b,
|  | int | sgn_y,
|  | v32acc64 | acc )

## ◆ msc_conv_32x4() [3/8]

v32acc64 msc_conv_32x4 | ( | v64int16 | a,
|  | v32int16 | b,
|  | v32acc64 | acc )

## ◆ msc_conv_32x4() [4/8]

v32acc64 msc_conv_32x4 | ( | v64int16 | a,
|  | v32uint16 | b,
|  | v32acc64 | acc )

## ◆ msc_conv_32x4() [5/8]

v32acc64 msc_conv_32x4 | ( | v64uint16 | a,
|  | int | sgn_x,
|  | v32int16 | b,
|  | int | sgn_y,
|  | v32acc64 | acc )

## ◆ msc_conv_32x4() [6/8]

v32acc64 msc_conv_32x4 | ( | v64uint16 | a,
|  | int | sgn_x,
|  | v32uint16 | b,
|  | int | sgn_y,
|  | v32acc64 | acc )

## ◆ msc_conv_32x4() [7/8]

v32acc64 msc_conv_32x4 | ( | v64uint16 | a,
|  | v32int16 | b,
|  | v32acc64 | acc )

## ◆ msc_conv_32x4() [8/8]

v32acc64 msc_conv_32x4 | ( | v64uint16 | a,
|  | v32uint16 | b,
|  | v32acc64 | acc )

## ◆ msc_conv_32x4_conf() [1/8]

v32acc64 msc_conv_32x4_conf | ( | v64int16 | a,
|  | int | sgn_x,
|  | v32int16 | b,
|  | int | sgn_y,
|  | v32acc64 | acc,
|  | int | zero_acc,
|  | int | shift16,
|  | int | sub_mul,
|  | int | sub_acc1 )

## ◆ msc_conv_32x4_conf() [2/8]

v32acc64 msc_conv_32x4_conf | ( | v64int16 | a,
|  | int | sgn_x,
|  | v32uint16 | b,
|  | int | sgn_y,
|  | v32acc64 | acc,
|  | int | zero_acc,
|  | int | shift16,
|  | int | sub_mul,
|  | int | sub_acc1 )

## ◆ msc_conv_32x4_conf() [3/8]

v32acc64 msc_conv_32x4_conf | ( | v64int16 | a,
|  | v32int16 | b,
|  | v32acc64 | acc,
|  | int | zero_acc,
|  | int | shift16,
|  | int | sub_mul,
|  | int | sub_acc1 )

## ◆ msc_conv_32x4_conf() [4/8]

v32acc64 msc_conv_32x4_conf | ( | v64int16 | a,
|  | v32uint16 | b,
|  | v32acc64 | acc,
|  | int | zero_acc,
|  | int | shift16,
|  | int | sub_mul,
|  | int | sub_acc1 )

## ◆ msc_conv_32x4_conf() [5/8]

v32acc64 msc_conv_32x4_conf | ( | v64uint16 | a,
|  | int | sgn_x,
|  | v32int16 | b,
|  | int | sgn_y,
|  | v32acc64 | acc,
|  | int | zero_acc,
|  | int | shift16,
|  | int | sub_mul,
|  | int | sub_acc1 )

## ◆ msc_conv_32x4_conf() [6/8]

v32acc64 msc_conv_32x4_conf | ( | v64uint16 | a,
|  | int | sgn_x,
|  | v32uint16 | b,
|  | int | sgn_y,
|  | v32acc64 | acc,
|  | int | zero_acc,
|  | int | shift16,
|  | int | sub_mul,
|  | int | sub_acc1 )

## ◆ msc_conv_32x4_conf() [7/8]

v32acc64 msc_conv_32x4_conf | ( | v64uint16 | a,
|  | v32int16 | b,
|  | v32acc64 | acc,
|  | int | zero_acc,
|  | int | shift16,
|  | int | sub_mul,
|  | int | sub_acc1 )

## ◆ msc_conv_32x4_conf() [8/8]

v32acc64 msc_conv_32x4_conf | ( | v64uint16 | a,
|  | v32uint16 | b,
|  | v32acc64 | acc,
|  | int | zero_acc,
|  | int | shift16,
|  | int | sub_mul,
|  | int | sub_acc1 )

## ◆ msc_conv_4x4_8ch() [1/8]

v32acc64 msc_conv_4x4_8ch | ( | v64int16 | a,
|  | int | sgn_x,
|  | v32int16 | b,
|  | int | sgn_y,
|  | v32acc64 | acc )

## ◆ msc_conv_4x4_8ch() [2/8]

v32acc64 msc_conv_4x4_8ch | ( | v64int16 | a,
|  | int | sgn_x,
|  | v32uint16 | b,
|  | int | sgn_y,
|  | v32acc64 | acc )

## ◆ msc_conv_4x4_8ch() [3/8]

v32acc64 msc_conv_4x4_8ch | ( | v64int16 | a,
|  | v32int16 | b,
|  | v32acc64 | acc )

## ◆ msc_conv_4x4_8ch() [4/8]

v32acc64 msc_conv_4x4_8ch | ( | v64int16 | a,
|  | v32uint16 | b,
|  | v32acc64 | acc )

## ◆ msc_conv_4x4_8ch() [5/8]

v32acc64 msc_conv_4x4_8ch | ( | v64uint16 | a,
|  | int | sgn_x,
|  | v32int16 | b,
|  | int | sgn_y,
|  | v32acc64 | acc )

## ◆ msc_conv_4x4_8ch() [6/8]

v32acc64 msc_conv_4x4_8ch | ( | v64uint16 | a,
|  | int | sgn_x,
|  | v32uint16 | b,
|  | int | sgn_y,
|  | v32acc64 | acc )

## ◆ msc_conv_4x4_8ch() [7/8]

v32acc64 msc_conv_4x4_8ch | ( | v64uint16 | a,
|  | v32int16 | b,
|  | v32acc64 | acc )

## ◆ msc_conv_4x4_8ch() [8/8]

v32acc64 msc_conv_4x4_8ch | ( | v64uint16 | a,
|  | v32uint16 | b,
|  | v32acc64 | acc )

## ◆ msc_conv_4x4_8ch_conf() [1/8]

v32acc64 msc_conv_4x4_8ch_conf | ( | v64int16 | a,
|  | int | sgn_x,
|  | v32int16 | b,
|  | int | sgn_y,
|  | v32acc64 | acc,
|  | int | zero_acc,
|  | int | shift16,
|  | int | sub_mul,
|  | int | sub_acc1 )

## ◆ msc_conv_4x4_8ch_conf() [2/8]

v32acc64 msc_conv_4x4_8ch_conf | ( | v64int16 | a,
|  | int | sgn_x,
|  | v32uint16 | b,
|  | int | sgn_y,
|  | v32acc64 | acc,
|  | int | zero_acc,
|  | int | shift16,
|  | int | sub_mul,
|  | int | sub_acc1 )

## ◆ msc_conv_4x4_8ch_conf() [3/8]

v32acc64 msc_conv_4x4_8ch_conf | ( | v64int16 | a,
|  | v32int16 | b,
|  | v32acc64 | acc,
|  | int | zero_acc,
|  | int | shift16,
|  | int | sub_mul,
|  | int | sub_acc1 )

## ◆ msc_conv_4x4_8ch_conf() [4/8]

v32acc64 msc_conv_4x4_8ch_conf | ( | v64int16 | a,
|  | v32uint16 | b,
|  | v32acc64 | acc,
|  | int | zero_acc,
|  | int | shift16,
|  | int | sub_mul,
|  | int | sub_acc1 )

## ◆ msc_conv_4x4_8ch_conf() [5/8]

v32acc64 msc_conv_4x4_8ch_conf | ( | v64uint16 | a,
|  | int | sgn_x,
|  | v32int16 | b,
|  | int | sgn_y,
|  | v32acc64 | acc,
|  | int | zero_acc,
|  | int | shift16,
|  | int | sub_mul,
|  | int | sub_acc1 )

## ◆ msc_conv_4x4_8ch_conf() [6/8]

v32acc64 msc_conv_4x4_8ch_conf | ( | v64uint16 | a,
|  | int | sgn_x,
|  | v32uint16 | b,
|  | int | sgn_y,
|  | v32acc64 | acc,
|  | int | zero_acc,
|  | int | shift16,
|  | int | sub_mul,
|  | int | sub_acc1 )

## ◆ msc_conv_4x4_8ch_conf() [7/8]

v32acc64 msc_conv_4x4_8ch_conf | ( | v64uint16 | a,
|  | v32int16 | b,
|  | v32acc64 | acc,
|  | int | zero_acc,
|  | int | shift16,
|  | int | sub_mul,
|  | int | sub_acc1 )

## ◆ msc_conv_4x4_8ch_conf() [8/8]

v32acc64 msc_conv_4x4_8ch_conf | ( | v64uint16 | a,
|  | v32uint16 | b,
|  | v32acc64 | acc,
|  | int | zero_acc,
|  | int | shift16,
|  | int | sub_mul,
|  | int | sub_acc1 )

## ◆ msc_elem_32() [1/32]

v32accfloat msc_elem_32 | ( | v32bfloat16 | a,
|  | bfloat16 | b,
|  | v32accfloat | acc )

## ◆ msc_elem_32() [2/32]

v32accfloat msc_elem_32 | ( | v32bfloat16 | a,
|  | float16 | b,
|  | v32accfloat | acc )

## ◆ msc_elem_32() [3/32]

v32accfloat msc_elem_32 | ( | v32bfloat16 | a,
|  | int | sgn_x,
|  | bfloat16 | b,
|  | int | sgn_y,
|  | v32accfloat | acc )

## ◆ msc_elem_32() [4/32]

v32accfloat msc_elem_32 | ( | v32bfloat16 | a,
|  | int | sgn_x,
|  | float16 | b,
|  | int | sgn_y,
|  | v32accfloat | acc )

## ◆ msc_elem_32() [5/32]

v32accfloat msc_elem_32 | ( | v32bfloat16 | a,
|  | int | sgn_x,
|  | v32bfloat16 | b,
|  | int | sgn_y,
|  | v32accfloat | acc )

## ◆ msc_elem_32() [6/32]

v32accfloat msc_elem_32 | ( | v32bfloat16 | a,
|  | int | sgn_x,
|  | v32float16 | b,
|  | int | sgn_y,
|  | v32accfloat | acc )

## ◆ msc_elem_32() [7/32]

v32accfloat msc_elem_32 | ( | v32bfloat16 | a,
|  | v32bfloat16 | b,
|  | v32accfloat | acc )

## ◆ msc_elem_32() [8/32]

v32accfloat msc_elem_32 | ( | v32bfloat16 | a,
|  | v32float16 | b,
|  | v32accfloat | acc )

## ◆ msc_elem_32() [9/32]

v32accfloat msc_elem_32 | ( | v32float16 | a,
|  | bfloat16 | b,
|  | v32accfloat | acc )

## ◆ msc_elem_32() [10/32]

v32accfloat msc_elem_32 | ( | v32float16 | a,
|  | float16 | b,
|  | v32accfloat | acc )

## ◆ msc_elem_32() [11/32]

v32accfloat msc_elem_32 | ( | v32float16 | a,
|  | int | sgn_x,
|  | bfloat16 | b,
|  | int | sgn_y,
|  | v32accfloat | acc )

## ◆ msc_elem_32() [12/32]

v32accfloat msc_elem_32 | ( | v32float16 | a,
|  | int | sgn_x,
|  | float16 | b,
|  | int | sgn_y,
|  | v32accfloat | acc )

## ◆ msc_elem_32() [13/32]

v32accfloat msc_elem_32 | ( | v32float16 | a,
|  | int | sgn_x,
|  | v32bfloat16 | b,
|  | int | sgn_y,
|  | v32accfloat | acc )

## ◆ msc_elem_32() [14/32]

v32accfloat msc_elem_32 | ( | v32float16 | a,
|  | int | sgn_x,
|  | v32float16 | b,
|  | int | sgn_y,
|  | v32accfloat | acc )

## ◆ msc_elem_32() [15/32]

v32accfloat msc_elem_32 | ( | v32float16 | a,
|  | v32bfloat16 | b,
|  | v32accfloat | acc )

## ◆ msc_elem_32() [16/32]

v32accfloat msc_elem_32 | ( | v32float16 | a,
|  | v32float16 | b,
|  | v32accfloat | acc )

## ◆ msc_elem_32() [17/32]

v32acc64 msc_elem_32 | ( | v32int16 | a,
|  | int | sgn_x,
|  | signed short | b,
|  | int | sgn_y,
|  | v32acc64 | acc )

## ◆ msc_elem_32() [18/32]

v32acc64 msc_elem_32 | ( | v32int16 | a,
|  | int | sgn_x,
|  | unsigned short | b,
|  | int | sgn_y,
|  | v32acc64 | acc )

## ◆ msc_elem_32() [19/32]

v32acc64 msc_elem_32 | ( | v32int16 | a,
|  | int | sgn_x,
|  | v32int16 | b,
|  | int | sgn_y,
|  | v32acc64 | acc )

## ◆ msc_elem_32() [20/32]

v32acc64 msc_elem_32 | ( | v32int16 | a,
|  | int | sgn_x,
|  | v32uint16 | b,
|  | int | sgn_y,
|  | v32acc64 | acc )

## ◆ msc_elem_32() [21/32]

v32acc64 msc_elem_32 | ( | v32int16 | a,
|  | signed short | b,
|  | v32acc64 | acc )

## ◆ msc_elem_32() [22/32]

v32acc64 msc_elem_32 | ( | v32int16 | a,
|  | unsigned short | b,
|  | v32acc64 | acc )

## ◆ msc_elem_32() [23/32]

v32acc64 msc_elem_32 | ( | v32int16 | a,
|  | v32int16 | b,
|  | v32acc64 | acc )

## ◆ msc_elem_32() [24/32]

v32acc64 msc_elem_32 | ( | v32int16 | a,
|  | v32uint16 | b,
|  | v32acc64 | acc )

## ◆ msc_elem_32() [25/32]

v32acc64 msc_elem_32 | ( | v32uint16 | a,
|  | int | sgn_x,
|  | signed short | b,
|  | int | sgn_y,
|  | v32acc64 | acc )

## ◆ msc_elem_32() [26/32]

v32acc64 msc_elem_32 | ( | v32uint16 | a,
|  | int | sgn_x,
|  | unsigned short | b,
|  | int | sgn_y,
|  | v32acc64 | acc )

## ◆ msc_elem_32() [27/32]

v32acc64 msc_elem_32 | ( | v32uint16 | a,
|  | int | sgn_x,
|  | v32int16 | b,
|  | int | sgn_y,
|  | v32acc64 | acc )

## ◆ msc_elem_32() [28/32]

v32acc64 msc_elem_32 | ( | v32uint16 | a,
|  | int | sgn_x,
|  | v32uint16 | b,
|  | int | sgn_y,
|  | v32acc64 | acc )

## ◆ msc_elem_32() [29/32]

v32acc64 msc_elem_32 | ( | v32uint16 | a,
|  | signed short | b,
|  | v32acc64 | acc )

## ◆ msc_elem_32() [30/32]

v32acc64 msc_elem_32 | ( | v32uint16 | a,
|  | unsigned short | b,
|  | v32acc64 | acc )

## ◆ msc_elem_32() [31/32]

v32acc64 msc_elem_32 | ( | v32uint16 | a,
|  | v32int16 | b,
|  | v32acc64 | acc )

## ◆ msc_elem_32() [32/32]

v32acc64 msc_elem_32 | ( | v32uint16 | a,
|  | v32uint16 | b,
|  | v32acc64 | acc )

## ◆ msc_elem_32_2() [1/8]

v32acc64 msc_elem_32_2 | ( | v64int16 | a,
|  | int | sgn_x,
|  | v64int16 | b,
|  | int | sgn_y,
|  | v32acc64 | acc )

## ◆ msc_elem_32_2() [2/8]

v32acc64 msc_elem_32_2 | ( | v64int16 | a,
|  | int | sgn_x,
|  | v64uint16 | b,
|  | int | sgn_y,
|  | v32acc64 | acc )

## ◆ msc_elem_32_2() [3/8]

v32acc64 msc_elem_32_2 | ( | v64int16 | a,
|  | v64int16 | b,
|  | v32acc64 | acc )

## ◆ msc_elem_32_2() [4/8]

v32acc64 msc_elem_32_2 | ( | v64int16 | a,
|  | v64uint16 | b,
|  | v32acc64 | acc )

## ◆ msc_elem_32_2() [5/8]

v32acc64 msc_elem_32_2 | ( | v64uint16 | a,
|  | int | sgn_x,
|  | v64int16 | b,
|  | int | sgn_y,
|  | v32acc64 | acc )

## ◆ msc_elem_32_2() [6/8]

v32acc64 msc_elem_32_2 | ( | v64uint16 | a,
|  | int | sgn_x,
|  | v64uint16 | b,
|  | int | sgn_y,
|  | v32acc64 | acc )

## ◆ msc_elem_32_2() [7/8]

v32acc64 msc_elem_32_2 | ( | v64uint16 | a,
|  | v64int16 | b,
|  | v32acc64 | acc )

## ◆ msc_elem_32_2() [8/8]

v32acc64 msc_elem_32_2 | ( | v64uint16 | a,
|  | v64uint16 | b,
|  | v32acc64 | acc )

## ◆ msc_elem_32_2_conf() [1/8]

v32acc64 msc_elem_32_2_conf | ( | v64int16 | a,
|  | int | sgn_x,
|  | v64int16 | b,
|  | int | sgn_y,
|  | v32acc64 | acc,
|  | int | zero_acc,
|  | int | shift16,
|  | int | sub_mul,
|  | int | sub_acc1 )

## ◆ msc_elem_32_2_conf() [2/8]

v32acc64 msc_elem_32_2_conf | ( | v64int16 | a,
|  | int | sgn_x,
|  | v64uint16 | b,
|  | int | sgn_y,
|  | v32acc64 | acc,
|  | int | zero_acc,
|  | int | shift16,
|  | int | sub_mul,
|  | int | sub_acc1 )

## ◆ msc_elem_32_2_conf() [3/8]

v32acc64 msc_elem_32_2_conf | ( | v64int16 | a,
|  | v64int16 | b,
|  | v32acc64 | acc,
|  | int | zero_acc,
|  | int | shift16,
|  | int | sub_mul,
|  | int | sub_acc1 )

## ◆ msc_elem_32_2_conf() [4/8]

v32acc64 msc_elem_32_2_conf | ( | v64int16 | a,
|  | v64uint16 | b,
|  | v32acc64 | acc,
|  | int | zero_acc,
|  | int | shift16,
|  | int | sub_mul,
|  | int | sub_acc1 )

## ◆ msc_elem_32_2_conf() [5/8]

v32acc64 msc_elem_32_2_conf | ( | v64uint16 | a,
|  | int | sgn_x,
|  | v64int16 | b,
|  | int | sgn_y,
|  | v32acc64 | acc,
|  | int | zero_acc,
|  | int | shift16,
|  | int | sub_mul,
|  | int | sub_acc1 )

## ◆ msc_elem_32_2_conf() [6/8]

v32acc64 msc_elem_32_2_conf | ( | v64uint16 | a,
|  | int | sgn_x,
|  | v64uint16 | b,
|  | int | sgn_y,
|  | v32acc64 | acc,
|  | int | zero_acc,
|  | int | shift16,
|  | int | sub_mul,
|  | int | sub_acc1 )

## ◆ msc_elem_32_2_conf() [7/8]

v32acc64 msc_elem_32_2_conf | ( | v64uint16 | a,
|  | v64int16 | b,
|  | v32acc64 | acc,
|  | int | zero_acc,
|  | int | shift16,
|  | int | sub_mul,
|  | int | sub_acc1 )

## ◆ msc_elem_32_2_conf() [8/8]

v32acc64 msc_elem_32_2_conf | ( | v64uint16 | a,
|  | v64uint16 | b,
|  | v32acc64 | acc,
|  | int | zero_acc,
|  | int | shift16,
|  | int | sub_mul,
|  | int | sub_acc1 )

## ◆ msc_elem_32_32b() [1/8]

v32acc32 msc_elem_32_32b | ( | v32int16 | a,
|  | int | sgn_x,
|  | v32int16 | b,
|  | int | sgn_y,
|  | v32acc32 | acc )

## ◆ msc_elem_32_32b() [2/8]

v32acc32 msc_elem_32_32b | ( | v32int16 | a,
|  | int | sgn_x,
|  | v32uint16 | b,
|  | int | sgn_y,
|  | v32acc32 | acc )

## ◆ msc_elem_32_32b() [3/8]

v32acc32 msc_elem_32_32b | ( | v32int16 | a,
|  | v32int16 | b,
|  | v32acc32 | acc )

## ◆ msc_elem_32_32b() [4/8]

v32acc32 msc_elem_32_32b | ( | v32int16 | a,
|  | v32uint16 | b,
|  | v32acc32 | acc )

## ◆ msc_elem_32_32b() [5/8]

v32acc32 msc_elem_32_32b | ( | v32uint16 | a,
|  | int | sgn_x,
|  | v32int16 | b,
|  | int | sgn_y,
|  | v32acc32 | acc )

## ◆ msc_elem_32_32b() [6/8]

v32acc32 msc_elem_32_32b | ( | v32uint16 | a,
|  | int | sgn_x,
|  | v32uint16 | b,
|  | int | sgn_y,
|  | v32acc32 | acc )

## ◆ msc_elem_32_32b() [7/8]

v32acc32 msc_elem_32_32b | ( | v32uint16 | a,
|  | v32int16 | b,
|  | v32acc32 | acc )

## ◆ msc_elem_32_32b() [8/8]

v32acc32 msc_elem_32_32b | ( | v32uint16 | a,
|  | v32uint16 | b,
|  | v32acc32 | acc )

## ◆ msc_elem_32_32b_conf() [1/8]

v32acc32 msc_elem_32_32b_conf | ( | v32int16 | a,
|  | int | sgn_x,
|  | v32int16 | b,
|  | int | sgn_y,
|  | v32acc32 | acc,
|  | int | zero_acc,
|  | int | shift16,
|  | int | sub_mul,
|  | int | sub_acc1 )

## ◆ msc_elem_32_32b_conf() [2/8]

v32acc32 msc_elem_32_32b_conf | ( | v32int16 | a,
|  | int | sgn_x,
|  | v32uint16 | b,
|  | int | sgn_y,
|  | v32acc32 | acc,
|  | int | zero_acc,
|  | int | shift16,
|  | int | sub_mul,
|  | int | sub_acc1 )

## ◆ msc_elem_32_32b_conf() [3/8]

v32acc32 msc_elem_32_32b_conf | ( | v32int16 | a,
|  | v32int16 | b,
|  | v32acc32 | acc,
|  | int | zero_acc,
|  | int | shift16,
|  | int | sub_mul,
|  | int | sub_acc1 )

## ◆ msc_elem_32_32b_conf() [4/8]

v32acc32 msc_elem_32_32b_conf | ( | v32int16 | a,
|  | v32uint16 | b,
|  | v32acc32 | acc,
|  | int | zero_acc,
|  | int | shift16,
|  | int | sub_mul,
|  | int | sub_acc1 )

## ◆ msc_elem_32_32b_conf() [5/8]

v32acc32 msc_elem_32_32b_conf | ( | v32uint16 | a,
|  | int | sgn_x,
|  | v32int16 | b,
|  | int | sgn_y,
|  | v32acc32 | acc,
|  | int | zero_acc,
|  | int | shift16,
|  | int | sub_mul,
|  | int | sub_acc1 )

## ◆ msc_elem_32_32b_conf() [6/8]

v32acc32 msc_elem_32_32b_conf | ( | v32uint16 | a,
|  | int | sgn_x,
|  | v32uint16 | b,
|  | int | sgn_y,
|  | v32acc32 | acc,
|  | int | zero_acc,
|  | int | shift16,
|  | int | sub_mul,
|  | int | sub_acc1 )

## ◆ msc_elem_32_32b_conf() [7/8]

v32acc32 msc_elem_32_32b_conf | ( | v32uint16 | a,
|  | v32int16 | b,
|  | v32acc32 | acc,
|  | int | zero_acc,
|  | int | shift16,
|  | int | sub_mul,
|  | int | sub_acc1 )

## ◆ msc_elem_32_32b_conf() [8/8]

v32acc32 msc_elem_32_32b_conf | ( | v32uint16 | a,
|  | v32uint16 | b,
|  | v32acc32 | acc,
|  | int | zero_acc,
|  | int | shift16,
|  | int | sub_mul,
|  | int | sub_acc1 )

## ◆ msc_elem_32_conf() [1/32]

v32accfloat msc_elem_32_conf | ( | v32bfloat16 | a,
|  | bfloat16 | b,
|  | v32accfloat | acc,
|  | int | zero_acc,
|  | int | sub_mul,
|  | int | sub_acc1 )

## ◆ msc_elem_32_conf() [2/32]

v32accfloat msc_elem_32_conf | ( | v32bfloat16 | a,
|  | float16 | b,
|  | v32accfloat | acc,
|  | int | zero_acc,
|  | int | sub_mul,
|  | int | sub_acc1 )

## ◆ msc_elem_32_conf() [3/32]

v32accfloat msc_elem_32_conf | ( | v32bfloat16 | a,
|  | int | sgn_x,
|  | bfloat16 | b,
|  | int | sgn_y,
|  | v32accfloat | acc,
|  | int | zero_acc,
|  | int | sub_mul,
|  | int | sub_acc1 )

## ◆ msc_elem_32_conf() [4/32]

v32accfloat msc_elem_32_conf | ( | v32bfloat16 | a,
|  | int | sgn_x,
|  | float16 | b,
|  | int | sgn_y,
|  | v32accfloat | acc,
|  | int | zero_acc,
|  | int | sub_mul,
|  | int | sub_acc1 )

## ◆ msc_elem_32_conf() [5/32]

v32accfloat msc_elem_32_conf | ( | v32bfloat16 | a,
|  | int | sgn_x,
|  | v32bfloat16 | b,
|  | int | sgn_y,
|  | v32accfloat | acc,
|  | int | zero_acc,
|  | int | sub_mul,
|  | int | sub_acc1 )

## ◆ msc_elem_32_conf() [6/32]

v32accfloat msc_elem_32_conf | ( | v32bfloat16 | a,
|  | int | sgn_x,
|  | v32float16 | b,
|  | int | sgn_y,
|  | v32accfloat | acc,
|  | int | zero_acc,
|  | int | sub_mul,
|  | int | sub_acc1 )

## ◆ msc_elem_32_conf() [7/32]

v32accfloat msc_elem_32_conf | ( | v32bfloat16 | a,
|  | v32bfloat16 | b,
|  | v32accfloat | acc,
|  | int | zero_acc,
|  | int | sub_mul,
|  | int | sub_acc1 )

## ◆ msc_elem_32_conf() [8/32]

v32accfloat msc_elem_32_conf | ( | v32bfloat16 | a,
|  | v32float16 | b,
|  | v32accfloat | acc,
|  | int | zero_acc,
|  | int | sub_mul,
|  | int | sub_acc1 )

## ◆ msc_elem_32_conf() [9/32]

v32accfloat msc_elem_32_conf | ( | v32float16 | a,
|  | bfloat16 | b,
|  | v32accfloat | acc,
|  | int | zero_acc,
|  | int | sub_mul,
|  | int | sub_acc1 )

## ◆ msc_elem_32_conf() [10/32]

v32accfloat msc_elem_32_conf | ( | v32float16 | a,
|  | float16 | b,
|  | v32accfloat | acc,
|  | int | zero_acc,
|  | int | sub_mul,
|  | int | sub_acc1 )

## ◆ msc_elem_32_conf() [11/32]

v32accfloat msc_elem_32_conf | ( | v32float16 | a,
|  | int | sgn_x,
|  | bfloat16 | b,
|  | int | sgn_y,
|  | v32accfloat | acc,
|  | int | zero_acc,
|  | int | sub_mul,
|  | int | sub_acc1 )

## ◆ msc_elem_32_conf() [12/32]

v32accfloat msc_elem_32_conf | ( | v32float16 | a,
|  | int | sgn_x,
|  | float16 | b,
|  | int | sgn_y,
|  | v32accfloat | acc,
|  | int | zero_acc,
|  | int | sub_mul,
|  | int | sub_acc1 )

## ◆ msc_elem_32_conf() [13/32]

v32accfloat msc_elem_32_conf | ( | v32float16 | a,
|  | int | sgn_x,
|  | v32bfloat16 | b,
|  | int | sgn_y,
|  | v32accfloat | acc,
|  | int | zero_acc,
|  | int | sub_mul,
|  | int | sub_acc1 )

## ◆ msc_elem_32_conf() [14/32]

v32accfloat msc_elem_32_conf | ( | v32float16 | a,
|  | int | sgn_x,
|  | v32float16 | b,
|  | int | sgn_y,
|  | v32accfloat | acc,
|  | int | zero_acc,
|  | int | sub_mul,
|  | int | sub_acc1 )

## ◆ msc_elem_32_conf() [15/32]

v32accfloat msc_elem_32_conf | ( | v32float16 | a,
|  | v32bfloat16 | b,
|  | v32accfloat | acc,
|  | int | zero_acc,
|  | int | sub_mul,
|  | int | sub_acc1 )

## ◆ msc_elem_32_conf() [16/32]

v32accfloat msc_elem_32_conf | ( | v32float16 | a,
|  | v32float16 | b,
|  | v32accfloat | acc,
|  | int | zero_acc,
|  | int | sub_mul,
|  | int | sub_acc1 )

## ◆ msc_elem_32_conf() [17/32]

v32acc64 msc_elem_32_conf | ( | v32int16 | a,
|  | int | sgn_x,
|  | signed short | b,
|  | int | sgn_y,
|  | v32acc64 | acc,
|  | int | zero_acc,
|  | int | shift16,
|  | int | sub_mul,
|  | int | sub_acc1 )

## ◆ msc_elem_32_conf() [18/32]

v32acc64 msc_elem_32_conf | ( | v32int16 | a,
|  | int | sgn_x,
|  | unsigned short | b,
|  | int | sgn_y,
|  | v32acc64 | acc,
|  | int | zero_acc,
|  | int | shift16,
|  | int | sub_mul,
|  | int | sub_acc1 )

## ◆ msc_elem_32_conf() [19/32]

v32acc64 msc_elem_32_conf | ( | v32int16 | a,
|  | int | sgn_x,
|  | v32int16 | b,
|  | int | sgn_y,
|  | v32acc64 | acc,
|  | int | zero_acc,
|  | int | shift16,
|  | int | sub_mul,
|  | int | sub_acc1 )

## ◆ msc_elem_32_conf() [20/32]

v32acc64 msc_elem_32_conf | ( | v32int16 | a,
|  | int | sgn_x,
|  | v32uint16 | b,
|  | int | sgn_y,
|  | v32acc64 | acc,
|  | int | zero_acc,
|  | int | shift16,
|  | int | sub_mul,
|  | int | sub_acc1 )

## ◆ msc_elem_32_conf() [21/32]

v32acc64 msc_elem_32_conf | ( | v32int16 | a,
|  | signed short | b,
|  | v32acc64 | acc,
|  | int | zero_acc,
|  | int | shift16,
|  | int | sub_mul,
|  | int | sub_acc1 )

## ◆ msc_elem_32_conf() [22/32]

v32acc64 msc_elem_32_conf | ( | v32int16 | a,
|  | unsigned short | b,
|  | v32acc64 | acc,
|  | int | zero_acc,
|  | int | shift16,
|  | int | sub_mul,
|  | int | sub_acc1 )

## ◆ msc_elem_32_conf() [23/32]

v32acc64 msc_elem_32_conf | ( | v32int16 | a,
|  | v32int16 | b,
|  | v32acc64 | acc,
|  | int | zero_acc,
|  | int | shift16,
|  | int | sub_mul,
|  | int | sub_acc1 )

## ◆ msc_elem_32_conf() [24/32]

v32acc64 msc_elem_32_conf | ( | v32int16 | a,
|  | v32uint16 | b,
|  | v32acc64 | acc,
|  | int | zero_acc,
|  | int | shift16,
|  | int | sub_mul,
|  | int | sub_acc1 )

## ◆ msc_elem_32_conf() [25/32]

v32acc64 msc_elem_32_conf | ( | v32uint16 | a,
|  | int | sgn_x,
|  | signed short | b,
|  | int | sgn_y,
|  | v32acc64 | acc,
|  | int | zero_acc,
|  | int | shift16,
|  | int | sub_mul,
|  | int | sub_acc1 )

## ◆ msc_elem_32_conf() [26/32]

v32acc64 msc_elem_32_conf | ( | v32uint16 | a,
|  | int | sgn_x,
|  | unsigned short | b,
|  | int | sgn_y,
|  | v32acc64 | acc,
|  | int | zero_acc,
|  | int | shift16,
|  | int | sub_mul,
|  | int | sub_acc1 )

## ◆ msc_elem_32_conf() [27/32]

v32acc64 msc_elem_32_conf | ( | v32uint16 | a,
|  | int | sgn_x,
|  | v32int16 | b,
|  | int | sgn_y,
|  | v32acc64 | acc,
|  | int | zero_acc,
|  | int | shift16,
|  | int | sub_mul,
|  | int | sub_acc1 )

## ◆ msc_elem_32_conf() [28/32]

v32acc64 msc_elem_32_conf | ( | v32uint16 | a,
|  | int | sgn_x,
|  | v32uint16 | b,
|  | int | sgn_y,
|  | v32acc64 | acc,
|  | int | zero_acc,
|  | int | shift16,
|  | int | sub_mul,
|  | int | sub_acc1 )

## ◆ msc_elem_32_conf() [29/32]

v32acc64 msc_elem_32_conf | ( | v32uint16 | a,
|  | signed short | b,
|  | v32acc64 | acc,
|  | int | zero_acc,
|  | int | shift16,
|  | int | sub_mul,
|  | int | sub_acc1 )

## ◆ msc_elem_32_conf() [30/32]

v32acc64 msc_elem_32_conf | ( | v32uint16 | a,
|  | unsigned short | b,
|  | v32acc64 | acc,
|  | int | zero_acc,
|  | int | shift16,
|  | int | sub_mul,
|  | int | sub_acc1 )

## ◆ msc_elem_32_conf() [31/32]

v32acc64 msc_elem_32_conf | ( | v32uint16 | a,
|  | v32int16 | b,
|  | v32acc64 | acc,
|  | int | zero_acc,
|  | int | shift16,
|  | int | sub_mul,
|  | int | sub_acc1 )

## ◆ msc_elem_32_conf() [32/32]

v32acc64 msc_elem_32_conf | ( | v32uint16 | a,
|  | v32uint16 | b,
|  | v32acc64 | acc,
|  | int | zero_acc,
|  | int | shift16,
|  | int | sub_mul,
|  | int | sub_acc1 )

## ◆ msc_elem_64() [1/8]

v64acc32 msc_elem_64 | ( | v64int16 | a,
|  | int | sgn_x,
|  | v64int16 | b,
|  | int | sgn_y,
|  | v64acc32 | acc )

## ◆ msc_elem_64() [2/8]

v64acc32 msc_elem_64 | ( | v64int16 | a,
|  | int | sgn_x,
|  | v64uint16 | b,
|  | int | sgn_y,
|  | v64acc32 | acc )

## ◆ msc_elem_64() [3/8]

v64acc32 msc_elem_64 | ( | v64int16 | a,
|  | v64int16 | b,
|  | v64acc32 | acc )

## ◆ msc_elem_64() [4/8]

v64acc32 msc_elem_64 | ( | v64int16 | a,
|  | v64uint16 | b,
|  | v64acc32 | acc )

## ◆ msc_elem_64() [5/8]

v64acc32 msc_elem_64 | ( | v64uint16 | a,
|  | int | sgn_x,
|  | v64int16 | b,
|  | int | sgn_y,
|  | v64acc32 | acc )

## ◆ msc_elem_64() [6/8]

v64acc32 msc_elem_64 | ( | v64uint16 | a,
|  | int | sgn_x,
|  | v64uint16 | b,
|  | int | sgn_y,
|  | v64acc32 | acc )

## ◆ msc_elem_64() [7/8]

v64acc32 msc_elem_64 | ( | v64uint16 | a,
|  | v64int16 | b,
|  | v64acc32 | acc )

## ◆ msc_elem_64() [8/8]

v64acc32 msc_elem_64 | ( | v64uint16 | a,
|  | v64uint16 | b,
|  | v64acc32 | acc )

## ◆ msc_elem_64_conf() [1/8]

v64acc32 msc_elem_64_conf | ( | v64int16 | a,
|  | int | sgn_x,
|  | v64int16 | b,
|  | int | sgn_y,
|  | v64acc32 | acc,
|  | int | zero_acc,
|  | int | shift16,
|  | int | sub_mul,
|  | int | sub_acc1 )

## ◆ msc_elem_64_conf() [2/8]

v64acc32 msc_elem_64_conf | ( | v64int16 | a,
|  | int | sgn_x,
|  | v64uint16 | b,
|  | int | sgn_y,
|  | v64acc32 | acc,
|  | int | zero_acc,
|  | int | shift16,
|  | int | sub_mul,
|  | int | sub_acc1 )

## ◆ msc_elem_64_conf() [3/8]

v64acc32 msc_elem_64_conf | ( | v64int16 | a,
|  | v64int16 | b,
|  | v64acc32 | acc,
|  | int | zero_acc,
|  | int | shift16,
|  | int | sub_mul,
|  | int | sub_acc1 )

## ◆ msc_elem_64_conf() [4/8]

v64acc32 msc_elem_64_conf | ( | v64int16 | a,
|  | v64uint16 | b,
|  | v64acc32 | acc,
|  | int | zero_acc,
|  | int | shift16,
|  | int | sub_mul,
|  | int | sub_acc1 )

## ◆ msc_elem_64_conf() [5/8]

v64acc32 msc_elem_64_conf | ( | v64uint16 | a,
|  | int | sgn_x,
|  | v64int16 | b,
|  | int | sgn_y,
|  | v64acc32 | acc,
|  | int | zero_acc,
|  | int | shift16,
|  | int | sub_mul,
|  | int | sub_acc1 )

## ◆ msc_elem_64_conf() [6/8]

v64acc32 msc_elem_64_conf | ( | v64uint16 | a,
|  | int | sgn_x,
|  | v64uint16 | b,
|  | int | sgn_y,
|  | v64acc32 | acc,
|  | int | zero_acc,
|  | int | shift16,
|  | int | sub_mul,
|  | int | sub_acc1 )

## ◆ msc_elem_64_conf() [7/8]

v64acc32 msc_elem_64_conf | ( | v64uint16 | a,
|  | v64int16 | b,
|  | v64acc32 | acc,
|  | int | zero_acc,
|  | int | shift16,
|  | int | sub_mul,
|  | int | sub_acc1 )

## ◆ msc_elem_64_conf() [8/8]

v64acc32 msc_elem_64_conf | ( | v64uint16 | a,
|  | v64uint16 | b,
|  | v64acc32 | acc,
|  | int | zero_acc,
|  | int | shift16,
|  | int | sub_mul,
|  | int | sub_acc1 )

## ◆ mul_4x4_4x8() [1/8]

v32acc64 mul_4x4_4x8 | ( | v32int16 | a,
|  | int | sgn_x,
|  | v32int16 | b,
|  | int | sgn_y )

## ◆ mul_4x4_4x8() [2/8]

v32acc64 mul_4x4_4x8 | ( | v32int16 | a,
|  | int | sgn_x,
|  | v32uint16 | b,
|  | int | sgn_y )

## ◆ mul_4x4_4x8() [3/8]

v32acc64 mul_4x4_4x8 | ( | v32int16 | a,
|  | v32int16 | b )

## ◆ mul_4x4_4x8() [4/8]

v32acc64 mul_4x4_4x8 | ( | v32int16 | a,
|  | v32uint16 | b )

## ◆ mul_4x4_4x8() [5/8]

v32acc64 mul_4x4_4x8 | ( | v32uint16 | a,
|  | int | sgn_x,
|  | v32int16 | b,
|  | int | sgn_y )

## ◆ mul_4x4_4x8() [6/8]

v32acc64 mul_4x4_4x8 | ( | v32uint16 | a,
|  | int | sgn_x,
|  | v32uint16 | b,
|  | int | sgn_y )

## ◆ mul_4x4_4x8() [7/8]

v32acc64 mul_4x4_4x8 | ( | v32uint16 | a,
|  | v32int16 | b )

## ◆ mul_4x4_4x8() [8/8]

v32acc64 mul_4x4_4x8 | ( | v32uint16 | a,
|  | v32uint16 | b )

## ◆ mul_4x4_4x8_conf() [1/8]

v32acc64 mul_4x4_4x8_conf | ( | v32int16 | a,
|  | int | sgn_x,
|  | v32int16 | b,
|  | int | sgn_y,
|  | int | sub_mul )

## ◆ mul_4x4_4x8_conf() [2/8]

v32acc64 mul_4x4_4x8_conf | ( | v32int16 | a,
|  | int | sgn_x,
|  | v32uint16 | b,
|  | int | sgn_y,
|  | int | sub_mul )

## ◆ mul_4x4_4x8_conf() [3/8]

v32acc64 mul_4x4_4x8_conf | ( | v32int16 | a,
|  | v32int16 | b,
|  | int | sub_mul )

## ◆ mul_4x4_4x8_conf() [4/8]

v32acc64 mul_4x4_4x8_conf | ( | v32int16 | a,
|  | v32uint16 | b,
|  | int | sub_mul )

## ◆ mul_4x4_4x8_conf() [5/8]

v32acc64 mul_4x4_4x8_conf | ( | v32uint16 | a,
|  | int | sgn_x,
|  | v32int16 | b,
|  | int | sgn_y,
|  | int | sub_mul )

## ◆ mul_4x4_4x8_conf() [6/8]

v32acc64 mul_4x4_4x8_conf | ( | v32uint16 | a,
|  | int | sgn_x,
|  | v32uint16 | b,
|  | int | sgn_y,
|  | int | sub_mul )

## ◆ mul_4x4_4x8_conf() [7/8]

v32acc64 mul_4x4_4x8_conf | ( | v32uint16 | a,
|  | v32int16 | b,
|  | int | sub_mul )

## ◆ mul_4x4_4x8_conf() [8/8]

v32acc64 mul_4x4_4x8_conf | ( | v32uint16 | a,
|  | v32uint16 | b,
|  | int | sub_mul )

## ◆ mul_8x2_2x8() [1/8]

v64acc32 mul_8x2_2x8 | ( | v32int16 | a,
|  | int | sgn_x,
|  | v32int16 | b,
|  | int | sgn_y )

## ◆ mul_8x2_2x8() [2/8]

v64acc32 mul_8x2_2x8 | ( | v32int16 | a,
|  | int | sgn_x,
|  | v32uint16 | b,
|  | int | sgn_y )

## ◆ mul_8x2_2x8() [3/8]

v64acc32 mul_8x2_2x8 | ( | v32int16 | a,
|  | v32int16 | b )

## ◆ mul_8x2_2x8() [4/8]

v64acc32 mul_8x2_2x8 | ( | v32int16 | a,
|  | v32uint16 | b )

## ◆ mul_8x2_2x8() [5/8]

v64acc32 mul_8x2_2x8 | ( | v32uint16 | a,
|  | int | sgn_x,
|  | v32int16 | b,
|  | int | sgn_y )

## ◆ mul_8x2_2x8() [6/8]

v64acc32 mul_8x2_2x8 | ( | v32uint16 | a,
|  | int | sgn_x,
|  | v32uint16 | b,
|  | int | sgn_y )

## ◆ mul_8x2_2x8() [7/8]

v64acc32 mul_8x2_2x8 | ( | v32uint16 | a,
|  | v32int16 | b )

## ◆ mul_8x2_2x8() [8/8]

v64acc32 mul_8x2_2x8 | ( | v32uint16 | a,
|  | v32uint16 | b )

## ◆ mul_8x2_2x8_conf() [1/8]

v64acc32 mul_8x2_2x8_conf | ( | v32int16 | a,
|  | int | sgn_x,
|  | v32int16 | b,
|  | int | sgn_y,
|  | int | sub_mul )

## ◆ mul_8x2_2x8_conf() [2/8]

v64acc32 mul_8x2_2x8_conf | ( | v32int16 | a,
|  | int | sgn_x,
|  | v32uint16 | b,
|  | int | sgn_y,
|  | int | sub_mul )

## ◆ mul_8x2_2x8_conf() [3/8]

v64acc32 mul_8x2_2x8_conf | ( | v32int16 | a,
|  | v32int16 | b,
|  | int | sub_mul )

## ◆ mul_8x2_2x8_conf() [4/8]

v64acc32 mul_8x2_2x8_conf | ( | v32int16 | a,
|  | v32uint16 | b,
|  | int | sub_mul )

## ◆ mul_8x2_2x8_conf() [5/8]

v64acc32 mul_8x2_2x8_conf | ( | v32uint16 | a,
|  | int | sgn_x,
|  | v32int16 | b,
|  | int | sgn_y,
|  | int | sub_mul )

## ◆ mul_8x2_2x8_conf() [6/8]

v64acc32 mul_8x2_2x8_conf | ( | v32uint16 | a,
|  | int | sgn_x,
|  | v32uint16 | b,
|  | int | sgn_y,
|  | int | sub_mul )

## ◆ mul_8x2_2x8_conf() [7/8]

v64acc32 mul_8x2_2x8_conf | ( | v32uint16 | a,
|  | v32int16 | b,
|  | int | sub_mul )

## ◆ mul_8x2_2x8_conf() [8/8]

v64acc32 mul_8x2_2x8_conf | ( | v32uint16 | a,
|  | v32uint16 | b,
|  | int | sub_mul )

## ◆ mul_conv_32x4() [1/8]

v32acc64 mul_conv_32x4 | ( | v64int16 | a,
|  | int | sgn_x,
|  | v32int16 | b,
|  | int | sgn_y )

## ◆ mul_conv_32x4() [2/8]

v32acc64 mul_conv_32x4 | ( | v64int16 | a,
|  | int | sgn_x,
|  | v32uint16 | b,
|  | int | sgn_y )

## ◆ mul_conv_32x4() [3/8]

v32acc64 mul_conv_32x4 | ( | v64int16 | a,
|  | v32int16 | b )

## ◆ mul_conv_32x4() [4/8]

v32acc64 mul_conv_32x4 | ( | v64int16 | a,
|  | v32uint16 | b )

## ◆ mul_conv_32x4() [5/8]

v32acc64 mul_conv_32x4 | ( | v64uint16 | a,
|  | int | sgn_x,
|  | v32int16 | b,
|  | int | sgn_y )

## ◆ mul_conv_32x4() [6/8]

v32acc64 mul_conv_32x4 | ( | v64uint16 | a,
|  | int | sgn_x,
|  | v32uint16 | b,
|  | int | sgn_y )

## ◆ mul_conv_32x4() [7/8]

v32acc64 mul_conv_32x4 | ( | v64uint16 | a,
|  | v32int16 | b )

## ◆ mul_conv_32x4() [8/8]

v32acc64 mul_conv_32x4 | ( | v64uint16 | a,
|  | v32uint16 | b )

## ◆ mul_conv_32x4_conf() [1/8]

v32acc64 mul_conv_32x4_conf | ( | v64int16 | a,
|  | int | sgn_x,
|  | v32int16 | b,
|  | int | sgn_y,
|  | int | sub_mul )

## ◆ mul_conv_32x4_conf() [2/8]

v32acc64 mul_conv_32x4_conf | ( | v64int16 | a,
|  | int | sgn_x,
|  | v32uint16 | b,
|  | int | sgn_y,
|  | int | sub_mul )

## ◆ mul_conv_32x4_conf() [3/8]

v32acc64 mul_conv_32x4_conf | ( | v64int16 | a,
|  | v32int16 | b,
|  | int | sub_mul )

## ◆ mul_conv_32x4_conf() [4/8]

v32acc64 mul_conv_32x4_conf | ( | v64int16 | a,
|  | v32uint16 | b,
|  | int | sub_mul )

## ◆ mul_conv_32x4_conf() [5/8]

v32acc64 mul_conv_32x4_conf | ( | v64uint16 | a,
|  | int | sgn_x,
|  | v32int16 | b,
|  | int | sgn_y,
|  | int | sub_mul )

## ◆ mul_conv_32x4_conf() [6/8]

v32acc64 mul_conv_32x4_conf | ( | v64uint16 | a,
|  | int | sgn_x,
|  | v32uint16 | b,
|  | int | sgn_y,
|  | int | sub_mul )

## ◆ mul_conv_32x4_conf() [7/8]

v32acc64 mul_conv_32x4_conf | ( | v64uint16 | a,
|  | v32int16 | b,
|  | int | sub_mul )

## ◆ mul_conv_32x4_conf() [8/8]

v32acc64 mul_conv_32x4_conf | ( | v64uint16 | a,
|  | v32uint16 | b,
|  | int | sub_mul )

## ◆ mul_conv_4x4_8ch() [1/8]

v32acc64 mul_conv_4x4_8ch | ( | v64int16 | a,
|  | int | sgn_x,
|  | v32int16 | b,
|  | int | sgn_y )

## ◆ mul_conv_4x4_8ch() [2/8]

v32acc64 mul_conv_4x4_8ch | ( | v64int16 | a,
|  | int | sgn_x,
|  | v32uint16 | b,
|  | int | sgn_y )

## ◆ mul_conv_4x4_8ch() [3/8]

v32acc64 mul_conv_4x4_8ch | ( | v64int16 | a,
|  | v32int16 | b )

## ◆ mul_conv_4x4_8ch() [4/8]

v32acc64 mul_conv_4x4_8ch | ( | v64int16 | a,
|  | v32uint16 | b )

## ◆ mul_conv_4x4_8ch() [5/8]

v32acc64 mul_conv_4x4_8ch | ( | v64uint16 | a,
|  | int | sgn_x,
|  | v32int16 | b,
|  | int | sgn_y )

## ◆ mul_conv_4x4_8ch() [6/8]

v32acc64 mul_conv_4x4_8ch | ( | v64uint16 | a,
|  | int | sgn_x,
|  | v32uint16 | b,
|  | int | sgn_y )

## ◆ mul_conv_4x4_8ch() [7/8]

v32acc64 mul_conv_4x4_8ch | ( | v64uint16 | a,
|  | v32int16 | b )

## ◆ mul_conv_4x4_8ch() [8/8]

v32acc64 mul_conv_4x4_8ch | ( | v64uint16 | a,
|  | v32uint16 | b )

## ◆ mul_conv_4x4_8ch_conf() [1/8]

v32acc64 mul_conv_4x4_8ch_conf | ( | v64int16 | a,
|  | int | sgn_x,
|  | v32int16 | b,
|  | int | sgn_y,
|  | int | sub_mul )

## ◆ mul_conv_4x4_8ch_conf() [2/8]

v32acc64 mul_conv_4x4_8ch_conf | ( | v64int16 | a,
|  | int | sgn_x,
|  | v32uint16 | b,
|  | int | sgn_y,
|  | int | sub_mul )

## ◆ mul_conv_4x4_8ch_conf() [3/8]

v32acc64 mul_conv_4x4_8ch_conf | ( | v64int16 | a,
|  | v32int16 | b,
|  | int | sub_mul )

## ◆ mul_conv_4x4_8ch_conf() [4/8]

v32acc64 mul_conv_4x4_8ch_conf | ( | v64int16 | a,
|  | v32uint16 | b,
|  | int | sub_mul )

## ◆ mul_conv_4x4_8ch_conf() [5/8]

v32acc64 mul_conv_4x4_8ch_conf | ( | v64uint16 | a,
|  | int | sgn_x,
|  | v32int16 | b,
|  | int | sgn_y,
|  | int | sub_mul )

## ◆ mul_conv_4x4_8ch_conf() [6/8]

v32acc64 mul_conv_4x4_8ch_conf | ( | v64uint16 | a,
|  | int | sgn_x,
|  | v32uint16 | b,
|  | int | sgn_y,
|  | int | sub_mul )

## ◆ mul_conv_4x4_8ch_conf() [7/8]

v32acc64 mul_conv_4x4_8ch_conf | ( | v64uint16 | a,
|  | v32int16 | b,
|  | int | sub_mul )

## ◆ mul_conv_4x4_8ch_conf() [8/8]

v32acc64 mul_conv_4x4_8ch_conf | ( | v64uint16 | a,
|  | v32uint16 | b,
|  | int | sub_mul )

## ◆ mul_elem_32() [1/32]

v32accfloat mul_elem_32 | ( | v32bfloat16 | a,
|  | bfloat16 | b )

## ◆ mul_elem_32() [2/32]

v32accfloat mul_elem_32 | ( | v32bfloat16 | a,
|  | float16 | b )

## ◆ mul_elem_32() [3/32]

v32accfloat mul_elem_32 | ( | v32bfloat16 | a,
|  | int | sgn_x,
|  | bfloat16 | b,
|  | int | sgn_y )

## ◆ mul_elem_32() [4/32]

v32accfloat mul_elem_32 | ( | v32bfloat16 | a,
|  | int | sgn_x,
|  | float16 | b,
|  | int | sgn_y )

## ◆ mul_elem_32() [5/32]

v32accfloat mul_elem_32 | ( | v32bfloat16 | a,
|  | int | sgn_x,
|  | v32bfloat16 | b,
|  | int | sgn_y )

## ◆ mul_elem_32() [6/32]

v32accfloat mul_elem_32 | ( | v32bfloat16 | a,
|  | int | sgn_x,
|  | v32float16 | b,
|  | int | sgn_y )

## ◆ mul_elem_32() [7/32]

v32accfloat mul_elem_32 | ( | v32bfloat16 | a,
|  | v32bfloat16 | b )

## ◆ mul_elem_32() [8/32]

v32accfloat mul_elem_32 | ( | v32bfloat16 | a,
|  | v32float16 | b )

## ◆ mul_elem_32() [9/32]

v32accfloat mul_elem_32 | ( | v32float16 | a,
|  | bfloat16 | b )

## ◆ mul_elem_32() [10/32]

v32accfloat mul_elem_32 | ( | v32float16 | a,
|  | float16 | b )

## ◆ mul_elem_32() [11/32]

v32accfloat mul_elem_32 | ( | v32float16 | a,
|  | int | sgn_x,
|  | bfloat16 | b,
|  | int | sgn_y )

## ◆ mul_elem_32() [12/32]

v32accfloat mul_elem_32 | ( | v32float16 | a,
|  | int | sgn_x,
|  | float16 | b,
|  | int | sgn_y )

## ◆ mul_elem_32() [13/32]

v32accfloat mul_elem_32 | ( | v32float16 | a,
|  | int | sgn_x,
|  | v32bfloat16 | b,
|  | int | sgn_y )

## ◆ mul_elem_32() [14/32]

v32accfloat mul_elem_32 | ( | v32float16 | a,
|  | int | sgn_x,
|  | v32float16 | b,
|  | int | sgn_y )

## ◆ mul_elem_32() [15/32]

v32accfloat mul_elem_32 | ( | v32float16 | a,
|  | v32bfloat16 | b )

## ◆ mul_elem_32() [16/32]

v32accfloat mul_elem_32 | ( | v32float16 | a,
|  | v32float16 | b )

## ◆ mul_elem_32() [17/32]

v32acc64 mul_elem_32 | ( | v32int16 | a,
|  | int | sgn_x,
|  | signed short | b,
|  | int | sgn_y )

## ◆ mul_elem_32() [18/32]

v32acc64 mul_elem_32 | ( | v32int16 | a,
|  | int | sgn_x,
|  | unsigned short | b,
|  | int | sgn_y )

## ◆ mul_elem_32() [19/32]

v32acc64 mul_elem_32 | ( | v32int16 | a,
|  | int | sgn_x,
|  | v32int16 | b,
|  | int | sgn_y )

## ◆ mul_elem_32() [20/32]

v32acc64 mul_elem_32 | ( | v32int16 | a,
|  | int | sgn_x,
|  | v32uint16 | b,
|  | int | sgn_y )

## ◆ mul_elem_32() [21/32]

v32acc64 mul_elem_32 | ( | v32int16 | a,
|  | signed short | b )

## ◆ mul_elem_32() [22/32]

v32acc64 mul_elem_32 | ( | v32int16 | a,
|  | unsigned short | b )

## ◆ mul_elem_32() [23/32]

v32acc64 mul_elem_32 | ( | v32int16 | a,
|  | v32int16 | b )

## ◆ mul_elem_32() [24/32]

v32acc64 mul_elem_32 | ( | v32int16 | a,
|  | v32uint16 | b )

## ◆ mul_elem_32() [25/32]

v32acc64 mul_elem_32 | ( | v32uint16 | a,
|  | int | sgn_x,
|  | signed short | b,
|  | int | sgn_y )

## ◆ mul_elem_32() [26/32]

v32acc64 mul_elem_32 | ( | v32uint16 | a,
|  | int | sgn_x,
|  | unsigned short | b,
|  | int | sgn_y )

## ◆ mul_elem_32() [27/32]

v32acc64 mul_elem_32 | ( | v32uint16 | a,
|  | int | sgn_x,
|  | v32int16 | b,
|  | int | sgn_y )

## ◆ mul_elem_32() [28/32]

v32acc64 mul_elem_32 | ( | v32uint16 | a,
|  | int | sgn_x,
|  | v32uint16 | b,
|  | int | sgn_y )

## ◆ mul_elem_32() [29/32]

v32acc64 mul_elem_32 | ( | v32uint16 | a,
|  | signed short | b )

## ◆ mul_elem_32() [30/32]

v32acc64 mul_elem_32 | ( | v32uint16 | a,
|  | unsigned short | b )

## ◆ mul_elem_32() [31/32]

v32acc64 mul_elem_32 | ( | v32uint16 | a,
|  | v32int16 | b )

## ◆ mul_elem_32() [32/32]

v32acc64 mul_elem_32 | ( | v32uint16 | a,
|  | v32uint16 | b )

## ◆ mul_elem_32_2() [1/8]

v32acc64 mul_elem_32_2 | ( | v64int16 | a,
|  | int | sgn_x,
|  | v64int16 | b,
|  | int | sgn_y )

## ◆ mul_elem_32_2() [2/8]

v32acc64 mul_elem_32_2 | ( | v64int16 | a,
|  | int | sgn_x,
|  | v64uint16 | b,
|  | int | sgn_y )

## ◆ mul_elem_32_2() [3/8]

v32acc64 mul_elem_32_2 | ( | v64int16 | a,
|  | v64int16 | b )

## ◆ mul_elem_32_2() [4/8]

v32acc64 mul_elem_32_2 | ( | v64int16 | a,
|  | v64uint16 | b )

## ◆ mul_elem_32_2() [5/8]

v32acc64 mul_elem_32_2 | ( | v64uint16 | a,
|  | int | sgn_x,
|  | v64int16 | b,
|  | int | sgn_y )

## ◆ mul_elem_32_2() [6/8]

v32acc64 mul_elem_32_2 | ( | v64uint16 | a,
|  | int | sgn_x,
|  | v64uint16 | b,
|  | int | sgn_y )

## ◆ mul_elem_32_2() [7/8]

v32acc64 mul_elem_32_2 | ( | v64uint16 | a,
|  | v64int16 | b )

## ◆ mul_elem_32_2() [8/8]

v32acc64 mul_elem_32_2 | ( | v64uint16 | a,
|  | v64uint16 | b )

## ◆ mul_elem_32_2_conf() [1/8]

v32acc64 mul_elem_32_2_conf | ( | v64int16 | a,
|  | int | sgn_x,
|  | v64int16 | b,
|  | int | sgn_y,
|  | int | sub_mul )

## ◆ mul_elem_32_2_conf() [2/8]

v32acc64 mul_elem_32_2_conf | ( | v64int16 | a,
|  | int | sgn_x,
|  | v64uint16 | b,
|  | int | sgn_y,
|  | int | sub_mul )

## ◆ mul_elem_32_2_conf() [3/8]

v32acc64 mul_elem_32_2_conf | ( | v64int16 | a,
|  | v64int16 | b,
|  | int | sub_mul )

## ◆ mul_elem_32_2_conf() [4/8]

v32acc64 mul_elem_32_2_conf | ( | v64int16 | a,
|  | v64uint16 | b,
|  | int | sub_mul )

## ◆ mul_elem_32_2_conf() [5/8]

v32acc64 mul_elem_32_2_conf | ( | v64uint16 | a,
|  | int | sgn_x,
|  | v64int16 | b,
|  | int | sgn_y,
|  | int | sub_mul )

## ◆ mul_elem_32_2_conf() [6/8]

v32acc64 mul_elem_32_2_conf | ( | v64uint16 | a,
|  | int | sgn_x,
|  | v64uint16 | b,
|  | int | sgn_y,
|  | int | sub_mul )

## ◆ mul_elem_32_2_conf() [7/8]

v32acc64 mul_elem_32_2_conf | ( | v64uint16 | a,
|  | v64int16 | b,
|  | int | sub_mul )

## ◆ mul_elem_32_2_conf() [8/8]

v32acc64 mul_elem_32_2_conf | ( | v64uint16 | a,
|  | v64uint16 | b,
|  | int | sub_mul )

## ◆ mul_elem_32_32b() [1/8]

v32acc32 mul_elem_32_32b | ( | v32int16 | a,
|  | int | sgn_x,
|  | v32int16 | b,
|  | int | sgn_y )

## ◆ mul_elem_32_32b() [2/8]

v32acc32 mul_elem_32_32b | ( | v32int16 | a,
|  | int | sgn_x,
|  | v32uint16 | b,
|  | int | sgn_y )

## ◆ mul_elem_32_32b() [3/8]

v32acc32 mul_elem_32_32b | ( | v32int16 | a,
|  | v32int16 | b )

## ◆ mul_elem_32_32b() [4/8]

v32acc32 mul_elem_32_32b | ( | v32int16 | a,
|  | v32uint16 | b )

## ◆ mul_elem_32_32b() [5/8]

v32acc32 mul_elem_32_32b | ( | v32uint16 | a,
|  | int | sgn_x,
|  | v32int16 | b,
|  | int | sgn_y )

## ◆ mul_elem_32_32b() [6/8]

v32acc32 mul_elem_32_32b | ( | v32uint16 | a,
|  | int | sgn_x,
|  | v32uint16 | b,
|  | int | sgn_y )

## ◆ mul_elem_32_32b() [7/8]

v32acc32 mul_elem_32_32b | ( | v32uint16 | a,
|  | v32int16 | b )

## ◆ mul_elem_32_32b() [8/8]

v32acc32 mul_elem_32_32b | ( | v32uint16 | a,
|  | v32uint16 | b )

## ◆ mul_elem_32_32b_conf() [1/8]

v32acc32 mul_elem_32_32b_conf | ( | v32int16 | a,
|  | int | sgn_x,
|  | v32int16 | b,
|  | int | sgn_y,
|  | int | sub_mul )

## ◆ mul_elem_32_32b_conf() [2/8]

v32acc32 mul_elem_32_32b_conf | ( | v32int16 | a,
|  | int | sgn_x,
|  | v32uint16 | b,
|  | int | sgn_y,
|  | int | sub_mul )

## ◆ mul_elem_32_32b_conf() [3/8]

v32acc32 mul_elem_32_32b_conf | ( | v32int16 | a,
|  | v32int16 | b,
|  | int | sub_mul )

## ◆ mul_elem_32_32b_conf() [4/8]

v32acc32 mul_elem_32_32b_conf | ( | v32int16 | a,
|  | v32uint16 | b,
|  | int | sub_mul )

## ◆ mul_elem_32_32b_conf() [5/8]

v32acc32 mul_elem_32_32b_conf | ( | v32uint16 | a,
|  | int | sgn_x,
|  | v32int16 | b,
|  | int | sgn_y,
|  | int | sub_mul )

## ◆ mul_elem_32_32b_conf() [6/8]

v32acc32 mul_elem_32_32b_conf | ( | v32uint16 | a,
|  | int | sgn_x,
|  | v32uint16 | b,
|  | int | sgn_y,
|  | int | sub_mul )

## ◆ mul_elem_32_32b_conf() [7/8]

v32acc32 mul_elem_32_32b_conf | ( | v32uint16 | a,
|  | v32int16 | b,
|  | int | sub_mul )

## ◆ mul_elem_32_32b_conf() [8/8]

v32acc32 mul_elem_32_32b_conf | ( | v32uint16 | a,
|  | v32uint16 | b,
|  | int | sub_mul )

## ◆ mul_elem_32_conf() [1/32]

v32accfloat mul_elem_32_conf | ( | v32bfloat16 | a,
|  | bfloat16 | b,
|  | int | sub_mul )

## ◆ mul_elem_32_conf() [2/32]

v32accfloat mul_elem_32_conf | ( | v32bfloat16 | a,
|  | float16 | b,
|  | int | sub_mul )

## ◆ mul_elem_32_conf() [3/32]

v32accfloat mul_elem_32_conf | ( | v32bfloat16 | a,
|  | int | sgn_x,
|  | bfloat16 | b,
|  | int | sgn_y,
|  | int | sub_mul )

## ◆ mul_elem_32_conf() [4/32]

v32accfloat mul_elem_32_conf | ( | v32bfloat16 | a,
|  | int | sgn_x,
|  | float16 | b,
|  | int | sgn_y,
|  | int | sub_mul )

## ◆ mul_elem_32_conf() [5/32]

v32accfloat mul_elem_32_conf | ( | v32bfloat16 | a,
|  | int | sgn_x,
|  | v32bfloat16 | b,
|  | int | sgn_y,
|  | int | sub_mul )

## ◆ mul_elem_32_conf() [6/32]

v32accfloat mul_elem_32_conf | ( | v32bfloat16 | a,
|  | int | sgn_x,
|  | v32float16 | b,
|  | int | sgn_y,
|  | int | sub_mul )

## ◆ mul_elem_32_conf() [7/32]

v32accfloat mul_elem_32_conf | ( | v32bfloat16 | a,
|  | v32bfloat16 | b,
|  | int | sub_mul )

## ◆ mul_elem_32_conf() [8/32]

v32accfloat mul_elem_32_conf | ( | v32bfloat16 | a,
|  | v32float16 | b,
|  | int | sub_mul )

## ◆ mul_elem_32_conf() [9/32]

v32accfloat mul_elem_32_conf | ( | v32float16 | a,
|  | bfloat16 | b,
|  | int | sub_mul )

## ◆ mul_elem_32_conf() [10/32]

v32accfloat mul_elem_32_conf | ( | v32float16 | a,
|  | float16 | b,
|  | int | sub_mul )

## ◆ mul_elem_32_conf() [11/32]

v32accfloat mul_elem_32_conf | ( | v32float16 | a,
|  | int | sgn_x,
|  | bfloat16 | b,
|  | int | sgn_y,
|  | int | sub_mul )

## ◆ mul_elem_32_conf() [12/32]

v32accfloat mul_elem_32_conf | ( | v32float16 | a,
|  | int | sgn_x,
|  | float16 | b,
|  | int | sgn_y,
|  | int | sub_mul )

## ◆ mul_elem_32_conf() [13/32]

v32accfloat mul_elem_32_conf | ( | v32float16 | a,
|  | int | sgn_x,
|  | v32bfloat16 | b,
|  | int | sgn_y,
|  | int | sub_mul )

## ◆ mul_elem_32_conf() [14/32]

v32accfloat mul_elem_32_conf | ( | v32float16 | a,
|  | int | sgn_x,
|  | v32float16 | b,
|  | int | sgn_y,
|  | int | sub_mul )

## ◆ mul_elem_32_conf() [15/32]

v32accfloat mul_elem_32_conf | ( | v32float16 | a,
|  | v32bfloat16 | b,
|  | int | sub_mul )

## ◆ mul_elem_32_conf() [16/32]

v32accfloat mul_elem_32_conf | ( | v32float16 | a,
|  | v32float16 | b,
|  | int | sub_mul )

## ◆ mul_elem_32_conf() [17/32]

v32acc64 mul_elem_32_conf | ( | v32int16 | a,
|  | int | sgn_x,
|  | signed short | b,
|  | int | sgn_y,
|  | int | sub_mul )

## ◆ mul_elem_32_conf() [18/32]

v32acc64 mul_elem_32_conf | ( | v32int16 | a,
|  | int | sgn_x,
|  | unsigned short | b,
|  | int | sgn_y,
|  | int | sub_mul )

## ◆ mul_elem_32_conf() [19/32]

v32acc64 mul_elem_32_conf | ( | v32int16 | a,
|  | int | sgn_x,
|  | v32int16 | b,
|  | int | sgn_y,
|  | int | sub_mul )

## ◆ mul_elem_32_conf() [20/32]

v32acc64 mul_elem_32_conf | ( | v32int16 | a,
|  | int | sgn_x,
|  | v32uint16 | b,
|  | int | sgn_y,
|  | int | sub_mul )

## ◆ mul_elem_32_conf() [21/32]

v32acc64 mul_elem_32_conf | ( | v32int16 | a,
|  | signed short | b,
|  | int | sub_mul )

## ◆ mul_elem_32_conf() [22/32]

v32acc64 mul_elem_32_conf | ( | v32int16 | a,
|  | unsigned short | b,
|  | int | sub_mul )

## ◆ mul_elem_32_conf() [23/32]

v32acc64 mul_elem_32_conf | ( | v32int16 | a,
|  | v32int16 | b,
|  | int | sub_mul )

## ◆ mul_elem_32_conf() [24/32]

v32acc64 mul_elem_32_conf | ( | v32int16 | a,
|  | v32uint16 | b,
|  | int | sub_mul )

## ◆ mul_elem_32_conf() [25/32]

v32acc64 mul_elem_32_conf | ( | v32uint16 | a,
|  | int | sgn_x,
|  | signed short | b,
|  | int | sgn_y,
|  | int | sub_mul )

## ◆ mul_elem_32_conf() [26/32]

v32acc64 mul_elem_32_conf | ( | v32uint16 | a,
|  | int | sgn_x,
|  | unsigned short | b,
|  | int | sgn_y,
|  | int | sub_mul )

## ◆ mul_elem_32_conf() [27/32]

v32acc64 mul_elem_32_conf | ( | v32uint16 | a,
|  | int | sgn_x,
|  | v32int16 | b,
|  | int | sgn_y,
|  | int | sub_mul )

## ◆ mul_elem_32_conf() [28/32]

v32acc64 mul_elem_32_conf | ( | v32uint16 | a,
|  | int | sgn_x,
|  | v32uint16 | b,
|  | int | sgn_y,
|  | int | sub_mul )

## ◆ mul_elem_32_conf() [29/32]

v32acc64 mul_elem_32_conf | ( | v32uint16 | a,
|  | signed short | b,
|  | int | sub_mul )

## ◆ mul_elem_32_conf() [30/32]

v32acc64 mul_elem_32_conf | ( | v32uint16 | a,
|  | unsigned short | b,
|  | int | sub_mul )

## ◆ mul_elem_32_conf() [31/32]

v32acc64 mul_elem_32_conf | ( | v32uint16 | a,
|  | v32int16 | b,
|  | int | sub_mul )

## ◆ mul_elem_32_conf() [32/32]

v32acc64 mul_elem_32_conf | ( | v32uint16 | a,
|  | v32uint16 | b,
|  | int | sub_mul )

## ◆ mul_elem_64() [1/8]

v64acc32 mul_elem_64 | ( | v64int16 | a,
|  | int | sgn_x,
|  | v64int16 | b,
|  | int | sgn_y )

## ◆ mul_elem_64() [2/8]

v64acc32 mul_elem_64 | ( | v64int16 | a,
|  | int | sgn_x,
|  | v64uint16 | b,
|  | int | sgn_y )

## ◆ mul_elem_64() [3/8]

v64acc32 mul_elem_64 | ( | v64int16 | a,
|  | v64int16 | b )

## ◆ mul_elem_64() [4/8]

v64acc32 mul_elem_64 | ( | v64int16 | a,
|  | v64uint16 | b )

## ◆ mul_elem_64() [5/8]

v64acc32 mul_elem_64 | ( | v64uint16 | a,
|  | int | sgn_x,
|  | v64int16 | b,
|  | int | sgn_y )

## ◆ mul_elem_64() [6/8]

v64acc32 mul_elem_64 | ( | v64uint16 | a,
|  | int | sgn_x,
|  | v64uint16 | b,
|  | int | sgn_y )

## ◆ mul_elem_64() [7/8]

v64acc32 mul_elem_64 | ( | v64uint16 | a,
|  | v64int16 | b )

## ◆ mul_elem_64() [8/8]

v64acc32 mul_elem_64 | ( | v64uint16 | a,
|  | v64uint16 | b )

## ◆ mul_elem_64_conf() [1/8]

v64acc32 mul_elem_64_conf | ( | v64int16 | a,
|  | int | sgn_x,
|  | v64int16 | b,
|  | int | sgn_y,
|  | int | sub_mul )

## ◆ mul_elem_64_conf() [2/8]

v64acc32 mul_elem_64_conf | ( | v64int16 | a,
|  | int | sgn_x,
|  | v64uint16 | b,
|  | int | sgn_y,
|  | int | sub_mul )

## ◆ mul_elem_64_conf() [3/8]

v64acc32 mul_elem_64_conf | ( | v64int16 | a,
|  | v64int16 | b,
|  | int | sub_mul )

## ◆ mul_elem_64_conf() [4/8]

v64acc32 mul_elem_64_conf | ( | v64int16 | a,
|  | v64uint16 | b,
|  | int | sub_mul )

## ◆ mul_elem_64_conf() [5/8]

v64acc32 mul_elem_64_conf | ( | v64uint16 | a,
|  | int | sgn_x,
|  | v64int16 | b,
|  | int | sgn_y,
|  | int | sub_mul )

## ◆ mul_elem_64_conf() [6/8]

v64acc32 mul_elem_64_conf | ( | v64uint16 | a,
|  | int | sgn_x,
|  | v64uint16 | b,
|  | int | sgn_y,
|  | int | sub_mul )

## ◆ mul_elem_64_conf() [7/8]

v64acc32 mul_elem_64_conf | ( | v64uint16 | a,
|  | v64int16 | b,
|  | int | sub_mul )

## ◆ mul_elem_64_conf() [8/8]

v64acc32 mul_elem_64_conf | ( | v64uint16 | a,
|  | v64uint16 | b,
|  | int | sub_mul )

## ◆ negmul_4x4_4x8() [1/8]

v32acc64 negmul_4x4_4x8 | ( | v32int16 | a,
|  | int | sgn_x,
|  | v32int16 | b,
|  | int | sgn_y )

## ◆ negmul_4x4_4x8() [2/8]

v32acc64 negmul_4x4_4x8 | ( | v32int16 | a,
|  | int | sgn_x,
|  | v32uint16 | b,
|  | int | sgn_y )

## ◆ negmul_4x4_4x8() [3/8]

v32acc64 negmul_4x4_4x8 | ( | v32int16 | a,
|  | v32int16 | b )

## ◆ negmul_4x4_4x8() [4/8]

v32acc64 negmul_4x4_4x8 | ( | v32int16 | a,
|  | v32uint16 | b )

## ◆ negmul_4x4_4x8() [5/8]

v32acc64 negmul_4x4_4x8 | ( | v32uint16 | a,
|  | int | sgn_x,
|  | v32int16 | b,
|  | int | sgn_y )

## ◆ negmul_4x4_4x8() [6/8]

v32acc64 negmul_4x4_4x8 | ( | v32uint16 | a,
|  | int | sgn_x,
|  | v32uint16 | b,
|  | int | sgn_y )

## ◆ negmul_4x4_4x8() [7/8]

v32acc64 negmul_4x4_4x8 | ( | v32uint16 | a,
|  | v32int16 | b )

## ◆ negmul_4x4_4x8() [8/8]

v32acc64 negmul_4x4_4x8 | ( | v32uint16 | a,
|  | v32uint16 | b )

## ◆ negmul_4x4_4x8_conf() [1/8]

v32acc64 negmul_4x4_4x8_conf | ( | v32int16 | a,
|  | int | sgn_x,
|  | v32int16 | b,
|  | int | sgn_y,
|  | int | sub_mul )

## ◆ negmul_4x4_4x8_conf() [2/8]

v32acc64 negmul_4x4_4x8_conf | ( | v32int16 | a,
|  | int | sgn_x,
|  | v32uint16 | b,
|  | int | sgn_y,
|  | int | sub_mul )

## ◆ negmul_4x4_4x8_conf() [3/8]

v32acc64 negmul_4x4_4x8_conf | ( | v32int16 | a,
|  | v32int16 | b,
|  | int | sub_mul )

## ◆ negmul_4x4_4x8_conf() [4/8]

v32acc64 negmul_4x4_4x8_conf | ( | v32int16 | a,
|  | v32uint16 | b,
|  | int | sub_mul )

## ◆ negmul_4x4_4x8_conf() [5/8]

v32acc64 negmul_4x4_4x8_conf | ( | v32uint16 | a,
|  | int | sgn_x,
|  | v32int16 | b,
|  | int | sgn_y,
|  | int | sub_mul )

## ◆ negmul_4x4_4x8_conf() [6/8]

v32acc64 negmul_4x4_4x8_conf | ( | v32uint16 | a,
|  | int | sgn_x,
|  | v32uint16 | b,
|  | int | sgn_y,
|  | int | sub_mul )

## ◆ negmul_4x4_4x8_conf() [7/8]

v32acc64 negmul_4x4_4x8_conf | ( | v32uint16 | a,
|  | v32int16 | b,
|  | int | sub_mul )

## ◆ negmul_4x4_4x8_conf() [8/8]

v32acc64 negmul_4x4_4x8_conf | ( | v32uint16 | a,
|  | v32uint16 | b,
|  | int | sub_mul )

## ◆ negmul_8x2_2x8() [1/8]

v64acc32 negmul_8x2_2x8 | ( | v32int16 | a,
|  | int | sgn_x,
|  | v32int16 | b,
|  | int | sgn_y )

## ◆ negmul_8x2_2x8() [2/8]

v64acc32 negmul_8x2_2x8 | ( | v32int16 | a,
|  | int | sgn_x,
|  | v32uint16 | b,
|  | int | sgn_y )

## ◆ negmul_8x2_2x8() [3/8]

v64acc32 negmul_8x2_2x8 | ( | v32int16 | a,
|  | v32int16 | b )

## ◆ negmul_8x2_2x8() [4/8]

v64acc32 negmul_8x2_2x8 | ( | v32int16 | a,
|  | v32uint16 | b )

## ◆ negmul_8x2_2x8() [5/8]

v64acc32 negmul_8x2_2x8 | ( | v32uint16 | a,
|  | int | sgn_x,
|  | v32int16 | b,
|  | int | sgn_y )

## ◆ negmul_8x2_2x8() [6/8]

v64acc32 negmul_8x2_2x8 | ( | v32uint16 | a,
|  | int | sgn_x,
|  | v32uint16 | b,
|  | int | sgn_y )

## ◆ negmul_8x2_2x8() [7/8]

v64acc32 negmul_8x2_2x8 | ( | v32uint16 | a,
|  | v32int16 | b )

## ◆ negmul_8x2_2x8() [8/8]

v64acc32 negmul_8x2_2x8 | ( | v32uint16 | a,
|  | v32uint16 | b )

## ◆ negmul_8x2_2x8_conf() [1/8]

v64acc32 negmul_8x2_2x8_conf | ( | v32int16 | a,
|  | int | sgn_x,
|  | v32int16 | b,
|  | int | sgn_y,
|  | int | sub_mul )

## ◆ negmul_8x2_2x8_conf() [2/8]

v64acc32 negmul_8x2_2x8_conf | ( | v32int16 | a,
|  | int | sgn_x,
|  | v32uint16 | b,
|  | int | sgn_y,
|  | int | sub_mul )

## ◆ negmul_8x2_2x8_conf() [3/8]

v64acc32 negmul_8x2_2x8_conf | ( | v32int16 | a,
|  | v32int16 | b,
|  | int | sub_mul )

## ◆ negmul_8x2_2x8_conf() [4/8]

v64acc32 negmul_8x2_2x8_conf | ( | v32int16 | a,
|  | v32uint16 | b,
|  | int | sub_mul )

## ◆ negmul_8x2_2x8_conf() [5/8]

v64acc32 negmul_8x2_2x8_conf | ( | v32uint16 | a,
|  | int | sgn_x,
|  | v32int16 | b,
|  | int | sgn_y,
|  | int | sub_mul )

## ◆ negmul_8x2_2x8_conf() [6/8]

v64acc32 negmul_8x2_2x8_conf | ( | v32uint16 | a,
|  | int | sgn_x,
|  | v32uint16 | b,
|  | int | sgn_y,
|  | int | sub_mul )

## ◆ negmul_8x2_2x8_conf() [7/8]

v64acc32 negmul_8x2_2x8_conf | ( | v32uint16 | a,
|  | v32int16 | b,
|  | int | sub_mul )

## ◆ negmul_8x2_2x8_conf() [8/8]

v64acc32 negmul_8x2_2x8_conf | ( | v32uint16 | a,
|  | v32uint16 | b,
|  | int | sub_mul )

## ◆ negmul_conv_32x4() [1/8]

v32acc64 negmul_conv_32x4 | ( | v64int16 | a,
|  | int | sgn_x,
|  | v32int16 | b,
|  | int | sgn_y )

## ◆ negmul_conv_32x4() [2/8]

v32acc64 negmul_conv_32x4 | ( | v64int16 | a,
|  | int | sgn_x,
|  | v32uint16 | b,
|  | int | sgn_y )

## ◆ negmul_conv_32x4() [3/8]

v32acc64 negmul_conv_32x4 | ( | v64int16 | a,
|  | v32int16 | b )

## ◆ negmul_conv_32x4() [4/8]

v32acc64 negmul_conv_32x4 | ( | v64int16 | a,
|  | v32uint16 | b )

## ◆ negmul_conv_32x4() [5/8]

v32acc64 negmul_conv_32x4 | ( | v64uint16 | a,
|  | int | sgn_x,
|  | v32int16 | b,
|  | int | sgn_y )

## ◆ negmul_conv_32x4() [6/8]

v32acc64 negmul_conv_32x4 | ( | v64uint16 | a,
|  | int | sgn_x,
|  | v32uint16 | b,
|  | int | sgn_y )

## ◆ negmul_conv_32x4() [7/8]

v32acc64 negmul_conv_32x4 | ( | v64uint16 | a,
|  | v32int16 | b )

## ◆ negmul_conv_32x4() [8/8]

v32acc64 negmul_conv_32x4 | ( | v64uint16 | a,
|  | v32uint16 | b )

## ◆ negmul_conv_32x4_conf() [1/8]

v32acc64 negmul_conv_32x4_conf | ( | v64int16 | a,
|  | int | sgn_x,
|  | v32int16 | b,
|  | int | sgn_y,
|  | int | sub_mul )

## ◆ negmul_conv_32x4_conf() [2/8]

v32acc64 negmul_conv_32x4_conf | ( | v64int16 | a,
|  | int | sgn_x,
|  | v32uint16 | b,
|  | int | sgn_y,
|  | int | sub_mul )

## ◆ negmul_conv_32x4_conf() [3/8]

v32acc64 negmul_conv_32x4_conf | ( | v64int16 | a,
|  | v32int16 | b,
|  | int | sub_mul )

## ◆ negmul_conv_32x4_conf() [4/8]

v32acc64 negmul_conv_32x4_conf | ( | v64int16 | a,
|  | v32uint16 | b,
|  | int | sub_mul )

## ◆ negmul_conv_32x4_conf() [5/8]

v32acc64 negmul_conv_32x4_conf | ( | v64uint16 | a,
|  | int | sgn_x,
|  | v32int16 | b,
|  | int | sgn_y,
|  | int | sub_mul )

## ◆ negmul_conv_32x4_conf() [6/8]

v32acc64 negmul_conv_32x4_conf | ( | v64uint16 | a,
|  | int | sgn_x,
|  | v32uint16 | b,
|  | int | sgn_y,
|  | int | sub_mul )

## ◆ negmul_conv_32x4_conf() [7/8]

v32acc64 negmul_conv_32x4_conf | ( | v64uint16 | a,
|  | v32int16 | b,
|  | int | sub_mul )

## ◆ negmul_conv_32x4_conf() [8/8]

v32acc64 negmul_conv_32x4_conf | ( | v64uint16 | a,
|  | v32uint16 | b,
|  | int | sub_mul )

## ◆ negmul_conv_4x4_8ch() [1/8]

v32acc64 negmul_conv_4x4_8ch | ( | v64int16 | a,
|  | int | sgn_x,
|  | v32int16 | b,
|  | int | sgn_y )

## ◆ negmul_conv_4x4_8ch() [2/8]

v32acc64 negmul_conv_4x4_8ch | ( | v64int16 | a,
|  | int | sgn_x,
|  | v32uint16 | b,
|  | int | sgn_y )

## ◆ negmul_conv_4x4_8ch() [3/8]

v32acc64 negmul_conv_4x4_8ch | ( | v64int16 | a,
|  | v32int16 | b )

## ◆ negmul_conv_4x4_8ch() [4/8]

v32acc64 negmul_conv_4x4_8ch | ( | v64int16 | a,
|  | v32uint16 | b )

## ◆ negmul_conv_4x4_8ch() [5/8]

v32acc64 negmul_conv_4x4_8ch | ( | v64uint16 | a,
|  | int | sgn_x,
|  | v32int16 | b,
|  | int | sgn_y )

## ◆ negmul_conv_4x4_8ch() [6/8]

v32acc64 negmul_conv_4x4_8ch | ( | v64uint16 | a,
|  | int | sgn_x,
|  | v32uint16 | b,
|  | int | sgn_y )

## ◆ negmul_conv_4x4_8ch() [7/8]

v32acc64 negmul_conv_4x4_8ch | ( | v64uint16 | a,
|  | v32int16 | b )

## ◆ negmul_conv_4x4_8ch() [8/8]

v32acc64 negmul_conv_4x4_8ch | ( | v64uint16 | a,
|  | v32uint16 | b )

## ◆ negmul_conv_4x4_8ch_conf() [1/8]

v32acc64 negmul_conv_4x4_8ch_conf | ( | v64int16 | a,
|  | int | sgn_x,
|  | v32int16 | b,
|  | int | sgn_y,
|  | int | sub_mul )

## ◆ negmul_conv_4x4_8ch_conf() [2/8]

v32acc64 negmul_conv_4x4_8ch_conf | ( | v64int16 | a,
|  | int | sgn_x,
|  | v32uint16 | b,
|  | int | sgn_y,
|  | int | sub_mul )

## ◆ negmul_conv_4x4_8ch_conf() [3/8]

v32acc64 negmul_conv_4x4_8ch_conf | ( | v64int16 | a,
|  | v32int16 | b,
|  | int | sub_mul )

## ◆ negmul_conv_4x4_8ch_conf() [4/8]

v32acc64 negmul_conv_4x4_8ch_conf | ( | v64int16 | a,
|  | v32uint16 | b,
|  | int | sub_mul )

## ◆ negmul_conv_4x4_8ch_conf() [5/8]

v32acc64 negmul_conv_4x4_8ch_conf | ( | v64uint16 | a,
|  | int | sgn_x,
|  | v32int16 | b,
|  | int | sgn_y,
|  | int | sub_mul )

## ◆ negmul_conv_4x4_8ch_conf() [6/8]

v32acc64 negmul_conv_4x4_8ch_conf | ( | v64uint16 | a,
|  | int | sgn_x,
|  | v32uint16 | b,
|  | int | sgn_y,
|  | int | sub_mul )

## ◆ negmul_conv_4x4_8ch_conf() [7/8]

v32acc64 negmul_conv_4x4_8ch_conf | ( | v64uint16 | a,
|  | v32int16 | b,
|  | int | sub_mul )

## ◆ negmul_conv_4x4_8ch_conf() [8/8]

v32acc64 negmul_conv_4x4_8ch_conf | ( | v64uint16 | a,
|  | v32uint16 | b,
|  | int | sub_mul )

## ◆ negmul_elem_32() [1/32]

v32accfloat negmul_elem_32 | ( | v32bfloat16 | a,
|  | bfloat16 | b )

## ◆ negmul_elem_32() [2/32]

v32accfloat negmul_elem_32 | ( | v32bfloat16 | a,
|  | float16 | b )

## ◆ negmul_elem_32() [3/32]

v32accfloat negmul_elem_32 | ( | v32bfloat16 | a,
|  | int | sgn_x,
|  | bfloat16 | b,
|  | int | sgn_y )

## ◆ negmul_elem_32() [4/32]

v32accfloat negmul_elem_32 | ( | v32bfloat16 | a,
|  | int | sgn_x,
|  | float16 | b,
|  | int | sgn_y )

## ◆ negmul_elem_32() [5/32]

v32accfloat negmul_elem_32 | ( | v32bfloat16 | a,
|  | int | sgn_x,
|  | v32bfloat16 | b,
|  | int | sgn_y )

## ◆ negmul_elem_32() [6/32]

v32accfloat negmul_elem_32 | ( | v32bfloat16 | a,
|  | int | sgn_x,
|  | v32float16 | b,
|  | int | sgn_y )

## ◆ negmul_elem_32() [7/32]

v32accfloat negmul_elem_32 | ( | v32bfloat16 | a,
|  | v32bfloat16 | b )

## ◆ negmul_elem_32() [8/32]

v32accfloat negmul_elem_32 | ( | v32bfloat16 | a,
|  | v32float16 | b )

## ◆ negmul_elem_32() [9/32]

v32accfloat negmul_elem_32 | ( | v32float16 | a,
|  | bfloat16 | b )

## ◆ negmul_elem_32() [10/32]

v32accfloat negmul_elem_32 | ( | v32float16 | a,
|  | float16 | b )

## ◆ negmul_elem_32() [11/32]

v32accfloat negmul_elem_32 | ( | v32float16 | a,
|  | int | sgn_x,
|  | bfloat16 | b,
|  | int | sgn_y )

## ◆ negmul_elem_32() [12/32]

v32accfloat negmul_elem_32 | ( | v32float16 | a,
|  | int | sgn_x,
|  | float16 | b,
|  | int | sgn_y )

## ◆ negmul_elem_32() [13/32]

v32accfloat negmul_elem_32 | ( | v32float16 | a,
|  | int | sgn_x,
|  | v32bfloat16 | b,
|  | int | sgn_y )

## ◆ negmul_elem_32() [14/32]

v32accfloat negmul_elem_32 | ( | v32float16 | a,
|  | int | sgn_x,
|  | v32float16 | b,
|  | int | sgn_y )

## ◆ negmul_elem_32() [15/32]

v32accfloat negmul_elem_32 | ( | v32float16 | a,
|  | v32bfloat16 | b )

## ◆ negmul_elem_32() [16/32]

v32accfloat negmul_elem_32 | ( | v32float16 | a,
|  | v32float16 | b )

## ◆ negmul_elem_32() [17/32]

v32acc64 negmul_elem_32 | ( | v32int16 | a,
|  | int | sgn_x,
|  | signed short | b,
|  | int | sgn_y )

## ◆ negmul_elem_32() [18/32]

v32acc64 negmul_elem_32 | ( | v32int16 | a,
|  | int | sgn_x,
|  | unsigned short | b,
|  | int | sgn_y )

## ◆ negmul_elem_32() [19/32]

v32acc64 negmul_elem_32 | ( | v32int16 | a,
|  | int | sgn_x,
|  | v32int16 | b,
|  | int | sgn_y )

## ◆ negmul_elem_32() [20/32]

v32acc64 negmul_elem_32 | ( | v32int16 | a,
|  | int | sgn_x,
|  | v32uint16 | b,
|  | int | sgn_y )

## ◆ negmul_elem_32() [21/32]

v32acc64 negmul_elem_32 | ( | v32int16 | a,
|  | signed short | b )

## ◆ negmul_elem_32() [22/32]

v32acc64 negmul_elem_32 | ( | v32int16 | a,
|  | unsigned short | b )

## ◆ negmul_elem_32() [23/32]

v32acc64 negmul_elem_32 | ( | v32int16 | a,
|  | v32int16 | b )

## ◆ negmul_elem_32() [24/32]

v32acc64 negmul_elem_32 | ( | v32int16 | a,
|  | v32uint16 | b )

## ◆ negmul_elem_32() [25/32]

v32acc64 negmul_elem_32 | ( | v32uint16 | a,
|  | int | sgn_x,
|  | signed short | b,
|  | int | sgn_y )

## ◆ negmul_elem_32() [26/32]

v32acc64 negmul_elem_32 | ( | v32uint16 | a,
|  | int | sgn_x,
|  | unsigned short | b,
|  | int | sgn_y )

## ◆ negmul_elem_32() [27/32]

v32acc64 negmul_elem_32 | ( | v32uint16 | a,
|  | int | sgn_x,
|  | v32int16 | b,
|  | int | sgn_y )

## ◆ negmul_elem_32() [28/32]

v32acc64 negmul_elem_32 | ( | v32uint16 | a,
|  | int | sgn_x,
|  | v32uint16 | b,
|  | int | sgn_y )

## ◆ negmul_elem_32() [29/32]

v32acc64 negmul_elem_32 | ( | v32uint16 | a,
|  | signed short | b )

## ◆ negmul_elem_32() [30/32]

v32acc64 negmul_elem_32 | ( | v32uint16 | a,
|  | unsigned short | b )

## ◆ negmul_elem_32() [31/32]

v32acc64 negmul_elem_32 | ( | v32uint16 | a,
|  | v32int16 | b )

## ◆ negmul_elem_32() [32/32]

v32acc64 negmul_elem_32 | ( | v32uint16 | a,
|  | v32uint16 | b )

## ◆ negmul_elem_32_2() [1/8]

v32acc64 negmul_elem_32_2 | ( | v64int16 | a,
|  | int | sgn_x,
|  | v64int16 | b,
|  | int | sgn_y )

## ◆ negmul_elem_32_2() [2/8]

v32acc64 negmul_elem_32_2 | ( | v64int16 | a,
|  | int | sgn_x,
|  | v64uint16 | b,
|  | int | sgn_y )

## ◆ negmul_elem_32_2() [3/8]

v32acc64 negmul_elem_32_2 | ( | v64int16 | a,
|  | v64int16 | b )

## ◆ negmul_elem_32_2() [4/8]

v32acc64 negmul_elem_32_2 | ( | v64int16 | a,
|  | v64uint16 | b )

## ◆ negmul_elem_32_2() [5/8]

v32acc64 negmul_elem_32_2 | ( | v64uint16 | a,
|  | int | sgn_x,
|  | v64int16 | b,
|  | int | sgn_y )

## ◆ negmul_elem_32_2() [6/8]

v32acc64 negmul_elem_32_2 | ( | v64uint16 | a,
|  | int | sgn_x,
|  | v64uint16 | b,
|  | int | sgn_y )

## ◆ negmul_elem_32_2() [7/8]

v32acc64 negmul_elem_32_2 | ( | v64uint16 | a,
|  | v64int16 | b )

## ◆ negmul_elem_32_2() [8/8]

v32acc64 negmul_elem_32_2 | ( | v64uint16 | a,
|  | v64uint16 | b )

## ◆ negmul_elem_32_2_conf() [1/8]

v32acc64 negmul_elem_32_2_conf | ( | v64int16 | a,
|  | int | sgn_x,
|  | v64int16 | b,
|  | int | sgn_y,
|  | int | sub_mul )

## ◆ negmul_elem_32_2_conf() [2/8]

v32acc64 negmul_elem_32_2_conf | ( | v64int16 | a,
|  | int | sgn_x,
|  | v64uint16 | b,
|  | int | sgn_y,
|  | int | sub_mul )

## ◆ negmul_elem_32_2_conf() [3/8]

v32acc64 negmul_elem_32_2_conf | ( | v64int16 | a,
|  | v64int16 | b,
|  | int | sub_mul )

## ◆ negmul_elem_32_2_conf() [4/8]

v32acc64 negmul_elem_32_2_conf | ( | v64int16 | a,
|  | v64uint16 | b,
|  | int | sub_mul )

## ◆ negmul_elem_32_2_conf() [5/8]

v32acc64 negmul_elem_32_2_conf | ( | v64uint16 | a,
|  | int | sgn_x,
|  | v64int16 | b,
|  | int | sgn_y,
|  | int | sub_mul )

## ◆ negmul_elem_32_2_conf() [6/8]

v32acc64 negmul_elem_32_2_conf | ( | v64uint16 | a,
|  | int | sgn_x,
|  | v64uint16 | b,
|  | int | sgn_y,
|  | int | sub_mul )

## ◆ negmul_elem_32_2_conf() [7/8]

v32acc64 negmul_elem_32_2_conf | ( | v64uint16 | a,
|  | v64int16 | b,
|  | int | sub_mul )

## ◆ negmul_elem_32_2_conf() [8/8]

v32acc64 negmul_elem_32_2_conf | ( | v64uint16 | a,
|  | v64uint16 | b,
|  | int | sub_mul )

## ◆ negmul_elem_32_32b() [1/8]

v32acc32 negmul_elem_32_32b | ( | v32int16 | a,
|  | int | sgn_x,
|  | v32int16 | b,
|  | int | sgn_y )

## ◆ negmul_elem_32_32b() [2/8]

v32acc32 negmul_elem_32_32b | ( | v32int16 | a,
|  | int | sgn_x,
|  | v32uint16 | b,
|  | int | sgn_y )

## ◆ negmul_elem_32_32b() [3/8]

v32acc32 negmul_elem_32_32b | ( | v32int16 | a,
|  | v32int16 | b )

## ◆ negmul_elem_32_32b() [4/8]

v32acc32 negmul_elem_32_32b | ( | v32int16 | a,
|  | v32uint16 | b )

## ◆ negmul_elem_32_32b() [5/8]

v32acc32 negmul_elem_32_32b | ( | v32uint16 | a,
|  | int | sgn_x,
|  | v32int16 | b,
|  | int | sgn_y )

## ◆ negmul_elem_32_32b() [6/8]

v32acc32 negmul_elem_32_32b | ( | v32uint16 | a,
|  | int | sgn_x,
|  | v32uint16 | b,
|  | int | sgn_y )

## ◆ negmul_elem_32_32b() [7/8]

v32acc32 negmul_elem_32_32b | ( | v32uint16 | a,
|  | v32int16 | b )

## ◆ negmul_elem_32_32b() [8/8]

v32acc32 negmul_elem_32_32b | ( | v32uint16 | a,
|  | v32uint16 | b )

## ◆ negmul_elem_32_32b_conf() [1/8]

v32acc32 negmul_elem_32_32b_conf | ( | v32int16 | a,
|  | int | sgn_x,
|  | v32int16 | b,
|  | int | sgn_y,
|  | int | sub_mul )

## ◆ negmul_elem_32_32b_conf() [2/8]

v32acc32 negmul_elem_32_32b_conf | ( | v32int16 | a,
|  | int | sgn_x,
|  | v32uint16 | b,
|  | int | sgn_y,
|  | int | sub_mul )

## ◆ negmul_elem_32_32b_conf() [3/8]

v32acc32 negmul_elem_32_32b_conf | ( | v32int16 | a,
|  | v32int16 | b,
|  | int | sub_mul )

## ◆ negmul_elem_32_32b_conf() [4/8]

v32acc32 negmul_elem_32_32b_conf | ( | v32int16 | a,
|  | v32uint16 | b,
|  | int | sub_mul )

## ◆ negmul_elem_32_32b_conf() [5/8]

v32acc32 negmul_elem_32_32b_conf | ( | v32uint16 | a,
|  | int | sgn_x,
|  | v32int16 | b,
|  | int | sgn_y,
|  | int | sub_mul )

## ◆ negmul_elem_32_32b_conf() [6/8]

v32acc32 negmul_elem_32_32b_conf | ( | v32uint16 | a,
|  | int | sgn_x,
|  | v32uint16 | b,
|  | int | sgn_y,
|  | int | sub_mul )

## ◆ negmul_elem_32_32b_conf() [7/8]

v32acc32 negmul_elem_32_32b_conf | ( | v32uint16 | a,
|  | v32int16 | b,
|  | int | sub_mul )

## ◆ negmul_elem_32_32b_conf() [8/8]

v32acc32 negmul_elem_32_32b_conf | ( | v32uint16 | a,
|  | v32uint16 | b,
|  | int | sub_mul )

## ◆ negmul_elem_32_conf() [1/32]

v32accfloat negmul_elem_32_conf | ( | v32bfloat16 | a,
|  | bfloat16 | b,
|  | int | sub_mul )

## ◆ negmul_elem_32_conf() [2/32]

v32accfloat negmul_elem_32_conf | ( | v32bfloat16 | a,
|  | float16 | b,
|  | int | sub_mul )

## ◆ negmul_elem_32_conf() [3/32]

v32accfloat negmul_elem_32_conf | ( | v32bfloat16 | a,
|  | int | sgn_x,
|  | bfloat16 | b,
|  | int | sgn_y,
|  | int | sub_mul )

## ◆ negmul_elem_32_conf() [4/32]

v32accfloat negmul_elem_32_conf | ( | v32bfloat16 | a,
|  | int | sgn_x,
|  | float16 | b,
|  | int | sgn_y,
|  | int | sub_mul )

## ◆ negmul_elem_32_conf() [5/32]

v32accfloat negmul_elem_32_conf | ( | v32bfloat16 | a,
|  | int | sgn_x,
|  | v32bfloat16 | b,
|  | int | sgn_y,
|  | int | sub_mul )

## ◆ negmul_elem_32_conf() [6/32]

v32accfloat negmul_elem_32_conf | ( | v32bfloat16 | a,
|  | int | sgn_x,
|  | v32float16 | b,
|  | int | sgn_y,
|  | int | sub_mul )

## ◆ negmul_elem_32_conf() [7/32]

v32accfloat negmul_elem_32_conf | ( | v32bfloat16 | a,
|  | v32bfloat16 | b,
|  | int | sub_mul )

## ◆ negmul_elem_32_conf() [8/32]

v32accfloat negmul_elem_32_conf | ( | v32bfloat16 | a,
|  | v32float16 | b,
|  | int | sub_mul )

## ◆ negmul_elem_32_conf() [9/32]

v32accfloat negmul_elem_32_conf | ( | v32float16 | a,
|  | bfloat16 | b,
|  | int | sub_mul )

## ◆ negmul_elem_32_conf() [10/32]

v32accfloat negmul_elem_32_conf | ( | v32float16 | a,
|  | float16 | b,
|  | int | sub_mul )

## ◆ negmul_elem_32_conf() [11/32]

v32accfloat negmul_elem_32_conf | ( | v32float16 | a,
|  | int | sgn_x,
|  | bfloat16 | b,
|  | int | sgn_y,
|  | int | sub_mul )

## ◆ negmul_elem_32_conf() [12/32]

v32accfloat negmul_elem_32_conf | ( | v32float16 | a,
|  | int | sgn_x,
|  | float16 | b,
|  | int | sgn_y,
|  | int | sub_mul )

## ◆ negmul_elem_32_conf() [13/32]

v32accfloat negmul_elem_32_conf | ( | v32float16 | a,
|  | int | sgn_x,
|  | v32bfloat16 | b,
|  | int | sgn_y,
|  | int | sub_mul )

## ◆ negmul_elem_32_conf() [14/32]

v32accfloat negmul_elem_32_conf | ( | v32float16 | a,
|  | int | sgn_x,
|  | v32float16 | b,
|  | int | sgn_y,
|  | int | sub_mul )

## ◆ negmul_elem_32_conf() [15/32]

v32accfloat negmul_elem_32_conf | ( | v32float16 | a,
|  | v32bfloat16 | b,
|  | int | sub_mul )

## ◆ negmul_elem_32_conf() [16/32]

v32accfloat negmul_elem_32_conf | ( | v32float16 | a,
|  | v32float16 | b,
|  | int | sub_mul )

## ◆ negmul_elem_32_conf() [17/32]

v32acc64 negmul_elem_32_conf | ( | v32int16 | a,
|  | int | sgn_x,
|  | signed short | b,
|  | int | sgn_y,
|  | int | sub_mul )

## ◆ negmul_elem_32_conf() [18/32]

v32acc64 negmul_elem_32_conf | ( | v32int16 | a,
|  | int | sgn_x,
|  | unsigned short | b,
|  | int | sgn_y,
|  | int | sub_mul )

## ◆ negmul_elem_32_conf() [19/32]

v32acc64 negmul_elem_32_conf | ( | v32int16 | a,
|  | int | sgn_x,
|  | v32int16 | b,
|  | int | sgn_y,
|  | int | sub_mul )

## ◆ negmul_elem_32_conf() [20/32]

v32acc64 negmul_elem_32_conf | ( | v32int16 | a,
|  | int | sgn_x,
|  | v32uint16 | b,
|  | int | sgn_y,
|  | int | sub_mul )

## ◆ negmul_elem_32_conf() [21/32]

v32acc64 negmul_elem_32_conf | ( | v32int16 | a,
|  | signed short | b,
|  | int | sub_mul )

## ◆ negmul_elem_32_conf() [22/32]

v32acc64 negmul_elem_32_conf | ( | v32int16 | a,
|  | unsigned short | b,
|  | int | sub_mul )

## ◆ negmul_elem_32_conf() [23/32]

v32acc64 negmul_elem_32_conf | ( | v32int16 | a,
|  | v32int16 | b,
|  | int | sub_mul )

## ◆ negmul_elem_32_conf() [24/32]

v32acc64 negmul_elem_32_conf | ( | v32int16 | a,
|  | v32uint16 | b,
|  | int | sub_mul )

## ◆ negmul_elem_32_conf() [25/32]

v32acc64 negmul_elem_32_conf | ( | v32uint16 | a,
|  | int | sgn_x,
|  | signed short | b,
|  | int | sgn_y,
|  | int | sub_mul )

## ◆ negmul_elem_32_conf() [26/32]

v32acc64 negmul_elem_32_conf | ( | v32uint16 | a,
|  | int | sgn_x,
|  | unsigned short | b,
|  | int | sgn_y,
|  | int | sub_mul )

## ◆ negmul_elem_32_conf() [27/32]

v32acc64 negmul_elem_32_conf | ( | v32uint16 | a,
|  | int | sgn_x,
|  | v32int16 | b,
|  | int | sgn_y,
|  | int | sub_mul )

## ◆ negmul_elem_32_conf() [28/32]

v32acc64 negmul_elem_32_conf | ( | v32uint16 | a,
|  | int | sgn_x,
|  | v32uint16 | b,
|  | int | sgn_y,
|  | int | sub_mul )

## ◆ negmul_elem_32_conf() [29/32]

v32acc64 negmul_elem_32_conf | ( | v32uint16 | a,
|  | signed short | b,
|  | int | sub_mul )

## ◆ negmul_elem_32_conf() [30/32]

v32acc64 negmul_elem_32_conf | ( | v32uint16 | a,
|  | unsigned short | b,
|  | int | sub_mul )

## ◆ negmul_elem_32_conf() [31/32]

v32acc64 negmul_elem_32_conf | ( | v32uint16 | a,
|  | v32int16 | b,
|  | int | sub_mul )

## ◆ negmul_elem_32_conf() [32/32]

v32acc64 negmul_elem_32_conf | ( | v32uint16 | a,
|  | v32uint16 | b,
|  | int | sub_mul )

## ◆ negmul_elem_64() [1/8]

v64acc32 negmul_elem_64 | ( | v64int16 | a,
|  | int | sgn_x,
|  | v64int16 | b,
|  | int | sgn_y )

## ◆ negmul_elem_64() [2/8]

v64acc32 negmul_elem_64 | ( | v64int16 | a,
|  | int | sgn_x,
|  | v64uint16 | b,
|  | int | sgn_y )

## ◆ negmul_elem_64() [3/8]

v64acc32 negmul_elem_64 | ( | v64int16 | a,
|  | v64int16 | b )

## ◆ negmul_elem_64() [4/8]

v64acc32 negmul_elem_64 | ( | v64int16 | a,
|  | v64uint16 | b )

## ◆ negmul_elem_64() [5/8]

v64acc32 negmul_elem_64 | ( | v64uint16 | a,
|  | int | sgn_x,
|  | v64int16 | b,
|  | int | sgn_y )

## ◆ negmul_elem_64() [6/8]

v64acc32 negmul_elem_64 | ( | v64uint16 | a,
|  | int | sgn_x,
|  | v64uint16 | b,
|  | int | sgn_y )

## ◆ negmul_elem_64() [7/8]

v64acc32 negmul_elem_64 | ( | v64uint16 | a,
|  | v64int16 | b )

## ◆ negmul_elem_64() [8/8]

v64acc32 negmul_elem_64 | ( | v64uint16 | a,
|  | v64uint16 | b )

## ◆ negmul_elem_64_conf() [1/8]

v64acc32 negmul_elem_64_conf | ( | v64int16 | a,
|  | int | sgn_x,
|  | v64int16 | b,
|  | int | sgn_y,
|  | int | sub_mul )

## ◆ negmul_elem_64_conf() [2/8]

v64acc32 negmul_elem_64_conf | ( | v64int16 | a,
|  | int | sgn_x,
|  | v64uint16 | b,
|  | int | sgn_y,
|  | int | sub_mul )

## ◆ negmul_elem_64_conf() [3/8]

v64acc32 negmul_elem_64_conf | ( | v64int16 | a,
|  | v64int16 | b,
|  | int | sub_mul )

## ◆ negmul_elem_64_conf() [4/8]

v64acc32 negmul_elem_64_conf | ( | v64int16 | a,
|  | v64uint16 | b,
|  | int | sub_mul )

## ◆ negmul_elem_64_conf() [5/8]

v64acc32 negmul_elem_64_conf | ( | v64uint16 | a,
|  | int | sgn_x,
|  | v64int16 | b,
|  | int | sgn_y,
|  | int | sub_mul )

## ◆ negmul_elem_64_conf() [6/8]

v64acc32 negmul_elem_64_conf | ( | v64uint16 | a,
|  | int | sgn_x,
|  | v64uint16 | b,
|  | int | sgn_y,
|  | int | sub_mul )

## ◆ negmul_elem_64_conf() [7/8]

v64acc32 negmul_elem_64_conf | ( | v64uint16 | a,
|  | v64int16 | b,
|  | int | sub_mul )

## ◆ negmul_elem_64_conf() [8/8]

v64acc32 negmul_elem_64_conf | ( | v64uint16 | a,
|  | v64uint16 | b,
|  | int | sub_mul )