| AI Engine-ML v2 Intrinsics User Guide (v2026.1)

Loading...
Searching...
No Matches
Topics
Streams
Load/Store Operations

## Topics
| Cascade read
| Cascade write
| Stream read
| Stream write

## Detailed Description

These intrinsics enable the AIE-ML v2 core to access the input/output streams. Some of these intrinsics are "blocking" and will stall the core when trying to read from an empty stream, or write to a full one. Non blocking intrinsics have "_nb" in their name.

Concerning performance :

- 32-bit streams can be read/written every clock cycle.

See also
  Control registers
  Status registers