| AI Engine-ML v2 Intrinsics User Guide (v2026.1)

Loading...
Searching...
No Matches
Vector x scalar multiply-accumulate of 16b x 16b datatypes
Vector Operations » Multiply Accumulate

## elem_64
v64acc32 | mul_elem_64 (v64uint16 a, unsigned short b)
v64acc32 | negmul_elem_64 (v64uint16 a, unsigned short b)
v64acc32 | mac_elem_64 (v64uint16 a, unsigned short b, v64acc32 acc)
v64acc32 | msc_elem_64 (v64uint16 a, unsigned short b, v64acc32 acc)
v64acc32 | addmac_elem_64 (v64uint16 a, unsigned short b, v64acc32 acc1, v64acc32 acc2)
v64acc32 | addmsc_elem_64 (v64uint16 a, unsigned short b, v64acc32 acc1, v64acc32 acc2)
v64acc32 | mul_elem_64 (v64uint16 a, signed short b)
v64acc32 | negmul_elem_64 (v64uint16 a, signed short b)
v64acc32 | mac_elem_64 (v64uint16 a, signed short b, v64acc32 acc)
v64acc32 | msc_elem_64 (v64uint16 a, signed short b, v64acc32 acc)
v64acc32 | addmac_elem_64 (v64uint16 a, signed short b, v64acc32 acc1, v64acc32 acc2)
v64acc32 | addmsc_elem_64 (v64uint16 a, signed short b, v64acc32 acc1, v64acc32 acc2)
v64acc32 | mul_elem_64 (v64int16 a, unsigned short b)
v64acc32 | negmul_elem_64 (v64int16 a, unsigned short b)
v64acc32 | mac_elem_64 (v64int16 a, unsigned short b, v64acc32 acc)
v64acc32 | msc_elem_64 (v64int16 a, unsigned short b, v64acc32 acc)
v64acc32 | addmac_elem_64 (v64int16 a, unsigned short b, v64acc32 acc1, v64acc32 acc2)
v64acc32 | addmsc_elem_64 (v64int16 a, unsigned short b, v64acc32 acc1, v64acc32 acc2)
v64acc32 | mul_elem_64 (v64int16 a, signed short b)
v64acc32 | negmul_elem_64 (v64int16 a, signed short b)
v64acc32 | mac_elem_64 (v64int16 a, signed short b, v64acc32 acc)
v64acc32 | msc_elem_64 (v64int16 a, signed short b, v64acc32 acc)
v64acc32 | addmac_elem_64 (v64int16 a, signed short b, v64acc32 acc1, v64acc32 acc2)
v64acc32 | addmsc_elem_64 (v64int16 a, signed short b, v64acc32 acc1, v64acc32 acc2)

## elem_64 with dynamic sign
v64acc32 | mul_elem_64 (v64uint16 a, int sgn_x, unsigned short b, int sgn_y)
v64acc32 | negmul_elem_64 (v64uint16 a, int sgn_x, unsigned short b, int sgn_y)
v64acc32 | mac_elem_64 (v64uint16 a, int sgn_x, unsigned short b, int sgn_y, v64acc32 acc)
v64acc32 | msc_elem_64 (v64uint16 a, int sgn_x, unsigned short b, int sgn_y, v64acc32 acc)
v64acc32 | addmac_elem_64 (v64uint16 a, int sgn_x, unsigned short b, int sgn_y, v64acc32 acc1, v64acc32 acc2)
v64acc32 | addmsc_elem_64 (v64uint16 a, int sgn_x, unsigned short b, int sgn_y, v64acc32 acc1, v64acc32 acc2)
v64acc32 | mul_elem_64 (v64uint16 a, int sgn_x, signed short b, int sgn_y)
v64acc32 | negmul_elem_64 (v64uint16 a, int sgn_x, signed short b, int sgn_y)
v64acc32 | mac_elem_64 (v64uint16 a, int sgn_x, signed short b, int sgn_y, v64acc32 acc)
v64acc32 | msc_elem_64 (v64uint16 a, int sgn_x, signed short b, int sgn_y, v64acc32 acc)
v64acc32 | addmac_elem_64 (v64uint16 a, int sgn_x, signed short b, int sgn_y, v64acc32 acc1, v64acc32 acc2)
v64acc32 | addmsc_elem_64 (v64uint16 a, int sgn_x, signed short b, int sgn_y, v64acc32 acc1, v64acc32 acc2)
v64acc32 | mul_elem_64 (v64int16 a, int sgn_x, unsigned short b, int sgn_y)
v64acc32 | negmul_elem_64 (v64int16 a, int sgn_x, unsigned short b, int sgn_y)
v64acc32 | mac_elem_64 (v64int16 a, int sgn_x, unsigned short b, int sgn_y, v64acc32 acc)
v64acc32 | msc_elem_64 (v64int16 a, int sgn_x, unsigned short b, int sgn_y, v64acc32 acc)
v64acc32 | addmac_elem_64 (v64int16 a, int sgn_x, unsigned short b, int sgn_y, v64acc32 acc1, v64acc32 acc2)
v64acc32 | addmsc_elem_64 (v64int16 a, int sgn_x, unsigned short b, int sgn_y, v64acc32 acc1, v64acc32 acc2)
v64acc32 | mul_elem_64 (v64int16 a, int sgn_x, signed short b, int sgn_y)
v64acc32 | negmul_elem_64 (v64int16 a, int sgn_x, signed short b, int sgn_y)
v64acc32 | mac_elem_64 (v64int16 a, int sgn_x, signed short b, int sgn_y, v64acc32 acc)
v64acc32 | msc_elem_64 (v64int16 a, int sgn_x, signed short b, int sgn_y, v64acc32 acc)
v64acc32 | addmac_elem_64 (v64int16 a, int sgn_x, signed short b, int sgn_y, v64acc32 acc1, v64acc32 acc2)
v64acc32 | addmsc_elem_64 (v64int16 a, int sgn_x, signed short b, int sgn_y, v64acc32 acc1, v64acc32 acc2)

## elem_64 with dynamic negation of multiplication result
v64acc32 | mul_elem_64_conf (v64uint16 a, unsigned short b, int sub_mul)
v64acc32 | negmul_elem_64_conf (v64uint16 a, unsigned short b, int sub_mul)
v64acc32 | mul_elem_64_conf (v64uint16 a, signed short b, int sub_mul)
v64acc32 | negmul_elem_64_conf (v64uint16 a, signed short b, int sub_mul)
v64acc32 | mul_elem_64_conf (v64int16 a, unsigned short b, int sub_mul)
v64acc32 | negmul_elem_64_conf (v64int16 a, unsigned short b, int sub_mul)
v64acc32 | mul_elem_64_conf (v64int16 a, signed short b, int sub_mul)
v64acc32 | negmul_elem_64_conf (v64int16 a, signed short b, int sub_mul)

## elem_64 with dynamic negation of multiplication result, zeroing of acc1, negation of acc1
v64acc32 | mac_elem_64_conf (v64uint16 a, unsigned short b, v64acc32 acc, int zero_acc, int shift16, int sub_mul, int sub_acc1)
v64acc32 | msc_elem_64_conf (v64uint16 a, unsigned short b, v64acc32 acc, int zero_acc, int shift16, int sub_mul, int sub_acc1)
v64acc32 | addmac_elem_64_conf (v64uint16 a, unsigned short b, v64acc32 acc1, v64acc32 acc2, int zero_acc1, int shift16, int sub_mul, int sub_acc1, int sub_acc2)
v64acc32 | addmsc_elem_64_conf (v64uint16 a, unsigned short b, v64acc32 acc1, v64acc32 acc2, int zero_acc1, int shift16, int sub_mul, int sub_acc1, int sub_acc2)
v64acc32 | mac_elem_64_conf (v64uint16 a, signed short b, v64acc32 acc, int zero_acc, int shift16, int sub_mul, int sub_acc1)
v64acc32 | msc_elem_64_conf (v64uint16 a, signed short b, v64acc32 acc, int zero_acc, int shift16, int sub_mul, int sub_acc1)
v64acc32 | addmac_elem_64_conf (v64uint16 a, signed short b, v64acc32 acc1, v64acc32 acc2, int zero_acc1, int shift16, int sub_mul, int sub_acc1, int sub_acc2)
v64acc32 | addmsc_elem_64_conf (v64uint16 a, signed short b, v64acc32 acc1, v64acc32 acc2, int zero_acc1, int shift16, int sub_mul, int sub_acc1, int sub_acc2)
v64acc32 | mac_elem_64_conf (v64int16 a, unsigned short b, v64acc32 acc, int zero_acc, int shift16, int sub_mul, int sub_acc1)
v64acc32 | msc_elem_64_conf (v64int16 a, unsigned short b, v64acc32 acc, int zero_acc, int shift16, int sub_mul, int sub_acc1)
v64acc32 | addmac_elem_64_conf (v64int16 a, unsigned short b, v64acc32 acc1, v64acc32 acc2, int zero_acc1, int shift16, int sub_mul, int sub_acc1, int sub_acc2)
v64acc32 | addmsc_elem_64_conf (v64int16 a, unsigned short b, v64acc32 acc1, v64acc32 acc2, int zero_acc1, int shift16, int sub_mul, int sub_acc1, int sub_acc2)
v64acc32 | mac_elem_64_conf (v64int16 a, signed short b, v64acc32 acc, int zero_acc, int shift16, int sub_mul, int sub_acc1)
v64acc32 | msc_elem_64_conf (v64int16 a, signed short b, v64acc32 acc, int zero_acc, int shift16, int sub_mul, int sub_acc1)
v64acc32 | addmac_elem_64_conf (v64int16 a, signed short b, v64acc32 acc1, v64acc32 acc2, int zero_acc1, int shift16, int sub_mul, int sub_acc1, int sub_acc2)
v64acc32 | addmsc_elem_64_conf (v64int16 a, signed short b, v64acc32 acc1, v64acc32 acc2, int zero_acc1, int shift16, int sub_mul, int sub_acc1, int sub_acc2)

## elem_64 with dynamic sign and dynamic negation of multiplication result
v64acc32 | mul_elem_64_conf (v64uint16 a, int sgn_x, unsigned short b, int sgn_y, int sub_mul)
v64acc32 | negmul_elem_64_conf (v64uint16 a, int sgn_x, unsigned short b, int sgn_y, int sub_mul)
v64acc32 | mac_elem_64_conf (v64uint16 a, int sgn_x, unsigned short b, int sgn_y, v64acc32 acc, int zero_acc, int shift16, int sub_mul, int sub_acc1)
v64acc32 | msc_elem_64_conf (v64uint16 a, int sgn_x, unsigned short b, int sgn_y, v64acc32 acc, int zero_acc, int shift16, int sub_mul, int sub_acc1)
v64acc32 | addmac_elem_64_conf (v64uint16 a, int sgn_x, unsigned short b, int sgn_y, v64acc32 acc1, v64acc32 acc2, int zero_acc1, int shift16, int sub_mul, int sub_acc1, int sub_acc2)
v64acc32 | addmsc_elem_64_conf (v64uint16 a, int sgn_x, unsigned short b, int sgn_y, v64acc32 acc1, v64acc32 acc2, int zero_acc1, int shift16, int sub_mul, int sub_acc1, int sub_acc2)
v64acc32 | mul_elem_64_conf (v64uint16 a, int sgn_x, signed short b, int sgn_y, int sub_mul)
v64acc32 | negmul_elem_64_conf (v64uint16 a, int sgn_x, signed short b, int sgn_y, int sub_mul)
v64acc32 | mac_elem_64_conf (v64uint16 a, int sgn_x, signed short b, int sgn_y, v64acc32 acc, int zero_acc, int shift16, int sub_mul, int sub_acc1)
v64acc32 | msc_elem_64_conf (v64uint16 a, int sgn_x, signed short b, int sgn_y, v64acc32 acc, int zero_acc, int shift16, int sub_mul, int sub_acc1)
v64acc32 | addmac_elem_64_conf (v64uint16 a, int sgn_x, signed short b, int sgn_y, v64acc32 acc1, v64acc32 acc2, int zero_acc1, int shift16, int sub_mul, int sub_acc1, int sub_acc2)
v64acc32 | addmsc_elem_64_conf (v64uint16 a, int sgn_x, signed short b, int sgn_y, v64acc32 acc1, v64acc32 acc2, int zero_acc1, int shift16, int sub_mul, int sub_acc1, int sub_acc2)
v64acc32 | mul_elem_64_conf (v64int16 a, int sgn_x, unsigned short b, int sgn_y, int sub_mul)
v64acc32 | negmul_elem_64_conf (v64int16 a, int sgn_x, unsigned short b, int sgn_y, int sub_mul)
v64acc32 | mac_elem_64_conf (v64int16 a, int sgn_x, unsigned short b, int sgn_y, v64acc32 acc, int zero_acc, int shift16, int sub_mul, int sub_acc1)
v64acc32 | msc_elem_64_conf (v64int16 a, int sgn_x, unsigned short b, int sgn_y, v64acc32 acc, int zero_acc, int shift16, int sub_mul, int sub_acc1)
v64acc32 | addmac_elem_64_conf (v64int16 a, int sgn_x, unsigned short b, int sgn_y, v64acc32 acc1, v64acc32 acc2, int zero_acc1, int shift16, int sub_mul, int sub_acc1, int sub_acc2)
v64acc32 | addmsc_elem_64_conf (v64int16 a, int sgn_x, unsigned short b, int sgn_y, v64acc32 acc1, v64acc32 acc2, int zero_acc1, int shift16, int sub_mul, int sub_acc1, int sub_acc2)
v64acc32 | mul_elem_64_conf (v64int16 a, int sgn_x, signed short b, int sgn_y, int sub_mul)
v64acc32 | negmul_elem_64_conf (v64int16 a, int sgn_x, signed short b, int sgn_y, int sub_mul)
v64acc32 | mac_elem_64_conf (v64int16 a, int sgn_x, signed short b, int sgn_y, v64acc32 acc, int zero_acc, int shift16, int sub_mul, int sub_acc1)
v64acc32 | msc_elem_64_conf (v64int16 a, int sgn_x, signed short b, int sgn_y, v64acc32 acc, int zero_acc, int shift16, int sub_mul, int sub_acc1)
v64acc32 | addmac_elem_64_conf (v64int16 a, int sgn_x, signed short b, int sgn_y, v64acc32 acc1, v64acc32 acc2, int zero_acc1, int shift16, int sub_mul, int sub_acc1, int sub_acc2)
v64acc32 | addmsc_elem_64_conf (v64int16 a, int sgn_x, signed short b, int sgn_y, v64acc32 acc1, v64acc32 acc2, int zero_acc1, int shift16, int sub_mul, int sub_acc1, int sub_acc2)

## elem_32
v32acc64 | mul_elem_32 (v32uint16 a, unsigned short b)
v32acc64 | negmul_elem_32 (v32uint16 a, unsigned short b)
v32acc64 | mac_elem_32 (v32uint16 a, unsigned short b, v32acc64 acc)
v32acc64 | msc_elem_32 (v32uint16 a, unsigned short b, v32acc64 acc)
v32acc64 | addmac_elem_32 (v32uint16 a, unsigned short b, v32acc64 acc1, v32acc64 acc2)
v32acc64 | addmsc_elem_32 (v32uint16 a, unsigned short b, v32acc64 acc1, v32acc64 acc2)
v32acc64 | mul_elem_32 (v32uint16 a, signed short b)
v32acc64 | negmul_elem_32 (v32uint16 a, signed short b)
v32acc64 | mac_elem_32 (v32uint16 a, signed short b, v32acc64 acc)
v32acc64 | msc_elem_32 (v32uint16 a, signed short b, v32acc64 acc)
v32acc64 | addmac_elem_32 (v32uint16 a, signed short b, v32acc64 acc1, v32acc64 acc2)
v32acc64 | addmsc_elem_32 (v32uint16 a, signed short b, v32acc64 acc1, v32acc64 acc2)
v32acc64 | mul_elem_32 (v32int16 a, unsigned short b)
v32acc64 | negmul_elem_32 (v32int16 a, unsigned short b)
v32acc64 | mac_elem_32 (v32int16 a, unsigned short b, v32acc64 acc)
v32acc64 | msc_elem_32 (v32int16 a, unsigned short b, v32acc64 acc)
v32acc64 | addmac_elem_32 (v32int16 a, unsigned short b, v32acc64 acc1, v32acc64 acc2)
v32acc64 | addmsc_elem_32 (v32int16 a, unsigned short b, v32acc64 acc1, v32acc64 acc2)
v32acc64 | mul_elem_32 (v32int16 a, signed short b)
v32acc64 | negmul_elem_32 (v32int16 a, signed short b)
v32acc64 | mac_elem_32 (v32int16 a, signed short b, v32acc64 acc)
v32acc64 | msc_elem_32 (v32int16 a, signed short b, v32acc64 acc)
v32acc64 | addmac_elem_32 (v32int16 a, signed short b, v32acc64 acc1, v32acc64 acc2)
v32acc64 | addmsc_elem_32 (v32int16 a, signed short b, v32acc64 acc1, v32acc64 acc2)

## elem_32 with dynamic sign
v32acc64 | mul_elem_32 (v32uint16 a, int sgn_x, unsigned short b, int sgn_y)
v32acc64 | negmul_elem_32 (v32uint16 a, int sgn_x, unsigned short b, int sgn_y)
v32acc64 | mac_elem_32 (v32uint16 a, int sgn_x, unsigned short b, int sgn_y, v32acc64 acc)
v32acc64 | msc_elem_32 (v32uint16 a, int sgn_x, unsigned short b, int sgn_y, v32acc64 acc)
v32acc64 | addmac_elem_32 (v32uint16 a, int sgn_x, unsigned short b, int sgn_y, v32acc64 acc1, v32acc64 acc2)
v32acc64 | addmsc_elem_32 (v32uint16 a, int sgn_x, unsigned short b, int sgn_y, v32acc64 acc1, v32acc64 acc2)
v32acc64 | mul_elem_32 (v32uint16 a, int sgn_x, signed short b, int sgn_y)
v32acc64 | negmul_elem_32 (v32uint16 a, int sgn_x, signed short b, int sgn_y)
v32acc64 | mac_elem_32 (v32uint16 a, int sgn_x, signed short b, int sgn_y, v32acc64 acc)
v32acc64 | msc_elem_32 (v32uint16 a, int sgn_x, signed short b, int sgn_y, v32acc64 acc)
v32acc64 | addmac_elem_32 (v32uint16 a, int sgn_x, signed short b, int sgn_y, v32acc64 acc1, v32acc64 acc2)
v32acc64 | addmsc_elem_32 (v32uint16 a, int sgn_x, signed short b, int sgn_y, v32acc64 acc1, v32acc64 acc2)
v32acc64 | mul_elem_32 (v32int16 a, int sgn_x, unsigned short b, int sgn_y)
v32acc64 | negmul_elem_32 (v32int16 a, int sgn_x, unsigned short b, int sgn_y)
v32acc64 | mac_elem_32 (v32int16 a, int sgn_x, unsigned short b, int sgn_y, v32acc64 acc)
v32acc64 | msc_elem_32 (v32int16 a, int sgn_x, unsigned short b, int sgn_y, v32acc64 acc)
v32acc64 | addmac_elem_32 (v32int16 a, int sgn_x, unsigned short b, int sgn_y, v32acc64 acc1, v32acc64 acc2)
v32acc64 | addmsc_elem_32 (v32int16 a, int sgn_x, unsigned short b, int sgn_y, v32acc64 acc1, v32acc64 acc2)
v32acc64 | mul_elem_32 (v32int16 a, int sgn_x, signed short b, int sgn_y)
v32acc64 | negmul_elem_32 (v32int16 a, int sgn_x, signed short b, int sgn_y)
v32acc64 | mac_elem_32 (v32int16 a, int sgn_x, signed short b, int sgn_y, v32acc64 acc)
v32acc64 | msc_elem_32 (v32int16 a, int sgn_x, signed short b, int sgn_y, v32acc64 acc)
v32acc64 | addmac_elem_32 (v32int16 a, int sgn_x, signed short b, int sgn_y, v32acc64 acc1, v32acc64 acc2)
v32acc64 | addmsc_elem_32 (v32int16 a, int sgn_x, signed short b, int sgn_y, v32acc64 acc1, v32acc64 acc2)

## elem_32 with dynamic negation of multiplication result
v32acc64 | mul_elem_32_conf (v32uint16 a, unsigned short b, int sub_mul)
v32acc64 | negmul_elem_32_conf (v32uint16 a, unsigned short b, int sub_mul)
v32acc64 | mul_elem_32_conf (v32uint16 a, signed short b, int sub_mul)
v32acc64 | negmul_elem_32_conf (v32uint16 a, signed short b, int sub_mul)
v32acc64 | mul_elem_32_conf (v32int16 a, unsigned short b, int sub_mul)
v32acc64 | negmul_elem_32_conf (v32int16 a, unsigned short b, int sub_mul)
v32acc64 | mul_elem_32_conf (v32int16 a, signed short b, int sub_mul)
v32acc64 | negmul_elem_32_conf (v32int16 a, signed short b, int sub_mul)

## elem_32 with dynamic negation of multiplication result, zeroing of acc1, negation of acc1
v32acc64 | mac_elem_32_conf (v32uint16 a, unsigned short b, v32acc64 acc, int zero_acc, int shift16, int sub_mul, int sub_acc1)
v32acc64 | msc_elem_32_conf (v32uint16 a, unsigned short b, v32acc64 acc, int zero_acc, int shift16, int sub_mul, int sub_acc1)
v32acc64 | addmac_elem_32_conf (v32uint16 a, unsigned short b, v32acc64 acc1, v32acc64 acc2, int zero_acc1, int shift16, int sub_mul, int sub_acc1, int sub_acc2)
v32acc64 | addmsc_elem_32_conf (v32uint16 a, unsigned short b, v32acc64 acc1, v32acc64 acc2, int zero_acc1, int shift16, int sub_mul, int sub_acc1, int sub_acc2)
v32acc64 | mac_elem_32_conf (v32uint16 a, signed short b, v32acc64 acc, int zero_acc, int shift16, int sub_mul, int sub_acc1)
v32acc64 | msc_elem_32_conf (v32uint16 a, signed short b, v32acc64 acc, int zero_acc, int shift16, int sub_mul, int sub_acc1)
v32acc64 | addmac_elem_32_conf (v32uint16 a, signed short b, v32acc64 acc1, v32acc64 acc2, int zero_acc1, int shift16, int sub_mul, int sub_acc1, int sub_acc2)
v32acc64 | addmsc_elem_32_conf (v32uint16 a, signed short b, v32acc64 acc1, v32acc64 acc2, int zero_acc1, int shift16, int sub_mul, int sub_acc1, int sub_acc2)
v32acc64 | mac_elem_32_conf (v32int16 a, unsigned short b, v32acc64 acc, int zero_acc, int shift16, int sub_mul, int sub_acc1)
v32acc64 | msc_elem_32_conf (v32int16 a, unsigned short b, v32acc64 acc, int zero_acc, int shift16, int sub_mul, int sub_acc1)
v32acc64 | addmac_elem_32_conf (v32int16 a, unsigned short b, v32acc64 acc1, v32acc64 acc2, int zero_acc1, int shift16, int sub_mul, int sub_acc1, int sub_acc2)
v32acc64 | addmsc_elem_32_conf (v32int16 a, unsigned short b, v32acc64 acc1, v32acc64 acc2, int zero_acc1, int shift16, int sub_mul, int sub_acc1, int sub_acc2)
v32acc64 | mac_elem_32_conf (v32int16 a, signed short b, v32acc64 acc, int zero_acc, int shift16, int sub_mul, int sub_acc1)
v32acc64 | msc_elem_32_conf (v32int16 a, signed short b, v32acc64 acc, int zero_acc, int shift16, int sub_mul, int sub_acc1)
v32acc64 | addmac_elem_32_conf (v32int16 a, signed short b, v32acc64 acc1, v32acc64 acc2, int zero_acc1, int shift16, int sub_mul, int sub_acc1, int sub_acc2)
v32acc64 | addmsc_elem_32_conf (v32int16 a, signed short b, v32acc64 acc1, v32acc64 acc2, int zero_acc1, int shift16, int sub_mul, int sub_acc1, int sub_acc2)

## elem_32 with dynamic sign and dynamic negation of multiplication result
v32acc64 | mul_elem_32_conf (v32uint16 a, int sgn_x, unsigned short b, int sgn_y, int sub_mul)
v32acc64 | negmul_elem_32_conf (v32uint16 a, int sgn_x, unsigned short b, int sgn_y, int sub_mul)
v32acc64 | mac_elem_32_conf (v32uint16 a, int sgn_x, unsigned short b, int sgn_y, v32acc64 acc, int zero_acc, int shift16, int sub_mul, int sub_acc1)
v32acc64 | msc_elem_32_conf (v32uint16 a, int sgn_x, unsigned short b, int sgn_y, v32acc64 acc, int zero_acc, int shift16, int sub_mul, int sub_acc1)
v32acc64 | addmac_elem_32_conf (v32uint16 a, int sgn_x, unsigned short b, int sgn_y, v32acc64 acc1, v32acc64 acc2, int zero_acc1, int shift16, int sub_mul, int sub_acc1, int sub_acc2)
v32acc64 | addmsc_elem_32_conf (v32uint16 a, int sgn_x, unsigned short b, int sgn_y, v32acc64 acc1, v32acc64 acc2, int zero_acc1, int shift16, int sub_mul, int sub_acc1, int sub_acc2)
v32acc64 | mul_elem_32_conf (v32uint16 a, int sgn_x, signed short b, int sgn_y, int sub_mul)
v32acc64 | negmul_elem_32_conf (v32uint16 a, int sgn_x, signed short b, int sgn_y, int sub_mul)
v32acc64 | mac_elem_32_conf (v32uint16 a, int sgn_x, signed short b, int sgn_y, v32acc64 acc, int zero_acc, int shift16, int sub_mul, int sub_acc1)
v32acc64 | msc_elem_32_conf (v32uint16 a, int sgn_x, signed short b, int sgn_y, v32acc64 acc, int zero_acc, int shift16, int sub_mul, int sub_acc1)
v32acc64 | addmac_elem_32_conf (v32uint16 a, int sgn_x, signed short b, int sgn_y, v32acc64 acc1, v32acc64 acc2, int zero_acc1, int shift16, int sub_mul, int sub_acc1, int sub_acc2)
v32acc64 | addmsc_elem_32_conf (v32uint16 a, int sgn_x, signed short b, int sgn_y, v32acc64 acc1, v32acc64 acc2, int zero_acc1, int shift16, int sub_mul, int sub_acc1, int sub_acc2)
v32acc64 | mul_elem_32_conf (v32int16 a, int sgn_x, unsigned short b, int sgn_y, int sub_mul)
v32acc64 | negmul_elem_32_conf (v32int16 a, int sgn_x, unsigned short b, int sgn_y, int sub_mul)
v32acc64 | mac_elem_32_conf (v32int16 a, int sgn_x, unsigned short b, int sgn_y, v32acc64 acc, int zero_acc, int shift16, int sub_mul, int sub_acc1)
v32acc64 | msc_elem_32_conf (v32int16 a, int sgn_x, unsigned short b, int sgn_y, v32acc64 acc, int zero_acc, int shift16, int sub_mul, int sub_acc1)
v32acc64 | addmac_elem_32_conf (v32int16 a, int sgn_x, unsigned short b, int sgn_y, v32acc64 acc1, v32acc64 acc2, int zero_acc1, int shift16, int sub_mul, int sub_acc1, int sub_acc2)
v32acc64 | addmsc_elem_32_conf (v32int16 a, int sgn_x, unsigned short b, int sgn_y, v32acc64 acc1, v32acc64 acc2, int zero_acc1, int shift16, int sub_mul, int sub_acc1, int sub_acc2)
v32acc64 | mul_elem_32_conf (v32int16 a, int sgn_x, signed short b, int sgn_y, int sub_mul)
v32acc64 | negmul_elem_32_conf (v32int16 a, int sgn_x, signed short b, int sgn_y, int sub_mul)
v32acc64 | mac_elem_32_conf (v32int16 a, int sgn_x, signed short b, int sgn_y, v32acc64 acc, int zero_acc, int shift16, int sub_mul, int sub_acc1)
v32acc64 | msc_elem_32_conf (v32int16 a, int sgn_x, signed short b, int sgn_y, v32acc64 acc, int zero_acc, int shift16, int sub_mul, int sub_acc1)
v32acc64 | addmac_elem_32_conf (v32int16 a, int sgn_x, signed short b, int sgn_y, v32acc64 acc1, v32acc64 acc2, int zero_acc1, int shift16, int sub_mul, int sub_acc1, int sub_acc2)
v32acc64 | addmsc_elem_32_conf (v32int16 a, int sgn_x, signed short b, int sgn_y, v32acc64 acc1, v32acc64 acc2, int zero_acc1, int shift16, int sub_mul, int sub_acc1, int sub_acc2)

## Detailed Description

## Function Documentation

## ◆ addmac_elem_32() [1/8]

v32acc64 addmac_elem_32 | ( | v32int16 | a,
|  | int | sgn_x,
|  | signed short | b,
|  | int | sgn_y,
|  | v32acc64 | acc1,
|  | v32acc64 | acc2 )

## ◆ addmac_elem_32() [2/8]

v32acc64 addmac_elem_32 | ( | v32int16 | a,
|  | int | sgn_x,
|  | unsigned short | b,
|  | int | sgn_y,
|  | v32acc64 | acc1,
|  | v32acc64 | acc2 )

## ◆ addmac_elem_32() [3/8]

v32acc64 addmac_elem_32 | ( | v32int16 | a,
|  | signed short | b,
|  | v32acc64 | acc1,
|  | v32acc64 | acc2 )

## ◆ addmac_elem_32() [4/8]

v32acc64 addmac_elem_32 | ( | v32int16 | a,
|  | unsigned short | b,
|  | v32acc64 | acc1,
|  | v32acc64 | acc2 )

## ◆ addmac_elem_32() [5/8]

v32acc64 addmac_elem_32 | ( | v32uint16 | a,
|  | int | sgn_x,
|  | signed short | b,
|  | int | sgn_y,
|  | v32acc64 | acc1,
|  | v32acc64 | acc2 )

## ◆ addmac_elem_32() [6/8]

v32acc64 addmac_elem_32 | ( | v32uint16 | a,
|  | int | sgn_x,
|  | unsigned short | b,
|  | int | sgn_y,
|  | v32acc64 | acc1,
|  | v32acc64 | acc2 )

## ◆ addmac_elem_32() [7/8]

v32acc64 addmac_elem_32 | ( | v32uint16 | a,
|  | signed short | b,
|  | v32acc64 | acc1,
|  | v32acc64 | acc2 )

## ◆ addmac_elem_32() [8/8]

v32acc64 addmac_elem_32 | ( | v32uint16 | a,
|  | unsigned short | b,
|  | v32acc64 | acc1,
|  | v32acc64 | acc2 )

## ◆ addmac_elem_32_conf() [1/8]

v32acc64 addmac_elem_32_conf | ( | v32int16 | a,
|  | int | sgn_x,
|  | signed short | b,
|  | int | sgn_y,
|  | v32acc64 | acc1,
|  | v32acc64 | acc2,
|  | int | zero_acc1,
|  | int | shift16,
|  | int | sub_mul,
|  | int | sub_acc1,
|  | int | sub_acc2 )

## ◆ addmac_elem_32_conf() [2/8]

v32acc64 addmac_elem_32_conf | ( | v32int16 | a,
|  | int | sgn_x,
|  | unsigned short | b,
|  | int | sgn_y,
|  | v32acc64 | acc1,
|  | v32acc64 | acc2,
|  | int | zero_acc1,
|  | int | shift16,
|  | int | sub_mul,
|  | int | sub_acc1,
|  | int | sub_acc2 )

## ◆ addmac_elem_32_conf() [3/8]

v32acc64 addmac_elem_32_conf | ( | v32int16 | a,
|  | signed short | b,
|  | v32acc64 | acc1,
|  | v32acc64 | acc2,
|  | int | zero_acc1,
|  | int | shift16,
|  | int | sub_mul,
|  | int | sub_acc1,
|  | int | sub_acc2 )

## ◆ addmac_elem_32_conf() [4/8]

v32acc64 addmac_elem_32_conf | ( | v32int16 | a,
|  | unsigned short | b,
|  | v32acc64 | acc1,
|  | v32acc64 | acc2,
|  | int | zero_acc1,
|  | int | shift16,
|  | int | sub_mul,
|  | int | sub_acc1,
|  | int | sub_acc2 )

## ◆ addmac_elem_32_conf() [5/8]

v32acc64 addmac_elem_32_conf | ( | v32uint16 | a,
|  | int | sgn_x,
|  | signed short | b,
|  | int | sgn_y,
|  | v32acc64 | acc1,
|  | v32acc64 | acc2,
|  | int | zero_acc1,
|  | int | shift16,
|  | int | sub_mul,
|  | int | sub_acc1,
|  | int | sub_acc2 )

## ◆ addmac_elem_32_conf() [6/8]

v32acc64 addmac_elem_32_conf | ( | v32uint16 | a,
|  | int | sgn_x,
|  | unsigned short | b,
|  | int | sgn_y,
|  | v32acc64 | acc1,
|  | v32acc64 | acc2,
|  | int | zero_acc1,
|  | int | shift16,
|  | int | sub_mul,
|  | int | sub_acc1,
|  | int | sub_acc2 )

## ◆ addmac_elem_32_conf() [7/8]

v32acc64 addmac_elem_32_conf | ( | v32uint16 | a,
|  | signed short | b,
|  | v32acc64 | acc1,
|  | v32acc64 | acc2,
|  | int | zero_acc1,
|  | int | shift16,
|  | int | sub_mul,
|  | int | sub_acc1,
|  | int | sub_acc2 )

## ◆ addmac_elem_32_conf() [8/8]

v32acc64 addmac_elem_32_conf | ( | v32uint16 | a,
|  | unsigned short | b,
|  | v32acc64 | acc1,
|  | v32acc64 | acc2,
|  | int | zero_acc1,
|  | int | shift16,
|  | int | sub_mul,
|  | int | sub_acc1,
|  | int | sub_acc2 )

## ◆ addmac_elem_64() [1/8]

v64acc32 addmac_elem_64 | ( | v64int16 | a,
|  | int | sgn_x,
|  | signed short | b,
|  | int | sgn_y,
|  | v64acc32 | acc1,
|  | v64acc32 | acc2 )

## ◆ addmac_elem_64() [2/8]

v64acc32 addmac_elem_64 | ( | v64int16 | a,
|  | int | sgn_x,
|  | unsigned short | b,
|  | int | sgn_y,
|  | v64acc32 | acc1,
|  | v64acc32 | acc2 )

## ◆ addmac_elem_64() [3/8]

v64acc32 addmac_elem_64 | ( | v64int16 | a,
|  | signed short | b,
|  | v64acc32 | acc1,
|  | v64acc32 | acc2 )

## ◆ addmac_elem_64() [4/8]

v64acc32 addmac_elem_64 | ( | v64int16 | a,
|  | unsigned short | b,
|  | v64acc32 | acc1,
|  | v64acc32 | acc2 )

## ◆ addmac_elem_64() [5/8]

v64acc32 addmac_elem_64 | ( | v64uint16 | a,
|  | int | sgn_x,
|  | signed short | b,
|  | int | sgn_y,
|  | v64acc32 | acc1,
|  | v64acc32 | acc2 )

## ◆ addmac_elem_64() [6/8]

v64acc32 addmac_elem_64 | ( | v64uint16 | a,
|  | int | sgn_x,
|  | unsigned short | b,
|  | int | sgn_y,
|  | v64acc32 | acc1,
|  | v64acc32 | acc2 )

## ◆ addmac_elem_64() [7/8]

v64acc32 addmac_elem_64 | ( | v64uint16 | a,
|  | signed short | b,
|  | v64acc32 | acc1,
|  | v64acc32 | acc2 )

## ◆ addmac_elem_64() [8/8]

v64acc32 addmac_elem_64 | ( | v64uint16 | a,
|  | unsigned short | b,
|  | v64acc32 | acc1,
|  | v64acc32 | acc2 )

## ◆ addmac_elem_64_conf() [1/8]

v64acc32 addmac_elem_64_conf | ( | v64int16 | a,
|  | int | sgn_x,
|  | signed short | b,
|  | int | sgn_y,
|  | v64acc32 | acc1,
|  | v64acc32 | acc2,
|  | int | zero_acc1,
|  | int | shift16,
|  | int | sub_mul,
|  | int | sub_acc1,
|  | int | sub_acc2 )

## ◆ addmac_elem_64_conf() [2/8]

v64acc32 addmac_elem_64_conf | ( | v64int16 | a,
|  | int | sgn_x,
|  | unsigned short | b,
|  | int | sgn_y,
|  | v64acc32 | acc1,
|  | v64acc32 | acc2,
|  | int | zero_acc1,
|  | int | shift16,
|  | int | sub_mul,
|  | int | sub_acc1,
|  | int | sub_acc2 )

## ◆ addmac_elem_64_conf() [3/8]

v64acc32 addmac_elem_64_conf | ( | v64int16 | a,
|  | signed short | b,
|  | v64acc32 | acc1,
|  | v64acc32 | acc2,
|  | int | zero_acc1,
|  | int | shift16,
|  | int | sub_mul,
|  | int | sub_acc1,
|  | int | sub_acc2 )

## ◆ addmac_elem_64_conf() [4/8]

v64acc32 addmac_elem_64_conf | ( | v64int16 | a,
|  | unsigned short | b,
|  | v64acc32 | acc1,
|  | v64acc32 | acc2,
|  | int | zero_acc1,
|  | int | shift16,
|  | int | sub_mul,
|  | int | sub_acc1,
|  | int | sub_acc2 )

## ◆ addmac_elem_64_conf() [5/8]

v64acc32 addmac_elem_64_conf | ( | v64uint16 | a,
|  | int | sgn_x,
|  | signed short | b,
|  | int | sgn_y,
|  | v64acc32 | acc1,
|  | v64acc32 | acc2,
|  | int | zero_acc1,
|  | int | shift16,
|  | int | sub_mul,
|  | int | sub_acc1,
|  | int | sub_acc2 )

## ◆ addmac_elem_64_conf() [6/8]

v64acc32 addmac_elem_64_conf | ( | v64uint16 | a,
|  | int | sgn_x,
|  | unsigned short | b,
|  | int | sgn_y,
|  | v64acc32 | acc1,
|  | v64acc32 | acc2,
|  | int | zero_acc1,
|  | int | shift16,
|  | int | sub_mul,
|  | int | sub_acc1,
|  | int | sub_acc2 )

## ◆ addmac_elem_64_conf() [7/8]

v64acc32 addmac_elem_64_conf | ( | v64uint16 | a,
|  | signed short | b,
|  | v64acc32 | acc1,
|  | v64acc32 | acc2,
|  | int | zero_acc1,
|  | int | shift16,
|  | int | sub_mul,
|  | int | sub_acc1,
|  | int | sub_acc2 )

## ◆ addmac_elem_64_conf() [8/8]

v64acc32 addmac_elem_64_conf | ( | v64uint16 | a,
|  | unsigned short | b,
|  | v64acc32 | acc1,
|  | v64acc32 | acc2,
|  | int | zero_acc1,
|  | int | shift16,
|  | int | sub_mul,
|  | int | sub_acc1,
|  | int | sub_acc2 )

## ◆ addmsc_elem_32() [1/8]

v32acc64 addmsc_elem_32 | ( | v32int16 | a,
|  | int | sgn_x,
|  | signed short | b,
|  | int | sgn_y,
|  | v32acc64 | acc1,
|  | v32acc64 | acc2 )

## ◆ addmsc_elem_32() [2/8]

v32acc64 addmsc_elem_32 | ( | v32int16 | a,
|  | int | sgn_x,
|  | unsigned short | b,
|  | int | sgn_y,
|  | v32acc64 | acc1,
|  | v32acc64 | acc2 )

## ◆ addmsc_elem_32() [3/8]

v32acc64 addmsc_elem_32 | ( | v32int16 | a,
|  | signed short | b,
|  | v32acc64 | acc1,
|  | v32acc64 | acc2 )

## ◆ addmsc_elem_32() [4/8]

v32acc64 addmsc_elem_32 | ( | v32int16 | a,
|  | unsigned short | b,
|  | v32acc64 | acc1,
|  | v32acc64 | acc2 )

## ◆ addmsc_elem_32() [5/8]

v32acc64 addmsc_elem_32 | ( | v32uint16 | a,
|  | int | sgn_x,
|  | signed short | b,
|  | int | sgn_y,
|  | v32acc64 | acc1,
|  | v32acc64 | acc2 )

## ◆ addmsc_elem_32() [6/8]

v32acc64 addmsc_elem_32 | ( | v32uint16 | a,
|  | int | sgn_x,
|  | unsigned short | b,
|  | int | sgn_y,
|  | v32acc64 | acc1,
|  | v32acc64 | acc2 )

## ◆ addmsc_elem_32() [7/8]

v32acc64 addmsc_elem_32 | ( | v32uint16 | a,
|  | signed short | b,
|  | v32acc64 | acc1,
|  | v32acc64 | acc2 )

## ◆ addmsc_elem_32() [8/8]

v32acc64 addmsc_elem_32 | ( | v32uint16 | a,
|  | unsigned short | b,
|  | v32acc64 | acc1,
|  | v32acc64 | acc2 )

## ◆ addmsc_elem_32_conf() [1/8]

v32acc64 addmsc_elem_32_conf | ( | v32int16 | a,
|  | int | sgn_x,
|  | signed short | b,
|  | int | sgn_y,
|  | v32acc64 | acc1,
|  | v32acc64 | acc2,
|  | int | zero_acc1,
|  | int | shift16,
|  | int | sub_mul,
|  | int | sub_acc1,
|  | int | sub_acc2 )

## ◆ addmsc_elem_32_conf() [2/8]

v32acc64 addmsc_elem_32_conf | ( | v32int16 | a,
|  | int | sgn_x,
|  | unsigned short | b,
|  | int | sgn_y,
|  | v32acc64 | acc1,
|  | v32acc64 | acc2,
|  | int | zero_acc1,
|  | int | shift16,
|  | int | sub_mul,
|  | int | sub_acc1,
|  | int | sub_acc2 )

## ◆ addmsc_elem_32_conf() [3/8]

v32acc64 addmsc_elem_32_conf | ( | v32int16 | a,
|  | signed short | b,
|  | v32acc64 | acc1,
|  | v32acc64 | acc2,
|  | int | zero_acc1,
|  | int | shift16,
|  | int | sub_mul,
|  | int | sub_acc1,
|  | int | sub_acc2 )

## ◆ addmsc_elem_32_conf() [4/8]

v32acc64 addmsc_elem_32_conf | ( | v32int16 | a,
|  | unsigned short | b,
|  | v32acc64 | acc1,
|  | v32acc64 | acc2,
|  | int | zero_acc1,
|  | int | shift16,
|  | int | sub_mul,
|  | int | sub_acc1,
|  | int | sub_acc2 )

## ◆ addmsc_elem_32_conf() [5/8]

v32acc64 addmsc_elem_32_conf | ( | v32uint16 | a,
|  | int | sgn_x,
|  | signed short | b,
|  | int | sgn_y,
|  | v32acc64 | acc1,
|  | v32acc64 | acc2,
|  | int | zero_acc1,
|  | int | shift16,
|  | int | sub_mul,
|  | int | sub_acc1,
|  | int | sub_acc2 )

## ◆ addmsc_elem_32_conf() [6/8]

v32acc64 addmsc_elem_32_conf | ( | v32uint16 | a,
|  | int | sgn_x,
|  | unsigned short | b,
|  | int | sgn_y,
|  | v32acc64 | acc1,
|  | v32acc64 | acc2,
|  | int | zero_acc1,
|  | int | shift16,
|  | int | sub_mul,
|  | int | sub_acc1,
|  | int | sub_acc2 )

## ◆ addmsc_elem_32_conf() [7/8]

v32acc64 addmsc_elem_32_conf | ( | v32uint16 | a,
|  | signed short | b,
|  | v32acc64 | acc1,
|  | v32acc64 | acc2,
|  | int | zero_acc1,
|  | int | shift16,
|  | int | sub_mul,
|  | int | sub_acc1,
|  | int | sub_acc2 )

## ◆ addmsc_elem_32_conf() [8/8]

v32acc64 addmsc_elem_32_conf | ( | v32uint16 | a,
|  | unsigned short | b,
|  | v32acc64 | acc1,
|  | v32acc64 | acc2,
|  | int | zero_acc1,
|  | int | shift16,
|  | int | sub_mul,
|  | int | sub_acc1,
|  | int | sub_acc2 )

## ◆ addmsc_elem_64() [1/8]

v64acc32 addmsc_elem_64 | ( | v64int16 | a,
|  | int | sgn_x,
|  | signed short | b,
|  | int | sgn_y,
|  | v64acc32 | acc1,
|  | v64acc32 | acc2 )

## ◆ addmsc_elem_64() [2/8]

v64acc32 addmsc_elem_64 | ( | v64int16 | a,
|  | int | sgn_x,
|  | unsigned short | b,
|  | int | sgn_y,
|  | v64acc32 | acc1,
|  | v64acc32 | acc2 )

## ◆ addmsc_elem_64() [3/8]

v64acc32 addmsc_elem_64 | ( | v64int16 | a,
|  | signed short | b,
|  | v64acc32 | acc1,
|  | v64acc32 | acc2 )

## ◆ addmsc_elem_64() [4/8]

v64acc32 addmsc_elem_64 | ( | v64int16 | a,
|  | unsigned short | b,
|  | v64acc32 | acc1,
|  | v64acc32 | acc2 )

## ◆ addmsc_elem_64() [5/8]

v64acc32 addmsc_elem_64 | ( | v64uint16 | a,
|  | int | sgn_x,
|  | signed short | b,
|  | int | sgn_y,
|  | v64acc32 | acc1,
|  | v64acc32 | acc2 )

## ◆ addmsc_elem_64() [6/8]

v64acc32 addmsc_elem_64 | ( | v64uint16 | a,
|  | int | sgn_x,
|  | unsigned short | b,
|  | int | sgn_y,
|  | v64acc32 | acc1,
|  | v64acc32 | acc2 )

## ◆ addmsc_elem_64() [7/8]

v64acc32 addmsc_elem_64 | ( | v64uint16 | a,
|  | signed short | b,
|  | v64acc32 | acc1,
|  | v64acc32 | acc2 )

## ◆ addmsc_elem_64() [8/8]

v64acc32 addmsc_elem_64 | ( | v64uint16 | a,
|  | unsigned short | b,
|  | v64acc32 | acc1,
|  | v64acc32 | acc2 )

## ◆ addmsc_elem_64_conf() [1/8]

v64acc32 addmsc_elem_64_conf | ( | v64int16 | a,
|  | int | sgn_x,
|  | signed short | b,
|  | int | sgn_y,
|  | v64acc32 | acc1,
|  | v64acc32 | acc2,
|  | int | zero_acc1,
|  | int | shift16,
|  | int | sub_mul,
|  | int | sub_acc1,
|  | int | sub_acc2 )

## ◆ addmsc_elem_64_conf() [2/8]

v64acc32 addmsc_elem_64_conf | ( | v64int16 | a,
|  | int | sgn_x,
|  | unsigned short | b,
|  | int | sgn_y,
|  | v64acc32 | acc1,
|  | v64acc32 | acc2,
|  | int | zero_acc1,
|  | int | shift16,
|  | int | sub_mul,
|  | int | sub_acc1,
|  | int | sub_acc2 )

## ◆ addmsc_elem_64_conf() [3/8]

v64acc32 addmsc_elem_64_conf | ( | v64int16 | a,
|  | signed short | b,
|  | v64acc32 | acc1,
|  | v64acc32 | acc2,
|  | int | zero_acc1,
|  | int | shift16,
|  | int | sub_mul,
|  | int | sub_acc1,
|  | int | sub_acc2 )

## ◆ addmsc_elem_64_conf() [4/8]

v64acc32 addmsc_elem_64_conf | ( | v64int16 | a,
|  | unsigned short | b,
|  | v64acc32 | acc1,
|  | v64acc32 | acc2,
|  | int | zero_acc1,
|  | int | shift16,
|  | int | sub_mul,
|  | int | sub_acc1,
|  | int | sub_acc2 )

## ◆ addmsc_elem_64_conf() [5/8]

v64acc32 addmsc_elem_64_conf | ( | v64uint16 | a,
|  | int | sgn_x,
|  | signed short | b,
|  | int | sgn_y,
|  | v64acc32 | acc1,
|  | v64acc32 | acc2,
|  | int | zero_acc1,
|  | int | shift16,
|  | int | sub_mul,
|  | int | sub_acc1,
|  | int | sub_acc2 )

## ◆ addmsc_elem_64_conf() [6/8]

v64acc32 addmsc_elem_64_conf | ( | v64uint16 | a,
|  | int | sgn_x,
|  | unsigned short | b,
|  | int | sgn_y,
|  | v64acc32 | acc1,
|  | v64acc32 | acc2,
|  | int | zero_acc1,
|  | int | shift16,
|  | int | sub_mul,
|  | int | sub_acc1,
|  | int | sub_acc2 )

## ◆ addmsc_elem_64_conf() [7/8]

v64acc32 addmsc_elem_64_conf | ( | v64uint16 | a,
|  | signed short | b,
|  | v64acc32 | acc1,
|  | v64acc32 | acc2,
|  | int | zero_acc1,
|  | int | shift16,
|  | int | sub_mul,
|  | int | sub_acc1,
|  | int | sub_acc2 )

## ◆ addmsc_elem_64_conf() [8/8]

v64acc32 addmsc_elem_64_conf | ( | v64uint16 | a,
|  | unsigned short | b,
|  | v64acc32 | acc1,
|  | v64acc32 | acc2,
|  | int | zero_acc1,
|  | int | shift16,
|  | int | sub_mul,
|  | int | sub_acc1,
|  | int | sub_acc2 )

## ◆ mac_elem_32() [1/8]

v32acc64 mac_elem_32 | ( | v32int16 | a,
|  | int | sgn_x,
|  | signed short | b,
|  | int | sgn_y,
|  | v32acc64 | acc )

## ◆ mac_elem_32() [2/8]

v32acc64 mac_elem_32 | ( | v32int16 | a,
|  | int | sgn_x,
|  | unsigned short | b,
|  | int | sgn_y,
|  | v32acc64 | acc )

## ◆ mac_elem_32() [3/8]

v32acc64 mac_elem_32 | ( | v32int16 | a,
|  | signed short | b,
|  | v32acc64 | acc )

## ◆ mac_elem_32() [4/8]

v32acc64 mac_elem_32 | ( | v32int16 | a,
|  | unsigned short | b,
|  | v32acc64 | acc )

## ◆ mac_elem_32() [5/8]

v32acc64 mac_elem_32 | ( | v32uint16 | a,
|  | int | sgn_x,
|  | signed short | b,
|  | int | sgn_y,
|  | v32acc64 | acc )

## ◆ mac_elem_32() [6/8]

v32acc64 mac_elem_32 | ( | v32uint16 | a,
|  | int | sgn_x,
|  | unsigned short | b,
|  | int | sgn_y,
|  | v32acc64 | acc )

## ◆ mac_elem_32() [7/8]

v32acc64 mac_elem_32 | ( | v32uint16 | a,
|  | signed short | b,
|  | v32acc64 | acc )

## ◆ mac_elem_32() [8/8]

v32acc64 mac_elem_32 | ( | v32uint16 | a,
|  | unsigned short | b,
|  | v32acc64 | acc )

## ◆ mac_elem_32_conf() [1/8]

v32acc64 mac_elem_32_conf | ( | v32int16 | a,
|  | int | sgn_x,
|  | signed short | b,
|  | int | sgn_y,
|  | v32acc64 | acc,
|  | int | zero_acc,
|  | int | shift16,
|  | int | sub_mul,
|  | int | sub_acc1 )

## ◆ mac_elem_32_conf() [2/8]

v32acc64 mac_elem_32_conf | ( | v32int16 | a,
|  | int | sgn_x,
|  | unsigned short | b,
|  | int | sgn_y,
|  | v32acc64 | acc,
|  | int | zero_acc,
|  | int | shift16,
|  | int | sub_mul,
|  | int | sub_acc1 )

## ◆ mac_elem_32_conf() [3/8]

v32acc64 mac_elem_32_conf | ( | v32int16 | a,
|  | signed short | b,
|  | v32acc64 | acc,
|  | int | zero_acc,
|  | int | shift16,
|  | int | sub_mul,
|  | int | sub_acc1 )

## ◆ mac_elem_32_conf() [4/8]

v32acc64 mac_elem_32_conf | ( | v32int16 | a,
|  | unsigned short | b,
|  | v32acc64 | acc,
|  | int | zero_acc,
|  | int | shift16,
|  | int | sub_mul,
|  | int | sub_acc1 )

## ◆ mac_elem_32_conf() [5/8]

v32acc64 mac_elem_32_conf | ( | v32uint16 | a,
|  | int | sgn_x,
|  | signed short | b,
|  | int | sgn_y,
|  | v32acc64 | acc,
|  | int | zero_acc,
|  | int | shift16,
|  | int | sub_mul,
|  | int | sub_acc1 )

## ◆ mac_elem_32_conf() [6/8]

v32acc64 mac_elem_32_conf | ( | v32uint16 | a,
|  | int | sgn_x,
|  | unsigned short | b,
|  | int | sgn_y,
|  | v32acc64 | acc,
|  | int | zero_acc,
|  | int | shift16,
|  | int | sub_mul,
|  | int | sub_acc1 )

## ◆ mac_elem_32_conf() [7/8]

v32acc64 mac_elem_32_conf | ( | v32uint16 | a,
|  | signed short | b,
|  | v32acc64 | acc,
|  | int | zero_acc,
|  | int | shift16,
|  | int | sub_mul,
|  | int | sub_acc1 )

## ◆ mac_elem_32_conf() [8/8]

v32acc64 mac_elem_32_conf | ( | v32uint16 | a,
|  | unsigned short | b,
|  | v32acc64 | acc,
|  | int | zero_acc,
|  | int | shift16,
|  | int | sub_mul,
|  | int | sub_acc1 )

## ◆ mac_elem_64() [1/8]

v64acc32 mac_elem_64 | ( | v64int16 | a,
|  | int | sgn_x,
|  | signed short | b,
|  | int | sgn_y,
|  | v64acc32 | acc )

## ◆ mac_elem_64() [2/8]

v64acc32 mac_elem_64 | ( | v64int16 | a,
|  | int | sgn_x,
|  | unsigned short | b,
|  | int | sgn_y,
|  | v64acc32 | acc )

## ◆ mac_elem_64() [3/8]

v64acc32 mac_elem_64 | ( | v64int16 | a,
|  | signed short | b,
|  | v64acc32 | acc )

## ◆ mac_elem_64() [4/8]

v64acc32 mac_elem_64 | ( | v64int16 | a,
|  | unsigned short | b,
|  | v64acc32 | acc )

## ◆ mac_elem_64() [5/8]

v64acc32 mac_elem_64 | ( | v64uint16 | a,
|  | int | sgn_x,
|  | signed short | b,
|  | int | sgn_y,
|  | v64acc32 | acc )

## ◆ mac_elem_64() [6/8]

v64acc32 mac_elem_64 | ( | v64uint16 | a,
|  | int | sgn_x,
|  | unsigned short | b,
|  | int | sgn_y,
|  | v64acc32 | acc )

## ◆ mac_elem_64() [7/8]

v64acc32 mac_elem_64 | ( | v64uint16 | a,
|  | signed short | b,
|  | v64acc32 | acc )

## ◆ mac_elem_64() [8/8]

v64acc32 mac_elem_64 | ( | v64uint16 | a,
|  | unsigned short | b,
|  | v64acc32 | acc )

## ◆ mac_elem_64_conf() [1/8]

v64acc32 mac_elem_64_conf | ( | v64int16 | a,
|  | int | sgn_x,
|  | signed short | b,
|  | int | sgn_y,
|  | v64acc32 | acc,
|  | int | zero_acc,
|  | int | shift16,
|  | int | sub_mul,
|  | int | sub_acc1 )

## ◆ mac_elem_64_conf() [2/8]

v64acc32 mac_elem_64_conf | ( | v64int16 | a,
|  | int | sgn_x,
|  | unsigned short | b,
|  | int | sgn_y,
|  | v64acc32 | acc,
|  | int | zero_acc,
|  | int | shift16,
|  | int | sub_mul,
|  | int | sub_acc1 )

## ◆ mac_elem_64_conf() [3/8]

v64acc32 mac_elem_64_conf | ( | v64int16 | a,
|  | signed short | b,
|  | v64acc32 | acc,
|  | int | zero_acc,
|  | int | shift16,
|  | int | sub_mul,
|  | int | sub_acc1 )

## ◆ mac_elem_64_conf() [4/8]

v64acc32 mac_elem_64_conf | ( | v64int16 | a,
|  | unsigned short | b,
|  | v64acc32 | acc,
|  | int | zero_acc,
|  | int | shift16,
|  | int | sub_mul,
|  | int | sub_acc1 )

## ◆ mac_elem_64_conf() [5/8]

v64acc32 mac_elem_64_conf | ( | v64uint16 | a,
|  | int | sgn_x,
|  | signed short | b,
|  | int | sgn_y,
|  | v64acc32 | acc,
|  | int | zero_acc,
|  | int | shift16,
|  | int | sub_mul,
|  | int | sub_acc1 )

## ◆ mac_elem_64_conf() [6/8]

v64acc32 mac_elem_64_conf | ( | v64uint16 | a,
|  | int | sgn_x,
|  | unsigned short | b,
|  | int | sgn_y,
|  | v64acc32 | acc,
|  | int | zero_acc,
|  | int | shift16,
|  | int | sub_mul,
|  | int | sub_acc1 )

## ◆ mac_elem_64_conf() [7/8]

v64acc32 mac_elem_64_conf | ( | v64uint16 | a,
|  | signed short | b,
|  | v64acc32 | acc,
|  | int | zero_acc,
|  | int | shift16,
|  | int | sub_mul,
|  | int | sub_acc1 )

## ◆ mac_elem_64_conf() [8/8]

v64acc32 mac_elem_64_conf | ( | v64uint16 | a,
|  | unsigned short | b,
|  | v64acc32 | acc,
|  | int | zero_acc,
|  | int | shift16,
|  | int | sub_mul,
|  | int | sub_acc1 )

## ◆ msc_elem_32() [1/8]

v32acc64 msc_elem_32 | ( | v32int16 | a,
|  | int | sgn_x,
|  | signed short | b,
|  | int | sgn_y,
|  | v32acc64 | acc )

## ◆ msc_elem_32() [2/8]

v32acc64 msc_elem_32 | ( | v32int16 | a,
|  | int | sgn_x,
|  | unsigned short | b,
|  | int | sgn_y,
|  | v32acc64 | acc )

## ◆ msc_elem_32() [3/8]

v32acc64 msc_elem_32 | ( | v32int16 | a,
|  | signed short | b,
|  | v32acc64 | acc )

## ◆ msc_elem_32() [4/8]

v32acc64 msc_elem_32 | ( | v32int16 | a,
|  | unsigned short | b,
|  | v32acc64 | acc )

## ◆ msc_elem_32() [5/8]

v32acc64 msc_elem_32 | ( | v32uint16 | a,
|  | int | sgn_x,
|  | signed short | b,
|  | int | sgn_y,
|  | v32acc64 | acc )

## ◆ msc_elem_32() [6/8]

v32acc64 msc_elem_32 | ( | v32uint16 | a,
|  | int | sgn_x,
|  | unsigned short | b,
|  | int | sgn_y,
|  | v32acc64 | acc )

## ◆ msc_elem_32() [7/8]

v32acc64 msc_elem_32 | ( | v32uint16 | a,
|  | signed short | b,
|  | v32acc64 | acc )

## ◆ msc_elem_32() [8/8]

v32acc64 msc_elem_32 | ( | v32uint16 | a,
|  | unsigned short | b,
|  | v32acc64 | acc )

## ◆ msc_elem_32_conf() [1/8]

v32acc64 msc_elem_32_conf | ( | v32int16 | a,
|  | int | sgn_x,
|  | signed short | b,
|  | int | sgn_y,
|  | v32acc64 | acc,
|  | int | zero_acc,
|  | int | shift16,
|  | int | sub_mul,
|  | int | sub_acc1 )

## ◆ msc_elem_32_conf() [2/8]

v32acc64 msc_elem_32_conf | ( | v32int16 | a,
|  | int | sgn_x,
|  | unsigned short | b,
|  | int | sgn_y,
|  | v32acc64 | acc,
|  | int | zero_acc,
|  | int | shift16,
|  | int | sub_mul,
|  | int | sub_acc1 )

## ◆ msc_elem_32_conf() [3/8]

v32acc64 msc_elem_32_conf | ( | v32int16 | a,
|  | signed short | b,
|  | v32acc64 | acc,
|  | int | zero_acc,
|  | int | shift16,
|  | int | sub_mul,
|  | int | sub_acc1 )

## ◆ msc_elem_32_conf() [4/8]

v32acc64 msc_elem_32_conf | ( | v32int16 | a,
|  | unsigned short | b,
|  | v32acc64 | acc,
|  | int | zero_acc,
|  | int | shift16,
|  | int | sub_mul,
|  | int | sub_acc1 )

## ◆ msc_elem_32_conf() [5/8]

v32acc64 msc_elem_32_conf | ( | v32uint16 | a,
|  | int | sgn_x,
|  | signed short | b,
|  | int | sgn_y,
|  | v32acc64 | acc,
|  | int | zero_acc,
|  | int | shift16,
|  | int | sub_mul,
|  | int | sub_acc1 )

## ◆ msc_elem_32_conf() [6/8]

v32acc64 msc_elem_32_conf | ( | v32uint16 | a,
|  | int | sgn_x,
|  | unsigned short | b,
|  | int | sgn_y,
|  | v32acc64 | acc,
|  | int | zero_acc,
|  | int | shift16,
|  | int | sub_mul,
|  | int | sub_acc1 )

## ◆ msc_elem_32_conf() [7/8]

v32acc64 msc_elem_32_conf | ( | v32uint16 | a,
|  | signed short | b,
|  | v32acc64 | acc,
|  | int | zero_acc,
|  | int | shift16,
|  | int | sub_mul,
|  | int | sub_acc1 )

## ◆ msc_elem_32_conf() [8/8]

v32acc64 msc_elem_32_conf | ( | v32uint16 | a,
|  | unsigned short | b,
|  | v32acc64 | acc,
|  | int | zero_acc,
|  | int | shift16,
|  | int | sub_mul,
|  | int | sub_acc1 )

## ◆ msc_elem_64() [1/8]

v64acc32 msc_elem_64 | ( | v64int16 | a,
|  | int | sgn_x,
|  | signed short | b,
|  | int | sgn_y,
|  | v64acc32 | acc )

## ◆ msc_elem_64() [2/8]

v64acc32 msc_elem_64 | ( | v64int16 | a,
|  | int | sgn_x,
|  | unsigned short | b,
|  | int | sgn_y,
|  | v64acc32 | acc )

## ◆ msc_elem_64() [3/8]

v64acc32 msc_elem_64 | ( | v64int16 | a,
|  | signed short | b,
|  | v64acc32 | acc )

## ◆ msc_elem_64() [4/8]

v64acc32 msc_elem_64 | ( | v64int16 | a,
|  | unsigned short | b,
|  | v64acc32 | acc )

## ◆ msc_elem_64() [5/8]

v64acc32 msc_elem_64 | ( | v64uint16 | a,
|  | int | sgn_x,
|  | signed short | b,
|  | int | sgn_y,
|  | v64acc32 | acc )

## ◆ msc_elem_64() [6/8]

v64acc32 msc_elem_64 | ( | v64uint16 | a,
|  | int | sgn_x,
|  | unsigned short | b,
|  | int | sgn_y,
|  | v64acc32 | acc )

## ◆ msc_elem_64() [7/8]

v64acc32 msc_elem_64 | ( | v64uint16 | a,
|  | signed short | b,
|  | v64acc32 | acc )

## ◆ msc_elem_64() [8/8]

v64acc32 msc_elem_64 | ( | v64uint16 | a,
|  | unsigned short | b,
|  | v64acc32 | acc )

## ◆ msc_elem_64_conf() [1/8]

v64acc32 msc_elem_64_conf | ( | v64int16 | a,
|  | int | sgn_x,
|  | signed short | b,
|  | int | sgn_y,
|  | v64acc32 | acc,
|  | int | zero_acc,
|  | int | shift16,
|  | int | sub_mul,
|  | int | sub_acc1 )

## ◆ msc_elem_64_conf() [2/8]

v64acc32 msc_elem_64_conf | ( | v64int16 | a,
|  | int | sgn_x,
|  | unsigned short | b,
|  | int | sgn_y,
|  | v64acc32 | acc,
|  | int | zero_acc,
|  | int | shift16,
|  | int | sub_mul,
|  | int | sub_acc1 )

## ◆ msc_elem_64_conf() [3/8]

v64acc32 msc_elem_64_conf | ( | v64int16 | a,
|  | signed short | b,
|  | v64acc32 | acc,
|  | int | zero_acc,
|  | int | shift16,
|  | int | sub_mul,
|  | int | sub_acc1 )

## ◆ msc_elem_64_conf() [4/8]

v64acc32 msc_elem_64_conf | ( | v64int16 | a,
|  | unsigned short | b,
|  | v64acc32 | acc,
|  | int | zero_acc,
|  | int | shift16,
|  | int | sub_mul,
|  | int | sub_acc1 )

## ◆ msc_elem_64_conf() [5/8]

v64acc32 msc_elem_64_conf | ( | v64uint16 | a,
|  | int | sgn_x,
|  | signed short | b,
|  | int | sgn_y,
|  | v64acc32 | acc,
|  | int | zero_acc,
|  | int | shift16,
|  | int | sub_mul,
|  | int | sub_acc1 )

## ◆ msc_elem_64_conf() [6/8]

v64acc32 msc_elem_64_conf | ( | v64uint16 | a,
|  | int | sgn_x,
|  | unsigned short | b,
|  | int | sgn_y,
|  | v64acc32 | acc,
|  | int | zero_acc,
|  | int | shift16,
|  | int | sub_mul,
|  | int | sub_acc1 )

## ◆ msc_elem_64_conf() [7/8]

v64acc32 msc_elem_64_conf | ( | v64uint16 | a,
|  | signed short | b,
|  | v64acc32 | acc,
|  | int | zero_acc,
|  | int | shift16,
|  | int | sub_mul,
|  | int | sub_acc1 )

## ◆ msc_elem_64_conf() [8/8]

v64acc32 msc_elem_64_conf | ( | v64uint16 | a,
|  | unsigned short | b,
|  | v64acc32 | acc,
|  | int | zero_acc,
|  | int | shift16,
|  | int | sub_mul,
|  | int | sub_acc1 )

## ◆ mul_elem_32() [1/8]

v32acc64 mul_elem_32 | ( | v32int16 | a,
|  | int | sgn_x,
|  | signed short | b,
|  | int | sgn_y )

## ◆ mul_elem_32() [2/8]

v32acc64 mul_elem_32 | ( | v32int16 | a,
|  | int | sgn_x,
|  | unsigned short | b,
|  | int | sgn_y )

## ◆ mul_elem_32() [3/8]

v32acc64 mul_elem_32 | ( | v32int16 | a,
|  | signed short | b )

## ◆ mul_elem_32() [4/8]

v32acc64 mul_elem_32 | ( | v32int16 | a,
|  | unsigned short | b )

## ◆ mul_elem_32() [5/8]

v32acc64 mul_elem_32 | ( | v32uint16 | a,
|  | int | sgn_x,
|  | signed short | b,
|  | int | sgn_y )

## ◆ mul_elem_32() [6/8]

v32acc64 mul_elem_32 | ( | v32uint16 | a,
|  | int | sgn_x,
|  | unsigned short | b,
|  | int | sgn_y )

## ◆ mul_elem_32() [7/8]

v32acc64 mul_elem_32 | ( | v32uint16 | a,
|  | signed short | b )

## ◆ mul_elem_32() [8/8]

v32acc64 mul_elem_32 | ( | v32uint16 | a,
|  | unsigned short | b )

## ◆ mul_elem_32_conf() [1/8]

v32acc64 mul_elem_32_conf | ( | v32int16 | a,
|  | int | sgn_x,
|  | signed short | b,
|  | int | sgn_y,
|  | int | sub_mul )

## ◆ mul_elem_32_conf() [2/8]

v32acc64 mul_elem_32_conf | ( | v32int16 | a,
|  | int | sgn_x,
|  | unsigned short | b,
|  | int | sgn_y,
|  | int | sub_mul )

## ◆ mul_elem_32_conf() [3/8]

v32acc64 mul_elem_32_conf | ( | v32int16 | a,
|  | signed short | b,
|  | int | sub_mul )

## ◆ mul_elem_32_conf() [4/8]

v32acc64 mul_elem_32_conf | ( | v32int16 | a,
|  | unsigned short | b,
|  | int | sub_mul )

## ◆ mul_elem_32_conf() [5/8]

v32acc64 mul_elem_32_conf | ( | v32uint16 | a,
|  | int | sgn_x,
|  | signed short | b,
|  | int | sgn_y,
|  | int | sub_mul )

## ◆ mul_elem_32_conf() [6/8]

v32acc64 mul_elem_32_conf | ( | v32uint16 | a,
|  | int | sgn_x,
|  | unsigned short | b,
|  | int | sgn_y,
|  | int | sub_mul )

## ◆ mul_elem_32_conf() [7/8]

v32acc64 mul_elem_32_conf | ( | v32uint16 | a,
|  | signed short | b,
|  | int | sub_mul )

## ◆ mul_elem_32_conf() [8/8]

v32acc64 mul_elem_32_conf | ( | v32uint16 | a,
|  | unsigned short | b,
|  | int | sub_mul )

## ◆ mul_elem_64() [1/8]

v64acc32 mul_elem_64 | ( | v64int16 | a,
|  | int | sgn_x,
|  | signed short | b,
|  | int | sgn_y )

## ◆ mul_elem_64() [2/8]

v64acc32 mul_elem_64 | ( | v64int16 | a,
|  | int | sgn_x,
|  | unsigned short | b,
|  | int | sgn_y )

## ◆ mul_elem_64() [3/8]

v64acc32 mul_elem_64 | ( | v64int16 | a,
|  | signed short | b )

## ◆ mul_elem_64() [4/8]

v64acc32 mul_elem_64 | ( | v64int16 | a,
|  | unsigned short | b )

## ◆ mul_elem_64() [5/8]

v64acc32 mul_elem_64 | ( | v64uint16 | a,
|  | int | sgn_x,
|  | signed short | b,
|  | int | sgn_y )

## ◆ mul_elem_64() [6/8]

v64acc32 mul_elem_64 | ( | v64uint16 | a,
|  | int | sgn_x,
|  | unsigned short | b,
|  | int | sgn_y )

## ◆ mul_elem_64() [7/8]

v64acc32 mul_elem_64 | ( | v64uint16 | a,
|  | signed short | b )

## ◆ mul_elem_64() [8/8]

v64acc32 mul_elem_64 | ( | v64uint16 | a,
|  | unsigned short | b )

## ◆ mul_elem_64_conf() [1/8]

v64acc32 mul_elem_64_conf | ( | v64int16 | a,
|  | int | sgn_x,
|  | signed short | b,
|  | int | sgn_y,
|  | int | sub_mul )

## ◆ mul_elem_64_conf() [2/8]

v64acc32 mul_elem_64_conf | ( | v64int16 | a,
|  | int | sgn_x,
|  | unsigned short | b,
|  | int | sgn_y,
|  | int | sub_mul )

## ◆ mul_elem_64_conf() [3/8]

v64acc32 mul_elem_64_conf | ( | v64int16 | a,
|  | signed short | b,
|  | int | sub_mul )

## ◆ mul_elem_64_conf() [4/8]

v64acc32 mul_elem_64_conf | ( | v64int16 | a,
|  | unsigned short | b,
|  | int | sub_mul )

## ◆ mul_elem_64_conf() [5/8]

v64acc32 mul_elem_64_conf | ( | v64uint16 | a,
|  | int | sgn_x,
|  | signed short | b,
|  | int | sgn_y,
|  | int | sub_mul )

## ◆ mul_elem_64_conf() [6/8]

v64acc32 mul_elem_64_conf | ( | v64uint16 | a,
|  | int | sgn_x,
|  | unsigned short | b,
|  | int | sgn_y,
|  | int | sub_mul )

## ◆ mul_elem_64_conf() [7/8]

v64acc32 mul_elem_64_conf | ( | v64uint16 | a,
|  | signed short | b,
|  | int | sub_mul )

## ◆ mul_elem_64_conf() [8/8]

v64acc32 mul_elem_64_conf | ( | v64uint16 | a,
|  | unsigned short | b,
|  | int | sub_mul )

## ◆ negmul_elem_32() [1/8]

v32acc64 negmul_elem_32 | ( | v32int16 | a,
|  | int | sgn_x,
|  | signed short | b,
|  | int | sgn_y )

## ◆ negmul_elem_32() [2/8]

v32acc64 negmul_elem_32 | ( | v32int16 | a,
|  | int | sgn_x,
|  | unsigned short | b,
|  | int | sgn_y )

## ◆ negmul_elem_32() [3/8]

v32acc64 negmul_elem_32 | ( | v32int16 | a,
|  | signed short | b )

## ◆ negmul_elem_32() [4/8]

v32acc64 negmul_elem_32 | ( | v32int16 | a,
|  | unsigned short | b )

## ◆ negmul_elem_32() [5/8]

v32acc64 negmul_elem_32 | ( | v32uint16 | a,
|  | int | sgn_x,
|  | signed short | b,
|  | int | sgn_y )

## ◆ negmul_elem_32() [6/8]

v32acc64 negmul_elem_32 | ( | v32uint16 | a,
|  | int | sgn_x,
|  | unsigned short | b,
|  | int | sgn_y )

## ◆ negmul_elem_32() [7/8]

v32acc64 negmul_elem_32 | ( | v32uint16 | a,
|  | signed short | b )

## ◆ negmul_elem_32() [8/8]

v32acc64 negmul_elem_32 | ( | v32uint16 | a,
|  | unsigned short | b )

## ◆ negmul_elem_32_conf() [1/8]

v32acc64 negmul_elem_32_conf | ( | v32int16 | a,
|  | int | sgn_x,
|  | signed short | b,
|  | int | sgn_y,
|  | int | sub_mul )

## ◆ negmul_elem_32_conf() [2/8]

v32acc64 negmul_elem_32_conf | ( | v32int16 | a,
|  | int | sgn_x,
|  | unsigned short | b,
|  | int | sgn_y,
|  | int | sub_mul )

## ◆ negmul_elem_32_conf() [3/8]

v32acc64 negmul_elem_32_conf | ( | v32int16 | a,
|  | signed short | b,
|  | int | sub_mul )

## ◆ negmul_elem_32_conf() [4/8]

v32acc64 negmul_elem_32_conf | ( | v32int16 | a,
|  | unsigned short | b,
|  | int | sub_mul )

## ◆ negmul_elem_32_conf() [5/8]

v32acc64 negmul_elem_32_conf | ( | v32uint16 | a,
|  | int | sgn_x,
|  | signed short | b,
|  | int | sgn_y,
|  | int | sub_mul )

## ◆ negmul_elem_32_conf() [6/8]

v32acc64 negmul_elem_32_conf | ( | v32uint16 | a,
|  | int | sgn_x,
|  | unsigned short | b,
|  | int | sgn_y,
|  | int | sub_mul )

## ◆ negmul_elem_32_conf() [7/8]

v32acc64 negmul_elem_32_conf | ( | v32uint16 | a,
|  | signed short | b,
|  | int | sub_mul )

## ◆ negmul_elem_32_conf() [8/8]

v32acc64 negmul_elem_32_conf | ( | v32uint16 | a,
|  | unsigned short | b,
|  | int | sub_mul )

## ◆ negmul_elem_64() [1/8]

v64acc32 negmul_elem_64 | ( | v64int16 | a,
|  | int | sgn_x,
|  | signed short | b,
|  | int | sgn_y )

## ◆ negmul_elem_64() [2/8]

v64acc32 negmul_elem_64 | ( | v64int16 | a,
|  | int | sgn_x,
|  | unsigned short | b,
|  | int | sgn_y )

## ◆ negmul_elem_64() [3/8]

v64acc32 negmul_elem_64 | ( | v64int16 | a,
|  | signed short | b )

## ◆ negmul_elem_64() [4/8]

v64acc32 negmul_elem_64 | ( | v64int16 | a,
|  | unsigned short | b )

## ◆ negmul_elem_64() [5/8]

v64acc32 negmul_elem_64 | ( | v64uint16 | a,
|  | int | sgn_x,
|  | signed short | b,
|  | int | sgn_y )

## ◆ negmul_elem_64() [6/8]

v64acc32 negmul_elem_64 | ( | v64uint16 | a,
|  | int | sgn_x,
|  | unsigned short | b,
|  | int | sgn_y )

## ◆ negmul_elem_64() [7/8]

v64acc32 negmul_elem_64 | ( | v64uint16 | a,
|  | signed short | b )

## ◆ negmul_elem_64() [8/8]

v64acc32 negmul_elem_64 | ( | v64uint16 | a,
|  | unsigned short | b )

## ◆ negmul_elem_64_conf() [1/8]

v64acc32 negmul_elem_64_conf | ( | v64int16 | a,
|  | int | sgn_x,
|  | signed short | b,
|  | int | sgn_y,
|  | int | sub_mul )

## ◆ negmul_elem_64_conf() [2/8]

v64acc32 negmul_elem_64_conf | ( | v64int16 | a,
|  | int | sgn_x,
|  | unsigned short | b,
|  | int | sgn_y,
|  | int | sub_mul )

## ◆ negmul_elem_64_conf() [3/8]

v64acc32 negmul_elem_64_conf | ( | v64int16 | a,
|  | signed short | b,
|  | int | sub_mul )

## ◆ negmul_elem_64_conf() [4/8]

v64acc32 negmul_elem_64_conf | ( | v64int16 | a,
|  | unsigned short | b,
|  | int | sub_mul )

## ◆ negmul_elem_64_conf() [5/8]

v64acc32 negmul_elem_64_conf | ( | v64uint16 | a,
|  | int | sgn_x,
|  | signed short | b,
|  | int | sgn_y,
|  | int | sub_mul )

## ◆ negmul_elem_64_conf() [6/8]

v64acc32 negmul_elem_64_conf | ( | v64uint16 | a,
|  | int | sgn_x,
|  | unsigned short | b,
|  | int | sgn_y,
|  | int | sub_mul )

## ◆ negmul_elem_64_conf() [7/8]

v64acc32 negmul_elem_64_conf | ( | v64uint16 | a,
|  | signed short | b,
|  | int | sub_mul )

## ◆ negmul_elem_64_conf() [8/8]

v64acc32 negmul_elem_64_conf | ( | v64uint16 | a,
|  | unsigned short | b,
|  | int | sub_mul )